[0x8086 0x29C0]
;This is PDT (PCI Device Template) file for intel 82P31/82G31 MCH chipset for SMB 2.08+
;on the 1st line is specified [vendor_id device_id] which will be probed
;line parameters (separated by one space) description:
;pci_function_block 32bit_register 32bit_mask bitshift format_string (optional: string4zero_value string4nonzero_value)
;
0 0x08 0x000000FF  0 "Revision ID: %lXh, "
0 0x08 0xFFFFFF00  8 "Class Code: %06lXh, "
0 0x04 0x0000FFFF  0 "PCI Command: %04lXh, "
0 0x04 0xFFFF0000 16 "Status: %04lXh\n"
0 0x2C 0x0000FFFF  0 "Subsystem Vendor ID: %04lXh, "
0 0x2E 0xFFFF0000 16 "Subsystem Identification: %04lXh\n"
0 0xA0 0x000003FF -6 "Total Physical Memory Size: %lu MB\n"
0 0x4C 0xFFFFFFFF  0 "MCH Base Address: %lX"
0 0x48 0xFFFFC000  0 "%08lXh (16 kB window) "
0 0x48 0x00000001  0 "- %s\n" "disabled" "enabled"
0 0x44 0xFFFFFFFF  0 "PCI-E Base Address: %lX"
0 0x40 0xFFFFF000  0 "%08lXh (4 kB window) "
0 0x40 0x00000001  0 "- %s\n" "disabled" "enabled"
0 0x64 0xFFFFFFFF  0 "PCI-E Register Range Base Address: %lX"
0 0x60 0xFC000000  0 "%08lXh (64-256 MB window) "
0 0x60 0x00000001  0 "- %s\n" "disabled" "enabled"
0 0x6C 0xFFFFFFFF  0 "DMI Base Address: %lX"
0 0x68 0xFFFFF000  0 "%08lXh (4 kB window) "
0 0x68 0x00000001  0 "- %s\n" "disabled" "enabled"
0 0xA4 0xFFF00000  0 "Graphics Base Address: %08lXh\n"
