FFMPEG-CODECS(1)

NAME
ffmpeg-codecs - FFmpeg codecs

DESCRIPTION
This document describes the codecs (decoders and encoders) provided by the libavcodec library.

CODEC OPTIONS
libavcodec provides some generic global options, which can be set on all the encoders and decoders. In addition each codec may support so-called private options, which are specific for a given codec.

Sometimes, a global option may only affect a specific kind of codec, and may be nonsensical or ignored by another, so you need to be aware of the meaning of the specified options. Also some options are meant only for decoding or encoding.

Options may be set by specifying -option value in the FFmpeg tools, or by setting the value explicitly in the "AVCodecContext" options or using the libavutil/opt.h API for programmatic use.

The list of supported options follow:

b integer (encoding,audio,video)
    Set bitrate in bits/s. Default value is 200K.

ab integer (encoding,audio)
    Set audio bitrate (in bits/s). Default value is 128K.

bt integer (encoding,video)
    Set video bitrate tolerance (in bits/s). In 1-pass mode, bitrate tolerance specifies how far ratecontrol is willing to deviate from the target average bitrate value. This is not related to min/max bitrate. Lowering tolerance too much has an adverse effect on quality.

flags flags (decoding/encoding,audio,video,subtitles)
    Set generic flags.

    Possible values:

    mv4 Use four motion vector by macroblock (mpeg4).

    qpel
        Use 1/4 pel motion compensation.

    loop
        Use loop filter.

    qscale
        Use fixed qscale.

    pass1
        Use internal 2pass ratecontrol in first pass mode.

    pass2
        Use internal 2pass ratecontrol in second pass mode.

    gray
        Only decode/encode grayscale.

    psnr
        Set error[?] variables during encoding.

    truncated
        Input bitstream might be randomly truncated.

    drop_changed
        Don't output frames whose parameters differ from first decoded frame in stream. Error AVERROR_INPUT_CHANGED is returned when a frame is dropped.

    ildct
        Use interlaced DCT.

    low_delay
        Force low delay.

    global_header
        Place global headers in extradata instead of every keyframe.

    bitexact
        Only write platform-, build- and time-independent data. (except (I)DCT). This ensures that file and data checksums are reproducible and match between platforms. Its primary use is for regression testing.

    aic Apply H263 advanced intra coding / mpeg4 ac prediction.

    ilme
        Apply interlaced motion estimation.

    cgop
        Use closed gop.

    output_corrupt
        Output even potentially corrupted frames.

time_base rational number
    Set codec time base.

    It is the fundamental unit of time (in seconds) in terms of which frame timestamps are represented. For fixed-fps content, timebase should be "1 / frame_rate" and timestamp increments should be identically 1.

g integer (encoding,video)
    Set the group of picture (GOP) size. Default value is 12.

ar integer (decoding/encoding,audio)
    Set audio sampling rate (in Hz).

ac integer (decoding/encoding,audio)
    Set number of audio channels.

cutoff integer (encoding,audio)
    Set cutoff bandwidth. (Supported only by selected encoders, see their respective documentation sections.)

frame_size integer (encoding,audio)
    Set audio frame size.

    Each submitted frame except the last must contain exactly frame_size samples per channel. May be 0 when the codec has CODEC_CAP_VARIABLE_FRAME_SIZE set, in that case the frame size is not restricted. It is set by some decoders to indicate constant frame size.

frame_number integer
    Set the frame number.

delay integer
qcomp float (encoding,video)
    Set video quantizer scale compression (VBR). It is used as a constant in the ratecontrol equation. Recommended range for default rc_eq: 0.0-1.0.

qblur float (encoding,video)
    Set video quantizer scale blur (VBR).

qmin integer (encoding,video)
    Set min video quantizer scale (VBR). Must be included between -1 and 69, default value is 2.

qmax integer (encoding,video)
    Set max video quantizer scale (VBR). Must be included between -1 and 1024, default value is 31.

qdiff integer (encoding,video)
    Set max difference between the quantizer scale (VBR).

bf integer (encoding,video)
    Set max number of B frames between non-B-frames.

    Must be an integer between -1 and 16. 0 means that B-frames are disabled. If a value of -1 is used, it will choose an automatic value depending on the encoder.

    Default value is 0.

b_qfactor float (encoding,video)
    Set qp factor between P and B frames.

b_strategy integer (encoding,video)
    Set strategy to choose between I/P/B-frames.

ps integer (encoding,video)
    Set RTP payload size in bytes.

mv_bits integer
header_bits integer
i_tex_bits integer
p_tex_bits integer
i_count integer
p_count integer
skip_count integer
misc_bits integer
frame_bits integer
codec_tag integer
bug flags (decoding,video)
    Workaround not auto detected encoder bugs.

    Possible values:

    autodetect
    xvid_ilace
        Xvid interlacing bug (autodetected if fourcc==XVIX)

    ump4
        (autodetected if fourcc==UMP4)

    no_padding
        padding bug (autodetected)

    amv
    qpel_chroma
    std_qpel
        old standard qpel (autodetected per fourcc/version)

    qpel_chroma2
    direct_blocksize
        direct-qpel-blocksize bug (autodetected per fourcc/version)

    edge
        edge padding bug (autodetected per fourcc/version)

    hpel_chroma
    dc_clip
    ms  Workaround various bugs in microsoft broken decoders.

    trunc
        trancated frames

strict integer (decoding/encoding,audio,video)
    Specify how strictly to follow the standards.

    Possible values:

    very
        strictly conform to an older more strict version of the spec or reference software

    strict
        strictly conform to all the things in the spec no matter what consequences

    normal
    unofficial
        allow unofficial extensions

    experimental
        allow non standardized experimental things, experimental (unfinished/work in progress/not well tested) decoders and encoders. Note: experimental decoders can pose a security risk, do not use this for decoding untrusted input.

b_qoffset float (encoding,video)
    Set QP offset between P and B frames.

err_detect flags (decoding,audio,video)
    Set error detection flags.

    Possible values:

    crccheck
        verify embedded CRCs

    bitstream
        detect bitstream specification deviations

    buffer
        detect improper bitstream length

    explode
        abort decoding on minor error detection

    ignore_err
        ignore decoding errors, and continue decoding. This is useful if you want to analyze the content of a video and thus want everything to be decoded no matter what. This option will not result in a video that is pleasing to watch in case of errors.

    careful
        consider things that violate the spec and have not been seen in the wild as errors

    compliant
        consider all spec non compliancies as errors

    aggressive
        consider things that a sane encoder should not do as an error

has_b_frames integer
block_align integer
mpeg_quant integer (encoding,video)
    Use MPEG quantizers instead of H.263.

rc_override_count integer
maxrate integer (encoding,audio,video)
    Set max bitrate tolerance (in bits/s). Requires bufsize to be set.

minrate integer (encoding,audio,video)
    Set min bitrate tolerance (in bits/s). Most useful in setting up a CBR encode. It is of little use elsewise.

bufsize integer (encoding,audio,video)
    Set ratecontrol buffer size (in bits).

i_qfactor float (encoding,video)
    Set QP factor between P and I frames.

i_qoffset float (encoding,video)
    Set QP offset between P and I frames.

dct integer (encoding,video)
    Set DCT algorithm.

    Possible values:

    auto
        autoselect a good one (default)

    fastint
        fast integer

    int accurate integer

    mmx
    altivec
    faan
        floating point AAN DCT

lumi_mask float (encoding,video)
    Compress bright areas stronger than medium ones.

tcplx_mask float (encoding,video)
    Set temporal complexity masking.

scplx_mask float (encoding,video)
    Set spatial complexity masking.

p_mask float (encoding,video)
    Set inter masking.

dark_mask float (encoding,video)
    Compress dark areas stronger than medium ones.

idct integer (decoding/encoding,video)
    Select IDCT implementation.

    Possible values:

    auto
    int
    simple
    simplemmx
    simpleauto
        Automatically pick a IDCT compatible with the simple one

    arm
    altivec
    sh4
    simplearm
    simplearmv5te
    simplearmv6
    simpleneon
    xvid
    faani
        floating point AAN IDCT

slice_count integer
ec flags (decoding,video)
    Set error concealment strategy.

    Possible values:

    guess_mvs
        iterative motion vector (MV) search (slow)

    deblock
        use strong deblock filter for damaged MBs

    favor_inter
        favor predicting from the previous frame instead of the current

bits_per_coded_sample integer
pred integer (encoding,video)
    Set prediction method.

    Possible values:

    left
    plane
    median
aspect rational number (encoding,video)
    Set sample aspect ratio.

sar rational number (encoding,video)
    Set sample aspect ratio. Alias to aspect.

debug flags (decoding/encoding,audio,video,subtitles)
    Print specific debug info.

    Possible values:

    pict
        picture info

    rc  rate control

    bitstream
    mb_type
        macroblock (MB) type

    qp  per-block quantization parameter (QP)

    dct_coeff
    green_metadata
        display complexity metadata for the upcoming frame, GoP or for a given duration.

    skip
    startcode
    er  error recognition

    mmco
        memory management control operations (H.264)

    bugs
    buffers
        picture buffer allocations

    thread_ops
        threading operations

    nomc
        skip motion compensation

cmp integer (encoding,video)
    Set full pel me compare function.

    Possible values:

    sad sum of absolute differences, fast (default)

    sse sum of squared errors

    satd
        sum of absolute Hadamard transformed differences

    dct sum of absolute DCT transformed differences

    psnr
        sum of squared quantization errors (avoid, low quality)

    bit number of bits needed for the block

    rd  rate distortion optimal, slow

    zero
        0

    vsad
        sum of absolute vertical differences

    vsse
        sum of squared vertical differences

    nsse
        noise preserving sum of squared differences

    w53 5/3 wavelet, only used in snow

    w97 9/7 wavelet, only used in snow

    dctmax
    chroma
subcmp integer (encoding,video)
    Set sub pel me compare function.

    Possible values:

    sad sum of absolute differences, fast (default)

    sse sum of squared errors

    satd
        sum of absolute Hadamard transformed differences

    dct sum of absolute DCT transformed differences

    psnr
        sum of squared quantization errors (avoid, low quality)

    bit number of bits needed for the block

    rd  rate distortion optimal, slow

    zero
        0

    vsad
        sum of absolute vertical differences

    vsse
        sum of squared vertical differences

    nsse
        noise preserving sum of squared differences

    w53 5/3 wavelet, only used in snow

    w97 9/7 wavelet, only used in snow

    dctmax
    chroma
mbcmp integer (encoding,video)
    Set macroblock compare function.

    Possible values:

    sad sum of absolute differences, fast (default)

    sse sum of squared errors

    satd
        sum of absolute Hadamard transformed differences

    dct sum of absolute DCT transformed differences

    psnr
        sum of squared quantization errors (avoid, low quality)

    bit number of bits needed for the block

    rd  rate distortion optimal, slow

    zero
        0

    vsad
        sum of absolute vertical differences

    vsse
        sum of squared vertical differences

    nsse
        noise preserving sum of squared differences

    w53 5/3 wavelet, only used in snow

    w97 9/7 wavelet, only used in snow

    dctmax
    chroma
ildctcmp integer (encoding,video)
    Set interlaced dct compare function.

    Possible values:

    sad sum of absolute differences, fast (default)

    sse sum of squared errors

    satd
        sum of absolute Hadamard transformed differences

    dct sum of absolute DCT transformed differences

    psnr
        sum of squared quantization errors (avoid, low quality)

    bit number of bits needed for the block

    rd  rate distortion optimal, slow

    zero
        0

    vsad
        sum of absolute vertical differences

    vsse
        sum of squared vertical differences

    nsse
        noise preserving sum of squared differences

    w53 5/3 wavelet, only used in snow

    w97 9/7 wavelet, only used in snow

    dctmax
    chroma
dia_size integer (encoding,video)
    Set diamond type & size for motion estimation.

    (1024, INT_MAX)
        full motion estimation(slowest)

    (768, 1024]
        umh motion estimation

    (512, 768]
        hex motion estimation

    (256, 512]
        l2s diamond motion estimation

    [2,256]
        var diamond motion estimation

    (-1,  2)
        small diamond motion estimation

    -1  funny diamond motion estimation

    (INT_MIN, -1)
        sab diamond motion estimation

last_pred integer (encoding,video)
    Set amount of motion predictors from the previous frame.

preme integer (encoding,video)
    Set pre motion estimation.

precmp integer (encoding,video)
    Set pre motion estimation compare function.

    Possible values:

    sad sum of absolute differences, fast (default)

    sse sum of squared errors

    satd
        sum of absolute Hadamard transformed differences

    dct sum of absolute DCT transformed differences

    psnr
        sum of squared quantization errors (avoid, low quality)

    bit number of bits needed for the block

    rd  rate distortion optimal, slow

    zero
        0

    vsad
        sum of absolute vertical differences

    vsse
        sum of squared vertical differences

    nsse
        noise preserving sum of squared differences

    w53 5/3 wavelet, only used in snow

    w97 9/7 wavelet, only used in snow

    dctmax
    chroma
pre_dia_size integer (encoding,video)
    Set diamond type & size for motion estimation pre-pass.

subq integer (encoding,video)
    Set sub pel motion estimation quality.

me_range integer (encoding,video)
    Set limit motion vectors range (1023 for DivX player).

global_quality integer (encoding,audio,video)
coder integer (encoding,video)
    Possible values:

    vlc variable length coder / huffman coder

    ac  arithmetic coder

    raw raw (no encoding)

    rle run-length coder

context integer (encoding,video)
    Set context model.

slice_flags integer
mbd integer (encoding,video)
    Set macroblock decision algorithm (high quality mode).

    Possible values:

    simple
        use mbcmp (default)

    bits
        use fewest bits

    rd  use best rate distortion

sc_threshold integer (encoding,video)
    Set scene change threshold.

nr integer (encoding,video)
    Set noise reduction.

rc_init_occupancy integer (encoding,video)
    Set number of bits which should be loaded into the rc buffer before decoding starts.

flags2 flags (decoding/encoding,audio,video,subtitles)
    Possible values:

    fast
        Allow non spec compliant speedup tricks.

    noout
        Skip bitstream encoding.

    ignorecrop
        Ignore cropping information from sps.

    local_header
        Place global headers at every keyframe instead of in extradata.

    chunks
        Frame data might be split into multiple chunks.

    showall
        Show all frames before the first keyframe.

    export_mvs
        Export motion vectors into frame side-data (see "AV_FRAME_DATA_MOTION_VECTORS") for codecs that support it. See also doc/examples/export_mvs.c.

    skip_manual
        Do not skip samples and export skip information as frame side data.

    ass_ro_flush_noop
        Do not reset ASS ReadOrder field on flush.

export_side_data flags (decoding/encoding,audio,video,subtitles)
    Possible values:

    mvs Export motion vectors into frame side-data (see "AV_FRAME_DATA_MOTION_VECTORS") for codecs that support it. See also doc/examples/export_mvs.c.

    prft
        Export encoder Producer Reference Time into packet side-data (see "AV_PKT_DATA_PRFT") for codecs that support it.

    venc_params
        Export video encoding parameters through frame side data (see "AV_FRAME_DATA_VIDEO_ENC_PARAMS") for codecs that support it. At present, those are H.264 and VP9.

    film_grain
        Export film grain parameters through frame side data (see "AV_FRAME_DATA_FILM_GRAIN_PARAMS"). Supported at present by AV1 decoders.

threads integer (decoding/encoding,video)
    Set the number of threads to be used, in case the selected codec implementation supports multi-threading.

    Possible values:

    auto, 0
        automatically select the number of threads to set

    Default value is auto.

dc integer (encoding,video)
    Set intra_dc_precision.

nssew integer (encoding,video)
    Set nsse weight.

skip_top integer (decoding,video)
    Set number of macroblock rows at the top which are skipped.

skip_bottom integer (decoding,video)
    Set number of macroblock rows at the bottom which are skipped.

profile integer (encoding,audio,video)
    Set encoder codec profile. Default value is unknown. Encoder specific profiles are documented in the relevant encoder documentation.

level integer (encoding,audio,video)
    Possible values:

    unknown
lowres integer (decoding,audio,video)
    Decode at 1= 1/2, 2=1/4, 3=1/8 resolutions.

skip_threshold integer (encoding,video)
    Set frame skip threshold.

skip_factor integer (encoding,video)
    Set frame skip factor.

skip_exp integer (encoding,video)
    Set frame skip exponent. Negative values behave identical to the corresponding positive ones, except that the score is normalized. Positive values exist primarily for compatibility reasons and are not so useful.

skipcmp integer (encoding,video)
    Set frame skip compare function.

    Possible values:

    sad sum of absolute differences, fast (default)

    sse sum of squared errors

    satd
        sum of absolute Hadamard transformed differences

    dct sum of absolute DCT transformed differences

    psnr
        sum of squared quantization errors (avoid, low quality)

    bit number of bits needed for the block

    rd  rate distortion optimal, slow

    zero
        0

    vsad
        sum of absolute vertical differences

    vsse
        sum of squared vertical differences

    nsse
        noise preserving sum of squared differences

    w53 5/3 wavelet, only used in snow

    w97 9/7 wavelet, only used in snow

    dctmax
    chroma
mblmin integer (encoding,video)
    Set min macroblock lagrange factor (VBR).

mblmax integer (encoding,video)
    Set max macroblock lagrange factor (VBR).

mepc integer (encoding,video)
    Set motion estimation bitrate penalty compensation (1.0 = 256).

skip_loop_filter integer (decoding,video)
skip_idct        integer (decoding,video)
skip_frame       integer (decoding,video)
    Make decoder discard processing depending on the frame type selected by the option value.

    skip_loop_filter skips frame loop filtering, skip_idct skips frame IDCT/dequantization, skip_frame skips decoding.

    Possible values:

    none
        Discard no frame.

    default
        Discard useless frames like 0-sized frames.

    noref
        Discard all non-reference frames.

    bidir
        Discard all bidirectional frames.

    nokey
        Discard all frames excepts keyframes.

    nointra
        Discard all frames except I frames.

    all Discard all frames.

    Default value is default.

bidir_refine integer (encoding,video)
    Refine the two motion vectors used in bidirectional macroblocks.

brd_scale integer (encoding,video)
    Downscale frames for dynamic B-frame decision.

keyint_min integer (encoding,video)
    Set minimum interval between IDR-frames.

refs integer (encoding,video)
    Set reference frames to consider for motion compensation.

chromaoffset integer (encoding,video)
    Set chroma qp offset from luma.

trellis integer (encoding,audio,video)
    Set rate-distortion optimal quantization.

mv0_threshold integer (encoding,video)
b_sensitivity integer (encoding,video)
    Adjust sensitivity of b_frame_strategy 1.

compression_level integer (encoding,audio,video)
min_prediction_order integer (encoding,audio)
max_prediction_order integer (encoding,audio)
timecode_frame_start integer (encoding,video)
    Set GOP timecode frame start number, in non drop frame format.

bits_per_raw_sample integer
channel_layout integer (decoding/encoding,audio)
    Possible values:

request_channel_layout integer (decoding,audio)
    Possible values:

rc_max_vbv_use float (encoding,video)
rc_min_vbv_use float (encoding,video)
ticks_per_frame integer (decoding/encoding,audio,video)
color_primaries integer (decoding/encoding,video)
    Possible values:

    bt709
        BT.709

    bt470m
        BT.470 M

    bt470bg
        BT.470 BG

    smpte170m
        SMPTE 170 M

    smpte240m
        SMPTE 240 M

    film
        Film

    bt2020
        BT.2020

    smpte428
    smpte428_1
        SMPTE ST 428-1

    smpte431
        SMPTE 431-2

    smpte432
        SMPTE 432-1

    jedec-p22
        JEDEC P22

color_trc integer (decoding/encoding,video)
    Possible values:

    bt709
        BT.709

    gamma22
        BT.470 M

    gamma28
        BT.470 BG

    smpte170m
        SMPTE 170 M

    smpte240m
        SMPTE 240 M

    linear
        Linear

    log
    log100
        Log

    log_sqrt
    log316
        Log square root

    iec61966_2_4
    iec61966-2-4
        IEC 61966-2-4

    bt1361
    bt1361e
        BT.1361

    iec61966_2_1
    iec61966-2-1
        IEC 61966-2-1

    bt2020_10
    bt2020_10bit
        BT.2020 - 10 bit

    bt2020_12
    bt2020_12bit
        BT.2020 - 12 bit

    smpte2084
        SMPTE ST 2084

    smpte428
    smpte428_1
        SMPTE ST 428-1

    arib-std-b67
        ARIB STD-B67

colorspace integer (decoding/encoding,video)
    Possible values:

    rgb RGB

    bt709
        BT.709

    fcc FCC

    bt470bg
        BT.470 BG

    smpte170m
        SMPTE 170 M

    smpte240m
        SMPTE 240 M

    ycocg
        YCOCG

    bt2020nc
    bt2020_ncl
        BT.2020 NCL

    bt2020c
    bt2020_cl
        BT.2020 CL

    smpte2085
        SMPTE 2085

    chroma-derived-nc
        Chroma-derived NCL

    chroma-derived-c
        Chroma-derived CL

    ictcp
        ICtCp

color_range integer (decoding/encoding,video)
    If used as input parameter, it serves as a hint to the decoder, which color_range the input has. Possible values:

    tv
    mpeg
        MPEG (219*2^(n-8))

    pc
    jpeg
        JPEG (2^n-1)

chroma_sample_location integer (decoding/encoding,video)
    Possible values:

    left
    center
    topleft
    top
    bottomleft
    bottom
log_level_offset integer
    Set the log level offset.

slices integer (encoding,video)
    Number of slices, used in parallelized encoding.

thread_type flags (decoding/encoding,video)
    Select which multithreading methods to use.

    Use of frame will increase decoding delay by one frame per thread, so clients which cannot provide future frames should not use it.

    Possible values:

    slice
        Decode more than one part of a single frame at once.

        Multithreading using slices works only when the video was encoded with slices.

    frame
        Decode more than one frame at once.

    Default value is slice+frame.

audio_service_type integer (encoding,audio)
    Set audio service type.

    Possible values:

    ma  Main Audio Service

    ef  Effects

    vi  Visually Impaired

    hi  Hearing Impaired

    di  Dialogue

    co  Commentary

    em  Emergency

    vo  Voice Over

    ka  Karaoke

request_sample_fmt sample_fmt (decoding,audio)
    Set sample format audio decoders should prefer. Default value is "none".

pkt_timebase rational number
sub_charenc encoding (decoding,subtitles)
    Set the input subtitles character encoding.

field_order  field_order (video)
    Set/override the field order of the video. Possible values:

    progressive
        Progressive video

    tt  Interlaced video, top field coded and displayed first

    bb  Interlaced video, bottom field coded and displayed first

    tb  Interlaced video, top coded first, bottom displayed first

    bt  Interlaced video, bottom coded first, top displayed first

skip_alpha bool (decoding,video)
    Set to 1 to disable processing alpha (transparency). This works like the gray flag in the flags option which skips chroma information instead of alpha. Default is 0.

codec_whitelist list (input)
    "," separated list of allowed decoders. By default all are allowed.

dump_separator string (input)
    Separator used to separate the fields printed on the command line about the Stream parameters. For example, to separate the fields with newlines and indentation:

            ffprobe -dump_separator "
                                      "  -i ~/videos/matrixbench_mpeg2.mpg

max_pixels integer (decoding/encoding,video)
    Maximum number of pixels per image. This value can be used to avoid out of memory failures due to large images.

apply_cropping bool (decoding,video)
    Enable cropping if cropping parameters are multiples of the required alignment for the left and top parameters. If the alignment is not met the cropping will be partially applied to maintain alignment. Default is 1 (enabled). Note: The required alignment depends on if "AV_CODEC_FLAG_UNALIGNED" is set and the CPU. "AV_CODEC_FLAG_UNALIGNED" cannot be changed from the command line. Also hardware decoders will not apply left/top Cropping.

DECODERS
Decoders are configured elements in FFmpeg which allow the decoding of multimedia streams.

When you configure your FFmpeg build, all the supported native decoders are enabled by default. Decoders requiring an external library must be enabled manually via the corresponding "--enable-lib" option. You can list all available decoders using the configure option "--list-decoders".

You can disable all the decoders with the configure option "--disable-decoders" and selectively enable / disable single decoders with the options "--enable-decoder=DECODER" / "--disable-decoder=DECODER".

The option "-decoders" of the ff* tools will display the list of enabled decoders.

VIDEO DECODERS
A description of some of the currently available video decoders follows.

  av1
AOMedia Video 1 (AV1) decoder.

Options

operating_point
    Select an operating point of a scalable AV1 bitstream (0 - 31). Default is 0.

  rawvideo
Raw video decoder.

This decoder decodes rawvideo streams.

Options

top top_field_first
    Specify the assumed field type of the input video.

    -1  the video is assumed to be progressive (default)

    0   bottom-field-first is assumed

    1   top-field-first is assumed

  libdav1d
dav1d AV1 decoder.

libdav1d allows libavcodec to decode the AOMedia Video 1 (AV1) codec. Requires the presence of the libdav1d headers and library during configuration. You need to explicitly configure the build with "--enable-libdav1d".

Options

The following options are supported by the libdav1d wrapper.

framethreads
    Set amount of frame threads to use during decoding. The default value is 0 (autodetect).

tilethreads
    Set amount of tile threads to use during decoding. The default value is 0 (autodetect).

filmgrain
    Apply film grain to the decoded video if present in the bitstream. Defaults to the internal default of the library.

oppoint
    Select an operating point of a scalable AV1 bitstream (0 - 31). Defaults to the internal default of the library.

alllayers
    Output all spatial layers of a scalable AV1 bitstream. The default value is false.

  libdavs2
AVS2-P2/IEEE1857.4 video decoder wrapper.

This decoder allows libavcodec to decode AVS2 streams with davs2 library.

  libuavs3d
AVS3-P2/IEEE1857.10 video decoder.

libuavs3d allows libavcodec to decode AVS3 streams. Requires the presence of the libuavs3d headers and library during configuration. You need to explicitly configure the build with "--enable-libuavs3d".

Options

The following option is supported by the libuavs3d wrapper.

frame_threads
    Set amount of frame threads to use during decoding. The default value is 0 (autodetect).

AUDIO DECODERS
A description of some of the currently available audio decoders follows.

  ac3
AC-3 audio decoder.

This decoder implements part of ATSC A/52:2010 and ETSI TS 102 366, as well as the undocumented RealAudio 3 (a.k.a. dnet).

AC-3 Decoder Options

-drc_scale value
    Dynamic Range Scale Factor. The factor to apply to dynamic range values from the AC-3 stream. This factor is applied exponentially. The default value is 1. There are 3 notable scale factor ranges:

    drc_scale == 0
        DRC disabled. Produces full range audio.

    0 < drc_scale <= 1
        DRC enabled. Applies a fraction of the stream DRC value. Audio reproduction is between full range and full compression.

    drc_scale > 1
        DRC enabled. Applies drc_scale asymmetrically. Loud sounds are fully compressed. Soft sounds are enhanced.

  flac
FLAC audio decoder.

This decoder aims to implement the complete FLAC specification from Xiph.

FLAC Decoder options

-use_buggy_lpc
    The lavc FLAC encoder used to produce buggy streams with high lpc values (like the default value). This option makes it possible to decode such streams correctly by using lavc's old buggy lpc logic for decoding.

  ffwavesynth
Internal wave synthesizer.

This decoder generates wave patterns according to predefined sequences. Its use is purely internal and the format of the data it accepts is not publicly documented.

  libcelt
libcelt decoder wrapper.

libcelt allows libavcodec to decode the Xiph CELT ultra-low delay audio codec. Requires the presence of the libcelt headers and library during configuration. You need to explicitly configure the build with "--enable-libcelt".

  libgsm
libgsm decoder wrapper.

libgsm allows libavcodec to decode the GSM full rate audio codec. Requires the presence of the libgsm headers and library during configuration. You need to explicitly configure the build with "--enable-libgsm".

This decoder supports both the ordinary GSM and the Microsoft variant.

  libilbc
libilbc decoder wrapper.

libilbc allows libavcodec to decode the Internet Low Bitrate Codec (iLBC) audio codec. Requires the presence of the libilbc headers and library during configuration. You need to explicitly configure the build with "--enable-libilbc".

Options

The following option is supported by the libilbc wrapper.

enhance
    Enable the enhancement of the decoded audio when set to 1. The default value is 0 (disabled).

  libopencore-amrnb
libopencore-amrnb decoder wrapper.

libopencore-amrnb allows libavcodec to decode the Adaptive Multi-Rate Narrowband audio codec. Using it requires the presence of the libopencore-amrnb headers and library during configuration. You need to explicitly configure the build with "--enable-libopencore-amrnb".

An FFmpeg native decoder for AMR-NB exists, so users can decode AMR-NB without this library.

  libopencore-amrwb
libopencore-amrwb decoder wrapper.

libopencore-amrwb allows libavcodec to decode the Adaptive Multi-Rate Wideband audio codec. Using it requires the presence of the libopencore-amrwb headers and library during configuration. You need to explicitly configure the build with "--enable-libopencore-amrwb".

An FFmpeg native decoder for AMR-WB exists, so users can decode AMR-WB without this library.

  libopus
libopus decoder wrapper.

libopus allows libavcodec to decode the Opus Interactive Audio Codec. Requires the presence of the libopus headers and library during configuration. You need to explicitly configure the build with "--enable-libopus".

An FFmpeg native decoder for Opus exists, so users can decode Opus without this library.

SUBTITLES DECODERS

  libaribb24
ARIB STD-B24 caption decoder.

Implements profiles A and C of the ARIB STD-B24 standard.

libaribb24 Decoder Options

-aribb24-base-path path
    Sets the base path for the libaribb24 library. This is utilized for reading of configuration files (for custom unicode conversions), and for dumping of non-text symbols as images under that location.

    Unset by default.

-aribb24-skip-ruby-text boolean
    Tells the decoder wrapper to skip text blocks that contain half-height ruby text.

    Enabled by default.

  dvbsub
Options

compute_clut
    -1  Compute clut if no matching CLUT is in the stream.

    0   Never compute CLUT

    1   Always compute CLUT and override the one provided in the stream.

dvb_substream
    Selects the dvb substream, or all substreams if -1 which is default.

  dvdsub
This codec decodes the bitmap subtitles used in DVDs; the same subtitles can also be found in VobSub file pairs and in some Matroska files.

Options

palette
    Specify the global palette used by the bitmaps. When stored in VobSub, the palette is normally specified in the index file; in Matroska, the palette is stored in the codec extra-data in the same format as in VobSub. In DVDs, the palette is stored in the IFO file, and therefore not available when reading from dumped VOB files.

    The format for this option is a string containing 16 24-bits hexadecimal numbers (without 0x prefix) separated by commas, for example "0d00ee, ee450d, 101010, eaeaea, 0ce60b, ec14ed, ebff0b, 0d617a, 7b7b7b, d1d1d1, 7b2a0e, 0d950c, 0f007b, cf0dec, cfa80c, 7c127b".

ifo_palette
    Specify the IFO file from which the global palette is obtained. (experimental)

forced_subs_only
    Only decode subtitle entries marked as forced. Some titles have forced and non-forced subtitles in the same track. Setting this flag to 1 will only keep the forced subtitles. Default value is 0.

  libzvbi-teletext
Libzvbi allows libavcodec to decode DVB teletext pages and DVB teletext subtitles. Requires the presence of the libzvbi headers and library during configuration. You need to explicitly configure the build with "--enable-libzvbi".

Options

txt_page
    List of teletext page numbers to decode. Pages that do not match the specified list are dropped. You may use the special "*" string to match all pages, or "subtitle" to match all subtitle pages. Default value is *.

txt_default_region
    Set default character set used for decoding, a value between 0 and 87 (see ETS 300 706, Section 15, Table 32). Default value is -1, which does not override the libzvbi default. This option is needed for some legacy level 1.0 transmissions which cannot signal the proper charset.

txt_chop_top
    Discards the top teletext line. Default value is 1.

txt_format
    Specifies the format of the decoded subtitles.

    bitmap
        The default format, you should use this for teletext pages, because certain graphics and colors cannot be expressed in simple text or even ASS.

    text
        Simple text based output without formatting.

    ass Formatted ASS output, subtitle pages and teletext pages are returned in different styles, subtitle pages are stripped down to text, but an effort is made to keep the text alignment and the formatting.

txt_left
    X offset of generated bitmaps, default is 0.

txt_top
    Y offset of generated bitmaps, default is 0.

txt_chop_spaces
    Chops leading and trailing spaces and removes empty lines from the generated text. This option is useful for teletext based subtitles where empty spaces may be present at the start or at the end of the lines or empty lines may be present between the subtitle lines because of double-sized teletext characters. Default value is 1.

txt_duration
    Sets the display duration of the decoded teletext pages or subtitles in milliseconds. Default value is -1 which means infinity or until the next subtitle event comes.

txt_transparent
    Force transparent background of the generated teletext bitmaps. Default value is 0 which means an opaque background.

txt_opacity
    Sets the opacity (0-255) of the teletext background. If txt_transparent is not set, it only affects characters between a start box and an end box, typically subtitles. Default value is 0 if txt_transparent is set, 255 otherwise.

ENCODERS
Encoders are configured elements in FFmpeg which allow the encoding of multimedia streams.

When you configure your FFmpeg build, all the supported native encoders are enabled by default. Encoders requiring an external library must be enabled manually via the corresponding "--enable-lib" option. You can list all available encoders using the configure option "--list-encoders".

You can disable all the encoders with the configure option "--disable-encoders" and selectively enable / disable single encoders with the options "--enable-encoder=ENCODER" / "--disable-encoder=ENCODER".

The option "-encoders" of the ff* tools will display the list of enabled encoders.

AUDIO ENCODERS
A description of some of the currently available audio encoders follows.

  aac
Advanced Audio Coding (AAC) encoder.

This encoder is the default AAC encoder, natively implemented into FFmpeg.

Options

b   Set bit rate in bits/s. Setting this automatically activates constant bit rate (CBR) mode. If this option is unspecified it is set to 128kbps.

q   Set quality for variable bit rate (VBR) mode. This option is valid only using the ffmpeg command-line tool. For library interface users, use global_quality.

cutoff
    Set cutoff frequency. If unspecified will allow the encoder to dynamically adjust the cutoff to improve clarity on low bitrates.

aac_coder
    Set AAC encoder coding method. Possible values:

    twoloop
        Two loop searching (TLS) method.

        This method first sets quantizers depending on band thresholds and then tries to find an optimal combination by adding or subtracting a specific value from all quantizers and adjusting some individual quantizer a little. Will tune itself based on whether aac_is, aac_ms and aac_pns are enabled.

    anmr
        Average noise to mask ratio (ANMR) trellis-based solution.

        This is an experimental coder which currently produces a lower quality, is more unstable and is slower than the default twoloop coder but has potential. Currently has no support for the aac_is or aac_pns options. Not currently recommended.

    fast
        Constant quantizer method.

        Uses a cheaper version of twoloop algorithm that doesn't try to do as many clever adjustments. Worse with low bitrates (less than 64kbps), but is better and much faster at higher bitrates. This is the default choice for a coder

aac_ms
    Sets mid/side coding mode. The default value of "auto" will automatically use M/S with bands which will benefit from such coding. Can be forced for all bands using the value "enable", which is mainly useful for debugging or disabled using "disable".

aac_is
    Sets intensity stereo coding tool usage. By default, it's enabled and will automatically toggle IS for similar pairs of stereo bands if it's beneficial. Can be disabled for debugging by setting the value to "disable".

aac_pns
    Uses perceptual noise substitution to replace low entropy high frequency bands with imperceptible white noise during the decoding process. By default, it's enabled, but can be disabled for debugging purposes by using "disable".

aac_tns
    Enables the use of a multitap FIR filter which spans through the high frequency bands to hide quantization noise during the encoding process and is reverted by the decoder. As well as decreasing unpleasant artifacts in the high range this also reduces the entropy in the high bands and allows for more bits to be used by the mid-low bands. By default it's enabled but can be disabled for debugging by setting the option to "disable".

aac_ltp
    Enables the use of the long term prediction extension which increases coding efficiency in very low bandwidth situations such as encoding of voice or solo piano music by extending constant harmonic peaks in bands throughout frames. This option is implied by profile:a aac_low and is incompatible with aac_pred. Use in conjunction with -ar to decrease the samplerate.

aac_pred
    Enables the use of a more traditional style of prediction where the spectral coefficients transmitted are replaced by the difference of the current coefficients minus the previous "predicted" coefficients. In theory and sometimes in practice this can improve quality for low to mid bitrate audio. This option implies the aac_main profile and is incompatible with aac_ltp.

profile
    Sets the encoding profile, possible values:

    aac_low
        The default, AAC "Low-complexity" profile. Is the most compatible and produces decent quality.

    mpeg2_aac_low
        Equivalent to "-profile:a aac_low -aac_pns 0". PNS was introduced with the MPEG4 specifications.

    aac_ltp
        Long term prediction profile, is enabled by and will enable the aac_ltp option. Introduced in MPEG4.

    aac_main
        Main-type prediction profile, is enabled by and will enable the aac_pred option. Introduced in MPEG2.

    If this option is unspecified it is set to aac_low.

  ac3 and ac3_fixed
AC-3 audio encoders.

These encoders implement part of ATSC A/52:2010 and ETSI TS 102 366, as well as the undocumented RealAudio 3 (a.k.a. dnet).

The ac3 encoder uses floating-point math, while the ac3_fixed encoder only uses fixed-point integer math. This does not mean that one is always faster, just that one or the other may be better suited to a particular system. The ac3_fixed encoder is not the default codec for any of the output formats, so it must be specified explicitly using the option "-acodec ac3_fixed" in order to use it.

AC-3 Metadata

The AC-3 metadata options are used to set parameters that describe the audio, but in most cases do not affect the audio encoding itself. Some of the options do directly affect or influence the decoding and playback of the resulting bitstream, while others are just for informational purposes. A few of the options will add bits to the output stream that could otherwise be used for audio data, and will thus affect the quality of the output. Those will be indicated accordingly with a note in the option list below.

These parameters are described in detail in several publicly-available documents.

*<<http://www.atsc.org/cms/standards/a_52-2010.pdf>>
*<<http://www.atsc.org/cms/standards/a_54a_with_corr_1.pdf>>
*<<http://www.dolby.com/uploadedFiles/zz-_Shared_Assets/English_PDFs/Professional/18_Metadata.Guide.pdf>>
*<<http://www.dolby.com/uploadedFiles/zz-_Shared_Assets/English_PDFs/Professional/46_DDEncodingGuidelines.pdf>>

Metadata Control Options

-per_frame_metadata boolean
    Allow Per-Frame Metadata. Specifies if the encoder should check for changing metadata for each frame.

    0   The metadata values set at initialization will be used for every frame in the stream. (default)

    1   Metadata values can be changed before encoding each frame.

Downmix Levels

-center_mixlev level
    Center Mix Level. The amount of gain the decoder should apply to the center channel when downmixing to stereo. This field will only be written to the bitstream if a center channel is present. The value is specified as a scale factor. There are 3 valid values:

    0.707
        Apply -3dB gain

    0.595
        Apply -4.5dB gain (default)

    0.500
        Apply -6dB gain

-surround_mixlev level
    Surround Mix Level. The amount of gain the decoder should apply to the surround channel(s) when downmixing to stereo. This field will only be written to the bitstream if one or more surround channels are present. The value is specified as a scale factor. There are 3 valid values:

    0.707
        Apply -3dB gain

    0.500
        Apply -6dB gain (default)

    0.000
        Silence Surround Channel(s)

Audio Production Information

Audio Production Information is optional information describing the mixing environment. Either none or both of the fields are written to the bitstream.

-mixing_level number
    Mixing Level. Specifies peak sound pressure level (SPL) in the production environment when the mix was mastered. Valid values are 80 to 111, or -1 for unknown or not indicated. The default value is -1, but that value cannot be used if the Audio Production Information is written to the bitstream. Therefore, if the "room_type" option is not the default value, the "mixing_level" option must not be -1.

-room_type type
    Room Type. Describes the equalization used during the final mixing session at the studio or on the dubbing stage. A large room is a dubbing stage with the industry standard X-curve equalization; a small room has flat equalization. This field will not be written to the bitstream if both the "mixing_level" option and the "room_type" option have the default values.

    0
    notindicated
        Not Indicated (default)

    1
    large
        Large Room

    2
    small
        Small Room

Other Metadata Options

-copyright boolean
    Copyright Indicator. Specifies whether a copyright exists for this audio.

    0
    off No Copyright Exists (default)

    1
    on  Copyright Exists

-dialnorm value
    Dialogue Normalization. Indicates how far the average dialogue level of the program is below digital 100% full scale (0 dBFS). This parameter determines a level shift during audio reproduction that sets the average volume of the dialogue to a preset level. The goal is to match volume level between program sources. A value of -31dB will result in no volume level change, relative to the source volume, during audio reproduction. Valid values are whole numbers in the range -31 to -1, with -31 being the default.

-dsur_mode mode
    Dolby Surround Mode. Specifies whether the stereo signal uses Dolby Surround (Pro Logic). This field will only be written to the bitstream if the audio stream is stereo. Using this option does NOT mean the encoder will actually apply Dolby Surround processing.

    0
    notindicated
        Not Indicated (default)

    1
    off Not Dolby Surround Encoded

    2
    on  Dolby Surround Encoded

-original boolean
    Original Bit Stream Indicator. Specifies whether this audio is from the original source and not a copy.

    0
    off Not Original Source

    1
    on  Original Source (default)

Extended Bitstream Information

The extended bitstream options are part of the Alternate Bit Stream Syntax as specified in Annex D of the A/52:2010 standard. It is grouped into 2 parts. If any one parameter in a group is specified, all values in that group will be written to the bitstream. Default values are used for those that are written but have not been specified. If the mixing levels are written, the decoder will use these values instead of the ones specified in the "center_mixlev" and "surround_mixlev" options if it supports the Alternate Bit Stream Syntax.

Extended Bitstream Information - Part 1

-dmix_mode mode
    Preferred Stereo Downmix Mode. Allows the user to select either Lt/Rt (Dolby Surround) or Lo/Ro (normal stereo) as the preferred stereo downmix mode.

    0
    notindicated
        Not Indicated (default)

    1
    ltrt
        Lt/Rt Downmix Preferred

    2
    loro
        Lo/Ro Downmix Preferred

-ltrt_cmixlev level
    Lt/Rt Center Mix Level. The amount of gain the decoder should apply to the center channel when downmixing to stereo in Lt/Rt mode.

    1.414
        Apply +3dB gain

    1.189
        Apply +1.5dB gain

    1.000
        Apply 0dB gain

    0.841
        Apply -1.5dB gain

    0.707
        Apply -3.0dB gain

    0.595
        Apply -4.5dB gain (default)

    0.500
        Apply -6.0dB gain

    0.000
        Silence Center Channel

-ltrt_surmixlev level
    Lt/Rt Surround Mix Level. The amount of gain the decoder should apply to the surround channel(s) when downmixing to stereo in Lt/Rt mode.

    0.841
        Apply -1.5dB gain

    0.707
        Apply -3.0dB gain

    0.595
        Apply -4.5dB gain

    0.500
        Apply -6.0dB gain (default)

    0.000
        Silence Surround Channel(s)

-loro_cmixlev level
    Lo/Ro Center Mix Level. The amount of gain the decoder should apply to the center channel when downmixing to stereo in Lo/Ro mode.

    1.414
        Apply +3dB gain

    1.189
        Apply +1.5dB gain

    1.000
        Apply 0dB gain

    0.841
        Apply -1.5dB gain

    0.707
        Apply -3.0dB gain

    0.595
        Apply -4.5dB gain (default)

    0.500
        Apply -6.0dB gain

    0.000
        Silence Center Channel

-loro_surmixlev level
    Lo/Ro Surround Mix Level. The amount of gain the decoder should apply to the surround channel(s) when downmixing to stereo in Lo/Ro mode.

    0.841
        Apply -1.5dB gain

    0.707
        Apply -3.0dB gain

    0.595
        Apply -4.5dB gain

    0.500
        Apply -6.0dB gain (default)

    0.000
        Silence Surround Channel(s)

Extended Bitstream Information - Part 2

-dsurex_mode mode
    Dolby Surround EX Mode. Indicates whether the stream uses Dolby Surround EX (7.1 matrixed to 5.1). Using this option does NOT mean the encoder will actually apply Dolby Surround EX processing.

    0
    notindicated
        Not Indicated (default)

    1
    on  Dolby Surround EX Off

    2
    off Dolby Surround EX On

-dheadphone_mode mode
    Dolby Headphone Mode. Indicates whether the stream uses Dolby Headphone encoding (multi-channel matrixed to 2.0 for use with headphones). Using this option does NOT mean the encoder will actually apply Dolby Headphone processing.

    0
    notindicated
        Not Indicated (default)

    1
    on  Dolby Headphone Off

    2
    off Dolby Headphone On

-ad_conv_type type
    A/D Converter Type. Indicates whether the audio has passed through HDCD A/D conversion.

    0
    standard
        Standard A/D Converter (default)

    1
    hdcd
        HDCD A/D Converter

Other AC-3 Encoding Options

-stereo_rematrixing boolean
    Stereo Rematrixing. Enables/Disables use of rematrixing for stereo input. This is an optional AC-3 feature that increases quality by selectively encoding the left/right channels as mid/side. This option is enabled by default, and it is highly recommended that it be left as enabled except for testing purposes.

cutoff frequency
    Set lowpass cutoff frequency. If unspecified, the encoder selects a default determined by various other encoding parameters.

Floating-Point-Only AC-3 Encoding Options

These options are only valid for the floating-point encoder and do not exist for the fixed-point encoder due to the corresponding features not being implemented in fixed-point.

-channel_coupling boolean
    Enables/Disables use of channel coupling, which is an optional AC-3 feature that increases quality by combining high frequency information from multiple channels into a single channel. The per-channel high frequency information is sent with less accuracy in both the frequency and time domains. This allows more bits to be used for lower frequencies while preserving enough information to reconstruct the high frequencies. This option is enabled by default for the floating-point encoder and should generally be left as enabled except for testing purposes or to increase encoding speed.

    -1
    auto
        Selected by Encoder (default)

    0
    off Disable Channel Coupling

    1
    on  Enable Channel Coupling

-cpl_start_band number
    Coupling Start Band. Sets the channel coupling start band, from 1 to 15. If a value higher than the bandwidth is used, it will be reduced to 1 less than the coupling end band. If auto is used, the start band will be determined by the encoder based on the bit rate, sample rate, and channel layout. This option has no effect if channel coupling is disabled.

    -1
    auto
        Selected by Encoder (default)

  flac
FLAC (Free Lossless Audio Codec) Encoder

Options

The following options are supported by FFmpeg's flac encoder.

compression_level
    Sets the compression level, which chooses defaults for many other options if they are not set explicitly. Valid values are from 0 to 12, 5 is the default.

frame_size
    Sets the size of the frames in samples per channel.

lpc_coeff_precision
    Sets the LPC coefficient precision, valid values are from 1 to 15, 15 is the default.

lpc_type
    Sets the first stage LPC algorithm

    none
        LPC is not used

    fixed
        fixed LPC coefficients

    levinson
    cholesky
lpc_passes
    Number of passes to use for Cholesky factorization during LPC analysis

min_partition_order
    The minimum partition order

max_partition_order
    The maximum partition order

prediction_order_method
    estimation
    2level
    4level
    8level
    search
        Bruteforce search

    log
ch_mode
    Channel mode

    auto
        The mode is chosen automatically for each frame

    indep
        Channels are independently coded

    left_side
    right_side
    mid_side
exact_rice_parameters
    Chooses if rice parameters are calculated exactly or approximately. if set to 1 then they are chosen exactly, which slows the code down slightly and improves compression slightly.

multi_dim_quant
    Multi Dimensional Quantization. If set to 1 then a 2nd stage LPC algorithm is applied after the first stage to finetune the coefficients. This is quite slow and slightly improves compression.

  opus
Opus encoder.

This is a native FFmpeg encoder for the Opus format. Currently its in development and only implements the CELT part of the codec. Its quality is usually worse and at best is equal to the libopus encoder.

Options

b   Set bit rate in bits/s. If unspecified it uses the number of channels and the layout to make a good guess.

opus_delay
    Sets the maximum delay in milliseconds. Lower delays than 20ms will very quickly decrease quality.

  libfdk_aac
libfdk-aac AAC (Advanced Audio Coding) encoder wrapper.

The libfdk-aac library is based on the Fraunhofer FDK AAC code from the Android project.

Requires the presence of the libfdk-aac headers and library during configuration. You need to explicitly configure the build with "--enable-libfdk-aac". The library is also incompatible with GPL, so if you allow the use of GPL, you should configure with "--enable-gpl --enable-nonfree --enable-libfdk-aac".

This encoder has support for the AAC-HE profiles.

VBR encoding, enabled through the vbr or flags +qscale options, is experimental and only works with some combinations of parameters.

Support for encoding 7.1 audio is only available with libfdk-aac 0.1.3 or higher.

For more information see the fdk-aac project at <http://sourceforge.net/p/opencore-amr/fdk-aac/>.

Options

The following options are mapped on the shared FFmpeg codec options.

b   Set bit rate in bits/s. If the bitrate is not explicitly specified, it is automatically set to a suitable value depending on the selected profile.

    In case VBR mode is enabled the option is ignored.

ar  Set audio sampling rate (in Hz).

channels
    Set the number of audio channels.

flags +qscale
    Enable fixed quality, VBR (Variable Bit Rate) mode. Note that VBR is implicitly enabled when the vbr value is positive.

cutoff
    Set cutoff frequency. If not specified (or explicitly set to 0) it will use a value automatically computed by the library. Default value is 0.

profile
    Set audio profile.

    The following profiles are recognized:

    aac_low
        Low Complexity AAC (LC)

    aac_he
        High Efficiency AAC (HE-AAC)

    aac_he_v2
        High Efficiency AAC version 2 (HE-AACv2)

    aac_ld
        Low Delay AAC (LD)

    aac_eld
        Enhanced Low Delay AAC (ELD)

    If not specified it is set to aac_low.

The following are private options of the libfdk_aac encoder.

afterburner
    Enable afterburner feature if set to 1, disabled if set to 0. This improves the quality but also the required processing power.

    Default value is 1.

eld_sbr
    Enable SBR (Spectral Band Replication) for ELD if set to 1, disabled if set to 0.

    Default value is 0.

eld_v2
    Enable ELDv2 (LD-MPS extension for ELD stereo signals) for ELDv2 if set to 1, disabled if set to 0.

    Note that option is available when fdk-aac version (AACENCODER_LIB_VL0.AACENCODER_LIB_VL1.AACENCODER_LIB_VL2) > (4.0.0).

    Default value is 0.

signaling
    Set SBR/PS signaling style.

    It can assume one of the following values:

    default
        choose signaling implicitly (explicit hierarchical by default, implicit if global header is disabled)

    implicit
        implicit backwards compatible signaling

    explicit_sbr
        explicit SBR, implicit PS signaling

    explicit_hierarchical
        explicit hierarchical signaling

    Default value is default.

latm
    Output LATM/LOAS encapsulated data if set to 1, disabled if set to 0.

    Default value is 0.

header_period
    Set StreamMuxConfig and PCE repetition period (in frames) for sending in-band configuration buffers within LATM/LOAS transport layer.

    Must be a 16-bits non-negative integer.

    Default value is 0.

vbr Set VBR mode, from 1 to 5. 1 is lowest quality (though still pretty good) and 5 is highest quality. A value of 0 will disable VBR, and CBR (Constant Bit Rate) is enabled.

    Currently only the aac_low profile supports VBR encoding.

    VBR modes 1-5 correspond to roughly the following average bit rates:

    1   32 kbps/channel

    2   40 kbps/channel

    3   48-56 kbps/channel

    4   64 kbps/channel

    5   about 80-96 kbps/channel

    Default value is 0.

Examples

•   Use ffmpeg to convert an audio file to VBR AAC in an M4A (MP4) container:

            ffmpeg -i input.wav -codec:a libfdk_aac -vbr 3 output.m4a

•   Use ffmpeg to convert an audio file to CBR 64k kbps AAC, using the High-Efficiency AAC profile:

            ffmpeg -i input.wav -c:a libfdk_aac -profile:a aac_he -b:a 64k output.m4a

  libmp3lame
LAME (Lame Ain't an MP3 Encoder) MP3 encoder wrapper.

Requires the presence of the libmp3lame headers and library during configuration. You need to explicitly configure the build with "--enable-libmp3lame".

See libshine for a fixed-point MP3 encoder, although with a lower quality.

Options

The following options are supported by the libmp3lame wrapper. The lame-equivalent of the options are listed in parentheses.

b (-b)
    Set bitrate expressed in bits/s for CBR or ABR. LAME "bitrate" is expressed in kilobits/s.

q (-V)
    Set constant quality setting for VBR. This option is valid only using the ffmpeg command-line tool. For library interface users, use global_quality.

compression_level (-q)
    Set algorithm quality. Valid arguments are integers in the 0-9 range, with 0 meaning highest quality but slowest, and 9 meaning fastest while producing the worst quality.

cutoff (--lowpass)
    Set lowpass cutoff frequency. If unspecified, the encoder dynamically adjusts the cutoff.

reservoir
    Enable use of bit reservoir when set to 1. Default value is 1. LAME has this enabled by default, but can be overridden by use --nores option.

joint_stereo (-m j)
    Enable the encoder to use (on a frame by frame basis) either L/R stereo or mid/side stereo. Default value is 1.

abr (--abr)
    Enable the encoder to use ABR when set to 1. The lame --abr sets the target bitrate, while this options only tells FFmpeg to use ABR still relies on b to set bitrate.

  libopencore-amrnb
OpenCORE Adaptive Multi-Rate Narrowband encoder.

Requires the presence of the libopencore-amrnb headers and library during configuration. You need to explicitly configure the build with "--enable-libopencore-amrnb --enable-version3".

This is a mono-only encoder. Officially it only supports 8000Hz sample rate, but you can override it by setting strict to unofficial or lower.

Options

b   Set bitrate in bits per second. Only the following bitrates are supported, otherwise libavcodec will round to the nearest valid bitrate.

    4750
    5150
    5900
    6700
    7400
    7950
    10200
    12200
dtx Allow discontinuous transmission (generate comfort noise) when set to 1. The default value is 0 (disabled).

  libopus
libopus Opus Interactive Audio Codec encoder wrapper.

Requires the presence of the libopus headers and library during configuration. You need to explicitly configure the build with "--enable-libopus".

Option Mapping

Most libopus options are modelled after the opusenc utility from opus-tools. The following is an option mapping chart describing options supported by the libopus wrapper, and their opusenc-equivalent in parentheses.

b (bitrate)
    Set the bit rate in bits/s. FFmpeg's b option is expressed in bits/s, while opusenc's bitrate in kilobits/s.

vbr (vbr, hard-cbr, and cvbr)
    Set VBR mode. The FFmpeg vbr option has the following valid arguments, with the opusenc equivalent options in parentheses:

    off (hard-cbr)
        Use constant bit rate encoding.

    on (vbr)
        Use variable bit rate encoding (the default).

    constrained (cvbr)
        Use constrained variable bit rate encoding.

compression_level (comp)
    Set encoding algorithm complexity. Valid options are integers in the 0-10 range. 0 gives the fastest encodes but lower quality, while 10 gives the highest quality but slowest encoding. The default is 10.

frame_duration (framesize)
    Set maximum frame size, or duration of a frame in milliseconds. The argument must be exactly the following: 2.5, 5, 10, 20, 40, 60. Smaller frame sizes achieve lower latency but less quality at a given bitrate. Sizes greater than 20ms are only interesting at fairly low bitrates. The default is 20ms.

packet_loss (expect-loss)
    Set expected packet loss percentage. The default is 0.

fec (n/a)
    Enable inband forward error correction. packet_loss must be non-zero to take advantage - frequency of FEC 'side-data' is proportional to expected packet loss. Default is disabled.

application (N.A.)
    Set intended application type. Valid options are listed below:

    voip
        Favor improved speech intelligibility.

    audio
        Favor faithfulness to the input (the default).

    lowdelay
        Restrict to only the lowest delay modes.

cutoff (N.A.)
    Set cutoff bandwidth in Hz. The argument must be exactly one of the following: 4000, 6000, 8000, 12000, or 20000, corresponding to narrowband, mediumband, wideband, super wideband, and fullband respectively. The default is 0 (cutoff disabled).

mapping_family (mapping_family)
    Set channel mapping family to be used by the encoder. The default value of -1 uses mapping family 0 for mono and stereo inputs, and mapping family 1 otherwise. The default also disables the surround masking and LFE bandwidth optimzations in libopus, and requires that the input contains 8 channels or fewer.

    Other values include 0 for mono and stereo, 1 for surround sound with masking and LFE bandwidth optimizations, and 255 for independent streams with an unspecified channel layout.

apply_phase_inv (N.A.) (requires libopus >= 1.2)
    If set to 0, disables the use of phase inversion for intensity stereo, improving the quality of mono downmixes, but slightly reducing normal stereo quality. The default is 1 (phase inversion enabled).

  libshine
Shine Fixed-Point MP3 encoder wrapper.

Shine is a fixed-point MP3 encoder. It has a far better performance on platforms without an FPU, e.g. armel CPUs, and some phones and tablets. However, as it is more targeted on performance than quality, it is not on par with LAME and other production-grade encoders quality-wise. Also, according to the project's homepage, this encoder may not be free of bugs as the code was written a long time ago and the project was dead for at least 5 years.

This encoder only supports stereo and mono input. This is also CBR-only.

The original project (last updated in early 2007) is at <http://sourceforge.net/projects/libshine-fxp/>. We only support the updated fork by the Savonet/Liquidsoap project at <https://github.com/savonet/shine>.

Requires the presence of the libshine headers and library during configuration. You need to explicitly configure the build with "--enable-libshine".

See also libmp3lame.

Options

The following options are supported by the libshine wrapper. The shineenc-equivalent of the options are listed in parentheses.

b (-b)
    Set bitrate expressed in bits/s for CBR. shineenc -b option is expressed in kilobits/s.

  libtwolame
TwoLAME MP2 encoder wrapper.

Requires the presence of the libtwolame headers and library during configuration. You need to explicitly configure the build with "--enable-libtwolame".

Options

The following options are supported by the libtwolame wrapper. The twolame-equivalent options follow the FFmpeg ones and are in parentheses.

b (-b)
    Set bitrate expressed in bits/s for CBR. twolame b option is expressed in kilobits/s. Default value is 128k.

q (-V)
    Set quality for experimental VBR support. Maximum value range is from -50 to 50, useful range is from -10 to 10. The higher the value, the better the quality. This option is valid only using the ffmpeg command-line tool. For library interface users, use global_quality.

mode (--mode)
    Set the mode of the resulting audio. Possible values:

    auto
        Choose mode automatically based on the input. This is the default.

    stereo
        Stereo

    joint_stereo
        Joint stereo

    dual_channel
        Dual channel

    mono
        Mono

psymodel (--psyc-mode)
    Set psychoacoustic model to use in encoding. The argument must be an integer between -1 and 4, inclusive. The higher the value, the better the quality. The default value is 3.

energy_levels (--energy)
    Enable energy levels extensions when set to 1. The default value is 0 (disabled).

error_protection (--protect)
    Enable CRC error protection when set to 1. The default value is 0 (disabled).

copyright (--copyright)
    Set MPEG audio copyright flag when set to 1. The default value is 0 (disabled).

original (--original)
    Set MPEG audio original flag when set to 1. The default value is 0 (disabled).

  libvo-amrwbenc
VisualOn Adaptive Multi-Rate Wideband encoder.

Requires the presence of the libvo-amrwbenc headers and library during configuration. You need to explicitly configure the build with "--enable-libvo-amrwbenc --enable-version3".

This is a mono-only encoder. Officially it only supports 16000Hz sample rate, but you can override it by setting strict to unofficial or lower.

Options

b   Set bitrate in bits/s. Only the following bitrates are supported, otherwise libavcodec will round to the nearest valid bitrate.

    6600
    8850
    12650
    14250
    15850
    18250
    19850
    23050
    23850
dtx Allow discontinuous transmission (generate comfort noise) when set to 1. The default value is 0 (disabled).

  libvorbis
libvorbis encoder wrapper.

Requires the presence of the libvorbisenc headers and library during configuration. You need to explicitly configure the build with "--enable-libvorbis".

Options

The following options are supported by the libvorbis wrapper. The oggenc-equivalent of the options are listed in parentheses.

To get a more accurate and extensive documentation of the libvorbis options, consult the libvorbisenc's and oggenc's documentations. See <http://xiph.org/vorbis/>, <http://wiki.xiph.org/Vorbis-tools>, and oggenc(1).

b (-b)
    Set bitrate expressed in bits/s for ABR. oggenc -b is expressed in kilobits/s.

q (-q)
    Set constant quality setting for VBR. The value should be a float number in the range of -1.0 to 10.0. The higher the value, the better the quality. The default value is 3.0.

    This option is valid only using the ffmpeg command-line tool. For library interface users, use global_quality.

cutoff (--advanced-encode-option lowpass_frequency=N)
    Set cutoff bandwidth in Hz, a value of 0 disables cutoff. oggenc's related option is expressed in kHz. The default value is 0 (cutoff disabled).

minrate (-m)
    Set minimum bitrate expressed in bits/s. oggenc -m is expressed in kilobits/s.

maxrate (-M)
    Set maximum bitrate expressed in bits/s. oggenc -M is expressed in kilobits/s. This only has effect on ABR mode.

iblock (--advanced-encode-option impulse_noisetune=N)
    Set noise floor bias for impulse blocks. The value is a float number from -15.0 to 0.0. A negative bias instructs the encoder to pay special attention to the crispness of transients in the encoded audio. The tradeoff for better transient response is a higher bitrate.

  mjpeg
Motion JPEG encoder.

Options

huffman
    Set the huffman encoding strategy. Possible values:

    default
        Use the default huffman tables. This is the default strategy.

    optimal
        Compute and use optimal huffman tables.

  wavpack
WavPack lossless audio encoder.

Options

The equivalent options for wavpack command line utility are listed in parentheses.

Shared options

The following shared options are effective for this encoder. Only special notes about this particular encoder will be documented here. For the general meaning of the options, see the Codec Options chapter.

frame_size (--blocksize)
    For this encoder, the range for this option is between 128 and 131072. Default is automatically decided based on sample rate and number of channel.

    For the complete formula of calculating default, see libavcodec/wavpackenc.c.

compression_level (-f, -h, -hh, and -x)

Private options

joint_stereo (-j)
    Set whether to enable joint stereo. Valid values are:

    on (1)
        Force mid/side audio encoding.

    off (0)
        Force left/right audio encoding.

    auto
        Let the encoder decide automatically.

optimize_mono
    Set whether to enable optimization for mono. This option is only effective for non-mono streams. Available values:

    on  enabled

    off disabled

VIDEO ENCODERS
A description of some of the currently available video encoders follows.

  GIF
GIF image/animation encoder.

Options

gifflags integer
    Sets the flags used for GIF encoding.

    offsetting
        Enables picture offsetting.

        Default is enabled.

    transdiff
        Enables transparency detection between frames.

        Default is enabled.

gifimage integer
    Enables encoding one full GIF image per frame, rather than an animated GIF.

    Default value is 0.

global_palette integer
    Writes a palette to the global GIF header where feasible.

    If disabled, every frame will always have a palette written, even if there is a global palette supplied.

    Default value is 1.

  Hap
Vidvox Hap video encoder.

Options

format integer
    Specifies the Hap format to encode.

    hap
    hap_alpha
    hap_q

    Default value is hap.

chunks integer
    Specifies the number of chunks to split frames into, between 1 and 64. This permits multithreaded decoding of large frames, potentially at the cost of data-rate. The encoder may modify this value to divide frames evenly.

    Default value is 1.

compressor integer
    Specifies the second-stage compressor to use. If set to none, chunks will be limited to 1, as chunked uncompressed frames offer no benefit.

    none
    snappy

    Default value is snappy.

  jpeg2000
The native jpeg 2000 encoder is lossy by default, the "-q:v" option can be used to set the encoding quality. Lossless encoding can be selected with "-pred 1".

Options

format integer
    Can be set to either "j2k" or "jp2" (the default) that makes it possible to store non-rgb pix_fmts.

tile_width integer
    Sets tile width. Range is 1 to 1073741824. Default is 256.

tile_height integer
    Sets tile height. Range is 1 to 1073741824. Default is 256.

pred integer
    Allows setting the discrete wavelet transform (DWT) type

    dwt97int (Lossy)
    dwt53 (Lossless)

    Default is "dwt97int"

sop boolean
    Enable this to add SOP marker at the start of each packet. Disabled by default.

eph boolean
    Enable this to add EPH marker at the end of each packet header. Disabled by default.

prog integer
    Sets the progression order to be used by the encoder. Possible values are:

    lrcp
    rlcp
    rpcl
    pcrl
    cprl

    Set to "lrcp" by default.

layer_rates string
    By default, when this option is not used, compression is done using the quality metric. This option allows for compression using compression ratio. The compression ratio for each level could be specified. The compression ratio of a layer "l" species the what ratio of total file size is contained in the first "l" layers.

    Example usage:

            ffmpeg -i input.bmp -c:v jpeg2000 -layer_rates "100,10,1" output.j2k

    This would compress the image to contain 3 layers, where the data contained in the first layer would be compressed by 1000 times, compressed by 100 in the first two layers, and shall contain all data while using all 3 layers.

  librav1e
rav1e AV1 encoder wrapper.

Requires the presence of the rav1e headers and library during configuration. You need to explicitly configure the build with "--enable-librav1e".

Options

qmax
    Sets the maximum quantizer to use when using bitrate mode.

qmin
    Sets the minimum quantizer to use when using bitrate mode.

qp  Uses quantizer mode to encode at the given quantizer (0-255).

speed
    Selects the speed preset (0-10) to encode with.

tiles
    Selects how many tiles to encode with.

tile-rows
    Selects how many rows of tiles to encode with.

tile-columns
    Selects how many columns of tiles to encode with.

rav1e-params
    Set rav1e options using a list of key=value pairs separated by ":". See rav1e --help for a list of options.

    For example to specify librav1e encoding options with -rav1e-params:

            ffmpeg -i input -c:v librav1e -b:v 500K -rav1e-params speed=5:low_latency=true output.mp4

  libaom-av1
libaom AV1 encoder wrapper.

Requires the presence of the libaom headers and library during configuration. You need to explicitly configure the build with "--enable-libaom".

Options

The wrapper supports the following standard libavcodec options:

b   Set bitrate target in bits/second. By default this will use variable-bitrate mode. If maxrate and minrate are also set to the same value then it will use constant-bitrate mode, otherwise if crf is set as well then it will use constrained-quality mode.

g keyint_min
    Set key frame placement. The GOP size sets the maximum distance between key frames; if zero the output stream will be intra-only. The minimum distance is ignored unless it is the same as the GOP size, in which case key frames will always appear at a fixed interval. Not set by default, so without this option the library has completely free choice about where to place key frames.

qmin qmax
    Set minimum/maximum quantisation values. Valid range is from 0 to 63 (warning: this does not match the quantiser values actually used by AV1 - divide by four to map real quantiser values to this range). Defaults to min/max (no constraint).

minrate maxrate bufsize rc_init_occupancy
    Set rate control buffering parameters. Not used if not set - defaults to unconstrained variable bitrate.

threads
    Set the number of threads to use while encoding. This may require the tiles or row-mt options to also be set to actually use the specified number of threads fully. Defaults to the number of hardware threads supported by the host machine.

profile
    Set the encoding profile. Defaults to using the profile which matches the bit depth and chroma subsampling of the input.

The wrapper also has some specific options:

cpu-used
    Set the quality/encoding speed tradeoff. Valid range is from 0 to 8, higher numbers indicating greater speed and lower quality. The default value is 1, which will be slow and high quality.

auto-alt-ref
    Enable use of alternate reference frames. Defaults to the internal default of the library.

arnr-max-frames (frames)
    Set altref noise reduction max frame count. Default is -1.

arnr-strength (strength)
    Set altref noise reduction filter strength. Range is -1 to 6. Default is -1.

aq-mode (aq-mode)
    Set adaptive quantization mode. Possible values:

    none (0)
        Disabled.

    variance (1)
        Variance-based.

    complexity (2)
        Complexity-based.

    cyclic (3)
        Cyclic refresh.

tune (tune)
    Set the distortion metric the encoder is tuned with. Default is "psnr".

    psnr (0)
    ssim (1)
lag-in-frames
    Set the maximum number of frames which the encoder may keep in flight at any one time for lookahead purposes. Defaults to the internal default of the library.

error-resilience
    Enable error resilience features:

    default
        Improve resilience against losses of whole frames.

    Not enabled by default.

crf Set the quality/size tradeoff for constant-quality (no bitrate target) and constrained-quality (with maximum bitrate target) modes. Valid range is 0 to 63, higher numbers indicating lower quality and smaller output size. Only used if set; by default only the bitrate target is used.

static-thresh
    Set a change threshold on blocks below which they will be skipped by the encoder. Defined in arbitrary units as a nonnegative integer, defaulting to zero (no blocks are skipped).

drop-threshold
    Set a threshold for dropping frames when close to rate control bounds. Defined as a percentage of the target buffer - when the rate control buffer falls below this percentage, frames will be dropped until it has refilled above the threshold. Defaults to zero (no frames are dropped).

denoise-noise-level (level)
    Amount of noise to be removed for grain synthesis. Grain synthesis is disabled if this option is not set or set to 0.

denoise-block-size (pixels)
    Block size used for denoising for grain synthesis. If not set, AV1 codec uses the default value of 32.

undershoot-pct (pct)
    Set datarate undershoot (min) percentage of the target bitrate. Range is -1 to 100. Default is -1.

overshoot-pct (pct)
    Set datarate overshoot (max) percentage of the target bitrate. Range is -1 to 1000. Default is -1.

minsection-pct (pct)
    Minimum percentage variation of the GOP bitrate from the target bitrate. If minsection-pct is not set, the libaomenc wrapper computes it as follows: "(minrate * 100 / bitrate)". Range is -1 to 100. Default is -1 (unset).

maxsection-pct (pct)
    Maximum percentage variation of the GOP bitrate from the target bitrate. If maxsection-pct is not set, the libaomenc wrapper computes it as follows: "(maxrate * 100 / bitrate)". Range is -1 to 5000. Default is -1 (unset).

frame-parallel (boolean)
    Enable frame parallel decodability features. Default is true.

tiles
    Set the number of tiles to encode the input video with, as columns x rows. Larger numbers allow greater parallelism in both encoding and decoding, but may decrease coding efficiency. Defaults to the minimum number of tiles required by the size of the input video (this is 1x1 (that is, a single tile) for sizes up to and including 4K).

tile-columns tile-rows
    Set the number of tiles as log2 of the number of tile rows and columns. Provided for compatibility with libvpx/VP9.

row-mt (Requires libaom >= 1.0.0-759-g90a15f4f2)
    Enable row based multi-threading. Disabled by default.

enable-cdef (boolean)
    Enable Constrained Directional Enhancement Filter. The libaom-av1 encoder enables CDEF by default.

enable-restoration (boolean)
    Enable Loop Restoration Filter. Default is true for libaom-av1.

enable-global-motion (boolean)
    Enable the use of global motion for block prediction. Default is true.

enable-intrabc (boolean)
    Enable block copy mode for intra block prediction. This mode is useful for screen content. Default is true.

enable-rect-partitions (boolean) (Requires libaom >= v2.0.0)
    Enable rectangular partitions. Default is true.

enable-1to4-partitions (boolean) (Requires libaom >= v2.0.0)
    Enable 1:4/4:1 partitions. Default is true.

enable-ab-partitions (boolean) (Requires libaom >= v2.0.0)
    Enable AB shape partitions. Default is true.

enable-angle-delta (boolean) (Requires libaom >= v2.0.0)
    Enable angle delta intra prediction. Default is true.

enable-cfl-intra (boolean) (Requires libaom >= v2.0.0)
    Enable chroma predicted from luma intra prediction. Default is true.

enable-filter-intra (boolean) (Requires libaom >= v2.0.0)
    Enable filter intra predictor. Default is true.

enable-intra-edge-filter (boolean) (Requires libaom >= v2.0.0)
    Enable intra edge filter. Default is true.

enable-smooth-intra (boolean) (Requires libaom >= v2.0.0)
    Enable smooth intra prediction mode. Default is true.

enable-paeth-intra (boolean) (Requires libaom >= v2.0.0)
    Enable paeth predictor in intra prediction. Default is true.

enable-palette (boolean) (Requires libaom >= v2.0.0)
    Enable palette prediction mode. Default is true.

enable-flip-idtx (boolean) (Requires libaom >= v2.0.0)
    Enable extended transform type, including FLIPADST_DCT, DCT_FLIPADST, FLIPADST_FLIPADST, ADST_FLIPADST, FLIPADST_ADST, IDTX, V_DCT, H_DCT, V_ADST, H_ADST, V_FLIPADST, H_FLIPADST. Default is true.

enable-tx64 (boolean) (Requires libaom >= v2.0.0)
    Enable 64-pt transform. Default is true.

reduced-tx-type-set (boolean) (Requires libaom >= v2.0.0)
    Use reduced set of transform types. Default is false.

use-intra-dct-only (boolean) (Requires libaom >= v2.0.0)
    Use DCT only for INTRA modes. Default is false.

use-inter-dct-only (boolean) (Requires libaom >= v2.0.0)
    Use DCT only for INTER modes. Default is false.

use-intra-default-tx-only (boolean) (Requires libaom >= v2.0.0)
    Use Default-transform only for INTRA modes. Default is false.

enable-ref-frame-mvs (boolean) (Requires libaom >= v2.0.0)
    Enable temporal mv prediction. Default is true.

enable-reduced-reference-set (boolean) (Requires libaom >= v2.0.0)
    Use reduced set of single and compound references. Default is false.

enable-obmc (boolean) (Requires libaom >= v2.0.0)
    Enable obmc. Default is true.

enable-dual-filter (boolean) (Requires libaom >= v2.0.0)
    Enable dual filter. Default is true.

enable-diff-wtd-comp (boolean) (Requires libaom >= v2.0.0)
    Enable difference-weighted compound. Default is true.

enable-dist-wtd-comp (boolean) (Requires libaom >= v2.0.0)
    Enable distance-weighted compound. Default is true.

enable-onesided-comp (boolean) (Requires libaom >= v2.0.0)
    Enable one sided compound. Default is true.

enable-interinter-wedge (boolean) (Requires libaom >= v2.0.0)
    Enable interinter wedge compound. Default is true.

enable-interintra-wedge (boolean) (Requires libaom >= v2.0.0)
    Enable interintra wedge compound. Default is true.

enable-masked-comp (boolean) (Requires libaom >= v2.0.0)
    Enable masked compound. Default is true.

enable-interintra-comp (boolean) (Requires libaom >= v2.0.0)
    Enable interintra compound. Default is true.

enable-smooth-interintra (boolean) (Requires libaom >= v2.0.0)
    Enable smooth interintra mode. Default is true.

aom-params
    Set libaom options using a list of key=value pairs separated by ":". For a list of supported options, see aomenc --help under the section "AV1 Specific Options".

    For example to specify libaom encoding options with -aom-params:

            ffmpeg -i input -c:v libaom-av1 -b:v 500K -aom-params tune=psnr:enable-tpl-model=1 output.mp4

  libsvtav1
SVT-AV1 encoder wrapper.

Requires the presence of the SVT-AV1 headers and library during configuration. You need to explicitly configure the build with "--enable-libsvtav1".

Options

profile
    Set the encoding profile.

level
    Set the operating point level.

tier
    Set the operating point tier.

rc  Set the rate control mode to use.

    Possible modes:

    cqp Constant quantizer: use fixed values of qindex (dependent on the frame type) throughout the stream. This mode is the default.

    vbr Variable bitrate: use a target bitrate for the whole stream.

    cvbr
        Constrained variable bitrate: use a target bitrate for each GOP.

qmax
    Set the maximum quantizer to use when using a bitrate mode.

qmin
    Set the minimum quantizer to use when using a bitrate mode.

qp  Set the quantizer used in cqp rate control mode (0-63).

sc_detection
    Enable scene change detection.

la_depth
    Set number of frames to look ahead (0-120).

preset
    Set the quality-speed tradeoff, in the range 0 to 8. Higher values are faster but lower quality. Defaults to 8 (highest speed).

tile_rows
    Set log2 of the number of rows of tiles to use (0-6).

tile_columns
    Set log2 of the number of columns of tiles to use (0-4).

  libkvazaar
Kvazaar H.265/HEVC encoder.

Requires the presence of the libkvazaar headers and library during configuration. You need to explicitly configure the build with --enable-libkvazaar.

Options

b   Set target video bitrate in bit/s and enable rate control.

kvazaar-params
    Set kvazaar parameters as a list of name=value pairs separated by commas (,). See kvazaar documentation for a list of options.

  libopenh264
Cisco libopenh264 H.264/MPEG-4 AVC encoder wrapper.

This encoder requires the presence of the libopenh264 headers and library during configuration. You need to explicitly configure the build with "--enable-libopenh264". The library is detected using pkg-config.

For more information about the library see <http://www.openh264.org>.

Options

The following FFmpeg global options affect the configurations of the libopenh264 encoder.

b   Set the bitrate (as a number of bits per second).

g   Set the GOP size.

maxrate
    Set the max bitrate (as a number of bits per second).

flags +global_header
    Set global header in the bitstream.

slices
    Set the number of slices, used in parallelized encoding. Default value is 0. This is only used when slice_mode is set to fixed.

slice_mode
    Set slice mode. Can assume one of the following possible values:

    fixed
        a fixed number of slices

    rowmb
        one slice per row of macroblocks

    auto
        automatic number of slices according to number of threads

    dyn dynamic slicing

    Default value is auto.

loopfilter
    Enable loop filter, if set to 1 (automatically enabled). To disable set a value of 0.

profile
    Set profile restrictions. If set to the value of main enable CABAC (set the "SEncParamExt.iEntropyCodingModeFlag" flag to 1).

max_nal_size
    Set maximum NAL size in bytes.

allow_skip_frames
    Allow skipping frames to hit the target bitrate if set to 1.

  libtheora
libtheora Theora encoder wrapper.

Requires the presence of the libtheora headers and library during configuration. You need to explicitly configure the build with "--enable-libtheora".

For more information about the libtheora project see <http://www.theora.org/>.

Options

The following global options are mapped to internal libtheora options which affect the quality and the bitrate of the encoded stream.

b   Set the video bitrate in bit/s for CBR (Constant Bit Rate) mode. In case VBR (Variable Bit Rate) mode is enabled this option is ignored.

flags
    Used to enable constant quality mode (VBR) encoding through the qscale flag, and to enable the "pass1" and "pass2" modes.

g   Set the GOP size.

global_quality
    Set the global quality as an integer in lambda units.

    Only relevant when VBR mode is enabled with "flags +qscale". The value is converted to QP units by dividing it by "FF_QP2LAMBDA", clipped in the [0 - 10] range, and then multiplied by 6.3 to get a value in the native libtheora range [0-63]. A higher value corresponds to a higher quality.

q   Enable VBR mode when set to a non-negative value, and set constant quality value as a double floating point value in QP units.

    The value is clipped in the [0-10] range, and then multiplied by 6.3 to get a value in the native libtheora range [0-63].

    This option is valid only using the ffmpeg command-line tool. For library interface users, use global_quality.

Examples

•   Set maximum constant quality (VBR) encoding with ffmpeg:

            ffmpeg -i INPUT -codec:v libtheora -q:v 10 OUTPUT.ogg

•   Use ffmpeg to convert a CBR 1000 kbps Theora video stream:

            ffmpeg -i INPUT -codec:v libtheora -b:v 1000k OUTPUT.ogg

  libvpx
VP8/VP9 format supported through libvpx.

Requires the presence of the libvpx headers and library during configuration. You need to explicitly configure the build with "--enable-libvpx".

Options

The following options are supported by the libvpx wrapper. The vpxenc-equivalent options or values are listed in parentheses for easy migration.

To reduce the duplication of documentation, only the private options and some others requiring special attention are documented here. For the documentation of the undocumented generic options, see the Codec Options chapter.

To get more documentation of the libvpx options, invoke the command ffmpeg -h encoder=libvpx, ffmpeg -h encoder=libvpx-vp9 or vpxenc --help. Further information is available in the libvpx API documentation.

b (target-bitrate)
    Set bitrate in bits/s. Note that FFmpeg's b option is expressed in bits/s, while vpxenc's target-bitrate is in kilobits/s.

g (kf-max-dist)
keyint_min (kf-min-dist)
qmin (min-q)
qmax (max-q)
bufsize (buf-sz, buf-optimal-sz)
    Set ratecontrol buffer size (in bits). Note vpxenc's options are specified in milliseconds, the libvpx wrapper converts this value as follows: "buf-sz = bufsize * 1000 / bitrate", "buf-optimal-sz = bufsize * 1000 / bitrate * 5 / 6".

rc_init_occupancy (buf-initial-sz)
    Set number of bits which should be loaded into the rc buffer before decoding starts. Note vpxenc's option is specified in milliseconds, the libvpx wrapper converts this value as follows: "rc_init_occupancy * 1000 / bitrate".

undershoot-pct
    Set datarate undershoot (min) percentage of the target bitrate.

overshoot-pct
    Set datarate overshoot (max) percentage of the target bitrate.

skip_threshold (drop-frame)
qcomp (bias-pct)
maxrate (maxsection-pct)
    Set GOP max bitrate in bits/s. Note vpxenc's option is specified as a percentage of the target bitrate, the libvpx wrapper converts this value as follows: "(maxrate * 100 / bitrate)".

minrate (minsection-pct)
    Set GOP min bitrate in bits/s. Note vpxenc's option is specified as a percentage of the target bitrate, the libvpx wrapper converts this value as follows: "(minrate * 100 / bitrate)".

minrate, maxrate, b end-usage=cbr
    "(minrate == maxrate == bitrate)".

crf (end-usage=cq, cq-level)
tune (tune)
    psnr (psnr)
    ssim (ssim)
quality, deadline (deadline)
    best
        Use best quality deadline. Poorly named and quite slow, this option should be avoided as it may give worse quality output than good.

    good
        Use good quality deadline. This is a good trade-off between speed and quality when used with the cpu-used option.

    realtime
        Use realtime quality deadline.

speed, cpu-used (cpu-used)
    Set quality/speed ratio modifier. Higher values speed up the encode at the cost of quality.

nr (noise-sensitivity)
static-thresh
    Set a change threshold on blocks below which they will be skipped by the encoder.

slices (token-parts)
    Note that FFmpeg's slices option gives the total number of partitions, while vpxenc's token-parts is given as "log2(partitions)".

max-intra-rate
    Set maximum I-frame bitrate as a percentage of the target bitrate. A value of 0 means unlimited.

force_key_frames
    "VPX_EFLAG_FORCE_KF"

Alternate reference frame related
    auto-alt-ref
        Enable use of alternate reference frames (2-pass only). Values greater than 1 enable multi-layer alternate reference frames (VP9 only).

    arnr-maxframes
        Set altref noise reduction max frame count.

    arnr-type
        Set altref noise reduction filter type: backward, forward, centered.

    arnr-strength
        Set altref noise reduction filter strength.

    rc-lookahead, lag-in-frames (lag-in-frames)
        Set number of frames to look ahead for frametype and ratecontrol.

error-resilient
    Enable error resiliency features.

sharpness integer
    Increase sharpness at the expense of lower PSNR. The valid range is [0, 7].

ts-parameters
    Sets the temporal scalability configuration using a :-separated list of key=value pairs. For example, to specify temporal scalability parameters with "ffmpeg":

            ffmpeg -i INPUT -c:v libvpx -ts-parameters ts_number_layers=3:\
            ts_target_bitrate=250,500,1000:ts_rate_decimator=4,2,1:\
            ts_periodicity=4:ts_layer_id=0,2,1,2:ts_layering_mode=3 OUTPUT

    Below is a brief explanation of each of the parameters, please refer to "struct vpx_codec_enc_cfg" in "vpx/vpx_encoder.h" for more details.

    ts_number_layers
        Number of temporal coding layers.

    ts_target_bitrate
        Target bitrate for each temporal layer (in kbps). (bitrate should be inclusive of the lower temporal layer).

    ts_rate_decimator
        Frame rate decimation factor for each temporal layer.

    ts_periodicity
        Length of the sequence defining frame temporal layer membership.

    ts_layer_id
        Template defining the membership of frames to temporal layers.

    ts_layering_mode
        (optional) Selecting the temporal structure from a set of pre-defined temporal layering modes. Currently supports the following options.

        0   No temporal layering flags are provided internally, relies on flags being passed in using "metadata" field in "AVFrame" with following keys.

            vp8-flags
                Sets the flags passed into the encoder to indicate the referencing scheme for the current frame. Refer to function "vpx_codec_encode" in "vpx/vpx_encoder.h" for more details.

            temporal_id
                Explicitly sets the temporal id of the current frame to encode.

        2   Two temporal layers. 0-1...

        3   Three temporal layers. 0-2-1-2...; with single reference frame.

        4   Same as option "3", except there is a dependency between the two temporal layer 2 frames within the temporal period.

VP9-specific options
    lossless
        Enable lossless mode.

    tile-columns
        Set number of tile columns to use. Note this is given as "log2(tile_columns)". For example, 8 tile columns would be requested by setting the tile-columns option to 3.

    tile-rows
        Set number of tile rows to use. Note this is given as "log2(tile_rows)". For example, 4 tile rows would be requested by setting the tile-rows option to 2.

    frame-parallel
        Enable frame parallel decodability features.

    aq-mode
        Set adaptive quantization mode (0: off (default), 1: variance 2: complexity, 3: cyclic refresh, 4: equator360).

    colorspace color-space
        Set input color space. The VP9 bitstream supports signaling the following colorspaces:

        rgb sRGB
        bt709 bt709
        unspecified unknown
        bt470bg bt601
        smpte170m smpte170
        smpte240m smpte240
        bt2020_ncl bt2020
    row-mt boolean
        Enable row based multi-threading.

    tune-content
        Set content type: default (0), screen (1), film (2).

    corpus-complexity
        Corpus VBR mode is a variant of standard VBR where the complexity distribution midpoint is passed in rather than calculated for a specific clip or chunk.

        The valid range is [0, 10000]. 0 (default) uses standard VBR.

    enable-tpl boolean
        Enable temporal dependency model.

    ref-frame-config
        Using per-frame metadata, set members of the structure "vpx_svc_ref_frame_config_t" in "vpx/vp8cx.h" to fine-control referencing schemes and frame buffer management. Use a :-separated list of key=value pairs. For example,

                av_dict_set(&av_frame->metadata, "ref-frame-config", \
                "rfc_update_buffer_slot=7:rfc_lst_fb_idx=0:rfc_gld_fb_idx=1:rfc_alt_fb_idx=2:rfc_reference_last=0:rfc_reference_golden=0:rfc_reference_alt_ref=0");

        rfc_update_buffer_slot
            Indicates the buffer slot number to update

        rfc_update_last
            Indicates whether to update the LAST frame

        rfc_update_golden
            Indicates whether to update GOLDEN frame

        rfc_update_alt_ref
            Indicates whether to update ALT_REF frame

        rfc_lst_fb_idx
            LAST frame buffer index

        rfc_gld_fb_idx
            GOLDEN frame buffer index

        rfc_alt_fb_idx
            ALT_REF frame buffer index

        rfc_reference_last
            Indicates whether to reference LAST frame

        rfc_reference_golden
            Indicates whether to reference GOLDEN frame

        rfc_reference_alt_ref
            Indicates whether to reference ALT_REF frame

        rfc_reference_duration
            Indicates frame duration

For more information about libvpx see: <http://www.webmproject.org/>

  libwebp
libwebp WebP Image encoder wrapper

libwebp is Google's official encoder for WebP images. It can encode in either lossy or lossless mode. Lossy images are essentially a wrapper around a VP8 frame. Lossless images are a separate codec developed by Google.

Pixel Format

Currently, libwebp only supports YUV420 for lossy and RGB for lossless due to limitations of the format and libwebp. Alpha is supported for either mode. Because of API limitations, if RGB is passed in when encoding lossy or YUV is passed in for encoding lossless, the pixel format will automatically be converted using functions from libwebp. This is not ideal and is done only for convenience.

Options

-lossless boolean
    Enables/Disables use of lossless mode. Default is 0.

-compression_level integer
    For lossy, this is a quality/speed tradeoff. Higher values give better quality for a given size at the cost of increased encoding time. For lossless, this is a size/speed tradeoff. Higher values give smaller size at the cost of increased encoding time. More specifically, it controls the number of extra algorithms and compression tools used, and varies the combination of these tools. This maps to the method option in libwebp. The valid range is 0 to 6. Default is 4.

-qscale float
    For lossy encoding, this controls image quality, 0 to 100. For lossless encoding, this controls the effort and time spent at compressing more. The default value is 75. Note that for usage via libavcodec, this option is called global_quality and must be multiplied by FF_QP2LAMBDA.

-preset type
    Configuration preset. This does some automatic settings based on the general type of the image.

    none
        Do not use a preset.

    default
        Use the encoder default.

    picture
        Digital picture, like portrait, inner shot

    photo
        Outdoor photograph, with natural lighting

    drawing
        Hand or line drawing, with high-contrast details

    icon
        Small-sized colorful images

    text
        Text-like

  libx264, libx264rgb
x264 H.264/MPEG-4 AVC encoder wrapper.

This encoder requires the presence of the libx264 headers and library during configuration. You need to explicitly configure the build with "--enable-libx264".

libx264 supports an impressive number of features, including 8x8 and 4x4 adaptive spatial transform, adaptive B-frame placement, CAVLC/CABAC entropy coding, interlacing (MBAFF), lossless mode, psy optimizations for detail retention (adaptive quantization, psy-RD, psy-trellis).

Many libx264 encoder options are mapped to FFmpeg global codec options, while unique encoder options are provided through private options. Additionally the x264opts and x264-params private options allows one to pass a list of key=value tuples as accepted by the libx264 "x264_param_parse" function.

The x264 project website is at <http://www.videolan.org/developers/x264.html>.

The libx264rgb encoder is the same as libx264, except it accepts packed RGB pixel formats as input instead of YUV.

Supported Pixel Formats

x264 supports 8- to 10-bit color spaces. The exact bit depth is controlled at x264's configure time.

Options

The following options are supported by the libx264 wrapper. The x264-equivalent options or values are listed in parentheses for easy migration.

To reduce the duplication of documentation, only the private options and some others requiring special attention are documented here. For the documentation of the undocumented generic options, see the Codec Options chapter.

To get a more accurate and extensive documentation of the libx264 options, invoke the command x264 --fullhelp or consult the libx264 documentation.

b (bitrate)
    Set bitrate in bits/s. Note that FFmpeg's b option is expressed in bits/s, while x264's bitrate is in kilobits/s.

bf (bframes)
g (keyint)
qmin (qpmin)
    Minimum quantizer scale.

qmax (qpmax)
    Maximum quantizer scale.

qdiff (qpstep)
    Maximum difference between quantizer scales.

qblur (qblur)
    Quantizer curve blur

qcomp (qcomp)
    Quantizer curve compression factor

refs (ref)
    Number of reference frames each P-frame can use. The range is from 0-16.

sc_threshold (scenecut)
    Sets the threshold for the scene change detection.

trellis (trellis)
    Performs Trellis quantization to increase efficiency. Enabled by default.

nr  (nr)
me_range (merange)
    Maximum range of the motion search in pixels.

me_method (me)
    Set motion estimation method. Possible values in the decreasing order of speed:

    dia (dia)
    epzs (dia)
        Diamond search with radius 1 (fastest). epzs is an alias for dia.

    hex (hex)
        Hexagonal search with radius 2.

    umh (umh)
        Uneven multi-hexagon search.

    esa (esa)
        Exhaustive search.

    tesa (tesa)
        Hadamard exhaustive search (slowest).

forced-idr
    Normally, when forcing a I-frame type, the encoder can select any type of I-frame. This option forces it to choose an IDR-frame.

subq (subme)
    Sub-pixel motion estimation method.

b_strategy (b-adapt)
    Adaptive B-frame placement decision algorithm. Use only on first-pass.

keyint_min (min-keyint)
    Minimum GOP size.

coder
    Set entropy encoder. Possible values:

    ac  Enable CABAC.

    vlc Enable CAVLC and disable CABAC. It generates the same effect as x264's --no-cabac option.

cmp Set full pixel motion estimation comparison algorithm. Possible values:

    chroma
        Enable chroma in motion estimation.

    sad Ignore chroma in motion estimation. It generates the same effect as x264's --no-chroma-me option.

threads (threads)
    Number of encoding threads.

thread_type
    Set multithreading technique. Possible values:

    slice
        Slice-based multithreading. It generates the same effect as x264's --sliced-threads option.

    frame
        Frame-based multithreading.

flags
    Set encoding flags. It can be used to disable closed GOP and enable open GOP by setting it to "-cgop". The result is similar to the behavior of x264's --open-gop option.

rc_init_occupancy (vbv-init)
preset (preset)
    Set the encoding preset.

tune (tune)
    Set tuning of the encoding params.

profile (profile)
    Set profile restrictions.

fastfirstpass
    Enable fast settings when encoding first pass, when set to 1. When set to 0, it has the same effect of x264's --slow-firstpass option.

crf (crf)
    Set the quality for constant quality mode.

crf_max (crf-max)
    In CRF mode, prevents VBV from lowering quality beyond this point.

qp (qp)
    Set constant quantization rate control method parameter.

aq-mode (aq-mode)
    Set AQ method. Possible values:

    none (0)
        Disabled.

    variance (1)
        Variance AQ (complexity mask).

    autovariance (2)
        Auto-variance AQ (experimental).

aq-strength (aq-strength)
    Set AQ strength, reduce blocking and blurring in flat and textured areas.

psy Use psychovisual optimizations when set to 1. When set to 0, it has the same effect as x264's --no-psy option.

psy-rd  (psy-rd)
    Set strength of psychovisual optimization, in psy-rd:psy-trellis format.

rc-lookahead (rc-lookahead)
    Set number of frames to look ahead for frametype and ratecontrol.

weightb
    Enable weighted prediction for B-frames when set to 1. When set to 0, it has the same effect as x264's --no-weightb option.

weightp (weightp)
    Set weighted prediction method for P-frames. Possible values:

    none (0)
        Disabled

    simple (1)
        Enable only weighted refs

    smart (2)
        Enable both weighted refs and duplicates

ssim (ssim)
    Enable calculation and printing SSIM stats after the encoding.

intra-refresh (intra-refresh)
    Enable the use of Periodic Intra Refresh instead of IDR frames when set to 1.

avcintra-class (class)
    Configure the encoder to generate AVC-Intra. Valid values are 50,100 and 200

bluray-compat (bluray-compat)
    Configure the encoder to be compatible with the bluray standard. It is a shorthand for setting "bluray-compat=1 force-cfr=1".

b-bias (b-bias)
    Set the influence on how often B-frames are used.

b-pyramid (b-pyramid)
    Set method for keeping of some B-frames as references. Possible values:

    none (none)
        Disabled.

    strict (strict)
        Strictly hierarchical pyramid.

    normal (normal)
        Non-strict (not Blu-ray compatible).

mixed-refs
    Enable the use of one reference per partition, as opposed to one reference per macroblock when set to 1. When set to 0, it has the same effect as x264's --no-mixed-refs option.

8x8dct
    Enable adaptive spatial transform (high profile 8x8 transform) when set to 1. When set to 0, it has the same effect as x264's --no-8x8dct option.

fast-pskip
    Enable early SKIP detection on P-frames when set to 1. When set to 0, it has the same effect as x264's --no-fast-pskip option.

aud (aud)
    Enable use of access unit delimiters when set to 1.

mbtree
    Enable use macroblock tree ratecontrol when set to 1. When set to 0, it has the same effect as x264's --no-mbtree option.

deblock (deblock)
    Set loop filter parameters, in alpha:beta form.

cplxblur (cplxblur)
    Set fluctuations reduction in QP (before curve compression).

partitions (partitions)
    Set partitions to consider as a comma-separated list of. Possible values in the list:

    p8x8
        8x8 P-frame partition.

    p4x4
        4x4 P-frame partition.

    b8x8
        4x4 B-frame partition.

    i8x8
        8x8 I-frame partition.

    i4x4
        4x4 I-frame partition. (Enabling p4x4 requires p8x8 to be enabled. Enabling i8x8 requires adaptive spatial transform (8x8dct option) to be enabled.)

    none (none)
        Do not consider any partitions.

    all (all)
        Consider every partition.

direct-pred (direct)
    Set direct MV prediction mode. Possible values:

    none (none)
        Disable MV prediction.

    spatial (spatial)
        Enable spatial predicting.

    temporal (temporal)
        Enable temporal predicting.

    auto (auto)
        Automatically decided.

slice-max-size (slice-max-size)
    Set the limit of the size of each slice in bytes. If not specified but RTP payload size (ps) is specified, that is used.

stats (stats)
    Set the file name for multi-pass stats.

nal-hrd (nal-hrd)
    Set signal HRD information (requires vbv-bufsize to be set). Possible values:

    none (none)
        Disable HRD information signaling.

    vbr (vbr)
        Variable bit rate.

    cbr (cbr)
        Constant bit rate (not allowed in MP4 container).

x264opts (N.A.)
    Set any x264 option, see x264 --fullhelp for a list.

    Argument is a list of key=value couples separated by ":". In filter and psy-rd options that use ":" as a separator themselves, use "," instead. They accept it as well since long ago but this is kept undocumented for some reason.

    For example to specify libx264 encoding options with ffmpeg:

            ffmpeg -i foo.mpg -c:v libx264 -x264opts keyint=123:min-keyint=20 -an out.mkv

a53cc boolean
    Import closed captions (which must be ATSC compatible format) into output. Only the mpeg2 and h264 decoders provide these. Default is 1 (on).

x264-params (N.A.)
    Override the x264 configuration using a :-separated list of key=value parameters.

    This option is functionally the same as the x264opts, but is duplicated for compatibility with the Libav fork.

    For example to specify libx264 encoding options with ffmpeg:

            ffmpeg -i INPUT -c:v libx264 -x264-params level=30:bframes=0:weightp=0:\
            cabac=0:ref=1:vbv-maxrate=768:vbv-bufsize=2000:analyse=all:me=umh:\
            no-fast-pskip=1:subq=6:8x8dct=0:trellis=0 OUTPUT

Encoding ffpresets for common usages are provided so they can be used with the general presets system (e.g. passing the pre option).

  libx265
x265 H.265/HEVC encoder wrapper.

This encoder requires the presence of the libx265 headers and library during configuration. You need to explicitly configure the build with --enable-libx265.

Options

b   Sets target video bitrate.

bf
g   Set the GOP size.

keyint_min
    Minimum GOP size.

refs
    Number of reference frames each P-frame can use. The range is from 1-16.

preset
    Set the x265 preset.

tune
    Set the x265 tune parameter.

profile
    Set profile restrictions.

crf Set the quality for constant quality mode.

qp  Set constant quantization rate control method parameter.

qmin
    Minimum quantizer scale.

qmax
    Maximum quantizer scale.

qdiff
    Maximum difference between quantizer scales.

qblur
    Quantizer curve blur

qcomp
    Quantizer curve compression factor

i_qfactor
b_qfactor
forced-idr
    Normally, when forcing a I-frame type, the encoder can select any type of I-frame. This option forces it to choose an IDR-frame.

x265-params
    Set x265 options using a list of key=value couples separated by ":". See x265 --help for a list of options.

    For example to specify libx265 encoding options with -x265-params:

            ffmpeg -i input -c:v libx265 -x265-params crf=26:psy-rd=1 output.mp4

  libxavs2
xavs2 AVS2-P2/IEEE1857.4 encoder wrapper.

This encoder requires the presence of the libxavs2 headers and library during configuration. You need to explicitly configure the build with --enable-libxavs2.

The following standard libavcodec options are used:

•   b / bit_rate

•   g / gop_size

•   bf / max_b_frames

The encoder also has its own specific options:

Options

lcu_row_threads
    Set the number of parallel threads for rows from 1 to 8 (default 5).

initial_qp
    Set the xavs2 quantization parameter from 1 to 63 (default 34). This is used to set the initial qp for the first frame.

qp  Set the xavs2 quantization parameter from 1 to 63 (default 34). This is used to set the qp value under constant-QP mode.

max_qp
    Set the max qp for rate control from 1 to 63 (default 55).

min_qp
    Set the min qp for rate control from 1 to 63 (default 20).

speed_level
    Set the Speed level from 0 to 9 (default 0). Higher is better but slower.

log_level
    Set the log level from -1 to 3 (default 0). -1: none, 0: error, 1: warning, 2: info, 3: debug.

xavs2-params
    Set xavs2 options using a list of key=value couples separated by ":".

    For example to specify libxavs2 encoding options with -xavs2-params:

            ffmpeg -i input -c:v libxavs2 -xavs2-params RdoqLevel=0 output.avs2

  libxvid
Xvid MPEG-4 Part 2 encoder wrapper.

This encoder requires the presence of the libxvidcore headers and library during configuration. You need to explicitly configure the build with "--enable-libxvid --enable-gpl".

The native "mpeg4" encoder supports the MPEG-4 Part 2 format, so users can encode to this format without this library.

Options

The following options are supported by the libxvid wrapper. Some of the following options are listed but are not documented, and correspond to shared codec options. See the Codec Options chapter for their documentation. The other shared options which are not listed have no effect for the libxvid encoder.

b
g
qmin
qmax
mpeg_quant
threads
bf
b_qfactor
b_qoffset
flags
    Set specific encoding flags. Possible values:

    mv4 Use four motion vector by macroblock.

    aic Enable high quality AC prediction.

    gray
        Only encode grayscale.

    gmc Enable the use of global motion compensation (GMC).

    qpel
        Enable quarter-pixel motion compensation.

    cgop
        Enable closed GOP.

    global_header
        Place global headers in extradata instead of every keyframe.

trellis
me_method
    Set motion estimation method. Possible values in decreasing order of speed and increasing order of quality:

    zero
        Use no motion estimation (default).

    phods
    x1
    log Enable advanced diamond zonal search for 16x16 blocks and half-pixel refinement for 16x16 blocks. x1 and log are aliases for phods.

    epzs
        Enable all of the things described above, plus advanced diamond zonal search for 8x8 blocks, half-pixel refinement for 8x8 blocks, and motion estimation on chroma planes.

    full
        Enable all of the things described above, plus extended 16x16 and 8x8 blocks search.

mbd Set macroblock decision algorithm. Possible values in the increasing order of quality:

    simple
        Use macroblock comparing function algorithm (default).

    bits
        Enable rate distortion-based half pixel and quarter pixel refinement for 16x16 blocks.

    rd  Enable all of the things described above, plus rate distortion-based half pixel and quarter pixel refinement for 8x8 blocks, and rate distortion-based search using square pattern.

lumi_aq
    Enable lumi masking adaptive quantization when set to 1. Default is 0 (disabled).

variance_aq
    Enable variance adaptive quantization when set to 1. Default is 0 (disabled).

    When combined with lumi_aq, the resulting quality will not be better than any of the two specified individually. In other words, the resulting quality will be the worse one of the two effects.

ssim
    Set structural similarity (SSIM) displaying method. Possible values:

    off Disable displaying of SSIM information.

    avg Output average SSIM at the end of encoding to stdout. The format of showing the average SSIM is:

                Average SSIM: %f

        For users who are not familiar with C, %f means a float number, or a decimal (e.g. 0.939232).

    frame
        Output both per-frame SSIM data during encoding and average SSIM at the end of encoding to stdout. The format of per-frame information is:

                       SSIM: avg: %1.3f min: %1.3f max: %1.3f

        For users who are not familiar with C, %1.3f means a float number rounded to 3 digits after the dot (e.g. 0.932).

ssim_acc
    Set SSIM accuracy. Valid options are integers within the range of 0-4, while 0 gives the most accurate result and 4 computes the fastest.

  MediaFoundation
This provides wrappers to encoders (both audio and video) in the MediaFoundation framework. It can access both SW and HW encoders. Video encoders can take input in either of nv12 or yuv420p form (some encoders support both, some support only either - in practice, nv12 is the safer choice, especially among HW encoders).

  mpeg2
MPEG-2 video encoder.

Options

profile
    Select the mpeg2 profile to encode:

    422
    high
    ss  Spatially Scalable

    snr SNR Scalable

    main
    simple
level
    Select the mpeg2 level to encode:

    high
    high1440
    main
    low
seq_disp_ext integer
    Specifies if the encoder should write a sequence_display_extension to the output.

    -1
    auto
        Decide automatically to write it or not (this is the default) by checking if the data to be written is different from the default or unspecified values.

    0
    never
        Never write it.

    1
    always
        Always write it.

video_format integer
    Specifies the video_format written into the sequence display extension indicating the source of the video pictures. The default is unspecified, can be component, pal, ntsc, secam or mac. For maximum compatibility, use component.

a53cc boolean
    Import closed captions (which must be ATSC compatible format) into output. Default is 1 (on).

  png
PNG image encoder.

Private options

dpi integer
    Set physical density of pixels, in dots per inch, unset by default

dpm integer
    Set physical density of pixels, in dots per meter, unset by default

  ProRes
Apple ProRes encoder.

FFmpeg contains 2 ProRes encoders, the prores-aw and prores-ks encoder. The used encoder can be chosen with the "-vcodec" option.

Private Options for prores-ks

profile integer
    Select the ProRes profile to encode

    proxy
    lt
    standard
    hq
    4444
    4444xq
quant_mat integer
    Select quantization matrix.

    auto
    default
    proxy
    lt
    standard
    hq

    If set to auto, the matrix matching the profile will be picked. If not set, the matrix providing the highest quality, default, will be picked.

bits_per_mb integer
    How many bits to allot for coding one macroblock. Different profiles use between 200 and 2400 bits per macroblock, the maximum is 8000.

mbs_per_slice integer
    Number of macroblocks in each slice (1-8); the default value (8) should be good in almost all situations.

vendor string
    Override the 4-byte vendor ID. A custom vendor ID like apl0 would claim the stream was produced by the Apple encoder.

alpha_bits integer
    Specify number of bits for alpha component. Possible values are 0, 8 and 16. Use 0 to disable alpha plane coding.

Speed considerations

In the default mode of operation the encoder has to honor frame constraints (i.e. not produce frames with size bigger than requested) while still making output picture as good as possible. A frame containing a lot of small details is harder to compress and the encoder would spend more time searching for appropriate quantizers for each slice.

Setting a higher bits_per_mb limit will improve the speed.

For the fastest encoding speed set the qscale parameter (4 is the recommended value) and do not set a size constraint.

  QSV encoders
The family of Intel QuickSync Video encoders (MPEG-2, H.264, HEVC, JPEG/MJPEG and VP9)

The ratecontrol method is selected as follows:

•   When global_quality is specified, a quality-based mode is used. Specifically this means either

    -   CQP - constant quantizer scale, when the qscale codec flag is also set (the -qscale ffmpeg option).

    -   LA_ICQ - intelligent constant quality with lookahead, when the look_ahead option is also set.

    -   ICQ -- intelligent constant quality otherwise.

•   Otherwise, a bitrate-based mode is used. For all of those, you should specify at least the desired average bitrate with the b option.

    -   LA - VBR with lookahead, when the look_ahead option is specified.

    -   VCM - video conferencing mode, when the vcm option is set.

    -   CBR - constant bitrate, when maxrate is specified and equal to the average bitrate.

    -   VBR - variable bitrate, when maxrate is specified, but is higher than the average bitrate.

    -   AVBR - average VBR mode, when maxrate is not specified. This mode is further configured by the avbr_accuracy and avbr_convergence options.

Note that depending on your system, a different mode than the one you specified may be selected by the encoder. Set the verbosity level to verbose or higher to see the actual settings used by the QSV runtime.

Additional libavcodec global options are mapped to MSDK options as follows:

•   g/gop_size -> GopPicSize

•   bf/max_b_frames+1 -> GopRefDist

•   rc_init_occupancy/rc_initial_buffer_occupancy -> InitialDelayInKB

•   slices -> NumSlice

•   refs -> NumRefFrame

•   b_strategy/b_frame_strategy -> BRefType

•   cgop/CLOSED_GOP codec flag -> GopOptFlag

•   For the CQP mode, the i_qfactor/i_qoffset and b_qfactor/b_qoffset set the difference between QPP and QPI, and QPP and QPB respectively.

•   Setting the coder option to the value vlc will make the H.264 encoder use CAVLC instead of CABAC.

  snow
Options

iterative_dia_size
    dia size for the iterative motion estimation

  VAAPI encoders
Wrappers for hardware encoders accessible via VAAPI.

These encoders only accept input in VAAPI hardware surfaces. If you have input in software frames, use the hwupload filter to upload them to the GPU.

The following standard libavcodec options are used:

•   g / gop_size

•   bf / max_b_frames

•   profile

    If not set, this will be determined automatically from the format of the input frames and the profiles supported by the driver.

•   level

•   b / bit_rate

•   maxrate / rc_max_rate

•   bufsize / rc_buffer_size

•   rc_init_occupancy / rc_initial_buffer_occupancy

•   compression_level

    Speed / quality tradeoff: higher values are faster / worse quality.

•   q / global_quality

    Size / quality tradeoff: higher values are smaller / worse quality.

•   qmin

•   qmax

•   i_qfactor / i_quant_factor

•   i_qoffset / i_quant_offset

•   b_qfactor / b_quant_factor

•   b_qoffset / b_quant_offset

•   slices

All encoders support the following options:

low_power
    Some drivers/platforms offer a second encoder for some codecs intended to use less power than the default encoder; setting this option will attempt to use that encoder. Note that it may support a reduced feature set, so some other options may not be available in this mode.

idr_interval
    Set the number of normal intra frames between full-refresh (IDR) frames in open-GOP mode. The intra frames are still IRAPs, but will not include global headers and may have non-decodable leading pictures.

b_depth
    Set the B-frame reference depth. When set to one (the default), all B-frames will refer only to P- or I-frames. When set to greater values multiple layers of B-frames will be present, frames in each layer only referring to frames in higher layers.

rc_mode
    Set the rate control mode to use. A given driver may only support a subset of modes.

    Possible modes:

    auto
        Choose the mode automatically based on driver support and the other options. This is the default.

    CQP Constant-quality.

    CBR Constant-bitrate.

    VBR Variable-bitrate.

    ICQ Intelligent constant-quality.

    QVBR
        Quality-defined variable-bitrate.

    AVBR
        Average variable bitrate.

Each encoder also has its own specific options:

h264_vaapi
    profile sets the value of profile_idc and the constraint_set*_flags. level sets the value of level_idc.

    coder
        Set entropy encoder (default is cabac). Possible values:

        ac
        cabac
            Use CABAC.

        vlc
        cavlc
            Use CAVLC.

    aud Include access unit delimiters in the stream (not included by default).

    sei Set SEI message types to include. Some combination of the following values:

        identifier
            Include a user_data_unregistered message containing information about the encoder.

        timing
            Include picture timing parameters (buffering_period and pic_timing messages).

        recovery_point
            Include recovery points where appropriate (recovery_point messages).

hevc_vaapi
    profile and level set the values of general_profile_idc and general_level_idc respectively.

    aud Include access unit delimiters in the stream (not included by default).

    tier
        Set general_tier_flag. This may affect the level chosen for the stream if it is not explicitly specified.

    sei Set SEI message types to include. Some combination of the following values:

        hdr Include HDR metadata if the input frames have it (mastering_display_colour_volume and content_light_level messages).

    tiles
        Set the number of tiles to encode the input video with, as columns x rows. Larger numbers allow greater parallelism in both encoding and decoding, but may decrease coding efficiency.

mjpeg_vaapi
    Only baseline DCT encoding is supported. The encoder always uses the standard quantisation and huffman tables - global_quality scales the standard quantisation table (range 1-100).

    For YUV, 4:2:0, 4:2:2 and 4:4:4 subsampling modes are supported. RGB is also supported, and will create an RGB JPEG.

    jfif
        Include JFIF header in each frame (not included by default).

    huffman
        Include standard huffman tables (on by default). Turning this off will save a few hundred bytes in each output frame, but may lose compatibility with some JPEG decoders which don't fully handle MJPEG.

mpeg2_vaapi
    profile and level set the value of profile_and_level_indication.

vp8_vaapi
    B-frames are not supported.

    global_quality sets the q_idx used for non-key frames (range 0-127).

    loop_filter_level
    loop_filter_sharpness
        Manually set the loop filter parameters.

vp9_vaapi
    global_quality sets the q_idx used for P-frames (range 0-255).

    loop_filter_level
    loop_filter_sharpness
        Manually set the loop filter parameters.

    B-frames are supported, but the output stream is always in encode order rather than display order. If B-frames are enabled, it may be necessary to use the vp9_raw_reorder bitstream filter to modify the output stream to display frames in the correct order.

    Only normal frames are produced - the vp9_superframe bitstream filter may be required to produce a stream usable with all decoders.

  vc2
SMPTE VC-2 (previously BBC Dirac Pro). This codec was primarily aimed at professional broadcasting but since it supports yuv420, yuv422 and yuv444 at 8 (limited range or full range), 10 or 12 bits, this makes it suitable for other tasks which require low overhead and low compression (like screen recording).

Options

b   Sets target video bitrate. Usually that's around 1:6 of the uncompressed video bitrate (e.g. for 1920x1080 50fps yuv422p10 that's around 400Mbps). Higher values (close to the uncompressed bitrate) turn on lossless compression mode.

field_order
    Enables field coding when set (e.g. to tt - top field first) for interlaced inputs. Should increase compression with interlaced content as it splits the fields and encodes each separately.

wavelet_depth
    Sets the total amount of wavelet transforms to apply, between 1 and 5 (default). Lower values reduce compression and quality. Less capable decoders may not be able to handle values of wavelet_depth over 3.

wavelet_type
    Sets the transform type. Currently only 5_3 (LeGall) and 9_7 (Deslauriers-Dubuc) are implemented, with 9_7 being the one with better compression and thus is the default.

slice_width
slice_height
    Sets the slice size for each slice. Larger values result in better compression. For compatibility with other more limited decoders use slice_width of 32 and slice_height of 8.

tolerance
    Sets the undershoot tolerance of the rate control system in percent. This is to prevent an expensive search from being run.

qm  Sets the quantization matrix preset to use by default or when wavelet_depth is set to 5

    -   default Uses the default quantization matrix from the specifications, extended with values for the fifth level. This provides a good balance between keeping detail and omitting artifacts.

    -   flat Use a completely zeroed out quantization matrix. This increases PSNR but might reduce perception. Use in bogus benchmarks.

    -   color Reduces detail but attempts to preserve color at extremely low bitrates.

SUBTITLES ENCODERS

  dvdsub
This codec encodes the bitmap subtitle format that is used in DVDs. Typically they are stored in VOBSUB file pairs (*.idx + *.sub), and they can also be used in Matroska files.

Options

palette
    Specify the global palette used by the bitmaps.

    The format for this option is a string containing 16 24-bits hexadecimal numbers (without 0x prefix) separated by commas, for example "0d00ee, ee450d, 101010, eaeaea, 0ce60b, ec14ed, ebff0b, 0d617a, 7b7b7b, d1d1d1, 7b2a0e, 0d950c, 0f007b, cf0dec, cfa80c, 7c127b".

even_rows_fix
    When set to 1, enable a work-around that makes the number of pixel rows even in all subtitles. This fixes a problem with some players that cut off the bottom row if the number is odd. The work-around just adds a fully transparent row if needed. The overhead is low, typically one byte per subtitle on average.

    By default, this work-around is disabled.

SEE ALSO
ffmpeg(1), ffplay(1), ffprobe(1), libavcodec(3)

AUTHORS
The FFmpeg developers.

For details about the authorship, see the Git history of the project (https://git.ffmpeg.org/ffmpeg), e.g. by typing the command git log in the FFmpeg source directory, or browsing the online repository at <https://git.ffmpeg.org/ffmpeg>.

Maintainers for the specific components are listed in the file MAINTAINERS in the source code tree.