Note:  This readme file is for floppy diskette installation.  
For CD-ROM installation, please use README.WRI in the root directory 
of this CD-ROM disk for correct instructions.

***********************************************************************

                WINDOWS NT DRIVER SETUP INFORMATION
                               for
                          Trident Users


***********************************************************************
Windows NT Device Drivers Version 4.00                   Sept 27, 1996
***********************************************************************

Contents

1.0     Introduction
2.0     Supported Resolutions
3.0     Installation Notes for Windows NT Version 3.5x

*****************************

1.0     Introduction

This Accelerate Driver runs on the following products:

     Trident 93XX/9440/9470/96XX, VESA or PCI local bus adapter

The Graphics Device Drivers supplied here are for the Microsoft
Windows NT 3.5x operating system English version.

*****************************

2.0     Supported Resolutions.

     This driver support resolution up to 1600x1200 and color depth
     up to TrueColor.

****************************

3.0     Installation Notes for Windows NT

This driver package containing:

  - TGIULNT.SYS         (Trident general linear addressing graphics miniport driver)
  - TGIUL35.DLL         (Trident general linear addressing accelerated graphics display  driver)
  - VGA.DLL             (Microsoft standard VGA display driver)
  - OEMSETUP.INF        (setup files used by Windows NT Setup program)
  - README              This README file for Windows NT Version 3.5

Windows NT drivers are included on Disk #2 of this package.  They are
located in the \NT35 sub-directory.

Procedure:

1. Run the Windows NT display Setup program located in the Control Panel, Main
   group.

2. Select "Change Display Type..." button from the Display Settings options.

3. Select "Change..." button from the Display Type options.

4. Select "Other..." button from the Select Device options.

5. Windows NT will prompt you for the correct path. Enter A:\NT35 if disk 2
   is loaded in drive A:.

6. Select "TGIULNT Compatible"

7. Restart Windows NT.  

8. Windows NT will start up with default 640x480x256 mode. Select your disired 
   display setting from the Display Setting.        

Note: After changing to Trident driver, the Display setting only allows selecting
      valid settings depends on your card.
        
