
[MAIN]
TXT1=Activates the TRS and XLR inputs. Switch between Mic/Line and HiZ/Line on the hardware unit. 
TXT2=Activates the Aux input for channels 1/2. Switch to Aux on the hardware unit.
TXT3=Activates the Phono input for channels 1/2. Switch to Phono on the hardware unit.
TXT4=Output channels 3/4 will be routed to input channels 1/2.
TXT5=An optional integrated sound module will be routed to input channels 1/2.
TXT6=All activated inputs for the channels 1/2 will be routed directly to outputs 1/2.
TXT7=Set the Direct signal to mono (only for Mic-HiZ-Line inputs).
TXT8=Activates the Aux input for channels 3/4. Switch to Aux on the hardware unit.
TXT9=Activates the Phono input for channels 3/4. Switch to Phono on the hardware unit.
TXT10=Output channels 1/2 will be routed to input channels 3/4.
TXT11=An optional integrated sound module will be routed to input channels 3/4.
TXT12=All activated Inputs for channels 3/4 will be routed directly to outputs 3/4.
TXT13=An optional integrated sound module will be routed to output channels 3/4.
TXT14=[IN/OUT] 24ms/46ms @44.1kHz - 22ms/47ms @48kHz - 12ms/57ms @88.2kHz - 96kHz: 11ms/58ms
TXT15=[IN/OUT] 13ms/36ms @44.1kHz - 12ms/37ms @48kHz - 6ms/43ms @88.2kHz- 96kHz: 6ms/43ms
TXT16=[IN/OUT] 7ms/22ms @44.1kHz - 6ms/23ms @48kHz - 3ms/26ms @88.2kHz- 3ms/26ms @96kHz
TXT17=[IN/OUT] 5ms/18ms @44.1kHz - 5ms/18ms @48kHz - 2ms/21ms @88.2kHz- 2ms/21ms @96kHz
TXT18=[IN/OUT] 4ms/11ms @44.1kHz - 4ms/11ms @48kHz- 2ms/13ms @88.2kHz- 2ms/13ms @96kHz
TXT19=[IN/OUT] 2ms/7ms @44.1kHz - 2ms/7ms @48kHz - 1ms/8ms @88.2kHz- 1ms/8ms @96kHz
TXT21=Samplerate indicator. Set by audiosoftware or digital input sources.
TXT22=Samplerate indicator. Set by audiosoftware or digital input sources.
TXT23=Samplerate indicator. Set by audiosoftware or digital input sources.	
TXT24=Samplerate indicator. Set by audiosoftware or digital input sources.
TXT26=Opens the Info window including additional settings.
TXT27=Set the Playback channels 1/2 to mono.
TXT28=Set the Playback channels 3/4 to mono.
TXT29=Close the PHASE X64 USB control panel.
TXT30=Playback channels 1/2 thru output channels 1/2.
TXT31=Playback channels 3/4 thru output channels 3/4.



   
