{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["일위대가","일위대가상세"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"일위대가","index":0,"n_rows":2438,"n_cols":11,"rows_kept":2438,"cut":false,"hidden":false,"merged":[[1,0,1,10],[0,0,0,10]]}
["일 위 대 가"]
["20240200009_2024년 표준일위대가(토목)_1800507771"]
["일위대가코드","번호","품명","규격","단위","재료비","노무비","경비","합계","비목구분","비고"]
["CAA15103000S",null,"작업대차 조립","방수 작업용 대차(L=10M)","회",125432,6271620,0,6397052,"합계"]
["CAA15203000S",null,"작업대차 해체","방수 작업용 대차(L=10M)","회",62716,3135810,0,3198526,"합계"]
["CAA16111000S",null,"강관 지주 설치","지주높이 3.5m 이하","M",576,12184,456,13216,"합계"]
["CAA16113000S",null,"강관 지주 설치","지주높이 6m 이하","M",735,17499,456,18690,"합계"]
["CAA16121000S",null,"강관 지주 해체","지주높이 3.5m 이하","M",228,4807,182,5217,"합계"]
["CAA16123000S",null,"강관 지주 해체","지주높이 6m 이하","M",288,6821,182,7291,"합계"]
["CAA16212000S",null,"H형강 지주 설치","지주높이 4m 이하","M",1387,23679,1551,26617,"합계"]
["CAA16214000S",null,"H형강 지주 설치","지주높이 7m 이하","M",2004,42217,1910,46131,"합계"]
["CAA16222000S",null,"H형강 지주 해체","지주높이 4m 이하","M",553,9530,615,10698,"합계"]
["CAA16224000S",null,"H형강 지주 해체","지주높이 7m 이하","M",805,17007,765,18577,"합계"]
["CAA16311000S",null,"가설울타리판 설치","설치높이 3m 이하","M",263,8782,0,9045,"합계"]
["CAA16313000S",null,"가설울타리판 설치","설치높이 6m 이하","M",307,10235,0,10542,"합계"]
["CAA16321000S",null,"가설울타리판 해체","설치높이 3m 이하","M",104,3466,0,3570,"합계"]
["CAA16323000S",null,"가설울타리판 해체","설치높이 6m 이하","M",125,4193,0,4318,"합계"]
["CAA16411000S",null,"세로형 가설방음판 설치","설치높이 3m 이하","M",246,8221,0,8467,"합계"]
["CAA16412000S",null,"세로형 가설방음판 설치","설치높이 6m 이하","M",285,9508,0,9793,"합계"]
["CAA16421000S",null,"세로형 가설방음판 해체","설치높이 3m 이하","M",99,3301,0,3400,"합계"]
["CAA16422000S",null,"세로형 가설방음판 해체","설치높이 6m 이하","M",112,3747,0,3859,"합계"]
["CAA16511000S",null,"가로형 가설방음판 설치","설치높이 3m 이하","M",1229,28984,949,31162,"합계"]
["CAA16512000S",null,"가로형 가설방음판 설치","설치높이 6m 이하","M",1434,33768,1109,36311,"합계"]
["CAA16521000S",null,"가로형 가설방음판 해체","설치높이 3m 이하","M",491,11583,379,12453,"합계"]
["CAA16522000S",null,"가로형 가설방음판 해체","설치높이 6m 이하","M",572,13600,439,14611,"합계"]
["CAA18110000S",null,"비탈면 보양",null,"M2",0,5939,0,5939,"합계"]
["CAA23110000S",null,"P.P. 마대 만들기","0.024m3/개","개",0,2483,0,2483,"합계"]
["CAA23120000S",null,"P.P. 마대 쌓기","0.024m3/개","개",0,993,0,993,"합계"]
["CAA23130000S",null,"P.P. 마대 헐기","0.024m3/개","개",0,993,0,993,"합계"]
["CAA23210000S",null,"톤 마대 만들기","0.7m3/개","개",1031,13754,1747,16532,"합계"]
["CAA23220000S",null,"톤 마대 쌓기","0.7m3/개","개",2118,8806,1953,12877,"합계"]
["CAA23230000S",null,"톤 마대 헐기","0.7m3/개","개",2118,8806,1953,12877,"합계"]
["CAA26110000S",null,"타워크레인 방호울타리 설치 및 해체","높이 2.0m 기준","M",673,33656,0,34329,"합계"]
["CAA26120000S",null,"건설용리프트 방호선반 설치 및 해체","싱글 1.2ton","개소",6189,309490,0,315679,"합계"]
["CAA26130000S",null,"보행자 안전통로 설치 및 해체","높이 3.0m이하, 폭 2.0m 기준","M",1121,56094,0,57215,"합계"]
["CAA26140000S",null,"PE드럼 설치 및 해체",null,"개",0,12853,0,12853,"합계"]
["CAA26150000S",null,"PE가설방호벽 설치 및 해체",null,"개",406,20696,211,21313,"합계"]
["CAA26160000S",null,"PC가설방호벽 설치 및 해체",null,"개",1634,35625,2098,39357,"합계"]
["CAA26170000S",null,"가설휀스(H-Beam기초) 설치 및 해체",null,"M",155,3086,199,3440,"합계"]
["CAA26180000S",null,"PE가설휀스 설치 및 해체",null,"개",0,4284,0,4284,"합계"]
["CAA26190000S",null,"가림막 가설휀스 설치 및 해체",null,"개",0,8568,0,8568,"합계"]
["CAA26210000S",null,"점멸등 설치 및 해체",null,"개",0,2142,0,2142,"합계"]
["CAA26220000S",null,"유도등 설치 및 해체",null,"M",0,2142,0,2142,"합계"]
["CAA27100000S",null,"낙하물 방지망(비계) 설치 및 해체","수평방향 3m 이하","M2",302,10069,0,10371,"합계"]
["CAA27200000S",null,"낙하물 방지망(플라잉넷) 설치 및 해체","수평방향 3m 이하","M2",217,7264,0,7481,"합계"]
["CAA27300000S",null,"낙하물 방지망(시스템방호) 설치 및 해체","수평방향 4m 이하","M2",173,8667,0,8840,"합계"]
["CAA27400000S",null,"교량 방호선반 설치 및 해체",null,"M2",682,11501,1594,13777,"합계"]
["CAA27500000S",null,"교량 낙하물방지망 설치 및 해체",null,"M2",256,6644,1299,8199,"합계"]
["CAA27600000S",null,"철골 안전망 설치 및 해체",null,"M2",0,5595,0,5595,"합계"]
["CAA27700000S",null,"비계주위 보호망 설치 및 해체",null,"M2",0,2804,0,2804,"합계"]
["CAA27800000S",null,"갱폼주위 보호망 설치 및 해체",null,"M2",0,1121,0,1121,"합계"]
["CAA27910000S",null,"수직형 추락방망 설치 및 해체","개구부 면적 1.0m2 이하","개소",274,13743,0,14017,"합계"]
["CAA27920000S",null,"수직형 추락방망 설치 및 해체","개구부 면적 1.0~3.0m2 이하","개소",353,17669,0,18022,"합계"]
["CAA27930000S",null,"수직형 추락방망 설치 및 해체","개구부 면적 3.0~6.0m2 이하","개소",566,28327,0,28893,"합계"]
["CAA27940000S",null,"수직형 추락방망 설치 및 해체","개구부 면적 6.0~9.0m2 이하","개소",729,36461,0,37190,"합계"]
["CAA27950000S",null,"수직형 추락방망 설치 및 해체","개구부 면적 9.0~12.0m2 이하","개소",897,44875,0,45772,"합계"]
["CAA28011100S",null,"안전난간대 설치 및 해체","브라켓형 2단, 난간기둥 간격 1.0m이하","M",345,17277,0,17622,"합계"]
["CAA28011200S",null,"안전난간대 설치 및 해체","브라켓형 2단, 난간기둥 간격 1.5m이하","M",314,15706,0,16020,"합계"]
["CAA28011300S",null,"안전난간대 설치 및 해체","브라켓형 2단, 난간기둥 간격 1.5m초과","M",282,14135,0,14417,"합계"]
["CAA28012100S",null,"안전난간대 설치 및 해체","브라켓형 3단, 난간기둥 간격 1.0m이하","M",382,19128,0,19510,"합계"]
["CAA28012200S",null,"안전난간대 설치 및 해체","브라켓형 3단, 난간기둥 간격 1.5m이하","M",347,17389,0,17736,"합계"]
["CAA28012300S",null,"안전난간대 설치 및 해체","브라켓형 3단, 난간기둥 간격 1.5m초과","M",313,15650,0,15963,"합계"]
["CAA28021100S",null,"안전난간대 설치 및 해체","앵커형 2단, 난간기둥 간격 1.0m이하","M",394,19745,0,20139,"합계"]
["CAA28021200S",null,"안전난간대 설치 및 해체","앵커형 2단, 난간기둥 간격 1.5m이하","M",359,17950,0,18309,"합계"]
["CAA28021300S",null,"안전난간대 설치 및 해체","앵커형 2단, 난간기둥 간격 1.5m초과","M",323,16155,0,16478,"합계"]
["CAA28022100S",null,"안전난간대 설치 및 해체","앵커형 3단, 난간기둥 간격 1.0m이하","M",431,21596,0,22027,"합계"]
["CAA28022200S",null,"안전난간대 설치 및 해체","앵커형 3단, 난간기둥 간격 1.5m이하","M",392,19633,0,20025,"합계"]
["CAA28022300S",null,"안전난간대 설치 및 해체","앵커형 3단, 난간기둥 간격 1.5m초과","M",353,17669,0,18022,"합계"]
["CAA28110000S",null,"계단난간대 설치 및 해체","브라켓형, 난간대 길이 2.5m이하, 2단 기준","개소",785,39266,0,40051,"합계"]
["CAA28120000S",null,"계단난간대 설치 및 해체","앵커형, 난간대 길이 2.5m이하, 2단 기준","개소",813,40668,0,41481,"합계"]
["CAA28211000S",null,"안전난간대 설치 및 해체(토목)","2단, 지주 간격 1.0m이하","M",382,19128,0,19510,"합계"]
["CAA28212000S",null,"안전난간대 설치 및 해체(토목)","2단, 지주 간격 1.5m이하","M",347,17389,0,17736,"합계"]
["CAA28213000S",null,"안전난간대 설치 및 해체(토목)","2단, 지주 간격 1.5m초과","M",313,15650,0,15963,"합계"]
["CAA28221000S",null,"안전난간대 설치 및 해체(토목)","3단, 지주 간격 1.0m이하","M",413,20670,0,21083,"합계"]
["CAA28222000S",null,"안전난간대 설치 및 해체(토목)","3단, 지주 간격 1.5m이하","M",375,18791,0,19166,"합계"]
["CAA28223000S",null,"안전난간대 설치 및 해체(토목)","3단, 지주 간격 1.5m초과","M",338,16912,0,17250,"합계"]
["CAA28300000S",null,"엘리베이터 난간틀 설치 및 해체","난간틀 높이 1.4m이하, 길이 1.3m이하 기준","개소",0,22437,0,22437,"합계"]
["CAA28400000S",null,"엘리베이터 추락방호망 설치 및 해체","추락방호망 5~9m2이하 기준","개소",841,42070,0,42911,"합계"]
["CAA28510000S",null,"개구부 수평보호덮개 설치 및 해체","개당 1.0M2이하","개",0,14023,0,14023,"합계"]
["CAA28520000S",null,"개구부 수평보호덮개 설치 및 해체","개당 3.0M2이하","개",0,19633,0,19633,"합계"]
["CAA28600000S",null,"강재거푸집 작업용 난간 설치 및 해체",null,"M",689,22998,0,23687,"합계"]
["CAA28700000S",null,"수평지지로프 설치 및 해체",null,"M",0,5609,0,5609,"합계"]
["CAA29010000S",null,"비계주위 보호막 설치 및 해체",null,"M2",0,5609,0,5609,"합계"]
["CAA29020000S",null,"방진망 설치 및 해체",null,"M2",0,4487,0,4487,"합계"]
["CAA29031000S",null,"터널방음문 설치",null,"개소",236416,2036848,935832,3209096,"합계"]
["CAA29032000S",null,"터널방음문 해체",null,"개소",164657,1384093,655082,2203832,"합계"]
["CAA29041100S",null,"박스형 간이흙막이 설치 및 해체","설치깊이 3.0m 이하","개",1746,60832,7826,70404,"합계"]
["CAA29041200S",null,"박스형 간이흙막이 설치 및 해체","설치깊이 4.0m 이하","개",2955,90820,13245,107020,"합계"]
["CAA29042100S",null,"조립식 간이흙막이 설치 및 해체","설치깊이 H=3.0m 이하","M",3090,77912,13847,94849,"합계"]
["CAA29042200S",null,"조립식 간이흙막이 설치 및 해체","설치깊이 H=4.0m 이하","M",6046,126666,27092,159804,"합계"]
["CAA29042300S",null,"조립식 간이흙막이 설치 및 해체","설치깊이 H=5.0m 이하","M",9942,192956,44552,247450,"합계"]
["CAA29042400S",null,"조립식 간이흙막이 설치 및 해체","설치깊이 H=6.0m 이하","M",14779,281066,66226,362071,"합계"]
["CAA31110000S",null,"강관비계 설치 및 해체","H=10m 이하 ","M2",346,17334,0,17680,"합계"]
["CAA31120000S",null,"강관비계 설치 및 해체","H=10m 초과, 20m 이하 ","M2",402,20139,0,20541,"합계"]
["CAA31130000S",null,"강관비계 설치 및 해체","H=20m 초과, 30m 이하 ","M2",458,22943,0,23401,"합계"]
["CAA31210000S",null,"시스템 비계 설치 및 해체","H=10m 이하 ","M2",0,12874,0,12874,"합계"]
["CAA31220000S",null,"시스템 비계 설치 및 해체","H=10m 초과, 20m 이하 ","M2",0,15679,0,15679,"합계"]
["CAA31230000S",null,"시스템 비계 설치 및 해체","H=20m 초과, 30m 이하 ","M2",0,18483,0,18483,"합계"]
["CAA31310000S",null,"강관틀 비계 설치 및 해체","10m 이하","M2",0,7264,0,7264,"합계"]
["CAA31320000S",null,"강관틀 비계 설치 및 해체","10m 초과, 20m 이하","M2",0,10069,0,10069,"합계"]
["CAA31410000S",null,"강관 조립말비계(이동식) 설치 및 해체","높이 2.0m","대당",0,93294,0,93294,"합계"]
["CAA31420000S",null,"강관 조립말비계(이동식) 설치 및 해체","높이 4.0m","대당",0,154724,0,154724,"합계"]
["CAA31500000S",null,"경사형 가설 계단 설치 및 해체","높이 6m 이하, 계단폭 0.9m 이하","M2",1812,90626,0,92438,"합계"]
["CAA31600000S",null,"타워형 가설 계단 설치 및 해체","계단폭 0.9m 이하","M2",403,71024,1806,73233,"합계"]
["CAA31711000S",null,"비계용 브라켓 설치","벽체용","개소당",0,12621,0,12621,"합계"]
["CAA31712000S",null,"비계용 브라켓 설치","슬라브, 발코니난간용","개소당",0,9536,0,9536,"합계"]
["CAA31721000S",null,"비계용 브라켓 해체","벽체용","개소당",0,9536,0,9536,"합계"]
["CAA31722000S",null,"비계용 브라켓 해체","슬라브, 발코니난간용","개소당",0,7292,0,7292,"합계"]
["CAA32100000S",null,"강관동바리 수평연결재 설치, 해체","1단설치","M2",0,7154,0,7154,"합계"]
["CAA32111000S",null,"강관동바리 설치 및 해체(토목) (H=2.5m 이하) ","설치간격 0.6m 이하","공M3",0,21990,0,21990,"합계"]
["CAA32112000S",null,"강관동바리 설치 및 해체(토목) (H=2.5m 이하) ","설치간격 0.6m 초과~0.8m 이하","공M3",0,18325,0,18325,"합계"]
["CAA32113000S",null,"강관동바리 설치 및 해체(토목) (H=2.5m 이하) ","설치간격 0.8m 초과","공M3",0,16492,0,16492,"합계"]
["CAA32121000S",null,"강관동바리 설치 및 해체(토목) (H=2.5m 초과, 3.5m 이하) ","설치간격 0.6m 이하","공M3",0,23707,0,23707,"합계"]
["CAA32122000S",null,"강관동바리 설치 및 해체(토목) (H=2.5m 초과, 3.5m 이하) ","설치간격 0.6m 초과~0.8m 이하","공M3",0,19756,0,19756,"합계"]
["CAA32123000S",null,"강관동바리 설치 및 해체(토목) (H=2.5m 초과, 3.5m 이하) ","설치간격 0.8m 초과","공M3",0,17780,0,17780,"합계"]
["CAA32131000S",null,"강관동바리 설치 및 해체(토목) (H=3.5m 초과, 4.5m 이하) ","설치간격 0.6m 이하","공M3",0,25754,0,25754,"합계"]
["CAA32132000S",null,"강관동바리 설치 및 해체(토목) (H=3.5m 초과, 4.5m 이하) ","설치간격 0.6m 초과~0.8m 이하","공M3",0,21462,0,21462,"합계"]
["CAA32133000S",null,"강관동바리 설치 및 해체(토목) (H=3.5m 초과, 4.5m 이하) ","설치간격 0.8m 초과","공M3",0,19315,0,19315,"합계"]
["CAA32311000S",null,"시스템 동바리 설치 및 해체 (H=10m 이하)","설치간격 0.6m 이하","공M3",141,23661,694,24496,"합계"]
["CAA32312000S",null,"시스템 동바리 설치 및 해체 (H=10m 이하)","설치간격 0.6m 초과~1.2m 이하","공M3",141,19875,694,20710,"합계"]
["CAA32313000S",null,"시스템 동바리 설치 및 해체 (H=10m 이하)","설치간격 1.2m 초과","공M3",141,17982,694,18817,"합계"]
["CAA32321000S",null,"시스템 동바리 설치 및 해체 (H=10m 초과, 20m 이하)","설치간격 0.6m 이하","공M3",207,28002,1021,29230,"합계"]
["CAA32322000S",null,"시스템 동바리 설치 및 해체 (H=10m 초과, 20m 이하)","설치간격 0.6m 초과~1.2m 이하","공M3",207,23567,1021,24795,"합계"]
["CAA32323000S",null,"시스템 동바리 설치 및 해체 (H=10m 초과, 20m 이하)","설치간격 1.2m 초과","공M3",207,21349,1021,22577,"합계"]
["CAA32331000S",null,"시스템 동바리 설치 및 해체 (H=20m 초과, 30m 이하)","설치간격 0.6m 이하","공M3",267,35630,1436,37333,"합계"]
["CAA32332000S",null,"시스템 동바리 설치 및 해체 (H=20m 초과, 30m 이하)","설치간격 0.6m 초과~1.2m 이하","공M3",267,29952,1436,31655,"합계"]
["CAA32333000S",null,"시스템 동바리 설치 및 해체 (H=20m 초과, 30m 이하)","설치간격 1.2m 초과","공M3",267,27113,1436,28816,"합계"]
["CAA32400000S",null,"알루미늄 폼 동바리 설치 및 해체",null,"M2",0,9904,0,9904,"합계"]
["CAA32500000S",null,"잭서포트 설치 및 해체","설치높이 5m이하","개",0,19809,0,19809,"합계"]
["CAA41100000S",null,"토공의 비탈 규준틀 설치 및 철거",null,"개소",0,66065,0,66065,"합계"]
["CAA42100000S",null,"도로용 목재 수평규준틀 설치 및 철거",null,"개소",0,87745,0,87745,"합계"]
["CAA42210000S",null,"도로용 철재 수평규준틀 설치 및 철거","5m이하","개소",0,57393,0,57393,"합계"]
["CAA42220000S",null,"도로용 철재 수평규준틀 설치 및 철거","10m이하","개소",0,68746,0,68746,"합계"]
["CAA43100000S",null,"평, 귀규준틀 설치 및 철거","평규준틀","개소",0,89872,0,89872,"합계"]
["CAA44100000S",null,"평, 귀규준틀 설치 및 철거","귀규준틀","개소",0,154912,0,154912,"합계"]
["CAB20203300S",null,"콘테이너형 가설건축물 설치 및 해체","3.0*3.0m","개소",13436,262148,60206,335790,"합계"]
["CAB20203600S",null,"콘테이너형 가설건축물 설치 및 해체","3.0*6.0m","개소",13436,346909,60206,420551,"합계"]
["CAB20203900S",null,"콘테이너형 가설건축물 설치 및 해체","3.0*9.0m","개소",13436,411572,60206,485214,"합계"]
["CAB21100000S",null,"철제조립식 가설건축물 설치 및 해체","사무실","M2",3034,98487,5719,107240,"합계"]
["CAB22100000S",null,"철제조립식 가설건축물 설치 및 해체","창고","M2",2377,76865,4515,83757,"합계"]
["CAC51000000S",null,"건설용리프트 설치 및 해체","싱글 1.2ton","대",50040,1130977,13273,1194290,"합계"]
["CAC52000000S",null,"마스트 설치 및 해체","지하층 및 1~3층","층",8072,269074,0,277146,"합계"]
["CAC53000000S",null,"축중계 설치 철거","설치, 철거","회당",0,10925,0,10925,"합계"]
["CAC54021000S",null,"파이프루프공 - 작업편성인원","추진관경 300∼600mm","일당",0,1400946,0,1400946,"합계"]
["CAC54022000S",null,"파이프루프공 - 작업편성인원","추진관경 700∼900mm","일당",0,1400946,0,1400946,"합계"]
["CAC54023000S",null,"파이프루프공 - 작업편성인원","추진관경 1000∼1200mm","일당",0,1566491,0,1566491,"합계"]
["CAC54030000S",null,"파이프루프공 - 작업편성장비","1일 8시간 작업기준","일당",186152,714168,2224288,3124608,"합계"]
["CAC54110000S",null,"파이프루프공 - 장비 조립","조립3일","회당",229128,3514662,1230864,4974654,"합계"]
["CAC54210000S",null,"파이프루프공 - 장비 해체","해체2일","회당",152752,2343108,820576,3316436,"합계"]
["CAD13100000S",null,"비산먼지 발생 억제를 위한 살수","물탱크(살수차), 16,000L","100M2",170,377,145,692,"합계"]
["CAD13210000S",null,"자동세륜기 설치",null,"회",24279,485432,78267,587978,"합계"]
["CAD13220000S",null,"자동세륜기 해체",null,"회",32623,706511,99339,838473,"합계"]
["CAD13300000S",null,"슬러지 제거","자동세륜기","회",17142,190659,13041,220842,"합계"]
["CAD16111000S",null,"건축물보양","부직포 깔기","M2",0,496,0,496,"합계"]
["CAD16112000S",null,"건축물보양","보양지 붙이기","M2",0,1655,0,1655,"합계"]
["CAD16113000S",null,"건축물보양","목재 붙이기","M2",0,8041,0,8041,"합계"]
["CAD16210000S",null,"건축물 현장정리","철근콘크리트조, 철골·철근콘크리트조","M2",0,21520,0,21520,"합계"]
["CAD16220000S",null,"건축물 현장정리","목조, 철골조, 조적조","M2",0,8277,0,8277,"합계"]
["CAD16310000S",null,"준공청소",null,"M2",0,3310,0,3310,"합계"]
["CAD16320000S",null,"입주청소",null,"M2",0,4966,0,4966,"합계"]
["CAD91000000S",null,"지능형 CCTV 설치 및 해체","지상 또는 건물설치","개당",2614,261490,0,264104,"합계"]
["CAD91020000S",null,"지능형 CCTV 설치 및 해체","타워크레인설치","개당",5877,587777,0,593654,"합계"]
["CAD92000000S",null,"지능형 출입관리 설치 및 해체",null,"개당",11755,1175555,0,1187310,"합계"]
["CAE13011400S",null,"흙막이판 설치",null,"M2",2268,37058,2503,41829,"합계"]
["CAE13020000S",null,"흙막이판 철거",null,"M2",1812,29492,2008,33312,"합계"]
["CAE15011100S",null,"H-Beam 설치 / 띠장","H=300∼500mm, L=5m이하","본",8465,181925,18700,209090,"합계"]
["CAE15011200S",null,"H-Beam 설치 / 띠장","H=300∼500mm, L=6∼8m","본",9656,200352,22666,232674,"합계"]
["CAE15011300S",null,"H-Beam 설치 / 띠장","H=300∼500mm, L=9∼11m","본",11959,240658,29466,282083,"합계"]
["CAE15011400S",null,"H-Beam 설치 / 띠장","H=300∼500mm, L=12∼14m","본",13417,264983,34000,312400,"합계"]
["CAE15011500S",null,"H-Beam 설치 / 띠장","H=300∼500mm, L=15∼18m","본",15034,291521,39100,345655,"합계"]
["CAE15012100S",null,"H-Beam 설치 / 띠장","H=600∼800mm, L=5m 이하","본",10750,230763,23800,265313,"합계"]
["CAE15012200S",null,"H-Beam 설치 / 띠장","H=600∼800mm, L=6∼8m","본",12447,259970,28900,301317,"합계"]
["CAE15012300S",null,"H-Beam 설치 / 띠장","H=600∼800mm, L=9∼11m","본",15146,304378,37400,356924,"합계"]
["CAE15012400S",null,"H-Beam 설치 / 띠장","H=600∼800mm, L=12∼14m","본",17058,334700,43633,395391,"합계"]
["CAE15012500S",null,"H-Beam 설치 / 띠장","H=600∼800mm, L=15∼18m","본",18338,365209,45900,429447,"합계"]
["CAE15021100S",null,"H-Beam 철거 / 띠장","H=300∼500mm, L=5m이하","본",5449,111782,13033,130264,"합계"]
["CAE15021200S",null,"H-Beam 철거 / 띠장","H=300∼500mm, L=6∼8m","본",6351,126664,15866,148881,"합계"]
["CAE15021300S",null,"H-Beam 철거 / 띠장","H=300∼500mm, L=9∼11m","본",7700,147304,20400,175404,"합계"]
["CAE15021400S",null,"H-Beam 철거 / 띠장","H=300∼500mm, L=12∼14m","본",8710,162743,23800,195253,"합계"]
["CAE15021500S",null,"H-Beam 철거 / 띠장","H=300∼500mm, L=15∼18m","본",9828,178740,27766,216334,"합계"]
["CAE15022100S",null,"H-Beam 철거 / 띠장","H=600∼800mm, L=5m 이하","본",6822,139318,16433,162573,"합계"]
["CAE15022200S",null,"H-Beam 철거 / 띠장","H=600∼800mm, L=6∼8m","본",8063,159401,20400,187864,"합계"]
["CAE15022300S",null,"H-Beam 철거 / 띠장","H=600∼800mm, L=9∼11m","본",9737,184840,26066,220643,"합계"]
["CAE15022400S",null,"H-Beam 철거 / 띠장","H=600∼800mm, L=12∼14m","본",11166,208150,30600,249916,"합계"]
["CAE15022500S",null,"H-Beam 철거 / 띠장","H=600∼800mm, L=15∼18m","본",12471,227374,35133,274978,"합계"]
["CAE16011100S",null,"H-Beam 설치 / 버팀보","H=300∼500mm, L=5m이하","본",7614,165730,16433,189777,"합계"]
["CAE16011200S",null,"H-Beam 설치 / 버팀보","H=300∼500mm, L=6∼8m","본",8617,180930,19833,209380,"합계"]
["CAE16011300S",null,"H-Beam 설치 / 버팀보","H=300∼500mm, L=9∼11m","본",10117,200551,25500,236168,"합계"]
["CAE16011400S",null,"H-Beam 설치 / 버팀보","H=300∼500mm, L=12∼14m","본",11409,219296,30033,260738,"합계"]
["CAE16011500S",null,"H-Beam 설치 / 버팀보","H=300∼500mm, L=15∼18m","본",12547,232941,34566,280054,"합계"]
["CAE16012100S",null,"H-Beam 설치 / 버팀보","H=600∼800mm, L=5m 이하","본",9575,209827,20400,239802,"합계"]
["CAE16012200S",null,"H-Beam 설치 / 버팀보","H=600∼800mm, L=6∼8m ","본",10867,228573,24933,264373,"합계"]
["CAE16012300S",null,"H-Beam 설치 / 버팀보","H=600∼800mm, L=9∼11m","본",12893,256622,32300,301815,"합계"]
["CAE16012400S",null,"H-Beam 설치 / 버팀보","H=600∼800mm, L=12∼14m","본",14400,276481,37966,328847,"합계"]
["CAE16012500S",null,"H-Beam 설치 / 버팀보","H=600∼800mm, L=15∼18m","본",15950,297757,43633,357340,"합계"]
["CAE16021100S",null,"H-Beam 철거 / 버팀보","H=300∼500mm, L=5m이하","본",4814,99710,11333,115857,"합계"]
["CAE16021200S",null,"H-Beam 철거 / 버팀보","H=300∼500mm, L=6∼8m","본",5471,109471,13600,128542,"합계"]
["CAE16021300S",null,"H-Beam 철거 / 버팀보","H=300∼500mm, L=9∼11m","본",6609,123115,18133,147857,"합계"]
["CAE16021400S",null,"H-Beam 철거 / 버팀보","H=300∼500mm, L=12∼14m","본",7424,135088,20966,163478,"합계"]
["CAE16021500S",null,"H-Beam 철거 / 버팀보","H=300∼500mm, L=15∼18m","본",8224,143532,24366,176122,"합계"]
["CAE16022100S",null,"H-Beam 철거 / 버팀보","H=600∼800mm, L=5m 이하","본",6130,128404,14166,148700,"합계"]
["CAE16022200S",null,"H-Beam 철거 / 버팀보","H=600∼800mm, L=6∼8m","본",7053,140935,17566,165554,"합계"]
["CAE16022300S",null,"H-Beam 철거 / 버팀보","H=600∼800mm, L=9∼11m","본",8379,157806,22666,188851,"합계"]
["CAE16022400S",null,"H-Beam 철거 / 버팀보","H=600∼800mm, L=12∼14m","본",9360,169238,26633,205231,"합계"]
["CAE16022500S",null,"H-Beam 철거 / 버팀보","H=600∼800mm, L=15∼18m","본",10464,184756,30600,225820,"합계"]
["CAM54110000S",null,"사석 / 적재 및 운반","0.03m3 이하 덤프트럭 대선 진입 적재","M3",19,993,0,1012,"합계"]
["CAM54120000S",null,"사석 / 적재 및 운반","0.1m3 이상 크레인 적재","M3",71,3583,0,3654,"합계"]
["CBC00000000S",null,"기계기구 설치","지반조사, 보링","개소",0,603225,0,603225,"합계"]
["CBC11010000S",null,"천공 (점토층)","BX, 20m 이내","M",0,201463,0,201463,"합계"]
["CBC12010000S",null,"천공 (점토층)","NX, 20m 이내","M",0,238831,0,238831,"합계"]
["CBC21010000S",null,"천공 (모래층)","BX, 20m 이내","M",0,232798,0,232798,"합계"]
["CBC22010000S",null,"천공 (모래층)","NX, 20m 이내","M",0,275037,0,275037,"합계"]
["CBC31010000S",null,"천공 (자갈층)","BX, 20m 이내","M",0,461156,0,461156,"합계"]
["CBC32010000S",null,"천공 (자갈층)","NX, 20m 이내","M",0,539509,0,539509,"합계"]
["CBC41010000S",null,"천공 (호박돌층)","BX, 20m 이내","M",0,631731,0,631731,"합계"]
["CBC42010000S",null,"천공 (호박돌층)","NX, 20m 이내","M",0,743666,0,743666,"합계"]
["CBC51010000S",null,"천공 (풍화암)","BX, 20m 이내","M",0,207496,0,207496,"합계"]
["CBC52010000S",null,"천공 (풍화암)","NX, 20m 이내","M",0,243702,0,243702,"합계"]
["CBC61010000S",null,"천공 (연암)","BX, 20m 이내","M",0,218399,0,218399,"합계"]
["CBC62010000S",null,"천공 (연암)","NX, 20m 이내","M",0,261225,0,261225,"합계"]
["CBC71010000S",null,"천공 (보통암)","BX, 20m 이내","M",0,244841,0,244841,"합계"]
["CBC72010000S",null,"천공 (보통암)","NX, 20m 이내","M",0,288827,0,288827,"합계"]
["CBC81010000S",null,"천공 (경암)","BX, 20m 이내","M",0,390491,0,390491,"합계"]
["CBC82010000S",null,"천공 (경암)","NX, 20m 이내","M",0,456871,0,456871,"합계"]
["CBC91010000S",null,"천공 (극경암)","BX, 20m 이내","M",0,446734,0,446734,"합계"]
["CBC92010000S",null,"천공 (극경암)","NX, 20m 이내","M",0,529069,0,529069,"합계"]
["CBD10000000S",null,"자연시료 채취",null,"회당",0,152605,0,152605,"합계"]
["CBD24100100S",null,"대구경보링 (토사층)","Ø100mm","M",15826,52215,31314,99355,"합계"]
["CBD24100150S",null,"대구경보링 (토사층)","Ø150mm","M",18841,63445,37279,119565,"합계"]
["CBD24100200S",null,"대구경보링 (토사층)","Ø200mm","M",22609,80918,44735,148262,"합계"]
["CBD24100250S",null,"대구경보링 (토사층)","Ø250mm","M",26378,89975,52191,168544,"합계"]
["CBD24100300S",null,"대구경보링 (토사층)","Ø300mm","M",30146,101175,59647,190968,"합계"]
["CBD24100350S",null,"대구경보링 (토사층)","Ø350mm","M",33914,115104,67103,216121,"합계"]
["CBD24100400S",null,"대구경보링 (토사층)","Ø400mm","M",36929,123605,73068,233602,"합계"]
["CBD24100450S",null,"대구경보링 (토사층)","Ø450mm","M",40697,139676,80524,260897,"합계"]
["CBD24100500S",null,"대구경보링 (토사층)","Ø500mm","M",44465,148733,87980,281178,"합계"]
["CBD24200100S",null,"대구경보링 (모래층)","Ø100mm","M",21102,71389,41753,134244,"합계"]
["CBD24200150S",null,"대구경보링 (모래층)","Ø150mm","M",25624,89418,50700,165742,"합계"]
["CBD24200200S",null,"대구경보링 (모래층)","Ø200mm","M",32407,111848,64121,208376,"합계"]
["CBD24200250S",null,"대구경보링 (모래층)","Ø250mm","M",38436,130991,76050,245477,"합계"]
["CBD24200300S",null,"대구경보링 (모래층)","Ø300mm","M",44465,152864,87980,285309,"합계"]
["CBD24200350S",null,"대구경보링 (모래층)","Ø350mm","M",48987,164621,96927,310535,"합계"]
["CBD24200400S",null,"대구경보링 (모래층)","Ø400mm","M",55770,193323,110348,359441,"합계"]
["CBD24200450S",null,"대구경보링 (모래층)","Ø450mm","M",61800,212466,122277,396543,"합계"]
["CBD24200500S",null,"대구경보링 (모래층)","Ø500mm","M",67829,242754,134207,444790,"합계"]
["CBD24300100S",null,"대구경보링 (자갈층)","Ø100mm","M",28639,100061,56665,185365,"합계"]
["CBD24300150S",null,"대구경보링 (자갈층)","Ø150mm","M",39190,131548,77541,248279,"합계"]
["CBD24300200S",null,"대구경보링 (자갈층)","Ø200mm","M",48987,164621,96927,310535,"합계"]
["CBD24300250S",null,"대구경보링 (자갈층)","Ø250mm","M",61046,205637,120786,387469,"합계"]
["CBD24300300S",null,"대구경보링 (자갈층)","Ø300mm","M",73105,246653,144645,464403,"합계"]
["CBD24300350S",null,"대구경보링 (자갈층)","Ø350mm","M",83656,286555,165522,535733,"합계"]
["CBD24300400S",null,"대구경보링 (자갈층)","Ø400mm","M",95714,327571,189381,612666,"합계"]
["CBD24300450S",null,"대구경보링 (자갈층)","Ø450mm","M",107019,368030,211748,686797,"합계"]
["CBD24300500S",null,"대구경보링 (자갈층)","Ø500mm","M",118324,408489,234116,760929,"합계"]
["CBD24400100S",null,"대구경보링 (호박돌)","Ø100mm","M",44465,152864,87980,285309,"합계"]
["CBD24400150S",null,"대구경보링 (호박돌)","Ø150mm","M",64814,216836,128242,409892,"합계"]
["CBD24400200S",null,"대구경보링 (호박돌)","Ø200mm","M",85917,294498,169995,550410,"합계"]
["CBD24400250S",null,"대구경보링 (호박돌)","Ø250mm","M",111541,379787,220696,712024,"합계"]
["CBD24400300S",null,"대구경보링 (호박돌)","Ø300mm","M",140180,480435,277361,897976,"합계"]
["CBD24400350S",null,"대구경보링 (호박돌)","Ø350mm","M",168066,573667,332535,1074268,"합계"]
["CBD24400400S",null,"대구경보링 (호박돌)","Ø400mm","M",197458,674286,390691,1262435,"합계"]
["CBD24400450S",null,"대구경보링 (호박돌)","Ø450mm","M",225344,767518,445865,1438727,"합계"]
["CBD24400500S",null,"대구경보링 (호박돌)","Ø500mm","M",253229,860750,501039,1615018,"합계"]
["CBD24500100S",null,"대구경보링 (풍화암)","Ø100mm","M",19595,70275,38770,128640,"합계"]
["CBD24500150S",null,"대구경보링 (풍화암)","Ø150mm","M",25624,89418,50700,165742,"합계"]
["CBD24500200S",null,"대구경보링 (풍화암)","Ø200mm","M",33914,115104,67103,216121,"합계"]
["CBD24500250S",null,"대구경보링 (풍화암)","Ø250mm","M",40697,141077,80524,262298,"합계"]
["CBD24500300S",null,"대구경보링 (풍화암)","Ø300mm","M",48234,164064,95436,307734,"합계"]
["CBD24500350S",null,"대구경보링 (풍화암)","Ø350mm","M",54263,183207,107365,344835,"합계"]
["CBD24500400S",null,"대구경보링 (풍화암)","Ø400mm","M",61800,212466,122277,396543,"합계"]
["CBD24500450S",null,"대구경보링 (풍화암)","Ø450mm","M",68583,232167,135698,436448,"합계"]
["CBD24500500S",null,"대구경보링 (풍화암)","Ø500mm","M",75366,254596,149119,479081,"합계"]
["CBD24600100S",null,"대구경보링 (연암)","Ø100mm","M",9797,33072,19385,62254,"합계"]
["CBD24600150S",null,"대구경보링 (연암)","Ø150mm","M",10551,39901,20876,71328,"합계"]
["CBD24600200S",null,"대구경보링 (연암)","Ø200mm","M",14319,48959,28332,91610,"합계"]
["CBD24600250S",null,"대구경보링 (연암)","Ø250mm","M",20348,70832,40262,131442,"합계"]
["CBD24600300S",null,"대구경보링 (연암)","Ø300mm","M",28639,93788,56665,179092,"합계"]
["CBD24600350S",null,"대구경보링 (연암)","Ø350mm","M",39943,134247,79033,253223,"합계"]
["CBD24700100S",null,"대구경보링 (보통암)","Ø100mm","M",19595,57729,38770,116094,"합계"]
["CBD24700150S",null,"대구경보링 (보통암)","Ø150mm","M",21856,74088,43244,139188,"합계"]
["CBD24700200S",null,"대구경보링 (보통암)","Ø200mm","M",23363,81475,46226,151064,"합계"]
["CBD24700250S",null,"대구경보링 (보통암)","Ø250mm","M",33914,115104,67103,216121,"합계"]
["CBD24700300S",null,"대구경보링 (보통암)","Ø300mm","M",45219,155563,89471,290253,"합계"]
["CBD24700350S",null,"대구경보링 (보통암)","Ø350mm","M",63307,215722,125259,404288,"합계"]
["CBD24800100S",null,"대구경보링 (경암)","Ø100mm","M",21856,71946,43244,137046,"합계"]
["CBD24800150S",null,"대구경보링 (경암)","Ø150mm","M",30900,104461,61138,196499,"합계"]
["CBD24800200S",null,"대구경보링 (경암)","Ø200mm","M",43712,152307,86489,282508,"합계"]
["CBD24800250S",null,"대구경보링 (경암)","Ø250mm","M",61800,206194,122277,390271,"합계"]
["CBD24800300S",null,"대구경보링 (경암)","Ø300mm","M",73858,247210,146136,467204,"합계"]
["CBD30000000S",null,"폐공 되메우기","Ø15.24cm, 200m 까지","10M",0,151371,0,151371,"합계"]
["CBD40000000S",null,"대구경보링 - 케이싱 설치","Ø250mm","M",0,129168,0,129168,"합계"]
["CBD50000000S",null,"대구경보링 - 에어써징",null,"M",0,11161,0,11161,"합계"]
["CBD60000000S",null,"대구경보링 - 우물 설치",null,"M",0,11161,0,11161,"합계"]
["CBD70000000S",null,"대구경보링 - 양수시험",null,"HR",0,158739,0,158739,"합계"]
["CBE11000000S",null,"표준관입시험",null,"회당",0,45541,0,45541,"합계"]
["CBE12000000S",null,"베인전단시험","75x150x3mm 블레이드","회당",0,355720,0,355720,"합계"]
["CBE14000000S",null,"2차원 전기비저항탐사",null,"1km당",0,16202479,0,16202479,"합계"]
["CBE15000000S",null,"굴절법 탄성파 탐사",null,"1km당",0,13637349,0,13637349,"합계"]
["CBE19000000S",null,"콘관입시험","정적콘관입시험, 전기식","개소",0,1220152,0,1220152,"합계"]
["CBE32000000S",null,"평판재하시험",null,"회당",0,1053205,0,1053205,"합계"]
["CCD22100000S",null,"플라스틱 보드 드레인(PBD)","장비조립 / 외부 반출 및 반입","회",289375,2722104,472912,3484391,"합계","적용장비확인"]
["CCD22200000S",null,"플라스틱 보드 드레인(PBD)","장비해체 / 외부 반출 및 반입","회",117224,1361052,236456,1714732,"합계","적용장비확인"]
["CCD22300000S",null,"플라스틱 보드 드레인(PBD)","장비 및 인력편성","일",437826,1039589,786832,2264247,"합계"]
["CCD40011000S",null,"고압분사 주입공법","장비조립 / 외부 반출 및 반입","회",361718,3402630,591140,4355488,"합계","적용장비확인"]
["CCD40012000S",null,"고압분사 주입공법","장비조립 / 작업구간 이동","회",217031,2041578,354684,2613293,"합계","적용장비확인"]
["CCD40021000S",null,"고압분사 주입공법","장비해체 / 외부 반출 및 반입","회",144687,1361052,236456,1742195,"합계","적용장비확인"]
["CCD40022000S",null,"고압분사 주입공법","장비해체 / 작업구간 이동","회",72343,680526,118228,871097,"합계","적용장비확인"]
["CCD40023000S",null,"고압분사 주입공법","인력편성(토사)","인/일",0,836947,0,836947,"합계"]
["CCD40033000S",null,"고압분사 주입공법","인력편성(자갈, 호박돌)","인/일",0,1216714,0,1216714,"합계"]
["CCD50111000S",null,"매트부설 / 육상","사면","M2",23,271,16,310,"합계"]
["CCD50112100S",null,"매트부설 / 육상","연약지반 : 도로/철도 ","M2",34,358,24,416,"합계"]
["CCD50112200S",null,"매트부설 / 육상","연약지반 : 매립지","M2",40,402,31,473,"합계"]
["CCD50121000S",null,"매트부설 / 수중","사면 (잠수조제외)","M2",21,541,0,562,"합계"]
["CCD50122000S",null,"매트부설 / 수중","연약지반 (잠수조제외)","M2",28,712,0,740,"합계"]
["CCD50211000S",null,"다짐말뚝","장비조립 / 외부 반출 및 반입","회",434062,4083156,709368,5226586,"합계","적용장비확인"]
["CCD50212000S",null,"다짐말뚝","장비조립 / 작업구간 이동","회",217031,2041578,354684,2613293,"합계","적용장비확인"]
["CCD50220000S",null,"다짐말뚝 / 인력편성",null,"식",0,603225,0,603225,"합계"]
["CCD50221000S",null,"다짐말뚝","장비해체 / 외부 반출 및 반입","회",217031,2041578,354684,2613293,"합계","적용장비확인"]
["CCD50222000S",null,"다짐말뚝","장비해체 / 작업구간 이동","회",144687,1361052,236456,1742195,"합계","적용장비확인"]
["CCD50231000S",null,"다짐말뚝 / 장비편성","L=20M 이하","일",1239392,1605368,1592360,4437120,"합계"]
["CCD50232000S",null,"다짐말뚝 / 장비편성","L=20M ~ 35M","일",1374496,1605368,2069896,5049760,"합계"]
["CCF00010000S",null,"비탈면 보강공","장비조립 및 해체","회",62272,1088705,79952,1230929,"합계"]
["CCF00020110S",null,"비탈면보강공 / 공용구간 / 보통토사","천공 및 보강재삽입, 크레인 제외","M",9081,53728,4431,67240,"합계"]
["CCF00020210S",null,"비탈면보강공 / 공용구간 / 혼합층","천공 및 보강재삽입, 크레인 제외","M",8429,49883,4113,62425,"합계"]
["CCF00020310S",null,"비탈면보강공 / 공용구간 / 풍화암","천공 및 보강재삽입, 크레인 제외","M",5253,30877,2563,38693,"합계"]
["CCF00020410S",null,"비탈면보강공 / 공용구간 / 연암","천공 및 보강재삽입, 크레인 제외","M",7289,42851,3556,53696,"합계"]
["CCF00020510S",null,"비탈면보강공 / 공용구간 / 보통암","천공 및 보강재삽입, 크레인 제외","M",9081,53728,4431,67240,"합계"]
["CCF00020610S",null,"비탈면보강공 / 공용구간 / 경암","천공 및 보강재삽입, 크레인 제외","M",12909,76366,6299,95574,"합계"]
["CCF00021100S",null,"비탈면 보강공 / 스키드형 / 토사","Ø105~127mm, 천공 및 보강재삽입","M",10311,61580,6935,78826,"합계","적용장비확인"]
["CCF00021200S",null,"비탈면 보강공 / 스키드형 / 혼합층","Ø105~127mm, 천공 및 보강재삽입","M",9568,57224,6435,73227,"합계","적용장비확인"]
["CCF00021300S",null,"비탈면 보강공 / 스키드형 / 풍화암","Ø105~127mm, 천공 및 보강재삽입","M",5949,35526,4001,45476,"합계","적용장비확인"]
["CCF00021400S",null,"비탈면 보강공 / 스키드형 / 연암","Ø105~127mm, 천공 및 보강재삽입","M",8279,49570,5568,63417,"합계","적용장비확인"]
["CCF00021500S",null,"비탈면 보강공 / 스키드형 / 보통암","Ø105~127mm, 천공 및 보강재삽입","M",10311,61580,6935,78826,"합계","적용장비확인"]
["CCF00021600S",null,"비탈면 보강공 / 스키드형 / 경암","Ø105~127mm, 천공 및 보강재삽입","M",14674,87633,9870,112177,"합계","적용장비확인"]
["CCF00022100S",null,"비탈면 보강공 / 크롤러형 / 토사","Ø105~127mm, 천공 및 보강재삽입","M",7941,46697,3874,58512,"합계"]
["CCF00022200S",null,"비탈면 보강공 / 크롤러형 / 혼합층","Ø105~127mm, 천공 및 보강재삽입","M",7371,43677,3596,54644,"합계"]
["CCF00022300S",null,"비탈면 보강공 / 크롤러형 / 풍화암","Ø105~127mm, 천공 및 보강재삽입","M",4601,27031,2245,33877,"합계"]
["CCF00022400S",null,"비탈면 보강공 / 크롤러형 / 연암","Ø105~127mm, 천공 및 보강재삽입","M",6352,37797,3099,47248,"합계"]
["CCF00022500S",null,"비탈면 보강공 / 크롤러형 / 보통암","Ø105~127mm, 천공 및 보강재삽입","M",7941,46697,3874,58512,"합계"]
["CCF00022600S",null,"비탈면 보강공 / 크롤러형 / 경암","Ø105~127mm, 천공 및 보강재삽입","M",11321,66863,5524,83708,"합계"]
["CCF00030000S",null,"비탈면 보강공","그라우팅","M3",49895,394763,94072,538730,"합계"]
["CCF00030010S",null,"비탈면보강공 / 공용구간","그라우팅","M3",53166,420504,100469,574139,"합계"]
["CCF00040000S",null,"비탈면 보강공","보강재 조립","TON",0,226320,0,226320,"합계"]
["CCG10020000S",null,"보강토옹벽 / 뒷채움 및 다짐",null,"M3",999,4548,1197,6744,"합계"]
["CCG11000000S",null,"보강토옹벽 / 블록 설치","블록식 옹벽(그리드)","M2",4426,87735,6737,98898,"합계"]
["CCG12000000S",null,"보강토옹벽 / 패널 설치","패널식 옹벽(1.5m x 1.5m)","M2",1770,61298,2695,65763,"합계"]
["CCG12010000S",null,"보강토옹벽 / 버팀목 설치. 해체","패널식 옹벽","M",214,21464,0,21678,"합계"]
["CDA10000000S",null,"벌개제근 / 뿌리뽑기 ","입목 본수도 50-60%, 수경 10∼20cm이하, 집재거리 L=100m 까지","M2",28,384,62,474,"합계"]
["CDA21000000S",null,"벌개제근 / 벌목","H=5.0m 미만, 집재거리 L=100m 까지","M2",81,756,44,881,"합계"]
["CDA22000000S",null,"벌개제근 / 벌목","H=5.0m~8.0m 미만, 집재거리 L=100m 까지","M2",106,988,58,1152,"합계"]
["CDA23000000S",null,"벌개제근 / 벌목","H=8.0m 이상, 집재거리 L=100m 까지","M2",138,1289,76,1503,"합계"]
["CDB11010000S",null,"답면고르기","2,000m2 미만","M2",30,200,27,257,"합계"]
["CDB11020000S",null,"답면고르기","2,000m2∼4,000m2 미만","M2",21,139,18,178,"합계"]
["CDB11030000S",null,"답면고르기","4,000m2∼6,000m2 미만","M2",16,105,14,135,"합계"]
["CDB11040000S",null,"답면고르기","6,000m2∼8,000m2 미만","M2",12,83,11,106,"합계"]
["CDB11050000S",null,"답면고르기","8,000m2∼10,000m2 미만","M2",10,72,9,91,"합계"]
["CDC11100000S",null,"콘크리트구조물 헐기(소형장비)","공압식, 철근","M3",16684,293909,5129,315722,"합계"]
["CDC11200000S",null,"콘크리트구조물 헐기(소형장비)","전기식, 철근","M3",2579,257902,1416,261897,"합계"]
["CDC12100000S",null,"콘크리트구조물 헐기(소형장비)","공압식, 무근","M3",6384,208888,1603,216875,"합계"]
["CDC12200000S",null,"콘크리트구조물 헐기(소형장비)","전기식, 무근","M3",2185,218548,1213,221946,"합계"]
["CDC31000000S",null,"석축헐기(인력, H=3.6m기준)","찰쌓기","M2",4966,99327,0,104293,"합계"]
["CDC32100000S",null,"석축헐기(인력, H=3.6m기준)","메쌓기 뒷길이 45-60cm","M2",1655,33109,0,34764,"합계"]
["CDC32200000S",null,"석축헐기(인력, H=3.6m기준)","메쌓기 뒷길이 60-90cm","M2",2483,49663,0,52146,"합계"]
["CDC33000000S",null,"석축헐기(인력, H=3.6m기준)","질석(마름돌) 쌓기","M3",10251,205032,0,215283,"합계"]
["CDC81000000S",null,"콘크리트구조물 헐기(대형장비)","장애물 미제거(기준높이 10m 이하)","M3",6764,23019,9139,38922,"합계"]
["CDC82000000S",null,"콘크리트구조물 헐기(대형장비)","장애물 제거(기준높이 10m 이하)","M3",10036,37170,18434,65640,"합계"]
["CDD30010000S",null,"암파쇄 / 유압식 할암공법",null,"M3",13947,103742,13030,130719,"합계"]
["CDD30020000S",null,"암발파 / 미진동굴착","TYPE-Ⅰ","M3",6987,27898,4334,39219,"합계","\n"]
["CDD30030000S",null,"암발파 / 정밀진동제어발파","TYPE-Ⅱ","M3",5330,16992,3117,25439,"합계"]
["CDD30040000S",null,"암발파 / 소규모진동 제어발파","TYPE-Ⅲ","M3",3090,9318,1561,13969,"합계"]
["CDD30050000S",null,"암발파 / 중규모진동 제어발파","TYPE-Ⅳ","M3",1428,4940,779,7147,"합계"]
["CDD30060000S",null,"암발파 / 일반발파","TYPE-Ⅴ","M3",1012,3235,583,4830,"합계"]
["CDD30070000S",null,"암발파 / 대규모발파","TYPE-Ⅵ","M3",781,1896,408,3085,"합계"]
["CDD30080000S",null,"암발파 / 소형브레이커",null,"M3",1550,40211,552,42313,"합계"]
["CDD30080010S",null,"발파암유용 기계소할 / 30cm 미만","굴삭기 0.7m3, 전체유용량의 15%","M3",2469,6127,3728,12324,"합계","적용장비확인"]
["CDD30080020S",null,"발파암유용 기계소할 / 30cm 이상","굴삭기 0.7m3, 전체유용량의 15%","M3",2043,5068,3084,10195,"합계","적용장비확인"]
["CDD30091100S",null,"수중발파 / 우물통발파","수심 2.5m 미만 (잠수조제외)","M3",2648,70376,967,73991,"합계"]
["CDD30091200S",null,"수중발파 / 우물통발파","수심 2.5m 이상 ~ 8m 미만 (잠수조제외)","M3",3310,87970,1209,92489,"합계"]
["CDD30091310S",null,"수중발파 / 우물통발파","수심 8m 이상 ~ 15m 미만 (잠수조제외)","M3",4965,131955,1813,138733,"합계"]
["CDD30092100S",null,"수중발파 / 우물통발파 이외","수심 2.5m 미만 (잠수조제외)","M3",1743,44196,636,46575,"합계"]
["CDD30092200S",null,"수중발파 / 우물통발파 이외","수심 2.5m 이상 ~ 8m 미만 (잠수조제외)","M3",2179,55246,796,58221,"합계"]
["CDD30092300S",null,"수중발파 / 우물통발파 이외","수심 8m 이상 ~ 15m 미만 (잠수조제외)","M3",3268,82869,1194,87331,"합계"]
["CDE10010000S",null,"인력굴착(토사)","보통토사, H=1m 이하","M3",0,33109,0,33109,"합계"]
["CDE10020000S",null,"인력굴착(토사)","경질토사, H=1m 이하","M3",0,43041,0,43041,"합계"]
["CDE10030000S",null,"인력굴착(토사)","고사점토 및 자갈섞인토사, H=1m 이하","M3",0,52974,0,52974,"합계"]
["CDE10040000S",null,"인력굴착(토사)","호박돌섞인토사, H=1m 이하","M3",0,94360,0,94360,"합계"]
["CDE20000000S",null,"인력굴착(암반)","풍화암, 10m3 미만","M3",5384,112547,1579,119510,"합계"]
["CDE30010000S",null,"인력굴착(암반)","연암, 10m3 미만","M3",8291,147662,2371,158324,"합계"]
["CDE30020000S",null,"인력굴착(암반)","보통암, 10m3 미만","M3",10551,203316,3103,216970,"합계"]
["CDE30030000S",null,"인력굴착(암반)","경암, 10m3 미만","M3",16934,330476,4992,352402,"합계"]
["CDE91010000S",null,"머신 가이던스(MG) 굴삭기 / 터파기","3D GNSS 머신 가이던스+굴삭기1.0m3","M3",319,523,465,1307,"합계"]
["CDE91020000S",null,"머신 가이던스(MG) 굴삭기 / 성토면고르기","3D GNSS 머신 가이던스+굴삭기1.0m3","M2",226,371,330,927,"합계"]
["CDE91100000S",null,"머신 가이던스(MG) 굴삭기","장비조립","회당",0,833735,0,833735,"합계"]
["CDE91200000S",null,"머신 가이던스(MG) 굴삭기","장비해체","회당",0,833735,0,833735,"합계"]
["CDE92010000S",null,"머신 컨트롤(MC) 굴삭기 / 터파기","3D GNSS 머신 컨트롤+굴삭기1.0m3","M3",309,506,504,1319,"합계"]
["CDE92100000S",null,"머신 컨트롤(MC) 굴삭기","장비조립","회당",0,1250602,0,1250602,"합계"]
["CDE92200000S",null,"머신 컨트롤(MC) 굴삭기","장비해체","회당",0,833735,0,833735,"합계"]
["CDE93010000S",null,"머신 가이던스(MG) 불도저 / 흙깍기","3D GNSS 머신 가이던스+불도저19ton","M3",529,707,723,1959,"합계"]
["CDE93100000S",null,"머신 가이던스(MG) 불도저","장비조립","회당",0,833735,0,833735,"합계"]
["CDE93200000S",null,"머신 가이던스(MG) 불도저","장비해체","회당",0,833735,0,833735,"합계"]
["CDF11010000S",null,"절토면 고르기","모래, 사질토, 점토, 점질토","M2",237,1663,329,2229,"합계"]
["CDF11020000S",null,"절토면 고르기","연질토, 부순자갈","M2",332,2659,461,3452,"합계"]
["CDF11030000S",null,"절토면 고르기","호박돌섞인고결토, 경질토","M2",379,2992,526,3897,"합계"]
["CDF12040000S",null,"절토면 고르기","풍화암","M2",712,5651,988,7351,"합계"]
["CDF13050000S",null,"절토면 고르기","연암","M2",1297,9037,2800,13134,"합계"]
["CDF13060000S",null,"절토면 고르기","보통암, 경암","M2",1693,11919,3654,17266,"합계"]
["CDF30090000S",null,"잔토처리","인력","M3",0,33109,0,33109,"합계"]
["CDF60010000S",null,"터널바닥 암반청소","공동구","M2",3249,38845,3033,45127,"합계"]
["CDF60020000S",null,"터널바닥 암반청소","바닥/인버트","M2",2647,24228,2585,29460,"합계"]
["CDF61100000S",null,"암반청소","댐","M2",3640,88293,5013,96946,"합계"]
["CDF61200000S",null,"암반청소","교량, 옹벽 등","M2",1743,70631,2400,74774,"합계"]
["CDH11111000S",null,"인력 흙 다지기","토사, 성토두께 15cm","M3",0,23176,0,23176,"합계"]
["CDH11111100S",null,"인력 흙 다지기","토사, 성토두께 15cm","M2",0,3542,0,3542,"합계"]
["CDH11112000S",null,"인력 흙 다지기","토사, 성토두께 30cm","M3",0,18209,0,18209,"합계"]
["CDH11112100S",null,"인력 흙 다지기","토사, 성토두께 30cm","M2",0,5512,0,5512,"합계"]
["CDH11121000S",null,"인력 흙 다지기","점토, 성토두께 15cm","M3",0,41386,0,41386,"합계"]
["CDH11121100S",null,"인력 흙 다지기","점토, 성토두께 15cm","M2",0,6290,0,6290,"합계"]
["CDH11122000S",null,"인력 흙 다지기","점토, 성토두께 30cm","M3",0,31453,0,31453,"합계"]
["CDH11122100S",null,"인력 흙 다지기","점토, 성토두께 30cm","M2",0,9436,0,9436,"합계"]
["CDH11200000S",null,"기초다짐 및 뒷채움","소형장비사용","M3",995,10573,1184,12752,"합계"]
["CDH11300000S",null,"기초다짐 및 뒷채움","대형장비사용","M3",1187,6041,1334,8562,"합계"]
["CDI11000000S",null,"성토면 고르기","점토, 점질토, 모래, 사질토","M2",142,501,197,840,"합계"]
["CDI51010000S",null,"차수재공 / 부직포","수직고 30m 이하","M2",43,702,76,821,"합계"]
["CDI51011000S",null,"차수재공 / 부직포","수직고 30m초과 ~ 50m이하","M2",48,702,139,889,"합계"]
["CDI53010000S",null,"차수재공 / 벤토나이트 매트","수직고 30m 이하","M2",48,914,76,1038,"합계"]
["CDI53011000S",null,"차수재공 / 벤토나이트 매트","수직고 30m초과 ~ 50m이하","M2",52,914,139,1105,"합계"]
["CDI54010000S",null,"차수재공 / 지오콤포지트","수직고 30m 이하","M2",48,914,76,1038,"합계"]
["CDI54011000S",null,"차수재공 / 지오콤포지트","수직고 30m초과 ~ 50m이하","M2",52,914,139,1105,"합계"]
["CDI54020000S",null,"차수재공 / HDPE 시트","수직고 30m 이하","M2",187,2153,229,2569,"합계"]
["CDI54021000S",null,"차수재공 / HDPE 시트","수직고 30m초과 ~ 50m이하","M2",200,2153,418,2771,"합계"]
["CDI70000000S",null,"식재면 고르기",null,"M2",0,1543,0,1543,"합계"]
["CDI80000000S",null,"암성토","다짐두께 60cm","M3",360,649,406,1415,"합계"]
["CDJ31020000S",null,"식생기반제 뿜어붙이기","기계기구 설치","회",31136,700140,39976,771252,"합계"]
["CDJ31110010S",null,"절토사면녹화 / 부착망 설치","H=20m 미만, t=10cm 이하","M2",528,7950,152,8630,"합계"]
["CDJ31110015S",null,"절토사면녹화 / 부착망 설치","H=20m 미만, t=15cm 이하","M2",667,9407,187,10261,"합계"]
["CDJ31120005S",null,"식생기반제 뿜어붙이기","H=20m 미만, t=5cm","M2",2659,11152,1933,15744,"합계"]
["CDJ31120007S",null,"식생기반제 뿜어붙이기","H=20m 미만, t=7cm","M2",3417,14212,2485,20114,"합계"]
["CDJ31120010S",null,"식생기반제 뿜어붙이기","H=20m 미만, t=10cm","M2",4837,19937,3521,28295,"합계"]
["CDJ31120015S",null,"식생기반제 뿜어붙이기","H=20m 미만, t=15cm","M2",7105,28904,5178,41187,"합계"]
["CDJ31210010S",null,"절토사면녹화 / 부착망 설치","H=20m~30m 미만, t=10cm 이하","M2",528,9339,152,10019,"합계"]
["CDJ31210015S",null,"절토사면녹화 / 부착망 설치","H=20m~30m 미만, t=15cm 이하","M2",667,11033,187,11887,"합계"]
["CDJ31220005S",null,"식생기반제 뿜어붙이기","H=20m~30m 미만, t=5cm","M2",2659,12089,1933,16681,"합계"]
["CDJ31220007S",null,"식생기반제 뿜어붙이기","H=20m~30m 미만, t=7cm","M2",3417,15392,2485,21294,"합계"]
["CDJ31220010S",null,"식생기반제 뿜어붙이기","H=20m~30m 미만, t=10cm","M2",4837,21568,3521,29926,"합계"]
["CDJ31220015S",null,"식생기반제 뿜어붙이기","H=20m~30m 미만, t=15cm","M2",7105,31221,5178,43504,"합계"]
["CDJ31310010S",null,"절토사면녹화 / 부착망 설치","H=30m~50m 미만, t=10cm 이하","M2",528,10033,152,10713,"합계"]
["CDJ31310015S",null,"절토사면녹화 / 부착망 설치","H=30m~50m 미만, t=15cm 이하","M2",667,11846,187,12700,"합계"]
["CDJ31320005S",null,"식생기반제 뿜어붙이기","H=30m~50m 미만, t=5cm","M2",2659,12557,1933,17149,"합계"]
["CDJ31320007S",null,"식생기반제 뿜어붙이기","H=30m~50m 미만, t=7cm","M2",3417,15982,2485,21884,"합계"]
["CDJ31320010S",null,"식생기반제 뿜어붙이기","H=30m~50m 미만, t=10cm","M2",4837,22384,3521,30742,"합계"]
["CDJ31320015S",null,"식생기반제 뿜어붙이기","H=30m~50m 미만, t=15cm","M2",7063,32237,5155,44455,"합계"]
["CDJ31410010S",null,"절토사면녹화 / 부착망 설치","H=50m 이상, t=10cm 이하","M2",528,10727,152,11407,"합계"]
["CDJ31410015S",null,"절토사면녹화 / 부착망 설치","H=50m 이상, t=15cm 이하","M2",667,12659,187,13513,"합계"]
["CDJ31420005S",null,"식생기반제 뿜어붙이기","H=50m 이상, t=5cm","M2",2659,13026,1933,17618,"합계"]
["CDJ31420007S",null,"식생기반제 뿜어붙이기","H=50m 이상, t=7cm","M2",3417,16572,2485,22474,"합계"]
["CDJ31420010S",null,"식생기반제 뿜어붙이기","H=50m 이상, t=10cm","M2",4837,23200,3521,31558,"합계"]
["CDJ31420015S",null,"식생기반제 뿜어붙이기","H=50m 이상, t=15cm","M2",7063,34554,5155,46772,"합계"]
["CDJ41110000S",null,"비탈면 보호공 / 프리캐스트 콘크리트 블록설치","인력, 비탈경사 1:1.5 이상","M2",0,34597,0,34597,"합계"]
["CDJ41120000S",null,"비탈면 보호공 / 프리캐스트 콘크리트 블록설치","인력, 비탈경사 1:1.0∼1.5 미만","M2",0,38346,0,38346,"합계"]
["CDJ41130000S",null,"비탈면 보호공 / 프리캐스트 콘크리트 블록설치","인력, 비탈경사 1:1.0 미만","M2",0,42095,0,42095,"합계"]
["CDJ41210000S",null,"비탈면 보호공 / 프리캐스트 콘크리트 블록설치","기계, 비탈경사 1:1.5 이상","M2",747,34985,3676,39408,"합계"]
["CDJ41220000S",null,"비탈면 보호공 / 프리캐스트 콘크리트 블록설치","기계, 비탈경사 1:1.0∼1.5 미만","M2",747,38189,3676,42612,"합계"]
["CDJ41230000S",null,"비탈면 보호공 / 프리캐스트 콘크리트 블록설치","기계, 비탈경사 1:1.0 미만","M2",747,41392,3676,45815,"합계"]
["CDJ43000000S",null,"지압판블록 설치","비탈경사 1:1.5이하, H=30M이하 기준","개소당",24163,188171,55025,267359,"합계","적용장비확인"]
["CDJ43000010S",null,"지압판블록 설치 / 공용구간","비탈경사 1:1.5이하, H=30m 기준","개소당",29480,229758,67751,326989,"합계"]
["CDJ65010000S",null,"어스앵커","장비조립 및 해체","회",62272,1088705,79952,1230929,"합계"]
["CDJ65021100S",null,"어스앵커 / 타격식 / 토사","Φ105~127mm, 천공 및 보강재삽입","M",7941,41555,3874,53370,"합계"]
["CDJ65021200S",null,"어스앵커 / 타격식 / 혼합층","Φ105~127mm, 천공 및 보강재삽입","M",7371,38750,3596,49717,"합계"]
["CDJ65021300S",null,"어스앵커 / 타격식 / 풍화암","Φ105~127mm, 천공 및 보강재삽입","M",4601,24032,2245,30878,"합계"]
["CDJ65021400S",null,"어스앵커 / 타격식 / 연암","Φ105~127mm, 천공 및 보강재삽입","M",6352,33513,3099,42964,"합계"]
["CDJ65021500S",null,"어스앵커 / 타격식 / 보통암","Φ105~127mm, 천공 및 보강재삽입","M",7941,41555,3874,53370,"합계"]
["CDJ65021600S",null,"어스앵커 / 타격식 / 경암","Φ105~127mm, 천공 및 보강재삽입","M",11321,59365,5524,76210,"합계"]
["CDJ65022100S",null,"어스앵커 / 회전식 / 토사","Φ105~127mm, 천공 및 보강재삽입","M",3259,20681,2612,26552,"합계"]
["CDJ65030000S",null,"어스앵커","그라우팅","M3",30435,276685,7160,314280,"합계"]
["CDJ65040000S",null,"어스앵커","인장","개소",6555,72839,1615,81009,"합계"]
["CDJ65050000S",null,"어스앵커","좌대설치","개소",0,24240,0,24240,"합계"]
["CDJ71000000S",null,"천연섬유 사면보호공 설치","비탈경사 1:1.0∼1.5, 수직고 30m","M2",0,3700,0,3700,"합계"]
["CEC05210000S",null,"콘크리트 현장비빔타설 / 인력비빔","소형구조물","M3",0,562196,0,562196,"합계"]
["CEC05220000S",null,"콘크리트 현장비빔타설 / 기계비빔","소형구조물","M3",0,218320,0,218320,"합계"]
["CEC10110000S",null,"레디믹스트콘크리트 타설 / 인력운반","무근구조물","M3",1109,55487,0,56596,"합계"]
["CEC10120000S",null,"레디믹스트콘크리트 타설 / 장비사용","무근구조물","M3",2589,22264,2937,27790,"합계","적용장비확인"]
["CEC10210000S",null,"콘크리트 현장비빔타설 / 인력비빔","무근구조물","M3",0,357837,0,357837,"합계"]
["CEC10220000S",null,"콘크리트 현장비빔타설 / 기계비빔","무근구조물","M3",0,115343,0,115343,"합계"]
["CEC10311110S",null,"무근콘크리트 펌프차 타설","8~12cm, Type-Ⅰ(매트기초), Type-Ⅰ(병렬타설)","M3",1402,8350,2491,12243,"합계"]
["CEC10311120S",null,"무근콘크리트 펌프차 타설","8~12cm, Type-Ⅰ(매트기초), Type-Ⅱ(순차타설)","M3",1685,10028,2995,14708,"합계"]
["CEC10311130S",null,"무근콘크리트 펌프차 타설","8~12cm, Type-Ⅰ(매트기초), Type-Ⅲ(연속타설어려움)","M3",2103,12517,3737,18357,"합계"]
["CEC10311210S",null,"무근콘크리트 펌프차 타설","8~12cm, Type-Ⅱ(벽,기둥,보,슬라브), Type-Ⅰ(병렬타설)","M3",1964,11675,3492,17131,"합계"]
["CEC10311220S",null,"무근콘크리트 펌프차 타설","8~12cm, Type-Ⅱ(벽,기둥,보,슬라브), Type-Ⅱ(순차타설)","M3",2357,14034,4186,20577,"합계"]
["CEC10311230S",null,"무근콘크리트 펌프차 타설","8~12cm, Type-Ⅱ(벽,기둥,보,슬라브), Type-Ⅲ(연속타설어려움))","M3",2945,17510,5234,25689,"합계"]
["CEC10311310S",null,"무근콘크리트 펌프차 타설","8~12cm, Type-Ⅲ(옹벽,줄기초 등), Type-Ⅰ(병렬타설)","M3",2455,14592,4363,21410,"합계"]
["CEC10311320S",null,"무근콘크리트 펌프차 타설","8~12cm, Type-Ⅲ(옹벽,줄기초 등), Type-Ⅱ(순차타설)","M3",2945,17510,5234,25689,"합계"]
["CEC10311330S",null,"무근콘크리트 펌프차 타설","8~12cm, Type-Ⅲ(옹벽,줄기초 등), Type-Ⅲ(연속타설어려움)","M3",3685,21918,6548,32151,"합계"]
["CEC10311410S",null,"무근콘크리트 펌프차 타설","8~12cm, Type-Ⅳ(비탈면 등), Type-Ⅰ(병렬타설)","M3",6548,38957,11633,57138,"합계"]
["CEC10311420S",null,"무근콘크리트 펌프차 타설","8~12cm, Type-Ⅳ(비탈면 등), Type-Ⅱ(순차타설)","M3",7858,46744,13961,68563,"합계"]
["CEC10311430S",null,"무근콘크리트 펌프차 타설","8~12cm, Type-Ⅳ(비탈면 등), Type-Ⅲ(연속타설어려움)","M3",9825,58462,17453,85740,"합계"]
["CEC10312110S",null,"무근콘크리트 펌프차 타설","15cm, Type-Ⅰ(매트기초), Type-Ⅰ(병렬타설)","M3",1351,8028,2402,11781,"합계"]
["CEC10312120S",null,"무근콘크리트 펌프차 타설","15cm, Type-Ⅰ(매트기초), Type-Ⅱ(순차타설)","M3",1621,9658,2879,14158,"합계"]
["CEC10312130S",null,"무근콘크리트 펌프차 타설","15cm, Type-Ⅰ(매트기초), Type-Ⅲ(연속타설어려움)","M3",2026,12040,3600,17666,"합계"]
["CEC10312210S",null,"무근콘크리트 펌프차 타설","15cm, Type-Ⅱ(벽,기둥,보,슬라브), Type-Ⅰ(병렬타설)","M3",1892,11246,3362,16500,"합계"]
["CEC10312220S",null,"무근콘크리트 펌프차 타설","15cm, Type-Ⅱ(벽,기둥,보,슬라브), Type-Ⅱ(순차타설)","M3",2271,13498,4036,19805,"합계"]
["CEC10312230S",null,"무근콘크리트 펌프차 타설","15cm, Type-Ⅱ(벽,기둥,보,슬라브), Type-Ⅲ(연속타설어려움))","M3",2839,16893,5044,24776,"합계"]
["CEC10312310S",null,"무근콘크리트 펌프차 타설","15cm, Type-Ⅲ(옹벽,줄기초 등), Type-Ⅰ(병렬타설)","M3",2363,14045,4199,20607,"합계"]
["CEC10312320S",null,"무근콘크리트 펌프차 타설","15cm, Type-Ⅲ(옹벽,줄기초 등), Type-Ⅱ(순차타설)","M3",2839,16893,5044,24776,"합계"]
["CEC10312330S",null,"무근콘크리트 펌프차 타설","15cm, Type-Ⅲ(옹벽,줄기초 등), Type-Ⅲ(연속타설어려움)","M3",3547,21093,6303,30943,"합계"]
["CEC10312410S",null,"무근콘크리트 펌프차 타설","15cm, Type-Ⅳ(비탈면 등), Type-Ⅰ(병렬타설)","M3",6307,37525,11204,55036,"합계"]
["CEC10312420S",null,"무근콘크리트 펌프차 타설","15cm, Type-Ⅳ(비탈면 등), Type-Ⅱ(순차타설)","M3",7568,45033,13444,66045,"합계"]
["CEC10312430S",null,"무근콘크리트 펌프차 타설","15cm, Type-Ⅳ(비탈면 등), Type-Ⅲ(연속타설어려움)","M3",9460,56279,16806,82545,"합계"]
["CEC10313110S",null,"무근콘크리트 펌프차 타설","18cm이상, Type-Ⅰ(매트기초), Type-Ⅰ(병렬타설)","M3",1256,7475,2232,10963,"합계"]
["CEC10313120S",null,"무근콘크리트 펌프차 타설","18cm이상, Type-Ⅰ(매트기초), Type-Ⅱ(순차타설)","M3",1510,8993,2681,13184,"합계"]
["CEC10313130S",null,"무근콘크리트 펌프차 타설","18cm이상, Type-Ⅰ(매트기초), Type-Ⅲ(연속타설어려움)","M3",1889,11240,3355,16484,"합계"]
["CEC10313210S",null,"무근콘크리트 펌프차 타설","18cm이상, Type-Ⅱ(벽,기둥,보,슬라브), Type-Ⅰ(병렬타설)","M3",1761,10463,3131,15355,"합계"]
["CEC10313220S",null,"무근콘크리트 펌프차 타설","18cm이상, Type-Ⅱ(벽,기둥,보,슬라브), Type-Ⅱ(순차타설)","M3",2115,12581,3757,18453,"합계"]
["CEC10313230S",null,"무근콘크리트 펌프차 타설","18cm이상, Type-Ⅱ(벽,기둥,보,슬라브), Type-Ⅲ(연속타설어려움))","M3",2643,15718,4696,23057,"합계"]
["CEC10313310S",null,"무근콘크리트 펌프차 타설","18cm이상, Type-Ⅲ(옹벽,줄기초 등), Type-Ⅰ(병렬타설)","M3",2204,13123,3914,19241,"합계"]
["CEC10313320S",null,"무근콘크리트 펌프차 타설","18cm이상, Type-Ⅲ(옹벽,줄기초 등), Type-Ⅱ(순차타설)","M3",2643,15718,4696,23057,"합계"]
["CEC10313330S",null,"무근콘크리트 펌프차 타설","18cm이상, Type-Ⅲ(옹벽,줄기초 등), Type-Ⅲ(연속타설어려움)","M3",3303,19655,5867,28825,"합계"]
["CEC10313410S",null,"무근콘크리트 펌프차 타설","18cm이상, Type-Ⅳ(비탈면 등), Type-Ⅰ(병렬타설)","M3",5874,34945,10435,51254,"합계"]
["CEC10313420S",null,"무근콘크리트 펌프차 타설","18cm이상, Type-Ⅳ(비탈면 등), Type-Ⅱ(순차타설)","M3",7047,41933,12518,61498,"합계"]
["CEC10313430S",null,"무근콘크리트 펌프차 타설","18cm이상, Type-Ⅳ(비탈면 등), Type-Ⅲ(연속타설어려움)","M3",8809,52396,15649,76854,"합계"]
["CEC15110000S",null,"레디믹스트콘크리트 타설 / 인력운반","무근, 소량(12m3 이하), 타설위치 산재","M3",2228,111402,0,113630,"합계"]
["CEC15120000S",null,"레디믹스트콘크리트 타설 / 장비사용","무근, 소량(12m3 이하), 타설위치 산재","M3",5174,44267,5874,55315,"합계"]
["CEC20110000S",null,"레디믹스트콘크리트 타설 / 인력운반","철근구조물","M3",1280,64024,0,65304,"합계"]
["CEC20120000S",null,"레디믹스트콘크리트 타설 / 장비사용","철근구조물","M3",2957,25426,3353,31736,"합계","적용장비확인"]
["CEC20210000S",null,"콘크리트 현장비빔타설 / 인력비빔","철근구조물","M3",0,391205,0,391205,"합계"]
["CEC20220000S",null,"콘크리트 현장비빔타설 / 기계비빔","철근구조물","M3",0,156988,0,156988,"합계"]
["CEC20311110S",null,"철근콘크리트 펌프차 타설","8~12cm, Type-Ⅰ(매트기초), Type-Ⅰ(병렬타설)","M3",1521,9916,2593,14030,"합계"]
["CEC20311120S",null,"철근콘크리트 펌프차 타설","8~12cm, Type-Ⅰ(매트기초), Type-Ⅱ(순차타설)","M3",1826,11914,3110,16850,"합계"]
["CEC20311130S",null,"철근콘크리트 펌프차 타설","8~12cm, Type-Ⅰ(매트기초), Type-Ⅲ(연속타설어려움)","M3",2281,14891,3886,21058,"합계"]
["CEC20311210S",null,"철근콘크리트 펌프차 타설","8~12cm, Type-Ⅱ(벽,기둥,보,슬라브), Type-Ⅰ(병렬타설)","M3",2130,13903,3628,19661,"합계"]
["CEC20311220S",null,"철근콘크리트 펌프차 타설","8~12cm, Type-Ⅱ(벽,기둥,보,슬라브), Type-Ⅱ(순차타설)","M3",2556,16677,4356,23589,"합계"]
["CEC20311230S",null,"철근콘크리트 펌프차 타설","8~12cm, Type-Ⅱ(벽,기둥,보,슬라브), Type-Ⅲ(연속타설어려움))","M3",3196,20847,5445,29488,"합계"]
["CEC20311310S",null,"철근콘크리트 펌프차 타설","8~12cm, Type-Ⅲ(옹벽,줄기초 등), Type-Ⅰ(병렬타설)","M3",2664,17367,4540,24571,"합계"]
["CEC20311320S",null,"철근콘크리트 펌프차 타설","8~12cm, Type-Ⅲ(옹벽,줄기초 등), Type-Ⅱ(순차타설)","M3",3196,20847,5445,29488,"합계"]
["CEC20311330S",null,"철근콘크리트 펌프차 타설","8~12cm, Type-Ⅲ(옹벽,줄기초 등), Type-Ⅲ(연속타설어려움)","M3",3995,26058,6807,36860,"합계"]
["CEC20311410S",null,"철근콘크리트 펌프차 타설","8~12cm, Type-Ⅳ(비탈면 등), Type-Ⅰ(병렬타설)","M3",7102,46317,12103,65522,"합계"]
["CEC20311420S",null,"철근콘크리트 펌프차 타설","8~12cm, Type-Ⅳ(비탈면 등), Type-Ⅱ(순차타설)","M3",8522,55597,14519,78638,"합계"]
["CEC20311430S",null,"철근콘크리트 펌프차 타설","8~12cm, Type-Ⅳ(비탈면 등), Type-Ⅲ(연속타설어려움)","M3",10654,69485,18154,98293,"합계"]
["CEC20312110S",null,"철근콘크리트 펌프차 타설","15cm, Type-Ⅰ(매트기초), Type-Ⅰ(병렬타설)","M3",1462,9552,2491,13505,"합계"]
["CEC20312120S",null,"철근콘크리트 펌프차 타설","15cm, Type-Ⅰ(매트기초), Type-Ⅱ(순차타설)","M3",1757,11465,2995,16217,"합계"]
["CEC20312130S",null,"철근콘크리트 펌프차 타설","15cm, Type-Ⅰ(매트기초), Type-Ⅲ(연속타설어려움)","M3",2194,14320,3737,20251,"합계"]
["CEC20312210S",null,"철근콘크리트 펌프차 타설","15cm, Type-Ⅱ(벽,기둥,보,슬라브), Type-Ⅰ(병렬타설)","M3",2048,13347,3492,18887,"합계"]
["CEC20312220S",null,"철근콘크리트 펌프차 타설","15cm, Type-Ⅱ(벽,기둥,보,슬라브), Type-Ⅱ(순차타설)","M3",2457,16046,4186,22689,"합계"]
["CEC20312230S",null,"철근콘크리트 펌프차 타설","15cm, Type-Ⅱ(벽,기둥,보,슬라브), Type-Ⅲ(연속타설어려움))","M3",3072,20044,5234,28350,"합계"]
["CEC20312310S",null,"철근콘크리트 펌프차 타설","15cm, Type-Ⅲ(옹벽,줄기초 등), Type-Ⅰ(병렬타설)","M3",2561,16709,4363,23633,"합계"]
["CEC20312320S",null,"철근콘크리트 펌프차 타설","15cm, Type-Ⅲ(옹벽,줄기초 등), Type-Ⅱ(순차타설)","M3",3072,20044,5234,28350,"합계"]
["CEC20312330S",null,"철근콘크리트 펌프차 타설","15cm, Type-Ⅲ(옹벽,줄기초 등), Type-Ⅲ(연속타설어려움)","M3",3842,25053,6548,35443,"합계"]
["CEC20312410S",null,"철근콘크리트 펌프차 타설","15cm, Type-Ⅳ(비탈면 등), Type-Ⅰ(병렬타설)","M3",6828,44548,11633,63009,"합계"]
["CEC20312420S",null,"철근콘크리트 펌프차 타설","15cm, Type-Ⅳ(비탈면 등), Type-Ⅱ(순차타설)","M3",8194,53459,13961,75614,"합계"]
["CEC20312430S",null,"철근콘크리트 펌프차 타설","15cm, Type-Ⅳ(비탈면 등), Type-Ⅲ(연속타설어려움)","M3",10243,66823,17453,94519,"합계"]
["CEC20313110S",null,"철근콘크리트 펌프차 타설","18cm이상, Type-Ⅰ(매트기초), Type-Ⅰ(병렬타설)","M3",1358,8868,2314,12540,"합계"]
["CEC20313120S",null,"철근콘크리트 펌프차 타설","18cm이상, Type-Ⅰ(매트기초), Type-Ⅱ(순차타설)","M3",1629,10631,2777,15037,"합계"]
["CEC20313130S",null,"철근콘크리트 펌프차 타설","18cm이상, Type-Ⅰ(매트기초), Type-Ⅲ(연속타설어려움)","M3",2038,13304,3471,18813,"합계"]
["CEC20313210S",null,"철근콘크리트 펌프차 타설","18cm이상, Type-Ⅱ(벽,기둥,보,슬라브), Type-Ⅰ(병렬타설)","M3",1902,12412,3240,17554,"합계"]
["CEC20313220S",null,"철근콘크리트 펌프차 타설","18cm이상, Type-Ⅱ(벽,기둥,보,슬라브), Type-Ⅱ(순차타설)","M3",2281,14891,3886,21058,"합계"]
["CEC20313230S",null,"철근콘크리트 펌프차 타설","18cm이상, Type-Ⅱ(벽,기둥,보,슬라브), Type-Ⅲ(연속타설어려움))","M3",2852,18612,4860,26324,"합계"]
["CEC20313310S",null,"철근콘크리트 펌프차 타설","18cm이상, Type-Ⅲ(옹벽,줄기초 등), Type-Ⅰ(병렬타설)","M3",2377,15517,4050,21944,"합계"]
["CEC20313320S",null,"철근콘크리트 펌프차 타설","18cm이상, Type-Ⅲ(옹벽,줄기초 등), Type-Ⅱ(순차타설)","M3",2852,18612,4860,26324,"합계"]
["CEC20313330S",null,"철근콘크리트 펌프차 타설","18cm이상, Type-Ⅲ(옹벽,줄기초 등), Type-Ⅲ(연속타설어려움)","M3",3567,23258,6078,32903,"합계"]
["CEC20313410S",null,"철근콘크리트 펌프차 타설","18cm이상, Type-Ⅳ(비탈면 등), Type-Ⅰ(병렬타설)","M3",6340,41367,10802,58509,"합계"]
["CEC20313420S",null,"철근콘크리트 펌프차 타설","18cm이상, Type-Ⅳ(비탈면 등), Type-Ⅱ(순차타설)","M3",7609,49621,12967,70197,"합계"]
["CEC20313430S",null,"철근콘크리트 펌프차 타설","18cm이상, Type-Ⅳ(비탈면 등), Type-Ⅲ(연속타설어려움)","M3",9511,62034,16207,87752,"합계"]
["CEC25110000S",null,"레디믹스트콘크리트 타설 / 인력운반","철근, 소량(12m3 이하), 타설위치 산재","M3",2560,128048,0,130608,"합계"]
["CEC25120000S",null,"레디믹스트콘크리트 타설 / 장비사용","철근, 소량(12m3 이하), 타설위치 산재","M3",5926,50648,6730,63304,"합계"]
["CED11100000S",null,"합판거푸집 / 인력투입","제물치장, 수직고 7m까지","M2",852,85299,0,86151,"합계"]
["CED11200000S",null,"합판거푸집 / 인력투입","매우복잡, 수직고 7m까지","M2",682,68239,0,68921,"합계"]
["CED11300000S",null,"합판거푸집 / 인력투입","복잡, 수직고 7m까지","M2",570,57012,0,57582,"합계"]
["CED11400000S",null,"합판거푸집 / 인력투입","보통, 수직고 7m까지","M2",378,37806,0,38184,"합계"]
["CED11500000S",null,"합판거푸집 / 인력투입","간단, 수직고 7m까지","M2",341,34119,0,34460,"합계"]
["CED21100000S",null,"강재거푸집 / 인력설치",null,"M2",0,37411,0,37411,"합계"]
["CED21200000S",null,"강재거푸집 / 해체",null,"M2",0,24745,0,24745,"합계"]
["CED22300000S",null,"강재거푸집 / 장비조합 설치 및 해체","일반","M2",1714,21470,5666,28850,"합계","적용장비확인"]
["CED22400000S",null,"강재거푸집 / 장비조합 설치 및 해체","코핑","M2",4921,44079,15463,64463,"합계","적용장비확인"]
["CED22500000S",null,"강재거푸집 / 장비조합 설치 및 해체","교각","M2",3817,31129,12597,47543,"합계","적용장비확인"]
["CED31300000S",null,"유로폼 설치 및 해체 / 인력투입","복잡, 수직고 7m까지","M2",1518,50618,0,52136,"합계"]
["CED31400000S",null,"유로폼 설치 및 해체 / 인력투입","보통, 수직고 7m까지","M2",1084,36148,0,37232,"합계"]
["CED31500000S",null,"유로폼 설치 및 해체 / 인력투입","간단, 수직고 7m까지","M2",949,31636,0,32585,"합계"]
["CED40000000S",null,"문양거푸집(판넬) 설치 및 해체",null,"M2",0,24214,0,24214,"합계"]
["CED51000740S",null,"합성수지(P.E)원형 맨홀 거푸집 / 기초 및 슬래브","Ø740mm","조",0,55991,0,55991,"합계"]
["CED51000900S",null,"합성수지(P.E)원형 맨홀 거푸집 / 기초 및 슬래브","Ø900mm","조",0,71377,0,71377,"합계"]
["CED51001200S",null,"합성수지(P.E)원형 맨홀 거푸집 / 기초 및 슬래브","Ø1200mm","조",0,81796,0,81796,"합계"]
["CED51001500S",null,"합성수지(P.E)원형 맨홀 거푸집 / 기초 및 슬래브","Ø1500mm","조",0,102635,0,102635,"합계"]
["CED51001800S",null,"합성수지(P.E)원형 맨홀 거푸집 / 기초 및 슬래브","Ø1800mm","조",0,127759,0,127759,"합계"]
["CED52000740S",null,"합성수지(P.E)원형 맨홀 거푸집 / 벽체","Ø740mm, H=1.0m","조",0,113833,0,113833,"합계"]
["CED52000900S",null,"합성수지(P.E)원형 맨홀 거푸집 / 벽체","Ø900mm, H=1.0m","조",0,133503,0,133503,"합계"]
["CED52001200S",null,"합성수지(P.E)원형 맨홀 거푸집 / 벽체","Ø1200mm, H=1.0m","조",0,170702,0,170702,"합계"]
["CED52001500S",null,"합성수지(P.E)원형 맨홀 거푸집 / 벽체","Ø1500mm, H=1.0m","조",0,211698,0,211698,"합계"]
["CED52001800S",null,"합성수지(P.E)원형 맨홀 거푸집 / 벽체","Ø1800mm, H=1.0m","조",0,250551,0,250551,"합계"]
["CED61100000S",null,"슬립폼 공법","설치","M2",3848,78230,13243,95321,"합계","적용장비확인"]
["CED61200000S",null,"슬립폼 공법","해체 ","M2",6331,63256,26431,96018,"합계","적용장비확인"]
["CED62000000S",null,"슬립폼 공법","인상","M2",0,20031,0,20031,"합계"]
["CED63000000S",null,"슬립폼 공법","철근조립콘크리트타설","TON",0,263401,0,263401,"합계"]
["CED71100000S",null,"알루미늄폼 설치 및 해체","셋팅층","M2",0,42034,0,42034,"합계"]
["CED71200000S",null,"알루미늄폼 설치 및 해체","마감층","M2",0,31636,0,31636,"합계"]
["CED72000000S",null,"알루미늄폼 설치 및 해체","일반층","M2",0,17991,0,17991,"합계"]
["CED81100000S",null,"갱폼 설치 및 해체","셋팅층","M2",4764,49650,17375,71789,"합계","적용장비확인"]
["CED81200000S",null,"갱폼 설치 및 해체","마감층","M2",616,30808,0,31424,"합계"]
["CED82000000S",null,"갱폼 설치 및 해체","일반층","M2",344,17219,0,17563,"합계"]
["CEE10010000S",null,"철근 현장가공","Type-Ⅰ","TON",18964,210711,0,229675,"합계"]
["CEE10020000S",null,"철근 현장가공","Type-Ⅱ","TON",21284,236488,0,257772,"합계"]
["CEE10030000S",null,"철근 현장가공","Type-Ⅲ","TON",24455,271725,0,296180,"합계"]
["CEE20010000S",null,"철근 현장조립","토목 Type-Ⅰ-1 (반중력식, L형옹벽,슬래브,매트기초 등)","TON",11110,555512,0,566622,"합계"]
["CEE20020000S",null,"철근 현장조립","토목 Type-Ⅰ-2 (빔제작,철근망 등)","TON",10958,547944,0,558902,"합계"]
["CEE20030000S",null,"철근 현장조립","토목 Type-Ⅱ-1 (라멘교,교대,암거,지하차도,부벽식옹벽 등)","TON",12538,626932,0,639470,"합계"]
["CEE20040000S",null,"철근 현장조립","토목 Type-Ⅱ-2 (측구,개거,중력식옹벽,일체형중앙분리대 등)","TON",12481,624095,0,636576,"합계"]
["CEE20050000S",null,"철근 현장조립","토목 Type-Ⅲ (교각,구주식교대,플랜트,원자력발전소 등)","TON",13569,678487,0,692056,"합계"]
["CEE20110000S",null,"철근 현장조립","토목 Type-Ⅰ-1 (개소별 소량 0.5ton 미만)","TON",22272,1113626,0,1135898,"합계"]
["CEE20120000S",null,"철근 현장조립","토목 Type-Ⅰ-2 (개소별 소량 0.5ton 미만)","TON",21950,1097544,0,1119494,"합계"]
["CEE20130000S",null,"철근 현장조립","토목 Type-Ⅱ-1 (개소별 소량 0.5ton 미만)","TON",25129,1256466,0,1281595,"합계"]
["CEE20140000S",null,"철근 현장조립","토목 Type-Ⅱ-2 (개소별 소량 0.5ton 미만)","TON",24963,1248190,0,1273153,"합계"]
["CEE20150000S",null,"철근 현장조립","토목 Type-Ⅲ (개소별 소량 0.5ton 미만)","TON",27224,1361231,0,1388455,"합계"]
["CEE30010000S",null,"철근 공장가공","Type-Ⅰ","TON",0,64797,38878,103675,"합계"]
["CEE30020000S",null,"철근 공장가공","Type-Ⅱ","TON",0,84662,50797,135459,"합계"]
["CEE30030000S",null,"철근 공장가공","Type-Ⅲ","TON",0,108784,65270,174054,"합계"]
["CEE71000000S",null,"철근 기계적이음","D35이상, H:10m미만","개소",0,89091,0,89091,"합계"]
["CEF10010900S",null,"교량신축이음 교체 / 1차로 차단","절단폭 900MM 이하, 일시공량 3.5m 적용","M",83277,769084,72306,924667,"합계","적용장비확인"]
["CEF10011200S",null,"교량신축이음 교체 / 1차로 차단","절단폭 1,200MM 이하, 일시공량 3.5m 적용","M",83277,769084,72306,924667,"합계","적용장비확인"]
["CEF10011500S",null,"교량신축이음 교체 / 1차로 차단","절단폭 1,500MM 이하, 일시공량 3.5m 적용","M",116581,896080,121511,1134172,"합계","적용장비확인"]
["CEF10011800S",null,"교량신축이음 교체 / 1차로 차단","절단폭 1,800MM 이하, 일시공량 3.5m 적용","M",119362,942432,121511,1183305,"합계","적용장비확인"]
["CEF10020900S",null,"교량신축이음 교체 / 2차로 차단","절단폭 900MM 이하, 일시공량 7m 적용","M",43125,410672,35995,489792,"합계","적용장비확인"]
["CEF10021200S",null,"교량신축이음 교체 / 2차로 차단","절단폭 1,200MM 이하, 일시공량 7m 적용","M",43125,410672,35995,489792,"합계","적용장비확인"]
["CEF10021500S",null,"교량신축이음 교체 / 2차로 차단","절단폭 1,500MM 이하, 일시공량 7m 적용","M",59923,474727,60813,595463,"합계","적용장비확인"]
["CEF10021800S",null,"교량신축이음 교체 / 2차로 차단","절단폭 1,800MM 이하, 일시공량 7m 적용","M",59923,474727,60813,595463,"합계","적용장비확인"]
["CEF10030000S",null,"신축이음 / 실링 마감","V컷팅, 프라이머바름, 백업재삽입, 실랭재주입 포함","M",51,5125,0,5176,"합계"]
["CEF10030900S",null,"교량신축이음 교체 / 3차로 차단","절단폭 900MM 이하, 일시공량 10.5m 적용","M",28647,271531,24060,324238,"합계","적용장비확인"]
["CEF10031200S",null,"교량신축이음 교체 / 3차로 차단","절단폭 1,200MM 이하, 일시공량 10.5m 적용","M",29868,291883,24060,345811,"합계","적용장비확인"]
["CEF10031500S",null,"교량신축이음 교체 / 3차로 차단","절단폭 1,500MM 이하, 일시공량 10.5m 적용","M",40999,334326,40504,415829,"합계","적용장비확인"]
["CEF10031800S",null,"교량신축이음 교체 / 3차로 차단","절단폭 1,800MM 이하, 일시공량 10.5m 적용","M",40999,334326,40504,415829,"합계","적용장비확인"]
["CEF10111000S",null,"교량신축이음장치 설치 / 도로교","절단폭 900mm 이하","M",13307,146863,13826,173996,"합계","적용장비확인"]
["CEF10112000S",null,"교량신축이음장치 설치 / 도로교","절단폭 1,200mm 이하","M",15067,166331,15646,197044,"합계","적용장비확인"]
["CEF10113000S",null,"교량신축이음장치 설치 / 도로교","절단폭 1,500mm 이하","M",17389,191983,18053,227425,"합계","적용장비확인"]
["CEF10114000S",null,"교량신축이음장치 설치 / 도로교","절단폭 1,800mm 이하","M",22605,249473,23484,295562,"합계","적용장비확인"]
["CEF10200000S",null,"교량신축이음장치 설치 / 철도교",null,"M",4051,135058,0,139109,"합계"]
["CEF30020000S",null,"신축이음 / 채움재 설치","채움재 두께 20mm ","M2",0,8967,0,8967,"합계"]
["CEF40010000S",null,"지수판설치 / PVC 용접",null,"M",1546,51550,0,53096,"합계"]
["CEF40020000S",null,"지수판설치 / 소켓 연결",null,"M",0,23009,0,23009,"합계"]
["CEF80010000S",null,"신축이음 / 다웰바 설치","설치 간격 150mm","EA",0,13313,0,13313,"합계"]
["CEG11100000S",null,"PSC 빔 제작 / 포스트텐션 / 쉬즈관설치","Ø85mm 이하","M",189,9459,0,9648,"합계"]
["CEG12000000S",null,"PSC 빔 제작 / 포스트텐션 / 정착구설치","쉬즈관규격 Ø85mm 이하","개당",1871,37430,0,39301,"합계"]
["CEG13010000S",null,"PSC 빔 제작 / 포스트텐션 / 강연선설치","강연선규격 Ø12.7mm","TON",17961,256590,0,274551,"합계"]
["CEG13020000S",null,"PSC 빔 제작 / 포스트텐션 / 강연선설치","강연선규격 Ø15.2mm","TON",14898,212840,0,227738,"합계"]
["CEG14310000S",null,"PSC 빔 제작 / 포스트텐션 / 인장","강연선규격 Ø12.7mm","개소당",3617,72353,5491,81461,"합계"]
["CEG14320000S",null,"PSC 빔 제작 / 포스트텐션 / 인장","강연선규격 Ø15.2mm","개소당",4148,82967,6498,93613,"합계"]
["CEG15000000S",null,"PSC 빔 제작 / 포스트텐션 / 그라우팅",null,"m3",44854,747571,8305,800730,"합계"]
["CEG16000000S",null,"PSC 빔 제작대 설치",null,"M",2321,32171,3121,37613,"합계"]
["CEG21110000S",null,"PSC BOX 제작 / 쉬즈관 설치","쉬즈관규격 Ø75mm 이하","M",222,11115,0,11337,"합계"]
["CEG21120000S",null,"PSC BOX 제작 / 쉬즈관 설치","쉬즈관규격 Ø100mm 이하","M",326,16317,0,16643,"합계"]
["CEG21130000S",null,"PSC BOX 제작 / 쉬즈관 설치","쉬즈관규격 Ø130mm 이하","M",463,23175,0,23638,"합계"]
["CEG22010000S",null,"PSC BOX 제작 / 정착구 설치","쉬즈관규격 Ø75mm 이하","EA",5371,134289,0,139660,"합계"]
["CEG22020000S",null,"PSC BOX 제작 / 정착구 설치","쉬즈관규격 Ø100mm 이하","EA",6802,170064,0,176866,"합계"]
["CEG22030000S",null,"PSC BOX 제작 / 정착구 설치","쉬즈관규격 Ø130mm 이하","EA",8267,206691,0,214958,"합계"]
["CEG23010000S",null,"PSC BOX 제작 / 강연선 설치","강연선규격 Ø12.7mm","TON",26321,526424,0,552745,"합계"]
["CEG23020000S",null,"PSC BOX 제작 / 강연선 설치","강연선규격 Ø15.2mm","TON",22714,454295,0,477009,"합계"]
["CEG24111000S",null,"PSC BOX 제작 / 1단 인장","7가닥, Ø12.7mm","개소",6198,123964,6396,136558,"합계"]
["CEG24112000S",null,"PSC BOX 제작 / 1단 인장","12가닥, Ø12.7mm","개소",8968,179373,9013,197354,"합계"]
["CEG24113000S",null,"PSC BOX 제작 / 1단 인장","19가닥, Ø12.7mm","개소",13905,278116,14053,306074,"합계"]
["CEG24114000S",null,"PSC BOX 제작 / 1단 인장","31가닥, Ø12.7mm","개소",20751,415031,21128,456910,"합계"]
["CEG24121000S",null,"PSC BOX 제작 / 1단 인장","7가닥, Ø15.2mm","개소",7259,145192,7365,159816,"합계"]
["CEG24122000S",null,"PSC BOX 제작 / 1단 인장","12가닥, Ø15.2mm","개소",10263,205276,10467,226006,"합계"]
["CEG24123000S",null,"PSC BOX 제작 / 1단 인장","19가닥, Ø15.2mm","개소",16038,320768,16282,353088,"합계"]
["CEG24124000S",null,"PSC BOX 제작 / 1단 인장","31가닥, Ø15.2mm","개소",24169,483392,24520,532081,"합계"]
["CEG24211000S",null,"PSC BOX 제작 / 양단 인장","7가닥, Ø12.7mm","개소",11666,233321,12890,257877,"합계"]
["CEG24212000S",null,"PSC BOX 제작 / 양단 인장","12가닥, Ø12.7mm","개소",16909,338199,18802,373910,"합계"]
["CEG24213000S",null,"PSC BOX 제작 / 양단 인장","19가닥, Ø12.7mm","개소",25464,509295,28494,563253,"합계"]
["CEG24214000S",null,"PSC BOX 제작 / 양단 인장","31가닥, Ø12.7mm","개소",35952,719051,40221,795224,"합계"]
["CEG24221000S",null,"PSC BOX 제작 / 양단 인장","7가닥, Ø15.2mm","개소",13375,267501,14828,295704,"합계"]
["CEG24222000S",null,"PSC BOX 제작 / 양단 인장","12가닥, Ø15.2mm","개소",19690,393803,21807,435300,"합계"]
["CEG24223000S",null,"PSC BOX 제작 / 양단 인장","19가닥, Ø15.2mm","개소",25688,513774,33049,572511,"합계"]
["CEG24224000S",null,"PSC BOX 제작 / 양단 인장","31가닥, Ø15.2mm","개소",36176,723530,46618,806324,"합계"]
["CEG25000000S",null,"PSC BOX 제작 / 그라우팅","재료비 별도","M3",51688,1033765,12687,1098140,"합계"]
["CER10000000S",null,"표면 마무리",null,"M2",0,907,0,907,"합계"]
["CER41010000S",null,"에폭시 콘크리트 접착체 바르기","신구-콘크리트 접착제 바르기","M2",601,30093,0,30694,"합계"]
["CER41020000S",null,"에폭시 콘크리트 접착체 바르기","콘크리트 및 고무기타 접착제 바르기","M2",601,30093,0,30694,"합계"]
["CER42000000S",null,"콘크리트 치핑","소형치핑장비활용","M2",2321,29017,0,31338,"합계"]
["CER81100000S",null,"콘크리트 균열 보수","표면처리공법","M",48,2427,0,2475,"합계"]
["CER81200000S",null,"콘크리트 균열 보수","주입공법","M",423,21169,0,21592,"합계"]
["CER81300000S",null,"콘크리트 균열 보수","페커주입공법","M",1011,33730,0,34741,"합계"]
["CER81400000S",null,"콘크리트 균열 보수","충전공법","M",489,16329,0,16818,"합계"]
["CER82000000S",null,"콘크리트 단면처리","보수두께 10MM 이하 ","M2",297,9912,0,10209,"합계"]
["CER83000000S",null,"콘크리트 단면복구","보수두께 50MM 이하","M2",3556,88903,0,92459,"합계"]
["CER84000000S",null,"워터젯 치핑","파쇄깊이는 3cm이상에 적용","M2",5680,23211,8786,37677,"합계"]
["CFE21000000S",null,"PC 기둥 설치","2ton미만 / 시공높이 30M이하","개소",15665,100238,15051,130954,"합계","적용장비확인"]
["CFE22000000S",null,"PC 기둥 설치","5ton미만 / 시공높이 30M이하","개소",16672,106701,16044,139417,"합계","적용장비확인"]
["CFE23000000S",null,"PC 기둥 설치","10ton미만 / 시공높이 30M이하","개소",20242,123269,25125,168636,"합계","적용장비확인"]
["CFE25000000S",null,"PC 기둥 설치","20ton미만 / 시공높이 30M이하","개소",28280,160162,45333,233775,"합계","적용장비확인"]
["CFE26000000S",null,"PC 기둥 설치","30ton미만 / 시공높이 30M이하","개소",41773,201577,65453,308803,"합계","적용장비확인"]
["CFF51000000S",null,"PC 슬래브 설치","2ton미만 / 시공높이 30M이하","개소",9593,67186,8910,85689,"합계","적용장비확인"]
["CFF52000000S",null,"PC 슬래브 설치","5ton미만 / 시공높이 30M이하","개소",10371,72633,9632,92636,"합계","적용장비확인"]
["CFF53000000S",null,"PC 슬래브 설치","10ton미만 / 시공높이 30M이하","개소",12339,82376,14870,109585,"합계","적용장비확인"]
["CFF60000000S",null,"모르타르 주입","PC건축물 부재의 접합","M3",160956,3219134,0,3380090,"합계"]
["CFF70100000S",null,"모듈러 건축설치 / 12층 이하","3m x 10m 이내 양중 및 설치","개소",31193,335811,76367,443371,"합계","적용장비확인"]
["CFF70200000S",null,"모듈러 건축설치 / 13층 이상","3m x 10m 이내 양중 및 설치","개소",46809,503023,114838,664670,"합계","적용장비확인"]
["CFH11010000S",null,"PC BOX 설치","5ton미만 / TYPE-Ⅰ","개소",4756,105051,13512,123319,"합계","적용장비확인"]
["CFH11020000S",null,"PC BOX 설치","5ton미만 / TYPE-Ⅱ","개소",6338,139987,18004,164329,"합계","적용장비확인"]
["CFH12010000S",null,"PC BOX 설치","10ton미만 / TYPE-Ⅰ","개소",6741,131313,22265,160319,"합계","적용장비확인"]
["CFH12020000S",null,"PC BOX 설치","10ton미만 / TYPE-Ⅱ","개소",8992,175165,29702,213859,"합계","적용장비확인"]
["CFH13010000S",null,"PC BOX 설치","15ton미만 / TYPE-Ⅰ","개소",8410,150167,31383,189960,"합계","적용장비확인"]
["CFH13020000S",null,"PC BOX 설치","15ton미만 / TYPE-Ⅱ","개소",10706,191137,39958,241801,"합계","적용장비확인"]
["CFH31000000S",null,"PC 벽체 설치","2ton미만 / 시공높이 30M이하","개소",20867,133542,20078,174487,"합계","적용장비확인"]
["CFH32000000S",null,"PC 벽체 설치","5ton미만 / 시공높이 30M이하","개소",22767,145691,21884,190342,"합계","적용장비확인"]
["CFH33000000S",null,"PC 벽체 설치","10ton미만 / 시공높이 30M이하","개소",26299,160162,32683,219144,"합계","적용장비확인"]
["CFH35000000S",null,"PC 벽체 설치","20ton미만 / 시공높이 30M이하","개소",35584,201577,56667,293828,"합계","적용장비확인"]
["CFH36000000S",null,"PC 벽체 설치","30ton미만 / 시공높이 30M이하","개소",55235,266199,87052,408486,"합계","적용장비확인"]
["CFH41000000S",null,"PC 거더 설치","2ton미만 / 시공높이 30M이하","개소",12359,86552,11469,110380,"합계","적용장비확인"]
["CFH42000000S",null,"PC 거더 설치","5ton미만 / 시공높이 30M이하","개소",13655,95632,12673,121960,"합계","적용장비확인"]
["CFH43000000S",null,"PC 거더 설치","10ton미만 / 시공높이 30M이하","개소",15998,106804,19242,142044,"합계","적용장비확인"]
["CFH44000000S",null,"PC 거더 설치","20ton미만 / 시공높이 30M이하","개소",19453,121053,30203,170709,"합계","적용장비확인"]
["CFH45000000S",null,"PC 거더 설치","30ton미만 / 시공높이 30M이하","개소",28447,151322,43657,223426,"합계","적용장비확인"]
["CGA21100250S",null,"원심력 철근콘크리트관/소켓관 부설 및 접합","Ø250mm","본",4311,60413,4566,69290,"합계"]
["CGA21100300S",null,"원심력 철근콘크리트관/소켓관 부설 및 접합","Ø300mm","본",5406,78244,5653,89303,"합계"]
["CGA21100350S",null,"원심력 철근콘크리트관/소켓관 부설 및 접합","Ø350mm","본",6502,96075,6740,109317,"합계"]
["CGA21100400S",null,"원심력 철근콘크리트관/소켓관 부설 및 접합","Ø400mm","본",7597,113905,7827,129329,"합계"]
["CGA21200250S",null,"원심력 철근콘크리트관/수밀밴드 접합 및 부설","Ø250mm","본",4262,57981,4566,66809,"합계"]
["CGA21200300S",null,"원심력 철근콘크리트관/수밀밴드 접합 및 부설","Ø300mm","본",5324,74157,5653,85134,"합계"]
["CGA21200350S",null,"원심력 철근콘크리트관/수밀밴드 접합 및 부설","Ø350mm","본",6371,89556,6740,102667,"합계"]
["CGA21200400S",null,"원심력 철근콘크리트관/수밀밴드 접합 및 부설","Ø400mm","본",7467,107387,7827,122681,"합계"]
["CGA21300250S",null,"원심력 철근콘크리트관 절단","Ø250mm","개소",490,8174,0,8664,"합계"]
["CGA21300300S",null,"원심력 철근콘크리트관 절단","Ø300mm","개소",735,12261,0,12996,"합계"]
["CGA21300350S",null,"원심력 철근콘크리트관 절단","Ø350mm","개소",735,12261,0,12996,"합계"]
["CGA21300400S",null,"원심력 철근콘크리트관 절단","Ø400mm","개소",980,16348,0,17328,"합계"]
["CGA21800025S",null,"원심력철근콘크리트관 철거","Ø250mm","본",2924,24021,4044,30989,"합계"]
["CGA21800030S",null,"원심력철근콘크리트관 철거","Ø300mm","본",3222,26387,4457,34066,"합계"]
["CGA21800035S",null,"원심력철근콘크리트관 철거","Ø350mm","본",3600,29477,4979,38056,"합계"]
["CGA21800040S",null,"원심력철근콘크리트관 철거","Ø400mm","본",4056,33288,5609,42953,"합계"]
["CGA31100450S",null,"원심력 철근콘크리트관/소켓관 부설 및 접합","Ø450mm","본",8693,131736,8914,149343,"합계"]
["CGA31100500S",null,"원심력 철근콘크리트관/소켓관 부설 및 접합","Ø500mm","본",9788,149567,10001,169356,"합계"]
["CGA31100600S",null,"원심력 철근콘크리트관/소켓관 부설 및 접합","Ø600mm","본",11979,185229,12176,209384,"합계"]
["CGA31200450S",null,"원심력 철근콘크리트관/수밀밴드 접합 및 부설","Ø450mm","본",8562,125218,8914,142694,"합계"]
["CGA31200500S",null,"원심력 철근콘크리트관/수밀밴드 접합 및 부설","Ø500mm","본",9609,140617,10001,160227,"합계"]
["CGA31200600S",null,"원심력 철근콘크리트관/수밀밴드 접합 및 부설","Ø600mm","본",11800,176278,12176,200254,"합계"]
["CGA31300450S",null,"원심력 철근콘크리트관 절단","Ø450mm","개소",980,16348,0,17328,"합계"]
["CGA31300500S",null,"원심력 철근콘크리트관 절단","Ø500mm","개소",1226,20435,0,21661,"합계"]
["CGA31300600S",null,"원심력 철근콘크리트관 절단","Ø600mm","개소",1716,28609,0,30325,"합계"]
["CGA31600150S",null,"원심력 철근콘크리트관/천공 및 접합","본관 Ø500mm이하, 연결관 Ø150mm","개소",1021,20435,0,21456,"합계"]
["CGA31600200S",null,"원심력 철근콘크리트관/천공 및 접합","본관 Ø500mm이하, 연결관 Ø200mm","개소",1430,28609,0,30039,"합계"]
["CGA31600250S",null,"원심력 철근콘크리트관/천공 및 접합","본관 Ø500mm이하, 연결관 Ø250mm","개소",1839,36784,0,38623,"합계"]
["CGA31600300S",null,"원심력 철근콘크리트관/천공 및 접합","본관 Ø500mm이하, 연결관 Ø300mm","개소",2452,49045,0,51497,"합계"]
["CGA31700500S",null,"PC관 부설 및 접합","Ø500mm","본",14060,323363,15437,352860,"합계"]
["CGA31700600S",null,"PC관 부설 및 접합","Ø600mm","본",16671,401514,18046,436231,"합계"]
["CGA31800045S",null,"원심력철근콘크리트관 철거","Ø450mm","본",4496,36732,6218,47446,"합계"]
["CGA31800050S",null,"원심력철근콘크리트관 철거","Ø500mm","본",4842,39561,6696,51099,"합계"]
["CGA31800060S",null,"원심력철근콘크리트관 철거","Ø600mm","본",5722,46769,7914,60405,"합계"]
["CGA41100700S",null,"원심력 철근콘크리트관/소켓관 부설 및 접합","Ø700mm","본",14170,220891,14350,249411,"합계"]
["CGA41100800S",null,"원심력 철근콘크리트관/소켓관 부설 및 접합","Ø800mm","본",16361,256552,16524,289437,"합계"]
["CGA41100900S",null,"원심력 철근콘크리트관/소켓관 부설 및 접합","Ø900mm","본",19471,292214,24188,335873,"합계"]
["CGA41200700S",null,"원심력 철근콘크리트관/수밀밴드 접합 및 부설","Ø700mm","본",13909,207853,14350,236112,"합계"]
["CGA41200800S",null,"원심력 철근콘크리트관/수밀밴드 접합 및 부설","Ø800mm","본",16051,241083,16524,273658,"합계"]
["CGA41200900S",null,"원심력 철근콘크리트관/수밀밴드 접합 및 부설","Ø900mm","본",18193,274313,18698,311204,"합계"]
["CGA41300700S",null,"원심력 철근콘크리트관 절단","Ø700mm","개소",1961,32697,0,34658,"합계"]
["CGA41300800S",null,"원심력 철근콘크리트관 절단","Ø800mm","개소",2452,40871,0,43323,"합계"]
["CGA41300900S",null,"원심력 철근콘크리트관 절단","Ø900mm","개소",2697,44958,0,47655,"합계"]
["CGA41600150S",null,"원심력 철근콘크리트관/천공 및 접합","본관 Ø500mm초과~Ø900mm이하, 연결관 Ø150mm","개소",1430,28609,0,30039,"합계"]
["CGA41600200S",null,"원심력 철근콘크리트관/천공 및 접합","본관 Ø500mm초과~Ø900mm이하, 연결관 Ø200mm","개소",1839,36784,0,38623,"합계"]
["CGA41600250S",null,"원심력 철근콘크리트관/천공 및 접합","본관 Ø500mm초과~Ø900mm이하, 연결관 Ø250mm","개소",2247,44958,0,47205,"합계"]
["CGA41600300S",null,"원심력 철근콘크리트관/천공 및 접합","본관 Ø500mm초과~Ø900mm이하, 연결관 Ø300mm","개소",2656,53132,0,55788,"합계"]
["CGA41700700S",null,"PC관 부설 및 접합","Ø700mm","본",19534,452173,25875,497582,"합계"]
["CGA41700800S",null,"PC관 부설 및 접합","Ø800mm","본",20296,504791,21743,546830,"합계"]
["CGA41700900S",null,"PC관 부설 및 접합","Ø900mm","본",22175,555449,23699,601323,"합계"]
["CGA41800070S",null,"원심력철근콘크리트관 철거","Ø700mm","본",6980,57232,9653,73865,"합계"]
["CGA41800080S",null,"원심력철근콘크리트관 철거","Ø800mm","본",7860,64440,10871,83171,"합계"]
["CGA41800090S",null,"원심력철근콘크리트관 철거","Ø900mm","본",10325,79241,17297,106863,"합계"]
["CGA51101000S",null,"원심력 철근콘크리트관/소켓관 부설 및 접합","Ø1000mm","본",21769,327876,27000,376645,"합계"]
["CGA51101100S",null,"원심력 철근콘크리트관/소켓관 부설 및 접합","Ø1100mm","본",24066,363537,29813,417416,"합계"]
["CGA51101200S",null,"원심력 철근콘크리트관/소켓관 부설 및 접합","Ø1200mm","본",26364,399199,32626,458189,"합계"]
["CGA51201000S",null,"원심력 철근콘크리트관/수밀밴드 접합 및 부설","Ø1000mm","본",21377,308319,27000,356696,"합계"]
["CGA51201100S",null,"원심력 철근콘크리트관/수밀밴드 접합 및 부설","Ø1100mm","본",23627,341549,29813,394989,"합계"]
["CGA51201200S",null,"원심력 철근콘크리트관/수밀밴드 접합 및 부설","Ø1200mm","본",25876,374779,32626,433281,"합계"]
["CGA51301000S",null,"원심력 철근콘크리트관 절단","Ø1,000mm","개소",3187,53132,0,56319,"합계"]
["CGA51301100S",null,"원심력 철근콘크리트관 절단","Ø1,100mm","개소",3433,57219,0,60652,"합계"]
["CGA51301200S",null,"원심력 철근콘크리트관 절단","Ø1,200mm","개소",3923,65394,0,69317,"합계"]
["CGA51600150S",null,"원심력 철근콘크리트관/천공 및 접합","본관 Ø900mm초과~Ø1200mm이하, 연결관 Ø150mm","개소",1634,32697,0,34331,"합계"]
["CGA51600200S",null,"원심력 철근콘크리트관/천공 및 접합","본관 Ø900mm초과~Ø1200mm이하, 연결관 Ø200mm","개소",2247,44958,0,47205,"합계"]
["CGA51600250S",null,"원심력 철근콘크리트관/천공 및 접합","본관 Ø900mm초과~Ø1200mm이하, 연결관 Ø250mm","개소",2452,49045,0,51497,"합계"]
["CGA51600300S",null,"원심력 철근콘크리트관/천공 및 접합","본관 Ø900mm초과~Ø1200mm이하, 연결관 Ø300mm","개소",3065,61306,0,64371,"합계"]
["CGA51701000S",null,"PC관 부설 및 접합","Ø1000mm","본",24786,633600,26309,684695,"합계"]
["CGA51701100S",null,"PC관 부설 및 접합","Ø1100mm","본",19290,724348,68723,812361,"합계"]
["CGA51701200S",null,"PC관 부설 및 접합","Ø1200mm","본",21143,801860,74877,897880,"합계"]
["CGA51800100S",null,"원심력철근콘크리트관 철거","Ø1,000mm","본",12206,93657,20447,126310,"합계"]
["CGA51800110S",null,"원심력철근콘크리트관 철거","Ø1,100mm","본",14943,113742,25032,153717,"합계"]
["CGA51800120S",null,"원심력철근콘크리트관 철거","Ø1,200mm","본",16790,129543,28126,174459,"합계"]
["CGA61101350S",null,"원심력 철근콘크리트관/소켓관 부설 및 접합","Ø1350mm","본",29811,452692,36845,519348,"합계"]
["CGA61101500S",null,"원심력 철근콘크리트관/소켓관 부설 및 접합","Ø1500mm","본",33257,506184,41063,580504,"합계"]
["CGA61201350S",null,"원심력 철근콘크리트관/수밀밴드 접합 및 부설","Ø1350mm","본",29274,425840,36845,491959,"합계"]
["CGA61201500S",null,"원심력 철근콘크리트관/수밀밴드 접합 및 부설","Ø1500mm","본",32639,475246,41063,548948,"합계"]
["CGA61301350S",null,"원심력 철근콘크리트관 절단","Ø1,350mm","개소",4414,73568,0,77982,"합계"]
["CGA61301500S",null,"원심력 철근콘크리트관 절단","Ø1,500mm","개소",4904,81742,0,86646,"합계"]
["CGA61701350S",null,"PC관 부설 및 접합","Ø1350mm","본",25685,986300,90263,1102248,"합계"]
["CGA61701500S",null,"PC관 부설 및 접합","Ø1500mm","본",29488,1141881,103084,1274453,"합계"]
["CGA61800135S",null,"원심력철근콘크리트관 철거","Ø1,350mm","본",22330,171205,37407,230942,"합계"]
["CGA61800150S",null,"원심력철근콘크리트관 철거","Ø1,500mm","본",26864,205945,45001,277810,"합계"]
["CGA71101650S",null,"원심력 철근콘크리트관/소켓관 부설 및 접합","Ø1650mm","본",36704,559677,45282,641663,"합계"]
["CGA71101800S",null,"원심력 철근콘크리트관/소켓관 부설 및 접합","Ø1800mm","본",40151,613169,49501,702821,"합계"]
["CGA71201650S",null,"원심력 철근콘크리트관/수밀밴드 접합 및 부설","Ø1650mm","본",36037,526307,45282,607626,"합계"]
["CGA71201800S",null,"원심력 철근콘크리트관/수밀밴드 접합 및 부설","Ø1800mm","본",39402,575712,49501,664615,"합계"]
["CGA71301650S",null,"원심력 철근콘크리트관 절단","Ø1,650mm","개소",5395,89916,0,95311,"합계"]
["CGA71301800S",null,"원심력 철근콘크리트관 절단","Ø1,800mm","개소",6130,102178,0,108308,"합계"]
["CGA81102000S",null,"원심력 철근콘크리트관/소켓관 부설 및 접합","Ø2000mm","본",44746,684493,55126,784365,"합계"]
["CGA81202000S",null,"원심력 철근콘크리트관/수밀밴드 접합 및 부설","Ø2000mm","본",43949,644604,55126,743679,"합계"]
["CGA81302000S",null,"원심력 철근콘크리트관 절단","Ø2,000mm","개소",6866,114439,0,121305,"합계"]
["CGB20000100S",null,"주철관 절단","Ø100mm 이하","개소",972,19453,0,20425,"합계"]
["CGB20000125S",null,"주철관 절단","Ø125mm","개소",1094,21885,0,22979,"합계"]
["CGB20000150S",null,"주철관 절단","Ø150mm","개소",1215,24316,0,25531,"합계"]
["CGB20000200S",null,"주철관 절단","Ø200mm","개소",1459,29180,0,30639,"합계"]
["CGB20100100S",null,"주철관 부설","Ø100mm 이하, L=6.0m","본",4716,33725,6522,44963,"합계"]
["CGB20100125S",null,"주철관 부설","Ø125mm, L=6.0m","본",5187,39229,7175,51591,"합계"]
["CGB20100150S",null,"주철관 부설","Ø150mm, L=6.0m","본",5659,47165,7827,60651,"합계"]
["CGB20100200S",null,"주철관 부설","Ø200mm, L=6.0m","본",6602,60605,9132,76339,"합계"]
["CGB20110080S",null,"주철관 부설 / 인력","Ø80mm, L=6.0m","본",0,41077,0,41077,"합계"]
["CGB20110100S",null,"주철관 부설 / 인력","Ø100mm, L=6.0m","본",0,51683,0,51683,"합계"]
["CGB20110120S",null,"주철관 부설 / 인력","Ø120mm, L=6.0m","본",0,60736,0,60736,"합계"]
["CGB20110150S",null,"주철관 부설 / 인력","Ø150mm, L=6.0m","본",0,91984,0,91984,"합계"]
["CGB20200100S",null,"K.P. 메커니컬 조인트관 접합","Ø100mm","개소",521,26075,0,26596,"합계"]
["CGB20200125S",null,"K.P. 메커니컬 조인트관 접합","Ø125mm","개소",603,30162,0,30765,"합계"]
["CGB20200150S",null,"K.P. 메커니컬 조인트관 접합","Ø150mm","개소",651,32594,0,33245,"합계"]
["CGB20200200S",null,"K.P. 메커니컬 조인트관 접합","Ø200mm","개소",863,43199,0,44062,"합계"]
["CGB20300100S",null,"타이튼 조인트관 접합","Ø100mm 이하","개소",391,19556,0,19947,"합계"]
["CGB20300125S",null,"타이튼 조인트관 접합","Ø125mm","개소",472,23643,0,24115,"합계"]
["CGB20300150S",null,"타이튼 조인트관 접합","Ø150mm","개소",521,26075,0,26596,"합계"]
["CGB20300200S",null,"타이튼 조인트관 접합","Ø200mm","개소",651,32594,0,33245,"합계"]
["CGB20400010S",null,"주철관 철거","Ø100mm 이하","본",2986,24618,4131,31735,"합계"]
["CGB20400012S",null,"주철관 철거","Ø120mm","본",3490,28737,4826,37053,"합계"]
["CGB20400015S",null,"주철관 철거","Ø150mm","본",3694,30246,5109,39049,"합계"]
["CGB20400020S",null,"주철관 철거","Ø200mm","본",3930,32259,5435,41624,"합계"]
["CGB30000250S",null,"주철관 절단","Ø250mm","개소",1702,34043,0,35745,"합계"]
["CGB30000300S",null,"주철관 절단","Ø300mm","개소",1945,38906,0,40851,"합계"]
["CGB30000350S",null,"주철관 절단","Ø350mm","개소",2188,43770,0,45958,"합계"]
["CGB30000400S",null,"주철관 절단","Ø400mm","개소",2431,48633,0,51064,"합계"]
["CGB30100250S",null,"주철관 부설","Ø250mm, L=6.0m","본",7546,74821,10436,92803,"합계"]
["CGB30100300S",null,"주철관 부설","Ø300mm, L=6.0m","본",8489,88261,11741,108491,"합계"]
["CGB30100350S",null,"주철관 부설","Ø350mm, L=6.0m","본",9432,101700,13045,124177,"합계"]
["CGB30100400S",null,"주철관 부설","Ø400mm, L=6.0m","본",10375,115140,14350,139865,"합계"]
["CGB30100450S",null,"주철관 부설","Ø450mm, L=6.0m","본",11319,129356,15654,156329,"합계"]
["CGB30200250S",null,"K.P. 메커니컬 조인트관 접합","Ø250mm","개소",994,49718,0,50712,"합계"]
["CGB30200300S",null,"K.P. 메커니컬 조인트관 접합","Ø300mm","개소",1206,60324,0,61530,"합계"]
["CGB30200350S",null,"K.P. 메커니컬 조인트관 접합","Ø350mm","개소",1385,69275,0,70660,"합계"]
["CGB30200400S",null,"K.P. 메커니컬 조인트관 접합","Ø400mm","개소",1515,75794,0,77309,"합계"]
["CGB30300250S",null,"타이튼 조인트관 접합","Ø250mm","개소",815,40768,0,41583,"합계"]
["CGB30300300S",null,"타이튼 조인트관 접합","Ø300mm","개소",945,47287,0,48232,"합계"]
["CGB30300350S",null,"타이튼 조인트관 접합","Ø350mm","개소",1076,53805,0,54881,"합계"]
["CGB30300400S",null,"타이튼 조인트관 접합","Ø400mm","개소",1255,62756,0,64011,"합계"]
["CGB30400025S",null,"주철관 철거","Ø250mm","본",4197,34365,5805,44367,"합계"]
["CGB30400030S",null,"주철관 철거","Ø300mm","본",4496,36732,6218,47446,"합계"]
["CGB30400035S",null,"주철관 철거","Ø350mm","본",4842,39561,6696,51099,"합계"]
["CGB40000450S",null,"주철관 절단","Ø450mm","개소",2674,53496,0,56170,"합계"]
["CGB40000500S",null,"주철관 절단","Ø500mm","개소",2918,58360,0,61278,"합계"]
["CGB40000600S",null,"주철관 절단","Ø600mm","개소",3404,68087,0,71491,"합계"]
["CGB40000700S",null,"주철관 절단","Ø700mm","개소",3890,77813,0,81703,"합계"]
["CGB40100500S",null,"주철관 부설","Ø500mm, L=6.0m","본",12262,142796,16959,172017,"합계"]
["CGB40100600S",null,"주철관 부설","Ø600mm, L=6.0m","본",14148,169676,19568,203392,"합계"]
["CGB40100700S",null,"주철관 부설","Ø700mm, L=6.0m","본",17125,197332,28688,243145,"합계"]
["CGB40200450S",null,"K.P. 메커니컬 조인트관 접합","Ø450mm","개소",1727,86399,0,88126,"합계"]
["CGB40200500S",null,"K.P. 메커니컬 조인트관 접합","Ø500mm","개소",1858,92918,0,94776,"합계"]
["CGB40200600S",null,"K.P. 메커니컬 조인트관 접합","Ø600mm","개소",2249,112475,0,114724,"합계"]
["CGB40200700S",null,"K.P. 메커니컬 조인트관 접합","Ø700mm","개소",2591,129599,0,132190,"합계"]
["CGB40300450S",null,"타이튼 조인트관 접합","Ø450mm","개소",1385,69275,0,70660,"합계"]
["CGB40300500S",null,"타이튼 조인트관 접합","Ø500mm","개소",1515,75794,0,77309,"합계"]
["CGB50000800S",null,"주철관 절단","Ø800mm","개소",4377,87540,0,91917,"합계"]
["CGB50000900S",null,"주철관 절단","Ø900mm","개소",4863,97267,0,102130,"합계"]
["CGB50001000S",null,"주철관 절단","Ø1000mm","개소",5349,106993,0,112342,"합계"]
["CGB50001100S",null,"주철관 절단","Ø1100mm","개소",5836,116720,0,122556,"합계"]
["CGB50100800S",null,"주철관 부설","Ø800mm, L=6.0m","본",19140,224211,32063,275414,"합계"]
["CGB50100900S",null,"주철관 부설","Ø900mm, L=6.0m","본",21155,251867,35438,308460,"합계"]
["CGB50101000S",null,"주철관 부설","Ø1000mm, L=6.0m","본",23170,278746,38813,340729,"합계"]
["CGB50101100S",null,"주철관 부설","Ø1100mm, L=6.0m","본",25185,306402,42189,373776,"합계"]
["CGB50200800S",null,"K.P. 메커니컬 조인트관 접합","Ø800mm","개소",2934,146724,0,149658,"합계"]
["CGB50200900S",null,"K.P. 메커니컬 조인트관 접합","Ø900mm","개소",3243,162194,0,165437,"합계"]
["CGB50201000S",null,"K.P. 메커니컬 조인트관 접합","Ø1000mm","개소",3586,179318,0,182904,"합계"]
["CGB50201100S",null,"K.P. 메커니컬 조인트관 접합","Ø1100mm","개소",3977,198875,0,202852,"합계"]
["CGB60001200S",null,"주철관 절단","Ø1200mm","개소",6322,126447,0,132769,"합계"]
["CGB60101200S",null,"주철관 부설","Ø1200mm, L=6.0m","본",27199,333282,45564,406045,"합계"]
["CGB60201200S",null,"K.P. 메커니컬 조인트관 접합","Ø1200mm","개소",4319,215999,0,220318,"합계"]
["CGC01400000S",null,"강관압입추진공 - 조명시설","(재료비별도)","M",105,3513,0,3618,"합계"]
["CGC22000100S",null,"강관 부설","Ø100mm, L=6.0m","본",10218,69709,14132,94059,"합계"]
["CGC22000125S",null,"강관 부설","Ø125mm, L=6.0m","본",10533,74741,14567,99841,"합계"]
["CGC22000150S",null,"강관 부설","Ø150mm, L=6.0m","본",10847,75686,15002,101535,"합계"]
["CGC22000200S",null,"강관 부설","Ø200mm, L=6.0m","본",11319,81966,15654,108939,"합계"]
["CGC22010080S",null,"강관 부설 / 인력","Ø80mm, L=6.0m","본",0,84586,0,84586,"합계"]
["CGC22010100S",null,"강관 부설 / 인력","Ø100mm, L=6.0m","본",0,105124,0,105124,"합계"]
["CGC22010125S",null,"강관 부설 / 인력","Ø125mm, L=6.0m","본",0,132958,0,132958,"합계"]
["CGC22010150S",null,"강관 부설 / 인력","Ø150mm, L=6.0m","본",0,160792,0,160792,"합계"]
["CGC22010200S",null,"강관 부설 / 인력","Ø200mm, L=6.0m","본",0,218012,0,218012,"합계"]
["CGC22010250S",null,"강관 부설 / 인력","Ø250mm, L=6.0m","본",0,275231,0,275231,"합계"]
["CGC23120100S",null,"강관접합 / A종 / 벨엔드용접","Ø100mm 이하","개소",1097,24047,362,25506,"합계"]
["CGC23120125S",null,"강관접합 / A종 / 벨엔드용접","Ø125mm","개소",1234,27053,408,28695,"합계"]
["CGC23120150S",null,"강관접합 / A종 / 벨엔드용접","Ø150mm","개소",1372,27388,453,29213,"합계"]
["CGC23120200S",null,"강관접합 / A종 / 벨엔드용접","Ø200mm","개소",1646,33400,544,35590,"합계"]
["CGC23130100S",null,"강관접합 / A종 / 베벨엔드용접","Ø100mm 이하","개소",1234,27053,408,28695,"합계"]
["CGC23130125S",null,"강관접합 / A종 / 베벨엔드용접","Ø125mm","개소",1372,30059,453,31884,"합계"]
["CGC23130150S",null,"강관접합 / A종 / 베벨엔드용접","Ø150mm","개소",1509,30394,498,32401,"합계"]
["CGC23130200S",null,"강관접합 / A종 / 베벨엔드용접","Ø200mm","개소",1921,36742,634,39297,"합계"]
["CGC25100080S",null,"강관 절단 / A종","Ø80mm","개소",427,21361,0,21788,"합계"]
["CGC25100100S",null,"강관 절단 / A종","Ø100mm","개소",427,21361,0,21788,"합계"]
["CGC25100125S",null,"강관 절단 / A종","Ø125mm","개소",480,24031,0,24511,"합계"]
["CGC25100150S",null,"강관 절단 / A종","Ø150mm","개소",534,26702,0,27236,"합계"]
["CGC25100200S",null,"강관 절단 / A종","Ø200mm","개소",694,34712,0,35406,"합계"]
["CGC31000250S",null,"파형강관 부설 및 접합","Ø250mm, L:6m","개소",1194,18705,1199,21098,"합계"]
["CGC31000300S",null,"파형강관 부설 및 접합","Ø300mm, L:6m","개소",1403,25696,1299,28398,"합계"]
["CGC31000400S",null,"파형강관 부설 및 접합","Ø400mm, L:6m","개소",1897,40150,1599,43646,"합계"]
["CGC32000250S",null,"강관 부설","Ø250mm, L=6.0m","본",11947,90374,16524,118845,"합계"]
["CGC32000300S",null,"강관 부설","Ø300mm, L=6.0m","본",12576,99558,17394,129528,"합계"]
["CGC32000350S",null,"강관 부설","Ø350mm, L=6.0m","본",13205,107967,18264,139436,"합계"]
["CGC32000400S",null,"강관 부설","Ø400mm, L=6.0m","본",13834,118806,19133,151773,"합계"]
["CGC33120250S",null,"강관접합 / A종 / 벨엔드용접","Ø250mm","개소",1921,39412,634,41967,"합계"]
["CGC33120300S",null,"강관접합 / A종 / 벨엔드용접","Ø300mm","개소",2332,45760,770,48862,"합계"]
["CGC33120350S",null,"강관접합 / A종 / 벨엔드용접","Ø350mm","개소",2744,54777,906,58427,"합계"]
["CGC33120400S",null,"강관접합 / A종 / 벨엔드용접","Ø400mm","개소",3293,64131,1088,68512,"합계"]
["CGC33130250S",null,"강관접합 / A종 / 베벨엔드용접","Ø250mm","개소",2195,42754,725,45674,"합계"]
["CGC33130300S",null,"강관접합 / A종 / 베벨엔드용접","Ø300mm","개소",2607,51771,861,55239,"합계"]
["CGC33130350S",null,"강관접합 / A종 / 베벨엔드용접","Ø350mm","개소",3156,61125,1042,65323,"합계"]
["CGC33130400S",null,"강관접합 / A종 / 베벨엔드용접","Ø400mm","개소",3704,70478,1224,75406,"합계"]
["CGC34400300S",null,"강관 외부도장","Ø300mm","개소",0,51761,0,51761,"합계"]
["CGC34400350S",null,"강관 외부도장","Ø350mm","개소",0,60940,0,60940,"합계"]
["CGC34400400S",null,"강관 외부도장","Ø400mm","개소",0,67611,0,67611,"합계"]
["CGC35100250S",null,"강관 절단 / A종","Ø250mm","개소",854,42723,0,43577,"합계"]
["CGC35100300S",null,"강관 절단 / A종","Ø300mm","개소",1068,53404,0,54472,"합계"]
["CGC35100350S",null,"강관 절단 / A종","Ø350mm","개소",1388,69425,0,70813,"합계"]
["CGC35100400S",null,"강관 절단 / A종","Ø400mm","개소",1655,82776,0,84431,"합계"]
["CGC41000450S",null,"파형강관 부설 및 접합","Ø450mm, L:6m","개소",2105,47142,1698,50945,"합계"]
["CGC41000500S",null,"파형강관 부설 및 접합","Ø500mm, L:6m","개소",2265,51701,1798,55764,"합계"]
["CGC41000600S",null,"파형강관 부설 및 접합","Ø600mm, L:6m","개소",2648,64028,1998,68674,"합계"]
["CGC41000700S",null,"파형강관 부설 및 접합","Ø700mm, L:6m","개소",3142,78482,2298,83922,"합계"]
["CGC42000450S",null,"강관 부설","Ø450mm, L=6.0m","본",14620,130118,20220,164958,"합계"]
["CGC42000500S",null,"강관 부설","Ø500mm, L=6.0m","본",15249,139303,21090,175642,"합계"]
["CGC42000600S",null,"강관 부설","Ø600mm, L=6.0m","본",16978,171349,23482,211809,"합계"]
["CGC42000700S",null,"강관 부설","Ø700mm, L=6.0m","본",18707,204172,25874,248753,"합계"]
["CGC43120450S",null,"강관접합 / A종 / 벨엔드용접","Ø450mm","개소",3979,76490,1314,81783,"합계"]
["CGC43120500S",null,"강관접합 / A종 / 벨엔드용접","Ø500mm","개소",4802,91856,1586,98244,"합계"]
["CGC43120600S",null,"강관접합 / A종 / 벨엔드용접","Ø600mm","개소",6998,129270,2312,138580,"합계"]
["CGC43120700S",null,"강관접합 / A종 / 벨엔드용접","Ø700mm","개소",10154,179714,3355,193223,"합계"]
["CGC43130450S",null,"강관접합 / A종 / 베벨엔드용접","Ø450mm","개소",4528,85844,1496,91868,"합계"]
["CGC43130500S",null,"강관접합 / A종 / 베벨엔드용접","Ø500mm","개소",5351,101209,1768,108328,"합계"]
["CGC43130600S",null,"강관접합 / A종 / 베벨엔드용접","Ø600mm","개소",7958,142300,2629,152887,"합계"]
["CGC43130700S",null,"강관접합 / A종 / 베벨엔드용접","Ø700mm","개소",11526,199093,3808,214427,"합계"]
["CGC44400450S",null,"강관 외부도장","Ø450mm","개소",0,72626,0,72626,"합계"]
["CGC44400500S",null,"강관 외부도장","Ø500mm","개소",0,79297,0,79297,"합계"]
["CGC44400600S",null,"강관 외부도장","Ø600mm","개소",0,86820,0,86820,"합계"]
["CGC44400700S",null,"강관 외부도장","Ø700mm","개소",0,93491,0,93491,"합계"]
["CGC45100450S",null,"강관 절단 / A종","Ø450mm","개소",1922,96127,0,98049,"합계"]
["CGC45100500S",null,"강관 절단 / A종","Ø500mm","개소",2189,109478,0,111667,"합계"]
["CGC45100600S",null,"강관 절단 / A종","Ø600mm","개소",2456,122829,0,125285,"합계"]
["CGC45100700S",null,"강관 절단 / A종","Ø700mm","개소",3311,165553,0,168864,"합계"]
["CGC45200700S",null,"강관 절단 / B종","Ø700mm","개소",2883,144191,0,147074,"합계"]
["CGC51000800S",null,"파형강관 부설 및 접합","Ø800mm, L:6m","개소",3510,90033,2498,96041,"합계"]
["CGC51001000S",null,"파형강관 부설 및 접합","Ø1000mm, L:6m","개소",4421,118470,2998,125889,"합계"]
["CGC51011080S",null,"강관압입추진공 - 보통토사","Ø800mm, 추진연장 : 0∼30m","M",116813,548997,185224,851034,"합계"]
["CGC51011090S",null,"강관압입추진공 - 보통토사","Ø900mm, 추진연장 : 0∼30m","M",120707,567297,191398,879402,"합계"]
["CGC51011100S",null,"강관압입추진공 - 보통토사","Ø1000mm, 추진연장 : 0∼30m","M",128495,603896,203747,936138,"합계"]
["CGC51011110S",null,"강관압입추진공 - 보통토사","Ø1100mm, 추진연장 : 0∼30m","M",132388,622196,222085,976669,"합계"]
["CGC51011120S",null,"강관압입추진공 - 보통토사","Ø1200mm, 추진연장 : 0∼30m","M",140176,658796,235149,1034121,"합계"]
["CGC51011135S",null,"강관압입추진공 - 보통토사","Ø1350mm, 추진연장 : 0∼30m","M",147964,695396,256147,1099507,"합계"]
["CGC51011150S",null,"강관압입추진공 - 보통토사","Ø1500mm, 추진연장 : 0∼30m","M",163539,768596,283110,1215245,"합계"]
["CGC51011165S",null,"강관압입추진공 - 보통토사","Ø1650mm, 추진연장 : 0∼30m","M",175220,823495,326192,1324907,"합계"]
["CGC51011180S",null,"강관압입추진공 - 보통토사","Ø1800mm, 추진연장 : 0∼30m","M",194689,914995,362436,1472120,"합계"]
["CGC51011200S",null,"강관압입추진공 - 보통토사","Ø2000mm, 추진연장 : 0∼30m","M",224432,1237464,444456,1906352,"합계"]
["CGC51011220S",null,"강관압입추진공 - 보통토사","Ø2200mm, 추진연장 : 0∼30m","M",236455,1303757,468266,2008478,"합계"]
["CGC51011240S",null,"강관압입추진공 - 보통토사","Ø2400mm, 추진연장 : 0∼30m","M",244039,1556539,468266,2268844,"합계"]
["CGC51011260S",null,"강관압입추진공 - 보통토사","Ø2600mm, 추진연장 : 0∼30m","M",260584,1662067,500013,2422664,"합계"]
["CGC51011280S",null,"강관압입추진공 - 보통토사","Ø2800mm, 추진연장 : 0∼30m","M",293674,1873123,563507,2730304,"합계"]
["CGC51011300S",null,"강관압입추진공 - 보통토사","Ø3000mm, 추진연장 : 0∼30m","M",293674,1873123,563507,2730304,"합계"]
["CGC51012080S",null,"강관압입추진공 - 보통토사","Ø800mm, 추진연장 : 30∼70m","M",124601,585597,197573,907771,"합계"]
["CGC51012090S",null,"강관압입추진공 - 보통토사","Ø900mm, 추진연장 : 30∼70m","M",132388,622196,209921,964505,"합계"]
["CGC51012100S",null,"강관압입추진공 - 보통토사","Ø1000mm, 추진연장 : 30∼70m","M",140176,658796,222269,1021241,"합계"]
["CGC51012110S",null,"강관압입추진공 - 보통토사","Ø1100mm, 추진연장 : 30∼70m","M",144070,677096,241681,1062847,"합계"]
["CGC51012120S",null,"강관압입추진공 - 보통토사","Ø1200mm, 추진연장 : 30∼70m","M",147964,695396,248212,1091572,"합계"]
["CGC51012135S",null,"강관압입추진공 - 보통토사","Ø1350mm, 추진연장 : 30∼70m","M",167433,786896,289850,1244179,"합계"]
["CGC51012150S",null,"강관압입추진공 - 보통토사","Ø1500mm, 추진연장 : 30∼70m","M",175220,823495,303332,1302047,"합계"]
["CGC51012165S",null,"강관압입추진공 - 보통토사","Ø1650mm, 추진연장 : 30∼70m","M",194689,914995,362436,1472120,"합계"]
["CGC51012180S",null,"강관압입추진공 - 보통토사","Ø1800mm, 추진연장 : 30∼70m","M",218052,1024794,405928,1648774,"합계"]
["CGC51012200S",null,"강관압입추진공 - 보통토사","Ø2000mm, 추진연장 : 30∼70m","M",236455,1303757,468266,2008478,"합계"]
["CGC51012220S",null,"강관압입추진공 - 보통토사","Ø2200mm, 추진연장 : 30∼70m","M",252486,1392147,500013,2144646,"합계"]
["CGC51012240S",null,"강관압입추진공 - 보통토사","Ø2400mm, 추진연장 : 30∼70m","M",260584,1662067,500013,2422664,"합계"]
["CGC51012260S",null,"강관압입추진공 - 보통토사","Ø2600mm, 추진연장 : 30∼70m","M",293674,1873123,563507,2730304,"합계"]
["CGC51012280S",null,"강관압입추진공 - 보통토사","Ø2800mm, 추진연장 : 30∼70m","M",318491,2031415,611127,2961033,"합계"]
["CGC51012300S",null,"강관압입추진공 - 보통토사","Ø3000mm, 추진연장 : 30∼70m","M",318491,2031415,611127,2961033,"합계"]
["CGC51013080S",null,"강관압입추진공 - 보통토사","Ø800mm, 추진연장 : 70∼100m","M",132388,622196,209921,964505,"합계"]
["CGC51013090S",null,"강관압입추진공 - 보통토사","Ø900mm, 추진연장 : 70∼100m","M",144070,677096,228443,1049609,"합계"]
["CGC51013100S",null,"강관압입추진공 - 보통토사","Ø1000mm, 추진연장 : 70∼100m","M",147964,695396,234618,1077978,"합계"]
["CGC51013110S",null,"강관압입추진공 - 보통토사","Ø1100mm, 추진연장 : 70∼100m","M",163539,768596,274340,1206475,"합계"]
["CGC51013120S",null,"강관압입추진공 - 보통토사","Ø1200mm, 추진연장 : 70∼100m","M",167433,786896,280872,1235201,"합계"]
["CGC51013135S",null,"강관압입추진공 - 보통토사","Ø1350mm, 추진연장 : 70∼100m","M",186901,878395,323554,1388850,"합계"]
["CGC51013150S",null,"강관압입추진공 - 보통토사","Ø1500mm, 추진연장 : 70∼100m","M",194689,914995,337036,1446720,"합계"]
["CGC51013165S",null,"강관압입추진공 - 보통토사","Ø1650mm, 추진연장 : 70∼100m","M",218052,1024794,405928,1648774,"합계"]
["CGC51013180S",null,"강관압입추진공 - 보통토사","Ø1800mm, 추진연장 : 70∼100m","M",229733,1079694,427674,1737101,"합계"]
["CGC51013200S",null,"강관압입추진공 - 보통토사","Ø2000mm, 추진연장 : 70∼100m","M",252486,1392147,500013,2144646,"합계"]
["CGC51013220S",null,"강관압입추진공 - 보통토사","Ø2200mm, 추진연장 : 70∼100m","M",284548,1568928,563507,2416983,"합계"]
["CGC51013240S",null,"강관압입추진공 - 보통토사","Ø2400mm, 추진연장 : 70∼100m","M",293674,1873123,563507,2730304,"합계"]
["CGC51013260S",null,"강관압입추진공 - 보통토사","Ø2600mm, 추진연장 : 70∼100m","M",318491,2031415,611127,2961033,"합계"]
["CGC51013280S",null,"강관압입추진공 - 보통토사","Ø2800mm, 추진연장 : 70∼100m","M",343309,2189707,658747,3191763,"합계"]
["CGC51013300S",null,"강관압입추진공 - 보통토사","Ø3000mm, 추진연장 : 70∼100m","M",343309,2189707,658747,3191763,"합계"]
["CGC51021080S",null,"강관압입추진공 - 경질토사","Ø800mm, 추진연장 : 0∼30m","M",140176,658796,222269,1021241,"합계"]
["CGC51021090S",null,"강관압입추진공 - 경질토사","Ø900mm, 추진연장 : 0∼30m","M",144070,677096,228443,1049609,"합계"]
["CGC51021100S",null,"강관압입추진공 - 경질토사","Ø1000mm, 추진연장 : 0∼30m","M",147964,695396,234618,1077978,"합계"]
["CGC51021110S",null,"강관압입추진공 - 경질토사","Ø1100mm, 추진연장 : 0∼30m","M",163539,768596,274340,1206475,"합계"]
["CGC51021120S",null,"강관압입추진공 - 경질토사","Ø1200mm, 추진연장 : 0∼30m","M",167433,786896,280872,1235201,"합계"]
["CGC51021135S",null,"강관압입추진공 - 경질토사","Ø1350mm, 추진연장 : 0∼30m","M",186901,878395,323554,1388850,"합계"]
["CGC51021150S",null,"강관압입추진공 - 경질토사","Ø1500mm, 추진연장 : 0∼30m","M",194689,914995,337036,1446720,"합계"]
["CGC51021165S",null,"강관압입추진공 - 경질토사","Ø1650mm, 추진연장 : 0∼30m","M",206370,969895,384182,1560447,"합계"]
["CGC51021180S",null,"강관압입추진공 - 경질토사","Ø1800mm, 추진연장 : 0∼30m","M",229733,1079694,427674,1737101,"합계"]
["CGC51021200S",null,"강관압입추진공 - 경질토사","Ø2000mm, 추진연장 : 0∼30m","M",284548,1568928,563507,2416983,"합계"]
["CGC51021220S",null,"강관압입추진공 - 경질토사","Ø2200mm, 추진연장 : 0∼30m","M",284548,1568928,563507,2416983,"합계"]
["CGC51021240S",null,"강관압입추진공 - 경질토사","Ø2400mm, 추진연장 : 0∼30m","M",293674,1873123,563507,2730304,"합계"]
["CGC51021260S",null,"강관압입추진공 - 경질토사","Ø2600mm, 추진연장 : 0∼30m","M",318491,2031415,611127,2961033,"합계"]
["CGC51021280S",null,"강관압입추진공 - 경질토사","Ø2800mm, 추진연장 : 0∼30m","M",343309,2189707,658747,3191763,"합계"]
["CGC51021300S",null,"강관압입추진공 - 경질토사","Ø3000mm, 추진연장 : 0∼30m","M",343309,2189707,658747,3191763,"합계"]
["CGC51022080S",null,"강관압입추진공 - 경질토사","Ø800mm, 추진연장 : 30∼70m","M",147964,695396,234618,1077978,"합계"]
["CGC51022090S",null,"강관압입추진공 - 경질토사","Ø900mm, 추진연장 : 30∼70m","M",163539,768596,259314,1191449,"합계"]
["CGC51022100S",null,"강관압입추진공 - 경질토사","Ø1000mm, 추진연장 : 30∼70m","M",167433,786896,265488,1219817,"합계"]
["CGC51022110S",null,"강관압입추진공 - 경질토사","Ø1100mm, 추진연장 : 30∼70m","M",175220,823495,293936,1292651,"합계"]
["CGC51022120S",null,"강관압입추진공 - 경질토사","Ø1200mm, 추진연장 : 30∼70m","M",186901,878395,313532,1378828,"합계"]
["CGC51022135S",null,"강관압입추진공 - 경질토사","Ø1350mm, 추진연장 : 30∼70m","M",194689,914995,337036,1446720,"합계"]
["CGC51022150S",null,"강관압입추진공 - 경질토사","Ø1500mm, 추진연장 : 30∼70m","M",206370,969895,357258,1533523,"합계"]
["CGC51022165S",null,"강관압입추진공 - 경질토사","Ø1650mm, 추진연장 : 30∼70m","M",229733,1079694,427674,1737101,"합계"]
["CGC51022180S",null,"강관압입추진공 - 경질토사","Ø1800mm, 추진연장 : 30∼70m","M",276459,1299293,514659,2090411,"합계"]
["CGC51022200S",null,"강관압입추진공 - 경질토사","Ø2000mm, 추진연장 : 30∼70m","M",284548,1568928,563507,2416983,"합계"]
["CGC51022220S",null,"강관압입추진공 - 경질토사","Ø2200mm, 추진연장 : 30∼70m","M",308594,1701513,611127,2621234,"합계"]
["CGC51022240S",null,"강관압입추진공 - 경질토사","Ø2400mm, 추진연장 : 30∼70m","M",318491,2031415,611127,2961033,"합계"]
["CGC51022260S",null,"강관압입추진공 - 경질토사","Ø2600mm, 추진연장 : 30∼70m","M",343309,2189707,658747,3191763,"합계"]
["CGC51022280S",null,"강관압입추진공 - 경질토사","Ø2800mm, 추진연장 : 30∼70m","M",376399,2400763,722241,3499403,"합계"]
["CGC51022300S",null,"강관압입추진공 - 경질토사","Ø3000mm, 추진연장 : 30∼70m","M",376399,2400763,722241,3499403,"합계"]
["CGC51023080S",null,"강관압입추진공 - 경질토사","Ø800mm, 추진연장 : 70∼100m","M",163539,768596,259314,1191449,"합계"]
["CGC51023090S",null,"강관압입추진공 - 경질토사","Ø900mm, 추진연장 : 70∼100m","M",175220,823495,277837,1276552,"합계"]
["CGC51023100S",null,"강관압입추진공 - 경질토사","Ø1000mm, 추진연장 : 70∼100m","M",186901,878395,296359,1361655,"합계"]
["CGC51023110S",null,"강관압입추진공 - 경질토사","Ø1100mm, 추진연장 : 70∼100m","M",194689,914995,326596,1436280,"합계"]
["CGC51023120S",null,"강관압입추진공 - 경질토사","Ø1200mm, 추진연장 : 70∼100m","M",194689,914995,326596,1436280,"합계"]
["CGC51023135S",null,"강관압입추진공 - 경질토사","Ø1350mm, 추진연장 : 70∼100m","M",218052,1024794,377480,1620326,"합계"]
["CGC51023150S",null,"강관압입추진공 - 경질토사","Ø1500mm, 추진연장 : 70∼100m","M",229733,1079694,397702,1707129,"합계"]
["CGC51023165S",null,"강관압입추진공 - 경질토사","Ø1650mm, 추진연장 : 70∼100m","M",276459,1299293,514659,2090411,"합계"]
["CGC51023180S",null,"강관압입추진공 - 경질토사","Ø1800mm, 추진연장 : 70∼100m","M",276459,1299293,514659,2090411,"합계"]
["CGC51023200S",null,"강관압입추진공 - 경질토사","Ø2000mm, 추진연장 : 70∼100m","M",308594,1701513,611127,2621234,"합계"]
["CGC51023220S",null,"강관압입추진공 - 경질토사","Ø2200mm, 추진연장 : 70∼100m","M",332640,1834099,658747,2825486,"합계"]
["CGC51023240S",null,"강관압입추진공 - 경질토사","Ø2400mm, 추진연장 : 70∼100m","M",343309,2189707,658747,3191763,"합계"]
["CGC51023260S",null,"강관압입추진공 - 경질토사","Ø2600mm, 추진연장 : 70∼100m","M",376399,2400763,722241,3499403,"합계"]
["CGC51023280S",null,"강관압입추진공 - 경질토사","Ø2800mm, 추진연장 : 70∼100m","M",413625,2638202,793672,3845499,"합계"]
["CGC51023300S",null,"강관압입추진공 - 경질토사","Ø3000mm, 추진연장 : 70∼100m","M",413625,2638202,793672,3845499,"합계"]
["CGC51031080S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø800mm, 추진연장 : 0∼30m","M",147964,695396,234618,1077978,"합계"]
["CGC51031090S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø900mm, 추진연장 : 0∼30m","M",163539,768596,259314,1191449,"합계"]
["CGC51031100S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø1000mm, 추진연장 : 0∼30m","M",167433,786896,265488,1219817,"합계"]
["CGC51031110S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø1100mm, 추진연장 : 0∼30m","M",175220,823495,293936,1292651,"합계"]
["CGC51031120S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø1200mm, 추진연장 : 0∼30m","M",186901,878395,313532,1378828,"합계"]
["CGC51031135S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø1350mm, 추진연장 : 0∼30m","M",194689,914995,337036,1446720,"합계"]
["CGC51031150S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø1500mm, 추진연장 : 0∼30m","M",206370,969895,357258,1533523,"합계"]
["CGC51031165S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø1650mm, 추진연장 : 0∼30m","M",229733,1079694,427674,1737101,"합계"]
["CGC51031180S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø1800mm, 추진연장 : 0∼30m","M",245308,1152894,456669,1854871,"합계"]
["CGC51031200S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø2000mm, 추진연장 : 0∼30m","M",308594,1701513,611127,2621234,"합계"]
["CGC51031220S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø2200mm, 추진연장 : 0∼30m","M",308594,1701513,611127,2621234,"합계"]
["CGC51031240S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø2400mm, 추진연장 : 0∼30m","M",318491,2031415,611127,2961033,"합계"]
["CGC51031260S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø2600mm, 추진연장 : 0∼30m","M",343309,2189707,658747,3191763,"합계"]
["CGC51031280S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø2800mm, 추진연장 : 0∼30m","M",376399,2400763,722241,3499403,"합계"]
["CGC51031300S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø3000mm, 추진연장 : 0∼30m","M",376399,2400763,722241,3499403,"합계"]
["CGC51032080S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø800mm, 추진연장 : 30∼70m","M",163539,768596,259314,1191449,"합계"]
["CGC51032090S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø900mm, 추진연장 : 30∼70m","M",175220,823495,277837,1276552,"합계"]
["CGC51032100S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø1000mm, 추진연장 : 30∼70m","M",186901,878395,296359,1361655,"합계"]
["CGC51032110S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø1100mm, 추진연장 : 30∼70m","M",194689,914995,326596,1436280,"합계"]
["CGC51032120S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø1200mm, 추진연장 : 30∼70m","M",194689,914995,337036,1446720,"합계"]
["CGC51032135S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø1350mm, 추진연장 : 30∼70m","M",218052,1024794,377480,1620326,"합계"]
["CGC51032150S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø1500mm, 추진연장 : 30∼70m","M",229733,1079694,397702,1707129,"합계"]
["CGC51032165S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø1650mm, 추진연장 : 30∼70m","M",245308,1152894,456669,1854871,"합계"]
["CGC51032180S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø1800mm, 추진연장 : 30∼70m","M",299821,1409093,558151,2267065,"합계"]
["CGC51032200S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø2000mm, 추진연장 : 30∼70m","M",308594,1701513,611127,2621234,"합계"]
["CGC51032220S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø2200mm, 추진연장 : 30∼70m","M",332640,1834099,658747,2825486,"합계"]
["CGC51032240S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø2400mm, 추진연장 : 30∼70m","M",343309,2189707,658747,3191763,"합계"]
["CGC51032260S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø2600mm, 추진연장 : 30∼70m","M",376399,2400763,722241,3499403,"합계"]
["CGC51032280S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø2800mm, 추진연장 : 30∼70m","M",413625,2638202,793672,3845499,"합계"]
["CGC51032300S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø3000mm, 추진연장 : 30∼70m","M",413625,2638202,793672,3845499,"합계"]
["CGC51033080S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø800mm, 추진연장 : 70∼100m","M",175220,823495,277837,1276552,"합계"]
["CGC51033090S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø900mm, 추진연장 : 70∼100m","M",194689,914995,308708,1418392,"합계"]
["CGC51033100S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø1000mm, 추진연장 : 70∼100m","M",194689,914995,308708,1418392,"합계"]
["CGC51033110S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø1100mm, 추진연장 : 70∼100m","M",206370,969895,346191,1522456,"합계"]
["CGC51033120S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø1200mm, 추진연장 : 70∼100m","M",218052,1024794,365787,1608633,"합계"]
["CGC51033135S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø1350mm, 추진연장 : 70∼100m","M",229733,1079694,397702,1707129,"합계"]
["CGC51033150S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø1500mm, 추진연장 : 70∼100m","M",245308,1152894,424665,1822867,"합계"]
["CGC51033165S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø1650mm, 추진연장 : 70∼100m","M",299821,1409093,558151,2267065,"합계"]
["CGC51033180S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø1800mm, 추진연장 : 70∼100m","M",299821,1409093,558151,2267065,"합계"]
["CGC51033200S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø2000mm, 추진연장 : 70∼100m","M",332640,1834099,658747,2825486,"합계"]
["CGC51033220S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø2200mm, 추진연장 : 70∼100m","M",364702,2010879,722241,3097822,"합계"]
["CGC51033240S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø2400mm, 추진연장 : 70∼100m","M",376399,2400763,722241,3499403,"합계"]
["CGC51033260S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø2600mm, 추진연장 : 70∼100m","M",413625,2638202,793672,3845499,"합계"]
["CGC51033280S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø2800mm, 추진연장 : 70∼100m","M",459124,2928404,880975,4268503,"합계"]
["CGC51033300S",null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø3000mm, 추진연장 : 70∼100m","M",459124,2928404,880975,4268503,"합계"]
["CGC51100090S",null,"강관압입추진공 / 장비 조립 및 해체","Ø800∼900mm","회",201480,2397744,337512,2936736,"합계"]
["CGC51200110S",null,"강관압입추진공 / 작업편성인원","Ø800∼1100mm","일당",0,1183575,0,1183575,"합계"]
["CGC51300100S",null,"강관압입추진공 / 작업편성장비","Ø800∼1000mm","일당",353872,646416,617416,1617704,"합계"]
["CGC52000800S",null,"강관 부설","Ø800mm, L=6.0m","본",20594,246419,28483,295496,"합계"]
["CGC52000900S",null,"강관 부설","Ø900mm, L=6.0m","본",22795,296128,31527,350450,"합계"]
["CGC52001000S",null,"강관 부설","Ø1000mm, L=6.0m","본",27199,376537,45564,449300,"합계"]
["CGC52001100S",null,"강관 부설","Ø1100mm, L=6.0m","본",30222,480960,50626,561808,"합계"]
["CGC53120800S",null,"강관접합 / A종 / 벨엔드용접","Ø800mm","개소",22778,357461,7526,387765,"합계"]
["CGC53120900S",null,"강관접합 / A종 / 벨엔드용접","Ø900mm","개소",29776,462699,9838,502313,"합계"]
["CGC53121100S",null,"강관접합 / A종 / 벨엔드용접","Ø1000mm","개소",36088,558248,11924,606260,"합계"]
["CGC53121110S",null,"강관접합 / A종 / 벨엔드용접","Ø1100mm","개소",41852,644444,13828,700124,"합계"]
["CGC53220800S",null,"강관접합 / B종 / 벨엔드용접","Ø800mm","개소",15505,246211,5123,266839,"합계"]
["CGC53220900S",null,"강관접합 / B종 / 벨엔드용접","Ø900mm","개소",20308,319376,6710,346394,"합계"]
["CGC53221000S",null,"강관접합 / B종 / 벨엔드용접","Ø1000mm","개소",24562,385857,8115,418534,"합계"]
["CGC53221100S",null,"강관접합 / B종 / 벨엔드용접","Ø1100mm","개소",28541,446327,9430,484298,"합계"]
["CGC54300800S",null,"강관 내부도장","Ø800mm","개소",0,79297,0,79297,"합계"]
["CGC54300900S",null,"강관 내부도장","Ø900mm","개소",0,81805,0,81805,"합계"]
["CGC54301000S",null,"강관 내부도장","Ø1000mm","개소",0,86820,0,86820,"합계"]
["CGC54301100S",null,"강관 내부도장","Ø1100mm","개소",0,90984,0,90984,"합계"]
["CGC54400800S",null,"강관 외부도장","Ø800mm","개소",0,98507,0,98507,"합계"]
["CGC54400900S",null,"강관 외부도장","Ø900mm","개소",0,105178,0,105178,"합계"]
["CGC54401000S",null,"강관 외부도장","Ø1000mm","개소",0,110193,0,110193,"합계"]
["CGC54401100S",null,"강관 외부도장","Ø1100mm","개소",0,116864,0,116864,"합계"]
["CGC55100800S",null,"강관 절단 / A종","Ø800mm","개소",3791,189584,0,193375,"합계"]
["CGC55100900S",null,"강관 절단 / A종","Ø900mm","개소",4218,210946,0,215164,"합계"]
["CGC55101000S",null,"강관 절단 / A종","Ø1000mm","개소",5126,256340,0,261466,"합계"]
["CGC55101100S",null,"강관 절단 / A종","Ø1100mm","개소",5554,277701,0,283255,"합계"]
["CGC55200800S",null,"강관 절단 / B종","Ø800mm","개소",3471,173563,0,177034,"합계"]
["CGC55200900S",null,"강관 절단 / B종","Ø900mm","개소",3738,186914,0,190652,"합계"]
["CGC55201000S",null,"강관 절단 / B종","Ø1000mm","개소",4539,226967,0,231506,"합계"]
["CGC55201100S",null,"강관 절단 / B종","Ø1100mm","개소",4646,232308,0,236954,"합계"]
["CGC61001200S",null,"파형강관 부설 및 접합","Ø1200mm, L:6m","개소",5250,142819,3497,151566,"합계"]
["CGC61001500S",null,"파형강관 부설 및 접합","Ø1500mm, L:6m","개소",6606,183279,4297,194182,"합계"]
["CGC61100120S",null,"강관압입추진공 / 장비 조립 및 해체","Ø1000∼1200mm","회",201480,2818452,337512,3357444,"합계"]
["CGC61100165S",null,"강관압입추진공 / 장비 조립 및 해체","Ø1350∼1650mm","회",268640,3757936,450016,4476592,"합계"]
["CGC61200180S",null,"강관압입추진공 / 작업편성인원","Ø1200∼1800mm","일당",0,1183575,0,1183575,"합계"]
["CGC61300120S",null,"강관압입추진공 / 작업편성장비","Ø1100∼1200mm","일당",353872,646416,653192,1653480,"합계"]
["CGC61300150S",null,"강관압입추진공 / 작업편성장비","Ø1350∼1500mm","일당",353872,646416,674072,1674360,"합계"]
["CGC62001200S",null,"강관 부설","Ø1200mm, L=6.0m","본",32740,576670,54845,664255,"합계"]
["CGC62001350S",null,"강관 부설","Ø1350mm, L=6.0m","본",36434,705746,61033,803213,"합계"]
["CGC62001500S",null,"강관 부설","Ø1500mm, L=6.0m","본",39624,821246,66377,927247,"합계"]
["CGC62001650S",null,"강관 부설","Ø1650mm, L=6.0m","본",42478,925196,71158,1038832,"합계"]
["CGC63121200S",null,"강관접합 / A종 / 벨엔드용접","Ø1200mm","개소",47066,723956,15551,786573,"합계"]
["CGC63121350S",null,"강관접합 / A종 / 벨엔드용접","Ø1350mm","개소",54064,831864,17863,903791,"합계"]
["CGC63121500S",null,"강관접합 / A종 / 벨엔드용접","Ø1500mm","개소",60376,927413,19949,1007738,"합계"]
["CGC63121650S",null,"강관접합 / A종 / 벨엔드용접","Ø1650mm","개소",66140,1013609,21853,1101602,"합계"]
["CGC63221200S",null,"강관접합 / B종 / 벨엔드용접","Ø1200mm","개소",32109,500449,10609,543167,"합계"]
["CGC63221350S",null,"강관접합 / B종 / 벨엔드용접","Ø1350mm","개소",36774,575948,12151,624873,"합계"]
["CGC63221500S",null,"강관접합 / B종 / 벨엔드용접","Ø1500mm","개소",41166,642765,13602,697533,"합계"]
["CGC63221650S",null,"강관접합 / B종 / 벨엔드용접","Ø1650mm","개소",45008,702899,14871,762778,"합계"]
["CGC64301200S",null,"강관 내부도장","Ø1200mm","개소",0,93491,0,93491,"합계"]
["CGC64301350S",null,"강관 내부도장","Ø1350mm","개소",0,95999,0,95999,"합계"]
["CGC64301500S",null,"강관 내부도장","Ø1500mm","개소",0,102670,0,102670,"합계"]
["CGC64301650S",null,"강관 내부도장","Ø1650mm","개소",0,105178,0,105178,"합계"]
["CGC64401200S",null,"강관 외부도장","Ø1200mm","개소",0,119372,0,119372,"합계"]
["CGC64401350S",null,"강관 외부도장","Ø1350mm","개소",0,126043,0,126043,"합계"]
["CGC64401500S",null,"강관 외부도장","Ø1500mm","개소",0,131059,0,131059,"합계"]
["CGC64401650S",null,"강관 외부도장","Ø1650mm","개소",0,133566,0,133566,"합계"]
["CGC65101200S",null,"강관 절단 / A종","Ø1200mm","개소",6408,320425,0,326833,"합계"]
["CGC65101350S",null,"강관 절단 / A종","Ø1350mm","개소",7850,392520,0,400370,"합계"]
["CGC65101500S",null,"강관 절단 / A종","Ø1500mm","개소",10039,501999,0,512038,"합계"]
["CGC65101650S",null,"강관 절단 / A종","Ø1650mm","개소",11428,571424,0,582852,"합계"]
["CGC65201200S",null,"강관 절단 / B종","Ø1200mm","개소",5287,264350,0,269637,"합계"]
["CGC65201350S",null,"강관 절단 / B종","Ø1350mm","개소",6568,328435,0,335003,"합계"]
["CGC65201500S",null,"강관 절단 / B종","Ø1500mm","개소",7903,395191,0,403094,"합계"]
["CGC65201650S",null,"강관 절단 / B종","Ø1650mm","개소",9132,456605,0,465737,"합계"]
["CGC71100240S",null,"강관압입추진공 / 장비 조립 및 해체","Ø1800∼2400mm","회",268640,3757936,450016,4476592,"합계"]
["CGC71200220S",null,"강관압입추진공 / 작업편성인원","Ø2000∼2200mm","일당",0,1563342,0,1563342,"합계"]
["CGC71300180S",null,"강관압입추진공 / 작업편성장비","Ø1650∼1800mm","일당",353872,646416,724872,1725160,"합계"]
["CGC72001800S",null,"강관 부설","Ø1800mm, L=6.0m","본",44997,1020907,75377,1141281,"합계"]
["CGC72002000S",null,"강관 부설","Ø2000mm, L=6.0m","본",48187,1136407,80721,1265315,"합계"]
["CGC72002200S",null,"강관 부설","Ø2200mm, L=6.0m","본",51209,1240829,85784,1377822,"합계"]
["CGC72002400S",null,"강관 부설","Ø2400mm, L=6.0m","본",53728,1334108,90003,1477839,"합계"]
["CGC73121800S",null,"강관접합 / A종 / 벨엔드용접","Ø1800mm","개소",71354,1090451,23576,1185381,"합계"]
["CGC73122000S",null,"강관접합 / A종 / 벨엔드용접","Ø2000mm","개소",77529,1185664,25617,1288810,"합계"]
["CGC73122200S",null,"강관접합 / A종 / 벨엔드용접","Ø2200mm","개소",83292,1274530,27521,1385343,"합계"]
["CGC73122400S",null,"강관접합 / A종 / 벨엔드용접","Ø2400mm","개소",88506,1351372,29244,1469122,"합계"]
["CGC73221800S",null,"강관접합 / B종 / 벨엔드용접","Ø1800mm","개소",48575,754351,16050,818976,"합계"]
["CGC73222000S",null,"강관접합 / B종 / 벨엔드용접","Ø2000mm","개소",52829,820832,17455,891116,"합계"]
["CGC73222200S",null,"강관접합 / B종 / 벨엔드용접","Ø2200mm","개소",56809,883972,18770,959551,"합계"]
["CGC73222400S",null,"강관접합 / B종 / 벨엔드용접","Ø2400mm","개소",60239,935088,19904,1015231,"합계"]
["CGC74301800S",null,"강관 내부도장","Ø1800mm","개소",0,107686,0,107686,"합계"]
["CGC74302000S",null,"강관 내부도장","Ø2000mm","개소",0,112701,0,112701,"합계"]
["CGC74302200S",null,"강관 내부도장","Ø2200mm","개소",0,116864,0,116864,"합계"]
["CGC74302400S",null,"강관 내부도장","Ø2400mm","개소",0,119372,0,119372,"합계"]
["CGC74401800S",null,"강관 외부도장","Ø1800mm","개소",0,140237,0,140237,"합계"]
["CGC74402000S",null,"강관 외부도장","Ø2000mm","개소",0,142745,0,142745,"합계"]
["CGC74402200S",null,"강관 외부도장","Ø2200mm","개소",0,149416,0,149416,"합계"]
["CGC74402400S",null,"강관 외부도장","Ø2400mm","개소",0,154432,0,154432,"합계"]
["CGC75101800S",null,"강관 절단 / A종","Ø1800mm","개소",12069,603467,0,615536,"합계"]
["CGC75102000S",null,"강관 절단 / A종","Ø2000mm","개소",13618,680903,0,694521,"합계"]
["CGC75102200S",null,"강관 절단 / A종","Ø2200mm","개소",14846,742318,0,757164,"합계"]
["CGC75102400S",null,"강관 절단 / A종","Ø2400mm","개소",16341,817084,0,833425,"합계"]
["CGC75201800S",null,"강관 절단 / B종","Ø1800mm","개소",9826,491318,0,501144,"합계"]
["CGC75202000S",null,"강관 절단 / B종","Ø2000mm","개소",12389,619488,0,631877,"합계"]
["CGC75202200S",null,"강관 절단 / B종","Ø2200mm","개소",12817,640850,0,653667,"합계"]
["CGC75202400S",null,"강관 절단 / B종","Ø2400mm","개소",14205,710275,0,724480,"합계"]
["CGC81100300S",null,"강관압입추진공 / 장비 조립 및 해체","Ø2600∼3000mm","회",335800,4697420,562520,5595740,"합계"]
["CGC81200300S",null,"강관압입추진공 / 작업편성인원","Ø2400∼3000mm","일당",0,1991786,0,1991786,"합계"]
["CGC81300300S",null,"강관압입추진공 / 작업편성장비","Ø2000∼3000mm","일당",353872,646416,793672,1793960,"합계"]
["CGD11000050S",null,"P.V.C.관 T.S 접합 및 부설","Ø50mm","개소",0,19556,0,19556,"합계"]
["CGD11000075S",null,"P.V.C.관 T.S 접합 및 부설","Ø75mm","개소",0,26075,0,26075,"합계"]
["CGD11000100S",null,"P.V.C.관 T.S 접합 및 부설","Ø100mm","개소",0,30162,0,30162,"합계"]
["CGD11000150S",null,"P.V.C.관 T.S 접합 및 부설","Ø150mm","개소",0,51374,0,51374,"합계"]
["CGD12000050S",null,"P.V.C.관 고무링 접합 및 부설","Ø50mm","개소",0,13037,0,13037,"합계"]
["CGD12000075S",null,"P.V.C.관 고무링 접합 및 부설","Ø75mm","개소",0,21988,0,21988,"합계"]
["CGD12000100S",null,"P.V.C.관 고무링 접합 및 부설","Ø100mm","개소",0,26075,0,26075,"합계"]
["CGD12000150S",null,"P.V.C.관 고무링 접합 및 부설","Ø150mm","개소",0,34249,0,34249,"합계"]
["CGD12000200S",null,"P.V.C.관 고무링 접합 및 부설","Ø200mm","개소",0,43199,0,43199,"합계"]
["CGD12000250S",null,"P.V.C.관 고무링 접합 및 부설","Ø250mm","개소",0,62756,0,62756,"합계"]
["CGD12000300S",null,"P.V.C.관 고무링 접합 및 부설","Ø300mm","개소",0,75794,0,75794,"합계"]
["CGE20100150S",null,"유리섬유복합관 부설 및 접합/비압력관","Ø150mm, L=6.0m","본",732,73259,0,73991,"합계"]
["CGE20100200S",null,"유리섬유복합관 부설 및 접합/비압력관","Ø200mm, L=6.0m","본",928,92815,0,93743,"합계"]
["CGE20200150S",null,"유리섬유복합관 부설 및 접합/압력관","Ø150mm, L=6.0m","본",797,79778,0,80575,"합계"]
["CGE20200200S",null,"유리섬유복합관 부설 및 접합/압력관","Ø200mm, L=6.0m","본",1017,101766,0,102783,"합계"]
["CGE30100250S",null,"유리섬유복합관 부설 및 접합/비압력관","Ø250mm, L=6.0m","본",2541,56728,2698,61967,"합계"]
["CGE30100300S",null,"유리섬유복합관 부설 및 접합/비압력관","Ø300mm, L=6.0m","본",2823,63008,2998,68829,"합계"]
["CGE30100350S",null,"유리섬유복합관 부설 및 접합/비압력관","Ø350mm, L=6.0m","본",3200,71416,3397,78013,"합계"]
["CGE30100400S",null,"유리섬유복합관 부설 및 접합/비압력관","Ø400mm, L=6.0m","본",3563,85871,3697,93131,"합계"]
["CGE30200250S",null,"유리섬유복합관 부설 및 접합/압력관","Ø250mm, L=6.0m","본",2823,63008,2998,68829,"합계"]
["CGE30200300S",null,"유리섬유복합관 부설 및 접합/압력관","Ø300mm, L=6.0m","본",3122,70944,3298,77364,"합계"]
["CGE30200350S",null,"유리섬유복합관 부설 및 접합/압력관","Ø350mm, L=6.0m","본",3498,79352,3697,86547,"합계"]
["CGE30200400S",null,"유리섬유복합관 부설 및 접합/압력관","Ø400mm, L=6.0m","본",3923,92624,4097,100644,"합계"]
["CGE40100450S",null,"유리섬유복합관 부설 및 접합/비압력관","Ø450mm, L=6.0m","본",3989,99142,4097,107228,"합계"]
["CGE40100500S",null,"유리섬유복합관 부설 및 접합/비압력관","Ø500mm, L=6.0m","본",4377,116029,4397,124803,"합계"]
["CGE40100600S",null,"유리섬유복합관 부설 및 접합/비압력관","Ø600mm, L=6.0m","본",5207,147842,5096,158145,"합계"]
["CGE40100700S",null,"유리섬유복합관 부설 및 접합/비압력관","Ø700mm, L=6.0m","본",6020,177999,5796,189815,"합계"]
["CGE40200450S",null,"유리섬유복합관 부설 및 접합/압력관","Ø450mm, L=6.0m","본",4365,107550,4497,116412,"합계"]
["CGE40200500S",null,"유리섬유복합관 부설 및 접합/압력관","Ø500mm, L=6.0m","본",4794,128524,4797,138115,"합계"]
["CGE40200600S",null,"유리섬유복합관 부설 및 접합/압력관","Ø600mm, L=6.0m","본",5726,163241,5596,174563,"합계"]
["CGE40200700S",null,"유리섬유복합관 부설 및 접합/압력관","Ø700mm, L=6.0m","본",6618,193871,6396,206885,"합계"]
["CGE50100800S",null,"유리섬유복합관 부설 및 접합/비압력관","Ø800mm, L=6.0m","본",6850,209812,6496,223158,"합계"]
["CGE50100900S",null,"유리섬유복합관 부설 및 접합/비압력관","Ø900mm, L=6.0m","본",7656,239194,7195,254045,"합계"]
["CGE50101000S",null,"유리섬유복합관 부설 및 접합/비압력관","Ø1000mm, L=6.0m","본",14739,269351,17176,301266,"합계"]
["CGE50101100S",null,"유리섬유복합관 부설 및 접합/비압력관","Ø1100mm, L=6.0m","본",16125,301165,18698,335988,"합계"]
["CGE50200800S",null,"유리섬유복합관 부설 및 접합/압력관","Ø800mm, L=6.0m","본",7550,228588,7195,243333,"합계"]
["CGE50200900S",null,"유리섬유복합관 부설 및 접합/압력관","Ø900mm, L=6.0m","본",8404,262833,7895,279132,"합계"]
["CGE50201000S",null,"유리섬유복합관 부설 및 접합/압력관","Ø1000mm, L=6.0m","본",16241,297550,18916,332707,"합계"]
["CGE50201100S",null,"유리섬유복합관 부설 및 접합/압력관","Ø1100mm, L=6.0m","본",17784,329835,20655,368274,"합계"]
["CGE60101200S",null,"유리섬유복합관 부설 및 접합/비압력관","Ø1200mm, L=6.0m","본",18488,331322,26157,375967,"합계"]
["CGE60101350S",null,"유리섬유복합관 부설 및 접합/비압력관","Ø1350mm, L=6.0m","본",20734,376407,29251,426392,"합계"]
["CGE60101500S",null,"유리섬유복합관 부설 및 접합/비압력관","Ø1500mm, L=6.0m","본",22853,425106,32063,480022,"합계"]
["CGE60101650S",null,"유리섬유복합관 부설 및 접합/비압력관","Ø1650mm, L=6.0m","본",25099,470190,35157,530446,"합계"]
["CGE60201200S",null,"유리섬유복합관 부설 및 접합/압력관","Ø1200mm, L=6.0m","본",20309,366512,28688,415509,"합계"]
["CGE60201350S",null,"유리섬유복합관 부설 및 접합/압력관","Ø1350mm, L=6.0m","본",22763,416155,32063,470981,"합계"]
["CGE60201500S",null,"유리섬유복합관 부설 및 접합/압력관","Ø1500mm, L=6.0m","본",25074,467759,35157,527990,"합계"]
["CGE60201650S",null,"유리섬유복합관 부설 및 접합/압력관","Ø1650mm, L=6.0m","본",27680,516220,38813,582713,"합계"]
["CGE70101800S",null,"유리섬유복합관 부설 및 접합/비압력관","Ø1800mm, L=6.0m","본",27193,516458,37970,581621,"합계"]
["CGE70102000S",null,"유리섬유복합관 부설 및 접합/비압력관","Ø2000mm, L=6.0m","본",30097,578429,41907,650433,"합계"]
["CGE70102200S",null,"유리섬유복합관 부설 및 접합/비압력관","Ø2200mm, L=6.0m","본",33748,640400,48063,722211,"합계"]
["CGE70102400S",null,"유리섬유복합관 부설 및 접합/비압력관","Ø2400mm, L=6.0m","본",36716,702370,52191,791277,"합계"]
["CGE70201800S",null,"유리섬유복합관 부설 및 접합/압력관","Ø1800mm, L=6.0m","본",30008,569478,41907,641393,"합계"]
["CGE70202000S",null,"유리섬유복합관 부설 및 접합/압력관","Ø2000mm, L=6.0m","본",33128,636785,46126,716039,"합계"]
["CGE70202200S",null,"유리섬유복합관 부설 및 접합/압력관","Ø2200mm, L=6.0m","본",37061,703315,52781,793157,"합계"]
["CGE70202400S",null,"유리섬유복합관 부설 및 접합/압력관","Ø2400mm, L=6.0m","본",40415,770317,57499,868231,"합계"]
["CGF11000015S",null,"P.E관 조임식 접합 및 부설","Ø15mm","개소",0,16245,0,16245,"합계"]
["CGF11000020S",null,"P.E관 조임식 접합 및 부설","Ø20mm","개소",0,17900,0,17900,"합계"]
["CGF11000025S",null,"P.E관 조임식 접합 및 부설","Ø25mm","개소",0,25196,0,25196,"합계"]
["CGF11000032S",null,"P.E관 조임식 접합 및 부설","Ø32mm","개소",0,29283,0,29283,"합계"]
["CGF11000040S",null,"P.E관 조임식 접합 및 부설","Ø40mm","개소",0,31714,0,31714,"합계"]
["CGF11000050S",null,"P.E관 조임식 접합 및 부설","Ø50mm","개소",0,39009,0,39009,"합계"]
["CGF12000050S",null,"P.E.관 밴드 접합 및 부설","Ø50mm","개소",782,26075,0,26857,"합계"]
["CGF12000075S",null,"P.E.관 밴드 접합 및 부설","Ø75mm","개소",977,32594,0,33571,"합계"]
["CGF13000040S",null,"P.E관 소켓융착 접합 및 부설","Ø40mm","개소",1539,21988,0,23527,"합계"]
["CGF13000050S",null,"P.E관 소켓융착 접합 및 부설","Ø50mm","개소",1995,28506,0,30501,"합계"]
["CGF13000065S",null,"P.E관 소켓융착 접합 및 부설","Ø65mm","개소",2962,42320,0,45282,"합계"]
["CGF13000075S",null,"P.E관 소켓융착 접합 및 부설","Ø75mm","개소",3759,53702,0,57461,"합계"]
["CGF14000040S",null,"P.E.관 바트융착 접합 및 부설","Ø40mm 이하","개소",3662,24419,0,28081,"합계"]
["CGF14000050S",null,"P.E.관 바트융착 접합 및 부설","Ø50mm","개소",5005,33370,0,38375,"합계"]
["CGF14000065S",null,"P.E.관 바트융착 접합 및 부설","Ø65mm","개소",7690,51271,0,58961,"합계"]
["CGF14000075S",null,"P.E.관 바트융착 접합 및 부설","Ø75mm","개소",9397,62653,0,72050,"합계"]
["CGF15000075S",null,"P.E.관 분기관 천공 및 접합","Ø75mm","개소",1629,32594,0,34223,"합계"]
["CGF22000100S",null,"P.E.관 밴드 접합 및 부설","Ø100mm","개소",1100,36681,0,37781,"합계"]
["CGF22000150S",null,"P.E.관 밴드 접합 및 부설","Ø150mm","개소",1491,49718,0,51209,"합계"]
["CGF22000200S",null,"P.E.관 밴드 접합 및 부설","Ø200mm","개소",1882,62756,0,64638,"합계"]
["CGF24000100S",null,"P.E.관 바트융착 접합 및 부설","Ø100mm","개소",11105,74035,0,85140,"합계"]
["CGF24000125S",null,"P.E.관 바트융착 접합 및 부설","Ø125mm","개소",13425,89504,0,102929,"합계"]
["CGF24000150S",null,"P.E.관 바트융착 접합 및 부설","Ø150mm","개소",13790,91936,0,105726,"합계"]
["CGF24000200S",null,"P.E.관 바트융착 접합 및 부설","Ø200mm","개소",17453,116356,0,133809,"합계"]
["CGF25000100S",null,"P.E.관 분기관 천공 및 접합","Ø100mm","개소",1834,36681,0,38515,"합계"]
["CGF25000150S",null,"P.E.관 분기관 천공 및 접합","Ø150mm","개소",2077,41544,0,43621,"합계"]
["CGF25000200S",null,"P.E.관 분기관 천공 및 접합","Ø200mm","개소",2403,48063,0,50466,"합계"]
["CGF32000250S",null,"P.E.관 밴드 접합 및 부설","Ø250mm","개소",2200,73362,0,75562,"합계"]
["CGF32000300S",null,"P.E.관 밴드 접합 및 부설","Ø300mm","개소",2542,84744,0,87286,"합계"]
["CGF32000350S",null,"P.E.관 밴드 접합 및 부설","Ø350mm","개소",2933,97782,0,100715,"합계"]
["CGF32000400S",null,"P.E.관 밴드 접합 및 부설","Ø400mm","개소",3251,108388,0,111639,"합계"]
["CGF34000250S",null,"P.E.관 바트융착 접합 및 부설","Ø250mm","개소",19890,132601,0,152491,"합계"]
["CGF34000300S",null,"P.E.관 바트융착 접합 및 부설","Ø300mm","개소",21481,143207,0,164688,"합계"]
["CGF34000350S",null,"P.E.관 바트융착 접합 및 부설","Ø350mm","개소",26693,157021,0,183714,"합계"]
["CGF34000400S",null,"P.E.관 바트융착 접합 및 부설","Ø400mm","개소",27801,163540,0,191341,"합계"]
["CGF35000250S",null,"P.E.관 분기관 천공 및 접합","Ø250mm","개소",2933,58669,0,61602,"합계"]
["CGF35000300S",null,"P.E.관 분기관 천공 및 접합","Ø300mm","개소",3259,65188,0,68447,"합계"]
["CGF42000450S",null,"P.E.관 밴드 접합 및 부설","Ø450mm","개소",3642,121425,0,125067,"합계"]
["CGF42000500S",null,"P.E.관 밴드 접합 및 부설","Ø500mm","개소",3960,132031,0,135991,"합계"]
["CGF44000450S",null,"P.E.관 바트융착 접합 및 부설","Ø450mm","개소",30150,177354,0,207504,"합계"]
["CGF44000500S",null,"P.E.관 바트융착 접합 및 부설","Ø500mm","개소",31671,186304,0,217975,"합계"]
["CGF44000550S",null,"P.E.관 바트융착 접합 및 부설","Ø550mm","개소",34301,201774,0,236075,"합계"]
["CGF44000600S",null,"P.E.관 바트융착 접합 및 부설","Ø600mm","개소",32520,192019,4997,229536,"합계"]
["CGF44000700S",null,"P.E.관 바트융착 접합 및 부설","Ø700mm","개소",53008,248888,6695,308591,"합계"]
["CGF54000800S",null,"P.E.관 바트융착 접합 및 부설","Ø800mm","개소",69030,323489,8195,400714,"합계"]
["CGP00300008S",null,"부단수 천공 분기점 분기","Ø80mm","개소",16305,161286,11193,188784,"합계"]
["CGP00300010S",null,"부단수 천공 분기점 분기","Ø100mm","개소",17243,172126,11593,200962,"합계"]
["CGP00300015S",null,"부단수 천공 분기점 분기","Ø150mm","개소",19287,198131,12092,229510,"합계"]
["CGP00300020S",null,"부단수 천공 분기점 분기","Ø200mm","개소",21456,215041,14291,250788,"합계"]
["CGP00300025S",null,"부단수 천공 분기점 분기","Ø250mm","개소",23161,234289,15090,272540,"합계"]
["CGP00300030S",null,"부단수 천공 분기점 분기","Ø300mm","개소",24774,251577,15990,292341,"합계"]
["CGP00300035S",null,"부단수 천공 분기점 분기","Ø350mm","개소",42880,327535,16889,387304,"합계"]
["CGP00300040S",null,"부단수 천공 분기점 분기","Ø400mm","개소",51481,397446,17889,466816,"합계"]
["CGP00300045S",null,"부단수 천공 분기점 분기","Ø450mm","개소",59456,461783,19088,540327,"합계"]
["CGP00300050S",null,"부단수 천공 분기점 분기","Ø500mm","개소",67352,525648,20187,613187,"합계"]
["CGP00300060S",null,"부단수 천공 분기점 분기","Ø600mm","개소",81814,641756,22686,746256,"합계"]
["CGP00411000S",null,"부단수 천공 새들분수전 분기점 분기","본관 Ø50mm, 지관 Ø13∼20mm","개소",2607,65188,0,67795,"합계"]
["CGP00412000S",null,"부단수 천공 새들분수전 분기점 분기","본관 Ø50mm, 지관 Ø25∼32mm","개소",3129,78225,0,81354,"합계"]
["CGP00413000S",null,"부단수 천공 새들분수전 분기점 분기","본관 Ø50mm, 지관 Ø40∼50mm","개소",3650,91263,0,94913,"합계"]
["CGP00421000S",null,"부단수 천공 새들분수전 분기점 분기","본관 Ø80mm, 지관 Ø13∼20mm","개소",3129,78225,0,81354,"합계"]
["CGP00422000S",null,"부단수 천공 새들분수전 분기점 분기","본관 Ø80mm, 지관 Ø25∼32mm","개소",3650,91263,0,94913,"합계"]
["CGP00423000S",null,"부단수 천공 새들분수전 분기점 분기","본관 Ø80mm, 지관 Ø40∼50mm","개소",4432,110819,0,115251,"합계"]
["CGP00431000S",null,"부단수 천공 새들분수전 분기점 분기","본관 Ø100mm, 지관 Ø13∼20mm","개소",3292,82312,0,85604,"합계"]
["CGP00432000S",null,"부단수 천공 새들분수전 분기점 분기","본관 Ø100mm, 지관 Ø25∼32mm","개소",3814,95350,0,99164,"합계"]
["CGP00433000S",null,"부단수 천공 새들분수전 분기점 분기","본관 Ø100mm, 지관 Ø40∼50mm","개소",4693,117338,0,122031,"합계"]
["CGP00441000S",null,"부단수 천공 새들분수전 분기점 분기","본관 Ø150mm, 지관 Ø13∼20mm","개소",3455,86399,0,89854,"합계"]
["CGP00442000S",null,"부단수 천공 새들분수전 분기점 분기","본관 Ø150mm, 지관 Ø25∼32mm","개소",3977,99437,0,103414,"합계"]
["CGP00443000S",null,"부단수 천공 새들분수전 분기점 분기","본관 Ø150mm, 지관 Ø40∼50mm","개소",4954,123857,0,128811,"합계"]
["CGP00451000S",null,"부단수 천공 새들분수전 분기점 분기","본관 Ø200mm, 지관 Ø13∼20mm","개소",3619,90487,0,94106,"합계"]
["CGP00452000S",null,"부단수 천공 새들분수전 분기점 분기","본관 Ø200mm, 지관 Ø25∼32mm","개소",4238,105956,0,110194,"합계"]
["CGP00453000S",null,"부단수 천공 새들분수전 분기점 분기","본관 Ø200mm, 지관 Ø40∼50mm","개소",5215,130376,0,135591,"합계"]
["CGP00461000S",null,"부단수 천공 새들분수전 분기점 분기","본관 Ø250mm, 지관 Ø13∼20mm","개소",3782,94574,0,98356,"합계"]
["CGP00462000S",null,"부단수 천공 새들분수전 분기점 분기","본관 Ø250mm, 지관 Ø25∼32mm","개소",4499,112475,0,116974,"합계"]
["CGP00463000S",null,"부단수 천공 새들분수전 분기점 분기","본관 Ø250mm, 지관 Ø40∼50mm","개소",5475,136894,0,142369,"합계"]
["CGP00471000S",null,"부단수 천공 새들분수전 분기점 분기","본관 Ø300mm, 지관 Ø13∼20mm","개소",3946,98661,0,102607,"합계"]
["CGP00472000S",null,"부단수 천공 새들분수전 분기점 분기","본관 Ø300mm, 지관 Ø25∼32mm","개소",4759,118993,0,123752,"합계"]
["CGP00473000S",null,"부단수 천공 새들분수전 분기점 분기","본관 Ø300mm, 지관 Ø40∼50mm","개소",5736,143413,0,149149,"합계"]
["CGP00481000S",null,"부단수 천공 새들분수전 분기점 분기","본관 Ø400mm, 지관 Ø13∼20mm","개소",4109,102748,0,106857,"합계"]
["CGP00482000S",null,"부단수 천공 새들분수전 분기점 분기","본관 Ø400mm, 지관 Ø25∼32mm","개소",5020,125512,0,130532,"합계"]
["CGP00483000S",null,"부단수 천공 새들분수전 분기점 분기","본관 Ø400mm, 지관 Ø40∼50mm","개소",5997,149932,0,155929,"합계"]
["CGP00500006S",null,"플랜지 조인트 접합","Ø65mm","개소",309,15469,0,15778,"합계"]
["CGP00500008S",null,"플랜지 조인트 접합","Ø80mm","개소",309,15469,0,15778,"합계"]
["CGP00500010S",null,"플랜지 조인트 접합","Ø100mm","개소",472,23643,0,24115,"합계"]
["CGP00500012S",null,"플랜지 조인트 접합","Ø125mm","개소",521,26075,0,26596,"합계"]
["CGP00500015S",null,"플랜지 조인트 접합","Ø150mm","개소",603,30162,0,30765,"합계"]
["CGP00500020S",null,"플랜지 조인트 접합","Ø200mm","개소",733,36681,0,37414,"합계"]
["CGP00500025S",null,"플랜지 조인트 접합","Ø250mm","개소",912,45631,0,46543,"합계"]
["CGP00500030S",null,"플랜지 조인트 접합","Ø300mm","개소",912,45631,0,46543,"합계"]
["CGP00500035S",null,"플랜지 조인트 접합","Ø350mm","개소",1043,52150,0,53193,"합계"]
["CGP00500040S",null,"플랜지 조인트 접합","Ø400mm","개소",1173,58669,0,59842,"합계"]
["CGP00500045S",null,"플랜지 조인트 접합","Ø450mm","개소",1303,65188,0,66491,"합계"]
["CGP00500050S",null,"플랜지 조인트 접합","Ø500mm","개소",1434,71706,0,73140,"합계"]
["CGP00500060S",null,"플랜지 조인트 접합","Ø600mm","개소",1564,78225,0,79789,"합계"]
["CGP00500070S",null,"플랜지 조인트 접합","Ø700mm","개소",1776,88831,0,90607,"합계"]
["CGP00500080S",null,"플랜지 조인트 접합","Ø800mm","개소",1873,93695,0,95568,"합계"]
["CGP00500090S",null,"플랜지 조인트 접합","Ø900mm","개소",2004,100213,0,102217,"합계"]
["CGP00500100S",null,"플랜지 조인트 접합","Ø1000mm","개소",2265,113251,0,115516,"합계"]
["CGP00500120S",null,"플랜지 조인트 접합","Ø1200mm","개소",2607,130376,0,132983,"합계"]
["CGP00500135S",null,"플랜지 조인트 접합","Ø1350mm","개소",2689,134463,0,137152,"합계"]
["CGP00500150S",null,"플랜지 조인트 접합","Ø1500mm","개소",2998,149932,0,152930,"합계"]
["CGP00500165S",null,"플랜지 조인트 접합","Ø1650mm","개소",3389,169489,0,172878,"합계"]
["CGP00500180S",null,"플랜지 조인트 접합","Ø1800mm","개소",3732,186613,0,190345,"합계"]
["CGP00500200S",null,"플랜지 조인트 접합","Ø2000mm","개소",4123,206170,0,210293,"합계"]
["CGP00500220S",null,"플랜지 조인트 접합","Ø2200mm","개소",4481,224071,0,228552,"합계"]
["CGP00500240S",null,"플랜지 조인트 접합","Ø2400mm","개소",4823,241195,0,246018,"합계"]
["CGP02100005S",null,"주철제 게이트 제수밸브 부설 및 접합","Ø50mm","기당",2881,34670,3198,40749,"합계"]
["CGP02100008S",null,"주철제 게이트 제수밸브 부설 및 접합","Ø80mm","기당",3528,46454,3797,53779,"합계"]
["CGP02100010S",null,"주철제 게이트 제수밸브 부설 및 접합","Ø100mm","기당",4154,53847,4497,62498,"합계"]
["CGP02100012S",null,"주철제 게이트 제수밸브 부설 및 접합","Ø125mm","기당",4392,58879,4697,67968,"합계"]
["CGP02100015S",null,"주철제 게이트 제수밸브 부설 및 접합","Ø150mm","기당",4644,64687,4897,74228,"합계"]
["CGP02100020S",null,"주철제 게이트 제수밸브 부설 및 접합","Ø200mm","기당",6285,95415,6396,108096,"합계"]
["CGP02100025S",null,"주철제 게이트 제수밸브 부설 및 접합","Ø250mm","기당",6600,100919,6695,114214,"합계"]
["CGP02100030S",null,"주철제 게이트 제수밸브 부설 및 접합","Ø300mm","기당",6886,108383,6895,122164,"합계"]
["CGP02100035S",null,"주철제 게이트 제수밸브 부설 및 접합","Ø350mm","기당",8163,161950,7195,177308,"합계"]
["CGP02100040S",null,"주철제 게이트 제수밸브 부설 및 접합","Ø400mm","기당",9179,202480,7495,219154,"합계"]
["CGP02100045S",null,"주철제 게이트 제수밸브 부설 및 접합","Ø450mm","기당",10194,243010,7795,260999,"합계"]
["CGP02100050S",null,"주철제 게이트 제수밸브 부설 및 접합","Ø500mm","기당",11080,277021,8095,296196,"합계"]
["CGP02100060S",null,"주철제 게이트 제수밸브 부설 및 접합","Ø600mm","기당",12798,338996,8794,360588,"합계"]
["CGP02100070S",null,"주철제 게이트 제수밸브 부설 및 접합","Ø700mm","기당",21530,389421,20220,431171,"합계"]
["CGP02100080S",null,"주철제 게이트 제수밸브 부설 및 접합","Ø800mm","기당",23857,439304,22177,485338,"합계"]
["CGP02100090S",null,"주철제 게이트 제수밸브 부설 및 접합","Ø900mm","기당",27193,480236,31219,538648,"합계"]
["CGP02100100S",null,"주철제 게이트 제수밸브 부설 및 접합","Ø1000mm","기당",28348,514247,32063,574658,"합계"]
["CGP02100110S",null,"주철제 게이트 제수밸브 부설 및 접합","Ø1100mm","기당",32022,555342,37126,624490,"합계"]
["CGP02100120S",null,"주철제 게이트 제수밸브 부설 및 접합","Ø1200mm","기당",33096,585266,37970,656332,"합계"]
["CGP02100135S",null,"주철제 게이트 제수밸브 부설 및 접합","Ø1350mm","기당",36516,629504,42470,708490,"합계"]
["CGP02100150S",null,"주철제 게이트 제수밸브 부설 및 접합","Ø1500mm","기당",42205,676268,50908,769381,"합계"]
["CGP02200060S",null,"강관제 게이트 제수밸브 부설 및 접합","Ø600mm","기당",15686,363701,12292,391679,"합계"]
["CGP02200070S",null,"강관제 게이트 제수밸브 부설 및 접합","Ø700mm","기당",17369,420510,13092,450971,"합계"]
["CGP02200080S",null,"강관제 게이트 제수밸브 부설 및 접합","Ø800mm","기당",30856,478903,31309,541068,"합계"]
["CGP02200090S",null,"강관제 게이트 제수밸브 부설 및 접합","Ø900mm","기당",33814,530778,34136,598728,"합계"]
["CGP02200100S",null,"강관제 게이트 제수밸브 부설 및 접합","Ø1000mm","기당",36849,566917,45282,649048,"합계"]
["CGP02200110S",null,"강관제 게이트 제수밸브 부설 및 접합","Ø1100mm","기당",41966,616757,52595,711318,"합계"]
["CGP02200120S",null,"강관제 게이트 제수밸브 부설 및 접합","Ø1200mm","기당",43406,657086,53720,754212,"합계"]
["CGP02200135S",null,"강관제 게이트 제수밸브 부설 및 접합","Ø1350mm","기당",47831,711963,59627,819421,"합계"]
["CGP02200150S",null,"강관제 게이트 제수밸브 부설 및 접합","Ø1500mm","기당",55947,785036,71440,912423,"합계"]
["CGP02200160S",null,"강관제 게이트 제수밸브 부설 및 접합","Ø1600mm","기당",57151,837294,71721,966166,"합계"]
["CGP02200165S",null,"강관제 게이트 제수밸브 부설 및 접합","Ø1650mm","기당",60289,854279,78140,992708,"합계"]
["CGP02200180S",null,"강관제 게이트 제수밸브 부설 및 접합","Ø1800mm","기당",66635,902562,87871,1057068,"합계"]
["CGP02200200S",null,"강관제 게이트 제수밸브 부설 및 접합","Ø2000mm","기당",76092,967825,102614,1146531,"합계"]
["CGP05000020S",null,"주철제/강관제 버터플라이 제수밸브 부설 및 접합","Ø200mm","기당",6694,103375,8594,118663,"합계"]
["CGP05000025S",null,"주철제/강관제 버터플라이 제수밸브 부설 및 접합","Ø250mm","기당",7005,111783,8994,127782,"합계"]
["CGP05000030S",null,"주철제/강관제 버터플라이 제수밸브 부설 및 접합","Ø300mm","기당",7239,119718,9294,136251,"합계"]
["CGP05000035S",null,"주철제/강관제 버터플라이 제수밸브 부설 및 접합","Ø350mm","기당",7550,173758,9694,191002,"합계"]
["CGP05000040S",null,"주철제/강관제 버터플라이 제수밸브 부설 및 접합","Ø400mm","기당",7861,218847,10093,236801,"합계"]
["CGP05000045S",null,"주철제/강관제 버터플라이 제수밸브 부설 및 접합","Ø450mm","기당",8173,259849,10493,278515,"합계"]
["CGP05000050S",null,"주철제/강관제 버터플라이 제수밸브 부설 및 접합","Ø500mm","기당",8484,295988,10893,315365,"합계"]
["CGP05000060S",null,"주철제/강관제 버터플라이 제수밸브 부설 및 접합","Ø600mm","기당",9107,362523,11692,383322,"합계"]
["CGP05000080S",null,"주철제/강관제 버터플라이 제수밸브 부설 및 접합","Ø800mm","기당",21537,457387,29787,508711,"합계"]
["CGP05000100S",null,"주철제/강관제 버터플라이 제수밸브 부설 및 접합","Ø1000mm","기당",24210,535468,33484,593162,"합계"]
["CGP05000110S",null,"주철제/강관제 버터플라이 제수밸브 부설 및 접합","Ø1100mm","기당",27983,582708,38702,649393,"합계"]
["CGP05000120S",null,"주철제/강관제 버터플라이 제수밸브 부설 및 접합","Ø1200mm","기당",28612,624692,39572,692876,"합계"]
["CGP05000135S",null,"주철제/강관제 버터플라이 제수밸브 부설 및 접합","Ø1350mm","기당",31756,682408,43920,758084,"합계"]
["CGP05000150S",null,"주철제/강관제 버터플라이 제수밸브 부설 및 접합","Ø1500mm","기당",38202,759975,52835,851012,"합계"]
["CGP05000165S",null,"주철제/강관제 버터플라이 제수밸브 부설 및 접합","Ø1650mm","기당",43637,802258,74602,920497,"합계"]
["CGP05000180S",null,"주철제/강관제 버터플라이 제수밸브 부설 및 접합","Ø1800mm","기당",48639,853619,83153,985411,"합계"]
["CGP05000200S",null,"주철제/강관제 버터플라이 제수밸브 부설 및 접합","Ø2000mm","기당",55883,872046,95537,1023466,"합계"]
["CGP05000220S",null,"주철제/강관제 버터플라이 제수밸브 부설 및 접합","Ø2200mm","기당",48569,1017313,94546,1160428,"합계"]
["CGP05000240S",null,"주철제/강관제 버터플라이 제수밸브 부설 및 접합","Ø2400mm","기당",55133,1082827,107322,1245282,"합계"]
["CGP05100070S",null,"주철제 버터플라이 제수밸브 부설 및 접합","Ø700mm","기당",19651,414365,27178,461194,"합계"]
["CGP05100090S",null,"주철제 버터플라이 제수밸브 부설 및 접합","Ø900mm","기당",25185,500984,42189,568358,"합계"]
["CGP05100160S",null,"주철제 버터플라이 제수밸브 부설 및 접합","Ø1600mm","기당",42085,785746,71948,899779,"합계"]
["CGP05100210S",null,"주철제 버터플라이 제수밸브 부설 및 접합","Ø2100mm","기당",45419,983510,88413,1117342,"합계"]
["CGP05200070S",null,"강관제 버터플라이 제수밸브 부설 및 접합","Ø700mm","기당",9730,414365,12492,436587,"합계"]
["CGP05200090S",null,"강관제 버터플라이 제수밸브 부설 및 접합","Ø900mm","기당",23581,500984,32614,557179,"합계"]
["CGP05200160S",null,"강관제 버터플라이 제수밸브 부설 및 접합","Ø1600mm","기당",40967,785746,68627,895340,"합계"]
["CGP05200210S",null,"강관제 버터플라이 제수밸브 부설 및 접합","Ø2100mm","기당",59678,954207,102025,1115910,"합계"]
["CGP08000008S",null,"부단수 할정자관 부설 및 접합","Ø80mm","개소",1270,63532,0,64802,"합계"]
["CGP08000010S",null,"부단수 할정자관 부설 및 접합","Ø100mm","개소",1352,67619,0,68971,"합계"]
["CGP08000015S",null,"부단수 할정자관 부설 및 접합","Ø150mm","개소",2089,63457,1199,66745,"합계"]
["CGP08000020S",null,"부단수 할정자관 부설 및 접합","Ø200mm","개소",2327,68489,1399,72215,"합계"]
["CGP08000025S",null,"부단수 할정자관 부설 및 접합","Ø250mm","개소",2564,73521,1599,77684,"합계"]
["CGP08000030S",null,"부단수 할정자관 부설 및 접합","Ø300mm","개소",2961,83112,1898,87971,"합계"]
["CGP08000035S",null,"부단수 할정자관 부설 및 접합","Ø350mm","개소",3403,91520,2298,97221,"합계"]
["CGP08000040S",null,"부단수 할정자관 부설 및 접합","Ø400mm","개소",3767,99456,2598,105821,"합계"]
["CGP08000045S",null,"부단수 할정자관 부설 및 접합","Ø450mm","개소",4209,107864,2998,115071,"합계"]
["CGP08000050S",null,"부단수 할정자관 부설 및 접합","Ø500mm","개소",4572,115799,3298,123669,"합계"]
["CGP08000060S",null,"부단수 할정자관 부설 및 접합","Ø600mm","개소",5427,134575,3997,143999,"합계"]
["CGP08000070S",null,"부단수 할정자관 부설 및 접합","Ø700mm","개소",6330,155782,4697,166809,"합계"]
["CGP08000080S",null,"부단수 할정자관 부설 및 접합","Ø800mm","개소",7217,176213,5396,188826,"합계"]
["CGP08000090S",null,"부단수 할정자관 부설 및 접합","Ø900mm","개소",8381,210458,6096,224935,"합계"]
["CGP12100005S",null,"주철제 게이트 제수밸브 부설 및 접합 / 인력","Ø50mm","기당",574,28712,0,29286,"합계"]
["CGP12100008S",null,"주철제 게이트 제수밸브 부설 및 접합 / 인력","Ø80mm","기당",982,49148,0,50130,"합계"]
["CGP12100010S",null,"주철제 게이트 제수밸브 부설 및 접합 / 인력","Ø100mm","기당",1179,58978,0,60157,"합계"]
["CGP12100012S",null,"주철제 게이트 제수밸브 부설 및 접합 / 인력","Ø125mm","기당",1343,67152,0,68495,"합계"]
["CGP12100015S",null,"주철제 게이트 제수밸브 부설 및 접합 / 인력","Ø150mm","기당",1506,75326,0,76832,"합계"]
["CGR10100500S",null,"내충격PVC수도관 부설 및 접합","Ø50mm","본",472,23643,0,24115,"합계"]
["CGR10100750S",null,"내충격PVC수도관 부설 및 접합","Ø75mm","본",603,30162,0,30765,"합계"]
["CGR20101000S",null,"내충격PVC수도관 부설 및 접합","Ø100mm","본",733,36681,0,37414,"합계"]
["CGR20101500S",null,"내충격PVC수도관 부설 및 접합","Ø150mm","본",994,49718,0,50712,"합계"]
["CGR20102000S",null,"내충격PVC수도관 부설 및 접합","Ø200mm","본",1255,62756,0,64011,"합계"]
["CGR30102500S",null,"내충격PVC수도관 부설 및 접합","Ø250mm","본",1515,75794,0,77309,"합계"]
["CGR30103000S",null,"내충격PVC수도관 부설 및 접합","Ø300mm","본",1776,88831,0,90607,"합계"]
["CHC25010000S",null,"L형측구 설치(포설식)","H=0.5m 이하","개소",460,3632,1157,5249,"합계"]
["CHC25020000S",null,"L형측구 설치(포설식)","H=1.2m","개소",726,5716,1828,8270,"합계"]
["CHC25030000S",null,"L형측구 설치(포설식)","H=2.3m","개소",1155,9074,2906,13135,"합계"]
["CHK12110020S",null,"관세관(스크레이퍼+워터젯트)","Ø150∼200mm","M",3555,21170,4775,29500,"합계"]
["CHK13000000S",null,"상수관 세척","300MM 이하의 물세척","구간",0,369901,0,369901,"합계"]
["CHK13110030S",null,"관세관(스크레이퍼+워터젯트)","Ø250∼300mm","M",3673,23161,4830,31664,"합계"]
["CHK14110050S",null,"관세관(스크레이퍼+워터젯트)","Ø400∼500mm","M",4280,24106,5821,34207,"합계"]
["CHK14110070S",null,"관세관(스크레이퍼+워터젯트)","Ø600∼700mm","M",4347,24441,5876,34664,"합계"]
["CHK15110090S",null,"관세관(스크레이퍼+워터젯트)","Ø800∼900mm","M",4994,26905,6821,38720,"합계"]
["CHL10100000S",null,"하수관 세정","A-TYPE","M",1409,4296,1748,7453,"합계"]
["CHL10200000S",null,"하수관 세정","B-TYPE","M",1095,5543,1405,8043,"합계"]
["CHL41000000S",null,"C.C.T.V 조사","기존 L=320m, (기계경비 제외)","M",0,1128,0,1128,"합계"]
["CHL42000000S",null,"C.C.T.V 조사","신설 L=520m, (기계경비 제외)","M",0,1862,0,1862,"합계"]
["CHL60000000S",null,"하수관 준설 / 버킷식",null,"M3",90580,1411507,354170,1856257,"합계"]
["CHL61000000S",null,"하수관 준설 / 흡입식","A-TYPE","M3",65547,171519,81302,318368,"합계"]
["CHL62000000S",null,"하수관 준설 / 흡입식","B-TYPE","M3",53057,230532,68113,351702,"합계"]
["CHL63000000S",null,"하수도 수로암거 준설 / 흡입식","800mm 이상","M3",52912,176339,64557,293808,"합계"]
["CHL73010030S",null,"하수관 수밀시험 ","300mm 이하, 시험기구 별도","개소",0,0,279950,279950,"경비"]
["CHL73020030S",null,"하수관 공기압시험","300MM 이하, 시험기구 별도","개소",0,0,74606,74606,"경비"]
["CHL74010060S",null,"하수관 수밀시험","600mm 이하, 시험기구 별도","개소",0,0,373720,373720,"경비"]
["CHL74020060S",null,"하수관 공기압시험","600MM 이하, 시험기구 별도","개소",0,0,101841,101841,"경비"]
["CHL75010080S",null,"하수관 수밀시험 ","800mm 이하, 시험기구 별도","개소",0,0,559900,559900,"경비"]
["CHL75020080S",null,"하수관 공기압시험 ","800MM 이하, 시험기구 별도","개소",0,0,140802,140802,"경비"]
["CIA10000000S",null,"강교제작(공장제작) - 플레이트거더","SS275, SM275, SM355, SM420, HSB380","TON",0,875553,0,875553,"합계"]
["CIA20000000S",null,"강교제작(공장제작) - 박스거더","SS275, SM275, SM355, SM420, HSB380","TON",0,905126,0,905126,"합계"]
["CIA30000000S",null,"강교제작(공장제작) - 강바닥판플레이트거더","SS275, SM275, SM355, SM420, HSB380","TON",0,1043950,0,1043950,"합계"]
["CIA40000000S",null,"강교제작(공장제작) - 강바닥판박스거더","SS275, SM275, SM355, SM420, HSB380","TON",0,1070153,0,1070153,"합계"]
["CIA50000000S",null,"강교제작(공장제작) - 트러스","SS275, SM275, SM355, SM420, HSB380","TON",0,810932,0,810932,"합계"]
["CIA60000000S",null,"강교제작(공장제작) - 아치","SS275, SM275, SM355, SM420, HSB380","TON",0,1200249,0,1200249,"합계"]
["CIA70000000S",null,"강교제작(공장제작) - 라멘","SS275, SM275, SM355, SM420, HSB380","TON",0,1235806,0,1235806,"합계"]
["CIC11010000S",null,"강재거더 지조립 / 불량","개구제형","개소",114113,569142,598646,1281901,"합계","적용장비확인"]
["CIC11020000S",null,"강재거더 지조립 / 보통","개구제형","개소",91290,455313,478916,1025519,"합계","적용장비확인"]
["CIC11030000S",null,"강재거더 지조립 / 양호","개구제형","개소",74519,376857,389119,840495,"합계","적용장비확인"]
["CIC12000000S",null,"강재거더 가설 / 육상","개구제형 ","개소",249224,1048750,1266822,2564796,"합계","적용장비확인"]
["CIC12200000S",null,"강재거더 가설 / 해상","개구제형","개소",256750,1296097,1266822,2819669,"합계","적용장비확인"]
["CIC21010000S",null,"강재거더 지조립 / 불량","폐합형 ","개소",146228,759755,799192,1705175,"합계","적용장비확인"]
["CIC21020000S",null,"강재거더 지조립 / 보통","폐합형","개소",109535,569142,598646,1277323,"합계","적용장비확인"]
["CIC21030000S",null,"강재거더 지조립 / 양호","폐합형 ","개소",87628,455313,478916,1021857,"합계","적용장비확인"]
["CIC22100000S",null,"강재거더 가설 / 육상","폐합형 ","개소",312793,1400844,1688214,3401851,"합계","적용장비확인"]
["CIC22200000S",null,"강재거더 가설 / 해상","폐합형 ","개소",316074,1727342,1688214,3731630,"합계","적용장비확인"]
["CIC30100000S",null,"기타부재설치 / 육상",null,"TON",91097,391059,478916,961072,"합계","적용장비확인"]
["CIC30200000S",null,"기타부재설치 / 해상",null,"TON",93667,433903,478916,1006486,"합계","적용장비확인"]
["CIE81100000S",null,"잡철물 제작 및 설치 / 제품 설치","일반철재","TON",95766,1197077,0,1292843,"합계"]
["CIE81200000S",null,"잡철물 제작 및 설치 / 제품 설치","경량철재","TON",93398,1556640,0,1650038,"합계"]
["CIE82100000S",null,"잡철물 제작 및 설치 / 규격철물 설치","일반철재","TON",236593,2957413,0,3194006,"합계"]
["CIE82200000S",null,"잡철물 제작 및 설치 / 규격철물 설치","경량철재","TON",230743,3845733,0,4076476,"합계"]
["CIE83100000S",null,"잡철물 제작 및 설치 / 현장제작 설치","일반철재","TON",410630,5132880,0,5543510,"합계"]
["CIE83200000S",null,"잡철물 제작 및 설치 / 현장제작 설치","경량철재","TON",400294,6671569,0,7071863,"합계"]
["CIG10010000S",null,"강교도장","소재표면처리","M2",0,2758,0,2758,"합계"]
["CIG10020000S",null,"강교도장","제품표면처리","M2",0,7774,0,7774,"합계"]
["CIG23000000S",null,"강교도장","공장도장","M2",0,4649,0,4649,"합계"]
["CIH15100000S",null,"강교보수 바탕처리 / 인력","A급","M2",4562,88402,2998,95962,"합계"]
["CIH15200000S",null,"강교보수 바탕처리 / 인력","B급","M2",2752,53542,1798,58092,"합계"]
["CIH15300000S",null,"강교보수 바탕처리 / 인력","C급","M2",1809,34859,1199,37867,"합계"]
["CIH23010000S",null,"강교도장","현장도장","M2",395,7904,0,8299,"합계"]
["CJA00003000S",null,"현장타설말뚝 / 인력편성","D=1000~3000mm","인/일",0,1084468,0,1084468,"합계"]
["CJA00101000S",null,"현장타설말뚝 ","장비조립 / 외부 반출 및 반입","회",521974,4083156,1672368,6277498,"합계","적용장비확인"]
["CJA00102000S",null,"현장타설말뚝 ","장비조립 / 작업구간 이동","회",260987,2041578,836184,3138749,"합계","적용장비확인"]
["CJA00201000S",null,"현장타설말뚝 ","장비해체 / 외부 반출 및 반입","회",260987,2041578,836184,3138749,"합계","적용장비확인"]
["CJA00202000S",null,"현장타설말뚝 ","장비해체 / 작업구간 이동","회",173991,1361052,557456,2092499,"합계","적용장비확인"]
["CJA03010000S",null,"말뚝박기천공 / 인력편성",null,"인/일",0,629624,0,629624,"합계"]
["CJA03100000S",null,"말뚝박기천공 ","장비조립","회",117224,1092388,236456,1446068,"합계","적용장비확인"]
["CJA03200000S",null,"말뚝박기천공 ","장비해체","회",58612,546194,118228,723034,"합계","적용장비확인"]
["CJB22100400S",null,"말뚝두부정리(강관)","D400","본",1011,18999,599,20609,"합계"]
["CJB22200400S",null,"말뚝두부정리(콘크리트)","D400","본",2332,18909,821,22062,"합계"]
["CJB23100500S",null,"말뚝두부정리(강관)","D500","본",1213,23226,678,25117,"합계"]
["CJB23200500S",null,"말뚝두부정리(콘크리트)","D500","본",3243,26280,1160,30683,"합계"]
["CJB24100600S",null,"말뚝두부정리(강관)","D600","본",1542,28987,912,31441,"합계"]
["CJB24200600S",null,"말뚝두부정리(콘크리트)","D600","본",3770,30558,1330,35658,"합계"]
["CJB25100700S",null,"말뚝두부정리(강관)","D700","본",1790,33549,1069,36408,"합계"]
["CJB25100800S",null,"말뚝두부정리(강관)","D800","본",2055,38543,1225,41823,"합계"]
["CJB25200700S",null,"말뚝두부정리(콘크리트)","D700","본",4241,34385,1486,40112,"합계"]
["CJB25200800S",null,"말뚝두부정리(콘크리트)","D800","본",4767,38663,1656,45086,"합계"]
["CJD00110000S",null,"기성말뚝 ","장비조립 / 외부 반출 및 반입","회",351672,4083156,709368,5144196,"합계","적용장비확인"]
["CJD00120000S",null,"기성말뚝 ","장비조립 / 작업구간 이동","회",234448,2722104,472912,3429464,"합계","적용장비확인"]
["CJD00210000S",null,"기성말뚝 ","장비해체 / 외부 반출 및 반입","회",175836,2041578,354684,2572098,"합계","적용장비확인"]
["CJD00220000S",null,"기성말뚝 ","장비해체 / 작업구간 이동","회",117224,1361052,236456,1714732,"합계","적용장비확인"]
["CJD00330000S",null,"기성말뚝 / 인력편성 / 이음필요","D=400~800mm 이하","인/일",0,1451700,0,1451700,"합계"]
["CJD00340000S",null,"기성말뚝 / 인력편성 / 이음불필요","D=400~800mm 이하","인/일",0,1184679,0,1184679,"합계"]
["CJI10000000S",null,"정재하시험","반력재하법","회당",0,2766494,0,2766494,"합계"]
["CJI20000000S",null,"동재하시험",null,"회당",0,299899,0,299899,"합계"]
["CKA11100000S",null,"교량받침 설치(육상) / 1기당중량 0.2ton 이하","설치높이 20m 이하","EA",26372,200076,94204,320652,"합계","적용장비확인"]
["CKA11200000S",null,"교량받침 설치(육상) / 1기당중량 0.3ton 이하","설치높이 20m 이하","EA",37254,281127,133289,451670,"합계","적용장비확인"]
["CKA11300000S",null,"교량받침 설치(육상) / 1기당중량 0.5ton 이하","설치높이 20m 이하","EA",46064,379736,160348,586148,"합계","적용장비확인"]
["CKA11400000S",null,"교량받침 설치(육상) / 1기당중량 1.0ton 이하","설치높이 20m 이하","EA",57580,474669,200436,732685,"합계","적용장비확인"]
["CKA11500000S",null,"교량받침 설치(육상) / 1기당중량 1.5ton 이하","설치높이 20m 이하","EA",67785,605368,229499,902652,"합계","적용장비확인"]
["CKA11600000S",null,"교량받침 설치(육상) / 1기당중량 1.5ton 초과","설치높이 20m 이하","EA",78933,702487,267582,1049002,"합계","적용장비확인"]
["CKA12100000S",null,"교량받침 설치(육상) / 1기당중량 0.2ton 이하","설치높이 40m 이하","EA",31904,240024,114248,386176,"합계","적용장비확인"]
["CKA12200000S",null,"교량받침 설치(육상) / 1기당중량 0.3ton 이하","설치높이 40m 이하","EA",44778,336891,160348,542017,"합계","적용장비확인"]
["CKA12300000S",null,"교량받침 설치(육상) / 1기당중량 0.5ton 이하","설치높이 40m 이하","EA",49516,474669,200436,724621,"합계","적용장비확인"]
["CKA12400000S",null,"교량받침 설치(육상) / 1기당중량 1.0ton 이하","설치높이 40m 이하","EA",65985,545386,229499,840870,"합계","적용장비확인"]
["CKA12500000S",null,"교량받침 설치(육상) / 1기당중량 1.5ton 이하","설치높이 40m 이하","EA",78933,702487,267582,1049002,"합계","적용장비확인"]
["CKA12600000S",null,"교량받침 설치(육상) / 1기당중량 1.5ton 초과","설치높이 40m 이하","EA",94699,845160,320697,1260556,"합계","적용장비확인"]
["CKA13100000S",null,"교량받침 설치(육상) / 1기당중량 0.2ton 이하","설치높이 40m 초과","EA",40548,304231,145316,490095,"합계","적용장비확인"]
["CKA13200000S",null,"교량받침 설치(육상) / 1기당중량 0.3ton 이하","설치높이 40m 초과","EA",55973,421114,200436,677523,"합계","적용장비확인"]
["CKA13300000S",null,"교량받침 설치(육상) / 1기당중량 0.5ton 이하","설치높이 40m 초과","EA",65985,545386,229499,840870,"합계","적용장비확인"]
["CKA13400000S",null,"교량받침 설치(육상) / 1기당중량 1.0ton 이하","설치높이 40m 초과","EA",76812,631794,267582,976188,"합계","적용장비확인"]
["CKA13500000S",null,"교량받침 설치(육상) / 1기당중량 1.5ton 이하","설치높이 40m 초과","EA",94699,845160,320697,1260556,"합계","적용장비확인"]
["CKA13600000S",null,"교량받침 설치(육상) / 1기당중량 1.5ton 초과","설치높이 40m 초과","EA",118373,1056451,400872,1575696,"합계","적용장비확인"]
["CKA21100000S",null,"교량받침 설치(수상) / 1기당중량 0.2ton 이하","설치높이 20m 이하","EA",44778,336891,160348,542017,"합계","적용장비확인"]
["CKA21200000S",null,"교량받침 설치(수상) / 1기당중량 0.3ton 이하","설치높이 20m 이하","EA",64122,483262,229499,776883,"합계","적용장비확인"]
["CKA21300000S",null,"교량받침 설치(수상) / 1기당중량 0.5ton 이하","설치높이 20m 이하","EA",76812,631794,267582,976188,"합계","적용장비확인"]
["CKA21400000S",null,"교량받침 설치(수상) / 1기당중량 1.0ton 이하","설치높이 20m 이하","EA",92128,759472,320697,1172297,"합계","적용장비확인"]
["CKA21500000S",null,"교량받침 설치(수상) / 1기당중량 1.5ton 이하","설치높이 20m 이하","EA",102920,916949,348758,1368627,"합계","적용장비확인"]
["CKA21600000S",null,"교량받침 설치(수상) / 1기당중량 1.5ton 초과","설치높이 20m 이하","EA",118373,1056451,400872,1575696,"합계","적용장비확인"]
["CKA22100000S",null,"교량받침 설치(수상) / 1기당중량 0.2ton 이하","설치높이 40m 이하","EA",55973,421114,200436,677523,"합계","적용장비확인"]
["CKA22200000S",null,"교량받침 설치(수상) / 1기당중량 0.3ton 이하","설치높이 40m 이하","EA",74691,561101,267582,903374,"합계","적용장비확인"]
["CKA22300000S",null,"교량받침 설치(수상) / 1기당중량 0.5ton 이하","설치높이 40m 이하","EA",92128,759472,320697,1172297,"합계","적용장비확인"]
["CKA22400000S",null,"교량받침 설치(수상) / 1기당중량 1.0ton 이하","설치높이 40m 이하","EA",115160,949340,400872,1465372,"합계","적용장비확인"]
["CKA22500000S",null,"교량받침 설치(수상) / 1기당중량 1.5ton 이하","설치높이 40m 이하","EA",131459,1174823,444967,1751249,"합계","적용장비확인"]
["CKA22600000S",null,"교량받침 설치(수상) / 1기당중량 1.5ton 초과","설치높이 40m 이하","EA",157813,1410414,534161,2102388,"합계","적용장비확인"]
["CKA23100000S",null,"교량받침 설치(수상) / 1기당중량 0.2ton 이하","설치높이 40m 초과","EA",64122,483262,229499,776883,"합계","적용장비확인"]
["CKA23200000S",null,"교량받침 설치(수상) / 1기당중량 0.3ton 이하","설치높이 40m 초과","EA",89557,673783,320697,1084037,"합계","적용장비확인"]
["CKA23300000S",null,"교량받침 설치(수상) / 1기당중량 0.5ton 이하","설치높이 40m 초과","EA",115160,949340,400872,1465372,"합계","적용장비확인"]
["CKA23400000S",null,"교량받침 설치(수상) / 1기당중량 1.0ton 이하","설치높이 40m 초과","EA",135577,1117049,472026,1724652,"합계","적용장비확인"]
["CKA23500000S",null,"교량받침 설치(수상) / 1기당중량 1.5ton 이하","설치높이 40m 초과","EA",157813,1410414,534161,2102388,"합계","적용장비확인"]
["CKA23600000S",null,"교량받침 설치(수상) / 1기당중량 1.5ton 초과","설치높이 40m 초과","EA",182048,1625905,616340,2424293,"합계","적용장비확인"]
["CKA31100000S",null,"교량받침 교체 / 1기당중량 0.2ton 이하","교대 및 교각높이 20m 이하","개",446309,3117276,1484228,5047813,"합계","적용장비확인"]
["CKA31200000S",null,"교량받침 교체 / 1기당중량 0.3ton 이하","교대 및 교각높이 20m 이하","개",535769,3741555,1781876,6059200,"합계","적용장비확인"]
["CKA31300000S",null,"교량받침 교체 / 1기당중량 0.5ton 이하","교대 및 교각높이 20m 이하","개",629564,4746700,2004360,7380624,"합계","적용장비확인"]
["CKA31400000S",null,"교량받침 교체 / 1기당중량 1.0ton 이하","교대 및 교각높이 20m 이하","개",839428,6327834,2672814,9840076,"합계","적용장비확인"]
["CKA31500000S",null,"교량받침 교체 / 1기당중량 1.5ton 이하","교대 및 교각높이 20m 이하","개",1009809,8127300,3083707,12220816,"합계","적용장비확인"]
["CKA31600000S",null,"교량받침 교체 / 1기당중량 1.5ton 초과","교대 및 교각높이 20m 이하","개",1193337,9605302,3643926,14442565,"합계","적용장비확인"]
["CKA32100000S",null,"교량받침 교체 / 1기당중량 0.2ton 이하","교대 및 교각높이 40m 이하","개",535769,3741555,1781876,6059200,"합계","적용장비확인"]
["CKA32200000S",null,"교량받침 교체 / 1기당중량 0.3ton 이하","교대 및 교각높이 40m 이하","개",634378,4431153,2109588,7175119,"합계","적용장비확인"]
["CKA32300000S",null,"교량받침 교체 / 1기당중량 0.5ton 이하","교대 및 교각높이 40m 이하","개",740614,5583148,2358129,8681891,"합계","적용장비확인"]
["CKA32400000S",null,"교량받침 교체 / 1기당중량 1.0ton 이하","교대 및 교각높이 40m 이하","개",1007302,7594720,3206976,11808998,"합계","적용장비확인"]
["CKA32500000S",null,"교량받침 교체 / 1기당중량 1.5ton 이하","교대 및 교각높이 40m 이하","개",1193337,9605302,3643926,14442565,"합계","적용장비확인"]
["CKA32600000S",null,"교량받침 교체 / 1기당중량 1.5ton 초과","교대 및 교각높이 40m 이하","개",1458499,11739333,4453687,17651519,"합계","적용장비확인"]
["CKA33100000S",null,"교량받침 교체 / 1기당중량 0.2ton 이하","교대 및 교각높이 40m 초과","개",634378,4431153,2109588,7175119,"합계","적용장비확인"]
["CKA33200000S",null,"교량받침 교체 / 1기당중량 0.3ton 이하","교대 및 교각높이 40m 초과","개",777949,5435569,2586626,8800144,"합계","적용장비확인"]
["CKA33300000S",null,"교량받침 교체 / 1기당중량 0.5ton 이하","교대 및 교각높이 40m 초과","개",899264,6779316,2863228,10541808,"합계","적용장비확인"]
["CKA33400000S",null,"교량받침 교체 / 1기당중량 1.0ton 이하","교대 및 교각높이 40m 초과","개",1199292,9041917,3818305,14059514,"합계","적용장비확인"]
["CKA33500000S",null,"교량받침 교체 / 1기당중량 1.5ton 이하","교대 및 교각높이 40m 초과","개",1458499,11739333,4453687,17651519,"합계","적용장비확인"]
["CKA33600000S",null,"교량받침 교체 / 1기당중량 1.5ton 초과","교대 및 교각높이 40m 초과","개",1750269,14087826,5344625,21182720,"합계","적용장비확인"]
["CKC40011000S",null,"중앙분리대 지주 설치(가드레일식)","지주간격 2m","M",1688,9693,1701,13082,"합계"]
["CKC40012000S",null,"중앙분리대 지주 설치(가드레일식)","지주간격 4m","M",843,4857,850,6550,"합계"]
["CKC40021100S",null,"중앙분리대 판 설치(가드레일식)","지주간격 2m, 2W","M",385,6028,190,6603,"합계"]
["CKC40021200S",null,"중앙분리대 판 설치(가드레일식)","지주간격 2m, 3W","M",455,7124,224,7803,"합계"]
["CKC40022100S",null,"중앙분리대 판 설치(가드레일식)","지주간격 4m, 2W","M",294,4614,144,5052,"합계"]
["CKC40022300S",null,"중앙분리대 판 설치(가드레일식)","지주간격 4m, 3W","M",357,5589,176,6122,"합계"]
["CKC41010000S",null,"중앙분리대 설치(콘크리트포설식)","높이 0.81m","M",1057,5721,1964,8742,"합계"]
["CKC41020000S",null,"중앙분리대 설치(콘크리트포설식)","높이 1.27m","M",1232,6672,2290,10194,"합계"]
["CKD10010000S",null,"교량배수시설 설치","Φ150mm~250mm이하","M",6270,87831,19850,113951,"합계","적용장비확인"]
["CKE11010000S",null,"교량점검시설 점검통로 설치","20M 이하","M2",2330,25896,4461,32687,"합계","적용장비확인"]
["CKE11020000S",null,"교량점검시설 점검통로 설치","40M 이하","M2",4573,33805,13793,52171,"합계","적용장비확인"]
["CKE14010000S",null,"교량점검시설 점검계단 설치","20M 이하","M2",8931,99388,17082,125401,"합계","적용장비확인"]
["CKE14020000S",null,"교량점검시설 점검계단 설치","40M 이하","M2",15239,112704,45950,173893,"합계","적용장비확인"]
["CKE90100000S",null,"프리캐스트 콘크리트 패널 설치","대차시공 (대차제외)","M2",3242,25661,12904,41807,"합계","적용장비확인"]
["CKE90200000S",null,"프리캐스트 콘크리트 패널 설치","크레인시공","M2",3932,30885,15649,50466,"합계","적용장비확인"]
["CKR10020000S",null,"빔 가설공 ","55ton/개 미만","TON",1753,8309,16895,26957,"합계","적용장비확인"]
["CKR10030000S",null,"빔 가설공","55~75ton/개 미만","TON",1288,6085,12423,19796,"합계","적용장비확인"]
["CKR10040000S",null,"빔 가설공","75~100ton/개 미만","TON",1057,5001,10188,16246,"합계","적용장비확인"]
["CKR10050000S",null,"빔 가설공 ","100~125ton/개 미만","TON",729,3449,7036,11214,"합계","적용장비확인"]
["CKR10060000S",null,"빔 가설공","125~150ton/개 미만 ","TON",553,2617,5336,8506,"합계","적용장비확인"]
["CKR10070000S",null,"빔 가설공 ","150~200ton/개 미만","TON",420,1989,4054,6463,"합계","적용장비확인"]
["CLA70010000S",null,"동상방지층 / 인력식 소규모장비 포설","t=20cm","M3",1293,9967,1383,12643,"합계"]
["CLA70020000S",null,"동상방지층 / 기계포설(길어깨)","t=20cm","M3",2145,7292,2060,11497,"합계"]
["CLA70030000S",null,"동상방지층 / 기계포설(본선)","t=20cm","M3",871,2477,1068,4416,"합계"]
["CLA80010000S",null,"입도조정기층 / 인력식 소규모장비 포설","t=20cm","M3",1581,12190,1691,15462,"합계"]
["CLA80020000S",null,"입도조정기층 / 기계포설(길어깨)","t=20cm","M3",2682,8288,2575,13545,"합계"]
["CLA80030000S",null,"입도조정기층 / 기계포설(본선)","t=20cm ","M3",1046,2984,1284,5314,"합계"]
["CLB00010000S",null,"보조기층 / 인력식 소규모장비 포설","t=20cm","M3",1422,10960,1521,13903,"합계"]
["CLB00020000S",null,"보조기층 / 기계포설(길어깨)","t=20cm","M3",2386,7368,2292,12046,"합계"]
["CLB00030000S",null,"보조기층 / 기계포설(본선)","t=20cm","M3",949,2701,1164,4814,"합계"]
["CLC11010000S",null,"텍코팅 및 프라임 코팅 살포","인력식","M3",1,74,0,75,"합계"]
["CLC11020000S",null,"텍코팅 및 프라임 코팅 살포","기계식","M3",6,30,6,42,"합계"]
["CLC30010000S",null,"아스팔트 기층 소규모포설","t=7.5cm 이하","M2",474,5801,353,6628,"합계"]
["CLC32021000S",null,"아스팔트 기층 기계포설(소형장비)","1층 포설두께 5~7cm","M2",272,1916,479,2667,"합계"]
["CLC32022100S",null,"아스팔트 기층 기계포설(대형장비)","2m≤시공폭<3m, 1층 포설두께 5~7㎝","M2",184,1172,299,1655,"합계"]
["CLC32022200S",null,"아스팔트 기층 기계포설(대형장비)","3m≤시공폭, 1층 포설두께 5~7㎝","M2",101,646,164,911,"합계"]
["CLC33021000S",null,"아스팔트 기층 기계포설(소형장비)","1층 포설두께 8~10cm","M2",297,2100,524,2921,"합계"]
["CLC33022100S",null,"아스팔트 기층 기계포설(대형장비)","2m≤시공폭<3m, 1층 포설두께 8~10㎝","M2",199,1267,323,1789,"합계"]
["CLC33022200S",null,"아스팔트 기층 기계포설(대형장비)","3m≤시공폭, 1층 포설두께 8~10㎝","M2",110,704,179,993,"합계"]
["CLC40010000S",null,"아스팔트 표층 소규모포설","t=7.5cm 이하","M2",505,6185,376,7066,"합계"]
["CLC40021000S",null,"아스팔트 표층 기계포설(소형장비)","1층 포설두께 5~7cm","M2",297,2100,524,2921,"합계"]
["CLC40022100S",null,"아스팔트 표층 기계포설(대형장비)","2m≤시공폭<3m, 1층 포설두께 5~7㎝","M2",191,1219,311,1721,"합계"]
["CLC40022200S",null,"아스팔트 표층 기계포설(대형장비)","3m≤시공폭, 1층 포설두께 5~7㎝","M2",103,660,168,931,"합계"]
["CLC81000100S",null,"투배수성 표층 포설","2m≤시공폭<3m, 1층 포설두께 5㎝","M2",242,1508,363,2113,"합계"]
["CLC81000200S",null,"투배수성 표층 포설","3m≤시공폭, 1층 포설두께 5㎝","M2",127,792,190,1109,"합계"]
["CLC81010000S",null,"투수아스팔트 표층 소규모포설","1층 포설두께 5~7cm","M2",606,7415,452,8473,"합계"]
["CLC81020000S",null,"투수아스팔트 표층 기계포설(소형장비)","1층 포설두께 5~7cm","M2",366,2426,652,3444,"합계"]
["CLC86000100S",null,"개질아스팔트 표층 포설","2m≤시공폭<3m, 1층 포설두께 5㎝","M2",204,1267,304,1775,"합계"]
["CLC86000200S",null,"개질아스팔트 표층 포설","3m≤시공폭, 1층 포설두께 5㎝","M2",113,704,169,986,"합계"]
["CLC91000000S",null,"포장 절단 / 아스팔트포장","포장두께 20cm 이하","M",170,1296,31,1497,"합계"]
["CLC92022000S",null,"아스팔트 절삭 후 아스팔트 덧씌우기","1회절삭, 2회포장 / B-TYPE / 밀링깊이 100mm이하","M2",1199,3440,2144,6783,"합계"]
["CLC92103000S",null,"아스팔트 절삭 및 덧씌우기 / 절삭","소규모포장 / 밀링깊이 70mm이하","M2",340,979,589,1908,"합계"]
["CLC92111000S",null,"아스팔트 절삭 후 아스팔트 덧씌우기","1회절삭, 1회포장 / A-TYPE / 밀링깊이 70mm이하","M2",442,1328,783,2553,"합계"]
["CLC92112000S",null,"아스팔트 절삭 후 아스팔트 덧씌우기","1회절삭, 2회포장 / A-TYPE / 밀링깊이 100mm이하","M2",850,2556,1506,4912,"합계"]
["CLC92121000S",null,"아스팔트 절삭 후 아스팔트 덧씌우기","1회절삭, 1회포장 / B-TYPE / 밀링깊이 70mm이하","M2",635,1822,1135,3592,"합계"]
["CLC92131000S",null,"아스팔트 절삭 후 아스팔트 덧씌우기","1회절삭, 1회포장 / C-TYPE / 밀링깊이 70mm이하","M2",824,2945,1393,5162,"합계"]
["CLC92202000S",null,"콘크리트 포장 절삭 후 아스팔트 덧씌우기","2회절삭, 2회포장 / 밀링깊이 100mm이하","M2",1578,4744,2797,9119,"합계"]
["CLC92303000S",null,"아스팔트 절삭 및 덧씌우기 / 덧씌우기","소규모포장 / 밀링깊이 70mm이하","M2",331,1912,474,2717,"합계"]
["CLC93110000S",null,"소파보수(표층) / 절삭 후 재포장","A-Type / 시공면적 61~120m2","M2",661,8254,893,9808,"합계"]
["CLC93120000S",null,"소파보수(표층) / 절삭 후 재포장","B-Type / 시공면적 31~60m2","M2",1888,23560,2553,28001,"합계"]
["CLC93130000S",null,"소파보수(표층) / 절삭 후 재포장","C-Type / 시공면적 11~20m2","M2",5289,66033,7153,78475,"합계"]
["CLC93210000S",null,"소파보수(포장복구) ","A-Type / 시공면적 17~24m2","M2",2220,30020,2912,35152,"합계"]
["CLC93220000S",null,"소파보수(포장복구) ","B-Type / 시공면적 11~20m2","M2",5435,73485,7128,86048,"합계"]
["CLC93230000S",null,"소파보수(포장복구) ","C-Type / 시공면적 7~12m2","M2",10276,147381,12250,169907,"합계"]
["CLC93310000S",null,"소파보수(도로복구) ","A-Type / 시공면적 13~24m2","M2",3632,47013,4279,54924,"합계"]
["CLC93320000S",null,"소파보수(도로복구) ","B-Type / 시공면적 9~16m2","M2",8844,114114,10419,133377,"합계"]
["CLC93330000S",null,"소파보수(도로복구) ","C-Type / 시공면적 5~8m2","M2",21435,272344,22969,316748,"합계"]
["CLC94100000S",null,"맨홀보수 / 하수도 및 기타 맨홀","인상높이 5cm이하","개소",48861,553365,31467,633693,"합계"]
["CLC94200000S",null,"맨홀보수 / 상수도 맨홀","인상높이 5cm이하","개소",73410,831675,47222,952307,"합계"]
["CLC95000000S",null,"슬러리실","포설두께 6mm","M2",102,347,137,586,"합계"]
["CLC96000000S",null,"표면평탄작업",null,"M2",723,1493,1296,3512,"합계"]
["CLC97000000S",null,"현장가열 표층재생공법","포설두께 5cm","M2",814,2046,4355,7215,"합계"]
["CLD11110000S",null,"린 콘크리트 기층 포설","일반포장","M3",783,3948,1405,6136,"합계"]
["CLD11120000S",null,"린 콘크리트 기층 포설","터널포장","M3",864,4369,1550,6783,"합계"]
["CLD11211000S",null,"콘크리트 표층 인력포설","A-Type, 20cm","M3",409,13645,0,14054,"합계"]
["CLD11212000S",null,"콘크리트 표층 인력포설","A-Type, 30cm","M3",272,9099,0,9371,"합계"]
["CLD11213000S",null,"콘크리트 표층 인력포설","A-Type, 40cm","M3",204,6822,0,7026,"합계"]
["CLD11221000S",null,"콘크리트 표층 인력포설","B-Type, 20cm","M3",818,27290,0,28108,"합계"]
["CLD11222000S",null,"콘크리트 표층 인력포설","B-Type, 30cm","M3",544,18162,0,18706,"합계"]
["CLD11223000S",null,"콘크리트 표층 인력포설","B-Type, 40cm","M3",409,13645,0,14054,"합계"]
["CLD11310000S",null,"콘크리트 표층 기계포설(소형장비)","일반포장","M3",1889,9582,2651,14122,"합계"]
["CLD11320000S",null,"콘크리트 표층 기계포설(소형장비)","터널포장","M3",2095,10630,2940,15665,"합계"]
["CLD11330000S",null,"콘크리트 표층 기계포설(소형장비)","공항포장, t=50cm 이하","M3",2058,10444,2889,15391,"합계"]
["CLD11410000S",null,"콘크리트 표층 기계포설(대형장비)","일반포장","M3",1106,4474,2346,7926,"합계"]
["CLD11420000S",null,"콘크리트 표층 기계포설(대형장비)","터널포장","M3",1291,5195,2738,9224,"합계"]
["CLD11430000S",null,"콘크리트 표층 기계포설(대형장비)","공항포장, t=50cm 이하","M3",1213,4882,2574,8669,"합계"]
["CLD11510000S",null,"기계포설 장비조립 및 해체(외부반출/반입)","조립","회당",474380,5427084,709368,6610832,"합계"]
["CLD11512000S",null,"기계포설 장비조립 및 해체(작업구간이동)","조립","회당",302228,3150548,472912,3925688,"합계"]
["CLD11520000S",null,"기계포설 장비조립 및 해체(외부반출/반입)","해체","회당",316253,3618056,472912,4407221,"합계"]
["CLD11522000S",null,"기계포설 장비조립 및 해체(작업구간이동)","해체","회당",151114,1575274,236456,1962844,"합계"]
["CLD61000000S",null,"포장 절단 / 콘크리트포장","포장두께 20cm 이하","M",189,1432,35,1656,"합계"]
["CLD62100000S",null,"아스팔트 절삭 후 콘크리트 덧씌우기","밀링깊이 100mm이하","M2",332,1581,712,2625,"합계"]
["CLD62200000S",null,"아스팔트 절삭 후 콘크리트 덧씌우기","밀링깊이 150mm이하","M2",519,2473,1113,4105,"합계"]
["CLE11000000S",null,"콘크리트 포장줄눈 설치",null,"M",0,1071,0,1071,"합계"]
["CLE40000000S",null,"콘크리트 포장줄눈 절단","절단깊이 10cm이하","M",146,1091,24,1261,"합계"]
["CLF30011100S",null,"보차도 및 도로경계블록 설치","A-Type / 아래폭+높이300㎜ 미만 / 직선구간","M",818,7370,771,8959,"합계"]
["CLF30012000S",null,"보차도 및 도로경계블록 설치","A-Type / 아래폭+높이300㎜ 미만 / 곡선구간","M",926,8362,872,10160,"합계"]
["CLF30012100S",null,"보차도 및 도로경계블록 설치","B-Type / 아래폭+높이300㎜ 미만 / 직선구간","M",638,9044,907,10589,"합계"]
["CLF30012200S",null,"보차도 및 도로경계블록 설치","B-Type / 아래폭+높이300㎜ 미만 / 곡선구간","M",667,9454,948,11069,"합계"]
["CLF30021100S",null,"보차도 및 도로경계블록 설치","A-Type / 아래폭+높이350㎜ 미만 / 직선구간","M",959,8651,904,10514,"합계"]
["CLF30021200S",null,"보차도 및 도로경계블록 설치","A-Type / 아래폭+높이350㎜ 미만 / 곡선구간","M",1112,10030,1048,12190,"합계"]
["CLF30022100S",null,"보차도 및 도로경계블록 설치","B-Type / 아래폭+높이350㎜ 미만 / 직선구간","M",734,10395,1043,12172,"합계"]
["CLF30022200S",null,"보차도 및 도로경계블록 설치","B-Type / 아래폭+높이350㎜ 미만 / 곡선구간","M",865,12363,1225,14453,"합계"]
["CLF30031100S",null,"보차도 및 도로경계블록 설치","A-Type / 아래폭+높이400㎜ 미만 / 직선구간","M",1069,9648,1007,11724,"합계"]
["CLF30031200S",null,"보차도 및 도로경계블록 설치","A-Type / 아래폭+높이400㎜ 미만 / 곡선구간","M",1263,11403,1190,13856,"합계"]
["CLF30032100S",null,"보차도 및 도로경계블록 설치","B-Type / 아래폭+높이400㎜ 미만 / 직선구간","M",815,11491,1160,13466,"합계"]
["CLF30032200S",null,"보차도 및 도로경계블록 설치","B-Type / 아래폭+높이400㎜ 미만 / 곡선구간","M",982,13895,1395,16272,"합계"]
["CLF30041100S",null,"보차도 및 도로경계블록 설치","A-Type / 아래폭+높이500㎜ 미만 / 직선구간","M",1545,13847,1457,16849,"합계"]
["CLF30041200S",null,"보차도 및 도로경계블록 설치","A-Type / 아래폭+높이500㎜ 미만 / 곡선구간","M",1742,15862,1637,19241,"합계"]
["CLF30042100S",null,"보차도 및 도로경계블록 설치","B-Type / 아래폭+높이500㎜ 미만 / 직선구간","M",1128,15975,1604,18707,"합계"]
["CLF30042200S",null,"보차도 및 도로경계블록 설치","B-Type / 아래폭+높이500㎜ 미만 / 곡선구간","M",1221,17291,1734,20246,"합계"]
["CLF30051100S",null,"보차도 및 도로경계블록 설치","A-Type / 아래폭+높이500㎜ 이상 / 직선구간","M",2313,20933,2178,25424,"합계"]
["CLF30051200S",null,"보차도 및 도로경계블록 설치","A-Type / 아래폭+높이500㎜ 이상 / 곡선구간","M",2781,25076,2620,30477,"합계"]
["CLF30052100S",null,"보차도 및 도로경계블록 설치","B-Type / 아래폭+높이500㎜ 이상 / 직선구간","M",1835,25989,2608,30432,"합계"]
["CLF30052200S",null,"보차도 및 도로경계블록 설치","B-Type / 아래폭+높이500㎜ 이상 / 곡선구간","M",2102,29766,2986,34854,"합계"]
["CLF30111000S",null,"보차도 및 도로경계블록 철거","A-Type / 아래폭+높이300㎜ 미만","M",327,2834,360,3521,"합계"]
["CLF30112000S",null,"보차도 및 도로경계블록 철거","A-Type / 아래폭+높이350㎜ 미만","M",388,3381,428,4197,"합계"]
["CLF30113000S",null,"보차도 및 도로경계블록 철거","A-Type / 아래폭+높이400㎜ 미만","M",419,3632,462,4513,"합계"]
["CLF30114000S",null,"보차도 및 도로경계블록 철거","A-Type / 아래폭+높이500㎜ 미만","M",605,5244,667,6516,"합계"]
["CLF30115000S",null,"보차도 및 도로경계블록 철거","A-Type / 아래폭+높이500㎜ 이상","M",963,8352,1061,10376,"합계"]
["CLF30121000S",null,"보차도 및 도로경계블록 철거","B-Type / 아래폭+높이300㎜ 미만","M",255,3543,384,4182,"합계"]
["CLF30122000S",null,"보차도 및 도로경계블록 철거","B-Type / 아래폭+높이350㎜ 미만","M",305,4241,459,5005,"합계"]
["CLF30123000S",null,"보차도 및 도로경계블록 철거","B-Type / 아래폭+높이400㎜ 미만","M",329,4577,495,5401,"합계"]
["CLF30124000S",null,"보차도 및 도로경계블록 철거","B-Type / 아래폭+높이500㎜ 미만","M",475,6599,714,7788,"합계"]
["CLF30125000S",null,"보차도 및 도로경계블록 철거","B-Type / 아래폭+높이500㎜ 이상","M",786,10903,1181,12870,"합계"]
["CLF30211100S",null,"보차도 및 도로경계블록 재설치","A-Type / 아래폭+높이300㎜ 미만 / 직선구간","M",1197,10879,1201,13277,"합계"]
["CLF30211200S",null,"보차도 및 도로경계블록 재설치","A-Type / 아래폭+높이300㎜ 미만 / 곡선구간","M",1382,12553,1386,15321,"합계"]
["CLF30212100S",null,"보차도 및 도로경계블록 재설치","A-Type / 아래폭+높이350㎜ 미만 / 직선구간","M",1498,13594,1503,16595,"합계"]
["CLF30212200S",null,"보차도 및 도로경계블록 재설치","A-Type / 아래폭+높이350㎜ 미만 / 곡선구간","M",1633,14837,1639,18109,"합계"]
["CLF30213100S",null,"보차도 및 도로경계블록 재설치","A-Type / 아래폭+높이400㎜ 미만 / 직선구간","M",1633,14837,1639,18109,"합계"]
["CLF30213200S",null,"보차도 및 도로경계블록 재설치","A-Type / 아래폭+높이400㎜ 미만 / 곡선구간","M",1891,17322,1893,21106,"합계"]
["CLF30214100S",null,"보차도 및 도로경계블록 재설치","A-Type / 아래폭+높이500㎜ 미만 / 직선구간","M",2251,20585,2254,25090,"합계"]
["CLF30214200S",null,"보차도 및 도로경계블록 재설치","A-Type / 아래폭+높이500㎜ 미만 / 곡선구간","M",2762,24997,2773,30532,"합계"]
["CLF30215100S",null,"보차도 및 도로경계블록 재설치","A-Type / 아래폭+높이500㎜ 이상 / 직선구간","M",3595,32633,3607,39835,"합계"]
["CLF30215200S",null,"보차도 및 도로경계블록 재설치","A-Type / 아래폭+높이500㎜ 이상 / 곡선구간","M",4000,36316,4013,44329,"합계"]
["CLF30221100S",null,"보차도 및 도로경계블록 재설치","B-Type / 아래폭+높이300㎜ 미만 / 직선구간","M",1037,12888,1396,15321,"합계"]
["CLF30221200S",null,"보차도 및 도로경계블록 재설치","B-Type / 아래폭+높이300㎜ 미만 / 곡선구간","M",1200,14965,1613,17778,"합계"]
["CLF30222100S",null,"보차도 및 도로경계블록 재설치","B-Type / 아래폭+높이350㎜ 미만 / 직선구간","M",1344,16803,1805,19952,"합계"]
["CLF30222200S",null,"보차도 및 도로경계블록 재설치","B-Type / 아래폭+높이350㎜ 미만 / 곡선구간","M",1526,18949,2055,22530,"합계"]
["CLF30223100S",null,"보차도 및 도로경계블록 재설치","B-Type / 아래폭+높이400㎜ 미만 / 직선구간","M",1428,17800,1921,21149,"합계"]
["CLF30223200S",null,"보차도 및 도로경계블록 재설치","B-Type / 아래폭+높이400㎜ 미만 / 곡선구간","M",1628,20264,2189,24081,"합계"]
["CLF30224100S",null,"보차도 및 도로경계블록 재설치","B-Type / 아래폭+높이500㎜ 미만 / 직선구간","M",2067,25616,2785,30468,"합계"]
["CLF30224200S",null,"보차도 및 도로경계블록 재설치","B-Type / 아래폭+높이500㎜ 미만 / 곡선구간","M",2853,35435,3842,42130,"합계"]
["CLF30225100S",null,"보차도 및 도로경계블록 재설치","B-Type / 아래폭+높이500㎜ 이상 / 직선구간","M",2853,35435,3842,42130,"합계"]
["CLF30225200S",null,"보차도 및 도로경계블록 재설치","B-Type / 아래폭+높이500㎜ 이상 / 곡선구간","M",3809,47298,5129,56236,"합계"]
["CLG82111000S",null,"보도용 블록 설치(소형)","A-Type / 블록정밀절단, 0.1m2 이하","M2",724,7511,601,8836,"합계"]
["CLG82112000S",null,"보도용 블록 설치(소형)","A-Type, 0.1m2 이하 ","M2",556,6783,601,7940,"합계"]
["CLG82121000S",null,"보도용 블록 설치(소형)","B-Type / 블록정밀절단, 0.1m2 이하","M2",1010,9597,714,11321,"합계"]
["CLG82122000S",null,"보도용 블록 설치(소형)","B-Type, 0.1m2 이하","M2",813,8483,714,10010,"합계"]
["CLG82210000S",null,"보도용 블록 인력철거","A-Type","M2",112,3422,136,3670,"합계"]
["CLG82211000S",null,"보도용 블록 설치(대형)","A-Type / 블록정밀절단, 0.1m2 ~ 0.25m2","M2",1141,11827,948,13916,"합계"]
["CLG82212000S",null,"보도용 블록 설치(대형)","A-Type, 0.1m2 ~ 0.25m2","M2",877,10713,948,12538,"합계"]
["CLG82220000S",null,"보도용 블록 인력철거","B-Type","M2",156,4073,190,4419,"합계"]
["CLG82221000S",null,"보도용 블록 설치(대형)","B-Type / 블록정밀절단, 0.1m2 ~ 0.25m2","M2",1601,15220,1131,17952,"합계"]
["CLG82222000S",null,"보도용 블록 설치(대형)","B-Type, 0.1m2 ~ 0.25m2","M2",1287,13420,1131,15838,"합계"]
["CLG82310000S",null,"보도용 블록 장비사용 철거","A-Type","M2",271,2089,299,2659,"합계"]
["CLG82320000S",null,"보도용 블록 장비사용 철거","B-Type","M2",222,2723,334,3279,"합계"]
["CLG82410000S",null,"보도용 블록 재설치(소형)","A-Type / 블록정밀절단","M2",977,10099,712,11788,"합계"]
["CLG82411000S",null,"보도용 블록 재설치(대형)","A-Type / 블록정밀절단","M2",1588,16429,1156,19173,"합계"]
["CLG82420000S",null,"보도용 블록 재설치(소형)","B-Type / 블록정밀절단","M2",951,12233,878,14062,"합계"]
["CLG82421000S",null,"보도용 블록 재설치(대형)","B-Type / 블록정밀절단","M2",1714,22027,1583,25324,"합계"]
["CLG82500000S",null,"보도용 블록 소규모보수","시공면적 61~110m2","M2",1773,18081,1681,21535,"합계"]
["CLH11000000S",null,"도로 표지판 설치","복주식+표지판 (8m2이하)","개소",9804,148257,9994,168055,"합계"]
["CLH12000000S",null,"도로 표지판 설치","편지식+표지판 (12m2이하)","개소",12805,156726,56667,226198,"합계"]
["CLH13000000S",null,"도로 표지판 설치","문형식+표지판 (8m2이하 2개)","개소",175924,1253811,695008,2124743,"합계"]
["CLH14010000S",null,"도로반사경 설치","1면 (지주포함)","본",2848,94941,0,97789,"합계"]
["CLH14020000S",null,"도로반사경 설치","2면 (지주포함)","본",3759,125323,0,129082,"합계"]
["CLH14210000S",null,"도로반사경 철거","1면","본",4340,63023,4114,71477,"합계"]
["CLH14220000S",null,"도로반사경 철거","2면","본",5784,84095,5478,95357,"합계"]
["CLH14300000S",null,"도로반사경 교체",null,"매",5802,107010,7032,119844,"합계"]
["CLH15000000S",null,"탄성포장재 포설","포설두께 7.5㎝","M2",125,15310,70,15505,"합계"]
["CLH15010000S",null,"교통 안전표지판 설치","지주","개소",6182,81018,6665,93865,"합계"]
["CLH15020000S",null,"교통 안전표지판 설치","표지판","개소",0,26943,0,26943,"합계"]
["CLH15200000S",null,"교통 안전표지판 철거","단주식","개소",3098,57291,2905,63294,"합계"]
["CLH15300000S",null,"교통 안전표지판 교체","단주식","개소",8060,127377,8204,143641,"합계"]
["CLH21111000S",null,"차선 밑그림","실선","M2",45,1255,54,1354,"합계"]
["CLH21112000S",null,"차선 밑그림","파선","M2",90,2511,109,2710,"합계"]
["CLH21113000S",null,"차선 밑그림","횡단보도, 주차장","M2",119,3307,144,3570,"합계"]
["CLH21114000S",null,"차선 밑그림","문자, 기호","M2",251,7004,304,7559,"합계"]
["CLH21121000S",null,"수용성형 페인트 수동식","실선","M2",103,1255,64,1422,"합계"]
["CLH21122000S",null,"수용성형 페인트 수동식","파선","M2",206,2511,128,2845,"합계"]
["CLH21123000S",null,"수용성형 페인트 수동식","횡단보도, 주차장","M2",271,3307,168,3746,"합계"]
["CLH21124000S",null,"수용성형 페인트 수동식","문자, 기호","M2",573,7004,355,7932,"합계"]
["CLH21131000S",null,"수용성형 페인트 기계식","실선","M2",48,194,32,274,"합계"]
["CLH21132000S",null,"수용성형 페인트 기계식","파선","M2",97,388,64,549,"합계"]
["CLH21141000S",null,"융착식 도료 수동식","실선","M2",268,2178,152,2598,"합계"]
["CLH21142000S",null,"융착식 도료 수동식","파선","M2",533,4327,306,5166,"합계"]
["CLH21143000S",null,"융착식 도료 수동식","횡단보도, 주차장","M2",702,5691,402,6795,"합계"]
["CLH21144000S",null,"융착식 도료 수동식","문자, 기호","M2",1484,12036,849,14369,"합계"]
["CLH21211000S",null,"차선 밑그림 / 공용구간","실선","M2",67,1881,82,2030,"합계"]
["CLH21212000S",null,"차선 밑그림 / 공용구간","파선","M2",135,3805,164,4104,"합계"]
["CLH21213000S",null,"차선 밑그림 / 공용구간","횡단보도, 주차장","M2",178,4999,216,5393,"합계"]
["CLH21214000S",null,"차선 밑그림 / 공용구간","문자, 기호","M2",377,10525,457,11359,"합계"]
["CLH21221000S",null,"수용성형 페인트 수동식 / 공용구간","실선","M2",154,1881,95,2130,"합계"]
["CLH21222000S",null,"수용성형 페인트 수동식 / 공용구간","파선","M2",310,3805,192,4307,"합계"]
["CLH21223000S",null,"수용성형 페인트 수동식 / 공용구간","횡단보도, 주차장","M2",408,4999,252,5659,"합계"]
["CLH21224000S",null,"수용성형 페인트 수동식 / 공용구간","문자, 기호","M2",861,10525,533,11919,"합계"]
["CLH21231000S",null,"수용성형 페인트 기계식 / 공용구간","실선","M2",64,256,42,362,"합계"]
["CLH21232000S",null,"수용성형 페인트 기계식 / 공용구간","파선","M2",129,512,85,726,"합계"]
["CLH21241000S",null,"융착식 도료 수동식 / 공용구간","실선","M2",373,3030,213,3616,"합계"]
["CLH21242000S",null,"융착식 도료 수동식 / 공용구간","파선","M2",747,6060,427,7234,"합계"]
["CLH21243000S",null,"융착식 도료 수동식 / 공용구간","횡단보도, 주차장","M2",982,7964,562,9508,"합계"]
["CLH21244000S",null,"융착식 도료 수동식 / 공용구간","문자, 기호","M2",2069,16761,1189,20019,"합계"]
["CLH21300000S",null,"차선도색제거",null,"M2",3327,37280,2229,42836,"합계"]
["CLH22000000S",null,"도로표지병 설치",null,"개소",265,5316,0,5581,"합계"]
["CLH22200000S",null,"도로반사경 제거",null,"개소",1431,17723,1233,20387,"합계"]
["CLH23010000S",null,"시선유도표지 설치","흙속매설용","개소",193,6455,0,6648,"합계"]
["CLH23020000S",null,"시선유도표지 설치","가드레일용","개소",76,2544,0,2620,"합계"]
["CLH23030000S",null,"시선유도표지 설치","옹벽용","개소",193,6455,0,6648,"합계"]
["CLH23210000S",null,"시선유도표지 철거","흙속 매설용","개소",400,5828,379,6607,"합계"]
["CLH23220000S",null,"시선유도표지 철거","가드레일용","개소",199,2897,190,3286,"합계"]
["CLH23230000S",null,"시선유도표지 철거","옹벽용","개소",400,5828,379,6607,"합계"]
["CLH25000000S",null,"볼라드 설치","100mm~150mm","개소",2286,45737,0,48023,"합계"]
["CLH26000000S",null,"주차 블록 설치","750mm~1000mm","개소",326,6533,0,6859,"합계"]
["CLH27000000S",null,"차선규제봉 설치","450mm~750mm","개소",296,5939,0,6235,"합계"]
["CLH28010000S",null,"표시못 설치","A-Type","개소",2415,37880,2467,42762,"합계"]
["CLH28020000S",null,"표시못 설치","B-Type","개소",935,12737,820,14492,"합계"]
["CLH31011000S",null,"가드레일 지주 설치","지주간격 2m","M",382,3381,702,4465,"합계"]
["CLH31012000S",null,"가드레일 지주 설치","지주간격 4m","M",191,1690,351,2232,"합계"]
["CLH31021100S",null,"가드레일 판 설치","지주간격 2m, 2W","M",192,3005,95,3292,"합계"]
["CLH31021200S",null,"가드레일 판 설치","지주간격 2m, 3W","M",227,3553,112,3892,"합계"]
["CLH31022100S",null,"가드레일 판 설치","지주간격 4m, 2W","M",147,2301,72,2520,"합계"]
["CLH31022300S",null,"가드레일 판 설치","지주간격 4m, 3W","M",178,2792,88,3058,"합계"]
["CLH80000000S",null,"미끄럼방지공 설치",null,"M2",5463,71313,3096,79872,"합계"]
["CLH81100000S",null,"재래난간 철거공 / 횡재부","강재난간","M",0,17943,0,17943,"합계"]
["CLH81200000S",null,"재래난간 철거공 / 횡재부","경량형강재난간","M",0,11962,0,11962,"합계"]
["CLH81300000S",null,"재래난간 철거공 / 횡재부","알루미늄합금재난간","M",0,33109,0,33109,"합계"]
["CLH82100000S",null,"재래난간 철거공 / 속주","강재난간","M",0,215208,0,215208,"합계"]
["CLH82200000S",null,"재래난간 철거공 / 속주","경량형강재난간","M",0,215208,0,215208,"합계"]
["CLH82300000S",null,"재래난간 철거공 / 속주","알루미늄합금재난간","M",0,165545,0,165545,"합계"]
["CLL31100150S",null,"플륨관 설치","중량50~150KG미만","본",1408,13952,3883,19243,"합계"]
["CLL31100300S",null,"플륨관 설치","중량150~300KG미만","본",1674,16948,4244,22866,"합계"]
["CLL31100500S",null,"플륨관 설치","중량300~500KG미만","본",2056,21353,4635,28044,"합계"]
["CLL31100700S",null,"플륨관 설치","중량500~700KG미만","본",2542,26696,5418,34656,"합계"]
["CLL31100900S",null,"플륨관 설치","중량700~900KG미만","본",2937,31267,5809,40013,"합계"]
["CLL31101100S",null,"플륨관 설치","중량900~1100KG미만","본",3319,35671,6201,45191,"합계"]
["CLL31101300S",null,"플륨관 설치","중량1100~1300KG미만","본",3812,41125,6953,51890,"합계"]
["CLL31101500S",null,"플륨관 설치","중량1300~1500KG미만","본",4756,50265,9783,64804,"합계"]
["CLL31101800S",null,"플륨관 설치","중량1500~1800KG미만","본",2465,57473,11047,70985,"합계"]
["CLL31102100S",null,"플륨관 설치","중량1800~2100KG미만","본",2801,66149,12552,81502,"합계"]
["CLL31300500S",null,"플륨관 해체 (유용할 목적)","본당중량 (50 ~ 500KG 미만)","본",638,12419,2859,15916,"합계"]
["CLL31300700S",null,"플륨관 해체 (유용할 목적)","본당중량 (500 ~ 700KG 미만)","본",812,15649,3642,20103,"합계"]
["CLL31300900S",null,"플륨관 해체 (유용할 목적)","본당중량 (700 ~ 900KG 미만)","본",940,18275,4214,23429,"합계"]
["CLL31301100S",null,"플륨관 해체 (유용할 목적)","본당중량 (900 ~ 1,100KG 미만)","본",1074,20791,4816,26681,"합계"]
["CLL31301300S",null,"플륨관 해체 (유용할 목적)","본당중량 (1,100 ~ 1,300KG 미만)","본",1222,23584,5478,30284,"합계"]
["CLL31301500S",null,"플륨관 해체 (유용할 목적)","본당중량 (1,300 ~ 1,500KG 미만)","본",1578,30529,7074,39181,"합계"]
["CLL31301800S",null,"플륨관 해체 (유용할 목적)","본당중량 (1,500 ~ 1,800KG 미만)","본",1793,34687,8037,44517,"합계"]
["CLL31302100S",null,"플륨관 해체 (유용할 목적)","본당중량 (1,800 ~ 2,100KG 미만)","본",2069,39941,9271,51281,"합계"]
["CLL50100900S",null,"조립식 PC맨홀 설치","Ø900(하부구체+상판)","EA",6583,195487,29500,231570,"합계"]
["CLL50101200S",null,"조립식 PC맨홀 설치","Ø1,200(하부구체+상판)","EA",7524,249149,33715,290388,"합계"]
["CLL50101500S",null,"조립식 PC맨홀 설치","Ø1,500(하부구체+상판)","EA",8397,303909,37628,349934,"합계"]
["CLL50101800S",null,"조립식 PC맨홀 설치","Ø1,800(하부구체+상판)","EA",9673,365322,43348,418343,"합계"]
["CLL50200900S",null,"조립식 PC맨홀 설치","Ø900(연직구체)","EA",3359,101270,15051,119680,"합계"]
["CLL50201200S",null,"조립식 PC맨홀 설치","Ø1,200(연직구체)","EA",3829,127273,17158,148260,"합계"]
["CLL50201500S",null,"조립식 PC맨홀 설치","Ø1,500(연직구체)","EA",4299,154932,19265,178496,"합계"]
["CLL50201800S",null,"조립식 PC맨홀 설치","Ø1,800(연직구체)","EA",5575,182848,24985,213408,"합계"]
["CLR10010000S",null,"낙석방지망 설치","기초 착암","M2",209,2561,69,2839,"합계"]
["CLR10021000S",null,"낙석방지망 설치","철망 및 와이어설치 (기계식)","M2",366,3426,1393,5185,"합계"]
["CLR10022000S",null,"낙석방지망 설치","철망 및 와이어설치 (인력식)","M2",0,9250,0,9250,"합계"]
["CLR20010000S",null,"낙석방지책 설치","지주 설치","개소",2390,42159,2695,47244,"합계"]
["CLR20020000S",null,"낙석방지책 설치","와이어 설치","M",118,5939,0,6057,"합계"]
["CLR20030000S",null,"낙석방지책 설치","철망 설치","M2",66,3304,0,3370,"합계"]
["CLR30010000S",null,"방음벽 설치","앵커볼트 설치","개소",474,15826,0,16300,"합계"]
["CLR32021100S",null,"방음벽 지주설치","지주높이 3m 이하, 지주간격 2m","개소",3833,53942,3477,61252,"합계"]
["CLR32021200S",null,"방음벽 지주설치","지주높이 3m 이하, 지주간격 3m","개소",4010,56432,3637,64079,"합계"]
["CLR32021300S",null,"방음벽 지주설치","지주높이 3m 이하, 지주간격 4m","개소",4206,59367,3807,67380,"합계"]
["CLR32031000S",null,"방음판 설치","지주높이 3m 이하, 개당 면적 1m2 이하","개소",919,15074,733,16726,"합계"]
["CLR32032000S",null,"방음판 설치","지주높이 3m 이하, 개당 면적 2m2 이하","개소",1152,18905,919,20976,"합계"]
["CLR32033000S",null,"방음판 설치","지주높이 3m 이하, 개당 면적 3m2 이하","개소",1180,19399,939,21518,"합계"]
["CLR32034000S",null,"방음판 설치","지주높이 3m 이하, 개당 면적 4m2 이하","개소",1395,22968,1109,25472,"합계"]
["CLR34031000S",null,"방음판 설치","지주높이 5m 이하, 개당 면적 1m2 이하","개소",1036,15849,1521,18406,"합계"]
["CLR34032000S",null,"방음판 설치","지주높이 5m 이하, 개당 면적 2m2 이하","개소",1182,18086,1734,21002,"합계"]
["CLR34033000S",null,"방음판 설치","지주높이 5m 이하, 개당 면적 3m2 이하","개소",1288,19695,1891,22874,"합계"]
["CLR34034000S",null,"방음판 설치","지주높이 5m 이하, 개당 면적 4m2 이하","개소",1859,28435,2728,33022,"합계"]
["CLR36022100S",null,"방음벽 지주설치","지주높이 7m 이하, 지주간격 2m","개소",4413,62232,3997,70642,"합계"]
["CLR36022200S",null,"방음벽 지주설치","지주높이 7m 이하, 지주간격 3m","개소",4648,65591,4207,74446,"합계"]
["CLR36022300S",null,"방음벽 지주설치","지주높이 7m 이하, 지주간격 4m","개소",4905,69277,4437,78619,"합계"]
["CLR36031000S",null,"방음판 설치","지주높이 7m 이하, 개당 면적 1m2 이하","개소",1109,16960,1626,19695,"합계"]
["CLR36032000S",null,"방음판 설치","지주높이 7m 이하, 개당 면적 2m2 이하","개소",1388,21226,2038,24652,"합계"]
["CLR36033000S",null,"방음판 설치","지주높이 7m 이하, 개당 면적 3m2 이하","개소",1586,24155,2335,28076,"합계"]
["CLR38023100S",null,"방음벽 지주설치","지주높이 9m 이하, 지주간격 2m","개소",5486,82920,4707,93113,"합계"]
["CLR38024100S",null,"방음벽 지주설치","지주높이 11m 이하, 지주간격 2m","개소",7171,108538,6146,121855,"합계"]
["CLR38031000S",null,"방음판 설치","지주높이 9m 이하, 개당 면적 1m2 이하","개소",1201,18373,1763,21337,"합계"]
["CLR38032000S",null,"방음판 설치","지주높이 9m 이하, 개당 면적 2m2 이하","개소",1504,23049,2204,26757,"합계"]
["CLR39031000S",null,"방음판 설치","지주높이 11m 이하, 개당 면적 1m2 이하","개소",1324,20250,1944,23518,"합계"]
["CLR39032000S",null,"방음판 설치","지주높이 11m 이하, 개당 면적 2m2 이하","개소",1667,25565,2440,29672,"합계"]
["CLR41010000S",null,"유도선 설치 및 해체","설치간격 6m 이하","M",0,439,0,439,"합계"]
["CLR41020000S",null,"유도선 설치 및 해체","설치간격 10m 이하","M",0,380,0,380,"합계"]
["CLR70000000S",null,"비탈면 점검로 설치","비탈경사 1:1.0 이하, 수직고 H=30m 이내","M",4222,140735,0,144957,"합계"]
["CMA11110000S",null,"자갈궤도 / 궤광조립","단선, 60kg, PCT","M",564,20547,746,21857,"합계"]
["CMA11120000S",null,"자갈궤도 / 궤광조립","복선, 60kg, PCT","M",521,19027,690,20238,"합계"]
["CMA11210000S",null,"자갈궤도 / 궤도양로 ","(60kg, 50mm)","M",75,7393,280,7748,"합계"]
["CMA12111000S",null,"콘크리트궤도 / 궤광조립","단선, 침목 매립식, 60kg","M",594,21628,786,23008,"합계"]
["CMA12112000S",null,"콘크리트궤도 / 궤광조립","단선, 직결식, 60kg","M",463,22093,506,23062,"합계"]
["CMA12121000S",null,"콘크리트궤도 / 궤광조립","복선, 침목 매립식, 60kg","M",564,20547,746,21857,"합계"]
["CMA12122000S",null,"콘크리트궤도 / 궤광조립","복선, 직결식, 60kg","M",440,20981,482,21903,"합계"]
["CMA12310100S",null,"콘크리트궤도 / 궤광거치","단선, 도상 정리 작업, 60kg","M",718,8765,612,10095,"합계"]
["CMA12310200S",null,"콘크리트궤도 / 궤광거치","단선, 궤광 조립대 설치, 60kg","M",0,8260,0,8260,"합계"]
["CMA12310300S",null,"콘크리트궤도 / 궤광거치","단선, 궤광 높이기, 60kg","M",79,11122,295,11496,"합계"]
["CMA12310400S",null,"콘크리트궤도 / 궤광거치","단선, 궤광 정정 및 타설 준비, 60kg","M",0,9429,0,9429,"합계"]
["CMA12310500S",null,"콘크리트궤도 / 타설 후 정리","단선, 60kg","M",79,14983,295,15357,"합계"]
["CMA12320100S",null,"콘크리트궤도 / 궤광거치","복선, 도상 정리 작업, 60kg","M",682,8327,581,9590,"합계"]
["CMA12320200S",null,"콘크리트궤도 / 궤광거치","복선, 궤광 조립대 설치, 60kg","M",0,7847,0,7847,"합계"]
["CMA12320300S",null,"콘크리트궤도 / 궤광거치","복선, 궤광 높이기, 60kg","M",75,10567,280,10922,"합계"]
["CMA12320400S",null,"콘크리트궤도 / 궤광거치","복선, 궤광 정정 및 타설 준비, 60kg","M",0,8960,0,8960,"합계"]
["CMA12320500S",null,"콘크리트궤도 / 타설 후 정리","복선, 60kg","M",75,14228,280,14583,"합계"]
["CMA21000000S",null,"궤도 정정","레일 이동범위 1m미만 작업","km",407835,17260090,875825,18543750,"합계"]
["CMA22000000S",null,"궤도 이설","레일 이동범위 1m~3m","km",3778379,54220795,7393549,65392723,"합계"]
["CMA31010000S",null,"궤광철거 / 목침목 구간","37kg/m","km",392445,12912930,842775,14148150,"합계"]
["CMA31020000S",null,"궤광철거 / 목침목 구간","50kg/m","km",469395,15475620,1008025,16953040,"합계"]
["CMA32010000S",null,"궤광철거 / P.C.T. 구간","37kg/m","km",415530,13454900,892350,14762780,"합계"]
["CMA32020000S",null,"궤광철거 / P.C.T. 구간","50kg/m","km",507870,16338315,1090650,17936835,"합계"]
["CMA33010000S",null,"궤광철거 / 터널, 교량","37kg/m","km",500175,16073290,1074125,17647590,"합계"]
["CMA33020000S",null,"궤광철거 / 터널, 교량","50kg/m","km",600210,19431055,1288950,21320215,"합계"]
["CMB11010000S",null,"분기기 부설","#8, 50kg, PCT","틀",103101,2415326,285142,2803569,"합계"]
["CMB11020000S",null,"분기기 부설","#10, 50kg, PCT","틀",120776,2829382,334023,3284181,"합계"]
["CMB11030000S",null,"분기기 부설","#12, 50kg, PCT","틀",135504,3174428,374758,3684690,"합계"]
["CMB11040000S",null,"분기기 부설","#15, 50kg, PCT","틀",169381,3968035,468447,4605863,"합계"]
["CMB11050000S",null,"분기기 부설","#18, 50kg, PCT","틀",195893,4589119,541770,5326782,"합계"]
["CMB12010000S",null,"분기기 부설","#8, 60kg, PCT","틀",110466,2587849,305509,3003824,"합계"]
["CMB12020000S",null,"분기기 부설","#10, 60kg, PCT","틀",132559,3105419,366611,3604589,"합계"]
["CMB12030000S",null,"분기기 부설","#12, 60kg, PCT","틀",147288,3450466,407346,4005100,"합계"]
["CMB12040000S",null,"분기기 부설","#15, 60kg, PCT","틀",176745,4140559,488815,4806119,"합계"]
["CMB12050000S",null,"분기기 부설","#18, 60kg, PCT","틀",204730,4796147,566210,5567087,"합계"]
["CMB30010000S",null,"분기기 철거","#8 분기기","틀",46170,2339890,99150,2485210,"합계"]
["CMB30020000S",null,"분기기 철거","#10 분기기","틀",61560,2660615,132200,2854375,"합계"]
["CMB30030000S",null,"분기기 철거","#10 분기기","틀",61560,3244810,132200,3438570,"합계"]
["CMB30040000S",null,"분기기 철거","#15 분기기","틀",84645,3830560,181775,4096980,"합계"]
["CMB40010000S",null,"분기기 / 신축이음매 부설","일단","틀",4331,106297,8432,119060,"합계"]
["CMB40020000S",null,"분기기 / 신축이음매 부설","양단","틀",8663,213283,16864,238810,"합계"]
["CMC10000050S",null,"궤도용접 / 가스압접","50kg","개소",0,119674,0,119674,"합계"]
["CMC10000060S",null,"궤도용접 / 가스압접","60kg ","개소",0,133527,0,133527,"합계"]
["CMC20000000S",null,"궤도용접 / 테르밋용접","50~60kg ","개소",0,158797,0,158797,"합계"]
["CMC70010000S",null,"장대레일 설정","레일인장법","KM",0,5055234,0,5055234,"합계"]
["CMC70020000S",null,"장대레일 설정","자연대기온도법","KM",0,4583946,0,4583946,"합계"]
["CMD10000000S",null,"자갈궤도 / 자갈살포","(모터카, 자갈화차 제외)","M3",0,1574,0,1574,"합계","적용장비확인"]
["CMD20000000S",null,"자갈궤도 / 자갈고르기","굴삭기+부착용집게 (0.2m3)","M3",256,3429,550,4235,"합계"]
["CMF11111100S",null,"레일교환 / 목침목 / 인력","50kg, 3시간 차단, 시공구간 30M 이하","km",0,47352615,0,47352615,"합계"]
["CMF11111200S",null,"레일교환 / 목침목 / 인력","60kg, 3시간 차단, 시공구간 30M 이하","km",0,50151825,0,50151825,"합계"]
["CMF11112100S",null,"레일교환 / 목침목 / 인력","50kg, 3시간 차단, 시공구간 100M 이하","km",0,39495400,0,39495400,"합계"]
["CMF11112200S",null,"레일교환 / 목침목 / 인력","60kg, 3시간 차단, 시공구간 100M 이하","km",0,42085285,0,42085285,"합계"]
["CMF11113100S",null,"레일교환 / 목침목 / 인력","50kg, 3시간 차단, 시공구간 100M 초과","km",0,32013055,0,32013055,"합계"]
["CMF11113200S",null,"레일교환 / 목침목 / 인력","60kg, 3시간 차단, 시공구간 100M 초과","km",0,33853200,0,33853200,"합계"]
["CMF11121100S",null,"레일교환 / 목침목 / 인력","50kg, 4시간 차단, 시공구간 30M 이하","km",0,43716105,0,43716105,"합계"]
["CMF11121200S",null,"레일교환 / 목침목 / 인력","60kg, 4시간 차단, 시공구간 30M 이하","km",0,46515315,0,46515315,"합계"]
["CMF11122100S",null,"레일교환 / 목침목 / 인력","50kg, 4시간 차단, 시공구간 100M 이하","km",0,36652410,0,36652410,"합계"]
["CMF11122200S",null,"레일교환 / 목침목 / 인력","60kg, 4시간 차단, 시공구간 100M 이하","km",0,38867425,0,38867425,"합계"]
["CMF11123100S",null,"레일교환 / 목침목 / 인력","50kg, 4시간 차단, 시공구간 100M 초과","km",0,29798040,0,29798040,"합계"]
["CMF11123200S",null,"레일교환 / 목침목 / 인력","60kg, 4시간 차단, 시공구간 100M 초과","km",0,31428860,0,31428860,"합계"]
["CMF11211100S",null,"레일교환 / P.C.T / 인력","50kg, 3시간 차단, 시공구간 30M 이하","km",0,43716105,0,43716105,"합계"]
["CMF11211200S",null,"레일교환 / P.C.T / 인력","60kg, 3시간 차단, 시공구간 30M 이하","km",0,48146135,0,48146135,"합계"]
["CMF11212100S",null,"레일교환 / P.C.T / 인력","50kg, 3시간 차단, 시공구간 100M 이하","km",0,36652410,0,36652410,"합계"]
["CMF11212200S",null,"레일교환 / P.C.T / 인력","60kg, 3시간 차단, 시공구간 100M 이하","km",0,40288920,0,40288920,"합계"]
["CMF11213100S",null,"레일교환 / P.C.T / 인력","50kg, 3시간 차단, 시공구간 100M 초과","km",0,29798040,0,29798040,"합계"]
["CMF11213200S",null,"레일교환 / P.C.T / 인력","60kg, 3시간 차단, 시공구간 100M 초과","km",0,32641030,0,32641030,"합계"]
["CMF11221100S",null,"레일교환 / P.C.T / 인력","50kg, 4시간 차단, 시공구간 30M 이하","km",0,40873115,0,40873115,"합계"]
["CMF11221200S",null,"레일교환 / P.C.T / 인력","60kg, 4시간 차단, 시공구간 30M 이하","km",0,44928275,0,44928275,"합계"]
["CMF11222100S",null,"레일교환 / P.C.T / 인력","50kg, 4시간 차단, 시공구간 100M 이하","km",0,34228070,0,34228070,"합계"]
["CMF11222200S",null,"레일교환 / P.C.T / 인력","60kg, 4시간 차단, 시공구간 100M 이하","km",0,37655255,0,37655255,"합계"]
["CMF11223100S",null,"레일교환 / P.C.T / 인력","50kg, 4시간 차단, 시공구간 100M 초과","km",0,27583025,0,27583025,"합계"]
["CMF11223200S",null,"레일교환 / P.C.T / 인력","60kg, 4시간 차단, 시공구간 100M 초과","km",0,30426015,0,30426015,"합계"]
["CMF11311100S",null,"레일교환 / 교량 / 인력","50kg, 3시간 차단, 시공구간 30M 이하","km",0,59430535,0,59430535,"합계"]
["CMF11311200S",null,"레일교환 / 교량 / 인력","60kg, 3시간 차단, 시공구간 30M 이하","km",0,64863410,0,64863410,"합계"]
["CMF11312100S",null,"레일교환 / 교량 / 인력","50kg, 3시간 차단, 시공구간 100M 이하","km",0,49567630,0,49567630,"합계"]
["CMF11312200S",null,"레일교환 / 교량 / 인력","60kg, 3시간 차단, 시공구간 100M 이하","km",0,54372530,0,54372530,"합계"]
["CMF11313100S",null,"레일교환 / 교량 / 인력","50kg, 3시간 차단, 시공구간 100M 초과","km",0,40288920,0,40288920,"합계"]
["CMF11313200S",null,"레일교환 / 교량 / 인력","60kg, 3시간 차단, 시공구간 100M 초과","km",0,43925430,0,43925430,"합계"]
["CMF11321100S",null,"레일교환 / 교량 / 인력","50kg, 4시간 차단, 시공구간 30M 이하","km",0,55584700,0,55584700,"합계"]
["CMF11321200S",null,"레일교환 / 교량 / 인력","60kg, 4시간 차단, 시공구간 30M 이하","km",0,60433380,0,60433380,"합계"]
["CMF11322100S",null,"레일교환 / 교량 / 인력","50kg, 4시간 차단, 시공구간 100M 이하","km",0,46305990,0,46305990,"합계"]
["CMF11322200S",null,"레일교환 / 교량 / 인력","60kg, 4시간 차단, 시공구간 100M 이하","km",0,50570475,0,50570475,"합계"]
["CMF11323100S",null,"레일교환 / 교량 / 인력","50kg, 4시간 차단, 시공구간 100M 초과","km",0,37655255,0,37655255,"합계"]
["CMF11323200S",null,"레일교환 / 교량 / 인력","60kg, 4시간 차단, 시공구간 100M 초과","km",0,41082440,0,41082440,"합계"]
["CMF11411100S",null,"레일교환 / 터널 / 인력","50kg, 3시간 차단, 시공구간 30M 이하","km",0,62648395,0,62648395,"합계"]
["CMF11411200S",null,"레일교환 / 터널 / 인력","60kg, 3시간 차단, 시공구간 30M 이하","km",0,64069890,0,64069890,"합계"]
["CMF11412100S",null,"레일교환 / 터널 / 인력","50kg, 3시간 차단, 시공구간 100M 이하","km",0,52366840,0,52366840,"합계"]
["CMF11412200S",null,"레일교환 / 터널 / 인력","60kg, 3시간 차단, 시공구간 100M 이하","km",0,53579010,0,53579010,"합계"]
["CMF11413100S",null,"레일교환 / 터널 / 인력","50kg, 3시간 차단, 시공구간 100M 초과","km",0,42503935,0,42503935,"합계"]
["CMF11413200S",null,"레일교환 / 터널 / 인력","60kg, 3시간 차단, 시공구간 100M 초과","km",0,43297455,0,43297455,"합계"]
["CMF11421100S",null,"레일교환 / 터널 / 인력","50kg, 4시간 차단, 시공구간 30M 이하","km",0,58218365,0,58218365,"합계"]
["CMF11421200S",null,"레일교환 / 터널 / 인력","60kg, 4시간 차단, 시공구간 30M 이하","km",0,59430535,0,59430535,"합계"]
["CMF11422100S",null,"레일교환 / 터널 / 인력","50kg, 4시간 차단, 시공구간 100M 이하","km",0,48730330,0,48730330,"합계"]
["CMF11422200S",null,"레일교환 / 터널 / 인력","60kg, 4시간 차단, 시공구간 100M 이하","km",0,49567630,0,49567630,"합계"]
["CMF11423100S",null,"레일교환 / 터널 / 인력","50kg, 4시간 차단, 시공구간 100M 초과","km",0,39495400,0,39495400,"합계"]
["CMF11423200S",null,"레일교환 / 터널 / 인력","60kg, 4시간 차단, 시공구간 100M 초과","km",0,40288920,0,40288920,"합계"]
["CMF12111100S",null,"레일교환 / 목침목 / 기계","3시간 차단","km",661770,27670940,1421150,29753860,"합계"]
["CMF12121100S",null,"레일교환 / 목침목 / 기계","4시간 차단","km",630990,25695555,1355050,27681595,"합계"]
["CMF12211100S",null,"레일교환 / P.C.T / 기계","3시간 차단","km",615600,25584155,1322000,27521755,"합계"]
["CMF12221100S",null,"레일교환 / P.C.T / 기계","4시간 차단","km",584820,24105405,1255900,25946125,"합계"]
["CMF12311100S",null,"레일교환 / 교량 / 기계","3시간 차단","km",831060,34825850,1784700,37441610,"합계"]
["CMF12321100S",null,"레일교환 / 교량 / 기계","4시간 차단","km",800280,32431815,1718600,34950695,"합계"]
["CMF12411100S",null,"레일교환 / 터널 / 기계","3시간 차단","km",877230,36537765,1883850,39298845,"합계"]
["CMF12421100S",null,"레일교환 / 터널 / 기계","4시간 차단","km",838755,34088030,1801225,36728010,"합계"]
["CMF21111000S",null,"분기기 교환 / 인력","#8 분기기, 3시간 차단","틀",0,10559290,0,10559290,"합계"]
["CMF21121000S",null,"분기기 교환 / 인력","#8 분기기, 4시간 차단","틀",0,9975095,0,9975095,"합계"]
["CMF21211000S",null,"분기기 교환 / 인력","#10 분기기, 3시간 차단","틀",0,11937005,0,11937005,"합계"]
["CMF21221000S",null,"분기기 교환 / 인력","#10 분기기, 4시간 차단","틀",0,11352810,0,11352810,"합계"]
["CMF21311000S",null,"분기기 교환 / 인력","#12 분기기, 3시간 차단","틀",0,13314720,0,13314720,"합계"]
["CMF21321000S",null,"분기기 교환 / 인력","#12 분기기, 4시간 차단","틀",0,12730525,0,12730525,"합계"]
["CMF21411000S",null,"분기기 교환 / 인력","#15 분기기, 3시간 차단","틀",0,18616255,0,18616255,"합계"]
["CMF21421000S",null,"분기기 교환 / 인력","#15 분기기, 4시간 차단","틀",0,17822735,0,17822735,"합계"]
["CMF22111000S",null,"분기기 교환 / 기계","#8 분기기, 3시간 차단","틀",253935,7392740,545325,8192000,"합계"]
["CMF22121000S",null,"분기기 교환 / 기계","#8 분기기, 4시간 차단","틀",246240,6962170,528800,7737210,"합계"]
["CMF22211000S",null,"분기기 교환 / 기계","#10 분기기, 3시간 차단","틀",300105,8729785,644475,9674365,"합계"]
["CMF22221000S",null,"분기기 교환 / 기계","#10 분기기, 4시간 차단","틀",284715,8409060,611425,9305200,"합계"]
["CMF22311000S",null,"분기기 교환 / 기계","#12 분기기, 3시간 차단","틀",454005,10427980,974975,11856960,"합계"]
["CMF22321000S",null,"분기기 교환 / 기계","#12 분기기, 4시간 차단","틀",430920,9886010,925400,11242330,"합계"]
["CMF22411000S",null,"분기기 교환 / 기계","#15 분기기, 3시간 차단","틀",600210,13866840,1288950,15756000,"합계"]
["CMF22421000S",null,"분기기 교환 / 기계","#15 분기기, 4시간 차단","틀",584820,13380570,1255900,15221290,"합계"]
["CMF31111000S",null,"침목교환 / 목침목-목침목 / 인력","3시간 차단 / A-Type","개",0,70992,0,70992,"합계"]
["CMF31112000S",null,"침목교환 / 목침목-목침목 / 인력","3시간 차단 / B-Type","개",0,52357,0,52357,"합계"]
["CMF31121000S",null,"침목교환 / 목침목-목침목 / 인력","4시간 차단 / A-Type","개",0,69989,0,69989,"합계"]
["CMF31122000S",null,"침목교환 / 목침목-목침목 / 인력","4시간 차단 / B-Type","개",0,51729,0,51729,"합계"]
["CMF31211000S",null,"침목교환 / 목침목-PCT / 인력","3시간 차단 / A-Type","개",0,170357,0,170357,"합계"]
["CMF31212000S",null,"침목교환 / 목침목-PCT / 인력","3시간 차단 / B-Type","개",0,117119,0,117119,"합계"]
["CMF31221000S",null,"침목교환 / 목침목-PCT / 인력","4시간 차단 / A-Type","개",0,167349,0,167349,"합계"]
["CMF31222000S",null,"침목교환 / 목침목-PCT / 인력","4시간 차단 / B-Type","개",0,123277,0,123277,"합계"]
["CMF31311000S",null,"침목교환 / PCT-PCT / 인력","3시간 차단 / A-Type","개",0,199308,0,199308,"합계"]
["CMF31312000S",null,"침목교환 / PCT-PCT / 인력","3시간 차단 / B-Type","개",0,146839,0,146839,"합계"]
["CMF31321000S",null,"침목교환 / PCT-PCT / 인력","4시간 차단 / A-Type","개",0,195881,0,195881,"합계"]
["CMF31322000S",null,"침목교환 / PCT-PCT / 인력","4시간 차단 / B-Type","개",0,144415,0,144415,"합계"]
["CMF31411000S",null,"침목교환 / 교량침목교환 / 인력","3시간 차단 / A-Type","개",0,258545,0,258545,"합계"]
["CMF31412000S",null,"침목교환 / 교량침목교환 / 인력","3시간 차단 / B-Type","개",0,190327,0,190327,"합계"]
["CMF31421000S",null,"침목교환 / 교량침목교환 / 인력","4시간 차단 / A-Type","개",0,254324,0,254324,"합계"]
["CMF31422000S",null,"침목교환 / 교량침목교환 / 인력","4시간 차단 / B-Type","개",0,187318,0,187318,"합계"]
["CMF32211000S",null,"침목교환 / 목침목-PCT / 기계","3시간 차단","개",500,25770,1074,27344,"합계"]
["CMF32221000S",null,"침목교환 / 목침목-PCT / 기계","4시간 차단","개",407,22468,875,23750,"합계"]
["CMF32311000S",null,"침목교환 / PCT-PCT / 기계","3시간 차단","개",807,33012,1735,35554,"합계"]
["CMF32321000S",null,"침목교환 / PCT-PCT / 기계","4시간 차단","개",661,28736,1421,30818,"합계"]
["CMF32411000S",null,"침목교환 / 교량침목교환 / 기계","3시간 차단","개",1646,78745,3536,83927,"합계"]
["CMF32421000S",null,"침목교환 / 교량침목교환 / 기계","4시간 차단","개",1346,68924,2891,73161,"합계"]
["CMF40111000S",null,"도상 갱환 / 가받침 설치","직선구간","M",0,62659,0,62659,"합계"]
["CMF40112000S",null,"도상 갱환 / 가받침 설치","곡선구간 (R=950미만)","M",0,65792,0,65792,"합계"]
["CMF40121000S",null,"도상 갱환 / 판넬 설치","직선구간","개",0,36076,0,36076,"합계"]
["CMF40122000S",null,"도상 갱환 / 판넬 설치","곡선구간 (R=950미만)","개",0,37880,0,37880,"합계"]
["CMF40131000S",null,"도상 갱환 / 가받침 설치, 해체","직선구간","M",0,67917,0,67917,"합계"]
["CMF40141000S",null,"도상 갱환 / 타설 후 정리 작업","직선구간","M",0,64411,0,64411,"합계"]
["CMF40142000S",null,"도상 갱환 / 타설 후 정리 작업","곡선구간 (R=950미만)","M",0,67632,0,67632,"합계"]
["CMF40232000S",null,"도상 갱환 / 가받침 설치, 해체","곡선구간 (R=950미만)","M",0,71313,0,71313,"합계"]
["CMF41000000S",null,"도상자갈 철거 / 인력",null,"M3",0,84911,0,84911,"합계"]
["CMF42011000S",null,"도상자갈 철거 / 기계","3시간 차단","M3",923,29956,1564,32443,"합계"]
["CMF42021000S",null,"도상자갈 철거 / 기계","4시간 차단","M3",846,27743,1434,30023,"합계"]
["CMG41000005S",null,"자갈채집 및 운반 (궤도)","L=50m","M3",0,167200,0,167200,"합계"]
["CMG41000010S",null,"자갈채집 및 운반 (궤도)","L=100m","M3",0,175477,0,175477,"합계"]
["CMG41000015S",null,"자갈채집 및 운반 (궤도)","L=150m","M3",0,187065,0,187065,"합계"]
["CMG41000020S",null,"자갈채집 및 운반 (궤도)","L=200m","M3",0,196998,0,196998,"합계"]
["CMG41000025S",null,"자갈채집 및 운반 (궤도)","L=250m","M3",0,206931,0,206931,"합계"]
["CMG41000030S",null,"자갈채집 및 운반 (궤도)","L=300m","M3",0,216863,0,216863,"합계"]
["CMG41000035S",null,"자갈채집 및 운반 (궤도)","L=350m","M3",0,228452,0,228452,"합계"]
["CMG41000040S",null,"자갈채집 및 운반 (궤도)","L=400m","M3",0,238384,0,238384,"합계"]
["CMR11000000S",null,"레일 천공","37~60kg","공당",112,2249,46,2407,"합계"]
["CMR12000000S",null,"침목 천공",null,"개소",115,2302,27,2444,"합계"]
["CMR13000037S",null,"레일 절단","37kg","개소",449,8996,226,9671,"합계"]
["CMR13000050S",null,"레일 절단","50kg","개소",468,9371,234,10073,"합계"]
["CMR13000060S",null,"레일 절단","60kg","개소",506,10121,251,10878,"합계"]
["CMR41000000S",null,"교상가드레일","철거","km",267786,10039105,575070,10881961,"합계"]
["CMR41100000S",null,"파워렌치 조임 및 해체","조임","개소",187,3748,151,4086,"합계"]
["CMR41200000S",null,"파워렌치 조임 및 해체","해체","개소",187,3748,151,4086,"합계"]
["CMR42000000S",null,"타이템퍼 다짐",null,"M3",146,2930,974,4050,"합계"]
["CMR42000001S",null,"목침목 탄성체결장치 철거",null,"개",0,9503,0,9503,"합계"]
["CMR43000000S",null,"교상발판 설치",null,"M",0,20075,0,20075,"합계"]
["CMR44000000S",null,"교상가드레일 설치",null,"KM",359356,12454520,771717,13585593,"합계"]
["CMR45000000S",null,"교량침목고정장치 설치",null,"개",0,7219,0,7219,"합계"]
["CMR46000000S",null,"목침목 탄성체결장치 설치",null,"개",0,9503,0,9503,"합계"]
["CNE13220000S",null,"터널철재거푸집 설치, 해체, 이동",null,"회",237656,3163346,544568,3945570,"합계","적용장비확인"]
["CNI10010000S",null,"터널 방수","일체식 터널 방수시트","M2",160,2669,0,2829,"합계"]
["COA61100250S",null,"배송관 접합 (플랜지)","Ø250mm 이하","개소",3458,20996,4783,29237,"합계"]
["COA61100300S",null,"배송관 접합 (플랜지)","Ø300mm","개소",3773,21941,5218,30932,"합계"]
["COA61100350S",null,"배송관 접합 (플랜지)","Ø350mm","개소",3930,24845,5435,34210,"합계"]
["COA61100400S",null,"배송관 접합 (플랜지)","Ø400mm","개소",4244,27445,5870,37559,"합계"]
["COA61100510S",null,"배송관 접합 (플랜지)","Ø510mm","개소",5187,36798,7175,49160,"합계"]
["COA61100560S",null,"배송관 접합 (플랜지)","Ø560mm","개소",5659,40646,7827,54132,"합계"]
["COA61100610S",null,"배송관 접합 (플랜지)","Ø610mm","개소",5973,44022,8262,58257,"합계"]
["COA61100630S",null,"배송관 접합 (플랜지)","Ø630mm","개소",6131,48582,8479,63192,"합계"]
["COA61100660S",null,"배송관 접합 (플랜지)","Ø660mm","개소",6288,49054,8697,64039,"합계"]
["COA61100685S",null,"배송관 접합 (플랜지)","Ø685mm","개소",6445,51958,8914,67317,"합계"]
["COA61100710S",null,"배송관 접합 (플랜지)","Ø710mm","개소",6602,52431,9132,68165,"합계"]
["COA61100760S",null,"배송관 접합 (플랜지)","Ø760mm","개소",7219,55334,12094,74647,"합계"]
["COA61100840S",null,"배송관 접합 (플랜지)","Ø840mm","개소",7891,61311,13219,82421,"합계"]
["COA61100860S",null,"배송관 접합 (플랜지)","Ø860mm","개소",8059,61783,13500,83342,"합계"]
["COA61200250S",null,"배송관 접합 (고무슬리브)","Ø250mm 이하","개소",2829,19107,3913,25849,"합계"]
["COA61200300S",null,"배송관 접합 (고무슬리브)","Ø300mm","개소",2986,19579,4131,26696,"합계"]
["COA61200350S",null,"배송관 접합 (고무슬리브)","Ø350mm","개소",3144,22483,4348,29975,"합계"]
["COA61200400S",null,"배송관 접합 (고무슬리브)","Ø400mm","개소",3458,25083,4783,33324,"합계"]
["COA61200510S",null,"배송관 접합 (고무슬리브)","Ø510mm","개소",4087,33491,5653,43231,"합계"]
["COA61200560S",null,"배송관 접합 (고무슬리브)","Ø560mm","개소",4559,37340,6305,48204,"합계"]
["COA61200610S",null,"배송관 접합 (고무슬리브)","Ø610mm","개소",4716,40244,6522,51482,"합계"]
["COA61200630S",null,"배송관 접합 (고무슬리브)","Ø630mm","개소",4873,44803,6740,56416,"합계"]
["COA61200660S",null,"배송관 접합 (고무슬리브)","Ø660mm","개소",5030,45276,6957,57263,"합계"]
["COA61200685S",null,"배송관 접합 (고무슬리브)","Ø685mm","개소",5187,48180,7175,60542,"합계"]
["COA61200710S",null,"배송관 접합 (고무슬리브)","Ø710mm","개소",5345,48652,7392,61389,"합계"]
["COA61200760S",null,"배송관 접합 (고무슬리브)","Ø760mm","개소",5708,51084,9562,66354,"합계"]
["COA61200840S",null,"배송관 접합 (고무슬리브)","Ø840mm","개소",6380,57060,10687,74127,"합계"]
["COA61200860S",null,"배송관 접합 (고무슬리브)","Ø860mm","개소",6380,57060,10687,74127,"합계"]
["COA62100250S",null,"배송관 철거 (플랜지)","Ø250mm 이하","개소",2421,14697,3348,20466,"합계"]
["COA62100300S",null,"배송관 철거 (플랜지)","Ø300mm","개소",2641,15358,3652,21651,"합계"]
["COA62100350S",null,"배송관 철거 (플랜지)","Ø350mm","개소",2751,17391,3804,23946,"합계"]
["COA62100400S",null,"배송관 철거 (플랜지)","Ø400mm","개소",2971,19211,4109,26291,"합계"]
["COA62100510S",null,"배송관 철거 (플랜지)","Ø510mm","개소",3631,25758,5022,34411,"합계"]
["COA62100560S",null,"배송관 철거 (플랜지)","Ø560mm","개소",3961,28452,5479,37892,"합계"]
["COA62100610S",null,"배송관 철거 (플랜지)","Ø610mm","개소",4181,30816,5783,40780,"합계"]
["COA62100630S",null,"배송관 철거 (플랜지)","Ø630mm","개소",4291,34007,5935,44233,"합계"]
["COA62100660S",null,"배송관 철거 (플랜지)","Ø660mm","개소",4401,34338,6088,44827,"합계"]
["COA62100685S",null,"배송관 철거 (플랜지)","Ø685mm","개소",4511,36371,6240,47122,"합계"]
["COA62100710S",null,"배송관 철거 (플랜지)","Ø710mm","개소",4621,36701,6392,47714,"합계"]
["COA62100760S",null,"배송관 철거 (플랜지)","Ø760mm","개소",5053,38734,8465,52252,"합계"]
["COA62100840S",null,"배송관 철거 (플랜지)","Ø840mm","개소",5523,42917,9253,57693,"합계"]
["COA62100860S",null,"배송관 철거 (플랜지)","Ø860mm","개소",5641,43248,9450,58339,"합계"]
["COA62200250S",null,"배송관 철거 (고무슬리브)","Ø250mm 이하","개소",1980,13375,2739,18094,"합계"]
["COA62200300S",null,"배송관 철거 (고무슬리브)","Ø300mm","개소",2090,13705,2891,18686,"합계"]
["COA62200350S",null,"배송관 철거 (고무슬리브)","Ø350mm","개소",2200,15738,3044,20982,"합계"]
["COA62200400S",null,"배송관 철거 (고무슬리브)","Ø400mm","개소",2421,17558,3348,23327,"합계"]
["COA62200510S",null,"배송관 철거 (고무슬리브)","Ø510mm","개소",2861,23444,3957,30262,"합계"]
["COA62200560S",null,"배송관 철거 (고무슬리브)","Ø560mm","개소",3191,26138,4413,33742,"합계"]
["COA62200610S",null,"배송관 철거 (고무슬리브)","Ø610mm","개소",3301,28171,4566,36038,"합계"]
["COA62200630S",null,"배송관 철거 (고무슬리브)","Ø630mm","개소",3411,31362,4718,39491,"합계"]
["COA62200660S",null,"배송관 철거 (고무슬리브)","Ø660mm","개소",3521,31693,4870,40084,"합계"]
["COA62200685S",null,"배송관 철거 (고무슬리브)","Ø685mm","개소",3631,33726,5022,42379,"합계"]
["COA62200710S",null,"배송관 철거 (고무슬리브)","Ø710mm","개소",3741,34056,5174,42971,"합계"]
["COA62200760S",null,"배송관 철거 (고무슬리브)","Ø760mm","개소",3996,35758,6693,46447,"합계"]
["COA62200840S",null,"배송관 철거 (고무슬리브)","Ø840mm","개소",4466,39942,7481,51889,"합계"]
["COA62200860S",null,"배송관 철거 (고무슬리브)","Ø860mm","개소",4466,39942,7481,51889,"합계"]
["COA71000430S",null,"배송관 띄우개(부함) 접합","Ø430*4.5m, 200mm","본",786,8301,1087,10174,"합계"]
["COA71000500S",null,"배송관 띄우개(부함) 접합","Ø500*4.5m, 250mm","본",786,8301,1087,10174,"합계"]
["COA71000600S",null,"배송관 띄우개(부함) 접합","Ø600*4.5m, 300mm","본",786,10443,1087,12316,"합계"]
["COA71000700S",null,"배송관 띄우개(부함) 접합","Ø700*4.5m, 350mm","본",786,10443,1087,12316,"합계"]
["COA71000900S",null,"배송관 띄우개(부함) 접합","Ø900*4.5m, 400mm","본",943,10915,1304,13162,"합계"]
["COA71001000S",null,"배송관 띄우개(부함) 접합","Ø1000*4.5m, 510mm","본",943,12571,1304,14818,"합계"]
["COA71001100S",null,"배송관 띄우개(부함) 접합","Ø1100*4.5m, 560mm","본",943,12571,1304,14818,"합계"]
["COA71001200S",null,"배송관 띄우개(부함) 접합","Ø1200*4.5m, 610~630mm","본",943,12571,1304,14818,"합계"]
["COA71001300S",null,"배송관 띄우개(부함) 접합","Ø1300*5.0m, 660mm","본",943,12571,1304,14818,"합계"]
["COA71001400S",null,"배송관 띄우개(부함) 접합","Ø1400*5.0m, 685~710mm","본",1100,15185,1522,17807,"합계"]
["COA71001500S",null,"배송관 띄우개(부함) 접합","Ø1500*5.0m, 760mm","본",1175,15185,1968,18328,"합계"]
["COA71001600S",null,"배송관 띄우개(부함) 접합","Ø1600*5.0m, 840~860mm","본",1175,15185,1968,18328,"합계"]
["COA72000430S",null,"배송관 띄우개(부함) 철거","Ø430*4.5m, 200mm","본",550,5810,760,7120,"합계"]
["COA72000500S",null,"배송관 띄우개(부함) 철거","Ø500*4.5m, 250mm","본",550,5810,760,7120,"합계"]
["COA72000600S",null,"배송관 띄우개(부함) 철거","Ø600*4.5m, 300mm","본",550,7310,760,8620,"합계"]
["COA72000700S",null,"배송관 띄우개(부함) 철거","Ø700*4.5m, 350mm","본",550,7310,760,8620,"합계"]
["COA72000900S",null,"배송관 띄우개(부함) 철거","Ø900*4.5m, 400mm","본",660,7641,913,9214,"합계"]
["COA72001000S",null,"배송관 띄우개(부함) 철거","Ø1000*4.5m, 510mm","본",660,8799,913,10372,"합계"]
["COA72001100S",null,"배송관 띄우개(부함) 철거","Ø1100*4.5m, 560mm","본",660,8799,913,10372,"합계"]
["COA72001200S",null,"배송관 띄우개(부함) 철거","Ø1200*4.5m, 610~630mm","본",660,8799,913,10372,"합계"]
["COA72001300S",null,"배송관 띄우개(부함) 철거","Ø1300*5.0m, 660mm","본",660,8799,913,10372,"합계"]
["COA72001400S",null,"배송관 띄우개(부함) 철거","Ø1400*5.0m, 685~710mm","본",770,10630,1065,12465,"합계"]
["COA72001500S",null,"배송관 띄우개(부함) 철거","Ø1500*5.0m, 760mm","본",822,10630,1378,12830,"합계"]
["COA72001600S",null,"배송관 띄우개(부함) 철거","Ø1600*5.0m, 840~860mm","본",822,10630,1378,12830,"합계"]
["COA80000200S",null,"배송관 진수","Ø200mm","SET당",943,6144,1304,8391,"합계"]
["COA80000250S",null,"배송관 진수","Ø250mm","SET당",1100,6617,1522,9239,"합계"]
["COA80000300S",null,"배송관 진수","Ø300mm","SET당",1257,7089,1739,10085,"합계"]
["COA80000350S",null,"배송관 진수","Ø350mm","SET당",1414,7561,1956,10931,"합계"]
["COA80000400S",null,"배송관 진수","Ø400mm","SET당",1572,9689,2174,13435,"합계"]
["COA80000510S",null,"배송관 진수","Ø510mm","SET당",2043,11106,2826,15975,"합계"]
["COA80000560S",null,"배송관 진수","Ø560mm","SET당",2515,14178,3478,20171,"합계"]
["COA80000610S",null,"배송관 진수","Ø610mm","SET당",2829,15123,3913,21865,"합계"]
["COA80000630S",null,"배송관 진수","Ø630mm","SET당",2829,16778,3913,23520,"합계"]
["COA80000660S",null,"배송관 진수","Ø660mm","SET당",3144,17723,4348,25215,"합계"]
["COA80000685S",null,"배송관 진수","Ø685mm","SET당",3144,17723,4348,25215,"합계"]
["COA80000710S",null,"배송관 진수","Ø710mm","SET당",3301,18195,4566,26062,"합계"]
["COA80000760S",null,"배송관 진수","Ø760mm","SET당",3525,18195,5906,27626,"합계"]
["COA80000840S",null,"배송관 진수","Ø840mm","SET당",4197,21740,7031,32968,"합계"]
["COA80000860S",null,"배송관 진수","Ø860mm","SET당",4533,24340,7594,36467,"합계"]
["COB12010000S",null,"사석 / 육상투하","0.03m3이하 덤프트럭+굴삭기 투하","M3",0,132,0,132,"합계"]
["COB12020000S",null,"사석 / 육상투하","0.1m3이상 크레인 투하 (잠수조제외)","M3",0,4936,0,4936,"합계"]
["COB14010000S",null,"사석 / 해상투하","0.03m3이하 굴삭기 투하 (잠수조제외)","M3",0,2843,0,2843,"합계"]
["COB14020000S",null,"사석 / 해상투하","0.1m3이상 크레인 투하 (잠수조제외)","M3",0,7926,0,7926,"합계"]
["COB15000000S",null,"사석부설","굴삭기(1.0㎥)","M3",817,2166,753,3736,"합계"]
["COC10000000S",null,"사석 / 수상고르기","기초 고르기","M2",5204,34658,4798,44660,"합계"]
["COC30000000S",null,"사석 / 수상고르기","피복석 고르기","M2",1354,31032,2061,34447,"합계"]
["COC30100000S",null,"사석 / 수상고르기","피복석 거친 고르기","M2",1204,27776,1832,30812,"합계"]
["COC50000000S",null,"사석 / 수상고르기","내부 사석 고르기","M2",4115,27776,3794,35685,"합계"]
["COC55000000S",null,"사석고르기","굴삭기+부착용집게(1.0㎥)","M2",2118,4726,2337,9181,"합계"]
["COC70000000S",null,"사석 / 수상고르기","필타사석 고르기","M2",938,3539,864,5341,"합계"]
["COD10110000S",null,"케이슨 진수","500ton 미만","개당",0,834570,0,834570,"합계","적용수량확인"]
["COD10120000S",null,"케이슨 진수","500∼1000ton","개당",0,1197815,0,1197815,"합계","적용수량확인"]
["COD10130000S",null,"케이슨 진수","1000∼2000ton","개당",0,1726604,0,1726604,"합계","적용수량확인"]
["COD10140000S",null,"케이슨 진수","2000∼3000ton","개당",0,2395630,0,2395630,"합계","적용수량확인"]
["COD10210000S",null,"케이슨 거치","500ton 미만 (잠수조제외)","개당",0,834570,0,834570,"합계","적용수량확인"]
["COD10220000S",null,"케이슨 거치","500∼1000ton (잠수조제외)","개당",0,1280587,0,1280587,"합계","적용수량확인"]
["COD10230000S",null,"케이슨 거치","1000∼2000ton (잠수조제외)","개당",0,1809377,0,1809377,"합계","적용수량확인"]
["COD10240000S",null,"케이슨 거치","2000∼3000ton (잠수조제외)","개당",0,2255394,0,2255394,"합계","적용수량확인"]
["COD31110000S",null,"일반블록 거치 / 수상","5ton 미만 ","개당",0,51542,0,51542,"합계","적용수량확인"]
["COD31120000S",null,"일반블록 거치 / 수상","5∼10ton","개당",0,62555,0,62555,"합계","적용수량확인"]
["COD31130000S",null,"일반블록 거치 / 수상","10∼15ton","개당",0,104807,0,104807,"합계","적용수량확인"]
["COD31140000S",null,"일반블록 거치 / 수상","15∼20ton","개당",0,125616,0,125616,"합계","적용수량확인"]
["COD31150000S",null,"일반블록 거치 / 수상","20∼30ton","개당",0,269248,0,269248,"합계","적용수량확인"]
["COD31160000S",null,"일반블록 거치 / 수상","30ton 이상","개당",0,314042,0,314042,"합계","적용수량확인"]
["COD31210000S",null,"소파블럭 거치 / 수상 / 층적","2ton 미만","개당",0,28434,0,28434,"합계","적용수량확인"]
["COD31211000S",null,"소파블럭 거치 / 수상 / 난적","2ton 미만","개당",0,23623,0,23623,"합계","적용수량확인"]
["COD31220000S",null,"소파블럭 거치 / 수상 / 층적","2∼5ton ","개당",0,33955,0,33955,"합계","적용수량확인"]
["COD31221000S",null,"소파블럭 거치 / 수상 / 난적","2∼5ton ","개당",0,27888,0,27888,"합계","적용수량확인"]
["COD31230000S",null,"소파블럭 거치 / 수상 / 층적","5∼10ton ","개당",0,44618,0,44618,"합계","적용수량확인"]
["COD31231000S",null,"소파블럭 거치 / 수상 / 난적","5∼10ton ","개당",0,36419,0,36419,"합계","적용수량확인"]
["COD31240000S",null,"소파블럭 거치 / 수상 / 층적","10∼15ton ","개당",0,50636,0,50636,"합계","적용수량확인"]
["COD31241000S",null,"소파블럭 거치 / 수상 / 난적","10∼15ton ","개당",0,43196,0,43196,"합계","적용수량확인"]
["COD31250000S",null,"소파블럭 거치 / 수상 / 층적","15∼20ton ","개당",0,59166,0,59166,"합계","적용수량확인"]
["COD31251000S",null,"소파블럭 거치 / 수상 / 난적","15∼20ton ","개당",0,49049,0,49049,"합계","적용수량확인"]
["COD31260000S",null,"소파블럭 거치 / 수상 / 층적","20∼30ton ","개당",0,99246,0,99246,"합계","적용수량확인"]
["COD31261000S",null,"소파블럭 거치 / 수상 / 난적","20∼30ton ","개당",0,80706,0,80706,"합계","적용수량확인"]
["COD31270000S",null,"소파블럭 거치 / 수상 / 층적","30ton 이상","개당",0,109062,0,109062,"합계","적용수량확인"]
["COD31271000S",null,"소파블럭 거치 / 수상 / 난적","30ton 이상","개당",0,90901,0,90901,"합계","적용수량확인"]
["COD32110000S",null,"일반블록 거치 / 수중","5ton 미만 (잠수조제외)","개당",0,38571,0,38571,"합계","적용수량확인"]
["COD32120000S",null,"일반블록 거치 / 수중","5∼10ton (잠수조제외)","개당",0,44531,0,44531,"합계","적용수량확인"]
["COD32130000S",null,"일반블록 거치 / 수중","10∼15ton (잠수조제외)","개당",0,78799,0,78799,"합계","적용수량확인"]
["COD32140000S",null,"일반블록 거치 / 수중","15∼20ton (잠수조제외)","개당",0,92705,0,92705,"합계","적용수량확인"]
["COD32150000S",null,"일반블록 거치 / 수중","20∼30ton (잠수조제외)","개당",0,132436,0,132436,"합계","적용수량확인"]
["COD32160000S",null,"일반블록 거치 / 수중","30ton 이상 (잠수조제외)","개당",0,165545,0,165545,"합계","적용수량확인"]
["COD32210000S",null,"소파블럭 거치 / 수중 / 층적","2ton 미만 (잠수조제외)","개당",0,26321,0,26321,"합계","적용수량확인"]
["COD32211000S",null,"소파블럭 거치 / 수중 / 난적","2ton 미만 (잠수조제외)","개당",0,21851,0,21851,"합계","적용수량확인"]
["COD32220000S",null,"소파블럭 거치 / 수중 / 층적","2∼5ton (잠수조제외)","개당",0,30460,0,30460,"합계","적용수량확인"]
["COD32221000S",null,"소파블럭 거치 / 수중 / 난적","2∼5ton (잠수조제외)","개당",0,25825,0,25825,"합계","적용수량확인"]
["COD32230000S",null,"소파블럭 거치 / 수중 / 층적","5∼10ton (잠수조제외)","개당",0,41386,0,41386,"합계","적용수량확인"]
["COD32231000S",null,"소파블럭 거치 / 수중 / 난적","5∼10ton (잠수조제외)","개당",0,35095,0,35095,"합계","적용수량확인"]
["COD32240000S",null,"소파블럭 거치 / 수중 / 층적","10∼15ton (잠수조제외)","개당",0,48339,0,48339,"합계","적용수량확인"]
["COD32241000S",null,"소파블럭 거치 / 수중 / 난적","10∼15ton (잠수조제외)","개당",0,39896,0,39896,"합계","적용수량확인"]
["COD32250000S",null,"소파블럭 거치 / 수중 / 층적","15∼20ton (잠수조제외)","개당",0,57940,0,57940,"합계","적용수량확인"]
["COD32251000S",null,"소파블럭 거치 / 수중 / 난적","15∼20ton (잠수조제외)","개당",0,48339,0,48339,"합계","적용수량확인"]
["COD32260000S",null,"소파블럭 거치 / 수중 / 층적","20∼30ton (잠수조제외)","개당",0,92705,0,92705,"합계","적용수량확인"]
["COD32261000S",null,"소파블럭 거치 / 수중 / 난적","20∼30ton (잠수조제외)","개당",0,75322,0,75322,"합계","적용수량확인"]
["COD32270000S",null,"소파블럭 거치 / 수중 / 층적","30ton 이상 (잠수조제외)","개당",0,104293,0,104293,"합계","적용수량확인"]
["COD32271000S",null,"소파블럭 거치 / 수중 / 난적","30ton 이상 (잠수조제외)","개당",0,87738,0,87738,"합계","적용수량확인"]
["COH13000040S",null,"타원형 돌망태 설치","돌망태높이 40cm","M2",786,15159,725,16670,"합계"]
["COH13000045S",null,"타원형 돌망태 설치","돌망태높이 45cm","M2",907,17056,837,18800,"합계"]
["COH13000050S",null,"타원형 돌망태 설치","돌망태높이 50cm","M2",998,19112,920,21030,"합계"]
["COH13000060S",null,"타원형 돌망태 설치","돌망태높이 60cm","M2",1210,23935,1116,26261,"합계"]
["COH13000070S",null,"타원형 돌망태 설치","돌망태높이 70cm","M2",1391,28261,1283,30935,"합계"]
["COH18000000S",null,"매트리스형 돌망태 설치","폭 200㎝, 높이 30㎝","M2",756,12181,697,13634,"합계"]
["COH20000000S",null,"돌망태형옹벽 설치","높이 H=5m이하","M3",4447,112923,6169,123539,"합계"]
["COH60010000S",null,"블록 붙이기(인력) / 호안블록",null,"M2",0,27206,0,27206,"합계"]
["COH60021000S",null,"블록 붙이기(기계) / 호안블록","크레인(무한궤도) 10ton","M2",424,7474,646,8544,"합계"]
["COH60022000S",null,"블록 붙이기(기계) / 호안블록","굴삭기 0.2m3","M2",484,8309,821,9614,"합계"]
["COH70010000S",null,"식생매트 설치",null,"M2",0,3495,0,3495,"합계"]
["COH70020000S",null,"식생매트 설치 / 복토","굴삭기 0.6㎥","M2",490,2554,680,3724,"합계"]
["CQH00000000S",null,"녹막이 페인트칠","철재면, 1회","M2",85,4258,0,4343,"합계"]
["CRB11000035S",null,"돌쌓기 / 메쌓기","뒷길이 35cm","M2",6172,55893,10703,72768,"합계"]
["CRB11000055S",null,"돌쌓기 / 메쌓기","뒷길이 55cm","M2",5856,50534,10154,66544,"합계"]
["CRB11000075S",null,"돌쌓기 / 메쌓기","뒷길이 75cm","M2",5539,45176,9605,60320,"합계"]
["CRB21000035S",null,"돌쌓기 / 찰쌓기","뒷길이 35cm","M2",4906,48848,8507,62261,"합계"]
["CRB21000055S",null,"돌쌓기 / 찰쌓기","뒷길이 55cm","M2",4748,44046,8233,57027,"합계"]
["CRB21000075S",null,"돌쌓기 / 찰쌓기","뒷길이 75cm","M2",4431,38687,7684,50802,"합계"]
["CRB31000000S",null,"전석쌓기","전석(0.3m3~0.5m2급)","M2",6806,60923,9441,77170,"합계"]
["CRB41000035S",null,"돌붙임 / 메붙임","뒷길이 35cm","M2",3957,54208,6860,65025,"합계"]
["CRB41000055S",null,"돌붙임 / 메붙임","뒷길이 55cm","M2",3798,49406,6586,59790,"합계"]
["CRB41000075S",null,"돌붙임 / 메붙임","뒷길이 75cm","M2",3482,44047,6037,53566,"합계"]
["CRB51000035S",null,"돌붙임 / 찰붙임","뒷길이 35cm","M2",3482,47358,6037,56877,"합계"]
["CRB51000055S",null,"돌붙임 / 찰붙임","뒷길이 55cm","M2",3323,42556,5763,51642,"합계"]
["CRB51000075S",null,"돌붙임 / 찰붙임","뒷길이 75cm","M2",3165,37755,5488,46408,"합계"]
["CRB71110000S",null,"석재판붙임 / 습식공법 / 테라조판","바닥","M2",871,87188,0,88059,"합계"]
["CRB71120000S",null,"석재판붙임 / 습식공법 / 테라조판","계단부","M2",966,96611,0,97577,"합계"]
["CRB71210000S",null,"석재판붙임 / 습식공법 / 화강석","바닥","M2",1034,103446,0,104480,"합계"]
["CRB71220000S",null,"석재판붙임 / 습식공법 / 화강석","계단부","M2",1171,117114,0,118285,"합계"]
["CRB72010000S",null,"석재판붙임 / 앵커지지공법","석재판 규격 0.3m2 이하","M2",3774,125816,0,129590,"합계"]
["CRB72020000S",null,"석재판붙임 / 앵커지지공법","석재판 규격 0.3m2 초과~0.8m2 이하","M2",3563,118769,0,122332,"합계"]
["CRB73110000S",null,"석재판붙임 / 강재트러스 설치","석재판 규격 0.3m2 이하","M2",2093,69766,0,71859,"합계"]
["CRB73120000S",null,"석재판붙임 / 강재트러스 석재판붙임","석재판 규격 0.3m2 이하","M2",2736,91220,0,93956,"합계"]
["CRB73210000S",null,"석재판붙임 / 강재트러스 설치","석재판 규격 0.3m2 초과~0.8m2 이하","M2",1862,62088,0,63950,"합계"]
["CRB73220000S",null,"석재판붙임 / 강재트러스 석재판붙임","석재판 규격 0.3m2 초과~0.8m2 이하","M2",2531,84386,0,86917,"합계"]
["CRB91000000S",null,"전석깔기","전석(0.3m3~0.5m2급)","M2",2690,28316,3732,34738,"합계"]
["CRC10000000S",null,"기초지정","모래지정","M3",536,7683,766,8985,"합계"]
["CRC20000000S",null,"기초지정","자갈지정","M3",718,8642,958,10318,"합계"]
["CRC30000000S",null,"기초지정","잡석지정","M3",810,9765,1071,11646,"합계"]
["CSA11000001S",null,"교목 굴취 / 나무높이 / 인력시공","2.0m 이하","주",0,17314,0,17314,"합계"]
["CSA11000002S",null,"교목 굴취 / 나무높이 / 인력시공","3.0m 이하","주",0,26822,0,26822,"합계"]
["CSA11000003S",null,"교목 굴취 / 나무높이 / 인력시공","5.0m 이하","주",0,40289,0,40289,"합계"]
["CSA11000004S",null,"교목 굴취 / 나무높이 / 기계시공","2.0m 이하","주",1367,14022,1457,16846,"합계"]
["CSA11000005S",null,"교목 굴취 / 나무높이 / 기계시공","3.0m 이하","주",2043,21198,2178,25419,"합계"]
["CSA11000006S",null,"교목 굴취 / 나무높이 / 기계시공","5.0m 이하","주",3072,31743,3275,38090,"합계"]
["CSA12000001S",null,"교목 굴취 / 근원(흉고) / 인력시공","5cm(4cm) 이하","주",0,24184,0,24184,"합계"]
["CSA12000002S",null,"교목 굴취 / 근원(흉고) / 인력시공","6~7cm(5~6cm)","주",0,40289,0,40289,"합계"]
["CSA12000003S",null,"교목 굴취 / 근원(흉고) / 인력시공","8~9cm(7~8cm)","주",0,80632,0,80632,"합계"]
["CSA12000101S",null,"교목 굴취 / 근원(흉고) / 기계시공","5cm(4cm) 이하","주",1751,18107,1867,21725,"합계"]
["CSA12000102S",null,"교목 굴취 / 근원(흉고) / 기계시공","6~7cm(5~6cm)","주",3072,31743,3275,38090,"합계"]
["CSA12000103S",null,"교목 굴취 / 근원(흉고) / 기계시공","8~9cm(7~8cm)","주",4916,50789,5240,60945,"합계"]
["CSA12000104S",null,"교목 굴취 / 근원(흉고) / 기계시공","10~14cm(8~12cm)","주",8188,84686,8729,101603,"합계"]
["CSA12000105S",null,"교목 굴취 / 근원(흉고) / 기계시공","15~19cm(13~16cm)","주",12290,126974,13102,152366,"합계"]
["CSA12000106S",null,"교목 굴취 / 근원(흉고) / 기계시공","20~29cm(17~24cm)","주",35965,234916,49817,320698,"합계","적용장비확인"]
["CSA12000107S",null,"교목 굴취 / 근원(흉고) / 기계시공","30~39cm(25~32cm)","주",52188,329518,80132,461838,"합계","적용장비확인"]
["CSA12000108S",null,"교목 굴취 / 근원(흉고) / 기계시공","40~49cm(33~41cm)","주",65604,428835,174820,669259,"합계","적용장비확인"]
["CSA12000109S",null,"교목 굴취 / 근원(흉고) / 기계시공","50~60cm(42~50cm)","주",87581,571600,233384,892565,"합계","적용장비확인"]
["CSA21000001S",null,"교목 식재 / 나무높이 / 인력시공","2.0m 이하","주",0,30230,0,30230,"합계"]
["CSA21000002S",null,"교목 식재 / 나무높이 / 인력시공","3.0m 이하","주",0,60461,0,60461,"합계"]
["CSA21000003S",null,"교목 식재 / 나무높이 / 인력시공","5.0m 이하","주",0,100750,0,100750,"합계"]
["CSA21000011S",null,"교목 식재 / 나무높이 / 기계시공","2.0m 이하","주",2227,23130,2374,27731,"합계"]
["CSA21000012S",null,"교목 식재 / 나무높이 / 기계시공","3.0m 이하","주",4101,42288,4372,50761,"합계"]
["CSA21000013S",null,"교목 식재 / 나무높이 / 기계시공","5.0m 이하","주",6145,63487,6551,76183,"합계"]
["CSA22000001S",null,"교목 식재 / 흉고(근원) / 인력시공","5cm(6cm) 이하","주",0,40289,0,40289,"합계"]
["CSA22000002S",null,"교목 식재 / 흉고(근원) / 인력시공","6~7cm(7~8cm)","주",0,80632,0,80632,"합계"]
["CSA22000101S",null,"교목 식재 / 흉고(근원) / 기계시공","5cm(6cm) 이하","주",2734,28265,2915,33914,"합계"]
["CSA22000102S",null,"교목 식재 / 흉고(근원) / 기계시공","6~7cm(7~8cm)","주",5592,57580,5961,69133,"합계"]
["CSA22000103S",null,"교목 식재 / 흉고(근원) / 기계시공","8~9cm(9~11cm)","주",7235,74639,7714,89588,"합계"]
["CSA22000104S",null,"교목 식재 / 흉고(근원) / 기계시공","10~17cm(12~20cm)","주",10247,105775,10924,126946,"합계"]
["CSA22000105S",null,"교목 식재 / 흉고(근원) / 기계시공","18~24cm(21~29cm)","주",28078,182264,38892,249234,"합계","적용장비확인"]
["CSA22000106S",null,"교목 식재 / 흉고(근원) / 기계시공","25~34cm(30~41cm)","주",37184,234916,57094,329194,"합계","적용장비확인"]
["CSA22000107S",null,"교목 식재 / 흉고(근원) / 기계시공","35~44cm(42~53cm)","주",52483,343068,139856,535407,"합계","적용장비확인"]
["CSA22000108S",null,"교목 식재 / 흉고(근원) / 기계시공","45~50cm(54~60cm)","주",65604,428835,174820,669259,"합계","적용장비확인"]
["CSA40000003S",null,"교목 뿌리돌림","근원직경 3cm","주",0,8241,0,8241,"합계"]
["CSA40000005S",null,"교목 뿌리돌림","근원직경 5cm","주",0,14827,0,14827,"합계"]
["CSA40000007S",null,"교목 뿌리돌림","근원직경 7cm","주",0,25804,0,25804,"합계"]
["CSA40000009S",null,"교목 뿌리돌림","근원직경 9cm","주",0,40631,0,40631,"합계"]
["CSA40000011S",null,"교목 뿌리돌림","근원직경 11cm","주",0,55458,0,55458,"합계"]
["CSA40000013S",null,"교목 뿌리돌림","근원직경 13cm","주",0,70826,0,70826,"합계"]
["CSA40000015S",null,"교목 뿌리돌림","근원직경 15cm","주",0,89504,0,89504,"합계"]
["CSA40000018S",null,"교목 뿌리돌림","근원직경 18cm","주",0,132871,0,132871,"합계"]
["CSA40000021S",null,"교목 뿌리돌림","근원직경 21cm","주",0,155940,0,155940,"합계"]
["CSA40000024S",null,"교목 뿌리돌림","근원직경 24cm","주",0,177353,0,177353,"합계"]
["CSA40000030S",null,"교목 뿌리돌림","근원직경 30cm","주",0,378315,0,378315,"합계"]
["CSA40000036S",null,"교목 뿌리돌림","근원직경 36cm","주",0,444751,0,444751,"합계"]
["CSA40000042S",null,"교목 뿌리돌림","근원직경 42cm","주",0,489233,0,489233,"합계"]
["CSA40000048S",null,"교목 뿌리돌림","근원직경 48cm","주",0,555669,0,555669,"합계"]
["CSA40000054S",null,"교목 뿌리돌림","근원직경 54cm","주",0,667126,0,667126,"합계"]
["CSA40000060S",null,"교목 뿌리돌림","근원직경 60cm","주",0,733562,0,733562,"합계"]
["CSA40000066S",null,"교목 뿌리돌림","근원직경 66cm","주",0,1000420,0,1000420,"합계"]
["CSA40000072S",null,"교목 뿌리돌림","근원직경 72cm","주",0,1111878,0,1111878,"합계"]
["CSA40000078S",null,"교목 뿌리돌림","근원직경 78cm","주",0,1246404,0,1246404,"합계"]
["CSA40000084S",null,"교목 뿌리돌림","근원직경 84cm","주",0,1558284,0,1558284,"합계"]
["CSA40000090S",null,"교목 뿌리돌림","근원직경 90cm","주",0,1690616,0,1690616,"합계"]
["CSA40000100S",null,"교목 뿌리돌림","근원직경 100cm","주",0,1891578,0,1891578,"합계"]
["CSB10000001S",null,"관목 굴취 / 나무높이","0.3m 미만","주",0,1730,0,1730,"합계"]
["CSB10000002S",null,"관목 굴취 / 나무높이","0.3~0.7m 이하","주",0,3565,0,3565,"합계"]
["CSB10000003S",null,"관목 굴취 / 나무높이","0.8~1.1m 이하","주",0,5499,0,5499,"합계"]
["CSB10000004S",null,"관목 굴취 / 나무높이","1.2~1.5m 이하","주",0,8241,0,8241,"합계"]
["CSB21000001S",null,"관목 식재(단식) / 나무높이","0.3m 미만","주",0,5170,0,5170,"합계"]
["CSB21000002S",null,"관목 식재(단식) / 나무높이","0.3~0.7m 이하","주",0,6593,0,6593,"합계"]
["CSB21000003S",null,"관목 식재(단식) / 나무높이","0.8~1.1m 이하","주",0,10933,0,10933,"합계"]
["CSB21000004S",null,"관목 식재(단식) / 나무높이","1.2~1.5m 이하","주",0,15054,0,15054,"합계"]
["CSB22000001S",null,"관목 식재(군식) / 나무높이","0.3m 미만","주",0,1873,0,1873,"합계"]
["CSB22000002S",null,"관목 식재(군식) / 나무높이","0.3~0.7m 이하","주",0,2741,0,2741,"합계"]
["CSB22000003S",null,"관목 식재(군식) / 나무높이","0.8~1.1m 이하","주",0,4120,0,4120,"합계"]
["CSB22000004S",null,"관목 식재(군식) / 나무높이","1.2~1.5m 이하","주",0,5873,0,5873,"합계"]
["CSD20000001S",null,"초화류 식재","양호","주",0,304,0,304,"합계"]
["CSD20000002S",null,"초화류 식재","보통","주",0,459,0,459,"합계"]
["CSD20000003S",null,"초화류 식재","불량","주",0,749,0,749,"합계"]
["CSE51000000S",null,"잔디 붙임","줄떼","M2",0,5185,0,5185,"합계"]
["CSE52000000S",null,"잔디 붙임","평떼","M2",0,5890,0,5890,"합계"]
["CSE80000000S",null,"거적 덮기",null,"M2",0,516,0,516,"합계"]
["CSF60000000S",null,"초류종자 살포(기계살포)",null,"M2",22,317,68,407,"합계"]
["CSH10100001S",null,"정원석 쌓기 ","20ton 미만","TON",19808,302668,15195,337671,"합계"]
["CSH10100002S",null,"정원석 쌓기","20ton 이상","TON",12312,266413,22668,301393,"합계"]
["CSH10200001S",null,"정원석 놓기","20ton 미만","TON",11826,249102,21570,282498,"합계"]
["CSH10200002S",null,"정원석 놓기","20ton 이상","TON",12312,221628,21325,255265,"합계"]
["CSH10300000S",null,"조경 유용석 쌓기 및 놓기",null,"TON",9734,110973,13503,134210,"합계"]
["CSH10400000S",null,"잔디블록 포장",null,"M2",2460,23561,3230,29251,"합계"]
["CSH10500001S",null,"야자섬유매트포장","폭 1.5m 이하","M2",0,6650,0,6650,"합계"]
["CSH10500002S",null,"야자섬유매트포장","폭 2.0m 이하","M2",0,4655,0,4655,"합계"]
["CSH21111000S",null,"일반전정 / 인력시공 / 낙엽수 ","흉고직경 11cm 미만","주",507,16929,0,17436,"합계"]
["CSH21112000S",null,"일반전정 / 인력시공 / 낙엽수","흉고직경 11~21cm 미만","주",822,27427,0,28249,"합계"]
["CSH21113000S",null,"일반전정 / 인력시공 / 낙엽수","흉고직경 21~31cm 미만","주",1396,46554,0,47950,"합계"]
["CSH21121000S",null,"일반전정 / 인력시공 / 상록수","흉고직경 11cm 미만","주",290,14510,0,14800,"합계"]
["CSH21122000S",null,"일반전정 / 인력시공 / 상록수","흉고직경 11~21cm 미만","주",755,25174,0,25929,"합계"]
["CSH21123000S",null,"일반전정 / 인력시공 / 상록수","흉고직경 21~31cm 미만","주",1208,40289,0,41497,"합계"]
["CSH21212000S",null,"일반전정 / 기계시공 / 낙엽수","흉고직경 11~21cm 미만","주",1170,20584,2713,24467,"합계"]
["CSH21213000S",null,"일반전정 / 기계시공 / 낙엽수","흉고직경 21~31cm 미만","주",1807,31752,4191,37750,"합계"]
["CSH21214000S",null,"일반전정 / 기계시공 / 낙엽수","흉고직경 31~41cm 미만","주",3109,54609,7213,64931,"합계"]
["CSH21215000S",null,"일반전정 / 기계시공 / 낙엽수","흉고직경 41~51cm 미만","주",4306,75601,9991,89898,"합계"]
["CSH21216000S",null,"일반전정 / 기계시공 / 낙엽수","흉고직경 51~61cm 미만","주",7023,123635,16247,146905,"합계"]
["CSH21217000S",null,"일반전정 / 기계시공 / 낙엽수","흉고직경 61cm 초과","주",9309,163405,21608,194322,"합계"]
["CSH21222000S",null,"일반전정 / 기계시공 / 상록수","흉고직경 11~21cm 미만","주",1002,17636,2323,20961,"합계"]
["CSH21223000S",null,"일반전정 / 기계시공 / 상록수","흉고직경 21~31cm 미만","주",1602,28129,3720,33451,"합계"]
["CSH21224000S",null,"일반전정 / 기계시공 / 상록수","흉고직경 31~41cm 미만","주",2549,44784,5913,53246,"합계"]
["CSH21225000S",null,"일반전정 / 기계시공 / 상록수","흉고직경 41~51cm 미만","주",3730,65463,8659,77852,"합계"]
["CSH21226000S",null,"일반전정 / 기계시공 / 상록수","흉고직경 51~61cm 미만","주",5598,98245,12997,116840,"합계"]
["CSH21227000S",null,"일반전정 / 기계시공 / 상록수","흉고직경 61cm 초과","주",7998,140684,18521,167203,"합계"]
["CSH22111000S",null,"조형전정 / 인력시공 / 낙엽수","흉고직경 11cm 미만","주",524,26217,0,26741,"합계"]
["CSH22112000S",null,"조형전정 / 인력시공 / 낙엽수","흉고직경 11~21cm 미만","주",862,43146,0,44008,"합계"]
["CSH22113000S",null,"조형전정 / 인력시공 / 낙엽수","흉고직경 21~31cm 미만","주",1528,76404,0,77932,"합계"]
["CSH22121000S",null,"조형전정 / 인력시공 / 상록수","흉고직경 11cm 미만","주",447,22370,0,22817,"합계"]
["CSH22122000S",null,"조형전정 / 인력시공 / 상록수","흉고직경 11~21cm 미만","주",757,37870,0,38627,"합계"]
["CSH22123000S",null,"조형전정 / 인력시공 / 상록수","흉고직경 21~31cm 미만","주",1209,60461,0,61670,"합계"]
["CSH22212000S",null,"조형전정 / 기계시공 / 낙엽수","흉고직경 11~21cm 미만","주",1611,31752,4191,37554,"합계"]
["CSH22213000S",null,"조형전정 / 기계시공 / 낙엽수","흉고직경 21~31cm 미만","주",2497,49122,6498,58117,"합계"]
["CSH22214000S",null,"조형전정 / 기계시공 / 낙엽수","흉고직경 31~41cm 미만","주",4163,81905,10836,96904,"합계"]
["CSH22215000S",null,"조형전정 / 기계시공 / 낙엽수","흉고직경 41~51cm 미만","주",6259,123635,16247,146141,"합계"]
["CSH22216000S",null,"조형전정 / 기계시공 / 낙엽수","흉고직경 51~61cm 미만","주",9988,196491,25995,232474,"합계"]
["CSH22217000S",null,"조형전정 / 기계시공 / 낙엽수","흉고직경 61cm 초과","주",12485,245614,32494,290593,"합계"]
["CSH22222000S",null,"조형전정 / 기계시공 / 상록수","흉고직경 11~21cm 미만","주",1388,27414,3606,32408,"합계"]
["CSH22223000S",null,"조형전정 / 기계시공 / 상록수","흉고직경 21~31cm 미만","주",2170,42654,5653,50477,"합계"]
["CSH22224000S",null,"조형전정 / 기계시공 / 상록수","흉고직경 31~41cm 미만","주",3564,70115,9277,82956,"합계"]
["CSH22225000S",null,"조형전정 / 기계시공 / 상록수","흉고직경 41~51cm 미만","주",4994,98245,12997,116236,"합계"]
["CSH22226000S",null,"조형전정 / 기계시공 / 상록수","흉고직경 51~61cm 미만","주",7130,140684,18521,166335,"합계"]
["CSH22227000S",null,"조형전정 / 기계시공 / 상록수","흉고직경 61cm 초과","주",9988,196491,25995,232474,"합계"]
["CSH23301000S",null,"가로수 전정 / 약전정","흉고직경 11cm 미만","주",1971,37215,4191,43377,"합계"]
["CSH23302000S",null,"가로수 전정 / 약전정","흉고직경 11∼21cm 미만","주",2899,54577,6190,63666,"합계"]
["CSH23303000S",null,"가로수 전정 / 약전정","흉고직경 21∼31cm 미만","주",3809,71750,8123,83682,"합계"]
["CSH23304000S",null,"가로수 전정 / 약전정","흉고직경 31∼41cm 미만","주",5084,95811,10836,111731,"합계"]
["CSH23305000S",null,"가로수 전정 / 약전정","흉고직경 41∼51cm 미만","주",6095,114800,12997,133892,"합계"]
["CSH23306000S",null,"가로수 전정 / 약전정","흉고직경 51∼61cm 미만","주",7619,143500,16247,167366,"합계"]
["CSH23307000S",null,"가로수 전정 / 약전정","흉고직경 61cm 초과","주",8743,165515,18521,192779,"합계"]
["CSH23401000S",null,"가로수 전정 / 강전정","흉고직경 11cm 미만","주",3204,60317,6839,70360,"합계"]
["CSH23402000S",null,"가로수 전정 / 강전정","흉고직경 11~21cm 미만","주",4353,82035,9277,95665,"합계"]
["CSH23403000S",null,"가로수 전정 / 강전정","흉고직경 21∼31cm 미만","주",6095,114800,12997,133892,"합계"]
["CSH23404000S",null,"가로수 전정 / 강전정","흉고직경 31∼41cm 미만","주",7619,143500,16247,167366,"합계"]
["CSH23405000S",null,"가로수 전정 / 강전정","흉고직경 41∼51cm 미만","주",8743,165515,18521,192779,"합계"]
["CSH23406000S",null,"가로수 전정 / 강전정","흉고직경 51∼61cm 미만","주",10104,189892,21608,221604,"합계"]
["CSH23407000S",null,"가로수 전정 / 강전정","흉고직경 61cm 초과","주",12190,229600,25995,267785,"합계"]
["CSH23501000S",null,"가로수 전정 / 조형전정","흉고직경 11cm 미만","주",3591,67684,7652,78927,"합계"]
["CSH23502000S",null,"가로수 전정 / 조형전정","흉고직경 11∼21cm 미만","주",5084,95811,10836,111731,"합계"]
["CSH23503000S",null,"가로수 전정 / 조형전정","흉고직경 21∼31cm 미만","주",6752,126752,14459,147963,"합계"]
["CSH23504000S",null,"가로수 전정 / 조형전정","흉고직경 31∼41cm 미만","주",8743,165515,18521,192779,"합계"]
["CSH23505000S",null,"가로수 전정 / 조형전정","흉고직경 41∼51cm 미만","주",10104,189892,21608,221604,"합계"]
["CSH23506000S",null,"가로수 전정 / 조형전정","흉고직경 51∼61cm 미만","주",15238,287001,32494,334733,"합계"]
["CSH23507000S",null,"가로수 전정 / 조형전정","흉고직경 61cm 초과","주",20371,384108,43379,447858,"합계"]
["CSH24600000S",null,"관목 전정","나무높이 0.9M 미만","M2",39,1126,0,1165,"합계"]
["CSH24700000S",null,"관목 전정","나무높이 0.9M 이상","M2",64,1835,0,1899,"합계"]
["CSH25111000S",null,"수간보호 / 조형","흉고직경 11cm 미만","주",0,25174,0,25174,"합계"]
["CSH25112000S",null,"수간보호 / 조형","흉고직경 11~21cm 미만","주",0,46554,0,46554,"합계"]
["CSH25113000S",null,"수간보호 / 조형","흉고직경 21~31cm 미만","주",0,100588,0,100588,"합계"]
["CSH25114000S",null,"수간보호 / 조형","흉고직경 31~41cm 미만","주",0,201716,0,201716,"합계"]
["CSH25115000S",null,"수간보호 / 조형","흉고직경 41~51cm 미만","주",0,302305,0,302305,"합계"]
["CSH25121000S",null,"수간보호 / 일반","흉고직경 11cm 미만","주",0,15939,0,15939,"합계"]
["CSH25122000S",null,"수간보호 / 일반","흉고직경 11~21cm 미만","주",0,25174,0,25174,"합계"]
["CSH25123000S",null,"수간보호 / 일반","흉고직경 21~31cm 미만","주",0,37870,0,37870,"합계"]
["CSH25124000S",null,"수간보호 / 일반","흉고직경 31~41cm 미만","주",0,55019,0,55019,"합계"]
["CSH25125000S",null,"수간보호 / 일반","흉고직경 41~51cm 미만","주",0,76404,0,76404,"합계"]
["CSH25201000S",null,"줄기감싸기","흉고직경 11cm 미만","주",0,7255,0,7255,"합계"]
["CSH25202000S",null,"줄기감싸기","흉고직경 11~21cm 미만","주",0,8849,0,8849,"합계"]
["CSH25203000S",null,"줄기감싸기","흉고직경 21~31cm 미만","주",0,11268,0,11268,"합계"]
["CSH25204000S",null,"줄기감싸기","흉고직경 31~41cm 미만","주",0,14510,0,14510,"합계"]
["CSH25205000S",null,"줄기감싸기","흉고직경 41~51cm 미만","주",0,20171,0,20171,"합계"]
["CSH26101000S",null,"인력 관수","흉고직경 10cm 미만","주",0,4966,0,4966,"합계"]
["CSH26102000S",null,"인력 관수","흉고직경 10~20cm 미만","주",0,6621,0,6621,"합계"]
["CSH26103000S",null,"인력 관수","흉고직경 20~30cm 미만","주",0,9767,0,9767,"합계"]
["CSH26104000S",null,"인력 관수","흉고직경 30~40cm 미만","주",0,12746,0,12746,"합계"]
["CSH26105000S",null,"인력 관수","흉고직경 40cm 이상","주",0,16554,0,16554,"합계"]
["CSH26201000S",null,"살수차 관수 / 소형장비","1,800L, 이동거리 5km까지","M2",154,770,80,1004,"합계"]
["CSH26202000S",null,"살수차 관수 / 중형장비","3,800L, 이동거리 5km까지","M2",103,493,59,655,"합계"]
["CSH26203000S",null,"살수차 관수 / 대형장비","5,500L, 이동거리 5km까지","M2",55,246,34,335,"합계"]
["CSH27101000S",null,"제초","일반 잔디지역","M2",0,746,0,746,"합계"]
["CSH27102000S",null,"제초","지장물 지역","M2",0,1047,0,1047,"합계"]
["CSH27201100S",null,"잔디깎기 / 배부식","연3회 이상 ","M2",19,244,0,263,"합계"]
["CSH27201200S",null,"잔디깎기 / 배부식","연2회 ","M2",24,307,0,331,"합계"]
["CSH27201300S",null,"잔디깎기 / 배부식","연1회 ","M2",27,349,0,376,"합계"]
["CSH27202100S",null,"잔디깎기 / 핸드가이드식","연3회 이상 ","M2",6,94,0,100,"합계"]
["CSH27202200S",null,"잔디깎기 / 핸드가이드식","연2회 ","M2",8,117,0,125,"합계"]
["CSH27202300S",null,"잔디깎기 / 핸드가이드식","연1회 ","M2",9,136,0,145,"합계"]
["CSH27301100S",null,"예초","연3회 이상 ","M2",19,323,0,342,"합계"]
["CSH27301110S",null,"예초 / 경사도 25˚이상","연3회 이상 ","M2",21,357,0,378,"합계"]
["CSH27301200S",null,"예초","연2회 ","M2",24,404,0,428,"합계"]
["CSH27301210S",null,"예초 / 경사도 25˚이상","연2회 ","M2",27,460,0,487,"합계"]
["CSH27301300S",null,"예초","연1회 ","M2",27,460,0,487,"합계"]
["CSH27301310S",null,"예초 / 경사도 25˚이상","연1회","M2",32,539,0,571,"합계"]
["CSH28111000S",null,"교목시비 / 환상시비","근원직경 11cm 미만","주",0,7859,0,7859,"합계"]
["CSH28112000S",null,"교목시비 / 환상시비","근원직경 11~21cm 미만","주",0,9893,0,9893,"합계"]
["CSH28113000S",null,"교목시비 / 환상시비","근원직경 21~31cm 미만","주",0,11872,0,11872,"합계"]
["CSH28114000S",null,"교목시비 / 환상시비","근원직경 31~41cm 미만","주",0,13686,0,13686,"합계"]
["CSH28115000S",null,"교목시비 / 환상시비","근원직경 41~51cm 미만","주",0,15939,0,15939,"합계"]
["CSH28116000S",null,"교목시비 / 환상시비","근원직경 51cm 이상","주",0,17753,0,17753,"합계"]
["CSH28121000S",null,"교목시비 / 방사형시비","근원직경 11cm 미만","주",0,6046,0,6046,"합계"]
["CSH28122000S",null,"교목시비 / 방사형시비","근원직경 11~21cm 미만","주",0,7255,0,7255,"합계"]
["CSH28123000S",null,"교목시비 / 방사형시비","근원직경 21~31cm 미만","주",0,8684,0,8684,"합계"]
["CSH28124000S",null,"교목시비 / 방사형시비","근원직경 31~41cm 미만","주",0,10278,0,10278,"합계"]
["CSH28125000S",null,"교목시비 / 방사형시비","근원직경 41~51cm 미만","주",0,11487,0,11487,"합계"]
["CSH28126000S",null,"교목시비 / 방사형시비","근원직경 51cm 이상","주",0,13081,0,13081,"합계"]
["CSH28200000S",null,"관목시비",null,"M2",0,2017,0,2017,"합계"]
["CSH28300000S",null,"잔디시비",null,"M2",1,43,2,46,"합계"]
["CSH29100000S",null,"약제살포 / 기계","수목류 약제살포","L",22,291,19,332,"합계"]
["CSH29200000S",null,"약제살포 / 인력","잔디 약제살포","M2",0,109,0,109,"합계"]
["CSH29310000S",null,"방풍벽 설치, 거적세우기","H=0.45m","M당",0,1731,0,1731,"합계"]
["CSH29320000S",null,"방풍벽 설치, 거적세우기","H=0.9m","M당",0,2418,0,2418,"합계"]
["CSH29401000S",null,"은행나무 과실채취","흉고직경 11cm 미만","주",823,32060,2826,35709,"합계"]
["CSH29402000S",null,"은행나무 과실채취","흉고직경 11~21cm 미만","주",1220,47810,4191,53221,"합계"]
["CSH29403000S",null,"은행나무 과실채취","흉고직경 21~31cm 미만","주",1646,64340,5653,71639,"합계"]
["CSH29404000S",null,"은행나무 과실채취","흉고직경 31~41cm 미만","주",2228,87053,7652,96933,"합계"]
["CSH29405000S",null,"은행나무 과실채취","흉고직경 41~51cm 미만","주",2521,98572,8659,109752,"합계"]
["CSH29406000S",null,"은행나무 과실채취","흉고직경 51~61cm 미만","주",2701,105707,9277,117685,"합계"]
["CSH29407000S",null,"은행나무 과실채취","흉고직경 61cm 초과","주",3784,147909,12997,164690,"합계"]
["CSH29500010S",null,"가로수 제거 / 나무베기","흉고직경 11cm 미만","주",3975,37845,6364,48184,"합계"]
["CSH29500020S",null,"가로수 제거 / 나무베기","흉고직경 11~21cm 미만","주",6066,56633,10922,73621,"합계"]
["CSH29500030S",null,"가로수 제거 / 나무베기","흉고직경 21~31cm 미만","주",9699,90353,17476,117528,"합계"]
["CSH29500040S",null,"가로수 제거 / 나무베기","흉고직경 31~41cm 미만","주",14915,139040,26869,180824,"합계"]
["CSH29500050S",null,"가로수 제거 / 나무베기","흉고직경 41~51cm 미만","주",24272,226710,43691,294673,"합계"]
["CSH29500060S",null,"가로수 제거 / 나무베기","흉고직경 51~61cm 미만","주",38796,361412,69905,470113,"합계"]
["CSH29500070S",null,"가로수 제거 / 나무베기","흉고직경 61cm 이상","주",64752,603509,116654,784915,"합계"]
["CSH29500110S",null,"가로수 제거 / 뿌리제거","흉고직경 11cm 미만","주",3155,28068,5785,37008,"합계"]
["CSH29500120S",null,"가로수 제거 / 뿌리제거","흉고직경 11~21cm 미만","주",4816,41583,12676,59075,"합계"]
["CSH29500130S",null,"가로수 제거 / 뿌리제거","흉고직경 21~31cm 미만","주",8021,69271,21114,98406,"합계"]
["CSH29500140S",null,"가로수 제거 / 뿌리제거","흉고직경 31~41cm 미만","주",12040,103958,31692,147690,"합계"]
["CSH29500150S",null,"가로수 제거 / 뿌리제거","흉고직경 41~51cm 미만","주",20016,172916,52687,245619,"합계"]
["CSH29500160S",null,"가로수 제거 / 뿌리제거","흉고직경 51~61cm 미만","주",30100,259897,79230,369227,"합계"]
["CSH29500170S",null,"가로수 제거 / 뿌리제거","흉고직경 61cm 이상","주",40183,346877,105772,492832,"합계"]

{"sheet":"일위대가상세","index":1,"n_rows":16244,"n_cols":22,"rows_kept":4500,"cut":true,"hidden":false,"merged":[[1,0,1,16],[0,0,0,16],[2,8,2,9],[2,10,2,11],[2,12,2,13],[2,14,2,15],[2,0,3,0],[2,3,3,3],[2,1,3,1],[2,4,3,4],[2,5,3,5],[2,16,3,16],[2,6,3,6],[2,7,3,7],[2,2,3,2]],"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
["일 위 대 가 상 세"]
["20240200009_2024년 표준일위대가(토목)_1800507771"]
["일위대가코드","자원구분","자원코드","계산제외","품명","규격","단위","수량","재료비",null,"노무비",null,"경비",null,"합계",null,"비고",null,"관급여부","계산제외","적용요율","계산여부"]
[null,null,null,null,null,null,null,null,"단가","금액","단가","금액","단가","금액","단가","금액"]
["CAA15103000S",null,null,null,"작업대차 조립","방수 작업용 대차(L=10M)","회",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA15103000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",20,0,0,280472,5609440,0,0,280472,5609440,null,null,"N","N","",1]
["CAA15103000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4,0,0,165545,662180,0,0,165545,662180,null,null,"N","N","",1]
["CAA15103000S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,125432.4,125432.4,0,0,0,0,125432.4,125432.4,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,125432,0,6271620,0,0,0,6397052,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA15203000S",null,null,null,"작업대차 해체","방수 작업용 대차(L=10M)","회",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA15203000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",10,0,0,280472,2804720,0,0,280472,2804720,null,null,"N","N","",1]
["CAA15203000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2,0,0,165545,331090,0,0,165545,331090,null,null,"N","N","",1]
["CAA15203000S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,62716.2,62716.2,0,0,0,0,62716.2,62716.2,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,62716,0,3135810,0,0,0,3198526,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16111000S",null,null,null,"강관 지주 설치","지주높이 3.5m 이하","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16111000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.03,0,0,280472,8414.1,0,0,280472,8414.1,null,null,"N","N","",1]
["CAA16111000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.0999999999999999E-2,0,0,165545,1820.9,0,0,165545,1820.9,null,null,"N","N","",1]
["CAA16111000S","기계경비","00000201002000000",null,"굴삭기(무한궤도)","0.2㎥","HR",3.5000000000000003E-2,7695,269.3,55700,1949.5,13041,456.4,76436,2675.2,null,null,"N","N","",1]
["CAA16111000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,307,307,0,0,0,0,307,307,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,576,0,12184,0,456,0,13216,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16113000S",null,null,null,"강관 지주 설치","지주높이 6m 이하","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16113000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",4.5999999999999999E-2,0,0,280472,12901.7,0,0,280472,12901.7,null,null,"N","N","",1]
["CAA16113000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.6E-2,0,0,165545,2648.7,0,0,165545,2648.7,null,null,"N","N","",1]
["CAA16113000S","기계경비","00000201002000000",null,"굴삭기(무한궤도)","0.2㎥","HR",3.5000000000000003E-2,7695,269.3,55700,1949.5,13041,456.4,76436,2675.2,null,null,"N","N","",1]
["CAA16113000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,466.5,466.5,0,0,0,0,466.5,466.5,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,735,0,17499,0,456,0,18690,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16121000S",null,null,null,"강관 지주 해체","지주높이 3.5m 이하","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16121000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",1.2E-2,0,0,280472,3365.6,0,0,280472,3365.6,null,null,"N","N","",1]
["CAA16121000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.0000000000000001E-3,0,0,165545,662.1,0,0,165545,662.1,null,null,"N","N","",1]
["CAA16121000S","기계경비","00000201002000000",null,"굴삭기(무한궤도)","0.2㎥","HR",1.4E-2,7695,107.7,55700,779.8,13041,182.5,76436,1070,null,null,"N","N","",1]
["CAA16121000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,120.8,120.8,0,0,0,0,120.8,120.8,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,228,0,4807,0,182,0,5217,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16123000S",null,null,null,"강관 지주 해체","지주높이 6m 이하","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16123000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",1.7999999999999999E-2,0,0,280472,5048.3999999999996,0,0,280472,5048.3999999999996,null,null,"N","N","",1]
["CAA16123000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.0000000000000001E-3,0,0,165545,993.2,0,0,165545,993.2,null,null,"N","N","",1]
["CAA16123000S","기계경비","00000201002000000",null,"굴삭기(무한궤도)","0.2㎥","HR",1.4E-2,7695,107.7,55700,779.8,13041,182.5,76436,1070,null,null,"N","N","",1]
["CAA16123000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,181.2,181.2,0,0,0,0,181.2,181.2,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,288,0,6821,0,182,0,7291,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16212000S",null,null,null,"H형강 지주 설치","지주높이 4m 이하","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16212000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",4.9000000000000002E-2,0,0,280472,13743.1,0,0,280472,13743.1,null,null,"N","N","",1]
["CAA16212000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.7999999999999999E-2,0,0,165545,2979.8,0,0,165545,2979.8,null,null,"N","N","",1]
["CAA16212000S","기계경비","00000201002000000",null,"굴삭기(무한궤도)","0.2㎥","HR",6.3E-2,7695,484.7,55700,3509.1,13041,821.5,76436,4815.3,null,null,"N","N","",1]
["CAA16212000S","기계경비","00002105000500000",null,"트럭탑재형 크레인","5ton","HR",7.2999999999999995E-2,7784,568.20000000000005,47231,3447.8,9994,729.5,65009,4745.5,null,null,"N","N","",1]
["CAA16212000S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,334.4,334.4,0,0,0,0,334.4,334.4,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,1387,0,23679,0,1551,0,26617,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16214000S",null,null,null,"H형강 지주 설치","지주높이 7m 이하","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16214000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",9.9000000000000005E-2,0,0,280472,27766.7,0,0,280472,27766.7,null,null,"N","N","",1]
["CAA16214000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.5000000000000003E-2,0,0,165545,5794,0,0,165545,5794,null,null,"N","N","",1]
["CAA16214000S","기계경비","00000201002000000",null,"굴삭기(무한궤도)","0.2㎥","HR",6.3E-2,7695,484.7,55700,3509.1,13041,821.5,76436,4815.3,null,null,"N","N","",1]
["CAA16214000S","기계경비","00002105000500000",null,"트럭탑재형 크레인","5ton","HR",0.109,7784,848.4,47231,5148.1000000000004,9994,1089.3,65009,7085.8,null,null,"N","N","",1]
["CAA16214000S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,671.2,671.2,0,0,0,0,671.2,671.2,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,2004,0,42217,0,1910,0,46131,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16222000S",null,null,null,"H형강 지주 해체","지주높이 4m 이하","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16222000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.02,0,0,280472,5609.4,0,0,280472,5609.4,null,null,"N","N","",1]
["CAA16222000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.0000000000000001E-3,0,0,165545,1158.8,0,0,165545,1158.8,null,null,"N","N","",1]
["CAA16222000S","기계경비","00000201002000000",null,"굴삭기(무한궤도)","0.2㎥","HR",2.5000000000000001E-2,7695,192.3,55700,1392.5,13041,326,76436,1910.8,null,null,"N","N","",1]
["CAA16222000S","기계경비","00002105000500000",null,"트럭탑재형 크레인","5ton","HR",2.9000000000000001E-2,7784,225.7,47231,1369.6,9994,289.8,65009,1885.1,null,null,"N","N","",1]
["CAA16222000S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,135.30000000000001,135.30000000000001,0,0,0,0,135.30000000000001,135.30000000000001,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,553,0,9530,0,615,0,10698,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16224000S",null,null,null,"H형강 지주 해체","지주높이 7m 이하","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16224000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.04,0,0,280472,11218.8,0,0,280472,11218.8,null,null,"N","N","",1]
["CAA16224000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.4E-2,0,0,165545,2317.6,0,0,165545,2317.6,null,null,"N","N","",1]
["CAA16224000S","기계경비","00000201002000000",null,"굴삭기(무한궤도)","0.2㎥","HR",2.5000000000000001E-2,7695,192.3,55700,1392.5,13041,326,76436,1910.8,null,null,"N","N","",1]
["CAA16224000S","기계경비","00002105000500000",null,"트럭탑재형 크레인","5ton","HR",4.3999999999999997E-2,7784,342.4,47231,2078.1,9994,439.7,65009,2860.2,null,null,"N","N","",1]
["CAA16224000S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,270.7,270.7,0,0,0,0,270.7,270.7,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,805,0,17007,0,765,0,18577,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16311000S",null,null,null,"가설울타리판 설치","설치높이 3m 이하","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16311000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",2.5999999999999999E-2,0,0,280472,7292.2,0,0,280472,7292.2,null,null,"N","N","",1]
["CAA16311000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",8.9999999999999993E-3,0,0,165545,1489.9,0,0,165545,1489.9,null,null,"N","N","",1]
["CAA16311000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,263.39999999999998,263.39999999999998,0,0,0,0,263.39999999999998,263.39999999999998,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,263,0,8782,0,0,0,9045,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16313000S",null,null,null,"가설울타리판 설치","설치높이 6m 이하","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16313000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.03,0,0,280472,8414.1,0,0,280472,8414.1,null,null,"N","N","",1]
["CAA16313000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.0999999999999999E-2,0,0,165545,1820.9,0,0,165545,1820.9,null,null,"N","N","",1]
["CAA16313000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,307,307,0,0,0,0,307,307,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,307,0,10235,0,0,0,10542,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16321000S",null,null,null,"가설울타리판 해체","설치높이 3m 이하","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16321000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.01,0,0,280472,2804.7,0,0,280472,2804.7,null,null,"N","N","",1]
["CAA16321000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.0000000000000001E-3,0,0,165545,662.1,0,0,165545,662.1,null,null,"N","N","",1]
["CAA16321000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,104,104,0,0,0,0,104,104,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,104,0,3466,0,0,0,3570,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16323000S",null,null,null,"가설울타리판 해체","설치높이 6m 이하","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16323000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",1.2E-2,0,0,280472,3365.6,0,0,280472,3365.6,null,null,"N","N","",1]
["CAA16323000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.0000000000000001E-3,0,0,165545,827.7,0,0,165545,827.7,null,null,"N","N","",1]
["CAA16323000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,125.7,125.7,0,0,0,0,125.7,125.7,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,125,0,4193,0,0,0,4318,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16411000S",null,null,null,"세로형 가설방음판 설치","설치높이 3m 이하","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16411000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",2.4E-2,0,0,280472,6731.3,0,0,280472,6731.3,null,null,"N","N","",1]
["CAA16411000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",8.9999999999999993E-3,0,0,165545,1489.9,0,0,165545,1489.9,null,null,"N","N","",1]
["CAA16411000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,246.6,246.6,0,0,0,0,246.6,246.6,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,246,0,8221,0,0,0,8467,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16412000S",null,null,null,"세로형 가설방음판 설치","설치높이 6m 이하","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16412000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",2.8000000000000001E-2,0,0,280472,7853.2,0,0,280472,7853.2,null,null,"N","N","",1]
["CAA16412000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.01,0,0,165545,1655.4,0,0,165545,1655.4,null,null,"N","N","",1]
["CAA16412000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,285.2,285.2,0,0,0,0,285.2,285.2,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,285,0,9508,0,0,0,9793,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16421000S",null,null,null,"세로형 가설방음판 해체","설치높이 3m 이하","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16421000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.01,0,0,280472,2804.7,0,0,280472,2804.7,null,null,"N","N","",1]
["CAA16421000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.0000000000000001E-3,0,0,165545,496.6,0,0,165545,496.6,null,null,"N","N","",1]
["CAA16421000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,99,99,0,0,0,0,99,99,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,99,0,3301,0,0,0,3400,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16422000S",null,null,null,"세로형 가설방음판 해체","설치높이 6m 이하","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16422000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",1.0999999999999999E-2,0,0,280472,3085.1,0,0,280472,3085.1,null,null,"N","N","",1]
["CAA16422000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.0000000000000001E-3,0,0,165545,662.1,0,0,165545,662.1,null,null,"N","N","",1]
["CAA16422000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,112.4,112.4,0,0,0,0,112.4,112.4,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,112,0,3747,0,0,0,3859,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16511000S",null,null,null,"가로형 가설방음판 설치","설치높이 3m 이하","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16511000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",7.1999999999999995E-2,0,0,280472,20193.900000000001,0,0,280472,20193.900000000001,null,null,"N","N","",1]
["CAA16511000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5999999999999999E-2,0,0,165545,4304.1000000000004,0,0,165545,4304.1000000000004,null,null,"N","N","",1]
["CAA16511000S","기계경비","00002105000500000",null,"트럭탑재형 크레인","5ton","HR",9.5000000000000001E-2,7784,739.4,47231,4486.8999999999996,9994,949.4,65009,6175.7,null,null,"N","N","",1]
["CAA16511000S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,489.9,489.9,0,0,0,0,489.9,489.9,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,1229,0,28984,0,949,0,31162,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16512000S",null,null,null,"가로형 가설방음판 설치","설치높이 6m 이하","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16512000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",8.4000000000000005E-2,0,0,280472,23559.599999999999,0,0,280472,23559.599999999999,null,null,"N","N","",1]
["CAA16512000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.03,0,0,165545,4966.3,0,0,165545,4966.3,null,null,"N","N","",1]
["CAA16512000S","기계경비","00002105000500000",null,"트럭탑재형 크레인","5ton","HR",0.111,7784,864,47231,5242.6000000000004,9994,1109.3,65009,7215.9,null,null,"N","N","",1]
["CAA16512000S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,570.5,570.5,0,0,0,0,570.5,570.5,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,1434,0,33768,0,1109,0,36311,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16521000S",null,null,null,"가로형 가설방음판 해체","설치높이 3m 이하","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16521000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",2.9000000000000001E-2,0,0,280472,8133.6,0,0,280472,8133.6,null,null,"N","N","",1]
["CAA16521000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.01,0,0,165545,1655.4,0,0,165545,1655.4,null,null,"N","N","",1]
["CAA16521000S","기계경비","00002105000500000",null,"트럭탑재형 크레인","5ton","HR",3.7999999999999999E-2,7784,295.7,47231,1794.7,9994,379.7,65009,2470.1,null,null,"N","N","",1]
["CAA16521000S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,195.7,195.7,0,0,0,0,195.7,195.7,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,491,0,11583,0,379,0,12453,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16522000S",null,null,null,"가로형 가설방음판 해체","설치높이 6m 이하","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA16522000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",3.4000000000000002E-2,0,0,280472,9536,0,0,280472,9536,null,null,"N","N","",1]
["CAA16522000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.2E-2,0,0,165545,1986.5,0,0,165545,1986.5,null,null,"N","N","",1]
["CAA16522000S","기계경비","00002105000500000",null,"트럭탑재형 크레인","5ton","HR",4.3999999999999997E-2,7784,342.4,47231,2078.1,9994,439.7,65009,2860.2,null,null,"N","N","",1]
["CAA16522000S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,230.4,230.4,0,0,0,0,230.4,230.4,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,572,0,13600,0,439,0,14611,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA18110000S",null,null,null,"비탈면 보양",null,"M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA18110000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.02,0,0,214222,4284.3999999999996,0,0,214222,4284.3999999999996,null,null,"N","N","",1]
["CAA18110000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.01,0,0,165545,1655.4,0,0,165545,1655.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,5939,0,0,0,5939,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA23110000S",null,null,null,"P.P. 마대 만들기","0.024m3/개","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA23110000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.4999999999999999E-2,0,0,165545,2483.1,0,0,165545,2483.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,2483,0,0,0,2483,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA23120000S",null,null,null,"P.P. 마대 쌓기","0.024m3/개","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA23120000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.0000000000000001E-3,0,0,165545,993.2,0,0,165545,993.2,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,993,0,0,0,993,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA23130000S",null,null,null,"P.P. 마대 헐기","0.024m3/개","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA23130000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.0000000000000001E-3,0,0,165545,993.2,0,0,165545,993.2,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,993,0,0,0,993,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA23210000S",null,null,null,"톤 마대 만들기","0.7m3/개","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA23210000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.7999999999999999E-2,0,0,165545,6290.7,0,0,165545,6290.7,null,null,"N","N","",1]
["CAA23210000S","기계경비","00000201002000000",null,"굴삭기(무한궤도)","0.2㎥","HR",0.13400000000000001,7695,1031.0999999999999,55700,7463.8,13041,1747.4,76436,10242.299999999999,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,1031,0,13754,0,1747,0,16532,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA23220000S",null,null,null,"톤 마대 쌓기","0.7m3/개","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA23220000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.7999999999999999E-2,0,0,165545,2979.8,0,0,165545,2979.8,null,null,"N","N","",1]
["CAA23220000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",8.9999999999999993E-3,0,0,214222,1927.9,0,0,214222,1927.9,null,null,"N","N","",1]
["CAA23220000S","기계경비","00000201010000000",null,"굴삭기(무한궤도)","1.0㎥","HR",7.0000000000000007E-2,30260,2118.1999999999998,55700,3899,27901,1953,113861,7970.2,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,2118,0,8806,0,1953,0,12877,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA23230000S",null,null,null,"톤 마대 헐기","0.7m3/개","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA23230000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.7999999999999999E-2,0,0,165545,2979.8,0,0,165545,2979.8,null,null,"N","N","",1]
["CAA23230000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",8.9999999999999993E-3,0,0,214222,1927.9,0,0,214222,1927.9,null,null,"N","N","",1]
["CAA23230000S","기계경비","00000201010000000",null,"굴삭기(무한궤도)","1.0㎥","HR",7.0000000000000007E-2,30260,2118.1999999999998,55700,3899,27901,1953,113861,7970.2,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,2118,0,8806,0,1953,0,12877,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA26110000S",null,null,null,"타워크레인 방호울타리 설치 및 해체","높이 2.0m 기준","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA26110000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.12,0,0,280472,33656.6,0,0,280472,33656.6,null,null,"N","N","",1]
["CAA26110000S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,673.1,673.1,0,0,0,0,673.1,673.1,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,673,0,33656,0,0,0,34329,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA26120000S",null,null,null,"건설용리프트 방호선반 설치 및 해체","싱글 1.2ton","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA26120000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.95,0,0,280472,266448.40000000002,0,0,280472,266448.40000000002,null,null,"N","N","",1]
["CAA26120000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.26,0,0,165545,43041.7,0,0,165545,43041.7,null,null,"N","N","",1]
["CAA26120000S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,6189.8,6189.8,0,0,0,0,6189.8,6189.8,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,6189,0,309490,0,0,0,315679,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA26130000S",null,null,null,"보행자 안전통로 설치 및 해체","높이 3.0m이하, 폭 2.0m 기준","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA26130000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.2,0,0,280472,56094.400000000001,0,0,280472,56094.400000000001,null,null,"N","N","",1]
["CAA26130000S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,1121.8,1121.8,0,0,0,0,1121.8,1121.8,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,1121,0,56094,0,0,0,57215,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA26140000S",null,null,null,"PE드럼 설치 및 해체",null,"개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA26140000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.06,0,0,214222,12853.3,0,0,214222,12853.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,12853,0,0,0,12853,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA26150000S",null,null,null,"PE가설방호벽 설치 및 해체",null,"개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA26150000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.09,0,0,214222,19279.900000000001,0,0,214222,19279.900000000001,null,null,"N","N","",1]
["CAA26150000S","기계경비","00007204001800000",null,"물탱크(살수차)","1800L","HR",0.03,13559,406.7,47231,1416.9,7041,211.2,67831,2034.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,406,0,20696,0,211,0,21313,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA26160000S",null,null,null,"PC가설방호벽 설치 및 해체",null,"개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA26160000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.12,0,0,214222,25706.6,0,0,214222,25706.6,null,null,"N","N","",1]
["CAA26160000S","기계경비","00002105000500000",null,"트럭탑재형 크레인","5ton","HR",0.21,7784,1634.6,47231,9918.5,9994,2098.6999999999998,65009,13651.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,1634,0,35625,0,2098,0,39357,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA26170000S",null,null,null,"가설휀스(H-Beam기초) 설치 및 해체",null,"M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA26170000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.01,0,0,214222,2142.1999999999998,0,0,214222,2142.1999999999998,null,null,"N","N","",1]
["CAA26170000S","기계경비","00002105000500000",null,"트럭탑재형 크레인","5ton","HR",0.02,7784,155.6,47231,944.6,9994,199.8,65009,1300,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,155,0,3086,0,199,0,3440,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA26180000S",null,null,null,"PE가설휀스 설치 및 해체",null,"개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA26180000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.02,0,0,214222,4284.3999999999996,0,0,214222,4284.3999999999996,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,4284,0,0,0,4284,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA26190000S",null,null,null,"가림막 가설휀스 설치 및 해체",null,"개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA26190000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.04,0,0,214222,8568.7999999999993,0,0,214222,8568.7999999999993,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,8568,0,0,0,8568,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA26210000S",null,null,null,"점멸등 설치 및 해체",null,"개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA26210000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.01,0,0,214222,2142.1999999999998,0,0,214222,2142.1999999999998,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,2142,0,0,0,2142,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA26220000S",null,null,null,"유도등 설치 및 해체",null,"M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA26220000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.01,0,0,214222,2142.1999999999998,0,0,214222,2142.1999999999998,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,2142,0,0,0,2142,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA27100000S",null,null,null,"낙하물 방지망(비계) 설치 및 해체","수평방향 3m 이하","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA27100000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.03,0,0,280472,8414.1,0,0,280472,8414.1,null,null,"N","N","",1]
["CAA27100000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.01,0,0,165545,1655.4,0,0,165545,1655.4,null,null,"N","N","",1]
["CAA27100000S","손료","RENT000000000001",null,"공구손료","인력품의 3%","식",1,302,302,0,0,0,0,302,302,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,302,0,10069,0,0,0,10371,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA27200000S",null,null,null,"낙하물 방지망(플라잉넷) 설치 및 해체","수평방향 3m 이하","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA27200000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.02,0,0,280472,5609.4,0,0,280472,5609.4,null,null,"N","N","",1]
["CAA27200000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.01,0,0,165545,1655.4,0,0,165545,1655.4,null,null,"N","N","",1]
["CAA27200000S","손료","RENT000000000001",null,"공구손료","인력품의 3%","식",1,217.9,217.9,0,0,0,0,217.9,217.9,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,217,0,7264,0,0,0,7481,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA27300000S",null,null,null,"낙하물 방지망(시스템방호) 설치 및 해체","수평방향 4m 이하","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA27300000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",2.5000000000000001E-2,0,0,280472,7011.8,0,0,280472,7011.8,null,null,"N","N","",1]
["CAA27300000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.01,0,0,165545,1655.4,0,0,165545,1655.4,null,null,"N","N","",1]
["CAA27300000S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,173.3,173.3,0,0,0,0,173.3,173.3,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,173,0,8667,0,0,0,8840,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA27400000S",null,null,null,"교량 방호선반 설치 및 해체",null,"M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA27400000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",2.5000000000000001E-2,0,0,280472,7011.8,0,0,280472,7011.8,null,null,"N","N","",1]
["CAA27400000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.2E-2,0,0,165545,1986.5,0,0,165545,1986.5,null,null,"N","N","",1]
["CAA27400000S","손료","RENT000000000001",null,"공구손료 및 경장비의 기계경비","인력품의 3%","식",1,269.89999999999998,269.89999999999998,0,0,0,0,269.89999999999998,269.89999999999998,null,null,"N","N",3,1]
["CAA27400000S","기계경비","00002105000500000",null,"트럭탑재형 크레인","5ton","HR",0.01,7784,77.8,47231,472.3,9994,99.9,65009,650,null,null,"N","N","",1]
["CAA27400000S","기계경비","00002106000500000",null,"고소작업차","5ton","HR",4.2999999999999997E-2,7784,334.7,47231,2030.9,34765,1494.8,89780,3860.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,682,0,11501,0,1594,0,13777,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA27500000S",null,null,null,"교량 낙하물방지망 설치 및 해체",null,"M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA27500000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",1.4E-2,0,0,280472,3926.6,0,0,280472,3926.6,null,null,"N","N","",1]
["CAA27500000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.0000000000000001E-3,0,0,165545,1158.8,0,0,165545,1158.8,null,null,"N","N","",1]
["CAA27500000S","손료","RENT000000000001",null,"공구손료 및 경장비의 기계경비","인력품의 3%","식",1,0,0,0,0,152.5,152.5,152.5,152.5,null,null,"N","N",3,1]
["CAA27500000S","기계경비","00002106000500000",null,"고소작업차","5ton","HR",3.3000000000000002E-2,7784,256.8,47231,1558.6,34765,1147.2,89780,2962.6,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,256,0,6644,0,1299,0,8199,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA27600000S",null,null,null,"철골 안전망 설치 및 해체",null,"M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA27600000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",1.7000000000000001E-2,0,0,280472,4768,0,0,280472,4768,null,null,"N","N","",1]
["CAA27600000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.0000000000000001E-3,0,0,165545,827.7,0,0,165545,827.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,5595,0,0,0,5595,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA27700000S",null,null,null,"비계주위 보호망 설치 및 해체",null,"M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA27700000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.01,0,0,280472,2804.7,0,0,280472,2804.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,2804,0,0,0,2804,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA27800000S",null,null,null,"갱폼주위 보호망 설치 및 해체",null,"M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA27800000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",4.0000000000000001E-3,0,0,280472,1121.8,0,0,280472,1121.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,1121,0,0,0,1121,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA27910000S",null,null,null,"수직형 추락방망 설치 및 해체","개구부 면적 1.0m2 이하","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA27910000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",4.9000000000000002E-2,0,0,280472,13743.1,0,0,280472,13743.1,null,null,"N","N","",1]
["CAA27910000S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,274.8,274.8,0,0,0,0,274.8,274.8,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,274,0,13743,0,0,0,14017,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA27920000S",null,null,null,"수직형 추락방망 설치 및 해체","개구부 면적 1.0~3.0m2 이하","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA27920000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",6.3E-2,0,0,280472,17669.7,0,0,280472,17669.7,null,null,"N","N","",1]
["CAA27920000S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,353.3,353.3,0,0,0,0,353.3,353.3,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,353,0,17669,0,0,0,18022,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA27930000S",null,null,null,"수직형 추락방망 설치 및 해체","개구부 면적 3.0~6.0m2 이하","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA27930000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.10100000000000001,0,0,280472,28327.599999999999,0,0,280472,28327.599999999999,null,null,"N","N","",1]
["CAA27930000S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,566.5,566.5,0,0,0,0,566.5,566.5,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,566,0,28327,0,0,0,28893,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA27940000S",null,null,null,"수직형 추락방망 설치 및 해체","개구부 면적 6.0~9.0m2 이하","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA27940000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.13,0,0,280472,36461.300000000003,0,0,280472,36461.300000000003,null,null,"N","N","",1]
["CAA27940000S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,729.2,729.2,0,0,0,0,729.2,729.2,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,729,0,36461,0,0,0,37190,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA27950000S",null,null,null,"수직형 추락방망 설치 및 해체","개구부 면적 9.0~12.0m2 이하","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA27950000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.16,0,0,280472,44875.5,0,0,280472,44875.5,null,null,"N","N","",1]
["CAA27950000S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,897.5,897.5,0,0,0,0,897.5,897.5,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,897,0,44875,0,0,0,45772,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28011100S",null,null,null,"안전난간대 설치 및 해체","브라켓형 2단, 난간기둥 간격 1.0m이하","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28011100S","노무","L001010101000006",null,"비계공","일반공사 직종","인",5.6000000000000001E-2,0,0,280472,15706.4,0,0,280472,15706.4,null,null,"N","Y","",0]
["CAA28011100S","손료","RENT000000000001",null,"요율적용","인력품의 110%","식",1,0,0,17277,17277,0,0,17277,17277,null,null,"N","N",110,1]
["CAA28011100S","손료","RENT000000000002",null,"공구손료","인력품의 2%","식",1,345.5,345.5,0,0,0,0,345.5,345.5,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,345,0,17277,0,0,0,17622,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28011200S",null,null,null,"안전난간대 설치 및 해체","브라켓형 2단, 난간기둥 간격 1.5m이하","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28011200S","노무","L001010101000006",null,"비계공","일반공사 직종","인",5.6000000000000001E-2,0,0,280472,15706.4,0,0,280472,15706.4,null,null,"N","Y","",0]
["CAA28011200S","손료","RENT000000000001",null,"요율적용","인력품의 100%","식",1,0,0,15706.4,15706.4,0,0,15706.4,15706.4,null,null,"N","N",100,1]
["CAA28011200S","손료","RENT000000000002",null,"공구손료","인력품의 2%","식",1,314.10000000000002,314.10000000000002,0,0,0,0,314.10000000000002,314.10000000000002,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,314,0,15706,0,0,0,16020,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28011300S",null,null,null,"안전난간대 설치 및 해체","브라켓형 2단, 난간기둥 간격 1.5m초과","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28011300S","노무","L001010101000006",null,"비계공","일반공사 직종","인",5.6000000000000001E-2,0,0,280472,15706.4,0,0,280472,15706.4,null,null,"N","Y","",0]
["CAA28011300S","손료","RENT000000000001",null,"요율적용","인력품의 90%","식",1,0,0,14135.7,14135.7,0,0,14135.7,14135.7,null,null,"N","N",90,1]
["CAA28011300S","손료","RENT000000000002",null,"공구손료","인력품의 2%","식",1,282.7,282.7,0,0,0,0,282.7,282.7,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,282,0,14135,0,0,0,14417,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28012100S",null,null,null,"안전난간대 설치 및 해체","브라켓형 3단, 난간기둥 간격 1.0m이하","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28012100S","노무","L001010101000006",null,"비계공","일반공사 직종","인",6.2E-2,0,0,280472,17389.2,0,0,280472,17389.2,null,null,"N","Y","",0]
["CAA28012100S","손료","RENT000000000001",null,"요율적용","인력품의 110%","식",1,0,0,19128.099999999999,19128.099999999999,0,0,19128.099999999999,19128.099999999999,null,null,"N","N",110,1]
["CAA28012100S","손료","RENT000000000002",null,"공구손료","인력품의 2%","식",1,382.5,382.5,0,0,0,0,382.5,382.5,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,382,0,19128,0,0,0,19510,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28012200S",null,null,null,"안전난간대 설치 및 해체","브라켓형 3단, 난간기둥 간격 1.5m이하","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28012200S","노무","L001010101000006",null,"비계공","일반공사 직종","인",6.2E-2,0,0,280472,17389.2,0,0,280472,17389.2,null,null,"N","Y","",0]
["CAA28012200S","손료","RENT000000000001",null,"요율적용","인력품의 100%","식",1,0,0,17389.2,17389.2,0,0,17389.2,17389.2,null,null,"N","N",100,1]
["CAA28012200S","손료","RENT000000000002",null,"공구손료","인력품의 2%","식",1,347.7,347.7,0,0,0,0,347.7,347.7,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,347,0,17389,0,0,0,17736,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28012300S",null,null,null,"안전난간대 설치 및 해체","브라켓형 3단, 난간기둥 간격 1.5m초과","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28012300S","노무","L001010101000006",null,"비계공","일반공사 직종","인",6.2E-2,0,0,280472,17389.2,0,0,280472,17389.2,null,null,"N","Y","",0]
["CAA28012300S","손료","RENT000000000001",null,"요율적용","인력품의 90%","식",1,0,0,15650.2,15650.2,0,0,15650.2,15650.2,null,null,"N","N",90,1]
["CAA28012300S","손료","RENT000000000002",null,"공구손료","인력품의 2%","식",1,313,313,0,0,0,0,313,313,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,313,0,15650,0,0,0,15963,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28021100S",null,null,null,"안전난간대 설치 및 해체","앵커형 2단, 난간기둥 간격 1.0m이하","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28021100S","노무","L001010101000006",null,"비계공","일반공사 직종","인",6.4000000000000001E-2,0,0,280472,17950.2,0,0,280472,17950.2,null,null,"N","Y","",0]
["CAA28021100S","손료","RENT000000000001",null,"요율적용","인력품의 110%","식",1,0,0,19745.2,19745.2,0,0,19745.2,19745.2,null,null,"N","N",110,1]
["CAA28021100S","손료","RENT000000000002",null,"공구손료","인력품의 2%","식",1,394.9,394.9,0,0,0,0,394.9,394.9,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,394,0,19745,0,0,0,20139,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28021200S",null,null,null,"안전난간대 설치 및 해체","앵커형 2단, 난간기둥 간격 1.5m이하","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28021200S","노무","L001010101000006",null,"비계공","일반공사 직종","인",6.4000000000000001E-2,0,0,280472,17950.2,0,0,280472,17950.2,null,null,"N","Y","",0]
["CAA28021200S","손료","RENT000000000001",null,"요율적용","인력품의 100%","식",1,0,0,17950.2,17950.2,0,0,17950.2,17950.2,null,null,"N","N",100,1]
["CAA28021200S","손료","RENT000000000002",null,"공구손료","인력품의 2%","식",1,359,359,0,0,0,0,359,359,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,359,0,17950,0,0,0,18309,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28021300S",null,null,null,"안전난간대 설치 및 해체","앵커형 2단, 난간기둥 간격 1.5m초과","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28021300S","노무","L001010101000006",null,"비계공","일반공사 직종","인",6.4000000000000001E-2,0,0,280472,17950.2,0,0,280472,17950.2,null,null,"N","Y","",0]
["CAA28021300S","손료","RENT000000000001",null,"요율적용","인력품의 90%","식",1,0,0,16155.1,16155.1,0,0,16155.1,16155.1,null,null,"N","N",90,1]
["CAA28021300S","손료","RENT000000000002",null,"공구손료","인력품의 2%","식",1,323.10000000000002,323.10000000000002,0,0,0,0,323.10000000000002,323.10000000000002,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,323,0,16155,0,0,0,16478,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28022100S",null,null,null,"안전난간대 설치 및 해체","앵커형 3단, 난간기둥 간격 1.0m이하","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28022100S","노무","L001010101000006",null,"비계공","일반공사 직종","인",7.0000000000000007E-2,0,0,280472,19633,0,0,280472,19633,null,null,"N","Y","",0]
["CAA28022100S","손료","RENT000000000001",null,"요율적용","인력품의 110%","식",1,0,0,21596.3,21596.3,0,0,21596.3,21596.3,null,null,"N","N",110,1]
["CAA28022100S","손료","RENT000000000002",null,"공구손료","인력품의 2%","식",1,431.9,431.9,0,0,0,0,431.9,431.9,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,431,0,21596,0,0,0,22027,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28022200S",null,null,null,"안전난간대 설치 및 해체","앵커형 3단, 난간기둥 간격 1.5m이하","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28022200S","노무","L001010101000006",null,"비계공","일반공사 직종","인",7.0000000000000007E-2,0,0,280472,19633,0,0,280472,19633,null,null,"N","Y","",0]
["CAA28022200S","손료","RENT000000000001",null,"요율적용","인력품의 100%","식",1,0,0,19633,19633,0,0,19633,19633,null,null,"N","N",100,1]
["CAA28022200S","손료","RENT000000000002",null,"공구손료","인력품의 2%","식",1,392.6,392.6,0,0,0,0,392.6,392.6,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,392,0,19633,0,0,0,20025,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28022300S",null,null,null,"안전난간대 설치 및 해체","앵커형 3단, 난간기둥 간격 1.5m초과","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28022300S","노무","L001010101000006",null,"비계공","일반공사 직종","인",7.0000000000000007E-2,0,0,280472,19633,0,0,280472,19633,null,null,"N","Y","",0]
["CAA28022300S","손료","RENT000000000001",null,"요율적용","인력품의 90%","식",1,0,0,17669.7,17669.7,0,0,17669.7,17669.7,null,null,"N","N",90,1]
["CAA28022300S","손료","RENT000000000002",null,"공구손료","인력품의 2%","식",1,353.3,353.3,0,0,0,0,353.3,353.3,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,353,0,17669,0,0,0,18022,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28110000S",null,null,null,"계단난간대 설치 및 해체","브라켓형, 난간대 길이 2.5m이하, 2단 기준","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28110000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.14000000000000001,0,0,280472,39266,0,0,280472,39266,null,null,"N","N","",1]
["CAA28110000S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,785.3,785.3,0,0,0,0,785.3,785.3,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,785,0,39266,0,0,0,40051,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28120000S",null,null,null,"계단난간대 설치 및 해체","앵커형, 난간대 길이 2.5m이하, 2단 기준","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28120000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.14499999999999999,0,0,280472,40668.400000000001,0,0,280472,40668.400000000001,null,null,"N","N","",1]
["CAA28120000S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,813.3,813.3,0,0,0,0,813.3,813.3,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,813,0,40668,0,0,0,41481,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28211000S",null,null,null,"안전난간대 설치 및 해체(토목)","2단, 지주 간격 1.0m이하","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28211000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",6.2E-2,0,0,280472,17389.2,0,0,280472,17389.2,null,null,"N","Y","",0]
["CAA28211000S","손료","RENT000000000001",null,"요율적용","인력품의 110%","식",1,0,0,19128.099999999999,19128.099999999999,0,0,19128.099999999999,19128.099999999999,null,null,"N","N",110,1]
["CAA28211000S","손료","RENT000000000002",null,"공구손료 및 경장비의 기계경비","인력품의 2%","식",1,382.5,382.5,0,0,0,0,382.5,382.5,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,382,0,19128,0,0,0,19510,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28212000S",null,null,null,"안전난간대 설치 및 해체(토목)","2단, 지주 간격 1.5m이하","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28212000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",6.2E-2,0,0,280472,17389.2,0,0,280472,17389.2,null,null,"N","Y","",0]
["CAA28212000S","손료","RENT000000000001",null,"요율적용","인력품의 100%","식",1,0,0,17389.2,17389.2,0,0,17389.2,17389.2,null,null,"N","N",100,1]
["CAA28212000S","손료","RENT000000000002",null,"공구손료 및 경장비의 기계경비","인력품의 2%","식",1,347.7,347.7,0,0,0,0,347.7,347.7,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,347,0,17389,0,0,0,17736,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28213000S",null,null,null,"안전난간대 설치 및 해체(토목)","2단, 지주 간격 1.5m초과","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28213000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",6.2E-2,0,0,280472,17389.2,0,0,280472,17389.2,null,null,"N","Y","",0]
["CAA28213000S","손료","RENT000000000001",null,"요율적용","인력품의 90%","식",1,0,0,15650.2,15650.2,0,0,15650.2,15650.2,null,null,"N","N",90,1]
["CAA28213000S","손료","RENT000000000002",null,"공구손료 및 경장비의 기계경비","인력품의 2%","식",1,313,313,0,0,0,0,313,313,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,313,0,15650,0,0,0,15963,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28221000S",null,null,null,"안전난간대 설치 및 해체(토목)","3단, 지주 간격 1.0m이하","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28221000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",6.7000000000000004E-2,0,0,280472,18791.599999999999,0,0,280472,18791.599999999999,null,null,"N","Y","",0]
["CAA28221000S","손료","RENT000000000001",null,"요율적용","노무비의 110%","식",1,0,0,20670.7,20670.7,0,0,20670.7,20670.7,null,null,"N","N",110,1]
["CAA28221000S","손료","RENT000000000002",null,"공구손료 및 경장비의 기계경비","노무비의 2%","식",1,413.4,413.4,0,0,0,0,413.4,413.4,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,413,0,20670,0,0,0,21083,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28222000S",null,null,null,"안전난간대 설치 및 해체(토목)","3단, 지주 간격 1.5m이하","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28222000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",6.7000000000000004E-2,0,0,280472,18791.599999999999,0,0,280472,18791.599999999999,null,null,"N","Y","",0]
["CAA28222000S","손료","RENT000000000001",null,"요율적용","노무비의 100%","식",1,0,0,18791.599999999999,18791.599999999999,0,0,18791.599999999999,18791.599999999999,null,null,"N","N",100,1]
["CAA28222000S","손료","RENT000000000002",null,"공구손료 및 경장비의 기계경비","노무비의 2%","식",1,375.8,375.8,0,0,0,0,375.8,375.8,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,375,0,18791,0,0,0,19166,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28223000S",null,null,null,"안전난간대 설치 및 해체(토목)","3단, 지주 간격 1.5m초과","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28223000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",6.7000000000000004E-2,0,0,280472,18791.599999999999,0,0,280472,18791.599999999999,null,null,"N","Y","",0]
["CAA28223000S","손료","RENT000000000001",null,"요율적용","노무비의 90%","식",1,0,0,16912.400000000001,16912.400000000001,0,0,16912.400000000001,16912.400000000001,null,null,"N","N",90,1]
["CAA28223000S","손료","RENT000000000002",null,"공구손료 및 경장비의 기계경비","노무비의 2%","식",1,338.2,338.2,0,0,0,0,338.2,338.2,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,338,0,16912,0,0,0,17250,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28300000S",null,null,null,"엘리베이터 난간틀 설치 및 해체","난간틀 높이 1.4m이하, 길이 1.3m이하 기준","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28300000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.08,0,0,280472,22437.7,0,0,280472,22437.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,22437,0,0,0,22437,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28400000S",null,null,null,"엘리베이터 추락방호망 설치 및 해체","추락방호망 5~9m2이하 기준","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28400000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.15,0,0,280472,42070.8,0,0,280472,42070.8,null,null,"N","N","",1]
["CAA28400000S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,841.4,841.4,0,0,0,0,841.4,841.4,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,841,0,42070,0,0,0,42911,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28510000S",null,null,null,"개구부 수평보호덮개 설치 및 해체","개당 1.0M2이하","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28510000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.05,0,0,280472,14023.6,0,0,280472,14023.6,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,14023,0,0,0,14023,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28520000S",null,null,null,"개구부 수평보호덮개 설치 및 해체","개당 3.0M2이하","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28520000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",7.0000000000000007E-2,0,0,280472,19633,0,0,280472,19633,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,19633,0,0,0,19633,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28600000S",null,null,null,"강재거푸집 작업용 난간 설치 및 해체",null,"M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28600000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",8.2000000000000003E-2,0,0,280472,22998.7,0,0,280472,22998.7,null,null,"N","N","",1]
["CAA28600000S","손료","RENT000000000001",null,"공구손료 및 경장비의 기계경비","인력품의 3%","식",1,689.9,689.9,0,0,0,0,689.9,689.9,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,689,0,22998,0,0,0,23687,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28700000S",null,null,null,"수평지지로프 설치 및 해체",null,"M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA28700000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.02,0,0,280472,5609.4,0,0,280472,5609.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,5609,0,0,0,5609,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA29010000S",null,null,null,"비계주위 보호막 설치 및 해체",null,"M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA29010000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.02,0,0,280472,5609.4,0,0,280472,5609.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,5609,0,0,0,5609,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA29020000S",null,null,null,"방진망 설치 및 해체",null,"M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA29020000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",1.6E-2,0,0,280472,4487.5,0,0,280472,4487.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,4487,0,0,0,4487,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA29031000S",null,null,null,"터널방음문 설치",null,"개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA29031000S","노무","L001010101000009",null,"철공","일반공사 직종","인",2.81,0,0,233754,656848.69999999995,0,0,233754,656848.69999999995,null,null,"N","N","",1]
["CAA29031000S","노무","L001010101000012",null,"용접공","일반공사 직종","인",1.1299999999999999,0,0,267021,301733.7,0,0,267021,301733.7,null,null,"N","N","",1]
["CAA29031000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.1299999999999999,0,0,165545,187065.8,0,0,165545,187065.8,null,null,"N","N","",1]
["CAA29031000S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,22912.9,22912.9,0,0,0,0,22912.9,22912.9,null,null,"N","N",2,1]
["CAA29031000S","기계경비","00002104005000000",null,"크레인(타이어)","50ton","HR",8,19970,159760,55700,445600,86876,695008,162546,1300368,null,null,"N","N","",1]
["CAA29031000S","기계경비","00002104001000000",null,"크레인(타이어)","10ton","HR",8,6718,53744,55700,445600,30103,240824,92521,740168,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,236416,0,2036848,0,935832,0,3209096,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA29032000S",null,null,null,"터널방음문 해체",null,"개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA29032000S","노무","L001010101000009",null,"철공","일반공사 직종","인",2.5299999999999998,0,0,233754,591397.6,0,0,233754,591397.6,null,null,"N","N","",1]
["CAA29032000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.02,0,0,165545,168855.9,0,0,165545,168855.9,null,null,"N","N","",1]
["CAA29032000S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,15205,15205,0,0,0,0,15205,15205,null,null,"N","N",2,1]
["CAA29032000S","기계경비","00002104005000000",null,"크레인(타이어)","50ton","HR",5.6,19970,111832,55700,311920,86876,486505.6,162546,910257.6,null,null,"N","N","",1]
["CAA29032000S","기계경비","00002104001000000",null,"크레인(타이어)","10ton","HR",5.6,6718,37620.800000000003,55700,311920,30103,168576.8,92521,518117.6,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,164657,0,1384093,0,655082,0,2203832,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA29041100S",null,null,null,"박스형 간이흙막이 설치 및 해체","설치깊이 3.0m 이하","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA29041100S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.17,0,0,214222,36417.699999999997,0,0,214222,36417.699999999997,null,null,"N","N","",1]
["CAA29041100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.06,0,0,165545,9932.7000000000007,0,0,165545,9932.7000000000007,null,null,"N","N","",1]
["CAA29041100S","기계경비","00002104001000000",null,"크레인(타이어)","10ton","HR",0.26,6718,1746.6,55700,14482,30103,7826.7,92521,24055.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,1746,0,60832,0,7826,0,70404,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA29041200S",null,null,null,"박스형 간이흙막이 설치 및 해체","설치깊이 4.0m 이하","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA29041200S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.24,0,0,214222,51413.2,0,0,214222,51413.2,null,null,"N","N","",1]
["CAA29041200S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.09,0,0,165545,14899,0,0,165545,14899,null,null,"N","N","",1]
["CAA29041200S","기계경비","00002104001000000",null,"크레인(타이어)","10ton","HR",0.44,6718,2955.9,55700,24508,30103,13245.3,92521,40709.199999999997,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,2955,0,90820,0,13245,0,107020,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA29042100S",null,null,null,"조립식 간이흙막이 설치 및 해체","설치깊이 H=3.0m 이하","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA29042100S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.19,0,0,214222,40702.1,0,0,214222,40702.1,null,null,"N","N","",1]
["CAA29042100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.0000000000000007E-2,0,0,165545,11588.1,0,0,165545,11588.1,null,null,"N","N","",1]
["CAA29042100S","기계경비","00002104001000000",null,"크레인(타이어)","10ton","HR",0.46,6718,3090.2,55700,25622,30103,13847.3,92521,42559.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,3090,0,77912,0,13847,0,94849,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA29042200S",null,null,null,"조립식 간이흙막이 설치 및 해체","설치깊이 H=4.0m 이하","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA29042200S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.28000000000000003,0,0,214222,59982.1,0,0,214222,59982.1,null,null,"N","N","",1]
["CAA29042200S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.1,0,0,165545,16554.5,0,0,165545,16554.5,null,null,"N","N","",1]
["CAA29042200S","기계경비","00002104001000000",null,"크레인(타이어)","10ton","HR",0.9,6718,6046.2,55700,50130,30103,27092.7,92521,83268.899999999994,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,6046,0,126666,0,27092,0,159804,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA29042300S",null,null,null,"조립식 간이흙막이 설치 및 해체","설치깊이 H=5.0m 이하","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA29042300S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.4,0,0,214222,85688.8,0,0,214222,85688.8,null,null,"N","N","",1]
["CAA29042300S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.15,0,0,165545,24831.7,0,0,165545,24831.7,null,null,"N","N","",1]
["CAA29042300S","기계경비","00002104001000000",null,"크레인(타이어)","10ton","HR",1.48,6718,9942.6,55700,82436,30103,44552.4,92521,136931,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,9942,0,192956,0,44552,0,247450,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA29042400S",null,null,null,"조립식 간이흙막이 설치 및 해체","설치깊이 H=6.0m 이하","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA29042400S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.56999999999999995,0,0,214222,122106.5,0,0,214222,122106.5,null,null,"N","N","",1]
["CAA29042400S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.22,0,0,165545,36419.9,0,0,165545,36419.9,null,null,"N","N","",1]
["CAA29042400S","기계경비","00002104001000000",null,"크레인(타이어)","10ton","HR",2.2000000000000002,6718,14779.6,55700,122540,30103,66226.600000000006,92521,203546.2,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,14779,0,281066,0,66226,0,362071,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA31110000S",null,null,null,"강관비계 설치 및 해체","H=10m 이하 ","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA31110000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.05,0,0,280472,14023.6,0,0,280472,14023.6,null,null,"N","N","",1]
["CAA31110000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.02,0,0,165545,3310.9,0,0,165545,3310.9,null,null,"N","N","",1]
["CAA31110000S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,346.6,346.6,0,0,0,0,346.6,346.6,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,346,0,17334,0,0,0,17680,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA31120000S",null,null,null,"강관비계 설치 및 해체","H=10m 초과, 20m 이하 ","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA31120000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.06,0,0,280472,16828.3,0,0,280472,16828.3,null,null,"N","N","",1]
["CAA31120000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.02,0,0,165545,3310.9,0,0,165545,3310.9,null,null,"N","N","",1]
["CAA31120000S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,402.7,402.7,0,0,0,0,402.7,402.7,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,402,0,20139,0,0,0,20541,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA31130000S",null,null,null,"강관비계 설치 및 해체","H=20m 초과, 30m 이하 ","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA31130000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",7.0000000000000007E-2,0,0,280472,19633,0,0,280472,19633,null,null,"N","N","",1]
["CAA31130000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.02,0,0,165545,3310.9,0,0,165545,3310.9,null,null,"N","N","",1]
["CAA31130000S","손료","RENT000000000001",null,"공구손료","합계의 2%","식",1,458.8,458.8,0,0,0,0,458.8,458.8,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,458,0,22943,0,0,0,23401,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA31210000S",null,null,null,"시스템 비계 설치 및 해체","H=10m 이하 ","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA31210000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.04,0,0,280472,11218.8,0,0,280472,11218.8,null,null,"N","N","",1]
["CAA31210000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.01,0,0,165545,1655.4,0,0,165545,1655.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,12874,0,0,0,12874,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA31220000S",null,null,null,"시스템 비계 설치 및 해체","H=10m 초과, 20m 이하 ","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA31220000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.05,0,0,280472,14023.6,0,0,280472,14023.6,null,null,"N","N","",1]
["CAA31220000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.01,0,0,165545,1655.4,0,0,165545,1655.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,15679,0,0,0,15679,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA31230000S",null,null,null,"시스템 비계 설치 및 해체","H=20m 초과, 30m 이하 ","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA31230000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.06,0,0,280472,16828.3,0,0,280472,16828.3,null,null,"N","N","",1]
["CAA31230000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.01,0,0,165545,1655.4,0,0,165545,1655.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,18483,0,0,0,18483,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA31310000S",null,null,null,"강관틀 비계 설치 및 해체","10m 이하","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA31310000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.02,0,0,280472,5609.4,0,0,280472,5609.4,null,null,"N","N","",1]
["CAA31310000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.01,0,0,165545,1655.4,0,0,165545,1655.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,7264,0,0,0,7264,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA31320000S",null,null,null,"강관틀 비계 설치 및 해체","10m 초과, 20m 이하","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA31320000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.03,0,0,280472,8414.1,0,0,280472,8414.1,null,null,"N","N","",1]
["CAA31320000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.01,0,0,165545,1655.4,0,0,165545,1655.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,10069,0,0,0,10069,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA31410000S",null,null,null,"강관 조립말비계(이동식) 설치 및 해체","높이 2.0m","대당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA31410000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.25,0,0,280472,70118,0,0,280472,70118,null,null,"N","N","",1]
["CAA31410000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.14000000000000001,0,0,165545,23176.3,0,0,165545,23176.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,93294,0,0,0,93294,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA31420000S",null,null,null,"강관 조립말비계(이동식) 설치 및 해체","높이 4.0m","대당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA31420000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.41,0,0,280472,114993.5,0,0,280472,114993.5,null,null,"N","N","",1]
["CAA31420000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.24,0,0,165545,39730.800000000003,0,0,165545,39730.800000000003,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,154724,0,0,0,154724,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA31500000S",null,null,null,"경사형 가설 계단 설치 및 해체","높이 6m 이하, 계단폭 0.9m 이하","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA31500000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.27,0,0,280472,75727.399999999994,0,0,280472,75727.399999999994,null,null,"N","N","",1]
["CAA31500000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.09,0,0,165545,14899,0,0,165545,14899,null,null,"N","N","",1]
["CAA31500000S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,1812.5,1812.5,0,0,0,0,1812.5,1812.5,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,1812,0,90626,0,0,0,92438,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA31600000S",null,null,null,"타워형 가설 계단 설치 및 해체","계단폭 0.9m 이하","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA31600000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.2,0,0,280472,56094.400000000001,0,0,280472,56094.400000000001,null,null,"N","N","",1]
["CAA31600000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.0000000000000007E-2,0,0,165545,11588.1,0,0,165545,11588.1,null,null,"N","N","",1]
["CAA31600000S","기계경비","00002104001000000",null,"크레인(타이어)","10ton","HR",0.06,6718,403,55700,3342,30103,1806.1,92521,5551.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,403,0,71024,0,1806,0,73233,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA31711000S",null,null,null,"비계용 브라켓 설치","벽체용","개소당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA31711000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",4.4999999999999998E-2,0,0,280472,12621.2,0,0,280472,12621.2,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,12621,0,0,0,12621,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA31712000S",null,null,null,"비계용 브라켓 설치","슬라브, 발코니난간용","개소당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA31712000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",3.4000000000000002E-2,0,0,280472,9536,0,0,280472,9536,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,9536,0,0,0,9536,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA31721000S",null,null,null,"비계용 브라켓 해체","벽체용","개소당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA31721000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",3.4000000000000002E-2,0,0,280472,9536,0,0,280472,9536,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,9536,0,0,0,9536,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA31722000S",null,null,null,"비계용 브라켓 해체","슬라브, 발코니난간용","개소당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA31722000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",2.5999999999999999E-2,0,0,280472,7292.2,0,0,280472,7292.2,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,7292,0,0,0,7292,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32100000S",null,null,null,"강관동바리 수평연결재 설치, 해체","1단설치","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32100000S","노무","L001010101000007",null,"형틀목공","일반공사 직종","인",0.02,0,0,274978,5499.5,0,0,274978,5499.5,null,null,"N","N","",1]
["CAA32100000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.01,0,0,165545,1655.4,0,0,165545,1655.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,7154,0,0,0,7154,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32111000S",null,null,null,"강관동바리 설치 및 해체(토목) (H=2.5m 이하) ","설치간격 0.6m 이하","공M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32111000S","노무","L001010101000007",null,"형틀목공","일반공사 직종","인",5.3999999999999999E-2,0,0,274978,14848.8,0,0,274978,14848.8,null,null,"N","Y","",0]
["CAA32111000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.1000000000000001E-2,0,0,165545,3476.4,0,0,165545,3476.4,null,null,"N","Y","",0]
["CAA32111000S","손료","RENT000000000001",null,"요율적용","인력품의 120%","식",1,0,0,21990.2,21990.2,0,0,21990.2,21990.2,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,21990,0,0,0,21990,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32112000S",null,null,null,"강관동바리 설치 및 해체(토목) (H=2.5m 이하) ","설치간격 0.6m 초과~0.8m 이하","공M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32112000S","노무","L001010101000007",null,"형틀목공","일반공사 직종","인",5.3999999999999999E-2,0,0,274978,14848.8,0,0,274978,14848.8,null,null,"N","N","",1]
["CAA32112000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.1000000000000001E-2,0,0,165545,3476.4,0,0,165545,3476.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,18325,0,0,0,18325,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32113000S",null,null,null,"강관동바리 설치 및 해체(토목) (H=2.5m 이하) ","설치간격 0.8m 초과","공M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32113000S","노무","L001010101000007",null,"형틀목공","일반공사 직종","인",5.3999999999999999E-2,0,0,274978,14848.8,0,0,274978,14848.8,null,null,"N","Y","",0]
["CAA32113000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.1000000000000001E-2,0,0,165545,3476.4,0,0,165545,3476.4,null,null,"N","Y","",0]
["CAA32113000S","손료","RENT000000000001",null,"요율적용","인력품의 90%","식",1,0,0,16492.599999999999,16492.599999999999,0,0,16492.599999999999,16492.599999999999,null,null,"N","N",90,1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,16492,0,0,0,16492,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32121000S",null,null,null,"강관동바리 설치 및 해체(토목) (H=2.5m 초과, 3.5m 이하) ","설치간격 0.6m 이하","공M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32121000S","노무","L001010101000007",null,"형틀목공","일반공사 직종","인",5.8000000000000003E-2,0,0,274978,15948.7,0,0,274978,15948.7,null,null,"N","Y","",0]
["CAA32121000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.3E-2,0,0,165545,3807.5,0,0,165545,3807.5,null,null,"N","Y","",0]
["CAA32121000S","손료","RENT000000000001",null,"요율적용","인력품의 120%","식",1,0,0,23707.4,23707.4,0,0,23707.4,23707.4,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,23707,0,0,0,23707,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32122000S",null,null,null,"강관동바리 설치 및 해체(토목) (H=2.5m 초과, 3.5m 이하) ","설치간격 0.6m 초과~0.8m 이하","공M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32122000S","노무","L001010101000007",null,"형틀목공","일반공사 직종","인",5.8000000000000003E-2,0,0,274978,15948.7,0,0,274978,15948.7,null,null,"N","N","",1]
["CAA32122000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.3E-2,0,0,165545,3807.5,0,0,165545,3807.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,19756,0,0,0,19756,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32123000S",null,null,null,"강관동바리 설치 및 해체(토목) (H=2.5m 초과, 3.5m 이하) ","설치간격 0.8m 초과","공M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32123000S","노무","L001010101000007",null,"형틀목공","일반공사 직종","인",5.8000000000000003E-2,0,0,274978,15948.7,0,0,274978,15948.7,null,null,"N","Y","",0]
["CAA32123000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.3E-2,0,0,165545,3807.5,0,0,165545,3807.5,null,null,"N","Y","",0]
["CAA32123000S","손료","RENT000000000001",null,"요율적용","인력품의 90%","식",1,0,0,17780.5,17780.5,0,0,17780.5,17780.5,null,null,"N","N",90,1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,17780,0,0,0,17780,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32131000S",null,null,null,"강관동바리 설치 및 해체(토목) (H=3.5m 초과, 4.5m 이하) ","설치간격 0.6m 이하","공M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32131000S","노무","L001010101000007",null,"형틀목공","일반공사 직종","인",6.3E-2,0,0,274978,17323.599999999999,0,0,274978,17323.599999999999,null,null,"N","Y","",0]
["CAA32131000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5000000000000001E-2,0,0,165545,4138.6000000000004,0,0,165545,4138.6000000000004,null,null,"N","Y","",0]
["CAA32131000S","손료","RENT000000000001",null,"요율적용","인력품의 120%","식",1,0,0,25754.6,25754.6,0,0,25754.6,25754.6,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,25754,0,0,0,25754,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32132000S",null,null,null,"강관동바리 설치 및 해체(토목) (H=3.5m 초과, 4.5m 이하) ","설치간격 0.6m 초과~0.8m 이하","공M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32132000S","노무","L001010101000007",null,"형틀목공","일반공사 직종","인",6.3E-2,0,0,274978,17323.599999999999,0,0,274978,17323.599999999999,null,null,"N","N","",1]
["CAA32132000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5000000000000001E-2,0,0,165545,4138.6000000000004,0,0,165545,4138.6000000000004,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,21462,0,0,0,21462,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32133000S",null,null,null,"강관동바리 설치 및 해체(토목) (H=3.5m 초과, 4.5m 이하) ","설치간격 0.8m 초과","공M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32133000S","노무","L001010101000007",null,"형틀목공","일반공사 직종","인",6.3E-2,0,0,274978,17323.599999999999,0,0,274978,17323.599999999999,null,null,"N","Y","",0]
["CAA32133000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5000000000000001E-2,0,0,165545,4138.6000000000004,0,0,165545,4138.6000000000004,null,null,"N","Y","",0]
["CAA32133000S","손료","RENT000000000001",null,"요율적용","인력품의 90%","식",1,0,0,19315.900000000001,19315.900000000001,0,0,19315.900000000001,19315.900000000001,null,null,"N","N",90,1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,19315,0,0,0,19315,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32311000S",null,null,null,"시스템 동바리 설치 및 해체 (H=10m 이하)","설치간격 0.6m 이하","공M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32311000S","노무","L001010101000007",null,"형틀목공","일반공사 직종","인",5.8000000000000003E-2,0,0,274978,15948.7,0,0,274978,15948.7,null,null,"N","Y","",0]
["CAA32311000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.7999999999999999E-2,0,0,165545,2979.8,0,0,165545,2979.8,null,null,"N","Y","",0]
["CAA32311000S","손료","RENT000000000001",null,"요율적용","인력품의 120%","식",1,0,0,22714.2,22714.2,0,0,22714.2,22714.2,null,null,"N","N",120,1]
["CAA32311000S","기계경비","00002104001500000",null,"크레인(타이어)","15ton","HR",1.7000000000000001E-2,8309,141.19999999999999,55700,946.9,40854,694.5,104863,1782.6,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,141,0,23661,0,694,0,24496,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32312000S",null,null,null,"시스템 동바리 설치 및 해체 (H=10m 이하)","설치간격 0.6m 초과~1.2m 이하","공M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32312000S","노무","L001010101000007",null,"형틀목공","일반공사 직종","인",5.8000000000000003E-2,0,0,274978,15948.7,0,0,274978,15948.7,null,null,"N","N","",1]
["CAA32312000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.7999999999999999E-2,0,0,165545,2979.8,0,0,165545,2979.8,null,null,"N","N","",1]
["CAA32312000S","기계경비","00002104001500000",null,"크레인(타이어)","15ton","HR",1.7000000000000001E-2,8309,141.19999999999999,55700,946.9,40854,694.5,104863,1782.6,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,141,0,19875,0,694,0,20710,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32313000S",null,null,null,"시스템 동바리 설치 및 해체 (H=10m 이하)","설치간격 1.2m 초과","공M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32313000S","노무","L001010101000007",null,"형틀목공","일반공사 직종","인",5.8000000000000003E-2,0,0,274978,15948.7,0,0,274978,15948.7,null,null,"N","Y","",0]
["CAA32313000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.7999999999999999E-2,0,0,165545,2979.8,0,0,165545,2979.8,null,null,"N","Y","",0]
["CAA32313000S","손료","RENT000000000001",null,"요율적용","인력품의 90%","식",1,0,0,17035.599999999999,17035.599999999999,0,0,17035.599999999999,17035.599999999999,null,null,"N","N",90,1]
["CAA32313000S","기계경비","00002104001500000",null,"크레인(타이어)","15ton","HR",1.7000000000000001E-2,8309,141.19999999999999,55700,946.9,40854,694.5,104863,1782.6,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,141,0,17982,0,694,0,18817,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32321000S",null,null,null,"시스템 동바리 설치 및 해체 (H=10m 초과, 20m 이하)","설치간격 0.6m 이하","공M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32321000S","노무","L001010101000007",null,"형틀목공","일반공사 직종","인",6.8000000000000005E-2,0,0,274978,18698.5,0,0,274978,18698.5,null,null,"N","Y","",0]
["CAA32321000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.1000000000000001E-2,0,0,165545,3476.4,0,0,165545,3476.4,null,null,"N","Y","",0]
["CAA32321000S","손료","RENT000000000001",null,"요율적용","인력품의 120%","식",1,0,0,26609.8,26609.8,0,0,26609.8,26609.8,null,null,"N","N",120,1]
["CAA32321000S","기계경비","00002104001500000",null,"크레인(타이어)","15ton","HR",2.5000000000000001E-2,8309,207.7,55700,1392.5,40854,1021.3,104863,2621.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,207,0,28002,0,1021,0,29230,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32322000S",null,null,null,"시스템 동바리 설치 및 해체 (H=10m 초과, 20m 이하)","설치간격 0.6m 초과~1.2m 이하","공M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32322000S","노무","L001010101000007",null,"형틀목공","일반공사 직종","인",6.8000000000000005E-2,0,0,274978,18698.5,0,0,274978,18698.5,null,null,"N","N","",1]
["CAA32322000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.1000000000000001E-2,0,0,165545,3476.4,0,0,165545,3476.4,null,null,"N","N","",1]
["CAA32322000S","기계경비","00002104001500000",null,"크레인(타이어)","15ton","HR",2.5000000000000001E-2,8309,207.7,55700,1392.5,40854,1021.3,104863,2621.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,207,0,23567,0,1021,0,24795,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32323000S",null,null,null,"시스템 동바리 설치 및 해체 (H=10m 초과, 20m 이하)","설치간격 1.2m 초과","공M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32323000S","노무","L001010101000007",null,"형틀목공","일반공사 직종","인",6.8000000000000005E-2,0,0,274978,18698.5,0,0,274978,18698.5,null,null,"N","Y","",0]
["CAA32323000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.1000000000000001E-2,0,0,165545,3476.4,0,0,165545,3476.4,null,null,"N","Y","",0]
["CAA32323000S","손료","RENT000000000001",null,"요율적용","인력품의 90%","식",1,0,0,19957.400000000001,19957.400000000001,0,0,19957.400000000001,19957.400000000001,null,null,"N","N",90,1]
["CAA32323000S","기계경비","00002104001500000",null,"크레인(타이어)","15ton","HR",2.5000000000000001E-2,8309,207.7,55700,1392.5,40854,1021.3,104863,2621.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,207,0,21349,0,1021,0,22577,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32331000S",null,null,null,"시스템 동바리 설치 및 해체 (H=20m 초과, 30m 이하)","설치간격 0.6m 이하","공M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32331000S","노무","L001010101000007",null,"형틀목공","일반공사 직종","인",8.6999999999999994E-2,0,0,274978,23923,0,0,274978,23923,null,null,"N","Y","",0]
["CAA32331000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.7E-2,0,0,165545,4469.7,0,0,165545,4469.7,null,null,"N","Y","",0]
["CAA32331000S","손료","RENT000000000001",null,"요율적용","인력품의 120%","식",1,0,0,34071.199999999997,34071.199999999997,0,0,34071.199999999997,34071.199999999997,null,null,"N","N",120,1]
["CAA32331000S","기계경비","00002104002000000",null,"크레인(타이어)","20ton","HR",2.8000000000000001E-2,9547,267.3,55700,1559.6,51286,1436,116533,3262.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,267,0,35630,0,1436,0,37333,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32332000S",null,null,null,"시스템 동바리 설치 및 해체 (H=20m 초과, 30m 이하)","설치간격 0.6m 초과~1.2m 이하","공M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32332000S","노무","L001010101000007",null,"형틀목공","일반공사 직종","인",8.6999999999999994E-2,0,0,274978,23923,0,0,274978,23923,null,null,"N","N","",1]
["CAA32332000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.7E-2,0,0,165545,4469.7,0,0,165545,4469.7,null,null,"N","N","",1]
["CAA32332000S","기계경비","00002104002000000",null,"크레인(타이어)","20ton","HR",2.8000000000000001E-2,9547,267.3,55700,1559.6,51286,1436,116533,3262.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,267,0,29952,0,1436,0,31655,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32333000S",null,null,null,"시스템 동바리 설치 및 해체 (H=20m 초과, 30m 이하)","설치간격 1.2m 초과","공M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32333000S","노무","L001010101000007",null,"형틀목공","일반공사 직종","인",8.6999999999999994E-2,0,0,274978,23923,0,0,274978,23923,null,null,"N","Y","",0]
["CAA32333000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.7E-2,0,0,165545,4469.7,0,0,165545,4469.7,null,null,"N","Y","",0]
["CAA32333000S","손료","RENT000000000001",null,"요율적용","인력품의 90%","식",1,0,0,25553.4,25553.4,0,0,25553.4,25553.4,null,null,"N","N",90,1]
["CAA32333000S","기계경비","00002104002000000",null,"크레인(타이어)","20ton","HR",2.8000000000000001E-2,9547,267.3,55700,1559.6,51286,1436,116533,3262.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,267,0,27113,0,1436,0,28816,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32400000S",null,null,null,"알루미늄 폼 동바리 설치 및 해체",null,"M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32400000S","노무","L001010101000007",null,"형틀목공","일반공사 직종","인",0.03,0,0,274978,8249.2999999999993,0,0,274978,8249.2999999999993,null,null,"N","N","",1]
["CAA32400000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.01,0,0,165545,1655.4,0,0,165545,1655.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,9904,0,0,0,9904,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32500000S",null,null,null,"잭서포트 설치 및 해체","설치높이 5m이하","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA32500000S","노무","L001010101000007",null,"형틀목공","일반공사 직종","인",0.06,0,0,274978,16498.599999999999,0,0,274978,16498.599999999999,null,null,"N","N","",1]
["CAA32500000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.02,0,0,165545,3310.9,0,0,165545,3310.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,19809,0,0,0,19809,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA41100000S",null,null,null,"토공의 비탈 규준틀 설치 및 철거",null,"개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA41100000S","노무","L001010101000023",null,"건축목공","일반공사 직종","인",0.16,0,0,268058,42889.2,0,0,268058,42889.2,null,null,"N","N","",1]
["CAA41100000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.14000000000000001,0,0,165545,23176.3,0,0,165545,23176.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,66065,0,0,0,66065,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA42100000S",null,null,null,"도로용 목재 수평규준틀 설치 및 철거",null,"개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA42100000S","노무","L001010101000023",null,"건축목공","일반공사 직종","인",0.21,0,0,268058,56292.1,0,0,268058,56292.1,null,null,"N","N","",1]
["CAA42100000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.19,0,0,165545,31453.5,0,0,165545,31453.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,87745,0,0,0,87745,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA42210000S",null,null,null,"도로용 철재 수평규준틀 설치 및 철거","5m이하","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA42210000S","노무","L001010101000023",null,"건축목공","일반공사 직종","인",0.14000000000000001,0,0,268058,37528.1,0,0,268058,37528.1,null,null,"N","N","",1]
["CAA42210000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.12,0,0,165545,19865.400000000001,0,0,165545,19865.400000000001,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,57393,0,0,0,57393,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA42220000S",null,null,null,"도로용 철재 수평규준틀 설치 및 철거","10m이하","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA42220000S","노무","L001010101000023",null,"건축목공","일반공사 직종","인",0.17,0,0,268058,45569.8,0,0,268058,45569.8,null,null,"N","N","",1]
["CAA42220000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.14000000000000001,0,0,165545,23176.3,0,0,165545,23176.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,68746,0,0,0,68746,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA43100000S",null,null,null,"평, 귀규준틀 설치 및 철거","평규준틀","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA43100000S","노무","L001010101000023",null,"건축목공","일반공사 직종","인",0.15,0,0,268058,40208.699999999997,0,0,268058,40208.699999999997,null,null,"N","N","",1]
["CAA43100000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.3,0,0,165545,49663.5,0,0,165545,49663.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,89872,0,0,0,89872,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA44100000S",null,null,null,"평, 귀규준틀 설치 및 철거","귀규준틀","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAA44100000S","노무","L001010101000023",null,"건축목공","일반공사 직종","인",0.3,0,0,268058,80417.399999999994,0,0,268058,80417.399999999994,null,null,"N","N","",1]
["CAA44100000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.45,0,0,165545,74495.199999999997,0,0,165545,74495.199999999997,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,154912,0,0,0,154912,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAB20203300S",null,null,null,"콘테이너형 가설건축물 설치 및 해체","3.0*3.0m","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAB20203300S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.4,0,0,280472,112188.8,0,0,280472,112188.8,null,null,"N","N","",1]
["CAB20203300S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.18,0,0,214222,38559.9,0,0,214222,38559.9,null,null,"N","N","",1]
["CAB20203300S","기계경비","00002104001000000",null,"크레인(타이어)","10ton","HR",2,6718,13436,55700,111400,30103,60206,92521,185042,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,13436,0,262148,0,60206,0,335790,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAB20203600S",null,null,null,"콘테이너형 가설건축물 설치 및 해체","3.0*6.0m","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAB20203600S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.57999999999999996,0,0,280472,162673.70000000001,0,0,280472,162673.70000000001,null,null,"N","N","",1]
["CAB20203600S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.34,0,0,214222,72835.399999999994,0,0,214222,72835.399999999994,null,null,"N","N","",1]
["CAB20203600S","기계경비","00002104001000000",null,"크레인(타이어)","10ton","HR",2,6718,13436,55700,111400,30103,60206,92521,185042,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,13436,0,346909,0,60206,0,420551,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAB20203900S",null,null,null,"콘테이너형 가설건축물 설치 및 해체","3.0*9.0m","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAB20203900S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.78,0,0,280472,218768.1,0,0,280472,218768.1,null,null,"N","N","",1]
["CAB20203900S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.38,0,0,214222,81404.3,0,0,214222,81404.3,null,null,"N","N","",1]
["CAB20203900S","기계경비","00002104001000000",null,"크레인(타이어)","10ton","HR",2,6718,13436,55700,111400,30103,60206,92521,185042,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,13436,0,411572,0,60206,0,485214,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAB21100000S",null,null,null,"철제조립식 가설건축물 설치 및 해체","사무실","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAB21100000S","노무","L001010101000023",null,"건축목공","일반공사 직종","인",0.26,0,0,268058,69695,0,0,268058,69695,null,null,"N","N","",1]
["CAB21100000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.11,0,0,165545,18209.900000000001,0,0,165545,18209.900000000001,null,null,"N","N","",1]
["CAB21100000S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,1758,1758,0,0,0,0,1758,1758,null,null,"N","N",2,1]
["CAB21100000S","기계경비","00002104001000000",null,"크레인(타이어)","10ton","HR",0.19,6718,1276.4000000000001,55700,10583,30103,5719.5,92521,17578.900000000001,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,3034,0,98487,0,5719,0,107240,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAB22100000S",null,null,null,"철제조립식 가설건축물 설치 및 해체","창고","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAB22100000S","노무","L001010101000023",null,"건축목공","일반공사 직종","인",0.2,0,0,268058,53611.6,0,0,268058,53611.6,null,null,"N","N","",1]
["CAB22100000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.09,0,0,165545,14899,0,0,165545,14899,null,null,"N","N","",1]
["CAB22100000S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,1370.2,1370.2,0,0,0,0,1370.2,1370.2,null,null,"N","N",2,1]
["CAB22100000S","기계경비","00002104001000000",null,"크레인(타이어)","10ton","HR",0.15,6718,1007.7,55700,8355,30103,4515.3999999999996,92521,13878.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,2377,0,76865,0,4515,0,83757,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAC51000000S",null,null,null,"건설용리프트 설치 및 해체","싱글 1.2ton","대",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAC51000000S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",1.31,0,0,233722,306175.8,0,0,233722,306175.8,null,null,"N","N","",1]
["CAC51000000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",2.04,0,0,280472,572162.80000000005,0,0,280472,572162.80000000005,null,null,"N","N","",1]
["CAC51000000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.87,0,0,165545,144024.1,0,0,165545,144024.1,null,null,"N","N","",1]
["CAC51000000S","손료","RENT000000000001",null,"공구손료","인력품의 3%","식",1,30670.799999999999,30670.799999999999,0,0,0,0,30670.799999999999,30670.799999999999,null,null,"N","N",3,1]
["CAC51000000S","기계경비","00002502005000000",null,"지게차","5.0ton","HR",1.95,9933,19369.3,55700,108615,6807,13273.6,72440,141257.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,50040,0,1130977,0,13273,0,1194290,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAC52000000S",null,null,null,"마스트 설치 및 해체","지하층 및 1~3층","층",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAC52000000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.8,0,0,280472,224377.60000000001,0,0,280472,224377.60000000001,null,null,"N","N","",1]
["CAC52000000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.27,0,0,165545,44697.1,0,0,165545,44697.1,null,null,"N","N","",1]
["CAC52000000S","손료","RENT000000000001",null,"공구손료","인력품의 3%","식",1,8072.2,8072.2,0,0,0,0,8072.2,8072.2,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,8072,0,269074,0,0,0,277146,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAC53000000S",null,null,null,"축중계 설치 철거","설치, 철거","회당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAC53000000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",5.0999999999999997E-2,0,0,214222,10925.3,0,0,214222,10925.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,10925,0,0,0,10925,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAC54021000S",null,null,null,"파이프루프공 - 작업편성인원","추진관경 300∼600mm","일당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAC54021000S","노무","L001020701000028",null,"중급기술자","건설","인",1,0,0,272915,272915,0,0,272915,272915,null,null,"N","N","",1]
["CAC54021000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",2,0,0,214222,428444,0,0,214222,428444,null,null,"N","N","",1]
["CAC54021000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1,0,0,165545,165545,0,0,165545,165545,null,null,"N","N","",1]
["CAC54021000S","노무","L001010101000012",null,"용접공","일반공사 직종","인",2,0,0,267021,534042,0,0,267021,534042,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,1400946,0,0,0,1400946,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAC54022000S",null,null,null,"파이프루프공 - 작업편성인원","추진관경 700∼900mm","일당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAC54022000S","노무","L001020701000028",null,"중급기술자","건설","인",1,0,0,272915,272915,0,0,272915,272915,null,null,"N","N","",1]
["CAC54022000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",2,0,0,214222,428444,0,0,214222,428444,null,null,"N","N","",1]
["CAC54022000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1,0,0,165545,165545,0,0,165545,165545,null,null,"N","N","",1]
["CAC54022000S","노무","L001010101000012",null,"용접공","일반공사 직종","인",2,0,0,267021,534042,0,0,267021,534042,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,1400946,0,0,0,1400946,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAC54023000S",null,null,null,"파이프루프공 - 작업편성인원","추진관경 1000∼1200mm","일당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAC54023000S","노무","L001020701000028",null,"중급기술자","건설","인",1,0,0,272915,272915,0,0,272915,272915,null,null,"N","N","",1]
["CAC54023000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",2,0,0,214222,428444,0,0,214222,428444,null,null,"N","N","",1]
["CAC54023000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2,0,0,165545,331090,0,0,165545,331090,null,null,"N","N","",1]
["CAC54023000S","노무","L001010101000012",null,"용접공","일반공사 직종","인",2,0,0,267021,534042,0,0,267021,534042,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,1566491,0,0,0,1566491,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAC54030000S",null,null,null,"파이프루프공 - 작업편성장비","1일 8시간 작업기준","일당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAC54030000S","기계경비","00005202030000000",null,"파이프추진기(오거부착유압식)","300ton, 1050m/m","HR",8,0,0,0,0,221629,1773032,221629,1773032,null,null,"N","N","",1]
["CAC54030000S","기계경비","00002104002000000",null,"크레인(타이어)","20ton","HR",8,9547,76376,55700,445600,51286,410288,116533,932264,null,null,"N","N","",1]
["CAC54030000S","기계경비","00007505005000000",null,"발전기","50kw","HR",8,13722,109776,33571,268568,4447,35576,51740,413920,null,null,"N","N","",1]
["CAC54030000S","기계경비","00007612020000000",null,"용접기(직류)","200Amp","HR",16,0,0,0,0,337,5392,337,5392,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,186152,0,714168,0,2224288,0,3124608,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAC54110000S",null,null,null,"파이프루프공 - 장비 조립","조립3일","회당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAC54110000S","노무","L001010101000050",null,"일반기계운전사","일반공사 직종","인",3,0,0,161142,483426,0,0,161142,483426,null,null,"N","N","",1]
["CAC54110000S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",3,0,0,233722,701166,0,0,233722,701166,null,null,"N","N","",1]
["CAC54110000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6,0,0,165545,993270,0,0,165545,993270,null,null,"N","N","",1]
["CAC54110000S","기계경비","00002104002000000",null,"크레인(타이어)","20ton","HR",24,9547,229128,55700,1336800,51286,1230864,116533,2796792,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,229128,0,3514662,0,1230864,0,4974654,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAC54210000S",null,null,null,"파이프루프공 - 장비 해체","해체2일","회당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAC54210000S","노무","L001010101000050",null,"일반기계운전사","일반공사 직종","인",2,0,0,161142,322284,0,0,161142,322284,null,null,"N","N","",1]
["CAC54210000S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",2,0,0,233722,467444,0,0,233722,467444,null,null,"N","N","",1]
["CAC54210000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4,0,0,165545,662180,0,0,165545,662180,null,null,"N","N","",1]
["CAC54210000S","기계경비","00002104002000000",null,"크레인(타이어)","20ton","HR",16,9547,152752,55700,891200,51286,820576,116533,1864528,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,152752,0,2343108,0,820576,0,3316436,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAD13100000S",null,null,null,"비산먼지 발생 억제를 위한 살수","물탱크(살수차), 16,000L","100M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAD13100000S","기계경비","00007204016000000",null,"물탱크(살수차)","16000L","HR",8.0000000000000002E-3,21331,170.6,47231,377.8,18163,145.30000000000001,86725,693.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,170,0,377,0,145,0,692,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAD13210000S",null,null,null,"자동세륜기 설치",null,"회",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAD13210000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",1.59,0,0,214222,340612.9,0,0,214222,340612.9,null,null,"N","N","",1]
["CAD13210000S","기계경비","00002104001000000",null,"크레인(타이어)","10ton","HR",2.6,6718,17466.8,55700,144820,30103,78267.8,92521,240554.6,null,null,"N","N","",1]
["CAD13210000S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,6812.2,6812.2,0,0,0,0,6812.2,6812.2,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,24279,0,485432,0,78267,0,587978,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAD13220000S",null,null,null,"자동세륜기 해체",null,"회",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAD13220000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",2.44,0,0,214222,522701.6,0,0,214222,522701.6,null,null,"N","N","",1]
["CAD13220000S","기계경비","00002104001000000",null,"크레인(타이어)","10ton","HR",3.3,6718,22169.4,55700,183810,30103,99339.9,92521,305319.3,null,null,"N","N","",1]
["CAD13220000S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,10454,10454,0,0,0,0,10454,10454,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,32623,0,706511,0,99339,0,838473,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAD13300000S",null,null,null,"슬러지 제거","자동세륜기","회",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAD13300000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.63,0,0,214222,134959.79999999999,0,0,214222,134959.79999999999,null,null,"N","N","",1]
["CAD13300000S","손료","RENT000000000001",null,"공구손료","인력품의 7%","식",1,9447.1,9447.1,0,0,0,0,9447.1,9447.1,null,null,"N","N",7,1]
["CAD13300000S","기계경비","00000201002000000",null,"굴삭기(무한궤도)","0.2㎥","HR",1,7695,7695,55700,55700,13041,13041,76436,76436,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,17142,0,190659,0,13041,0,220842,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAD16111000S",null,null,null,"건축물보양","부직포 깔기","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAD16111000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.0000000000000001E-3,0,0,165545,496.6,0,0,165545,496.6,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,496,0,0,0,496,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAD16112000S",null,null,null,"건축물보양","보양지 붙이기","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAD16112000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.01,0,0,165545,1655.4,0,0,165545,1655.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,1655,0,0,0,1655,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAD16113000S",null,null,null,"건축물보양","목재 붙이기","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAD16113000S","노무","L001010101000023",null,"건축목공","일반공사 직종","인",0.03,0,0,268058,8041.7,0,0,268058,8041.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,8041,0,0,0,8041,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAD16210000S",null,null,null,"건축물 현장정리","철근콘크리트조, 철골·철근콘크리트조","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAD16210000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.13,0,0,165545,21520.799999999999,0,0,165545,21520.799999999999,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,21520,0,0,0,21520,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAD16220000S",null,null,null,"건축물 현장정리","목조, 철골조, 조적조","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAD16220000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.05,0,0,165545,8277.2000000000007,0,0,165545,8277.2000000000007,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,8277,0,0,0,8277,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAD16310000S",null,null,null,"준공청소",null,"M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAD16310000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.02,0,0,165545,3310.9,0,0,165545,3310.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,3310,0,0,0,3310,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAD16320000S",null,null,null,"입주청소",null,"M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAD16320000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.03,0,0,165545,4966.3,0,0,165545,4966.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,4966,0,0,0,4966,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAD91000000S",null,null,null,"지능형 CCTV 설치 및 해체","지상 또는 건물설치","개당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAD91000000S","노무","L001010201000094",null,"S/W시험사","광전자 직종","인",0.2,0,0,433747,86749.4,0,0,433747,86749.4,null,null,"N","N","",1]
["CAD91000000S","노무","L001020601000020",null,"중급기술자","정보통신","인",0.5,0,0,263793,131896.5,0,0,263793,131896.5,null,null,"N","N","",1]
["CAD91000000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.2,0,0,214222,42844.4,0,0,214222,42844.4,null,null,"N","N","",1]
["CAD91000000S","손료","RENT000000000001",null,"공구손료","노무비의 1%","식",1,2614.9,2614.9,0,0,0,0,2614.9,2614.9,null,null,"N","N",1,1]
[null,null,null,null,"[합 계]",null,null,0,0,2614,0,261490,0,0,0,264104,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAD91020000S",null,null,null,"지능형 CCTV 설치 및 해체","타워크레인설치","개당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAD91020000S","노무","L001010201000094",null,"S/W시험사","광전자 직종","인",0.5,0,0,433747,216873.5,0,0,433747,216873.5,null,null,"N","N","",1]
["CAD91020000S","노무","L001020601000020",null,"중급기술자","정보통신","인",1,0,0,263793,263793,0,0,263793,263793,null,null,"N","N","",1]
["CAD91020000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.5,0,0,214222,107111,0,0,214222,107111,null,null,"N","N","",1]
["CAD91020000S","손료","RENT000000000001",null,"공구손료","노무비의 1%","식",1,5877.7,5877.7,0,0,0,0,5877.7,5877.7,null,null,"N","N",1,1]
[null,null,null,null,"[합 계]",null,null,0,0,5877,0,587777,0,0,0,593654,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAD92000000S",null,null,null,"지능형 출입관리 설치 및 해체",null,"개당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAD92000000S","노무","L001010201000094",null,"S/W시험사","광전자 직종","인",1,0,0,433747,433747,0,0,433747,433747,null,null,"N","N","",1]
["CAD92000000S","노무","L001020601000020",null,"중급기술자","정보통신","인",2,0,0,263793,527586,0,0,263793,527586,null,null,"N","N","",1]
["CAD92000000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",1,0,0,214222,214222,0,0,214222,214222,null,null,"N","N","",1]
["CAD92000000S","손료","RENT000000000001",null,"공구손료","노무비의 1%","식",1,11755.5,11755.5,0,0,0,0,11755.5,11755.5,null,null,"N","N",1,1]
[null,null,null,null,"[합 계]",null,null,0,0,11755,0,1175555,0,0,0,1187310,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE13011400S",null,null,null,"흙막이판 설치",null,"M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE13011400S","노무","L001010101000007",null,"형틀목공","일반공사 직종","인",7.2999999999999995E-2,0,0,274978,20073.3,0,0,274978,20073.3,null,null,"N","N","",1]
["CAE13011400S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.7999999999999999E-2,0,0,165545,6290.7,0,0,165545,6290.7,null,null,"N","N","",1]
["CAE13011400S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,790.9,790.9,0,0,0,0,790.9,790.9,null,null,"N","N",3,1]
["CAE13011400S","기계경비","00000201002000000",null,"굴삭기(무한궤도)","0.2㎥","HR",0.192,7695,1477.4,55700,10694.4,13041,2503.8000000000002,76436,14675.6,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,2268,0,37058,0,2503,0,41829,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE13020000S",null,null,null,"흙막이판 철거",null,"M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE13020000S","노무","L001010101000007",null,"형틀목공","일반공사 직종","인",5.8000000000000003E-2,0,0,274978,15948.7,0,0,274978,15948.7,null,null,"N","N","",1]
["CAE13020000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.03,0,0,165545,4966.3,0,0,165545,4966.3,null,null,"N","N","",1]
["CAE13020000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,627.4,627.4,0,0,0,0,627.4,627.4,null,null,"N","N",3,1]
["CAE13020000S","기계경비","00000201002000000",null,"굴삭기(무한궤도)","0.2㎥","HR",0.154,7695,1185,55700,8577.7999999999993,13041,2008.3,76436,11771.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,1812,0,29492,0,2008,0,33312,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15011100S",null,null,null,"H-Beam 설치 / 띠장","H=300∼500mm, L=5m이하","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15011100S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.16,0,0,243126,38900.1,0,0,243126,38900.1,null,null,"N","N","",1]
["CAE15011100S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.38,0,0,267021,101467.9,0,0,267021,101467.9,null,null,"N","N","",1]
["CAE15011100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.14000000000000001,0,0,165545,23176.3,0,0,165545,23176.3,null,null,"N","N","",1]
["CAE15011100S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,4906.3,4906.3,0,0,0,0,4906.3,4906.3,null,null,"N","N",3,1]
["CAE15011100S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.33,10785,3559,55700,18381,56667,18700.099999999999,123152,40640.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,8465,0,181925,0,18700,0,209090,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15011200S",null,null,null,"H-Beam 설치 / 띠장","H=300∼500mm, L=6∼8m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15011200S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.18,0,0,243126,43762.6,0,0,243126,43762.6,null,null,"N","N","",1]
["CAE15011200S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.41,0,0,267021,109478.6,0,0,267021,109478.6,null,null,"N","N","",1]
["CAE15011200S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.15,0,0,165545,24831.7,0,0,165545,24831.7,null,null,"N","N","",1]
["CAE15011200S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,5342.1,5342.1,0,0,0,0,5342.1,5342.1,null,null,"N","N",3,1]
["CAE15011200S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.4,10785,4314,55700,22280,56667,22666.799999999999,123152,49260.800000000003,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,9656,0,200352,0,22666,0,232674,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15011300S",null,null,null,"H-Beam 설치 / 띠장","H=300∼500mm, L=9∼11m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15011300S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.21,0,0,243126,51056.4,0,0,243126,51056.4,null,null,"N","N","",1]
["CAE15011300S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.49,0,0,267021,130840.2,0,0,267021,130840.2,null,null,"N","N","",1]
["CAE15011300S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.18,0,0,165545,29798.1,0,0,165545,29798.1,null,null,"N","N","",1]
["CAE15011300S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,6350.8,6350.8,0,0,0,0,6350.8,6350.8,null,null,"N","N",3,1]
["CAE15011300S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.52,10785,5608.2,55700,28964,56667,29466.799999999999,123152,64039,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,11959,0,240658,0,29466,0,282083,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15011400S",null,null,null,"H-Beam 설치 / 띠장","H=300∼500mm, L=12∼14m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15011400S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.23,0,0,243126,55918.9,0,0,243126,55918.9,null,null,"N","N","",1]
["CAE15011400S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.54,0,0,267021,144191.29999999999,0,0,267021,144191.29999999999,null,null,"N","N","",1]
["CAE15011400S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.19,0,0,165545,31453.5,0,0,165545,31453.5,null,null,"N","N","",1]
["CAE15011400S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,6946.9,6946.9,0,0,0,0,6946.9,6946.9,null,null,"N","N",3,1]
["CAE15011400S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.6,10785,6471,55700,33420,56667,34000.199999999997,123152,73891.199999999997,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,13417,0,264983,0,34000,0,312400,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15011500S",null,null,null,"H-Beam 설치 / 띠장","H=300∼500mm, L=15∼18m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15011500S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.25,0,0,243126,60781.5,0,0,243126,60781.5,null,null,"N","N","",1]
["CAE15011500S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.59,0,0,267021,157542.29999999999,0,0,267021,157542.29999999999,null,null,"N","N","",1]
["CAE15011500S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.21,0,0,165545,34764.400000000001,0,0,165545,34764.400000000001,null,null,"N","N","",1]
["CAE15011500S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,7592.6,7592.6,0,0,0,0,7592.6,7592.6,null,null,"N","N",3,1]
["CAE15011500S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.69,10785,7441.6,55700,38433,56667,39100.199999999997,123152,84974.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,15034,0,291521,0,39100,0,345655,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15012100S",null,null,null,"H-Beam 설치 / 띠장","H=600∼800mm, L=5m 이하","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15012100S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.21,0,0,243126,51056.4,0,0,243126,51056.4,null,null,"N","N","",1]
["CAE15012100S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.48,0,0,267021,128170,0,0,267021,128170,null,null,"N","N","",1]
["CAE15012100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.17,0,0,165545,28142.6,0,0,165545,28142.6,null,null,"N","N","",1]
["CAE15012100S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,6221,6221,0,0,0,0,6221,6221,null,null,"N","N",3,1]
["CAE15012100S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.42,10785,4529.7,55700,23394,56667,23800.1,123152,51723.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,10750,0,230763,0,23800,0,265313,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15012200S",null,null,null,"H-Beam 설치 / 띠장","H=600∼800mm, L=6∼8m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15012200S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.23,0,0,243126,55918.9,0,0,243126,55918.9,null,null,"N","N","",1]
["CAE15012200S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.54,0,0,267021,144191.29999999999,0,0,267021,144191.29999999999,null,null,"N","N","",1]
["CAE15012200S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.19,0,0,165545,31453.5,0,0,165545,31453.5,null,null,"N","N","",1]
["CAE15012200S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,6946.9,6946.9,0,0,0,0,6946.9,6946.9,null,null,"N","N",3,1]
["CAE15012200S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.51,10785,5500.3,55700,28407,56667,28900.1,123152,62807.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,12447,0,259970,0,28900,0,301317,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15012300S",null,null,null,"H-Beam 설치 / 띠장","H=600∼800mm, L=9∼11m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15012300S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.27,0,0,243126,65644,0,0,243126,65644,null,null,"N","N","",1]
["CAE15012300S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.62,0,0,267021,165553,0,0,267021,165553,null,null,"N","N","",1]
["CAE15012300S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.22,0,0,165545,36419.9,0,0,165545,36419.9,null,null,"N","N","",1]
["CAE15012300S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,8028.5,8028.5,0,0,0,0,8028.5,8028.5,null,null,"N","N",3,1]
["CAE15012300S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.66,10785,7118.1,55700,36762,56667,37400.199999999997,123152,81280.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,15146,0,304378,0,37400,0,356924,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15012400S",null,null,null,"H-Beam 설치 / 띠장","H=600∼800mm, L=12∼14m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15012400S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.28999999999999998,0,0,243126,70506.5,0,0,243126,70506.5,null,null,"N","N","",1]
["CAE15012400S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.68,0,0,267021,181574.2,0,0,267021,181574.2,null,null,"N","N","",1]
["CAE15012400S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.24,0,0,165545,39730.800000000003,0,0,165545,39730.800000000003,null,null,"N","N","",1]
["CAE15012400S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,8754.2999999999993,8754.2999999999993,0,0,0,0,8754.2999999999993,8754.2999999999993,null,null,"N","N",3,1]
["CAE15012400S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.77,10785,8304.4,55700,42889,56667,43633.5,123152,94826.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,17058,0,334700,0,43633,0,395391,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15012500S",null,null,null,"H-Beam 설치 / 띠장","H=600∼800mm, L=15∼18m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15012500S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.32,0,0,243126,77800.3,0,0,243126,77800.3,null,null,"N","N","",1]
["CAE15012500S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.74,0,0,267021,197595.5,0,0,267021,197595.5,null,null,"N","N","",1]
["CAE15012500S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.27,0,0,165545,44697.1,0,0,165545,44697.1,null,null,"N","N","",1]
["CAE15012500S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,9602.7000000000007,9602.7000000000007,0,0,0,0,9602.7000000000007,9602.7000000000007,null,null,"N","N",3,1]
["CAE15012500S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.81,10785,8735.7999999999993,55700,45117,56667,45900.2,123152,99753,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,18338,0,365209,0,45900,0,429447,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15021100S",null,null,null,"H-Beam 철거 / 띠장","H=300∼500mm, L=5m이하","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15021100S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.1,0,0,243126,24312.6,0,0,243126,24312.6,null,null,"N","N","",1]
["CAE15021100S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.23,0,0,267021,61414.8,0,0,267021,61414.8,null,null,"N","N","",1]
["CAE15021100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.08,0,0,165545,13243.6,0,0,165545,13243.6,null,null,"N","N","",1]
["CAE15021100S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,2969.1,2969.1,0,0,0,0,2969.1,2969.1,null,null,"N","N",3,1]
["CAE15021100S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.23,10785,2480.5,55700,12811,56667,13033.4,123152,28324.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,5449,0,111782,0,13033,0,130264,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15021200S",null,null,null,"H-Beam 철거 / 띠장","H=300∼500mm, L=6∼8m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15021200S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.11,0,0,243126,26743.8,0,0,243126,26743.8,null,null,"N","N","",1]
["CAE15021200S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.26,0,0,267021,69425.399999999994,0,0,267021,69425.399999999994,null,null,"N","N","",1]
["CAE15021200S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.09,0,0,165545,14899,0,0,165545,14899,null,null,"N","N","",1]
["CAE15021200S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,3332,3332,0,0,0,0,3332,3332,null,null,"N","N",3,1]
["CAE15021200S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.28000000000000003,10785,3019.8,55700,15596,56667,15866.7,123152,34482.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,6351,0,126664,0,15866,0,148881,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15021300S",null,null,null,"H-Beam 철거 / 띠장","H=300∼500mm, L=9∼11m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15021300S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.13,0,0,243126,31606.3,0,0,243126,31606.3,null,null,"N","N","",1]
["CAE15021300S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.28999999999999998,0,0,267021,77436,0,0,267021,77436,null,null,"N","N","",1]
["CAE15021300S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.11,0,0,165545,18209.900000000001,0,0,165545,18209.900000000001,null,null,"N","N","",1]
["CAE15021300S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,3817.5,3817.5,0,0,0,0,3817.5,3817.5,null,null,"N","N",3,1]
["CAE15021300S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.36,10785,3882.6,55700,20052,56667,20400.099999999999,123152,44334.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,7700,0,147304,0,20400,0,175404,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15021400S",null,null,null,"H-Beam 철거 / 띠장","H=300∼500mm, L=12∼14m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15021400S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.14000000000000001,0,0,243126,34037.599999999999,0,0,243126,34037.599999999999,null,null,"N","N","",1]
["CAE15021400S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.32,0,0,267021,85446.7,0,0,267021,85446.7,null,null,"N","N","",1]
["CAE15021400S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.12,0,0,165545,19865.400000000001,0,0,165545,19865.400000000001,null,null,"N","N","",1]
["CAE15021400S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,4180.3999999999996,4180.3999999999996,0,0,0,0,4180.3999999999996,4180.3999999999996,null,null,"N","N",3,1]
["CAE15021400S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.42,10785,4529.7,55700,23394,56667,23800.1,123152,51723.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,8710,0,162743,0,23800,0,195253,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15021500S",null,null,null,"H-Beam 철거 / 띠장","H=300∼500mm, L=15∼18m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15021500S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.15,0,0,243126,36468.9,0,0,243126,36468.9,null,null,"N","N","",1]
["CAE15021500S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.35,0,0,267021,93457.3,0,0,267021,93457.3,null,null,"N","N","",1]
["CAE15021500S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.13,0,0,165545,21520.799999999999,0,0,165545,21520.799999999999,null,null,"N","N","",1]
["CAE15021500S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,4543.3999999999996,4543.3999999999996,0,0,0,0,4543.3999999999996,4543.3999999999996,null,null,"N","N",3,1]
["CAE15021500S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.49,10785,5284.6,55700,27293,56667,27766.799999999999,123152,60344.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,9828,0,178740,0,27766,0,216334,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15022100S",null,null,null,"H-Beam 철거 / 띠장","H=600∼800mm, L=5m 이하","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15022100S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.12,0,0,243126,29175.1,0,0,243126,29175.1,null,null,"N","N","",1]
["CAE15022100S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.28999999999999998,0,0,267021,77436,0,0,267021,77436,null,null,"N","N","",1]
["CAE15022100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.1,0,0,165545,16554.5,0,0,165545,16554.5,null,null,"N","N","",1]
["CAE15022100S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,3694.9,3694.9,0,0,0,0,3694.9,3694.9,null,null,"N","N",3,1]
["CAE15022100S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.28999999999999998,10785,3127.6,55700,16153,56667,16433.400000000001,123152,35714,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,6822,0,139318,0,16433,0,162573,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15022200S",null,null,null,"H-Beam 철거 / 띠장","H=600∼800mm, L=6∼8m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15022200S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.14000000000000001,0,0,243126,34037.599999999999,0,0,243126,34037.599999999999,null,null,"N","N","",1]
["CAE15022200S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.32,0,0,267021,85446.7,0,0,267021,85446.7,null,null,"N","N","",1]
["CAE15022200S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.12,0,0,165545,19865.400000000001,0,0,165545,19865.400000000001,null,null,"N","N","",1]
["CAE15022200S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,4180.3999999999996,4180.3999999999996,0,0,0,0,4180.3999999999996,4180.3999999999996,null,null,"N","N",3,1]
["CAE15022200S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.36,10785,3882.6,55700,20052,56667,20400.099999999999,123152,44334.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,8063,0,159401,0,20400,0,187864,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15022300S",null,null,null,"H-Beam 철거 / 띠장","H=600∼800mm, L=9∼11m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15022300S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.16,0,0,243126,38900.1,0,0,243126,38900.1,null,null,"N","N","",1]
["CAE15022300S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.37,0,0,267021,98797.7,0,0,267021,98797.7,null,null,"N","N","",1]
["CAE15022300S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.13,0,0,165545,21520.799999999999,0,0,165545,21520.799999999999,null,null,"N","N","",1]
["CAE15022300S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,4776.5,4776.5,0,0,0,0,4776.5,4776.5,null,null,"N","N",3,1]
["CAE15022300S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.46,10785,4961.1000000000004,55700,25622,56667,26066.799999999999,123152,56649.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,9737,0,184840,0,26066,0,220643,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15022400S",null,null,null,"H-Beam 철거 / 띠장","H=600∼800mm, L=12∼14m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15022400S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.18,0,0,243126,43762.6,0,0,243126,43762.6,null,null,"N","N","",1]
["CAE15022400S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.41,0,0,267021,109478.6,0,0,267021,109478.6,null,null,"N","N","",1]
["CAE15022400S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.15,0,0,165545,24831.7,0,0,165545,24831.7,null,null,"N","N","",1]
["CAE15022400S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,5342.1,5342.1,0,0,0,0,5342.1,5342.1,null,null,"N","N",3,1]
["CAE15022400S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.54,10785,5823.9,55700,30078,56667,30600.1,123152,66502,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,11166,0,208150,0,30600,0,249916,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15022500S",null,null,null,"H-Beam 철거 / 띠장","H=600∼800mm, L=15∼18m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE15022500S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.19,0,0,243126,46193.9,0,0,243126,46193.9,null,null,"N","N","",1]
["CAE15022500S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.45,0,0,267021,120159.4,0,0,267021,120159.4,null,null,"N","N","",1]
["CAE15022500S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.16,0,0,165545,26487.200000000001,0,0,165545,26487.200000000001,null,null,"N","N","",1]
["CAE15022500S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,5785.2,5785.2,0,0,0,0,5785.2,5785.2,null,null,"N","N",3,1]
["CAE15022500S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.62,10785,6686.7,55700,34534,56667,35133.5,123152,76354.2,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,12471,0,227374,0,35133,0,274978,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16011100S",null,null,null,"H-Beam 설치 / 버팀보","H=300∼500mm, L=5m이하","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16011100S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.34,0,0,243126,82662.8,0,0,243126,82662.8,null,null,"N","N","",1]
["CAE16011100S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.17,0,0,267021,45393.5,0,0,267021,45393.5,null,null,"N","N","",1]
["CAE16011100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.13,0,0,165545,21520.799999999999,0,0,165545,21520.799999999999,null,null,"N","N","",1]
["CAE16011100S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,4487.3,4487.3,0,0,0,0,4487.3,4487.3,null,null,"N","N",3,1]
["CAE16011100S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.28999999999999998,10785,3127.6,55700,16153,56667,16433.400000000001,123152,35714,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,7614,0,165730,0,16433,0,189777,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16011200S",null,null,null,"H-Beam 설치 / 버팀보","H=300∼500mm, L=6∼8m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16011200S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.36,0,0,243126,87525.3,0,0,243126,87525.3,null,null,"N","N","",1]
["CAE16011200S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.19,0,0,267021,50733.9,0,0,267021,50733.9,null,null,"N","N","",1]
["CAE16011200S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.14000000000000001,0,0,165545,23176.3,0,0,165545,23176.3,null,null,"N","N","",1]
["CAE16011200S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,4843,4843,0,0,0,0,4843,4843,null,null,"N","N",3,1]
["CAE16011200S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.35,10785,3774.7,55700,19495,56667,19833.400000000001,123152,43103.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,8617,0,180930,0,19833,0,209380,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16011300S",null,null,null,"H-Beam 설치 / 버팀보","H=300∼500mm, L=9∼11m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16011300S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.4,0,0,243126,97250.4,0,0,243126,97250.4,null,null,"N","N","",1]
["CAE16011300S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.2,0,0,267021,53404.2,0,0,267021,53404.2,null,null,"N","N","",1]
["CAE16011300S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.15,0,0,165545,24831.7,0,0,165545,24831.7,null,null,"N","N","",1]
["CAE16011300S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,5264.5,5264.5,0,0,0,0,5264.5,5264.5,null,null,"N","N",3,1]
["CAE16011300S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.45,10785,4853.2,55700,25065,56667,25500.1,123152,55418.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,10117,0,200551,0,25500,0,236168,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16011400S",null,null,null,"H-Beam 설치 / 버팀보","H=300∼500mm, L=12∼14m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16011400S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.43,0,0,243126,104544.1,0,0,243126,104544.1,null,null,"N","N","",1]
["CAE16011400S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.22,0,0,267021,58744.6,0,0,267021,58744.6,null,null,"N","N","",1]
["CAE16011400S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.16,0,0,165545,26487.200000000001,0,0,165545,26487.200000000001,null,null,"N","N","",1]
["CAE16011400S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,5693.2,5693.2,0,0,0,0,5693.2,5693.2,null,null,"N","N",3,1]
["CAE16011400S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.53,10785,5716,55700,29521,56667,30033.5,123152,65270.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,11409,0,219296,0,30033,0,260738,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16011500S",null,null,null,"H-Beam 설치 / 버팀보","H=300∼500mm, L=15∼18m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16011500S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.45,0,0,243126,109406.7,0,0,243126,109406.7,null,null,"N","N","",1]
["CAE16011500S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.23,0,0,267021,61414.8,0,0,267021,61414.8,null,null,"N","N","",1]
["CAE16011500S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.17,0,0,165545,28142.6,0,0,165545,28142.6,null,null,"N","N","",1]
["CAE16011500S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,5968.9,5968.9,0,0,0,0,5968.9,5968.9,null,null,"N","N",3,1]
["CAE16011500S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.61,10785,6578.8,55700,33977,56667,34566.800000000003,123152,75122.600000000006,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,12547,0,232941,0,34566,0,280054,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16012100S",null,null,null,"H-Beam 설치 / 버팀보","H=600∼800mm, L=5m 이하","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16012100S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.43,0,0,243126,104544.1,0,0,243126,104544.1,null,null,"N","N","",1]
["CAE16012100S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.22,0,0,267021,58744.6,0,0,267021,58744.6,null,null,"N","N","",1]
["CAE16012100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.16,0,0,165545,26487.200000000001,0,0,165545,26487.200000000001,null,null,"N","N","",1]
["CAE16012100S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,5693.2,5693.2,0,0,0,0,5693.2,5693.2,null,null,"N","N",3,1]
["CAE16012100S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.36,10785,3882.6,55700,20052,56667,20400.099999999999,123152,44334.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,9575,0,209827,0,20400,0,239802,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16012200S",null,null,null,"H-Beam 설치 / 버팀보","H=600∼800mm, L=6∼8m ","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16012200S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.46,0,0,243126,111837.9,0,0,243126,111837.9,null,null,"N","N","",1]
["CAE16012200S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.24,0,0,267021,64085,0,0,267021,64085,null,null,"N","N","",1]
["CAE16012200S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.17,0,0,165545,28142.6,0,0,165545,28142.6,null,null,"N","N","",1]
["CAE16012200S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,6121.9,6121.9,0,0,0,0,6121.9,6121.9,null,null,"N","N",3,1]
["CAE16012200S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.44,10785,4745.3999999999996,55700,24508,56667,24933.4,123152,54186.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,10867,0,228573,0,24933,0,264373,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16012300S",null,null,null,"H-Beam 설치 / 버팀보","H=600∼800mm, L=9∼11m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16012300S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.51,0,0,243126,123994.2,0,0,243126,123994.2,null,null,"N","N","",1]
["CAE16012300S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.26,0,0,267021,69425.399999999994,0,0,267021,69425.399999999994,null,null,"N","N","",1]
["CAE16012300S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.19,0,0,165545,31453.5,0,0,165545,31453.5,null,null,"N","N","",1]
["CAE16012300S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,6746.1,6746.1,0,0,0,0,6746.1,6746.1,null,null,"N","N",3,1]
["CAE16012300S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.56999999999999995,10785,6147.4,55700,31749,56667,32300.1,123152,70196.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,12893,0,256622,0,32300,0,301815,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16012400S",null,null,null,"H-Beam 설치 / 버팀보","H=600∼800mm, L=12∼14m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16012400S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.54,0,0,243126,131288,0,0,243126,131288,null,null,"N","N","",1]
["CAE16012400S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.28000000000000003,0,0,267021,74765.8,0,0,267021,74765.8,null,null,"N","N","",1]
["CAE16012400S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.2,0,0,165545,33109,0,0,165545,33109,null,null,"N","N","",1]
["CAE16012400S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,7174.8,7174.8,0,0,0,0,7174.8,7174.8,null,null,"N","N",3,1]
["CAE16012400S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.67,10785,7225.9,55700,37319,56667,37966.800000000003,123152,82511.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,14400,0,276481,0,37966,0,328847,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16012500S",null,null,null,"H-Beam 설치 / 버팀보","H=600∼800mm, L=15∼18m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16012500S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.57999999999999996,0,0,243126,141013,0,0,243126,141013,null,null,"N","N","",1]
["CAE16012500S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.28999999999999998,0,0,267021,77436,0,0,267021,77436,null,null,"N","N","",1]
["CAE16012500S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.22,0,0,165545,36419.9,0,0,165545,36419.9,null,null,"N","N","",1]
["CAE16012500S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,7646,7646,0,0,0,0,7646,7646,null,null,"N","N",3,1]
["CAE16012500S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.77,10785,8304.4,55700,42889,56667,43633.5,123152,94826.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,15950,0,297757,0,43633,0,357340,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16021100S",null,null,null,"H-Beam 철거 / 버팀보","H=300∼500mm, L=5m이하","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16021100S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.2,0,0,243126,48625.2,0,0,243126,48625.2,null,null,"N","N","",1]
["CAE16021100S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.1,0,0,267021,26702.1,0,0,267021,26702.1,null,null,"N","N","",1]
["CAE16021100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.08,0,0,165545,13243.6,0,0,165545,13243.6,null,null,"N","N","",1]
["CAE16021100S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,2657.1,2657.1,0,0,0,0,2657.1,2657.1,null,null,"N","N",3,1]
["CAE16021100S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.2,10785,2157,55700,11140,56667,11333.4,123152,24630.400000000001,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,4814,0,99710,0,11333,0,115857,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16021200S",null,null,null,"H-Beam 철거 / 버팀보","H=300∼500mm, L=6∼8m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16021200S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.22,0,0,243126,53487.7,0,0,243126,53487.7,null,null,"N","N","",1]
["CAE16021200S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.11,0,0,267021,29372.3,0,0,267021,29372.3,null,null,"N","N","",1]
["CAE16021200S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.08,0,0,165545,13243.6,0,0,165545,13243.6,null,null,"N","N","",1]
["CAE16021200S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,2883.1,2883.1,0,0,0,0,2883.1,2883.1,null,null,"N","N",3,1]
["CAE16021200S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.24,10785,2588.4,55700,13368,56667,13600,123152,29556.400000000001,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,5471,0,109471,0,13600,0,128542,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16021300S",null,null,null,"H-Beam 철거 / 버팀보","H=300∼500mm, L=9∼11m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16021300S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.24,0,0,243126,58350.2,0,0,243126,58350.2,null,null,"N","N","",1]
["CAE16021300S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.12,0,0,267021,32042.5,0,0,267021,32042.5,null,null,"N","N","",1]
["CAE16021300S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.09,0,0,165545,14899,0,0,165545,14899,null,null,"N","N","",1]
["CAE16021300S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,3158.7,3158.7,0,0,0,0,3158.7,3158.7,null,null,"N","N",3,1]
["CAE16021300S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.32,10785,3451.2,55700,17824,56667,18133.400000000001,123152,39408.6,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,6609,0,123115,0,18133,0,147857,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16021400S",null,null,null,"H-Beam 철거 / 버팀보","H=300∼500mm, L=12∼14m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16021400S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.26,0,0,243126,63212.7,0,0,243126,63212.7,null,null,"N","N","",1]
["CAE16021400S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.13,0,0,267021,34712.699999999997,0,0,267021,34712.699999999997,null,null,"N","N","",1]
["CAE16021400S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.1,0,0,165545,16554.5,0,0,165545,16554.5,null,null,"N","N","",1]
["CAE16021400S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,3434.3,3434.3,0,0,0,0,3434.3,3434.3,null,null,"N","N",3,1]
["CAE16021400S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.37,10785,3990.4,55700,20609,56667,20966.7,123152,45566.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,7424,0,135088,0,20966,0,163478,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16021500S",null,null,null,"H-Beam 철거 / 버팀보","H=300∼500mm, L=15∼18m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16021500S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.27,0,0,243126,65644,0,0,243126,65644,null,null,"N","N","",1]
["CAE16021500S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.14000000000000001,0,0,267021,37382.9,0,0,267021,37382.9,null,null,"N","N","",1]
["CAE16021500S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.1,0,0,165545,16554.5,0,0,165545,16554.5,null,null,"N","N","",1]
["CAE16021500S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,3587.4,3587.4,0,0,0,0,3587.4,3587.4,null,null,"N","N",3,1]
["CAE16021500S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.43,10785,4637.5,55700,23951,56667,24366.799999999999,123152,52955.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,8224,0,143532,0,24366,0,176122,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16022100S",null,null,null,"H-Beam 철거 / 버팀보","H=600∼800mm, L=5m 이하","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16022100S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.26,0,0,243126,63212.7,0,0,243126,63212.7,null,null,"N","N","",1]
["CAE16022100S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.13,0,0,267021,34712.699999999997,0,0,267021,34712.699999999997,null,null,"N","N","",1]
["CAE16022100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.1,0,0,165545,16554.5,0,0,165545,16554.5,null,null,"N","N","",1]
["CAE16022100S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,3434.3,3434.3,0,0,0,0,3434.3,3434.3,null,null,"N","N",3,1]
["CAE16022100S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.25,10785,2696.2,55700,13925,56667,14166.7,123152,30787.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,6130,0,128404,0,14166,0,148700,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16022200S",null,null,null,"H-Beam 철거 / 버팀보","H=600∼800mm, L=6∼8m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16022200S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.28000000000000003,0,0,243126,68075.199999999997,0,0,243126,68075.199999999997,null,null,"N","N","",1]
["CAE16022200S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.14000000000000001,0,0,267021,37382.9,0,0,267021,37382.9,null,null,"N","N","",1]
["CAE16022200S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.11,0,0,165545,18209.900000000001,0,0,165545,18209.900000000001,null,null,"N","N","",1]
["CAE16022200S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,3710,3710,0,0,0,0,3710,3710,null,null,"N","N",3,1]
["CAE16022200S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.31,10785,3343.3,55700,17267,56667,17566.7,123152,38177,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,7053,0,140935,0,17566,0,165554,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16022300S",null,null,null,"H-Beam 철거 / 버팀보","H=600∼800mm, L=9∼11m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16022300S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.3,0,0,243126,72937.8,0,0,243126,72937.8,null,null,"N","N","",1]
["CAE16022300S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.16,0,0,267021,42723.3,0,0,267021,42723.3,null,null,"N","N","",1]
["CAE16022300S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.12,0,0,165545,19865.400000000001,0,0,165545,19865.400000000001,null,null,"N","N","",1]
["CAE16022300S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,4065.7,4065.7,0,0,0,0,4065.7,4065.7,null,null,"N","N",3,1]
["CAE16022300S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.4,10785,4314,55700,22280,56667,22666.799999999999,123152,49260.800000000003,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,8379,0,157806,0,22666,0,188851,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16022400S",null,null,null,"H-Beam 철거 / 버팀보","H=600∼800mm, L=12∼14m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16022400S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.32,0,0,243126,77800.3,0,0,243126,77800.3,null,null,"N","N","",1]
["CAE16022400S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.17,0,0,267021,45393.5,0,0,267021,45393.5,null,null,"N","N","",1]
["CAE16022400S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.12,0,0,165545,19865.400000000001,0,0,165545,19865.400000000001,null,null,"N","N","",1]
["CAE16022400S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,4291.7,4291.7,0,0,0,0,4291.7,4291.7,null,null,"N","N",3,1]
["CAE16022400S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.47,10785,5068.8999999999996,55700,26179,56667,26633.4,123152,57881.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,9360,0,169238,0,26633,0,205231,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16022500S",null,null,null,"H-Beam 철거 / 버팀보","H=600∼800mm, L=15∼18m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAE16022500S","노무","L001010101000011",null,"철골공","일반공사 직종","인",0.35,0,0,243126,85094.1,0,0,243126,85094.1,null,null,"N","N","",1]
["CAE16022500S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.18,0,0,267021,48063.7,0,0,267021,48063.7,null,null,"N","N","",1]
["CAE16022500S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.13,0,0,165545,21520.799999999999,0,0,165545,21520.799999999999,null,null,"N","N","",1]
["CAE16022500S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,4640.3,4640.3,0,0,0,0,4640.3,4640.3,null,null,"N","N",3,1]
["CAE16022500S","기계경비","00002104002500000",null,"크레인(타이어)","25ton","HR",0.54,10785,5823.9,55700,30078,56667,30600.1,123152,66502,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,10464,0,184756,0,30600,0,225820,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAM54110000S",null,null,null,"사석 / 적재 및 운반","0.03m3 이하 덤프트럭 대선 진입 적재","M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAM54110000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.0000000000000001E-3,0,0,165545,993.2,0,0,165545,993.2,null,null,"N","N","",1]
["CAM54110000S","손료","RENT000000000001",null,"잡재료","인력품의 2%","식",1,19.8,19.8,0,0,0,0,19.8,19.8,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,19,0,993,0,0,0,1012,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAM54120000S",null,null,null,"사석 / 적재 및 운반","0.1m3 이상 크레인 적재","M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CAM54120000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",8.9999999999999993E-3,0,0,214222,1927.9,0,0,214222,1927.9,null,null,"N","N","",1]
["CAM54120000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.01,0,0,165545,1655.4,0,0,165545,1655.4,null,null,"N","N","",1]
["CAM54120000S","손료","RENT000000000001",null,"잡재료","인력품의 2%","식",1,71.599999999999994,71.599999999999994,0,0,0,0,71.599999999999994,71.599999999999994,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,71,0,3583,0,0,0,3654,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC00000000S",null,null,null,"기계기구 설치","지반조사, 보링","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC00000000S","노무","L001010101000014",null,"보링공","일반공사 직종","인",1,0,0,223458,223458,0,0,223458,223458,null,null,"N","N","",1]
["CBC00000000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",1,0,0,214222,214222,0,0,214222,214222,null,null,"N","N","",1]
["CBC00000000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1,0,0,165545,165545,0,0,165545,165545,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,603225,0,0,0,603225,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC11010000S",null,null,null,"천공 (점토층)","BX, 20m 이내","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC11010000S","노무","L001020701000028",null,"중급기술자","건설","인",0.16,0,0,272915,43666.400000000001,0,0,272915,43666.400000000001,null,null,"N","N","",1]
["CBC11010000S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.28999999999999998,0,0,223458,64802.8,0,0,223458,64802.8,null,null,"N","N","",1]
["CBC11010000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.21,0,0,214222,44986.6,0,0,214222,44986.6,null,null,"N","N","",1]
["CBC11010000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.28999999999999998,0,0,165545,48008,0,0,165545,48008,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,201463,0,0,0,201463,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC12010000S",null,null,null,"천공 (점토층)","NX, 20m 이내","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC12010000S","노무","L001020701000028",null,"중급기술자","건설","인",0.18,0,0,272915,49124.7,0,0,272915,49124.7,null,null,"N","N","",1]
["CBC12010000S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.35,0,0,223458,78210.3,0,0,223458,78210.3,null,null,"N","N","",1]
["CBC12010000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.25,0,0,214222,53555.5,0,0,214222,53555.5,null,null,"N","N","",1]
["CBC12010000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.35,0,0,165545,57940.7,0,0,165545,57940.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,238831,0,0,0,238831,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC21010000S",null,null,null,"천공 (모래층)","BX, 20m 이내","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC21010000S","노무","L001020701000028",null,"중급기술자","건설","인",0.18,0,0,272915,49124.7,0,0,272915,49124.7,null,null,"N","N","",1]
["CBC21010000S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.34,0,0,223458,75975.7,0,0,223458,75975.7,null,null,"N","N","",1]
["CBC21010000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.24,0,0,214222,51413.2,0,0,214222,51413.2,null,null,"N","N","",1]
["CBC21010000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.34,0,0,165545,56285.3,0,0,165545,56285.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,232798,0,0,0,232798,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC22010000S",null,null,null,"천공 (모래층)","NX, 20m 이내","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC22010000S","노무","L001020701000028",null,"중급기술자","건설","인",0.21,0,0,272915,57312.1,0,0,272915,57312.1,null,null,"N","N","",1]
["CBC22010000S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.4,0,0,223458,89383.2,0,0,223458,89383.2,null,null,"N","N","",1]
["CBC22010000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.28999999999999998,0,0,214222,62124.3,0,0,214222,62124.3,null,null,"N","N","",1]
["CBC22010000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.4,0,0,165545,66218,0,0,165545,66218,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,275037,0,0,0,275037,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC31010000S",null,null,null,"천공 (자갈층)","BX, 20m 이내","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC31010000S","노무","L001020701000028",null,"중급기술자","건설","인",0.39,0,0,272915,106436.8,0,0,272915,106436.8,null,null,"N","N","",1]
["CBC31010000S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.62,0,0,223458,138543.9,0,0,223458,138543.9,null,null,"N","N","",1]
["CBC31010000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.53,0,0,214222,113537.60000000001,0,0,214222,113537.60000000001,null,null,"N","N","",1]
["CBC31010000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.62,0,0,165545,102637.9,0,0,165545,102637.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,461156,0,0,0,461156,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC32010000S",null,null,null,"천공 (자갈층)","NX, 20m 이내","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC32010000S","노무","L001020701000028",null,"중급기술자","건설","인",0.45,0,0,272915,122811.7,0,0,272915,122811.7,null,null,"N","N","",1]
["CBC32010000S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.72,0,0,223458,160889.70000000001,0,0,223458,160889.70000000001,null,null,"N","N","",1]
["CBC32010000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.63,0,0,214222,134959.79999999999,0,0,214222,134959.79999999999,null,null,"N","N","",1]
["CBC32010000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.73,0,0,165545,120847.8,0,0,165545,120847.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,539509,0,0,0,539509,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC41010000S",null,null,null,"천공 (호박돌층)","BX, 20m 이내","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC41010000S","노무","L001020701000028",null,"중급기술자","건설","인",0.65,0,0,272915,177394.7,0,0,272915,177394.7,null,null,"N","N","",1]
["CBC41010000S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.81,0,0,223458,181000.9,0,0,223458,181000.9,null,null,"N","N","",1]
["CBC41010000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.65,0,0,214222,139244.29999999999,0,0,214222,139244.29999999999,null,null,"N","N","",1]
["CBC41010000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.81,0,0,165545,134091.4,0,0,165545,134091.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,631731,0,0,0,631731,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC42010000S",null,null,null,"천공 (호박돌층)","NX, 20m 이내","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC42010000S","노무","L001020701000028",null,"중급기술자","건설","인",0.76,0,0,272915,207415.4,0,0,272915,207415.4,null,null,"N","N","",1]
["CBC42010000S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.96,0,0,223458,214519.6,0,0,223458,214519.6,null,null,"N","N","",1]
["CBC42010000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.76,0,0,214222,162808.70000000001,0,0,214222,162808.70000000001,null,null,"N","N","",1]
["CBC42010000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.96,0,0,165545,158923.20000000001,0,0,165545,158923.20000000001,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,743666,0,0,0,743666,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC51010000S",null,null,null,"천공 (풍화암)","BX, 20m 이내","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC51010000S","노무","L001020701000028",null,"중급기술자","건설","인",0.16,0,0,272915,43666.400000000001,0,0,272915,43666.400000000001,null,null,"N","N","",1]
["CBC51010000S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.3,0,0,223458,67037.399999999994,0,0,223458,67037.399999999994,null,null,"N","N","",1]
["CBC51010000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.22,0,0,214222,47128.800000000003,0,0,214222,47128.800000000003,null,null,"N","N","",1]
["CBC51010000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.3,0,0,165545,49663.5,0,0,165545,49663.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,207496,0,0,0,207496,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC52010000S",null,null,null,"천공 (풍화암)","NX, 20m 이내","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC52010000S","노무","L001020701000028",null,"중급기술자","건설","인",0.19,0,0,272915,51853.8,0,0,272915,51853.8,null,null,"N","N","",1]
["CBC52010000S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.35,0,0,223458,78210.3,0,0,223458,78210.3,null,null,"N","N","",1]
["CBC52010000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.26,0,0,214222,55697.7,0,0,214222,55697.7,null,null,"N","N","",1]
["CBC52010000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.35,0,0,165545,57940.7,0,0,165545,57940.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,243702,0,0,0,243702,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC61010000S",null,null,null,"천공 (연암)","BX, 20m 이내","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC61010000S","노무","L001020701000028",null,"중급기술자","건설","인",0.17,0,0,272915,46395.5,0,0,272915,46395.5,null,null,"N","N","",1]
["CBC61010000S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.31,0,0,223458,69271.899999999994,0,0,223458,69271.899999999994,null,null,"N","N","",1]
["CBC61010000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.24,0,0,214222,51413.2,0,0,214222,51413.2,null,null,"N","N","",1]
["CBC61010000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.31,0,0,165545,51318.9,0,0,165545,51318.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,218399,0,0,0,218399,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC62010000S",null,null,null,"천공 (연암)","NX, 20m 이내","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC62010000S","노무","L001020701000028",null,"중급기술자","건설","인",0.21,0,0,272915,57312.1,0,0,272915,57312.1,null,null,"N","N","",1]
["CBC62010000S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.37,0,0,223458,82679.399999999994,0,0,223458,82679.399999999994,null,null,"N","N","",1]
["CBC62010000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.28000000000000003,0,0,214222,59982.1,0,0,214222,59982.1,null,null,"N","N","",1]
["CBC62010000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.37,0,0,165545,61251.6,0,0,165545,61251.6,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,261225,0,0,0,261225,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC71010000S",null,null,null,"천공 (보통암)","BX, 20m 이내","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC71010000S","노무","L001020701000028",null,"중급기술자","건설","인",0.17,0,0,272915,46395.5,0,0,272915,46395.5,null,null,"N","N","",1]
["CBC71010000S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.4,0,0,223458,89383.2,0,0,223458,89383.2,null,null,"N","N","",1]
["CBC71010000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.2,0,0,214222,42844.4,0,0,214222,42844.4,null,null,"N","N","",1]
["CBC71010000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.4,0,0,165545,66218,0,0,165545,66218,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,244841,0,0,0,244841,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC72010000S",null,null,null,"천공 (보통암)","NX, 20m 이내","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC72010000S","노무","L001020701000028",null,"중급기술자","건설","인",0.2,0,0,272915,54583,0,0,272915,54583,null,null,"N","N","",1]
["CBC72010000S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.47,0,0,223458,105025.2,0,0,223458,105025.2,null,null,"N","N","",1]
["CBC72010000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.24,0,0,214222,51413.2,0,0,214222,51413.2,null,null,"N","N","",1]
["CBC72010000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.47,0,0,165545,77806.100000000006,0,0,165545,77806.100000000006,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,288827,0,0,0,288827,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC81010000S",null,null,null,"천공 (경암)","BX, 20m 이내","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC81010000S","노무","L001020701000028",null,"중급기술자","건설","인",0.33,0,0,272915,90061.9,0,0,272915,90061.9,null,null,"N","N","",1]
["CBC81010000S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.53,0,0,223458,118432.7,0,0,223458,118432.7,null,null,"N","N","",1]
["CBC81010000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.44,0,0,214222,94257.600000000006,0,0,214222,94257.600000000006,null,null,"N","N","",1]
["CBC81010000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.53,0,0,165545,87738.8,0,0,165545,87738.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,390491,0,0,0,390491,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC82010000S",null,null,null,"천공 (경암)","NX, 20m 이내","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC82010000S","노무","L001020701000028",null,"중급기술자","건설","인",0.39,0,0,272915,106436.8,0,0,272915,106436.8,null,null,"N","N","",1]
["CBC82010000S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.62,0,0,223458,138543.9,0,0,223458,138543.9,null,null,"N","N","",1]
["CBC82010000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.51,0,0,214222,109253.2,0,0,214222,109253.2,null,null,"N","N","",1]
["CBC82010000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.62,0,0,165545,102637.9,0,0,165545,102637.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,456871,0,0,0,456871,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC91010000S",null,null,null,"천공 (극경암)","BX, 20m 이내","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC91010000S","노무","L001020701000028",null,"중급기술자","건설","인",0.37,0,0,272915,100978.5,0,0,272915,100978.5,null,null,"N","N","",1]
["CBC91010000S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.63,0,0,223458,140778.5,0,0,223458,140778.5,null,null,"N","N","",1]
["CBC91010000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.47,0,0,214222,100684.3,0,0,214222,100684.3,null,null,"N","N","",1]
["CBC91010000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.63,0,0,165545,104293.3,0,0,165545,104293.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,446734,0,0,0,446734,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC92010000S",null,null,null,"천공 (극경암)","NX, 20m 이내","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBC92010000S","노무","L001020701000028",null,"중급기술자","건설","인",0.43,0,0,272915,117353.4,0,0,272915,117353.4,null,null,"N","N","",1]
["CBC92010000S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.75,0,0,223458,167593.5,0,0,223458,167593.5,null,null,"N","N","",1]
["CBC92010000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.56000000000000005,0,0,214222,119964.3,0,0,214222,119964.3,null,null,"N","N","",1]
["CBC92010000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.75,0,0,165545,124158.7,0,0,165545,124158.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,529069,0,0,0,529069,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD10000000S",null,null,null,"자연시료 채취",null,"회당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD10000000S","노무","L001020701000028",null,"중급기술자","건설","인",0.12,0,0,272915,32749.8,0,0,272915,32749.8,null,null,"N","N","",1]
["CBD10000000S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.22,0,0,223458,49160.7,0,0,223458,49160.7,null,null,"N","N","",1]
["CBD10000000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.16,0,0,214222,34275.5,0,0,214222,34275.5,null,null,"N","N","",1]
["CBD10000000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.22,0,0,165545,36419.9,0,0,165545,36419.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,152605,0,0,0,152605,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24100100S",null,null,null,"대구경보링 (토사층)","Ø100mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24100100S","노무","L001020701000028",null,"중급기술자","건설","인",0.01,0,0,272915,2729.1,0,0,272915,2729.1,null,null,"N","N","",1]
["CBD24100100S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.05,0,0,238259,11912.9,0,0,238259,11912.9,null,null,"N","N","",1]
["CBD24100100S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.05,0,0,223458,11172.9,0,0,223458,11172.9,null,null,"N","N","",1]
["CBD24100100S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.03,0,0,214222,6426.6,0,0,214222,6426.6,null,null,"N","N","",1]
["CBD24100100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.05,0,0,165545,8277.2000000000007,0,0,165545,8277.2000000000007,null,null,"N","N","",1]
["CBD24100100S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.21,75366,15826.8,55700,11697,149119,31314.9,280185,58838.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,15826,0,52215,0,31314,0,99355,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24100150S",null,null,null,"대구경보링 (토사층)","Ø150mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24100150S","노무","L001020701000028",null,"중급기술자","건설","인",0.02,0,0,272915,5458.3,0,0,272915,5458.3,null,null,"N","N","",1]
["CBD24100150S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.06,0,0,238259,14295.5,0,0,238259,14295.5,null,null,"N","N","",1]
["CBD24100150S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.06,0,0,223458,13407.4,0,0,223458,13407.4,null,null,"N","N","",1]
["CBD24100150S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.03,0,0,214222,6426.6,0,0,214222,6426.6,null,null,"N","N","",1]
["CBD24100150S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.06,0,0,165545,9932.7000000000007,0,0,165545,9932.7000000000007,null,null,"N","N","",1]
["CBD24100150S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.25,75366,18841.5,55700,13925,149119,37279.699999999997,280185,70046.2,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,18841,0,63445,0,37279,0,119565,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24100200S",null,null,null,"대구경보링 (토사층)","Ø200mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24100200S","노무","L001020701000028",null,"중급기술자","건설","인",0.02,0,0,272915,5458.3,0,0,272915,5458.3,null,null,"N","N","",1]
["CBD24100200S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.08,0,0,238259,19060.7,0,0,238259,19060.7,null,null,"N","N","",1]
["CBD24100200S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.08,0,0,223458,17876.599999999999,0,0,223458,17876.599999999999,null,null,"N","N","",1]
["CBD24100200S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.04,0,0,214222,8568.7999999999993,0,0,214222,8568.7999999999993,null,null,"N","N","",1]
["CBD24100200S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.08,0,0,165545,13243.6,0,0,165545,13243.6,null,null,"N","N","",1]
["CBD24100200S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.3,75366,22609.8,55700,16710,149119,44735.7,280185,84055.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,22609,0,80918,0,44735,0,148262,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24100250S",null,null,null,"대구경보링 (토사층)","Ø250mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24100250S","노무","L001020701000028",null,"중급기술자","건설","인",0.02,0,0,272915,5458.3,0,0,272915,5458.3,null,null,"N","N","",1]
["CBD24100250S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.09,0,0,238259,21443.3,0,0,238259,21443.3,null,null,"N","N","",1]
["CBD24100250S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.09,0,0,223458,20111.2,0,0,223458,20111.2,null,null,"N","N","",1]
["CBD24100250S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.04,0,0,214222,8568.7999999999993,0,0,214222,8568.7999999999993,null,null,"N","N","",1]
["CBD24100250S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.09,0,0,165545,14899,0,0,165545,14899,null,null,"N","N","",1]
["CBD24100250S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.35,75366,26378.1,55700,19495,149119,52191.6,280185,98064.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,26378,0,89975,0,52191,0,168544,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24100300S",null,null,null,"대구경보링 (토사층)","Ø300mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24100300S","노무","L001020701000028",null,"중급기술자","건설","인",0.02,0,0,272915,5458.3,0,0,272915,5458.3,null,null,"N","N","",1]
["CBD24100300S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.1,0,0,238259,23825.9,0,0,238259,23825.9,null,null,"N","N","",1]
["CBD24100300S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.1,0,0,223458,22345.8,0,0,223458,22345.8,null,null,"N","N","",1]
["CBD24100300S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.05,0,0,214222,10711.1,0,0,214222,10711.1,null,null,"N","N","",1]
["CBD24100300S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.1,0,0,165545,16554.5,0,0,165545,16554.5,null,null,"N","N","",1]
["CBD24100300S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.4,75366,30146.400000000001,55700,22280,149119,59647.6,280185,112074,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,30146,0,101175,0,59647,0,190968,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24100350S",null,null,null,"대구경보링 (토사층)","Ø350mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24100350S","노무","L001020701000028",null,"중급기술자","건설","인",0.03,0,0,272915,8187.4,0,0,272915,8187.4,null,null,"N","N","",1]
["CBD24100350S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.11,0,0,238259,26208.400000000001,0,0,238259,26208.400000000001,null,null,"N","N","",1]
["CBD24100350S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.11,0,0,223458,24580.3,0,0,223458,24580.3,null,null,"N","N","",1]
["CBD24100350S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.06,0,0,214222,12853.3,0,0,214222,12853.3,null,null,"N","N","",1]
["CBD24100350S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.11,0,0,165545,18209.900000000001,0,0,165545,18209.900000000001,null,null,"N","N","",1]
["CBD24100350S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.45,75366,33914.699999999997,55700,25065,149119,67103.5,280185,126083.2,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,33914,0,115104,0,67103,0,216121,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24100400S",null,null,null,"대구경보링 (토사층)","Ø400mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24100400S","노무","L001020701000028",null,"중급기술자","건설","인",0.03,0,0,272915,8187.4,0,0,272915,8187.4,null,null,"N","N","",1]
["CBD24100400S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.12,0,0,238259,28591,0,0,238259,28591,null,null,"N","N","",1]
["CBD24100400S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.12,0,0,223458,26814.9,0,0,223458,26814.9,null,null,"N","N","",1]
["CBD24100400S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.06,0,0,214222,12853.3,0,0,214222,12853.3,null,null,"N","N","",1]
["CBD24100400S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.12,0,0,165545,19865.400000000001,0,0,165545,19865.400000000001,null,null,"N","N","",1]
["CBD24100400S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.49,75366,36929.300000000003,55700,27293,149119,73068.3,280185,137290.6,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,36929,0,123605,0,73068,0,233602,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24100450S",null,null,null,"대구경보링 (토사층)","Ø450mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24100450S","노무","L001020701000028",null,"중급기술자","건설","인",0.04,0,0,272915,10916.6,0,0,272915,10916.6,null,null,"N","N","",1]
["CBD24100450S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.13,0,0,238259,30973.599999999999,0,0,238259,30973.599999999999,null,null,"N","N","",1]
["CBD24100450S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.13,0,0,223458,29049.5,0,0,223458,29049.5,null,null,"N","N","",1]
["CBD24100450S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.08,0,0,214222,17137.7,0,0,214222,17137.7,null,null,"N","N","",1]
["CBD24100450S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.13,0,0,165545,21520.799999999999,0,0,165545,21520.799999999999,null,null,"N","N","",1]
["CBD24100450S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.54,75366,40697.599999999999,55700,30078,149119,80524.2,280185,151299.79999999999,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,40697,0,139676,0,80524,0,260897,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24100500S",null,null,null,"대구경보링 (토사층)","Ø500mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24100500S","노무","L001020701000028",null,"중급기술자","건설","인",0.04,0,0,272915,10916.6,0,0,272915,10916.6,null,null,"N","N","",1]
["CBD24100500S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.14000000000000001,0,0,238259,33356.199999999997,0,0,238259,33356.199999999997,null,null,"N","N","",1]
["CBD24100500S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.14000000000000001,0,0,223458,31284.1,0,0,223458,31284.1,null,null,"N","N","",1]
["CBD24100500S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.08,0,0,214222,17137.7,0,0,214222,17137.7,null,null,"N","N","",1]
["CBD24100500S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.14000000000000001,0,0,165545,23176.3,0,0,165545,23176.3,null,null,"N","N","",1]
["CBD24100500S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.59,75366,44465.9,55700,32863,149119,87980.2,280185,165309.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,44465,0,148733,0,87980,0,281178,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24200100S",null,null,null,"대구경보링 (모래층)","Ø100mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24200100S","노무","L001020701000028",null,"중급기술자","건설","인",0.02,0,0,272915,5458.3,0,0,272915,5458.3,null,null,"N","N","",1]
["CBD24200100S","노무","L001020701000031",null,"중급숙련기술자","건설","인",7.0000000000000007E-2,0,0,238259,16678.099999999999,0,0,238259,16678.099999999999,null,null,"N","N","",1]
["CBD24200100S","노무","L001010101000014",null,"보링공","일반공사 직종","인",7.0000000000000007E-2,0,0,223458,15642,0,0,223458,15642,null,null,"N","N","",1]
["CBD24200100S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.03,0,0,214222,6426.6,0,0,214222,6426.6,null,null,"N","N","",1]
["CBD24200100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.0000000000000007E-2,0,0,165545,11588.1,0,0,165545,11588.1,null,null,"N","N","",1]
["CBD24200100S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.28000000000000003,75366,21102.400000000001,55700,15596,149119,41753.300000000003,280185,78451.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,21102,0,71389,0,41753,0,134244,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24200150S",null,null,null,"대구경보링 (모래층)","Ø150mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24200150S","노무","L001020701000028",null,"중급기술자","건설","인",0.02,0,0,272915,5458.3,0,0,272915,5458.3,null,null,"N","N","",1]
["CBD24200150S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.09,0,0,238259,21443.3,0,0,238259,21443.3,null,null,"N","N","",1]
["CBD24200150S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.09,0,0,223458,20111.2,0,0,223458,20111.2,null,null,"N","N","",1]
["CBD24200150S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.04,0,0,214222,8568.7999999999993,0,0,214222,8568.7999999999993,null,null,"N","N","",1]
["CBD24200150S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.09,0,0,165545,14899,0,0,165545,14899,null,null,"N","N","",1]
["CBD24200150S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.34,75366,25624.400000000001,55700,18938,149119,50700.4,280185,95262.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,25624,0,89418,0,50700,0,165742,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24200200S",null,null,null,"대구경보링 (모래층)","Ø200mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24200200S","노무","L001020701000028",null,"중급기술자","건설","인",0.03,0,0,272915,8187.4,0,0,272915,8187.4,null,null,"N","N","",1]
["CBD24200200S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.11,0,0,238259,26208.400000000001,0,0,238259,26208.400000000001,null,null,"N","N","",1]
["CBD24200200S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.11,0,0,223458,24580.3,0,0,223458,24580.3,null,null,"N","N","",1]
["CBD24200200S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.05,0,0,214222,10711.1,0,0,214222,10711.1,null,null,"N","N","",1]
["CBD24200200S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.11,0,0,165545,18209.900000000001,0,0,165545,18209.900000000001,null,null,"N","N","",1]
["CBD24200200S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.43,75366,32407.3,55700,23951,149119,64121.1,280185,120479.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,32407,0,111848,0,64121,0,208376,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24200250S",null,null,null,"대구경보링 (모래층)","Ø250mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24200250S","노무","L001020701000028",null,"중급기술자","건설","인",0.03,0,0,272915,8187.4,0,0,272915,8187.4,null,null,"N","N","",1]
["CBD24200250S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.13,0,0,238259,30973.599999999999,0,0,238259,30973.599999999999,null,null,"N","N","",1]
["CBD24200250S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.13,0,0,223458,29049.5,0,0,223458,29049.5,null,null,"N","N","",1]
["CBD24200250S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.06,0,0,214222,12853.3,0,0,214222,12853.3,null,null,"N","N","",1]
["CBD24200250S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.13,0,0,165545,21520.799999999999,0,0,165545,21520.799999999999,null,null,"N","N","",1]
["CBD24200250S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.51,75366,38436.6,55700,28407,149119,76050.600000000006,280185,142894.20000000001,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,38436,0,130991,0,76050,0,245477,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24200300S",null,null,null,"대구경보링 (모래층)","Ø300mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24200300S","노무","L001020701000028",null,"중급기술자","건설","인",0.04,0,0,272915,10916.6,0,0,272915,10916.6,null,null,"N","N","",1]
["CBD24200300S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.15,0,0,238259,35738.800000000003,0,0,238259,35738.800000000003,null,null,"N","N","",1]
["CBD24200300S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.15,0,0,223458,33518.699999999997,0,0,223458,33518.699999999997,null,null,"N","N","",1]
["CBD24200300S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",7.0000000000000007E-2,0,0,214222,14995.5,0,0,214222,14995.5,null,null,"N","N","",1]
["CBD24200300S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.15,0,0,165545,24831.7,0,0,165545,24831.7,null,null,"N","N","",1]
["CBD24200300S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.59,75366,44465.9,55700,32863,149119,87980.2,280185,165309.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,44465,0,152864,0,87980,0,285309,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24200350S",null,null,null,"대구경보링 (모래층)","Ø350mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24200350S","노무","L001020701000028",null,"중급기술자","건설","인",0.04,0,0,272915,10916.6,0,0,272915,10916.6,null,null,"N","N","",1]
["CBD24200350S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.16,0,0,238259,38121.4,0,0,238259,38121.4,null,null,"N","N","",1]
["CBD24200350S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.16,0,0,223458,35753.199999999997,0,0,223458,35753.199999999997,null,null,"N","N","",1]
["CBD24200350S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.08,0,0,214222,17137.7,0,0,214222,17137.7,null,null,"N","N","",1]
["CBD24200350S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.16,0,0,165545,26487.200000000001,0,0,165545,26487.200000000001,null,null,"N","N","",1]
["CBD24200350S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.65,75366,48987.9,55700,36205,149119,96927.3,280185,182120.2,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,48987,0,164621,0,96927,0,310535,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24200400S",null,null,null,"대구경보링 (모래층)","Ø400mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24200400S","노무","L001020701000028",null,"중급기술자","건설","인",0.05,0,0,272915,13645.7,0,0,272915,13645.7,null,null,"N","N","",1]
["CBD24200400S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.19,0,0,238259,45269.2,0,0,238259,45269.2,null,null,"N","N","",1]
["CBD24200400S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.19,0,0,223458,42457,0,0,223458,42457,null,null,"N","N","",1]
["CBD24200400S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.09,0,0,214222,19279.900000000001,0,0,214222,19279.900000000001,null,null,"N","N","",1]
["CBD24200400S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.19,0,0,165545,31453.5,0,0,165545,31453.5,null,null,"N","N","",1]
["CBD24200400S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.74,75366,55770.8,55700,41218,149119,110348,280185,207336.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,55770,0,193323,0,110348,0,359441,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24200450S",null,null,null,"대구경보링 (모래층)","Ø450mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24200450S","노무","L001020701000028",null,"중급기술자","건설","인",0.05,0,0,272915,13645.7,0,0,272915,13645.7,null,null,"N","N","",1]
["CBD24200450S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.21,0,0,238259,50034.3,0,0,238259,50034.3,null,null,"N","N","",1]
["CBD24200450S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.21,0,0,223458,46926.1,0,0,223458,46926.1,null,null,"N","N","",1]
["CBD24200450S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.1,0,0,214222,21422.2,0,0,214222,21422.2,null,null,"N","N","",1]
["CBD24200450S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.21,0,0,165545,34764.400000000001,0,0,165545,34764.400000000001,null,null,"N","N","",1]
["CBD24200450S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.82,75366,61800.1,55700,45674,149119,122277.5,280185,229751.6,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,61800,0,212466,0,122277,0,396543,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24200500S",null,null,null,"대구경보링 (모래층)","Ø500mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24200500S","노무","L001020701000028",null,"중급기술자","건설","인",0.06,0,0,272915,16374.9,0,0,272915,16374.9,null,null,"N","N","",1]
["CBD24200500S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.24,0,0,238259,57182.1,0,0,238259,57182.1,null,null,"N","N","",1]
["CBD24200500S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.24,0,0,223458,53629.9,0,0,223458,53629.9,null,null,"N","N","",1]
["CBD24200500S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.12,0,0,214222,25706.6,0,0,214222,25706.6,null,null,"N","N","",1]
["CBD24200500S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.24,0,0,165545,39730.800000000003,0,0,165545,39730.800000000003,null,null,"N","N","",1]
["CBD24200500S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.9,75366,67829.399999999994,55700,50130,149119,134207.1,280185,252166.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,67829,0,242754,0,134207,0,444790,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24300100S",null,null,null,"대구경보링 (자갈층)","Ø100mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24300100S","노무","L001020701000028",null,"중급기술자","건설","인",0.02,0,0,272915,5458.3,0,0,272915,5458.3,null,null,"N","N","",1]
["CBD24300100S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.1,0,0,238259,23825.9,0,0,238259,23825.9,null,null,"N","N","",1]
["CBD24300100S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.1,0,0,223458,22345.8,0,0,223458,22345.8,null,null,"N","N","",1]
["CBD24300100S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.05,0,0,214222,10711.1,0,0,214222,10711.1,null,null,"N","N","",1]
["CBD24300100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.1,0,0,165545,16554.5,0,0,165545,16554.5,null,null,"N","N","",1]
["CBD24300100S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.38,75366,28639,55700,21166,149119,56665.2,280185,106470.2,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,28639,0,100061,0,56665,0,185365,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24300150S",null,null,null,"대구경보링 (자갈층)","Ø150mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24300150S","노무","L001020701000028",null,"중급기술자","건설","인",0.03,0,0,272915,8187.4,0,0,272915,8187.4,null,null,"N","N","",1]
["CBD24300150S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.13,0,0,238259,30973.599999999999,0,0,238259,30973.599999999999,null,null,"N","N","",1]
["CBD24300150S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.13,0,0,223458,29049.5,0,0,223458,29049.5,null,null,"N","N","",1]
["CBD24300150S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.06,0,0,214222,12853.3,0,0,214222,12853.3,null,null,"N","N","",1]
["CBD24300150S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.13,0,0,165545,21520.799999999999,0,0,165545,21520.799999999999,null,null,"N","N","",1]
["CBD24300150S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.52,75366,39190.300000000003,55700,28964,149119,77541.8,280185,145696.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,39190,0,131548,0,77541,0,248279,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24300200S",null,null,null,"대구경보링 (자갈층)","Ø200mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24300200S","노무","L001020701000028",null,"중급기술자","건설","인",0.04,0,0,272915,10916.6,0,0,272915,10916.6,null,null,"N","N","",1]
["CBD24300200S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.16,0,0,238259,38121.4,0,0,238259,38121.4,null,null,"N","N","",1]
["CBD24300200S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.16,0,0,223458,35753.199999999997,0,0,223458,35753.199999999997,null,null,"N","N","",1]
["CBD24300200S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.08,0,0,214222,17137.7,0,0,214222,17137.7,null,null,"N","N","",1]
["CBD24300200S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.16,0,0,165545,26487.200000000001,0,0,165545,26487.200000000001,null,null,"N","N","",1]
["CBD24300200S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.65,75366,48987.9,55700,36205,149119,96927.3,280185,182120.2,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,48987,0,164621,0,96927,0,310535,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24300250S",null,null,null,"대구경보링 (자갈층)","Ø250mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24300250S","노무","L001020701000028",null,"중급기술자","건설","인",0.05,0,0,272915,13645.7,0,0,272915,13645.7,null,null,"N","N","",1]
["CBD24300250S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.2,0,0,238259,47651.8,0,0,238259,47651.8,null,null,"N","N","",1]
["CBD24300250S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.2,0,0,223458,44691.6,0,0,223458,44691.6,null,null,"N","N","",1]
["CBD24300250S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.1,0,0,214222,21422.2,0,0,214222,21422.2,null,null,"N","N","",1]
["CBD24300250S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.2,0,0,165545,33109,0,0,165545,33109,null,null,"N","N","",1]
["CBD24300250S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.81,75366,61046.400000000001,55700,45117,149119,120786.3,280185,226949.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,61046,0,205637,0,120786,0,387469,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24300300S",null,null,null,"대구경보링 (자갈층)","Ø300mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24300300S","노무","L001020701000028",null,"중급기술자","건설","인",0.06,0,0,272915,16374.9,0,0,272915,16374.9,null,null,"N","N","",1]
["CBD24300300S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.24,0,0,238259,57182.1,0,0,238259,57182.1,null,null,"N","N","",1]
["CBD24300300S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.24,0,0,223458,53629.9,0,0,223458,53629.9,null,null,"N","N","",1]
["CBD24300300S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.12,0,0,214222,25706.6,0,0,214222,25706.6,null,null,"N","N","",1]
["CBD24300300S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.24,0,0,165545,39730.800000000003,0,0,165545,39730.800000000003,null,null,"N","N","",1]
["CBD24300300S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.97,75366,73105,55700,54029,149119,144645.4,280185,271779.40000000002,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,73105,0,246653,0,144645,0,464403,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24300350S",null,null,null,"대구경보링 (자갈층)","Ø350mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24300350S","노무","L001020701000028",null,"중급기술자","건설","인",7.0000000000000007E-2,0,0,272915,19104,0,0,272915,19104,null,null,"N","N","",1]
["CBD24300350S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.28000000000000003,0,0,238259,66712.5,0,0,238259,66712.5,null,null,"N","N","",1]
["CBD24300350S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.28000000000000003,0,0,223458,62568.2,0,0,223458,62568.2,null,null,"N","N","",1]
["CBD24300350S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.14000000000000001,0,0,214222,29991,0,0,214222,29991,null,null,"N","N","",1]
["CBD24300350S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.28000000000000003,0,0,165545,46352.6,0,0,165545,46352.6,null,null,"N","N","",1]
["CBD24300350S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",1.1100000000000001,75366,83656.2,55700,61827,149119,165522,280185,311005.2,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,83656,0,286555,0,165522,0,535733,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24300400S",null,null,null,"대구경보링 (자갈층)","Ø400mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24300400S","노무","L001020701000028",null,"중급기술자","건설","인",0.08,0,0,272915,21833.200000000001,0,0,272915,21833.200000000001,null,null,"N","N","",1]
["CBD24300400S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.32,0,0,238259,76242.8,0,0,238259,76242.8,null,null,"N","N","",1]
["CBD24300400S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.32,0,0,223458,71506.5,0,0,223458,71506.5,null,null,"N","N","",1]
["CBD24300400S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.16,0,0,214222,34275.5,0,0,214222,34275.5,null,null,"N","N","",1]
["CBD24300400S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.32,0,0,165545,52974.400000000001,0,0,165545,52974.400000000001,null,null,"N","N","",1]
["CBD24300400S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",1.27,75366,95714.8,55700,70739,149119,189381.1,280185,355834.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,95714,0,327571,0,189381,0,612666,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24300450S",null,null,null,"대구경보링 (자갈층)","Ø450mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24300450S","노무","L001020701000028",null,"중급기술자","건설","인",0.09,0,0,272915,24562.3,0,0,272915,24562.3,null,null,"N","N","",1]
["CBD24300450S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.36,0,0,238259,85773.2,0,0,238259,85773.2,null,null,"N","N","",1]
["CBD24300450S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.36,0,0,223458,80444.800000000003,0,0,223458,80444.800000000003,null,null,"N","N","",1]
["CBD24300450S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.18,0,0,214222,38559.9,0,0,214222,38559.9,null,null,"N","N","",1]
["CBD24300450S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.36,0,0,165545,59596.2,0,0,165545,59596.2,null,null,"N","N","",1]
["CBD24300450S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",1.42,75366,107019.7,55700,79094,149119,211748.9,280185,397862.6,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,107019,0,368030,0,211748,0,686797,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24300500S",null,null,null,"대구경보링 (자갈층)","Ø500mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24300500S","노무","L001020701000028",null,"중급기술자","건설","인",0.1,0,0,272915,27291.5,0,0,272915,27291.5,null,null,"N","N","",1]
["CBD24300500S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.4,0,0,238259,95303.6,0,0,238259,95303.6,null,null,"N","N","",1]
["CBD24300500S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.4,0,0,223458,89383.2,0,0,223458,89383.2,null,null,"N","N","",1]
["CBD24300500S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.2,0,0,214222,42844.4,0,0,214222,42844.4,null,null,"N","N","",1]
["CBD24300500S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.4,0,0,165545,66218,0,0,165545,66218,null,null,"N","N","",1]
["CBD24300500S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",1.57,75366,118324.6,55700,87449,149119,234116.8,280185,439890.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,118324,0,408489,0,234116,0,760929,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24400100S",null,null,null,"대구경보링 (호박돌)","Ø100mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24400100S","노무","L001020701000028",null,"중급기술자","건설","인",0.04,0,0,272915,10916.6,0,0,272915,10916.6,null,null,"N","N","",1]
["CBD24400100S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.15,0,0,238259,35738.800000000003,0,0,238259,35738.800000000003,null,null,"N","N","",1]
["CBD24400100S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.15,0,0,223458,33518.699999999997,0,0,223458,33518.699999999997,null,null,"N","N","",1]
["CBD24400100S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",7.0000000000000007E-2,0,0,214222,14995.5,0,0,214222,14995.5,null,null,"N","N","",1]
["CBD24400100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.15,0,0,165545,24831.7,0,0,165545,24831.7,null,null,"N","N","",1]
["CBD24400100S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.59,75366,44465.9,55700,32863,149119,87980.2,280185,165309.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,44465,0,152864,0,87980,0,285309,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24400150S",null,null,null,"대구경보링 (호박돌)","Ø150mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24400150S","노무","L001020701000028",null,"중급기술자","건설","인",0.05,0,0,272915,13645.7,0,0,272915,13645.7,null,null,"N","N","",1]
["CBD24400150S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.21,0,0,238259,50034.3,0,0,238259,50034.3,null,null,"N","N","",1]
["CBD24400150S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.21,0,0,223458,46926.1,0,0,223458,46926.1,null,null,"N","N","",1]
["CBD24400150S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.11,0,0,214222,23564.400000000001,0,0,214222,23564.400000000001,null,null,"N","N","",1]
["CBD24400150S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.21,0,0,165545,34764.400000000001,0,0,165545,34764.400000000001,null,null,"N","N","",1]
["CBD24400150S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.86,75366,64814.7,55700,47902,149119,128242.3,280185,240959,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,64814,0,216836,0,128242,0,409892,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24400200S",null,null,null,"대구경보링 (호박돌)","Ø200mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24400200S","노무","L001020701000028",null,"중급기술자","건설","인",7.0000000000000007E-2,0,0,272915,19104,0,0,272915,19104,null,null,"N","N","",1]
["CBD24400200S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.28999999999999998,0,0,238259,69095.100000000006,0,0,238259,69095.100000000006,null,null,"N","N","",1]
["CBD24400200S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.28999999999999998,0,0,223458,64802.8,0,0,223458,64802.8,null,null,"N","N","",1]
["CBD24400200S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.14000000000000001,0,0,214222,29991,0,0,214222,29991,null,null,"N","N","",1]
["CBD24400200S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.28999999999999998,0,0,165545,48008,0,0,165545,48008,null,null,"N","N","",1]
["CBD24400200S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",1.1399999999999999,75366,85917.2,55700,63498,149119,169995.6,280185,319410.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,85917,0,294498,0,169995,0,550410,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24400250S",null,null,null,"대구경보링 (호박돌)","Ø250mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24400250S","노무","L001020701000028",null,"중급기술자","건설","인",0.09,0,0,272915,24562.3,0,0,272915,24562.3,null,null,"N","N","",1]
["CBD24400250S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.37,0,0,238259,88155.8,0,0,238259,88155.8,null,null,"N","N","",1]
["CBD24400250S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.37,0,0,223458,82679.399999999994,0,0,223458,82679.399999999994,null,null,"N","N","",1]
["CBD24400250S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.19,0,0,214222,40702.1,0,0,214222,40702.1,null,null,"N","N","",1]
["CBD24400250S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.37,0,0,165545,61251.6,0,0,165545,61251.6,null,null,"N","N","",1]
["CBD24400250S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",1.48,75366,111541.6,55700,82436,149119,220696.1,280185,414673.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,111541,0,379787,0,220696,0,712024,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24400300S",null,null,null,"대구경보링 (호박돌)","Ø300mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24400300S","노무","L001020701000028",null,"중급기술자","건설","인",0.12,0,0,272915,32749.8,0,0,272915,32749.8,null,null,"N","N","",1]
["CBD24400300S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.47,0,0,238259,111981.7,0,0,238259,111981.7,null,null,"N","N","",1]
["CBD24400300S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.47,0,0,223458,105025.2,0,0,223458,105025.2,null,null,"N","N","",1]
["CBD24400300S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.23,0,0,214222,49271,0,0,214222,49271,null,null,"N","N","",1]
["CBD24400300S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.47,0,0,165545,77806.100000000006,0,0,165545,77806.100000000006,null,null,"N","N","",1]
["CBD24400300S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",1.86,75366,140180.70000000001,55700,103602,149119,277361.3,280185,521144,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,140180,0,480435,0,277361,0,897976,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24400350S",null,null,null,"대구경보링 (호박돌)","Ø350mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24400350S","노무","L001020701000028",null,"중급기술자","건설","인",0.14000000000000001,0,0,272915,38208.1,0,0,272915,38208.1,null,null,"N","N","",1]
["CBD24400350S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.56000000000000005,0,0,238259,133425,0,0,238259,133425,null,null,"N","N","",1]
["CBD24400350S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.56000000000000005,0,0,223458,125136.4,0,0,223458,125136.4,null,null,"N","N","",1]
["CBD24400350S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.28000000000000003,0,0,214222,59982.1,0,0,214222,59982.1,null,null,"N","N","",1]
["CBD24400350S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.56000000000000005,0,0,165545,92705.2,0,0,165545,92705.2,null,null,"N","N","",1]
["CBD24400350S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",2.23,75366,168066.1,55700,124211,149119,332535.3,280185,624812.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,168066,0,573667,0,332535,0,1074268,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24400400S",null,null,null,"대구경보링 (호박돌)","Ø400mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24400400S","노무","L001020701000028",null,"중급기술자","건설","인",0.16,0,0,272915,43666.400000000001,0,0,272915,43666.400000000001,null,null,"N","N","",1]
["CBD24400400S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.66,0,0,238259,157250.9,0,0,238259,157250.9,null,null,"N","N","",1]
["CBD24400400S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.66,0,0,223458,147482.20000000001,0,0,223458,147482.20000000001,null,null,"N","N","",1]
["CBD24400400S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.33,0,0,214222,70693.2,0,0,214222,70693.2,null,null,"N","N","",1]
["CBD24400400S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.66,0,0,165545,109259.7,0,0,165545,109259.7,null,null,"N","N","",1]
["CBD24400400S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",2.62,75366,197458.9,55700,145934,149119,390691.7,280185,734084.6,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,197458,0,674286,0,390691,0,1262435,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24400450S",null,null,null,"대구경보링 (호박돌)","Ø450mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24400450S","노무","L001020701000028",null,"중급기술자","건설","인",0.18,0,0,272915,49124.7,0,0,272915,49124.7,null,null,"N","N","",1]
["CBD24400450S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.75,0,0,238259,178694.2,0,0,238259,178694.2,null,null,"N","N","",1]
["CBD24400450S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.75,0,0,223458,167593.5,0,0,223458,167593.5,null,null,"N","N","",1]
["CBD24400450S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.38,0,0,214222,81404.3,0,0,214222,81404.3,null,null,"N","N","",1]
["CBD24400450S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.75,0,0,165545,124158.7,0,0,165545,124158.7,null,null,"N","N","",1]
["CBD24400450S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",2.99,75366,225344.3,55700,166543,149119,445865.8,280185,837753.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,225344,0,767518,0,445865,0,1438727,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24400500S",null,null,null,"대구경보링 (호박돌)","Ø500mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24400500S","노무","L001020701000028",null,"중급기술자","건설","인",0.2,0,0,272915,54583,0,0,272915,54583,null,null,"N","N","",1]
["CBD24400500S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.84,0,0,238259,200137.5,0,0,238259,200137.5,null,null,"N","N","",1]
["CBD24400500S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.84,0,0,223458,187704.7,0,0,223458,187704.7,null,null,"N","N","",1]
["CBD24400500S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.43,0,0,214222,92115.4,0,0,214222,92115.4,null,null,"N","N","",1]
["CBD24400500S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.84,0,0,165545,139057.79999999999,0,0,165545,139057.79999999999,null,null,"N","N","",1]
["CBD24400500S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",3.36,75366,253229.7,55700,187152,149119,501039.8,280185,941421.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,253229,0,860750,0,501039,0,1615018,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24500100S",null,null,null,"대구경보링 (풍화암)","Ø100mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24500100S","노무","L001020701000028",null,"중급기술자","건설","인",0.02,0,0,272915,5458.3,0,0,272915,5458.3,null,null,"N","N","",1]
["CBD24500100S","노무","L001020701000031",null,"중급숙련기술자","건설","인",7.0000000000000007E-2,0,0,238259,16678.099999999999,0,0,238259,16678.099999999999,null,null,"N","N","",1]
["CBD24500100S","노무","L001010101000014",null,"보링공","일반공사 직종","인",7.0000000000000007E-2,0,0,223458,15642,0,0,223458,15642,null,null,"N","N","",1]
["CBD24500100S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.03,0,0,214222,6426.6,0,0,214222,6426.6,null,null,"N","N","",1]
["CBD24500100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.0000000000000007E-2,0,0,165545,11588.1,0,0,165545,11588.1,null,null,"N","N","",1]
["CBD24500100S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.26,75366,19595.099999999999,55700,14482,149119,38770.9,280185,72848,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,19595,0,70275,0,38770,0,128640,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24500150S",null,null,null,"대구경보링 (풍화암)","Ø150mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24500150S","노무","L001020701000028",null,"중급기술자","건설","인",0.02,0,0,272915,5458.3,0,0,272915,5458.3,null,null,"N","N","",1]
["CBD24500150S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.09,0,0,238259,21443.3,0,0,238259,21443.3,null,null,"N","N","",1]
["CBD24500150S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.09,0,0,223458,20111.2,0,0,223458,20111.2,null,null,"N","N","",1]
["CBD24500150S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.04,0,0,214222,8568.7999999999993,0,0,214222,8568.7999999999993,null,null,"N","N","",1]
["CBD24500150S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.09,0,0,165545,14899,0,0,165545,14899,null,null,"N","N","",1]
["CBD24500150S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.34,75366,25624.400000000001,55700,18938,149119,50700.4,280185,95262.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,25624,0,89418,0,50700,0,165742,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24500200S",null,null,null,"대구경보링 (풍화암)","Ø200mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24500200S","노무","L001020701000028",null,"중급기술자","건설","인",0.03,0,0,272915,8187.4,0,0,272915,8187.4,null,null,"N","N","",1]
["CBD24500200S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.11,0,0,238259,26208.400000000001,0,0,238259,26208.400000000001,null,null,"N","N","",1]
["CBD24500200S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.11,0,0,223458,24580.3,0,0,223458,24580.3,null,null,"N","N","",1]
["CBD24500200S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.06,0,0,214222,12853.3,0,0,214222,12853.3,null,null,"N","N","",1]
["CBD24500200S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.11,0,0,165545,18209.900000000001,0,0,165545,18209.900000000001,null,null,"N","N","",1]
["CBD24500200S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.45,75366,33914.699999999997,55700,25065,149119,67103.5,280185,126083.2,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,33914,0,115104,0,67103,0,216121,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24500250S",null,null,null,"대구경보링 (풍화암)","Ø250mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24500250S","노무","L001020701000028",null,"중급기술자","건설","인",0.03,0,0,272915,8187.4,0,0,272915,8187.4,null,null,"N","N","",1]
["CBD24500250S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.14000000000000001,0,0,238259,33356.199999999997,0,0,238259,33356.199999999997,null,null,"N","N","",1]
["CBD24500250S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.14000000000000001,0,0,223458,31284.1,0,0,223458,31284.1,null,null,"N","N","",1]
["CBD24500250S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",7.0000000000000007E-2,0,0,214222,14995.5,0,0,214222,14995.5,null,null,"N","N","",1]
["CBD24500250S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.14000000000000001,0,0,165545,23176.3,0,0,165545,23176.3,null,null,"N","N","",1]
["CBD24500250S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.54,75366,40697.599999999999,55700,30078,149119,80524.2,280185,151299.79999999999,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,40697,0,141077,0,80524,0,262298,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24500300S",null,null,null,"대구경보링 (풍화암)","Ø300mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24500300S","노무","L001020701000028",null,"중급기술자","건설","인",0.04,0,0,272915,10916.6,0,0,272915,10916.6,null,null,"N","N","",1]
["CBD24500300S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.16,0,0,238259,38121.4,0,0,238259,38121.4,null,null,"N","N","",1]
["CBD24500300S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.16,0,0,223458,35753.199999999997,0,0,223458,35753.199999999997,null,null,"N","N","",1]
["CBD24500300S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.08,0,0,214222,17137.7,0,0,214222,17137.7,null,null,"N","N","",1]
["CBD24500300S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.16,0,0,165545,26487.200000000001,0,0,165545,26487.200000000001,null,null,"N","N","",1]
["CBD24500300S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.64,75366,48234.2,55700,35648,149119,95436.1,280185,179318.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,48234,0,164064,0,95436,0,307734,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24500350S",null,null,null,"대구경보링 (풍화암)","Ø350mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24500350S","노무","L001020701000028",null,"중급기술자","건설","인",0.04,0,0,272915,10916.6,0,0,272915,10916.6,null,null,"N","N","",1]
["CBD24500350S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.18,0,0,238259,42886.6,0,0,238259,42886.6,null,null,"N","N","",1]
["CBD24500350S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.18,0,0,223458,40222.400000000001,0,0,223458,40222.400000000001,null,null,"N","N","",1]
["CBD24500350S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.09,0,0,214222,19279.900000000001,0,0,214222,19279.900000000001,null,null,"N","N","",1]
["CBD24500350S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.18,0,0,165545,29798.1,0,0,165545,29798.1,null,null,"N","N","",1]
["CBD24500350S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.72,75366,54263.5,55700,40104,149119,107365.6,280185,201733.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,54263,0,183207,0,107365,0,344835,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24500400S",null,null,null,"대구경보링 (풍화암)","Ø400mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24500400S","노무","L001020701000028",null,"중급기술자","건설","인",0.05,0,0,272915,13645.7,0,0,272915,13645.7,null,null,"N","N","",1]
["CBD24500400S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.21,0,0,238259,50034.3,0,0,238259,50034.3,null,null,"N","N","",1]
["CBD24500400S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.21,0,0,223458,46926.1,0,0,223458,46926.1,null,null,"N","N","",1]
["CBD24500400S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.1,0,0,214222,21422.2,0,0,214222,21422.2,null,null,"N","N","",1]
["CBD24500400S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.21,0,0,165545,34764.400000000001,0,0,165545,34764.400000000001,null,null,"N","N","",1]
["CBD24500400S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.82,75366,61800.1,55700,45674,149119,122277.5,280185,229751.6,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,61800,0,212466,0,122277,0,396543,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24500450S",null,null,null,"대구경보링 (풍화암)","Ø450mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24500450S","노무","L001020701000028",null,"중급기술자","건설","인",0.05,0,0,272915,13645.7,0,0,272915,13645.7,null,null,"N","N","",1]
["CBD24500450S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.23,0,0,238259,54799.5,0,0,238259,54799.5,null,null,"N","N","",1]
["CBD24500450S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.23,0,0,223458,51395.3,0,0,223458,51395.3,null,null,"N","N","",1]
["CBD24500450S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.11,0,0,214222,23564.400000000001,0,0,214222,23564.400000000001,null,null,"N","N","",1]
["CBD24500450S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.23,0,0,165545,38075.300000000003,0,0,165545,38075.300000000003,null,null,"N","N","",1]
["CBD24500450S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.91,75366,68583,55700,50687,149119,135698.20000000001,280185,254968.2,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,68583,0,232167,0,135698,0,436448,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24500500S",null,null,null,"대구경보링 (풍화암)","Ø500mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24500500S","노무","L001020701000028",null,"중급기술자","건설","인",0.06,0,0,272915,16374.9,0,0,272915,16374.9,null,null,"N","N","",1]
["CBD24500500S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.25,0,0,238259,59564.7,0,0,238259,59564.7,null,null,"N","N","",1]
["CBD24500500S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.25,0,0,223458,55864.5,0,0,223458,55864.5,null,null,"N","N","",1]
["CBD24500500S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.12,0,0,214222,25706.6,0,0,214222,25706.6,null,null,"N","N","",1]
["CBD24500500S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.25,0,0,165545,41386.199999999997,0,0,165545,41386.199999999997,null,null,"N","N","",1]
["CBD24500500S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",1,75366,75366,55700,55700,149119,149119,280185,280185,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,75366,0,254596,0,149119,0,479081,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24600100S",null,null,null,"대구경보링 (연암)","Ø100mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24600100S","노무","L001020701000028",null,"중급기술자","건설","인",0.01,0,0,272915,2729.1,0,0,272915,2729.1,null,null,"N","N","",1]
["CBD24600100S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.03,0,0,238259,7147.7,0,0,238259,7147.7,null,null,"N","N","",1]
["CBD24600100S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.03,0,0,223458,6703.7,0,0,223458,6703.7,null,null,"N","N","",1]
["CBD24600100S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.02,0,0,214222,4284.3999999999996,0,0,214222,4284.3999999999996,null,null,"N","N","",1]
["CBD24600100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.03,0,0,165545,4966.3,0,0,165545,4966.3,null,null,"N","N","",1]
["CBD24600100S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.13,75366,9797.5,55700,7241,149119,19385.400000000001,280185,36423.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,9797,0,33072,0,19385,0,62254,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24600150S",null,null,null,"대구경보링 (연암)","Ø150mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24600150S","노무","L001020701000028",null,"중급기술자","건설","인",0.01,0,0,272915,2729.1,0,0,272915,2729.1,null,null,"N","N","",1]
["CBD24600150S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.04,0,0,238259,9530.2999999999993,0,0,238259,9530.2999999999993,null,null,"N","N","",1]
["CBD24600150S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.04,0,0,223458,8938.2999999999993,0,0,223458,8938.2999999999993,null,null,"N","N","",1]
["CBD24600150S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.02,0,0,214222,4284.3999999999996,0,0,214222,4284.3999999999996,null,null,"N","N","",1]
["CBD24600150S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.04,0,0,165545,6621.8,0,0,165545,6621.8,null,null,"N","N","",1]
["CBD24600150S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.14000000000000001,75366,10551.2,55700,7798,149119,20876.599999999999,280185,39225.800000000003,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,10551,0,39901,0,20876,0,71328,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24600200S",null,null,null,"대구경보링 (연암)","Ø200mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24600200S","노무","L001020701000028",null,"중급기술자","건설","인",0.01,0,0,272915,2729.1,0,0,272915,2729.1,null,null,"N","N","",1]
["CBD24600200S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.05,0,0,238259,11912.9,0,0,238259,11912.9,null,null,"N","N","",1]
["CBD24600200S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.05,0,0,223458,11172.9,0,0,223458,11172.9,null,null,"N","N","",1]
["CBD24600200S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.02,0,0,214222,4284.3999999999996,0,0,214222,4284.3999999999996,null,null,"N","N","",1]
["CBD24600200S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.05,0,0,165545,8277.2000000000007,0,0,165545,8277.2000000000007,null,null,"N","N","",1]
["CBD24600200S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.19,75366,14319.5,55700,10583,149119,28332.6,280185,53235.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,14319,0,48959,0,28332,0,91610,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24600250S",null,null,null,"대구경보링 (연암)","Ø250mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24600250S","노무","L001020701000028",null,"중급기술자","건설","인",0.02,0,0,272915,5458.3,0,0,272915,5458.3,null,null,"N","N","",1]
["CBD24600250S","노무","L001020701000031",null,"중급숙련기술자","건설","인",7.0000000000000007E-2,0,0,238259,16678.099999999999,0,0,238259,16678.099999999999,null,null,"N","N","",1]
["CBD24600250S","노무","L001010101000014",null,"보링공","일반공사 직종","인",7.0000000000000007E-2,0,0,223458,15642,0,0,223458,15642,null,null,"N","N","",1]
["CBD24600250S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.03,0,0,214222,6426.6,0,0,214222,6426.6,null,null,"N","N","",1]
["CBD24600250S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.0000000000000007E-2,0,0,165545,11588.1,0,0,165545,11588.1,null,null,"N","N","",1]
["CBD24600250S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.27,75366,20348.8,55700,15039,149119,40262.1,280185,75649.899999999994,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,20348,0,70832,0,40262,0,131442,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24600300S",null,null,null,"대구경보링 (연암)","Ø300mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24600300S","노무","L001020701000028",null,"중급기술자","건설","인",0.02,0,0,272915,5458.3,0,0,272915,5458.3,null,null,"N","N","",1]
["CBD24600300S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.09,0,0,238259,21443.3,0,0,238259,21443.3,null,null,"N","N","",1]
["CBD24600300S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.09,0,0,223458,20111.2,0,0,223458,20111.2,null,null,"N","N","",1]
["CBD24600300S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.05,0,0,214222,10711.1,0,0,214222,10711.1,null,null,"N","N","",1]
["CBD24600300S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.09,0,0,165545,14899,0,0,165545,14899,null,null,"N","N","",1]
["CBD24600300S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.38,75366,28639,55700,21166,149119,56665.2,280185,106470.2,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,28639,0,93788,0,56665,0,179092,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24600350S",null,null,null,"대구경보링 (연암)","Ø350mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24600350S","노무","L001020701000028",null,"중급기술자","건설","인",0.03,0,0,272915,8187.4,0,0,272915,8187.4,null,null,"N","N","",1]
["CBD24600350S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.13,0,0,238259,30973.599999999999,0,0,238259,30973.599999999999,null,null,"N","N","",1]
["CBD24600350S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.13,0,0,223458,29049.5,0,0,223458,29049.5,null,null,"N","N","",1]
["CBD24600350S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",7.0000000000000007E-2,0,0,214222,14995.5,0,0,214222,14995.5,null,null,"N","N","",1]
["CBD24600350S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.13,0,0,165545,21520.799999999999,0,0,165545,21520.799999999999,null,null,"N","N","",1]
["CBD24600350S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.53,75366,39943.9,55700,29521,149119,79033,280185,148497.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,39943,0,134247,0,79033,0,253223,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24700100S",null,null,null,"대구경보링 (보통암)","Ø100mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24700100S","노무","L001020701000028",null,"중급기술자","건설","인",0.02,0,0,272915,5458.3,0,0,272915,5458.3,null,null,"N","N","",1]
["CBD24700100S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.05,0,0,238259,11912.9,0,0,238259,11912.9,null,null,"N","N","",1]
["CBD24700100S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.05,0,0,223458,11172.9,0,0,223458,11172.9,null,null,"N","N","",1]
["CBD24700100S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.03,0,0,214222,6426.6,0,0,214222,6426.6,null,null,"N","N","",1]
["CBD24700100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.05,0,0,165545,8277.2000000000007,0,0,165545,8277.2000000000007,null,null,"N","N","",1]
["CBD24700100S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.26,75366,19595.099999999999,55700,14482,149119,38770.9,280185,72848,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,19595,0,57729,0,38770,0,116094,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24700150S",null,null,null,"대구경보링 (보통암)","Ø150mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24700150S","노무","L001020701000028",null,"중급기술자","건설","인",0.02,0,0,272915,5458.3,0,0,272915,5458.3,null,null,"N","N","",1]
["CBD24700150S","노무","L001020701000031",null,"중급숙련기술자","건설","인",7.0000000000000007E-2,0,0,238259,16678.099999999999,0,0,238259,16678.099999999999,null,null,"N","N","",1]
["CBD24700150S","노무","L001010101000014",null,"보링공","일반공사 직종","인",7.0000000000000007E-2,0,0,223458,15642,0,0,223458,15642,null,null,"N","N","",1]
["CBD24700150S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.04,0,0,214222,8568.7999999999993,0,0,214222,8568.7999999999993,null,null,"N","N","",1]
["CBD24700150S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.0000000000000007E-2,0,0,165545,11588.1,0,0,165545,11588.1,null,null,"N","N","",1]
["CBD24700150S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.28999999999999998,75366,21856.1,55700,16153,149119,43244.5,280185,81253.600000000006,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,21856,0,74088,0,43244,0,139188,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24700200S",null,null,null,"대구경보링 (보통암)","Ø200mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24700200S","노무","L001020701000028",null,"중급기술자","건설","인",0.02,0,0,272915,5458.3,0,0,272915,5458.3,null,null,"N","N","",1]
["CBD24700200S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.08,0,0,238259,19060.7,0,0,238259,19060.7,null,null,"N","N","",1]
["CBD24700200S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.08,0,0,223458,17876.599999999999,0,0,223458,17876.599999999999,null,null,"N","N","",1]
["CBD24700200S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.04,0,0,214222,8568.7999999999993,0,0,214222,8568.7999999999993,null,null,"N","N","",1]
["CBD24700200S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.08,0,0,165545,13243.6,0,0,165545,13243.6,null,null,"N","N","",1]
["CBD24700200S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.31,75366,23363.4,55700,17267,149119,46226.8,280185,86857.2,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,23363,0,81475,0,46226,0,151064,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24700250S",null,null,null,"대구경보링 (보통암)","Ø250mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24700250S","노무","L001020701000028",null,"중급기술자","건설","인",0.03,0,0,272915,8187.4,0,0,272915,8187.4,null,null,"N","N","",1]
["CBD24700250S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.11,0,0,238259,26208.400000000001,0,0,238259,26208.400000000001,null,null,"N","N","",1]
["CBD24700250S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.11,0,0,223458,24580.3,0,0,223458,24580.3,null,null,"N","N","",1]
["CBD24700250S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.06,0,0,214222,12853.3,0,0,214222,12853.3,null,null,"N","N","",1]
["CBD24700250S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.11,0,0,165545,18209.900000000001,0,0,165545,18209.900000000001,null,null,"N","N","",1]
["CBD24700250S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.45,75366,33914.699999999997,55700,25065,149119,67103.5,280185,126083.2,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,33914,0,115104,0,67103,0,216121,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24700300S",null,null,null,"대구경보링 (보통암)","Ø300mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24700300S","노무","L001020701000028",null,"중급기술자","건설","인",0.04,0,0,272915,10916.6,0,0,272915,10916.6,null,null,"N","N","",1]
["CBD24700300S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.15,0,0,238259,35738.800000000003,0,0,238259,35738.800000000003,null,null,"N","N","",1]
["CBD24700300S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.15,0,0,223458,33518.699999999997,0,0,223458,33518.699999999997,null,null,"N","N","",1]
["CBD24700300S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.08,0,0,214222,17137.7,0,0,214222,17137.7,null,null,"N","N","",1]
["CBD24700300S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.15,0,0,165545,24831.7,0,0,165545,24831.7,null,null,"N","N","",1]
["CBD24700300S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.6,75366,45219.6,55700,33420,149119,89471.4,280185,168111,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,45219,0,155563,0,89471,0,290253,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24700350S",null,null,null,"대구경보링 (보통암)","Ø350mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24700350S","노무","L001020701000028",null,"중급기술자","건설","인",0.05,0,0,272915,13645.7,0,0,272915,13645.7,null,null,"N","N","",1]
["CBD24700350S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.21,0,0,238259,50034.3,0,0,238259,50034.3,null,null,"N","N","",1]
["CBD24700350S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.21,0,0,223458,46926.1,0,0,223458,46926.1,null,null,"N","N","",1]
["CBD24700350S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.11,0,0,214222,23564.400000000001,0,0,214222,23564.400000000001,null,null,"N","N","",1]
["CBD24700350S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.21,0,0,165545,34764.400000000001,0,0,165545,34764.400000000001,null,null,"N","N","",1]
["CBD24700350S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.84,75366,63307.4,55700,46788,149119,125259.9,280185,235355.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,63307,0,215722,0,125259,0,404288,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24800100S",null,null,null,"대구경보링 (경암)","Ø100mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24800100S","노무","L001020701000028",null,"중급기술자","건설","인",0.02,0,0,272915,5458.3,0,0,272915,5458.3,null,null,"N","N","",1]
["CBD24800100S","노무","L001020701000031",null,"중급숙련기술자","건설","인",7.0000000000000007E-2,0,0,238259,16678.099999999999,0,0,238259,16678.099999999999,null,null,"N","N","",1]
["CBD24800100S","노무","L001010101000014",null,"보링공","일반공사 직종","인",7.0000000000000007E-2,0,0,223458,15642,0,0,223458,15642,null,null,"N","N","",1]
["CBD24800100S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.03,0,0,214222,6426.6,0,0,214222,6426.6,null,null,"N","N","",1]
["CBD24800100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.0000000000000007E-2,0,0,165545,11588.1,0,0,165545,11588.1,null,null,"N","N","",1]
["CBD24800100S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.28999999999999998,75366,21856.1,55700,16153,149119,43244.5,280185,81253.600000000006,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,21856,0,71946,0,43244,0,137046,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24800150S",null,null,null,"대구경보링 (경암)","Ø150mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24800150S","노무","L001020701000028",null,"중급기술자","건설","인",0.03,0,0,272915,8187.4,0,0,272915,8187.4,null,null,"N","N","",1]
["CBD24800150S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.1,0,0,238259,23825.9,0,0,238259,23825.9,null,null,"N","N","",1]
["CBD24800150S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.1,0,0,223458,22345.8,0,0,223458,22345.8,null,null,"N","N","",1]
["CBD24800150S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.05,0,0,214222,10711.1,0,0,214222,10711.1,null,null,"N","N","",1]
["CBD24800150S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.1,0,0,165545,16554.5,0,0,165545,16554.5,null,null,"N","N","",1]
["CBD24800150S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.41,75366,30900,55700,22837,149119,61138.7,280185,114875.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,30900,0,104461,0,61138,0,196499,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24800200S",null,null,null,"대구경보링 (경암)","Ø200mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24800200S","노무","L001020701000028",null,"중급기술자","건설","인",0.04,0,0,272915,10916.6,0,0,272915,10916.6,null,null,"N","N","",1]
["CBD24800200S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.15,0,0,238259,35738.800000000003,0,0,238259,35738.800000000003,null,null,"N","N","",1]
["CBD24800200S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.15,0,0,223458,33518.699999999997,0,0,223458,33518.699999999997,null,null,"N","N","",1]
["CBD24800200S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",7.0000000000000007E-2,0,0,214222,14995.5,0,0,214222,14995.5,null,null,"N","N","",1]
["CBD24800200S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.15,0,0,165545,24831.7,0,0,165545,24831.7,null,null,"N","N","",1]
["CBD24800200S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.57999999999999996,75366,43712.2,55700,32306,149119,86489,280185,162507.20000000001,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,43712,0,152307,0,86489,0,282508,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24800250S",null,null,null,"대구경보링 (경암)","Ø250mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24800250S","노무","L001020701000028",null,"중급기술자","건설","인",0.05,0,0,272915,13645.7,0,0,272915,13645.7,null,null,"N","N","",1]
["CBD24800250S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.2,0,0,238259,47651.8,0,0,238259,47651.8,null,null,"N","N","",1]
["CBD24800250S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.2,0,0,223458,44691.6,0,0,223458,44691.6,null,null,"N","N","",1]
["CBD24800250S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.1,0,0,214222,21422.2,0,0,214222,21422.2,null,null,"N","N","",1]
["CBD24800250S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.2,0,0,165545,33109,0,0,165545,33109,null,null,"N","N","",1]
["CBD24800250S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.82,75366,61800.1,55700,45674,149119,122277.5,280185,229751.6,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,61800,0,206194,0,122277,0,390271,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24800300S",null,null,null,"대구경보링 (경암)","Ø300mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD24800300S","노무","L001020701000028",null,"중급기술자","건설","인",0.06,0,0,272915,16374.9,0,0,272915,16374.9,null,null,"N","N","",1]
["CBD24800300S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.24,0,0,238259,57182.1,0,0,238259,57182.1,null,null,"N","N","",1]
["CBD24800300S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.24,0,0,223458,53629.9,0,0,223458,53629.9,null,null,"N","N","",1]
["CBD24800300S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.12,0,0,214222,25706.6,0,0,214222,25706.6,null,null,"N","N","",1]
["CBD24800300S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.24,0,0,165545,39730.800000000003,0,0,165545,39730.800000000003,null,null,"N","N","",1]
["CBD24800300S","기계경비","00007101045000000",null,"고성능 착정기","335.7kw","HR",0.98,75366,73858.600000000006,55700,54586,149119,146136.6,280185,274581.2,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,73858,0,247210,0,146136,0,467204,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD30000000S",null,null,null,"폐공 되메우기","Ø15.24cm, 200m 까지","10M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD30000000S","노무","L001020701000028",null,"중급기술자","건설","인",6.7000000000000004E-2,0,0,272915,18285.3,0,0,272915,18285.3,null,null,"N","N","",1]
["CBD30000000S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.13300000000000001,0,0,238259,31688.400000000001,0,0,238259,31688.400000000001,null,null,"N","N","",1]
["CBD30000000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.26700000000000002,0,0,214222,57197.2,0,0,214222,57197.2,null,null,"N","N","",1]
["CBD30000000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.26700000000000002,0,0,165545,44200.5,0,0,165545,44200.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,151371,0,0,0,151371,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD40000000S",null,null,null,"대구경보링 - 케이싱 설치","Ø250mm","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD40000000S","노무","L001020701000028",null,"중급기술자","건설","인",0.03,0,0,272915,8187.4,0,0,272915,8187.4,null,null,"N","N","",1]
["CBD40000000S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.13,0,0,238259,30973.599999999999,0,0,238259,30973.599999999999,null,null,"N","N","",1]
["CBD40000000S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.13,0,0,223458,29049.5,0,0,223458,29049.5,null,null,"N","N","",1]
["CBD40000000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.13,0,0,214222,27848.799999999999,0,0,214222,27848.799999999999,null,null,"N","N","",1]
["CBD40000000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.2,0,0,165545,33109,0,0,165545,33109,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,129168,0,0,0,129168,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD50000000S",null,null,null,"대구경보링 - 에어써징",null,"M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD50000000S","노무","L001020701000028",null,"중급기술자","건설","인",4.0000000000000001E-3,0,0,272915,1091.5999999999999,0,0,272915,1091.5999999999999,null,null,"N","N","",1]
["CBD50000000S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.01,0,0,238259,2382.5,0,0,238259,2382.5,null,null,"N","N","",1]
["CBD50000000S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.01,0,0,223458,2234.5,0,0,223458,2234.5,null,null,"N","N","",1]
["CBD50000000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.01,0,0,214222,2142.1999999999998,0,0,214222,2142.1999999999998,null,null,"N","N","",1]
["CBD50000000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.02,0,0,165545,3310.9,0,0,165545,3310.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,11161,0,0,0,11161,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD60000000S",null,null,null,"대구경보링 - 우물 설치",null,"M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD60000000S","노무","L001020701000028",null,"중급기술자","건설","인",4.0000000000000001E-3,0,0,272915,1091.5999999999999,0,0,272915,1091.5999999999999,null,null,"N","N","",1]
["CBD60000000S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.01,0,0,238259,2382.5,0,0,238259,2382.5,null,null,"N","N","",1]
["CBD60000000S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.01,0,0,223458,2234.5,0,0,223458,2234.5,null,null,"N","N","",1]
["CBD60000000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.01,0,0,214222,2142.1999999999998,0,0,214222,2142.1999999999998,null,null,"N","N","",1]
["CBD60000000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.02,0,0,165545,3310.9,0,0,165545,3310.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,11161,0,0,0,11161,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD70000000S",null,null,null,"대구경보링 - 양수시험",null,"HR",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBD70000000S","노무","L001020701000028",null,"중급기술자","건설","인",0.06,0,0,272915,16374.9,0,0,272915,16374.9,null,null,"N","N","",1]
["CBD70000000S","노무","L001020701000031",null,"중급숙련기술자","건설","인",0.12,0,0,238259,28591,0,0,238259,28591,null,null,"N","N","",1]
["CBD70000000S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.12,0,0,223458,26814.9,0,0,223458,26814.9,null,null,"N","N","",1]
["CBD70000000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.12,0,0,214222,25706.6,0,0,214222,25706.6,null,null,"N","N","",1]
["CBD70000000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.37,0,0,165545,61251.6,0,0,165545,61251.6,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,158739,0,0,0,158739,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBE11000000S",null,null,null,"표준관입시험",null,"회당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBE11000000S","노무","L001020701000028",null,"중급기술자","건설","인",0.02,0,0,272915,5458.3,0,0,272915,5458.3,null,null,"N","N","",1]
["CBE11000000S","노무","L001010101000014",null,"보링공","일반공사 직종","인",7.0000000000000007E-2,0,0,223458,15642,0,0,223458,15642,null,null,"N","N","",1]
["CBE11000000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.06,0,0,214222,12853.3,0,0,214222,12853.3,null,null,"N","N","",1]
["CBE11000000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.0000000000000007E-2,0,0,165545,11588.1,0,0,165545,11588.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,45541,0,0,0,45541,null,null,null,null,"",1]
["CBE12000000S","노무","L001020701000030",null,"고급숙련기술자","건설","인",0.4,0,0,252328,100931.2,0,0,252328,100931.2,null,null,"N","N","",1]
["CBE14000000S",null,null,null,"2차원 전기비저항탐사",null,"1km당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CBE15000000S","노무","L001020701000028",null,"중급기술자","건설","인",14.6,0,0,272915,3984559,0,0,272915,3984559,null,null,"N","N","",1]
["CBE19000000S","노무","L001020701000031",null,"중급숙련기술자","건설","인",1,0,0,238259,238259,0,0,238259,238259,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,1053205,0,0,0,1053205,null,null,null,null,"",1]
["CCD22100000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",2,0,0,214222,428444,0,0,214222,428444,null,null,"N","N","",1]
["CCD22200000S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",1,0,0,233722,233722,0,0,233722,233722,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CCD40011000S",null,null,null,"고압분사 주입공법","장비조립 / 외부 반출 및 반입","회",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CCD40012000S",null,null,null,"고압분사 주입공법","장비조립 / 작업구간 이동","회",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CCD40012000S","기계경비","00002101002500000",null,"크레인(무한궤도)","25ton(0.76㎥)","HR",12,14653,175836,55700,668400,29557,354684,99910,1198920,null,null,"N","N","",1]
["CCD40021000S","기계경비","00002101002500000",null,"크레인(무한궤도)","25ton(0.76㎥)","HR",8,14653,117224,55700,445600,29557,236456,99910,799280,null,null,"N","N","",1]
["CCD40022000S","기계경비","00002101002500000",null,"크레인(무한궤도)","25ton(0.76㎥)","HR",4,14653,58612,55700,222800,29557,118228,99910,399640,null,null,"N","N","",1]
["CCD40023000S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",1,0,0,233722,233722,0,0,233722,233722,null,null,"N","N","",1]
["CCD40033000S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",1,0,0,233722,233722,0,0,233722,233722,null,null,"N","N","",1]
["CCD50112100S",null,null,null,"매트부설 / 육상","연약지반 : 도로/철도 ","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CCD50112100S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",8.9999999999999998E-4,0,0,214222,192.7,0,0,214222,192.7,null,null,"N","N","",1]
["CCD50112200S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.0000000000000001E-4,0,0,165545,82.7,0,0,165545,82.7,null,null,"N","N","",1]
["CCD50122000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",2.3999999999999998E-3,0,0,214222,514.1,0,0,214222,514.1,null,null,"N","N","",1]
["CCD50122000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.1999999999999999E-3,0,0,165545,198.6,0,0,165545,198.6,null,null,"N","N","",1]
["CCD50212000S",null,null,null,"다짐말뚝","장비조립 / 작업구간 이동","회",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CCD50220000S",null,null,null,"다짐말뚝 / 인력편성",null,"식",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CCD50220000S","노무","L001010101000014",null,"보링공","일반공사 직종","인",1,0,0,223458,223458,0,0,223458,223458,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,217031,0,2041578,0,354684,0,2613293,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,144687,0,1361052,0,236456,0,1742195,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CCD50232000S","기계경비","00005205021000000",null,"공기압축기(이동식)","21.0㎥/min","HR",8,40724,325792,55700,445600,7556,60448,103980,831840,null,null,"N","N","",1]
["CCF00010000S","기계경비","00002105000500000",null,"트럭탑재형 크레인","5ton","HR",8,7784,62272,47231,377848,9994,79952,65009,520072,null,null,"N","N","",1]
["CCF00020110S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",8.4000000000000005E-2,0,0,214222,17994.599999999999,0,0,214222,17994.599999999999,null,null,"N","N","",1]
["CCF00020210S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",7.8E-2,0,0,214222,16709.3,0,0,214222,16709.3,null,null,"N","N","",1]
["CCF00020210S","기계경비","00005205021000000",null,"공기압축기(이동식)","21.0㎥/min","HR",0.20699999999999999,40724,8429.7999999999993,55700,11529.9,7556,1564,103980,21523.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,5253,0,30877,0,2563,0,38693,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,7289,0,42851,0,3556,0,53696,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,9081,0,53728,0,4431,0,67240,null,null,null,null,"",1]
["CCF00020610S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.04,0,0,165545,6621.8,0,0,165545,6621.8,null,null,"N","N","",1]
["CCF00021100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5999999999999999E-2,0,0,165545,4304.1000000000004,0,0,165545,4304.1000000000004,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,9568,0,57224,0,6435,0,73227,null,null,null,null,"",1]
["CCF00021300S","노무","L001010101000014",null,"보링공","일반공사 직종","인",1.4999999999999999E-2,0,0,223458,3351.8,0,0,223458,3351.8,null,null,"N","N","",1]
["CCF00021400S","노무","L001010101000014",null,"보링공","일반공사 직종","인",2.1000000000000001E-2,0,0,223458,4692.6000000000004,0,0,223458,4692.6000000000004,null,null,"N","N","",1]
["CCF00021500S",null,null,null,"비탈면 보강공 / 스키드형 / 보통암","Ø105~127mm, 천공 및 보강재삽입","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CCF00021500S","기계경비","00005401001700000",null,"크롤러드릴(공기식)","17㎥/min(120mm)","HR",0.20799999999999999,0,0,55700,11585.6,12315,2561.5,68015,14147.1,null,null,"N","N","",1]
["CCF00021600S","기계경비","00005205021000000",null,"공기압축기(이동식)","21.0㎥/min","HR",0.29599999999999999,40724,12054.3,55700,16487.2,7556,2236.5,103980,30778,null,null,"N","N","",1]
["CCF00022100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.4E-2,0,0,165545,3973,0,0,165545,3973,null,null,"N","N","",1]
["CCF00022200S",null,null,null,"비탈면 보강공 / 크롤러형 / 혼합층","Ø105~127mm, 천공 및 보강재삽입","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CCF00022300S",null,null,null,"비탈면 보강공 / 크롤러형 / 풍화암","Ø105~127mm, 천공 및 보강재삽입","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CCF00022400S","기계경비","00005205021000000",null,"공기압축기(이동식)","21.0㎥/min","HR",0.156,40724,6352.9,55700,8689.2000000000007,7556,1178.7,103980,16220.8,null,null,"N","N","",1]
["CCF00022500S","기계경비","00005205021000000",null,"공기압축기(이동식)","21.0㎥/min","HR",0.19500000000000001,40724,7941.1,55700,10861.5,7556,1473.4,103980,20276,null,null,"N","N","",1]
["CCF00022600S","노무","L001010101000014",null,"보링공","일반공사 직종","인",3.5000000000000003E-2,0,0,223458,7821,0,0,223458,7821,null,null,"N","N","",1]
["CCF00030000S","노무","L001010101000014",null,"보링공","일반공사 직종","인",0.31,0,0,223458,69271.899999999994,0,0,223458,69271.899999999994,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CCF00030010S","손료","RENT000000000001",null,"공구손료","노무비의 11%","식",1,32383.7,32383.7,0,0,0,0,32383.7,32383.7,null,null,"N","N",11,1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,226320,0,0,0,226320,null,null,null,null,"",1]
["CCG10020000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.0000000000000001E-3,0,0,165545,1158.8,0,0,165545,1158.8,null,null,"N","N","",1]
["CCG11000000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.09,0,0,165545,14899,0,0,165545,14899,null,null,"N","N","",1]
["CCG12000000S","노무","L001010101000007",null,"형틀목공","일반공사 직종","인",0.04,0,0,274978,10999.1,0,0,274978,10999.1,null,null,"N","N","",1]
["CCG12010000S","노무","L001010101000007",null,"형틀목공","일반공사 직종","인",0.06,0,0,274978,16498.599999999999,0,0,274978,16498.599999999999,null,null,"N","N","",1]
["CDA10000000S","기계경비","00007206002000000",null,"부착용 집게","0.2㎥","HR",3.7599999999999999E-3,0,0,0,0,3484,13,3484,13,null,null,"N","N","",1]
["CDA21000000S","기계경비","00007206002000000",null,"부착용 집게","0.2㎥","HR",2.7100000000000002E-3,0,0,0,0,3484,9.4,3484,9.4,null,null,"N","N","",1]
["CDA22000000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.6E-4,0,0,165545,109.2,0,0,165545,109.2,null,null,"N","N","",1]
["CDA23000000S","기계경비","00000201002000000",null,"굴삭기(무한궤도)","0.2㎥","HR",4.6100000000000004E-3,7695,35.4,55700,256.7,13041,60.1,76436,352.2,null,null,"N","N","",1]
["CDB11020000S","기계경비","00000121000400000",null,"습지 불도저","4ton","HR",2.5000000000000001E-3,8448,21.1,55700,139.19999999999999,7590,18.899999999999999,71738,179.2,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,21,0,139,0,18,0,178,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,12,0,83,0,11,0,106,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,16684,0,293909,0,5129,0,315722,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CDC12100000S",null,null,null,"콘크리트구조물 헐기(소형장비)","공압식, 무근","M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CDC12200000S","손료","RENT000000000001",null,"잡재료","인력품의 1%","식",1,2185.4,2185.4,0,0,0,0,2185.4,2185.4,null,null,"N","N",1,1]
["CDC31000000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.6,0,0,165545,99327,0,0,165545,99327,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CDC33000000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.1000000000000001,0,0,165545,182099.5,0,0,165545,182099.5,null,null,"N","N","",1]
["CDC33000000S","손료","RENT000000000001",null,"잡재료","인력품의 5%","식",1,10251.6,10251.6,0,0,0,0,10251.6,10251.6,null,null,"N","N",5,1]
["CDC82000000S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.02,0,0,267021,5340.4,0,0,267021,5340.4,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CDD30010000S","손료","RENT000000000001",null,"소모자재(비트,로드,생그로드,슬리브)","크롤러드릴 기계경비의 24%","식",1,3139.8,3139.8,0,0,0,0,3139.8,3139.8,null,null,"N","N",24,1]
["CDD30020000S",null,null,null,"암발파 / 미진동굴착","TYPE-Ⅰ","M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CDD30020000S","기계경비","00000201010000001",null,"굴삭기(무한궤도)","1.0㎥(암석)","HR",0.04,30260,1210.4000000000001,55700,2228,32183,1287.3,118143,4725.7,null,null,"N","N","",1]
["CDD30030000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.2000000000000001E-2,0,0,165545,5297.4,0,0,165545,5297.4,null,null,"N","N","",1]
["CDD30040000S",null,null,null,"암발파 / 소규모진동 제어발파","TYPE-Ⅲ","M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CDD30050000S",null,null,null,"암발파 / 중규모진동 제어발파","TYPE-Ⅳ","M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CDD30050000S","기계경비","00000201010000001",null,"굴삭기(무한궤도)","1.0㎥(암석)","HR",8.9999999999999993E-3,30260,272.3,55700,501.3,32183,289.60000000000002,118143,1063.2,null,null,"N","N","",1]
["CDD30060000S","기계경비","00000201010000001",null,"굴삭기(무한궤도)","1.0㎥(암석)","HR",8.0000000000000002E-3,30260,242,55700,445.6,32183,257.39999999999998,118143,945,null,null,"N","N","",1]
["CDD30070000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.0000000000000001E-3,0,0,165545,496.6,0,0,165545,496.6,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,781,0,1896,0,408,0,3085,null,null,null,null,"",1]
["CDD30080010S","기계경비","00000201007000004",null,"굴삭기(유압식백호우)","0.7 ㎥, (브레이커조합)","HR",0.11,17116,1882.7,55700,6127,33897,3728.6,106713,11738.3,null,null,"N","N","",1]
["CDD30080020S","기계경비","00000201007000004",null,"굴삭기(유압식백호우)","0.7 ㎥, (브레이커조합)","HR",9.0999999999999998E-2,17116,1557.5,55700,5068.7,33897,3084.6,106713,9710.7999999999993,null,null,"N","N","",1]
["CDD30091200S",null,null,null,"수중발파 / 우물통발파","수심 2.5m 이상 ~ 8m 미만 (잠수조제외)","M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CDD30091310S",null,null,null,"수중발파 / 우물통발파","수심 8m 이상 ~ 15m 미만 (잠수조제외)","M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CDD30092100S","일위대가","CDD30092200S",null,"수중발파 / 우물통발파 이외","수심 2.5m 이상 ~ 8m 미만 (잠수조제외)","M3",0.8,2179,1743.2,55246,44196.800000000003,796,636.79999999999995,58221,46576.800000000003,null,null,"N","N","",1]
["CDD30092200S","기계경비","00005205010300000",null,"공기압축기(이동식)","10.3㎥/min","HR",0.104,20952,2179,55700,5792.8,5474,569.20000000000005,82126,8541,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,3268,0,82869,0,1194,0,87331,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CDE10040000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.56999999999999995,0,0,165545,94360.6,0,0,165545,94360.6,null,null,"N","N","",1]
["CDE20000000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.16,0,0,165545,26487.200000000001,0,0,165545,26487.200000000001,null,null,"N","N","",1]
["CDE30010000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.21,0,0,165545,34764.400000000001,0,0,165545,34764.400000000001,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CDE91100000S",null,null,null,"머신 가이던스(MG) 굴삭기","장비조립","회당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CDE91200000S","노무","L001010101000012",null,"용접공","일반공사 직종","인",1,0,0,267021,267021,0,0,267021,267021,null,null,"N","N","",1]
["CDE92010000S","기계경비","00000201010000030",null,"굴삭기(무한궤도)","1.0㎥ (3D GNSS 조합)","HR",9.1000000000000004E-3,33981,309.2,55700,506.8,27901,253.8,117582,1069.8,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,833735,0,0,0,833735,null,null,null,null,"",1]
["CDE93100000S","노무","L001020701000027",null,"고급기술자","건설","인",1,0,0,293799,293799,0,0,293799,293799,null,null,"N","N","",1]
["CDE93200000S","노무","L001010101000012",null,"용접공","일반공사 직종","인",1,0,0,267021,267021,0,0,267021,267021,null,null,"N","N","",1]
["CDF11010000S","기계경비","00000201006000000",null,"굴삭기(무한궤도)","0.6㎥","HR",1.4999999999999999E-2,15828,237.4,55700,835.5,21957,329.3,93485,1402.2,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CDF13050000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.7E-2,0,0,165545,4469.7,0,0,165545,4469.7,null,null,"N","N","",1]
["CDF13050000S","기계경비","00000201006000001",null,"굴삭기(무한궤도)","0.6㎥(암석)","HR",8.2000000000000003E-2,15828,1297.8,55700,4567.3999999999996,25327,2076.8000000000002,96855,7942,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,1693,0,11919,0,3654,0,17266,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,3249,0,38845,0,3033,0,45127,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CDF61200000S","기계경비","00000201002000000",null,"굴삭기(무한궤도)","0.2㎥","HR",0.18099999999999999,7695,1392.7,55700,10081.700000000001,13041,2360.4,76436,13834.8,null,null,"N","N","",1]
["CDF61200000S","기계경비","00007993002000000",null,"양수기","1.49kw","HR",0.158,0,0,0,0,12,1.8,12,1.8,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CDH11121000S",null,null,null,"인력 흙 다지기","점토, 성토두께 15cm","M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CDH11122100S",null,null,null,"인력 흙 다지기","점토, 성토두께 30cm","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CDH11200000S","기계경비","00001305000700000",null,"진동롤러(핸드가이드식)","0.7ton","HR",9.6000000000000002E-2,3162,303.5,33571,3222.8,1846,177.2,38579,3703.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,995,0,10573,0,1184,0,12752,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,142,0,501,0,197,0,840,null,null,null,null,"",1]
["CDI51010000S",null,null,null,"차수재공 / 부직포","수직고 30m 이하","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CDI51011000S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,11.8,11.8,0,0,0,0,11.8,11.8,null,null,"N","N",2,1]
["CDI53010000S","기계경비","00002101003000000",null,"크레인(무한궤도)","30ton(1.15㎥)","HR",2E-3,16027,32,55700,111.4,38329,76.599999999999994,110056,220,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,52,0,914,0,139,0,1105,null,null,null,null,"",1]
["CDI54010000S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,16,16,0,0,0,0,16,16,null,null,"N","N",2,1]
["CDI54011000S","기계경비","00002101005000000",null,"크레인(무한궤도)","50ton(1.91㎥)","HR",2E-3,18316,36.6,55700,111.4,69682,139.30000000000001,143698,287.3,null,null,"N","N","",1]
["CDI54020000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2E-3,0,0,165545,331,0,0,165545,331,null,null,"N","N","",1]
["CDI54021000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2E-3,0,0,165545,331,0,0,165545,331,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,1543,0,0,0,1543,null,null,null,null,"",1]
["CDI80000000S","기계경비","00001306010000000",null,"진동롤러(자주식)","10ton","HR",4.7000000000000002E-3,23811,111.9,55700,261.7,25460,119.6,104971,493.2,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CDJ31110015S","기계경비","00007505005000000",null,"발전기","50kw","HR",3.1E-2,13722,425.3,33571,1040.7,4447,137.80000000000001,51740,1603.8,null,null,"N","N","",1]
["CDJ31120005S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.0000000000000001E-3,0,0,165545,1158.8,0,0,165545,1158.8,null,null,"N","N","",1]
["CDJ31120005S","기계경비","00002105000500000",null,"트럭탑재형 크레인","5ton","HR",2.8000000000000001E-2,7784,217.9,47231,1322.4,9994,279.8,65009,1820.1,null,null,"N","N","",1]
["CDJ31120007S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.01,0,0,214222,2142.1999999999998,0,0,214222,2142.1999999999998,null,null,"N","N","",1]
["CDJ31120007S","기계경비","00007204005500000",null,"물탱크(살수차)","5500L","HR",3.5999999999999997E-2,15378,553.6,47231,1700.3,9470,340.9,72079,2594.8000000000002,null,null,"N","N","",1]
["CDJ31120010S","노무","L001010101000038",null,"조경공","일반공사 직종","인",7.0000000000000001E-3,0,0,219533,1536.7,0,0,219533,1536.7,null,null,"N","N","",1]
["CDJ31120010S","기계경비","00002105000500000",null,"트럭탑재형 크레인","5ton","HR",5.0999999999999997E-2,7784,396.9,47231,2408.6999999999998,9994,509.6,65009,3315.2,null,null,"N","N","",1]
["CDJ31120015S",null,null,null,"식생기반제 뿜어붙이기","H=20m 미만, t=15cm","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CDJ31120015S","기계경비","00007505005000000",null,"발전기","50kw","HR",7.4999999999999997E-2,13722,1029.0999999999999,33571,2517.8000000000002,4447,333.5,51740,3880.4,null,null,"N","N","",1]
["CDJ31210010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.0000000000000001E-3,0,0,165545,1158.8,0,0,165545,1158.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,528,0,9339,0,152,0,10019,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,667,0,11033,0,187,0,11887,null,null,null,null,"",1]
["CDJ31220005S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.0000000000000001E-3,0,0,165545,1158.8,0,0,165545,1158.8,null,null,"N","N","",1]
["CDJ31220005S","기계경비","00007505005000000",null,"발전기","50kw","HR",2.8000000000000001E-2,13722,384.2,33571,939.9,4447,124.5,51740,1448.6,null,null,"N","N","",1]
["CDJ31220007S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",5.0000000000000001E-3,0,0,233722,1168.5999999999999,0,0,233722,1168.5999999999999,null,null,"N","N","",1]
["CDJ31220007S","기계경비","00007750002500000",null,"취부기(녹생토 암절개면 보호식재용)","18.65kw","HR",3.5999999999999997E-2,0,0,0,0,29714,1069.7,29714,1069.7,null,null,"N","N","",1]
["CDJ31220010S",null,null,null,"식생기반제 뿜어붙이기","H=20m~30m 미만, t=10cm","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CDJ31220010S","기계경비","00005205021000000",null,"공기압축기(이동식)","21.0㎥/min","HR",5.0999999999999997E-2,40724,2076.9,55700,2840.7,7556,385.3,103980,5302.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,4837,0,21568,0,3521,0,29926,null,null,null,null,"",1]
["CDJ31220015S","기계경비","00005205021000000",null,"공기압축기(이동식)","21.0㎥/min","HR",7.4999999999999997E-2,40724,3054.3,55700,4177.5,7556,566.70000000000005,103980,7798.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,7105,0,31221,0,5178,0,43504,null,null,null,null,"",1]
["CDJ31310010S","손료","RENT000000000001",null,"노임할증","인력품의 30%","식",1,0,0,2082.8000000000002,2082.8000000000002,0,0,2082.8000000000002,2082.8000000000002,null,null,"N","N",30,1]
["CDJ31310015S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",8.9999999999999993E-3,0,0,165545,1489.9,0,0,165545,1489.9,null,null,"N","N","",1]
["CDJ31320005S","손료","RENT000000000001",null,"노임할증","인력품의 30%","식",1,0,0,1405.6,1405.6,0,0,1405.6,1405.6,null,null,"N","N",30,1]
["CDJ31320005S","손료","RENT000000000002",null,"공구손료","인력품의 2%","식",1,93.7,93.7,0,0,0,0,93.7,93.7,null,null,"N","N",2,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CDJ31320007S","기계경비","00007204005500000",null,"물탱크(살수차)","5500L","HR",3.5999999999999997E-2,15378,553.6,47231,1700.3,9470,340.9,72079,2594.8000000000002,null,null,"N","N","",1]
["CDJ31320010S",null,null,null,"식생기반제 뿜어붙이기","H=30m~50m 미만, t=10cm","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CDJ31320010S","기계경비","00005205021000000",null,"공기압축기(이동식)","21.0㎥/min","HR",5.0999999999999997E-2,40724,2076.9,55700,2840.7,7556,385.3,103980,5302.9,null,null,"N","N","",1]
["CDJ31320015S","노무","L001010101000038",null,"조경공","일반공사 직종","인",0.01,0,0,219533,2195.3000000000002,0,0,219533,2195.3000000000002,null,null,"N","N","",1]
["CDJ31320015S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",0.01,0,0,233722,2337.1999999999998,0,0,233722,2337.1999999999998,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,528,0,10727,0,152,0,11407,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CDJ31410015S","기계경비","00002105000500000",null,"트럭탑재형 크레인","5ton","HR",5.0000000000000001E-3,7784,38.9,47231,236.1,9994,49.9,65009,324.89999999999998,null,null,"N","N","",1]
["CDJ31420005S","기계경비","00007505005000000",null,"발전기","50kw","HR",2.8000000000000001E-2,13722,384.2,33571,939.9,4447,124.5,51740,1448.6,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CDJ31420007S","기계경비","00007750002500000",null,"취부기(녹생토 암절개면 보호식재용)","18.65kw","HR",3.5999999999999997E-2,0,0,0,0,29714,1069.7,29714,1069.7,null,null,"N","N","",1]
["CDJ31420010S",null,null,null,"식생기반제 뿜어붙이기","H=50m 이상, t=10cm","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CDJ31420010S","손료","RENT000000000001",null,"노임할증","인력품의 40%","식",1,0,0,3263.3,3263.3,0,0,3263.3,3263.3,null,null,"N","N",40,1]
[null,null,null,null,"[합 계]",null,null,0,0,4837,0,23200,0,3521,0,31558,null,null,null,null,"",1]
["CDJ31420015S","손료","RENT000000000002",null,"공구손료","인력품의 2%","식",1,231.6,231.6,0,0,0,0,231.6,231.6,null,null,"N","N",2,1]
["CDJ31420015S","기계경비","00007750002500000",null,"취부기(녹생토 암절개면 보호식재용)","18.65kw","HR",7.4999999999999997E-2,0,0,0,0,29714,2228.5,29714,2228.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,34597,0,0,0,34597,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,38346,0,0,0,38346,null,null,null,null,"",1]
["CDJ41210000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",7.4999999999999997E-2,0,0,214222,16066.6,0,0,214222,16066.6,null,null,"N","N","",1]
["CDJ41220000S","기계경비","00002104001500000",null,"크레인(타이어)","15ton","HR",0.09,8309,747.8,55700,5013,40854,3676.8,104863,9437.6,null,null,"N","N","",1]
["CDJ41230000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.10199999999999999,0,0,165545,16885.5,0,0,165545,16885.5,null,null,"N","N","",1]
["CDJ43000000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.18,0,0,165545,29798.1,0,0,165545,29798.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,24163,0,188171,0,55025,0,267359,null,null,null,null,"",1]
["CDJ43000010S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.22,0,0,214222,47128.800000000003,0,0,214222,47128.800000000003,null,null,"N","N","",1]
["CDJ65010000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3,0,0,165545,496635,0,0,165545,496635,null,null,"N","N","",1]
["CDJ65021100S","노무","L001010101000014",null,"보링공","일반공사 직종","인",2.4E-2,0,0,223458,5362.9,0,0,223458,5362.9,null,null,"N","N","",1]
["CDJ65021200S","노무","L001010101000014",null,"보링공","일반공사 직종","인",2.3E-2,0,0,223458,5139.5,0,0,223458,5139.5,null,null,"N","N","",1]
["CDJ65021300S","노무","L001010101000014",null,"보링공","일반공사 직종","인",1.4E-2,0,0,223458,3128.4,0,0,223458,3128.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,4601,0,24032,0,2245,0,30878,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,6352,0,33513,0,3099,0,42964,null,null,null,null,"",1]
["CDJ65021500S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.4E-2,0,0,165545,3973,0,0,165545,3973,null,null,"N","N","",1]
["CDJ65021600S","노무","L001010101000014",null,"보링공","일반공사 직종","인",3.5000000000000003E-2,0,0,223458,7821,0,0,223458,7821,null,null,"N","N","",1]
["CDJ65022100S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",4.2000000000000003E-2,0,0,214222,8997.2999999999993,0,0,214222,8997.2999999999993,null,null,"N","N","",1]
["CDJ65030000S",null,null,null,"어스앵커","그라우팅","M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CDJ65040000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.7000000000000004E-2,0,0,165545,11091.5,0,0,165545,11091.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,24240,0,0,0,24240,null,null,null,null,"",1]
["CEC05210000S","노무","L001010101000013",null,"콘크리트공","일반공사 직종","인",1.29,0,0,261283,337055,0,0,261283,337055,null,null,"N","N","",1]
["CEC05220000S","노무","L001010101000013",null,"콘크리트공","일반공사 직종","인",0.24,0,0,261283,62707.9,0,0,261283,62707.9,null,null,"N","N","",1]
["CEC10110000S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,1109.7,1109.7,0,0,0,0,1109.7,1109.7,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,2589,0,22264,0,2937,0,27790,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,357837,0,0,0,357837,null,null,null,null,"",1]
["CEC10311110S","노무","L001010101000013",null,"콘크리트공","일반공사 직종","인",1.37E-2,0,0,261283,3579.5,0,0,261283,3579.5,null,null,"N","N","",1]
["CEC10311120S","기계경비","00004504003200000",null,"콘크리트 펌프차","32m(80∼95㎥/hr)","HR",4.3999999999999997E-2,29707,1307.0999999999999,55700,2450.8000000000002,68071,2995.1,153478,6753,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,1685,0,10028,0,2995,0,14708,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,2103,0,12517,0,3737,0,18357,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CEC10311220S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",1.54E-2,0,0,214222,3299,0,0,214222,3299,null,null,"N","N","",1]
["CEC10311230S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",1.9199999999999998E-2,0,0,214222,4113,0,0,214222,4113,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,2455,0,14592,0,4363,0,21410,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CEC10311330S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.2E-2,0,0,165545,1986.5,0,0,165545,1986.5,null,null,"N","N","",1]
["CEC10311410S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.1399999999999999E-2,0,0,165545,3542.6,0,0,165545,3542.6,null,null,"N","N","",1]
["CEC10311410S","손료","RENT000000000001",null,"공구손료","인력품의 5%","식",1,1471.9,1471.9,0,0,0,0,1471.9,1471.9,null,null,"N","N",5,1]
[null,null,null,null,"[합 계]",null,null,0,0,7858,0,46744,0,13961,0,68563,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CEC10312110S","손료","RENT000000000001",null,"공구손료","인력품의 5%","식",1,303.10000000000002,303.10000000000002,0,0,0,0,303.10000000000002,303.10000000000002,null,null,"N","N",5,1]
["CEC10312120S","손료","RENT000000000001",null,"공구손료","인력품의 5%","식",1,365.1,365.1,0,0,0,0,365.1,365.1,null,null,"N","N",5,1]
["CEC10312130S","손료","RENT000000000001",null,"공구손료","인력품의 5%","식",1,454.6,454.6,0,0,0,0,454.6,454.6,null,null,"N","N",5,1]
["CEC10312210S","노무","L001010101000013",null,"콘크리트공","일반공사 직종","인",1.8499999999999999E-2,0,0,261283,4833.7,0,0,261283,4833.7,null,null,"N","N","",1]
["CEC10312220S","노무","L001010101000013",null,"콘크리트공","일반공사 직종","인",2.2200000000000001E-2,0,0,261283,5800.4,0,0,261283,5800.4,null,null,"N","N","",1]
["CEC10312230S","노무","L001010101000013",null,"콘크리트공","일반공사 직종","인",2.7799999999999998E-2,0,0,261283,7263.6,0,0,261283,7263.6,null,null,"N","N","",1]
["CEC10312230S","기계경비","00004504003200000",null,"콘크리트 펌프차","32m(80∼95㎥/hr)","HR",7.4099999999999999E-2,29707,2201.1999999999998,55700,4127.3,68071,5044,153478,11372.5,null,null,"N","N","",1]
["CEC10312310S","기계경비","00004504003200000",null,"콘크리트 펌프차","32m(80∼95㎥/hr)","HR",6.1699999999999998E-2,29707,1832.9,55700,3436.6,68071,4199.8999999999996,153478,9469.4,null,null,"N","N","",1]
["CEC10312320S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",1.8499999999999999E-2,0,0,214222,3963.1,0,0,214222,3963.1,null,null,"N","N","",1]
["CEC10312330S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",2.3099999999999999E-2,0,0,214222,4948.5,0,0,214222,4948.5,null,null,"N","N","",1]
["CEC10312410S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",4.1200000000000001E-2,0,0,214222,8825.9,0,0,214222,8825.9,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CEC10313110S","손료","RENT000000000001",null,"공구손료","인력품의 5%","식",1,282.39999999999998,282.39999999999998,0,0,0,0,282.39999999999998,282.39999999999998,null,null,"N","N",5,1]
["CEC10313120S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.8999999999999998E-3,0,0,165545,811.1,0,0,165545,811.1,null,null,"N","N","",1]
["CEC10313130S",null,null,null,"무근콘크리트 펌프차 타설","18cm이상, Type-Ⅰ(매트기초), Type-Ⅲ(연속타설어려움)","M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CEC10313210S",null,null,null,"무근콘크리트 펌프차 타설","18cm이상, Type-Ⅱ(벽,기둥,보,슬라브), Type-Ⅰ(병렬타설)","M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CEC10313220S",null,null,null,"무근콘크리트 펌프차 타설","18cm이상, Type-Ⅱ(벽,기둥,보,슬라브), Type-Ⅱ(순차타설)","M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CEC10313220S","기계경비","00004504003200000",null,"콘크리트 펌프차","32m(80∼95㎥/hr)","HR",5.5199999999999999E-2,29707,1639.8,55700,3074.6,68071,3757.5,153478,8471.9,null,null,"N","N","",1]
["CEC10313230S","기계경비","00004504003200000",null,"콘크리트 펌프차","32m(80∼95㎥/hr)","HR",6.9000000000000006E-2,29707,2049.6999999999998,55700,3843.3,68071,4696.8,153478,10589.8,null,null,"N","N","",1]
["CEC10313310S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",1.44E-2,0,0,214222,3084.7,0,0,214222,3084.7,null,null,"N","N","",1]
["CEC10313320S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",8.6E-3,0,0,165545,1423.6,0,0,165545,1423.6,null,null,"N","N","",1]
["CEC10313330S","노무","L001010101000013",null,"콘크리트공","일반공사 직종","인",3.2300000000000002E-2,0,0,261283,8439.4,0,0,261283,8439.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,3303,0,19655,0,5867,0,28825,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,5874,0,34945,0,10435,0,51254,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,7047,0,41933,0,12518,0,61498,null,null,null,null,"",1]
["CEC10313430S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.87E-2,0,0,165545,4751.1000000000004,0,0,165545,4751.1000000000004,null,null,"N","N","",1]
["CEC15110000S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,2228,2228,0,0,0,0,2228,2228,null,null,"N","N",2,1]
["CEC15120000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.2000000000000001E-2,0,0,165545,5297.4,0,0,165545,5297.4,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CEC20120000S","기계경비","00000201007000000",null,"굴삭기(무한궤도)","0.7㎥","HR",0.14499999999999999,18001,2610.1,55700,8076.5,23128,3353.5,96829,14040.1,null,null,"N","N","",1]
["CEC20210000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.99,0,0,165545,163889.5,0,0,165545,163889.5,null,null,"N","N","",1]
["CEC20311110S",null,null,null,"철근콘크리트 펌프차 타설","8~12cm, Type-Ⅰ(매트기초), Type-Ⅰ(병렬타설)","M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CEC20311120S","손료","RENT000000000001",null,"공구손료","인력품의 5%","식",1,468.4,468.4,0,0,0,0,468.4,468.4,null,null,"N","N",5,1]
["CEC20311120S","기계경비","00004504003200000",null,"콘크리트 펌프차","32m(80∼95㎥/hr)","HR",4.5699999999999998E-2,29707,1357.6,55700,2545.4,68071,3110.8,153478,7013.8,null,null,"N","N","",1]
["CEC20311130S","기계경비","00004504003200000",null,"콘크리트 펌프차","32m(80∼95㎥/hr)","HR",5.7099999999999998E-2,29707,1696.2,55700,3180.4,68071,3886.8,153478,8763.4,null,null,"N","N","",1]
["CEC20311210S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.7000000000000002E-3,0,0,165545,1109.0999999999999,0,0,165545,1109.0999999999999,null,null,"N","N","",1]
["CEC20311220S","노무","L001010101000013",null,"콘크리트공","일반공사 직종","인",3.2000000000000001E-2,0,0,261283,8361,0,0,261283,8361,null,null,"N","N","",1]
["CEC20311230S","노무","L001010101000013",null,"콘크리트공","일반공사 직종","인",0.04,0,0,261283,10451.299999999999,0,0,261283,10451.299999999999,null,null,"N","N","",1]
["CEC20311310S","기계경비","00004504003200000",null,"콘크리트 펌프차","32m(80∼95㎥/hr)","HR",6.6699999999999995E-2,29707,1981.4,55700,3715.1,68071,4540.3,153478,10236.799999999999,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,2664,0,17367,0,4540,0,24571,null,null,null,null,"",1]
["CEC20311330S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",2.5000000000000001E-2,0,0,214222,5355.5,0,0,214222,5355.5,null,null,"N","N","",1]
["CEC20311410S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",4.4400000000000002E-2,0,0,214222,9511.4,0,0,214222,9511.4,null,null,"N","N","",1]
["CEC20311410S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.2200000000000001E-2,0,0,165545,3675,0,0,165545,3675,null,null,"N","N","",1]
["CEC20311420S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",5.33E-2,0,0,214222,11418,0,0,214222,11418,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,10654,0,69485,0,18154,0,98293,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CEC20312120S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.4999999999999997E-3,0,0,165545,910.4,0,0,165545,910.4,null,null,"N","N","",1]
["CEC20312130S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.8999999999999999E-3,0,0,165545,1142.2,0,0,165545,1142.2,null,null,"N","N","",1]
["CEC20312210S",null,null,null,"철근콘크리트 펌프차 타설","15cm, Type-Ⅱ(벽,기둥,보,슬라브), Type-Ⅰ(병렬타설)","M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CEC20312220S",null,null,null,"철근콘크리트 펌프차 타설","15cm, Type-Ⅱ(벽,기둥,보,슬라브), Type-Ⅱ(순차타설)","M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CEC20312230S",null,null,null,"철근콘크리트 펌프차 타설","15cm, Type-Ⅱ(벽,기둥,보,슬라브), Type-Ⅲ(연속타설어려움))","M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CEC20312230S","노무","L001010101000013",null,"콘크리트공","일반공사 직종","인",3.85E-2,0,0,261283,10059.299999999999,0,0,261283,10059.299999999999,null,null,"N","N","",1]
["CEC20312310S","손료","RENT000000000001",null,"공구손료","인력품의 5%","식",1,656.9,656.9,0,0,0,0,656.9,656.9,null,null,"N","N",5,1]
["CEC20312320S","노무","L001010101000013",null,"콘크리트공","일반공사 직종","인",3.85E-2,0,0,261283,10059.299999999999,0,0,261283,10059.299999999999,null,null,"N","N","",1]
["CEC20312330S","노무","L001010101000013",null,"콘크리트공","일반공사 직종","인",4.8099999999999997E-2,0,0,261283,12567.7,0,0,261283,12567.7,null,null,"N","N","",1]
["CEC20312410S","노무","L001010101000013",null,"콘크리트공","일반공사 직종","인",8.5500000000000007E-2,0,0,261283,22339.599999999999,0,0,261283,22339.599999999999,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,6828,0,44548,0,11633,0,63009,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,8194,0,53459,0,13961,0,75614,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,10243,0,66823,0,17453,0,94519,null,null,null,null,"",1]
["CEC20313110S",null,null,null,"철근콘크리트 펌프차 타설","18cm이상, Type-Ⅰ(매트기초), Type-Ⅰ(병렬타설)","M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CEC20313120S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",1.0200000000000001E-2,0,0,214222,2185,0,0,214222,2185,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CEC20313220S","손료","RENT000000000001",null,"공구손료","인력품의 5%","식",1,585.5,585.5,0,0,0,0,585.5,585.5,null,null,"N","N",5,1]
["CEC20313230S","손료","RENT000000000001",null,"공구손료","인력품의 5%","식",1,731.7,731.7,0,0,0,0,731.7,731.7,null,null,"N","N",5,1]
["CEC20313310S","노무","L001010101000013",null,"콘크리트공","일반공사 직종","인",2.98E-2,0,0,261283,7786.2,0,0,261283,7786.2,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CEC20313330S",null,null,null,"철근콘크리트 펌프차 타설","18cm이상, Type-Ⅲ(옹벽,줄기초 등), Type-Ⅲ(연속타설어려움)","M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CEC20313330S","기계경비","00004504003200000",null,"콘크리트 펌프차","32m(80∼95㎥/hr)","HR",8.9300000000000004E-2,29707,2652.8,55700,4974,68071,6078.7,153478,13705.5,null,null,"N","N","",1]
["CEC20313410S","기계경비","00004504003200000",null,"콘크리트 펌프차","32m(80∼95㎥/hr)","HR",0.15870000000000001,29707,4714.5,55700,8839.5,68071,10802.8,153478,24356.799999999999,null,null,"N","N","",1]
["CEC20313420S","기계경비","00004504003200000",null,"콘크리트 펌프차","32m(80∼95㎥/hr)","HR",0.1905,29707,5659.1,55700,10610.8,68071,12967.5,153478,29237.4,null,null,"N","N","",1]
["CEC20313430S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",5.9499999999999997E-2,0,0,214222,12746.2,0,0,214222,12746.2,null,null,"N","N","",1]
["CEC25110000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.3,0,0,165545,49663.5,0,0,165545,49663.5,null,null,"N","N","",1]
["CEC25120000S","기계경비","00000201007000000",null,"굴삭기(무한궤도)","0.7㎥","HR",0.29099999999999998,18001,5238.2,55700,16208.7,23128,6730.2,96829,28177.1,null,null,"N","N","",1]
["CED11100000S","노무","L001010101000007",null,"형틀목공","일반공사 직종","인",0.25,0,0,274978,68744.5,0,0,274978,68744.5,null,null,"N","N","",1]
["CED11200000S","손료","RENT000000000001",null,"공구손료","노무비의 1%","식",1,682.3,682.3,0,0,0,0,682.3,682.3,null,null,"N","N",1,1]
["CED11300000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.7000000000000004E-2,0,0,165545,11091.5,0,0,165545,11091.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,378,0,37806,0,0,0,38184,null,null,null,null,"",1]
["CED21100000S",null,null,null,"강재거푸집 / 인력설치",null,"M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CED22300000S","노무","L001010101000007",null,"형틀목공","일반공사 직종","인",0.05,0,0,274978,13748.9,0,0,274978,13748.9,null,null,"N","N","",1]
["CED22400000S","손료","RENT000000000001",null,"공구손료","노무비의 4%","식",1,1366.5,1366.5,0,0,0,0,1366.5,1366.5,null,null,"N","N",4,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CED31300000S",null,null,null,"유로폼 설치 및 해체 / 인력투입","복잡, 수직고 7m까지","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CED31500000S",null,null,null,"유로폼 설치 및 해체 / 인력투입","간단, 수직고 7m까지","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CED31500000S","노무","L001010101000007",null,"형틀목공","일반공사 직종","인",0.1,0,0,274978,27497.8,0,0,274978,27497.8,null,null,"N","N","",1]
["CED51000740S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.17,0,0,165545,28142.6,0,0,165545,28142.6,null,null,"N","N","",1]
["CED51001200S",null,null,null,"합성수지(P.E)원형 맨홀 거푸집 / 기초 및 슬래브","Ø1200mm","조",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CED51001200S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.15,0,0,214222,32133.3,0,0,214222,32133.3,null,null,"N","N","",1]
["CED51001800S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.21,0,0,214222,44986.6,0,0,214222,44986.6,null,null,"N","N","",1]
["CED52000900S",null,null,null,"합성수지(P.E)원형 맨홀 거푸집 / 벽체","Ø900mm, H=1.0m","조",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CED52000900S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.26,0,0,214222,55697.7,0,0,214222,55697.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,211698,0,0,0,211698,null,null,null,null,"",1]
["CED61100000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.19900000000000001,0,0,280472,55813.9,0,0,280472,55813.9,null,null,"N","N","",1]
["CED61200000S",null,null,null,"슬립폼 공법","해체 ","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CED62000000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.2999999999999995E-2,0,0,165545,12084.7,0,0,165545,12084.7,null,null,"N","N","",1]
["CED71100000S",null,null,null,"알루미늄폼 설치 및 해체","셋팅층","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CED72000000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.4E-2,0,0,165545,2317.6,0,0,165545,2317.6,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,4764,0,49650,0,17375,0,71789,null,null,null,null,"",1]
["CED81200000S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,616.1,616.1,0,0,0,0,616.1,616.1,null,null,"N","N",2,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,18964,0,210711,0,0,0,229675,null,null,null,null,"",1]
["CEE10030000S",null,null,null,"철근 현장가공","Type-Ⅲ","TON",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CEE20010000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.59,0,0,165545,97671.5,0,0,165545,97671.5,null,null,"N","N","",1]
["CEE20020000S","노무","L001010101000008",null,"철근공","일반공사 직종","인",1.82,0,0,260137,473449.3,0,0,260137,473449.3,null,null,"N","N","",1]
["CEE20030000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.77,0,0,165545,127469.6,0,0,165545,127469.6,null,null,"N","N","",1]
["CEE20040000S","노무","L001010101000008",null,"철근공","일반공사 직종","인",1.82,0,0,260137,473449.3,0,0,260137,473449.3,null,null,"N","N","",1]
["CEE20050000S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,13569.7,13569.7,0,0,0,0,13569.7,13569.7,null,null,"N","N",2,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,21950,0,1097544,0,0,0,1119494,null,null,null,null,"",1]
["CEE20140000S",null,null,null,"철근 현장조립","토목 Type-Ⅱ-2 (개소별 소량 0.5ton 미만)","TON",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CEE20150000S",null,null,null,"철근 현장조립","토목 Type-Ⅲ (개소별 소량 0.5ton 미만)","TON",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CEE30010000S",null,null,null,"철근 공장가공","Type-Ⅰ","TON",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CEE30020000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.04,0,0,165545,6621.8,0,0,165545,6621.8,null,null,"N","N","",1]
["CEE30030000S","노무","L001010101000008",null,"철근공","일반공사 직종","인",0.38,0,0,260137,98852,0,0,260137,98852,null,null,"N","N","",1]
["CEE71000000S","노무","L001010101000008",null,"철근공","일반공사 직종","인",0.09,0,0,260137,23412.3,0,0,260137,23412.3,null,null,"N","N","",1]
["CEF10010900S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.28999999999999998,0,0,165545,48008,0,0,165545,48008,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CEF10011200S","기계경비","00002105000500000",null,"트럭탑재형 크레인","5ton","HR",2.29,7784,17825.3,47231,108158.9,9994,22886.2,65009,148870.39999999999,null,null,"N","N","",1]
["CEF10011500S","노무","L001010101000013",null,"콘크리트공","일반공사 직종","인",0.56999999999999995,0,0,261283,148931.29999999999,0,0,261283,148931.29999999999,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CEF10011800S","기계경비","00002105000500000",null,"트럭탑재형 크레인","5ton","HR",2.29,7784,17825.3,47231,108158.9,9994,22886.2,65009,148870.39999999999,null,null,"N","N","",1]
["CEF10020900S","노무","L001010101000013",null,"콘크리트공","일반공사 직종","인",0.28999999999999998,0,0,261283,75772,0,0,261283,75772,null,null,"N","N","",1]
["CEF10021200S",null,null,null,"교량신축이음 교체 / 2차로 차단","절단폭 1,200MM 이하, 일시공량 7m 적용","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,43125,0,410672,0,35995,0,489792,null,null,null,null,"",1]
["CEF10021500S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.43,0,0,214222,92115.4,0,0,214222,92115.4,null,null,"N","N","",1]
["CEF10021800S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.28999999999999998,0,0,267021,77436,0,0,267021,77436,null,null,"N","N","",1]
["CEF10021800S","기계경비","00002105000500000",null,"트럭탑재형 크레인","5ton","HR",1.1399999999999999,7784,8873.7000000000007,47231,53843.3,9994,11393.1,65009,74110.100000000006,null,null,"N","N","",1]
["CEF10030000S","손료","RENT000000000001",null,"공구손료","노무비의 1%","식",1,51.2,51.2,0,0,0,0,51.2,51.2,null,null,"N","N",1,1]
["CEF10030900S","손료","RENT000000000001",null,"공구손료","노무비의 6%","식",1,11585.9,11585.9,0,0,0,0,11585.9,11585.9,null,null,"N","N",6,1]
["CEF10031200S","기계경비","00002105000500000",null,"트럭탑재형 크레인","5ton","HR",0.76200000000000001,7784,5931.4,47231,35990,9994,7615.4,65009,49536.800000000003,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,29868,0,291883,0,24060,0,345811,null,null,null,null,"",1]
["CEF10031500S","기계경비","00000201004000004",null,"굴삭기(유압식백호우)","0.4 ㎥, (브레이커조합)","HR",1.524,14607,22261,55700,84886.8,21581,32889.4,91888,140037.20000000001,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,40999,0,334326,0,40504,0,415829,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CEF10111000S","기계경비","00002101001000000",null,"크레인(무한궤도)","10ton(0.29㎥)","HR",0.47099999999999997,8853,4169.7,55700,26234.7,13475,6346.7,78028,36751.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,15067,0,166331,0,15646,0,197044,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CEF10114000S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.2,0,0,267021,53404.2,0,0,267021,53404.2,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,4051,0,135058,0,0,0,139109,null,null,null,null,"",1]
["CEF40010000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.151,0,0,214222,32347.5,0,0,214222,32347.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,23009,0,0,0,23009,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CEG13010000S","노무","L001010101000008",null,"철근공","일반공사 직종","인",0.77,0,0,260137,200305.4,0,0,260137,200305.4,null,null,"N","N","",1]
["CEG13020000S",null,null,null,"PSC 빔 제작 / 포스트텐션 / 강연선설치","강연선규격 Ø15.2mm","TON",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CEG14310000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.12,0,0,214222,25706.6,0,0,214222,25706.6,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,44854,0,747571,0,8305,0,800730,null,null,null,null,"",1]
["CEG16000000S",null,null,null,"PSC 빔 제작대 설치",null,"M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CEG21110000S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,222.3,222.3,0,0,0,0,222.3,222.3,null,null,"N","N",2,1]
["CEG21120000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.02,0,0,165545,3310.9,0,0,165545,3310.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,463,0,23175,0,0,0,23638,null,null,null,null,"",1]
["CEG22020000S",null,null,null,"PSC BOX 제작 / 정착구 설치","쉬즈관규격 Ø100mm 이하","EA",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CEG23010000S","노무","L001010101000008",null,"철근공","일반공사 직종","인",1.61,0,0,260137,418820.5,0,0,260137,418820.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,22714,0,454295,0,0,0,477009,null,null,null,null,"",1]
["CEG24111000S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",0.26,0,0,233722,60767.7,0,0,233722,60767.7,null,null,"N","N","",1]
["CEG24112000S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",0.37,0,0,233722,86477.1,0,0,233722,86477.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,8968,0,179373,0,9013,0,197354,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,13905,0,278116,0,14053,0,306074,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,20751,0,415031,0,21128,0,456910,null,null,null,null,"",1]
["CEG24121000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.13,0,0,165545,21520.799999999999,0,0,165545,21520.799999999999,null,null,"N","N","",1]
["CEG24122000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.18,0,0,165545,29798.1,0,0,165545,29798.1,null,null,"N","N","",1]
["CEG24123000S","기계경비","00006516030000000",null,"강연선인장기","300ton","HR",1.68,0,0,0,0,9692,16282.5,9692,16282.5,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CEG24211000S","손료","RENT000000000001",null,"공구손료","노무비의 5%","식",1,11666,11666,0,0,0,0,11666,11666,null,null,"N","N",5,1]
["CEG24212000S","손료","RENT000000000001",null,"공구손료","노무비의 5%","식",1,16909.900000000001,16909.900000000001,0,0,0,0,16909.900000000001,16909.900000000001,null,null,"N","N",5,1]
["CEG24213000S","손료","RENT000000000001",null,"공구손료","노무비의 5%","식",1,25464.7,25464.7,0,0,0,0,25464.7,25464.7,null,null,"N","N",5,1]
["CEG24214000S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",1.51,0,0,233722,352920.2,0,0,233722,352920.2,null,null,"N","N","",1]
["CEG24221000S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",0.56000000000000005,0,0,233722,130884.3,0,0,233722,130884.3,null,null,"N","N","",1]
["CEG24222000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.67,0,0,214222,143528.70000000001,0,0,214222,143528.70000000001,null,null,"N","N","",1]
["CEG24222000S","기계경비","00006516030000000",null,"강연선인장기","300ton","HR",2.25,0,0,0,0,9692,21807,9692,21807,null,null,"N","N","",1]
["CEG24223000S","기계경비","00006516030000000",null,"강연선인장기","300ton","HR",3.41,0,0,0,0,9692,33049.699999999997,9692,33049.699999999997,null,null,"N","N","",1]
["CEG25000000S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",1.43,0,0,233722,334222.40000000002,0,0,233722,334222.40000000002,null,null,"N","N","",1]
["CEG25000000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",2.4,0,0,214222,514132.8,0,0,214222,514132.8,null,null,"N","N","",1]
["CER10000000S","노무","L001010101000027",null,"미장공","일반공사 직종","인",3.3999999999999998E-3,0,0,266787,907,0,0,266787,907,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CER42000000S",null,null,null,"콘크리트 치핑","소형치핑장비활용","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CER81300000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.2000000000000003E-2,0,0,165545,6952.8,0,0,165545,6952.8,null,null,"N","N","",1]
["CER81300000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,1011.9,1011.9,0,0,0,0,1011.9,1011.9,null,null,"N","N",3,1]
["CER82000000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,297.3,297.3,0,0,0,0,297.3,297.3,null,null,"N","N",3,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CER84000000S",null,null,null,"워터젯 치핑","파쇄깊이는 3cm이상에 적용","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CFE21000000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.125,0,0,165545,20693.099999999999,0,0,165545,20693.099999999999,null,null,"N","N","",1]
["CFE22000000S","손료","RENT000000000001",null,"공구손료","노무비의 17%","식",1,13092.2,13092.2,0,0,0,0,13092.2,13092.2,null,null,"N","N",17,1]
["CFE23000000S",null,null,null,"PC 기둥 설치","10ton미만 / 시공높이 30M이하","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CFE25000000S","노무","L001010101000007",null,"형틀목공","일반공사 직종","인",0.3,0,0,274978,82493.399999999994,0,0,274978,82493.399999999994,null,null,"N","N","",1]
["CFE26000000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.25,0,0,165545,41386.199999999997,0,0,165545,41386.199999999997,null,null,"N","N","",1]
["CFF51000000S",null,null,null,"PC 슬래브 설치","2ton미만 / 시공높이 30M이하","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CFF52000000S",null,null,null,"PC 슬래브 설치","5ton미만 / 시공높이 30M이하","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CFF52000000S","기계경비","00002104001000000",null,"크레인(타이어)","10ton","HR",0.32,6718,2149.6999999999998,55700,17824,30103,9632.9,92521,29606.6,null,null,"N","N","",1]
["CFF53000000S","기계경비","00002104001500000",null,"크레인(타이어)","15ton","HR",0.36399999999999999,8309,3024.4,55700,20274.8,40854,14870.8,104863,38170,null,null,"N","N","",1]
["CFF60000000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.33,0,0,165545,551264.80000000005,0,0,165545,551264.80000000005,null,null,"N","N","",1]
["CFF70100000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.17,0,0,165545,28142.6,0,0,165545,28142.6,null,null,"N","N","",1]
["CFF70200000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.25,0,0,165545,41386.199999999997,0,0,165545,41386.199999999997,null,null,"N","N","",1]
["CFH11010000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.1,0,0,165545,16554.5,0,0,165545,16554.5,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,6338,0,139987,0,18004,0,164329,null,null,null,null,"",1]
["CFH12010000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.125,0,0,165545,20693.099999999999,0,0,165545,20693.099999999999,null,null,"N","N","",1]
["CFH12020000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.33300000000000002,0,0,214222,71335.899999999994,0,0,214222,71335.899999999994,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CFH13010000S","기계경비","00002104002000000",null,"크레인(타이어)","20ton","HR",0.57099999999999995,9547,5451.3,55700,31804.7,51286,29284.3,116533,66540.3,null,null,"N","N","",1]
["CFH13020000S","손료","RENT000000000001",null,"공구손료","노무비의 2.5%","식",1,3766,3766,0,0,0,0,3766,3766,null,null,"N","N",2.5,1]
["CFH31000000S",null,null,null,"PC 벽체 설치","2ton미만 / 시공높이 30M이하","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CFH32000000S","노무","L001010101000007",null,"형틀목공","일반공사 직종","인",0.27300000000000002,0,0,274978,75068.899999999994,0,0,274978,75068.899999999994,null,null,"N","N","",1]
["CFH33000000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.2,0,0,165545,33109,0,0,165545,33109,null,null,"N","N","",1]
["CFH35000000S",null,null,null,"PC 벽체 설치","20ton미만 / 시공높이 30M이하","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CFH36000000S","노무","L001010101000007",null,"형틀목공","일반공사 직종","인",0.5,0,0,274978,137489,0,0,274978,137489,null,null,"N","N","",1]
["CFH41000000S","노무","L001010101000007",null,"형틀목공","일반공사 직종","인",0.14299999999999999,0,0,274978,39321.800000000003,0,0,274978,39321.800000000003,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,12359,0,86552,0,11469,0,110380,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,13655,0,95632,0,12673,0,121960,null,null,null,null,"",1]
["CFH43000000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.11799999999999999,0,0,165545,19534.3,0,0,165545,19534.3,null,null,"N","N","",1]
["CFH44000000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.13300000000000001,0,0,165545,22017.4,0,0,165545,22017.4,null,null,"N","N","",1]
["CFH45000000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.16700000000000001,0,0,165545,27646,0,0,165545,27646,null,null,"N","N","",1]
["CGA21100250S",null,null,null,"원심력 철근콘크리트관/소켓관 부설 및 접합","Ø250mm","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGA21100300S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.21,0,0,243168,51065.2,0,0,243168,51065.2,null,null,"N","N","",1]
["CGA21100350S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.11,0,0,165545,18209.900000000001,0,0,165545,18209.900000000001,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGA21200250S",null,null,null,"원심력 철근콘크리트관/수밀밴드 접합 및 부설","Ø250mm","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,5324,0,74157,0,5653,0,85134,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGA21200400S",null,null,null,"원심력 철근콘크리트관/수밀밴드 접합 및 부설","Ø400mm","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGA21300300S",null,null,null,"원심력 철근콘크리트관 절단","Ø300mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGA21300350S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.03,0,0,243168,7295,0,0,243168,7295,null,null,"N","N","",1]
["CGA21800025S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",4.7E-2,0,0,243168,11428.8,0,0,243168,11428.8,null,null,"N","N","",1]
["CGA21800025S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.3E-2,0,0,165545,3807.5,0,0,165545,3807.5,null,null,"N","N","",1]
["CGA21800035S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.9000000000000001E-2,0,0,165545,4800.8,0,0,165545,4800.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,4056,0,33288,0,5609,0,42953,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGA31100500S","기계경비","00002105001000000",null,"트럭탑재형 크레인","10ton","HR",0.46,15721,7231.6,47231,21726.2,21743,10001.700000000001,84695,38959.5,null,null,"N","N","",1]
["CGA31100600S","기계경비","00002105001000000",null,"트럭탑재형 크레인","10ton","HR",0.56000000000000005,15721,8803.7000000000007,47231,26449.3,21743,12176,84695,47429,null,null,"N","N","",1]
["CGA31200450S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.14000000000000001,0,0,165545,23176.3,0,0,165545,23176.3,null,null,"N","N","",1]
["CGA31200500S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,2377.8000000000002,2377.8000000000002,0,0,0,0,2377.8000000000002,2377.8000000000002,null,null,"N","N",2,1]
["CGA31200600S","기계경비","00002105001000000",null,"트럭탑재형 크레인","10ton","HR",0.56000000000000005,15721,8803.7000000000007,47231,26449.3,21743,12176,84695,47429,null,null,"N","N","",1]
["CGA31300450S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.04,0,0,165545,6621.8,0,0,165545,6621.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,1226,0,20435,0,0,0,21661,null,null,null,null,"",1]
["CGA31600150S",null,null,null,"원심력 철근콘크리트관/천공 및 접합","본관 Ø500mm이하, 연결관 Ø150mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGA31600250S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.09,0,0,243168,21885.1,0,0,243168,21885.1,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGA31700500S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.94,0,0,243168,228577.9,0,0,243168,228577.9,null,null,"N","N","",1]
["CGA31700600S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.47,0,0,165545,77806.100000000006,0,0,165545,77806.100000000006,null,null,"N","N","",1]
["CGA31800045S",null,null,null,"원심력철근콘크리트관 철거","Ø450mm","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGA31800050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.7999999999999999E-2,0,0,165545,6290.7,0,0,165545,6290.7,null,null,"N","N","",1]
["CGA31800060S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",9.0999999999999998E-2,0,0,243168,22128.2,0,0,243168,22128.2,null,null,"N","N","",1]
["CGA41100700S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,3794.3,3794.3,0,0,0,0,3794.3,3794.3,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,16361,0,256552,0,16524,0,289437,null,null,null,null,"",1]
["CGA41100900S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.81,0,0,243168,196966,0,0,243168,196966,null,null,"N","N","",1]
["CGA41200700S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.23,0,0,165545,38075.300000000003,0,0,165545,38075.300000000003,null,null,"N","N","",1]
["CGA41200800S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,4103.7,4103.7,0,0,0,0,4103.7,4103.7,null,null,"N","N",2,1]
["CGA41200900S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.75,0,0,243168,182376,0,0,243168,182376,null,null,"N","N","",1]
["CGA41300700S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.08,0,0,165545,13243.6,0,0,165545,13243.6,null,null,"N","N","",1]
["CGA41300800S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.1,0,0,243168,24316.799999999999,0,0,243168,24316.799999999999,null,null,"N","N","",1]
["CGA41300900S","손료","RENT000000000001",null,"공구손료","노무비의 6%","식",1,2697.4,2697.4,0,0,0,0,2697.4,2697.4,null,null,"N","N",6,1]
["CGA41600200S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.09,0,0,243168,21885.1,0,0,243168,21885.1,null,null,"N","N","",1]
["CGA41600200S","손료","RENT000000000001",null,"공구손료","노무비의 5%","식",1,1839.2,1839.2,0,0,0,0,1839.2,1839.2,null,null,"N","N",5,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,2656,0,53132,0,0,0,55788,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGA41700900S",null,null,null,"PC관 부설 및 접합","Ø900mm","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,22175,0,555449,0,23699,0,601323,null,null,null,null,"",1]
["CGA41800080S",null,null,null,"원심력철근콘크리트관 철거","Ø800mm","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGA51101000S",null,null,null,"원심력 철근콘크리트관/소켓관 부설 및 접합","Ø1000mm","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGA51101100S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",1.01,0,0,243168,245599.6,0,0,243168,245599.6,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGA51201000S",null,null,null,"원심력 철근콘크리트관/수밀밴드 접합 및 부설","Ø1000mm","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGA51201100S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.94,0,0,243168,228577.9,0,0,243168,228577.9,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGA51301000S",null,null,null,"원심력 철근콘크리트관 절단","Ø1,000mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGA51301200S",null,null,null,"원심력 철근콘크리트관 절단","Ø1,200mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGA51600150S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.08,0,0,243168,19453.400000000001,0,0,243168,19453.400000000001,null,null,"N","N","",1]
["CGA51600150S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.08,0,0,165545,13243.6,0,0,165545,13243.6,null,null,"N","N","",1]
["CGA51600250S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.12,0,0,165545,19865.400000000001,0,0,165545,19865.400000000001,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,3065,0,61306,0,0,0,64371,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGA51701100S","기계경비","00002104002000000",null,"크레인(타이어)","20ton","HR",1.34,9547,12792.9,55700,74638,51286,68723.199999999997,116533,156154.1,null,null,"N","N","",1]
["CGA51701200S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",2.33,0,0,243168,566581.4,0,0,243168,566581.4,null,null,"N","N","",1]
["CGA51800100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",9.0999999999999998E-2,0,0,165545,15064.5,0,0,165545,15064.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,14943,0,113742,0,25032,0,153717,null,null,null,null,"",1]
["CGA61101350S",null,null,null,"원심력 철근콘크리트관/소켓관 부설 및 접합","Ø1350mm","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,29811,0,452692,0,36845,0,519348,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGA61201500S",null,null,null,"원심력 철근콘크리트관/수밀밴드 접합 및 부설","Ø1500mm","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,32639,0,475246,0,41063,0,548948,null,null,null,null,"",1]
["CGA61301350S","손료","RENT000000000001",null,"공구손료","노무비의 6%","식",1,4414,4414,0,0,0,0,4414,4414,null,null,"N","N",6,1]
[null,null,null,null,"[합 계]",null,null,0,0,4904,0,81742,0,0,0,86646,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGA61800135S",null,null,null,"원심력철근콘크리트관 철거","Ø1,350mm","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGA71101650S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",1.56,0,0,243168,379342,0,0,243168,379342,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGA71201650S",null,null,null,"원심력 철근콘크리트관/수밀밴드 접합 및 부설","Ø1650mm","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,39402,0,575712,0,49501,0,664615,null,null,null,null,"",1]
["CGA71301800S",null,null,null,"원심력 철근콘크리트관 절단","Ø1,800mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGA81102000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.77,0,0,165545,127469.6,0,0,165545,127469.6,null,null,"N","N","",1]
["CGA81202000S",null,null,null,"원심력 철근콘크리트관/수밀밴드 접합 및 부설","Ø2000mm","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGA81302000S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.28000000000000003,0,0,243168,68087,0,0,243168,68087,null,null,"N","N","",1]
["CGB20000100S",null,null,null,"주철관 절단","Ø100mm 이하","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,1094,0,21885,0,0,0,22979,null,null,null,null,"",1]
["CGB20000200S",null,null,null,"주철관 절단","Ø200mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGB20100100S",null,null,null,"주철관 부설","Ø100mm 이하, L=6.0m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGB20100125S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.04,0,0,165545,6621.8,0,0,165545,6621.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,5659,0,47165,0,7827,0,60651,null,null,null,null,"",1]
["CGB20100200S","기계경비","00002105001000000",null,"트럭탑재형 크레인","10ton","HR",0.42,15721,6602.8,47231,19837,21743,9132,84695,35571.800000000003,null,null,"N","N","",1]
["CGB20110100S",null,null,null,"주철관 부설 / 인력","Ø100mm, L=6.0m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGB20110120S",null,null,null,"주철관 부설 / 인력","Ø120mm, L=6.0m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,91984,0,0,0,91984,null,null,null,null,"",1]
["CGB20200125S",null,null,null,"K.P. 메커니컬 조인트관 접합","Ø125mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,603,0,30162,0,0,0,30765,null,null,null,null,"",1]
["CGB20200200S",null,null,null,"K.P. 메커니컬 조인트관 접합","Ø200mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGB20300125S",null,null,null,"타이튼 조인트관 접합","Ø125mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGB20300125S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",7.0000000000000007E-2,0,0,243168,17021.7,0,0,243168,17021.7,null,null,"N","N","",1]
["CGB20300150S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,521.5,521.5,0,0,0,0,521.5,521.5,null,null,"N","N",2,1]
["CGB20400010S","기계경비","00002105001000000",null,"트럭탑재형 크레인","10ton","HR",0.19,15721,2986.9,47231,8973.7999999999993,21743,4131.1000000000004,84695,16091.8,null,null,"N","N","",1]
["CGB20400012S","기계경비","00002105001000000",null,"트럭탑재형 크레인","10ton","HR",0.222,15721,3490,47231,10485.200000000001,21743,4826.8999999999996,84695,18802.099999999999,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGB30000250S",null,null,null,"주철관 절단","Ø250mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGB30000350S","손료","RENT000000000001",null,"공구손료","노무비의 5%","식",1,2188.5,2188.5,0,0,0,0,2188.5,2188.5,null,null,"N","N",5,1]
["CGB30100250S",null,null,null,"주철관 부설","Ø250mm, L=6.0m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGB30100250S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.16,0,0,243168,38906.800000000003,0,0,243168,38906.800000000003,null,null,"N","N","",1]
["CGB30100350S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.22,0,0,243168,53496.9,0,0,243168,53496.9,null,null,"N","N","",1]
["CGB30100400S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.14000000000000001,0,0,165545,23176.3,0,0,165545,23176.3,null,null,"N","N","",1]
["CGB30100400S","기계경비","00002105001000000",null,"트럭탑재형 크레인","10ton","HR",0.66,15721,10375.799999999999,47231,31172.400000000001,21743,14350.3,84695,55898.5,null,null,"N","N","",1]
["CGB30200250S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,994.3,994.3,0,0,0,0,994.3,994.3,null,null,"N","N",2,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,1385,0,69275,0,0,0,70660,null,null,null,null,"",1]
["CGB30300250S",null,null,null,"타이튼 조인트관 접합","Ø250mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGB30300300S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.08,0,0,165545,13243.6,0,0,165545,13243.6,null,null,"N","N","",1]
["CGB30300350S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.16,0,0,243168,38906.800000000003,0,0,243168,38906.800000000003,null,null,"N","N","",1]
["CGB30300400S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,1255.0999999999999,1255.0999999999999,0,0,0,0,1255.0999999999999,1255.0999999999999,null,null,"N","N",2,1]
["CGB30400025S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",6.7000000000000004E-2,0,0,243168,16292.2,0,0,243168,16292.2,null,null,"N","N","",1]
["CGB30400030S","기계경비","00002105001000000",null,"트럭탑재형 크레인","10ton","HR",0.28599999999999998,15721,4496.2,47231,13508,21743,6218.4,84695,24222.6,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGB40000600S","손료","RENT000000000001",null,"공구손료","노무비의 5%","식",1,3404.3,3404.3,0,0,0,0,3404.3,3404.3,null,null,"N","N",5,1]
["CGB40100500S",null,null,null,"주철관 부설","Ø500mm, L=6.0m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGB40100700S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.24,0,0,165545,39730.800000000003,0,0,165545,39730.800000000003,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGB40200500S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.28000000000000003,0,0,243168,68087,0,0,243168,68087,null,null,"N","N","",1]
["CGB40200600S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,2249.5,2249.5,0,0,0,0,2249.5,2249.5,null,null,"N","N",2,1]
["CGB40200700S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.21,0,0,165545,34764.400000000001,0,0,165545,34764.400000000001,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,1385,0,69275,0,0,0,70660,null,null,null,null,"",1]
["CGB40300500S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,1515.8,1515.8,0,0,0,0,1515.8,1515.8,null,null,"N","N",2,1]
["CGB50000900S",null,null,null,"주철관 절단","Ø900mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGB50001100S",null,null,null,"주철관 절단","Ø1100mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGB50001100S","손료","RENT000000000001",null,"공구손료","노무비의 5%","식",1,5836,5836,0,0,0,0,5836,5836,null,null,"N","N",5,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGB50101000S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.64,0,0,243168,155627.5,0,0,243168,155627.5,null,null,"N","N","",1]
["CGB50101100S",null,null,null,"주철관 부설","Ø1100mm, L=6.0m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGB50200800S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.24,0,0,165545,39730.800000000003,0,0,165545,39730.800000000003,null,null,"N","N","",1]
["CGB50200900S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.49,0,0,243168,119152.3,0,0,243168,119152.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,3586,0,179318,0,0,0,182904,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,3977,0,198875,0,0,0,202852,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,6322,0,126447,0,0,0,132769,null,null,null,null,"",1]
["CGB60201200S",null,null,null,"K.P. 메커니컬 조인트관 접합","Ø1200mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC01400000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,105.3,105.3,0,0,0,0,105.3,105.3,null,null,"N","N",3,1]
["CGC22000100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.03,0,0,165545,4966.3,0,0,165545,4966.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,10533,0,74741,0,14567,0,99841,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,11319,0,81966,0,15654,0,108939,null,null,null,null,"",1]
["CGC22010080S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.13,0,0,243168,31611.8,0,0,243168,31611.8,null,null,"N","N","",1]
["CGC22010100S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.16,0,0,243168,38906.800000000003,0,0,243168,38906.800000000003,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,160792,0,0,0,160792,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC23120100S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.08,0,0,267021,21361.599999999999,0,0,267021,21361.599999999999,null,null,"N","N","",1]
["CGC23120125S","기계경비","00007611020000000",null,"용접기(교류)","200Amp","HR",0.09,0,0,0,0,87,7.8,87,7.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,1234,0,27053,0,408,0,28695,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,1646,0,33400,0,544,0,35590,null,null,null,null,"",1]
["CGC23130100S","기계경비","00007505005000000",null,"발전기","50kw","HR",0.09,13722,1234.9000000000001,33571,3021.3,4447,400.2,51740,4656.3999999999996,null,null,"N","N","",1]
["CGC23130125S",null,null,null,"강관접합 / A종 / 베벨엔드용접","Ø125mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC23130200S",null,null,null,"강관접합 / A종 / 베벨엔드용접","Ø200mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC25100080S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,427.2,427.2,0,0,0,0,427.2,427.2,null,null,"N","N",2,1]
["CGC25100100S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,427.2,427.2,0,0,0,0,427.2,427.2,null,null,"N","N",2,1]
["CGC25100150S",null,null,null,"강관 절단 / A종","Ø150mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,694,0,34712,0,0,0,35406,null,null,null,null,"",1]
["CGC31000250S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,260.7,260.7,0,0,0,0,260.7,260.7,null,null,"N","N",2,1]
["CGC31000300S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.06,0,0,243168,14590,0,0,243168,14590,null,null,"N","N","",1]
["CGC31000400S","기계경비","00002105000500000",null,"트럭탑재형 크레인","5ton","HR",0.16,7784,1245.4000000000001,47231,7556.9,9994,1599,65009,10401.299999999999,null,null,"N","N","",1]
["CGC32000250S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.05,0,0,165545,8277.2000000000007,0,0,165545,8277.2000000000007,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,12576,0,99558,0,17394,0,129528,null,null,null,null,"",1]
["CGC32000350S","기계경비","00002105001000000",null,"트럭탑재형 크레인","10ton","HR",0.84,15721,13205.6,47231,39674,21743,18264.099999999999,84695,71143.7,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC33120300S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.15,0,0,267021,40053.1,0,0,267021,40053.1,null,null,"N","N","",1]
["CGC33120350S",null,null,null,"강관접합 / A종 / 벨엔드용접","Ø350mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC33120400S",null,null,null,"강관접합 / A종 / 벨엔드용접","Ø400mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC33130250S",null,null,null,"강관접합 / A종 / 베벨엔드용접","Ø250mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC33130300S","기계경비","00007505005000000",null,"발전기","50kw","HR",0.19,13722,2607.1,33571,6378.4,4447,844.9,51740,9830.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,3156,0,61125,0,1042,0,65323,null,null,null,null,"",1]
["CGC33130400S","기계경비","00007611020000000",null,"용접기(교류)","200Amp","HR",0.27,0,0,0,0,87,23.4,87,23.4,null,null,"N","N","",1]
["CGC34400350S",null,null,null,"강관 외부도장","Ø350mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,67611,0,0,0,67611,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,854,0,42723,0,0,0,43577,null,null,null,null,"",1]
["CGC35100350S",null,null,null,"강관 절단 / A종","Ø350mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC35100400S",null,null,null,"강관 절단 / A종","Ø400mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC41000450S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,782.2,782.2,0,0,0,0,782.2,782.2,null,null,"N","N",2,1]
["CGC41000500S","기계경비","00002105000500000",null,"트럭탑재형 크레인","5ton","HR",0.18,7784,1401.1,47231,8501.5,9994,1798.9,65009,11701.5,null,null,"N","N","",1]
["CGC41000600S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.08,0,0,165545,13243.6,0,0,165545,13243.6,null,null,"N","N","",1]
["CGC41000700S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,1352.3,1352.3,0,0,0,0,1352.3,1352.3,null,null,"N","N",2,1]
["CGC42000450S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.3,0,0,243168,72950.399999999994,0,0,243168,72950.399999999994,null,null,"N","N","",1]
["CGC42000600S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.42,0,0,243168,102130.5,0,0,243168,102130.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,16978,0,171349,0,23482,0,211809,null,null,null,null,"",1]
["CGC42000700S","기계경비","00002105001000000",null,"트럭탑재형 크레인","10ton","HR",1.19,15721,18707.900000000001,47231,56204.800000000003,21743,25874.1,84695,100786.8,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC43120600S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.42,0,0,267021,112148.8,0,0,267021,112148.8,null,null,"N","N","",1]
["CGC43120700S",null,null,null,"강관접합 / A종 / 벨엔드용접","Ø700mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC43130450S","기계경비","00007505005000000",null,"발전기","50kw","HR",0.33,13722,4528.2,33571,11078.4,4447,1467.5,51740,17074.099999999999,null,null,"N","N","",1]
["CGC43130600S","기계경비","00007505005000000",null,"발전기","50kw","HR",0.57999999999999996,13722,7958.7,33571,19471.099999999999,4447,2579.1999999999998,51740,30009,null,null,"N","N","",1]
["CGC43130700S","기계경비","00007505005000000",null,"발전기","50kw","HR",0.84,13722,11526.4,33571,28199.599999999999,4447,3735.4,51740,43461.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,11526,0,199093,0,3808,0,214427,null,null,null,null,"",1]
["CGC44400600S",null,null,null,"강관 외부도장","Ø600mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC44400600S","노무","L001010101000029",null,"도장공","일반공사 직종","인",0.3,0,0,250776,75232.800000000003,0,0,250776,75232.800000000003,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC45100600S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.46,0,0,267021,122829.6,0,0,267021,122829.6,null,null,"N","N","",1]
["CGC45100600S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,2456.5,2456.5,0,0,0,0,2456.5,2456.5,null,null,"N","N",2,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC51001000S",null,null,null,"파형강관 부설 및 접합","Ø1000mm, L:6m","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC51011100S","일위대가","CGC51200110S",null,"강관압입추진공 / 작업편성인원","Ø800∼1100mm","일당",0.33,0,0,1183575,390579.7,0,0,1183575,390579.7,null,null,"N","N","",1]
["CGC51011110S",null,null,null,"강관압입추진공 - 보통토사","Ø1100mm, 추진연장 : 0∼30m","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC51011120S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,12782.6,12782.6,0,0,0,0,12782.6,12782.6,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,147964,0,695396,0,256147,0,1099507,null,null,null,null,"",1]
["CGC51011150S","일위대가","CGC61300150S",null,"강관압입추진공 / 작업편성장비","Ø1350∼1500mm","일당",0.42,353872,148626.20000000001,646416,271494.7,674072,283110.2,1674360,703231.1,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC51011200S",null,null,null,"강관압입추진공 - 보통토사","Ø2000mm, 추진연장 : 0∼30m","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC51011240S","일위대가","CGC81200300S",null,"강관압입추진공 / 작업편성인원","Ø2400∼3000mm","일당",0.59,0,0,1991786,1175153.7,0,0,1991786,1175153.7,null,null,"N","N","",1]
["CGC51011260S",null,null,null,"강관압입추진공 - 보통토사","Ø2600mm, 추진연장 : 0∼30m","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC51011280S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,42425,42425,0,0,0,0,42425,42425,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,293674,0,1873123,0,563507,0,2730304,null,null,null,null,"",1]
["CGC51012080S","일위대가","CGC51300100S",null,"강관압입추진공 / 작업편성장비","Ø800∼1000mm","일당",0.32,353872,113239,646416,206853.1,617416,197573.1,1617704,517665.2,null,null,"N","N","",1]
["CGC51012100S",null,null,null,"강관압입추진공 - 보통토사","Ø1000mm, 추진연장 : 30∼70m","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC51012100S","일위대가","CGC51300100S",null,"강관압입추진공 / 작업편성장비","Ø800∼1000mm","일당",0.36,353872,127393.9,646416,232709.7,617416,222269.7,1617704,582373.30000000005,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC51012135S","일위대가","CGC61200180S",null,"강관압입추진공 / 작업편성인원","Ø1200∼1800mm","일당",0.43,0,0,1183575,508937.2,0,0,1183575,508937.2,null,null,"N","N","",1]
["CGC51012150S",null,null,null,"강관압입추진공 - 보통토사","Ø1500mm, 추진연장 : 30∼70m","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC51012165S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,17753.599999999999,17753.599999999999,0,0,0,0,17753.599999999999,17753.599999999999,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,218052,0,1024794,0,405928,0,1648774,null,null,null,null,"",1]
["CGC51012200S","일위대가","CGC81300300S",null,"강관압입추진공 / 작업편성장비","Ø2000∼3000mm","일당",0.59,353872,208784.4,646416,381385.4,793672,468266.4,1793960,1058436.2,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,252486,0,1392147,0,500013,0,2144646,null,null,null,null,"",1]
["CGC51012240S","일위대가","CGC81300300S",null,"강관압입추진공 / 작업편성장비","Ø2000∼3000mm","일당",0.63,353872,222939.3,646416,407242,793672,500013.3,1793960,1130194.6000000001,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC51012300S","일위대가","CGC81200300S",null,"강관압입추진공 / 작업편성인원","Ø2400∼3000mm","일당",0.77,0,0,1991786,1533675.2,0,0,1991786,1533675.2,null,null,"N","N","",1]
["CGC51013080S",null,null,null,"강관압입추진공 - 보통토사","Ø800mm, 추진연장 : 70∼100m","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC51013090S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,13137.6,13137.6,0,0,0,0,13137.6,13137.6,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,147964,0,695396,0,234618,0,1077978,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,163539,0,768596,0,274340,0,1206475,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,167433,0,786896,0,280872,0,1235201,null,null,null,null,"",1]
["CGC51013135S","일위대가","CGC61300150S",null,"강관압입추진공 / 작업편성장비","Ø1350∼1500mm","일당",0.48,353872,169858.5,646416,310279.59999999998,674072,323554.5,1674360,803692.6,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC51013180S","일위대가","CGC61200180S",null,"강관압입추진공 / 작업편성인원","Ø1200∼1800mm","일당",0.59,0,0,1183575,698309.2,0,0,1183575,698309.2,null,null,"N","N","",1]
["CGC51013200S",null,null,null,"강관압입추진공 - 보통토사","Ø2000mm, 추진연장 : 70∼100m","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC51013220S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,33299.1,33299.1,0,0,0,0,33299.1,33299.1,null,null,"N","N",3,1]
["CGC51013260S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,46010.2,46010.2,0,0,0,0,46010.2,46010.2,null,null,"N","N",3,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,343309,0,2189707,0,658747,0,3191763,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,140176,0,658796,0,222269,0,1021241,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC51021100S","일위대가","CGC51200110S",null,"강관압입추진공 / 작업편성인원","Ø800∼1100mm","일당",0.38,0,0,1183575,449758.5,0,0,1183575,449758.5,null,null,"N","N","",1]
["CGC51021120S","일위대가","CGC61200180S",null,"강관압입추진공 / 작업편성인원","Ø1200∼1800mm","일당",0.43,0,0,1183575,508937.2,0,0,1183575,508937.2,null,null,"N","N","",1]
["CGC51021120S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,15268.1,15268.1,0,0,0,0,15268.1,15268.1,null,null,"N","N",3,1]
["CGC51021150S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,17753.599999999999,17753.599999999999,0,0,0,0,17753.599999999999,17753.599999999999,null,null,"N","N",3,1]
["CGC51021165S",null,null,null,"강관압입추진공 - 경질토사","Ø1650mm, 추진연장 : 0∼30m","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,206370,0,969895,0,384182,0,1560447,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,284548,0,1568928,0,563507,0,2416983,null,null,null,null,"",1]
["CGC51021240S",null,null,null,"강관압입추진공 - 경질토사","Ø2400mm, 추진연장 : 0∼30m","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC51021240S","일위대가","CGC81200300S",null,"강관압입추진공 / 작업편성인원","Ø2400∼3000mm","일당",0.71,0,0,1991786,1414168,0,0,1991786,1414168,null,null,"N","N","",1]
["CGC51021280S","일위대가","CGC81200300S",null,"강관압입추진공 / 작업편성인원","Ø2400∼3000mm","일당",0.83,0,0,1991786,1653182.3,0,0,1991786,1653182.3,null,null,"N","N","",1]
["CGC51021300S","일위대가","CGC81300300S",null,"강관압입추진공 / 작업편성장비","Ø2000∼3000mm","일당",0.83,353872,293713.7,646416,536525.19999999995,793672,658747.69999999995,1793960,1488986.6,null,null,"N","N","",1]
["CGC51022080S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,13492.7,13492.7,0,0,0,0,13492.7,13492.7,null,null,"N","N",3,1]
["CGC51022090S","일위대가","CGC51200110S",null,"강관압입추진공 / 작업편성인원","Ø800∼1100mm","일당",0.42,0,0,1183575,497101.5,0,0,1183575,497101.5,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,175220,0,823495,0,293936,0,1292651,null,null,null,null,"",1]
["CGC51022135S",null,null,null,"강관압입추진공 - 경질토사","Ø1350mm, 추진연장 : 30∼70m","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC51022165S","일위대가","CGC61200180S",null,"강관압입추진공 / 작업편성인원","Ø1200∼1800mm","일당",0.59,0,0,1183575,698309.2,0,0,1183575,698309.2,null,null,"N","N","",1]
["CGC51022180S","일위대가","CGC71300180S",null,"강관압입추진공 / 작업편성장비","Ø1650∼1800mm","일당",0.71,353872,251249.1,646416,458955.3,724872,514659.1,1725160,1224863.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,284548,0,1568928,0,563507,0,2416983,null,null,null,null,"",1]
["CGC51022220S","일위대가","CGC81300300S",null,"강관압입추진공 / 작업편성장비","Ø2000∼3000mm","일당",0.77,353872,272481.40000000002,646416,497740.3,793672,611127.4,1793960,1381349.1,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,343309,0,2189707,0,658747,0,3191763,null,null,null,null,"",1]
["CGC51022300S",null,null,null,"강관압입추진공 - 경질토사","Ø3000mm, 추진연장 : 30∼70m","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC51023090S","일위대가","CGC51200110S",null,"강관압입추진공 / 작업편성인원","Ø800∼1100mm","일당",0.45,0,0,1183575,532608.69999999995,0,0,1183575,532608.69999999995,null,null,"N","N","",1]
["CGC51023100S","일위대가","CGC51300100S",null,"강관압입추진공 / 작업편성장비","Ø800∼1000mm","일당",0.48,353872,169858.5,646416,310279.59999999998,617416,296359.59999999998,1617704,776497.7,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC51023120S","일위대가","CGC61300120S",null,"강관압입추진공 / 작업편성장비","Ø1100∼1200mm","일당",0.5,353872,176936,646416,323208,653192,326596,1653480,826740,null,null,"N","N","",1]
["CGC51023135S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,19884,19884,0,0,0,0,19884,19884,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,229733,0,1079694,0,397702,0,1707129,null,null,null,null,"",1]
["CGC51023180S",null,null,null,"강관압입추진공 - 경질토사","Ø1800mm, 추진연장 : 70∼100m","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC51023220S","일위대가","CGC71200220S",null,"강관압입추진공 / 작업편성인원","Ø2000∼2200mm","일당",0.83,0,0,1563342,1297573.8,0,0,1563342,1297573.8,null,null,"N","N","",1]
["CGC51023240S","일위대가","CGC81300300S",null,"강관압입추진공 / 작업편성장비","Ø2000∼3000mm","일당",0.83,353872,293713.7,646416,536525.19999999995,793672,658747.69999999995,1793960,1488986.6,null,null,"N","N","",1]
["CGC51023280S",null,null,null,"강관압입추진공 - 경질토사","Ø2800mm, 추진연장 : 70∼100m","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC51023280S","일위대가","CGC81300300S",null,"강관압입추진공 / 작업편성장비","Ø2000∼3000mm","일당",1,353872,353872,646416,646416,793672,793672,1793960,1793960,null,null,"N","N","",1]
["CGC51023300S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,59753.5,59753.5,0,0,0,0,59753.5,59753.5,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,147964,0,695396,0,234618,0,1077978,null,null,null,null,"",1]
["CGC51031100S",null,null,null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø1000mm, 추진연장 : 0∼30m","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC51031120S","일위대가","CGC61200180S",null,"강관압입추진공 / 작업편성인원","Ø1200∼1800mm","일당",0.48,0,0,1183575,568116,0,0,1183575,568116,null,null,"N","N","",1]
["CGC51031135S","일위대가","CGC61300150S",null,"강관압입추진공 / 작업편성장비","Ø1350∼1500mm","일당",0.5,353872,176936,646416,323208,674072,337036,1674360,837180,null,null,"N","N","",1]
["CGC51031165S","일위대가","CGC61200180S",null,"강관압입추진공 / 작업편성인원","Ø1200∼1800mm","일당",0.59,0,0,1183575,698309.2,0,0,1183575,698309.2,null,null,"N","N","",1]
["CGC51031165S","일위대가","CGC71300180S",null,"강관압입추진공 / 작업편성장비","Ø1650∼1800mm","일당",0.59,353872,208784.4,646416,381385.4,724872,427674.4,1725160,1017844.2,null,null,"N","N","",1]
["CGC51031200S","일위대가","CGC81300300S",null,"강관압입추진공 / 작업편성장비","Ø2000∼3000mm","일당",0.77,353872,272481.40000000002,646416,497740.3,793672,611127.4,1793960,1381349.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,308594,0,1701513,0,611127,0,2621234,null,null,null,null,"",1]
["CGC51031240S",null,null,null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø2400mm, 추진연장 : 0∼30m","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC51031280S",null,null,null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø2800mm, 추진연장 : 0∼30m","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC51031280S","일위대가","CGC81200300S",null,"강관압입추진공 / 작업편성인원","Ø2400∼3000mm","일당",0.91,0,0,1991786,1812525.2,0,0,1991786,1812525.2,null,null,"N","N","",1]
["CGC51032080S","일위대가","CGC51200110S",null,"강관압입추진공 / 작업편성인원","Ø800∼1100mm","일당",0.42,0,0,1183575,497101.5,0,0,1183575,497101.5,null,null,"N","N","",1]
["CGC51032090S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,15978.2,15978.2,0,0,0,0,15978.2,15978.2,null,null,"N","N",3,1]
["CGC51032090S","일위대가","CGC51300100S",null,"강관압입추진공 / 작업편성장비","Ø800∼1000mm","일당",0.45,353872,159242.4,646416,290887.2,617416,277837.2,1617704,727966.8,null,null,"N","N","",1]
["CGC51032110S","일위대가","CGC61300120S",null,"강관압입추진공 / 작업편성장비","Ø1100∼1200mm","일당",0.5,353872,176936,646416,323208,653192,326596,1653480,826740,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC51032135S",null,null,null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø1350mm, 추진연장 : 30∼70m","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC51032165S",null,null,null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø1650mm, 추진연장 : 30∼70m","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC51032180S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,27340.5,27340.5,0,0,0,0,27340.5,27340.5,null,null,"N","N",3,1]
["CGC51032200S","일위대가","CGC71200220S",null,"강관압입추진공 / 작업편성인원","Ø2000∼2200mm","일당",0.77,0,0,1563342,1203773.3,0,0,1563342,1203773.3,null,null,"N","N","",1]
["CGC51032220S","일위대가","CGC81300300S",null,"강관압입추진공 / 작업편성장비","Ø2000∼3000mm","일당",0.83,353872,293713.7,646416,536525.19999999995,793672,658747.69999999995,1793960,1488986.6,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,343309,0,2189707,0,658747,0,3191763,null,null,null,null,"",1]
["CGC51032260S","일위대가","CGC81300300S",null,"강관압입추진공 / 작업편성장비","Ø2000∼3000mm","일당",0.91,353872,322023.5,646416,588238.5,793672,722241.5,1793960,1632503.5,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,413625,0,2638202,0,793672,0,3845499,null,null,null,null,"",1]
["CGC51033090S",null,null,null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø900mm, 추진연장 : 70∼100m","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC51033100S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,17753.599999999999,17753.599999999999,0,0,0,0,17753.599999999999,17753.599999999999,null,null,"N","N",3,1]
["CGC51033110S",null,null,null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø1100mm, 추진연장 : 70∼100m","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC51033120S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,19884,19884,0,0,0,0,19884,19884,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,229733,0,1079694,0,397702,0,1707129,null,null,null,null,"",1]
["CGC51033150S","일위대가","CGC61300150S",null,"강관압입추진공 / 작업편성장비","Ø1350∼1500mm","일당",0.63,353872,222939.3,646416,407242,674072,424665.3,1674360,1054846.6000000001,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,299821,0,1409093,0,558151,0,2267065,null,null,null,null,"",1]
["CGC51033220S",null,null,null,"강관압입추진공 - 고사점토 및 자갈섞인토사","Ø2200mm, 추진연장 : 70∼100m","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC51033240S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,54375.7,54375.7,0,0,0,0,54375.7,54375.7,null,null,"N","N",3,1]
["CGC51033260S","일위대가","CGC81200300S",null,"강관압입추진공 / 작업편성인원","Ø2400∼3000mm","일당",1,0,0,1991786,1991786,0,0,1991786,1991786,null,null,"N","N","",1]
["CGC51033280S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,66326.399999999994,66326.399999999994,0,0,0,0,66326.399999999994,66326.399999999994,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,459124,0,2928404,0,880975,0,4268503,null,null,null,null,"",1]
["CGC51100090S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",1.5,0,0,233722,350583,0,0,233722,350583,null,null,"N","N","",1]
["CGC51200110S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",4,0,0,214222,856888,0,0,214222,856888,null,null,"N","N","",1]
["CGC51300100S","기계경비","00005204020000000",null,"유압잭","200ton","HR",16,0,0,0,0,21824,349184,21824,349184,null,null,"N","N","",1]
["CGC52000800S","기계경비","00002105001000000",null,"트럭탑재형 크레인","10ton","HR",1.31,15721,20594.5,47231,61872.6,21743,28483.3,84695,110950.39999999999,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,22778,0,357461,0,7526,0,387765,null,null,null,null,"",1]
["CGC53121100S",null,null,null,"강관접합 / A종 / 벨엔드용접","Ø1000mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC53121110S","기계경비","00007505005000000",null,"발전기","50kw","HR",3.05,13722,41852.1,33571,102391.5,4447,13563.3,51740,157806.9,null,null,"N","N","",1]
["CGC53220800S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.78,0,0,267021,208276.3,0,0,267021,208276.3,null,null,"N","N","",1]
["CGC53220900S","기계경비","00007611020000000",null,"용접기(교류)","200Amp","HR",1.48,0,0,0,0,87,128.69999999999999,87,128.69999999999999,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC54300800S",null,null,null,"강관 내부도장","Ø800mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC54300900S",null,null,null,"강관 내부도장","Ø900mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC54301100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.08,0,0,165545,13243.6,0,0,165545,13243.6,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,90984,0,0,0,90984,null,null,null,null,"",1]
["CGC54400900S","노무","L001010101000029",null,"도장공","일반공사 직종","인",0.36,0,0,250776,90279.3,0,0,250776,90279.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,116864,0,0,0,116864,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC55100900S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,4218.8999999999996,4218.8999999999996,0,0,0,0,4218.8999999999996,4218.8999999999996,null,null,"N","N",2,1]
["CGC55101100S",null,null,null,"강관 절단 / A종","Ø1100mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC55201000S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.85,0,0,267021,226967.8,0,0,267021,226967.8,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC61001200S",null,null,null,"파형강관 부설 및 접합","Ø1200mm, L:6m","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,6606,0,183279,0,4297,0,194182,null,null,null,null,"",1]
["CGC61100120S","기계경비","00002105001500000",null,"트럭탑재형 크레인","15ton","HR",12,16790,201480,47231,566772,28126,337512,92147,1105764,null,null,"N","N","",1]
["CGC61100165S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",2,0,0,233722,467444,0,0,233722,467444,null,null,"N","N","",1]
["CGC61200180S",null,null,null,"강관압입추진공 / 작업편성인원","Ø1200∼1800mm","일당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC61300120S","기계경비","00002105001500000",null,"트럭탑재형 크레인","15ton","HR",8,16790,134320,47231,377848,28126,225008,92147,737176,null,null,"N","N","",1]
["CGC61300150S","기계경비","00005204040000000",null,"유압잭","400ton","HR",16,0,0,0,0,25365,405840,25365,405840,null,null,"N","N","",1]
["CGC62001200S","기계경비","00002105001500000",null,"트럭탑재형 크레인","15ton","HR",1.95,16790,32740.5,47231,92100.4,28126,54845.7,92147,179686.6,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,39624,0,821246,0,66377,0,927247,null,null,null,null,"",1]
["CGC63121200S",null,null,null,"강관접합 / A종 / 벨엔드용접","Ø1200mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC63121350S","노무","L001010101000012",null,"용접공","일반공사 직종","인",2.62,0,0,267021,699595,0,0,267021,699595,null,null,"N","N","",1]
["CGC63121500S",null,null,null,"강관접합 / A종 / 벨엔드용접","Ø1500mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC63121650S","기계경비","00007505005000000",null,"발전기","50kw","HR",4.82,13722,66140,33571,161812.20000000001,4447,21434.5,51740,249386.7,null,null,"N","N","",1]
["CGC63221200S","노무","L001010101000012",null,"용접공","일반공사 직종","인",1.58,0,0,267021,421893.1,0,0,267021,421893.1,null,null,"N","N","",1]
["CGC63221350S","기계경비","00007611020000000",null,"용접기(교류)","200Amp","HR",2.68,0,0,0,0,87,233.1,87,233.1,null,null,"N","N","",1]
["CGC63221500S","기계경비","00007505005000000",null,"발전기","50kw","HR",3,13722,41166,33571,100713,4447,13341,51740,155220,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,45008,0,702899,0,14871,0,762778,null,null,null,null,"",1]
["CGC64301350S","노무","L001010101000029",null,"도장공","일반공사 직종","인",0.33,0,0,250776,82756,0,0,250776,82756,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,105178,0,0,0,105178,null,null,null,null,"",1]
["CGC64401350S","노무","L001010101000029",null,"도장공","일반공사 직종","인",0.43,0,0,250776,107833.60000000001,0,0,250776,107833.60000000001,null,null,"N","N","",1]
["CGC64401500S","노무","L001010101000029",null,"도장공","일반공사 직종","인",0.45,0,0,250776,112849.2,0,0,250776,112849.2,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC65101500S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,10039.9,10039.9,0,0,0,0,10039.9,10039.9,null,null,"N","N",2,1]
["CGC65201200S",null,null,null,"강관 절단 / B종","Ø1200mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC65201500S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,7903.8,7903.8,0,0,0,0,7903.8,7903.8,null,null,"N","N",2,1]
["CGC71100240S",null,null,null,"강관압입추진공 / 장비 조립 및 해체","Ø1800∼2400mm","회",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC71100240S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4,0,0,165545,662180,0,0,165545,662180,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,1563342,0,0,0,1563342,null,null,null,null,"",1]
["CGC71300180S","기계경비","00007505010000000",null,"발전기","100kw","HR",8,27444,219552,33571,268568,5403,43224,66418,531344,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC72002200S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",3.85,0,0,243168,936196.8,0,0,243168,936196.8,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC73121800S","노무","L001010101000012",null,"용접공","일반공사 직종","인",3.43,0,0,267021,915882,0,0,267021,915882,null,null,"N","N","",1]
["CGC73122200S","노무","L001010101000012",null,"용접공","일반공사 직종","인",4.01,0,0,267021,1070754.2,0,0,267021,1070754.2,null,null,"N","N","",1]
["CGC73122200S","기계경비","00007505005000000",null,"발전기","50kw","HR",6.07,13722,83292.5,33571,203775.9,4447,26993.200000000001,51740,314061.59999999998,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,88506,0,1351372,0,29244,0,1469122,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,52829,0,820832,0,17455,0,891116,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,60239,0,935088,0,19904,0,1015231,null,null,null,null,"",1]
["CGC74302000S","노무","L001010101000029",null,"도장공","일반공사 직종","인",0.39,0,0,250776,97802.6,0,0,250776,97802.6,null,null,"N","N","",1]
["CGC74302000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.09,0,0,165545,14899,0,0,165545,14899,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGC74402000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.12,0,0,165545,19865.400000000001,0,0,165545,19865.400000000001,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,142745,0,0,0,142745,null,null,null,null,"",1]
["CGC75101800S",null,null,null,"강관 절단 / A종","Ø1800mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,13618,0,680903,0,0,0,694521,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,14846,0,742318,0,0,0,757164,null,null,null,null,"",1]
["CGC75201800S",null,null,null,"강관 절단 / B종","Ø1800mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,12389,0,619488,0,0,0,631877,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,12817,0,640850,0,0,0,653667,null,null,null,null,"",1]
["CGC81100300S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",2.5,0,0,214222,535555,0,0,214222,535555,null,null,"N","N","",1]
["CGC81200300S",null,null,null,"강관압입추진공 / 작업편성인원","Ø2400∼3000mm","일당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGD11000050S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.06,0,0,243168,14590,0,0,243168,14590,null,null,"N","N","",1]
["CGD11000075S",null,null,null,"P.V.C.관 T.S 접합 및 부설","Ø75mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,30162,0,0,0,30162,null,null,null,null,"",1]
["CGD12000050S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.04,0,0,243168,9726.7000000000007,0,0,243168,9726.7000000000007,null,null,"N","N","",1]
["CGD12000075S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",7.0000000000000007E-2,0,0,243168,17021.7,0,0,243168,17021.7,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGD12000200S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.0000000000000007E-2,0,0,165545,11588.1,0,0,165545,11588.1,null,null,"N","N","",1]
["CGD12000250S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.1,0,0,165545,16554.5,0,0,165545,16554.5,null,null,"N","N","",1]
["CGE20100150S",null,null,null,"유리섬유복합관 부설 및 접합/비압력관","Ø150mm, L=6.0m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGE20200150S",null,null,null,"유리섬유복합관 부설 및 접합/압력관","Ø150mm, L=6.0m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGE20200200S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.13,0,0,165545,21520.799999999999,0,0,165545,21520.799999999999,null,null,"N","N","",1]
["CGE30100250S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.14000000000000001,0,0,243168,34043.5,0,0,243168,34043.5,null,null,"N","N","",1]
["CGE30100300S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.06,0,0,165545,9932.7000000000007,0,0,165545,9932.7000000000007,null,null,"N","N","",1]
["CGE30100350S",null,null,null,"유리섬유복합관 부설 및 접합/비압력관","Ø350mm, L=6.0m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGE30100400S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.22,0,0,243168,53496.9,0,0,243168,53496.9,null,null,"N","N","",1]
["CGE30200250S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.06,0,0,165545,9932.7000000000007,0,0,165545,9932.7000000000007,null,null,"N","N","",1]
["CGE30200300S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.18,0,0,243168,43770.2,0,0,243168,43770.2,null,null,"N","N","",1]
["CGE30200350S",null,null,null,"유리섬유복합관 부설 및 접합/압력관","Ø350mm, L=6.0m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGE30200400S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.24,0,0,243168,58360.3,0,0,243168,58360.3,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGE40100500S",null,null,null,"유리섬유복합관 부설 및 접합/비압력관","Ø500mm, L=6.0m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,4377,0,116029,0,4397,0,124803,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGE40200450S",null,null,null,"유리섬유복합관 부설 및 접합/압력관","Ø450mm, L=6.0m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGE40200500S",null,null,null,"유리섬유복합관 부설 및 접합/압력관","Ø500mm, L=6.0m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,4794,0,128524,0,4797,0,138115,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGE40200700S","기계경비","00002105000500000",null,"트럭탑재형 크레인","5ton","HR",0.64,7784,4981.7,47231,30227.8,9994,6396.1,65009,41605.599999999999,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,6850,0,209812,0,6496,0,223158,null,null,null,null,"",1]
["CGE50101000S","손료","RENT000000000001",null,"공구손료","노무비의 1%","식",1,2320.3000000000002,2320.3000000000002,0,0,0,0,2320.3000000000002,2320.3000000000002,null,null,"N","N",1,1]
["CGE50101000S","기계경비","00002105001000000",null,"트럭탑재형 크레인","10ton","HR",0.79,15721,12419.5,47231,37312.400000000001,21743,17176.900000000001,84695,66908.800000000003,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,16125,0,301165,0,18698,0,335988,null,null,null,null,"",1]
["CGE50200900S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.28999999999999998,0,0,165545,48008,0,0,165545,48008,null,null,"N","N","",1]
["CGE50200900S","손료","RENT000000000001",null,"공구손료","노무비의 1%","식",1,2255.1999999999998,2255.1999999999998,0,0,0,0,2255.1999999999998,2255.1999999999998,null,null,"N","N",1,1]
["CGE50201100S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.92,0,0,243168,223714.5,0,0,243168,223714.5,null,null,"N","N","",1]
["CGE60101200S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.37,0,0,165545,61251.6,0,0,165545,61251.6,null,null,"N","N","",1]
["CGE60101200S","손료","RENT000000000001",null,"공구손료","노무비의 1%","식",1,2873.9,2873.9,0,0,0,0,2873.9,2873.9,null,null,"N","N",1,1]
["CGE60101500S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",1.2,0,0,243168,291801.59999999998,0,0,243168,291801.59999999998,null,null,"N","N","",1]
["CGE60101650S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.53,0,0,165545,87738.8,0,0,165545,87738.8,null,null,"N","N","",1]
["CGE60101650S","기계경비","00002105001500000",null,"트럭탑재형 크레인","15ton","HR",1.25,16790,20987.5,47231,59038.7,28126,35157.5,92147,115183.7,null,null,"N","N","",1]
["CGE60201350S",null,null,null,"유리섬유복합관 부설 및 접합/압력관","Ø1350mm, L=6.0m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGE60201500S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",1.32,0,0,243168,320981.7,0,0,243168,320981.7,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGE70101800S",null,null,null,"유리섬유복합관 부설 및 접합/비압력관","Ø1800mm, L=6.0m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGE70102000S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",1.64,0,0,243168,398795.5,0,0,243168,398795.5,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGE70102400S",null,null,null,"유리섬유복합관 부설 및 접합/비압력관","Ø2400mm, L=6.0m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGE70201800S",null,null,null,"유리섬유복합관 부설 및 접합/압력관","Ø1800mm, L=6.0m","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,30008,0,569478,0,41907,0,641393,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGE70202200S","기계경비","00002105001800000",null,"트럭탑재형 크레인","18ton","HR",1.79,17248,30873.9,47231,84543.4,29487,52781.7,93966,168199,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,40415,0,770317,0,57499,0,868231,null,null,null,null,"",1]
["CGF11000020S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.06,0,0,243168,14590,0,0,243168,14590,null,null,"N","N","",1]
["CGF11000025S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.09,0,0,243168,21885.1,0,0,243168,21885.1,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGF11000050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.03,0,0,165545,4966.3,0,0,165545,4966.3,null,null,"N","N","",1]
["CGF12000050S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.08,0,0,243168,19453.400000000001,0,0,243168,19453.400000000001,null,null,"N","N","",1]
["CGF12000075S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,977.8,977.8,0,0,0,0,977.8,977.8,null,null,"N","N",3,1]
["CGF13000040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.03,0,0,165545,4966.3,0,0,165545,4966.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,1995,0,28506,0,0,0,30501,null,null,null,null,"",1]
["CGF13000075S",null,null,null,"P.E관 소켓융착 접합 및 부설","Ø75mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGF14000050S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.11,0,0,243168,26748.400000000001,0,0,243168,26748.400000000001,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,7690,0,51271,0,0,0,58961,null,null,null,null,"",1]
["CGF14000075S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.21,0,0,243168,51065.2,0,0,243168,51065.2,null,null,"N","N","",1]
["CGF15000075S","손료","RENT000000000001",null,"공구손료","노무비의 5%","식",1,1629.7,1629.7,0,0,0,0,1629.7,1629.7,null,null,"N","N",5,1]
["CGF22000100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.06,0,0,165545,9932.7000000000007,0,0,165545,9932.7000000000007,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,1491,0,49718,0,0,0,51209,null,null,null,null,"",1]
["CGF22000200S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,1882.6,1882.6,0,0,0,0,1882.6,1882.6,null,null,"N","N",3,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGF24000150S","손료","RENT000000000001",null,"공구손료","노무비의 15%","식",1,13790.4,13790.4,0,0,0,0,13790.4,13790.4,null,null,"N","N",15,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGF25000100S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.11,0,0,243168,26748.400000000001,0,0,243168,26748.400000000001,null,null,"N","N","",1]
["CGF25000150S","손료","RENT000000000001",null,"공구손료","노무비의 5%","식",1,2077.1999999999998,2077.1999999999998,0,0,0,0,2077.1999999999998,2077.1999999999998,null,null,"N","N",5,1]
["CGF25000200S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.0000000000000007E-2,0,0,165545,11588.1,0,0,165545,11588.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,2200,0,73362,0,0,0,75562,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,2933,0,97782,0,0,0,100715,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,19890,0,132601,0,0,0,152491,null,null,null,null,"",1]
["CGF34000350S",null,null,null,"P.E.관 바트융착 접합 및 부설","Ø350mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGF34000350S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.53,0,0,243168,128879,0,0,243168,128879,null,null,"N","N","",1]
["CGF34000400S","손료","RENT000000000001",null,"공구손료","노무비의 17%","식",1,27801.8,27801.8,0,0,0,0,27801.8,27801.8,null,null,"N","N",17,1]
["CGF35000300S","손료","RENT000000000001",null,"공구손료","노무비의 5%","식",1,3259.4,3259.4,0,0,0,0,3259.4,3259.4,null,null,"N","N",5,1]
[null,null,null,null,"[합 계]",null,null,0,0,3259,0,65188,0,0,0,68447,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,3960,0,132031,0,0,0,135991,null,null,null,null,"",1]
["CGF44000500S",null,null,null,"P.E.관 바트융착 접합 및 부설","Ø500mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGF44000600S",null,null,null,"P.E.관 바트융착 접합 및 부설","Ø600mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGF44000700S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.73,0,0,243168,177512.6,0,0,243168,177512.6,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGP00300008S",null,null,null,"부단수 천공 분기점 분기","Ø80mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGP00300010S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.36,0,0,243168,87540.4,0,0,243168,87540.4,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGP00300020S",null,null,null,"부단수 천공 분기점 분기","Ø200mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,23161,0,234289,0,15090,0,272540,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGP00300035S","기계경비","00002105000500000",null,"트럭탑재형 크레인","5ton","HR",1.69,7784,13154.9,47231,79820.3,9994,16889.8,65009,109865,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,51481,0,397446,0,17889,0,466816,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGP00300050S","기계경비","00002105000500000",null,"트럭탑재형 크레인","5ton","HR",2.02,7784,15723.6,47231,95406.6,9994,20187.8,65009,131318,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,81814,0,641756,0,22686,0,746256,null,null,null,null,"",1]
["CGP00411000S","손료","RENT000000000001",null,"공구손료","인력품의 4%","식",1,2607.5,2607.5,0,0,0,0,2607.5,2607.5,null,null,"N","N",4,1]
[null,null,null,null,"[합 계]",null,null,0,0,3129,0,78225,0,0,0,81354,null,null,null,null,"",1]
["CGP00421000S",null,null,null,"부단수 천공 새들분수전 분기점 분기","본관 Ø80mm, 지관 Ø13∼20mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGP00423000S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.34,0,0,243168,82677.100000000006,0,0,243168,82677.100000000006,null,null,"N","N","",1]
["CGP00431000S","손료","RENT000000000001",null,"공구손료","인력품의 4%","식",1,3292.5,3292.5,0,0,0,0,3292.5,3292.5,null,null,"N","N",4,1]
["CGP00432000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.15,0,0,165545,24831.7,0,0,165545,24831.7,null,null,"N","N","",1]
["CGP00433000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.18,0,0,165545,29798.1,0,0,165545,29798.1,null,null,"N","N","",1]
["CGP00441000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.14000000000000001,0,0,165545,23176.3,0,0,165545,23176.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,3977,0,99437,0,0,0,103414,null,null,null,null,"",1]
["CGP00451000S",null,null,null,"부단수 천공 새들분수전 분기점 분기","본관 Ø200mm, 지관 Ø13∼20mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGP00453000S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.4,0,0,243168,97267.199999999997,0,0,243168,97267.199999999997,null,null,"N","N","",1]
["CGP00461000S","손료","RENT000000000001",null,"공구손료","인력품의 4%","식",1,3782.9,3782.9,0,0,0,0,3782.9,3782.9,null,null,"N","N",4,1]
["CGP00462000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.18,0,0,165545,29798.1,0,0,165545,29798.1,null,null,"N","N","",1]
["CGP00463000S","손료","RENT000000000001",null,"공구손료","인력품의 4%","식",1,5475.7,5475.7,0,0,0,0,5475.7,5475.7,null,null,"N","N",4,1]
["CGP00471000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.17,0,0,165545,28142.6,0,0,165545,28142.6,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,4759,0,118993,0,0,0,123752,null,null,null,null,"",1]
["CGP00481000S",null,null,null,"부단수 천공 새들분수전 분기점 분기","본관 Ø400mm, 지관 Ø13∼20mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGP00483000S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.46,0,0,243168,111857.2,0,0,243168,111857.2,null,null,"N","N","",1]
["CGP00500008S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.05,0,0,243168,12158.4,0,0,243168,12158.4,null,null,"N","N","",1]
["CGP00500008S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.02,0,0,165545,3310.9,0,0,165545,3310.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,472,0,23643,0,0,0,24115,null,null,null,null,"",1]
["CGP00500015S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,603.20000000000005,603.20000000000005,0,0,0,0,603.20000000000005,603.20000000000005,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,603,0,30162,0,0,0,30765,null,null,null,null,"",1]
["CGP00500025S",null,null,null,"플랜지 조인트 접합","Ø250mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGP00500035S",null,null,null,"플랜지 조인트 접합","Ø350mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGP00500035S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.16,0,0,243168,38906.800000000003,0,0,243168,38906.800000000003,null,null,"N","N","",1]
["CGP00500045S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.2,0,0,243168,48633.599999999999,0,0,243168,48633.599999999999,null,null,"N","N","",1]
["CGP00500050S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,1434.1,1434.1,0,0,0,0,1434.1,1434.1,null,null,"N","N",2,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGP00500070S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,1776.6,1776.6,0,0,0,0,1776.6,1776.6,null,null,"N","N",2,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,2004,0,100213,0,0,0,102217,null,null,null,null,"",1]
["CGP00500120S",null,null,null,"플랜지 조인트 접합","Ø1200mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGP00500135S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.21,0,0,165545,34764.400000000001,0,0,165545,34764.400000000001,null,null,"N","N","",1]
["CGP00500150S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.46,0,0,243168,111857.2,0,0,243168,111857.2,null,null,"N","N","",1]
["CGP00500165S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,3389.7,3389.7,0,0,0,0,3389.7,3389.7,null,null,"N","N",2,1]
["CGP00500180S",null,null,null,"플랜지 조인트 접합","Ø1800mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGP00500200S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,4123.3999999999996,4123.3999999999996,0,0,0,0,4123.3999999999996,4123.3999999999996,null,null,"N","N",2,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,4823,0,241195,0,0,0,246018,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGP02100010S",null,null,null,"주철제 게이트 제수밸브 부설 및 접합","Ø100mm","기당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,4154,0,53847,0,4497,0,62498,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGP02100015S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,830.8,830.8,0,0,0,0,830.8,830.8,null,null,"N","N",2,1]
["CGP02100020S","기계경비","00002105000500000",null,"트럭탑재형 크레인","5ton","HR",0.64,7784,4981.7,47231,30227.8,9994,6396.1,65009,41605.599999999999,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,6600,0,100919,0,6695,0,114214,null,null,null,null,"",1]
["CGP02100030S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,1515.8,1515.8,0,0,0,0,1515.8,1515.8,null,null,"N","N",2,1]
["CGP02100035S","기계경비","00002105000500000",null,"트럭탑재형 크레인","5ton","HR",0.72,7784,5604.4,47231,34006.300000000003,9994,7195.6,65009,46806.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,9179,0,202480,0,7495,0,219154,null,null,null,null,"",1]
["CGP02100045S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,4123.3999999999996,4123.3999999999996,0,0,0,0,4123.3999999999996,4123.3999999999996,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,11080,0,277021,0,8095,0,296196,null,null,null,null,"",1]
["CGP02100060S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.91,0,0,243168,221282.8,0,0,243168,221282.8,null,null,"N","N","",1]
["CGP02100070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.53,0,0,165545,87738.8,0,0,165545,87738.8,null,null,"N","N","",1]
["CGP02100080S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,7822.5,7822.5,0,0,0,0,7822.5,7822.5,null,null,"N","N",2,1]
["CGP02100090S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",1.31,0,0,243168,318550,0,0,243168,318550,null,null,"N","N","",1]
["CGP02100100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.71,0,0,165545,117536.9,0,0,165545,117536.9,null,null,"N","N","",1]
["CGP02100110S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,9859.9,9859.9,0,0,0,0,9859.9,9859.9,null,null,"N","N",2,1]
["CGP02100120S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",1.6,0,0,243168,389068.79999999999,0,0,243168,389068.79999999999,null,null,"N","N","",1]
["CGP02100135S","기계경비","00002105001500000",null,"트럭탑재형 크레인","15ton","HR",1.51,16790,25352.9,47231,71318.8,28126,42470.2,92147,139141.9,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGP02200060S",null,null,null,"강관제 게이트 제수밸브 부설 및 접합","Ø600mm","기당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGP02200070S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",1.08,0,0,243168,262621.40000000002,0,0,243168,262621.40000000002,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGP02200090S",null,null,null,"강관제 게이트 제수밸브 부설 및 접합","Ø900mm","기당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGP02200100S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",1.44,0,0,243168,350161.9,0,0,243168,350161.9,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGP02200120S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,11337.5,11337.5,0,0,0,0,11337.5,11337.5,null,null,"N","N",2,1]
["CGP02200135S","기계경비","00002105001500000",null,"트럭탑재형 크레인","15ton","HR",2.12,16790,35594.800000000003,47231,100129.7,28126,59627.1,92147,195351.6,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,47831,0,711963,0,59627,0,819421,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGP02200165S","기계경비","00002105001800000",null,"트럭탑재형 크레인","18ton","HR",2.65,17248,45707.199999999997,47231,125162.1,29487,78140.5,93966,249009.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,60289,0,854279,0,78140,0,992708,null,null,null,null,"",1]
["CGP02200200S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,16069.2,16069.2,0,0,0,0,16069.2,16069.2,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,6694,0,103375,0,8594,0,118663,null,null,null,null,"",1]
["CGP05000025S","기계경비","00002105000500000",null,"트럭탑재형 크레인","5ton","HR",0.9,7784,7005.6,47231,42507.9,9994,8994.6,65009,58508.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,7239,0,119718,0,9294,0,136251,null,null,null,null,"",1]
["CGP05000040S",null,null,null,"주철제/강관제 버터플라이 제수밸브 부설 및 접합","Ø400mm","기당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGP05000040S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.52,0,0,243168,126447.3,0,0,243168,126447.3,null,null,"N","N","",1]
["CGP05000050S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.74,0,0,243168,179944.3,0,0,243168,179944.3,null,null,"N","N","",1]
["CGP05000060S","기계경비","00002105000500000",null,"트럭탑재형 크레인","5ton","HR",1.17,7784,9107.2000000000007,47231,55260.2,9994,11692.9,65009,76060.3,null,null,"N","N","",1]
["CGP05000080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.57999999999999996,0,0,165545,96016.1,0,0,165545,96016.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,24210,0,535468,0,33484,0,593162,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,27983,0,582708,0,38702,0,649393,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,28612,0,624692,0,39572,0,692876,null,null,null,null,"",1]
["CGP05000150S",null,null,null,"주철제/강관제 버터플라이 제수밸브 부설 및 접합","Ø1500mm","기당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGP05000180S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",2.0299999999999998,0,0,243168,493631,0,0,243168,493631,null,null,"N","N","",1]
["CGP05000200S","기계경비","00002105001800000",null,"트럭탑재형 크레인","18ton","HR",3.24,17248,55883.5,47231,153028.4,29487,95537.8,93966,304449.7,null,null,"N","N","",1]
["CGP05000220S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.61,0,0,165545,266527.40000000002,0,0,165545,266527.40000000002,null,null,"N","N","",1]
["CGP05000240S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",2.3199999999999998,0,0,243168,564149.69999999995,0,0,243168,564149.69999999995,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,25185,0,500984,0,42189,0,568358,null,null,null,null,"",1]
["CGP05100210S",null,null,null,"주철제 버터플라이 제수밸브 부설 및 접합","Ø2100mm","기당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGP05200090S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",1.34,0,0,243168,325845.09999999998,0,0,243168,325845.09999999998,null,null,"N","N","",1]
["CGP05200160S","기계경비","00002105001500000",null,"트럭탑재형 크레인","15ton","HR",2.44,16790,40967.599999999999,47231,115243.6,28126,68627.399999999994,92147,224838.6,null,null,"N","N","",1]
["CGP05200210S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.56,0,0,165545,258250.2,0,0,165545,258250.2,null,null,"N","N","",1]
["CGP08000008S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.09,0,0,165545,14899,0,0,165545,14899,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGP08000015S","기계경비","00002105000500000",null,"트럭탑재형 크레인","5ton","HR",0.12,7784,934,47231,5667.7,9994,1199.2,65009,7800.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,2327,0,68489,0,1399,0,72215,null,null,null,null,"",1]
["CGP08000025S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,1319.2,1319.2,0,0,0,0,1319.2,1319.2,null,null,"N","N",2,1]
["CGP08000030S","기계경비","00002105000500000",null,"트럭탑재형 크레인","5ton","HR",0.19,7784,1478.9,47231,8973.7999999999993,9994,1898.8,65009,12351.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,3403,0,91520,0,2298,0,97221,null,null,null,null,"",1]
["CGP08000040S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,1743.5,1743.5,0,0,0,0,1743.5,1743.5,null,null,"N","N",2,1]
["CGP08000045S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,1873.9,1873.9,0,0,0,0,1873.9,1873.9,null,null,"N","N",2,1]
["CGP08000050S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.31,0,0,243168,75382,0,0,243168,75382,null,null,"N","N","",1]
["CGP08000060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.17,0,0,165545,28142.6,0,0,165545,28142.6,null,null,"N","N","",1]
["CGP08000070S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,2671.6,2671.6,0,0,0,0,2671.6,2671.6,null,null,"N","N",2,1]
["CGP08000080S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.47,0,0,243168,114288.9,0,0,243168,114288.9,null,null,"N","N","",1]
["CGP08000090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.26,0,0,165545,43041.7,0,0,165545,43041.7,null,null,"N","N","",1]
["CGP12100005S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,574.20000000000005,574.20000000000005,0,0,0,0,574.20000000000005,574.20000000000005,null,null,"N","N",2,1]
["CGP12100008S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.15,0,0,165545,24831.7,0,0,165545,24831.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,1179,0,58978,0,0,0,60157,null,null,null,null,"",1]
["CGP12100015S","손료","RENT000000000001",null,"공구손료","인력품의 2%","식",1,1506.5,1506.5,0,0,0,0,1506.5,1506.5,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,1506,0,75326,0,0,0,76832,null,null,null,null,"",1]
["CGR10100750S",null,null,null,"내충격PVC수도관 부설 및 접합","Ø75mm","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGR20101500S",null,null,null,"내충격PVC수도관 부설 및 접합","Ø150mm","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CGR20101500S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.15,0,0,243168,36475.199999999997,0,0,243168,36475.199999999997,null,null,"N","N","",1]
["CGR20102000S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,1255.0999999999999,1255.0999999999999,0,0,0,0,1255.0999999999999,1255.0999999999999,null,null,"N","N",2,1]
["CGR30103000S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,1776.6,1776.6,0,0,0,0,1776.6,1776.6,null,null,"N","N",2,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CHC25020000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.7000000000000002E-3,0,0,165545,943.6,0,0,165545,943.6,null,null,"N","N","",1]
["CHC25030000S","기계경비","00003611014200000",null,"콘크리트 피니셔(중앙분리대용)","105.9kw","HR",3.6400000000000002E-2,15910,579.1,55700,2027.4,57886,2107,129496,4713.5,null,null,"N","N","",1]
["CHC25030000S","기계경비","00000201006000000",null,"굴삭기(무한궤도)","0.6㎥","HR",3.6400000000000002E-2,15828,576.1,55700,2027.4,21957,799.2,93485,3402.7,null,null,"N","N","",1]
["CHK12110020S","기계경비","00007204005500000",null,"물탱크(살수차)","5500L","HR",0.05,15378,768.9,47231,2361.5,9470,473.5,72079,3603.9,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CHK13110030S","노무","L001010101000050",null,"일반기계운전사","일반공사 직종","인",0.01,0,0,161142,1611.4,0,0,161142,1611.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,3673,0,23161,0,4830,0,31664,null,null,null,null,"",1]
["CHK14110050S","기계경비","00006540013100000",null,"워터젯트","96kw","HR",0.06,37524,2251.4,0,0,79559,4773.5,117083,7024.9,null,null,"N","N","",1]
["CHK14110050S","기계경비","00007740008000000",null,"수중모터 펌프","80ℓ/min","HR",0.05,0,0,0,0,307,15.3,307,15.3,null,null,"N","N","",1]
["CHK14110070S","손료","RENT000000000001",null,"잡재료","인력품의 3%","식",1,553.5,553.5,0,0,0,0,553.5,553.5,null,null,"N","N",3,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CHK15110090S","노무","L001010101000050",null,"일반기계운전사","일반공사 직종","인",0.01,0,0,161142,1611.4,0,0,161142,1611.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,4994,0,26905,0,6821,0,38720,null,null,null,null,"",1]
["CHL10100000S","기계경비","00007110002500000",null,"진공흡입 준설차","25ton(7.64㎥적)","HR",0.02,49150,983,55700,1114,69259,1385.1,174109,3482.1,null,null,"N","N","",1]
["CHL10200000S","기계경비","00007204005500000",null,"물탱크(살수차)","5500L","HR",2.58E-2,15378,396.7,47231,1218.5,9470,244.3,72079,1859.5,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CHL61000000S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.23,0,0,243168,55928.6,0,0,243168,55928.6,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CHL63000000S",null,null,null,"하수도 수로암거 준설 / 흡입식","800mm 이상","M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CHL73010030S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.5,0,0,243168,121584,0,0,243168,121584,null,null,"N","N","",1]
["CHL73020030S",null,null,null,"하수관 공기압시험","300MM 이하, 시험기구 별도","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CHL74010060S","기계경비","00000602002500000",null,"덤프트럭","2.5ton","HR",2.67,5090,13590.3,47231,126106.7,6169,16471.2,58490,156168.20000000001,null,null,"N","N","",1]
["CHL74020060S","기계경비","00000602002500000",null,"덤프트럭","2.5ton","HR",0.72699999999999998,5090,3700.4,47231,34336.9,6169,4484.8,58490,42522.1,null,null,"N","N","",1]
["CHL75010080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.5,0,0,165545,82772.5,0,0,165545,82772.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,0,0,140802,0,140802,null,null,null,null,"",1]
["CIA10000000S","노무","L001010101000009",null,"철공","일반공사 직종","인",0.97,0,0,233754,226741.3,0,0,233754,226741.3,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CIA40000000S","노무","L001010101000010",null,"철판공","일반공사 직종","인",1.87,0,0,211998,396436.2,0,0,211998,396436.2,null,null,"N","N","",1]
["CIA50000000S",null,null,null,"강교제작(공장제작) - 트러스","SS275, SM275, SM355, SM420, HSB380","TON",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,1200249,0,0,0,1200249,null,null,null,null,"",1]
["CIA70000000S","노무","L001010101000009",null,"철공","일반공사 직종","인",1.65,0,0,233754,385694.1,0,0,233754,385694.1,null,null,"N","N","",1]
["CIC11010000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.5,0,0,214222,107111,0,0,214222,107111,null,null,"N","N","",1]
["CIC11020000S","손료","RENT000000000001",null,"공구손료","노무비의 5%","식",1,18309.599999999999,18309.599999999999,0,0,0,0,18309.599999999999,18309.599999999999,null,null,"N","N",5,1]
["CIC11030000S","노무","L001010101000009",null,"철공","일반공사 직종","인",1,0,0,233754,233754,0,0,233754,233754,null,null,"N","N","",1]
["CIC12000000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.5,0,0,280472,140236,0,0,280472,140236,null,null,"N","N","",1]
["CIC12200000S",null,null,null,"강재거더 가설 / 해상","개구제형","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CIC12200000S","손료","RENT000000000001",null,"공구손료","노무비의 6%","식",1,58730.1,58730.1,0,0,0,0,58730.1,58730.1,null,null,"N","N",6,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CIC21030000S",null,null,null,"강재거더 지조립 / 양호","폐합형 ","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CIC21030000S","노무","L001010101000009",null,"철공","일반공사 직종","인",1.2,0,0,233754,280504.8,0,0,233754,280504.8,null,null,"N","N","",1]
["CIC22100000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",0.67,0,0,280472,187916.2,0,0,280472,187916.2,null,null,"N","N","",1]
["CIC22200000S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.67,0,0,267021,178904,0,0,267021,178904,null,null,"N","N","",1]
["CIC22200000S","손료","RENT000000000001",null,"공구손료","노무비의 4%","식",1,52174.1,52174.1,0,0,0,0,52174.1,52174.1,null,null,"N","N",4,1]
["CIC30100000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.2,0,0,214222,42844.4,0,0,214222,42844.4,null,null,"N","N","",1]
["CIC30200000S","기계경비","00002104020000000",null,"크레인(타이어)","200ton","HR",1.6,45613,72980.800000000003,55700,89120,299323,478916.8,400636,641017.59999999998,null,null,"N","N","",1]
["CIE81100000S","노무","L001010101000012",null,"용접공","일반공사 직종","인",1.04,0,0,267021,277701.8,0,0,267021,277701.8,null,null,"N","N","",1]
["CIE81200000S",null,null,null,"잡철물 제작 및 설치 / 제품 설치","경량철재","TON",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CIE82100000S",null,null,null,"잡철물 제작 및 설치 / 규격철물 설치","일반철재","TON",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CIE82200000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",2.5,0,0,214222,535555,0,0,214222,535555,null,null,"N","N","",1]
["CIE83100000S","노무","L001010101000012",null,"용접공","일반공사 직종","인",3.38,0,0,267021,902530.9,0,0,267021,902530.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,410630,0,5132880,0,0,0,5543510,null,null,null,null,"",1]
["CIE83200000S","노무","L001010101000012",null,"용접공","일반공사 직종","인",4.3899999999999997,0,0,267021,1172222.1000000001,0,0,267021,1172222.1000000001,null,null,"N","N","",1]
["CIG10020000S",null,null,null,"강교도장","제품표면처리","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CIG23000000S","노무","L001010101000029",null,"도장공","일반공사 직종","인",0.01,0,0,250776,2507.6999999999998,0,0,250776,2507.6999999999998,null,null,"N","N","",1]
["CIH15100000S","기계경비","00002105000500000",null,"트럭탑재형 크레인","5ton","HR",0.3,7784,2335.1999999999998,47231,14169.3,9994,2998.2,65009,19502.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,2752,0,53542,0,1798,0,58092,null,null,null,null,"",1]
["CIH15300000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,875.7,875.7,0,0,0,0,875.7,875.7,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,395,0,7904,0,0,0,8299,null,null,null,null,"",1]
["CJA00003000S","노무","L001010101000012",null,"용접공","일반공사 직종","인",1,0,0,267021,267021,0,0,267021,267021,null,null,"N","N","",1]
["CJA00101000S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",3,0,0,233722,701166,0,0,233722,701166,null,null,"N","N","",1]
["CJA00102000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",1.5,0,0,214222,321333,0,0,214222,321333,null,null,"N","N","",1]
["CJA00201000S",null,null,null,"현장타설말뚝 ","장비해체 / 외부 반출 및 반입","회",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CJA00202000S",null,null,null,"현장타설말뚝 ","장비해체 / 작업구간 이동","회",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CJA03010000S",null,null,null,"말뚝박기천공 / 인력편성",null,"인/일",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,629624,0,0,0,629624,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CJA03200000S","기계경비","00002101002500000",null,"크레인(무한궤도)","25ton(0.76㎥)","HR",4,14653,58612,55700,222800,29557,118228,99910,399640,null,null,"N","N","",1]
["CJB22100400S","손료","RENT000000000001",null,"공구손료","인력품의 4%","식",1,657.4,657.4,0,0,0,0,657.4,657.4,null,null,"N","N",4,1]
["CJB22200400S","기계경비","00000201002000000",null,"굴삭기(무한궤도)","0.2㎥","HR",6.3E-2,7695,484.7,55700,3509.1,13041,821.5,76436,4815.3,null,null,"N","N","",1]
["CJB23100500S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.7E-2,0,0,165545,7780.6,0,0,165545,7780.6,null,null,"N","N","",1]
["CJB23200500S","손료","RENT000000000001",null,"공구손료","인력품의 3%","식",1,639.6,639.6,0,0,0,0,639.6,639.6,null,null,"N","N",3,1]
["CJB24100600S",null,null,null,"말뚝두부정리(강관)","D600","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CJB24200600S","노무","L001010101000017",null,"할석공","일반공사 직종","인",6.3E-2,0,0,229326,14447.5,0,0,229326,14447.5,null,null,"N","N","",1]
["CJB25100700S","노무","L001010101000012",null,"용접공","일반공사 직종","인",6.7000000000000004E-2,0,0,267021,17890.400000000001,0,0,267021,17890.400000000001,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CJB25200800S","손료","RENT000000000002",null,"잡재료 및 소모재료","인력품의 9%","식",1,2843,2843,0,0,0,0,2843,2843,null,null,"N","N",9,1]
["CJD00110000S","기계경비","00002101002500000",null,"크레인(무한궤도)","25ton(0.76㎥)","HR",24,14653,351672,55700,1336800,29557,709368,99910,2397840,null,null,"N","N","",1]
["CJD00120000S","노무","L001010101000009",null,"철공","일반공사 직종","인",4,0,0,233754,935016,0,0,233754,935016,null,null,"N","N","",1]
["CJD00210000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",1.5,0,0,214222,321333,0,0,214222,321333,null,null,"N","N","",1]
["CJD00220000S","기계경비","00002101002500000",null,"크레인(무한궤도)","25ton(0.76㎥)","HR",8,14653,117224,55700,445600,29557,236456,99910,799280,null,null,"N","N","",1]
["CJD00330000S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",1,0,0,233722,233722,0,0,233722,233722,null,null,"N","N","",1]
["CJD00340000S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",1,0,0,233722,233722,0,0,233722,233722,null,null,"N","N","",1]
["CJI10000000S","노무","L001020701000028",null,"중급기술자","건설","인",4.2,0,0,272915,1146243,0,0,272915,1146243,null,null,"N","N","",1]
["CJI20000000S",null,null,null,"동재하시험",null,"회당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CKA11100000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.12,0,0,165545,19865.400000000001,0,0,165545,19865.400000000001,null,null,"N","N","",1]
["CKA11200000S","기계경비","00002104004000000",null,"크레인(타이어)","40ton","HR",1.33,16974,22575.4,55700,74081,65453,87052.4,138127,183708.79999999999,null,null,"N","N","",1]
["CKA11200000S","기계경비","00002106000500000",null,"고소작업차","5ton","HR",1.33,7784,10352.700000000001,47231,62817.2,34765,46237.4,89780,119407.3,null,null,"N","N","",1]
["CKA11300000S","기계경비","00002104004000000",null,"크레인(타이어)","40ton","HR",1.6,16974,27158.400000000001,55700,89120,65453,104724.8,138127,221003.2,null,null,"N","N","",1]
["CKA11400000S","기계경비","00002106000500000",null,"고소작업차","5ton","HR",2,7784,15568,47231,94462,34765,69530,89780,179560,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CKA11600000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.33,0,0,165545,54629.8,0,0,165545,54629.8,null,null,"N","N","",1]
["CKA12100000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.28999999999999998,0,0,214222,62124.3,0,0,214222,62124.3,null,null,"N","N","",1]
["CKA12100000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.14000000000000001,0,0,165545,23176.3,0,0,165545,23176.3,null,null,"N","N","",1]
["CKA12200000S","기계경비","00002104004000000",null,"크레인(타이어)","40ton","HR",1.6,16974,27158.400000000001,55700,89120,65453,104724.8,138127,221003.2,null,null,"N","N","",1]
["CKA12300000S","손료","RENT000000000001",null,"공구손료","재료비의 3%","식",1,0,0,0,0,0,0,0,0,null,null,"N","N",3,1]
["CKA12300000S","기계경비","00002104004000000",null,"크레인(타이어)","40ton","HR",2,16974,33948,55700,111400,65453,130906,138127,276254,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,65985,0,545386,0,229499,0,840870,null,null,null,null,"",1]
["CKA12500000S","기계경비","00002106000500000",null,"고소작업차","5ton","HR",2.67,7784,20783.2,47231,126106.7,34765,92822.5,89780,239712.4,null,null,"N","N","",1]
["CKA12600000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.4,0,0,165545,66218,0,0,165545,66218,null,null,"N","N","",1]
["CKA13100000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.36,0,0,214222,77119.899999999994,0,0,214222,77119.899999999994,null,null,"N","N","",1]
["CKA13200000S",null,null,null,"교량받침 설치(육상) / 1기당중량 0.3ton 이하","설치높이 40m 초과","EA",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CKA13200000S","기계경비","00002104004000000",null,"크레인(타이어)","40ton","HR",2,16974,33948,55700,111400,65453,130906,138127,276254,null,null,"N","N","",1]
["CKA13300000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,9290.2000000000007,9290.2000000000007,0,0,0,0,9290.2000000000007,9290.2000000000007,null,null,"N","N",3,1]
["CKA13400000S",null,null,null,"교량받침 설치(육상) / 1기당중량 1.0ton 이하","설치높이 40m 초과","EA",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CKA13500000S","기계경비","00002106000500000",null,"고소작업차","5ton","HR",3.2,7784,24908.799999999999,47231,151139.20000000001,34765,111248,89780,287296,null,null,"N","N","",1]
["CKA13600000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.5,0,0,165545,82772.5,0,0,165545,82772.5,null,null,"N","N","",1]
["CKA21100000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.4,0,0,214222,85688.8,0,0,214222,85688.8,null,null,"N","N","",1]
["CKA21200000S",null,null,null,"교량받침 설치(수상) / 1기당중량 0.3ton 이하","설치높이 20m 이하","EA",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CKA21200000S","기계경비","00002104004000000",null,"크레인(타이어)","40ton","HR",2.29,16974,38870.400000000001,55700,127553,65453,149887.29999999999,138127,316310.7,null,null,"N","N","",1]
["CKA21300000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,10709,10709,0,0,0,0,10709,10709,null,null,"N","N",3,1]
["CKA21400000S",null,null,null,"교량받침 설치(수상) / 1기당중량 1.0ton 이하","설치높이 20m 이하","EA",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CKA21500000S",null,null,null,"교량받침 설치(수상) / 1기당중량 1.5ton 이하","설치높이 20m 이하","EA",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CKA21500000S","기계경비","00002106000500000",null,"고소작업차","5ton","HR",3.48,7784,27088.3,47231,164363.79999999999,34765,120982.2,89780,312434.3,null,null,"N","N","",1]
["CKA21600000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.5,0,0,165545,82772.5,0,0,165545,82772.5,null,null,"N","N","",1]
["CKA22100000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.5,0,0,214222,107111,0,0,214222,107111,null,null,"N","N","",1]
["CKA22200000S",null,null,null,"교량받침 설치(수상) / 1기당중량 0.3ton 이하","설치높이 40m 이하","EA",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CKA22200000S","기계경비","00002104004000000",null,"크레인(타이어)","40ton","HR",2.67,16974,45320.5,55700,148719,65453,174759.5,138127,368799,null,null,"N","N","",1]
["CKA22300000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,12902.7,12902.7,0,0,0,0,12902.7,12902.7,null,null,"N","N",3,1]
["CKA22400000S",null,null,null,"교량받침 설치(수상) / 1기당중량 1.0ton 이하","설치높이 40m 이하","EA",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CKA22500000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",2.2200000000000002,0,0,214222,475572.8,0,0,214222,475572.8,null,null,"N","N","",1]
["CKA22500000S","기계경비","00002106000500000",null,"고소작업차","5ton","HR",4.4400000000000004,7784,34560.9,47231,209705.60000000001,34765,154356.6,89780,398623.1,null,null,"N","N","",1]
["CKA22600000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.67,0,0,165545,110915.1,0,0,165545,110915.1,null,null,"N","N","",1]
["CKA23100000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.56999999999999995,0,0,214222,122106.5,0,0,214222,122106.5,null,null,"N","N","",1]
["CKA23100000S","기계경비","00002106000500000",null,"고소작업차","5ton","HR",2.29,7784,17825.3,47231,108158.9,34765,79611.8,89780,205596,null,null,"N","N","",1]
["CKA23200000S","기계경비","00002104004000000",null,"크레인(타이어)","40ton","HR",3.2,16974,54316.800000000003,55700,178240,65453,209449.60000000001,138127,442006.4,null,null,"N","N","",1]
["CKA23300000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,16128.4,16128.4,0,0,0,0,16128.4,16128.4,null,null,"N","N",3,1]
["CKA23400000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",1.76,0,0,214222,377030.7,0,0,214222,377030.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,135577,0,1117049,0,472026,0,1724652,null,null,null,null,"",1]
["CKA23500000S","기계경비","00002106000500000",null,"고소작업차","5ton","HR",5.33,7784,41488.699999999997,47231,251741.2,34765,185297.4,89780,478527.3,null,null,"N","N","",1]
["CKA23600000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.77,0,0,165545,127469.6,0,0,165545,127469.6,null,null,"N","N","",1]
["CKA31100000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",3.7,0,0,214222,792621.4,0,0,214222,792621.4,null,null,"N","N","",1]
["CKA31200000S","손료","RENT000000000001",null,"공구손료","노무비의 5%","식",1,95572.1,95572.1,0,0,0,0,95572.1,95572.1,null,null,"N","N",5,1]
["CKA31200000S","기계경비","00002104004000000",null,"크레인(타이어)","40ton","HR",17.78,16974,301797.7,55700,990346,65453,1163754.3,138127,2455898,null,null,"N","N","",1]
["CKA31300000S","손료","RENT000000000001",null,"공구손료","노무비의 5%","식",1,134404,134404,0,0,0,0,134404,134404,null,null,"N","N",5,1]
["CKA31400000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.33,0,0,165545,551264.80000000005,0,0,165545,551264.80000000005,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,839428,0,6327834,0,2672814,0,9840076,null,null,null,null,"",1]
["CKA31500000S","기계경비","00002106000500000",null,"고소작업차","5ton","HR",30.77,7784,239513.60000000001,47231,1453297.8,34765,1069719,89780,2762530.4,null,null,"N","N","",1]
["CKA32100000S",null,null,null,"교량받침 교체 / 1기당중량 0.2ton 이하","교대 및 교각높이 40m 이하","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CKA32100000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",4.4400000000000004,0,0,214222,951145.6,0,0,214222,951145.6,null,null,"N","N","",1]
["CKA32200000S","손료","RENT000000000001",null,"공구손료","노무비의 5%","식",1,113222.8,113222.8,0,0,0,0,113222.8,113222.8,null,null,"N","N",5,1]
["CKA32300000S","노무","L001010101000012",null,"용접공","일반공사 직종","인",2.94,0,0,267021,785041.7,0,0,267021,785041.7,null,null,"N","N","",1]
["CKA32300000S","손료","RENT000000000001",null,"공구손료","노무비의 5%","식",1,158059.1,158059.1,0,0,0,0,158059.1,158059.1,null,null,"N","N",5,1]
["CKA32400000S","노무","L001010101000012",null,"용접공","일반공사 직종","인",4,0,0,267021,1068084,0,0,267021,1068084,null,null,"N","N","",1]
["CKA32500000S","기계경비","00002104004000000",null,"크레인(타이어)","40ton","HR",36.36,16974,617174.6,55700,2025252,65453,2379871,138127,5022297.5999999996,null,null,"N","N","",1]
["CKA32600000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",22.22,0,0,214222,4760012.7999999998,0,0,214222,4760012.7999999998,null,null,"N","N","",1]
["CKA33100000S",null,null,null,"교량받침 교체 / 1기당중량 0.2ton 이하","교대 및 교각높이 40m 초과","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CKA33200000S","손료","RENT000000000001",null,"공구손료","노무비의 5%","식",1,138946,138946,0,0,0,0,138946,138946,null,null,"N","N",5,1]
["CKA33300000S","노무","L001010101000012",null,"용접공","일반공사 직종","인",3.57,0,0,267021,953264.9,0,0,267021,953264.9,null,null,"N","N","",1]
["CKA33400000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.76,0,0,165545,787994.2,0,0,165545,787994.2,null,null,"N","N","",1]
["CKA33400000S","손료","RENT000000000001",null,"공구손료","노무비의 5%","식",1,256012.3,256012.3,0,0,0,0,256012.3,256012.3,null,null,"N","N",5,1]
["CKA33500000S","기계경비","00002104004000000",null,"크레인(타이어)","40ton","HR",44.44,16974,754324.5,55700,2475308,65453,2908731.3,138127,6138363.7999999998,null,null,"N","N","",1]
["CKA33600000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",26.67,0,0,214222,5713300.7000000002,0,0,214222,5713300.7000000002,null,null,"N","N","",1]
["CKC40011000S",null,null,null,"중앙분리대 지주 설치(가드레일식)","지주간격 2m","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CKC40012000S","기계경비","00005401001700000",null,"크롤러드릴(공기식)","17㎥/min(120mm)","HR",1.54E-2,0,0,55700,857.7,12315,189.6,68015,1047.3,null,null,"N","N","",1]
["CKC40021100S","기계경비","00000602002500000",null,"덤프트럭","2.5ton","HR",3.0800000000000001E-2,5090,156.69999999999999,47231,1454.7,6169,190,58490,1801.4,null,null,"N","N","",1]
["CKC40021200S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",1.8200000000000001E-2,0,0,214222,3898.8,0,0,214222,3898.8,null,null,"N","N","",1]
["CKC40022100S",null,null,null,"중앙분리대 판 설치(가드레일식)","지주간격 4m, 2W","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CKC40022300S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.1000000000000004E-3,0,0,165545,1175.3,0,0,165545,1175.3,null,null,"N","N","",1]
["CKC41010000S",null,null,null,"중앙분리대 설치(콘크리트포설식)","높이 0.81m","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CKC41020000S",null,null,null,"중앙분리대 설치(콘크리트포설식)","높이 1.27m","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CKD10010000S",null,null,null,"교량배수시설 설치","Φ150mm~250mm이하","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,6270,0,87831,0,19850,0,113951,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,2330,0,25896,0,4461,0,32687,null,null,null,null,"",1]
["CKE11020000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,520,520,0,0,0,0,520,520,null,null,"N","N",3,1]
["CKE14010000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.8999999999999997E-2,0,0,165545,9767.1,0,0,165545,9767.1,null,null,"N","N","",1]
["CKE14020000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.7000000000000004E-2,0,0,165545,11091.5,0,0,165545,11091.5,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CKR10020000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,168.3,168.3,0,0,0,0,168.3,168.3,null,null,"N","N",3,1]
["CKR10030000S","노무","L001010101000012",null,"용접공","일반공사 직종","인",4.7000000000000002E-3,0,0,267021,1254.9000000000001,0,0,267021,1254.9000000000001,null,null,"N","N","",1]
["CKR10040000S","노무","L001010101000012",null,"용접공","일반공사 직종","인",3.8E-3,0,0,267021,1014.6,0,0,267021,1014.6,null,null,"N","N","",1]
["CKR10040000S","기계경비","00002106000500000",null,"고소작업차","5ton","HR",1.03E-2,7784,80.099999999999994,47231,486.4,34765,358,89780,924.5,null,null,"N","N","",1]
["CKR10050000S","기계경비","00002101030000000",null,"크레인(무한궤도)","300ton","HR",1.4160000000000001E-2,42739,605.1,55700,788.7,479550,6790.4,577989,8184.2,null,null,"N","N","",1]
["CKR10060000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",4.7000000000000002E-3,0,0,214222,1006.8,0,0,214222,1006.8,null,null,"N","N","",1]
["CKR10070000S",null,null,null,"빔 가설공 ","150~200ton/개 미만","TON",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLA70010000S","기계경비","00000201006000000",null,"굴삭기(무한궤도)","0.6㎥","HR",4.8500000000000001E-2,15828,767.6,55700,2701.4,21957,1064.9000000000001,93485,4533.8999999999996,null,null,"N","N","",1]
["CLA70010000S","기계경비","00001305000700000",null,"진동롤러(핸드가이드식)","0.7ton","HR",4.8500000000000001E-2,3162,153.30000000000001,33571,1628.1,1846,89.5,38579,1870.9,null,null,"N","N","",1]
["CLA70020000S","기계경비","00001306012000000",null,"진동롤러(자주식)","12ton","HR",3.2000000000000001E-2,26126,836,55700,1782.4,27402,876.8,109228,3495.2,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLA80010000S","노무","L001010101000018",null,"포설공","일반공사 직종","인",1.4800000000000001E-2,0,0,205982,3048.5,0,0,205982,3048.5,null,null,"N","N","",1]
["CLA80020000S","노무","L001010101000018",null,"포설공","일반공사 직종","인",0.01,0,0,205982,2059.8000000000002,0,0,205982,2059.8000000000002,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,1046,0,2984,0,1284,0,5314,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLB00020000S","기계경비","00000201010000000",null,"굴삭기(무한궤도)","1.0㎥","HR",3.56E-2,30260,1077.2,55700,1982.9,27901,993.2,113861,4053.3,null,null,"N","N","",1]
["CLB00030000S","기계경비","00001306012000000",null,"진동롤러(자주식)","12ton","HR",1.4500000000000001E-2,26126,378.8,55700,807.6,27402,397.3,109228,1583.7,null,null,"N","N","",1]
["CLB00030000S","기계경비","00007204016000000",null,"물탱크(살수차)","16000L","HR",7.3000000000000001E-3,21331,155.69999999999999,47231,344.7,18163,132.5,86725,632.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,6,0,30,0,6,0,42,null,null,null,null,"",1]
["CLC30010000S","기계경비","00007204005500000",null,"물탱크(살수차)","5500L","HR",1.2500000000000001E-2,15378,192.2,47231,590.29999999999995,9470,118.3,72079,900.8,null,null,"N","N","",1]
["CLC32021000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.6999999999999998E-4,0,0,165545,94.3,0,0,165545,94.3,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLC32022100S","기계경비","00007204016000000",null,"물탱크(살수차)","16000L","HR",1.48E-3,21331,31.5,47231,69.900000000000006,18163,26.8,86725,128.19999999999999,null,null,"N","N","",1]
["CLC32022200S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.0000000000000001E-4,0,0,165545,33.1,0,0,165545,33.1,null,null,"N","N","",1]
["CLC33021000S",null,null,null,"아스팔트 기층 기계포설(소형장비)","1층 포설두께 8~10cm","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLC33021000S","기계경비","00007204005500000",null,"물탱크(살수차)","5500L","HR",2.5000000000000001E-3,15378,38.4,47231,118,9470,23.6,72079,180,null,null,"N","N","",1]
["CLC33022100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.0000000000000002E-4,0,0,165545,66.2,0,0,165545,66.2,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLC33022200S","기계경비","00001106001200000",null,"머캐덤 롤러(자주식)","10∼12ton","HR",1.7799999999999999E-3,13958,24.8,55700,99.1,12102,21.5,81760,145.4,null,null,"N","N","",1]
["CLC40010000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.3E-3,0,0,165545,546.20000000000005,0,0,165545,546.20000000000005,null,null,"N","N","",1]
["CLC40021000S","노무","L001010101000019",null,"포장공","일반공사 직종","인",1.8799999999999999E-3,0,0,258360,485.7,0,0,258360,485.7,null,null,"N","N","",1]
["CLC40021000S","기계경비","00001406000800000",null,"타이어 롤러(자주식)","5∼8ton","HR",5.0000000000000001E-3,7666,38.299999999999997,55700,278.5,11458,57.2,74824,374,null,null,"N","N","",1]
["CLC40022100S","기계경비","00003201000300000",null,"아스팔트 피니셔","3m","HR",3.0799999999999998E-3,17693,54.4,55700,171.5,53540,164.9,126933,390.8,null,null,"N","N","",1]
["CLC40022200S","노무","L001010101000019",null,"포장공","일반공사 직종","인",8.3000000000000001E-4,0,0,258360,214.4,0,0,258360,214.4,null,null,"N","N","",1]
["CLC40022200S","기계경비","00007204016000000",null,"물탱크(살수차)","16000L","HR",8.3000000000000001E-4,21331,17.7,47231,39.200000000000003,18163,15,86725,71.900000000000006,null,null,"N","N","",1]
["CLC81000100S","기계경비","00003201000300000",null,"아스팔트 피니셔","3m","HR",3.81E-3,17693,67.400000000000006,55700,212.2,53540,203.9,126933,483.5,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,127,0,792,0,190,0,1109,null,null,null,null,"",1]
["CLC81010000S","기계경비","00007204005500000",null,"물탱크(살수차)","5500L","HR",1.6E-2,15378,246,47231,755.6,9470,151.5,72079,1153.0999999999999,null,null,"N","N","",1]
["CLC81020000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",8.3000000000000001E-4,0,0,165545,137.4,0,0,165545,137.4,null,null,"N","N","",1]
["CLC86000100S",null,null,null,"개질아스팔트 표층 포설","2m≤시공폭<3m, 1층 포설두께 5㎝","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLC86000100S","기계경비","00001206000800000",null,"탠덤롤러(자주식)","5∼8ton","HR",3.2000000000000002E-3,7504,24,55700,178.2,8525,27.2,71729,229.4,null,null,"N","N","",1]
["CLC86000200S","기계경비","00003201000300000",null,"아스팔트 피니셔","3m","HR",1.7799999999999999E-3,17693,31.4,55700,99.1,53540,95.3,126933,225.8,null,null,"N","N","",1]
["CLC91000000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2E-3,0,0,165545,331,0,0,165545,331,null,null,"N","N","",1]
["CLC92022000S",null,null,null,"아스팔트 절삭 후 아스팔트 덧씌우기","1회절삭, 2회포장 / B-TYPE / 밀링깊이 100mm이하","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLC92022000S","기계경비","00001106001200000",null,"머캐덤 롤러(자주식)","10∼12ton","HR",4.4400000000000004E-3,13958,61.9,55700,247.3,12102,53.7,81760,362.9,null,null,"N","N","",1]
["CLC92103000S","노무","L001010101000019",null,"포장공","일반공사 직종","인",6.8999999999999997E-4,0,0,258360,178.2,0,0,258360,178.2,null,null,"N","N","",1]
["CLC92103000S","기계경비","00000302005700000",null,"로더(타이어)","0.57㎥","HR",5.5199999999999997E-3,6410,35.299999999999997,55700,307.39999999999998,6979,38.5,69089,381.2,null,null,"N","N","",1]
["CLC92111000S","기계경비","00000302009500000",null,"로더(타이어)","0.95㎥","HR",1.6000000000000001E-3,11356,18.100000000000001,55700,89.1,9059,14.4,76115,121.6,null,null,"N","N","",1]
["CLC92111000S","기계경비","00001206000800000",null,"탠덤롤러(자주식)","5∼8ton","HR",1.6000000000000001E-3,7504,12,55700,89.1,8525,13.6,71729,114.7,null,null,"N","N","",1]
["CLC92112000S","노무","L001010101000019",null,"포장공","일반공사 직종","인",1.5399999999999999E-3,0,0,258360,397.8,0,0,258360,397.8,null,null,"N","N","",1]
["CLC92112000S","기계경비","00001406001500000",null,"타이어 롤러(자주식)","8∼15ton","HR",3.0799999999999998E-3,12516,38.5,55700,171.5,17929,55.2,86145,265.2,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLC92121000S","기계경비","00003201000300000",null,"아스팔트 피니셔","3m","HR",2.3500000000000001E-3,17693,41.5,55700,130.80000000000001,53540,125.8,126933,298.10000000000002,null,null,"N","N","",1]
["CLC92131000S",null,null,null,"아스팔트 절삭 후 아스팔트 덧씌우기","1회절삭, 1회포장 / C-TYPE / 밀링깊이 70mm이하","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLC92131000S","기계경비","00005702009500000",null,"소형노면파쇄기","0.95m3","HR",4.4400000000000004E-3,0,0,0,0,10721,47.6,10721,47.6,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,824,0,2945,0,1393,0,5162,null,null,null,null,"",1]
["CLC92202000S","기계경비","00005702009500000",null,"소형노면파쇄기","0.95m3","HR",5.7099999999999998E-3,0,0,0,0,10721,61.2,10721,61.2,null,null,"N","N","",1]
["CLC92202000S","기계경비","00001206000800000",null,"탠덤롤러(자주식)","5∼8ton","HR",5.7099999999999998E-3,7504,42.8,55700,318,8525,48.6,71729,409.4,null,null,"N","N","",1]
["CLC92303000S","기계경비","00000302005700000",null,"로더(타이어)","0.57㎥","HR",4.0000000000000001E-3,6410,25.6,55700,222.8,6979,27.9,69089,276.3,null,null,"N","N","",1]
["CLC93110000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5000000000000001E-3,0,0,165545,413.8,0,0,165545,413.8,null,null,"N","N","",1]
["CLC93110000S","기계경비","00000302009500000",null,"로더(타이어)","0.95㎥","HR",0.02,11356,227.1,55700,1114,9059,181.1,76115,1522.2,null,null,"N","N","",1]
["CLC93120000S","기계경비","00005702009500000",null,"소형노면파쇄기","0.95m3","HR",5.7099999999999998E-2,0,0,0,0,10721,612.1,10721,612.1,null,null,"N","N","",1]
["CLC93130000S","노무","L001010101000019",null,"포장공","일반공사 직종","인",0.06,0,0,258360,15501.6,0,0,258360,15501.6,null,null,"N","N","",1]
["CLC93130000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.02,0,0,165545,3310.9,0,0,165545,3310.9,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLC93220000S",null,null,null,"소파보수(포장복구) ","B-Type / 시공면적 11~20m2","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLC93220000S","노무","L001010101000019",null,"포장공","일반공사 직종","인",6.7000000000000004E-2,0,0,258360,17310.099999999999,0,0,258360,17310.099999999999,null,null,"N","N","",1]
["CLC93230000S","기계경비","00000211001800000",null,"굴삭기(타이어)","0.18㎥","HR",0.4,8832,3532.8,55700,22280,15117,6046.8,79649,31859.599999999999,null,null,"N","N","",1]
["CLC93310000S","노무","L001010101000019",null,"포장공","일반공사 직종","인",4.7E-2,0,0,258360,12142.9,0,0,258360,12142.9,null,null,"N","N","",1]
["CLC93310000S","기계경비","00004430040000000",null,"커터(콘크리트 및 아스팔트용)","320∼400mm","HR",9.4E-2,9562,898.8,33571,3155.6,1876,176.3,45009,4230.7,null,null,"N","N","",1]
["CLC93320000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.7000000000000002E-2,0,0,165545,9436,0,0,165545,9436,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,8844,0,114114,0,10419,0,133377,null,null,null,null,"",1]
["CLC93330000S",null,null,null,"소파보수(도로복구) ","C-Type / 시공면적 5~8m2","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLC93330000S","기계경비","00000602002500000",null,"덤프트럭","2.5ton","HR",1.0669999999999999,5090,5431,47231,50395.4,6169,6582.3,58490,62408.7,null,null,"N","N","",1]
["CLC94100000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.5,0,0,214222,107111,0,0,214222,107111,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,48861,0,553365,0,31467,0,633693,null,null,null,null,"",1]
["CLC94200000S","기계경비","00005220001500000",null,"소형브레이커(전기식)","1.5kw","HR",4,0,0,0,0,322,1288,322,1288,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLC96000000S",null,null,null,"표면평탄작업",null,"M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLC96000000S","기계경비","00005701002000000",null,"노면파쇄기","2m","HR",7.2700000000000004E-3,77759,565.29999999999995,55700,404.9,161850,1176.5999999999999,295309,2146.8000000000002,null,null,"N","N","",1]
["CLC97000000S","기계경비","00001106001200000",null,"머캐덤 롤러(자주식)","10∼12ton","HR",2.8600000000000001E-3,13958,39.9,55700,159.30000000000001,12102,34.6,81760,233.8,null,null,"N","N","",1]
["CLD11110000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.5999999999999999E-3,0,0,165545,595.9,0,0,165545,595.9,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLD11212000S","노무","L001010101000019",null,"포장공","일반공사 직종","인",2.6700000000000002E-2,0,0,258360,6898.2,0,0,258360,6898.2,null,null,"N","N","",1]
["CLD11213000S",null,null,null,"콘크리트 표층 인력포설","A-Type, 40cm","M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLD11221000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.04,0,0,165545,6621.8,0,0,165545,6621.8,null,null,"N","N","",1]
["CLD11222000S",null,null,null,"콘크리트 표층 인력포설","B-Type, 30cm","M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLD11223000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.02,0,0,165545,3310.9,0,0,165545,3310.9,null,null,"N","N","",1]
["CLD11310000S","기계경비","00003601020200000",null,"콘크리트 피니셔(포장용)","160.4kw","HR",2.6700000000000002E-2,29871,797.5,55700,1487.1,62364,1665.1,147935,3949.7,null,null,"N","N","",1]
["CLD11320000S",null,null,null,"콘크리트 표층 기계포설(소형장비)","터널포장","M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,2058,0,10444,0,2889,0,15391,null,null,null,null,"",1]
["CLD11410000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.8999999999999998E-3,0,0,165545,480,0,0,165545,480,null,null,"N","N","",1]
["CLD11420000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",3.3E-3,0,0,214222,706.9,0,0,214222,706.9,null,null,"N","N","",1]
["CLD11430000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",3.0999999999999999E-3,0,0,214222,664,0,0,214222,664,null,null,"N","N","",1]
["CLD11430000S","기계경비","00000201010000000",null,"굴삭기(무한궤도)","1.0㎥","HR",1.2500000000000001E-2,30260,378.2,55700,696.2,27901,348.7,113861,1423.1,null,null,"N","N","",1]
["CLD11510000S","기계경비","00002101002500000",null,"크레인(무한궤도)","25ton(0.76㎥)","HR",24,14653,351672,55700,1336800,29557,709368,99910,2397840,null,null,"N","N","",1]
["CLD11512000S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",2,0,0,233722,467444,0,0,233722,467444,null,null,"N","N","",1]
["CLD11520000S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",2,0,0,233722,467444,0,0,233722,467444,null,null,"N","N","",1]
["CLD11522000S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",1,0,0,233722,233722,0,0,233722,233722,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,151114,0,1575274,0,236456,0,1962844,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLD62200000S","노무","L001010101000019",null,"포장공","일반공사 직종","인",2.5000000000000001E-3,0,0,258360,645.9,0,0,258360,645.9,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLF30011100S",null,null,null,"보차도 및 도로경계블록 설치","A-Type / 아래폭+높이300㎜ 미만 / 직선구간","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,926,0,8362,0,872,0,10160,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLF30012200S",null,null,null,"보차도 및 도로경계블록 설치","B-Type / 아래폭+높이300㎜ 미만 / 곡선구간","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLF30021100S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,111.5,111.5,0,0,0,0,111.5,111.5,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,1112,0,10030,0,1048,0,12190,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLF30022200S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,142.5,142.5,0,0,0,0,142.5,142.5,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,1069,0,9648,0,1007,0,11724,null,null,null,null,"",1]
["CLF30031200S","기계경비","00000201004000000",null,"굴삭기(무한궤도)","0.4㎥","HR",7.2700000000000001E-2,15363,1116.8,55700,4049.3,16378,1190.5999999999999,87441,6356.7,null,null,"N","N","",1]
["CLF30032100S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,130.6,130.6,0,0,0,0,130.6,130.6,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,982,0,13895,0,1395,0,16272,null,null,null,null,"",1]
["CLF30041100S","기계경비","00000201004000000",null,"굴삭기(무한궤도)","0.4㎥","HR",8.8999999999999996E-2,15363,1367.3,55700,4957.3,16378,1457.6,87441,7782.2,null,null,"N","N","",1]
["CLF30041200S","기계경비","00000201004000000",null,"굴삭기(무한궤도)","0.4㎥","HR",0.1,15363,1536.3,55700,5570,16378,1637.8,87441,8744.1,null,null,"N","N","",1]
["CLF30042100S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,182.4,182.4,0,0,0,0,182.4,182.4,null,null,"N","N",2,1]
["CLF30042200S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.7000000000000001E-2,0,0,165545,2814.2,0,0,165545,2814.2,null,null,"N","N","",1]
["CLF30051100S","기계경비","00000201004000000",null,"굴삭기(무한궤도)","0.4㎥","HR",0.13300000000000001,15363,2043.2,55700,7408.1,16378,2178.1999999999998,87441,11629.5,null,null,"N","N","",1]
["CLF30051200S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.06,0,0,214222,12853.3,0,0,214222,12853.3,null,null,"N","N","",1]
["CLF30052100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5000000000000001E-2,0,0,165545,4138.6000000000004,0,0,165545,4138.6000000000004,null,null,"N","N","",1]
["CLF30052200S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",5.7000000000000002E-2,0,0,214222,12210.6,0,0,214222,12210.6,null,null,"N","N","",1]
["CLF30111000S",null,null,null,"보차도 및 도로경계블록 철거","A-Type / 아래폭+높이300㎜ 미만","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLF30112000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",4.7999999999999996E-3,0,0,214222,1028.2,0,0,214222,1028.2,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLF30114000S",null,null,null,"보차도 및 도로경계블록 철거","A-Type / 아래폭+높이500㎜ 미만","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLF30115000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",1.18E-2,0,0,214222,2527.8000000000002,0,0,214222,2527.8000000000002,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLF30122000S",null,null,null,"보차도 및 도로경계블록 철거","B-Type / 아래폭+높이350㎜ 미만","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLF30123000S",null,null,null,"보차도 및 도로경계블록 철거","B-Type / 아래폭+높이400㎜ 미만","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,329,0,4577,0,495,0,5401,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLF30125000S","기계경비","00000602002500000",null,"덤프트럭","2.5ton","HR",6.1499999999999999E-2,5090,313,47231,2904.7,6169,379.3,58490,3597,null,null,"N","N","",1]
["CLF30211100S","기계경비","00000602002500000",null,"덤프트럭","2.5ton","HR",5.33E-2,5090,271.2,47231,2517.4,6169,328.8,58490,3117.4,null,null,"N","N","",1]
["CLF30211200S","기계경비","00000602002500000",null,"덤프트럭","2.5ton","HR",6.1499999999999999E-2,5090,313,47231,2904.7,6169,379.3,58490,3597,null,null,"N","N","",1]
["CLF30212100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",8.3000000000000001E-3,0,0,165545,1374,0,0,165545,1374,null,null,"N","N","",1]
["CLF30212200S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",9.1000000000000004E-3,0,0,165545,1506.4,0,0,165545,1506.4,null,null,"N","N","",1]
["CLF30213100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",9.1000000000000004E-3,0,0,165545,1506.4,0,0,165545,1506.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,1633,0,14837,0,1639,0,18109,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,1891,0,17322,0,1893,0,21106,null,null,null,null,"",1]
["CLF30214100S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,205.8,205.8,0,0,0,0,205.8,205.8,null,null,"N","N",2,1]
["CLF30214200S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,246.7,246.7,0,0,0,0,246.7,246.7,null,null,"N","N",2,1]
["CLF30215100S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,323.2,323.2,0,0,0,0,323.2,323.2,null,null,"N","N",2,1]
["CLF30215200S",null,null,null,"보차도 및 도로경계블록 재설치","A-Type / 아래폭+높이500㎜ 이상 / 곡선구간","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLF30221100S",null,null,null,"보차도 및 도로경계블록 재설치","B-Type / 아래폭+높이300㎜ 미만 / 직선구간","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLF30221200S","기계경비","00000201002000000",null,"굴삭기(무한궤도)","0.2㎥","HR",8.4000000000000005E-2,7695,646.29999999999995,55700,4678.8,13041,1095.4000000000001,76436,6420.5,null,null,"N","N","",1]
["CLF30222100S","기계경비","00000201002000000",null,"굴삭기(무한궤도)","0.2㎥","HR",9.4E-2,7695,723.3,55700,5235.8,13041,1225.8,76436,7184.9,null,null,"N","N","",1]
["CLF30223100S",null,null,null,"보차도 및 도로경계블록 재설치","B-Type / 아래폭+높이400㎜ 미만 / 직선구간","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLF30223100S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",2.5000000000000001E-2,0,0,214222,5355.5,0,0,214222,5355.5,null,null,"N","N","",1]
["CLF30223200S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",2.9000000000000001E-2,0,0,214222,6212.4,0,0,214222,6212.4,null,null,"N","N","",1]
["CLF30224100S","기계경비","00000602002500000",null,"덤프트럭","2.5ton","HR",0.14499999999999999,5090,738,47231,6848.4,6169,894.5,58490,8480.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,2067,0,25616,0,2785,0,30468,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,2853,0,35435,0,3842,0,42130,null,null,null,null,"",1]
["CLF30225200S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",6.7000000000000004E-2,0,0,214222,14352.8,0,0,214222,14352.8,null,null,"N","N","",1]
["CLF30225200S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.3000000000000002E-2,0,0,165545,5462.9,0,0,165545,5462.9,null,null,"N","N","",1]
["CLG82111000S","손료","RENT000000000001",null,"공구손료","노무비의 5%","식",1,256.3,256.3,0,0,0,0,256.3,256.3,null,null,"N","N",5,1]
["CLG82112000S","기계경비","00001730001500000",null,"플레이트 콤팩터","1.5ton","HR",2.6700000000000002E-2,1707,45.5,33571,896.3,582,15.5,35860,957.3,null,null,"N","N","",1]
["CLG82121000S","노무","L001010101000019",null,"포장공","일반공사 직종","인",1.0500000000000001E-2,0,0,258360,2712.7,0,0,258360,2712.7,null,null,"N","N","",1]
["CLG82122000S",null,null,null,"보도용 블록 설치(소형)","B-Type, 0.1m2 이하","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLG82122000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",5.3E-3,0,0,214222,1135.3,0,0,214222,1135.3,null,null,"N","N","",1]
["CLG82210000S","기계경비","00000602002500000",null,"덤프트럭","2.5ton","HR",2.2200000000000001E-2,5090,112.9,47231,1048.5,6169,136.9,58490,1298.3,null,null,"N","N","",1]
["CLG82211000S","기계경비","00001730001500000",null,"플레이트 콤팩터","1.5ton","HR",4.2099999999999999E-2,1707,71.8,33571,1413.3,582,24.5,35860,1509.6,null,null,"N","N","",1]
["CLG82212000S","기계경비","00000201006000000",null,"굴삭기(무한궤도)","0.6㎥","HR",4.2099999999999999E-2,15828,666.3,55700,2344.9,21957,924.3,93485,3935.5,null,null,"N","N","",1]
["CLG82220000S",null,null,null,"보도용 블록 인력철거","B-Type","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLG82221000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",1.67E-2,0,0,214222,3577.5,0,0,214222,3577.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,1601,0,15220,0,1131,0,17952,null,null,null,null,"",1]
["CLG82222000S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,149.30000000000001,149.30000000000001,0,0,0,0,149.30000000000001,149.30000000000001,null,null,"N","N",2,1]
["CLG82310000S",null,null,null,"보도용 블록 장비사용 철거","A-Type","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLG82320000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.2000000000000001E-3,0,0,165545,364.1,0,0,165545,364.1,null,null,"N","N","",1]
["CLG82410000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.7000000000000002E-3,0,0,165545,1274.5999999999999,0,0,165545,1274.5999999999999,null,null,"N","N","",1]
["CLG82411000S","노무","L001010101000019",null,"포장공","일반공사 직종","인",1.8800000000000001E-2,0,0,258360,4857.1000000000004,0,0,258360,4857.1000000000004,null,null,"N","N","",1]
["CLG82411000S","기계경비","00001730001500000",null,"플레이트 콤팩터","1.5ton","HR",0.05,1707,85.3,33571,1678.5,582,29.1,35860,1792.9,null,null,"N","N","",1]
["CLG82420000S","손료","RENT000000000001",null,"공구손료","노무비의 5%","식",1,308.60000000000002,308.60000000000002,0,0,0,0,308.60000000000002,308.60000000000002,null,null,"N","N",5,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLG82421000S","기계경비","00000602002500000",null,"덤프트럭","2.5ton","HR",0.08,5090,407.2,47231,3778.4,6169,493.5,58490,4679.1000000000004,null,null,"N","N","",1]
["CLG82500000S","노무","L001010101000019",null,"포장공","일반공사 직종","인",1.8200000000000001E-2,0,0,258360,4702.1000000000004,0,0,258360,4702.1000000000004,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLH12000000S",null,null,null,"도로 표지판 설치","편지식+표지판 (12m2이하)","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,12805,0,156726,0,56667,0,226198,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLH14020000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.33,0,0,214222,70693.2,0,0,214222,70693.2,null,null,"N","N","",1]
["CLH14210000S",null,null,null,"도로반사경 철거","1면","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLH14220000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.111,0,0,214222,23778.6,0,0,214222,23778.6,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLH15000000S",null,null,null,"탄성포장재 포설","포설두께 7.5㎝","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLH15010000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",8.3000000000000004E-2,0,0,165545,13740.2,0,0,165545,13740.2,null,null,"N","N","",1]
["CLH15020000S",null,null,null,"교통 안전표지판 설치","표지판","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLH15200000S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,700.9,700.9,0,0,0,0,700.9,700.9,null,null,"N","N",2,1]
["CLH15300000S","기계경비","00000602002500000",null,"덤프트럭","2.5ton","HR",1.33,5090,6769.7,47231,62817.2,6169,8204.7000000000007,58490,77791.600000000006,null,null,"N","N","",1]
["CLH21111000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.2000000000000001E-3,0,0,165545,364.1,0,0,165545,364.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,90,0,2511,0,109,0,2710,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,119,0,3307,0,144,0,3570,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,251,0,7004,0,304,0,7559,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLH21123000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,66,66,0,0,0,0,66,66,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,271,0,3307,0,168,0,3746,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLH21132000S","기계경비","00000602002500000",null,"덤프트럭","2.5ton","HR",3.0200000000000001E-3,5090,15.3,47231,142.6,6169,18.600000000000001,58490,176.5,null,null,"N","N","",1]
["CLH21141000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",2.8999999999999998E-3,0,0,214222,621.20000000000005,0,0,214222,621.20000000000005,null,null,"N","N","",1]
["CLH21142000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",5.7000000000000002E-3,0,0,214222,1221,0,0,214222,1221,null,null,"N","N","",1]
["CLH21143000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",7.4999999999999997E-3,0,0,214222,1606.6,0,0,214222,1606.6,null,null,"N","N","",1]
["CLH21143000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.4999999999999997E-3,0,0,165545,1241.5,0,0,165545,1241.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,1484,0,12036,0,849,0,14369,null,null,null,null,"",1]
["CLH21212000S",null,null,null,"차선 밑그림 / 공용구간","파선","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLH21212000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",6.7000000000000002E-3,0,0,214222,1435.2,0,0,214222,1435.2,null,null,"N","N","",1]
["CLH21214000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",1.8499999999999999E-2,0,0,214222,3963.1,0,0,214222,3963.1,null,null,"N","N","",1]
["CLH21221000S",null,null,null,"수용성형 페인트 수동식 / 공용구간","실선","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLH21222000S",null,null,null,"수용성형 페인트 수동식 / 공용구간","파선","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLH21223000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",8.8000000000000005E-3,0,0,214222,1885.1,0,0,214222,1885.1,null,null,"N","N","",1]
["CLH21224000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.8499999999999999E-2,0,0,165545,3062.5,0,0,165545,3062.5,null,null,"N","N","",1]
["CLH21231000S",null,null,null,"수용성형 페인트 기계식 / 공용구간","실선","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLH21232000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",5.0000000000000001E-4,0,0,214222,107.1,0,0,214222,107.1,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLH21242000S","손료","RENT000000000001",null,"공구손료","노무비의 10%","식",1,303.8,303.8,0,0,0,0,303.8,303.8,null,null,"N","N",10,1]
["CLH21243000S","기계경비","00000602002500000",null,"덤프트럭","2.5ton","HR",4.2099999999999999E-2,5090,214.2,47231,1988.4,6169,259.7,58490,2462.3000000000002,null,null,"N","N","",1]
["CLH21244000S","기계경비","00000602002500000",null,"덤프트럭","2.5ton","HR",8.8999999999999996E-2,5090,453,47231,4203.5,6169,549,58490,5205.5,null,null,"N","N","",1]
["CLH21300000S","기계경비","00007360009000000",null,"차선 제거기","6.71kw","HR",0.22900000000000001,9442,2162.1999999999998,47231,10815.8,3568,817,60241,13795,null,null,"N","N","",1]
["CLH22000000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",1.4E-2,0,0,214222,2999.1,0,0,214222,2999.1,null,null,"N","N","",1]
["CLH22200000S","기계경비","00000602002500000",null,"덤프트럭","2.5ton","HR",0.2,5090,1018,47231,9446.2000000000007,6169,1233.8,58490,11698,null,null,"N","N","",1]
["CLH23010000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.7000000000000001E-2,0,0,165545,2814.2,0,0,165545,2814.2,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,76,0,2544,0,0,0,2620,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLH23210000S","기계경비","00000602002500000",null,"덤프트럭","2.5ton","HR",6.1499999999999999E-2,5090,313,47231,2904.7,6169,379.3,58490,3597,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,199,0,2897,0,190,0,3286,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,2286,0,45737,0,0,0,48023,null,null,null,null,"",1]
["CLH27000000S",null,null,null,"차선규제봉 설치","450mm~750mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLH28020000S",null,null,null,"표시못 설치","B-Type","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLH31011000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",4.7999999999999996E-3,0,0,214222,1028.2,0,0,214222,1028.2,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,382,0,3381,0,702,0,4465,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLH31021100S","손료","RENT000000000001",null,"공구손료","노무비의 5%","식",1,113.9,113.9,0,0,0,0,113.9,113.9,null,null,"N","N",5,1]
[null,null,null,null,"[합 계]",null,null,0,0,227,0,3553,0,112,0,3892,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLH31022300S","손료","RENT000000000001",null,"공구손료","노무비의 5%","식",1,105.8,105.8,0,0,0,0,105.8,105.8,null,null,"N","N",5,1]
["CLH80000000S","기계경비","00007505005000000",null,"발전기","50kw","HR",0.22900000000000001,13722,3142.3,33571,7687.7,4447,1018.3,51740,11848.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,17943,0,0,0,17943,null,null,null,null,"",1]
["CLH81200000S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.02,0,0,267021,5340.4,0,0,267021,5340.4,null,null,"N","N","",1]
["CLH82100000S",null,null,null,"재래난간 철거공 / 속주","강재난간","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLL31100150S",null,null,null,"플륨관 설치","중량50~150KG미만","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLL31100150S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.02,0,0,214222,4284.3999999999996,0,0,214222,4284.3999999999996,null,null,"N","N","",1]
["CLL31100300S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.02,0,0,165545,3310.9,0,0,165545,3310.9,null,null,"N","N","",1]
["CLL31100700S",null,null,null,"플륨관 설치","중량500~700KG미만","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLL31100700S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.05,0,0,214222,10711.1,0,0,214222,10711.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,2937,0,31267,0,5809,0,40013,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLL31101300S",null,null,null,"플륨관 설치","중량1100~1300KG미만","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,4756,0,50265,0,9783,0,64804,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLL31102100S",null,null,null,"플륨관 설치","중량1800~2100KG미만","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLL31300700S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.03,0,0,214222,6426.6,0,0,214222,6426.6,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLL31301300S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",4.4999999999999998E-2,0,0,214222,9639.9,0,0,214222,9639.9,null,null,"N","N","",1]
["CLL31301500S","기계경비","00002104001000000",null,"크레인(타이어)","10ton","HR",0.23499999999999999,6718,1578.7,55700,13089.5,30103,7074.2,92521,21742.400000000001,null,null,"N","N","",1]
["CLL31301800S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.3000000000000002E-2,0,0,165545,5462.9,0,0,165545,5462.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,2069,0,39941,0,9271,0,51281,null,null,null,null,"",1]
["CLL50101200S",null,null,null,"조립식 PC맨홀 설치","Ø1,200(하부구체+상판)","EA",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLL50101500S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.38,0,0,165545,62907.1,0,0,165545,62907.1,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLL50201200S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.33,0,0,214222,70693.2,0,0,214222,70693.2,null,null,"N","N","",1]
["CLL50201500S","기계경비","00002104001000000",null,"크레인(타이어)","10ton","HR",0.64,6718,4299.5,55700,35648,30103,19265.900000000001,92521,59213.4,null,null,"N","N","",1]
["CLL50201800S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.23,0,0,165545,38075.300000000003,0,0,165545,38075.300000000003,null,null,"N","N","",1]
["CLR10010000S","기계경비","00005205010300000",null,"공기압축기(이동식)","10.3㎥/min","HR",0.01,20952,209.5,55700,557,5474,54.7,82126,821.2,null,null,"N","N","",1]
["CLR10021000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",5.0000000000000001E-3,0,0,214222,1071.0999999999999,0,0,214222,1071.0999999999999,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,9250,0,0,0,9250,null,null,null,null,"",1]
["CLR20010000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",7.4999999999999997E-2,0,0,214222,16066.6,0,0,214222,16066.6,null,null,"N","N","",1]
["CLR20020000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.01,0,0,165545,1655.4,0,0,165545,1655.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,66,0,3304,0,0,0,3370,null,null,null,null,"",1]
["CLR32021100S",null,null,null,"방음벽 지주설치","지주높이 3m 이하, 지주간격 2m","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,3833,0,53942,0,3477,0,61252,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLR32021300S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,1241.0999999999999,1241.0999999999999,0,0,0,0,1241.0999999999999,1241.0999999999999,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,919,0,15074,0,733,0,16726,null,null,null,null,"",1]
["CLR32032000S","기계경비","00002105000500000",null,"트럭탑재형 크레인","5ton","HR",9.1999999999999998E-2,7784,716.1,47231,4345.2,9994,919.4,65009,5980.7,null,null,"N","N","",1]
["CLR32033000S","기계경비","00002105000500000",null,"트럭탑재형 크레인","5ton","HR",9.4E-2,7784,731.6,47231,4439.7,9994,939.4,65009,6110.7,null,null,"N","N","",1]
["CLR32034000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,531.70000000000005,531.70000000000005,0,0,0,0,531.70000000000005,531.70000000000005,null,null,"N","N",3,1]
["CLR34031000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,311.10000000000002,311.10000000000002,0,0,0,0,311.10000000000002,311.10000000000002,null,null,"N","N",3,1]
["CLR34032000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.4799999999999999E-2,0,0,165545,4105.5,0,0,165545,4105.5,null,null,"N","N","",1]
["CLR34033000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.7E-2,0,0,165545,4469.7,0,0,165545,4469.7,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLR36022100S","노무","L001010101000009",null,"철공","일반공사 직종","인",0.15,0,0,233754,35063.1,0,0,233754,35063.1,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLR36022200S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,1371.2,1371.2,0,0,0,0,1371.2,1371.2,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,4905,0,69277,0,4437,0,78619,null,null,null,null,"",1]
["CLR36032000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.9100000000000001E-2,0,0,165545,4817.3,0,0,165545,4817.3,null,null,"N","N","",1]
["CLR36032000S","기계경비","00002105000500000",null,"트럭탑재형 크레인","5ton","HR",7.7700000000000005E-2,7784,604.79999999999995,47231,3669.8,9994,776.5,65009,5051.1000000000004,null,null,"N","N","",1]
["CLR36033000S","기계경비","00002105000500000",null,"트럭탑재형 크레인","5ton","HR",8.8999999999999996E-2,7784,692.7,47231,4203.5,9994,889.4,65009,5785.6,null,null,"N","N","",1]
["CLR38024100S",null,null,null,"방음벽 지주설치","지주높이 11m 이하, 지주간격 2m","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CLR38024100S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,2384.6999999999998,2384.6999999999998,0,0,0,0,2384.6999999999998,2384.6999999999998,null,null,"N","N",3,1]
["CLR38031000S","노무","L001010101000009",null,"철공","일반공사 직종","인",3.3599999999999998E-2,0,0,233754,7854.1,0,0,233754,7854.1,null,null,"N","N","",1]
["CLR38032000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,453.4,453.4,0,0,0,0,453.4,453.4,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,1504,0,23049,0,2204,0,26757,null,null,null,null,"",1]
["CLR39032000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.5000000000000003E-2,0,0,165545,5794,0,0,165545,5794,null,null,"N","N","",1]
["CLR41010000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.3999999999999999E-4,0,0,165545,122.5,0,0,165545,122.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,439,0,0,0,439,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CMA11110000S","기계경비","00002502005000000",null,"지게차","5.0ton","HR",3.2000000000000001E-2,9933,317.8,55700,1782.4,6807,217.8,72440,2318,null,null,"N","N","",1]
["CMA11120000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.4800000000000001E-2,0,0,165545,2450,0,0,165545,2450,null,null,"N","N","",1]
["CMA11210000S","노무","L001010101000046",null,"궤도공","일반공사 직종","인",1.6E-2,0,0,209325,3349.2,0,0,209325,3349.2,null,null,"N","N","",1]
["CMA12111000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.6799999999999999E-2,0,0,165545,2781.1,0,0,165545,2781.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,594,0,21628,0,786,0,23008,null,null,null,null,"",1]
["CMA12112000S","기계경비","00007206002000000",null,"부착용 집게","0.2㎥","HR",1.6799999999999999E-2,0,0,0,0,3484,58.5,3484,58.5,null,null,"N","N","",1]
["CMA12121000S","기계경비","00000201002000000",null,"굴삭기(무한궤도)","0.2㎥","HR",3.2000000000000001E-2,7695,246.2,55700,1782.4,13041,417.3,76436,2445.9,null,null,"N","N","",1]
["CMA12122000S","노무","L001010101000046",null,"궤도공","일반공사 직종","인",6.4000000000000001E-2,0,0,209325,13396.8,0,0,209325,13396.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,440,0,20981,0,482,0,21903,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,718,0,8765,0,612,0,10095,null,null,null,null,"",1]
["CMA12310300S","노무","L001010101000046",null,"궤도공","일반공사 직종","인",2.9499999999999998E-2,0,0,209325,6175,0,0,209325,6175,null,null,"N","N","",1]
["CMA12310400S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",8.3999999999999995E-3,0,0,165545,1390.5,0,0,165545,1390.5,null,null,"N","N","",1]
["CMA12310500S","노무","L001010101000046",null,"궤도공","일반공사 직종","인",3.7900000000000003E-2,0,0,209325,7933.4,0,0,209325,7933.4,null,null,"N","N","",1]
["CMA12320100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.5999999999999997E-2,0,0,165545,5959.6,0,0,165545,5959.6,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CMA12320300S","기계경비","00007954111900000",null,"양로기","11.19kw","HR",3.2000000000000001E-2,2360,75.5,55700,1782.4,8767,280.5,66827,2138.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,8960,0,0,0,8960,null,null,null,null,"",1]
["CMA12320500S","노무","L001040101000324",null,"중급기술자","측량기술계","인",4.0000000000000001E-3,0,0,234406,937.6,0,0,234406,937.6,null,null,"N","N","",1]
["CMA21000000S","기계경비","00007206002000000",null,"부착용 집게","0.2㎥","HR",53,0,0,0,0,3484,184652,3484,184652,null,null,"N","N","",1]
["CMA22000000S","기계경비","00000201006000000",null,"굴삭기(무한궤도)","0.6㎥","HR",153,15828,2421684,55700,8522100,21957,3359421,93485,14303205,null,null,"N","N","",1]
["CMA31010000S",null,null,null,"궤광철거 / 목침목 구간","37kg/m","km",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CMA31020000S","노무","L001010101000046",null,"궤도공","일반공사 직종","인",49,0,0,209325,10256925,0,0,209325,10256925,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,415530,0,13454900,0,892350,0,14762780,null,null,null,null,"",1]
["CMA33010000S",null,null,null,"궤광철거 / 터널, 교량","37kg/m","km",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,500175,0,16073290,0,1074125,0,17647590,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CMB11010000S","손료","RENT000000000001",null,"할증","합계의 70%","식",1,103101.6,103101.6,2415326.2000000002,2415326.2000000002,285142.2,285142.2,2803570,2803570,null,null,"N","N",70,1]
["CMB11020000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3,0,0,165545,496635,0,0,165545,496635,null,null,"N","Y","",0]
["CMB11030000S",null,null,null,"분기기 부설","#12, 50kg, PCT","틀",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CMB11030000S","기계경비","00000201002000000",null,"굴삭기(무한궤도)","0.2㎥","HR",12,7695,92340,55700,668400,13041,156492,76436,917232,null,null,"N","Y","",0]
["CMB11040000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3,0,0,165545,496635,0,0,165545,496635,null,null,"N","Y","",0]
["CMB11050000S",null,null,null,"분기기 부설","#18, 50kg, PCT","틀",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CMB11050000S","기계경비","00000201002000000",null,"굴삭기(무한궤도)","0.2㎥","HR",12,7695,92340,55700,668400,13041,156492,76436,917232,null,null,"N","Y","",0]
["CMB12010000S","노무","L001040101000324",null,"중급기술자","측량기술계","인",1,0,0,234406,234406,0,0,234406,234406,null,null,"N","Y","",0]
["CMB12020000S","노무","L001010101000046",null,"궤도공","일반공사 직종","인",9,0,0,209325,1883925,0,0,209325,1883925,null,null,"N","Y","",0]
["CMB12020000S","기계경비","00007206002000000",null,"부착용 집게","0.2㎥","HR",12,0,0,0,0,3484,41808,3484,41808,null,null,"N","Y","",0]
["CMB12030000S","기계경비","00002101005000000",null,"크레인(무한궤도)","50ton(1.91㎥)","HR",3,18316,54948,55700,167100,69682,209046,143698,431094,null,null,"N","N","",1]
["CMB12040000S","손료","RENT000000000001",null,"할증","합계의 120%","식",1,176745.60000000001,176745.60000000001,4140559.2,4140559.2,488815.2,488815.2,4806120,4806120,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,176745,0,4140559,0,488815,0,4806119,null,null,null,null,"",1]
["CMB12050000S","기계경비","00000201002000000",null,"굴삭기(무한궤도)","0.2㎥","HR",12,7695,92340,55700,668400,13041,156492,76436,917232,null,null,"N","Y","",0]
["CMB30020000S",null,null,null,"분기기 철거","#10 분기기","틀",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CMB30020000S","노무","L001010101000046",null,"궤도공","일반공사 직종","인",9,0,0,209325,1883925,0,0,209325,1883925,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CMB40010000S",null,null,null,"분기기 / 신축이음매 부설","일단","틀",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CMB40010000S","노무","L001010101000046",null,"궤도공","일반공사 직종","인",0.25,0,0,209325,52331.199999999997,0,0,209325,52331.199999999997,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CMC10000050S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.25,0,0,267021,66755.199999999997,0,0,267021,66755.199999999997,null,null,"N","N","",1]
["CMC10000060S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.28000000000000003,0,0,267021,74765.8,0,0,267021,74765.8,null,null,"N","N","",1]
["CMC70010000S","노무","L001010101000046",null,"궤도공","일반공사 직종","인",16.600000000000001,0,0,209325,3474795,0,0,209325,3474795,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,4583946,0,0,0,4583946,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,1574,0,0,0,1574,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CMF11111200S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",45,0,0,165545,7449525,0,0,165545,7449525,null,null,"N","N","",1]
["CMF11112100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",35,0,0,165545,5794075,0,0,165545,5794075,null,null,"N","N","",1]
["CMF11112200S",null,null,null,"레일교환 / 목침목 / 인력","60kg, 3시간 차단, 시공구간 100M 이하","km",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CMF11121100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",39,0,0,165545,6456255,0,0,165545,6456255,null,null,"N","N","",1]
["CMF11122100S",null,null,null,"레일교환 / 목침목 / 인력","50kg, 4시간 차단, 시공구간 100M 이하","km",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CMF11122200S",null,null,null,"레일교환 / 목침목 / 인력","60kg, 4시간 차단, 시공구간 100M 이하","km",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,29798040,0,0,0,29798040,null,null,null,null,"",1]
["CMF11211100S","노무","L001010101000046",null,"궤도공","일반공사 직종","인",178,0,0,209325,37259850,0,0,209325,37259850,null,null,"N","N","",1]
["CMF11211200S","노무","L001010101000046",null,"궤도공","일반공사 직종","인",196,0,0,209325,41027700,0,0,209325,41027700,null,null,"N","N","",1]
["CMF11212100S",null,null,null,"레일교환 / P.C.T / 인력","50kg, 3시간 차단, 시공구간 100M 이하","km",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,40288920,0,0,0,40288920,null,null,null,null,"",1]
["CMF11213200S","노무","L001010101000046",null,"궤도공","일반공사 직종","인",133,0,0,209325,27840225,0,0,209325,27840225,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CMF11222200S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",34,0,0,165545,5628530,0,0,165545,5628530,null,null,"N","N","",1]
["CMF11223200S",null,null,null,"레일교환 / P.C.T / 인력","60kg, 4시간 차단, 시공구간 100M 초과","km",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CMF11311100S","노무","L001010101000046",null,"궤도공","일반공사 직종","인",242,0,0,209325,50656650,0,0,209325,50656650,null,null,"N","N","",1]
["CMF11311200S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",58,0,0,165545,9601610,0,0,165545,9601610,null,null,"N","N","",1]
["CMF11312100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",44,0,0,165545,7283980,0,0,165545,7283980,null,null,"N","N","",1]
["CMF11313100S",null,null,null,"레일교환 / 교량 / 인력","50kg, 3시간 차단, 시공구간 100M 초과","km",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,43925430,0,0,0,43925430,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,55584700,0,0,0,55584700,null,null,null,null,"",1]
["CMF11322100S","노무","L001010101000046",null,"궤도공","일반공사 직종","인",188,0,0,209325,39353100,0,0,209325,39353100,null,null,"N","N","",1]
["CMF11322200S","노무","L001010101000046",null,"궤도공","일반공사 직종","인",206,0,0,209325,43120950,0,0,209325,43120950,null,null,"N","N","",1]
["CMF11323200S","노무","L001010101000046",null,"궤도공","일반공사 직종","인",167,0,0,209325,34957275,0,0,209325,34957275,null,null,"N","N","",1]
["CMF11411100S","노무","L001010101000046",null,"궤도공","일반공사 직종","인",255,0,0,209325,53377875,0,0,209325,53377875,null,null,"N","N","",1]
["CMF11411200S","노무","L001010101000046",null,"궤도공","일반공사 직종","인",261,0,0,209325,54633825,0,0,209325,54633825,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CMF11413100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",38,0,0,165545,6290710,0,0,165545,6290710,null,null,"N","N","",1]
["CMF11413200S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",39,0,0,165545,6456255,0,0,165545,6456255,null,null,"N","N","",1]
["CMF11421200S",null,null,null,"레일교환 / 터널 / 인력","60kg, 4시간 차단, 시공구간 30M 이하","km",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CMF11422200S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",44,0,0,165545,7283980,0,0,165545,7283980,null,null,"N","N","",1]
["CMF11423100S","노무","L001010101000046",null,"궤도공","일반공사 직종","인",161,0,0,209325,33701325,0,0,209325,33701325,null,null,"N","N","",1]
["CMF11423200S",null,null,null,"레일교환 / 터널 / 인력","60kg, 4시간 차단, 시공구간 100M 초과","km",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CMF12121100S",null,null,null,"레일교환 / 목침목 / 기계","4시간 차단","km",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CMF12121100S","노무","L001010101000046",null,"궤도공","일반공사 직종","인",78,0,0,209325,16327350,0,0,209325,16327350,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CMF12311100S",null,null,null,"레일교환 / 교량 / 기계","3시간 차단","km",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CMF12311100S","노무","L001010101000046",null,"궤도공","일반공사 직종","인",106,0,0,209325,22188450,0,0,209325,22188450,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CMF12411100S","기계경비","00007206002000000",null,"부착용 집게","0.2㎥","HR",114,0,0,0,0,3484,397176,3484,397176,null,null,"N","N","",1]
["CMF12421100S",null,null,null,"레일교환 / 터널 / 기계","4시간 차단","km",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CMF21121000S",null,null,null,"분기기 교환 / 인력","#8 분기기, 4시간 차단","틀",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,11937005,0,0,0,11937005,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,11352810,0,0,0,11352810,null,null,null,null,"",1]
["CMF21321000S","노무","L001010101000046",null,"궤도공","일반공사 직종","인",45,0,0,209325,9419625,0,0,209325,9419625,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,253935,0,7392740,0,545325,0,8192000,null,null,null,null,"",1]
["CMF22211000S",null,null,null,"분기기 교환 / 기계","#10 분기기, 3시간 차단","틀",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,300105,0,8729785,0,644475,0,9674365,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CMF22311000S","기계경비","00007206002000000",null,"부착용 집게","0.2㎥","HR",59,0,0,0,0,3484,205556,3484,205556,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,430920,0,9886010,0,925400,0,11242330,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CMF22421000S","노무","L001010101000046",null,"궤도공","일반공사 직종","인",35,0,0,209325,7326375,0,0,209325,7326375,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CMF31122000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.1999999999999998E-2,0,0,165545,8608.2999999999993,0,0,165545,8608.2999999999993,null,null,"N","N","",1]
["CMF31212000S",null,null,null,"침목교환 / 목침목-PCT / 인력","3시간 차단 / B-Type","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CMF31221000S",null,null,null,"침목교환 / 목침목-PCT / 인력","4시간 차단 / A-Type","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,123277,0,0,0,123277,null,null,null,null,"",1]
["CMF31312000S","노무","L001010101000046",null,"궤도공","일반공사 직종","인",0.57099999999999995,0,0,209325,119524.5,0,0,209325,119524.5,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,144415,0,0,0,144415,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,258545,0,0,0,258545,null,null,null,null,"",1]
["CMF31421000S","노무","L001010101000046",null,"궤도공","일반공사 직종","인",0.98799999999999999,0,0,209325,206813.1,0,0,209325,206813.1,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CMF32211000S","기계경비","00007206002000000",null,"부착용 집게","0.2㎥","HR",6.5000000000000002E-2,0,0,0,0,3484,226.4,3484,226.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,407,0,22468,0,875,0,23750,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CMF32321000S","기계경비","00000201002000000",null,"굴삭기(무한궤도)","0.2㎥","HR",8.5999999999999993E-2,7695,661.7,55700,4790.2,13041,1121.5,76436,6573.4,null,null,"N","N","",1]
["CMF32411000S","기계경비","00007206002000000",null,"부착용 집게","0.2㎥","HR",0.214,0,0,0,0,3484,745.5,3484,745.5,null,null,"N","N","",1]
["CMF32421000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.3999999999999999E-2,0,0,165545,8939.4,0,0,165545,8939.4,null,null,"N","N","",1]
["CMF40111000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.2,0,0,165545,33109,0,0,165545,33109,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,65792,0,0,0,65792,null,null,null,null,"",1]
["CMF40121000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.05,0,0,214222,10711.1,0,0,214222,10711.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,37880,0,0,0,37880,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CMF40142000S",null,null,null,"도상 갱환 / 타설 후 정리 작업","곡선구간 (R=950미만)","M",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CMF40232000S","노무","L001010101000046",null,"궤도공","일반공사 직종","인",0.09,0,0,209325,18839.2,0,0,209325,18839.2,null,null,"N","N","",1]
["CMF42011000S",null,null,null,"도상자갈 철거 / 기계","3시간 차단","M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CMF42011000S","노무","L001010101000046",null,"궤도공","일반공사 직종","인",0.04,0,0,209325,8373,0,0,209325,8373,null,null,"N","N","",1]
["CMF42021000S","기계경비","00000201002000000",null,"굴삭기(무한궤도)","0.2㎥","HR",0.11,7695,846.4,55700,6127,13041,1434.5,76436,8407.9,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CMG41000015S",null,null,null,"자갈채집 및 운반 (궤도)","L=150m","M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CMG41000025S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.46,0,0,165545,76150.7,0,0,165545,76150.7,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CMG41000035S",null,null,null,"자갈채집 및 운반 (궤도)","L=350m","M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CMR11000000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.0000000000000001E-3,0,0,165545,993.2,0,0,165545,993.2,null,null,"N","N","",1]
["CMR12000000S","기계경비","00007952024600000",null,"침목천공기","2.46kw","HR",0.09,0,0,0,0,304,27.3,304,27.3,null,null,"N","N","",1]
["CMR13000037S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.4E-2,0,0,165545,3973,0,0,165545,3973,null,null,"N","N","",1]
["CMR13000050S","손료","RENT000000000001",null,"잡재료","노무비의 5%","식",1,468.5,468.5,0,0,0,0,468.5,468.5,null,null,"N","N",5,1]
["CMR13000060S","기계경비","00007620000300000",null,"절단기","40.64cm","HR",0.215,0,0,0,0,1168,251.1,1168,251.1,null,null,"N","N","",1]
["CMR41000000S","노무","L001010101000046",null,"궤도공","일반공사 직종","인",30,0,0,209325,6279750,0,0,209325,6279750,null,null,"N","N","",1]
["CMR41100000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.01,0,0,165545,1655.4,0,0,165545,1655.4,null,null,"N","N","",1]
["CMR41200000S","손료","RENT000000000001",null,"잡재료","노무비의 5%","식",1,187.4,187.4,0,0,0,0,187.4,187.4,null,null,"N","N",5,1]
["CMR42000000S","노무","L001010101000046",null,"궤도공","일반공사 직종","인",1.4E-2,0,0,209325,2930.5,0,0,209325,2930.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,9503,0,0,0,9503,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,20075,0,0,0,20075,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CMR46000000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.1999999999999999E-2,0,0,165545,3641.9,0,0,165545,3641.9,null,null,"N","N","",1]
["CNE13220000S","노무","L001010101000013",null,"콘크리트공","일반공사 직종","인",2,0,0,261283,522566,0,0,261283,522566,null,null,"N","N","",1]
["CNI10010000S","노무","L001010101000026",null,"방수공","일반공사 직종","인",1.0999999999999999E-2,0,0,212562,2338.1,0,0,212562,2338.1,null,null,"N","N","",1]
["COA61100250S","기계경비","00002105001000000",null,"트럭탑재형 크레인","10ton","HR",0.22,15721,3458.6,47231,10390.799999999999,21743,4783.3999999999996,84695,18632.8,null,null,"N","N","",1]
["COA61100300S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.02,0,0,165545,3310.9,0,0,165545,3310.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,3930,0,24845,0,5435,0,34210,null,null,null,null,"",1]
["COA61100400S","기계경비","00002105001000000",null,"트럭탑재형 크레인","10ton","HR",0.27,15721,4244.6000000000004,47231,12752.3,21743,5870.6,84695,22867.5,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["COA61100610S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.08,0,0,243168,19453.400000000001,0,0,243168,19453.400000000001,null,null,"N","N","",1]
["COA61100630S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.09,0,0,243168,21885.1,0,0,243168,21885.1,null,null,"N","N","",1]
["COA61100660S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.09,0,0,243168,21885.1,0,0,243168,21885.1,null,null,"N","N","",1]
["COA61100685S",null,null,null,"배송관 접합 (플랜지)","Ø685mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["COA61100710S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.05,0,0,165545,8277.2000000000007,0,0,165545,8277.2000000000007,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,7219,0,55334,0,12094,0,74647,null,null,null,null,"",1]
["COA61100840S","기계경비","00002105001500000",null,"트럭탑재형 크레인","15ton","HR",0.47,16790,7891.3,47231,22198.5,28126,13219.2,92147,43309,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["COA61200300S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.03,0,0,243168,7295,0,0,243168,7295,null,null,"N","N","",1]
["COA61200350S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.02,0,0,165545,3310.9,0,0,165545,3310.9,null,null,"N","N","",1]
["COA61200400S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.04,0,0,243168,9726.7000000000007,0,0,243168,9726.7000000000007,null,null,"N","N","",1]
["COA61200510S",null,null,null,"배송관 접합 (고무슬리브)","Ø510mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["COA61200560S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.04,0,0,165545,6621.8,0,0,165545,6621.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,4716,0,40244,0,6522,0,51482,null,null,null,null,"",1]
["COA61200630S","기계경비","00002105001000000",null,"트럭탑재형 크레인","10ton","HR",0.31,15721,4873.5,47231,14641.6,21743,6740.3,84695,26255.4,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["COA61200760S","기계경비","00002105001500000",null,"트럭탑재형 크레인","15ton","HR",0.34,16790,5708.6,47231,16058.5,28126,9562.7999999999993,92147,31329.9,null,null,"N","N","",1]
["COA61200840S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.12,0,0,243168,29180.1,0,0,243168,29180.1,null,null,"N","N","",1]
["COA62100250S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.03,0,0,243168,7295,0,0,243168,7295,null,null,"N","Y","",0]
["COA62100250S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.02,0,0,165545,3310.9,0,0,165545,3310.9,null,null,"N","Y","",0]
["COA62100300S","기계경비","00002105001000000",null,"트럭탑재형 크레인","10ton","HR",0.24,15721,3773,47231,11335.4,21743,5218.3,84695,20326.7,null,null,"N","Y","",0]
["COA62100400S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.04,0,0,243168,9726.7000000000007,0,0,243168,9726.7000000000007,null,null,"N","Y","",0]
["COA62100400S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.03,0,0,165545,4966.3,0,0,165545,4966.3,null,null,"N","Y","",0]
["COA62100560S",null,null,null,"배송관 철거 (플랜지)","Ø560mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,3961,0,28452,0,5479,0,37892,null,null,null,null,"",1]
["COA62100610S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.08,0,0,243168,19453.400000000001,0,0,243168,19453.400000000001,null,null,"N","Y","",0]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["COA62100685S",null,null,null,"배송관 철거 (플랜지)","Ø685mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["COA62100685S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.1,0,0,243168,24316.799999999999,0,0,243168,24316.799999999999,null,null,"N","Y","",0]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["COA62100840S",null,null,null,"배송관 철거 (플랜지)","Ø840mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["COA62100840S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.12,0,0,243168,29180.1,0,0,243168,29180.1,null,null,"N","Y","",0]
[null,null,null,null,"[합 계]",null,null,0,0,5641,0,43248,0,9450,0,58339,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["COA62200300S","손료","RENT000000000001",null,"철거","합계의 70%","식",1,2090.8000000000002,2090.8000000000002,13705.7,13705.7,2891.7,2891.7,18688.2,18688.2,null,null,"N","N",70,1]
[null,null,null,null,"[합 계]",null,null,0,0,2200,0,15738,0,3044,0,20982,null,null,null,null,"",1]
["COA62200400S","기계경비","00002105001000000",null,"트럭탑재형 크레인","10ton","HR",0.22,15721,3458.6,47231,10390.799999999999,21743,4783.3999999999996,84695,18632.8,null,null,"N","Y","",0]
["COA62200510S","손료","RENT000000000001",null,"철거","합계의 70%","식",1,2861.1,2861.1,23444.2,23444.2,3957.1,3957.1,30262.400000000001,30262.400000000001,null,null,"N","N",70,1]
[null,null,null,null,"[합 계]",null,null,0,0,3191,0,26138,0,4413,0,33742,null,null,null,null,"",1]
["COA62200610S",null,null,null,"배송관 철거 (고무슬리브)","Ø610mm","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["COA62200630S","기계경비","00002105001000000",null,"트럭탑재형 크레인","10ton","HR",0.31,15721,4873.5,47231,14641.6,21743,6740.3,84695,26255.4,null,null,"N","Y","",0]
["COA62200660S","손료","RENT000000000001",null,"철거","합계의 70%","식",1,3521.4,3521.4,31693.3,31693.3,4870.3,4870.3,40085,40085,null,null,"N","N",70,1]
["COA62200685S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.05,0,0,165545,8277.2000000000007,0,0,165545,8277.2000000000007,null,null,"N","Y","",0]
["COA62200710S","기계경비","00002105001000000",null,"트럭탑재형 크레인","10ton","HR",0.34,15721,5345.1,47231,16058.5,21743,7392.6,84695,28796.2,null,null,"N","Y","",0]
["COA62200760S","노무","L001010101000040",null,"배관공(수도)","일반공사 직종","인",0.11,0,0,243168,26748.400000000001,0,0,243168,26748.400000000001,null,null,"N","Y","",0]
["COA62200840S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.06,0,0,165545,9932.7000000000007,0,0,165545,9932.7000000000007,null,null,"N","Y","",0]
["COA62200860S","기계경비","00002105001500000",null,"트럭탑재형 크레인","15ton","HR",0.38,16790,6380.2,47231,17947.7,28126,10687.8,92147,35015.699999999997,null,null,"N","Y","",0]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["COA71000500S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.01,0,0,165545,1655.4,0,0,165545,1655.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,786,0,10443,0,1087,0,12316,null,null,null,null,"",1]
["COA71000700S","기계경비","00002105001000000",null,"트럭탑재형 크레인","10ton","HR",0.05,15721,786,47231,2361.5,21743,1087.0999999999999,84695,4234.6000000000004,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,943,0,12571,0,1304,0,14818,null,null,null,null,"",1]
["COA71001200S",null,null,null,"배송관 띄우개(부함) 접합","Ø1200*4.5m, 610~630mm","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["COA71001300S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.02,0,0,165545,3310.9,0,0,165545,3310.9,null,null,"N","N","",1]
["COA71001400S",null,null,null,"배송관 띄우개(부함) 접합","Ø1400*5.0m, 685~710mm","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["COA71001500S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.02,0,0,165545,3310.9,0,0,165545,3310.9,null,null,"N","N","",1]
["COA71001600S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.04,0,0,214222,8568.7999999999993,0,0,214222,8568.7999999999993,null,null,"N","N","",1]
["COA72000430S","기계경비","00002105001000000",null,"트럭탑재형 크레인","10ton","HR",0.05,15721,786,47231,2361.5,21743,1087.0999999999999,84695,4234.6000000000004,null,null,"N","Y","",0]
["COA72000500S","손료","RENT000000000001",null,"철거","합계의 70%","식",1,550.20000000000005,550.20000000000005,5810.9,5810.9,760.9,760.9,7122,7122,null,null,"N","N",70,1]
["COA72000600S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.01,0,0,165545,1655.4,0,0,165545,1655.4,null,null,"N","Y","",0]
["COA72000700S","기계경비","00002105001000000",null,"트럭탑재형 크레인","10ton","HR",0.05,15721,786,47231,2361.5,21743,1087.0999999999999,84695,4234.6000000000004,null,null,"N","Y","",0]
["COA72000900S","손료","RENT000000000001",null,"철거","합계의 70%","식",1,660.2,660.2,7641,7641,913.1,913.1,9214.2999999999993,9214.2999999999993,null,null,"N","N",70,1]
["COA72001000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.02,0,0,165545,3310.9,0,0,165545,3310.9,null,null,"N","Y","",0]
["COA72001100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.02,0,0,165545,3310.9,0,0,165545,3310.9,null,null,"N","Y","",0]
["COA72001300S",null,null,null,"배송관 띄우개(부함) 철거","Ø1300*5.0m, 660mm","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["COA72001300S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.03,0,0,214222,6426.6,0,0,214222,6426.6,null,null,"N","Y","",0]
["COA72001400S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.02,0,0,165545,3310.9,0,0,165545,3310.9,null,null,"N","Y","",0]
["COA72001600S",null,null,null,"배송관 띄우개(부함) 철거","Ø1600*5.0m, 840~860mm","본",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["COA72001600S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.04,0,0,214222,8568.7999999999993,0,0,214222,8568.7999999999993,null,null,"N","Y","",0]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,1257,0,7089,0,1739,0,10085,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["COA80000510S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.03,0,0,165545,4966.3,0,0,165545,4966.3,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["COA80000610S",null,null,null,"배송관 진수","Ø610mm","SET당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["COA80000660S","기계경비","00002105001000000",null,"트럭탑재형 크레인","10ton","HR",0.2,15721,3144.2,47231,9446.2000000000007,21743,4348.6000000000004,84695,16939,null,null,"N","N","",1]
["COA80000710S",null,null,null,"배송관 진수","Ø710mm","SET당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["COA80000840S","기계경비","00002105001500000",null,"트럭탑재형 크레인","15ton","HR",0.25,16790,4197.5,47231,11807.7,28126,7031.5,92147,23036.7,null,null,"N","N","",1]
["COB12010000S",null,null,null,"사석 / 육상투하","0.03m3이하 덤프트럭+굴삭기 투하","M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["COB12020000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",1.2999999999999999E-2,0,0,214222,2784.8,0,0,214222,2784.8,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["COB15000000S","기계경비","00000201010000000",null,"굴삭기(무한궤도)","1.0㎥","HR",2.7E-2,30260,817,55700,1503.9,27901,753.3,113861,3074.2,null,null,"N","N","",1]
["COC10000000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.2000000000000003E-2,0,0,165545,6952.8,0,0,165545,6952.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,1354,0,31032,0,2061,0,34447,null,null,null,null,"",1]
["COC30100000S","기계경비","00002101001000000",null,"크레인(무한궤도)","10ton(0.29㎥)","HR",0.13600000000000001,8853,1204,55700,7575.2,13475,1832.6,78028,10611.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,4115,0,27776,0,3794,0,35685,null,null,null,null,"",1]
["COC70000000S",null,null,null,"사석 / 수상고르기","필타사석 고르기","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["COD10110000S",null,null,null,"케이슨 진수","500ton 미만","개당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,1197815,0,0,0,1197815,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,1726604,0,0,0,1726604,null,null,null,null,"",1]
["COD10210000S","노무","L001010101000006",null,"비계공","일반공사 직종","인",1.5,0,0,280472,420708,0,0,280472,420708,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["COD10240000S",null,null,null,"케이슨 거치","2000∼3000ton (잠수조제외)","개당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["COD31110000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",5.8999999999999997E-2,0,0,214222,12639,0,0,214222,12639,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["COD31150000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.07,0,0,165545,177133.1,0,0,165545,177133.1,null,null,"N","N","",1]
["COD31160000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.25,0,0,165545,206931.20000000001,0,0,165545,206931.20000000001,null,null,"N","N","",1]
["COD31211000S",null,null,null,"소파블럭 거치 / 수상 / 난적","2ton 미만","개당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,33955,0,0,0,33955,null,null,null,null,"",1]
["COD31230000S",null,null,null,"소파블럭 거치 / 수상 / 층적","5∼10ton ","개당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["COD31231000S",null,null,null,"소파블럭 거치 / 수상 / 난적","5∼10ton ","개당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,50636,0,0,0,50636,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,43196,0,0,0,43196,null,null,null,null,"",1]
["COD31251000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",6.9000000000000006E-2,0,0,214222,14781.3,0,0,214222,14781.3,null,null,"N","N","",1]
["COD31260000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.182,0,0,214222,38988.400000000001,0,0,214222,38988.400000000001,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["COD31271000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.33300000000000002,0,0,165545,55126.400000000001,0,0,165545,55126.400000000001,null,null,"N","N","",1]
["COD32110000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.23300000000000001,0,0,165545,38571.9,0,0,165545,38571.9,null,null,"N","N","",1]
["COD32130000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.47599999999999998,0,0,165545,78799.399999999994,0,0,165545,78799.399999999994,null,null,"N","N","",1]
["COD32160000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1,0,0,165545,165545,0,0,165545,165545,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,165545,0,0,0,165545,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,21851,0,0,0,21851,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,41386,0,0,0,41386,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["COD32241000S",null,null,null,"소파블럭 거치 / 수중 / 난적","10∼15ton (잠수조제외)","개당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,48339,0,0,0,48339,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["COH13000040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.0000000000000001E-3,0,0,165545,827.7,0,0,165545,827.7,null,null,"N","N","",1]
["COH13000040S","기계경비","00000201010000000",null,"굴삭기(무한궤도)","1.0㎥","HR",2.5999999999999999E-2,30260,786.7,55700,1448.2,27901,725.4,113861,2960.3,null,null,"N","N","",1]
["COH13000050S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",1.6E-2,0,0,214222,3427.5,0,0,214222,3427.5,null,null,"N","N","",1]
["COH13000060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",8.0000000000000002E-3,0,0,165545,1324.3,0,0,165545,1324.3,null,null,"N","N","",1]
["COH13000060S","기계경비","00000201010000000",null,"굴삭기(무한궤도)","1.0㎥","HR",0.04,30260,1210.4000000000001,55700,2228,27901,1116,113861,4554.3999999999996,null,null,"N","N","",1]
["COH18000000S","노무","L001010101000033",null,"석공","일반공사 직종","인",2.7E-2,0,0,258935,6991.2,0,0,258935,6991.2,null,null,"N","N","",1]
["COH20000000S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.13400000000000001,0,0,214222,28705.7,0,0,214222,28705.7,null,null,"N","N","",1]
["COH60010000S",null,null,null,"블록 붙이기(인력) / 호안블록",null,"M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["COH60021000S","기계경비","00002101001000000",null,"크레인(무한궤도)","10ton(0.29㎥)","HR",4.8000000000000001E-2,8853,424.9,55700,2673.6,13475,646.79999999999995,78028,3745.3,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CQH00000000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.0000000000000001E-3,0,0,165545,496.6,0,0,165545,496.6,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,85,0,4258,0,0,0,4343,null,null,null,null,"",1]
["CRB11000055S","노무","L001010101000033",null,"석공","일반공사 직종","인",0.09,0,0,258935,23304.1,0,0,258935,23304.1,null,null,"N","N","",1]
["CRB11000075S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.03,0,0,165545,4966.3,0,0,165545,4966.3,null,null,"N","N","",1]
["CRB21000035S",null,null,null,"돌쌓기 / 찰쌓기","뒷길이 35cm","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CRB21000055S","노무","L001010101000033",null,"석공","일반공사 직종","인",0.08,0,0,258935,20714.8,0,0,258935,20714.8,null,null,"N","N","",1]
["CRB21000075S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.03,0,0,165545,4966.3,0,0,165545,4966.3,null,null,"N","N","",1]
["CRB31000000S",null,null,null,"전석쌓기","전석(0.3m3~0.5m2급)","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CRB41000035S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.04,0,0,165545,6621.8,0,0,165545,6621.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,3957,0,54208,0,6860,0,65025,null,null,null,null,"",1]
["CRB41000075S",null,null,null,"돌붙임 / 메붙임","뒷길이 75cm","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CRB51000035S","노무","L001010101000033",null,"석공","일반공사 직종","인",0.11,0,0,258935,28482.799999999999,0,0,258935,28482.799999999999,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CRB51000075S",null,null,null,"돌붙임 / 찰붙임","뒷길이 75cm","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,3165,0,37755,0,5488,0,46408,null,null,null,null,"",1]
["CRB71120000S",null,null,null,"석재판붙임 / 습식공법 / 테라조판","계단부","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CRB71210000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.14000000000000001,0,0,165545,23176.3,0,0,165545,23176.3,null,null,"N","N","",1]
["CRB71220000S",null,null,null,"석재판붙임 / 습식공법 / 화강석","계단부","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CRB72010000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.15,0,0,165545,24831.7,0,0,165545,24831.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,3563,0,118769,0,0,0,122332,null,null,null,null,"",1]
["CRB73110000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,2093,2093,0,0,0,0,2093,2093,null,null,"N","N",3,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,1862,0,62088,0,0,0,63950,null,null,null,null,"",1]
["CRB91000000S",null,null,null,"전석깔기","전석(0.3m3~0.5m2급)","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CRC20000000S",null,null,null,"기초지정","자갈지정","M3",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CRC30000000S","기계경비","00000201002000000",null,"굴삭기(무한궤도)","0.2㎥","HR",7.0000000000000007E-2,7695,538.6,55700,3899,13041,912.8,76436,5350.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,26822,0,0,0,26822,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSA11000004S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.0999999999999999E-2,0,0,165545,1820.9,0,0,165545,1820.9,null,null,"N","N","",1]
["CSA11000006S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5000000000000001E-2,0,0,165545,4138.6000000000004,0,0,165545,4138.6000000000004,null,null,"N","N","",1]
["CSA11000006S","기계경비","00000201004000000",null,"굴삭기(무한궤도)","0.4㎥","HR",0.2,15363,3072.6,55700,11140,16378,3275.6,87441,17488.2,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSA12000101S","노무","L001010101000038",null,"조경공","일반공사 직종","인",4.2999999999999997E-2,0,0,219533,9439.9,0,0,219533,9439.9,null,null,"N","N","",1]
["CSA12000101S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.4E-2,0,0,165545,2317.6,0,0,165545,2317.6,null,null,"N","N","",1]
["CSA12000103S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.04,0,0,165545,6621.8,0,0,165545,6621.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,8188,0,84686,0,8729,0,101603,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,35965,0,234916,0,49817,0,320698,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,65604,0,428835,0,174820,0,669259,null,null,null,null,"",1]
["CSA12000109S","기계경비","00002104004000000",null,"크레인(타이어)","40ton","HR",2.67,16974,45320.5,55700,148719,65453,174759.5,138127,368799,null,null,"N","N","",1]
["CSA21000002S",null,null,null,"교목 식재 / 나무높이 / 인력시공","3.0m 이하","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSA21000003S",null,null,null,"교목 식재 / 나무높이 / 인력시공","5.0m 이하","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSA21000011S","기계경비","00000201004000000",null,"굴삭기(무한궤도)","0.4㎥","HR",0.14499999999999999,15363,2227.6,55700,8076.5,16378,2374.8000000000002,87441,12678.9,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,6145,0,63487,0,6551,0,76183,null,null,null,null,"",1]
["CSA22000002S","노무","L001010101000038",null,"조경공","일반공사 직종","인",0.26700000000000002,0,0,219533,58615.3,0,0,219533,58615.3,null,null,"N","N","",1]
["CSA22000101S","노무","L001010101000038",null,"조경공","일반공사 직종","인",6.7000000000000004E-2,0,0,219533,14708.7,0,0,219533,14708.7,null,null,"N","N","",1]
["CSA22000102S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.4999999999999998E-2,0,0,165545,7449.5,0,0,165545,7449.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,7235,0,74639,0,7714,0,89588,null,null,null,null,"",1]
["CSA22000104S","기계경비","00000201004000000",null,"굴삭기(무한궤도)","0.4㎥","HR",0.66700000000000004,15363,10247.1,55700,37151.9,16378,10924.1,87441,58323.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,28078,0,182264,0,38892,0,249234,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSA22000107S","기계경비","00002104004000000",null,"크레인(타이어)","40ton","HR",1.6,16974,27158.400000000001,55700,89120,65453,104724.8,138127,221003.2,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,65604,0,428835,0,174820,0,669259,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSA40000007S",null,null,null,"교목 뿌리돌림","근원직경 7cm","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,40631,0,0,0,40631,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,55458,0,0,0,55458,null,null,null,null,"",1]
["CSA40000015S","노무","L001010101000038",null,"조경공","일반공사 직종","인",0.37,0,0,219533,81227.199999999997,0,0,219533,81227.199999999997,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSA40000030S","노무","L001010101000038",null,"조경공","일반공사 직종","인",1.58,0,0,219533,346862.1,0,0,219533,346862.1,null,null,"N","N","",1]
["CSA40000036S","노무","L001010101000038",null,"조경공","일반공사 직종","인",1.86,0,0,219533,408331.3,0,0,219533,408331.3,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSA40000054S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.33,0,0,165545,54629.8,0,0,165545,54629.8,null,null,"N","N","",1]
["CSA40000060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.36,0,0,165545,59596.2,0,0,165545,59596.2,null,null,"N","N","",1]
["CSA40000072S",null,null,null,"교목 뿌리돌림","근원직경 72cm","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSA40000078S",null,null,null,"교목 뿌리돌림","근원직경 78cm","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,1558284,0,0,0,1558284,null,null,null,null,"",1]
["CSA40000100S","노무","L001010101000038",null,"조경공","일반공사 직종","인",7.9,0,0,219533,1734310.7,0,0,219533,1734310.7,null,null,"N","N","",1]
["CSB10000001S",null,null,null,"관목 굴취 / 나무높이","0.3m 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,3565,0,0,0,3565,null,null,null,null,"",1]
["CSB10000004S","노무","L001010101000038",null,"조경공","일반공사 직종","인",0.03,0,0,219533,6585.9,0,0,219533,6585.9,null,null,"N","N","",1]
["CSB21000001S","노무","L001010101000038",null,"조경공","일반공사 직종","인",1.8800000000000001E-2,0,0,219533,4127.2,0,0,219533,4127.2,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSB22000001S","노무","L001010101000038",null,"조경공","일반공사 직종","인",6.7999999999999996E-3,0,0,219533,1492.8,0,0,219533,1492.8,null,null,"N","N","",1]
["CSB22000001S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.3E-3,0,0,165545,380.7,0,0,165545,380.7,null,null,"N","N","",1]
["CSB22000003S","노무","L001010101000038",null,"조경공","일반공사 직종","인",1.4999999999999999E-2,0,0,219533,3292.9,0,0,219533,3292.9,null,null,"N","N","",1]
["CSD20000001S","노무","L001010101000038",null,"조경공","일반공사 직종","인",1.1100000000000001E-3,0,0,219533,243.6,0,0,219533,243.6,null,null,"N","N","",1]
["CSD20000001S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.6999999999999999E-4,0,0,165545,61.2,0,0,165545,61.2,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSE52000000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.6700000000000002E-2,0,0,165545,4420,0,0,165545,4420,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,5890,0,0,0,5890,null,null,null,null,"",1]
["CSF60000000S","기계경비","00007730005000000",null,"건설용펌프(자흡식)","50mm(1.49kw*10m)","HR",2.5799999999999998E-3,0,0,0,0,67,0.1,67,0.1,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH10100002S","손료","RENT000000000001",null,"공구손료","인력품의 3%","식",1,0,0,0,0,6849.4,6849.4,6849.4,6849.4,null,null,"N","N",3,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH10300000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",7.6999999999999999E-2,0,0,219533,16904,0,0,219533,16904,null,null,"N","N","",1]
["CSH10400000S",null,null,null,"잔디블록 포장",null,"M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH10500001S","노무","L001010101000038",null,"조경공","일반공사 직종","인",2.1999999999999999E-2,0,0,219533,4829.7,0,0,219533,4829.7,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,507,0,16929,0,0,0,17436,null,null,null,null,"",1]
["CSH21113000S",null,null,null,"일반전정 / 인력시공 / 낙엽수","흉고직경 21~31cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,1396,0,46554,0,0,0,47950,null,null,null,null,"",1]
["CSH21122000S",null,null,null,"일반전정 / 인력시공 / 상록수","흉고직경 11~21cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH21123000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.7000000000000004E-2,0,0,165545,11091.5,0,0,165545,11091.5,null,null,"N","N","",1]
["CSH21212000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",4.2000000000000003E-2,0,0,219533,9220.2999999999993,0,0,219533,9220.2999999999993,null,null,"N","N","",1]
["CSH21213000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.2000000000000001E-2,0,0,165545,5297.4,0,0,165545,5297.4,null,null,"N","N","",1]
["CSH21214000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,1009.1,1009.1,0,0,0,0,1009.1,1009.1,null,null,"N","N",3,1]
["CSH21215000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",0.154,0,0,219533,33808,0,0,219533,33808,null,null,"N","N","",1]
["CSH21216000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,2292.1,2292.1,0,0,0,0,2292.1,2292.1,null,null,"N","N",3,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH21222000S",null,null,null,"일반전정 / 기계시공 / 상록수","흉고직경 11~21cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH21223000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",5.7000000000000002E-2,0,0,219533,12513.3,0,0,219533,12513.3,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH21225000S",null,null,null,"일반전정 / 기계시공 / 상록수","흉고직경 41~51cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH21226000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",0.2,0,0,219533,43906.6,0,0,219533,43906.6,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH22111000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.2999999999999997E-2,0,0,165545,7118.4,0,0,165545,7118.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,524,0,26217,0,0,0,26741,null,null,null,null,"",1]
["CSH22113000S",null,null,null,"조형전정 / 인력시공 / 낙엽수","흉고직경 21~31cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH22121000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.6999999999999998E-2,0,0,165545,6125.1,0,0,165545,6125.1,null,null,"N","N","",1]
["CSH22122000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",0.125,0,0,219533,27441.599999999999,0,0,219533,27441.599999999999,null,null,"N","N","",1]
["CSH22123000S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,1209.2,1209.2,0,0,0,0,1209.2,1209.2,null,null,"N","N",2,1]
["CSH22212000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.2000000000000001E-2,0,0,165545,5297.4,0,0,165545,5297.4,null,null,"N","N","",1]
["CSH22213000S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,604.6,604.6,0,0,0,0,604.6,604.6,null,null,"N","N",2,1]
["CSH22215000S",null,null,null,"조형전정 / 기계시공 / 낙엽수","흉고직경 41~51cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH22215000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",0.25,0,0,219533,54883.199999999997,0,0,219533,54883.199999999997,null,null,"N","N","",1]
["CSH22216000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.2,0,0,165545,33109,0,0,165545,33109,null,null,"N","N","",1]
["CSH22217000S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,3023,3023,0,0,0,0,3023,3023,null,null,"N","N",2,1]
["CSH22222000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",5.6000000000000001E-2,0,0,219533,12293.8,0,0,219533,12293.8,null,null,"N","N","",1]
["CSH22223000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.2999999999999997E-2,0,0,165545,7118.4,0,0,165545,7118.4,null,null,"N","N","",1]
["CSH22225000S",null,null,null,"조형전정 / 기계시공 / 상록수","흉고직경 41~51cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH22225000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",0.2,0,0,219533,43906.6,0,0,219533,43906.6,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH23301000S",null,null,null,"가로수 전정 / 약전정","흉고직경 11cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH23302000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",9.5000000000000001E-2,0,0,219533,20855.599999999999,0,0,219533,20855.599999999999,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH23304000S",null,null,null,"가로수 전정 / 약전정","흉고직경 31∼41cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,6095,0,114800,0,12997,0,133892,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,8743,0,165515,0,18521,0,192779,null,null,null,null,"",1]
["CSH23401000S","기계경비","00002106000300000",null,"고소작업차","3ton","HR",0.42099999999999999,4731,1991.7,47231,19884.2,16247,6839.9,68209,28715.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,4353,0,82035,0,9277,0,95665,null,null,null,null,"",1]
["CSH23403000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,2310.4,2310.4,0,0,0,0,2310.4,2310.4,null,null,"N","N",3,1]
["CSH23404000S","기계경비","00002106000300000",null,"고소작업차","3ton","HR",1,4731,4731,47231,47231,16247,16247,68209,68209,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,8743,0,165515,0,18521,0,192779,null,null,null,null,"",1]
["CSH23406000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,3812.2,3812.2,0,0,0,0,3812.2,3812.2,null,null,"N","N",3,1]
["CSH23407000S","기계경비","00002106000300000",null,"고소작업차","3ton","HR",1.6,4731,7569.6,47231,75569.600000000006,16247,25995.200000000001,68209,109134.39999999999,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH23501000S",null,null,null,"가로수 전정 / 조형전정","흉고직경 11cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH23501000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",0.11799999999999999,0,0,219533,25904.799999999999,0,0,219533,25904.799999999999,null,null,"N","N","",1]
["CSH23501000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.11799999999999999,0,0,165545,19534.3,0,0,165545,19534.3,null,null,"N","N","",1]
["CSH23501000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,1363.1,1363.1,0,0,0,0,1363.1,1363.1,null,null,"N","N",3,1]
["CSH23501000S","기계경비","00002106000300000",null,"고소작업차","3ton","HR",0.47099999999999997,4731,2228.3000000000002,47231,22245.8,16247,7652.3,68209,32126.400000000001,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,3591,0,67684,0,7652,0,78927,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH23502000S",null,null,null,"가로수 전정 / 조형전정","흉고직경 11∼21cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH23502000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",0.16700000000000001,0,0,219533,36662,0,0,219533,36662,null,null,"N","N","",1]
["CSH23502000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.16700000000000001,0,0,165545,27646,0,0,165545,27646,null,null,"N","N","",1]
["CSH23502000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,1929.2,1929.2,0,0,0,0,1929.2,1929.2,null,null,"N","N",3,1]
["CSH23502000S","기계경비","00002106000300000",null,"고소작업차","3ton","HR",0.66700000000000004,4731,3155.5,47231,31503,16247,10836.7,68209,45495.199999999997,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,5084,0,95811,0,10836,0,111731,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH23503000S",null,null,null,"가로수 전정 / 조형전정","흉고직경 21∼31cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH23503000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",0.22,0,0,219533,48297.2,0,0,219533,48297.2,null,null,"N","N","",1]
["CSH23503000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.22,0,0,165545,36419.9,0,0,165545,36419.9,null,null,"N","N","",1]
["CSH23503000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,2541.5,2541.5,0,0,0,0,2541.5,2541.5,null,null,"N","N",3,1]
["CSH23503000S","기계경비","00002106000300000",null,"고소작업차","3ton","HR",0.89,4731,4210.5,47231,42035.5,16247,14459.8,68209,60705.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,6752,0,126752,0,14459,0,147963,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH23504000S",null,null,null,"가로수 전정 / 조형전정","흉고직경 31∼41cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH23504000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",0.28999999999999998,0,0,219533,63664.5,0,0,219533,63664.5,null,null,"N","N","",1]
["CSH23504000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.28999999999999998,0,0,165545,48008,0,0,165545,48008,null,null,"N","N","",1]
["CSH23504000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,3350.1,3350.1,0,0,0,0,3350.1,3350.1,null,null,"N","N",3,1]
["CSH23504000S","기계경비","00002106000300000",null,"고소작업차","3ton","HR",1.1399999999999999,4731,5393.3,47231,53843.3,16247,18521.5,68209,77758.100000000006,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,8743,0,165515,0,18521,0,192779,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH23505000S",null,null,null,"가로수 전정 / 조형전정","흉고직경 41∼51cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH23505000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",0.33,0,0,219533,72445.8,0,0,219533,72445.8,null,null,"N","N","",1]
["CSH23505000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.33,0,0,165545,54629.8,0,0,165545,54629.8,null,null,"N","N","",1]
["CSH23505000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,3812.2,3812.2,0,0,0,0,3812.2,3812.2,null,null,"N","N",3,1]
["CSH23505000S","기계경비","00002106000300000",null,"고소작업차","3ton","HR",1.33,4731,6292.2,47231,62817.2,16247,21608.5,68209,90717.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,10104,0,189892,0,21608,0,221604,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH23506000S",null,null,null,"가로수 전정 / 조형전정","흉고직경 51∼61cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH23506000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",0.5,0,0,219533,109766.5,0,0,219533,109766.5,null,null,"N","N","",1]
["CSH23506000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.5,0,0,165545,82772.5,0,0,165545,82772.5,null,null,"N","N","",1]
["CSH23506000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,5776.1,5776.1,0,0,0,0,5776.1,5776.1,null,null,"N","N",3,1]
["CSH23506000S","기계경비","00002106000300000",null,"고소작업차","3ton","HR",2,4731,9462,47231,94462,16247,32494,68209,136418,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,15238,0,287001,0,32494,0,334733,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH23507000S",null,null,null,"가로수 전정 / 조형전정","흉고직경 61cm 초과","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH23507000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",0.67,0,0,219533,147087.1,0,0,219533,147087.1,null,null,"N","N","",1]
["CSH23507000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.67,0,0,165545,110915.1,0,0,165545,110915.1,null,null,"N","N","",1]
["CSH23507000S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,7740,7740,0,0,0,0,7740,7740,null,null,"N","N",3,1]
["CSH23507000S","기계경비","00002106000300000",null,"고소작업차","3ton","HR",2.67,4731,12631.7,47231,126106.7,16247,43379.4,68209,182117.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,20371,0,384108,0,43379,0,447858,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH24600000S",null,null,null,"관목 전정","나무높이 0.9M 미만","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH24600000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",3.7000000000000002E-3,0,0,219533,812.2,0,0,219533,812.2,null,null,"N","N","",1]
["CSH24600000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.9E-3,0,0,165545,314.5,0,0,165545,314.5,null,null,"N","N","",1]
["CSH24600000S","손료","RENT000000000001",null,"공구손료","노무비의 3.5%","식",1,39.4,39.4,0,0,0,0,39.4,39.4,null,null,"N","N",3.5,1]
[null,null,null,null,"[합 계]",null,null,0,0,39,0,1126,0,0,0,1165,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH24700000S",null,null,null,"관목 전정","나무높이 0.9M 이상","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH24700000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",6.1000000000000004E-3,0,0,219533,1339.1,0,0,219533,1339.1,null,null,"N","N","",1]
["CSH24700000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.0000000000000001E-3,0,0,165545,496.6,0,0,165545,496.6,null,null,"N","N","",1]
["CSH24700000S","손료","RENT000000000001",null,"공구손료","노무비의 3.5%","식",1,64.2,64.2,0,0,0,0,64.2,64.2,null,null,"N","N",3.5,1]
[null,null,null,null,"[합 계]",null,null,0,0,64,0,1835,0,0,0,1899,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH25111000S",null,null,null,"수간보호 / 조형","흉고직경 11cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH25111000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",8.3000000000000004E-2,0,0,219533,18221.2,0,0,219533,18221.2,null,null,"N","N","",1]
["CSH25111000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.2000000000000003E-2,0,0,165545,6952.8,0,0,165545,6952.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,25174,0,0,0,25174,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH25112000S",null,null,null,"수간보호 / 조형","흉고직경 11~21cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH25112000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",0.154,0,0,219533,33808,0,0,219533,33808,null,null,"N","N","",1]
["CSH25112000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.6999999999999999E-2,0,0,165545,12746.9,0,0,165545,12746.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,46554,0,0,0,46554,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH25113000S",null,null,null,"수간보호 / 조형","흉고직경 21~31cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH25113000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",0.33,0,0,219533,72445.8,0,0,219533,72445.8,null,null,"N","N","",1]
["CSH25113000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.17,0,0,165545,28142.6,0,0,165545,28142.6,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,100588,0,0,0,100588,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH25114000S",null,null,null,"수간보호 / 조형","흉고직경 31~41cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH25114000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",0.67,0,0,219533,147087.1,0,0,219533,147087.1,null,null,"N","N","",1]
["CSH25114000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.33,0,0,165545,54629.8,0,0,165545,54629.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,201716,0,0,0,201716,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH25115000S",null,null,null,"수간보호 / 조형","흉고직경 41~51cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH25115000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",1,0,0,219533,219533,0,0,219533,219533,null,null,"N","N","",1]
["CSH25115000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.5,0,0,165545,82772.5,0,0,165545,82772.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,302305,0,0,0,302305,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH25121000S",null,null,null,"수간보호 / 일반","흉고직경 11cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH25121000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",5.2999999999999999E-2,0,0,219533,11635.2,0,0,219533,11635.2,null,null,"N","N","",1]
["CSH25121000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5999999999999999E-2,0,0,165545,4304.1000000000004,0,0,165545,4304.1000000000004,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,15939,0,0,0,15939,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH25122000S",null,null,null,"수간보호 / 일반","흉고직경 11~21cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH25122000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",8.3000000000000004E-2,0,0,219533,18221.2,0,0,219533,18221.2,null,null,"N","N","",1]
["CSH25122000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.2000000000000003E-2,0,0,165545,6952.8,0,0,165545,6952.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,25174,0,0,0,25174,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH25123000S",null,null,null,"수간보호 / 일반","흉고직경 21~31cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH25123000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",0.125,0,0,219533,27441.599999999999,0,0,219533,27441.599999999999,null,null,"N","N","",1]
["CSH25123000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.3E-2,0,0,165545,10429.299999999999,0,0,165545,10429.299999999999,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,37870,0,0,0,37870,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH25124000S",null,null,null,"수간보호 / 일반","흉고직경 31~41cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH25124000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",0.182,0,0,219533,39955,0,0,219533,39955,null,null,"N","N","",1]
["CSH25124000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",9.0999999999999998E-2,0,0,165545,15064.5,0,0,165545,15064.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,55019,0,0,0,55019,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH25125000S",null,null,null,"수간보호 / 일반","흉고직경 41~51cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH25125000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",0.25,0,0,219533,54883.199999999997,0,0,219533,54883.199999999997,null,null,"N","N","",1]
["CSH25125000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.13,0,0,165545,21520.799999999999,0,0,165545,21520.799999999999,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,76404,0,0,0,76404,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH25201000S",null,null,null,"줄기감싸기","흉고직경 11cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH25201000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",2.4E-2,0,0,219533,5268.7,0,0,219533,5268.7,null,null,"N","N","",1]
["CSH25201000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.2E-2,0,0,165545,1986.5,0,0,165545,1986.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,7255,0,0,0,7255,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH25202000S",null,null,null,"줄기감싸기","흉고직경 11~21cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH25202000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",2.9000000000000001E-2,0,0,219533,6366.4,0,0,219533,6366.4,null,null,"N","N","",1]
["CSH25202000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.4999999999999999E-2,0,0,165545,2483.1,0,0,165545,2483.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,8849,0,0,0,8849,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH25203000S",null,null,null,"줄기감싸기","흉고직경 21~31cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH25203000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",3.6999999999999998E-2,0,0,219533,8122.7,0,0,219533,8122.7,null,null,"N","N","",1]
["CSH25203000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.9E-2,0,0,165545,3145.3,0,0,165545,3145.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,11268,0,0,0,11268,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH25204000S",null,null,null,"줄기감싸기","흉고직경 31~41cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH25204000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",4.8000000000000001E-2,0,0,219533,10537.5,0,0,219533,10537.5,null,null,"N","N","",1]
["CSH25204000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.4E-2,0,0,165545,3973,0,0,165545,3973,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,14510,0,0,0,14510,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH25205000S",null,null,null,"줄기감싸기","흉고직경 41~51cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH25205000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",6.7000000000000004E-2,0,0,219533,14708.7,0,0,219533,14708.7,null,null,"N","N","",1]
["CSH25205000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.3000000000000002E-2,0,0,165545,5462.9,0,0,165545,5462.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,20171,0,0,0,20171,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH26101000S",null,null,null,"인력 관수","흉고직경 10cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH26101000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.03,0,0,165545,4966.3,0,0,165545,4966.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,4966,0,0,0,4966,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH26102000S",null,null,null,"인력 관수","흉고직경 10~20cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH26102000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.04,0,0,165545,6621.8,0,0,165545,6621.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,6621,0,0,0,6621,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH26103000S",null,null,null,"인력 관수","흉고직경 20~30cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH26103000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.8999999999999997E-2,0,0,165545,9767.1,0,0,165545,9767.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,9767,0,0,0,9767,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH26104000S",null,null,null,"인력 관수","흉고직경 30~40cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH26104000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.6999999999999999E-2,0,0,165545,12746.9,0,0,165545,12746.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,12746,0,0,0,12746,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH26105000S",null,null,null,"인력 관수","흉고직경 40cm 이상","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH26105000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.1,0,0,165545,16554.5,0,0,165545,16554.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,16554,0,0,0,16554,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH26201000S",null,null,null,"살수차 관수 / 소형장비","1,800L, 이동거리 5km까지","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH26201000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.4E-3,0,0,165545,231.7,0,0,165545,231.7,null,null,"N","N","",1]
["CSH26201000S","기계경비","00007204001800000",null,"물탱크(살수차)","1800L","HR",1.14E-2,13559,154.5,47231,538.4,7041,80.2,67831,773.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,154,0,770,0,80,0,1004,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH26202000S",null,null,null,"살수차 관수 / 중형장비","3,800L, 이동거리 5km까지","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH26202000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",9.1E-4,0,0,165545,150.6,0,0,165545,150.6,null,null,"N","N","",1]
["CSH26202000S","기계경비","00007204003800000",null,"물탱크(살수차)","3800L","HR",7.2700000000000004E-3,14220,103.3,47231,343.3,8165,59.3,69616,505.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,103,0,493,0,59,0,655,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH26203000S",null,null,null,"살수차 관수 / 대형장비","5,500L, 이동거리 5km까지","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH26203000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.4999999999999999E-4,0,0,165545,74.400000000000006,0,0,165545,74.400000000000006,null,null,"N","N","",1]
["CSH26203000S","기계경비","00007204005500000",null,"물탱크(살수차)","5500L","HR",3.64E-3,15378,55.9,47231,171.9,9470,34.4,72079,262.2,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,55,0,246,0,34,0,335,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH27101000S",null,null,null,"제초","일반 잔디지역","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH27101000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",7.1000000000000002E-4,0,0,219533,155.80000000000001,0,0,219533,155.80000000000001,null,null,"N","N","",1]
["CSH27101000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.5699999999999998E-3,0,0,165545,590.9,0,0,165545,590.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,746,0,0,0,746,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH27102000S",null,null,null,"제초","지장물 지역","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH27102000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",1E-3,0,0,219533,219.5,0,0,219533,219.5,null,null,"N","N","",1]
["CSH27102000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.0000000000000001E-3,0,0,165545,827.7,0,0,165545,827.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,1047,0,0,0,1047,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH27201100S",null,null,null,"잔디깎기 / 배부식","연3회 이상 ","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH27201100S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",9.1E-4,0,0,214222,194.9,0,0,214222,194.9,null,null,"N","N","",1]
["CSH27201100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.9999999999999997E-4,0,0,165545,49.6,0,0,165545,49.6,null,null,"N","N","",1]
["CSH27201100S","손료","RENT000000000001",null,"공구손료","노무비의 8%","식",1,19.5,19.5,0,0,0,0,19.5,19.5,null,null,"N","N",8,1]
[null,null,null,null,"[합 계]",null,null,0,0,19,0,244,0,0,0,263,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH27201200S",null,null,null,"잔디깎기 / 배부식","연2회 ","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH27201200S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",1.14E-3,0,0,214222,244.2,0,0,214222,244.2,null,null,"N","N","",1]
["CSH27201200S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.8000000000000002E-4,0,0,165545,62.9,0,0,165545,62.9,null,null,"N","N","",1]
["CSH27201200S","손료","RENT000000000001",null,"공구손료","노무비의 8%","식",1,24.5,24.5,0,0,0,0,24.5,24.5,null,null,"N","N",8,1]
[null,null,null,null,"[합 계]",null,null,0,0,24,0,307,0,0,0,331,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH27201300S",null,null,null,"잔디깎기 / 배부식","연1회 ","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH27201300S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",1.2999999999999999E-3,0,0,214222,278.39999999999998,0,0,214222,278.39999999999998,null,null,"N","N","",1]
["CSH27201300S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.2999999999999999E-4,0,0,165545,71.099999999999994,0,0,165545,71.099999999999994,null,null,"N","N","",1]
["CSH27201300S","손료","RENT000000000001",null,"공구손료","노무비의 8%","식",1,27.9,27.9,0,0,0,0,27.9,27.9,null,null,"N","N",8,1]
[null,null,null,null,"[합 계]",null,null,0,0,27,0,349,0,0,0,376,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH27202100S",null,null,null,"잔디깎기 / 핸드가이드식","연3회 이상 ","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH27202100S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",2.5000000000000001E-4,0,0,214222,53.5,0,0,214222,53.5,null,null,"N","N","",1]
["CSH27202100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5000000000000001E-4,0,0,165545,41.3,0,0,165545,41.3,null,null,"N","N","",1]
["CSH27202100S","손료","RENT000000000001",null,"공구손료","노무비의 7%","식",1,6.6,6.6,0,0,0,0,6.6,6.6,null,null,"N","N",7,1]
[null,null,null,null,"[합 계]",null,null,0,0,6,0,94,0,0,0,100,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH27202200S",null,null,null,"잔디깎기 / 핸드가이드식","연2회 ","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH27202200S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",3.1E-4,0,0,214222,66.400000000000006,0,0,214222,66.400000000000006,null,null,"N","N","",1]
["CSH27202200S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.1E-4,0,0,165545,51.3,0,0,165545,51.3,null,null,"N","N","",1]
["CSH27202200S","손료","RENT000000000001",null,"공구손료","노무비의 7%","식",1,8.1999999999999993,8.1999999999999993,0,0,0,0,8.1999999999999993,8.1999999999999993,null,null,"N","N",7,1]
[null,null,null,null,"[합 계]",null,null,0,0,8,0,117,0,0,0,125,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH27202300S",null,null,null,"잔디깎기 / 핸드가이드식","연1회 ","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH27202300S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",3.6000000000000002E-4,0,0,214222,77.099999999999994,0,0,214222,77.099999999999994,null,null,"N","N","",1]
["CSH27202300S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.6000000000000002E-4,0,0,165545,59.5,0,0,165545,59.5,null,null,"N","N","",1]
["CSH27202300S","손료","RENT000000000001",null,"공구손료","노무비의 7%","식",1,9.5,9.5,0,0,0,0,9.5,9.5,null,null,"N","N",7,1]
[null,null,null,null,"[합 계]",null,null,0,0,9,0,136,0,0,0,145,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH27301100S",null,null,null,"예초","연3회 이상 ","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH27301100S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",1.1999999999999999E-3,0,0,214222,257,0,0,214222,257,null,null,"N","N","",1]
["CSH27301100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.0000000000000002E-4,0,0,165545,66.2,0,0,165545,66.2,null,null,"N","N","",1]
["CSH27301100S","손료","RENT000000000001",null,"공구손료","노무비의 6%","식",1,19.3,19.3,0,0,0,0,19.3,19.3,null,null,"N","N",6,1]
[null,null,null,null,"[합 계]",null,null,0,0,19,0,323,0,0,0,342,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH27301110S",null,null,null,"예초 / 경사도 25˚이상","연3회 이상 ","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH27301110S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",1.33E-3,0,0,214222,284.89999999999998,0,0,214222,284.89999999999998,null,null,"N","N","",1]
["CSH27301110S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.4000000000000002E-4,0,0,165545,72.8,0,0,165545,72.8,null,null,"N","N","",1]
["CSH27301110S","손료","RENT000000000001",null,"공구손료","노무비의 6%","식",1,21.4,21.4,0,0,0,0,21.4,21.4,null,null,"N","N",6,1]
[null,null,null,null,"[합 계]",null,null,0,0,21,0,357,0,0,0,378,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH27301200S",null,null,null,"예초","연2회 ","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH27301200S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",1.5E-3,0,0,214222,321.3,0,0,214222,321.3,null,null,"N","N","",1]
["CSH27301200S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.0000000000000001E-4,0,0,165545,82.7,0,0,165545,82.7,null,null,"N","N","",1]
["CSH27301200S","손료","RENT000000000001",null,"공구손료","노무비의 6%","식",1,24.2,24.2,0,0,0,0,24.2,24.2,null,null,"N","N",6,1]
[null,null,null,null,"[합 계]",null,null,0,0,24,0,404,0,0,0,428,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH27301210S",null,null,null,"예초 / 경사도 25˚이상","연2회 ","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH27301210S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",1.7099999999999999E-3,0,0,214222,366.3,0,0,214222,366.3,null,null,"N","N","",1]
["CSH27301210S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.6999999999999998E-4,0,0,165545,94.3,0,0,165545,94.3,null,null,"N","N","",1]
["CSH27301210S","손료","RENT000000000001",null,"공구손료","노무비의 6%","식",1,27.6,27.6,0,0,0,0,27.6,27.6,null,null,"N","N",6,1]
[null,null,null,null,"[합 계]",null,null,0,0,27,0,460,0,0,0,487,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH27301300S",null,null,null,"예초","연1회 ","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH27301300S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",1.7099999999999999E-3,0,0,214222,366.3,0,0,214222,366.3,null,null,"N","N","",1]
["CSH27301300S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.6999999999999998E-4,0,0,165545,94.3,0,0,165545,94.3,null,null,"N","N","",1]
["CSH27301300S","손료","RENT000000000001",null,"공구손료","노무비의 6%","식",1,27.6,27.6,0,0,0,0,27.6,27.6,null,null,"N","N",6,1]
[null,null,null,null,"[합 계]",null,null,0,0,27,0,460,0,0,0,487,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH27301310S",null,null,null,"예초 / 경사도 25˚이상","연1회","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH27301310S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",2E-3,0,0,214222,428.4,0,0,214222,428.4,null,null,"N","N","",1]
["CSH27301310S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.7000000000000002E-4,0,0,165545,110.9,0,0,165545,110.9,null,null,"N","N","",1]
["CSH27301310S","손료","RENT000000000001",null,"공구손료","노무비의 6%","식",1,32.299999999999997,32.299999999999997,0,0,0,0,32.299999999999997,32.299999999999997,null,null,"N","N",6,1]
[null,null,null,null,"[합 계]",null,null,0,0,32,0,539,0,0,0,571,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH28111000S",null,null,null,"교목시비 / 환상시비","근원직경 11cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH28111000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",2.5999999999999999E-2,0,0,219533,5707.8,0,0,219533,5707.8,null,null,"N","N","",1]
["CSH28111000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.2999999999999999E-2,0,0,165545,2152,0,0,165545,2152,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,7859,0,0,0,7859,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH28112000S",null,null,null,"교목시비 / 환상시비","근원직경 11~21cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH28112000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",3.3000000000000002E-2,0,0,219533,7244.5,0,0,219533,7244.5,null,null,"N","N","",1]
["CSH28112000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.6E-2,0,0,165545,2648.7,0,0,165545,2648.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,9893,0,0,0,9893,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH28113000S",null,null,null,"교목시비 / 환상시비","근원직경 21~31cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH28113000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",3.9E-2,0,0,219533,8561.7000000000007,0,0,219533,8561.7000000000007,null,null,"N","N","",1]
["CSH28113000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.02,0,0,165545,3310.9,0,0,165545,3310.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,11872,0,0,0,11872,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH28114000S",null,null,null,"교목시비 / 환상시비","근원직경 31~41cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH28114000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",4.4999999999999998E-2,0,0,219533,9878.9,0,0,219533,9878.9,null,null,"N","N","",1]
["CSH28114000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.3E-2,0,0,165545,3807.5,0,0,165545,3807.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,13686,0,0,0,13686,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH28115000S",null,null,null,"교목시비 / 환상시비","근원직경 41~51cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH28115000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",5.2999999999999999E-2,0,0,219533,11635.2,0,0,219533,11635.2,null,null,"N","N","",1]
["CSH28115000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5999999999999999E-2,0,0,165545,4304.1000000000004,0,0,165545,4304.1000000000004,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,15939,0,0,0,15939,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH28116000S",null,null,null,"교목시비 / 환상시비","근원직경 51cm 이상","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH28116000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",5.8999999999999997E-2,0,0,219533,12952.4,0,0,219533,12952.4,null,null,"N","N","",1]
["CSH28116000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.9000000000000001E-2,0,0,165545,4800.8,0,0,165545,4800.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,17753,0,0,0,17753,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH28121000S",null,null,null,"교목시비 / 방사형시비","근원직경 11cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH28121000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",0.02,0,0,219533,4390.6000000000004,0,0,219533,4390.6000000000004,null,null,"N","N","",1]
["CSH28121000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.01,0,0,165545,1655.4,0,0,165545,1655.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,6046,0,0,0,6046,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH28122000S",null,null,null,"교목시비 / 방사형시비","근원직경 11~21cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH28122000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",2.4E-2,0,0,219533,5268.7,0,0,219533,5268.7,null,null,"N","N","",1]
["CSH28122000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.2E-2,0,0,165545,1986.5,0,0,165545,1986.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,7255,0,0,0,7255,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH28123000S",null,null,null,"교목시비 / 방사형시비","근원직경 21~31cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH28123000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",2.9000000000000001E-2,0,0,219533,6366.4,0,0,219533,6366.4,null,null,"N","N","",1]
["CSH28123000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.4E-2,0,0,165545,2317.6,0,0,165545,2317.6,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,8684,0,0,0,8684,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH28124000S",null,null,null,"교목시비 / 방사형시비","근원직경 31~41cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH28124000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",3.4000000000000002E-2,0,0,219533,7464.1,0,0,219533,7464.1,null,null,"N","N","",1]
["CSH28124000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.7000000000000001E-2,0,0,165545,2814.2,0,0,165545,2814.2,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,10278,0,0,0,10278,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH28125000S",null,null,null,"교목시비 / 방사형시비","근원직경 41~51cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH28125000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",3.7999999999999999E-2,0,0,219533,8342.2000000000007,0,0,219533,8342.2000000000007,null,null,"N","N","",1]
["CSH28125000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.9E-2,0,0,165545,3145.3,0,0,165545,3145.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,11487,0,0,0,11487,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH28126000S",null,null,null,"교목시비 / 방사형시비","근원직경 51cm 이상","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH28126000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",4.2999999999999997E-2,0,0,219533,9439.9,0,0,219533,9439.9,null,null,"N","N","",1]
["CSH28126000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.1999999999999999E-2,0,0,165545,3641.9,0,0,165545,3641.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,13081,0,0,0,13081,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH28200000S",null,null,null,"관목시비",null,"M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH28200000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",6.7000000000000002E-3,0,0,219533,1470.8,0,0,219533,1470.8,null,null,"N","N","",1]
["CSH28200000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.3E-3,0,0,165545,546.20000000000005,0,0,165545,546.20000000000005,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,2017,0,0,0,2017,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH28300000S",null,null,null,"잔디시비",null,"M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH28300000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",8.8999999999999995E-5,0,0,219533,19.5,0,0,219533,19.5,null,null,"N","N","",1]
["CSH28300000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.3999999999999999E-5,0,0,165545,7.2,0,0,165545,7.2,null,null,"N","N","",1]
["CSH28300000S","기계경비","00000602002500000",null,"덤프트럭","2.5ton","HR",3.5599999999999998E-4,5090,1.8,47231,16.8,6169,2.1,58490,20.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,1,0,43,0,2,0,46,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29100000S",null,null,null,"약제살포 / 기계","수목류 약제살포","L",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29100000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",3.8000000000000002E-4,0,0,219533,83.4,0,0,219533,83.4,null,null,"N","N","",1]
["CSH29100000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.8000000000000002E-4,0,0,165545,62.9,0,0,165545,62.9,null,null,"N","N","",1]
["CSH29100000S","기계경비","00007210048500000",null,"동력분무기","4.85kw","HR",3.0799999999999998E-3,2219,6.8,0,0,244,0.7,2463,7.5,null,null,"N","N","",1]
["CSH29100000S","기계경비","00000602002500000",null,"덤프트럭","2.5ton","HR",3.0799999999999998E-3,5090,15.6,47231,145.4,6169,19,58490,180,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,22,0,291,0,19,0,332,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29200000S",null,null,null,"약제살포 / 인력","잔디 약제살포","M2",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29200000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",5.0000000000000001E-4,0,0,219533,109.7,0,0,219533,109.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,109,0,0,0,109,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29310000S",null,null,null,"방풍벽 설치, 거적세우기","H=0.45m","M당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29310000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",5.7000000000000002E-3,0,0,219533,1251.3,0,0,219533,1251.3,null,null,"N","N","",1]
["CSH29310000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.8999999999999998E-3,0,0,165545,480,0,0,165545,480,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,1731,0,0,0,1731,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29320000S",null,null,null,"방풍벽 설치, 거적세우기","H=0.9m","M당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29320000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",8.0000000000000002E-3,0,0,219533,1756.2,0,0,219533,1756.2,null,null,"N","N","",1]
["CSH29320000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.0000000000000001E-3,0,0,165545,662.1,0,0,165545,662.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,2418,0,0,0,2418,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29401000S",null,null,null,"은행나무 과실채취","흉고직경 11cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29401000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",4.2999999999999997E-2,0,0,219533,9439.9,0,0,219533,9439.9,null,null,"N","N","",1]
["CSH29401000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",8.6999999999999994E-2,0,0,165545,14402.4,0,0,165545,14402.4,null,null,"N","N","",1]
["CSH29401000S","기계경비","00002106000300000",null,"고소작업차","3ton","HR",0.17399999999999999,4731,823.1,47231,8218.1,16247,2826.9,68209,11868.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,823,0,32060,0,2826,0,35709,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29402000S",null,null,null,"은행나무 과실채취","흉고직경 11~21cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29402000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",6.5000000000000002E-2,0,0,219533,14269.6,0,0,219533,14269.6,null,null,"N","N","",1]
["CSH29402000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.129,0,0,165545,21355.3,0,0,165545,21355.3,null,null,"N","N","",1]
["CSH29402000S","기계경비","00002106000300000",null,"고소작업차","3ton","HR",0.25800000000000001,4731,1220.5,47231,12185.5,16247,4191.7,68209,17597.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,1220,0,47810,0,4191,0,53221,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29403000S",null,null,null,"은행나무 과실채취","흉고직경 21~31cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29403000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",8.6999999999999994E-2,0,0,219533,19099.3,0,0,219533,19099.3,null,null,"N","N","",1]
["CSH29403000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.17399999999999999,0,0,165545,28804.799999999999,0,0,165545,28804.799999999999,null,null,"N","N","",1]
["CSH29403000S","기계경비","00002106000300000",null,"고소작업차","3ton","HR",0.34799999999999998,4731,1646.3,47231,16436.3,16247,5653.9,68209,23736.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,1646,0,64340,0,5653,0,71639,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29404000S",null,null,null,"은행나무 과실채취","흉고직경 31~41cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29404000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",0.11799999999999999,0,0,219533,25904.799999999999,0,0,219533,25904.799999999999,null,null,"N","N","",1]
["CSH29404000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.23499999999999999,0,0,165545,38903,0,0,165545,38903,null,null,"N","N","",1]
["CSH29404000S","기계경비","00002106000300000",null,"고소작업차","3ton","HR",0.47099999999999997,4731,2228.3000000000002,47231,22245.8,16247,7652.3,68209,32126.400000000001,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,2228,0,87053,0,7652,0,96933,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29405000S",null,null,null,"은행나무 과실채취","흉고직경 41~51cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29405000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",0.13300000000000001,0,0,219533,29197.8,0,0,219533,29197.8,null,null,"N","N","",1]
["CSH29405000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.26700000000000002,0,0,165545,44200.5,0,0,165545,44200.5,null,null,"N","N","",1]
["CSH29405000S","기계경비","00002106000300000",null,"고소작업차","3ton","HR",0.53300000000000003,4731,2521.6,47231,25174.1,16247,8659.6,68209,36355.300000000003,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,2521,0,98572,0,8659,0,109752,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29406000S",null,null,null,"은행나무 과실채취","흉고직경 51~61cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29406000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",0.14299999999999999,0,0,219533,31393.200000000001,0,0,219533,31393.200000000001,null,null,"N","N","",1]
["CSH29406000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.28599999999999998,0,0,165545,47345.8,0,0,165545,47345.8,null,null,"N","N","",1]
["CSH29406000S","기계경비","00002106000300000",null,"고소작업차","3ton","HR",0.57099999999999995,4731,2701.4,47231,26968.9,16247,9277,68209,38947.300000000003,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,2701,0,105707,0,9277,0,117685,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29407000S",null,null,null,"은행나무 과실채취","흉고직경 61cm 초과","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29407000S","노무","L001010101000038",null,"조경공","일반공사 직종","인",0.2,0,0,219533,43906.6,0,0,219533,43906.6,null,null,"N","N","",1]
["CSH29407000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.4,0,0,165545,66218,0,0,165545,66218,null,null,"N","N","",1]
["CSH29407000S","기계경비","00002106000300000",null,"고소작업차","3ton","HR",0.8,4731,3784.8,47231,37784.800000000003,16247,12997.6,68209,54567.199999999997,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,3784,0,147909,0,12997,0,164690,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29500010S",null,null,null,"가로수 제거 / 나무베기","흉고직경 11cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29500010S","노무","L001010101000037",null,"벌목부","일반공사 직종","인",4.2000000000000003E-2,0,0,243490,10226.5,0,0,243490,10226.5,null,null,"N","N","",1]
["CSH29500010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.3E-2,0,0,165545,10429.299999999999,0,0,165545,10429.299999999999,null,null,"N","N","",1]
["CSH29500010S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,619.6,619.6,0,0,0,0,619.6,619.6,null,null,"N","N",3,1]
["CSH29500010S","기계경비","00000201004000000",null,"굴삭기(무한궤도)","0.4㎥","HR",0.16700000000000001,15363,2565.6,55700,9301.9,16378,2735.1,87441,14602.6,null,null,"N","N","",1]
["CSH29500010S","기계경비","00007206007000000",null,"부착용 집게","0.7~0.8㎥","HR",0.16700000000000001,0,0,0,0,5487,916.3,5487,916.3,null,null,"N","N","",1]
["CSH29500010S","기계경비","00002106000300000",null,"고소작업차","3ton","HR",0.16700000000000001,4731,790,47231,7887.5,16247,2713.2,68209,11390.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,3975,0,37845,0,6364,0,48184,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29500020S",null,null,null,"가로수 제거 / 나무베기","흉고직경 11~21cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29500020S","노무","L001010101000037",null,"벌목부","일반공사 직종","인",6.3E-2,0,0,243490,15339.8,0,0,243490,15339.8,null,null,"N","N","",1]
["CSH29500020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",9.4E-2,0,0,165545,15561.2,0,0,165545,15561.2,null,null,"N","N","",1]
["CSH29500020S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,927,927,0,0,0,0,927,927,null,null,"N","N",3,1]
["CSH29500020S","기계경비","00000201006000000",null,"굴삭기(무한궤도)","0.6㎥","HR",0.25,15828,3957,55700,13925,21957,5489.2,93485,23371.200000000001,null,null,"N","N","",1]
["CSH29500020S","기계경비","00007206007000000",null,"부착용 집게","0.7~0.8㎥","HR",0.25,0,0,0,0,5487,1371.7,5487,1371.7,null,null,"N","N","",1]
["CSH29500020S","기계경비","00002106000300000",null,"고소작업차","3ton","HR",0.25,4731,1182.7,47231,11807.7,16247,4061.7,68209,17052.099999999999,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,6066,0,56633,0,10922,0,73621,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29500030S",null,null,null,"가로수 제거 / 나무베기","흉고직경 21~31cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29500030S","노무","L001010101000037",null,"벌목부","일반공사 직종","인",0.1,0,0,243490,24349,0,0,243490,24349,null,null,"N","N","",1]
["CSH29500030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.15,0,0,165545,24831.7,0,0,165545,24831.7,null,null,"N","N","",1]
["CSH29500030S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,1475.4,1475.4,0,0,0,0,1475.4,1475.4,null,null,"N","N",3,1]
["CSH29500030S","기계경비","00000201006000000",null,"굴삭기(무한궤도)","0.6㎥","HR",0.4,15828,6331.2,55700,22280,21957,8782.7999999999993,93485,37394,null,null,"N","N","",1]
["CSH29500030S","기계경비","00007206007000000",null,"부착용 집게","0.7~0.8㎥","HR",0.4,0,0,0,0,5487,2194.8000000000002,5487,2194.8000000000002,null,null,"N","N","",1]
["CSH29500030S","기계경비","00002106000300000",null,"고소작업차","3ton","HR",0.4,4731,1892.4,47231,18892.400000000001,16247,6498.8,68209,27283.599999999999,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,9699,0,90353,0,17476,0,117528,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29500040S",null,null,null,"가로수 제거 / 나무베기","흉고직경 31~41cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29500040S","노무","L001010101000037",null,"벌목부","일반공사 직종","인",0.154,0,0,243490,37497.4,0,0,243490,37497.4,null,null,"N","N","",1]
["CSH29500040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.23100000000000001,0,0,165545,38240.800000000003,0,0,165545,38240.800000000003,null,null,"N","N","",1]
["CSH29500040S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,2272.1,2272.1,0,0,0,0,2272.1,2272.1,null,null,"N","N",3,1]
["CSH29500040S","기계경비","00000201006000000",null,"굴삭기(무한궤도)","0.6㎥","HR",0.61499999999999999,15828,9734.2000000000007,55700,34255.5,21957,13503.5,93485,57493.2,null,null,"N","N","",1]
["CSH29500040S","기계경비","00007206007000000",null,"부착용 집게","0.7~0.8㎥","HR",0.61499999999999999,0,0,0,0,5487,3374.5,5487,3374.5,null,null,"N","N","",1]
["CSH29500040S","기계경비","00002106000300000",null,"고소작업차","3ton","HR",0.61499999999999999,4731,2909.5,47231,29047,16247,9991.9,68209,41948.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,14915,0,139040,0,26869,0,180824,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29500050S",null,null,null,"가로수 제거 / 나무베기","흉고직경 41~51cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29500050S","노무","L001010101000037",null,"벌목부","일반공사 직종","인",0.25,0,0,243490,60872.5,0,0,243490,60872.5,null,null,"N","N","",1]
["CSH29500050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.38,0,0,165545,62907.1,0,0,165545,62907.1,null,null,"N","N","",1]
["CSH29500050S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,3713.3,3713.3,0,0,0,0,3713.3,3713.3,null,null,"N","N",3,1]
["CSH29500050S","기계경비","00000201006000000",null,"굴삭기(무한궤도)","0.6㎥","HR",1,15828,15828,55700,55700,21957,21957,93485,93485,null,null,"N","N","",1]
["CSH29500050S","기계경비","00007206007000000",null,"부착용 집게","0.7~0.8㎥","HR",1,0,0,0,0,5487,5487,5487,5487,null,null,"N","N","",1]
["CSH29500050S","기계경비","00002106000300000",null,"고소작업차","3ton","HR",1,4731,4731,47231,47231,16247,16247,68209,68209,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,24272,0,226710,0,43691,0,294673,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29500060S",null,null,null,"가로수 제거 / 나무베기","흉고직경 51~61cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29500060S","노무","L001010101000037",null,"벌목부","일반공사 직종","인",0.4,0,0,243490,97396,0,0,243490,97396,null,null,"N","N","",1]
["CSH29500060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.6,0,0,165545,99327,0,0,165545,99327,null,null,"N","N","",1]
["CSH29500060S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,5901.6,5901.6,0,0,0,0,5901.6,5901.6,null,null,"N","N",3,1]
["CSH29500060S","기계경비","00000201006000000",null,"굴삭기(무한궤도)","0.6㎥","HR",1.6,15828,25324.799999999999,55700,89120,21957,35131.199999999997,93485,149576,null,null,"N","N","",1]
["CSH29500060S","기계경비","00007206007000000",null,"부착용 집게","0.7~0.8㎥","HR",1.6,0,0,0,0,5487,8779.2000000000007,5487,8779.2000000000007,null,null,"N","N","",1]
["CSH29500060S","기계경비","00002106000300000",null,"고소작업차","3ton","HR",1.6,4731,7569.6,47231,75569.600000000006,16247,25995.200000000001,68209,109134.39999999999,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,38796,0,361412,0,69905,0,470113,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29500070S",null,null,null,"가로수 제거 / 나무베기","흉고직경 61cm 이상","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29500070S","노무","L001010101000037",null,"벌목부","일반공사 직종","인",0.67,0,0,243490,163138.29999999999,0,0,243490,163138.29999999999,null,null,"N","N","",1]
["CSH29500070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1,0,0,165545,165545,0,0,165545,165545,null,null,"N","N","",1]
["CSH29500070S","손료","RENT000000000001",null,"공구손료","노무비의 3%","식",1,9860.4,9860.4,0,0,0,0,9860.4,9860.4,null,null,"N","N",3,1]
["CSH29500070S","기계경비","00000201006000000",null,"굴삭기(무한궤도)","0.6㎥","HR",2.67,15828,42260.7,55700,148719,21957,58625.1,93485,249604.8,null,null,"N","N","",1]
["CSH29500070S","기계경비","00007206007000000",null,"부착용 집게","0.7~0.8㎥","HR",2.67,0,0,0,0,5487,14650.2,5487,14650.2,null,null,"N","N","",1]
["CSH29500070S","기계경비","00002106000300000",null,"고소작업차","3ton","HR",2.67,4731,12631.7,47231,126106.7,16247,43379.4,68209,182117.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,64752,0,603509,0,116654,0,784915,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29500110S",null,null,null,"가로수 제거 / 뿌리제거","흉고직경 11cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29500110S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",5.3999999999999999E-2,0,0,214222,11567.9,0,0,214222,11567.9,null,null,"N","N","",1]
["CSH29500110S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.7E-2,0,0,165545,4469.7,0,0,165545,4469.7,null,null,"N","N","",1]
["CSH29500110S","기계경비","00000201004000004",null,"굴삭기(유압식백호우)","0.4 ㎥, (브레이커조합)","HR",0.216,14607,3155.1,55700,12031.2,21581,4661.3999999999996,91888,19847.7,null,null,"N","N","",1]
["CSH29500110S","기계경비","00000230000400000",null,"대형 브레이커","0.4㎥용","HR",0.216,0,0,0,0,5202,1123.5999999999999,5202,1123.5999999999999,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,3155,0,28068,0,5785,0,37008,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29500120S",null,null,null,"가로수 제거 / 뿌리제거","흉고직경 11~21cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29500120S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.08,0,0,214222,17137.7,0,0,214222,17137.7,null,null,"N","N","",1]
["CSH29500120S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.04,0,0,165545,6621.8,0,0,165545,6621.8,null,null,"N","N","",1]
["CSH29500120S","기계경비","00000201006000004",null,"굴삭기(유압식백호우)","0.6 ㎥, (브레이커조합)","HR",0.32,15050,4816,55700,17824,30786,9851.5,101536,32491.5,null,null,"N","N","",1]
["CSH29500120S","기계경비","00000230000600000",null,"대형 브레이커","0.6㎥용","HR",0.32,0,0,0,0,8829,2825.2,8829,2825.2,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,4816,0,41583,0,12676,0,59075,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29500130S",null,null,null,"가로수 제거 / 뿌리제거","흉고직경 21~31cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29500130S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.13300000000000001,0,0,214222,28491.5,0,0,214222,28491.5,null,null,"N","N","",1]
["CSH29500130S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.7000000000000004E-2,0,0,165545,11091.5,0,0,165545,11091.5,null,null,"N","N","",1]
["CSH29500130S","기계경비","00000201006000004",null,"굴삭기(유압식백호우)","0.6 ㎥, (브레이커조합)","HR",0.53300000000000003,15050,8021.6,55700,29688.1,30786,16408.900000000001,101536,54118.6,null,null,"N","N","",1]
["CSH29500130S","기계경비","00000230000600000",null,"대형 브레이커","0.6㎥용","HR",0.53300000000000003,0,0,0,0,8829,4705.8,8829,4705.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,8021,0,69271,0,21114,0,98406,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29500140S",null,null,null,"가로수 제거 / 뿌리제거","흉고직경 31~41cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29500140S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.2,0,0,214222,42844.4,0,0,214222,42844.4,null,null,"N","N","",1]
["CSH29500140S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.1,0,0,165545,16554.5,0,0,165545,16554.5,null,null,"N","N","",1]
["CSH29500140S","기계경비","00000201006000004",null,"굴삭기(유압식백호우)","0.6 ㎥, (브레이커조합)","HR",0.8,15050,12040,55700,44560,30786,24628.799999999999,101536,81228.800000000003,null,null,"N","N","",1]
["CSH29500140S","기계경비","00000230000600000",null,"대형 브레이커","0.6㎥용","HR",0.8,0,0,0,0,8829,7063.2,8829,7063.2,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,12040,0,103958,0,31692,0,147690,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29500150S",null,null,null,"가로수 제거 / 뿌리제거","흉고직경 41~51cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29500150S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.33,0,0,214222,70693.2,0,0,214222,70693.2,null,null,"N","N","",1]
["CSH29500150S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.17,0,0,165545,28142.6,0,0,165545,28142.6,null,null,"N","N","",1]
["CSH29500150S","기계경비","00000201006000004",null,"굴삭기(유압식백호우)","0.6 ㎥, (브레이커조합)","HR",1.33,15050,20016.5,55700,74081,30786,40945.300000000003,101536,135042.79999999999,null,null,"N","N","",1]
["CSH29500150S","기계경비","00000230000600000",null,"대형 브레이커","0.6㎥용","HR",1.33,0,0,0,0,8829,11742.5,8829,11742.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,20016,0,172916,0,52687,0,245619,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29500160S",null,null,null,"가로수 제거 / 뿌리제거","흉고직경 51~61cm 미만","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29500160S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.5,0,0,214222,107111,0,0,214222,107111,null,null,"N","N","",1]
["CSH29500160S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.25,0,0,165545,41386.199999999997,0,0,165545,41386.199999999997,null,null,"N","N","",1]
["CSH29500160S","기계경비","00000201006000004",null,"굴삭기(유압식백호우)","0.6 ㎥, (브레이커조합)","HR",2,15050,30100,55700,111400,30786,61572,101536,203072,null,null,"N","N","",1]
["CSH29500160S","기계경비","00000230000600000",null,"대형 브레이커","0.6㎥용","HR",2,0,0,0,0,8829,17658,8829,17658,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,30100,0,259897,0,79230,0,369227,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29500170S",null,null,null,"가로수 제거 / 뿌리제거","흉고직경 61cm 이상","주",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["CSH29500170S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.67,0,0,214222,143528.70000000001,0,0,214222,143528.70000000001,null,null,"N","N","",1]
["CSH29500170S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.33,0,0,165545,54629.8,0,0,165545,54629.8,null,null,"N","N","",1]
["CSH29500170S","기계경비","00000201006000004",null,"굴삭기(유압식백호우)","0.6 ㎥, (브레이커조합)","HR",2.67,15050,40183.5,55700,148719,30786,82198.600000000006,101536,271101.09999999998,null,null,"N","N","",1]
["CSH29500170S","기계경비","00000230000600000",null,"대형 브레이커","0.6㎥용","HR",2.67,0,0,0,0,8829,23573.4,8829,23573.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,40183,0,346877,0,105772,0,492832,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]