{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["일위대가","일위대가상세"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"일위대가","index":0,"n_rows":3044,"n_cols":11,"rows_kept":3044,"cut":false,"hidden":false,"merged":[[1,0,1,10],[0,0,0,10]]}
["일 위 대 가"]
["20240200043_2024년 표준일위대가(기계)_1800520820"]
["일위대가코드","번호","품명","규격","단위","재료비","노무비","경비","합계","비목구분","비고"]
["MBA00010010S",null,"강관 용접 접합(아크용접)","D15","개소",288,9612,0,9900,"합계"]
["MBA00010020S",null,"강관 용접 접합(아크용접)","D20","개소",344,11481,0,11825,"합계"]
["MBA00010030S",null,"강관 용접 접합(아크용접)","D25","개소",416,13885,0,14301,"합계"]
["MBA00010040S",null,"강관 용접 접합(아크용접)","D32","개소",496,16555,0,17051,"합계"]
["MBA00010050S",null,"강관 용접 접합(아크용접)","D40","개소",560,18691,0,19251,"합계"]
["MBA00010060S",null,"강관 용접 접합(아크용접)","D50","개소",680,22696,0,23376,"합계"]
["MBA00010070S",null,"강관 용접 접합(아크용접)","D65","개소",841,28037,0,28878,"합계"]
["MBA00010080S",null,"강관 용접 접합(아크용접)","D80","개소",969,32309,0,33278,"합계"]
["MBA00010090S",null,"강관 용접 접합(아크용접)","D100","개소",1217,40587,0,41804,"합계"]
["MBA00010100S",null,"강관 용접 접합(아크용접)","D125","개소",1473,49131,0,50604,"합계"]
["MBA00010110S",null,"강관 용접 접합(아크용접)","D150","개소",1730,57676,0,59406,"합계"]
["MBA00010120S",null,"강관 용접 접합(아크용접)","D200","개소",2250,75032,0,77282,"합계"]
["MBA00010130S",null,"강관 용접 접합(아크용접)","D250","개소",2763,92122,0,94885,"합계"]
["MBA00010140S",null,"강관 용접 접합(아크용접)","D300","개소",3276,109211,0,112487,"합계"]
["MBA00010150S",null,"강관 용접 접합(아크용접)","D350","개소",3652,121761,0,125413,"합계"]
["MBA00010160S",null,"강관 용접 접합(아크용접)","D400","개소",4157,138583,0,142740,"합계"]
["MBA00110010S",null,"강관 용접 접합(아크용접)","D15, 고소작업대 사용","개소",1249,7690,0,8939,"합계"]
["MBA00110020S",null,"강관 용접 접합(아크용접)","D20, 고소작업대 사용","개소",1492,9185,0,10677,"합계"]
["MBA00110030S",null,"강관 용접 접합(아크용접)","D25, 고소작업대 사용","개소",1805,11108,0,12913,"합계"]
["MBA00110040S",null,"강관 용접 접합(아크용접)","D32, 고소작업대 사용","개소",2152,13244,0,15396,"합계"]
["MBA00110050S",null,"강관 용접 접합(아크용접)","D40, 고소작업대 사용","개소",2429,14953,0,17382,"합계"]
["MBA00110060S",null,"강관 용접 접합(아크용접)","D50, 고소작업대 사용","개소",2950,18157,0,21107,"합계"]
["MBA00110070S",null,"강관 용접 접합(아크용접)","D65, 고소작업대 사용","개소",3644,22429,0,26073,"합계"]
["MBA00110080S",null,"강관 용접 접합(아크용접)","D80, 고소작업대 사용","개소",4200,25847,0,30047,"합계"]
["MBA00110090S",null,"강관 용접 접합(아크용접)","D100, 고소작업대 사용","개소",5276,32469,0,37745,"합계"]
["MBA00110100S",null,"강관 용접 접합(아크용접)","D125, 고소작업대 사용","개소",6387,39305,0,45692,"합계"]
["MBA00110110S",null,"강관 용접 접합(아크용접)","D150, 고소작업대 사용","개소",7497,46141,0,53638,"합계"]
["MBA00110120S",null,"강관 용접 접합(아크용접)","D200, 고소작업대 사용","개소",9754,60026,0,69780,"합계"]
["MBA00110130S",null,"강관 용접 접합(아크용접)","D250, 고소작업대 사용","개소",11975,73697,0,85672,"합계"]
["MBA00110140S",null,"강관 용접 접합(아크용접)","D300, 고소작업대 사용","개소",14197,87369,0,101566,"합계"]
["MBA00110150S",null,"강관 용접 접합(아크용접)","D350, 고소작업대 사용","개소",15828,97409,0,113237,"합계"]
["MBA00110160S",null,"강관 용접 접합(아크용접)","D400, 고소작업대 사용","개소",18015,110867,0,128882,"합계"]
["MBA10010010S",null,"강관 용접 배관","D15, 옥내일반","m",205,10296,0,10501,"합계"]
["MBA10010020S",null,"강관 용접 배관","D20, 옥내일반","m",227,11380,0,11607,"합계"]
["MBA10010030S",null,"강관 용접 배관","D25, 옥내일반","m",283,14171,0,14454,"합계"]
["MBA10010040S",null,"강관 용접 배관","D32, 옥내일반","m",330,16504,0,16834,"합계"]
["MBA10010050S",null,"강관 용접 배관","D40, 옥내일반","m",364,18212,0,18576,"합계"]
["MBA10010060S",null,"강관 용접 배관","D50, 옥내일반","m",462,23106,0,23568,"합계"]
["MBA10010070S",null,"강관 용접 배관","D65, 옥내일반","m",542,27147,0,27689,"합계"]
["MBA10010080S",null,"강관 용접 배관","D80, 옥내일반","m",687,34374,0,35061,"합계"]
["MBA10010090S",null,"강관 용접 배관","D100, 옥내일반","m",926,46330,0,47256,"합계"]
["MBA10010100S",null,"강관 용접 배관","D125, 옥내일반","m",1186,59305,0,60491,"합계"]
["MBA10010110S",null,"강관 용접 배관","D150, 옥내일반","m",1391,69553,0,70944,"합계"]
["MBA10010120S",null,"강관 용접 배관","D200, 옥내일반","m",2132,106606,0,108738,"합계"]
["MBA10010130S",null,"강관 용접 배관","D250, 옥내일반","m",2843,142180,0,145023,"합계"]
["MBA10010140S",null,"강관 용접 배관","D300, 옥내일반","m",3677,183897,0,187574,"합계"]
["MBA10010150S",null,"강관 용접 배관","D350, 옥내일반","m",4428,221409,0,225837,"합계"]
["MBA10010160S",null,"강관 용접 배관","D400, 옥내일반","m",5245,262273,0,267518,"합계"]
["MBA10110010S",null,"강관 용접 배관","D15, 옥내일반, 고소작업대 사용","m",1029,8237,0,9266,"합계"]
["MBA10110020S",null,"강관 용접 배관","D20, 옥내일반, 고소작업대 사용","m",1138,9104,0,10242,"합계"]
["MBA10110030S",null,"강관 용접 배관","D25, 옥내일반, 고소작업대 사용","m",1417,11337,0,12754,"합계"]
["MBA10110040S",null,"강관 용접 배관","D32, 옥내일반, 고소작업대 사용","m",1650,13203,0,14853,"합계"]
["MBA10110050S",null,"강관 용접 배관","D40, 옥내일반, 고소작업대 사용","m",1821,14569,0,16390,"합계"]
["MBA10110060S",null,"강관 용접 배관","D50, 옥내일반, 고소작업대 사용","m",2310,18485,0,20795,"합계"]
["MBA10110070S",null,"강관 용접 배관","D65, 옥내일반, 고소작업대 사용","m",2714,21717,0,24431,"합계"]
["MBA10110080S",null,"강관 용접 배관","D80, 옥내일반, 고소작업대 사용","m",3437,27499,0,30936,"합계"]
["MBA10110090S",null,"강관 용접 배관","D100, 옥내일반, 고소작업대 사용","m",4633,37064,0,41697,"합계"]
["MBA10110100S",null,"강관 용접 배관","D125, 옥내일반, 고소작업대 사용","m",5930,47444,0,53374,"합계"]
["MBA10110110S",null,"강관 용접 배관","D150, 옥내일반, 고소작업대 사용","m",6955,55642,0,62597,"합계"]
["MBA10110120S",null,"강관 용접 배관","D200, 옥내일반, 고소작업대 사용","m",10660,85284,0,95944,"합계"]
["MBA10110130S",null,"강관 용접 배관","D250, 옥내일반, 고소작업대 사용","m",14218,113744,0,127962,"합계"]
["MBA10110140S",null,"강관 용접 배관","D300, 옥내일반, 고소작업대 사용","m",18389,147118,0,165507,"합계"]
["MBA10110150S",null,"강관 용접 배관","D350, 옥내일반, 고소작업대 사용","m",22140,177127,0,199267,"합계"]
["MBA10110160S",null,"강관 용접 배관","D400, 옥내일반, 고소작업대 사용","m",26227,209818,0,236045,"합계"]
["MBA11010010S",null,"강관 용접 배관","D15, 기계실","m",205,13385,0,13590,"합계"]
["MBA11010020S",null,"강관 용접 배관","D20, 기계실","m",227,14794,0,15021,"합계"]
["MBA11010030S",null,"강관 용접 배관","D25, 기계실","m",283,18423,0,18706,"합계"]
["MBA11010040S",null,"강관 용접 배관","D32, 기계실","m",330,21455,0,21785,"합계"]
["MBA11010050S",null,"강관 용접 배관","D40, 기계실","m",364,23675,0,24039,"합계"]
["MBA11010060S",null,"강관 용접 배관","D50, 기계실","m",462,30038,0,30500,"합계"]
["MBA11010070S",null,"강관 용접 배관","D65, 기계실","m",542,35291,0,35833,"합계"]
["MBA11010080S",null,"강관 용접 배관","D80, 기계실","m",687,44686,0,45373,"합계"]
["MBA11010090S",null,"강관 용접 배관","D100, 기계실","m",926,60229,0,61155,"합계"]
["MBA11010100S",null,"강관 용접 배관","D125, 기계실","m",1186,77097,0,78283,"합계"]
["MBA11010110S",null,"강관 용접 배관","D150, 기계실","m",1391,90419,0,91810,"합계"]
["MBA11010120S",null,"강관 용접 배관","D200, 기계실","m",2132,138587,0,140719,"합계"]
["MBA11010130S",null,"강관 용접 배관","D250, 기계실","m",2843,184834,0,187677,"합계"]
["MBA11010140S",null,"강관 용접 배관","D300, 기계실","m",3677,239067,0,242744,"합계"]
["MBA11010150S",null,"강관 용접 배관","D350, 기계실","m",4428,287832,0,292260,"합계"]
["MBA11010160S",null,"강관 용접 배관","D400, 기계실","m",5245,340955,0,346200,"합계"]
["MBA11110010S",null,"강관 용접 배관","D15, 기계실, 고소작업대 사용","m",1029,11326,0,12355,"합계"]
["MBA11110020S",null,"강관 용접 배관","D20, 기계실, 고소작업대 사용","m",1138,12518,0,13656,"합계"]
["MBA11110030S",null,"강관 용접 배관","D25, 기계실, 고소작업대 사용","m",1417,15588,0,17005,"합계"]
["MBA11110040S",null,"강관 용접 배관","D32, 기계실, 고소작업대 사용","m",1650,18154,0,19804,"합계"]
["MBA11110050S",null,"강관 용접 배관","D40, 기계실, 고소작업대 사용","m",1821,20033,0,21854,"합계"]
["MBA11110060S",null,"강관 용접 배관","D50, 기계실, 고소작업대 사용","m",2310,25417,0,27727,"합계"]
["MBA11110070S",null,"강관 용접 배관","D65, 기계실, 고소작업대 사용","m",2714,29861,0,32575,"합계"]
["MBA11110080S",null,"강관 용접 배관","D80, 기계실, 고소작업대 사용","m",3437,37811,0,41248,"합계"]
["MBA11110090S",null,"강관 용접 배관","D100, 기계실, 고소작업대 사용","m",4633,50963,0,55596,"합계"]
["MBA11110100S",null,"강관 용접 배관","D125, 기계실, 고소작업대 사용","m",5930,65236,0,71166,"합계"]
["MBA11110110S",null,"강관 용접 배관","D150, 기계실, 고소작업대 사용","m",6955,76508,0,83463,"합계"]
["MBA11110120S",null,"강관 용접 배관","D200, 기계실, 고소작업대 사용","m",10660,117266,0,127926,"합계"]
["MBA11110130S",null,"강관 용접 배관","D250, 기계실, 고소작업대 사용","m",14218,156398,0,170616,"합계"]
["MBA11110140S",null,"강관 용접 배관","D300, 기계실, 고소작업대 사용","m",18389,202287,0,220676,"합계"]
["MBA11110150S",null,"강관 용접 배관","D350, 기계실, 고소작업대 사용","m",22140,243550,0,265690,"합계"]
["MBA11110160S",null,"강관 용접 배관","D400, 기계실, 고소작업대 사용","m",26227,288500,0,314727,"합계"]
["MBA12010010S",null,"강관 용접 배관","D15, 화장실","m",205,12356,0,12561,"합계"]
["MBA12010020S",null,"강관 용접 배관","D20, 화장실","m",227,13656,0,13883,"합계"]
["MBA12010030S",null,"강관 용접 배관","D25, 화장실","m",283,17006,0,17289,"합계"]
["MBA12010040S",null,"강관 용접 배관","D32, 화장실","m",330,19805,0,20135,"합계"]
["MBA12010050S",null,"강관 용접 배관","D40, 화장실","m",364,21854,0,22218,"합계"]
["MBA12010060S",null,"강관 용접 배관","D50, 화장실","m",462,27728,0,28190,"합계"]
["MBA12010070S",null,"강관 용접 배관","D65, 화장실","m",542,32576,0,33118,"합계"]
["MBA12010080S",null,"강관 용접 배관","D80, 화장실","m",687,41248,0,41935,"합계"]
["MBA12010090S",null,"강관 용접 배관","D100, 화장실","m",926,55596,0,56522,"합계"]
["MBA12010100S",null,"강관 용접 배관","D125, 화장실","m",1186,71166,0,72352,"합계"]
["MBA12010110S",null,"강관 용접 배관","D150, 화장실","m",1391,83463,0,84854,"합계"]
["MBA12010120S",null,"강관 용접 배관","D200, 화장실","m",2132,127927,0,130059,"합계"]
["MBA12010130S",null,"강관 용접 배관","D250, 화장실","m",2843,170616,0,173459,"합계"]
["MBA12010140S",null,"강관 용접 배관","D300, 화장실","m",3677,220677,0,224354,"합계"]
["MBA12010150S",null,"강관 용접 배관","D350, 화장실","m",4428,265691,0,270119,"합계"]
["MBA12010160S",null,"강관 용접 배관","D400, 화장실","m",5245,314727,0,319972,"합계"]
["MBA12110010S",null,"강관 용접 배관","D15, 화장실, 고소작업대 사용","m",1029,10296,0,11325,"합계"]
["MBA12110020S",null,"강관 용접 배관","D20, 화장실, 고소작업대 사용","m",1138,11380,0,12518,"합계"]
["MBA12110030S",null,"강관 용접 배관","D25, 화장실, 고소작업대 사용","m",1417,14171,0,15588,"합계"]
["MBA12110040S",null,"강관 용접 배관","D32, 화장실, 고소작업대 사용","m",1650,16504,0,18154,"합계"]
["MBA12110050S",null,"강관 용접 배관","D40, 화장실, 고소작업대 사용","m",1821,18212,0,20033,"합계"]
["MBA12110060S",null,"강관 용접 배관","D50, 화장실, 고소작업대 사용","m",2310,23106,0,25416,"합계"]
["MBA12110070S",null,"강관 용접 배관","D65, 화장실, 고소작업대 사용","m",2714,27147,0,29861,"합계"]
["MBA12110080S",null,"강관 용접 배관","D80, 화장실, 고소작업대 사용","m",3437,34374,0,37811,"합계"]
["MBA12110090S",null,"강관 용접 배관","D100, 화장실, 고소작업대 사용","m",4633,46330,0,50963,"합계"]
["MBA12110100S",null,"강관 용접 배관","D125, 화장실, 고소작업대 사용","m",5930,59305,0,65235,"합계"]
["MBA12110110S",null,"강관 용접 배관","D150, 화장실, 고소작업대 사용","m",6955,69553,0,76508,"합계"]
["MBA12110120S",null,"강관 용접 배관","D200, 화장실, 고소작업대 사용","m",10660,106606,0,117266,"합계"]
["MBA12110130S",null,"강관 용접 배관","D250, 화장실, 고소작업대 사용","m",14218,142180,0,156398,"합계"]
["MBA12110140S",null,"강관 용접 배관","D300, 화장실, 고소작업대 사용","m",18389,183897,0,202286,"합계"]
["MBA12110150S",null,"강관 용접 배관","D350, 화장실, 고소작업대 사용","m",22140,221409,0,243549,"합계"]
["MBA12110160S",null,"강관 용접 배관","D400, 화장실, 고소작업대 사용","m",26227,262273,0,288500,"합계"]
["MBA13010010S",null,"강관 용접 배관","D15, 옥외배관","m",205,9267,0,9472,"합계"]
["MBA13010020S",null,"강관 용접 배관","D20, 옥외배관","m",227,10242,0,10469,"합계"]
["MBA13010030S",null,"강관 용접 배관","D25, 옥외배관","m",283,12754,0,13037,"합계"]
["MBA13010040S",null,"강관 용접 배관","D32, 옥외배관","m",330,14853,0,15183,"합계"]
["MBA13010050S",null,"강관 용접 배관","D40, 옥외배관","m",364,16390,0,16754,"합계"]
["MBA13010060S",null,"강관 용접 배관","D50, 옥외배관","m",462,20796,0,21258,"합계"]
["MBA13010070S",null,"강관 용접 배관","D65, 옥외배관","m",542,24432,0,24974,"합계"]
["MBA13010080S",null,"강관 용접 배관","D80, 옥외배관","m",687,30936,0,31623,"합계"]
["MBA13010090S",null,"강관 용접 배관","D100, 옥외배관","m",926,41697,0,42623,"합계"]
["MBA13010100S",null,"강관 용접 배관","D125, 옥외배관","m",1186,53374,0,54560,"합계"]
["MBA13010110S",null,"강관 용접 배관","D150, 옥외배관","m",1391,62597,0,63988,"합계"]
["MBA13010120S",null,"강관 용접 배관","D200, 옥외배관","m",2132,95945,0,98077,"합계"]
["MBA13010130S",null,"강관 용접 배관","D250, 옥외배관","m",2843,127962,0,130805,"합계"]
["MBA13010140S",null,"강관 용접 배관","D300, 옥외배관","m",3677,165508,0,169185,"합계"]
["MBA13010150S",null,"강관 용접 배관","D350, 옥외배관","m",4428,199268,0,203696,"합계"]
["MBA13010160S",null,"강관 용접 배관","D400, 옥외배관","m",5245,236045,0,241290,"합계"]
["MBA13110010S",null,"강관 용접 배관","D15, 옥외배관, 고소작업대 사용","m",1029,7207,0,8236,"합계"]
["MBA13110020S",null,"강관 용접 배관","D20, 옥외배관, 고소작업대 사용","m",1138,7966,0,9104,"합계"]
["MBA13110030S",null,"강관 용접 배관","D25, 옥외배관, 고소작업대 사용","m",1417,9920,0,11337,"합계"]
["MBA13110040S",null,"강관 용접 배관","D32, 옥외배관, 고소작업대 사용","m",1650,11553,0,13203,"합계"]
["MBA13110050S",null,"강관 용접 배관","D40, 옥외배관, 고소작업대 사용","m",1821,12748,0,14569,"합계"]
["MBA13110060S",null,"강관 용접 배관","D50, 옥외배관, 고소작업대 사용","m",2310,16174,0,18484,"합계"]
["MBA13110070S",null,"강관 용접 배관","D65, 옥외배관, 고소작업대 사용","m",2714,19003,0,21717,"합계"]
["MBA13110080S",null,"강관 용접 배관","D80, 옥외배관, 고소작업대 사용","m",3437,24061,0,27498,"합계"]
["MBA13110090S",null,"강관 용접 배관","D100, 옥외배관, 고소작업대 사용","m",4633,32431,0,37064,"합계"]
["MBA13110100S",null,"강관 용접 배관","D125, 옥외배관, 고소작업대 사용","m",5930,41513,0,47443,"합계"]
["MBA13110110S",null,"강관 용접 배관","D150, 옥외배관, 고소작업대 사용","m",6955,48687,0,55642,"합계"]
["MBA13110120S",null,"강관 용접 배관","D200, 옥외배관, 고소작업대 사용","m",10660,74624,0,85284,"합계"]
["MBA13110130S",null,"강관 용접 배관","D250, 옥외배관, 고소작업대 사용","m",14218,99526,0,113744,"합계"]
["MBA13110140S",null,"강관 용접 배관","D300, 옥외배관, 고소작업대 사용","m",18389,128728,0,147117,"합계"]
["MBA13110150S",null,"강관 용접 배관","D350, 옥외배관, 고소작업대 사용","m",22140,154986,0,177126,"합계"]
["MBA13110160S",null,"강관 용접 배관","D400, 옥외배관, 고소작업대 사용","m",26227,183591,0,209818,"합계"]
["MBA20010010S",null,"나사식 접합 및 배관","D15, 옥내일반","m",247,12373,0,12620,"합계"]
["MBA20010020S",null,"나사식 접합 및 배관","D20, 옥내일반","m",273,13686,0,13959,"합계"]
["MBA20010030S",null,"나사식 접합 및 배관","D25, 옥내일반","m",346,17332,0,17678,"합계"]
["MBA20010040S",null,"나사식 접합 및 배관","D32, 옥내일반","m",407,20352,0,20759,"합계"]
["MBA20010050S",null,"나사식 접합 및 배관","D40, 옥내일반","m",445,22290,0,22735,"합계"]
["MBA20010060S",null,"나사식 접합 및 배관","D50, 옥내일반","m",574,28727,0,29301,"합계"]
["MBA20110010S",null,"나사식 접합 및 배관","D15, 옥내일반, 고소작업대 사용","m",1237,9898,0,11135,"합계"]
["MBA20110020S",null,"나사식 접합 및 배관","D20, 옥내일반, 고소작업대 사용","m",1368,10949,0,12317,"합계"]
["MBA20110030S",null,"나사식 접합 및 배관","D25, 옥내일반, 고소작업대 사용","m",1733,13865,0,15598,"합계"]
["MBA20110040S",null,"나사식 접합 및 배관","D32, 옥내일반, 고소작업대 사용","m",2035,16282,0,18317,"합계"]
["MBA20110050S",null,"나사식 접합 및 배관","D40, 옥내일반, 고소작업대 사용","m",2229,17832,0,20061,"합계"]
["MBA20110060S",null,"나사식 접합 및 배관","D50, 옥내일반, 고소작업대 사용","m",2872,22981,0,25853,"합계"]
["MBA21010010S",null,"나사식 접합 및 배관","D15, 기계실","m",247,16085,0,16332,"합계"]
["MBA21010020S",null,"나사식 접합 및 배관","D20, 기계실","m",273,17792,0,18065,"합계"]
["MBA21010030S",null,"나사식 접합 및 배관","D25, 기계실","m",346,22531,0,22877,"합계"]
["MBA21010040S",null,"나사식 접합 및 배관","D32, 기계실","m",407,26458,0,26865,"합계"]
["MBA21010050S",null,"나사식 접합 및 배관","D40, 기계실","m",445,28977,0,29422,"합계"]
["MBA21010060S",null,"나사식 접합 및 배관","D50, 기계실","m",574,37345,0,37919,"합계"]
["MBA21110010S",null,"나사식 접합 및 배관","D15, 기계실, 고소작업대 사용","m",1237,13611,0,14848,"합계"]
["MBA21110020S",null,"나사식 접합 및 배관","D20, 기계실, 고소작업대 사용","m",1368,15055,0,16423,"합계"]
["MBA21110030S",null,"나사식 접합 및 배관","D25, 기계실, 고소작업대 사용","m",1733,19065,0,20798,"합계"]
["MBA21110040S",null,"나사식 접합 및 배관","D32, 기계실, 고소작업대 사용","m",2035,22388,0,24423,"합계"]
["MBA21110050S",null,"나사식 접합 및 배관","D40, 기계실, 고소작업대 사용","m",2229,24519,0,26748,"합계"]
["MBA21110060S",null,"나사식 접합 및 배관","D50, 기계실, 고소작업대 사용","m",2872,31600,0,34472,"합계"]
["MBA22010010S",null,"나사식 접합 및 배관","D15, 화장실","m",247,14848,0,15095,"합계"]
["MBA22010020S",null,"나사식 접합 및 배관","D20, 화장실","m",273,16423,0,16696,"합계"]
["MBA22010030S",null,"나사식 접합 및 배관","D25, 화장실","m",346,20798,0,21144,"합계"]
["MBA22010040S",null,"나사식 접합 및 배관","D32, 화장실","m",407,24423,0,24830,"합계"]
["MBA22010050S",null,"나사식 접합 및 배관","D40, 화장실","m",445,26748,0,27193,"합계"]
["MBA22010060S",null,"나사식 접합 및 배관","D50, 화장실","m",574,34472,0,35046,"합계"]
["MBA22110010S",null,"나사식 접합 및 배관","D15, 화장실, 고소작업대 사용","m",1237,12373,0,13610,"합계"]
["MBA22110020S",null,"나사식 접합 및 배관","D20, 화장실, 고소작업대 사용","m",1368,13686,0,15054,"합계"]
["MBA22110030S",null,"나사식 접합 및 배관","D25, 화장실, 고소작업대 사용","m",1733,17332,0,19065,"합계"]
["MBA22110040S",null,"나사식 접합 및 배관","D32, 화장실, 고소작업대 사용","m",2035,20352,0,22387,"합계"]
["MBA22110050S",null,"나사식 접합 및 배관","D40, 화장실, 고소작업대 사용","m",2229,22290,0,24519,"합계"]
["MBA22110060S",null,"나사식 접합 및 배관","D50, 화장실, 고소작업대 사용","m",2872,28727,0,31599,"합계"]
["MBA23010010S",null,"나사식 접합 및 배관","D15, 옥외배관","m",247,11136,0,11383,"합계"]
["MBA23010020S",null,"나사식 접합 및 배관","D20, 옥외배관","m",273,12317,0,12590,"합계"]
["MBA23010030S",null,"나사식 접합 및 배관","D25, 옥외배관","m",346,15598,0,15944,"합계"]
["MBA23010040S",null,"나사식 접합 및 배관","D32, 옥외배관","m",407,18317,0,18724,"합계"]
["MBA23010050S",null,"나사식 접합 및 배관","D40, 옥외배관","m",445,20061,0,20506,"합계"]
["MBA23010060S",null,"나사식 접합 및 배관","D50, 옥외배관","m",574,25854,0,26428,"합계"]
["MBA23110010S",null,"나사식 접합 및 배관","D15, 옥외배관, 고소작업대 사용","m",1237,8661,0,9898,"합계"]
["MBA23110020S",null,"나사식 접합 및 배관","D20, 옥외배관, 고소작업대 사용","m",1368,9580,0,10948,"합계"]
["MBA23110030S",null,"나사식 접합 및 배관","D25, 옥외배관, 고소작업대 사용","m",1733,12132,0,13865,"합계"]
["MBA23110040S",null,"나사식 접합 및 배관","D32, 옥외배관, 고소작업대 사용","m",2035,14247,0,16282,"합계"]
["MBA23110050S",null,"나사식 접합 및 배관","D40, 옥외배관, 고소작업대 사용","m",2229,15603,0,17832,"합계"]
["MBA23110060S",null,"나사식 접합 및 배관","D50, 옥외배관, 고소작업대 사용","m",2872,20109,0,22981,"합계"]
["MBA30010010S",null,"그루브조인트식 접합 및 배관","D25, 옥내일반","m",310,15548,0,15858,"합계"]
["MBA30010020S",null,"그루브조인트식 접합 및 배관","D32, 옥내일반","m",379,18964,0,19343,"합계"]
["MBA30010030S",null,"그루브조인트식 접합 및 배관","D40, 옥내일반","m",422,21131,0,21553,"합계"]
["MBA30010040S",null,"그루브조인트식 접합 및 배관","D50, 옥내일반","m",559,27963,0,28522,"합계"]
["MBA30010050S",null,"그루브조인트식 접합 및 배관","D65, 옥내일반","m",663,33151,0,33814,"합계"]
["MBA30010060S",null,"그루브조인트식 접합 및 배관","D80, 옥내일반","m",844,42214,0,43058,"합계"]
["MBA30010070S",null,"그루브조인트식 접합 및 배관","D100, 옥내일반","m",1226,61348,0,62574,"합계"]
["MBA30010080S",null,"그루브조인트식 접합 및 배관","D125, 옥내일반","m",1454,72743,0,74197,"합계"]
["MBA30010090S",null,"그루브조인트식 접합 및 배관","D150, 옥내일반","m",1769,88461,0,90230,"합계"]
["MBA30010100S",null,"그루브조인트식 접합 및 배관","D200, 옥내일반","m",2421,121093,0,123514,"합계"]
["MBA30010110S",null,"그루브조인트식 접합 및 배관","D250, 옥내일반","m",3131,156569,0,159700,"합계"]
["MBA30010120S",null,"그루브조인트식 접합 및 배관","D300, 옥내일반","m",3915,195769,0,199684,"합계"]
["MBA30010130S",null,"그루브조인트식 접합 및 배관","D350, 옥내일반","m",4687,234394,0,239081,"합계"]
["MBA30010140S",null,"그루브조인트식 접합 및 배관","D400, 옥내일반","m",5522,276104,0,281626,"합계"]
["MBA30010150S",null,"그루브조인트식 접합 및 배관","D450, 옥내일반","m",6192,309642,0,315834,"합계"]
["MBA30010160S",null,"그루브조인트식 접합 및 배관","D500, 옥내일반","m",6863,343181,0,350044,"합계"]
["MBA30010170S",null,"그루브조인트식 접합 및 배관","D550, 옥내일반","m",7508,375406,0,382914,"합계"]
["MBA30010180S",null,"그루브조인트식 접합 및 배관","D600, 옥내일반","m",8183,409175,0,417358,"합계"]
["MBA30110010S",null,"그루브조인트식 접합 및 배관","D25, 옥내일반, 고소작업대 사용","m",1554,12438,0,13992,"합계"]
["MBA30110020S",null,"그루브조인트식 접합 및 배관","D32, 옥내일반, 고소작업대 사용","m",1896,15171,0,17067,"합계"]
["MBA30110030S",null,"그루브조인트식 접합 및 배관","D40, 옥내일반, 고소작업대 사용","m",2113,16905,0,19018,"합계"]
["MBA30110040S",null,"그루브조인트식 접합 및 배관","D50, 옥내일반, 고소작업대 사용","m",2796,22370,0,25166,"합계"]
["MBA30110050S",null,"그루브조인트식 접합 및 배관","D65, 옥내일반, 고소작업대 사용","m",3315,26521,0,29836,"합계"]
["MBA30110060S",null,"그루브조인트식 접합 및 배관","D80, 옥내일반, 고소작업대 사용","m",4221,33771,0,37992,"합계"]
["MBA30110070S",null,"그루브조인트식 접합 및 배관","D100, 옥내일반, 고소작업대 사용","m",6134,49078,0,55212,"합계"]
["MBA30110080S",null,"그루브조인트식 접합 및 배관","D125, 옥내일반, 고소작업대 사용","m",7274,58194,0,65468,"합계"]
["MBA30110090S",null,"그루브조인트식 접합 및 배관","D150, 옥내일반, 고소작업대 사용","m",8846,70768,0,79614,"합계"]
["MBA30110100S",null,"그루브조인트식 접합 및 배관","D200, 옥내일반, 고소작업대 사용","m",12109,96874,0,108983,"합계"]
["MBA30110110S",null,"그루브조인트식 접합 및 배관","D250, 옥내일반, 고소작업대 사용","m",15656,125255,0,140911,"합계"]
["MBA30110120S",null,"그루브조인트식 접합 및 배관","D300, 옥내일반, 고소작업대 사용","m",19576,156615,0,176191,"합계"]
["MBA30110130S",null,"그루브조인트식 접합 및 배관","D350, 옥내일반, 고소작업대 사용","m",23439,187515,0,210954,"합계"]
["MBA30110140S",null,"그루브조인트식 접합 및 배관","D400, 옥내일반, 고소작업대 사용","m",27610,220883,0,248493,"합계"]
["MBA30110150S",null,"그루브조인트식 접합 및 배관","D450, 옥내일반, 고소작업대 사용","m",30964,247714,0,278678,"합계"]
["MBA30110160S",null,"그루브조인트식 접합 및 배관","D500, 옥내일반, 고소작업대 사용","m",34318,274544,0,308862,"합계"]
["MBA30110170S",null,"그루브조인트식 접합 및 배관","D550, 옥내일반, 고소작업대 사용","m",37540,300325,0,337865,"합계"]
["MBA30110180S",null,"그루브조인트식 접합 및 배관","D600, 옥내일반, 고소작업대 사용","m",40917,327340,0,368257,"합계"]
["MBA31010010S",null,"그루브조인트식 접합 및 배관","D25, 기계실","m",310,20213,0,20523,"합계"]
["MBA31010020S",null,"그루브조인트식 접합 및 배관","D32, 기계실","m",379,24654,0,25033,"합계"]
["MBA31010030S",null,"그루브조인트식 접합 및 배관","D40, 기계실","m",422,27471,0,27893,"합계"]
["MBA31010040S",null,"그루브조인트식 접합 및 배관","D50, 기계실","m",559,36352,0,36911,"합계"]
["MBA31010050S",null,"그루브조인트식 접합 및 배관","D65, 기계실","m",663,43096,0,43759,"합계"]
["MBA31010060S",null,"그루브조인트식 접합 및 배관","D80, 기계실","m",844,54878,0,55722,"합계"]
["MBA31010070S",null,"그루브조인트식 접합 및 배관","D100, 기계실","m",1226,79752,0,80978,"합계"]
["MBA31010080S",null,"그루브조인트식 접합 및 배관","D125, 기계실","m",1454,94566,0,96020,"합계"]
["MBA31010090S",null,"그루브조인트식 접합 및 배관","D150, 기계실","m",1769,114999,0,116768,"합계"]
["MBA31010100S",null,"그루브조인트식 접합 및 배관","D200, 기계실","m",2421,157421,0,159842,"합계"]
["MBA31010110S",null,"그루브조인트식 접합 및 배관","D250, 기계실","m",3131,203539,0,206670,"합계"]
["MBA31010120S",null,"그루브조인트식 접합 및 배관","D300, 기계실","m",3915,254500,0,258415,"합계"]
["MBA31010130S",null,"그루브조인트식 접합 및 배관","D350, 기계실","m",4687,304712,0,309399,"합계"]
["MBA31010140S",null,"그루브조인트식 접합 및 배관","D400, 기계실","m",5522,358935,0,364457,"합계"]
["MBA31010150S",null,"그루브조인트식 접합 및 배관","D450, 기계실","m",6192,402535,0,408727,"합계"]
["MBA31010160S",null,"그루브조인트식 접합 및 배관","D500, 기계실","m",6863,446135,0,452998,"합계"]
["MBA31010170S",null,"그루브조인트식 접합 및 배관","D550, 기계실","m",7508,488028,0,495536,"합계"]
["MBA31010180S",null,"그루브조인트식 접합 및 배관","D600, 기계실","m",8183,531927,0,540110,"합계"]
["MBA31110010S",null,"그루브조인트식 접합 및 배관","D25, 기계실, 고소작업대 사용","m",1554,17103,0,18657,"합계"]
["MBA31110020S",null,"그루브조인트식 접합 및 배관","D32, 기계실, 고소작업대 사용","m",1896,20861,0,22757,"합계"]
["MBA31110030S",null,"그루브조인트식 접합 및 배관","D40, 기계실, 고소작업대 사용","m",2113,23244,0,25357,"합계"]
["MBA31110040S",null,"그루브조인트식 접합 및 배관","D50, 기계실, 고소작업대 사용","m",2796,30759,0,33555,"합계"]
["MBA31110050S",null,"그루브조인트식 접합 및 배관","D65, 기계실, 고소작업대 사용","m",3315,36466,0,39781,"합계"]
["MBA31110060S",null,"그루브조인트식 접합 및 배관","D80, 기계실, 고소작업대 사용","m",4221,46435,0,50656,"합계"]
["MBA31110070S",null,"그루브조인트식 접합 및 배관","D100, 기계실, 고소작업대 사용","m",6134,67482,0,73616,"합계"]
["MBA31110080S",null,"그루브조인트식 접합 및 배관","D125, 기계실, 고소작업대 사용","m",7274,80017,0,87291,"합계"]
["MBA31110090S",null,"그루브조인트식 접합 및 배관","D150, 기계실, 고소작업대 사용","m",8846,97307,0,106153,"합계"]
["MBA31110100S",null,"그루브조인트식 접합 및 배관","D200, 기계실, 고소작업대 사용","m",12109,133202,0,145311,"합계"]
["MBA31110110S",null,"그루브조인트식 접합 및 배관","D250, 기계실, 고소작업대 사용","m",15656,172226,0,187882,"합계"]
["MBA31110120S",null,"그루브조인트식 접합 및 배관","D300, 기계실, 고소작업대 사용","m",19576,215346,0,234922,"합계"]
["MBA31110130S",null,"그루브조인트식 접합 및 배관","D350, 기계실, 고소작업대 사용","m",23439,257833,0,281272,"합계"]
["MBA31110140S",null,"그루브조인트식 접합 및 배관","D400, 기계실, 고소작업대 사용","m",27610,303714,0,331324,"합계"]
["MBA31110150S",null,"그루브조인트식 접합 및 배관","D450, 기계실, 고소작업대 사용","m",30964,340606,0,371570,"합계"]
["MBA31110160S",null,"그루브조인트식 접합 및 배관","D500, 기계실, 고소작업대 사용","m",34318,377499,0,411817,"합계"]
["MBA31110170S",null,"그루브조인트식 접합 및 배관","D550, 기계실, 고소작업대 사용","m",37540,412947,0,450487,"합계"]
["MBA31110180S",null,"그루브조인트식 접합 및 배관","D600, 기계실, 고소작업대 사용","m",40917,450092,0,491009,"합계"]
["MBA32010010S",null,"그루브조인트식 접합 및 배관","D25, 화장실","m",310,18658,0,18968,"합계"]
["MBA32010020S",null,"그루브조인트식 접합 및 배관","D32, 화장실","m",379,22757,0,23136,"합계"]
["MBA32010030S",null,"그루브조인트식 접합 및 배관","D40, 화장실","m",422,25357,0,25779,"합계"]
["MBA32010040S",null,"그루브조인트식 접합 및 배관","D50, 화장실","m",559,33556,0,34115,"합계"]
["MBA32010050S",null,"그루브조인트식 접합 및 배관","D65, 화장실","m",663,39781,0,40444,"합계"]
["MBA32010060S",null,"그루브조인트식 접합 및 배관","D80, 화장실","m",844,50657,0,51501,"합계"]
["MBA32010070S",null,"그루브조인트식 접합 및 배관","D100, 화장실","m",1226,73617,0,74843,"합계"]
["MBA32010080S",null,"그루브조인트식 접합 및 배관","D125, 화장실","m",1454,87291,0,88745,"합계"]
["MBA32010090S",null,"그루브조인트식 접합 및 배관","D150, 화장실","m",1769,106153,0,107922,"합계"]
["MBA32010100S",null,"그루브조인트식 접합 및 배관","D200, 화장실","m",2421,145311,0,147732,"합계"]
["MBA32010110S",null,"그루브조인트식 접합 및 배관","D250, 화장실","m",3131,187883,0,191014,"합계"]
["MBA32010120S",null,"그루브조인트식 접합 및 배관","D300, 화장실","m",3915,234923,0,238838,"합계"]
["MBA32010130S",null,"그루브조인트식 접합 및 배관","D350, 화장실","m",4687,281273,0,285960,"합계"]
["MBA32010140S",null,"그루브조인트식 접합 및 배관","D400, 화장실","m",5522,331324,0,336846,"합계"]
["MBA32010150S",null,"그루브조인트식 접합 및 배관","D450, 화장실","m",6192,371571,0,377763,"합계"]
["MBA32010160S",null,"그루브조인트식 접합 및 배관","D500, 화장실","m",6863,411817,0,418680,"합계"]
["MBA32010170S",null,"그루브조인트식 접합 및 배관","D550, 화장실","m",7508,450488,0,457996,"합계"]
["MBA32010180S",null,"그루브조인트식 접합 및 배관","D600, 화장실","m",8183,491010,0,499193,"합계"]
["MBA32110010S",null,"그루브조인트식 접합 및 배관","D25, 화장실, 고소작업대 사용","m",1554,15548,0,17102,"합계"]
["MBA32110020S",null,"그루브조인트식 접합 및 배관","D32, 화장실, 고소작업대 사용","m",1896,18964,0,20860,"합계"]
["MBA32110030S",null,"그루브조인트식 접합 및 배관","D40, 화장실, 고소작업대 사용","m",2113,21131,0,23244,"합계"]
["MBA32110040S",null,"그루브조인트식 접합 및 배관","D50, 화장실, 고소작업대 사용","m",2796,27963,0,30759,"합계"]
["MBA32110050S",null,"그루브조인트식 접합 및 배관","D65, 화장실, 고소작업대 사용","m",3315,33151,0,36466,"합계"]
["MBA32110060S",null,"그루브조인트식 접합 및 배관","D80, 화장실, 고소작업대 사용","m",4221,42214,0,46435,"합계"]
["MBA32110070S",null,"그루브조인트식 접합 및 배관","D100, 화장실, 고소작업대 사용","m",6134,61348,0,67482,"합계"]
["MBA32110080S",null,"그루브조인트식 접합 및 배관","D125, 화장실, 고소작업대 사용","m",7274,72743,0,80017,"합계"]
["MBA32110090S",null,"그루브조인트식 접합 및 배관","D150, 화장실, 고소작업대 사용","m",8846,88461,0,97307,"합계"]
["MBA32110100S",null,"그루브조인트식 접합 및 배관","D200, 화장실, 고소작업대 사용","m",12109,121093,0,133202,"합계"]
["MBA32110110S",null,"그루브조인트식 접합 및 배관","D250, 화장실, 고소작업대 사용","m",15656,156569,0,172225,"합계"]
["MBA32110120S",null,"그루브조인트식 접합 및 배관","D300, 화장실, 고소작업대 사용","m",19576,195769,0,215345,"합계"]
["MBA32110130S",null,"그루브조인트식 접합 및 배관","D350, 화장실, 고소작업대 사용","m",23439,234394,0,257833,"합계"]
["MBA32110140S",null,"그루브조인트식 접합 및 배관","D400, 화장실, 고소작업대 사용","m",27610,276104,0,303714,"합계"]
["MBA32110150S",null,"그루브조인트식 접합 및 배관","D450, 화장실, 고소작업대 사용","m",30964,309642,0,340606,"합계"]
["MBA32110160S",null,"그루브조인트식 접합 및 배관","D500, 화장실, 고소작업대 사용","m",34318,343181,0,377499,"합계"]
["MBA32110170S",null,"그루브조인트식 접합 및 배관","D550, 화장실, 고소작업대 사용","m",37540,375406,0,412946,"합계"]
["MBA32110180S",null,"그루브조인트식 접합 및 배관","D600, 화장실, 고소작업대 사용","m",40917,409175,0,450092,"합계"]
["MBA33010010S",null,"그루브조인트식 접합 및 배관","D25, 옥외배관","m",310,13993,0,14303,"합계"]
["MBA33010020S",null,"그루브조인트식 접합 및 배관","D32, 옥외배관","m",379,17068,0,17447,"합계"]
["MBA33010030S",null,"그루브조인트식 접합 및 배관","D40, 옥외배관","m",422,19018,0,19440,"합계"]
["MBA33010040S",null,"그루브조인트식 접합 및 배관","D50, 옥외배관","m",559,25167,0,25726,"합계"]
["MBA33010050S",null,"그루브조인트식 접합 및 배관","D65, 옥외배관","m",663,29836,0,30499,"합계"]
["MBA33010060S",null,"그루브조인트식 접합 및 배관","D80, 옥외배관","m",844,37992,0,38836,"합계"]
["MBA33010070S",null,"그루브조인트식 접합 및 배관","D100, 옥외배관","m",1226,55213,0,56439,"합계"]
["MBA33010080S",null,"그루브조인트식 접합 및 배관","D125, 옥외배관","m",1454,65468,0,66922,"합계"]
["MBA33010090S",null,"그루브조인트식 접합 및 배관","D150, 옥외배관","m",1769,79614,0,81383,"합계"]
["MBA33010100S",null,"그루브조인트식 접합 및 배관","D200, 옥외배관","m",2421,108983,0,111404,"합계"]
["MBA33010110S",null,"그루브조인트식 접합 및 배관","D250, 옥외배관","m",3131,140912,0,144043,"합계"]
["MBA33010120S",null,"그루브조인트식 접합 및 배관","D300, 옥외배관","m",3915,176192,0,180107,"합계"]
["MBA33010130S",null,"그루브조인트식 접합 및 배관","D350, 옥외배관","m",4687,210954,0,215641,"합계"]
["MBA33010140S",null,"그루브조인트식 접합 및 배관","D400, 옥외배관","m",5522,248493,0,254015,"합계"]
["MBA33010150S",null,"그루브조인트식 접합 및 배관","D450, 옥외배관","m",6192,278678,0,284870,"합계"]
["MBA33010160S",null,"그루브조인트식 접합 및 배관","D500, 옥외배관","m",6863,308863,0,315726,"합계"]
["MBA33010170S",null,"그루브조인트식 접합 및 배관","D550, 옥외배관","m",7508,337866,0,345374,"합계"]
["MBA33010180S",null,"그루브조인트식 접합 및 배관","D600, 옥외배관","m",8183,368257,0,376440,"합계"]
["MBA33110010S",null,"그루브조인트식 접합 및 배관","D25, 옥외배관, 고소작업대 사용","m",1554,10884,0,12438,"합계"]
["MBA33110020S",null,"그루브조인트식 접합 및 배관","D32, 옥외배관, 고소작업대 사용","m",1896,13275,0,15171,"합계"]
["MBA33110030S",null,"그루브조인트식 접합 및 배관","D40, 옥외배관, 고소작업대 사용","m",2113,14792,0,16905,"합계"]
["MBA33110040S",null,"그루브조인트식 접합 및 배관","D50, 옥외배관, 고소작업대 사용","m",2796,19574,0,22370,"합계"]
["MBA33110050S",null,"그루브조인트식 접합 및 배관","D65, 옥외배관, 고소작업대 사용","m",3315,23205,0,26520,"합계"]
["MBA33110060S",null,"그루브조인트식 접합 및 배관","D80, 옥외배관, 고소작업대 사용","m",4221,29549,0,33770,"합계"]
["MBA33110070S",null,"그루브조인트식 접합 및 배관","D100, 옥외배관, 고소작업대 사용","m",6134,42943,0,49077,"합계"]
["MBA33110080S",null,"그루브조인트식 접합 및 배관","D125, 옥외배관, 고소작업대 사용","m",7274,50920,0,58194,"합계"]
["MBA33110090S",null,"그루브조인트식 접합 및 배관","D150, 옥외배관, 고소작업대 사용","m",8846,61922,0,70768,"합계"]
["MBA33110100S",null,"그루브조인트식 접합 및 배관","D200, 옥외배관, 고소작업대 사용","m",12109,84765,0,96874,"합계"]
["MBA33110110S",null,"그루브조인트식 접합 및 배관","D250, 옥외배관, 고소작업대 사용","m",15656,109598,0,125254,"합계"]
["MBA33110120S",null,"그루브조인트식 접합 및 배관","D300, 옥외배관, 고소작업대 사용","m",19576,137038,0,156614,"합계"]
["MBA33110130S",null,"그루브조인트식 접합 및 배관","D350, 옥외배관, 고소작업대 사용","m",23439,164076,0,187515,"합계"]
["MBA33110140S",null,"그루브조인트식 접합 및 배관","D400, 옥외배관, 고소작업대 사용","m",27610,193272,0,220882,"합계"]
["MBA33110150S",null,"그루브조인트식 접합 및 배관","D450, 옥외배관, 고소작업대 사용","m",30964,216749,0,247713,"합계"]
["MBA33110160S",null,"그루브조인트식 접합 및 배관","D500, 옥외배관, 고소작업대 사용","m",34318,240226,0,274544,"합계"]
["MBA33110170S",null,"그루브조인트식 접합 및 배관","D550, 옥외배관, 고소작업대 사용","m",37540,262784,0,300324,"합계"]
["MBA33110180S",null,"그루브조인트식 접합 및 배관","D600, 옥외배관, 고소작업대 사용","m",40917,286422,0,327339,"합계"]
["MBC00010010S",null,"동관 용접 접합","D8","개소",112,3738,0,3850,"합계"]
["MBC00010020S",null,"동관 용접 접합","D10","개소",144,4806,0,4950,"합계"]
["MBC00010030S",null,"동관 용접 접합","D15","개소",176,5874,0,6050,"합계"]
["MBC00010040S",null,"동관 용접 접합","D20","개소",240,8010,0,8250,"합계"]
["MBC00010050S",null,"동관 용접 접합","D25","개소",304,10146,0,10450,"합계"]
["MBC00010060S",null,"동관 용접 접합","D32","개소",360,12015,0,12375,"합계"]
["MBC00010070S",null,"동관 용접 접합","D40","개소",424,14152,0,14576,"합계"]
["MBC00010080S",null,"동관 용접 접합","D50","개소",536,17890,0,18426,"합계"]
["MBC00010090S",null,"동관 용접 접합","D65","개소",712,23764,0,24476,"합계"]
["MBC00010100S",null,"동관 용접 접합","D80","개소",841,28037,0,28878,"합계"]
["MBC00010110S",null,"동관 용접 접합","D100","개소",1097,36581,0,37678,"합계"]
["MBC00010120S",null,"동관 용접 접합","D125","개소",1353,45126,0,46479,"합계"]
["MBC00010130S",null,"동관 용접 접합","D150","개소",1610,53671,0,55281,"합계"]
["MBC00010140S",null,"동관 용접 접합","D200","개소",2122,70760,0,72882,"합계"]
["MBC00010150S",null,"동관 용접 접합","D250","개소",2635,87849,0,90484,"합계"]
["MBC00110010S",null,"동관 용접 접합","D8, 고소작업대 사용","개소",485,2990,0,3475,"합계"]
["MBC00110020S",null,"동관 용접 접합","D10, 고소작업대 사용","개소",624,3845,0,4469,"합계"]
["MBC00110030S",null,"동관 용접 접합","D15, 고소작업대 사용","개소",763,4699,0,5462,"합계"]
["MBC00110040S",null,"동관 용접 접합","D20, 고소작업대 사용","개소",1041,6408,0,7449,"합계"]
["MBC00110050S",null,"동관 용접 접합","D25, 고소작업대 사용","개소",1319,8117,0,9436,"합계"]
["MBC00110060S",null,"동관 용접 접합","D32, 고소작업대 사용","개소",1562,9612,0,11174,"합계"]
["MBC00110070S",null,"동관 용접 접합","D40, 고소작업대 사용","개소",1839,11321,0,13160,"합계"]
["MBC00110080S",null,"동관 용접 접합","D50, 고소작업대 사용","개소",2325,14312,0,16637,"합계"]
["MBC00110090S",null,"동관 용접 접합","D65, 고소작업대 사용","개소",3089,19011,0,22100,"합계"]
["MBC00110100S",null,"동관 용접 접합","D80, 고소작업대 사용","개소",3644,22429,0,26073,"합계"]
["MBC00110110S",null,"동관 용접 접합","D100, 고소작업대 사용","개소",4755,29265,0,34020,"합계"]
["MBC00110120S",null,"동관 용접 접합","D125, 고소작업대 사용","개소",5866,36101,0,41967,"합계"]
["MBC00110130S",null,"동관 용접 접합","D150, 고소작업대 사용","개소",6977,42936,0,49913,"합계"]
["MBC00110140S",null,"동관 용접 접합","D200, 고소작업대 사용","개소",9198,56608,0,65806,"합계"]
["MBC00110150S",null,"동관 용접 접합","D250, 고소작업대 사용","개소",11420,70279,0,81699,"합계"]
["MBC10010010S",null,"동관 용접 배관","D8, 옥내일반","m",129,6474,0,6603,"합계"]
["MBC10010020S",null,"동관 용접 배관","D10, 옥내일반","m",148,7430,0,7578,"합계"]
["MBC10010030S",null,"동관 용접 배관","D15, 옥내일반","m",172,8615,0,8787,"합계"]
["MBC10010040S",null,"동관 용접 배관","D20, 옥내일반","m",203,10195,0,10398,"합계"]
["MBC10010050S",null,"동관 용접 배관","D25, 옥내일반","m",247,12399,0,12646,"합계"]
["MBC10010060S",null,"동관 용접 배관","D32, 옥내일반","m",297,14898,0,15195,"합계"]
["MBC10010070S",null,"동관 용접 배관","D40, 옥내일반","m",347,17395,0,17742,"합계"]
["MBC10010080S",null,"동관 용접 배관","D50, 옥내일반","m",455,22787,0,23242,"합계"]
["MBC10010090S",null,"동관 용접 배관","D65, 옥내일반","m",536,26827,0,27363,"합계"]
["MBC10010100S",null,"동관 용접 배관","D80, 옥내일반","m",672,33633,0,34305,"합계"]
["MBC10010110S",null,"동관 용접 배관","D100, 옥내일반","m",911,45562,0,46473,"합계"]
["MBC10010120S",null,"동관 용접 배관","D125, 옥내일반","m",1134,56702,0,57836,"합계"]
["MBC10010130S",null,"동관 용접 배관","D150, 옥내일반","m",1361,68071,0,69432,"합계"]
["MBC10010140S",null,"동관 용접 배관","D200, 옥내일반","m",2024,101222,0,103246,"합계"]
["MBC10010150S",null,"동관 용접 배관","D250, 옥내일반","m",2674,133712,0,136386,"합계"]
["MBC10110010S",null,"동관 용접 배관","D8, 옥내일반, 고소작업대 사용","m",647,5179,0,5826,"합계"]
["MBC10110020S",null,"동관 용접 배관","D10, 옥내일반, 고소작업대 사용","m",743,5944,0,6687,"합계"]
["MBC10110030S",null,"동관 용접 배관","D15, 옥내일반, 고소작업대 사용","m",861,6892,0,7753,"합계"]
["MBC10110040S",null,"동관 용접 배관","D20, 옥내일반, 고소작업대 사용","m",1019,8156,0,9175,"합계"]
["MBC10110050S",null,"동관 용접 배관","D25, 옥내일반, 고소작업대 사용","m",1239,9919,0,11158,"합계"]
["MBC10110060S",null,"동관 용접 배관","D32, 옥내일반, 고소작업대 사용","m",1489,11918,0,13407,"합계"]
["MBC10110070S",null,"동관 용접 배관","D40, 옥내일반, 고소작업대 사용","m",1739,13916,0,15655,"합계"]
["MBC10110080S",null,"동관 용접 배관","D50, 옥내일반, 고소작업대 사용","m",2278,18229,0,20507,"합계"]
["MBC10110090S",null,"동관 용접 배관","D65, 옥내일반, 고소작업대 사용","m",2682,21462,0,24144,"합계"]
["MBC10110100S",null,"동관 용접 배관","D80, 옥내일반, 고소작업대 사용","m",3363,26906,0,30269,"합계"]
["MBC10110110S",null,"동관 용접 배관","D100, 옥내일반, 고소작업대 사용","m",4556,36450,0,41006,"합계"]
["MBC10110120S",null,"동관 용접 배관","D125, 옥내일반, 고소작업대 사용","m",5670,45361,0,51031,"합계"]
["MBC10110130S",null,"동관 용접 배관","D150, 옥내일반, 고소작업대 사용","m",6807,54457,0,61264,"합계"]
["MBC10110140S",null,"동관 용접 배관","D200, 옥내일반, 고소작업대 사용","m",10122,80978,0,91100,"합계"]
["MBC10110150S",null,"동관 용접 배관","D250, 옥내일반, 고소작업대 사용","m",13371,106969,0,120340,"합계"]
["MBC11010010S",null,"동관 용접 배관","D8, 기계실","m",129,8416,0,8545,"합계"]
["MBC11010020S",null,"동관 용접 배관","D10, 기계실","m",148,9659,0,9807,"합계"]
["MBC11010030S",null,"동관 용접 배관","D15, 기계실","m",172,11199,0,11371,"합계"]
["MBC11010040S",null,"동관 용접 배관","D20, 기계실","m",203,13253,0,13456,"합계"]
["MBC11010050S",null,"동관 용접 배관","D25, 기계실","m",247,16119,0,16366,"합계"]
["MBC11010060S",null,"동관 용접 배관","D32, 기계실","m",297,19367,0,19664,"합계"]
["MBC11010070S",null,"동관 용접 배관","D40, 기계실","m",347,22614,0,22961,"합계"]
["MBC11010080S",null,"동관 용접 배관","D50, 기계실","m",455,29623,0,30078,"합계"]
["MBC11010090S",null,"동관 용접 배관","D65, 기계실","m",536,34875,0,35411,"합계"]
["MBC11010100S",null,"동관 용접 배관","D80, 기계실","m",672,43723,0,44395,"합계"]
["MBC11010110S",null,"동관 용접 배관","D100, 기계실","m",911,59231,0,60142,"합계"]
["MBC11010120S",null,"동관 용접 배관","D125, 기계실","m",1134,73712,0,74846,"합계"]
["MBC11010130S",null,"동관 용접 배관","D150, 기계실","m",1361,88492,0,89853,"합계"]
["MBC11010140S",null,"동관 용접 배관","D200, 기계실","m",2024,131589,0,133613,"합계"]
["MBC11010150S",null,"동관 용접 배관","D250, 기계실","m",2674,173825,0,176499,"합계"]
["MBC11110010S",null,"동관 용접 배관","D8, 기계실, 고소작업대 사용","m",647,7121,0,7768,"합계"]
["MBC11110020S",null,"동관 용접 배관","D10, 기계실, 고소작업대 사용","m",743,8173,0,8916,"합계"]
["MBC11110030S",null,"동관 용접 배관","D15, 기계실, 고소작업대 사용","m",861,9476,0,10337,"합계"]
["MBC11110040S",null,"동관 용접 배관","D20, 기계실, 고소작업대 사용","m",1019,11214,0,12233,"합계"]
["MBC11110050S",null,"동관 용접 배관","D25, 기계실, 고소작업대 사용","m",1239,13639,0,14878,"합계"]
["MBC11110060S",null,"동관 용접 배관","D32, 기계실, 고소작업대 사용","m",1489,16387,0,17876,"합계"]
["MBC11110070S",null,"동관 용접 배관","D40, 기계실, 고소작업대 사용","m",1739,19135,0,20874,"합계"]
["MBC11110080S",null,"동관 용접 배관","D50, 기계실, 고소작업대 사용","m",2278,25065,0,27343,"합계"]
["MBC11110090S",null,"동관 용접 배관","D65, 기계실, 고소작업대 사용","m",2682,29510,0,32192,"합계"]
["MBC11110100S",null,"동관 용접 배관","D80, 기계실, 고소작업대 사용","m",3363,36996,0,40359,"합계"]
["MBC11110110S",null,"동관 용접 배관","D100, 기계실, 고소작업대 사용","m",4556,50119,0,54675,"합계"]
["MBC11110120S",null,"동관 용접 배관","D125, 기계실, 고소작업대 사용","m",5670,62372,0,68042,"합계"]
["MBC11110130S",null,"동관 용접 배관","D150, 기계실, 고소작업대 사용","m",6807,74878,0,81685,"합계"]
["MBC11110140S",null,"동관 용접 배관","D200, 기계실, 고소작업대 사용","m",10122,111345,0,121467,"합계"]
["MBC11110150S",null,"동관 용접 배관","D250, 기계실, 고소작업대 사용","m",13371,147083,0,160454,"합계"]
["MBC12010010S",null,"동관 용접 배관","D8, 화장실","m",129,7769,0,7898,"합계"]
["MBC12010020S",null,"동관 용접 배관","D10, 화장실","m",148,8916,0,9064,"합계"]
["MBC12010030S",null,"동관 용접 배관","D15, 화장실","m",172,10338,0,10510,"합계"]
["MBC12010040S",null,"동관 용접 배관","D20, 화장실","m",203,12234,0,12437,"합계"]
["MBC12010050S",null,"동관 용접 배관","D25, 화장실","m",247,14879,0,15126,"합계"]
["MBC12010060S",null,"동관 용접 배관","D32, 화장실","m",297,17877,0,18174,"합계"]
["MBC12010070S",null,"동관 용접 배관","D40, 화장실","m",347,20875,0,21222,"합계"]
["MBC12010080S",null,"동관 용접 배관","D50, 화장실","m",455,27344,0,27799,"합계"]
["MBC12010090S",null,"동관 용접 배관","D65, 화장실","m",536,32193,0,32729,"합계"]
["MBC12010100S",null,"동관 용접 배관","D80, 화장실","m",672,40359,0,41031,"합계"]
["MBC12010110S",null,"동관 용접 배관","D100, 화장실","m",911,54675,0,55586,"합계"]
["MBC12010120S",null,"동관 용접 배관","D125, 화장실","m",1134,68042,0,69176,"합계"]
["MBC12010130S",null,"동관 용접 배관","D150, 화장실","m",1361,81685,0,83046,"합계"]
["MBC12010140S",null,"동관 용접 배관","D200, 화장실","m",2024,121467,0,123491,"합계"]
["MBC12010150S",null,"동관 용접 배관","D250, 화장실","m",2674,160454,0,163128,"합계"]
["MBC12110010S",null,"동관 용접 배관","D8, 화장실, 고소작업대 사용","m",647,6474,0,7121,"합계"]
["MBC12110020S",null,"동관 용접 배관","D10, 화장실, 고소작업대 사용","m",743,7430,0,8173,"합계"]
["MBC12110030S",null,"동관 용접 배관","D15, 화장실, 고소작업대 사용","m",861,8615,0,9476,"합계"]
["MBC12110040S",null,"동관 용접 배관","D20, 화장실, 고소작업대 사용","m",1019,10195,0,11214,"합계"]
["MBC12110050S",null,"동관 용접 배관","D25, 화장실, 고소작업대 사용","m",1239,12399,0,13638,"합계"]
["MBC12110060S",null,"동관 용접 배관","D32, 화장실, 고소작업대 사용","m",1489,14898,0,16387,"합계"]
["MBC12110070S",null,"동관 용접 배관","D40, 화장실, 고소작업대 사용","m",1739,17395,0,19134,"합계"]
["MBC12110080S",null,"동관 용접 배관","D50, 화장실, 고소작업대 사용","m",2278,22787,0,25065,"합계"]
["MBC12110090S",null,"동관 용접 배관","D65, 화장실, 고소작업대 사용","m",2682,26827,0,29509,"합계"]
["MBC12110100S",null,"동관 용접 배관","D80, 화장실, 고소작업대 사용","m",3363,33633,0,36996,"합계"]
["MBC12110110S",null,"동관 용접 배관","D100, 화장실, 고소작업대 사용","m",4556,45562,0,50118,"합계"]
["MBC12110120S",null,"동관 용접 배관","D125, 화장실, 고소작업대 사용","m",5670,56702,0,62372,"합계"]
["MBC12110130S",null,"동관 용접 배관","D150, 화장실, 고소작업대 사용","m",6807,68071,0,74878,"합계"]
["MBC12110140S",null,"동관 용접 배관","D200, 화장실, 고소작업대 사용","m",10122,101222,0,111344,"합계"]
["MBC12110150S",null,"동관 용접 배관","D250, 화장실, 고소작업대 사용","m",13371,133712,0,147083,"합계"]
["MBC13010010S",null,"동관 용접 배관","D8, 옥외배관","m",129,5827,0,5956,"합계"]
["MBC13010020S",null,"동관 용접 배관","D10, 옥외배관","m",148,6687,0,6835,"합계"]
["MBC13010030S",null,"동관 용접 배관","D15, 옥외배관","m",172,7753,0,7925,"합계"]
["MBC13010040S",null,"동관 용접 배관","D20, 옥외배관","m",203,9175,0,9378,"합계"]
["MBC13010050S",null,"동관 용접 배관","D25, 옥외배관","m",247,11159,0,11406,"합계"]
["MBC13010060S",null,"동관 용접 배관","D32, 옥외배관","m",297,13408,0,13705,"합계"]
["MBC13010070S",null,"동관 용접 배관","D40, 옥외배관","m",347,15656,0,16003,"합계"]
["MBC13010080S",null,"동관 용접 배관","D50, 옥외배관","m",455,20508,0,20963,"합계"]
["MBC13010090S",null,"동관 용접 배관","D65, 옥외배관","m",536,24144,0,24680,"합계"]
["MBC13010100S",null,"동관 용접 배관","D80, 옥외배관","m",672,30269,0,30941,"합계"]
["MBC13010110S",null,"동관 용접 배관","D100, 옥외배관","m",911,41006,0,41917,"합계"]
["MBC13010120S",null,"동관 용접 배관","D125, 옥외배관","m",1134,51032,0,52166,"합계"]
["MBC13010130S",null,"동관 용접 배관","D150, 옥외배관","m",1361,61264,0,62625,"합계"]
["MBC13010140S",null,"동관 용접 배관","D200, 옥외배관","m",2024,91100,0,93124,"합계"]
["MBC13010150S",null,"동관 용접 배관","D250, 옥외배관","m",2674,120340,0,123014,"합계"]
["MBC13110010S",null,"동관 용접 배관","D8, 옥외배관, 고소작업대 사용","m",647,4532,0,5179,"합계"]
["MBC13110020S",null,"동관 용접 배관","D10, 옥외배관, 고소작업대 사용","m",743,5201,0,5944,"합계"]
["MBC13110030S",null,"동관 용접 배관","D15, 옥외배관, 고소작업대 사용","m",861,6030,0,6891,"합계"]
["MBC13110040S",null,"동관 용접 배관","D20, 옥외배관, 고소작업대 사용","m",1019,7136,0,8155,"합계"]
["MBC13110050S",null,"동관 용접 배관","D25, 옥외배관, 고소작업대 사용","m",1239,8679,0,9918,"합계"]
["MBC13110060S",null,"동관 용접 배관","D32, 옥외배관, 고소작업대 사용","m",1489,10428,0,11917,"합계"]
["MBC13110070S",null,"동관 용접 배관","D40, 옥외배관, 고소작업대 사용","m",1739,12177,0,13916,"합계"]
["MBC13110080S",null,"동관 용접 배관","D50, 옥외배관, 고소작업대 사용","m",2278,15950,0,18228,"합계"]
["MBC13110090S",null,"동관 용접 배관","D65, 옥외배관, 고소작업대 사용","m",2682,18779,0,21461,"합계"]
["MBC13110100S",null,"동관 용접 배관","D80, 옥외배관, 고소작업대 사용","m",3363,23543,0,26906,"합계"]
["MBC13110110S",null,"동관 용접 배관","D100, 옥외배관, 고소작업대 사용","m",4556,31893,0,36449,"합계"]
["MBC13110120S",null,"동관 용접 배관","D125, 옥외배관, 고소작업대 사용","m",5670,39691,0,45361,"합계"]
["MBC13110130S",null,"동관 용접 배관","D150, 옥외배관, 고소작업대 사용","m",6807,47649,0,54456,"합계"]
["MBC13110140S",null,"동관 용접 배관","D200, 옥외배관, 고소작업대 사용","m",10122,70856,0,80978,"합계"]
["MBC13110150S",null,"동관 용접 배관","D250, 옥외배관, 고소작업대 사용","m",13371,93598,0,106969,"합계"]
["MBE00010010S",null,"스텐관 용접 접합","D6","개소",384,9612,0,9996,"합계"]
["MBE00010020S",null,"스텐관 용접 접합","D8","개소",427,10680,0,11107,"합계"]
["MBE00010030S",null,"스텐관 용접 접합","D10","개소",480,12015,0,12495,"합계"]
["MBE00010040S",null,"스텐관 용접 접합","D15","개소",534,13351,0,13885,"합계"]
["MBE00010050S",null,"스텐관 용접 접합","D20","개소",608,15220,0,15828,"합계"]
["MBE00010060S",null,"스텐관 용접 접합","D25","개소",704,17623,0,18327,"합계"]
["MBE00010070S",null,"스텐관 용접 접합","D32","개소",822,20560,0,21382,"합계"]
["MBE00010080S",null,"스텐관 용접 접합","D40","개소",897,22429,0,23326,"합계"]
["MBE00010090S",null,"스텐관 용접 접합","D50","개소",1057,26435,0,27492,"합계"]
["MBE00010100S",null,"스텐관 용접 접합","D65","개소",1271,31775,0,33046,"합계"]
["MBE00010110S",null,"스텐관 용접 접합","D80","개소",1441,36047,0,37488,"합계"]
["MBE00010120S",null,"스텐관 용접 접합","D90","개소",1612,40320,0,41932,"합계"]
["MBE00010130S",null,"스텐관 용접 접합","D100","개소",1783,44592,0,46375,"합계"]
["MBE00010140S",null,"스텐관 용접 접합","D125","개소",2125,53137,0,55262,"합계"]
["MBE00010150S",null,"스텐관 용접 접합","D150","개소",2467,61681,0,64148,"합계"]
["MBE00010160S",null,"스텐관 용접 접합","D200","개소",3150,78771,0,81921,"합계"]
["MBE00010170S",null,"스텐관 용접 접합","D250","개소",3834,95860,0,99694,"합계"]
["MBE00010180S",null,"스텐관 용접 접합","D300","개소",4517,112949,0,117466,"합계"]
["MBE00110010S",null,"스텐관 용접 접합","D6, 고소작업대 사용","개소",1249,7690,0,8939,"합계"]
["MBE00110020S",null,"스텐관 용접 접합","D8, 고소작업대 사용","개소",1388,8544,0,9932,"합계"]
["MBE00110030S",null,"스텐관 용접 접합","D10, 고소작업대 사용","개소",1562,9612,0,11174,"합계"]
["MBE00110040S",null,"스텐관 용접 접합","D15, 고소작업대 사용","개소",1735,10680,0,12415,"합계"]
["MBE00110050S",null,"스텐관 용접 접합","D20, 고소작업대 사용","개소",1978,12176,0,14154,"합계"]
["MBE00110060S",null,"스텐관 용접 접합","D25, 고소작업대 사용","개소",2291,14098,0,16389,"합계"]
["MBE00110070S",null,"스텐관 용접 접합","D32, 고소작업대 사용","개소",2672,16448,0,19120,"합계"]
["MBE00110080S",null,"스텐관 용접 접합","D40, 고소작업대 사용","개소",2915,17943,0,20858,"합계"]
["MBE00110090S",null,"스텐관 용접 접합","D50, 고소작업대 사용","개소",3436,21148,0,24584,"합계"]
["MBE00110100S",null,"스텐관 용접 접합","D65, 고소작업대 사용","개소",4130,25420,0,29550,"합계"]
["MBE00110110S",null,"스텐관 용접 접합","D80, 고소작업대 사용","개소",4686,28838,0,33524,"합계"]
["MBE00110120S",null,"스텐관 용접 접합","D90, 고소작업대 사용","개소",5241,32256,0,37497,"합계"]
["MBE00110130S",null,"스텐관 용접 접합","D100, 고소작업대 사용","개소",5797,35674,0,41471,"합계"]
["MBE00110140S",null,"스텐관 용접 접합","D125, 고소작업대 사용","개소",6907,42509,0,49416,"합계"]
["MBE00110150S",null,"스텐관 용접 접합","D150, 고소작업대 사용","개소",8018,49345,0,57363,"합계"]
["MBE00110160S",null,"스텐관 용접 접합","D200, 고소작업대 사용","개소",10240,63016,0,73256,"합계"]
["MBE00110170S",null,"스텐관 용접 접합","D250, 고소작업대 사용","개소",12461,76688,0,89149,"합계"]
["MBE00110180S",null,"스텐관 용접 접합","D300, 고소작업대 사용","개소",14683,90359,0,105042,"합계"]
["MBE10010010S",null,"스텐관 용접 배관","D6, 옥내일반","m",134,6741,0,6875,"합계"]
["MBE10010020S",null,"스텐관 용접 배관","D8, 옥내일반","m",139,6971,0,7110,"합계"]
["MBE10010030S",null,"스텐관 용접 배관","D10, 옥내일반","m",165,8284,0,8449,"합계"]
["MBE10010040S",null,"스텐관 용접 배관","D15, 옥내일반","m",178,8908,0,9086,"합계"]
["MBE10010050S",null,"스텐관 용접 배관","D20, 옥내일반","m",207,10387,0,10594,"합계"]
["MBE10010060S",null,"스텐관 용접 배관","D25, 옥내일반","m",293,14657,0,14950,"합계"]
["MBE10010070S",null,"스텐관 용접 배관","D32, 옥내일반","m",353,17678,0,18031,"합계"]
["MBE10010080S",null,"스텐관 용접 배관","D40, 옥내일반","m",387,19386,0,19773,"합계"]
["MBE10010090S",null,"스텐관 용접 배관","D50, 옥내일반","m",468,23426,0,23894,"합계"]
["MBE10010100S",null,"스텐관 용접 배관","D65, 옥내일반","m",577,28881,0,29458,"합계"]
["MBE10010110S",null,"스텐관 용접 배관","D80, 옥내일반","m",653,32692,0,33345,"합계"]
["MBE10010120S",null,"스텐관 용접 배관","D90, 옥내일반","m",859,42978,0,43837,"합계"]
["MBE10010130S",null,"스텐관 용접 배관","D100, 옥내일반","m",943,47184,0,48127,"합계"]
["MBE10010140S",null,"스텐관 용접 배관","D125, 옥내일반","m",1259,62988,0,64247,"합계"]
["MBE10010150S",null,"스텐관 용접 배관","D150, 옥내일반","m",1435,71795,0,73230,"합계"]
["MBE10010160S",null,"스텐관 용접 배관","D200, 옥내일반","m",2012,100601,0,102613,"합계"]
["MBE10010170S",null,"스텐관 용접 배관","D250, 옥내일반","m",2721,136059,0,138780,"합계"]
["MBE10010180S",null,"스텐관 용접 배관","D300, 옥내일반","m",3601,180060,0,183661,"합계"]
["MBE10110010S",null,"스텐관 용접 배관","D6, 옥내일반, 고소작업대 사용","m",674,5393,0,6067,"합계"]
["MBE10110020S",null,"스텐관 용접 배관","D8, 옥내일반, 고소작업대 사용","m",697,5576,0,6273,"합계"]
["MBE10110030S",null,"스텐관 용접 배관","D10, 옥내일반, 고소작업대 사용","m",828,6627,0,7455,"합계"]
["MBE10110040S",null,"스텐관 용접 배관","D15, 옥내일반, 고소작업대 사용","m",890,7126,0,8016,"합계"]
["MBE10110050S",null,"스텐관 용접 배관","D20, 옥내일반, 고소작업대 사용","m",1038,8309,0,9347,"합계"]
["MBE10110060S",null,"스텐관 용접 배관","D25, 옥내일반, 고소작업대 사용","m",1465,11725,0,13190,"합계"]
["MBE10110070S",null,"스텐관 용접 배관","D32, 옥내일반, 고소작업대 사용","m",1767,14142,0,15909,"합계"]
["MBE10110080S",null,"스텐관 용접 배관","D40, 옥내일반, 고소작업대 사용","m",1938,15508,0,17446,"합계"]
["MBE10110090S",null,"스텐관 용접 배관","D50, 옥내일반, 고소작업대 사용","m",2342,18741,0,21083,"합계"]
["MBE10110100S",null,"스텐관 용접 배관","D65, 옥내일반, 고소작업대 사용","m",2888,23105,0,25993,"합계"]
["MBE10110110S",null,"스텐관 용접 배관","D80, 옥내일반, 고소작업대 사용","m",3269,26154,0,29423,"합계"]
["MBE10110120S",null,"스텐관 용접 배관","D90, 옥내일반, 고소작업대 사용","m",4297,34382,0,38679,"합계"]
["MBE10110130S",null,"스텐관 용접 배관","D100, 옥내일반, 고소작업대 사용","m",4718,37747,0,42465,"합계"]
["MBE10110140S",null,"스텐관 용접 배관","D125, 옥내일반, 고소작업대 사용","m",6298,50390,0,56688,"합계"]
["MBE10110150S",null,"스텐관 용접 배관","D150, 옥내일반, 고소작업대 사용","m",7179,57436,0,64615,"합계"]
["MBE10110160S",null,"스텐관 용접 배관","D200, 옥내일반, 고소작업대 사용","m",10060,80481,0,90541,"합계"]
["MBE10110170S",null,"스텐관 용접 배관","D250, 옥내일반, 고소작업대 사용","m",13605,108847,0,122452,"합계"]
["MBE10110180S",null,"스텐관 용접 배관","D300, 옥내일반, 고소작업대 사용","m",18006,144048,0,162054,"합계"]
["MBE11010010S",null,"스텐관 용접 배관","D6, 기계실","m",134,8764,0,8898,"합계"]
["MBE11010020S",null,"스텐관 용접 배관","D8, 기계실","m",139,9062,0,9201,"합계"]
["MBE11010030S",null,"스텐관 용접 배관","D10, 기계실","m",165,10769,0,10934,"합계"]
["MBE11010040S",null,"스텐관 용접 배관","D15, 기계실","m",178,11581,0,11759,"합계"]
["MBE11010050S",null,"스텐관 용접 배관","D20, 기계실","m",207,13503,0,13710,"합계"]
["MBE11010060S",null,"스텐관 용접 배관","D25, 기계실","m",293,19054,0,19347,"합계"]
["MBE11010070S",null,"스텐관 용접 배관","D32, 기계실","m",353,22981,0,23334,"합계"]
["MBE11010080S",null,"스텐관 용접 배관","D40, 기계실","m",387,25201,0,25588,"합계"]
["MBE11010090S",null,"스텐관 용접 배관","D50, 기계실","m",468,30454,0,30922,"합계"]
["MBE11010100S",null,"스텐관 용접 배관","D65, 기계실","m",577,37545,0,38122,"합계"]
["MBE11010110S",null,"스텐관 용접 배관","D80, 기계실","m",653,42500,0,43153,"합계"]
["MBE11010120S",null,"스텐관 용접 배관","D90, 기계실","m",859,55871,0,56730,"합계"]
["MBE11010130S",null,"스텐관 용접 배관","D100, 기계실","m",943,61339,0,62282,"합계"]
["MBE11010140S",null,"스텐관 용접 배관","D125, 기계실","m",1259,81885,0,83144,"합계"]
["MBE11010150S",null,"스텐관 용접 배관","D150, 기계실","m",1435,93334,0,94769,"합계"]
["MBE11010160S",null,"스텐관 용접 배관","D200, 기계실","m",2012,130782,0,132794,"합계"]
["MBE11010170S",null,"스텐관 용접 배관","D250, 기계실","m",2721,176877,0,179598,"합계"]
["MBE11010180S",null,"스텐관 용접 배관","D300, 기계실","m",3601,234078,0,237679,"합계"]
["MBE11110010S",null,"스텐관 용접 배관","D6, 기계실, 고소작업대 사용","m",674,7415,0,8089,"합계"]
["MBE11110020S",null,"스텐관 용접 배관","D8, 기계실, 고소작업대 사용","m",697,7668,0,8365,"합계"]
["MBE11110030S",null,"스텐관 용접 배관","D10, 기계실, 고소작업대 사용","m",828,9112,0,9940,"합계"]
["MBE11110040S",null,"스텐관 용접 배관","D15, 기계실, 고소작업대 사용","m",890,9799,0,10689,"합계"]
["MBE11110050S",null,"스텐관 용접 배관","D20, 기계실, 고소작업대 사용","m",1038,11425,0,12463,"합계"]
["MBE11110060S",null,"스텐관 용접 배관","D25, 기계실, 고소작업대 사용","m",1465,16122,0,17587,"합계"]
["MBE11110070S",null,"스텐관 용접 배관","D32, 기계실, 고소작업대 사용","m",1767,19445,0,21212,"합계"]
["MBE11110080S",null,"스텐관 용접 배관","D40, 기계실, 고소작업대 사용","m",1938,21324,0,23262,"합계"]
["MBE11110090S",null,"스텐관 용접 배관","D50, 기계실, 고소작업대 사용","m",2342,25769,0,28111,"합계"]
["MBE11110100S",null,"스텐관 용접 배관","D65, 기계실, 고소작업대 사용","m",2888,31769,0,34657,"합계"]
["MBE11110110S",null,"스텐관 용접 배관","D80, 기계실, 고소작업대 사용","m",3269,35961,0,39230,"합계"]
["MBE11110120S",null,"스텐관 용접 배관","D90, 기계실, 고소작업대 사용","m",4297,47275,0,51572,"합계"]
["MBE11110130S",null,"스텐관 용접 배관","D100, 기계실, 고소작업대 사용","m",4718,51902,0,56620,"합계"]
["MBE11110140S",null,"스텐관 용접 배관","D125, 기계실, 고소작업대 사용","m",6298,69287,0,75585,"합계"]
["MBE11110150S",null,"스텐관 용접 배관","D150, 기계실, 고소작업대 사용","m",7179,78975,0,86154,"합계"]
["MBE11110160S",null,"스텐관 용접 배관","D200, 기계실, 고소작업대 사용","m",10060,110661,0,120721,"합계"]
["MBE11110170S",null,"스텐관 용접 배관","D250, 기계실, 고소작업대 사용","m",13605,149665,0,163270,"합계"]
["MBE11110180S",null,"스텐관 용접 배관","D300, 기계실, 고소작업대 사용","m",18006,198066,0,216072,"합계"]
["MBE12010010S",null,"스텐관 용접 배관","D6, 화장실","m",134,8089,0,8223,"합계"]
["MBE12010020S",null,"스텐관 용접 배관","D8, 화장실","m",139,8365,0,8504,"합계"]
["MBE12010030S",null,"스텐관 용접 배관","D10, 화장실","m",165,9940,0,10105,"합계"]
["MBE12010040S",null,"스텐관 용접 배관","D15, 화장실","m",178,10690,0,10868,"합계"]
["MBE12010050S",null,"스텐관 용접 배관","D20, 화장실","m",207,12464,0,12671,"합계"]
["MBE12010060S",null,"스텐관 용접 배관","D25, 화장실","m",293,17588,0,17881,"합계"]
["MBE12010070S",null,"스텐관 용접 배관","D32, 화장실","m",353,21213,0,21566,"합계"]
["MBE12010080S",null,"스텐관 용접 배관","D40, 화장실","m",387,23263,0,23650,"합계"]
["MBE12010090S",null,"스텐관 용접 배관","D50, 화장실","m",468,28111,0,28579,"합계"]
["MBE12010100S",null,"스텐관 용접 배관","D65, 화장실","m",577,34657,0,35234,"합계"]
["MBE12010110S",null,"스텐관 용접 배관","D80, 화장실","m",653,39231,0,39884,"합계"]
["MBE12010120S",null,"스텐관 용접 배관","D90, 화장실","m",859,51573,0,52432,"합계"]
["MBE12010130S",null,"스텐관 용접 배관","D100, 화장실","m",943,56620,0,57563,"합계"]
["MBE12010140S",null,"스텐관 용접 배관","D125, 화장실","m",1259,75586,0,76845,"합계"]
["MBE12010150S",null,"스텐관 용접 배관","D150, 화장실","m",1435,86154,0,87589,"합계"]
["MBE12010160S",null,"스텐관 용접 배관","D200, 화장실","m",2012,120722,0,122734,"합계"]
["MBE12010170S",null,"스텐관 용접 배관","D250, 화장실","m",2721,163271,0,165992,"합계"]
["MBE12010180S",null,"스텐관 용접 배관","D300, 화장실","m",3601,216072,0,219673,"합계"]
["MBE12110010S",null,"스텐관 용접 배관","D6, 화장실, 고소작업대 사용","m",674,6741,0,7415,"합계"]
["MBE12110020S",null,"스텐관 용접 배관","D8, 화장실, 고소작업대 사용","m",697,6971,0,7668,"합계"]
["MBE12110030S",null,"스텐관 용접 배관","D10, 화장실, 고소작업대 사용","m",828,8284,0,9112,"합계"]
["MBE12110040S",null,"스텐관 용접 배관","D15, 화장실, 고소작업대 사용","m",890,8908,0,9798,"합계"]
["MBE12110050S",null,"스텐관 용접 배관","D20, 화장실, 고소작업대 사용","m",1038,10387,0,11425,"합계"]
["MBE12110060S",null,"스텐관 용접 배관","D25, 화장실, 고소작업대 사용","m",1465,14657,0,16122,"합계"]
["MBE12110070S",null,"스텐관 용접 배관","D32, 화장실, 고소작업대 사용","m",1767,17678,0,19445,"합계"]
["MBE12110080S",null,"스텐관 용접 배관","D40, 화장실, 고소작업대 사용","m",1938,19386,0,21324,"합계"]
["MBE12110090S",null,"스텐관 용접 배관","D50, 화장실, 고소작업대 사용","m",2342,23426,0,25768,"합계"]
["MBE12110100S",null,"스텐관 용접 배관","D65, 화장실, 고소작업대 사용","m",2888,28881,0,31769,"합계"]
["MBE12110110S",null,"스텐관 용접 배관","D80, 화장실, 고소작업대 사용","m",3269,32692,0,35961,"합계"]
["MBE12110120S",null,"스텐관 용접 배관","D90, 화장실, 고소작업대 사용","m",4297,42978,0,47275,"합계"]
["MBE12110130S",null,"스텐관 용접 배관","D100, 화장실, 고소작업대 사용","m",4718,47184,0,51902,"합계"]
["MBE12110140S",null,"스텐관 용접 배관","D125, 화장실, 고소작업대 사용","m",6298,62988,0,69286,"합계"]
["MBE12110150S",null,"스텐관 용접 배관","D150, 화장실, 고소작업대 사용","m",7179,71795,0,78974,"합계"]
["MBE12110160S",null,"스텐관 용접 배관","D200, 화장실, 고소작업대 사용","m",10060,100601,0,110661,"합계"]
["MBE12110170S",null,"스텐관 용접 배관","D250, 화장실, 고소작업대 사용","m",13605,136059,0,149664,"합계"]
["MBE12110180S",null,"스텐관 용접 배관","D300, 화장실, 고소작업대 사용","m",18006,180060,0,198066,"합계"]
["MBE13010010S",null,"스텐관 용접 배관","D6, 옥외배관","m",134,6067,0,6201,"합계"]
["MBE13010020S",null,"스텐관 용접 배관","D8, 옥외배관","m",139,6273,0,6412,"합계"]
["MBE13010030S",null,"스텐관 용접 배관","D10, 옥외배관","m",165,7455,0,7620,"합계"]
["MBE13010040S",null,"스텐관 용접 배관","D15, 옥외배관","m",178,8017,0,8195,"합계"]
["MBE13010050S",null,"스텐관 용접 배관","D20, 옥외배관","m",207,9348,0,9555,"합계"]
["MBE13010060S",null,"스텐관 용접 배관","D25, 옥외배관","m",293,13191,0,13484,"합계"]
["MBE13010070S",null,"스텐관 용접 배관","D32, 옥외배관","m",353,15910,0,16263,"합계"]
["MBE13010080S",null,"스텐관 용접 배관","D40, 옥외배관","m",387,17447,0,17834,"합계"]
["MBE13010090S",null,"스텐관 용접 배관","D50, 옥외배관","m",468,21083,0,21551,"합계"]
["MBE13010100S",null,"스텐관 용접 배관","D65, 옥외배관","m",577,25993,0,26570,"합계"]
["MBE13010110S",null,"스텐관 용접 배관","D80, 옥외배관","m",653,29423,0,30076,"합계"]
["MBE13010120S",null,"스텐관 용접 배관","D90, 옥외배관","m",859,38680,0,39539,"합계"]
["MBE13010130S",null,"스텐관 용접 배관","D100, 옥외배관","m",943,42465,0,43408,"합계"]
["MBE13010140S",null,"스텐관 용접 배관","D125, 옥외배관","m",1259,56689,0,57948,"합계"]
["MBE13010150S",null,"스텐관 용접 배관","D150, 옥외배관","m",1435,64616,0,66051,"합계"]
["MBE13010160S",null,"스텐관 용접 배관","D200, 옥외배관","m",2012,90541,0,92553,"합계"]
["MBE13010170S",null,"스텐관 용접 배관","D250, 옥외배관","m",2721,122453,0,125174,"합계"]
["MBE13010180S",null,"스텐관 용접 배관","D300, 옥외배관","m",3601,162054,0,165655,"합계"]
["MBE13110010S",null,"스텐관 용접 배관","D6, 옥외배관, 고소작업대 사용","m",674,4719,0,5393,"합계"]
["MBE13110020S",null,"스텐관 용접 배관","D8, 옥외배관, 고소작업대 사용","m",697,4879,0,5576,"합계"]
["MBE13110030S",null,"스텐관 용접 배관","D10, 옥외배관, 고소작업대 사용","m",828,5798,0,6626,"합계"]
["MBE13110040S",null,"스텐관 용접 배관","D15, 옥외배관, 고소작업대 사용","m",890,6235,0,7125,"합계"]
["MBE13110050S",null,"스텐관 용접 배관","D20, 옥외배관, 고소작업대 사용","m",1038,7270,0,8308,"합계"]
["MBE13110060S",null,"스텐관 용접 배관","D25, 옥외배관, 고소작업대 사용","m",1465,10259,0,11724,"합계"]
["MBE13110070S",null,"스텐관 용접 배관","D32, 옥외배관, 고소작업대 사용","m",1767,12374,0,14141,"합계"]
["MBE13110080S",null,"스텐관 용접 배관","D40, 옥외배관, 고소작업대 사용","m",1938,13570,0,15508,"합계"]
["MBE13110090S",null,"스텐관 용접 배관","D50, 옥외배관, 고소작업대 사용","m",2342,16398,0,18740,"합계"]
["MBE13110100S",null,"스텐관 용접 배관","D65, 옥외배관, 고소작업대 사용","m",2888,20217,0,23105,"합계"]
["MBE13110110S",null,"스텐관 용접 배관","D80, 옥외배관, 고소작업대 사용","m",3269,22884,0,26153,"합계"]
["MBE13110120S",null,"스텐관 용접 배관","D90, 옥외배관, 고소작업대 사용","m",4297,30084,0,34381,"합계"]
["MBE13110130S",null,"스텐관 용접 배관","D100, 옥외배관, 고소작업대 사용","m",4718,33028,0,37746,"합계"]
["MBE13110140S",null,"스텐관 용접 배관","D125, 옥외배관, 고소작업대 사용","m",6298,44092,0,50390,"합계"]
["MBE13110150S",null,"스텐관 용접 배관","D150, 옥외배관, 고소작업대 사용","m",7179,50256,0,57435,"합계"]
["MBE13110160S",null,"스텐관 용접 배관","D200, 옥외배관, 고소작업대 사용","m",10060,70421,0,80481,"합계"]
["MBE13110170S",null,"스텐관 용접 배관","D250, 옥외배관, 고소작업대 사용","m",13605,95241,0,108846,"합계"]
["MBE13110180S",null,"스텐관 용접 배관","D300, 옥외배관, 고소작업대 사용","m",18006,126042,0,144048,"합계"]
["MBE20010010S",null,"프레스식 접합 및 배관","D13, 옥내일반","m",212,10616,0,10828,"합계"]
["MBE20010020S",null,"프레스식 접합 및 배관","D20, 옥내일반","m",282,14134,0,14416,"합계"]
["MBE20010030S",null,"프레스식 접합 및 배관","D25, 옥내일반","m",332,16632,0,16964,"합계"]
["MBE20010040S",null,"프레스식 접합 및 배관","D30, 옥내일반","m",420,21003,0,21423,"합계"]
["MBE20010050S",null,"프레스식 접합 및 배관","D40, 옥내일반","m",490,24521,0,25011,"합계"]
["MBE20010060S",null,"프레스식 접합 및 배관","D50, 옥내일반","m",527,26394,0,26921,"합계"]
["MBE20010070S",null,"프레스식 접합 및 배관","D60, 옥내일반","m",688,34449,0,35137,"합계"]
["MBE20010080S",null,"프레스식 접합 및 배관","D75, 옥내일반","m",796,39840,0,40636,"합계"]
["MBE20010090S",null,"프레스식 접합 및 배관","D80, 옥내일반","m",1045,52266,0,53311,"합계"]
["MBE20010100S",null,"프레스식 접합 및 배관","D100, 옥내일반","m",1218,60946,0,62164,"합계"]
["MBE20110010S",null,"프레스식 접합 및 배관","D13, 옥내일반, 고소작업대 사용","m",1061,8493,0,9554,"합계"]
["MBE20110020S",null,"프레스식 접합 및 배관","D20, 옥내일반, 고소작업대 사용","m",1413,11307,0,12720,"합계"]
["MBE20110030S",null,"프레스식 접합 및 배관","D25, 옥내일반, 고소작업대 사용","m",1663,13305,0,14968,"합계"]
["MBE20110040S",null,"프레스식 접합 및 배관","D30, 옥내일반, 고소작업대 사용","m",2100,16802,0,18902,"합계"]
["MBE20110050S",null,"프레스식 접합 및 배관","D40, 옥내일반, 고소작업대 사용","m",2452,19617,0,22069,"합계"]
["MBE20110060S",null,"프레스식 접합 및 배관","D50, 옥내일반, 고소작업대 사용","m",2639,21115,0,23754,"합계"]
["MBE20110070S",null,"프레스식 접합 및 배관","D60, 옥내일반, 고소작업대 사용","m",3444,27559,0,31003,"합계"]
["MBE20110080S",null,"프레스식 접합 및 배관","D75, 옥내일반, 고소작업대 사용","m",3984,31872,0,35856,"합계"]
["MBE20110090S",null,"프레스식 접합 및 배관","D80, 옥내일반, 고소작업대 사용","m",5226,41813,0,47039,"합계"]
["MBE20110100S",null,"프레스식 접합 및 배관","D100, 옥내일반, 고소작업대 사용","m",6094,48756,0,54850,"합계"]
["MBE21010010S",null,"프레스식 접합 및 배관","D13, 기계실","m",212,13801,0,14013,"합계"]
["MBE21010020S",null,"프레스식 접합 및 배관","D20, 기계실","m",282,18374,0,18656,"합계"]
["MBE21010030S",null,"프레스식 접합 및 배관","D25, 기계실","m",332,21621,0,21953,"합계"]
["MBE21010040S",null,"프레스식 접합 및 배관","D30, 기계실","m",420,27304,0,27724,"합계"]
["MBE21010050S",null,"프레스식 접합 및 배관","D40, 기계실","m",490,31877,0,32367,"합계"]
["MBE21010060S",null,"프레스식 접합 및 배관","D50, 기계실","m",527,34313,0,34840,"합계"]
["MBE21010070S",null,"프레스식 접합 및 배관","D60, 기계실","m",688,44784,0,45472,"합계"]
["MBE21010080S",null,"프레스식 접합 및 배관","D75, 기계실","m",796,51792,0,52588,"합계"]
["MBE21010090S",null,"프레스식 접합 및 배관","D80, 기계실","m",1045,67946,0,68991,"합계"]
["MBE21010100S",null,"프레스식 접합 및 배관","D100, 기계실","m",1218,79229,0,80447,"합계"]
["MBE21110010S",null,"프레스식 접합 및 배관","D13, 기계실, 고소작업대 사용","m",1061,11678,0,12739,"합계"]
["MBE21110020S",null,"프레스식 접합 및 배관","D20, 기계실, 고소작업대 사용","m",1413,15547,0,16960,"합계"]
["MBE21110030S",null,"프레스식 접합 및 배관","D25, 기계실, 고소작업대 사용","m",1663,18295,0,19958,"합계"]
["MBE21110040S",null,"프레스식 접합 및 배관","D30, 기계실, 고소작업대 사용","m",2100,23104,0,25204,"합계"]
["MBE21110050S",null,"프레스식 접합 및 배관","D40, 기계실, 고소작업대 사용","m",2452,26973,0,29425,"합계"]
["MBE21110060S",null,"프레스식 접합 및 배관","D50, 기계실, 고소작업대 사용","m",2639,29034,0,31673,"합계"]
["MBE21110070S",null,"프레스식 접합 및 배관","D60, 기계실, 고소작업대 사용","m",3444,37894,0,41338,"합계"]
["MBE21110080S",null,"프레스식 접합 및 배관","D75, 기계실, 고소작업대 사용","m",3984,43824,0,47808,"합계"]
["MBE21110090S",null,"프레스식 접합 및 배관","D80, 기계실, 고소작업대 사용","m",5226,57493,0,62719,"합계"]
["MBE21110100S",null,"프레스식 접합 및 배관","D100, 기계실, 고소작업대 사용","m",6094,67040,0,73134,"합계"]
["MBE22010010S",null,"프레스식 접합 및 배관","D13, 화장실","m",212,12739,0,12951,"합계"]
["MBE22010020S",null,"프레스식 접합 및 배관","D20, 화장실","m",282,16960,0,17242,"합계"]
["MBE22010030S",null,"프레스식 접합 및 배관","D25, 화장실","m",332,19958,0,20290,"합계"]
["MBE22010040S",null,"프레스식 접합 및 배관","D30, 화장실","m",420,25204,0,25624,"합계"]
["MBE22010050S",null,"프레스식 접합 및 배관","D40, 화장실","m",490,29425,0,29915,"합계"]
["MBE22010060S",null,"프레스식 접합 및 배관","D50, 화장실","m",527,31673,0,32200,"합계"]
["MBE22010070S",null,"프레스식 접합 및 배관","D60, 화장실","m",688,41339,0,42027,"합계"]
["MBE22010080S",null,"프레스식 접합 및 배관","D75, 화장실","m",796,47808,0,48604,"합계"]
["MBE22010090S",null,"프레스식 접합 및 배관","D80, 화장실","m",1045,62720,0,63765,"합계"]
["MBE22010100S",null,"프레스식 접합 및 배관","D100, 화장실","m",1218,73135,0,74353,"합계"]
["MBE22110010S",null,"프레스식 접합 및 배관","D13, 화장실, 고소작업대 사용","m",1061,10616,0,11677,"합계"]
["MBE22110020S",null,"프레스식 접합 및 배관","D20, 화장실, 고소작업대 사용","m",1413,14134,0,15547,"합계"]
["MBE22110030S",null,"프레스식 접합 및 배관","D25, 화장실, 고소작업대 사용","m",1663,16632,0,18295,"합계"]
["MBE22110040S",null,"프레스식 접합 및 배관","D30, 화장실, 고소작업대 사용","m",2100,21003,0,23103,"합계"]
["MBE22110050S",null,"프레스식 접합 및 배관","D40, 화장실, 고소작업대 사용","m",2452,24521,0,26973,"합계"]
["MBE22110060S",null,"프레스식 접합 및 배관","D50, 화장실, 고소작업대 사용","m",2639,26394,0,29033,"합계"]
["MBE22110070S",null,"프레스식 접합 및 배관","D60, 화장실, 고소작업대 사용","m",3444,34449,0,37893,"합계"]
["MBE22110080S",null,"프레스식 접합 및 배관","D75, 화장실, 고소작업대 사용","m",3984,39840,0,43824,"합계"]
["MBE22110090S",null,"프레스식 접합 및 배관","D80, 화장실, 고소작업대 사용","m",5226,52266,0,57492,"합계"]
["MBE22110100S",null,"프레스식 접합 및 배관","D100, 화장실, 고소작업대 사용","m",6094,60946,0,67040,"합계"]
["MBE23010010S",null,"프레스식 접합 및 배관","D13, 옥외배관","m",212,9554,0,9766,"합계"]
["MBE23010020S",null,"프레스식 접합 및 배관","D20, 옥외배관","m",282,12720,0,13002,"합계"]
["MBE23010030S",null,"프레스식 접합 및 배관","D25, 옥외배관","m",332,14968,0,15300,"합계"]
["MBE23010040S",null,"프레스식 접합 및 배관","D30, 옥외배관","m",420,18903,0,19323,"합계"]
["MBE23010050S",null,"프레스식 접합 및 배관","D40, 옥외배관","m",490,22069,0,22559,"합계"]
["MBE23010060S",null,"프레스식 접합 및 배관","D50, 옥외배관","m",527,23755,0,24282,"합계"]
["MBE23010070S",null,"프레스식 접합 및 배관","D60, 옥외배관","m",688,31004,0,31692,"합계"]
["MBE23010080S",null,"프레스식 접합 및 배관","D75, 옥외배관","m",796,35856,0,36652,"합계"]
["MBE23010090S",null,"프레스식 접합 및 배관","D80, 옥외배관","m",1045,47040,0,48085,"합계"]
["MBE23010100S",null,"프레스식 접합 및 배관","D100, 옥외배관","m",1218,54851,0,56069,"합계"]
["MBE23110010S",null,"프레스식 접합 및 배관","D13, 옥외배관, 고소작업대 사용","m",1061,7431,0,8492,"합계"]
["MBE23110020S",null,"프레스식 접합 및 배관","D20, 옥외배관, 고소작업대 사용","m",1413,9893,0,11306,"합계"]
["MBE23110030S",null,"프레스식 접합 및 배관","D25, 옥외배관, 고소작업대 사용","m",1663,11642,0,13305,"합계"]
["MBE23110040S",null,"프레스식 접합 및 배관","D30, 옥외배관, 고소작업대 사용","m",2100,14702,0,16802,"합계"]
["MBE23110050S",null,"프레스식 접합 및 배관","D40, 옥외배관, 고소작업대 사용","m",2452,17164,0,19616,"합계"]
["MBE23110060S",null,"프레스식 접합 및 배관","D50, 옥외배관, 고소작업대 사용","m",2639,18476,0,21115,"합계"]
["MBE23110070S",null,"프레스식 접합 및 배관","D60, 옥외배관, 고소작업대 사용","m",3444,24114,0,27558,"합계"]
["MBE23110080S",null,"프레스식 접합 및 배관","D75, 옥외배관, 고소작업대 사용","m",3984,27888,0,31872,"합계"]
["MBE23110090S",null,"프레스식 접합 및 배관","D80, 옥외배관, 고소작업대 사용","m",5226,36586,0,41812,"합계"]
["MBE23110100S",null,"프레스식 접합 및 배관","D100, 옥외배관, 고소작업대 사용","m",6094,42662,0,48756,"합계"]
["MBE30010010S",null,"주름관 접합 및 배관","D15","m",245,12272,0,12517,"합계"]
["MBE30010020S",null,"주름관 접합 및 배관","D20","m",281,14081,0,14362,"합계"]
["MBE30110010S",null,"주름관 접합 및 배관","D15, 고소작업대 사용","m",1227,9817,0,11044,"합계"]
["MBE30110020S",null,"주름관 접합 및 배관","D20, 고소작업대 사용","m",1408,11265,0,12673,"합계"]
["MBG00010010S",null,"기계식 접합 및 배관","D50","개소",965,48290,0,49255,"합계"]
["MBG00010020S",null,"기계식 접합 및 배관","D65","개소",1180,59023,0,60203,"합계"]
["MBG00010030S",null,"기계식 접합 및 배관","D75","개소",1316,65817,0,67133,"합계"]
["MBG00010040S",null,"기계식 접합 및 배관","D100","개소",1671,83574,0,85245,"합계"]
["MBG00010050S",null,"기계식 접합 및 배관","D125","개소",2012,100643,0,102655,"합계"]
["MBG00010060S",null,"기계식 접합 및 배관","D150","개소",2261,113084,0,115345,"합계"]
["MBG00010070S",null,"기계식 접합 및 배관","D200","개소",2910,145512,0,148422,"합계"]
["MBG00110010S",null,"기계식 접합 및 배관","D50, 고소작업대 사용","개소",4829,38632,0,43461,"합계"]
["MBG00110020S",null,"기계식 접합 및 배관","D65, 고소작업대 사용","개소",5902,47218,0,53120,"합계"]
["MBG00110030S",null,"기계식 접합 및 배관","D75, 고소작업대 사용","개소",6581,52654,0,59235,"합계"]
["MBG00110040S",null,"기계식 접합 및 배관","D100, 고소작업대 사용","개소",8357,66859,0,75216,"합계"]
["MBG00110050S",null,"기계식 접합 및 배관","D125, 고소작업대 사용","개소",10064,80514,0,90578,"합계"]
["MBG00110060S",null,"기계식 접합 및 배관","D150, 고소작업대 사용","개소",11308,90467,0,101775,"합계"]
["MBG00110070S",null,"기계식 접합 및 배관","D200, 고소작업대 사용","개소",14551,116410,0,130961,"합계"]
["MBG10010010S",null," 수밀밴드접합 및 배관","D50","개소",874,43741,0,44615,"합계"]
["MBG10010020S",null," 수밀밴드접합 및 배관","D65","개소",1077,53899,0,54976,"합계"]
["MBG10010030S",null," 수밀밴드접합 및 배관","D75","개소",1210,60539,0,61749,"합계"]
["MBG10010040S",null," 수밀밴드접합 및 배관","D100","개소",1542,77107,0,78649,"합계"]
["MBG10010050S",null," 수밀밴드접합 및 배관","D125","개소",1873,93676,0,95549,"합계"]
["MBG10010060S",null," 수밀밴드접합 및 배관","D150","개소",2209,110474,0,112683,"합계"]
["MBG10010070S",null," 수밀밴드접합 및 배관","D200","개소",2720,136015,0,138735,"합계"]
["MBG10110010S",null," 수밀밴드접합 및 배관","D50, 고소작업대 사용","개소",4374,34993,0,39367,"합계"]
["MBG10110020S",null," 수밀밴드접합 및 배관","D65, 고소작업대 사용","개소",5389,43119,0,48508,"합계"]
["MBG10110030S",null," 수밀밴드접합 및 배관","D75, 고소작업대 사용","개소",6053,48431,0,54484,"합계"]
["MBG10110040S",null," 수밀밴드접합 및 배관","D100, 고소작업대 사용","개소",7710,61686,0,69396,"합계"]
["MBG10110050S",null," 수밀밴드접합 및 배관","D125, 고소작업대 사용","개소",9367,74941,0,84308,"합계"]
["MBG10110060S",null," 수밀밴드접합 및 배관","D150, 고소작업대 사용","개소",11047,88379,0,99426,"합계"]
["MBG10110070S",null," 수밀밴드접합 및 배관","D200, 고소작업대 사용","개소",13601,108812,0,122413,"합계"]
["MBI00010010S",null,"PVC관 접착제 접합 및 배관","D25","m",338,16910,0,17248,"합계"]
["MBI00010020S",null,"PVC관 접착제 접합 및 배관","D30","m",380,19013,0,19393,"합계"]
["MBI00010030S",null,"PVC관 접착제 접합 및 배관","D35","m",411,20556,0,20967,"합계"]
["MBI00010040S",null,"PVC관 접착제 접합 및 배관","D40","m",449,22493,0,22942,"합계"]
["MBI00010050S",null,"PVC관 접착제 접합 및 배관","D50","m",550,27516,0,28066,"합계"]
["MBI00010060S",null,"PVC관 접착제 접합 및 배관","D65","m",672,33633,0,34305,"합계"]
["MBI00010070S",null,"PVC관 접착제 접합 및 배관","D75","m",745,37278,0,38023,"합계"]
["MBI00010080S",null,"PVC관 접착제 접합 및 배관","D100","m",919,45984,0,46903,"합계"]
["MBI00010090S",null,"PVC관 접착제 접합 및 배관","D125","m",1098,54919,0,56017,"합계"]
["MBI00010100S",null,"PVC관 접착제 접합 및 배관","D150","m",1257,62898,0,64155,"합계"]
["MBI00010110S",null,"PVC관 접착제 접합 및 배관","D200","m",1591,79583,0,81174,"합계"]
["MBI00110010S",null,"PVC관 접착제 접합 및 배관","D25, 고소작업대 사용","m",1691,13528,0,15219,"합계"]
["MBI00110020S",null,"PVC관 접착제 접합 및 배관","D30, 고소작업대 사용","m",1901,15211,0,17112,"합계"]
["MBI00110030S",null,"PVC관 접착제 접합 및 배관","D35, 고소작업대 사용","m",2055,16444,0,18499,"합계"]
["MBI00110040S",null,"PVC관 접착제 접합 및 배관","D40, 고소작업대 사용","m",2249,17994,0,20243,"합계"]
["MBI00110050S",null,"PVC관 접착제 접합 및 배관","D50, 고소작업대 사용","m",2751,22012,0,24763,"합계"]
["MBI00110060S",null,"PVC관 접착제 접합 및 배관","D65, 고소작업대 사용","m",3363,26906,0,30269,"합계"]
["MBI00110070S",null,"PVC관 접착제 접합 및 배관","D75, 고소작업대 사용","m",3727,29822,0,33549,"합계"]
["MBI00110080S",null,"PVC관 접착제 접합 및 배관","D100, 고소작업대 사용","m",4598,36787,0,41385,"합계"]
["MBI00110090S",null,"PVC관 접착제 접합 및 배관","D125, 고소작업대 사용","m",5491,43935,0,49426,"합계"]
["MBI00110100S",null,"PVC관 접착제 접합 및 배관","D150, 고소작업대 사용","m",6289,50318,0,56607,"합계"]
["MBI00110110S",null,"PVC관 접착제 접합 및 배관","D200, 고소작업대 사용","m",7958,63666,0,71624,"합계"]
["MBI10010010S",null,"PVC관 소켓 접합 및 배관","D10","m",132,6640,0,6772,"합계"]
["MBI10010020S",null,"PVC관 소켓 접합 및 배관","D13","m",136,6805,0,6941,"합계"]
["MBI10010030S",null,"PVC관 소켓 접합 및 배관","D16","m",140,7035,0,7175,"합계"]
["MBI10010040S",null,"PVC관 소켓 접합 및 배관","D20","m",148,7430,0,7578,"합계"]
["MBI10010050S",null,"PVC관 소켓 접합 및 배관","D25","m",161,8054,0,8215,"합계"]
["MBI10010060S",null,"PVC관 소켓 접합 및 배관","D30","m",165,8284,0,8449,"합계"]
["MBI10010070S",null,"PVC관 소켓 접합 및 배관","D35","m",173,8679,0,8852,"합계"]
["MBI10010080S",null,"PVC관 소켓 접합 및 배관","D40","m",186,9303,0,9489,"합계"]
["MBI10010090S",null,"PVC관 소켓 접합 및 배관","D50","m",215,10782,0,10997,"합계"]
["MBI10010100S",null,"PVC관 소켓 접합 및 배관","D65","m",243,12196,0,12439,"합계"]
["MBI10010110S",null,"PVC관 소켓 접합 및 배관","D75","m",310,15548,0,15858,"합계"]
["MBI10010111S",null,"PVC관 소켓 접합 및 배관","D100","m",406,20315,0,20721,"합계"]
["MBI10010112S",null,"PVC관 소켓 접합 및 배관","D125","m",479,23998,0,24477,"합계"]
["MBI10010113S",null,"PVC관 소켓 접합 및 배관","D150","m",600,30014,0,30614,"합계"]
["MBI10010114S",null,"PVC관 소켓 접합 및 배관","D200","m",753,37673,0,38426,"합계"]
["MBI10110010S",null,"PVC관 소켓 접합 및 배관","D10, 고소작업대 사용","m",664,5312,0,5976,"합계"]
["MBI10110020S",null,"PVC관 소켓 접합 및 배관","D13, 고소작업대 사용","m",680,5444,0,6124,"합계"]
["MBI10110030S",null,"PVC관 소켓 접합 및 배관","D16, 고소작업대 사용","m",703,5628,0,6331,"합계"]
["MBI10110040S",null,"PVC관 소켓 접합 및 배관","D20, 고소작업대 사용","m",743,5944,0,6687,"합계"]
["MBI10110050S",null,"PVC관 소켓 접합 및 배관","D25, 고소작업대 사용","m",805,6443,0,7248,"합계"]
["MBI10110060S",null,"PVC관 소켓 접합 및 배관","D30, 고소작업대 사용","m",828,6627,0,7455,"합계"]
["MBI10110070S",null,"PVC관 소켓 접합 및 배관","D35, 고소작업대 사용","m",867,6943,0,7810,"합계"]
["MBI10110080S",null,"PVC관 소켓 접합 및 배관","D40, 고소작업대 사용","m",930,7442,0,8372,"합계"]
["MBI10110090S",null,"PVC관 소켓 접합 및 배관","D50, 고소작업대 사용","m",1078,8625,0,9703,"합계"]
["MBI10110100S",null,"PVC관 소켓 접합 및 배관","D65, 고소작업대 사용","m",1219,9757,0,10976,"합계"]
["MBI10110110S",null,"PVC관 소켓 접합 및 배관","D75, 고소작업대 사용","m",1554,12438,0,13992,"합계"]
["MBI10110120S",null,"PVC관 소켓 접합 및 배관","D100, 고소작업대 사용","m",2031,16252,0,18283,"합계"]
["MBI10110130S",null,"PVC관 소켓 접합 및 배관","D125, 고소작업대 사용","m",2399,19198,0,21597,"합계"]
["MBI10110140S",null,"PVC관 소켓 접합 및 배관","D150, 고소작업대 사용","m",3001,24011,0,27012,"합계"]
["MBI10110150S",null,"PVC관 소켓 접합 및 배관","D200, 고소작업대 사용","m",3767,30138,0,33905,"합계"]
["MBK00010010S",null,"PB관 일반접합 및 배관","D16","m",112,11203,0,11315,"합계"]
["MBK00010020S",null,"PB관 일반접합 및 배관","D20","m",124,12452,0,12576,"합계"]
["MBK10010010S",null,"PB 이중관 접합 및 배관","D16","m",144,14491,0,14635,"합계"]
["MBK10010020S",null,"PB 이중관 접합 및 배관","D20","m",159,15970,0,16129,"합계"]
["MBK20010010S",null,"PE관 접합 및 배관","D16","m",89,8972,0,9061,"합계"]
["MBK20010020S",null,"PE관 접합 및 배관","D20","m",112,11241,0,11353,"합계"]
["MCA10000000S",null,"아연도금강판덕트(스파이럴덕트) 설치","고소작업대 미사용/철판두께, 덕트 직경에 따른 시공량(m) 참조","인/일",15733,786689,0,802422,"합계"]
["MCA10010010S",null,"아연도금강판 스파이럴덕트 설치","D80∼150, t 0.5mm ","m",582,29107,0,29689,"합계"]
["MCA10010020S",null,"아연도금강판 스파이럴덕트 설치","D160, t 0.5mm ","m",712,35608,0,36320,"합계"]
["MCA10010030S",null,"아연도금강판 스파이럴덕트 설치","D180, t 0.5mm ","m",712,35608,0,36320,"합계"]
["MCA10010040S",null,"아연도금강판 스파이럴덕트 설치","D200, t 0.5mm ","m",712,35608,0,36320,"합계"]
["MCA10010050S",null,"아연도금강판 스파이럴덕트 설치","D225, t 0.6mm ","m",876,43847,0,44723,"합계"]
["MCA10010060S",null,"아연도금강판 스파이럴덕트 설치","D250, t 0.6mm ","m",876,43847,0,44723,"합계"]
["MCA10010070S",null,"아연도금강판 스파이럴덕트 설치","D275, t 0.6mm ","m",1050,52501,0,53551,"합계"]
["MCA10010080S",null,"아연도금강판 스파이럴덕트 설치","D300, t 0.6mm ","m",1050,52501,0,53551,"합계"]
["MCA10010090S",null,"아연도금강판 스파이럴덕트 설치","D350, t 0.6mm ","m",1310,65502,0,66812,"합계"]
["MCA10010100S",null,"아연도금강판 스파이럴덕트 설치","D400, t 0.6mm ","m",1310,65502,0,66812,"합계"]
["MCA10010110S",null,"아연도금강판 스파이럴덕트 설치","D450, t 0.6mm ","m",1730,86535,0,88265,"합계"]
["MCA10010120S",null,"아연도금강판 스파이럴덕트 설치","D500, t 0.6mm ","m",1730,86535,0,88265,"합계"]
["MCA10010130S",null,"아연도금강판 스파이럴덕트 설치","D550, t 0.6mm ","m",2244,112206,0,114450,"합계"]
["MCA10010140S",null,"아연도금강판 스파이럴덕트 설치","D600, t 0.6mm ","m",2244,112206,0,114450,"합계"]
["MCA10010150S",null,"아연도금강판 스파이럴덕트 설치","D650, t 0.8mm ","m",2633,131666,0,134299,"합계"]
["MCA10010160S",null,"아연도금강판 스파이럴덕트 설치","D700, t 0.8mm ","m",2633,131666,0,134299,"합계"]
["MCA10010170S",null,"아연도금강판 스파이럴덕트 설치","D750, t 0.8mm ","m",2633,131666,0,134299,"합계"]
["MCA10010180S",null,"아연도금강판 스파이럴덕트 설치","D800, t 0.8mm ","m",2633,131666,0,134299,"합계"]
["MCA10010190S",null,"아연도금강판 스파이럴덕트 설치","D850, t 1.0mm ","m",3146,157337,0,160483,"합계"]
["MCA10010200S",null,"아연도금강판 스파이럴덕트 설치","D900, t 1.0mm ","m",3146,157337,0,160483,"합계"]
["MCA10010210S",null,"아연도금강판 스파이럴덕트 설치","D950, t 1.0mm ","m",3146,157337,0,160483,"합계"]
["MCA10010220S",null,"아연도금강판 스파이럴덕트 설치","D1000, t 1.0mm ","m",3146,157337,0,160483,"합계"]
["MCA10100000S",null,"아연도금강판덕트(스파이럴덕트) 설치","고소작업대 사용/철판두께, 덕트 직경에 따른 시공량(m) 참조","인/일",78668,786689,0,865357,"합계"]
["MCA10110010S",null,"아연도금강판 스파이럴덕트 설치","D80∼150, t 0.5mm, 고소작업대 사용","m",2575,25753,0,28328,"합계"]
["MCA10110020S",null,"아연도금강판 스파이럴덕트 설치","D160, t 0.5mm, 고소작업대 사용","m",3167,31674,0,34841,"합계"]
["MCA10110030S",null,"아연도금강판 스파이럴덕트 설치","D180, t 0.5mm , 고소작업대 사용","m",3167,31674,0,34841,"합계"]
["MCA10110040S",null,"아연도금강판 스파이럴덕트 설치","D200, t 0.5mm , 고소작업대 사용","m",3167,31674,0,34841,"합계"]
["MCA10110050S",null,"아연도금강판 스파이럴덕트 설치","D225, t 0.6mm , 고소작업대 사용","m",3854,38547,0,42401,"합계"]
["MCA10110060S",null,"아연도금강판 스파이럴덕트 설치","D250, t 0.6mm , 고소작업대 사용","m",3854,38547,0,42401,"합계"]
["MCA10110070S",null,"아연도금강판 스파이럴덕트 설치","D275, t 0.6mm , 고소작업대 사용","m",4641,46414,0,51055,"합계"]
["MCA10110080S",null,"아연도금강판 스파이럴덕트 설치","D300, t 0.6mm , 고소작업대 사용","m",4641,46414,0,51055,"합계"]
["MCA10110090S",null,"아연도금강판 스파이럴덕트 설치","D350, t 0.6mm , 고소작업대 사용","m",5800,58007,0,63807,"합계"]
["MCA10110100S",null,"아연도금강판 스파이럴덕트 설치","D400, t 0.6mm , 고소작업대 사용","m",5800,58007,0,63807,"합계"]
["MCA10110110S",null,"아연도금강판 스파이럴덕트 설치","D450, t 0.6mm , 고소작업대 사용","m",7730,77302,0,85032,"합계"]
["MCA10110120S",null,"아연도금강판 스파이럴덕트 설치","D500, t 0.6mm , 고소작업대 사용","m",7730,77302,0,85032,"합계"]
["MCA10110130S",null,"아연도금강판 스파이럴덕트 설치","D550, t 0.6mm , 고소작업대 사용","m",10019,100199,0,110218,"합계"]
["MCA10110140S",null,"아연도금강판 스파이럴덕트 설치","D600, t 0.6mm, 고소작업대 사용 ","m",10019,100199,0,110218,"합계"]
["MCA10110150S",null,"아연도금강판 스파이럴덕트 설치","D650, t 0.8mm , 고소작업대 사용","m",11593,115932,0,127525,"합계"]
["MCA10110160S",null,"아연도금강판 스파이럴덕트 설치","D700, t 0.8mm , 고소작업대 사용","m",11593,115932,0,127525,"합계"]
["MCA10110170S",null,"아연도금강판 스파이럴덕트 설치","D750, t 0.8mm , 고소작업대 사용","m",11593,115932,0,127525,"합계"]
["MCA10110180S",null,"아연도금강판 스파이럴덕트 설치","D800, t 0.8mm , 고소작업대 사용","m",11593,115932,0,127525,"합계"]
["MCA10110190S",null,"아연도금강판 스파이럴덕트 설치","D850, t 1.0mm , 고소작업대 사용","m",13953,139533,0,153486,"합계"]
["MCA10110200S",null,"아연도금강판 스파이럴덕트 설치","D900, t 1.0mm , 고소작업대 사용","m",13953,139533,0,153486,"합계"]
["MCA10110210S",null,"아연도금강판 스파이럴덕트 설치","D950, t 1.0mm , 고소작업대 사용","m",13953,139533,0,153486,"합계"]
["MCA10110220S",null,"아연도금강판 스파이럴덕트 설치","D1000, t 1.0mm , 고소작업대 사용","m",13953,139533,0,153486,"합계"]
["MCA30000000S",null,"PVC덕트 설치","두께 3mm/일 시공량 15㎡","인/일",15733,786689,0,802422,"합계"]
["MCA30010010S",null,"PVC덕트 설치","3mm","㎡",1005,50267,0,51272,"합계"]
["MCA40000000S",null,"세대내 환기덕트 설치","204x60mm 이하/일 시공량 100m","인/일",11592,579641,0,591233,"합계"]
["MCA40010010S",null,"세대내 환기덕트 설치","204x60mm 이하 설치","m",115,5796,0,5911,"합계"]
["MCA50010010S",null,"플렉시블덕트 설치","D100","개소",0,10352,0,10352,"합계"]
["MCA50010020S",null,"플렉시블덕트 설치","D125","개소",0,12422,0,12422,"합계"]
["MCA50010030S",null,"플렉시블덕트 설치","D150","개소",0,16563,0,16563,"합계"]
["MCA50010040S",null,"플렉시블덕트 설치","D175","개소",0,18634,0,18634,"합계"]
["MCA50010050S",null,"플렉시블덕트 설치","D200","개소",0,20704,0,20704,"합계"]
["MCA50010060S",null,"플렉시블덕트 설치","D225","개소",0,22775,0,22775,"합계"]
["MCA50010070S",null,"플렉시블덕트 설치","D250","개소",0,24845,0,24845,"합계"]
["MCA50010080S",null,"플렉시블덕트 설치","D275","개소",0,28986,0,28986,"합계"]
["MCA50010090S",null,"플렉시블덕트 설치","D300","개소",0,35198,0,35198,"합계"]
["MCA50010100S",null,"플렉시블덕트 설치","D350","개소",0,43480,0,43480,"합계"]
["MCA50010110S",null,"플렉시블덕트 설치","D400","개소",0,51762,0,51762,"합계"]
["MCB00010010S",null,"취출구 설치","아네모디퓨저, 목지름100mm 이하","개",0,76193,0,76193,"합계"]
["MCB00010020S",null,"취출구 설치","아네모디퓨저, 목지름200mm 이하","개",0,89030,0,89030,"합계"]
["MCB00010030S",null,"취출구 설치","아네모디퓨저, 목지름300mm 이하","개",0,95242,0,95242,"합계"]
["MCB00010040S",null,"취출구 설치","아네모디퓨저, 목지름400mm 이하","개",0,101453,0,101453,"합계"]
["MCB00010050S",null,"취출구 설치","아네모디퓨저, 목지름500mm 이하","개",0,104559,0,104559,"합계"]
["MCB00010060S",null,"취출구 설치","아네모디퓨저, 목지름600mm 이하","개",0,114290,0,114290,"합계"]
["MCB00110010S",null,"취출구 설치","유니버설형, 단면적 0.04㎡ 이하","개",0,65220,0,65220,"합계"]
["MCB00110020S",null,"취출구 설치","유니버설형, 단면적 0.06㎡ 이하","개",0,66669,0,66669,"합계"]
["MCB00110030S",null,"취출구 설치","유니버설형, 단면적 0.08㎡ 이하","개",0,72052,0,72052,"합계"]
["MCB00110040S",null,"취출구 설치","유니버설형, 단면적 0.10㎡ 이하","개",0,75572,0,75572,"합계"]
["MCB00110050S",null,"취출구 설치","유니버설형, 단면적 0.15㎡ 이하","개",0,79092,0,79092,"합계"]
["MCB00110060S",null,"취출구 설치","유니버설형, 단면적 0.20㎡ 이하","개",0,87995,0,87995,"합계"]
["MCB00110070S",null,"취출구 설치","유니버설형, 단면적 0.25㎡ 이하","개",0,94827,0,94827,"합계"]
["MCB00110080S",null,"취출구 설치","유니버설형, 단면적 0.30㎡ 이하","개",0,107043,0,107043,"합계"]
["MCB00110090S",null,"취출구 설치","유니버설형, 단면적 0.35㎡ 이하","개",0,115946,0,115946,"합계"]
["MCB00110100S",null,"취출구 설치","유니버설형, 단면적 0.40㎡ 이하","개",0,138722,0,138722,"합계"]
["MCB00210010S",null,"취출구 설치","펀칭메탈형, 길이 1m 미만","개",0,52797,0,52797,"합계"]
["MCB00210020S",null,"취출구 설치","펀칭메탈형, 길이 1m 미만(셔터)","개",0,73709,0,73709,"합계"]
["MCB00210030S",null,"취출구 설치","펀칭메탈형, 길이 1m 이상","개",0,149281,0,149281,"합계"]
["MCB00210040S",null,"취출구 설치","펀칭메탈형, 길이 1m 이상(셔터)","개",0,209118,0,209118,"합계"]
["MCB00310010S",null,"취출구 설치","슬릿형, 변길이1m 미만","개",0,80748,0,80748,"합계"]
["MCB00310020S",null,"취출구 설치","슬릿형, 변길이1m 이상 ","개",0,228166,0,228166,"합계"]
["MCB10010010S",null,"흡입구 설치","도어그릴, 장변길이1m 미만","개",0,108700,0,108700,"합계"]
["MCB10010020S",null,"흡입구 설치","도어그릴, 장변길이1m 이상","개",0,173920,0,173920,"합계"]
["MCB10110010S",null,"흡입구 설치","점검구, 300x300 이하","개",0,73502,0,73502,"합계"]
["MCB10210010S",null,"흡입구 설치","후드 일반, 투영면적 ㎡당","개",0,165638,0,165638,"합계"]
["MCB10310010S",null,"흡입구 설치","후드 2중, 투영면적 ㎡당","개",0,198766,0,198766,"합계"]
["MCB10410010S",null,"흡입구 설치","후드 그리스필터, 투영면적 ㎡당","개",0,178061,0,178061,"합계"]
["MCB10510010S",null,"흡입구 설치","후드 2중그리스필터, 투영면적 ㎡당","개",0,207048,0,207048,"합계"]
["MCB20010010S",null,"덕트 플렉시블조인트","송풍기규격 032(#2)","개소",0,52708,0,52708,"합계"]
["MCB20010020S",null,"덕트 플렉시블조인트","송풍기규격 036(#2⅓)","개소",0,58629,0,58629,"합계"]
["MCB20010030S",null,"덕트 플렉시블조인트","송풍기규격 040(#2⅔)","개소",0,64922,0,64922,"합계"]
["MCB20010040S",null,"덕트 플렉시블조인트","송풍기규격 045(#3)","개소",0,73411,0,73411,"합계"]
["MCB20010050S",null,"덕트 플렉시블조인트","송풍기규격 050(#3⅓)","개소",0,82313,0,82313,"합계"]
["MCB20010060S",null,"덕트 플렉시블조인트","송풍기규격 056(#3⅔)","개소",0,93947,0,93947,"합계"]
["MCB20010070S",null,"덕트 플렉시블조인트","송풍기규격 063(#4)","개소",0,108356,0,108356,"합계"]
["MCB20010080S",null,"덕트 플렉시블조인트","송풍기규격 071(#4⅔)","개소",0,126699,0,126699,"합계"]
["MCB20010090S",null,"덕트 플렉시블조인트","송풍기규격 080(#5⅓)","개소",0,148602,0,148602,"합계"]
["MCB20010100S",null,"덕트 플렉시블조인트","송풍기규격 090(#6)","개소",0,175474,0,175474,"합계"]
["MCB20010110S",null,"덕트 플렉시블조인트","송풍기규격 100(#6⅔)","개소",0,204664,0,204664,"합계"]
["MCB20010120S",null,"덕트 플렉시블조인트","송풍기규격 112(#7½)","개소",0,242964,0,242964,"합계"]
["MCB20010130S",null,"덕트 플렉시블조인트","송풍기규격 125(#8⅓)","개소",0,288137,0,288137,"합계"]
["MCB20010140S",null,"덕트 플렉시블조인트","송풍기규격 140(#9⅓)","개소",0,345193,0,345193,"합계"]
["MCB20010150S",null,"덕트 플렉시블조인트","송풍기규격 160(#10⅔)","개소",0,429659,0,429659,"합계"]
["MCB20010160S",null,"덕트 플렉시블조인트","송풍기규격 180(#12)","개소",0,523607,0,523607,"합계"]
["MCB30010010S",null,"일반댐퍼(사각) 설치"," 방화댐퍼, 0.1㎡이하","개",0,85924,0,85924,"합계"]
["MCB30010020S",null,"일반댐퍼(사각) 설치"," 방화댐퍼, 0.1㎡ 증마다 가산","개",0,25881,0,25881,"합계"]
["MCB30110010S",null,"일반댐퍼(사각) 설치","풍량조절댐퍼(수동식), 0.1㎡이하","개",0,77643,0,77643,"합계"]
["MCB30110020S",null,"일반댐퍼(사각) 설치","풍량조절댐퍼(수동식), 0.1㎡ 증마다 가산","개",0,22775,0,22775,"합계"]
["MCB40010010S",null,"일반댐퍼(원형) 설치"," 방화댐퍼, D100이하","개",0,60458,0,60458,"합계"]
["MCB40010020S",null,"일반댐퍼(원형) 설치"," 방화댐퍼, D200이하","개",0,71638,0,71638,"합계"]
["MCB40010030S",null,"일반댐퍼(원형) 설치"," 방화댐퍼, D300이하","개",0,83440,0,83440,"합계"]
["MCB40110010S",null,"일반댐퍼(원형) 설치","풍량조절댐퍼(수동식), D100 이하","개",0,54660,0,54660,"합계"]
["MCB40110020S",null,"일반댐퍼(원형) 설치","풍량조절댐퍼(수동식), D200 이하","개",0,64806,0,64806,"합계"]
["MCB40110030S",null,"일반댐퍼(원형) 설치","풍량조절댐퍼(수동식), D300 이하","개",0,75365,0,75365,"합계"]
["MCB50010010S",null,"제연댐퍼 설치 ","수직덕트연결방식","㎡",10398,519925,0,530323,"합계"]
["MCB50110010S",null,"제연댐퍼 설치 ","승강로 연결방식","㎡",6194,309711,0,315905,"합계"]
["MDA00000000S",null,"일반마감 배관보온","보온재 재질, 두께, 마감방식, 시공위치 등에 따른 시공량(m)  참조","인/일",0,574115,0,574115,"합계"]
["MDA00010010S",null,"관보온/고무발포보온재","D15, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,6685,0,6685,"합계"]
["MDA00010020S",null,"관보온/고무발포보온재","D20, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,7463,0,7463,"합계"]
["MDA00010030S",null,"관보온/고무발포보온재","D25, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,8407,0,8407,"합계"]
["MDA00010040S",null,"관보온/고무발포보온재","D32, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,9759,0,9759,"합계"]
["MDA00010050S",null,"관보온/고무발포보온재","D40, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,11482,0,11482,"합계"]
["MDA00010060S",null,"관보온/고무발포보온재","D50, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,13574,0,13574,"합계"]
["MDA00010070S",null,"관보온/고무발포보온재","D65, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,15705,0,15705,"합계"]
["MDA00010080S",null,"관보온/고무발포보온재","D80, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,19149,0,19149,"합계"]
["MDA00010090S",null,"관보온/고무발포보온재","D100, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,22390,0,22390,"합계"]
["MDA00010100S",null,"관보온/고무발포보온재","D125, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,27187,0,27187,"합계"]
["MDA00010110S",null,"관보온/고무발포보온재","D150, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,32354,0,32354,"합계"]
["MDA00010120S",null,"관보온/고무발포보온재","D200, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,43058,0,43058,"합계"]
["MDA00010130S",null,"관보온/고무발포보온재","D250, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,51670,0,51670,"합계"]
["MDA00010140S",null,"관보온/고무발포보온재","D300, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,57411,0,57411,"합계"]
["MDA00110010S",null,"관보온/고무발포보온재","D15, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,7463,0,7463,"합계"]
["MDA00110020S",null,"관보온/고무발포보온재","D20, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,8407,0,8407,"합계"]
["MDA00110030S",null,"관보온/고무발포보온재","D25, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,9185,0,9185,"합계"]
["MDA00110040S",null,"관보온/고무발포보온재","D32, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,10908,0,10908,"합계"]
["MDA00110050S",null,"관보온/고무발포보온재","D40, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,12630,0,12630,"합계"]
["MDA00110060S",null,"관보온/고무발포보온재","D50, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,15131,0,15131,"합계"]
["MDA00110070S",null,"관보온/고무발포보온재","D65, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,17427,0,17427,"합계"]
["MDA00110080S",null,"관보온/고무발포보온재","D80, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,21242,0,21242,"합계"]
["MDA00110090S",null,"관보온/고무발포보온재","D100, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,24891,0,24891,"합계"]
["MDA00110100S",null,"관보온/고무발포보온재","D125, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,30223,0,30223,"합계"]
["MDA00110110S",null,"관보온/고무발포보온재","D150, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,35964,0,35964,"합계"]
["MDA00110120S",null,"관보온/고무발포보온재","D200, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,47855,0,47855,"합계"]
["MDA00110130S",null,"관보온/고무발포보온재","D250, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,57411,0,57411,"합계"]
["MDA00110140S",null,"관보온/고무발포보온재","D300, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,63152,0,63152,"합계"]
["MDA00210010S",null,"관보온/고무발포보온재","D15, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,8611,0,8611,"합계"]
["MDA00210020S",null,"관보온/고무발포보온재","D20, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,9759,0,9759,"합계"]
["MDA00210030S",null,"관보온/고무발포보온재","D25, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,10703,0,10703,"합계"]
["MDA00210040S",null,"관보온/고무발포보온재","D32, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,12426,0,12426,"합계"]
["MDA00210050S",null,"관보온/고무발포보온재","D40, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,14722,0,14722,"합계"]
["MDA00210060S",null,"관보온/고무발포보온재","D50, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,17223,0,17223,"합계"]
["MDA00210070S",null,"관보온/고무발포보온재","D65, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,20093,0,20093,"합계"]
["MDA00210080S",null,"관보온/고무발포보온재","D80, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,24482,0,24482,"합계"]
["MDA00210090S",null,"관보온/고무발포보온재","D100, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,28705,0,28705,"합계"]
["MDA00210100S",null,"관보온/고무발포보온재","D125, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,34651,0,34651,"합계"]
["MDA00210110S",null,"관보온/고무발포보온재","D150, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,41336,0,41336,"합계"]
["MDA00210120S",null,"관보온/고무발포보온재","D200, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,55115,0,55115,"합계"]
["MDA00210130S",null,"관보온/고무발포보온재","D250, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,65195,0,65195,"합계"]
["MDA00210140S",null,"관보온/고무발포보온재","D300, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,74634,0,74634,"합계"]
["MDA00310010S",null,"관보온/고무발포보온재","D15, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,10908,0,10908,"합계"]
["MDA00310020S",null,"관보온/고무발포보온재","D20, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,12260,0,12260,"합계"]
["MDA00310030S",null,"관보온/고무발포보온재","D25, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,13000,0,13000,"합계"]
["MDA00310040S",null,"관보온/고무발포보온재","D32, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,15131,0,15131,"합계"]
["MDA00310050S",null,"관보온/고무발포보온재","D40, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,17797,0,17797,"합계"]
["MDA00310060S",null,"관보온/고무발포보온재","D50, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,20668,0,20668,"합계"]
["MDA00310070S",null,"관보온/고무발포보온재","D65, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,22390,0,22390,"합계"]
["MDA00310080S",null,"관보온/고무발포보온재","D80, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,25835,0,25835,"합계"]
["MDA00310090S",null,"관보온/고무발포보온재","D100, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,28705,0,28705,"합계"]
["MDA00310100S",null,"관보온/고무발포보온재","D125, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,34446,0,34446,"합계"]
["MDA00310110S",null,"관보온/고무발포보온재","D150, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,39818,0,39818,"합계"]
["MDA00310120S",null,"관보온/고무발포보온재","D200, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,47077,0,47077,"합계"]
["MDA00310130S",null,"관보온/고무발포보온재","D250, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,57411,0,57411,"합계"]
["MDA00310140S",null,"관보온/고무발포보온재","D300, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,65195,0,65195,"합계"]
["MDA00410010S",null,"관보온/고무발포보온재","D15, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,12260,0,12260,"합계"]
["MDA00410020S",null,"관보온/고무발포보온재","D20, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,13778,0,13778,"합계"]
["MDA00410030S",null,"관보온/고무발포보온재","D25, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,14352,0,14352,"합계"]
["MDA00410040S",null,"관보온/고무발포보온재","D32, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,16853,0,16853,"합계"]
["MDA00410050S",null,"관보온/고무발포보온재","D40, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,19724,0,19724,"합계"]
["MDA00410060S",null,"관보온/고무발포보온재","D50, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,22964,0,22964,"합계"]
["MDA00410070S",null,"관보온/고무발포보온재","D65, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,24891,0,24891,"합계"]
["MDA00410080S",null,"관보온/고무발포보온재","D80, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,28705,0,28705,"합계"]
["MDA00410090S",null,"관보온/고무발포보온재","D100, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,31946,0,31946,"합계"]
["MDA00410100S",null,"관보온/고무발포보온재","D125, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,38261,0,38261,"합계"]
["MDA00410110S",null,"관보온/고무발포보온재","D150, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,44206,0,44206,"합계"]
["MDA00410120S",null,"관보온/고무발포보온재","D200, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,52244,0,52244,"합계"]
["MDA00410130S",null,"관보온/고무발포보온재","D250, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,63152,0,63152,"합계"]
["MDA00410140S",null,"관보온/고무발포보온재","D300, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,72592,0,72592,"합계"]
["MDA00510010S",null,"관보온/고무발포보온재","D15, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,13982,0,13982,"합계"]
["MDA00510020S",null,"관보온/고무발포보온재","D20, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,15705,0,15705,"합계"]
["MDA00510030S",null,"관보온/고무발포보온재","D25, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,16445,0,16445,"합계"]
["MDA00510040S",null,"관보온/고무발포보온재","D32, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,19519,0,19519,"합계"]
["MDA00510050S",null,"관보온/고무발포보온재","D40, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,22760,0,22760,"합계"]
["MDA00510060S",null,"관보온/고무발포보온재","D50, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,26409,0,26409,"합계"]
["MDA00510070S",null,"관보온/고무발포보온재","D65, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,28705,0,28705,"합계"]
["MDA00510080S",null,"관보온/고무발포보온재","D80, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,32928,0,32928,"합계"]
["MDA00510090S",null,"관보온/고무발포보온재","D100, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,36743,0,36743,"합계"]
["MDA00510100S",null,"관보온/고무발포보온재","D125, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,44002,0,44002,"합계"]
["MDA00510110S",null,"관보온/고무발포보온재","D150, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,50726,0,50726,"합계"]
["MDA00510120S",null,"관보온/고무발포보온재","D200, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,59454,0,59454,"합계"]
["MDA00510130S",null,"관보온/고무발포보온재","D250, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,74634,0,74634,"합계"]
["MDA00510140S",null,"관보온/고무발포보온재","D300, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,82418,0,82418,"합계"]
["MDA01010010S",null,"관보온/고무발포보온재","D15, 보온두께 25mm 이하, 일반접합, 기계실","m",0,8037,0,8037,"합계"]
["MDA01010020S",null,"관보온/고무발포보온재","D20, 보온두께 25mm 이하, 일반접합, 기계실","m",0,8981,0,8981,"합계"]
["MDA01010030S",null,"관보온/고무발포보온재","D25, 보온두께 25mm 이하, 일반접합, 기계실","m",0,9759,0,9759,"합계"]
["MDA01010040S",null,"관보온/고무발포보온재","D32, 보온두께 25mm 이하, 일반접합, 기계실","m",0,11482,0,11482,"합계"]
["MDA01010050S",null,"관보온/고무발포보온재","D40, 보온두께 25mm 이하, 일반접합, 기계실","m",0,13574,0,13574,"합계"]
["MDA01010060S",null,"관보온/고무발포보온재","D50, 보온두께 25mm 이하, 일반접합, 기계실","m",0,16075,0,16075,"합계"]
["MDA01010070S",null,"관보온/고무발포보온재","D65, 보온두께 25mm 이하, 일반접합, 기계실","m",0,18371,0,18371,"합계"]
["MDA01010080S",null,"관보온/고무발포보온재","D80, 보온두께 25mm 이하, 일반접합, 기계실","m",0,22594,0,22594,"합계"]
["MDA01010090S",null,"관보온/고무발포보온재","D100, 보온두께 25mm 이하, 일반접합, 기계실","m",0,26613,0,26613,"합계"]
["MDA01010100S",null,"관보온/고무발포보온재","D125, 보온두께 25mm 이하, 일반접합, 기계실","m",0,32150,0,32150,"합계"]
["MDA01010110S",null,"관보온/고무발포보온재","D150, 보온두께 25mm 이하, 일반접합, 기계실","m",0,38095,0,38095,"합계"]
["MDA01010120S",null,"관보온/고무발포보온재","D200, 보온두께 25mm 이하, 일반접합, 기계실","m",0,50891,0,50891,"합계"]
["MDA01010130S",null,"관보온/고무발포보온재","D250, 보온두께 25mm 이하, 일반접합, 기계실","m",0,61109,0,61109,"합계"]
["MDA01010140S",null,"관보온/고무발포보온재","D300, 보온두께 25mm 이하, 일반접합, 기계실","m",0,68893,0,68893,"합계"]
["MDA01110010S",null,"관보온/고무발포보온재","D15, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,8981,0,8981,"합계"]
["MDA01110020S",null,"관보온/고무발포보온재","D20, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,10129,0,10129,"합계"]
["MDA01110030S",null,"관보온/고무발포보온재","D25, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,11112,0,11112,"합계"]
["MDA01110040S",null,"관보온/고무발포보온재","D32, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,13000,0,13000,"합계"]
["MDA01110050S",null,"관보온/고무발포보온재","D40, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,15501,0,15501,"합계"]
["MDA01110060S",null,"관보온/고무발포보온재","D50, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,18167,0,18167,"합계"]
["MDA01110070S",null,"관보온/고무발포보온재","D65, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,21037,0,21037,"합계"]
["MDA01110080S",null,"관보온/고무발포보온재","D80, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,25630,0,25630,"합계"]
["MDA01110090S",null,"관보온/고무발포보온재","D100, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,30058,0,30058,"합계"]
["MDA01110100S",null,"관보온/고무발포보온재","D125, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,36373,0,36373,"합계"]
["MDA01110110S",null,"관보온/고무발포보온재","D150, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,43262,0,43262,"합계"]
["MDA01110120S",null,"관보온/고무발포보온재","D200, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,57411,0,57411,"합계"]
["MDA01110130S",null,"관보온/고무발포보온재","D250, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,68893,0,68893,"합계"]
["MDA01110140S",null,"관보온/고무발포보온재","D300, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,76677,0,76677,"합계"]
["MDA01210010S",null,"관보온/고무발포보온재","D15, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,10703,0,10703,"합계"]
["MDA01210020S",null,"관보온/고무발포보온재","D20, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,12056,0,12056,"합계"]
["MDA01210030S",null,"관보온/고무발포보온재","D25, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,13204,0,13204,"합계"]
["MDA01210040S",null,"관보온/고무발포보온재","D32, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,15501,0,15501,"합계"]
["MDA01210050S",null,"관보온/고무발포보온재","D40, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,18167,0,18167,"합계"]
["MDA01210060S",null,"관보온/고무발포보온재","D50, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,21612,0,21612,"합계"]
["MDA01210070S",null,"관보온/고무발포보온재","D65, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,24891,0,24891,"합계"]
["MDA01210080S",null,"관보온/고무발포보온재","D80, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,30428,0,30428,"합계"]
["MDA01210090S",null,"관보온/고무발포보온재","D100, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,35595,0,35595,"합계"]
["MDA01210100S",null,"관보온/고무발포보온재","D125, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,43058,0,43058,"합계"]
["MDA01210110S",null,"관보온/고무발포보온재","D150, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,51300,0,51300,"합계"]
["MDA01210120S",null,"관보온/고무발포보온재","D200, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,68893,0,68893,"합계"]
["MDA01210130S",null,"관보온/고무발포보온재","D250, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,82418,0,82418,"합계"]
["MDA01210140S",null,"관보온/고무발포보온재","D300, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,91858,0,91858,"합계"]
["MDA01310010S",null,"관보온/고무발포보온재","D15, 보온두께 50mm 이하, 일반접합, 기계실","m",0,13000,0,13000,"합계"]
["MDA01310020S",null,"관보온/고무발포보온재","D20, 보온두께 50mm 이하, 일반접합, 기계실","m",0,14557,0,14557,"합계"]
["MDA01310030S",null,"관보온/고무발포보온재","D25, 보온두께 50mm 이하, 일반접합, 기계실","m",0,15296,0,15296,"합계"]
["MDA01310040S",null,"관보온/고무발포보온재","D32, 보온두께 50mm 이하, 일반접합, 기계실","m",0,18001,0,18001,"합계"]
["MDA01310050S",null,"관보온/고무발포보온재","D40, 보온두께 50mm 이하, 일반접합, 기계실","m",0,21037,0,21037,"합계"]
["MDA01310060S",null,"관보온/고무발포보온재","D50, 보온두께 50mm 이하, 일반접합, 기계실","m",0,24482,0,24482,"합계"]
["MDA01310070S",null,"관보온/고무발포보온재","D65, 보온두께 50mm 이하, 일반접합, 기계실","m",0,26613,0,26613,"합계"]
["MDA01310080S",null,"관보온/고무발포보온재","D80, 보온두께 50mm 이하, 일반접합, 기계실","m",0,30428,0,30428,"합계"]
["MDA01310090S",null,"관보온/고무발포보온재","D100, 보온두께 50mm 이하, 일반접합, 기계실","m",0,33872,0,33872,"합계"]
["MDA01310100S",null,"관보온/고무발포보온재","D125, 보온두께 50mm 이하, 일반접합, 기계실","m",0,40762,0,40762,"합계"]
["MDA01310110S",null,"관보온/고무발포보온재","D150, 보온두께 50mm 이하, 일반접합, 기계실","m",0,47077,0,47077,"합계"]
["MDA01310120S",null,"관보온/고무발포보온재","D200, 보온두께 50mm 이하, 일반접합, 기계실","m",0,55484,0,55484,"합계"]
["MDA01310130S",null,"관보온/고무발포보온재","D250, 보온두께 50mm 이하, 일반접합, 기계실","m",0,68893,0,68893,"합계"]
["MDA01310140S",null,"관보온/고무발포보온재","D300, 보온두께 50mm 이하, 일반접합, 기계실","m",0,76677,0,76677,"합계"]
["MDA01410010S",null,"관보온/고무발포보온재","D15, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,14722,0,14722,"합계"]
["MDA01410020S",null,"관보온/고무발포보온재","D20, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,16445,0,16445,"합계"]
["MDA01410030S",null,"관보온/고무발포보온재","D25, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,17223,0,17223,"합계"]
["MDA01410040S",null,"관보온/고무발포보온재","D32, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,20298,0,20298,"합계"]
["MDA01410050S",null,"관보온/고무발포보온재","D40, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,23908,0,23908,"합계"]
["MDA01410060S",null,"관보온/고무발포보온재","D50, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,27557,0,27557,"합계"]
["MDA01410070S",null,"관보온/고무발포보온재","D65, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,30058,0,30058,"합계"]
["MDA01410080S",null,"관보온/고무발포보온재","D80, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,34446,0,34446,"합계"]
["MDA01410090S",null,"관보온/고무발포보온재","D100, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,38465,0,38465,"합계"]
["MDA01410100S",null,"관보온/고무발포보온재","D125, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,46133,0,46133,"합계"]
["MDA01410110S",null,"관보온/고무발포보온재","D150, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,53188,0,53188,"합계"]
["MDA01410120S",null,"관보온/고무발포보온재","D200, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,63152,0,63152,"합계"]
["MDA01410130S",null,"관보온/고무발포보온재","D250, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,76677,0,76677,"합계"]
["MDA01410140S",null,"관보온/고무발포보온재","D300, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,86117,0,86117,"합계"]
["MDA01510010S",null,"관보온/고무발포보온재","D15, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,17427,0,17427,"합계"]
["MDA01510020S",null,"관보온/고무발포보온재","D20, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,19519,0,19519,"합계"]
["MDA01510030S",null,"관보온/고무발포보온재","D25, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,20463,0,20463,"합계"]
["MDA01510040S",null,"관보온/고무발포보온재","D32, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,24112,0,24112,"합계"]
["MDA01510050S",null,"관보온/고무발포보온재","D40, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,28335,0,28335,"합계"]
["MDA01510060S",null,"관보온/고무발포보온재","D50, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,32724,0,32724,"합계"]
["MDA01510070S",null,"관보온/고무발포보온재","D65, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,35595,0,35595,"합계"]
["MDA01510080S",null,"관보온/고무발포보온재","D80, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,40966,0,40966,"합계"]
["MDA01510090S",null,"관보온/고무발포보온재","D100, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,45559,0,45559,"합계"]
["MDA01510100S",null,"관보온/고무발포보온재","D125, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,54540,0,54540,"합계"]
["MDA01510110S",null,"관보온/고무발포보온재","D150, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,63152,0,63152,"합계"]
["MDA01510120S",null,"관보온/고무발포보온재","D200, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,74634,0,74634,"합계"]
["MDA01510130S",null,"관보온/고무발포보온재","D250, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,91858,0,91858,"합계"]
["MDA01510140S",null,"관보온/고무발포보온재","D300, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,103340,0,103340,"합계"]
["MDA10010010S",null,"관보온/고무발포보온재","D15, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,7259,0,7259,"합계"]
["MDA10010020S",null,"관보온/고무발포보온재","D20, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,8241,0,8241,"합계"]
["MDA10010030S",null,"관보온/고무발포보온재","D25, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,9185,0,9185,"합계"]
["MDA10010040S",null,"관보온/고무발포보온재","D32, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,10538,0,10538,"합계"]
["MDA10010050S",null,"관보온/고무발포보온재","D40, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,12630,0,12630,"합계"]
["MDA10010060S",null,"관보온/고무발포보온재","D50, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,14926,0,14926,"합계"]
["MDA10010070S",null,"관보온/고무발포보온재","D65, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,17019,0,17019,"합계"]
["MDA10010080S",null,"관보온/고무발포보온재","D80, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,20872,0,20872,"합계"]
["MDA10010090S",null,"관보온/고무발포보온재","D100, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,24482,0,24482,"합계"]
["MDA10010100S",null,"관보온/고무발포보온재","D125, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,29649,0,29649,"합계"]
["MDA10010110S",null,"관보온/고무발포보온재","D150, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,35225,0,35225,"합계"]
["MDA10010120S",null,"관보온/고무발포보온재","D200, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,46873,0,46873,"합계"]
["MDA10010130S",null,"관보온/고무발포보온재","D250, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,56263,0,56263,"합계"]
["MDA10010140S",null,"관보온/고무발포보온재","D300, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,63152,0,63152,"합계"]
["MDA10110010S",null,"관보온/고무발포보온재","D15, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,8241,0,8241,"합계"]
["MDA10110020S",null,"관보온/고무발포보온재","D20, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,9185,0,9185,"합계"]
["MDA10110030S",null,"관보온/고무발포보온재","D25, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,10129,0,10129,"합계"]
["MDA10110040S",null,"관보온/고무발포보온재","D32, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,11852,0,11852,"합계"]
["MDA10110050S",null,"관보온/고무발포보온재","D40, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,13982,0,13982,"합계"]
["MDA10110060S",null,"관보온/고무발포보온재","D50, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,16649,0,16649,"합계"]
["MDA10110070S",null,"관보온/고무발포보온재","D65, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,19149,0,19149,"합계"]
["MDA10110080S",null,"관보온/고무발포보온재","D80, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,23334,0,23334,"합계"]
["MDA10110090S",null,"관보온/고무발포보온재","D100, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,27557,0,27557,"합계"]
["MDA10110100S",null,"관보온/고무발포보온재","D125, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,33298,0,33298,"합계"]
["MDA10110110S",null,"관보온/고무발포보온재","D150, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,39409,0,39409,"합계"]
["MDA10110120S",null,"관보온/고무발포보온재","D200, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,52614,0,52614,"합계"]
["MDA10110130S",null,"관보온/고무발포보온재","D250, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,63152,0,63152,"합계"]
["MDA10110140S",null,"관보온/고무발포보온재","D300, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,68893,0,68893,"합계"]
["MDA10210010S",null,"관보온/고무발포보온재","D15, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,9555,0,9555,"합계"]
["MDA10210020S",null,"관보온/고무발포보온재","D20, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,10908,0,10908,"합계"]
["MDA10210030S",null,"관보온/고무발포보온재","D25, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,11852,0,11852,"합계"]
["MDA10210040S",null,"관보온/고무발포보온재","D32, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,13778,0,13778,"합계"]
["MDA10210050S",null,"관보온/고무발포보온재","D40, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,16279,0,16279,"합계"]
["MDA10210060S",null,"관보온/고무발포보온재","D50, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,19315,0,19315,"합계"]
["MDA10210070S",null,"관보온/고무발포보온재","D65, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,22390,0,22390,"합계"]
["MDA10210080S",null,"관보온/고무발포보온재","D80, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,27187,0,27187,"합계"]
["MDA10210090S",null,"관보온/고무발포보온재","D100, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,31946,0,31946,"합계"]
["MDA10210100S",null,"관보온/고무발포보온재","D125, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,38669,0,38669,"합계"]
["MDA10210110S",null,"관보온/고무발포보온재","D150, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,45929,0,45929,"합계"]
["MDA10210120S",null,"관보온/고무발포보온재","D200, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,61109,0,61109,"합계"]
["MDA10210130S",null,"관보온/고무발포보온재","D250, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,74634,0,74634,"합계"]
["MDA10210140S",null,"관보온/고무발포보온재","D300, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,80376,0,80376,"합계"]
["MDA10310010S",null,"관보온/고무발포보온재","D15, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,12056,0,12056,"합계"]
["MDA10310020S",null,"관보온/고무발포보온재","D20, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,13408,0,13408,"합계"]
["MDA10310030S",null,"관보온/고무발포보온재","D25, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,14148,0,14148,"합계"]
["MDA10310040S",null,"관보온/고무발포보온재","D32, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,16649,0,16649,"합계"]
["MDA10310050S",null,"관보온/고무발포보온재","D40, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,19519,0,19519,"합계"]
["MDA10310060S",null,"관보온/고무발포보온재","D50, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,22390,0,22390,"합계"]
["MDA10310070S",null,"관보온/고무발포보온재","D65, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,24482,0,24482,"합계"]
["MDA10310080S",null,"관보온/고무발포보온재","D80, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,28131,0,28131,"합계"]
["MDA10310090S",null,"관보온/고무발포보온재","D100, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,31206,0,31206,"합계"]
["MDA10310100S",null,"관보온/고무발포보온재","D125, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,37521,0,37521,"합계"]
["MDA10310110S",null,"관보온/고무발포보온재","D150, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,43262,0,43262,"합계"]
["MDA10310120S",null,"관보온/고무발포보온재","D200, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,51096,0,51096,"합계"]
["MDA10310130S",null,"관보온/고무발포보온재","D250, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,63152,0,63152,"합계"]
["MDA10310140S",null,"관보온/고무발포보온재","D300, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,70936,0,70936,"합계"]
["MDA10410010S",null,"관보온/고무발포보온재","D15, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,13408,0,13408,"합계"]
["MDA10410020S",null,"관보온/고무발포보온재","D20, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,14926,0,14926,"합계"]
["MDA10410030S",null,"관보온/고무발포보온재","D25, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,15705,0,15705,"합계"]
["MDA10410040S",null,"관보온/고무발포보온재","D32, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,18575,0,18575,"합계"]
["MDA10410050S",null,"관보온/고무발포보온재","D40, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,21816,0,21816,"합계"]
["MDA10410060S",null,"관보온/고무발포보온재","D50, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,25260,0,25260,"합계"]
["MDA10410070S",null,"관보온/고무발포보온재","D65, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,27557,0,27557,"합계"]
["MDA10410080S",null,"관보온/고무발포보온재","D80, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,31576,0,31576,"합계"]
["MDA10410090S",null,"관보온/고무발포보온재","D100, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,35020,0,35020,"합계"]
["MDA10410100S",null,"관보온/고무발포보온재","D125, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,42114,0,42114,"합계"]
["MDA10410110S",null,"관보온/고무발포보온재","D150, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,48595,0,48595,"합계"]
["MDA10410120S",null,"관보온/고무발포보온재","D200, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,57411,0,57411,"합계"]
["MDA10410130S",null,"관보온/고무발포보온재","D250, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,68893,0,68893,"합계"]
["MDA10410140S",null,"관보온/고무발포보온재","D300, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,78333,0,78333,"합계"]
["MDA10510010S",null,"관보온/고무발포보온재","D15, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,15705,0,15705,"합계"]
["MDA10510020S",null,"관보온/고무발포보온재","D20, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,17593,0,17593,"합계"]
["MDA10510030S",null,"관보온/고무발포보온재","D25, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,18371,0,18371,"합계"]
["MDA10510040S",null,"관보온/고무발포보온재","D32, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,21612,0,21612,"합계"]
["MDA10510050S",null,"관보온/고무발포보온재","D40, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,25260,0,25260,"합계"]
["MDA10510060S",null,"관보온/고무발포보온재","D50, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,29484,0,29484,"합계"]
["MDA10510070S",null,"관보온/고무발포보온재","D65, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,31946,0,31946,"합계"]
["MDA10510080S",null,"관보온/고무발포보온재","D80, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,36743,0,36743,"합계"]
["MDA10510090S",null,"관보온/고무발포보온재","D100, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,40762,0,40762,"합계"]
["MDA10510100S",null,"관보온/고무발포보온재","D125, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,49004,0,49004,"합계"]
["MDA10510110S",null,"관보온/고무발포보온재","D150, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,56633,0,56633,"합계"]
["MDA10510120S",null,"관보온/고무발포보온재","D200, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,66850,0,66850,"합계"]
["MDA10510130S",null,"관보온/고무발포보온재","D250, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,80376,0,80376,"합계"]
["MDA10510140S",null,"관보온/고무발포보온재","D300, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,91858,0,91858,"합계"]
["MDA11010010S",null,"관보온/고무발포보온재","D15, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,8815,0,8815,"합계"]
["MDA11010020S",null,"관보온/고무발포보온재","D20, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,9964,0,9964,"합계"]
["MDA11010030S",null,"관보온/고무발포보온재","D25, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,10908,0,10908,"합계"]
["MDA11010040S",null,"관보온/고무발포보온재","D32, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,12630,0,12630,"합계"]
["MDA11010050S",null,"관보온/고무발포보온재","D40, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,14926,0,14926,"합계"]
["MDA11010060S",null,"관보온/고무발포보온재","D50, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,17797,0,17797,"합계"]
["MDA11010070S",null,"관보온/고무발포보온재","D65, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,20463,0,20463,"합계"]
["MDA11010080S",null,"관보온/고무발포보온재","D80, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,25056,0,25056,"합계"]
["MDA11010090S",null,"관보온/고무발포보온재","D100, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,29279,0,29279,"합계"]
["MDA11010100S",null,"관보온/고무발포보온재","D125, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,35595,0,35595,"합계"]
["MDA11010110S",null,"관보온/고무발포보온재","D150, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,42280,0,42280,"합계"]
["MDA11010120S",null,"관보온/고무발포보온재","D200, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,56263,0,56263,"합계"]
["MDA11010130S",null,"관보온/고무발포보온재","D250, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,68893,0,68893,"합계"]
["MDA11010140S",null,"관보온/고무발포보온재","D300, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,74634,0,74634,"합계"]
["MDA11110010S",null,"관보온/고무발포보온재","D15, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,10129,0,10129,"합계"]
["MDA11110020S",null,"관보온/고무발포보온재","D20, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,11482,0,11482,"합계"]
["MDA11110030S",null,"관보온/고무발포보온재","D25, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,12630,0,12630,"합계"]
["MDA11110040S",null,"관보온/고무발포보온재","D32, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,14557,0,14557,"합계"]
["MDA11110050S",null,"관보온/고무발포보온재","D40, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,17223,0,17223,"합계"]
["MDA11110060S",null,"관보온/고무발포보온재","D50, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,20463,0,20463,"합계"]
["MDA11110070S",null,"관보온/고무발포보온재","D65, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,23538,0,23538,"합계"]
["MDA11110080S",null,"관보온/고무발포보온재","D80, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,28705,0,28705,"합계"]
["MDA11110090S",null,"관보온/고무발포보온재","D100, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,33872,0,33872,"합계"]
["MDA11110100S",null,"관보온/고무발포보온재","D125, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,40762,0,40762,"합계"]
["MDA11110110S",null,"관보온/고무발포보온재","D150, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,48429,0,48429,"합계"]
["MDA11110120S",null,"관보온/고무발포보온재","D200, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,65195,0,65195,"합계"]
["MDA11110130S",null,"관보온/고무발포보온재","D250, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,78333,0,78333,"합계"]
["MDA11110140S",null,"관보온/고무발포보온재","D300, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,86117,0,86117,"합계"]
["MDA11210010S",null,"관보온/고무발포보온재","D15, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,12260,0,12260,"합계"]
["MDA11210020S",null,"관보온/고무발포보온재","D20, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,13778,0,13778,"합계"]
["MDA11210030S",null,"관보온/고무발포보온재","D25, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,15131,0,15131,"합계"]
["MDA11210040S",null,"관보온/고무발포보온재","D32, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,17797,0,17797,"합계"]
["MDA11210050S",null,"관보온/고무발포보온재","D40, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,20872,0,20872,"합계"]
["MDA11210060S",null,"관보온/고무발포보온재","D50, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,24686,0,24686,"합계"]
["MDA11210070S",null,"관보온/고무발포보온재","D65, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,28501,0,28501,"합계"]
["MDA11210080S",null,"관보온/고무발포보온재","D80, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,34816,0,34816,"합계"]
["MDA11210090S",null,"관보온/고무발포보온재","D100, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,40966,0,40966,"합계"]
["MDA11210100S",null,"관보온/고무발포보온재","D125, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,49578,0,49578,"합계"]
["MDA11210110S",null,"관보온/고무발포보온재","D150, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,57411,0,57411,"합계"]
["MDA11210120S",null,"관보온/고무발포보온재","D200, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,78333,0,78333,"합계"]
["MDA11210130S",null,"관보온/고무발포보온재","D250, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,93901,0,93901,"합계"]
["MDA11210140S",null,"관보온/고무발포보온재","D300, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,103340,0,103340,"합계"]
["MDA11310010S",null,"관보온/고무발포보온재","D15, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,14352,0,14352,"합계"]
["MDA11310020S",null,"관보온/고무발포보온재","D20, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,16075,0,16075,"합계"]
["MDA11310030S",null,"관보온/고무발포보온재","D25, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,16853,0,16853,"합계"]
["MDA11310040S",null,"관보온/고무발포보온재","D32, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,19889,0,19889,"합계"]
["MDA11310050S",null,"관보온/고무발포보온재","D40, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,23334,0,23334,"합계"]
["MDA11310060S",null,"관보온/고무발포보온재","D50, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,26983,0,26983,"합계"]
["MDA11310070S",null,"관보온/고무발포보온재","D65, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,29279,0,29279,"합계"]
["MDA11310080S",null,"관보온/고무발포보온재","D80, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,33872,0,33872,"합계"]
["MDA11310090S",null,"관보온/고무발포보온재","D100, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,37521,0,37521,"합계"]
["MDA11310100S",null,"관보온/고무발포보온재","D125, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,44985,0,44985,"합계"]
["MDA11310110S",null,"관보온/고무발포보온재","D150, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,51874,0,51874,"합계"]
["MDA11310120S",null,"관보온/고무발포보온재","D200, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,61109,0,61109,"합계"]
["MDA11310130S",null,"관보온/고무발포보온재","D250, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,74634,0,74634,"합계"]
["MDA11310140S",null,"관보온/고무발포보온재","D300, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,84074,0,84074,"합계"]
["MDA11410010S",null,"관보온/고무발포보온재","D15, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,16649,0,16649,"합계"]
["MDA11410020S",null,"관보온/고무발포보온재","D20, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,18371,0,18371,"합계"]
["MDA11410030S",null,"관보온/고무발포보온재","D25, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,19519,0,19519,"합계"]
["MDA11410040S",null,"관보온/고무발포보온재","D32, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,22760,0,22760,"합계"]
["MDA11410050S",null,"관보온/고무발포보온재","D40, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,26779,0,26779,"합계"]
["MDA11410060S",null,"관보온/고무발포보온재","D50, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,31002,0,31002,"합계"]
["MDA11410070S",null,"관보온/고무발포보온재","D65, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,33872,0,33872,"합계"]
["MDA11410080S",null,"관보온/고무발포보온재","D80, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,38835,0,38835,"합계"]
["MDA11410090S",null,"관보온/고무발포보온재","D100, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,43058,0,43058,"합계"]
["MDA11410100S",null,"관보온/고무발포보온재","D125, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,51670,0,51670,"합계"]
["MDA11410110S",null,"관보온/고무발포보온재","D150, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,59454,0,59454,"합계"]
["MDA11410120S",null,"관보온/고무발포보온재","D200, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,70936,0,70936,"합계"]
["MDA11410130S",null,"관보온/고무발포보온재","D250, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,86117,0,86117,"합계"]
["MDA11410140S",null,"관보온/고무발포보온재","D300, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,97599,0,97599,"합계"]
["MDA11510010S",null,"관보온/고무발포보온재","D15, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,20093,0,20093,"합계"]
["MDA11510020S",null,"관보온/고무발포보온재","D20, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,22390,0,22390,"합계"]
["MDA11510030S",null,"관보온/고무발포보온재","D25, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,23538,0,23538,"합계"]
["MDA11510040S",null,"관보온/고무발포보온재","D32, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,27557,0,27557,"합계"]
["MDA11510050S",null,"관보온/고무발포보온재","D40, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,32520,0,32520,"합계"]
["MDA11510060S",null,"관보온/고무발포보온재","D50, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,37687,0,37687,"합계"]
["MDA11510070S",null,"관보온/고무발포보온재","D65, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,40966,0,40966,"합계"]
["MDA11510080S",null,"관보온/고무발포보온재","D80, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,47077,0,47077,"합계"]
["MDA11510090S",null,"관보온/고무발포보온재","D100, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,52244,0,52244,"합계"]
["MDA11510100S",null,"관보온/고무발포보온재","D125, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,63152,0,63152,"합계"]
["MDA11510110S",null,"관보온/고무발포보온재","D150, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,72592,0,72592,"합계"]
["MDA11510120S",null,"관보온/고무발포보온재","D200, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,86117,0,86117,"합계"]
["MDA11510130S",null,"관보온/고무발포보온재","D250, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,103340,0,103340,"합계"]
["MDA11510140S",null,"관보온/고무발포보온재","D300, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,116865,0,116865,"합계"]
["MDA20010010S",null,"관보온/발포폴리에틸렌보온재","D15, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,4592,0,4592,"합계"]
["MDA20010020S",null,"관보온/발포폴리에틸렌보온재","D20, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,5371,0,5371,"합계"]
["MDA20010030S",null,"관보온/발포폴리에틸렌보온재","D25, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,5945,0,5945,"합계"]
["MDA20010040S",null,"관보온/발포폴리에틸렌보온재","D32, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,7093,0,7093,"합계"]
["MDA20010050S",null,"관보온/발포폴리에틸렌보온재","D40, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,8241,0,8241,"합계"]
["MDA20010060S",null,"관보온/발포폴리에틸렌보온재","D50, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,9555,0,9555,"합계"]
["MDA20010070S",null,"관보온/발포폴리에틸렌보온재","D65, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,11482,0,11482,"합계"]
["MDA20010080S",null,"관보온/발포폴리에틸렌보온재","D80, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,13574,0,13574,"합계"]
["MDA20010090S",null,"관보온/발포폴리에틸렌보온재","D100, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,16075,0,16075,"합계"]
["MDA20010100S",null,"관보온/발포폴리에틸렌보온재","D125, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,19889,0,19889,"합계"]
["MDA20010110S",null,"관보온/발포폴리에틸렌보온재","D150, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,23538,0,23538,"합계"]
["MDA20010120S",null,"관보온/발포폴리에틸렌보온재","D200, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,30428,0,30428,"합계"]
["MDA20010130S",null,"관보온/발포폴리에틸렌보온재","D250, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,36947,0,36947,"합계"]
["MDA20010140S",null,"관보온/발포폴리에틸렌보온재","D300, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,43058,0,43058,"합계"]
["MDA20110010S",null,"관보온/발포폴리에틸렌보온재","D15, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,5167,0,5167,"합계"]
["MDA20110020S",null,"관보온/발포폴리에틸렌보온재","D20, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,6110,0,6110,"합계"]
["MDA20110030S",null,"관보온/발포폴리에틸렌보온재","D25, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,6685,0,6685,"합계"]
["MDA20110040S",null,"관보온/발포폴리에틸렌보온재","D32, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,7833,0,7833,"합계"]
["MDA20110050S",null,"관보온/발포폴리에틸렌보온재","D40, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,9185,0,9185,"합계"]
["MDA20110060S",null,"관보온/발포폴리에틸렌보온재","D50, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,10703,0,10703,"합계"]
["MDA20110070S",null,"관보온/발포폴리에틸렌보온재","D65, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,12630,0,12630,"합계"]
["MDA20110080S",null,"관보온/발포폴리에틸렌보온재","D80, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,15131,0,15131,"합계"]
["MDA20110090S",null,"관보온/발포폴리에틸렌보온재","D100, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,18001,0,18001,"합계"]
["MDA20110100S",null,"관보온/발포폴리에틸렌보온재","D125, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,22020,0,22020,"합계"]
["MDA20110110S",null,"관보온/발포폴리에틸렌보온재","D150, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,26039,0,26039,"합계"]
["MDA20110120S",null,"관보온/발포폴리에틸렌보온재","D200, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,33872,0,33872,"합계"]
["MDA20110130S",null,"관보온/발포폴리에틸렌보온재","D250, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,40966,0,40966,"합계"]
["MDA20110140S",null,"관보온/발포폴리에틸렌보온재","D300, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,47855,0,47855,"합계"]
["MDA20210010S",null,"관보온/발포폴리에틸렌보온재","D15, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,5945,0,5945,"합계"]
["MDA20210020S",null,"관보온/발포폴리에틸렌보온재","D20, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,6889,0,6889,"합계"]
["MDA20210030S",null,"관보온/발포폴리에틸렌보온재","D25, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,7667,0,7667,"합계"]
["MDA20210040S",null,"관보온/발포폴리에틸렌보온재","D32, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,8981,0,8981,"합계"]
["MDA20210050S",null,"관보온/발포폴리에틸렌보온재","D40, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,10334,0,10334,"합계"]
["MDA20210060S",null,"관보온/발포폴리에틸렌보온재","D50, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,12260,0,12260,"합계"]
["MDA20210070S",null,"관보온/발포폴리에틸렌보온재","D65, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,14722,0,14722,"합계"]
["MDA20210080S",null,"관보온/발포폴리에틸렌보온재","D80, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,17223,0,17223,"합계"]
["MDA20210090S",null,"관보온/발포폴리에틸렌보온재","D100, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,20668,0,20668,"합계"]
["MDA20210100S",null,"관보온/발포폴리에틸렌보온재","D125, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,25260,0,25260,"합계"]
["MDA20210110S",null,"관보온/발포폴리에틸렌보온재","D150, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,29853,0,29853,"합계"]
["MDA20210120S",null,"관보온/발포폴리에틸렌보온재","D200, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,38835,0,38835,"합계"]
["MDA20210130S",null,"관보온/발포폴리에틸렌보온재","D250, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,47077,0,47077,"합계"]
["MDA20210140S",null,"관보온/발포폴리에틸렌보온재","D300, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,55115,0,55115,"합계"]
["MDA20310010S",null,"관보온/발포폴리에틸렌보온재","D15, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,7833,0,7833,"합계"]
["MDA20310020S",null,"관보온/발포폴리에틸렌보온재","D20, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,8981,0,8981,"합계"]
["MDA20310030S",null,"관보온/발포폴리에틸렌보온재","D25, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,9185,0,9185,"합계"]
["MDA20310040S",null,"관보온/발포폴리에틸렌보온재","D32, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,10908,0,10908,"합계"]
["MDA20310050S",null,"관보온/발포폴리에틸렌보온재","D40, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,12630,0,12630,"합계"]
["MDA20310060S",null,"관보온/발포폴리에틸렌보온재","D50, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,14722,0,14722,"합계"]
["MDA20310070S",null,"관보온/발포폴리에틸렌보온재","D65, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,15705,0,15705,"합계"]
["MDA20310080S",null,"관보온/발포폴리에틸렌보온재","D80, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,17797,0,17797,"합계"]
["MDA20310090S",null,"관보온/발포폴리에틸렌보온재","D100, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,20668,0,20668,"합계"]
["MDA20310100S",null,"관보온/발포폴리에틸렌보온재","D125, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,24686,0,24686,"합계"]
["MDA20310110S",null,"관보온/발포폴리에틸렌보온재","D150, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,28705,0,28705,"합계"]
["MDA20310120S",null,"관보온/발포폴리에틸렌보온재","D200, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,34446,0,34446,"합계"]
["MDA20310130S",null,"관보온/발포폴리에틸렌보온재","D250, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,39818,0,39818,"합계"]
["MDA20310140S",null,"관보온/발포폴리에틸렌보온재","D300, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,43058,0,43058,"합계"]
["MDA20410010S",null,"관보온/발포폴리에틸렌보온재","D15, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,8611,0,8611,"합계"]
["MDA20410020S",null,"관보온/발포폴리에틸렌보온재","D20, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,9759,0,9759,"합계"]
["MDA20410030S",null,"관보온/발포폴리에틸렌보온재","D25, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,10334,0,10334,"합계"]
["MDA20410040S",null,"관보온/발포폴리에틸렌보온재","D32, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,12056,0,12056,"합계"]
["MDA20410050S",null,"관보온/발포폴리에틸렌보온재","D40, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,13982,0,13982,"합계"]
["MDA20410060S",null,"관보온/발포폴리에틸렌보온재","D50, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,16445,0,16445,"합계"]
["MDA20410070S",null,"관보온/발포폴리에틸렌보온재","D65, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,17427,0,17427,"합계"]
["MDA20410080S",null,"관보온/발포폴리에틸렌보온재","D80, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,19724,0,19724,"합계"]
["MDA20410090S",null,"관보온/발포폴리에틸렌보온재","D100, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,22964,0,22964,"합계"]
["MDA20410100S",null,"관보온/발포폴리에틸렌보온재","D125, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,27353,0,27353,"합계"]
["MDA20410110S",null,"관보온/발포폴리에틸렌보온재","D150, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,31946,0,31946,"합계"]
["MDA20410120S",null,"관보온/발포폴리에틸렌보온재","D200, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,38261,0,38261,"합계"]
["MDA20410130S",null,"관보온/발포폴리에틸렌보온재","D250, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,44206,0,44206,"합계"]
["MDA20410140S",null,"관보온/발포폴리에틸렌보온재","D300, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,47855,0,47855,"합계"]
["MDA20510010S",null,"관보온/발포폴리에틸렌보온재","D15, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,9964,0,9964,"합계"]
["MDA20510020S",null,"관보온/발포폴리에틸렌보온재","D20, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,11482,0,11482,"합계"]
["MDA20510030S",null,"관보온/발포폴리에틸렌보온재","D25, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,11852,0,11852,"합계"]
["MDA20510040S",null,"관보온/발포폴리에틸렌보온재","D32, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,13778,0,13778,"합계"]
["MDA20510050S",null,"관보온/발포폴리에틸렌보온재","D40, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,16075,0,16075,"합계"]
["MDA20510060S",null,"관보온/발포폴리에틸렌보온재","D50, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,18945,0,18945,"합계"]
["MDA20510070S",null,"관보온/발포폴리에틸렌보온재","D65, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,20093,0,20093,"합계"]
["MDA20510080S",null,"관보온/발포폴리에틸렌보온재","D80, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,22760,0,22760,"합계"]
["MDA20510090S",null,"관보온/발포폴리에틸렌보온재","D100, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,26409,0,26409,"합계"]
["MDA20510100S",null,"관보온/발포폴리에틸렌보온재","D125, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,31371,0,31371,"합계"]
["MDA20510110S",null,"관보온/발포폴리에틸렌보온재","D150, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,36743,0,36743,"합계"]
["MDA20510120S",null,"관보온/발포폴리에틸렌보온재","D200, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,44002,0,44002,"합계"]
["MDA20510130S",null,"관보온/발포폴리에틸렌보온재","D250, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,50726,0,50726,"합계"]
["MDA20510140S",null,"관보온/발포폴리에틸렌보온재","D300, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,55115,0,55115,"합계"]
["MDA21010010S",null,"관보온/발포폴리에틸렌보온재","D15, 보온두께 25mm 이하, 일반접합, 기계실","m",0,5536,0,5536,"합계"]
["MDA21010020S",null,"관보온/발포폴리에틸렌보온재","D20, 보온두께 25mm 이하, 일반접합, 기계실","m",0,6315,0,6315,"합계"]
["MDA21010030S",null,"관보온/발포폴리에틸렌보온재","D25, 보온두께 25mm 이하, 일반접합, 기계실","m",0,7093,0,7093,"합계"]
["MDA21010040S",null,"관보온/발포폴리에틸렌보온재","D32, 보온두께 25mm 이하, 일반접합, 기계실","m",0,8407,0,8407,"합계"]
["MDA21010050S",null,"관보온/발포폴리에틸렌보온재","D40, 보온두께 25mm 이하, 일반접합, 기계실","m",0,9759,0,9759,"합계"]
["MDA21010060S",null,"관보온/발포폴리에틸렌보온재","D50, 보온두께 25mm 이하, 일반접합, 기계실","m",0,11278,0,11278,"합계"]
["MDA21010070S",null,"관보온/발포폴리에틸렌보온재","D65, 보온두께 25mm 이하, 일반접합, 기계실","m",0,13574,0,13574,"합계"]
["MDA21010080S",null,"관보온/발포폴리에틸렌보온재","D80, 보온두께 25mm 이하, 일반접합, 기계실","m",0,16075,0,16075,"합계"]
["MDA21010090S",null,"관보온/발포폴리에틸렌보온재","D100, 보온두께 25mm 이하, 일반접합, 기계실","m",0,18945,0,18945,"합계"]
["MDA21010100S",null,"관보온/발포폴리에틸렌보온재","D125, 보온두께 25mm 이하, 일반접합, 기계실","m",0,23538,0,23538,"합계"]
["MDA21010110S",null,"관보온/발포폴리에틸렌보온재","D150, 보온두께 25mm 이하, 일반접합, 기계실","m",0,27761,0,27761,"합계"]
["MDA21010120S",null,"관보온/발포폴리에틸렌보온재","D200, 보온두께 25mm 이하, 일반접합, 기계실","m",0,35964,0,35964,"합계"]
["MDA21010130S",null,"관보온/발포폴리에틸렌보온재","D250, 보온두께 25mm 이하, 일반접합, 기계실","m",0,43632,0,43632,"합계"]
["MDA21010140S",null,"관보온/발포폴리에틸렌보온재","D300, 보온두께 25mm 이하, 일반접합, 기계실","m",0,50891,0,50891,"합계"]
["MDA21110010S",null,"관보온/발포폴리에틸렌보온재","D15, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,6315,0,6315,"합계"]
["MDA21110020S",null,"관보온/발포폴리에틸렌보온재","D20, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,7259,0,7259,"합계"]
["MDA21110030S",null,"관보온/발포폴리에틸렌보온재","D25, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,8037,0,8037,"합계"]
["MDA21110040S",null,"관보온/발포폴리에틸렌보온재","D32, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,9555,0,9555,"합계"]
["MDA21110050S",null,"관보온/발포폴리에틸렌보온재","D40, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,10908,0,10908,"합계"]
["MDA21110060S",null,"관보온/발포폴리에틸렌보온재","D50, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,12834,0,12834,"합계"]
["MDA21110070S",null,"관보온/발포폴리에틸렌보온재","D65, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,15501,0,15501,"합계"]
["MDA21110080S",null,"관보온/발포폴리에틸렌보온재","D80, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,18167,0,18167,"합계"]
["MDA21110090S",null,"관보온/발포폴리에틸렌보온재","D100, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,21612,0,21612,"합계"]
["MDA21110100S",null,"관보온/발포폴리에틸렌보온재","D125, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,26613,0,26613,"합계"]
["MDA21110110S",null,"관보온/발포폴리에틸렌보온재","D150, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,31576,0,31576,"합계"]
["MDA21110120S",null,"관보온/발포폴리에틸렌보온재","D200, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,40762,0,40762,"합계"]
["MDA21110130S",null,"관보온/발포폴리에틸렌보온재","D250, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,49373,0,49373,"합계"]
["MDA21110140S",null,"관보온/발포폴리에틸렌보온재","D300, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,57411,0,57411,"합계"]
["MDA21210010S",null,"관보온/발포폴리에틸렌보온재","D15, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,7463,0,7463,"합계"]
["MDA21210020S",null,"관보온/발포폴리에틸렌보온재","D20, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,8611,0,8611,"합계"]
["MDA21210030S",null,"관보온/발포폴리에틸렌보온재","D25, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,9555,0,9555,"합계"]
["MDA21210040S",null,"관보온/발포폴리에틸렌보온재","D32, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,11278,0,11278,"합계"]
["MDA21210050S",null,"관보온/발포폴리에틸렌보온재","D40, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,13000,0,13000,"합계"]
["MDA21210060S",null,"관보온/발포폴리에틸렌보온재","D50, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,15131,0,15131,"합계"]
["MDA21210070S",null,"관보온/발포폴리에틸렌보온재","D65, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,18167,0,18167,"합계"]
["MDA21210080S",null,"관보온/발포폴리에틸렌보온재","D80, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,21612,0,21612,"합계"]
["MDA21210090S",null,"관보온/발포폴리에틸렌보온재","D100, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,25630,0,25630,"합계"]
["MDA21210100S",null,"관보온/발포폴리에틸렌보온재","D125, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,31576,0,31576,"합계"]
["MDA21210110S",null,"관보온/발포폴리에틸렌보온재","D150, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,37317,0,37317,"합계"]
["MDA21210120S",null,"관보온/발포폴리에틸렌보온재","D200, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,48225,0,48225,"합계"]
["MDA21210130S",null,"관보온/발포폴리에틸렌보온재","D250, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,57411,0,57411,"합계"]
["MDA21210140S",null,"관보온/발포폴리에틸렌보온재","D300, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,68893,0,68893,"합계"]
["MDA21310010S",null,"관보온/발포폴리에틸렌보온재","D15, 보온두께 50mm 이하, 일반접합, 기계실","m",0,9185,0,9185,"합계"]
["MDA21310020S",null,"관보온/발포폴리에틸렌보온재","D20, 보온두께 50mm 이하, 일반접합, 기계실","m",0,10538,0,10538,"합계"]
["MDA21310030S",null,"관보온/발포폴리에틸렌보온재","D25, 보온두께 50mm 이하, 일반접합, 기계실","m",0,10908,0,10908,"합계"]
["MDA21310040S",null,"관보온/발포폴리에틸렌보온재","D32, 보온두께 50mm 이하, 일반접합, 기계실","m",0,12630,0,12630,"합계"]
["MDA21310050S",null,"관보온/발포폴리에틸렌보온재","D40, 보온두께 50mm 이하, 일반접합, 기계실","m",0,14926,0,14926,"합계"]
["MDA21310060S",null,"관보온/발포폴리에틸렌보온재","D50, 보온두께 50mm 이하, 일반접합, 기계실","m",0,17427,0,17427,"합계"]
["MDA21310070S",null,"관보온/발포폴리에틸렌보온재","D65, 보온두께 50mm 이하, 일반접합, 기계실","m",0,18371,0,18371,"합계"]
["MDA21310080S",null,"관보온/발포폴리에틸렌보온재","D80, 보온두께 50mm 이하, 일반접합, 기계실","m",0,21037,0,21037,"합계"]
["MDA21310090S",null,"관보온/발포폴리에틸렌보온재","D100, 보온두께 50mm 이하, 일반접합, 기계실","m",0,24482,0,24482,"합계"]
["MDA21310100S",null,"관보온/발포폴리에틸렌보온재","D125, 보온두께 50mm 이하, 일반접합, 기계실","m",0,29075,0,29075,"합계"]
["MDA21310110S",null,"관보온/발포폴리에틸렌보온재","D150, 보온두께 50mm 이하, 일반접합, 기계실","m",0,33872,0,33872,"합계"]
["MDA21310120S",null,"관보온/발포폴리에틸렌보온재","D200, 보온두께 50mm 이하, 일반접합, 기계실","m",0,40762,0,40762,"합계"]
["MDA21310130S",null,"관보온/발포폴리에틸렌보온재","D250, 보온두께 50mm 이하, 일반접합, 기계실","m",0,47077,0,47077,"합계"]
["MDA21310140S",null,"관보온/발포폴리에틸렌보온재","D300, 보온두께 50mm 이하, 일반접합, 기계실","m",0,50891,0,50891,"합계"]
["MDA21410010S",null,"관보온/발포폴리에틸렌보온재","D15, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,10538,0,10538,"합계"]
["MDA21410020S",null,"관보온/발포폴리에틸렌보온재","D20, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,12056,0,12056,"합계"]
["MDA21410030S",null,"관보온/발포폴리에틸렌보온재","D25, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,12426,0,12426,"합계"]
["MDA21410040S",null,"관보온/발포폴리에틸렌보온재","D32, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,14352,0,14352,"합계"]
["MDA21410050S",null,"관보온/발포폴리에틸렌보온재","D40, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,16853,0,16853,"합계"]
["MDA21410060S",null,"관보온/발포폴리에틸렌보온재","D50, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,19724,0,19724,"합계"]
["MDA21410070S",null,"관보온/발포폴리에틸렌보온재","D65, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,21037,0,21037,"합계"]
["MDA21410080S",null,"관보온/발포폴리에틸렌보온재","D80, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,23908,0,23908,"합계"]
["MDA21410090S",null,"관보온/발포폴리에틸렌보온재","D100, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,27557,0,27557,"합계"]
["MDA21410100S",null,"관보온/발포폴리에틸렌보온재","D125, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,32928,0,32928,"합계"]
["MDA21410110S",null,"관보온/발포폴리에틸렌보온재","D150, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,38465,0,38465,"합계"]
["MDA21410120S",null,"관보온/발포폴리에틸렌보온재","D200, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,46133,0,46133,"합계"]
["MDA21410130S",null,"관보온/발포폴리에틸렌보온재","D250, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,53188,0,53188,"합계"]
["MDA21410140S",null,"관보온/발포폴리에틸렌보온재","D300, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,57411,0,57411,"합계"]
["MDA21510010S",null,"관보온/발포폴리에틸렌보온재","D15, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,12426,0,12426,"합계"]
["MDA21510020S",null,"관보온/발포폴리에틸렌보온재","D20, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,14148,0,14148,"합계"]
["MDA21510030S",null,"관보온/발포폴리에틸렌보온재","D25, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,14722,0,14722,"합계"]
["MDA21510040S",null,"관보온/발포폴리에틸렌보온재","D32, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,17223,0,17223,"합계"]
["MDA21510050S",null,"관보온/발포폴리에틸렌보온재","D40, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,20093,0,20093,"합계"]
["MDA21510060S",null,"관보온/발포폴리에틸렌보온재","D50, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,23538,0,23538,"합계"]
["MDA21510070S",null,"관보온/발포폴리에틸렌보온재","D65, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,24891,0,24891,"합계"]
["MDA21510080S",null,"관보온/발포폴리에틸렌보온재","D80, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,28335,0,28335,"합계"]
["MDA21510090S",null,"관보온/발포폴리에틸렌보온재","D100, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,32724,0,32724,"합계"]
["MDA21510100S",null,"관보온/발포폴리에틸렌보온재","D125, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,39039,0,39039,"합계"]
["MDA21510110S",null,"관보온/발포폴리에틸렌보온재","D150, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,45559,0,45559,"합계"]
["MDA21510120S",null,"관보온/발포폴리에틸렌보온재","D200, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,54540,0,54540,"합계"]
["MDA21510130S",null,"관보온/발포폴리에틸렌보온재","D250, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,63152,0,63152,"합계"]
["MDA21510140S",null,"관보온/발포폴리에틸렌보온재","D300, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,68893,0,68893,"합계"]
["MDA30010010S",null,"관보온/발포폴리에틸렌보온재","D15, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,5167,0,5167,"합계"]
["MDA30010020S",null,"관보온/발포폴리에틸렌보온재","D20, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,5945,0,5945,"합계"]
["MDA30010030S",null,"관보온/발포폴리에틸렌보온재","D25, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,6519,0,6519,"합계"]
["MDA30010040S",null,"관보온/발포폴리에틸렌보온재","D32, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,7667,0,7667,"합계"]
["MDA30010050S",null,"관보온/발포폴리에틸렌보온재","D40, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,8981,0,8981,"합계"]
["MDA30010060S",null,"관보온/발포폴리에틸렌보온재","D50, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,10334,0,10334,"합계"]
["MDA30010070S",null,"관보온/발포폴리에틸렌보온재","D65, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,12630,0,12630,"합계"]
["MDA30010080S",null,"관보온/발포폴리에틸렌보온재","D80, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,14926,0,14926,"합계"]
["MDA30010090S",null,"관보온/발포폴리에틸렌보온재","D100, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,17593,0,17593,"합계"]
["MDA30010100S",null,"관보온/발포폴리에틸렌보온재","D125, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,21612,0,21612,"합계"]
["MDA30010110S",null,"관보온/발포폴리에틸렌보온재","D150, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,25630,0,25630,"합계"]
["MDA30010120S",null,"관보온/발포폴리에틸렌보온재","D200, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,33094,0,33094,"합계"]
["MDA30010130S",null,"관보온/발포폴리에틸렌보온재","D250, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,40188,0,40188,"합계"]
["MDA30010140S",null,"관보온/발포폴리에틸렌보온재","D300, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,46873,0,46873,"합계"]
["MDA30110010S",null,"관보온/발포폴리에틸렌보온재","D15, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,5741,0,5741,"합계"]
["MDA30110020S",null,"관보온/발포폴리에틸렌보온재","D20, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,6685,0,6685,"합계"]
["MDA30110030S",null,"관보온/발포폴리에틸렌보온재","D25, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,7463,0,7463,"합계"]
["MDA30110040S",null,"관보온/발포폴리에틸렌보온재","D32, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,8611,0,8611,"합계"]
["MDA30110050S",null,"관보온/발포폴리에틸렌보온재","D40, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,9964,0,9964,"합계"]
["MDA30110060S",null,"관보온/발포폴리에틸렌보온재","D50, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,11686,0,11686,"합계"]
["MDA30110070S",null,"관보온/발포폴리에틸렌보온재","D65, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,13982,0,13982,"합계"]
["MDA30110080S",null,"관보온/발포폴리에틸렌보온재","D80, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,16649,0,16649,"합계"]
["MDA30110090S",null,"관보온/발포폴리에틸렌보온재","D100, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,19724,0,19724,"합계"]
["MDA30110100S",null,"관보온/발포폴리에틸렌보온재","D125, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,24317,0,24317,"합계"]
["MDA30110110S",null,"관보온/발포폴리에틸렌보온재","D150, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,28705,0,28705,"합계"]
["MDA30110120S",null,"관보온/발포폴리에틸렌보온재","D200, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,37113,0,37113,"합계"]
["MDA30110130S",null,"관보온/발포폴리에틸렌보온재","D250, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,44985,0,44985,"합계"]
["MDA30110140S",null,"관보온/발포폴리에틸렌보온재","D300, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,52614,0,52614,"합계"]
["MDA30210010S",null,"관보온/발포폴리에틸렌보온재","D15, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,6685,0,6685,"합계"]
["MDA30210020S",null,"관보온/발포폴리에틸렌보온재","D20, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,7667,0,7667,"합계"]
["MDA30210030S",null,"관보온/발포폴리에틸렌보온재","D25, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,8611,0,8611,"합계"]
["MDA30210040S",null,"관보온/발포폴리에틸렌보온재","D32, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,10129,0,10129,"합계"]
["MDA30210050S",null,"관보온/발포폴리에틸렌보온재","D40, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,11686,0,11686,"합계"]
["MDA30210060S",null,"관보온/발포폴리에틸렌보온재","D50, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,13574,0,13574,"합계"]
["MDA30210070S",null,"관보온/발포폴리에틸렌보온재","D65, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,16279,0,16279,"합계"]
["MDA30210080S",null,"관보온/발포폴리에틸렌보온재","D80, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,19315,0,19315,"합계"]
["MDA30210090S",null,"관보온/발포폴리에틸렌보온재","D100, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,22964,0,22964,"합계"]
["MDA30210100S",null,"관보온/발포폴리에틸렌보온재","D125, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,28335,0,28335,"합계"]
["MDA30210110S",null,"관보온/발포폴리에틸렌보온재","D150, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,33502,0,33502,"합계"]
["MDA30210120S",null,"관보온/발포폴리에틸렌보온재","D200, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,43262,0,43262,"합계"]
["MDA30210130S",null,"관보온/발포폴리에틸렌보온재","D250, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,52614,0,52614,"합계"]
["MDA30210140S",null,"관보온/발포폴리에틸렌보온재","D300, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,61109,0,61109,"합계"]
["MDA30310010S",null,"관보온/발포폴리에틸렌보온재","D15, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,8611,0,8611,"합계"]
["MDA30310020S",null,"관보온/발포폴리에틸렌보온재","D20, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,9759,0,9759,"합계"]
["MDA30310030S",null,"관보온/발포폴리에틸렌보온재","D25, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,10129,0,10129,"합계"]
["MDA30310040S",null,"관보온/발포폴리에틸렌보온재","D32, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,11686,0,11686,"합계"]
["MDA30310050S",null,"관보온/발포폴리에틸렌보온재","D40, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,13778,0,13778,"합계"]
["MDA30310060S",null,"관보온/발포폴리에틸렌보온재","D50, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,16075,0,16075,"합계"]
["MDA30310070S",null,"관보온/발포폴리에틸렌보온재","D65, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,17019,0,17019,"합계"]
["MDA30310080S",null,"관보온/발포폴리에틸렌보온재","D80, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,19519,0,19519,"합계"]
["MDA30310090S",null,"관보온/발포폴리에틸렌보온재","D100, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,22390,0,22390,"합계"]
["MDA30310100S",null,"관보온/발포폴리에틸렌보온재","D125, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,26779,0,26779,"합계"]
["MDA30310110S",null,"관보온/발포폴리에틸렌보온재","D150, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,31206,0,31206,"합계"]
["MDA30310120S",null,"관보온/발포폴리에틸렌보온재","D200, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,37521,0,37521,"합계"]
["MDA30310130S",null,"관보온/발포폴리에틸렌보온재","D250, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,43262,0,43262,"합계"]
["MDA30310140S",null,"관보온/발포폴리에틸렌보온재","D300, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,46873,0,46873,"합계"]
["MDA30410010S",null,"관보온/발포폴리에틸렌보온재","D15, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,9555,0,9555,"합계"]
["MDA30410020S",null,"관보온/발포폴리에틸렌보온재","D20, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,10908,0,10908,"합계"]
["MDA30410030S",null,"관보온/발포폴리에틸렌보온재","D25, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,11278,0,11278,"합계"]
["MDA30410040S",null,"관보온/발포폴리에틸렌보온재","D32, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,13204,0,13204,"합계"]
["MDA30410050S",null,"관보온/발포폴리에틸렌보온재","D40, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,15501,0,15501,"합계"]
["MDA30410060S",null,"관보온/발포폴리에틸렌보온재","D50, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,18001,0,18001,"합계"]
["MDA30410070S",null,"관보온/발포폴리에틸렌보온재","D65, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,19149,0,19149,"합계"]
["MDA30410080S",null,"관보온/발포폴리에틸렌보온재","D80, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,21816,0,21816,"합계"]
["MDA30410090S",null,"관보온/발포폴리에틸렌보온재","D100, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,25260,0,25260,"합계"]
["MDA30410100S",null,"관보온/발포폴리에틸렌보온재","D125, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,30058,0,30058,"합계"]
["MDA30410110S",null,"관보온/발포폴리에틸렌보온재","D150, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,35020,0,35020,"합계"]
["MDA30410120S",null,"관보온/발포폴리에틸렌보온재","D200, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,42114,0,42114,"합계"]
["MDA30410130S",null,"관보온/발포폴리에틸렌보온재","D250, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,48595,0,48595,"합계"]
["MDA30410140S",null,"관보온/발포폴리에틸렌보온재","D300, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,52614,0,52614,"합계"]
["MDA30510010S",null,"관보온/발포폴리에틸렌보온재","D15, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,11112,0,11112,"합계"]
["MDA30510020S",null,"관보온/발포폴리에틸렌보온재","D20, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,12630,0,12630,"합계"]
["MDA30510030S",null,"관보온/발포폴리에틸렌보온재","D25, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,13204,0,13204,"합계"]
["MDA30510040S",null,"관보온/발포폴리에틸렌보온재","D32, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,15296,0,15296,"합계"]
["MDA30510050S",null,"관보온/발포폴리에틸렌보온재","D40, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,18001,0,18001,"합계"]
["MDA30510060S",null,"관보온/발포폴리에틸렌보온재","D50, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,21037,0,21037,"합계"]
["MDA30510070S",null,"관보온/발포폴리에틸렌보온재","D65, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,22390,0,22390,"합계"]
["MDA30510080S",null,"관보온/발포폴리에틸렌보온재","D80, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,25260,0,25260,"합계"]
["MDA30510090S",null,"관보온/발포폴리에틸렌보온재","D100, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,29484,0,29484,"합계"]
["MDA30510100S",null,"관보온/발포폴리에틸렌보온재","D125, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,35020,0,35020,"합계"]
["MDA30510110S",null,"관보온/발포폴리에틸렌보온재","D150, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,40762,0,40762,"합계"]
["MDA30510120S",null,"관보온/발포폴리에틸렌보온재","D200, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,49004,0,49004,"합계"]
["MDA30510130S",null,"관보온/발포폴리에틸렌보온재","D250, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,56633,0,56633,"합계"]
["MDA30510140S",null,"관보온/발포폴리에틸렌보온재","D300, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,61109,0,61109,"합계"]
["MDA31010010S",null,"관보온/발포폴리에틸렌보온재","D15, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,6110,0,6110,"합계"]
["MDA31010020S",null,"관보온/발포폴리에틸렌보온재","D20, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,7093,0,7093,"합계"]
["MDA31010030S",null,"관보온/발포폴리에틸렌보온재","D25, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,7833,0,7833,"합계"]
["MDA31010040S",null,"관보온/발포폴리에틸렌보온재","D32, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,9185,0,9185,"합계"]
["MDA31010050S",null,"관보온/발포폴리에틸렌보온재","D40, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,10703,0,10703,"합계"]
["MDA31010060S",null,"관보온/발포폴리에틸렌보온재","D50, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,12630,0,12630,"합계"]
["MDA31010070S",null,"관보온/발포폴리에틸렌보온재","D65, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,14926,0,14926,"합계"]
["MDA31010080S",null,"관보온/발포폴리에틸렌보온재","D80, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,17797,0,17797,"합계"]
["MDA31010090S",null,"관보온/발포폴리에틸렌보온재","D100, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,21242,0,21242,"합계"]
["MDA31010100S",null,"관보온/발포폴리에틸렌보온재","D125, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,25835,0,25835,"합계"]
["MDA31010110S",null,"관보온/발포폴리에틸렌보온재","D150, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,30632,0,30632,"합계"]
["MDA31010120S",null,"관보온/발포폴리에틸렌보온재","D200, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,39613,0,39613,"합계"]
["MDA31010130S",null,"관보온/발포폴리에틸렌보온재","D250, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,48225,0,48225,"합계"]
["MDA31010140S",null,"관보온/발포폴리에틸렌보온재","D300, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,56263,0,56263,"합계"]
["MDA31110010S",null,"관보온/발포폴리에틸렌보온재","D15, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,7093,0,7093,"합계"]
["MDA31110020S",null,"관보온/발포폴리에틸렌보온재","D20, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,8037,0,8037,"합계"]
["MDA31110030S",null,"관보온/발포폴리에틸렌보온재","D25, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,8981,0,8981,"합계"]
["MDA31110040S",null,"관보온/발포폴리에틸렌보온재","D32, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,10703,0,10703,"합계"]
["MDA31110050S",null,"관보온/발포폴리에틸렌보온재","D40, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,12260,0,12260,"합계"]
["MDA31110060S",null,"관보온/발포폴리에틸렌보온재","D50, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,14352,0,14352,"합계"]
["MDA31110070S",null,"관보온/발포폴리에틸렌보온재","D65, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,17223,0,17223,"합계"]
["MDA31110080S",null,"관보온/발포폴리에틸렌보온재","D80, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,20463,0,20463,"합계"]
["MDA31110090S",null,"관보온/발포폴리에틸렌보온재","D100, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,24112,0,24112,"합계"]
["MDA31110100S",null,"관보온/발포폴리에틸렌보온재","D125, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,29853,0,29853,"합계"]
["MDA31110110S",null,"관보온/발포폴리에틸렌보온재","D150, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,35225,0,35225,"합계"]
["MDA31110120S",null,"관보온/발포폴리에틸렌보온재","D200, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,45559,0,45559,"합계"]
["MDA31110130S",null,"관보온/발포폴리에틸렌보온재","D250, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,55484,0,55484,"합계"]
["MDA31110140S",null,"관보온/발포폴리에틸렌보온재","D300, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,65195,0,65195,"합계"]
["MDA31210010S",null,"관보온/발포폴리에틸렌보온재","D15, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,8611,0,8611,"합계"]
["MDA31210020S",null,"관보온/발포폴리에틸렌보온재","D20, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,9964,0,9964,"합계"]
["MDA31210030S",null,"관보온/발포폴리에틸렌보온재","D25, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,10908,0,10908,"합계"]
["MDA31210040S",null,"관보온/발포폴리에틸렌보온재","D32, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,12834,0,12834,"합계"]
["MDA31210050S",null,"관보온/발포폴리에틸렌보온재","D40, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,14926,0,14926,"합계"]
["MDA31210060S",null,"관보온/발포폴리에틸렌보온재","D50, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,17427,0,17427,"합계"]
["MDA31210070S",null,"관보온/발포폴리에틸렌보온재","D65, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,20872,0,20872,"합계"]
["MDA31210080S",null,"관보온/발포폴리에틸렌보온재","D80, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,24686,0,24686,"합계"]
["MDA31210090S",null,"관보온/발포폴리에틸렌보온재","D100, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,29279,0,29279,"합계"]
["MDA31210100S",null,"관보온/발포폴리에틸렌보온재","D125, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,36169,0,36169,"합계"]
["MDA31210110S",null,"관보온/발포폴리에틸렌보온재","D150, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,42854,0,42854,"합계"]
["MDA31210120S",null,"관보온/발포폴리에틸렌보온재","D200, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,55319,0,55319,"합계"]
["MDA31210130S",null,"관보온/발포폴리에틸렌보온재","D250, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,66850,0,66850,"합계"]
["MDA31210140S",null,"관보온/발포폴리에틸렌보온재","D300, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,78333,0,78333,"합계"]
["MDA31310010S",null,"관보온/발포폴리에틸렌보온재","D15, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,10334,0,10334,"합계"]
["MDA31310020S",null,"관보온/발포폴리에틸렌보온재","D20, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,11686,0,11686,"합계"]
["MDA31310030S",null,"관보온/발포폴리에틸렌보온재","D25, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,12056,0,12056,"합계"]
["MDA31310040S",null,"관보온/발포폴리에틸렌보온재","D32, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,14148,0,14148,"합계"]
["MDA31310050S",null,"관보온/발포폴리에틸렌보온재","D40, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,16445,0,16445,"합계"]
["MDA31310060S",null,"관보온/발포폴리에틸렌보온재","D50, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,19315,0,19315,"합계"]
["MDA31310070S",null,"관보온/발포폴리에틸렌보온재","D65, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,20463,0,20463,"합계"]
["MDA31310080S",null,"관보온/발포폴리에틸렌보온재","D80, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,23334,0,23334,"합계"]
["MDA31310090S",null,"관보온/발포폴리에틸렌보온재","D100, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,26983,0,26983,"합계"]
["MDA31310100S",null,"관보온/발포폴리에틸렌보온재","D125, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,32150,0,32150,"합계"]
["MDA31310110S",null,"관보온/발포폴리에틸렌보온재","D150, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,37521,0,37521,"합계"]
["MDA31310120S",null,"관보온/발포폴리에틸렌보온재","D200, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,44985,0,44985,"합계"]
["MDA31310130S",null,"관보온/발포폴리에틸렌보온재","D250, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,51874,0,51874,"합계"]
["MDA31310140S",null,"관보온/발포폴리에틸렌보온재","D300, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,56263,0,56263,"합계"]
["MDA31410010S",null,"관보온/발포폴리에틸렌보온재","D15, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,11686,0,11686,"합계"]
["MDA31410020S",null,"관보온/발포폴리에틸렌보온재","D20, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,13408,0,13408,"합계"]
["MDA31410030S",null,"관보온/발포폴리에틸렌보온재","D25, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,13778,0,13778,"합계"]
["MDA31410040S",null,"관보온/발포폴리에틸렌보온재","D32, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,16075,0,16075,"합계"]
["MDA31410050S",null,"관보온/발포폴리에틸렌보온재","D40, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,18945,0,18945,"합계"]
["MDA31410060S",null,"관보온/발포폴리에틸렌보온재","D50, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,22186,0,22186,"합계"]
["MDA31410070S",null,"관보온/발포폴리에틸렌보온재","D65, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,23538,0,23538,"합계"]
["MDA31410080S",null,"관보온/발포폴리에틸렌보온재","D80, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,26779,0,26779,"합계"]
["MDA31410090S",null,"관보온/발포폴리에틸렌보온재","D100, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,31002,0,31002,"합계"]
["MDA31410100S",null,"관보온/발포폴리에틸렌보온재","D125, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,36947,0,36947,"합계"]
["MDA31410110S",null,"관보온/발포폴리에틸렌보온재","D150, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,43058,0,43058,"합계"]
["MDA31410120S",null,"관보온/발포폴리에틸렌보온재","D200, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,51670,0,51670,"합계"]
["MDA31410130S",null,"관보온/발포폴리에틸렌보온재","D250, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,59454,0,59454,"합계"]
["MDA31410140S",null,"관보온/발포폴리에틸렌보온재","D300, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,65195,0,65195,"합계"]
["MDA31510010S",null,"관보온/발포폴리에틸렌보온재","D15, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,14352,0,14352,"합계"]
["MDA31510020S",null,"관보온/발포폴리에틸렌보온재","D20, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,16279,0,16279,"합계"]
["MDA31510030S",null,"관보온/발포폴리에틸렌보온재","D25, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,16853,0,16853,"합계"]
["MDA31510040S",null,"관보온/발포폴리에틸렌보온재","D32, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,19519,0,19519,"합계"]
["MDA31510050S",null,"관보온/발포폴리에틸렌보온재","D40, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,22964,0,22964,"합계"]
["MDA31510060S",null,"관보온/발포폴리에틸렌보온재","D50, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,26983,0,26983,"합계"]
["MDA31510070S",null,"관보온/발포폴리에틸렌보온재","D65, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,28501,0,28501,"합계"]
["MDA31510080S",null,"관보온/발포폴리에틸렌보온재","D80, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,32520,0,32520,"합계"]
["MDA31510090S",null,"관보온/발포폴리에틸렌보온재","D100, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,37687,0,37687,"합계"]
["MDA31510100S",null,"관보온/발포폴리에틸렌보온재","D125, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,44780,0,44780,"합계"]
["MDA31510110S",null,"관보온/발포폴리에틸렌보온재","D150, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,52244,0,52244,"합계"]
["MDA31510120S",null,"관보온/발포폴리에틸렌보온재","D200, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,63152,0,63152,"합계"]
["MDA31510130S",null,"관보온/발포폴리에틸렌보온재","D250, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,72592,0,72592,"합계"]
["MDA31510140S",null,"관보온/발포폴리에틸렌보온재","D300, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,78333,0,78333,"합계"]
["MDA40010010S",null,"관보온/유리솜보온재","D15, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,6110,0,6110,"합계"]
["MDA40010020S",null,"관보온/유리솜보온재","D20, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,6889,0,6889,"합계"]
["MDA40010030S",null,"관보온/유리솜보온재","D25, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,7463,0,7463,"합계"]
["MDA40010040S",null,"관보온/유리솜보온재","D32, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,8815,0,8815,"합계"]
["MDA40010050S",null,"관보온/유리솜보온재","D40, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,10334,0,10334,"합계"]
["MDA40010060S",null,"관보온/유리솜보온재","D50, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,12260,0,12260,"합계"]
["MDA40010070S",null,"관보온/유리솜보온재","D65, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,14352,0,14352,"합계"]
["MDA40010080S",null,"관보온/유리솜보온재","D80, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,17223,0,17223,"합계"]
["MDA40010090S",null,"관보온/유리솜보온재","D100, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,19889,0,19889,"합계"]
["MDA40010100S",null,"관보온/유리솜보온재","D125, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,24686,0,24686,"합계"]
["MDA40010110S",null,"관보온/유리솜보온재","D150, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,28705,0,28705,"합계"]
["MDA40010120S",null,"관보온/유리솜보온재","D200, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,39818,0,39818,"합계"]
["MDA40010130S",null,"관보온/유리솜보온재","D250, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,47077,0,47077,"합계"]
["MDA40010140S",null,"관보온/유리솜보온재","D300, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,51670,0,51670,"합계"]
["MDA40110010S",null,"관보온/유리솜보온재","D15, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,6889,0,6889,"합계"]
["MDA40110020S",null,"관보온/유리솜보온재","D20, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,7463,0,7463,"합계"]
["MDA40110030S",null,"관보온/유리솜보온재","D25, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,8241,0,8241,"합계"]
["MDA40110040S",null,"관보온/유리솜보온재","D32, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,9759,0,9759,"합계"]
["MDA40110050S",null,"관보온/유리솜보온재","D40, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,11482,0,11482,"합계"]
["MDA40110060S",null,"관보온/유리솜보온재","D50, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,13778,0,13778,"합계"]
["MDA40110070S",null,"관보온/유리솜보온재","D65, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,16075,0,16075,"합계"]
["MDA40110080S",null,"관보온/유리솜보온재","D80, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,19149,0,19149,"합계"]
["MDA40110090S",null,"관보온/유리솜보온재","D100, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,22020,0,22020,"합계"]
["MDA40110100S",null,"관보온/유리솜보온재","D125, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,27353,0,27353,"합계"]
["MDA40110110S",null,"관보온/유리솜보온재","D150, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,31946,0,31946,"합계"]
["MDA40110120S",null,"관보온/유리솜보온재","D200, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,44206,0,44206,"합계"]
["MDA40110130S",null,"관보온/유리솜보온재","D250, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,52244,0,52244,"합계"]
["MDA40110140S",null,"관보온/유리솜보온재","D300, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,57411,0,57411,"합계"]
["MDA40210010S",null,"관보온/유리솜보온재","D15, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,7833,0,7833,"합계"]
["MDA40210020S",null,"관보온/유리솜보온재","D20, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,8611,0,8611,"합계"]
["MDA40210030S",null,"관보온/유리솜보온재","D25, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,9555,0,9555,"합계"]
["MDA40210040S",null,"관보온/유리솜보온재","D32, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,11112,0,11112,"합계"]
["MDA40210050S",null,"관보온/유리솜보온재","D40, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,13204,0,13204,"합계"]
["MDA40210060S",null,"관보온/유리솜보온재","D50, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,15705,0,15705,"합계"]
["MDA40210070S",null,"관보온/유리솜보온재","D65, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,18371,0,18371,"합계"]
["MDA40210080S",null,"관보온/유리솜보온재","D80, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,22020,0,22020,"합계"]
["MDA40210090S",null,"관보온/유리솜보온재","D100, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,25260,0,25260,"합계"]
["MDA40210100S",null,"관보온/유리솜보온재","D125, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,31371,0,31371,"합계"]
["MDA40210110S",null,"관보온/유리솜보온재","D150, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,36743,0,36743,"합계"]
["MDA40210120S",null,"관보온/유리솜보온재","D200, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,50726,0,50726,"합계"]
["MDA40210130S",null,"관보온/유리솜보온재","D250, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,59454,0,59454,"합계"]
["MDA40210140S",null,"관보온/유리솜보온재","D300, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,65195,0,65195,"합계"]
["MDA40310010S",null,"관보온/유리솜보온재","D15, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,9964,0,9964,"합계"]
["MDA40310020S",null,"관보온/유리솜보온재","D20, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,10908,0,10908,"합계"]
["MDA40310030S",null,"관보온/유리솜보온재","D25, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,11686,0,11686,"합계"]
["MDA40310040S",null,"관보온/유리솜보온재","D32, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,13574,0,13574,"합계"]
["MDA40310050S",null,"관보온/유리솜보온재","D40, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,16075,0,16075,"합계"]
["MDA40310060S",null,"관보온/유리솜보온재","D50, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,18371,0,18371,"합계"]
["MDA40310070S",null,"관보온/유리솜보온재","D65, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,19889,0,19889,"합계"]
["MDA40310080S",null,"관보온/유리솜보온재","D80, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,23538,0,23538,"합계"]
["MDA40310090S",null,"관보온/유리솜보온재","D100, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,25835,0,25835,"합계"]
["MDA40310100S",null,"관보온/유리솜보온재","D125, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,30428,0,30428,"합계"]
["MDA40310110S",null,"관보온/유리솜보온재","D150, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,36947,0,36947,"합계"]
["MDA40310120S",null,"관보온/유리솜보온재","D200, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,43058,0,43058,"합계"]
["MDA40310130S",null,"관보온/유리솜보온재","D250, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,51670,0,51670,"합계"]
["MDA40310140S",null,"관보온/유리솜보온재","D300, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,57411,0,57411,"합계"]
["MDA40410010S",null,"관보온/유리솜보온재","D15, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,10908,0,10908,"합계"]
["MDA40410020S",null,"관보온/유리솜보온재","D20, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,12260,0,12260,"합계"]
["MDA40410030S",null,"관보온/유리솜보온재","D25, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,13000,0,13000,"합계"]
["MDA40410040S",null,"관보온/유리솜보온재","D32, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,15131,0,15131,"합계"]
["MDA40410050S",null,"관보온/유리솜보온재","D40, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,18001,0,18001,"합계"]
["MDA40410060S",null,"관보온/유리솜보온재","D50, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,20463,0,20463,"합계"]
["MDA40410070S",null,"관보온/유리솜보온재","D65, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,22020,0,22020,"합계"]
["MDA40410080S",null,"관보온/유리솜보온재","D80, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,26039,0,26039,"합계"]
["MDA40410090S",null,"관보온/유리솜보온재","D100, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,28705,0,28705,"합계"]
["MDA40410100S",null,"관보온/유리솜보온재","D125, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,33872,0,33872,"합계"]
["MDA40410110S",null,"관보온/유리솜보온재","D150, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,40966,0,40966,"합계"]
["MDA40410120S",null,"관보온/유리솜보온재","D200, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,47855,0,47855,"합계"]
["MDA40410130S",null,"관보온/유리솜보온재","D250, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,57411,0,57411,"합계"]
["MDA40410140S",null,"관보온/유리솜보온재","D300, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,63152,0,63152,"합계"]
["MDA40510010S",null,"관보온/유리솜보온재","D15, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,12630,0,12630,"합계"]
["MDA40510020S",null,"관보온/유리솜보온재","D20, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,13982,0,13982,"합계"]
["MDA40510030S",null,"관보온/유리솜보온재","D25, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,14926,0,14926,"합계"]
["MDA40510040S",null,"관보온/유리솜보온재","D32, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,17223,0,17223,"합계"]
["MDA40510050S",null,"관보온/유리솜보온재","D40, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,20668,0,20668,"합계"]
["MDA40510060S",null,"관보온/유리솜보온재","D50, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,23538,0,23538,"합계"]
["MDA40510070S",null,"관보온/유리솜보온재","D65, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,25260,0,25260,"합계"]
["MDA40510080S",null,"관보온/유리솜보온재","D80, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,29853,0,29853,"합계"]
["MDA40510090S",null,"관보온/유리솜보온재","D100, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,32928,0,32928,"합계"]
["MDA40510100S",null,"관보온/유리솜보온재","D125, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,38835,0,38835,"합계"]
["MDA40510110S",null,"관보온/유리솜보온재","D150, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,47077,0,47077,"합계"]
["MDA40510120S",null,"관보온/유리솜보온재","D200, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,55115,0,55115,"합계"]
["MDA40510130S",null,"관보온/유리솜보온재","D250, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,65195,0,65195,"합계"]
["MDA40510140S",null,"관보온/유리솜보온재","D300, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,74634,0,74634,"합계"]
["MDA41010010S",null,"관보온/유리솜보온재","D15, 보온두께 25mm 이하, 일반접합, 기계실","m",0,7259,0,7259,"합계"]
["MDA41010020S",null,"관보온/유리솜보온재","D20, 보온두께 25mm 이하, 일반접합, 기계실","m",0,8037,0,8037,"합계"]
["MDA41010030S",null,"관보온/유리솜보온재","D25, 보온두께 25mm 이하, 일반접합, 기계실","m",0,8815,0,8815,"합계"]
["MDA41010040S",null,"관보온/유리솜보온재","D32, 보온두께 25mm 이하, 일반접합, 기계실","m",0,10334,0,10334,"합계"]
["MDA41010050S",null,"관보온/유리솜보온재","D40, 보온두께 25mm 이하, 일반접합, 기계실","m",0,12260,0,12260,"합계"]
["MDA41010060S",null,"관보온/유리솜보온재","D50, 보온두께 25mm 이하, 일반접합, 기계실","m",0,14557,0,14557,"합계"]
["MDA41010070S",null,"관보온/유리솜보온재","D65, 보온두께 25mm 이하, 일반접합, 기계실","m",0,17019,0,17019,"합계"]
["MDA41010080S",null,"관보온/유리솜보온재","D80, 보온두께 25mm 이하, 일반접합, 기계실","m",0,20298,0,20298,"합계"]
["MDA41010090S",null,"관보온/유리솜보온재","D100, 보온두께 25mm 이하, 일반접합, 기계실","m",0,23538,0,23538,"합계"]
["MDA41010100S",null,"관보온/유리솜보온재","D125, 보온두께 25mm 이하, 일반접합, 기계실","m",0,29075,0,29075,"합계"]
["MDA41010110S",null,"관보온/유리솜보온재","D150, 보온두께 25mm 이하, 일반접합, 기계실","m",0,33872,0,33872,"합계"]
["MDA41010120S",null,"관보온/유리솜보온재","D200, 보온두께 25mm 이하, 일반접합, 기계실","m",0,47077,0,47077,"합계"]
["MDA41010130S",null,"관보온/유리솜보온재","D250, 보온두께 25mm 이하, 일반접합, 기계실","m",0,55484,0,55484,"합계"]
["MDA41010140S",null,"관보온/유리솜보온재","D300, 보온두께 25mm 이하, 일반접합, 기계실","m",0,61109,0,61109,"합계"]
["MDA41110010S",null,"관보온/유리솜보온재","D15, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,8037,0,8037,"합계"]
["MDA41110020S",null,"관보온/유리솜보온재","D20, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,9185,0,9185,"합계"]
["MDA41110030S",null,"관보온/유리솜보온재","D25, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,9964,0,9964,"합계"]
["MDA41110040S",null,"관보온/유리솜보온재","D32, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,11686,0,11686,"합계"]
["MDA41110050S",null,"관보온/유리솜보온재","D40, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,13778,0,13778,"합계"]
["MDA41110060S",null,"관보온/유리솜보온재","D50, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,16445,0,16445,"합계"]
["MDA41110070S",null,"관보온/유리솜보온재","D65, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,19149,0,19149,"합계"]
["MDA41110080S",null,"관보온/유리솜보온재","D80, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,22964,0,22964,"합계"]
["MDA41110090S",null,"관보온/유리솜보온재","D100, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,26613,0,26613,"합계"]
["MDA41110100S",null,"관보온/유리솜보온재","D125, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,32928,0,32928,"합계"]
["MDA41110110S",null,"관보온/유리솜보온재","D150, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,38465,0,38465,"합계"]
["MDA41110120S",null,"관보온/유리솜보온재","D200, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,53188,0,53188,"합계"]
["MDA41110130S",null,"관보온/유리솜보온재","D250, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,63152,0,63152,"합계"]
["MDA41110140S",null,"관보온/유리솜보온재","D300, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,68893,0,68893,"합계"]
["MDA41210010S",null,"관보온/유리솜보온재","D15, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,9759,0,9759,"합계"]
["MDA41210020S",null,"관보온/유리솜보온재","D20, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,10908,0,10908,"합계"]
["MDA41210030S",null,"관보온/유리솜보온재","D25, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,11852,0,11852,"합계"]
["MDA41210040S",null,"관보온/유리솜보온재","D32, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,13778,0,13778,"합계"]
["MDA41210050S",null,"관보온/유리솜보온재","D40, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,16445,0,16445,"합계"]
["MDA41210060S",null,"관보온/유리솜보온재","D50, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,19519,0,19519,"합계"]
["MDA41210070S",null,"관보온/유리솜보온재","D65, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,22760,0,22760,"합계"]
["MDA41210080S",null,"관보온/유리솜보온재","D80, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,27353,0,27353,"합계"]
["MDA41210090S",null,"관보온/유리솜보온재","D100, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,31576,0,31576,"합계"]
["MDA41210100S",null,"관보온/유리솜보온재","D125, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,39039,0,39039,"합계"]
["MDA41210110S",null,"관보온/유리솜보온재","D150, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,45559,0,45559,"합계"]
["MDA41210120S",null,"관보온/유리솜보온재","D200, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,63152,0,63152,"합계"]
["MDA41210130S",null,"관보온/유리솜보온재","D250, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,74634,0,74634,"합계"]
["MDA41210140S",null,"관보온/유리솜보온재","D300, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,82418,0,82418,"합계"]
["MDA41310010S",null,"관보온/유리솜보온재","D15, 보온두께 50mm 이하, 일반접합, 기계실","m",0,11686,0,11686,"합계"]
["MDA41310020S",null,"관보온/유리솜보온재","D20, 보온두께 50mm 이하, 일반접합, 기계실","m",0,13000,0,13000,"합계"]
["MDA41310030S",null,"관보온/유리솜보온재","D25, 보온두께 50mm 이하, 일반접합, 기계실","m",0,13778,0,13778,"합계"]
["MDA41310040S",null,"관보온/유리솜보온재","D32, 보온두께 50mm 이하, 일반접합, 기계실","m",0,16075,0,16075,"합계"]
["MDA41310050S",null,"관보온/유리솜보온재","D40, 보온두께 50mm 이하, 일반접합, 기계실","m",0,18945,0,18945,"합계"]
["MDA41310060S",null,"관보온/유리솜보온재","D50, 보온두께 50mm 이하, 일반접합, 기계실","m",0,21816,0,21816,"합계"]
["MDA41310070S",null,"관보온/유리솜보온재","D65, 보온두께 50mm 이하, 일반접합, 기계실","m",0,23538,0,23538,"합계"]
["MDA41310080S",null,"관보온/유리솜보온재","D80, 보온두께 50mm 이하, 일반접합, 기계실","m",0,27761,0,27761,"합계"]
["MDA41310090S",null,"관보온/유리솜보온재","D100, 보온두께 50mm 이하, 일반접합, 기계실","m",0,30428,0,30428,"합계"]
["MDA41310100S",null,"관보온/유리솜보온재","D125, 보온두께 50mm 이하, 일반접합, 기계실","m",0,35964,0,35964,"합계"]
["MDA41310110S",null,"관보온/유리솜보온재","D150, 보온두께 50mm 이하, 일반접합, 기계실","m",0,43632,0,43632,"합계"]
["MDA41310120S",null,"관보온/유리솜보온재","D200, 보온두께 50mm 이하, 일반접합, 기계실","m",0,50891,0,50891,"합계"]
["MDA41310130S",null,"관보온/유리솜보온재","D250, 보온두께 50mm 이하, 일반접합, 기계실","m",0,61109,0,61109,"합계"]
["MDA41310140S",null,"관보온/유리솜보온재","D300, 보온두께 50mm 이하, 일반접합, 기계실","m",0,68893,0,68893,"합계"]
["MDA41410010S",null,"관보온/유리솜보온재","D15, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,13204,0,13204,"합계"]
["MDA41410020S",null,"관보온/유리솜보온재","D20, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,14722,0,14722,"합계"]
["MDA41410030S",null,"관보온/유리솜보온재","D25, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,15705,0,15705,"합계"]
["MDA41410040S",null,"관보온/유리솜보온재","D32, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,18167,0,18167,"합계"]
["MDA41410050S",null,"관보온/유리솜보온재","D40, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,21612,0,21612,"합계"]
["MDA41410060S",null,"관보온/유리솜보온재","D50, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,24686,0,24686,"합계"]
["MDA41410070S",null,"관보온/유리솜보온재","D65, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,26613,0,26613,"합계"]
["MDA41410080S",null,"관보온/유리솜보온재","D80, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,31576,0,31576,"합계"]
["MDA41410090S",null,"관보온/유리솜보온재","D100, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,34446,0,34446,"합계"]
["MDA41410100S",null,"관보온/유리솜보온재","D125, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,40762,0,40762,"합계"]
["MDA41410110S",null,"관보온/유리솜보온재","D150, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,49373,0,49373,"합계"]
["MDA41410120S",null,"관보온/유리솜보온재","D200, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,57411,0,57411,"합계"]
["MDA41410130S",null,"관보온/유리솜보온재","D250, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,68893,0,68893,"합계"]
["MDA41410140S",null,"관보온/유리솜보온재","D300, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,76677,0,76677,"합계"]
["MDA41510010S",null,"관보온/유리솜보온재","D15, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,15705,0,15705,"합계"]
["MDA41510020S",null,"관보온/유리솜보온재","D20, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,17427,0,17427,"합계"]
["MDA41510030S",null,"관보온/유리솜보온재","D25, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,18575,0,18575,"합계"]
["MDA41510040S",null,"관보온/유리솜보온재","D32, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,21612,0,21612,"합계"]
["MDA41510050S",null,"관보온/유리솜보온재","D40, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,25630,0,25630,"합계"]
["MDA41510060S",null,"관보온/유리솜보온재","D50, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,29279,0,29279,"합계"]
["MDA41510070S",null,"관보온/유리솜보온재","D65, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,31576,0,31576,"합계"]
["MDA41510080S",null,"관보온/유리솜보온재","D80, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,37317,0,37317,"합계"]
["MDA41510090S",null,"관보온/유리솜보온재","D100, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,40966,0,40966,"합계"]
["MDA41510100S",null,"관보온/유리솜보온재","D125, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,48225,0,48225,"합계"]
["MDA41510110S",null,"관보온/유리솜보온재","D150, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,57411,0,57411,"합계"]
["MDA41510120S",null,"관보온/유리솜보온재","D200, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,68893,0,68893,"합계"]
["MDA41510130S",null,"관보온/유리솜보온재","D250, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,82418,0,82418,"합계"]
["MDA41510140S",null,"관보온/유리솜보온재","D300, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,91858,0,91858,"합계"]
["MDA50010010S",null,"관보온/유리솜보온재","D15, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,6685,0,6685,"합계"]
["MDA50010020S",null,"관보온/유리솜보온재","D20, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,7463,0,7463,"합계"]
["MDA50010030S",null,"관보온/유리솜보온재","D25, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,8037,0,8037,"합계"]
["MDA50010040S",null,"관보온/유리솜보온재","D32, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,9555,0,9555,"합계"]
["MDA50010050S",null,"관보온/유리솜보온재","D40, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,11278,0,11278,"합계"]
["MDA50010060S",null,"관보온/유리솜보온재","D50, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,13408,0,13408,"합계"]
["MDA50010070S",null,"관보온/유리솜보온재","D65, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,15501,0,15501,"합계"]
["MDA50010080S",null,"관보온/유리솜보온재","D80, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,18741,0,18741,"합계"]
["MDA50010090S",null,"관보온/유리솜보온재","D100, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,21612,0,21612,"합계"]
["MDA50010100S",null,"관보온/유리솜보온재","D125, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,26779,0,26779,"합계"]
["MDA50010110S",null,"관보온/유리솜보온재","D150, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,31206,0,31206,"합계"]
["MDA50010120S",null,"관보온/유리솜보온재","D200, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,43262,0,43262,"합계"]
["MDA50010130S",null,"관보온/유리솜보온재","D250, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,51096,0,51096,"합계"]
["MDA50010140S",null,"관보온/유리솜보온재","D300, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,56263,0,56263,"합계"]
["MDA50110010S",null,"관보온/유리솜보온재","D15, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,7463,0,7463,"합계"]
["MDA50110020S",null,"관보온/유리솜보온재","D20, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,8241,0,8241,"합계"]
["MDA50110030S",null,"관보온/유리솜보온재","D25, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,9185,0,9185,"합계"]
["MDA50110040S",null,"관보온/유리솜보온재","D32, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,10703,0,10703,"합계"]
["MDA50110050S",null,"관보온/유리솜보온재","D40, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,12630,0,12630,"합계"]
["MDA50110060S",null,"관보온/유리솜보온재","D50, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,14926,0,14926,"합계"]
["MDA50110070S",null,"관보온/유리솜보온재","D65, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,17593,0,17593,"합계"]
["MDA50110080S",null,"관보온/유리솜보온재","D80, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,21037,0,21037,"합계"]
["MDA50110090S",null,"관보온/유리솜보온재","D100, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,24317,0,24317,"합계"]
["MDA50110100S",null,"관보온/유리솜보온재","D125, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,30058,0,30058,"합계"]
["MDA50110110S",null,"관보온/유리솜보온재","D150, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,35020,0,35020,"합계"]
["MDA50110120S",null,"관보온/유리솜보온재","D200, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,48595,0,48595,"합계"]
["MDA50110130S",null,"관보온/유리솜보온재","D250, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,57411,0,57411,"합계"]
["MDA50110140S",null,"관보온/유리솜보온재","D300, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,63152,0,63152,"합계"]
["MDA50210010S",null,"관보온/유리솜보온재","D15, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,8611,0,8611,"합계"]
["MDA50210020S",null,"관보온/유리솜보온재","D20, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,9759,0,9759,"합계"]
["MDA50210030S",null,"관보온/유리솜보온재","D25, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,10703,0,10703,"합계"]
["MDA50210040S",null,"관보온/유리솜보온재","D32, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,12426,0,12426,"합계"]
["MDA50210050S",null,"관보온/유리솜보온재","D40, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,14722,0,14722,"합계"]
["MDA50210060S",null,"관보온/유리솜보온재","D50, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,17593,0,17593,"합계"]
["MDA50210070S",null,"관보온/유리솜보온재","D65, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,20463,0,20463,"합계"]
["MDA50210080S",null,"관보온/유리솜보온재","D80, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,24482,0,24482,"합계"]
["MDA50210090S",null,"관보온/유리솜보온재","D100, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,28335,0,28335,"합계"]
["MDA50210100S",null,"관보온/유리솜보온재","D125, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,35020,0,35020,"합계"]
["MDA50210110S",null,"관보온/유리솜보온재","D150, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,40762,0,40762,"합계"]
["MDA50210120S",null,"관보온/유리솜보온재","D200, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,56633,0,56633,"합계"]
["MDA50210130S",null,"관보온/유리솜보온재","D250, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,66850,0,66850,"합계"]
["MDA50210140S",null,"관보온/유리솜보온재","D300, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,74634,0,74634,"합계"]
["MDA50310010S",null,"관보온/유리솜보온재","D15, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,10908,0,10908,"합계"]
["MDA50310020S",null,"관보온/유리솜보온재","D20, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,12056,0,12056,"합계"]
["MDA50310030S",null,"관보온/유리솜보온재","D25, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,12834,0,12834,"합계"]
["MDA50310040S",null,"관보온/유리솜보온재","D32, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,14926,0,14926,"합계"]
["MDA50310050S",null,"관보온/유리솜보온재","D40, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,17593,0,17593,"합계"]
["MDA50310060S",null,"관보온/유리솜보온재","D50, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,20093,0,20093,"합계"]
["MDA50310070S",null,"관보온/유리솜보온재","D65, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,21612,0,21612,"합계"]
["MDA50310080S",null,"관보온/유리솜보온재","D80, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,25630,0,25630,"합계"]
["MDA50310090S",null,"관보온/유리솜보온재","D100, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,28131,0,28131,"합계"]
["MDA50310100S",null,"관보온/유리솜보온재","D125, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,33094,0,33094,"합계"]
["MDA50310110S",null,"관보온/유리솜보온재","D150, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,40188,0,40188,"합계"]
["MDA50310120S",null,"관보온/유리솜보온재","D200, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,46873,0,46873,"합계"]
["MDA50310130S",null,"관보온/유리솜보온재","D250, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,56263,0,56263,"합계"]
["MDA50310140S",null,"관보온/유리솜보온재","D300, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,63152,0,63152,"합계"]
["MDA50410010S",null,"관보온/유리솜보온재","D15, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,12056,0,12056,"합계"]
["MDA50410020S",null,"관보온/유리솜보온재","D20, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,13408,0,13408,"합계"]
["MDA50410030S",null,"관보온/유리솜보온재","D25, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,14352,0,14352,"합계"]
["MDA50410040S",null,"관보온/유리솜보온재","D32, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,16649,0,16649,"합계"]
["MDA50410050S",null,"관보온/유리솜보온재","D40, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,19724,0,19724,"합계"]
["MDA50410060S",null,"관보온/유리솜보온재","D50, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,22390,0,22390,"합계"]
["MDA50410070S",null,"관보온/유리솜보온재","D65, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,24317,0,24317,"합계"]
["MDA50410080S",null,"관보온/유리솜보온재","D80, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,28705,0,28705,"합계"]
["MDA50410090S",null,"관보온/유리솜보온재","D100, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,31576,0,31576,"합계"]
["MDA50410100S",null,"관보온/유리솜보온재","D125, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,37113,0,37113,"합계"]
["MDA50410110S",null,"관보온/유리솜보온재","D150, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,44985,0,44985,"합계"]
["MDA50410120S",null,"관보온/유리솜보온재","D200, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,52614,0,52614,"합계"]
["MDA50410130S",null,"관보온/유리솜보온재","D250, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,63152,0,63152,"합계"]
["MDA50410140S",null,"관보온/유리솜보온재","D300, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,68893,0,68893,"합계"]
["MDA50510010S",null,"관보온/유리솜보온재","D15, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,14148,0,14148,"합계"]
["MDA50510020S",null,"관보온/유리솜보온재","D20, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,15705,0,15705,"합계"]
["MDA50510030S",null,"관보온/유리솜보온재","D25, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,16649,0,16649,"합계"]
["MDA50510040S",null,"관보온/유리솜보온재","D32, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,19315,0,19315,"합계"]
["MDA50510050S",null,"관보온/유리솜보온재","D40, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,22964,0,22964,"합계"]
["MDA50510060S",null,"관보온/유리솜보온재","D50, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,26409,0,26409,"합계"]
["MDA50510070S",null,"관보온/유리솜보온재","D65, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,28335,0,28335,"합계"]
["MDA50510080S",null,"관보온/유리솜보온재","D80, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,33502,0,33502,"합계"]
["MDA50510090S",null,"관보온/유리솜보온재","D100, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,36743,0,36743,"합계"]
["MDA50510100S",null,"관보온/유리솜보온재","D125, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,43262,0,43262,"합계"]
["MDA50510110S",null,"관보온/유리솜보온재","D150, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,52614,0,52614,"합계"]
["MDA50510120S",null,"관보온/유리솜보온재","D200, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,61109,0,61109,"합계"]
["MDA50510130S",null,"관보온/유리솜보온재","D250, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,74634,0,74634,"합계"]
["MDA50510140S",null,"관보온/유리솜보온재","D300, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,80376,0,80376,"합계"]
["MDA51010010S",null,"관보온/유리솜보온재","D15, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,8037,0,8037,"합계"]
["MDA51010020S",null,"관보온/유리솜보온재","D20, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,8815,0,8815,"합계"]
["MDA51010030S",null,"관보온/유리솜보온재","D25, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,9759,0,9759,"합계"]
["MDA51010040S",null,"관보온/유리솜보온재","D32, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,11482,0,11482,"합계"]
["MDA51010050S",null,"관보온/유리솜보온재","D40, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,13574,0,13574,"합계"]
["MDA51010060S",null,"관보온/유리솜보온재","D50, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,16075,0,16075,"합계"]
["MDA51010070S",null,"관보온/유리솜보온재","D65, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,18741,0,18741,"합계"]
["MDA51010080S",null,"관보온/유리솜보온재","D80, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,22390,0,22390,"합계"]
["MDA51010090S",null,"관보온/유리솜보온재","D100, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,25835,0,25835,"합계"]
["MDA51010100S",null,"관보온/유리솜보온재","D125, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,32150,0,32150,"합계"]
["MDA51010110S",null,"관보온/유리솜보온재","D150, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,37521,0,37521,"합계"]
["MDA51010120S",null,"관보온/유리솜보온재","D200, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,51874,0,51874,"합계"]
["MDA51010130S",null,"관보온/유리솜보온재","D250, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,61109,0,61109,"합계"]
["MDA51010140S",null,"관보온/유리솜보온재","D300, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,68893,0,68893,"합계"]
["MDA51110010S",null,"관보온/유리솜보온재","D15, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,9185,0,9185,"합계"]
["MDA51110020S",null,"관보온/유리솜보온재","D20, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,10334,0,10334,"합계"]
["MDA51110021S",null,"관보온/유리솜보온재","D25, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,11278,0,11278,"합계"]
["MDA51110022S",null,"관보온/유리솜보온재","D32, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,13204,0,13204,"합계"]
["MDA51110023S",null,"관보온/유리솜보온재","D40, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,15501,0,15501,"합계"]
["MDA51110024S",null,"관보온/유리솜보온재","D50, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,18371,0,18371,"합계"]
["MDA51110025S",null,"관보온/유리솜보온재","D65, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,21612,0,21612,"합계"]
["MDA51110026S",null,"관보온/유리솜보온재","D80, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,25835,0,25835,"합계"]
["MDA51110027S",null,"관보온/유리솜보온재","D100, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,29853,0,29853,"합계"]
["MDA51110028S",null,"관보온/유리솜보온재","D125, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,36947,0,36947,"합계"]
["MDA51110029S",null,"관보온/유리솜보온재","D150, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,43058,0,43058,"합계"]
["MDA51110030S",null,"관보온/유리솜보온재","D200, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,59454,0,59454,"합계"]
["MDA51110031S",null,"관보온/유리솜보온재","D250, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,70936,0,70936,"합계"]
["MDA51110032S",null,"관보온/유리솜보온재","D300, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,78333,0,78333,"합계"]
["MDA51210010S",null,"관보온/유리솜보온재","D15, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,11112,0,11112,"합계"]
["MDA51210020S",null,"관보온/유리솜보온재","D20, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,12426,0,12426,"합계"]
["MDA51210030S",null,"관보온/유리솜보온재","D25, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,13778,0,13778,"합계"]
["MDA51210040S",null,"관보온/유리솜보온재","D32, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,16075,0,16075,"합계"]
["MDA51210050S",null,"관보온/유리솜보온재","D40, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,18945,0,18945,"합계"]
["MDA51210060S",null,"관보온/유리솜보온재","D50, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,22390,0,22390,"합계"]
["MDA51210070S",null,"관보온/유리솜보온재","D65, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,26204,0,26204,"합계"]
["MDA51210080S",null,"관보온/유리솜보온재","D80, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,31371,0,31371,"합계"]
["MDA51210090S",null,"관보온/유리솜보온재","D100, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,36169,0,36169,"합계"]
["MDA51210100S",null,"관보온/유리솜보온재","D125, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,44780,0,44780,"합계"]
["MDA51210110S",null,"관보온/유리솜보온재","D150, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,52244,0,52244,"합계"]
["MDA51210120S",null,"관보온/유리솜보온재","D200, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,72592,0,72592,"합계"]
["MDA51210130S",null,"관보온/유리솜보온재","D250, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,86117,0,86117,"합계"]
["MDA51210140S",null,"관보온/유리솜보온재","D300, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,93901,0,93901,"합계"]
["MDA51310010S",null,"관보온/유리솜보온재","D15, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,13000,0,13000,"합계"]
["MDA51310020S",null,"관보온/유리솜보온재","D20, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,14352,0,14352,"합계"]
["MDA51310030S",null,"관보온/유리솜보온재","D25, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,15296,0,15296,"합계"]
["MDA51310040S",null,"관보온/유리솜보온재","D32, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,17797,0,17797,"합계"]
["MDA51310050S",null,"관보온/유리솜보온재","D40, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,21242,0,21242,"합계"]
["MDA51310060S",null,"관보온/유리솜보온재","D50, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,24112,0,24112,"합계"]
["MDA51310070S",null,"관보온/유리솜보온재","D65, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,25835,0,25835,"합계"]
["MDA51310080S",null,"관보온/유리솜보온재","D80, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,30632,0,30632,"합계"]
["MDA51310090S",null,"관보온/유리솜보온재","D100, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,33872,0,33872,"합계"]
["MDA51310100S",null,"관보온/유리솜보온재","D125, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,39613,0,39613,"합계"]
["MDA51310110S",null,"관보온/유리솜보온재","D150, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,48225,0,48225,"합계"]
["MDA51310120S",null,"관보온/유리솜보온재","D200, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,56263,0,56263,"합계"]
["MDA51310130S",null,"관보온/유리솜보온재","D250, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,68893,0,68893,"합계"]
["MDA51310140S",null,"관보온/유리솜보온재","D300, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,74634,0,74634,"합계"]
["MDA51410010S",null,"관보온/유리솜보온재","D15, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,14926,0,14926,"합계"]
["MDA51410020S",null,"관보온/유리솜보온재","D20, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,16649,0,16649,"합계"]
["MDA51410030S",null,"관보온/유리솜보온재","D25, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,17593,0,17593,"합계"]
["MDA51410040S",null,"관보온/유리솜보온재","D32, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,20463,0,20463,"합계"]
["MDA51410050S",null,"관보온/유리솜보온재","D40, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,24112,0,24112,"합계"]
["MDA51410060S",null,"관보온/유리솜보온재","D50, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,27761,0,27761,"합계"]
["MDA51410070S",null,"관보온/유리솜보온재","D65, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,29853,0,29853,"합계"]
["MDA51410080S",null,"관보온/유리솜보온재","D80, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,35225,0,35225,"합계"]
["MDA51410090S",null,"관보온/유리솜보온재","D100, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,38835,0,38835,"합계"]
["MDA51410100S",null,"관보온/유리솜보온재","D125, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,45559,0,45559,"합계"]
["MDA51410110S",null,"관보온/유리솜보온재","D150, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,55484,0,55484,"합계"]
["MDA51410120S",null,"관보온/유리솜보온재","D200, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,65195,0,65195,"합계"]
["MDA51410130S",null,"관보온/유리솜보온재","D250, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,78333,0,78333,"합계"]
["MDA51410140S",null,"관보온/유리솜보온재","D300, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,86117,0,86117,"합계"]
["MDA51510010S",null,"관보온/유리솜보온재","D15, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,18167,0,18167,"합계"]
["MDA51510020S",null,"관보온/유리솜보온재","D20, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,20093,0,20093,"합계"]
["MDA51510030S",null,"관보온/유리솜보온재","D25, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,21446,0,21446,"합계"]
["MDA51510040S",null,"관보온/유리솜보온재","D32, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,24686,0,24686,"합계"]
["MDA51510050S",null,"관보온/유리솜보온재","D40, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,29279,0,29279,"합계"]
["MDA51510060S",null,"관보온/유리솜보온재","D50, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,33668,0,33668,"합계"]
["MDA51510070S",null,"관보온/유리솜보온재","D65, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,36169,0,36169,"합계"]
["MDA51510080S",null,"관보온/유리솜보온재","D80, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,42854,0,42854,"합계"]
["MDA51510090S",null,"관보온/유리솜보온재","D100, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,47077,0,47077,"합계"]
["MDA51510100S",null,"관보온/유리솜보온재","D125, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,55319,0,55319,"합계"]
["MDA51510110S",null,"관보온/유리솜보온재","D150, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,66850,0,66850,"합계"]
["MDA51510120S",null,"관보온/유리솜보온재","D200, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,78333,0,78333,"합계"]
["MDA51510130S",null,"관보온/유리솜보온재","D250, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,93901,0,93901,"합계"]
["MDA51510140S",null,"관보온/유리솜보온재","D300, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,103340,0,103340,"합계"]
["MDA60000000S",null,"칼라함석마감 배관보온","보온재 두께, 배관규격에 따른 시공량(m) 참조","인/일",0,574115,0,574115,"합계"]
["MDA60010010S",null,"관보온/칼라함석마감"," D15, 보온두께 25mm","m",0,17427,0,17427,"합계"]
["MDA60010020S",null,"관보온/칼라함석마감"," D20, 보온두께 25mm","m",0,18575,0,18575,"합계"]
["MDA60010030S",null,"관보온/칼라함석마감"," D25, 보온두께 25mm","m",0,19149,0,19149,"합계"]
["MDA60010040S",null,"관보온/칼라함석마감"," D32, 보온두께 25mm","m",0,20463,0,20463,"합계"]
["MDA60010050S",null,"관보온/칼라함석마감"," D40, 보온두께 25mm","m",0,21242,0,21242,"합계"]
["MDA60010060S",null,"관보온/칼라함석마감"," D50, 보온두께 25mm","m",0,23908,0,23908,"합계"]
["MDA60110010S",null,"관보온/칼라함석마감"," D65, 보온두께 40mm","m",0,28705,0,28705,"합계"]
["MDA60110020S",null,"관보온/칼라함석마감"," D80, 보온두께 40mm","m",0,33872,0,33872,"합계"]
["MDA60110030S",null,"관보온/칼라함석마감"," D100, 보온두께 40mm","m",0,38261,0,38261,"합계"]
["MDA60110040S",null,"관보온/칼라함석마감"," D125, 보온두께 40mm","m",0,40966,0,40966,"합계"]
["MDA60110050S",null,"관보온/칼라함석마감"," D150, 보온두께 40mm","m",0,47855,0,47855,"합계"]
["MDA60210010S",null,"관보온/칼라함석마감"," D200, 보온두께 50mm","m",0,57411,0,57411,"합계"]
["MDA60210020S",null,"관보온/칼라함석마감"," D250, 보온두께 50mm","m",0,63152,0,63152,"합계"]
["MDA60210030S",null,"관보온/칼라함석마감"," D300, 보온두께 50mm","m",0,72592,0,72592,"합계"]
["MDC00010010S",null,"밸브보온/고무발포보온재","D15, 보온두께 25mm 이하, 일반밸브, 옥내일반","개소",0,51374,0,51374,"합계"]
["MDC00010020S",null,"밸브보온/고무발포보온재","D20, 보온두께 25mm 이하, 일반밸브, 옥내일반","개소",0,52931,0,52931,"합계"]
["MDC00010030S",null,"밸브보온/고무발포보온재","D25, 보온두께 25mm 이하, 일반밸브, 옥내일반","개소",0,54692,0,54692,"합계"]
["MDC00010040S",null,"밸브보온/고무발포보온재","D32, 보온두께 25mm 이하, 일반밸브, 옥내일반","개소",0,57027,0,57027,"합계"]
["MDC00010050S",null,"밸브보온/고무발포보온재","D40, 보온두께 25mm 이하, 일반밸브, 옥내일반","개소",0,59566,0,59566,"합계"]
["MDC00010060S",null,"밸브보온/고무발포보온재","D50, 보온두께 25mm 이하, 일반밸브, 옥내일반","개소",0,63050,0,63050,"합계"]
["MDC00010070S",null,"밸브보온/고무발포보온재","D65, 보온두께 25mm 이하, 일반밸브, 옥내일반","개소",0,66942,0,66942,"합계"]
["MDC00010080S",null,"밸브보온/고무발포보온재","D80, 보온두께 25mm 이하, 일반밸브, 옥내일반","개소",0,74726,0,74726,"합계"]
["MDC00010090S",null,"밸브보온/고무발포보온재","D100, 보온두께 25mm 이하, 일반밸브, 옥내일반","개소",0,88571,0,88571,"합계"]
["MDC00010100S",null,"밸브보온/고무발포보온재","D125, 보온두께 25mm 이하, 일반밸브, 옥내일반","개소",0,93612,0,93612,"합계"]
["MDC00010110S",null,"밸브보온/고무발포보온재","D150, 보온두께 25mm 이하, 일반밸브, 옥내일반","개소",0,99265,0,99265,"합계"]
["MDC00010120S",null,"밸브보온/고무발포보온재","D200, 보온두께 25mm 이하, 일반밸브, 옥내일반","개소",0,108236,0,108236,"합계"]
["MDC00010130S",null,"밸브보온/고무발포보온재","D250, 보온두께 25mm 이하, 일반밸브, 옥내일반","개소",0,114054,0,114054,"합계"]
["MDC00010140S",null,"밸브보온/고무발포보온재","D300, 보온두께 25mm 이하, 일반밸브, 옥내일반","개소",0,133719,0,133719,"합계"]
["MDC00110010S",null,"밸브보온/고무발포보온재","D15, 보온두께 50mm 이하, 일반밸브, 옥내일반","개소",0,86402,0,86402,"합계"]
["MDC00110020S",null,"밸브보온/고무발포보온재","D20, 보온두께 50mm 이하, 일반밸브, 옥내일반","개소",0,89146,0,89146,"합계"]
["MDC00110030S",null,"밸브보온/고무발포보온재","D25, 보온두께 50mm 이하, 일반밸브, 옥내일반","개소",0,92055,0,92055,"합계"]
["MDC00110040S",null,"밸브보온/고무발포보온재","D32, 보온두께 50mm 이하, 일반밸브, 옥내일반","개소",0,96151,0,96151,"합계"]
["MDC00110050S",null,"밸브보온/고무발포보온재","D40, 보온두께 50mm 이하, 일반밸브, 옥내일반","개소",0,100617,0,100617,"합계"]
["MDC00110060S",null,"밸브보온/고무발포보온재","D50, 보온두께 50mm 이하, 일반밸브, 옥내일반","개소",0,106270,0,106270,"합계"]
["MDC00110070S",null,"밸브보온/고무발포보온재","D65, 보온두께 50mm 이하, 일반밸브, 옥내일반","개소",0,114054,0,114054,"합계"]
["MDC00110080S",null,"밸브보온/고무발포보온재","D80, 보온두께 50mm 이하, 일반밸브, 옥내일반","개소",0,122043,0,122043,"합계"]
["MDC00110090S",null,"밸브보온/고무발포보온재","D100, 보온두께 50mm 이하, 일반밸브, 옥내일반","개소",0,137611,0,137611,"합계"]
["MDC00110100S",null,"밸브보온/고무발포보온재","D125, 보온두께 50mm 이하, 일반밸브, 옥내일반","개소",0,153383,0,153383,"합계"]
["MDC00110110S",null,"밸브보온/고무발포보온재","D150, 보온두께 50mm 이하, 일반밸브, 옥내일반","개소",0,165263,0,165263,"합계"]
["MDC00110120S",null,"밸브보온/고무발포보온재","D200, 보온두께 50mm 이하, 일반밸브, 옥내일반","개소",0,169155,0,169155,"합계"]
["MDC00110130S",null,"밸브보온/고무발포보온재","D250, 보온두께 50mm 이하, 일반밸브, 옥내일반","개소",0,192877,0,192877,"합계"]
["MDC00110140S",null,"밸브보온/고무발포보온재","D300, 보온두께 50mm 이하, 일반밸브, 옥내일반","개소",0,200661,0,200661,"합계"]
["MDC01010010S",null,"밸브보온/고무발포보온재","D15, 보온두께 25mm 이하, 일반밸브, 기계실","개소",0,61649,0,61649,"합계"]
["MDC01010020S",null,"밸브보온/고무발포보온재","D20, 보온두께 25mm 이하, 일반밸브, 기계실","개소",0,63517,0,63517,"합계"]
["MDC01010030S",null,"밸브보온/고무발포보온재","D25, 보온두께 25mm 이하, 일반밸브, 기계실","개소",0,65630,0,65630,"합계"]
["MDC01010040S",null,"밸브보온/고무발포보온재","D32, 보온두께 25mm 이하, 일반밸브, 기계실","개소",0,68432,0,68432,"합계"]
["MDC01010050S",null,"밸브보온/고무발포보온재","D40, 보온두께 25mm 이하, 일반밸브, 기계실","개소",0,71480,0,71480,"합계"]
["MDC01010060S",null,"밸브보온/고무발포보온재","D50, 보온두께 25mm 이하, 일반밸브, 기계실","개소",0,75660,0,75660,"합계"]
["MDC01010070S",null,"밸브보온/고무발포보온재","D65, 보온두께 25mm 이하, 일반밸브, 기계실","개소",0,80330,0,80330,"합계"]
["MDC01010080S",null,"밸브보온/고무발포보온재","D80, 보온두께 25mm 이하, 일반밸브, 기계실","개소",0,89671,0,89671,"합계"]
["MDC01010090S",null,"밸브보온/고무발포보온재","D100, 보온두께 25mm 이하, 일반밸브, 기계실","개소",0,106286,0,106286,"합계"]
["MDC01010100S",null,"밸브보온/고무발포보온재","D125, 보온두께 25mm 이하, 일반밸브, 기계실","개소",0,112334,0,112334,"합계"]
["MDC01010110S",null,"밸브보온/고무발포보온재","D150, 보온두께 25mm 이하, 일반밸브, 기계실","개소",0,119118,0,119118,"합계"]
["MDC01010120S",null,"밸브보온/고무발포보온재","D200, 보온두께 25mm 이하, 일반밸브, 기계실","개소",0,129883,0,129883,"합계"]
["MDC01010130S",null,"밸브보온/고무발포보온재","D250, 보온두께 25mm 이하, 일반밸브, 기계실","개소",0,136865,0,136865,"합계"]
["MDC01010140S",null,"밸브보온/고무발포보온재","D300, 보온두께 25mm 이하, 일반밸브, 기계실","개소",0,160462,0,160462,"합계"]
["MDC01110010S",null,"밸브보온/고무발포보온재","D15, 보온두께 50mm 이하, 일반밸브, 기계실","개소",0,103682,0,103682,"합계"]
["MDC01110020S",null,"밸브보온/고무발포보온재","D20, 보온두께 50mm 이하, 일반밸브, 기계실","개소",0,106975,0,106975,"합계"]
["MDC01110030S",null,"밸브보온/고무발포보온재","D25, 보온두께 50mm 이하, 일반밸브, 기계실","개소",0,110466,0,110466,"합계"]
["MDC01110040S",null,"밸브보온/고무발포보온재","D32, 보온두께 50mm 이하, 일반밸브, 기계실","개소",0,115382,0,115382,"합계"]
["MDC01110050S",null,"밸브보온/고무발포보온재","D40, 보온두께 50mm 이하, 일반밸브, 기계실","개소",0,120741,0,120741,"합계"]
["MDC01110060S",null,"밸브보온/고무발포보온재","D50, 보온두께 50mm 이하, 일반밸브, 기계실","개소",0,127525,0,127525,"합계"]
["MDC01110070S",null,"밸브보온/고무발포보온재","D65, 보온두께 50mm 이하, 일반밸브, 기계실","개소",0,136865,0,136865,"합계"]
["MDC01110080S",null,"밸브보온/고무발포보온재","D80, 보온두께 50mm 이하, 일반밸브, 기계실","개소",0,146451,0,146451,"합계"]
["MDC01110090S",null,"밸브보온/고무발포보온재","D100, 보온두께 50mm 이하, 일반밸브, 기계실","개소",0,165133,0,165133,"합계"]
["MDC01110100S",null,"밸브보온/고무발포보온재","D125, 보온두께 50mm 이하, 일반밸브, 기계실","개소",0,184060,0,184060,"합계"]
["MDC01110110S",null,"밸브보온/고무발포보온재","D150, 보온두께 50mm 이하, 일반밸브, 기계실","개소",0,198316,0,198316,"합계"]
["MDC01110120S",null,"밸브보온/고무발포보온재","D200, 보온두께 50mm 이하, 일반밸브, 기계실","개소",0,202986,0,202986,"합계"]
["MDC01110130S",null,"밸브보온/고무발포보온재","D250, 보온두께 50mm 이하, 일반밸브, 기계실","개소",0,231453,0,231453,"합계"]
["MDC01110140S",null,"밸브보온/고무발포보온재","D300, 보온두께 50mm 이하, 일반밸브, 기계실","개소",0,240793,0,240793,"합계"]
["MDC10010010S",null,"밸브보온/고무발포보온재","D15, 보온두께 25mm 이하, 각종부속부착, 옥내일반","개소",0,64217,0,64217,"합계"]
["MDC10010020S",null,"밸브보온/고무발포보온재","D20, 보온두께 25mm 이하, 각종부속부착, 옥내일반","개소",0,66163,0,66163,"합계"]
["MDC10010030S",null,"밸브보온/고무발포보온재","D25, 보온두께 25mm 이하, 각종부속부착, 옥내일반","개소",0,68365,0,68365,"합계"]
["MDC10010040S",null,"밸브보온/고무발포보온재","D32, 보온두께 25mm 이하, 각종부속부착, 옥내일반","개소",0,71284,0,71284,"합계"]
["MDC10010050S",null,"밸브보온/고무발포보온재","D40, 보온두께 25mm 이하, 각종부속부착, 옥내일반","개소",0,74458,0,74458,"합계"]
["MDC10010060S",null,"밸브보온/고무발포보온재","D50, 보온두께 25mm 이하, 각종부속부착, 옥내일반","개소",0,78812,0,78812,"합계"]
["MDC10010070S",null,"밸브보온/고무발포보온재","D65, 보온두께 25mm 이하, 각종부속부착, 옥내일반","개소",0,83677,0,83677,"합계"]
["MDC10010080S",null,"밸브보온/고무발포보온재","D80, 보온두께 25mm 이하, 각종부속부착, 옥내일반","개소",0,93407,0,93407,"합계"]
["MDC10010090S",null,"밸브보온/고무발포보온재","D100, 보온두께 25mm 이하, 각종부속부착, 옥내일반","개소",0,110714,0,110714,"합계"]
["MDC10010100S",null,"밸브보온/고무발포보온재","D125, 보온두께 25mm 이하, 각종부속부착, 옥내일반","개소",0,117015,0,117015,"합계"]
["MDC10010110S",null,"밸브보온/고무발포보온재","D150, 보온두께 25mm 이하, 각종부속부착, 옥내일반","개소",0,124081,0,124081,"합계"]
["MDC10010120S",null,"밸브보온/고무발포보온재","D200, 보온두께 25mm 이하, 각종부속부착, 옥내일반","개소",0,135295,0,135295,"합계"]
["MDC10010130S",null,"밸브보온/고무발포보온재","D250, 보온두께 25mm 이하, 각종부속부착, 옥내일반","개소",0,142568,0,142568,"합계"]
["MDC10010140S",null,"밸브보온/고무발포보온재","D300, 보온두께 25mm 이하, 각종부속부착, 옥내일반","개소",0,167148,0,167148,"합계"]
["MDC10110010S",null,"밸브보온/고무발포보온재","D15, 보온두께 50mm 이하, 각종부속부착, 옥내일반","개소",0,108002,0,108002,"합계"]
["MDC10110020S",null,"밸브보온/고무발포보온재","D20, 보온두께 50mm 이하, 각종부속부착, 옥내일반","개소",0,111432,0,111432,"합계"]
["MDC10110030S",null,"밸브보온/고무발포보온재","D25, 보온두께 50mm 이하, 각종부속부착, 옥내일반","개소",0,115069,0,115069,"합계"]
["MDC10110040S",null,"밸브보온/고무발포보온재","D32, 보온두께 50mm 이하, 각종부속부착, 옥내일반","개소",0,120189,0,120189,"합계"]
["MDC10110050S",null,"밸브보온/고무발포보온재","D40, 보온두께 50mm 이하, 각종부속부착, 옥내일반","개소",0,125772,0,125772,"합계"]
["MDC10110060S",null,"밸브보온/고무발포보온재","D50, 보온두께 50mm 이하, 각종부속부착, 옥내일반","개소",0,132838,0,132838,"합계"]
["MDC10110070S",null,"밸브보온/고무발포보온재","D65, 보온두께 50mm 이하, 각종부속부착, 옥내일반","개소",0,142568,0,142568,"합계"]
["MDC10110080S",null,"밸브보온/고무발포보온재","D80, 보온두께 50mm 이하, 각종부속부착, 옥내일반","개소",0,152554,0,152554,"합계"]
["MDC10110090S",null,"밸브보온/고무발포보온재","D100, 보온두께 50mm 이하, 각종부속부착, 옥내일반","개소",0,172014,0,172014,"합계"]
["MDC10110100S",null,"밸브보온/고무발포보온재","D125, 보온두께 50mm 이하, 각종부속부착, 옥내일반","개소",0,191729,0,191729,"합계"]
["MDC10110110S",null,"밸브보온/고무발포보온재","D150, 보온두께 50mm 이하, 각종부속부착, 옥내일반","개소",0,206579,0,206579,"합계"]
["MDC10110120S",null,"밸브보온/고무발포보온재","D200, 보온두께 50mm 이하, 각종부속부착, 옥내일반","개소",0,211444,0,211444,"합계"]
["MDC10110130S",null,"밸브보온/고무발포보온재","D250, 보온두께 50mm 이하, 각종부속부착, 옥내일반","개소",0,241097,0,241097,"합계"]
["MDC10110140S",null,"밸브보온/고무발포보온재","D300, 보온두께 50mm 이하, 각종부속부착, 옥내일반","개소",0,250826,0,250826,"합계"]
["MDC11010010S",null,"밸브보온/고무발포보온재","D15, 보온두께 25mm 이하, 각종부속부착, 기계실","개소",0,74492,0,74492,"합계"]
["MDC11010020S",null,"밸브보온/고무발포보온재","D20, 보온두께 25mm 이하, 각종부속부착, 기계실","개소",0,76750,0,76750,"합계"]
["MDC11010030S",null,"밸브보온/고무발포보온재","D25, 보온두께 25mm 이하, 각종부속부착, 기계실","개소",0,79303,0,79303,"합계"]
["MDC11010040S",null,"밸브보온/고무발포보온재","D32, 보온두께 25mm 이하, 각종부속부착, 기계실","개소",0,82689,0,82689,"합계"]
["MDC11010050S",null,"밸브보온/고무발포보온재","D40, 보온두께 25mm 이하, 각종부속부착, 기계실","개소",0,86372,0,86372,"합계"]
["MDC11010060S",null,"밸브보온/고무발포보온재","D50, 보온두께 25mm 이하, 각종부속부착, 기계실","개소",0,91422,0,91422,"합계"]
["MDC11010070S",null,"밸브보온/고무발포보온재","D65, 보온두께 25mm 이하, 각종부속부착, 기계실","개소",0,97066,0,97066,"합계"]
["MDC11010080S",null,"밸브보온/고무발포보온재","D80, 보온두께 25mm 이하, 각종부속부착, 기계실","개소",0,108353,0,108353,"합계"]
["MDC11010090S",null,"밸브보온/고무발포보온재","D100, 보온두께 25mm 이하, 각종부속부착, 기계실","개소",0,128429,0,128429,"합계"]
["MDC11010100S",null,"밸브보온/고무발포보온재","D125, 보온두께 25mm 이하, 각종부속부착, 기계실","개소",0,135737,0,135737,"합계"]
["MDC11010110S",null,"밸브보온/고무발포보온재","D150, 보온두께 25mm 이하, 각종부속부착, 기계실","개소",0,143934,0,143934,"합계"]
["MDC11010120S",null,"밸브보온/고무발포보온재","D200, 보온두께 25mm 이하, 각종부속부착, 기계실","개소",0,156942,0,156942,"합계"]
["MDC11010130S",null,"밸브보온/고무발포보온재","D250, 보온두께 25mm 이하, 각종부속부착, 기계실","개소",0,165379,0,165379,"합계"]
["MDC11010140S",null,"밸브보온/고무발포보온재","D300, 보온두께 25mm 이하, 각종부속부착, 기계실","개소",0,193892,0,193892,"합계"]
["MDC11110010S",null,"밸브보온/고무발포보온재","D15, 보온두께 50mm 이하, 각종부속부착, 기계실","개소",0,125283,0,125283,"합계"]
["MDC11110020S",null,"밸브보온/고무발포보온재","D20, 보온두께 50mm 이하, 각종부속부착, 기계실","개소",0,129261,0,129261,"합계"]
["MDC11110030S",null,"밸브보온/고무발포보온재","D25, 보온두께 50mm 이하, 각종부속부착, 기계실","개소",0,133480,0,133480,"합계"]
["MDC11110040S",null,"밸브보온/고무발포보온재","D32, 보온두께 50mm 이하, 각종부속부착, 기계실","개소",0,139419,0,139419,"합계"]
["MDC11110050S",null,"밸브보온/고무발포보온재","D40, 보온두께 50mm 이하, 각종부속부착, 기계실","개소",0,145895,0,145895,"합계"]
["MDC11110060S",null,"밸브보온/고무발포보온재","D50, 보온두께 50mm 이하, 각종부속부착, 기계실","개소",0,154092,0,154092,"합계"]
["MDC11110070S",null,"밸브보온/고무발포보온재","D65, 보온두께 50mm 이하, 각종부속부착, 기계실","개소",0,165379,0,165379,"합계"]
["MDC11110080S",null,"밸브보온/고무발포보온재","D80, 보온두께 50mm 이하, 각종부속부착, 기계실","개소",0,176962,0,176962,"합계"]
["MDC11110090S",null,"밸브보온/고무발포보온재","D100, 보온두께 50mm 이하, 각종부속부착, 기계실","개소",0,199536,0,199536,"합계"]
["MDC11110100S",null,"밸브보온/고무발포보온재","D125, 보온두께 50mm 이하, 각종부속부착, 기계실","개소",0,222406,0,222406,"합계"]
["MDC11110110S",null,"밸브보온/고무발포보온재","D150, 보온두께 50mm 이하, 각종부속부착, 기계실","개소",0,239632,0,239632,"합계"]
["MDC11110120S",null,"밸브보온/고무발포보온재","D200, 보온두께 50mm 이하, 각종부속부착, 기계실","개소",0,245275,0,245275,"합계"]
["MDC11110130S",null,"밸브보온/고무발포보온재","D250, 보온두께 50mm 이하, 각종부속부착, 기계실","개소",0,279672,0,279672,"합계"]
["MDC11110140S",null,"밸브보온/고무발포보온재","D300, 보온두께 50mm 이하, 각종부속부착, 기계실","개소",0,290959,0,290959,"합계"]
["MDC20010010S",null,"밸브보온/발포폴리에틸렌보온재","D15, 보온두께 25mm 이하, 일반밸브, 옥내일반","개소",0,38550,0,38550,"합계"]
["MDC20010020S",null,"밸브보온/발포폴리에틸렌보온재","D20, 보온두께 25mm 이하, 일반밸브, 옥내일반","개소",0,39698,0,39698,"합계"]
["MDC20010030S",null,"밸브보온/발포폴리에틸렌보온재","D25, 보온두께 25mm 이하, 일반밸브, 옥내일반","개소",0,40885,0,40885,"합계"]
["MDC20010040S",null,"밸브보온/발포폴리에틸렌보온재","D32, 보온두께 25mm 이하, 일반밸브, 옥내일반","개소",0,42811,0,42811,"합계"]
["MDC20010050S",null,"밸브보온/발포폴리에틸렌보온재","D40, 보온두께 25mm 이하, 일반밸브, 옥내일반","개소",0,44777,0,44777,"합계"]
["MDC20010060S",null,"밸브보온/발포폴리에틸렌보온재","D50, 보온두께 25mm 이하, 일반밸브, 옥내일반","개소",0,47482,0,47482,"합계"]
["MDC20010070S",null,"밸브보온/발포폴리에틸렌보온재","D65, 보온두께 25mm 이하, 일반밸브, 옥내일반","개소",0,50226,0,50226,"합계"]
["MDC20010080S",null,"밸브보온/발포폴리에틸렌보온재","D80, 보온두께 25mm 이하, 일반밸브, 옥내일반","개소",0,56249,0,56249,"합계"]
["MDC20010090S",null,"밸브보온/발포폴리에틸렌보온재","D100, 보온두께 25mm 이하, 일반밸브, 옥내일반","개소",0,66572,0,66572,"합계"]
["MDC20010100S",null,"밸브보온/발포폴리에틸렌보온재","D125, 보온두께 25mm 이하, 일반밸브, 옥내일반","개소",0,70260,0,70260,"합계"]
["MDC20010110S",null,"밸브보온/발포폴리에틸렌보온재","D150, 보온두께 25mm 이하, 일반밸브, 옥내일반","개소",0,74726,0,74726,"합계"]
["MDC20010120S",null,"밸브보온/발포폴리에틸렌보온재","D200, 보온두께 25mm 이하, 일반밸브, 옥내일반","개소",0,81362,0,81362,"합계"]
["MDC20010130S",null,"밸브보온/발포폴리에틸렌보온재","D250, 보온두께 25mm 이하, 일반밸브, 옥내일반","개소",0,85828,0,85828,"합계"]
["MDC20010140S",null,"밸브보온/발포폴리에틸렌보온재","D300, 보온두께 25mm 이하, 일반밸브, 옥내일반","개소",0,100617,0,100617,"합계"]
["MDC20110010S",null,"밸브보온/발포폴리에틸렌보온재","D15, 보온두께 50mm 이하, 일반밸브, 옥내일반","개소",0,65015,0,65015,"합계"]
["MDC20110020S",null,"밸브보온/발포폴리에틸렌보온재","D20, 보온두께 50mm 이하, 일반밸브, 옥내일반","개소",0,67146,0,67146,"합계"]
["MDC20110030S",null,"밸브보온/발포폴리에틸렌보온재","D25, 보온두께 50mm 이하, 일반밸브, 옥내일반","개소",0,69277,0,69277,"합계"]
["MDC20110040S",null,"밸브보온/발포폴리에틸렌보온재","D32, 보온두께 50mm 이하, 일반밸브, 옥내일반","개소",0,72225,0,72225,"합계"]
["MDC20110050S",null,"밸브보온/발포폴리에틸렌보온재","D40, 보온두께 50mm 이하, 일반밸브, 옥내일반","개소",0,75709,0,75709,"합계"]
["MDC20110060S",null,"밸브보온/발포폴리에틸렌보온재","D50, 보온두께 50mm 이하, 일반밸브, 옥내일반","개소",0,79805,0,79805,"합계"]
["MDC20110070S",null,"밸브보온/발포폴리에틸렌보온재","D65, 보온두께 50mm 이하, 일반밸브, 옥내일반","개소",0,85828,0,85828,"합계"]
["MDC20110080S",null,"밸브보온/발포폴리에틸렌보온재","D80, 보온두께 50mm 이하, 일반밸브, 옥내일반","개소",0,91685,0,91685,"합계"]
["MDC20110090S",null,"밸브보온/발포폴리에틸렌보온재","D100, 보온두께 50mm 이하, 일반밸브, 옥내일반","개소",0,103565,0,103565,"합계"]
["MDC20110100S",null,"밸브보온/발포폴리에틸렌보온재","D125, 보온두께 50mm 이하, 일반밸브, 옥내일반","개소",0,115407,0,115407,"합계"]
["MDC20110110S",null,"밸브보온/발포폴리에틸렌보온재","D150, 보온두께 50mm 이하, 일반밸브, 옥내일반","개소",0,124174,0,124174,"합계"]
["MDC20110120S",null,"밸브보온/발포폴리에틸렌보온재","D200, 보온두께 50mm 이하, 일반밸브, 옥내일반","개소",0,127287,0,127287,"합계"]
["MDC20110130S",null,"밸브보온/발포폴리에틸렌보온재","D250, 보온두께 50mm 이하, 일반밸브, 옥내일반","개소",0,144821,0,144821,"합계"]
["MDC20110140S",null,"밸브보온/발포폴리에틸렌보온재","D300, 보온두께 50mm 이하, 일반밸브, 옥내일반","개소",0,150843,0,150843,"합계"]
["MDC21010010S",null,"밸브보온/발포폴리에틸렌보온재","D15, 보온두께 25mm 이하, 일반밸브, 기계실","개소",0,46260,0,46260,"합계"]
["MDC21010020S",null,"밸브보온/발포폴리에틸렌보온재","D20, 보온두께 25mm 이하, 일반밸브, 기계실","개소",0,47637,0,47637,"합계"]
["MDC21010030S",null,"밸브보온/발포폴리에틸렌보온재","D25, 보온두께 25mm 이하, 일반밸브, 기계실","개소",0,49062,0,49062,"합계"]
["MDC21010040S",null,"밸브보온/발포폴리에틸렌보온재","D32, 보온두께 25mm 이하, 일반밸브, 기계실","개소",0,51374,0,51374,"합계"]
["MDC21010050S",null,"밸브보온/발포폴리에틸렌보온재","D40, 보온두께 25mm 이하, 일반밸브, 기계실","개소",0,53732,0,53732,"합계"]
["MDC21010060S",null,"밸브보온/발포폴리에틸렌보온재","D50, 보온두께 25mm 이하, 일반밸브, 기계실","개소",0,56978,0,56978,"합계"]
["MDC21010070S",null,"밸브보온/발포폴리에틸렌보온재","D65, 보온두께 25mm 이하, 일반밸브, 기계실","개소",0,60271,0,60271,"합계"]
["MDC21010080S",null,"밸브보온/발포폴리에틸렌보온재","D80, 보온두께 25mm 이하, 일반밸브, 기계실","개소",0,67498,0,67498,"합계"]
["MDC21010090S",null,"밸브보온/발포폴리에틸렌보온재","D100, 보온두께 25mm 이하, 일반밸브, 기계실","개소",0,79887,0,79887,"합계"]
["MDC21010100S",null,"밸브보온/발포폴리에틸렌보온재","D125, 보온두께 25mm 이하, 일반밸브, 기계실","개소",0,84312,0,84312,"합계"]
["MDC21010110S",null,"밸브보온/발포폴리에틸렌보온재","D150, 보온두께 25mm 이하, 일반밸브, 기계실","개소",0,89671,0,89671,"합계"]
["MDC21010120S",null,"밸브보온/발포폴리에틸렌보온재","D200, 보온두께 25mm 이하, 일반밸브, 기계실","개소",0,97634,0,97634,"합계"]
["MDC21010130S",null,"밸브보온/발포폴리에틸렌보온재","D250, 보온두께 25mm 이하, 일반밸브, 기계실","개소",0,102993,0,102993,"합계"]
["MDC21010140S",null,"밸브보온/발포폴리에틸렌보온재","D300, 보온두께 25mm 이하, 일반밸브, 기계실","개소",0,120741,0,120741,"합계"]
["MDC21110010S",null,"밸브보온/발포폴리에틸렌보온재","D15, 보온두께 50mm 이하, 일반밸브, 기계실","개소",0,78018,0,78018,"합계"]
["MDC21110020S",null,"밸브보온/발포폴리에틸렌보온재","D20, 보온두께 50mm 이하, 일반밸브, 기계실","개소",0,80575,0,80575,"합계"]
["MDC21110030S",null,"밸브보온/발포폴리에틸렌보온재","D25, 보온두께 50mm 이하, 일반밸브, 기계실","개소",0,83133,0,83133,"합계"]
["MDC21110040S",null,"밸브보온/발포폴리에틸렌보온재","D32, 보온두께 50mm 이하, 일반밸브, 기계실","개소",0,86670,0,86670,"합계"]
["MDC21110050S",null,"밸브보온/발포폴리에틸렌보온재","D40, 보온두께 50mm 이하, 일반밸브, 기계실","개소",0,90850,0,90850,"합계"]
["MDC21110060S",null,"밸브보온/발포폴리에틸렌보온재","D50, 보온두께 50mm 이하, 일반밸브, 기계실","개소",0,95766,0,95766,"합계"]
["MDC21110070S",null,"밸브보온/발포폴리에틸렌보온재","D65, 보온두께 50mm 이하, 일반밸브, 기계실","개소",0,102993,0,102993,"합계"]
["MDC21110080S",null,"밸브보온/발포폴리에틸렌보온재","D80, 보온두께 50mm 이하, 일반밸브, 기계실","개소",0,110022,0,110022,"합계"]
["MDC21110090S",null,"밸브보온/발포폴리에틸렌보온재","D100, 보온두께 50mm 이하, 일반밸브, 기계실","개소",0,124279,0,124279,"합계"]
["MDC21110100S",null,"밸브보온/발포폴리에틸렌보온재","D125, 보온두께 50mm 이하, 일반밸브, 기계실","개소",0,138488,0,138488,"합계"]
["MDC21110110S",null,"밸브보온/발포폴리에틸렌보온재","D150, 보온두께 50mm 이하, 일반밸브, 기계실","개소",0,149008,0,149008,"합계"]
["MDC21110120S",null,"밸브보온/발포폴리에틸렌보온재","D200, 보온두께 50mm 이하, 일반밸브, 기계실","개소",0,152745,0,152745,"합계"]
["MDC21110130S",null,"밸브보온/발포폴리에틸렌보온재","D250, 보온두께 50mm 이하, 일반밸브, 기계실","개소",0,173785,0,173785,"합계"]
["MDC21110140S",null,"밸브보온/발포폴리에틸렌보온재","D300, 보온두께 50mm 이하, 일반밸브, 기계실","개소",0,181012,0,181012,"합계"]
["MDC30010010S",null,"밸브보온/발포폴리에틸렌보온재","D15, 보온두께 25mm 이하, 각종부속부착, 옥내일반","개소",0,48187,0,48187,"합계"]
["MDC30010020S",null,"밸브보온/발포폴리에틸렌보온재","D20, 보온두께 25mm 이하, 각종부속부착, 옥내일반","개소",0,49622,0,49622,"합계"]
["MDC30010030S",null,"밸브보온/발포폴리에틸렌보온재","D25, 보온두께 25mm 이하, 각종부속부착, 옥내일반","개소",0,51106,0,51106,"합계"]
["MDC30010040S",null,"밸브보온/발포폴리에틸렌보온재","D32, 보온두께 25mm 이하, 각종부속부착, 옥내일반","개소",0,53514,0,53514,"합계"]
["MDC30010050S",null,"밸브보온/발포폴리에틸렌보온재","D40, 보온두께 25mm 이하, 각종부속부착, 옥내일반","개소",0,55971,0,55971,"합계"]
["MDC30010060S",null,"밸브보온/발포폴리에틸렌보온재","D50, 보온두께 25mm 이하, 각종부속부착, 옥내일반","개소",0,59352,0,59352,"합계"]
["MDC30010070S",null,"밸브보온/발포폴리에틸렌보온재","D65, 보온두께 25mm 이하, 각종부속부착, 옥내일반","개소",0,62782,0,62782,"합계"]
["MDC30010080S",null,"밸브보온/발포폴리에틸렌보온재","D80, 보온두께 25mm 이하, 각종부속부착, 옥내일반","개소",0,70311,0,70311,"합계"]
["MDC30010090S",null,"밸브보온/발포폴리에틸렌보온재","D100, 보온두께 25mm 이하, 각종부속부착, 옥내일반","개소",0,83215,0,83215,"합계"]
["MDC30010100S",null,"밸브보온/발포폴리에틸렌보온재","D125, 보온두께 25mm 이하, 각종부속부착, 옥내일반","개소",0,87825,0,87825,"합계"]
["MDC30010110S",null,"밸브보온/발포폴리에틸렌보온재","D150, 보온두께 25mm 이하, 각종부속부착, 옥내일반","개소",0,93407,0,93407,"합계"]
["MDC30010120S",null,"밸브보온/발포폴리에틸렌보온재","D200, 보온두께 25mm 이하, 각종부속부착, 옥내일반","개소",0,101702,0,101702,"합계"]
["MDC30010130S",null,"밸브보온/발포폴리에틸렌보온재","D250, 보온두께 25mm 이하, 각종부속부착, 옥내일반","개소",0,107285,0,107285,"합계"]
["MDC30010140S",null,"밸브보온/발포폴리에틸렌보온재","D300, 보온두께 25mm 이하, 각종부속부착, 옥내일반","개소",0,125772,0,125772,"합계"]
["MDC30110010S",null,"밸브보온/발포폴리에틸렌보온재","D15, 보온두께 50mm 이하, 각종부속부착, 옥내일반","개소",0,81269,0,81269,"합계"]
["MDC30110020S",null,"밸브보온/발포폴리에틸렌보온재","D20, 보온두께 50mm 이하, 각종부속부착, 옥내일반","개소",0,83933,0,83933,"합계"]
["MDC30110030S",null,"밸브보온/발포폴리에틸렌보온재","D25, 보온두께 50mm 이하, 각종부속부착, 옥내일반","개소",0,86596,0,86596,"합계"]
["MDC30110040S",null,"밸브보온/발포폴리에틸렌보온재","D32, 보온두께 50mm 이하, 각종부속부착, 옥내일반","개소",0,90282,0,90282,"합계"]
["MDC30110050S",null,"밸브보온/발포폴리에틸렌보온재","D40, 보온두께 50mm 이하, 각종부속부착, 옥내일반","개소",0,94636,0,94636,"합계"]
["MDC30110060S",null,"밸브보온/발포폴리에틸렌보온재","D50, 보온두께 50mm 이하, 각종부속부착, 옥내일반","개소",0,99756,0,99756,"합계"]
["MDC30110070S",null,"밸브보온/발포폴리에틸렌보온재","D65, 보온두께 50mm 이하, 각종부속부착, 옥내일반","개소",0,107285,0,107285,"합계"]
["MDC30110080S",null,"밸브보온/발포폴리에틸렌보온재","D80, 보온두께 50mm 이하, 각종부속부착, 옥내일반","개소",0,114606,0,114606,"합계"]
["MDC30110090S",null,"밸브보온/발포폴리에틸렌보온재","D100, 보온두께 50mm 이하, 각종부속부착, 옥내일반","개소",0,129457,0,129457,"합계"]
["MDC30110100S",null,"밸브보온/발포폴리에틸렌보온재","D125, 보온두께 50mm 이하, 각종부속부착, 옥내일반","개소",0,144259,0,144259,"합계"]
["MDC30110110S",null,"밸브보온/발포폴리에틸렌보온재","D150, 보온두께 50mm 이하, 각종부속부착, 옥내일반","개소",0,155217,0,155217,"합계"]
["MDC30110120S",null,"밸브보온/발포폴리에틸렌보온재","D200, 보온두께 50mm 이하, 각종부속부착, 옥내일반","개소",0,159109,0,159109,"합계"]
["MDC30110130S",null,"밸브보온/발포폴리에틸렌보온재","D250, 보온두께 50mm 이하, 각종부속부착, 옥내일반","개소",0,181026,0,181026,"합계"]
["MDC30110140S",null,"밸브보온/발포폴리에틸렌보온재","D300, 보온두께 50mm 이하, 각종부속부착, 옥내일반","개소",0,188554,0,188554,"합계"]
["MDC31010010S",null,"밸브보온/발포폴리에틸렌보온재","D15, 보온두께 25mm 이하, 각종부속부착, 기계실","개소",0,55897,0,55897,"합계"]
["MDC31010020S",null,"밸브보온/발포폴리에틸렌보온재","D20, 보온두께 25mm 이하, 각종부속부착, 기계실","개소",0,57562,0,57562,"합계"]
["MDC31010030S",null,"밸브보온/발포폴리에틸렌보온재","D25, 보온두께 25mm 이하, 각종부속부착, 기계실","개소",0,59283,0,59283,"합계"]
["MDC31010040S",null,"밸브보온/발포폴리에틸렌보온재","D32, 보온두께 25mm 이하, 각종부속부착, 기계실","개소",0,62077,0,62077,"합계"]
["MDC31010050S",null,"밸브보온/발포폴리에틸렌보온재","D40, 보온두께 25mm 이하, 각종부속부착, 기계실","개소",0,64927,0,64927,"합계"]
["MDC31010060S",null,"밸브보온/발포폴리에틸렌보온재","D50, 보온두께 25mm 이하, 각종부속부착, 기계실","개소",0,68849,0,68849,"합계"]
["MDC31010070S",null,"밸브보온/발포폴리에틸렌보온재","D65, 보온두께 25mm 이하, 각종부속부착, 기계실","개소",0,72827,0,72827,"합계"]
["MDC31010080S",null,"밸브보온/발포폴리에틸렌보온재","D80, 보온두께 25mm 이하, 각종부속부착, 기계실","개소",0,81561,0,81561,"합계"]
["MDC31010090S",null,"밸브보온/발포폴리에틸렌보온재","D100, 보온두께 25mm 이하, 각종부속부착, 기계실","개소",0,96530,0,96530,"합계"]
["MDC31010100S",null,"밸브보온/발포폴리에틸렌보온재","D125, 보온두께 25mm 이하, 각종부속부착, 기계실","개소",0,101877,0,101877,"합계"]
["MDC31010110S",null,"밸브보온/발포폴리에틸렌보온재","D150, 보온두께 25mm 이하, 각종부속부착, 기계실","개소",0,108353,0,108353,"합계"]
["MDC31010120S",null,"밸브보온/발포폴리에틸렌보온재","D200, 보온두께 25mm 이하, 각종부속부착, 기계실","개소",0,117974,0,117974,"합계"]
["MDC31010130S",null,"밸브보온/발포폴리에틸렌보온재","D250, 보온두께 25mm 이하, 각종부속부착, 기계실","개소",0,124450,0,124450,"합계"]
["MDC31010140S",null,"밸브보온/발포폴리에틸렌보온재","D300, 보온두께 25mm 이하, 각종부속부착, 기계실","개소",0,145895,0,145895,"합계"]
["MDC31110010S",null,"밸브보온/발포폴리에틸렌보온재","D15, 보온두께 50mm 이하, 각종부속부착, 기계실","개소",0,94272,0,94272,"합계"]
["MDC31110020S",null,"밸브보온/발포폴리에틸렌보온재","D20, 보온두께 50mm 이하, 각종부속부착, 기계실","개소",0,97362,0,97362,"합계"]
["MDC31110030S",null,"밸브보온/발포폴리에틸렌보온재","D25, 보온두께 50mm 이하, 각종부속부착, 기계실","개소",0,100452,0,100452,"합계"]
["MDC31110040S",null,"밸브보온/발포폴리에틸렌보온재","D32, 보온두께 50mm 이하, 각종부속부착, 기계실","개소",0,104727,0,104727,"합계"]
["MDC31110050S",null,"밸브보온/발포폴리에틸렌보온재","D40, 보온두께 50mm 이하, 각종부속부착, 기계실","개소",0,109778,0,109778,"합계"]
["MDC31110060S",null,"밸브보온/발포폴리에틸렌보온재","D50, 보온두께 50mm 이하, 각종부속부착, 기계실","개소",0,115717,0,115717,"합계"]
["MDC31110070S",null,"밸브보온/발포폴리에틸렌보온재","D65, 보온두께 50mm 이하, 각종부속부착, 기계실","개소",0,124450,0,124450,"합계"]
["MDC31110080S",null,"밸브보온/발포폴리에틸렌보온재","D80, 보온두께 50mm 이하, 각종부속부착, 기계실","개소",0,132943,0,132943,"합계"]
["MDC31110090S",null,"밸브보온/발포폴리에틸렌보온재","D100, 보온두께 50mm 이하, 각종부속부착, 기계실","개소",0,150170,0,150170,"합계"]
["MDC31110100S",null,"밸브보온/발포폴리에틸렌보온재","D125, 보온두께 50mm 이하, 각종부속부착, 기계실","개소",0,167340,0,167340,"합계"]
["MDC31110110S",null,"밸브보온/발포폴리에틸렌보온재","D150, 보온두께 50mm 이하, 각종부속부착, 기계실","개소",0,180052,0,180052,"합계"]
["MDC31110120S",null,"밸브보온/발포폴리에틸렌보온재","D200, 보온두께 50mm 이하, 각종부속부착, 기계실","개소",0,184567,0,184567,"합계"]
["MDC31110130S",null,"밸브보온/발포폴리에틸렌보온재","D250, 보온두께 50mm 이하, 각종부속부착, 기계실","개소",0,209990,0,209990,"합계"]
["MDC31110140S",null,"밸브보온/발포폴리에틸렌보온재","D300, 보온두께 50mm 이하, 각종부속부착, 기계실","개소",0,218723,0,218723,"합계"]
["MDC40010010S",null,"밸브보온/함석마감","D50 이하","개소",0,47545,0,47545,"합계"]
["MDC40010020S",null,"밸브보온/함석마감","D65","개소",0,53149,0,53149,"합계"]
["MDC40010030S",null,"밸브보온/함석마감","D80","개소",0,58714,0,58714,"합계"]
["MDC40010040S",null,"밸브보온/함석마감","D100","개소",0,66449,0,66449,"합계"]
["MDC40010050S",null,"밸브보온/함석마감","D125","개소",0,75818,0,75818,"합계"]
["MDC40010060S",null,"밸브보온/함석마감","D150","개소",0,85187,0,85187,"합계"]
["MDC40010070S",null,"밸브보온/함석마감","D200","개소",0,104090,0,104090,"합계"]
["MDC40010080S",null,"밸브보온/함석마감","D250","개소",0,122993,0,122993,"합계"]
["MDC40010090S",null,"밸브보온/함석마감","D300","개소",0,141897,0,141897,"합계"]
["MDE00000000S",null,"각형덕트 보온","보온재 재질 및 두께에 따른 시공량(㎡) 참조","인/일",0,574115,0,574115,"합계"]
["MDE00010010S",null,"각형덕트보온/고무발포보온재","보온두께 25mm 이하","㎡",0,61109,0,61109,"합계"]
["MDE00110010S",null,"각형덕트보온/고무발포보온재","보온두께 50mm 이하","㎡",0,68893,0,68893,"합계"]
["MDE01010010S",null,"각형덕트보온/발포폴리에틸렌","보온두께 25mm 이하","㎡",0,61109,0,61109,"합계"]
["MDE01110010S",null,"각형덕트보온/발포폴리에틸렌","보온두께 50mm 이하","㎡",0,68893,0,68893,"합계"]
["MDE02010010S",null,"각형덕트보온/유리솜보온재","보온두께 25mm 이하","㎡",0,72592,0,72592,"합계"]
["MDE02110010S",null,"각형덕트보온/유리솜보온재","보온두께 50mm 이하","㎡",0,82418,0,82418,"합계"]
["MDE10000000S",null,"원형덕트 보온","보온재 재질 및 두께에 따른 시공량(㎡) 참조","인/일",0,574115,0,574115,"합계"]
["MDE10010010S",null,"원형덕트보온/고무발포보온재","보온두께 25mm 이하","㎡",0,61109,0,61109,"합계"]
["MDE10110010S",null,"원형덕트보온/고무발포보온재","보온두께 50mm 이하","㎡",0,68893,0,68893,"합계"]
["MDE11010010S",null,"원형덕트보온/발포폴리에틸렌","보온두께 25mm 이하","㎡",0,61109,0,61109,"합계"]
["MDE11110010S",null,"원형덕트보온/발포폴리에틸렌","보온두께 50mm 이하","㎡",0,68893,0,68893,"합계"]
["MDE12010010S",null,"원형덕트보온/유리솜보온재","보온두께 25mm 이하","㎡",0,72592,0,72592,"합계"]
["MDE12110010S",null,"원형덕트보온/유리솜보온재","보온두께 50mm 이하","㎡",0,82418,0,82418,"합계"]
["MDG00010010S",null,"발열선 설치","세대내","m",0,3505,0,3505,"합계"]
["MDG00110010S",null,"발열선 설치","공용부위","m",0,4966,0,4966,"합계"]
["MDG10010010S",null,"분전함 설치","분전함(제어부)","개소",0,85687,0,85687,"합계"]
["MEA00010010S",null,"일반펌프 설치","0.75 kw 이하","대",6632,221079,0,227711,"합계"]
["MEA00010020S",null,"일반펌프 설치","1.5 kw 이하","대",7341,244714,0,252055,"합계"]
["MEA00010030S",null,"일반펌프 설치","2.2 kw 이하","대",8459,281982,0,290441,"합계"]
["MEA00010040S",null,"일반펌프 설치","3.7 kw 이하","대",9714,323818,0,333532,"합계"]
["MEA00010050S",null,"일반펌프 설치","5.5 kw 이하","대",11704,390156,0,401860,"합계"]
["MEA00010060S",null,"일반펌프 설치","7.5 kw 이하","대",14767,492262,0,507029,"합계"]
["MEA00010070S",null,"일반펌프 설치","11 kw 이하","대",18559,618636,0,637195,"합계"]
["MEA00010080S",null,"일반펌프 설치","15 kw 이하","대",19703,656772,0,676475,"합계"]
["MEA00010090S",null,"일반펌프 설치","22 kw 이하","대",31830,1061029,0,1092859,"합계"]
["MEA00010100S",null,"일반펌프 설치","37 kw 이하","대",41098,1369948,0,1411046,"합계"]
["MEA00010110S",null,"일반펌프 설치","55 kw 이하","대",66119,2203997,0,2270116,"합계"]
["MEA00010120S",null,"일반펌프 설치","75 kw 이하","대",80998,2699960,0,2780958,"합계"]
["MEA10010010S",null,"배수펌프 설치","0.75 kw 이하","대",11629,387653,0,399282,"합계"]
["MEA10010020S",null,"배수펌프 설치","1.5 kw 이하","대",13150,438350,0,451500,"합계"]
["MEA10010030S",null,"배수펌프 설치","2.2 kw 이하","대",14569,485650,0,500219,"합계"]
["MEA10010040S",null,"배수펌프 설치","3.7 kw 이하","대",17599,586646,0,604245,"합계"]
["MEA10010050S",null,"배수펌프 설치","5.5 kw 이하","대",21244,708141,0,729385,"합계"]
["MEA10010060S",null,"배수펌프 설치","7.5 kw 이하","대",25291,843036,0,868327,"합계"]
["MEA20010010S",null,"펌프 방진가대 설치","0.75 kw 이하","대",0,186187,0,186187,"합계"]
["MEA20010020S",null,"펌프 방진가대 설치","1.5 kw 이하","대",0,193354,0,193354,"합계"]
["MEA20010030S",null,"펌프 방진가대 설치","2.2 kw 이하","대",0,204855,0,204855,"합계"]
["MEA20010040S",null,"펌프 방진가대 설치","3.7 kw 이하","대",0,217456,0,217456,"합계"]
["MEA20010050S",null,"펌프 방진가대 설치","5.5 kw 이하","대",0,237858,0,237858,"합계"]
["MEA20010060S",null,"펌프 방진가대 설치","7.5 kw 이하","대",0,255261,0,255261,"합계"]
["MEA20010070S",null,"펌프 방진가대 설치","11 kw 이하","대",0,282830,0,282830,"합계"]
["MEA20010080S",null,"펌프 방진가대 설치","15 kw 이하","대",0,292597,0,292597,"합계"]
["MEA20010090S",null,"펌프 방진가대 설치","22 kw 이하","대",0,386475,0,386475,"합계"]
["MEA20010100S",null,"펌프 방진가대 설치","37 kw 이하","대",0,448615,0,448615,"합계"]
["MEA20010110S",null,"펌프 방진가대 설치","55 kw 이하","대",0,569594,0,569594,"합계"]
["MEA20010120S",null,"펌프 방진가대 설치","75 kw 이하","대",0,681274,0,681274,"합계"]
["MEB00010010S",null,"송풍기 설치","호칭번호 032(#2), 편흡입","대",8840,294691,0,303531,"합계"]
["MEB00010020S",null,"송풍기 설치","호칭번호 036(#2⅓), 편흡입","대",9428,314294,0,323722,"합계"]
["MEB00010030S",null,"송풍기 설치","호칭번호 040(#2⅔), 편흡입","대",10182,339400,0,349582,"합계"]
["MEB00010040S",null,"송풍기 설치","호칭번호 045(#3), 편흡입","대",11143,371439,0,382582,"합계"]
["MEB00010050S",null,"송풍기 설치","호칭번호 050(#3⅓), 편흡입","대",12222,407412,0,419634,"합계"]
["MEB00010060S",null,"송풍기 설치","호칭번호 056(#3⅔), 편흡입","대",13688,456289,0,469977,"합계"]
["MEB00010070S",null,"송풍기 설치","호칭번호 063(#4), 편흡입","대",15639,521302,0,536941,"합계"]
["MEB00010080S",null,"송풍기 설치","호칭번호 071(#4⅔), 편흡입","대",18177,605919,0,624096,"합계"]
["MEB00010090S",null,"송풍기 설치","호칭번호 080(#5⅓), 편흡입","대",21436,714540,0,735976,"합계"]
["MEB00010100S",null,"송풍기 설치","호칭번호 090(#6), 편흡입","대",25578,852600,0,878178,"합계"]
["MEB00010110S",null,"송풍기 설치","호칭번호 100(#6⅔), 편흡입","대",30255,1008531,0,1038786,"합계"]
["MEB00010120S",null,"송풍기 설치","호칭번호 112(#7½), 편흡입","대",35445,1181532,0,1216977,"합계"]
["MEB00010130S",null,"송풍기 설치","호칭번호 125(#8⅓), 편흡입","대",39089,1302989,0,1342078,"합계"]
["MEB00010140S",null,"송풍기 설치","호칭번호 140(#9⅓), 편흡입","대",43833,1461120,0,1504953,"합계"]
["MEB00010150S",null,"송풍기 설치","호칭번호 160(#10⅔), 편흡입","대",57371,1912375,0,1969746,"합계"]
["MEB00010160S",null,"송풍기 설치","호칭번호 180(#12), 편흡입","대",65191,2173060,0,2238251,"합계"]
["MEB00110010S",null,"송풍기 설치","호칭번호 032(#2), 양흡입","대",11686,389543,0,401229,"합계"]
["MEB00110020S",null,"송풍기 설치","호칭번호 036(#2⅓), 양흡입","대",12465,415515,0,427980,"합계"]
["MEB00110030S",null,"송풍기 설치","호칭번호 040(#2⅔), 양흡입","대",13459,448654,0,462113,"합계"]
["MEB00110040S",null,"송풍기 설치","호칭번호 045(#3), 양흡입","대",14722,490763,0,505485,"합계"]
["MEB00110050S",null,"송풍기 설치","호칭번호 050(#3⅓), 양흡입","대",16149,538305,0,554454,"합계"]
["MEB00110060S",null,"송풍기 설치","호칭번호 056(#3⅔), 양흡입","대",18092,603085,0,621177,"합계"]
["MEB00110070S",null,"송풍기 설치","호칭번호 063(#4), 양흡입","대",20664,688802,0,709466,"합계"]
["MEB00110080S",null,"송풍기 설치","호칭번호 071(#4⅔), 양흡입","대",24014,800491,0,824505,"합계"]
["MEB00110090S",null,"송풍기 설치","호칭번호 080(#5⅓), 양흡입","대",28326,944219,0,972545,"합계"]
["MEB00110100S",null,"송풍기 설치","호칭번호 090(#6), 양흡입","대",33795,1126520,0,1160315,"합계"]
["MEB00110110S",null,"송풍기 설치","호칭번호 100(#6⅔), 양흡입","대",39979,1332661,0,1372640,"합계"]
["MEB00110120S",null,"송풍기 설치","호칭번호 112(#7½), 양흡입","대",46837,1561239,0,1608076,"합계"]
["MEB00110130S",null,"송풍기 설치","호칭번호 125(#8⅓), 양흡입","대",51647,1721571,0,1773218,"합계"]
["MEB00110140S",null,"송풍기 설치","호칭번호 140(#9⅓), 양흡입","대",57914,1930478,0,1988392,"합계"]
["MEB00110150S",null,"송풍기 설치","호칭번호 160(#10⅔), 양흡입","대",75810,2527029,0,2602839,"합계"]
["MEB00110160S",null,"송풍기 설치","호칭번호 180(#12), 양흡입","대",86136,2871230,0,2957366,"합계"]
["MEB01010010S",null,"송풍기 설치","호칭번호 032(#2), 편흡입, 천장행거형","대",8840,500975,0,509815,"합계"]
["MEB01010020S",null,"송풍기 설치","호칭번호 036(#2⅓), 편흡입, 천장행거형","대",9428,534301,0,543729,"합계"]
["MEB01010030S",null,"송풍기 설치","호칭번호 040(#2⅔), 편흡입, 천장행거형","대",10182,576980,0,587162,"합계"]
["MEB01010040S",null,"송풍기 설치","호칭번호 045(#3), 편흡입, 천장행거형","대",11143,631446,0,642589,"합계"]
["MEB01010050S",null,"송풍기 설치","호칭번호 050(#3⅓), 편흡입, 천장행거형","대",12222,692601,0,704823,"합계"]
["MEB01010060S",null,"송풍기 설치","호칭번호 056(#3⅔), 편흡입, 천장행거형","대",13688,775692,0,789380,"합계"]
["MEB01010070S",null,"송풍기 설치","호칭번호 063(#4), 편흡입, 천장행거형","대",15639,886214,0,901853,"합계"]
["MEB01010080S",null,"송풍기 설치","호칭번호 071(#4⅔), 편흡입, 천장행거형","대",18177,1030062,0,1048239,"합계"]
["MEB01010090S",null,"송풍기 설치","호칭번호 080(#5⅓), 편흡입, 천장행거형","대",21436,1214718,0,1236154,"합계"]
["MEB01010100S",null,"송풍기 설치","호칭번호 090(#6), 편흡입, 천장행거형","대",25578,1449421,0,1474999,"합계"]
["MEB01010110S",null,"송풍기 설치","호칭번호 100(#6⅔), 편흡입, 천장행거형","대",30255,1714502,0,1744757,"합계"]
["MEB01010120S",null,"송풍기 설치","호칭번호 112(#7½), 편흡입, 천장행거형","대",35445,2008605,0,2044050,"합계"]
["MEB01010130S",null,"송풍기 설치","호칭번호 125(#8⅓), 편흡입, 천장행거형","대",39089,2215081,0,2254170,"합계"]
["MEB01010140S",null,"송풍기 설치","호칭번호 140(#9⅓), 편흡입, 천장행거형","대",43833,2483904,0,2527737,"합계"]
["MEB01010150S",null,"송풍기 설치","호칭번호 160(#10⅔), 편흡입, 천장행거형","대",57371,3251037,0,3308408,"합계"]
["MEB01010160S",null,"송풍기 설치","호칭번호 180(#12), 편흡입, 천장행거형","대",65191,3694202,0,3759393,"합계"]
["MEB01110010S",null,"송풍기 설치","호칭번호 032(#2), 양흡입, 천장행거형","대",11686,662223,0,673909,"합계"]
["MEB01110020S",null,"송풍기 설치","호칭번호 036(#2⅓), 양흡입, 천장행거형","대",12465,706375,0,718840,"합계"]
["MEB01110030S",null,"송풍기 설치","호칭번호 040(#2⅔), 양흡입, 천장행거형","대",13459,762712,0,776171,"합계"]
["MEB01110040S",null,"송풍기 설치","호칭번호 045(#3), 양흡입, 천장행거형","대",14722,834297,0,849019,"합계"]
["MEB01110050S",null,"송풍기 설치","호칭번호 050(#3⅓), 양흡입, 천장행거형","대",16149,915119,0,931268,"합계"]
["MEB01110060S",null,"송풍기 설치","호칭번호 056(#3⅔), 양흡입, 천장행거형","대",18092,1025244,0,1043336,"합계"]
["MEB01110070S",null,"송풍기 설치","호칭번호 063(#4), 양흡입, 천장행거형","대",20664,1170963,0,1191627,"합계"]
["MEB01110080S",null,"송풍기 설치","호칭번호 071(#4⅔), 양흡입, 천장행거형","대",24014,1360834,0,1384848,"합계"]
["MEB01110090S",null,"송풍기 설치","호칭번호 080(#5⅓), 양흡입, 천장행거형","대",28326,1605172,0,1633498,"합계"]
["MEB01110100S",null,"송풍기 설치","호칭번호 090(#6), 양흡입, 천장행거형","대",33795,1915085,0,1948880,"합계"]
["MEB01110110S",null,"송풍기 설치","호칭번호 100(#6⅔), 양흡입, 천장행거형","대",39979,2265524,0,2305503,"합계"]
["MEB01110120S",null,"송풍기 설치","호칭번호 112(#7½), 양흡입, 천장행거형","대",46837,2654107,0,2700944,"합계"]
["MEB01110130S",null,"송풍기 설치","호칭번호 125(#8⅓), 양흡입, 천장행거형","대",51647,2926672,0,2978319,"합계"]
["MEB01110140S",null,"송풍기 설치","호칭번호 140(#9⅓), 양흡입, 천장행거형","대",57914,3281813,0,3339727,"합계"]
["MEB01110150S",null,"송풍기 설치","호칭번호 160(#10⅔), 양흡입, 천장행거형","대",75810,4295949,0,4371759,"합계"]
["MEB01110160S",null,"송풍기 설치","호칭번호 180(#12), 양흡입, 천장행거형","대",86136,4881092,0,4967228,"합계"]
["MEB10010010S",null,"벽걸이 배기팬 설치","200mm","대",0,70116,0,70116,"합계"]
["MEB10010020S",null,"벽걸이 배기팬 설치","300mm","대",0,93488,0,93488,"합계"]
["MEB10010030S",null,"벽걸이 배기팬 설치","400mm","대",0,116861,0,116861,"합계"]
["MEB10010040S",null,"벽걸이 배기팬 설치","600mm","대",0,186977,0,186977,"합계"]
["MEB20010010S",null,"욕실배기팬 설치","100mm 이하","대",0,26351,0,26351,"합계"]
["MEB20010020S",null,"욕실배기팬 설치","200mm 이하","대",0,35213,0,35213,"합계"]
["MEB30010010S",null,"무덕트 유인팬 설치","풍량 1,600㎥/h 이하","대",0,81898,0,81898,"합계"]
["MEB30010020S",null,"무덕트 유인팬 설치","풍량 2,400㎥/h 이하","대",0,87624,0,87624,"합계"]
["MEB40010010S",null,"레인지후드 설치","700㎜ 이하(가정용, 최대풍량 6~12㎥/분)","대",0,34103,0,34103,"합계"]
["MEB40010020S",null,"레인지후드 설치","900㎜ 이하(가정용, 최대풍량 6~12㎥/분)","대",0,40803,0,40803,"합계"]
["MFA00010010S",null,"일반밸브 및 콕류 설치","D15∼25","개",229,11474,0,11703,"합계"]
["MFA00010020S",null,"일반밸브 및 콕류 설치","D32∼50","개",339,16981,0,17320,"합계"]
["MFA00010030S",null,"일반밸브 및 콕류 설치","D65","개",737,36868,0,37605,"합계"]
["MFA00010040S",null,"일반밸브 및 콕류 설치","D80","개",921,46097,0,47018,"합계"]
["MFA00010050S",null,"일반밸브 및 콕류 설치","D100","개",1329,66491,0,67820,"합계"]
["MFA00010060S",null,"일반밸브 및 콕류 설치","D125","개",1676,83826,0,85502,"합계"]
["MFA00010070S",null,"일반밸브 및 콕류 설치","D150","개",2060,103047,0,105107,"합계"]
["MFA00010080S",null,"일반밸브 및 콕류 설치","D200","개",2784,139208,0,141992,"합계"]
["MFA00010090S",null,"일반밸브 및 콕류 설치","D250","개",3588,179436,0,183024,"합계"]
["MFA00010100S",null,"일반밸브 및 콕류 설치","D300","개",4480,224039,0,228519,"합계"]
["MFA10010010S",null,"감압밸브장치 설치","D15","개",10266,513335,0,523601,"합계"]
["MFA10010020S",null,"감압밸브장치 설치","D20","개",12574,628736,0,641310,"합계"]
["MFA10010030S",null,"감압밸브장치 설치","D25","개",14720,736041,0,750761,"합계"]
["MFA10010040S",null,"감압밸브장치 설치","D32","개",17531,876576,0,894107,"합계"]
["MFA10010050S",null,"감압밸브장치 설치","D40","개",20532,1026645,0,1047177,"합계"]
["MFA10010060S",null,"감압밸브장치 설치","D50","개",24059,1202995,0,1227054,"합계"]
["MFA10010070S",null,"감압밸브장치 설치","D65","개",28603,1430198,0,1458801,"합계"]
["MFA10010080S",null,"감압밸브장치 설치","D80","개",32860,1643007,0,1675867,"합계"]
["MFA10010090S",null,"감압밸브장치 설치","D100","개",38537,1926863,0,1965400,"합계"]
["MFA10010100S",null,"감압밸브장치 설치","D125","개",45635,2281766,0,2327401,"합계"]
["MFA10010110S",null,"감압밸브장치 설치","D150","개",52730,2636504,0,2689234,"합계"]
["MFA10010120S",null,"감압밸브장치 설치","D200","개",65155,3257793,0,3322948,"합계"]
["MFB00010010S",null,"스팀트랩 장치 설치","D15","개",3678,183935,0,187613,"합계"]
["MFB00010020S",null,"스팀트랩 장치 설치","D20","개",4984,249245,0,254229,"합계"]
["MFB00010030S",null,"스팀트랩 장치 설치","D25","개",6292,314619,0,320911,"합계"]
["MFB00010040S",null,"스팀트랩 장치 설치","D32","개",8125,406274,0,414399,"합계"]
["MFB00010050S",null,"스팀트랩 장치 설치","D40","개",10221,511071,0,521292,"합계"]
["MFB00010060S",null,"스팀트랩 장치 설치","D50","개",12839,641984,0,654823,"합계"]
["MFC00010010S",null,"익스팬션조인트","D20∼25, 복식","개",1475,73763,0,75238,"합계"]
["MFC00010020S",null,"익스팬션조인트","D32, 복식","개",2234,111719,0,113953,"합계"]
["MFC00010030S",null,"익스팬션조인트","D40, 복식","개",2914,145725,0,148639,"합계"]
["MFC00010040S",null,"익스팬션조인트","D50, 복식","개",3800,190042,0,193842,"합계"]
["MFC00010050S",null,"익스팬션조인트","D65, 복식","개",5208,260400,0,265608,"합계"]
["MFC00010060S",null,"익스팬션조인트","D80, 복식","개",6685,334265,0,340950,"합계"]
["MFC00010070S",null,"익스팬션조인트","D100, 복식","개",8748,437447,0,446195,"합계"]
["MFC00010080S",null,"익스팬션조인트","D125, 복식","개",11464,573224,0,584688,"합계"]
["MFC00010090S",null,"익스팬션조인트","D150, 복식","개",14314,715719,0,730033,"합계"]
["MFC00010100S",null,"익스팬션조인트","D200, 복식","개",20339,1016966,0,1037305,"합계"]
["MFC00110010S",null,"익스팬션조인트","D20∼25, 단식","개",1298,64945,0,66243,"합계"]
["MFC00110020S",null,"익스팬션조인트","D32, 단식","개",1963,98198,0,100161,"합계"]
["MFC00110030S",null,"익스팬션조인트","D40, 단식","개",2564,128227,0,130791,"합계"]
["MFC00110040S",null,"익스팬션조인트","D50, 단식","개",3350,167548,0,170898,"합계"]
["MFC00110050S",null,"익스팬션조인트","D65, 단식","개",4589,229495,0,234084,"합계"]
["MFC00110060S",null,"익스팬션조인트","D80, 단식","개",5894,294718,0,300612,"합계"]
["MFC00110070S",null,"익스팬션조인트","D100, 단식","개",7716,385842,0,393558,"합계"]
["MFC00110080S",null,"익스팬션조인트","D125, 단식","개",10121,506082,0,516203,"합계"]
["MFC00110090S",null,"익스팬션조인트","D150, 단식","개",12637,631892,0,644529,"합계"]
["MFC00110100S",null,"익스팬션조인트","D200, 단식","개",17967,898392,0,916359,"합계"]
["MFC10010010S",null,"플랙시블커넥터 설치","D15∼25","개",238,11940,0,12178,"합계"]
["MFC10010020S",null,"플랙시블커넥터 설치","D32∼50","개",533,26662,0,27195,"합계"]
["MFC10010030S",null,"플랙시블커넥터 설치","D65","개",1191,59557,0,60748,"합계"]
["MFC10010040S",null,"플랙시블커넥터 설치","D80","개",1570,78537,0,80107,"합계"]
["MFC10010050S",null,"플랙시블커넥터 설치","D100","개",2335,116790,0,119125,"합계"]
["MFC10010060S",null,"플랙시블커넥터 설치","D125","개",3209,160460,0,163669,"합계"]
["MFC10010070S",null,"플랙시블커넥터 설치","D150","개",3979,198953,0,202932,"합계"]
["MFC10010080S",null,"플랙시블커넥터 설치","D200","개",5485,274285,0,279770,"합계"]
["MFC10010090S",null,"플랙시블커넥터 설치","D250","개",7038,351911,0,358949,"합계"]
["MFC10010100S",null,"플랙시블커넥터 설치","D300","개",8465,423292,0,431757,"합계"]
["MFD00010010S",null,"수격방지기","D15∼25","개",128,6425,0,6553,"합계"]
["MFD00010020S",null,"수격방지기","D32∼50","개",257,12850,0,13107,"합계"]
["MFD00010030S",null,"수격방지기","D65","개",414,20725,0,21139,"합계"]
["MFD00010040S",null,"수격방지기","D80","개",568,28411,0,28979,"합계"]
["MFD00010050S",null,"수격방지기","D100","개",773,38659,0,39432,"합계"]
["MFD00010060S",null,"수격방지기","D125","개",1029,51468,0,52497,"합계"]
["MFD00010070S",null,"수격방지기","D150","개",1285,64278,0,65563,"합계"]
["MFD00010080S",null,"수격방지기","D200","개",1797,89898,0,91695,"합계"]
["MGA00010010S",null,"직독식 유량계 설치","D13∼15","개",371,37132,0,37503,"합계"]
["MGA00010020S",null,"직독식 유량계 설치","D20∼32","개",446,44637,0,45083,"합계"]
["MGA00010030S",null,"직독식 유량계 설치","D40∼50","개",564,56488,0,57052,"합계"]
["MGA00010040S",null,"직독식 유량계 설치","D65∼80","개",1761,176181,0,177942,"합계"]
["MGA00010050S",null,"직독식 유량계 설치","D100∼150","개",2105,210549,0,212654,"합계"]
["MGA00010060S",null,"직독식 유량계 설치","D200∼300","개",3310,331032,0,334342,"합계"]
["MGA00110010S",null,"보호통 설치","D13∼15","개",584,58463,0,59047,"합계"]
["MGA00110020S",null,"보호통 설치","D20∼32","개",742,74265,0,75007,"합계"]
["MGA00110030S",null,"보호통 설치","D40∼50","개",999,99941,0,100940,"합계"]
["MGA10010010S",null,"원격식 유량계 설치","D13∼15","개",442,44242,0,44684,"합계"]
["MGA10010020S",null,"원격식 유량계 설치","D20∼32","개",521,52143,0,52664,"합계"]
["MGB00010010S",null,"적산열량계 세대용","D13∼15","개",481,48193,0,48674,"합계"]
["MGB00010020S",null,"적산열량계 세대용","D20∼32","개",560,56093,0,56653,"합계"]
["MGB10010010S",null,"적산열량계 건물용","D50","개",1674,167491,0,169165,"합계"]
["MGB10010020S",null,"적산열량계 건물용","D65","개",1888,188822,0,190710,"합계"]
["MGB10010030S",null,"적산열량계 건물용","D80","개",1931,193168,0,195099,"합계"]
["MGB10010040S",null,"적산열량계 건물용","D125","개",2058,205809,0,207867,"합계"]
["MGB10010050S",null,"적산열량계 건물용","D150","개",2504,250447,0,252951,"합계"]
["MGB20010010S",null,"적산열량계 산업용","D32","개",5867,586755,0,592622,"합계"]
["MGB20010020S",null,"적산열량계 산업용","D50","개",6198,619811,0,626009,"합계"]
["MGB20010030S",null,"적산열량계 산업용","D100","개",7024,702453,0,709477,"합계"]
["MGB20010040S",null,"적산열량계 산업용","D150","개",7850,785095,0,792945,"합계"]
["MHA00010010S",null,"소변기 설치","F.V형, 거치형","개",0,199196,0,199196,"합계"]
["MHA00010020S",null,"소변기 설치","F.V형, 벽걸이형","개",0,209073,0,209073,"합계"]
["MHA00010030S",null,"소변기 설치","전자감응기 일체형, 거치형","개",0,209645,0,209645,"합계"]
["MHA00010040S",null,"소변기 설치","전자감응기 일체형, 벽걸이형","개",0,219949,0,219949,"합계"]
["MHA00010050S",null,"소변기 설치","전자감응기 노출형, 거치형","개",0,233316,0,233316,"합계"]
["MHA00010060S",null,"소변기 설치","전자감응기 노출형, 벽걸이형","개",0,244899,0,244899,"합계"]
["MHA00010070S",null,"소변기 설치","전자감응기 벽매립형, 거치형","개",0,239074,0,239074,"합계"]
["MHA00010080S",null,"소변기 설치","전자감응기 벽매립형, 벽걸이형","개",0,250870,0,250870,"합계"]
["MHA10010010S",null,"대변기 설치","동양식대변기(F.V형)","개",0,157822,0,157822,"합계"]
["MHA10010020S",null,"대변기 설치","서양식대변기(탱크형)","개",0,181106,0,181106,"합계"]
["MHA10010030S",null,"대변기 설치","서양식대변기(F.V형)","개",0,174616,0,174616,"합계"]
["MHA20010010S",null,"도기세면기 설치","벽붙임 도기세면기","개",0,69404,0,69404,"합계"]
["MHA30010010S",null,"카운터형세면기 설치","카운터일체형","개",0,66741,0,66741,"합계"]
["MHA40010010S",null,"카운터형세면기 설치","카운터분리형","개",0,79318,0,79318,"합계"]
["MHA50010010S",null,"욕조 설치","욕조","개",0,168808,0,168808,"합계"]
["MHA60010010S",null,"청소용 수채 설치","청소용 수채","개",0,69205,0,69205,"합계"]
["MHB00010010S",null,"매립형 욕조수전 설치","욕조혼합수전","개",0,246362,0,246362,"합계"]
["MHB10010010S",null,"샤워수전 설치","벽붙임 혼합수전 노출형","개",0,22172,0,22172,"합계"]
["MHB10010020S",null,"샤워수전 설치","벽붙임 혼합수전 선반형","개",0,22977,0,22977,"합계"]
["MHB10010030S",null,"샤워수전 설치","고정식 샤워헤드걸이","개",0,15140,0,15140,"합계"]
["MHB10010040S",null,"샤워수전 설치","높이조절식 샤워헤드걸이","개",0,21112,0,21112,"합계"]
["MHB20010010S",null,"세면기수전 설치","대붙임 혼합수전","개",0,34277,0,34277,"합계"]
["MHB20010020S",null,"세면기수전 설치","대붙임 혼합수전, 냉수 또는 온수 전용","개",0,23994,0,23994,"합계"]
["MHB30010010S",null,"씽크수전 설치","대붙임 혼합수전","개",0,40436,0,40436,"합계"]
["MHB40010010S",null,"손빨래수전 설치","벽붙임 혼합수전","개",0,21367,0,21367,"합계"]
["MHB40010020S",null,"손빨래수전 설치","벽붙임 혼합수전, 냉수 또는 온수 전용","개",0,14957,0,14957,"합계"]
["MHC00010010S",null,"욕실거울 설치","0.5 ㎡ 미만","개",0,43020,0,43020,"합계"]
["MHC00010020S",null,"욕실거울 설치","1.0 ㎡ 미만","개",0,52117,0,52117,"합계"]
["MHC00010030S",null,"욕실거울 설치","1.5 ㎡ 미만","개",0,66354,0,66354,"합계"]
["MHC10010010S",null,"욕실금구류 설치","수건걸이, BAR형","개",0,21112,0,21112,"합계"]
["MHC10010020S",null,"욕실금구류 설치","수건걸이, 환형","개",0,15140,0,15140,"합계"]
["MHC10010030S",null,"욕실금구류 설치","휴지걸이, 노출형","개",0,15140,0,15140,"합계"]
["MHC10010040S",null,"욕실금구류 설치","휴지걸이, 매립형","개",0,31987,0,31987,"합계"]
["MHC10010050S",null,"욕실금구류 설치","비누대/컵대","개",0,15140,0,15140,"합계"]
["MHC10010060S",null,"욕실금구류 설치","옷걸이","개",0,15140,0,15140,"합계"]
["MHC20010010S",null,"바닥배수구 설치","D50mm","개소",0,32846,0,32846,"합계"]
["MHC20010020S",null,"바닥배수구 설치","D75mm","개소",0,43094,0,43094,"합계"]
["MHC20010030S",null,"바닥배수구 설치","D100mm","개소",0,46739,0,46739,"합계"]
["MHC30010010S",null,"안전손잡이 설치","고정단 2개","개",0,23146,0,23146,"합계"]
["MHC30010020S",null,"안전손잡이 설치","고정단 3개","개",0,25444,0,25444,"합계"]
["MHC30010030S",null,"안전손잡이 설치","고정단 4개","개",0,27742,0,27742,"합계"]
["MHC30010040S",null,"안전손잡이 설치","고정단 6개","개",0,30040,0,30040,"합계"]
["MIA00010010S",null,"냉동기 반입 ","지하1층 1회, 냉동U.S. 10톤","식",0,1055638,0,1055638,"합계"]
["MIA00010020S",null,"냉동기 반입 ","지하1층 1회, 냉동U.S. 20톤","식",0,1550332,0,1550332,"합계"]
["MIA00010030S",null,"냉동기 반입 ","지하1층 1회, 냉동U.S. 30톤","식",0,2045026,0,2045026,"합계"]
["MIA00010040S",null,"냉동기 반입 ","지하1층 1회, 냉동U.S. 50톤","식",0,2605970,0,2605970,"합계"]
["MIA00010050S",null,"냉동기 반입 ","지하1층 1회, 냉동U.S. 80톤","식",0,3875830,0,3875830,"합계"]
["MIA00010060S",null,"냉동기 반입 ","지하1층 1회, 냉동U.S. 100톤","식",0,5211940,0,5211940,"합계"]
["MIA00010070S",null,"냉동기 반입 ","지하1층 1회, 냉동U.S. 150톤","식",0,7965882,0,7965882,"합계"]
["MIA00010080S",null,"냉동기 반입 ","지하1층 1회, 냉동U.S. 200톤","식",0,10490130,0,10490130,"합계"]
["MIA00010090S",null,"냉동기 반입 ","지하1층 1회, 냉동U.S. 300톤","식",0,15503320,0,15503320,"합계"]
["MIA00010100S",null,"냉동기 반입 ","지하1층 1회, 냉동U.S. 400톤","식",0,20450260,0,20450260,"합계"]
["MIA00010110S",null,"냉동기 반입 ","지하1층 1회, 냉동U.S. 500톤","식",0,25397200,0,25397200,"합계"]
["MIA00010120S",null,"냉동기 반입 ","지하1층 1회, 냉동U.S. 600톤","식",0,30344140,0,30344140,"합계"]
["MIA01010010S",null,"냉동기 반입 ","지하2층 1회, 냉동U.S. 10톤","식",0,1269860,0,1269860,"합계"]
["MIA01010020S",null,"냉동기 반입 ","지하2층 1회, 냉동U.S. 20톤","식",0,1764554,0,1764554,"합계"]
["MIA01010030S",null,"냉동기 반입 ","지하2층 1회, 냉동U.S. 30톤","식",0,2259248,0,2259248,"합계"]
["MIA01010040S",null,"냉동기 반입 ","지하2층 1회, 냉동U.S. 50톤","식",0,2820192,0,2820192,"합계"]
["MIA01010050S",null,"냉동기 반입 ","지하2층 1회, 냉동U.S. 80톤","식",0,4865218,0,4865218,"합계"]
["MIA01010060S",null,"냉동기 반입 ","지하2층 1회, 냉동U.S. 100톤","식",0,6201328,0,6201328,"합계"]
["MIA01010070S",null,"냉동기 반입 ","지하2층 1회, 냉동U.S. 150톤","식",0,9730436,0,9730436,"합계"]
["MIA01010080S",null,"냉동기 반입 ","지하2층 1회, 냉동U.S. 200톤","식",0,12402656,0,12402656,"합계"]
["MIA01010090S",null,"냉동기 반입 ","지하2층 1회, 냉동U.S. 300톤","식",0,18338984,0,18338984,"합계"]
["MIA01010100S",null,"냉동기 반입 ","지하2층 1회, 냉동U.S. 400톤","식",0,24275312,0,24275312,"합계"]
["MIA01010110S",null,"냉동기 반입 ","지하2층 1회, 냉동U.S. 500톤","식",0,30344140,0,30344140,"합계"]
["MIA01010120S",null,"냉동기 반입 ","지하2층 1회, 냉동U.S. 600톤","식",0,36412968,0,36412968,"합계"]
["MIA01110010S",null,"냉동기 반입 ","지하2층 2회, 냉동U.S. 10톤","식",0,2111276,0,2111276,"합계"]
["MIA01110020S",null,"냉동기 반입 ","지하2층 2회, 냉동U.S. 20톤","식",0,2820192,0,2820192,"합계"]
["MIA01110030S",null,"냉동기 반입 ","지하2층 2회, 냉동U.S. 30톤","식",0,3875830,0,3875830,"합계"]
["MIA01110040S",null,"냉동기 반입 ","지하2층 2회, 냉동U.S. 50톤","식",0,5211940,0,5211940,"합계"]
["MIA01110050S",null,"냉동기 반입 ","지하2층 2회, 냉동U.S. 80톤","식",0,8164632,0,8164632,"합계"]
["MIA01110060S",null,"냉동기 반입 ","지하2층 2회, 냉동U.S. 100톤","식",0,10556380,0,10556380,"합계"]
["MIA01110070S",null,"냉동기 반입 ","지하2층 2회, 냉동U.S. 150톤","식",0,16757708,0,16757708,"합계"]
["MIA01110080S",null,"냉동기 반입 ","지하2층 2회, 냉동U.S. 200톤","식",0,21112760,0,21112760,"합계"]
["MIA01110090S",null,"냉동기 반입 ","지하2층 2회, 냉동U.S. 300톤","식",0,31006640,0,31006640,"합계"]
["MIA01110100S",null,"냉동기 반입 ","지하2층 2회, 냉동U.S. 400톤","식",0,40900520,0,40900520,"합계"]
["MIA01110110S",null,"냉동기 반입 ","지하2층 2회, 냉동U.S. 500톤","식",0,50794400,0,50794400,"합계"]
["MIA01110120S",null,"냉동기 반입 ","지하2층 2회, 냉동U.S. 600톤","식",0,60688280,0,60688280,"합계"]
["MIA02010010S",null,"냉동기 반입 ","지하3층 1회, 냉동U.S. 10톤","식",0,1269860,0,1269860,"합계"]
["MIA02010020S",null,"냉동기 반입 ","지하3층 1회, 냉동U.S. 20톤","식",0,2045026,0,2045026,"합계"]
["MIA02010030S",null,"냉동기 반입 ","지하3층 1회, 냉동U.S. 30톤","식",0,2820192,0,2820192,"합계"]
["MIA02010040S",null,"냉동기 반입 ","지하3층 1회, 냉동U.S. 50톤","식",0,3595358,0,3595358,"합계"]
["MIA02010050S",null,"냉동기 반입 ","지하3층 1회, 냉동U.S. 80톤","식",0,5706634,0,5706634,"합계"]
["MIA02010060S",null,"냉동기 반입 ","지하3층 1회, 냉동U.S. 100톤","식",0,7323216,0,7323216,"합계"]
["MIA02010070S",null,"냉동기 반입 ","지하3층 1회, 냉동U.S. 150톤","식",0,11693740,0,11693740,"합계"]
["MIA02010080S",null,"냉동기 반입 ","지하3층 1회, 냉동U.S. 200톤","식",0,14646432,0,14646432,"합계"]
["MIA02010090S",null,"냉동기 반입 ","지하3층 1회, 냉동U.S. 300톤","식",0,21704648,0,21704648,"합계"]
["MIA02010100S",null,"냉동기 반입 ","지하3층 1회, 냉동U.S. 400톤","식",0,28762864,0,28762864,"합계"]
["MIA02010110S",null,"냉동기 반입 ","지하3층 1회, 냉동U.S. 500톤","식",0,35953580,0,35953580,"합계"]
["MIA02010120S",null,"냉동기 반입 ","지하3층 1회, 냉동U.S. 600톤","식",0,43144296,0,43144296,"합계"]
["MIA02110010S",null,"냉동기 반입 ","지하3층 2회, 냉동U.S. 10톤","식",0,2391748,0,2391748,"합계"]
["MIA02110020S",null,"냉동기 반입 ","지하3층 2회, 냉동U.S. 20톤","식",0,3661608,0,3661608,"합계"]
["MIA02110030S",null,"냉동기 반입 ","지하3층 2회, 냉동U.S. 30톤","식",0,4865218,0,4865218,"합계"]
["MIA02110040S",null,"냉동기 반입 ","지하3층 2회, 냉동U.S. 50톤","식",0,6201328,0,6201328,"합계"]
["MIA02110050S",null,"냉동기 반입 ","지하3층 2회, 냉동U.S. 80톤","식",0,9995436,0,9995436,"합계"]
["MIA02110060S",null,"냉동기 반입 ","지하3층 2회, 냉동U.S. 100톤","식",0,12667656,0,12667656,"합계"]
["MIA02110070S",null,"냉동기 반입 ","지하3층 2회, 냉동U.S. 150톤","식",0,20271344,0,20271344,"합계"]
["MIA02110080S",null,"냉동기 반입 ","지하3층 2회, 냉동U.S. 200톤","식",0,25335312,0,25335312,"합계"]
["MIA02110090S",null,"냉동기 반입 ","지하3층 2회, 냉동U.S. 300톤","식",0,36810468,0,36810468,"합계"]
["MIA02110100S",null,"냉동기 반입 ","지하3층 2회, 냉동U.S. 400톤","식",0,48550624,0,48550624,"합계"]
["MIA02110110S",null,"냉동기 반입 ","지하3층 2회, 냉동U.S. 500톤","식",0,60688280,0,60688280,"합계"]
["MIA02110120S",null,"냉동기 반입 ","지하3층 2회, 냉동U.S. 600톤","식",0,73106408,0,73106408,"합계"]
["MIA03010010S",null,"냉동기 소운반","10m 거리내, 냉동U.S. 10톤","식",0,280472,0,280472,"합계"]
["MIA03010020S",null,"냉동기 소운반","10m 거리내, 냉동U.S. 20톤","식",0,560944,0,560944,"합계"]
["MIA03010030S",null,"냉동기 소운반","10m 거리내, 냉동U.S. 30톤","식",0,560944,0,560944,"합계"]
["MIA03010040S",null,"냉동기 소운반","10m 거리내, 냉동U.S. 50톤","식",0,775166,0,775166,"합계"]
["MIA03010050S",null,"냉동기 소운반","10m 거리내, 냉동U.S. 80톤","식",0,1336110,0,1336110,"합계"]
["MIA03010060S",null,"냉동기 소운반","10m 거리내, 냉동U.S. 100톤","식",0,1550332,0,1550332,"합계"]
["MIA03010070S",null,"냉동기 소운반","10m 거리내, 냉동U.S. 150톤","식",0,2325498,0,2325498,"합계"]
["MIA03010080S",null,"냉동기 소운반","10m 거리내, 냉동U.S. 200톤","식",0,2820192,0,2820192,"합계"]
["MIA03010090S",null,"냉동기 소운반","10m 거리내, 냉동U.S. 300톤","식",0,4650996,0,4650996,"합계"]
["MIA03010100S",null,"냉동기 소운반","10m 거리내, 냉동U.S. 400톤","식",0,6201328,0,6201328,"합계"]
["MIA03010110S",null,"냉동기 소운반","10m 거리내, 냉동U.S. 500톤","식",0,7751660,0,7751660,"합계"]
["MIA03010120S",null,"냉동기 소운반","10m 거리내, 냉동U.S. 600톤","식",0,9301992,0,9301992,"합계"]
["MIA03110010S",null,"냉동기 가조립 ","설치기초상, 냉동U.S. 10톤","식",0,560944,0,560944,"합계"]
["MIA03110020S",null,"냉동기 가조립 ","설치기초상, 냉동U.S. 20톤","식",0,841416,0,841416,"합계"]
["MIA03110030S",null,"냉동기 가조립 ","설치기초상, 냉동U.S. 30톤","식",0,1336110,0,1336110,"합계"]
["MIA03110040S",null,"냉동기 가조립 ","설치기초상, 냉동U.S. 50톤","식",0,1550332,0,1550332,"합계"]
["MIA03110050S",null,"냉동기 가조립 ","설치기초상, 냉동U.S. 80톤","식",0,2605970,0,2605970,"합계"]
["MIA03110060S",null,"냉동기 가조립 ","설치기초상, 냉동U.S. 100톤","식",0,2820192,0,2820192,"합계"]
["MIA03110070S",null,"냉동기 가조립 ","설치기초상, 냉동U.S. 150톤","식",0,4931468,0,4931468,"합계"]
["MIA03110080S",null,"냉동기 가조립 ","설치기초상, 냉동U.S. 200톤","식",0,6201328,0,6201328,"합계"]
["MIA03110090S",null,"냉동기 가조립 ","설치기초상, 냉동U.S. 300톤","식",0,9301992,0,9301992,"합계"]
["MIA03110100S",null,"냉동기 가조립 ","설치기초상, 냉동U.S. 400톤","식",0,12535156,0,12535156,"합계"]
["MIA03110110S",null,"냉동기 가조립 ","설치기초상, 냉동U.S. 500톤","식",0,15503320,0,15503320,"합계"]
["MIA03110120S",null,"냉동기 가조립 ","설치기초상, 냉동U.S. 600톤","식",0,18603984,0,18603984,"합계"]
["MIA10010010S",null,"냉동기 설치","왕복동식냉동기 5 냉동톤","대",0,683009,0,683009,"합계"]
["MIA10010020S",null,"냉동기 설치","왕복동식냉동기 7.5 냉동톤","대",0,852791,0,852791,"합계"]
["MIA10010030S",null,"냉동기 설치","왕복동식냉동기 15 냉동톤","대",0,1054780,0,1054780,"합계"]
["MIA10010040S",null,"냉동기 설치","왕복동식냉동기 20 냉동톤","대",0,1229643,0,1229643,"합계"]
["MIA10010050S",null,"냉동기 설치","왕복동식냉동기 30 냉동톤","대",0,1575418,0,1575418,"합계"]
["MIA10010060S",null,"냉동기 설치","왕복동식냉동기 50 냉동톤","대",0,1985309,0,1985309,"합계"]
["MIA10010070S",null,"냉동기 설치","왕복동식냉동기 80 냉동톤","대",0,3739039,0,3739039,"합계"]
["MID00010010S",null,"공기가열기, 공기냉각기, 공기여과기 설치","유효길이 610㎜","대",0,566771,0,566771,"합계"]
["MID00010020S",null,"공기가열기, 공기냉각기, 공기여과기 설치","유효길이 762㎜","대",0,708463,0,708463,"합계"]
["MID00010030S",null,"공기가열기, 공기냉각기, 공기여과기 설치","유효길이 914㎜","대",0,850156,0,850156,"합계"]
["MID00010040S",null,"공기가열기, 공기냉각기, 공기여과기 설치","유효길이 1,067㎜","대",0,983572,0,983572,"합계"]
["MID00010050S",null,"공기가열기, 공기냉각기, 공기여과기 설치","유효길이 1,219㎜","대",0,1133542,0,1133542,"합계"]
["MID00010060S",null,"공기가열기, 공기냉각기, 공기여과기 설치","유효길이 1,372㎜","대",0,1266957,0,1266957,"합계"]
["MID00010070S",null,"공기가열기, 공기냉각기, 공기여과기 설치","유효길이1,524㎜","대",0,1416927,0,1416927,"합계"]
["MID00010080S",null,"공기가열기, 공기냉각기, 공기여과기 설치","유효길이 1,676㎜","대",0,1550343,0,1550343,"합계"]
["MID00010090S",null,"공기가열기, 공기냉각기, 공기여과기 설치","유효길이 1,829㎜","대",0,1700313,0,1700313,"합계"]
["MID00010100S",null,"공기가열기, 공기냉각기, 공기여과기 설치","유효길이 1,981㎜","대",0,1833728,0,1833728,"합계"]
["MID00010110S",null,"공기가열기, 공기냉각기, 공기여과기 설치","유효길이 2,134㎜","대",0,1983698,0,1983698,"합계"]
["MID00010120S",null,"공기가열기, 공기냉각기, 공기여과기 설치","유효길이 2,286㎜","대",0,2117114,0,2117114,"합계"]
["MID00010130S",null,"공기가열기, 공기냉각기, 공기여과기 설치","유효길이 2,438㎜","대",0,2267084,0,2267084,"합계"]
["MID00010140S",null,"공기가열기, 공기냉각기, 공기여과기 설치","유효길이 2,591㎜","대",0,2400499,0,2400499,"합계"]
["MID00010150S",null,"공기가열기, 공기냉각기, 공기여과기 설치","유효길이 2,875㎜","대",0,2833855,0,2833855,"합계"]
["MID00010160S",null,"공기가열기, 공기냉각기, 공기여과기 설치","유효길이 3,048㎜","대",0,3117240,0,3117240,"합계"]
["MID20010010S",null,"공조기(A.H.U)","0.75㎾이하, 수냉식 패키지형","대",0,199633,0,199633,"합계"]
["MID20010020S",null,"공조기(A.H.U)","1.1㎾이하, 수냉식 패키지형","대",0,239560,0,239560,"합계"]
["MID20010030S",null,"공조기(A.H.U)","1.5㎾이하, 수냉식 패키지형","대",0,399267,0,399267,"합계"]
["MID20010040S",null,"공조기(A.H.U)","2.2㎾이하, 수냉식 패키지형","대",0,519047,0,519047,"합계"]
["MID20010050S",null,"공조기(A.H.U)","3.7㎾이하, 수냉식 패키지형","대",0,598900,0,598900,"합계"]
["MID20010060S",null,"공조기(A.H.U)","10.8㎾이하, 수냉식 패키지형","대",0,798534,0,798534,"합계"]
["MID20010070S",null,"공조기(A.H.U)","30.0㎾이하, 수냉식 패키지형","대",0,1197801,0,1197801,"합계"]
["MID20010080S",null,"공조기(A.H.U)","37.0㎾이하, 수냉식 패키지형","대",0,1397434,0,1397434,"합계"]
["MID20110010S",null,"공조기(A.H.U)","2.2㎾이하, 공냉식 패키지형","대",0,399267,0,399267,"합계"]
["MID20110020S",null,"공조기(A.H.U)","3.7㎾이하, 공냉식 패키지형","대",0,519047,0,519047,"합계"]
["MID20110030S",null,"공조기(A.H.U)","7.5㎾이하, 공냉식 패키지형","대",0,598900,0,598900,"합계"]
["MID20210010S",null,"공조기(A.H.U)","7.5㎾이하, 핸들링 유닛","대",0,1133542,0,1133542,"합계"]
["MID20210020S",null,"공조기(A.H.U)","15㎾이하, 핸들링 유닛","대",0,1700313,0,1700313,"합계"]
["MID20210030S",null,"공조기(A.H.U)","15㎾이상, 핸들링 유닛","대",0,2049916,0,2049916,"합계"]
["MID20310010S",null,"공조기(A.H.U)","팬코일유닛(상치형) 풍량 510㎥/hr 이하","대",0,233722,0,233722,"합계"]
["MID20310020S",null,"공조기(A.H.U)","팬코일유닛(상치형) 풍량 680㎥/hr 이상","대",0,266831,0,266831,"합계"]
["MID20410010S",null,"공조기(A.H.U)","팬코일유닛(천정형) 풍량 510㎥/hr 이하","대",0,433355,0,433355,"합계"]
["MID20410020S",null,"공조기(A.H.U)","팬코일유닛(천정형) 풍량 680㎥/hr 이상","대",0,550216,0,550216,"합계"]
["MID20510010S",null,"공조기(A.H.U)","0.4㎾이하, 윈도우타입","대",0,316494,0,316494,"합계"]
["MID20510020S",null,"공조기(A.H.U)","0.55㎾ 이하, 윈도우타입","대",0,386611,0,386611,"합계"]
["MID20510030S",null,"공조기(A.H.U)","0.75㎾ 이하, 윈도우타입","대",0,516128,0,516128,"합계"]
["MID30010010S",null,"천장형 에어컨 설치 ","실내기, 냉방능력 16kW 이하","대",2831,141594,0,144425,"합계"]
["MID30110010S",null,"천장형 에어컨 설치 ","실외기, 냉방능력 6~12kW 이하","대",6329,316494,0,322823,"합계"]
["MID30110020S",null,"천장형 에어컨 설치 ","실외기, 냉방능력 16kW 이하","대",8435,421765,0,430200,"합계"]
["MID40010010S",null,"전열교환기 설치","풍량 250㎥/h 이하","대",1378,68947,0,70325,"합계"]
["MID40010020S",null,"전열교환기 설치","풍량 500㎥/h 이하","대",1838,91929,0,93767,"합계"]
["MID40010030S",null,"전열교환기 설치","풍량 800㎥/h 이하","대",2344,117248,0,119592,"합계"]
["MIE00010010S",null,"보일러 설치","주철제, 1호(20∼60 미만) 1,000Kcal/hr","절",0,262547,0,262547,"합계"]
["MIE00010020S",null,"보일러 설치","주철제, 2호(60∼135 미만) 1,000Kcal/hr","절",0,306609,0,306609,"합계"]
["MIE00010030S",null,"보일러 설치","주철제, 3호(135∼230 미만) 1,000Kcal/hr","절",0,306609,0,306609,"합계"]
["MIE00010040S",null,"보일러 설치","주철제, 4호(230∼33 미만) 1,000Kcal/hr","절",0,569766,0,569766,"합계"]
["MIE00010050S",null,"보일러 설치","주철제, 5호(330∼640 미만) 1,000Kcal/hr","절",0,810891,0,810891,"합계"]
["MIE00010060S",null,"보일러 설치","주철제, 6호(640∼1,180 미만) 1,000Kcal/hr","절",0,1141359,0,1141359,"합계"]
["MIE00110010S",null,"보일러 설치","강판제","중량톤",0,435752,0,435752,"합계"]
["MIE00210010S",null,"보일러 설치","패키지형수관식","중량톤",0,1750316,0,1750316,"합계"]
["MIE10010010S",null,"경유보일러 설치","15,000 Kcal/hr","대",0,294044,0,294044,"합계"]
["MIE20010010S",null,"가스보일러 설치","가정용벽걸이형, 13,000 Kcal/hr","대",0,213312,0,213312,"합계"]
["MIE20010020S",null,"가스보일러 설치","가정용벽걸이형, 16,000 Kcal/hr","대",0,240197,0,240197,"합계"]
["MIE20010030S",null,"가스보일러 설치","가정용벽걸이형, 20,000 Kcal/hr","대",0,259424,0,259424,"합계"]
["MIE20010040S",null,"가스보일러 설치","가정용벽걸이형, 25,000 Kcal/hr","대",0,283333,0,283333,"합계"]
["MIE20010050S",null,"가스보일러 설치","가정용벽걸이형, 30,000 Kcal/hr","대",0,307408,0,307408,"합계"]
["MIE30010010S",null,"온수보일러 설치","70×1,000kcal/hr 이하","대",0,445904,0,445904,"합계"]
["MIE30010020S",null,"온수보일러 설치","120×1,000kcal/hr 이하","대",0,631646,0,631646,"합계"]
["MIE30010030S",null,"온수보일러 설치","150×1,000kcal/hr 이하","대",0,756250,0,756250,"합계"]
["MIE30010040S",null,"온수보일러 설치","240×1,000kcal/hr 이하","대",0,928896,0,928896,"합계"]
["MIE30010050S",null,"온수보일러 설치","360×1,000kcal/hr 이하","대",0,1178103,0,1178103,"합계"]
["MIE40010010S",null,"전기보일러 설치","135,000kcal (30㎾)","대",23352,1623964,29982,1677298,"합계"]
["MIE50010010S",null,"방열기 설치","주철제 바닥설치 20절 이하","조",0,268984,0,268984,"합계"]
["MIE50010020S",null,"방열기 설치","주철제 바닥설치 21절 이상","조",0,360777,0,360777,"합계"]
["MIE50010030S",null,"방열기 설치","벽걸이 3절","조",0,400280,0,400280,"합계"]
["MIE50010040S",null,"방열기 설치","천장달기 3절","조",0,656477,0,656477,"합계"]
["MIE50010050S",null,"방열기 설치","1m 길트","본",0,177191,0,177191,"합계"]
["MIE50110010S",null,"방열기 설치","컨벡터 길이 1m 미만","조",0,200140,0,200140,"합계"]
["MIE50110020S",null,"방열기 설치","컨벡터 길이 1m 이상","조",0,268984,0,268984,"합계"]
["MIE50210010S",null,"방열기 설치","베이스보드 1단형 길이 2m 미만","단",0,469124,0,469124,"합계"]
["MIE50210020S",null,"방열기 설치","베이스보드 1단형 길이 2m 이상","단",0,583865,0,583865,"합계"]
["MIE50310010S",null,"방열기 설치","강판제/알루미늄제 방열기 1m 미만","조",0,110904,0,110904,"합계"]
["MIE50310020S",null,"방열기 설치","강판제/알루미늄제 방열기 1m 이상","조",0,147621,0,147621,"합계"]
["MIE60010010S",null,"전기콘벡터 설치","벽걸이형, 740×440×105mm 기준","대",631,21034,0,21665,"합계"]
["MIF00010010S",null,"전기온수기 설치","350ℓ","대",0,524765,0,524765,"합계"]
["MIF10010010S",null,"전기온수기 설치","벽걸이형, 15L","대",980,49041,0,50021,"합계"]
["MIF10010020S",null,"전기온수기 설치","벽걸이형, 30L","대",1057,52899,0,53956,"합계"]
["MIF10010030S",null,"전기온수기 설치","벽걸이형, 50L","대",1311,65570,0,66881,"합계"]
["MIF20010010S",null,"온수분배기 설치","공급 및 환수 헤더, 2구","개",1809,90463,0,92272,"합계"]
["MIF20010020S",null,"온수분배기 설치","공급 및 환수 헤더, 3구","개",2128,106433,0,108561,"합계"]
["MIF20010030S",null,"온수분배기 설치","공급 및 환수 헤더, 4구","개",2436,121843,0,124279,"합계"]
["MIF20010040S",null,"온수분배기 설치","공급 및 환수 헤더, 5구","개",2681,134066,0,136747,"합계"]
["MIF20010050S",null,"온수분배기 설치","공급 및 환수 헤더, 6구","개",2909,145499,0,148408,"합계"]
["MIF20010060S",null,"온수분배기 설치","공급 및 환수 헤더, 7구","개",3113,155683,0,158796,"합계"]
["MJA00010010S",null,"입상관 방진가대 설치","D50","조",1385,46174,0,47559,"합계"]
["MJA00010020S",null,"입상관 방진가대 설치","D65","조",1385,46174,0,47559,"합계"]
["MJA00010030S",null,"입상관 방진가대 설치","D80","조",1623,54118,0,55741,"합계"]
["MJA00010040S",null,"입상관 방진가대 설치","D100","조",1861,62062,0,63923,"합계"]
["MJA00010050S",null,"입상관 방진가대 설치","D125","조",1861,62062,0,63923,"합계"]
["MJA00010060S",null,"입상관 방진가대 설치","D150","조",2085,69510,0,71595,"합계"]
["MJA00010070S",null,"입상관 방진가대 설치","D200","조",2323,77454,0,79777,"합계"]
["MJA00010080S",null,"입상관 방진가대 설치","D250","조",2934,97811,0,100745,"합계"]
["MJA00010090S",null,"입상관 방진가대 설치","D300","조",3559,118664,0,122223,"합계"]
["MJA00010100S",null,"입상관 방진가대 설치","D350","조",4185,139517,0,143702,"합계"]
["MJA10010010S",null,"잡철물 제작 및 설치","제품설치, 일반철재","톤",95766,1197077,0,1292843,"합계"]
["MJA10010020S",null,"잡철물 제작 및 설치","규격철물설치, 일반철재","톤",236593,2957413,0,3194006,"합계"]
["MJA10010030S",null,"잡철물 제작 및 설치","현장제작설치, 일반철재","톤",410630,5132880,0,5543510,"합계"]
["MJA10110010S",null,"잡철물 제작 및 설치","제품설치, 경량철재","톤",93398,1556640,0,1650038,"합계"]
["MJA10110020S",null,"잡철물 제작 및 설치","규격철물설치, 경량철재","톤",230743,3845733,0,4076476,"합계"]
["MJA10110030S",null,"잡철물 제작 및 설치","현장제작설치, 경량철재","톤",400294,6671569,0,7071863,"합계"]
["MJB10010010S",null,"녹막이페인트 칠","D50㎜ 이하, 붓칠 1회","m",56,2838,0,2894,"합계"]
["MJB10010020S",null,"녹막이페인트 칠","D100㎜ 이하, 붓칠 1회","m",85,4258,0,4343,"합계"]
["MJB10010030S",null,"녹막이페인트 칠","D200㎜ 이하, 붓칠 1회","m",133,6680,0,6813,"합계"]
["MJB10010040S",null,"녹막이페인트 칠","D300㎜ 이하, 붓칠 1회","m",190,9519,0,9709,"합계"]
["MJB20010010S",null,"유성페인트 칠","D50㎜ 이하, 롤러칠 1회","m",43,2171,0,2214,"합계"]
["MJB20010020S",null,"유성페인트 칠","D100㎜ 이하, 롤러칠 1회","m",66,3340,0,3406,"합계"]
["MJB20010030S",null,"유성페인트 칠","D200㎜ 이하, 롤러칠 1회","m",118,5928,0,6046,"합계"]
["MJB20010040S",null,"유성페인트 칠","D300㎜ 이하, 롤러칠 1회","m",167,8350,0,8517,"합계"]
["MJC00010010S",null,"슬리브 설치","D25∼50, 바닥","개소",135,13509,0,13644,"합계"]
["MJC00010020S",null,"슬리브 설치","D65∼100, 바닥","개소",174,17422,0,17596,"합계"]
["MJC00010030S",null,"슬리브 설치","D125∼150, 바닥","개소",209,20939,0,21148,"합계"]
["MJC00010040S",null,"슬리브 설치","D200∼250, 바닥","개소",244,24457,0,24701,"합계"]
["MJC00010050S",null,"슬리브 설치","D300∼400, 바닥","개소",282,28204,0,28486,"합계"]
["MJC00110010S",null,"슬리브 설치","D25∼50, 벽체","개소",157,15755,0,15912,"합계"]
["MJC00110020S",null,"슬리브 설치","D65∼100, 벽체","개소",188,18814,0,19002,"합계"]
["MJC00110030S",null,"슬리브 설치","D125∼150, 벽체","개소",243,24306,0,24549,"합계"]
["MJC00110040S",null,"슬리브 설치","D200∼250, 벽체","개소",316,31646,0,31962,"합계"]
["MJC00110050S",null,"슬리브 설치","D300∼400, 벽체","개소",403,40374,0,40777,"합계"]
["MJC01010010S",null,"슬리브 설치","D25∼50, 단열재 설치구간, 바닥","개소",135,16211,0,16346,"합계"]
["MJC01010020S",null,"슬리브 설치","D65∼100, 단열재 설치구간, 바닥","개소",174,20906,0,21080,"합계"]
["MJC01010030S",null,"슬리브 설치","D125∼150, 단열재 설치구간, 바닥","개소",209,25127,0,25336,"합계"]
["MJC01010040S",null,"슬리브 설치","D200∼250, 단열재 설치구간, 바닥","개소",244,29348,0,29592,"합계"]
["MJC01010050S",null,"슬리브 설치","D300∼400, 단열재 설치구간, 바닥","개소",282,33845,0,34127,"합계"]
["MJC01110010S",null,"슬리브 설치","D25∼50, 단열재 설치구간, 벽체","개소",157,18906,0,19063,"합계"]
["MJC01110020S",null,"슬리브 설치","D65∼100, 단열재 설치구간, 벽체","개소",188,22576,0,22764,"합계"]
["MJC01110030S",null,"슬리브 설치","D125∼150, 단열재 설치구간, 벽체","개소",243,29168,0,29411,"합계"]
["MJC01110040S",null,"슬리브 설치","D200∼250, 단열재 설치구간, 벽체","개소",316,37976,0,38292,"합계"]
["MJC01110050S",null,"슬리브 설치","D300∼400, 단열재 설치구간, 벽체","개소",403,48449,0,48852,"합계"]
["MJC10010010S",null,"배관을 위한 구멍뚫기","25mm, 콘크리트 두께 150mm, 바닥","개소",721,36066,0,36787,"합계"]
["MJC10010020S",null,"배관을 위한 구멍뚫기","50mm, 콘크리트 두께 150mm, 바닥","개소",894,44707,0,45601,"합계"]
["MJC10010030S",null,"배관을 위한 구멍뚫기","75mm, 콘크리트 두께 150mm, 바닥","개소",1066,53348,0,54414,"합계"]
["MJC10010040S",null,"배관을 위한 구멍뚫기","100mm, 콘크리트 두께 150mm, 바닥","개소",1239,61989,0,63228,"합계"]
["MJC10010050S",null,"배관을 위한 구멍뚫기","150mm, 콘크리트 두께 150mm, 바닥","개소",1577,78896,0,80473,"합계"]
["MJC10010060S",null,"배관을 위한 구멍뚫기","200mm, 콘크리트 두께 150mm, 바닥","개소",1893,94675,0,96568,"합계"]
["MJC10010070S",null,"배관을 위한 구멍뚫기","250mm, 콘크리트 두께 150mm, 바닥","개소",2216,110830,0,113046,"합계"]
["MJC10010080S",null,"배관을 위한 구멍뚫기","300mm, 콘크리트 두께 150mm, 바닥","개소",2547,127361,0,129908,"합계"]
["MJC10010090S",null,"배관을 위한 구멍뚫기","350mm, 콘크리트 두께 150mm, 바닥","개소",2885,144267,0,147152,"합계"]
["MJC10010100S",null,"배관을 위한 구멍뚫기","400mm, 콘크리트 두께 150mm, 바닥","개소",3200,160046,0,163246,"합계"]
["MJC10110010S",null,"배관을 위한 구멍뚫기","25mm, 콘크리트 두께 150mm, 벽체","개소",924,46210,0,47134,"합계"]
["MJC10110020S",null,"배관을 위한 구멍뚫기","50mm, 콘크리트 두께 150mm, 벽체","개소",1142,57105,0,58247,"합계"]
["MJC10110030S",null,"배관을 위한 구멍뚫기","75mm, 콘크리트 두께 150mm, 벽체","개소",1360,68001,0,69361,"합계"]
["MJC10110040S",null,"배관을 위한 구멍뚫기","100mm, 콘크리트 두께 150mm, 벽체","개소",1585,79271,0,80856,"합계"]
["MJC10110050S",null,"배관을 위한 구멍뚫기","150mm, 콘크리트 두께 150mm, 벽체","개소",2013,100686,0,102699,"합계"]
["MJC10110060S",null,"배관을 위한 구멍뚫기","200mm, 콘크리트 두께 150mm, 벽체","개소",2419,120974,0,123393,"합계"]
["MJC10110070S",null,"배관을 위한 구멍뚫기","250mm, 콘크리트 두께 150mm, 벽체","개소",2832,141637,0,144469,"합계"]
["MJC10110080S",null,"배관을 위한 구멍뚫기","300mm, 콘크리트 두께 150mm, 벽체","개소",3261,163052,0,166313,"합계"]
["MJC10110090S",null,"배관을 위한 구멍뚫기","350mm, 콘크리트 두께 150mm, 벽체","개소",3689,184467,0,188156,"합계"]
["MJC10110100S",null,"배관을 위한 구멍뚫기","400mm, 콘크리트 두께 150mm, 벽체","개소",4087,204379,0,208466,"합계"]
["MJC11010010S",null,"배관을 위한 구멍뚫기","25mm, 콘크리트 두께 300mm, 바닥","개소",1269,63492,0,64761,"합계"]
["MJC11010020S",null,"배관을 위한 구멍뚫기","50mm, 콘크리트 두께 300mm, 바닥","개소",1562,78144,0,79706,"합계"]
["MJC11010030S",null,"배관을 위한 구멍뚫기","75mm, 콘크리트 두께 300mm, 바닥","개소",1863,93172,0,95035,"합계"]
["MJC11010040S",null,"배관을 위한 구멍뚫기","100mm, 콘크리트 두께 300mm, 바닥","개소",2156,107825,0,109981,"합계"]
["MJC11010050S",null,"배관을 위한 구멍뚫기","150mm, 콘크리트 두께 300mm, 바닥","개소",2757,137880,0,140637,"합계"]
["MJC11010060S",null,"배관을 위한 구멍뚫기","200mm, 콘크리트 두께 300mm, 바닥","개소",3351,167560,0,170911,"합계"]
["MJC11010070S",null,"배관을 위한 구멍뚫기","250mm, 콘크리트 두께 300mm, 바닥","개소",3944,197240,0,201184,"합계"]
["MJC11010080S",null,"배관을 위한 구멍뚫기","300mm, 콘크리트 두께 300mm, 바닥","개소",4538,226920,0,231458,"합계"]
["MJC11010090S",null,"배관을 위한 구멍뚫기","350mm, 콘크리트 두께 300mm, 바닥","개소",5132,256601,0,261733,"합계"]
["MJC11010100S",null,"배관을 위한 구멍뚫기","400mm, 콘크리트 두께 300mm, 바닥","개소",5725,286281,0,292006,"합계"]
["MJC11110010S",null,"배관을 위한 구멍뚫기","25mm, 콘크리트 두께 300mm, 벽체","개소",1623,81150,0,82773,"합계"]
["MJC11110020S",null,"배관을 위한 구멍뚫기","50mm, 콘크리트 두께 300mm, 벽체","개소",1998,99935,0,101933,"합계"]
["MJC11110030S",null,"배관을 위한 구멍뚫기","75mm, 콘크리트 두께 300mm, 벽체","개소",2381,119095,0,121476,"합계"]
["MJC11110040S",null,"배관을 위한 구멍뚫기","100mm, 콘크리트 두께 300mm, 벽체","개소",2765,138256,0,141021,"합계"]
["MJC11110050S",null,"배관을 위한 구멍뚫기","150mm, 콘크리트 두께 300mm, 벽체","개소",3524,176201,0,179725,"합계"]
["MJC11110060S",null,"배관을 위한 구멍뚫기","200mm, 콘크리트 두께 300mm, 벽체","개소",4282,214147,0,218429,"합계"]
["MJC11110070S",null,"배관을 위한 구멍뚫기","250mm, 콘크리트 두께 300mm, 벽체","개소",5041,252092,0,257133,"합계"]
["MJC11110080S",null,"배관을 위한 구멍뚫기","300mm, 콘크리트 두께 300mm, 벽체","개소",5800,290038,0,295838,"합계"]
["MJC11110090S",null,"배관을 위한 구멍뚫기","350mm, 콘크리트 두께 300mm, 벽체","개소",6567,328359,0,334926,"합계"]
["MJC11110100S",null,"배관을 위한 구멍뚫기","400mm, 콘크리트 두께 300mm, 벽체","개소",7326,366304,0,373630,"합계"]
["MJD00010010S",null,"기밀시험","지상노출관","회당",4424,55303,0,59727,"합계"]
["MJD00010020S",null,"기밀시험","지하매설관","회당",6004,75055,0,81059,"합계"]
["MJD10010010S",null,"시험점화","단독주택","호당",790,39502,0,40292,"합계"]
["MJD10010020S",null,"시험점화","집단아파트","호당",395,19751,0,20146,"합계"]
["MKA00010010S",null,"옥내소화전함 설치","매립형","조",0,269989,0,269989,"합계"]
["MKA00010020S",null,"옥내소화전함 설치","노출형","조",0,243211,0,243211,"합계"]
["MKA10010010S",null,"소화용구 격납상자 설치","소화용구 격납상자","조",0,184812,0,184812,"합계"]
["MKB00010010S",null,"알람밸브 설치","D65","조",0,282262,0,282262,"합계"]
["MKB00010020S",null,"알람밸브 설치","D80","조",0,346517,0,346517,"합계"]
["MKB00010030S",null,"알람밸브 설치","D100","조",0,380940,0,380940,"합계"]
["MKB00010040S",null,"알람밸브 설치","D125","조",0,449110,0,449110,"합계"]
["MKB00010050S",null,"알람밸브 설치","D150","조",0,495007,0,495007,"합계"]
["MKB10010010S",null,"준비작동식밸브 설치","D80","조",0,419952,0,419952,"합계"]
["MKB10010020S",null,"준비작동식밸브 설치","D100","조",0,461258,0,461258,"합계"]
["MKB10010030S",null,"준비작동식밸브 설치","D125","조",0,534019,0,534019,"합계"]
["MKB10010040S",null,"준비작동식밸브 설치","D150","조",0,591389,0,591389,"합계"]
["MKB20010010S",null,"드라이밸브 설치","D100","조",0,484207,0,484207,"합계"]
["MKB20010020S",null,"드라이밸브 설치","D150","조",0,618927,0,618927,"합계"]
["MKB30010010S",null,"관말시험밸브 설치","관말시험밸브","조",0,105533,0,105533,"합계"]
["MKC00010010S",null,"옥외소화전 설치","지하식, 단구형","조",0,114741,0,114741,"합계"]
["MKC00010020S",null,"옥외소화전 설치","지하식, 쌍구형","조",0,137689,0,137689,"합계"]
["MKC10010010S",null,"옥외소화전 설치","지상식, 단구형","조",0,142278,0,142278,"합계"]
["MKC10010020S",null,"옥외소화전 설치","지상식, 쌍구형","조",0,344223,0,344223,"합계"]
["MKD00010010S",null,"일반송수구 설치","단구형","조",0,91792,0,91792,"합계"]
["MKD00010020S",null,"일반송수구 설치","쌍구형","조",0,137689,0,137689,"합계"]
["MKD00010030S",null,"일반송수구 설치","단구스탠드형","조",0,183585,0,183585,"합계"]
["MKD00010040S",null,"일반송수구 설치","쌍구스탠드형","조",0,275378,0,275378,"합계"]
["MKD10010010S",null,"방수구 설치","40㎜","조",0,17899,0,17899,"합계"]
["MKD10010020S",null,"방수구 설치","65㎜","조",0,26390,0,26390,"합계"]
["MKD20010010S",null,"연결송수구 설치","연결송수구 ","대",0,142278,0,142278,"합계"]
["MKE00010010S",null,"압력공기탱크 설치","압력공기탱크","개",0,527798,0,527798,"합계"]
["MKE10010010S",null,"마중물탱크 설치","100 ∼150ℓ","대",0,472732,0,472732,"합계"]
["MKF00010010S",null,"유량측정장치 설치","유량측정장치","조",0,236366,0,236366,"합계"]
["MKG00010010S",null,"스프링클러 헤드설치","스프링클러 헤드","개",0,27237,0,27237,"합계"]
["MKG10010010S",null,"스프링클러 전기설비 설치","펌프기동반 7.5㎾ 이하","면",0,592063,0,592063,"합계"]
["MKG10010020S",null,"스프링클러 전기설비 설치","펌프기동반 11 ∼ 19㎾","면",0,663202,0,663202,"합계"]
["MKG10010030S",null,"스프링클러 전기설비 설치","펌프기동반 22㎾ 이하","면",0,780238,0,780238,"합계"]
["MKG10010040S",null,"스프링클러 전기설비 설치","벨","개",0,48191,0,48191,"합계"]
["MKH00010010S",null,"소화약제 소화설비 설치","선택밸브, D25 이하","개",0,119330,0,119330,"합계"]
["MKH00010020S",null,"소화약제 소화설비 설치","선택밸브, D32 이하","개",0,188175,0,188175,"합계"]
["MKH00010030S",null,"소화약제 소화설비 설치","선택밸브, D40 이하","개",0,188175,0,188175,"합계"]
["MKH00010040S",null,"소화약제 소화설비 설치","선택밸브, D50 이하","개",0,188175,0,188175,"합계"]
["MKH00010050S",null,"소화약제 소화설비 설치","선택밸브, D65 이하","개",0,236366,0,236366,"합계"]
["MKH00010060S",null,"소화약제 소화설비 설치","선택밸브, D80 이하","개",0,284557,0,284557,"합계"]
["MKH00010070S",null,"소화약제 소화설비 설치","선택밸브, D100 이하","개",0,472732,0,472732,"합계"]
["MKH00010080S",null,"소화약제 소화설비 설치","선택밸브, D125 이하","개",0,472732,0,472732,"합계"]
["MKH00010090S",null,"소화약제 소화설비 설치","선택밸브, D150 이하","개",0,472732,0,472732,"합계"]
["MKH00110010S",null,"소화약제 소화설비 설치","가스분사헤드, 노출형","개",0,48191,0,48191,"합계"]
["MKH00110020S",null,"소화약제 소화설비 설치","가스분사헤드, 매립형","개",0,94087,0,94087,"합계"]
["MKH00210010S",null,"소화약제 소화설비 설치","용기지지대, 5본 이하","조",0,236366,0,236366,"합계"]
["MKH00210020S",null,"소화약제 소화설비 설치","용기지지대, 6~10본","조",0,355697,0,355697,"합계"]
["MKH00210030S",null,"소화약제 소화설비 설치","용기지지대, 11~20본","조",0,472732,0,472732,"합계"]
["MKH00310010S",null,"소화약제 소화설비 설치","용기집합함, 5본 이하","조",0,96382,0,96382,"합계"]
["MKH00310020S",null,"소화약제 소화설비 설치","용기집합함, 6~10본","조",0,165227,0,165227,"합계"]
["MKH00410010S",null,"소화약제 소화설비 설치","기동용기","조",0,142278,0,142278,"합계"]
["MKH00510010S",null,"소화약제 소화설비 설치","수동기동함","개",0,94087,0,94087,"합계"]
["MKH00610010S",null,"소화약제 소화설비 설치","압력스위치","개",0,71139,0,71139,"합계"]
["MKH00710010S",null,"소화약제 소화설비 설치","역지밸브","개",0,22948,0,22948,"합계"]
["MKH01010010S",null,"소화약제 소화설비 설치","배전반, 1~3실용","면",0,472732,0,472732,"합계"]
["MKH01010020S",null,"소화약제 소화설비 설치","배전반, 4~6실용","면",0,709099,0,709099,"합계"]
["MKH01110010S",null,"소화약제 소화설비 설치","단자함, 대형","면",0,94087,0,94087,"합계"]
["MKH01110020S",null,"소화약제 소화설비 설치","단자함, 소형","면",0,48191,0,48191,"합계"]
["MKH01210010S",null,"소화약제 소화설비 설치","가스방출표시등함","개",0,94087,0,94087,"합계"]
["MKH01310010S",null,"소화약제 소화설비 설치","모터사이렌","개",0,71139,0,71139,"합계"]
["MKH01410010S",null,"소화약제 소화설비 설치","벨","개",0,48191,0,48191,"합계"]
["MKH10010010S",null,"자동식 소화기 설치","자동식 소화기","개",0,68917,0,68917,"합계"]
["MKI00010010S",null,"완강기 설치","피난용 완강기","개",0,29584,0,29584,"합계"]
["MLA00010010S",null,"가스용 강관 용접 접합(알곤용접)","D15","개소",377,12587,0,12964,"합계"]
["MLA00010020S",null,"가스용 강관 용접 접합(알곤용접)","D20","개소",420,14018,0,14438,"합계"]
["MLA00010030S",null,"가스용 강관 용접 접합(알곤용접)","D25","개소",497,16592,0,17089,"합계"]
["MLA00010040S",null,"가스용 강관 용접 접합(알곤용접)","D32","개소",592,19739,0,20331,"합계"]
["MLA00010050S",null,"가스용 강관 용접 접합(알곤용접)","D40","개소",652,21742,0,22394,"합계"]
["MLA00010060S",null,"가스용 강관 용접 접합(알곤용접)","D50","개소",781,26033,0,26814,"합계"]
["MLA00010070S",null,"가스용 강관 용접 접합(알곤용접)","D65","개소",952,31755,0,32707,"합계"]
["MLA00010080S",null,"가스용 강관 용접 접합(알곤용접)","D80","개소",1089,36332,0,37421,"합계"]
["MLA00010090S",null,"가스용 강관 용접 접합(알곤용접)","D100","개소",1364,45487,0,46851,"합계"]
["MLA00010100S",null,"가스용 강관 용접 접합(알곤용접)","D125","개소",1639,54641,0,56280,"합계"]
["MLA00010110S",null,"가스용 강관 용접 접합(알곤용접)","D150","개소",1913,63796,0,65709,"합계"]
["MLA00010120S",null,"가스용 강관 용접 접합(알곤용접)","D200","개소",2463,82105,0,84568,"합계"]
["MLA00010130S",null,"가스용 강관 용접 접합(알곤용접)","D250","개소",3012,100415,0,103427,"합계"]
["MLA00010140S",null,"가스용 강관 용접 접합(알곤용접)","D300","개소",3561,118724,0,122285,"합계"]
["MLA00010150S",null,"가스용 강관 용접 접합(알곤용접)","D350","개소",3965,132170,0,136135,"합계"]
["MLA00010160S",null,"가스용 강관 용접 접합(알곤용접)","D400","개소",4514,150479,0,154993,"합계"]
["MLA00110010S",null,"가스용 강관 용접 접합(아크용접)","D15","개소",377,11958,0,12335,"합계"]
["MLA00110020S",null,"가스용 강관 용접 접합(아크용접)","D20","개소",420,13317,0,13737,"합계"]
["MLA00110030S",null,"가스용 강관 용접 접합(아크용접)","D25","개소",497,15763,0,16260,"합계"]
["MLA00110040S",null,"가스용 강관 용접 접합(아크용접)","D32","개소",592,18752,0,19344,"합계"]
["MLA00110050S",null,"가스용 강관 용접 접합(아크용접)","D40","개소",652,20655,0,21307,"합계"]
["MLA00110060S",null,"가스용 강관 용접 접합(아크용접)","D50","개소",781,24731,0,25512,"합계"]
["MLA00110070S",null,"가스용 강관 용접 접합(아크용접)","D65","개소",952,30167,0,31119,"합계"]
["MLA00110080S",null,"가스용 강관 용접 접합(아크용접)","D80","개소",1089,34515,0,35604,"합계"]
["MLA00110090S",null,"가스용 강관 용접 접합(아크용접)","D100","개소",1364,43212,0,44576,"합계"]
["MLA00110100S",null,"가스용 강관 용접 접합(아크용접)","D125","개소",1639,51909,0,53548,"합계"]
["MLA00110110S",null,"가스용 강관 용접 접합(아크용접)","D150","개소",1913,60606,0,62519,"합계"]
["MLA00110120S",null,"가스용 강관 용접 접합(아크용접)","D200","개소",2463,78000,0,80463,"합계"]
["MLA00110130S",null,"가스용 강관 용접 접합(아크용접)","D250","개소",3012,95394,0,98406,"합계"]
["MLA00110140S",null,"가스용 강관 용접 접합(아크용접)","D300","개소",3561,112788,0,116349,"합계"]
["MLA00110150S",null,"가스용 강관 용접 접합(아크용접)","D350","개소",3965,125561,0,129526,"합계"]
["MLA00110160S",null,"가스용 강관 용접 접합(아크용접)","D400","개소",4514,142955,0,147469,"합계"]
["MLA10010010S",null,"가스용 강관 용접식 부설","D15, 인력시공","m",58,5876,0,5934,"합계"]
["MLA10010020S",null,"가스용 강관 용접식 부설","D20, 인력시공","m",65,6500,0,6565,"합계"]
["MLA10010030S",null,"가스용 강관 용접식 부설","D25, 인력시공","m",85,8502,0,8587,"합계"]
["MLA10010040S",null,"가스용 강관 용접식 부설","D32, 인력시공","m",98,9815,0,9913,"합계"]
["MLA10010050S",null,"가스용 강관 용접식 부설","D40, 인력시공","m",115,11523,0,11638,"합계"]
["MLA10010060S",null,"가스용 강관 용접식 부설","D50, 인력시공","m",139,13919,0,14058,"합계"]
["MLA10010070S",null,"가스용 강관 용접식 부설","D65, 인력시공","m",160,16086,0,16246,"합계"]
["MLA10010080S",null,"가스용 강관 용접식 부설","D80, 인력시공","m",193,19336,0,19529,"합계"]
["MLA10010090S",null,"가스용 강관 용접식 부설","D100, 인력시공","m",252,25213,0,25465,"합계"]
["MLA10010100S",null,"가스용 강관 용접식 부설","D125, 인력시공","m",313,31319,0,31632,"합계"]
["MLA10010110S",null,"가스용 강관 용접식 부설","D150, 인력시공","m",363,36341,0,36704,"합계"]
["MLA10010120S",null,"가스용 강관 용접식 부설","D200, 인력시공","m",541,54135,0,54676,"합계"]
["MLA10010130S",null,"가스용 강관 용접식 부설","D250, 인력시공","m",711,71140,0,71851,"합계"]
["MLA10010140S",null,"가스용 강관 용접식 부설","D300, 인력시공","m",891,89164,0,90055,"합계"]
["MLA10010150S",null,"가스용 강관 용접식 부설","D350, 인력시공","m",1094,109419,0,110513,"합계"]
["MLA10010160S",null,"가스용 강관 용접식 부설","D400, 인력시공","m",1289,128985,0,130274,"합계"]
["MLA10110010S",null,"가스용 강관 용접식 부설","D150, 기계시공","m",1039,15579,869,17487,"합계"]
["MLA10110020S",null,"가스용 강관 용접식 부설","D200, 기계시공","m",1555,23254,1304,26113,"합계"]
["MLA10110030S",null,"가스용 강관 용접식 부설","D250, 기계시공","m",1903,30061,1522,33486,"합계"]
["MLA10110040S",null,"가스용 강관 용접식 부설","D300, 기계시공","m",2426,37966,1956,42348,"합계"]
["MLA10110050S",null,"가스용 강관 용접식 부설","D350, 기계시공","m",2963,46329,2391,51683,"합계"]
["MLA10110060S",null,"가스용 강관 용접식 부설","D400, 기계시공","m",3505,54858,2826,61189,"합계"]
["MLA20010010S",null,"가스용 강관 나사식 접합 및 배관","D20","개소",840,16812,0,17652,"합계"]
["MLA20010020S",null,"가스용 강관 나사식 접합 및 배관","D25","개소",1196,23937,0,25133,"합계"]
["MLA20010030S",null,"가스용 강관 나사식 접합 및 배관","D32","개소",1498,29979,0,31477,"합계"]
["MLA20010040S",null,"가스용 강관 나사식 접합 및 배관","D40","개소",1692,33854,0,35546,"합계"]
["MLA20010050S",null,"가스용 강관 나사식 접합 및 배관","D50","개소",2308,46167,0,48475,"합계"]
["MLB00010010S",null,"가스용 PE관 버트융착식 접합 및 부설","D25","개소",1086,21733,0,22819,"합계"]
["MLB00010020S",null,"가스용 PE관 버트융착식 접합 및 부설","D32","개소",1260,25213,0,26473,"합계"]
["MLB00010030S",null,"가스용 PE관 버트융착식 접합 및 부설","D40","개소",1446,28922,0,30368,"합계"]
["MLB00010040S",null,"가스용 PE관 버트융착식 접합 및 부설","D50","개소",1890,37819,0,39709,"합계"]
["MLB00010050S",null,"가스용 PE관 버트융착식 접합 및 부설","D63","개소",2467,49343,0,51810,"합계"]
["MLB00010060S",null,"가스용 PE관 버트융착식 접합 및 부설","D75","개소",2815,56302,0,59117,"합계"]
["MLB00010070S",null,"가스용 PE관 버트융착식 접합 및 부설","D90","개소",3271,65429,0,68700,"합계"]
["MLB00010080S",null,"가스용 PE관 버트융착식 접합 및 부설","D110","개소",3859,77182,0,81041,"합계"]
["MLB00010090S",null,"가스용 PE관 버트융착식 접합 및 부설","D125","개소",4315,86309,0,90624,"합계"]
["MLB00010100S",null,"가스용 PE관 버트융착식 접합 및 부설","D140","개소",4760,95206,0,99966,"합계"]
["MLB00010110S",null,"가스용 PE관 버트융착식 접합 및 부설","D160","개소",5367,107354,0,112721,"합계"]
["MLB00010120S",null,"가스용 PE관 버트융착식 접합 및 부설","D180","개소",5955,119106,0,125061,"합계"]
["MLB00010130S",null,"가스용 PE관 버트융착식 접합 및 부설","D200","개소",6554,131088,0,137642,"합계"]
["MLB00010140S",null,"가스용 PE관 버트융착식 접합 및 부설","D225","개소",7304,146091,0,153395,"합계"]
["MLB00010150S",null,"가스용 PE관 버트융착식 접합 및 부설","D250","개소",8054,161094,0,169148,"합계"]
["MLB00010160S",null,"가스용 PE관 버트융착식 접합 및 부설","D280","개소",8944,178889,0,187833,"합계"]
["MLB00010170S",null,"가스용 PE관 버트융착식 접합 및 부설","D315","개소",9988,199768,0,209756,"합계"]
["MLB00010180S",null,"가스용 PE관 버트융착식 접합 및 부설","D355","개소",11194,223898,0,235092,"합계"]
["MLB00010190S",null,"가스용 PE관 버트융착식 접합 및 부설","D400","개소",12540,250819,0,263359,"합계"]
["MLC00010010S",null,"분기공 설치","D20∼25","개",1494,149437,0,150931,"합계"]
["MLC00010020S",null,"분기공 설치","D40∼50","개",2090,209066,0,211156,"합계"]
["MLC00010030S",null,"분기공 설치","D65","개",2451,245175,0,247626,"합계"]
["MLC00010040S",null,"분기공 설치","D80","개",2812,281220,0,284032,"합계"]
["MLC00010050S",null,"분기공 설치","D100","개",3291,329172,0,332463,"합계"]
["MLC00010060S",null,"분기공 설치","D125","개",3890,389031,0,392921,"합계"]
["MLC00010070S",null,"분기공 설치","D150","개",4491,449112,0,453603,"합계"]
["MLC00010080S",null,"분기공 설치","D200","개",5690,569053,0,574743,"합계"]
["MLC00010090S",null,"분기공 설치","D250","개",6887,688707,0,695594,"합계"]
["MLC00010100S",null,"분기공 설치","D300","개",8088,808813,0,816901,"합계"]
["MLC00010110S",null,"분기공 설치","D350","개",9287,928753,0,938040,"합계"]
["MLC00010120S",null,"분기공 설치","D400","개",10484,1048464,0,1058948,"합계"]
["MLC10010010S",null,"가스용 밸브설치","D15∼25","개",1116,55802,0,56918,"합계"]
["MLC10010020S",null,"가스용 밸브설치","D32∼50","개",1744,87234,0,88978,"합계"]
["MLC10010030S",null,"가스용 밸브설치","D65","개",2121,106086,0,108207,"합계"]
["MLC10010040S",null,"가스용 밸브설치","D80","개",2502,125103,0,127605,"합계"]
["MLC10010050S",null,"가스용 밸브설치","D100","개",3006,150328,0,153334,"합계"]
["MLC10010060S",null,"가스용 밸브설치","D125","개",3635,181760,0,185395,"합계"]
["MLC10010070S",null,"가스용 밸브설치","D150","개",4268,213422,0,217690,"합계"]
["MLC10010080S",null,"가스용 밸브설치","D200","개",5525,276286,0,281811,"합계"]
["MLC10010090S",null,"가스용 밸브설치","D250","개",6790,339545,0,346335,"합계"]
["MLC10010100S",null,"가스용 밸브설치","D300","개",8052,402639,0,410691,"합계"]
["MLC10010110S",null,"가스용 밸브설치","D350","개",9314,465733,0,475047,"합계"]
["MLC10010120S",null,"가스용 밸브설치","D400","개",10576,528827,0,539403,"합계"]
["MLC20010010S",null,"직독식 가스미터 설치","D15","개소",0,56570,0,56570,"합계"]
["MLC20010020S",null,"직독식 가스미터 설치","D20∼25","개소",0,67799,0,67799,"합계"]
["MLC30010010S",null,"원격식 가스미터 설치","D15","개소",0,62216,0,62216,"합계"]
["MLC30010020S",null,"원격식 가스미터 설치","D20∼25","개소",0,73217,0,73217,"합계"]
["MQA00010010S",null,"배관 해체/강관","D15mm이하, 강관","m",81,4078,0,4159,"합계"]
["MQA00010020S",null,"배관 해체/강관","D20mm이하, 강관","m",89,4473,0,4562,"합계"]
["MQA00010030S",null,"배관 해체/강관","D25mm이하, 강관","m",114,5722,0,5836,"합계"]
["MQA00010040S",null,"배관 해체/강관","D32mm이하, 강관","m",130,6512,0,6642,"합계"]
["MQA00010050S",null,"배관 해체/강관","D40mm이하, 강관","m",142,7136,0,7278,"합계"]
["MQA00010060S",null,"배관 해체/강관","D50mm이하, 강관","m",183,9175,0,9358,"합계"]
["MQA00010070S",null,"배관 해체/강관","D65mm이하, 강관","m",211,10590,0,10801,"합계"]
["MQA00010080S",null,"배관 해체/강관","D80mm이하, 강관","m",265,13253,0,13518,"합계"]
["MQA00010090S",null,"배관 해체/강관","D100mm이하, 강관","m",359,17956,0,18315,"합계"]
["MQA00010100S",null,"배관 해체/강관","D125mm이하, 강관","m",456,22824,0,23280,"합계"]
["MQA00010110S",null,"배관 해체/강관","D150mm이하, 강관","m",538,26902,0,27440,"합계"]
["MQA00010120S",null,"배관 해체/강관","D200mm이하, 강관","m",820,41010,0,41830,"합계"]
["MQA00010130S",null,"배관 해체/강관","D250mm이하, 강관","m",1093,54659,0,55752,"합계"]
["MQA00010140S",null,"배관 해체/강관","D300mm이하, 강관","m",1414,70742,0,72156,"합계"]
["MQA00010150S",null,"배관 해체/강관","D350mm이하, 강관","m",1700,85016,0,86716,"합계"]
["MQA00010160S",null,"배관 해체/강관","D400mm이하, 강관","m",2010,100538,0,102548,"합계"]
["MQA01010010S",null,"배관 해체/동관","D15mm이하, 동관","m",69,3453,0,3522,"합계"]
["MQA01010020S",null,"배관 해체/동관","D20mm이하, 동관","m",81,4078,0,4159,"합계"]
["MQA01010030S",null,"배관 해체/동관","D25mm이하, 동관","m",101,5097,0,5198,"합계"]
["MQA01010040S",null,"배관 해체/동관","D32mm이하, 동관","m",122,6117,0,6239,"합계"]
["MQA01010050S",null,"배관 해체/동관","D40mm이하, 동관","m",138,6907,0,7045,"합계"]
["MQA01010060S",null,"배관 해체/동관","D50mm이하, 동관","m",183,9175,0,9358,"합계"]
["MQA01010070S",null,"배관 해체/동관","D65mm이하, 동관","m",211,10590,0,10801,"합계"]
["MQA01010080S",null,"배관 해체/동관","D80mm이하, 동관","m",265,13253,0,13518,"합계"]
["MQA01010090S",null,"배관 해체/동관","D100mm이하, 동관","m",359,17956,0,18315,"합계"]
["MQA01010100S",null,"배관 해체/동관","D125mm이하, 동관","m",448,22429,0,22877,"합계"]
["MQA01010110S",null,"배관 해체/동관","D150mm이하, 동관","m",530,26507,0,27037,"합계"]
["MQA01010120S",null,"배관 해체/동관","D200mm이하, 동관","m",787,39366,0,40153,"합계"]
["MQA01010130S",null,"배관 해체/동관","D250mm이하, 동관","m",1039,51996,0,53035,"합계"]
["MQA10010010S",null,"각형덕트 해체","t 0.5mm","㎡",407,20369,0,20776,"합계"]
["MQA10010020S",null,"각형덕트 해체","t 0.6mm","㎡",380,19044,0,19424,"합계"]
["MQA10010030S",null,"각형덕트 해체","t 0.8mm","㎡",399,19996,0,20395,"합계"]
["MQA10010040S",null,"각형덕트 해체","t 1.0mm","㎡",487,24385,0,24872,"합계"]
["MQA10010050S",null,"각형덕트 해체","t 1.2mm","㎡",563,28194,0,28757,"합계"]
["MQA10010060S",null,"각형덕트 해체","t 1.6mm","㎡",704,35232,0,35936,"합계"]
["MQA20010010S",null,"스파이럴덕트 해체","D150이하, t 0.5mm ","m",228,11426,0,11654,"합계"]
["MQA20010020S",null,"스파이럴덕트 해체","D160이하, t 0.5mm ","m",235,11799,0,12034,"합계"]
["MQA20010030S",null,"스파이럴덕트 해체","D180이하, t 0.5mm ","m",262,13124,0,13386,"합계"]
["MQA20010040S",null,"스파이럴덕트 해체","D200이하, t 0.5mm ","m",285,14283,0,14568,"합계"]
["MQA20010050S",null,"스파이럴덕트 해체","D225이하, t 0.6mm ","m",316,15815,0,16131,"합계"]
["MQA20010060S",null,"스파이럴덕트 해체","D250이하, t 0.6mm ","m",346,17347,0,17693,"합계"]
["MQA20010070S",null,"스파이럴덕트 해체","D275이하, t 0.6mm ","m",376,18837,0,19213,"합계"]
["MQA20010080S",null,"스파이럴덕트 해체","D300이하, t 0.6mm ","m",407,20369,0,20776,"합계"]
["MQA20010090S",null,"스파이럴덕트 해체","D350이하, t 0.6mm ","m",468,23433,0,23901,"합계"]
["MQA20010100S",null,"스파이럴덕트 해체","D400이하, t 0.6mm ","m",533,26662,0,27195,"합계"]
["MQA20010110S",null,"스파이럴덕트 해체","D450이하, t 0.6mm ","m",659,32955,0,33614,"합계"]
["MQA20010120S",null,"스파이럴덕트 해체","D500이하, t 0.6mm ","m",723,36184,0,36907,"합계"]
["MQA20010130S",null,"스파이럴덕트 해체","D550이하, t 0.6mm ","m",780,39041,0,39821,"합계"]
["MQA20010140S",null,"스파이럴덕트 해체","D600이하, t 0.6mm ","m",837,41898,0,42735,"합계"]
["MQA30010010S",null,"배관보온 해체/고무발포보온재","D15, 보온두께 50mm 이하, 고무발포보온재","m",0,4515,0,4515,"합계"]
["MQA30010020S",null,"배관보온 해체/고무발포보온재","D20, 보온두께 50mm 이하, 고무발포보온재","m",0,5089,0,5089,"합계"]
["MQA30010030S",null,"배관보온 해체/고무발포보온재","D25, 보온두께 50mm 이하, 고무발포보온재","m",0,5293,0,5293,"합계"]
["MQA30010040S",null,"배관보온 해체/고무발포보온재","D32, 보온두께 50mm 이하, 고무발포보온재","m",0,6237,0,6237,"합계"]
["MQA30010050S",null,"배관보온 해체/고무발포보온재","D40, 보온두께 50mm 이하, 고무발포보온재","m",0,7347,0,7347,"합계"]
["MQA30010060S",null,"배관보온 해체/고무발포보온재","D50, 보온두께 50mm 이하, 고무발포보온재","m",0,8495,0,8495,"합계"]
["MQA30010070S",null,"배관보온 해체/고무발포보온재","D65, 보온두께 50mm 이하, 고무발포보온재","m",0,9235,0,9235,"합계"]
["MQA30010080S",null,"배관보온 해체/고무발포보온재","D80, 보온두께 50mm 이하, 고무발포보온재","m",0,10383,0,10383,"합계"]
["MQA30010090S",null,"배관보온 해체/고무발포보온재","D100, 보온두께 50mm 이하, 고무발포보온재","m",0,11901,0,11901,"합계"]
["MQA30010100S",null,"배관보온 해체/고무발포보온재","D125, 보온두께 50mm 이하, 고무발포보온재","m",0,14363,0,14363,"합계"]
["MQA30010110S",null,"배관보온 해체/고무발포보온재","D150, 보온두께 50mm 이하, 고무발포보온재","m",0,16621,0,16621,"합계"]
["MQA30010120S",null,"배관보온 해체/고무발포보온재","D200, 보온두께 50mm 이하, 고무발포보온재","m",0,20027,0,20027,"합계"]
["MQA30010130S",null,"배관보온 해체/고무발포보온재","D250, 보온두께 50mm 이하, 고무발포보온재","m",0,23024,0,23024,"합계"]
["MQA30010140S",null,"배관보온 해체/고무발포보온재","D300, 보온두께 50mm 이하, 고무발포보온재","m",0,26060,0,26060,"합계"]
["MQA31010010S",null,"배관보온 해체/발포폴리에틸렌보온재","D15, 보온두께 50mm 이하, 발포폴리에틸렌보온재","m",0,3201,0,3201,"합계"]
["MQA31010020S",null,"배관보온 해체/발포폴리에틸렌보온재","D20, 보온두께 50mm 이하, 발포폴리에틸렌보온재","m",0,3775,0,3775,"합계"]
["MQA31010030S",null,"배관보온 해체/발포폴리에틸렌보온재","D25, 보온두께 50mm 이하, 발포폴리에틸렌보온재","m",0,3775,0,3775,"합계"]
["MQA31010040S",null,"배관보온 해체/발포폴리에틸렌보온재","D32, 보온두께 50mm 이하, 발포폴리에틸렌보온재","m",0,4515,0,4515,"합계"]
["MQA31010050S",null,"배관보온 해체/발포폴리에틸렌보온재","D40, 보온두께 50mm 이하, 발포폴리에틸렌보온재","m",0,5293,0,5293,"합계"]
["MQA31010060S",null,"배관보온 해체/발포폴리에틸렌보온재","D50, 보온두께 50mm 이하, 발포폴리에틸렌보온재","m",0,6033,0,6033,"합계"]
["MQA31010070S",null,"배관보온 해체/발포폴리에틸렌보온재","D65, 보온두께 50mm 이하, 발포폴리에틸렌보온재","m",0,6607,0,6607,"합계"]
["MQA31010080S",null,"배관보온 해체/발포폴리에틸렌보온재","D80, 보온두께 50mm 이하, 발포폴리에틸렌보온재","m",0,7551,0,7551,"합계"]
["MQA31010090S",null,"배관보온 해체/발포폴리에틸렌보온재","D100, 보온두께 50mm 이하, 발포폴리에틸렌보온재","m",0,8495,0,8495,"합계"]
["MQA31010100S",null,"배관보온 해체/발포폴리에틸렌보온재","D125, 보온두께 50mm 이하, 발포폴리에틸렌보온재","m",0,10383,0,10383,"합계"]
["MQA31010110S",null,"배관보온 해체/발포폴리에틸렌보온재","D150, 보온두께 50mm 이하, 발포폴리에틸렌보온재","m",0,11901,0,11901,"합계"]
["MQA31010120S",null,"배관보온 해체/발포폴리에틸렌보온재","D200, 보온두께 50mm 이하, 발포폴리에틸렌보온재","m",0,14159,0,14159,"합계"]
["MQA31010130S",null,"배관보온 해체/발포폴리에틸렌보온재","D250, 보온두께 50mm 이하, 발포폴리에틸렌보온재","m",0,16416,0,16416,"합계"]
["MQA31010140S",null,"배관보온 해체/발포폴리에틸렌보온재","D300, 보온두께 50mm 이하, 발포폴리에틸렌보온재","m",0,18509,0,18509,"합계"]
["MQA32010010S",null,"배관보온 해체/유리면보온재(글라스울)","D15, 보온두께 50mm 이하, 유리면보온재(글라스울)","m",0,5089,0,5089,"합계"]
["MQA32010020S",null,"배관보온 해체/유리면보온재(글라스울)","D20, 보온두께 50mm 이하, 유리면보온재(글라스울)","m",0,5663,0,5663,"합계"]
["MQA32010030S",null,"배관보온 해체/유리면보온재(글라스울)","D25, 보온두께 50mm 이하, 유리면보온재(글라스울)","m",0,6033,0,6033,"합계"]
["MQA32010040S",null,"배관보온 해체/유리면보온재(글라스울)","D32, 보온두께 50mm 이하, 유리면보온재(글라스울)","m",0,7181,0,7181,"합계"]
["MQA32010050S",null,"배관보온 해체/유리면보온재(글라스울)","D40, 보온두께 50mm 이하, 유리면보온재(글라스울)","m",0,8125,0,8125,"합계"]
["MQA32010060S",null,"배관보온 해체/유리면보온재(글라스울)","D50, 보온두께 50mm 이하, 유리면보온재(글라스울)","m",0,9643,0,9643,"합계"]
["MQA32010070S",null,"배관보온 해체/유리면보온재(글라스울)","D65, 보온두께 50mm 이하, 유리면보온재(글라스울)","m",0,10383,0,10383,"합계"]
["MQA32010080S",null,"배관보온 해체/유리면보온재(글라스울)","D80, 보온두께 50mm 이하, 유리면보온재(글라스울)","m",0,11901,0,11901,"합계"]
["MQA32010090S",null,"배관보온 해체/유리면보온재(글라스울)","D100, 보온두께 50mm 이하, 유리면보온재(글라스울)","m",0,13419,0,13419,"합계"]
["MQA32010100S",null,"배관보온 해체/유리면보온재(글라스울)","D125, 보온두께 50mm 이하, 유리면보온재(글라스울)","m",0,16047,0,16047,"합계"]
["MQA32010110S",null,"배관보온 해체/유리면보온재(글라스울)","D150, 보온두께 50mm 이하, 유리면보온재(글라스울)","m",0,18878,0,18878,"합계"]
["MQA32010120S",null,"배관보온 해체/유리면보온재(글라스울)","D200, 보온두께 50mm 이하, 유리면보온재(글라스울)","m",0,22654,0,22654,"합계"]
["MQA32010130S",null,"배관보온 해체/유리면보온재(글라스울)","D250, 보온두께 50mm 이하, 유리면보온재(글라스울)","m",0,25856,0,25856,"합계"]
["MQA32010140S",null,"배관보온 해체/유리면보온재(글라스울)","D300, 보온두께 50mm 이하, 유리면보온재(글라스울)","m",0,29262,0,29262,"합계"]
["MQA40010010S",null,"덕트보온 해체/고무발포보온재","고무발포보온재","㎡",0,25486,0,25486,"합계"]
["MQA41010010S",null,"덕트보온 해체/발포폴리에틸렌보온재","발포폴리에틸렌보온재","㎡",0,25486,0,25486,"합계"]
["MQA42010010S",null,"덕트보온 해체/유리면보온재(글라스울)","유리면보온재(글라스울)","㎡",0,30206,0,30206,"합계"]
["MQA50010010S",null,"펌프 해체","0.75kW 이하, 일반펌프","대",1684,84245,0,85929,"합계"]
["MQA50010020S",null,"펌프 해체","1.5kW 이하, 일반펌프","대",1866,93302,0,95168,"합계"]
["MQA50010030S",null,"펌프 해체","2.2kW 이하, 일반펌프","대",2147,107354,0,109501,"합계"]
["MQA50010040S",null,"펌프 해체","3.7kW 이하, 일반펌프","대",2469,123471,0,125940,"합계"]
["MQA50010050S",null,"펌프 해체","5.5kW 이하, 일반펌프","대",2972,148644,0,151616,"합계"]
["MQA50010060S",null,"펌프 해체","7.5kW 이하, 일반펌프","대",3749,187471,0,191220,"합계"]
["MQA50010070S",null,"펌프 해체","11kW 이하, 일반펌프","대",4715,235753,0,240468,"합계"]
["MQA50010080S",null,"펌프 해체","15kW 이하, 일반펌프","대",5004,250205,0,255209,"합계"]
["MQA50010090S",null,"펌프 해체","22kW 이하, 일반펌프","대",8084,404245,0,412329,"합계"]
["MQA50010100S",null,"펌프 해체","37kW 이하, 일반펌프","대",10438,521922,0,532360,"합계"]
["MQA50010110S",null,"펌프 해체","55kW 이하, 일반펌프","대",16792,839623,0,856415,"합계"]
["MQA50010120S",null,"펌프 해체","75kW 이하, 일반펌프","대",20570,1028526,0,1049096,"합계"]
["MQC00010010S",null,"유량계 교체/보호통","ø13~15mm, 급수급탕난방용","개",671,67154,0,67825,"합계"]
["MQC00010020S",null,"유량계 교체/보호통","ø20~32mm, 급수급탕난방용","개",790,79005,0,79795,"합계"]
["MQC00010030S",null,"유량계 교체/보호통","ø40~50mm, 급수급탕난방용","개",987,98756,0,99743,"합계"]
["MQC01010010S",null,"유량계 교체/유량계","ø13~15mm, 급수급탕난방용","개",513,51353,0,51866,"합계"]
["MQC01010020S",null,"유량계 교체/유량계","ø20~32mm, 급수급탕난방용","개",553,55303,0,55856,"합계"]
["MQC01010030S",null,"유량계 교체/유량계","ø40~50mm, 급수급탕난방용","개",671,67154,0,67825,"합계"]
["MQC01010040S",null,"유량계 교체/유량계","ø65~80mm, 급수급탕난방용","개",1975,197513,0,199488,"합계"]
["MQC01010050S",null,"유량계 교체/유량계","ø100~150mm, 급수급탕난방용","개",2646,264668,0,267314,"합계"]
["MQC01010060S",null,"유량계 교체/유량계","ø200~300mm, 급수급탕난방용","개",3950,395027,0,398977,"합계"]
["MQC10010010S",null,"관갱생공","D15mm","m",0,24234,0,24234,"합계"]
["MQC10010020S",null,"관갱생공","D20mm","m",0,24234,0,24234,"합계"]
["MQC10010030S",null,"관갱생공","D25mm","m",0,24234,0,24234,"합계"]
["MQC10010040S",null,"관갱생공","D32mm","m",0,24234,0,24234,"합계"]
["MQC10010050S",null,"관갱생공","D40mm","m",0,24234,0,24234,"합계"]
["MQC10010060S",null,"관갱생공","D50mm","m",0,24234,0,24234,"합계"]
["MQC10010070S",null,"관갱생공","D65mm","m",0,26942,0,26942,"합계"]
["MQC10010080S",null,"관갱생공","D80mm","m",0,26942,0,26942,"합계"]
["MQC10010090S",null,"관갱생공","D100mm","m",0,26942,0,26942,"합계"]
["MQC10010100S",null,"관갱생공","D125mm","m",0,33888,0,33888,"합계"]
["MQC10010110S",null,"관갱생공","D150mm","m",0,33888,0,33888,"합계"]
["MQC10010120S",null,"관갱생공","D200mm","m",0,33888,0,33888,"합계"]
["MQC10010130S",null,"관갱생공","D250mm","m",0,37468,0,37468,"합계"]
["MQC10010140S",null,"관갱생공","D300mm","m",0,37468,0,37468,"합계"]
["MQC20010010S",null,"배관누수 검사","급수급탕난방용 옥내배관(D50mm이하)","회",4887,162932,0,167819,"합계"]

{"sheet":"일위대가상세","index":1,"n_rows":17251,"n_cols":22,"rows_kept":4500,"cut":true,"hidden":false,"merged":[[1,0,1,16],[0,0,0,16],[2,8,2,9],[2,10,2,11],[2,12,2,13],[2,14,2,15],[2,0,3,0],[2,3,3,3],[2,1,3,1],[2,4,3,4],[2,5,3,5],[2,16,3,16],[2,6,3,6],[2,7,3,7],[2,2,3,2]],"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
["일 위 대 가 상 세"]
["20240200043_2024년 표준일위대가(기계)_1800520820"]
["일위대가코드","자원구분","자원코드","계산제외","품명","규격","단위","수량","재료비",null,"노무비",null,"경비",null,"합계",null,"비고",null,"관급여부","계산제외","적용요율","계산여부"]
[null,null,null,null,null,null,null,null,"단가","금액","단가","금액","단가","금액","단가","금액"]
["MBA00010010S",null,null,null,"강관 용접 접합(아크용접)","D15","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00010010S","노무","L001010101000012",null,"용접공","일반공사 직종","인",3.5999999999999997E-2,0,0,267021,9612.7000000000007,0,0,267021,9612.7000000000007,null,null,"N","N","",1]
["MBA00010010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,288.3,288.3,0,0,0,0,288.3,288.3,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,288,0,9612,0,0,0,9900,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00010020S",null,null,null,"강관 용접 접합(아크용접)","D20","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00010020S","노무","L001010101000012",null,"용접공","일반공사 직종","인",4.2999999999999997E-2,0,0,267021,11481.9,0,0,267021,11481.9,null,null,"N","N","",1]
["MBA00010020S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,344.4,344.4,0,0,0,0,344.4,344.4,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,344,0,11481,0,0,0,11825,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00010030S",null,null,null,"강관 용접 접합(아크용접)","D25","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00010030S","노무","L001010101000012",null,"용접공","일반공사 직종","인",5.1999999999999998E-2,0,0,267021,13885,0,0,267021,13885,null,null,"N","N","",1]
["MBA00010030S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,416.5,416.5,0,0,0,0,416.5,416.5,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,416,0,13885,0,0,0,14301,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00010040S",null,null,null,"강관 용접 접합(아크용접)","D32","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00010040S","노무","L001010101000012",null,"용접공","일반공사 직종","인",6.2E-2,0,0,267021,16555.3,0,0,267021,16555.3,null,null,"N","N","",1]
["MBA00010040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,496.6,496.6,0,0,0,0,496.6,496.6,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,496,0,16555,0,0,0,17051,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00010050S",null,null,null,"강관 용접 접합(아크용접)","D40","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00010050S","노무","L001010101000012",null,"용접공","일반공사 직종","인",7.0000000000000007E-2,0,0,267021,18691.400000000001,0,0,267021,18691.400000000001,null,null,"N","N","",1]
["MBA00010050S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,560.70000000000005,560.70000000000005,0,0,0,0,560.70000000000005,560.70000000000005,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,560,0,18691,0,0,0,19251,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00010060S",null,null,null,"강관 용접 접합(아크용접)","D50","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00010060S","노무","L001010101000012",null,"용접공","일반공사 직종","인",8.5000000000000006E-2,0,0,267021,22696.7,0,0,267021,22696.7,null,null,"N","N","",1]
["MBA00010060S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,680.9,680.9,0,0,0,0,680.9,680.9,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,680,0,22696,0,0,0,23376,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00010070S",null,null,null,"강관 용접 접합(아크용접)","D65","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00010070S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.105,0,0,267021,28037.200000000001,0,0,267021,28037.200000000001,null,null,"N","N","",1]
["MBA00010070S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,841.1,841.1,0,0,0,0,841.1,841.1,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,841,0,28037,0,0,0,28878,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00010080S",null,null,null,"강관 용접 접합(아크용접)","D80","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00010080S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.121,0,0,267021,32309.5,0,0,267021,32309.5,null,null,"N","N","",1]
["MBA00010080S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,969.2,969.2,0,0,0,0,969.2,969.2,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,969,0,32309,0,0,0,33278,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00010090S",null,null,null,"강관 용접 접합(아크용접)","D100","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00010090S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.152,0,0,267021,40587.1,0,0,267021,40587.1,null,null,"N","N","",1]
["MBA00010090S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,1217.5999999999999,1217.5999999999999,0,0,0,0,1217.5999999999999,1217.5999999999999,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,1217,0,40587,0,0,0,41804,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00010100S",null,null,null,"강관 용접 접합(아크용접)","D125","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00010100S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.184,0,0,267021,49131.8,0,0,267021,49131.8,null,null,"N","N","",1]
["MBA00010100S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,1473.9,1473.9,0,0,0,0,1473.9,1473.9,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,1473,0,49131,0,0,0,50604,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00010110S",null,null,null,"강관 용접 접합(아크용접)","D150","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00010110S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.216,0,0,267021,57676.5,0,0,267021,57676.5,null,null,"N","N","",1]
["MBA00010110S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,1730.2,1730.2,0,0,0,0,1730.2,1730.2,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,1730,0,57676,0,0,0,59406,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00010120S",null,null,null,"강관 용접 접합(아크용접)","D200","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00010120S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.28100000000000003,0,0,267021,75032.899999999994,0,0,267021,75032.899999999994,null,null,"N","N","",1]
["MBA00010120S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,2250.9,2250.9,0,0,0,0,2250.9,2250.9,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,2250,0,75032,0,0,0,77282,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00010130S",null,null,null,"강관 용접 접합(아크용접)","D250","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00010130S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.34499999999999997,0,0,267021,92122.2,0,0,267021,92122.2,null,null,"N","N","",1]
["MBA00010130S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,2763.6,2763.6,0,0,0,0,2763.6,2763.6,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,2763,0,92122,0,0,0,94885,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00010140S",null,null,null,"강관 용접 접합(아크용접)","D300","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00010140S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.40899999999999997,0,0,267021,109211.5,0,0,267021,109211.5,null,null,"N","N","",1]
["MBA00010140S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,3276.3,3276.3,0,0,0,0,3276.3,3276.3,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,3276,0,109211,0,0,0,112487,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00010150S",null,null,null,"강관 용접 접합(아크용접)","D350","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00010150S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.45600000000000002,0,0,267021,121761.5,0,0,267021,121761.5,null,null,"N","N","",1]
["MBA00010150S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,3652.8,3652.8,0,0,0,0,3652.8,3652.8,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,3652,0,121761,0,0,0,125413,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00010160S",null,null,null,"강관 용접 접합(아크용접)","D400","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00010160S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.51900000000000002,0,0,267021,138583.79999999999,0,0,267021,138583.79999999999,null,null,"N","N","",1]
["MBA00010160S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,4157.5,4157.5,0,0,0,0,4157.5,4157.5,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,4157,0,138583,0,0,0,142740,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00110010S",null,null,null,"강관 용접 접합(아크용접)","D15, 고소작업대 사용","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00110010S","노무","L001010101000012",null,"용접공","일반공사 직종","인",3.5999999999999997E-2,0,0,267021,9612.7000000000007,0,0,267021,9612.7000000000007,null,null,"N","Y","",0]
["MBA00110010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 13%","식",1,1249.5999999999999,1249.5999999999999,0,0,0,0,1249.5999999999999,1249.5999999999999,null,null,"N","N",13,1]
["MBA00110010S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,7690.1,7690.1,0,0,7690.1,7690.1,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,1249,0,7690,0,0,0,8939,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00110020S",null,null,null,"강관 용접 접합(아크용접)","D20, 고소작업대 사용","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00110020S","노무","L001010101000012",null,"용접공","일반공사 직종","인",4.2999999999999997E-2,0,0,267021,11481.9,0,0,267021,11481.9,null,null,"N","Y","",0]
["MBA00110020S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 13%","식",1,1492.6,1492.6,0,0,0,0,1492.6,1492.6,null,null,"N","N",13,1]
["MBA00110020S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,9185.5,9185.5,0,0,9185.5,9185.5,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,1492,0,9185,0,0,0,10677,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00110030S",null,null,null,"강관 용접 접합(아크용접)","D25, 고소작업대 사용","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00110030S","노무","L001010101000012",null,"용접공","일반공사 직종","인",5.1999999999999998E-2,0,0,267021,13885,0,0,267021,13885,null,null,"N","Y","",0]
["MBA00110030S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 13%","식",1,1805,1805,0,0,0,0,1805,1805,null,null,"N","N",13,1]
["MBA00110030S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,11108,11108,0,0,11108,11108,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,1805,0,11108,0,0,0,12913,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00110040S",null,null,null,"강관 용접 접합(아크용접)","D32, 고소작업대 사용","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00110040S","노무","L001010101000012",null,"용접공","일반공사 직종","인",6.2E-2,0,0,267021,16555.3,0,0,267021,16555.3,null,null,"N","Y","",0]
["MBA00110040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 13%","식",1,2152.1,2152.1,0,0,0,0,2152.1,2152.1,null,null,"N","N",13,1]
["MBA00110040S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,13244.2,13244.2,0,0,13244.2,13244.2,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,2152,0,13244,0,0,0,15396,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00110050S",null,null,null,"강관 용접 접합(아크용접)","D40, 고소작업대 사용","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00110050S","노무","L001010101000012",null,"용접공","일반공사 직종","인",7.0000000000000007E-2,0,0,267021,18691.400000000001,0,0,267021,18691.400000000001,null,null,"N","Y","",0]
["MBA00110050S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 13%","식",1,2429.8000000000002,2429.8000000000002,0,0,0,0,2429.8000000000002,2429.8000000000002,null,null,"N","N",13,1]
["MBA00110050S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,14953.1,14953.1,0,0,14953.1,14953.1,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,2429,0,14953,0,0,0,17382,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00110060S",null,null,null,"강관 용접 접합(아크용접)","D50, 고소작업대 사용","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00110060S","노무","L001010101000012",null,"용접공","일반공사 직종","인",8.5000000000000006E-2,0,0,267021,22696.7,0,0,267021,22696.7,null,null,"N","Y","",0]
["MBA00110060S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 13%","식",1,2950.5,2950.5,0,0,0,0,2950.5,2950.5,null,null,"N","N",13,1]
["MBA00110060S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,18157.3,18157.3,0,0,18157.3,18157.3,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,2950,0,18157,0,0,0,21107,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00110070S",null,null,null,"강관 용접 접합(아크용접)","D65, 고소작업대 사용","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00110070S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.105,0,0,267021,28037.200000000001,0,0,267021,28037.200000000001,null,null,"N","Y","",0]
["MBA00110070S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 13%","식",1,3644.8,3644.8,0,0,0,0,3644.8,3644.8,null,null,"N","N",13,1]
["MBA00110070S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,22429.7,22429.7,0,0,22429.7,22429.7,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,3644,0,22429,0,0,0,26073,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00110080S",null,null,null,"강관 용접 접합(아크용접)","D80, 고소작업대 사용","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00110080S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.121,0,0,267021,32309.5,0,0,267021,32309.5,null,null,"N","Y","",0]
["MBA00110080S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 13%","식",1,4200.2,4200.2,0,0,0,0,4200.2,4200.2,null,null,"N","N",13,1]
["MBA00110080S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,25847.599999999999,25847.599999999999,0,0,25847.599999999999,25847.599999999999,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,4200,0,25847,0,0,0,30047,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00110090S",null,null,null,"강관 용접 접합(아크용접)","D100, 고소작업대 사용","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00110090S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.152,0,0,267021,40587.1,0,0,267021,40587.1,null,null,"N","Y","",0]
["MBA00110090S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 13%","식",1,5276.3,5276.3,0,0,0,0,5276.3,5276.3,null,null,"N","N",13,1]
["MBA00110090S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,32469.599999999999,32469.599999999999,0,0,32469.599999999999,32469.599999999999,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,5276,0,32469,0,0,0,37745,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00110100S",null,null,null,"강관 용접 접합(아크용접)","D125, 고소작업대 사용","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00110100S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.184,0,0,267021,49131.8,0,0,267021,49131.8,null,null,"N","Y","",0]
["MBA00110100S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 13%","식",1,6387.1,6387.1,0,0,0,0,6387.1,6387.1,null,null,"N","N",13,1]
["MBA00110100S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,39305.4,39305.4,0,0,39305.4,39305.4,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,6387,0,39305,0,0,0,45692,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00110110S",null,null,null,"강관 용접 접합(아크용접)","D150, 고소작업대 사용","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00110110S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.216,0,0,267021,57676.5,0,0,267021,57676.5,null,null,"N","Y","",0]
["MBA00110110S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 13%","식",1,7497.9,7497.9,0,0,0,0,7497.9,7497.9,null,null,"N","N",13,1]
["MBA00110110S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,46141.2,46141.2,0,0,46141.2,46141.2,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,7497,0,46141,0,0,0,53638,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00110120S",null,null,null,"강관 용접 접합(아크용접)","D200, 고소작업대 사용","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00110120S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.28100000000000003,0,0,267021,75032.899999999994,0,0,267021,75032.899999999994,null,null,"N","Y","",0]
["MBA00110120S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 13%","식",1,9754.2000000000007,9754.2000000000007,0,0,0,0,9754.2000000000007,9754.2000000000007,null,null,"N","N",13,1]
["MBA00110120S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,60026.3,60026.3,0,0,60026.3,60026.3,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,9754,0,60026,0,0,0,69780,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00110130S",null,null,null,"강관 용접 접합(아크용접)","D250, 고소작업대 사용","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00110130S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.34499999999999997,0,0,267021,92122.2,0,0,267021,92122.2,null,null,"N","Y","",0]
["MBA00110130S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 13%","식",1,11975.8,11975.8,0,0,0,0,11975.8,11975.8,null,null,"N","N",13,1]
["MBA00110130S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,73697.7,73697.7,0,0,73697.7,73697.7,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,11975,0,73697,0,0,0,85672,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00110140S",null,null,null,"강관 용접 접합(아크용접)","D300, 고소작업대 사용","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00110140S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.40899999999999997,0,0,267021,109211.5,0,0,267021,109211.5,null,null,"N","Y","",0]
["MBA00110140S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 13%","식",1,14197.4,14197.4,0,0,0,0,14197.4,14197.4,null,null,"N","N",13,1]
["MBA00110140S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,87369.2,87369.2,0,0,87369.2,87369.2,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,14197,0,87369,0,0,0,101566,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00110150S",null,null,null,"강관 용접 접합(아크용접)","D350, 고소작업대 사용","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00110150S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.45600000000000002,0,0,267021,121761.5,0,0,267021,121761.5,null,null,"N","Y","",0]
["MBA00110150S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 13%","식",1,15828.9,15828.9,0,0,0,0,15828.9,15828.9,null,null,"N","N",13,1]
["MBA00110150S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,97409.2,97409.2,0,0,97409.2,97409.2,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,15828,0,97409,0,0,0,113237,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00110160S",null,null,null,"강관 용접 접합(아크용접)","D400, 고소작업대 사용","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA00110160S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.51900000000000002,0,0,267021,138583.79999999999,0,0,267021,138583.79999999999,null,null,"N","Y","",0]
["MBA00110160S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 13%","식",1,18015.8,18015.8,0,0,0,0,18015.8,18015.8,null,null,"N","N",13,1]
["MBA00110160S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,110867,110867,0,0,110867,110867,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,18015,0,110867,0,0,0,128882,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10010010S",null,null,null,"강관 용접 배관","D15, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10010010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",2.9000000000000001E-2,0,0,229482,6654.9,0,0,229482,6654.9,null,null,"N","N","",1]
["MBA10010010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.1999999999999999E-2,0,0,165545,3641.9,0,0,165545,3641.9,null,null,"N","N","",1]
["MBA10010010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,205.9,205.9,0,0,0,0,205.9,205.9,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,205,0,10296,0,0,0,10501,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10010020S",null,null,null,"강관 용접 배관","D20, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10010020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",3.3000000000000002E-2,0,0,229482,7572.9,0,0,229482,7572.9,null,null,"N","N","",1]
["MBA10010020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.3E-2,0,0,165545,3807.5,0,0,165545,3807.5,null,null,"N","N","",1]
["MBA10010020S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,227.6,227.6,0,0,0,0,227.6,227.6,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,227,0,11380,0,0,0,11607,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10010030S",null,null,null,"강관 용접 배관","D25, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10010030S","노무","L001010101000039",null,"배관공","일반공사 직종","인",4.2999999999999997E-2,0,0,229482,9867.7000000000007,0,0,229482,9867.7000000000007,null,null,"N","N","",1]
["MBA10010030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5999999999999999E-2,0,0,165545,4304.1000000000004,0,0,165545,4304.1000000000004,null,null,"N","N","",1]
["MBA10010030S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,283.39999999999998,283.39999999999998,0,0,0,0,283.39999999999998,283.39999999999998,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,283,0,14171,0,0,0,14454,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10010040S",null,null,null,"강관 용접 배관","D32, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10010040S","노무","L001010101000039",null,"배관공","일반공사 직종","인",5.0999999999999997E-2,0,0,229482,11703.5,0,0,229482,11703.5,null,null,"N","N","",1]
["MBA10010040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.9000000000000001E-2,0,0,165545,4800.8,0,0,165545,4800.8,null,null,"N","N","",1]
["MBA10010040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,330,330,0,0,0,0,330,330,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,330,0,16504,0,0,0,16834,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10010050S",null,null,null,"강관 용접 배관","D40, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10010050S","노무","L001010101000039",null,"배관공","일반공사 직종","인",5.7000000000000002E-2,0,0,229482,13080.4,0,0,229482,13080.4,null,null,"N","N","",1]
["MBA10010050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.1E-2,0,0,165545,5131.8,0,0,165545,5131.8,null,null,"N","N","",1]
["MBA10010050S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,364.2,364.2,0,0,0,0,364.2,364.2,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,364,0,18212,0,0,0,18576,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10010060S",null,null,null,"강관 용접 배관","D50, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10010060S","노무","L001010101000039",null,"배관공","일반공사 직종","인",7.3999999999999996E-2,0,0,229482,16981.599999999999,0,0,229482,16981.599999999999,null,null,"N","N","",1]
["MBA10010060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.6999999999999998E-2,0,0,165545,6125.1,0,0,165545,6125.1,null,null,"N","N","",1]
["MBA10010060S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,462.1,462.1,0,0,0,0,462.1,462.1,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,462,0,23106,0,0,0,23568,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10010070S",null,null,null,"강관 용접 배관","D65, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10010070S","노무","L001010101000039",null,"배관공","일반공사 직종","인",8.7999999999999995E-2,0,0,229482,20194.400000000001,0,0,229482,20194.400000000001,null,null,"N","N","",1]
["MBA10010070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.2000000000000003E-2,0,0,165545,6952.8,0,0,165545,6952.8,null,null,"N","N","",1]
["MBA10010070S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,542.9,542.9,0,0,0,0,542.9,542.9,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,542,0,27147,0,0,0,27689,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10010080S",null,null,null,"강관 용접 배관","D80, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10010080S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.113,0,0,229482,25931.4,0,0,229482,25931.4,null,null,"N","N","",1]
["MBA10010080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.0999999999999997E-2,0,0,165545,8442.7000000000007,0,0,165545,8442.7000000000007,null,null,"N","N","",1]
["MBA10010080S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,687.4,687.4,0,0,0,0,687.4,687.4,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,687,0,34374,0,0,0,35061,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10010090S",null,null,null,"강관 용접 배관","D100, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10010090S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.155,0,0,229482,35569.699999999997,0,0,229482,35569.699999999997,null,null,"N","N","",1]
["MBA10010090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.5000000000000002E-2,0,0,165545,10760.4,0,0,165545,10760.4,null,null,"N","N","",1]
["MBA10010090S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,926.6,926.6,0,0,0,0,926.6,926.6,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,926,0,46330,0,0,0,47256,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10010100S",null,null,null,"강관 용접 배관","D125, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10010100S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.2,0,0,229482,45896.4,0,0,229482,45896.4,null,null,"N","N","",1]
["MBA10010100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",8.1000000000000003E-2,0,0,165545,13409.1,0,0,165545,13409.1,null,null,"N","N","",1]
["MBA10010100S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,1186.0999999999999,1186.0999999999999,0,0,0,0,1186.0999999999999,1186.0999999999999,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,1186,0,59305,0,0,0,60491,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10010110S",null,null,null,"강관 용접 배관","D150, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10010110S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.23599999999999999,0,0,229482,54157.7,0,0,229482,54157.7,null,null,"N","N","",1]
["MBA10010110S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",9.2999999999999999E-2,0,0,165545,15395.6,0,0,165545,15395.6,null,null,"N","N","",1]
["MBA10010110S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,1391,1391,0,0,0,0,1391,1391,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,1391,0,69553,0,0,0,70944,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10010120S",null,null,null,"강관 용접 배관","D200, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10010120S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.36499999999999999,0,0,229482,83760.899999999994,0,0,229482,83760.899999999994,null,null,"N","N","",1]
["MBA10010120S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.13800000000000001,0,0,165545,22845.200000000001,0,0,165545,22845.200000000001,null,null,"N","N","",1]
["MBA10010120S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,2132.1,2132.1,0,0,0,0,2132.1,2132.1,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,2132,0,106606,0,0,0,108738,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10010130S",null,null,null,"강관 용접 배관","D250, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10010130S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.48899999999999999,0,0,229482,112216.6,0,0,229482,112216.6,null,null,"N","N","",1]
["MBA10010130S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.18099999999999999,0,0,165545,29963.599999999999,0,0,165545,29963.599999999999,null,null,"N","N","",1]
["MBA10010130S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,2843.6,2843.6,0,0,0,0,2843.6,2843.6,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,2843,0,142180,0,0,0,145023,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10010140S",null,null,null,"강관 용접 배관","D300, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10010140S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.63400000000000001,0,0,229482,145491.5,0,0,229482,145491.5,null,null,"N","N","",1]
["MBA10010140S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.23200000000000001,0,0,165545,38406.400000000001,0,0,165545,38406.400000000001,null,null,"N","N","",1]
["MBA10010140S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,3677.9,3677.9,0,0,0,0,3677.9,3677.9,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,3677,0,183897,0,0,0,187574,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10010150S",null,null,null,"강관 용접 배관","D350, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10010150S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.76500000000000001,0,0,229482,175553.7,0,0,229482,175553.7,null,null,"N","N","",1]
["MBA10010150S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.27700000000000002,0,0,165545,45855.9,0,0,165545,45855.9,null,null,"N","N","",1]
["MBA10010150S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,4428.1000000000004,4428.1000000000004,0,0,0,0,4428.1000000000004,4428.1000000000004,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,4428,0,221409,0,0,0,225837,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10010160S",null,null,null,"강관 용접 배관","D400, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10010160S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.90700000000000003,0,0,229482,208140.1,0,0,229482,208140.1,null,null,"N","N","",1]
["MBA10010160S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.32700000000000001,0,0,165545,54133.2,0,0,165545,54133.2,null,null,"N","N","",1]
["MBA10010160S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,5245.4,5245.4,0,0,0,0,5245.4,5245.4,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,5245,0,262273,0,0,0,267518,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10110010S",null,null,null,"강관 용접 배관","D15, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10110010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",2.9000000000000001E-2,0,0,229482,6654.9,0,0,229482,6654.9,null,null,"N","Y","",0]
["MBA10110010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.1999999999999999E-2,0,0,165545,3641.9,0,0,165545,3641.9,null,null,"N","Y","",0]
["MBA10110010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1029.5999999999999,1029.5999999999999,0,0,0,0,1029.5999999999999,1029.5999999999999,null,null,"N","N",10,1]
["MBA10110010S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,8237.4,8237.4,0,0,8237.4,8237.4,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,1029,0,8237,0,0,0,9266,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10110020S",null,null,null,"강관 용접 배관","D20, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10110020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",3.3000000000000002E-2,0,0,229482,7572.9,0,0,229482,7572.9,null,null,"N","Y","",0]
["MBA10110020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.3E-2,0,0,165545,3807.5,0,0,165545,3807.5,null,null,"N","Y","",0]
["MBA10110020S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1138,1138,0,0,0,0,1138,1138,null,null,"N","N",10,1]
["MBA10110020S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,9104.2999999999993,9104.2999999999993,0,0,9104.2999999999993,9104.2999999999993,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,1138,0,9104,0,0,0,10242,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10110030S",null,null,null,"강관 용접 배관","D25, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10110030S","노무","L001010101000039",null,"배관공","일반공사 직종","인",4.2999999999999997E-2,0,0,229482,9867.7000000000007,0,0,229482,9867.7000000000007,null,null,"N","Y","",0]
["MBA10110030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5999999999999999E-2,0,0,165545,4304.1000000000004,0,0,165545,4304.1000000000004,null,null,"N","Y","",0]
["MBA10110030S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1417.1,1417.1,0,0,0,0,1417.1,1417.1,null,null,"N","N",10,1]
["MBA10110030S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,11337.4,11337.4,0,0,11337.4,11337.4,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,1417,0,11337,0,0,0,12754,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10110040S",null,null,null,"강관 용접 배관","D32, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10110040S","노무","L001010101000039",null,"배관공","일반공사 직종","인",5.0999999999999997E-2,0,0,229482,11703.5,0,0,229482,11703.5,null,null,"N","Y","",0]
["MBA10110040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.9000000000000001E-2,0,0,165545,4800.8,0,0,165545,4800.8,null,null,"N","Y","",0]
["MBA10110040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1650.4,1650.4,0,0,0,0,1650.4,1650.4,null,null,"N","N",10,1]
["MBA10110040S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,13203.4,13203.4,0,0,13203.4,13203.4,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,1650,0,13203,0,0,0,14853,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10110050S",null,null,null,"강관 용접 배관","D40, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10110050S","노무","L001010101000039",null,"배관공","일반공사 직종","인",5.7000000000000002E-2,0,0,229482,13080.4,0,0,229482,13080.4,null,null,"N","Y","",0]
["MBA10110050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.1E-2,0,0,165545,5131.8,0,0,165545,5131.8,null,null,"N","Y","",0]
["MBA10110050S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1821.2,1821.2,0,0,0,0,1821.2,1821.2,null,null,"N","N",10,1]
["MBA10110050S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,14569.7,14569.7,0,0,14569.7,14569.7,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,1821,0,14569,0,0,0,16390,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10110060S",null,null,null,"강관 용접 배관","D50, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10110060S","노무","L001010101000039",null,"배관공","일반공사 직종","인",7.3999999999999996E-2,0,0,229482,16981.599999999999,0,0,229482,16981.599999999999,null,null,"N","Y","",0]
["MBA10110060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.6999999999999998E-2,0,0,165545,6125.1,0,0,165545,6125.1,null,null,"N","Y","",0]
["MBA10110060S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,2310.6,2310.6,0,0,0,0,2310.6,2310.6,null,null,"N","N",10,1]
["MBA10110060S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,18485.3,18485.3,0,0,18485.3,18485.3,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,2310,0,18485,0,0,0,20795,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10110070S",null,null,null,"강관 용접 배관","D65, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10110070S","노무","L001010101000039",null,"배관공","일반공사 직종","인",8.7999999999999995E-2,0,0,229482,20194.400000000001,0,0,229482,20194.400000000001,null,null,"N","Y","",0]
["MBA10110070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.2000000000000003E-2,0,0,165545,6952.8,0,0,165545,6952.8,null,null,"N","Y","",0]
["MBA10110070S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,2714.7,2714.7,0,0,0,0,2714.7,2714.7,null,null,"N","N",10,1]
["MBA10110070S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,21717.7,21717.7,0,0,21717.7,21717.7,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,2714,0,21717,0,0,0,24431,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10110080S",null,null,null,"강관 용접 배관","D80, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10110080S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.113,0,0,229482,25931.4,0,0,229482,25931.4,null,null,"N","Y","",0]
["MBA10110080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.0999999999999997E-2,0,0,165545,8442.7000000000007,0,0,165545,8442.7000000000007,null,null,"N","Y","",0]
["MBA10110080S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,3437.4,3437.4,0,0,0,0,3437.4,3437.4,null,null,"N","N",10,1]
["MBA10110080S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,27499.200000000001,27499.200000000001,0,0,27499.200000000001,27499.200000000001,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,3437,0,27499,0,0,0,30936,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10110090S",null,null,null,"강관 용접 배관","D100, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10110090S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.155,0,0,229482,35569.699999999997,0,0,229482,35569.699999999997,null,null,"N","Y","",0]
["MBA10110090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.5000000000000002E-2,0,0,165545,10760.4,0,0,165545,10760.4,null,null,"N","Y","",0]
["MBA10110090S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,4633,4633,0,0,0,0,4633,4633,null,null,"N","N",10,1]
["MBA10110090S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,37064,37064,0,0,37064,37064,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,4633,0,37064,0,0,0,41697,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10110100S",null,null,null,"강관 용접 배관","D125, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10110100S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.2,0,0,229482,45896.4,0,0,229482,45896.4,null,null,"N","Y","",0]
["MBA10110100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",8.1000000000000003E-2,0,0,165545,13409.1,0,0,165545,13409.1,null,null,"N","Y","",0]
["MBA10110100S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,5930.5,5930.5,0,0,0,0,5930.5,5930.5,null,null,"N","N",10,1]
["MBA10110100S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,47444.4,47444.4,0,0,47444.4,47444.4,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,5930,0,47444,0,0,0,53374,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10110110S",null,null,null,"강관 용접 배관","D150, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10110110S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.23599999999999999,0,0,229482,54157.7,0,0,229482,54157.7,null,null,"N","Y","",0]
["MBA10110110S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",9.2999999999999999E-2,0,0,165545,15395.6,0,0,165545,15395.6,null,null,"N","Y","",0]
["MBA10110110S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,6955.3,6955.3,0,0,0,0,6955.3,6955.3,null,null,"N","N",10,1]
["MBA10110110S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,55642.6,55642.6,0,0,55642.6,55642.6,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,6955,0,55642,0,0,0,62597,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10110120S",null,null,null,"강관 용접 배관","D200, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10110120S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.36499999999999999,0,0,229482,83760.899999999994,0,0,229482,83760.899999999994,null,null,"N","Y","",0]
["MBA10110120S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.13800000000000001,0,0,165545,22845.200000000001,0,0,165545,22845.200000000001,null,null,"N","Y","",0]
["MBA10110120S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,10660.6,10660.6,0,0,0,0,10660.6,10660.6,null,null,"N","N",10,1]
["MBA10110120S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,85284.800000000003,85284.800000000003,0,0,85284.800000000003,85284.800000000003,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,10660,0,85284,0,0,0,95944,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10110130S",null,null,null,"강관 용접 배관","D250, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10110130S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.48899999999999999,0,0,229482,112216.6,0,0,229482,112216.6,null,null,"N","Y","",0]
["MBA10110130S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.18099999999999999,0,0,165545,29963.599999999999,0,0,165545,29963.599999999999,null,null,"N","Y","",0]
["MBA10110130S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,14218,14218,0,0,0,0,14218,14218,null,null,"N","N",10,1]
["MBA10110130S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,113744.1,113744.1,0,0,113744.1,113744.1,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,14218,0,113744,0,0,0,127962,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10110140S",null,null,null,"강관 용접 배관","D300, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10110140S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.63400000000000001,0,0,229482,145491.5,0,0,229482,145491.5,null,null,"N","Y","",0]
["MBA10110140S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.23200000000000001,0,0,165545,38406.400000000001,0,0,165545,38406.400000000001,null,null,"N","Y","",0]
["MBA10110140S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,18389.7,18389.7,0,0,0,0,18389.7,18389.7,null,null,"N","N",10,1]
["MBA10110140S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,147118.29999999999,147118.29999999999,0,0,147118.29999999999,147118.29999999999,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,18389,0,147118,0,0,0,165507,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10110150S",null,null,null,"강관 용접 배관","D350, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10110150S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.76500000000000001,0,0,229482,175553.7,0,0,229482,175553.7,null,null,"N","Y","",0]
["MBA10110150S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.27700000000000002,0,0,165545,45855.9,0,0,165545,45855.9,null,null,"N","Y","",0]
["MBA10110150S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,22140.9,22140.9,0,0,0,0,22140.9,22140.9,null,null,"N","N",10,1]
["MBA10110150S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,177127.6,177127.6,0,0,177127.6,177127.6,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,22140,0,177127,0,0,0,199267,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10110160S",null,null,null,"강관 용접 배관","D400, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA10110160S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.90700000000000003,0,0,229482,208140.1,0,0,229482,208140.1,null,null,"N","Y","",0]
["MBA10110160S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.32700000000000001,0,0,165545,54133.2,0,0,165545,54133.2,null,null,"N","Y","",0]
["MBA10110160S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,26227.3,26227.3,0,0,0,0,26227.3,26227.3,null,null,"N","N",10,1]
["MBA10110160S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,209818.6,209818.6,0,0,209818.6,209818.6,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,26227,0,209818,0,0,0,236045,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11010010S",null,null,null,"강관 용접 배관","D15, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11010010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",2.9000000000000001E-2,0,0,229482,6654.9,0,0,229482,6654.9,null,null,"N","Y","",0]
["MBA11010010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.1999999999999999E-2,0,0,165545,3641.9,0,0,165545,3641.9,null,null,"N","Y","",0]
["MBA11010010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,205.9,205.9,0,0,0,0,205.9,205.9,null,null,"N","N",2,1]
["MBA11010010S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,13385.8,13385.8,0,0,13385.8,13385.8,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,205,0,13385,0,0,0,13590,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11010020S",null,null,null,"강관 용접 배관","D20, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11010020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",3.3000000000000002E-2,0,0,229482,7572.9,0,0,229482,7572.9,null,null,"N","Y","",0]
["MBA11010020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.3E-2,0,0,165545,3807.5,0,0,165545,3807.5,null,null,"N","Y","",0]
["MBA11010020S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,227.6,227.6,0,0,0,0,227.6,227.6,null,null,"N","N",2,1]
["MBA11010020S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,14794.5,14794.5,0,0,14794.5,14794.5,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,227,0,14794,0,0,0,15021,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11010030S",null,null,null,"강관 용접 배관","D25, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11010030S","노무","L001010101000039",null,"배관공","일반공사 직종","인",4.2999999999999997E-2,0,0,229482,9867.7000000000007,0,0,229482,9867.7000000000007,null,null,"N","Y","",0]
["MBA11010030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5999999999999999E-2,0,0,165545,4304.1000000000004,0,0,165545,4304.1000000000004,null,null,"N","Y","",0]
["MBA11010030S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,283.39999999999998,283.39999999999998,0,0,0,0,283.39999999999998,283.39999999999998,null,null,"N","N",2,1]
["MBA11010030S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,18423.3,18423.3,0,0,18423.3,18423.3,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,283,0,18423,0,0,0,18706,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11010040S",null,null,null,"강관 용접 배관","D32, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11010040S","노무","L001010101000039",null,"배관공","일반공사 직종","인",5.0999999999999997E-2,0,0,229482,11703.5,0,0,229482,11703.5,null,null,"N","Y","",0]
["MBA11010040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.9000000000000001E-2,0,0,165545,4800.8,0,0,165545,4800.8,null,null,"N","Y","",0]
["MBA11010040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,330,330,0,0,0,0,330,330,null,null,"N","N",2,1]
["MBA11010040S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,21455.5,21455.5,0,0,21455.5,21455.5,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,330,0,21455,0,0,0,21785,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11010050S",null,null,null,"강관 용접 배관","D40, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11010050S","노무","L001010101000039",null,"배관공","일반공사 직종","인",5.7000000000000002E-2,0,0,229482,13080.4,0,0,229482,13080.4,null,null,"N","Y","",0]
["MBA11010050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.1E-2,0,0,165545,5131.8,0,0,165545,5131.8,null,null,"N","Y","",0]
["MBA11010050S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,364.2,364.2,0,0,0,0,364.2,364.2,null,null,"N","N",2,1]
["MBA11010050S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,23675.8,23675.8,0,0,23675.8,23675.8,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,364,0,23675,0,0,0,24039,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11010060S",null,null,null,"강관 용접 배관","D50, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11010060S","노무","L001010101000039",null,"배관공","일반공사 직종","인",7.3999999999999996E-2,0,0,229482,16981.599999999999,0,0,229482,16981.599999999999,null,null,"N","Y","",0]
["MBA11010060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.6999999999999998E-2,0,0,165545,6125.1,0,0,165545,6125.1,null,null,"N","Y","",0]
["MBA11010060S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,462.1,462.1,0,0,0,0,462.1,462.1,null,null,"N","N",2,1]
["MBA11010060S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,30038.7,30038.7,0,0,30038.7,30038.7,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,462,0,30038,0,0,0,30500,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11010070S",null,null,null,"강관 용접 배관","D65, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11010070S","노무","L001010101000039",null,"배관공","일반공사 직종","인",8.7999999999999995E-2,0,0,229482,20194.400000000001,0,0,229482,20194.400000000001,null,null,"N","Y","",0]
["MBA11010070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.2000000000000003E-2,0,0,165545,6952.8,0,0,165545,6952.8,null,null,"N","Y","",0]
["MBA11010070S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,542.9,542.9,0,0,0,0,542.9,542.9,null,null,"N","N",2,1]
["MBA11010070S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,35291.300000000003,35291.300000000003,0,0,35291.300000000003,35291.300000000003,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,542,0,35291,0,0,0,35833,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11010080S",null,null,null,"강관 용접 배관","D80, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11010080S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.113,0,0,229482,25931.4,0,0,229482,25931.4,null,null,"N","Y","",0]
["MBA11010080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.0999999999999997E-2,0,0,165545,8442.7000000000007,0,0,165545,8442.7000000000007,null,null,"N","Y","",0]
["MBA11010080S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,687.4,687.4,0,0,0,0,687.4,687.4,null,null,"N","N",2,1]
["MBA11010080S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,44686.3,44686.3,0,0,44686.3,44686.3,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,687,0,44686,0,0,0,45373,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11010090S",null,null,null,"강관 용접 배관","D100, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11010090S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.155,0,0,229482,35569.699999999997,0,0,229482,35569.699999999997,null,null,"N","Y","",0]
["MBA11010090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.5000000000000002E-2,0,0,165545,10760.4,0,0,165545,10760.4,null,null,"N","Y","",0]
["MBA11010090S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,926.6,926.6,0,0,0,0,926.6,926.6,null,null,"N","N",2,1]
["MBA11010090S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,60229.1,60229.1,0,0,60229.1,60229.1,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,926,0,60229,0,0,0,61155,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11010100S",null,null,null,"강관 용접 배관","D125, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11010100S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.2,0,0,229482,45896.4,0,0,229482,45896.4,null,null,"N","Y","",0]
["MBA11010100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",8.1000000000000003E-2,0,0,165545,13409.1,0,0,165545,13409.1,null,null,"N","Y","",0]
["MBA11010100S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,1186.0999999999999,1186.0999999999999,0,0,0,0,1186.0999999999999,1186.0999999999999,null,null,"N","N",2,1]
["MBA11010100S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,77097.100000000006,77097.100000000006,0,0,77097.100000000006,77097.100000000006,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,1186,0,77097,0,0,0,78283,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11010110S",null,null,null,"강관 용접 배관","D150, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11010110S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.23599999999999999,0,0,229482,54157.7,0,0,229482,54157.7,null,null,"N","Y","",0]
["MBA11010110S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",9.2999999999999999E-2,0,0,165545,15395.6,0,0,165545,15395.6,null,null,"N","Y","",0]
["MBA11010110S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,1391,1391,0,0,0,0,1391,1391,null,null,"N","N",2,1]
["MBA11010110S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,90419.199999999997,90419.199999999997,0,0,90419.199999999997,90419.199999999997,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,1391,0,90419,0,0,0,91810,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11010120S",null,null,null,"강관 용접 배관","D200, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11010120S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.36499999999999999,0,0,229482,83760.899999999994,0,0,229482,83760.899999999994,null,null,"N","Y","",0]
["MBA11010120S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.13800000000000001,0,0,165545,22845.200000000001,0,0,165545,22845.200000000001,null,null,"N","Y","",0]
["MBA11010120S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,2132.1,2132.1,0,0,0,0,2132.1,2132.1,null,null,"N","N",2,1]
["MBA11010120S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,138587.9,138587.9,0,0,138587.9,138587.9,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,2132,0,138587,0,0,0,140719,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11010130S",null,null,null,"강관 용접 배관","D250, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11010130S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.48899999999999999,0,0,229482,112216.6,0,0,229482,112216.6,null,null,"N","Y","",0]
["MBA11010130S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.18099999999999999,0,0,165545,29963.599999999999,0,0,165545,29963.599999999999,null,null,"N","Y","",0]
["MBA11010130S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,2843.6,2843.6,0,0,0,0,2843.6,2843.6,null,null,"N","N",2,1]
["MBA11010130S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,184834.2,184834.2,0,0,184834.2,184834.2,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,2843,0,184834,0,0,0,187677,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11010140S",null,null,null,"강관 용접 배관","D300, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11010140S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.63400000000000001,0,0,229482,145491.5,0,0,229482,145491.5,null,null,"N","Y","",0]
["MBA11010140S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.23200000000000001,0,0,165545,38406.400000000001,0,0,165545,38406.400000000001,null,null,"N","Y","",0]
["MBA11010140S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,3677.9,3677.9,0,0,0,0,3677.9,3677.9,null,null,"N","N",2,1]
["MBA11010140S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,239067.2,239067.2,0,0,239067.2,239067.2,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,3677,0,239067,0,0,0,242744,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11010150S",null,null,null,"강관 용접 배관","D350, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11010150S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.76500000000000001,0,0,229482,175553.7,0,0,229482,175553.7,null,null,"N","Y","",0]
["MBA11010150S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.27700000000000002,0,0,165545,45855.9,0,0,165545,45855.9,null,null,"N","Y","",0]
["MBA11010150S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,4428.1000000000004,4428.1000000000004,0,0,0,0,4428.1000000000004,4428.1000000000004,null,null,"N","N",2,1]
["MBA11010150S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,287832.40000000002,287832.40000000002,0,0,287832.40000000002,287832.40000000002,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,4428,0,287832,0,0,0,292260,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11010160S",null,null,null,"강관 용접 배관","D400, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11010160S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.90700000000000003,0,0,229482,208140.1,0,0,229482,208140.1,null,null,"N","Y","",0]
["MBA11010160S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.32700000000000001,0,0,165545,54133.2,0,0,165545,54133.2,null,null,"N","Y","",0]
["MBA11010160S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,5245.4,5245.4,0,0,0,0,5245.4,5245.4,null,null,"N","N",2,1]
["MBA11010160S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,340955.2,340955.2,0,0,340955.2,340955.2,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,5245,0,340955,0,0,0,346200,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11110010S",null,null,null,"강관 용접 배관","D15, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11110010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",2.9000000000000001E-2,0,0,229482,6654.9,0,0,229482,6654.9,null,null,"N","Y","",0]
["MBA11110010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.1999999999999999E-2,0,0,165545,3641.9,0,0,165545,3641.9,null,null,"N","Y","",0]
["MBA11110010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1029.5999999999999,1029.5999999999999,0,0,0,0,1029.5999999999999,1029.5999999999999,null,null,"N","N",10,1]
["MBA11110010S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,11326.4,11326.4,0,0,11326.4,11326.4,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,1029,0,11326,0,0,0,12355,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11110020S",null,null,null,"강관 용접 배관","D20, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11110020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",3.3000000000000002E-2,0,0,229482,7572.9,0,0,229482,7572.9,null,null,"N","Y","",0]
["MBA11110020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.3E-2,0,0,165545,3807.5,0,0,165545,3807.5,null,null,"N","Y","",0]
["MBA11110020S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1138,1138,0,0,0,0,1138,1138,null,null,"N","N",10,1]
["MBA11110020S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,12518.4,12518.4,0,0,12518.4,12518.4,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,1138,0,12518,0,0,0,13656,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11110030S",null,null,null,"강관 용접 배관","D25, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11110030S","노무","L001010101000039",null,"배관공","일반공사 직종","인",4.2999999999999997E-2,0,0,229482,9867.7000000000007,0,0,229482,9867.7000000000007,null,null,"N","Y","",0]
["MBA11110030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5999999999999999E-2,0,0,165545,4304.1000000000004,0,0,165545,4304.1000000000004,null,null,"N","Y","",0]
["MBA11110030S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1417.1,1417.1,0,0,0,0,1417.1,1417.1,null,null,"N","N",10,1]
["MBA11110030S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,15588.9,15588.9,0,0,15588.9,15588.9,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,1417,0,15588,0,0,0,17005,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11110040S",null,null,null,"강관 용접 배관","D32, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11110040S","노무","L001010101000039",null,"배관공","일반공사 직종","인",5.0999999999999997E-2,0,0,229482,11703.5,0,0,229482,11703.5,null,null,"N","Y","",0]
["MBA11110040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.9000000000000001E-2,0,0,165545,4800.8,0,0,165545,4800.8,null,null,"N","Y","",0]
["MBA11110040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1650.4,1650.4,0,0,0,0,1650.4,1650.4,null,null,"N","N",10,1]
["MBA11110040S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,18154.7,18154.7,0,0,18154.7,18154.7,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,1650,0,18154,0,0,0,19804,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11110050S",null,null,null,"강관 용접 배관","D40, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11110050S","노무","L001010101000039",null,"배관공","일반공사 직종","인",5.7000000000000002E-2,0,0,229482,13080.4,0,0,229482,13080.4,null,null,"N","Y","",0]
["MBA11110050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.1E-2,0,0,165545,5131.8,0,0,165545,5131.8,null,null,"N","Y","",0]
["MBA11110050S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1821.2,1821.2,0,0,0,0,1821.2,1821.2,null,null,"N","N",10,1]
["MBA11110050S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,20033.400000000001,20033.400000000001,0,0,20033.400000000001,20033.400000000001,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,1821,0,20033,0,0,0,21854,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11110060S",null,null,null,"강관 용접 배관","D50, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11110060S","노무","L001010101000039",null,"배관공","일반공사 직종","인",7.3999999999999996E-2,0,0,229482,16981.599999999999,0,0,229482,16981.599999999999,null,null,"N","Y","",0]
["MBA11110060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.6999999999999998E-2,0,0,165545,6125.1,0,0,165545,6125.1,null,null,"N","Y","",0]
["MBA11110060S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,2310.6,2310.6,0,0,0,0,2310.6,2310.6,null,null,"N","N",10,1]
["MBA11110060S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,25417.3,25417.3,0,0,25417.3,25417.3,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,2310,0,25417,0,0,0,27727,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11110070S",null,null,null,"강관 용접 배관","D65, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11110070S","노무","L001010101000039",null,"배관공","일반공사 직종","인",8.7999999999999995E-2,0,0,229482,20194.400000000001,0,0,229482,20194.400000000001,null,null,"N","Y","",0]
["MBA11110070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.2000000000000003E-2,0,0,165545,6952.8,0,0,165545,6952.8,null,null,"N","Y","",0]
["MBA11110070S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,2714.7,2714.7,0,0,0,0,2714.7,2714.7,null,null,"N","N",10,1]
["MBA11110070S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,29861.9,29861.9,0,0,29861.9,29861.9,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,2714,0,29861,0,0,0,32575,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11110080S",null,null,null,"강관 용접 배관","D80, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11110080S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.113,0,0,229482,25931.4,0,0,229482,25931.4,null,null,"N","Y","",0]
["MBA11110080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.0999999999999997E-2,0,0,165545,8442.7000000000007,0,0,165545,8442.7000000000007,null,null,"N","Y","",0]
["MBA11110080S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,3437.4,3437.4,0,0,0,0,3437.4,3437.4,null,null,"N","N",10,1]
["MBA11110080S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,37811.5,37811.5,0,0,37811.5,37811.5,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,3437,0,37811,0,0,0,41248,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11110090S",null,null,null,"강관 용접 배관","D100, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11110090S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.155,0,0,229482,35569.699999999997,0,0,229482,35569.699999999997,null,null,"N","Y","",0]
["MBA11110090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.5000000000000002E-2,0,0,165545,10760.4,0,0,165545,10760.4,null,null,"N","Y","",0]
["MBA11110090S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,4633,4633,0,0,0,0,4633,4633,null,null,"N","N",10,1]
["MBA11110090S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,50963.1,50963.1,0,0,50963.1,50963.1,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,4633,0,50963,0,0,0,55596,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11110100S",null,null,null,"강관 용접 배관","D125, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11110100S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.2,0,0,229482,45896.4,0,0,229482,45896.4,null,null,"N","Y","",0]
["MBA11110100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",8.1000000000000003E-2,0,0,165545,13409.1,0,0,165545,13409.1,null,null,"N","Y","",0]
["MBA11110100S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,5930.5,5930.5,0,0,0,0,5930.5,5930.5,null,null,"N","N",10,1]
["MBA11110100S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,65236,65236,0,0,65236,65236,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,5930,0,65236,0,0,0,71166,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11110110S",null,null,null,"강관 용접 배관","D150, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11110110S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.23599999999999999,0,0,229482,54157.7,0,0,229482,54157.7,null,null,"N","Y","",0]
["MBA11110110S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",9.2999999999999999E-2,0,0,165545,15395.6,0,0,165545,15395.6,null,null,"N","Y","",0]
["MBA11110110S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,6955.3,6955.3,0,0,0,0,6955.3,6955.3,null,null,"N","N",10,1]
["MBA11110110S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,76508.600000000006,76508.600000000006,0,0,76508.600000000006,76508.600000000006,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,6955,0,76508,0,0,0,83463,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11110120S",null,null,null,"강관 용접 배관","D200, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11110120S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.36499999999999999,0,0,229482,83760.899999999994,0,0,229482,83760.899999999994,null,null,"N","Y","",0]
["MBA11110120S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.13800000000000001,0,0,165545,22845.200000000001,0,0,165545,22845.200000000001,null,null,"N","Y","",0]
["MBA11110120S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,10660.6,10660.6,0,0,0,0,10660.6,10660.6,null,null,"N","N",10,1]
["MBA11110120S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,117266.7,117266.7,0,0,117266.7,117266.7,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,10660,0,117266,0,0,0,127926,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11110130S",null,null,null,"강관 용접 배관","D250, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11110130S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.48899999999999999,0,0,229482,112216.6,0,0,229482,112216.6,null,null,"N","Y","",0]
["MBA11110130S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.18099999999999999,0,0,165545,29963.599999999999,0,0,165545,29963.599999999999,null,null,"N","Y","",0]
["MBA11110130S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,14218,14218,0,0,0,0,14218,14218,null,null,"N","N",10,1]
["MBA11110130S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,156398.20000000001,156398.20000000001,0,0,156398.20000000001,156398.20000000001,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,14218,0,156398,0,0,0,170616,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11110140S",null,null,null,"강관 용접 배관","D300, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11110140S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.63400000000000001,0,0,229482,145491.5,0,0,229482,145491.5,null,null,"N","Y","",0]
["MBA11110140S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.23200000000000001,0,0,165545,38406.400000000001,0,0,165545,38406.400000000001,null,null,"N","Y","",0]
["MBA11110140S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,18389.7,18389.7,0,0,0,0,18389.7,18389.7,null,null,"N","N",10,1]
["MBA11110140S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,202287.6,202287.6,0,0,202287.6,202287.6,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,18389,0,202287,0,0,0,220676,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11110150S",null,null,null,"강관 용접 배관","D350, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11110150S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.76500000000000001,0,0,229482,175553.7,0,0,229482,175553.7,null,null,"N","Y","",0]
["MBA11110150S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.27700000000000002,0,0,165545,45855.9,0,0,165545,45855.9,null,null,"N","Y","",0]
["MBA11110150S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,22140.9,22140.9,0,0,0,0,22140.9,22140.9,null,null,"N","N",10,1]
["MBA11110150S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,243550.5,243550.5,0,0,243550.5,243550.5,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,22140,0,243550,0,0,0,265690,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11110160S",null,null,null,"강관 용접 배관","D400, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA11110160S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.90700000000000003,0,0,229482,208140.1,0,0,229482,208140.1,null,null,"N","Y","",0]
["MBA11110160S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.32700000000000001,0,0,165545,54133.2,0,0,165545,54133.2,null,null,"N","Y","",0]
["MBA11110160S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,26227.3,26227.3,0,0,0,0,26227.3,26227.3,null,null,"N","N",10,1]
["MBA11110160S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,288500.59999999998,288500.59999999998,0,0,288500.59999999998,288500.59999999998,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,26227,0,288500,0,0,0,314727,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12010010S",null,null,null,"강관 용접 배관","D15, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12010010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",2.9000000000000001E-2,0,0,229482,6654.9,0,0,229482,6654.9,null,null,"N","Y","",0]
["MBA12010010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.1999999999999999E-2,0,0,165545,3641.9,0,0,165545,3641.9,null,null,"N","Y","",0]
["MBA12010010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,205.9,205.9,0,0,0,0,205.9,205.9,null,null,"N","N",2,1]
["MBA12010010S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,12356.1,12356.1,0,0,12356.1,12356.1,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,205,0,12356,0,0,0,12561,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12010020S",null,null,null,"강관 용접 배관","D20, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12010020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",3.3000000000000002E-2,0,0,229482,7572.9,0,0,229482,7572.9,null,null,"N","Y","",0]
["MBA12010020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.3E-2,0,0,165545,3807.5,0,0,165545,3807.5,null,null,"N","Y","",0]
["MBA12010020S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,227.6,227.6,0,0,0,0,227.6,227.6,null,null,"N","N",2,1]
["MBA12010020S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,13656.4,13656.4,0,0,13656.4,13656.4,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,227,0,13656,0,0,0,13883,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12010030S",null,null,null,"강관 용접 배관","D25, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12010030S","노무","L001010101000039",null,"배관공","일반공사 직종","인",4.2999999999999997E-2,0,0,229482,9867.7000000000007,0,0,229482,9867.7000000000007,null,null,"N","Y","",0]
["MBA12010030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5999999999999999E-2,0,0,165545,4304.1000000000004,0,0,165545,4304.1000000000004,null,null,"N","Y","",0]
["MBA12010030S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,283.39999999999998,283.39999999999998,0,0,0,0,283.39999999999998,283.39999999999998,null,null,"N","N",2,1]
["MBA12010030S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,17006.099999999999,17006.099999999999,0,0,17006.099999999999,17006.099999999999,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,283,0,17006,0,0,0,17289,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12010040S",null,null,null,"강관 용접 배관","D32, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12010040S","노무","L001010101000039",null,"배관공","일반공사 직종","인",5.0999999999999997E-2,0,0,229482,11703.5,0,0,229482,11703.5,null,null,"N","Y","",0]
["MBA12010040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.9000000000000001E-2,0,0,165545,4800.8,0,0,165545,4800.8,null,null,"N","Y","",0]
["MBA12010040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,330,330,0,0,0,0,330,330,null,null,"N","N",2,1]
["MBA12010040S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,19805.099999999999,19805.099999999999,0,0,19805.099999999999,19805.099999999999,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,330,0,19805,0,0,0,20135,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12010050S",null,null,null,"강관 용접 배관","D40, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12010050S","노무","L001010101000039",null,"배관공","일반공사 직종","인",5.7000000000000002E-2,0,0,229482,13080.4,0,0,229482,13080.4,null,null,"N","Y","",0]
["MBA12010050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.1E-2,0,0,165545,5131.8,0,0,165545,5131.8,null,null,"N","Y","",0]
["MBA12010050S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,364.2,364.2,0,0,0,0,364.2,364.2,null,null,"N","N",2,1]
["MBA12010050S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,21854.6,21854.6,0,0,21854.6,21854.6,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,364,0,21854,0,0,0,22218,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12010060S",null,null,null,"강관 용접 배관","D50, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12010060S","노무","L001010101000039",null,"배관공","일반공사 직종","인",7.3999999999999996E-2,0,0,229482,16981.599999999999,0,0,229482,16981.599999999999,null,null,"N","Y","",0]
["MBA12010060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.6999999999999998E-2,0,0,165545,6125.1,0,0,165545,6125.1,null,null,"N","Y","",0]
["MBA12010060S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,462.1,462.1,0,0,0,0,462.1,462.1,null,null,"N","N",2,1]
["MBA12010060S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,27728,27728,0,0,27728,27728,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,462,0,27728,0,0,0,28190,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12010070S",null,null,null,"강관 용접 배관","D65, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12010070S","노무","L001010101000039",null,"배관공","일반공사 직종","인",8.7999999999999995E-2,0,0,229482,20194.400000000001,0,0,229482,20194.400000000001,null,null,"N","Y","",0]
["MBA12010070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.2000000000000003E-2,0,0,165545,6952.8,0,0,165545,6952.8,null,null,"N","Y","",0]
["MBA12010070S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,542.9,542.9,0,0,0,0,542.9,542.9,null,null,"N","N",2,1]
["MBA12010070S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,32576.6,32576.6,0,0,32576.6,32576.6,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,542,0,32576,0,0,0,33118,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12010080S",null,null,null,"강관 용접 배관","D80, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12010080S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.113,0,0,229482,25931.4,0,0,229482,25931.4,null,null,"N","Y","",0]
["MBA12010080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.0999999999999997E-2,0,0,165545,8442.7000000000007,0,0,165545,8442.7000000000007,null,null,"N","Y","",0]
["MBA12010080S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,687.4,687.4,0,0,0,0,687.4,687.4,null,null,"N","N",2,1]
["MBA12010080S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,41248.9,41248.9,0,0,41248.9,41248.9,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,687,0,41248,0,0,0,41935,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12010090S",null,null,null,"강관 용접 배관","D100, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12010090S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.155,0,0,229482,35569.699999999997,0,0,229482,35569.699999999997,null,null,"N","Y","",0]
["MBA12010090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.5000000000000002E-2,0,0,165545,10760.4,0,0,165545,10760.4,null,null,"N","Y","",0]
["MBA12010090S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,926.6,926.6,0,0,0,0,926.6,926.6,null,null,"N","N",2,1]
["MBA12010090S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,55596.1,55596.1,0,0,55596.1,55596.1,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,926,0,55596,0,0,0,56522,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12010100S",null,null,null,"강관 용접 배관","D125, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12010100S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.2,0,0,229482,45896.4,0,0,229482,45896.4,null,null,"N","Y","",0]
["MBA12010100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",8.1000000000000003E-2,0,0,165545,13409.1,0,0,165545,13409.1,null,null,"N","Y","",0]
["MBA12010100S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,1186.0999999999999,1186.0999999999999,0,0,0,0,1186.0999999999999,1186.0999999999999,null,null,"N","N",2,1]
["MBA12010100S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,71166.600000000006,71166.600000000006,0,0,71166.600000000006,71166.600000000006,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,1186,0,71166,0,0,0,72352,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12010110S",null,null,null,"강관 용접 배관","D150, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12010110S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.23599999999999999,0,0,229482,54157.7,0,0,229482,54157.7,null,null,"N","Y","",0]
["MBA12010110S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",9.2999999999999999E-2,0,0,165545,15395.6,0,0,165545,15395.6,null,null,"N","Y","",0]
["MBA12010110S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,1391,1391,0,0,0,0,1391,1391,null,null,"N","N",2,1]
["MBA12010110S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,83463.899999999994,83463.899999999994,0,0,83463.899999999994,83463.899999999994,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,1391,0,83463,0,0,0,84854,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12010120S",null,null,null,"강관 용접 배관","D200, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12010120S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.36499999999999999,0,0,229482,83760.899999999994,0,0,229482,83760.899999999994,null,null,"N","Y","",0]
["MBA12010120S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.13800000000000001,0,0,165545,22845.200000000001,0,0,165545,22845.200000000001,null,null,"N","Y","",0]
["MBA12010120S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,2132.1,2132.1,0,0,0,0,2132.1,2132.1,null,null,"N","N",2,1]
["MBA12010120S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,127927.3,127927.3,0,0,127927.3,127927.3,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,2132,0,127927,0,0,0,130059,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12010130S",null,null,null,"강관 용접 배관","D250, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12010130S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.48899999999999999,0,0,229482,112216.6,0,0,229482,112216.6,null,null,"N","Y","",0]
["MBA12010130S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.18099999999999999,0,0,165545,29963.599999999999,0,0,165545,29963.599999999999,null,null,"N","Y","",0]
["MBA12010130S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,2843.6,2843.6,0,0,0,0,2843.6,2843.6,null,null,"N","N",2,1]
["MBA12010130S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,170616.2,170616.2,0,0,170616.2,170616.2,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,2843,0,170616,0,0,0,173459,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12010140S",null,null,null,"강관 용접 배관","D300, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12010140S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.63400000000000001,0,0,229482,145491.5,0,0,229482,145491.5,null,null,"N","Y","",0]
["MBA12010140S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.23200000000000001,0,0,165545,38406.400000000001,0,0,165545,38406.400000000001,null,null,"N","Y","",0]
["MBA12010140S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,3677.9,3677.9,0,0,0,0,3677.9,3677.9,null,null,"N","N",2,1]
["MBA12010140S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,220677.4,220677.4,0,0,220677.4,220677.4,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,3677,0,220677,0,0,0,224354,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12010150S",null,null,null,"강관 용접 배관","D350, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12010150S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.76500000000000001,0,0,229482,175553.7,0,0,229482,175553.7,null,null,"N","Y","",0]
["MBA12010150S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.27700000000000002,0,0,165545,45855.9,0,0,165545,45855.9,null,null,"N","Y","",0]
["MBA12010150S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,4428.1000000000004,4428.1000000000004,0,0,0,0,4428.1000000000004,4428.1000000000004,null,null,"N","N",2,1]
["MBA12010150S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,265691.5,265691.5,0,0,265691.5,265691.5,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,4428,0,265691,0,0,0,270119,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12010160S",null,null,null,"강관 용접 배관","D400, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12010160S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.90700000000000003,0,0,229482,208140.1,0,0,229482,208140.1,null,null,"N","Y","",0]
["MBA12010160S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.32700000000000001,0,0,165545,54133.2,0,0,165545,54133.2,null,null,"N","Y","",0]
["MBA12010160S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,5245.4,5245.4,0,0,0,0,5245.4,5245.4,null,null,"N","N",2,1]
["MBA12010160S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,314727.90000000002,314727.90000000002,0,0,314727.90000000002,314727.90000000002,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,5245,0,314727,0,0,0,319972,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12110010S",null,null,null,"강관 용접 배관","D15, 화장실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12110010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",2.9000000000000001E-2,0,0,229482,6654.9,0,0,229482,6654.9,null,null,"N","Y","",0]
["MBA12110010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.1999999999999999E-2,0,0,165545,3641.9,0,0,165545,3641.9,null,null,"N","Y","",0]
["MBA12110010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1029.5999999999999,1029.5999999999999,0,0,0,0,1029.5999999999999,1029.5999999999999,null,null,"N","N",10,1]
["MBA12110010S","손료","RENT000000000002",null,"노무할증 20%증+20%감","노무비의 100%","식",1,0,0,10296.799999999999,10296.799999999999,0,0,10296.799999999999,10296.799999999999,null,null,"N","N",100,1]
[null,null,null,null,"[합 계]",null,null,0,0,1029,0,10296,0,0,0,11325,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12110020S",null,null,null,"강관 용접 배관","D20, 화장실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12110020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",3.3000000000000002E-2,0,0,229482,7572.9,0,0,229482,7572.9,null,null,"N","Y","",0]
["MBA12110020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.3E-2,0,0,165545,3807.5,0,0,165545,3807.5,null,null,"N","Y","",0]
["MBA12110020S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1138,1138,0,0,0,0,1138,1138,null,null,"N","N",10,1]
["MBA12110020S","손료","RENT000000000002",null,"노무할증 20%증+20%감","노무비의 100%","식",1,0,0,11380.4,11380.4,0,0,11380.4,11380.4,null,null,"N","N",100,1]
[null,null,null,null,"[합 계]",null,null,0,0,1138,0,11380,0,0,0,12518,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12110030S",null,null,null,"강관 용접 배관","D25, 화장실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12110030S","노무","L001010101000039",null,"배관공","일반공사 직종","인",4.2999999999999997E-2,0,0,229482,9867.7000000000007,0,0,229482,9867.7000000000007,null,null,"N","Y","",0]
["MBA12110030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5999999999999999E-2,0,0,165545,4304.1000000000004,0,0,165545,4304.1000000000004,null,null,"N","Y","",0]
["MBA12110030S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1417.1,1417.1,0,0,0,0,1417.1,1417.1,null,null,"N","N",10,1]
["MBA12110030S","손료","RENT000000000002",null,"노무할증 20%증+20%감","노무비의 100%","식",1,0,0,14171.8,14171.8,0,0,14171.8,14171.8,null,null,"N","N",100,1]
[null,null,null,null,"[합 계]",null,null,0,0,1417,0,14171,0,0,0,15588,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12110040S",null,null,null,"강관 용접 배관","D32, 화장실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12110040S","노무","L001010101000039",null,"배관공","일반공사 직종","인",5.0999999999999997E-2,0,0,229482,11703.5,0,0,229482,11703.5,null,null,"N","Y","",0]
["MBA12110040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.9000000000000001E-2,0,0,165545,4800.8,0,0,165545,4800.8,null,null,"N","Y","",0]
["MBA12110040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1650.4,1650.4,0,0,0,0,1650.4,1650.4,null,null,"N","N",10,1]
["MBA12110040S","손료","RENT000000000002",null,"노무할증 20%증+20%감","노무비의 100%","식",1,0,0,16504.3,16504.3,0,0,16504.3,16504.3,null,null,"N","N",100,1]
[null,null,null,null,"[합 계]",null,null,0,0,1650,0,16504,0,0,0,18154,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12110050S",null,null,null,"강관 용접 배관","D40, 화장실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12110050S","노무","L001010101000039",null,"배관공","일반공사 직종","인",5.7000000000000002E-2,0,0,229482,13080.4,0,0,229482,13080.4,null,null,"N","Y","",0]
["MBA12110050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.1E-2,0,0,165545,5131.8,0,0,165545,5131.8,null,null,"N","Y","",0]
["MBA12110050S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1821.2,1821.2,0,0,0,0,1821.2,1821.2,null,null,"N","N",10,1]
["MBA12110050S","손료","RENT000000000002",null,"노무할증 20%증+20%감","노무비의 100%","식",1,0,0,18212.2,18212.2,0,0,18212.2,18212.2,null,null,"N","N",100,1]
[null,null,null,null,"[합 계]",null,null,0,0,1821,0,18212,0,0,0,20033,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12110060S",null,null,null,"강관 용접 배관","D50, 화장실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12110060S","노무","L001010101000039",null,"배관공","일반공사 직종","인",7.3999999999999996E-2,0,0,229482,16981.599999999999,0,0,229482,16981.599999999999,null,null,"N","Y","",0]
["MBA12110060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.6999999999999998E-2,0,0,165545,6125.1,0,0,165545,6125.1,null,null,"N","Y","",0]
["MBA12110060S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,2310.6,2310.6,0,0,0,0,2310.6,2310.6,null,null,"N","N",10,1]
["MBA12110060S","손료","RENT000000000002",null,"노무할증 20%증+20%감","노무비의 100%","식",1,0,0,23106.7,23106.7,0,0,23106.7,23106.7,null,null,"N","N",100,1]
[null,null,null,null,"[합 계]",null,null,0,0,2310,0,23106,0,0,0,25416,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12110070S",null,null,null,"강관 용접 배관","D65, 화장실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12110070S","노무","L001010101000039",null,"배관공","일반공사 직종","인",8.7999999999999995E-2,0,0,229482,20194.400000000001,0,0,229482,20194.400000000001,null,null,"N","Y","",0]
["MBA12110070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.2000000000000003E-2,0,0,165545,6952.8,0,0,165545,6952.8,null,null,"N","Y","",0]
["MBA12110070S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,2714.7,2714.7,0,0,0,0,2714.7,2714.7,null,null,"N","N",10,1]
["MBA12110070S","손료","RENT000000000002",null,"노무할증 20%증+20%감","노무비의 100%","식",1,0,0,27147.200000000001,27147.200000000001,0,0,27147.200000000001,27147.200000000001,null,null,"N","N",100,1]
[null,null,null,null,"[합 계]",null,null,0,0,2714,0,27147,0,0,0,29861,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12110080S",null,null,null,"강관 용접 배관","D80, 화장실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12110080S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.113,0,0,229482,25931.4,0,0,229482,25931.4,null,null,"N","Y","",0]
["MBA12110080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.0999999999999997E-2,0,0,165545,8442.7000000000007,0,0,165545,8442.7000000000007,null,null,"N","Y","",0]
["MBA12110080S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,3437.4,3437.4,0,0,0,0,3437.4,3437.4,null,null,"N","N",10,1]
["MBA12110080S","손료","RENT000000000002",null,"노무할증 20%증+20%감","노무비의 100%","식",1,0,0,34374.1,34374.1,0,0,34374.1,34374.1,null,null,"N","N",100,1]
[null,null,null,null,"[합 계]",null,null,0,0,3437,0,34374,0,0,0,37811,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12110090S",null,null,null,"강관 용접 배관","D100, 화장실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12110090S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.155,0,0,229482,35569.699999999997,0,0,229482,35569.699999999997,null,null,"N","Y","",0]
["MBA12110090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.5000000000000002E-2,0,0,165545,10760.4,0,0,165545,10760.4,null,null,"N","Y","",0]
["MBA12110090S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,4633,4633,0,0,0,0,4633,4633,null,null,"N","N",10,1]
["MBA12110090S","손료","RENT000000000002",null,"노무할증 20%증+20%감","노무비의 100%","식",1,0,0,46330.1,46330.1,0,0,46330.1,46330.1,null,null,"N","N",100,1]
[null,null,null,null,"[합 계]",null,null,0,0,4633,0,46330,0,0,0,50963,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12110100S",null,null,null,"강관 용접 배관","D125, 화장실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12110100S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.2,0,0,229482,45896.4,0,0,229482,45896.4,null,null,"N","Y","",0]
["MBA12110100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",8.1000000000000003E-2,0,0,165545,13409.1,0,0,165545,13409.1,null,null,"N","Y","",0]
["MBA12110100S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,5930.5,5930.5,0,0,0,0,5930.5,5930.5,null,null,"N","N",10,1]
["MBA12110100S","손료","RENT000000000002",null,"노무할증 20%증+20%감","노무비의 100%","식",1,0,0,59305.5,59305.5,0,0,59305.5,59305.5,null,null,"N","N",100,1]
[null,null,null,null,"[합 계]",null,null,0,0,5930,0,59305,0,0,0,65235,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12110110S",null,null,null,"강관 용접 배관","D150, 화장실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12110110S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.23599999999999999,0,0,229482,54157.7,0,0,229482,54157.7,null,null,"N","Y","",0]
["MBA12110110S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",9.2999999999999999E-2,0,0,165545,15395.6,0,0,165545,15395.6,null,null,"N","Y","",0]
["MBA12110110S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,6955.3,6955.3,0,0,0,0,6955.3,6955.3,null,null,"N","N",10,1]
["MBA12110110S","손료","RENT000000000002",null,"노무할증 20%증+20%감","노무비의 100%","식",1,0,0,69553.3,69553.3,0,0,69553.3,69553.3,null,null,"N","N",100,1]
[null,null,null,null,"[합 계]",null,null,0,0,6955,0,69553,0,0,0,76508,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12110120S",null,null,null,"강관 용접 배관","D200, 화장실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12110120S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.36499999999999999,0,0,229482,83760.899999999994,0,0,229482,83760.899999999994,null,null,"N","Y","",0]
["MBA12110120S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.13800000000000001,0,0,165545,22845.200000000001,0,0,165545,22845.200000000001,null,null,"N","Y","",0]
["MBA12110120S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,10660.6,10660.6,0,0,0,0,10660.6,10660.6,null,null,"N","N",10,1]
["MBA12110120S","손료","RENT000000000002",null,"노무할증 20%증+20%감","노무비의 100%","식",1,0,0,106606.1,106606.1,0,0,106606.1,106606.1,null,null,"N","N",100,1]
[null,null,null,null,"[합 계]",null,null,0,0,10660,0,106606,0,0,0,117266,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12110130S",null,null,null,"강관 용접 배관","D250, 화장실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12110130S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.48899999999999999,0,0,229482,112216.6,0,0,229482,112216.6,null,null,"N","Y","",0]
["MBA12110130S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.18099999999999999,0,0,165545,29963.599999999999,0,0,165545,29963.599999999999,null,null,"N","Y","",0]
["MBA12110130S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,14218,14218,0,0,0,0,14218,14218,null,null,"N","N",10,1]
["MBA12110130S","손료","RENT000000000002",null,"노무할증 20%증+20%감","노무비의 100%","식",1,0,0,142180.20000000001,142180.20000000001,0,0,142180.20000000001,142180.20000000001,null,null,"N","N",100,1]
[null,null,null,null,"[합 계]",null,null,0,0,14218,0,142180,0,0,0,156398,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12110140S",null,null,null,"강관 용접 배관","D300, 화장실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12110140S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.63400000000000001,0,0,229482,145491.5,0,0,229482,145491.5,null,null,"N","Y","",0]
["MBA12110140S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.23200000000000001,0,0,165545,38406.400000000001,0,0,165545,38406.400000000001,null,null,"N","Y","",0]
["MBA12110140S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,18389.7,18389.7,0,0,0,0,18389.7,18389.7,null,null,"N","N",10,1]
["MBA12110140S","손료","RENT000000000002",null,"노무할증 20%증+20%감","노무비의 100%","식",1,0,0,183897.9,183897.9,0,0,183897.9,183897.9,null,null,"N","N",100,1]
[null,null,null,null,"[합 계]",null,null,0,0,18389,0,183897,0,0,0,202286,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12110150S",null,null,null,"강관 용접 배관","D350, 화장실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12110150S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.76500000000000001,0,0,229482,175553.7,0,0,229482,175553.7,null,null,"N","Y","",0]
["MBA12110150S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.27700000000000002,0,0,165545,45855.9,0,0,165545,45855.9,null,null,"N","Y","",0]
["MBA12110150S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,22140.9,22140.9,0,0,0,0,22140.9,22140.9,null,null,"N","N",10,1]
["MBA12110150S","손료","RENT000000000002",null,"노무할증 20%증+20%감","노무비의 100%","식",1,0,0,221409.6,221409.6,0,0,221409.6,221409.6,null,null,"N","N",100,1]
[null,null,null,null,"[합 계]",null,null,0,0,22140,0,221409,0,0,0,243549,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12110160S",null,null,null,"강관 용접 배관","D400, 화장실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA12110160S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.90700000000000003,0,0,229482,208140.1,0,0,229482,208140.1,null,null,"N","Y","",0]
["MBA12110160S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.32700000000000001,0,0,165545,54133.2,0,0,165545,54133.2,null,null,"N","Y","",0]
["MBA12110160S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,26227.3,26227.3,0,0,0,0,26227.3,26227.3,null,null,"N","N",10,1]
["MBA12110160S","손료","RENT000000000002",null,"노무할증 20%증+20%감","노무비의 100%","식",1,0,0,262273.3,262273.3,0,0,262273.3,262273.3,null,null,"N","N",100,1]
[null,null,null,null,"[합 계]",null,null,0,0,26227,0,262273,0,0,0,288500,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13010010S",null,null,null,"강관 용접 배관","D15, 옥외배관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13010010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",2.9000000000000001E-2,0,0,229482,6654.9,0,0,229482,6654.9,null,null,"N","Y","",0]
["MBA13010010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.1999999999999999E-2,0,0,165545,3641.9,0,0,165545,3641.9,null,null,"N","Y","",0]
["MBA13010010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,205.9,205.9,0,0,0,0,205.9,205.9,null,null,"N","N",2,1]
["MBA13010010S","손료","RENT000000000002",null,"노무할증 10%감","노무비의 90%","식",1,0,0,9267.1,9267.1,0,0,9267.1,9267.1,null,null,"N","N",90,1]
[null,null,null,null,"[합 계]",null,null,0,0,205,0,9267,0,0,0,9472,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13010020S",null,null,null,"강관 용접 배관","D20, 옥외배관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13010020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",3.3000000000000002E-2,0,0,229482,7572.9,0,0,229482,7572.9,null,null,"N","Y","",0]
["MBA13010020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.3E-2,0,0,165545,3807.5,0,0,165545,3807.5,null,null,"N","Y","",0]
["MBA13010020S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,227.6,227.6,0,0,0,0,227.6,227.6,null,null,"N","N",2,1]
["MBA13010020S","손료","RENT000000000002",null,"노무할증 10%감","노무비의 90%","식",1,0,0,10242.299999999999,10242.299999999999,0,0,10242.299999999999,10242.299999999999,null,null,"N","N",90,1]
[null,null,null,null,"[합 계]",null,null,0,0,227,0,10242,0,0,0,10469,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13010030S",null,null,null,"강관 용접 배관","D25, 옥외배관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13010030S","노무","L001010101000039",null,"배관공","일반공사 직종","인",4.2999999999999997E-2,0,0,229482,9867.7000000000007,0,0,229482,9867.7000000000007,null,null,"N","Y","",0]
["MBA13010030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5999999999999999E-2,0,0,165545,4304.1000000000004,0,0,165545,4304.1000000000004,null,null,"N","Y","",0]
["MBA13010030S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,283.39999999999998,283.39999999999998,0,0,0,0,283.39999999999998,283.39999999999998,null,null,"N","N",2,1]
["MBA13010030S","손료","RENT000000000002",null,"노무할증 10%감","노무비의 90%","식",1,0,0,12754.6,12754.6,0,0,12754.6,12754.6,null,null,"N","N",90,1]
[null,null,null,null,"[합 계]",null,null,0,0,283,0,12754,0,0,0,13037,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13010040S",null,null,null,"강관 용접 배관","D32, 옥외배관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13010040S","노무","L001010101000039",null,"배관공","일반공사 직종","인",5.0999999999999997E-2,0,0,229482,11703.5,0,0,229482,11703.5,null,null,"N","Y","",0]
["MBA13010040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.9000000000000001E-2,0,0,165545,4800.8,0,0,165545,4800.8,null,null,"N","Y","",0]
["MBA13010040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,330,330,0,0,0,0,330,330,null,null,"N","N",2,1]
["MBA13010040S","손료","RENT000000000002",null,"노무할증 10%감","노무비의 90%","식",1,0,0,14853.8,14853.8,0,0,14853.8,14853.8,null,null,"N","N",90,1]
[null,null,null,null,"[합 계]",null,null,0,0,330,0,14853,0,0,0,15183,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13010050S",null,null,null,"강관 용접 배관","D40, 옥외배관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13010050S","노무","L001010101000039",null,"배관공","일반공사 직종","인",5.7000000000000002E-2,0,0,229482,13080.4,0,0,229482,13080.4,null,null,"N","Y","",0]
["MBA13010050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.1E-2,0,0,165545,5131.8,0,0,165545,5131.8,null,null,"N","Y","",0]
["MBA13010050S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,364.2,364.2,0,0,0,0,364.2,364.2,null,null,"N","N",2,1]
["MBA13010050S","손료","RENT000000000002",null,"노무할증 10%감","노무비의 90%","식",1,0,0,16390.900000000001,16390.900000000001,0,0,16390.900000000001,16390.900000000001,null,null,"N","N",90,1]
[null,null,null,null,"[합 계]",null,null,0,0,364,0,16390,0,0,0,16754,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13010060S",null,null,null,"강관 용접 배관","D50, 옥외배관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13010060S","노무","L001010101000039",null,"배관공","일반공사 직종","인",7.3999999999999996E-2,0,0,229482,16981.599999999999,0,0,229482,16981.599999999999,null,null,"N","Y","",0]
["MBA13010060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.6999999999999998E-2,0,0,165545,6125.1,0,0,165545,6125.1,null,null,"N","Y","",0]
["MBA13010060S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,462.1,462.1,0,0,0,0,462.1,462.1,null,null,"N","N",2,1]
["MBA13010060S","손료","RENT000000000002",null,"노무할증 10%감","노무비의 90%","식",1,0,0,20796,20796,0,0,20796,20796,null,null,"N","N",90,1]
[null,null,null,null,"[합 계]",null,null,0,0,462,0,20796,0,0,0,21258,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13010070S",null,null,null,"강관 용접 배관","D65, 옥외배관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13010070S","노무","L001010101000039",null,"배관공","일반공사 직종","인",8.7999999999999995E-2,0,0,229482,20194.400000000001,0,0,229482,20194.400000000001,null,null,"N","Y","",0]
["MBA13010070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.2000000000000003E-2,0,0,165545,6952.8,0,0,165545,6952.8,null,null,"N","Y","",0]
["MBA13010070S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,542.9,542.9,0,0,0,0,542.9,542.9,null,null,"N","N",2,1]
["MBA13010070S","손료","RENT000000000002",null,"노무할증 10%감","노무비의 90%","식",1,0,0,24432.400000000001,24432.400000000001,0,0,24432.400000000001,24432.400000000001,null,null,"N","N",90,1]
[null,null,null,null,"[합 계]",null,null,0,0,542,0,24432,0,0,0,24974,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13010080S",null,null,null,"강관 용접 배관","D80, 옥외배관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13010080S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.113,0,0,229482,25931.4,0,0,229482,25931.4,null,null,"N","Y","",0]
["MBA13010080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.0999999999999997E-2,0,0,165545,8442.7000000000007,0,0,165545,8442.7000000000007,null,null,"N","Y","",0]
["MBA13010080S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,687.4,687.4,0,0,0,0,687.4,687.4,null,null,"N","N",2,1]
["MBA13010080S","손료","RENT000000000002",null,"노무할증 10%감","노무비의 90%","식",1,0,0,30936.6,30936.6,0,0,30936.6,30936.6,null,null,"N","N",90,1]
[null,null,null,null,"[합 계]",null,null,0,0,687,0,30936,0,0,0,31623,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13010090S",null,null,null,"강관 용접 배관","D100, 옥외배관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13010090S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.155,0,0,229482,35569.699999999997,0,0,229482,35569.699999999997,null,null,"N","Y","",0]
["MBA13010090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.5000000000000002E-2,0,0,165545,10760.4,0,0,165545,10760.4,null,null,"N","Y","",0]
["MBA13010090S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,926.6,926.6,0,0,0,0,926.6,926.6,null,null,"N","N",2,1]
["MBA13010090S","손료","RENT000000000002",null,"노무할증 10%감","노무비의 90%","식",1,0,0,41697,41697,0,0,41697,41697,null,null,"N","N",90,1]
[null,null,null,null,"[합 계]",null,null,0,0,926,0,41697,0,0,0,42623,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13010100S",null,null,null,"강관 용접 배관","D125, 옥외배관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13010100S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.2,0,0,229482,45896.4,0,0,229482,45896.4,null,null,"N","Y","",0]
["MBA13010100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",8.1000000000000003E-2,0,0,165545,13409.1,0,0,165545,13409.1,null,null,"N","Y","",0]
["MBA13010100S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,1186.0999999999999,1186.0999999999999,0,0,0,0,1186.0999999999999,1186.0999999999999,null,null,"N","N",2,1]
["MBA13010100S","손료","RENT000000000002",null,"노무할증 10%감","노무비의 90%","식",1,0,0,53374.9,53374.9,0,0,53374.9,53374.9,null,null,"N","N",90,1]
[null,null,null,null,"[합 계]",null,null,0,0,1186,0,53374,0,0,0,54560,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13010110S",null,null,null,"강관 용접 배관","D150, 옥외배관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13010110S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.23599999999999999,0,0,229482,54157.7,0,0,229482,54157.7,null,null,"N","Y","",0]
["MBA13010110S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",9.2999999999999999E-2,0,0,165545,15395.6,0,0,165545,15395.6,null,null,"N","Y","",0]
["MBA13010110S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,1391,1391,0,0,0,0,1391,1391,null,null,"N","N",2,1]
["MBA13010110S","손료","RENT000000000002",null,"노무할증 10%감","노무비의 90%","식",1,0,0,62597.9,62597.9,0,0,62597.9,62597.9,null,null,"N","N",90,1]
[null,null,null,null,"[합 계]",null,null,0,0,1391,0,62597,0,0,0,63988,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13010120S",null,null,null,"강관 용접 배관","D200, 옥외배관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13010120S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.36499999999999999,0,0,229482,83760.899999999994,0,0,229482,83760.899999999994,null,null,"N","Y","",0]
["MBA13010120S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.13800000000000001,0,0,165545,22845.200000000001,0,0,165545,22845.200000000001,null,null,"N","Y","",0]
["MBA13010120S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,2132.1,2132.1,0,0,0,0,2132.1,2132.1,null,null,"N","N",2,1]
["MBA13010120S","손료","RENT000000000002",null,"노무할증 10%감","노무비의 90%","식",1,0,0,95945.4,95945.4,0,0,95945.4,95945.4,null,null,"N","N",90,1]
[null,null,null,null,"[합 계]",null,null,0,0,2132,0,95945,0,0,0,98077,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13010130S",null,null,null,"강관 용접 배관","D250, 옥외배관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13010130S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.48899999999999999,0,0,229482,112216.6,0,0,229482,112216.6,null,null,"N","Y","",0]
["MBA13010130S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.18099999999999999,0,0,165545,29963.599999999999,0,0,165545,29963.599999999999,null,null,"N","Y","",0]
["MBA13010130S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,2843.6,2843.6,0,0,0,0,2843.6,2843.6,null,null,"N","N",2,1]
["MBA13010130S","손료","RENT000000000002",null,"노무할증 10%감","노무비의 90%","식",1,0,0,127962.1,127962.1,0,0,127962.1,127962.1,null,null,"N","N",90,1]
[null,null,null,null,"[합 계]",null,null,0,0,2843,0,127962,0,0,0,130805,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13010140S",null,null,null,"강관 용접 배관","D300, 옥외배관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13010140S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.63400000000000001,0,0,229482,145491.5,0,0,229482,145491.5,null,null,"N","Y","",0]
["MBA13010140S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.23200000000000001,0,0,165545,38406.400000000001,0,0,165545,38406.400000000001,null,null,"N","Y","",0]
["MBA13010140S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,3677.9,3677.9,0,0,0,0,3677.9,3677.9,null,null,"N","N",2,1]
["MBA13010140S","손료","RENT000000000002",null,"노무할증 10%감","노무비의 90%","식",1,0,0,165508.1,165508.1,0,0,165508.1,165508.1,null,null,"N","N",90,1]
[null,null,null,null,"[합 계]",null,null,0,0,3677,0,165508,0,0,0,169185,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13010150S",null,null,null,"강관 용접 배관","D350, 옥외배관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13010150S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.76500000000000001,0,0,229482,175553.7,0,0,229482,175553.7,null,null,"N","Y","",0]
["MBA13010150S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.27700000000000002,0,0,165545,45855.9,0,0,165545,45855.9,null,null,"N","Y","",0]
["MBA13010150S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,4428.1000000000004,4428.1000000000004,0,0,0,0,4428.1000000000004,4428.1000000000004,null,null,"N","N",2,1]
["MBA13010150S","손료","RENT000000000002",null,"노무할증 10%감","노무비의 90%","식",1,0,0,199268.6,199268.6,0,0,199268.6,199268.6,null,null,"N","N",90,1]
[null,null,null,null,"[합 계]",null,null,0,0,4428,0,199268,0,0,0,203696,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13010160S",null,null,null,"강관 용접 배관","D400, 옥외배관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13010160S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.90700000000000003,0,0,229482,208140.1,0,0,229482,208140.1,null,null,"N","Y","",0]
["MBA13010160S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.32700000000000001,0,0,165545,54133.2,0,0,165545,54133.2,null,null,"N","Y","",0]
["MBA13010160S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,5245.4,5245.4,0,0,0,0,5245.4,5245.4,null,null,"N","N",2,1]
["MBA13010160S","손료","RENT000000000002",null,"노무할증 10%감","노무비의 90%","식",1,0,0,236045.9,236045.9,0,0,236045.9,236045.9,null,null,"N","N",90,1]
[null,null,null,null,"[합 계]",null,null,0,0,5245,0,236045,0,0,0,241290,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13110010S",null,null,null,"강관 용접 배관","D15, 옥외배관, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13110010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",2.9000000000000001E-2,0,0,229482,6654.9,0,0,229482,6654.9,null,null,"N","Y","",0]
["MBA13110010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.1999999999999999E-2,0,0,165545,3641.9,0,0,165545,3641.9,null,null,"N","Y","",0]
["MBA13110010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1029.5999999999999,1029.5999999999999,0,0,0,0,1029.5999999999999,1029.5999999999999,null,null,"N","N",10,1]
["MBA13110010S","손료","RENT000000000002",null,"노무할증 10%감+20%감","노무비의 70%","식",1,0,0,7207.7,7207.7,0,0,7207.7,7207.7,null,null,"N","N",70,1]
[null,null,null,null,"[합 계]",null,null,0,0,1029,0,7207,0,0,0,8236,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13110020S",null,null,null,"강관 용접 배관","D20, 옥외배관, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13110020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",3.3000000000000002E-2,0,0,229482,7572.9,0,0,229482,7572.9,null,null,"N","Y","",0]
["MBA13110020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.3E-2,0,0,165545,3807.5,0,0,165545,3807.5,null,null,"N","Y","",0]
["MBA13110020S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1138,1138,0,0,0,0,1138,1138,null,null,"N","N",10,1]
["MBA13110020S","손료","RENT000000000002",null,"노무할증 10%감+20%감","노무비의 70%","식",1,0,0,7966.2,7966.2,0,0,7966.2,7966.2,null,null,"N","N",70,1]
[null,null,null,null,"[합 계]",null,null,0,0,1138,0,7966,0,0,0,9104,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13110030S",null,null,null,"강관 용접 배관","D25, 옥외배관, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13110030S","노무","L001010101000039",null,"배관공","일반공사 직종","인",4.2999999999999997E-2,0,0,229482,9867.7000000000007,0,0,229482,9867.7000000000007,null,null,"N","Y","",0]
["MBA13110030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5999999999999999E-2,0,0,165545,4304.1000000000004,0,0,165545,4304.1000000000004,null,null,"N","Y","",0]
["MBA13110030S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1417.1,1417.1,0,0,0,0,1417.1,1417.1,null,null,"N","N",10,1]
["MBA13110030S","손료","RENT000000000002",null,"노무할증 10%감+20%감","노무비의 70%","식",1,0,0,9920.2000000000007,9920.2000000000007,0,0,9920.2000000000007,9920.2000000000007,null,null,"N","N",70,1]
[null,null,null,null,"[합 계]",null,null,0,0,1417,0,9920,0,0,0,11337,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13110040S",null,null,null,"강관 용접 배관","D32, 옥외배관, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13110040S","노무","L001010101000039",null,"배관공","일반공사 직종","인",5.0999999999999997E-2,0,0,229482,11703.5,0,0,229482,11703.5,null,null,"N","Y","",0]
["MBA13110040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.9000000000000001E-2,0,0,165545,4800.8,0,0,165545,4800.8,null,null,"N","Y","",0]
["MBA13110040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1650.4,1650.4,0,0,0,0,1650.4,1650.4,null,null,"N","N",10,1]
["MBA13110040S","손료","RENT000000000002",null,"노무할증 10%감+20%감","노무비의 70%","식",1,0,0,11553,11553,0,0,11553,11553,null,null,"N","N",70,1]
[null,null,null,null,"[합 계]",null,null,0,0,1650,0,11553,0,0,0,13203,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13110050S",null,null,null,"강관 용접 배관","D40, 옥외배관, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13110050S","노무","L001010101000039",null,"배관공","일반공사 직종","인",5.7000000000000002E-2,0,0,229482,13080.4,0,0,229482,13080.4,null,null,"N","Y","",0]
["MBA13110050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.1E-2,0,0,165545,5131.8,0,0,165545,5131.8,null,null,"N","Y","",0]
["MBA13110050S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1821.2,1821.2,0,0,0,0,1821.2,1821.2,null,null,"N","N",10,1]
["MBA13110050S","손료","RENT000000000002",null,"노무할증 10%감+20%감","노무비의 70%","식",1,0,0,12748.5,12748.5,0,0,12748.5,12748.5,null,null,"N","N",70,1]
[null,null,null,null,"[합 계]",null,null,0,0,1821,0,12748,0,0,0,14569,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13110060S",null,null,null,"강관 용접 배관","D50, 옥외배관, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13110060S","노무","L001010101000039",null,"배관공","일반공사 직종","인",7.3999999999999996E-2,0,0,229482,16981.599999999999,0,0,229482,16981.599999999999,null,null,"N","Y","",0]
["MBA13110060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.6999999999999998E-2,0,0,165545,6125.1,0,0,165545,6125.1,null,null,"N","Y","",0]
["MBA13110060S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,2310.6,2310.6,0,0,0,0,2310.6,2310.6,null,null,"N","N",10,1]
["MBA13110060S","손료","RENT000000000002",null,"노무할증 10%감+20%감","노무비의 70%","식",1,0,0,16174.6,16174.6,0,0,16174.6,16174.6,null,null,"N","N",70,1]
[null,null,null,null,"[합 계]",null,null,0,0,2310,0,16174,0,0,0,18484,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13110070S",null,null,null,"강관 용접 배관","D65, 옥외배관, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13110070S","노무","L001010101000039",null,"배관공","일반공사 직종","인",8.7999999999999995E-2,0,0,229482,20194.400000000001,0,0,229482,20194.400000000001,null,null,"N","Y","",0]
["MBA13110070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.2000000000000003E-2,0,0,165545,6952.8,0,0,165545,6952.8,null,null,"N","Y","",0]
["MBA13110070S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,2714.7,2714.7,0,0,0,0,2714.7,2714.7,null,null,"N","N",10,1]
["MBA13110070S","손료","RENT000000000002",null,"노무할증 10%감+20%감","노무비의 70%","식",1,0,0,19003,19003,0,0,19003,19003,null,null,"N","N",70,1]
[null,null,null,null,"[합 계]",null,null,0,0,2714,0,19003,0,0,0,21717,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13110080S",null,null,null,"강관 용접 배관","D80, 옥외배관, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13110080S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.113,0,0,229482,25931.4,0,0,229482,25931.4,null,null,"N","Y","",0]
["MBA13110080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.0999999999999997E-2,0,0,165545,8442.7000000000007,0,0,165545,8442.7000000000007,null,null,"N","Y","",0]
["MBA13110080S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,3437.4,3437.4,0,0,0,0,3437.4,3437.4,null,null,"N","N",10,1]
["MBA13110080S","손료","RENT000000000002",null,"노무할증 10%감+20%감","노무비의 70%","식",1,0,0,24061.8,24061.8,0,0,24061.8,24061.8,null,null,"N","N",70,1]
[null,null,null,null,"[합 계]",null,null,0,0,3437,0,24061,0,0,0,27498,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13110090S",null,null,null,"강관 용접 배관","D100, 옥외배관, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13110090S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.155,0,0,229482,35569.699999999997,0,0,229482,35569.699999999997,null,null,"N","Y","",0]
["MBA13110090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.5000000000000002E-2,0,0,165545,10760.4,0,0,165545,10760.4,null,null,"N","Y","",0]
["MBA13110090S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,4633,4633,0,0,0,0,4633,4633,null,null,"N","N",10,1]
["MBA13110090S","손료","RENT000000000002",null,"노무할증 10%감+20%감","노무비의 70%","식",1,0,0,32431,32431,0,0,32431,32431,null,null,"N","N",70,1]
[null,null,null,null,"[합 계]",null,null,0,0,4633,0,32431,0,0,0,37064,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13110100S",null,null,null,"강관 용접 배관","D125, 옥외배관, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13110100S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.2,0,0,229482,45896.4,0,0,229482,45896.4,null,null,"N","Y","",0]
["MBA13110100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",8.1000000000000003E-2,0,0,165545,13409.1,0,0,165545,13409.1,null,null,"N","Y","",0]
["MBA13110100S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,5930.5,5930.5,0,0,0,0,5930.5,5930.5,null,null,"N","N",10,1]
["MBA13110100S","손료","RENT000000000002",null,"노무할증 10%감+20%감","노무비의 70%","식",1,0,0,41513.800000000003,41513.800000000003,0,0,41513.800000000003,41513.800000000003,null,null,"N","N",70,1]
[null,null,null,null,"[합 계]",null,null,0,0,5930,0,41513,0,0,0,47443,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13110110S",null,null,null,"강관 용접 배관","D150, 옥외배관, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13110110S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.23599999999999999,0,0,229482,54157.7,0,0,229482,54157.7,null,null,"N","Y","",0]
["MBA13110110S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",9.2999999999999999E-2,0,0,165545,15395.6,0,0,165545,15395.6,null,null,"N","Y","",0]
["MBA13110110S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,6955.3,6955.3,0,0,0,0,6955.3,6955.3,null,null,"N","N",10,1]
["MBA13110110S","손료","RENT000000000002",null,"노무할증 10%감+20%감","노무비의 70%","식",1,0,0,48687.3,48687.3,0,0,48687.3,48687.3,null,null,"N","N",70,1]
[null,null,null,null,"[합 계]",null,null,0,0,6955,0,48687,0,0,0,55642,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13110120S",null,null,null,"강관 용접 배관","D200, 옥외배관, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13110120S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.36499999999999999,0,0,229482,83760.899999999994,0,0,229482,83760.899999999994,null,null,"N","Y","",0]
["MBA13110120S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.13800000000000001,0,0,165545,22845.200000000001,0,0,165545,22845.200000000001,null,null,"N","Y","",0]
["MBA13110120S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,10660.6,10660.6,0,0,0,0,10660.6,10660.6,null,null,"N","N",10,1]
["MBA13110120S","손료","RENT000000000002",null,"노무할증 10%감+20%감","노무비의 70%","식",1,0,0,74624.2,74624.2,0,0,74624.2,74624.2,null,null,"N","N",70,1]
[null,null,null,null,"[합 계]",null,null,0,0,10660,0,74624,0,0,0,85284,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13110130S",null,null,null,"강관 용접 배관","D250, 옥외배관, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13110130S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.48899999999999999,0,0,229482,112216.6,0,0,229482,112216.6,null,null,"N","Y","",0]
["MBA13110130S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.18099999999999999,0,0,165545,29963.599999999999,0,0,165545,29963.599999999999,null,null,"N","Y","",0]
["MBA13110130S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,14218,14218,0,0,0,0,14218,14218,null,null,"N","N",10,1]
["MBA13110130S","손료","RENT000000000002",null,"노무할증 10%감+20%감","노무비의 70%","식",1,0,0,99526.1,99526.1,0,0,99526.1,99526.1,null,null,"N","N",70,1]
[null,null,null,null,"[합 계]",null,null,0,0,14218,0,99526,0,0,0,113744,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13110140S",null,null,null,"강관 용접 배관","D300, 옥외배관, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13110140S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.63400000000000001,0,0,229482,145491.5,0,0,229482,145491.5,null,null,"N","Y","",0]
["MBA13110140S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.23200000000000001,0,0,165545,38406.400000000001,0,0,165545,38406.400000000001,null,null,"N","Y","",0]
["MBA13110140S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,18389.7,18389.7,0,0,0,0,18389.7,18389.7,null,null,"N","N",10,1]
["MBA13110140S","손료","RENT000000000002",null,"노무할증 10%감+20%감","노무비의 70%","식",1,0,0,128728.5,128728.5,0,0,128728.5,128728.5,null,null,"N","N",70,1]
[null,null,null,null,"[합 계]",null,null,0,0,18389,0,128728,0,0,0,147117,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13110150S",null,null,null,"강관 용접 배관","D350, 옥외배관, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13110150S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.76500000000000001,0,0,229482,175553.7,0,0,229482,175553.7,null,null,"N","Y","",0]
["MBA13110150S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.27700000000000002,0,0,165545,45855.9,0,0,165545,45855.9,null,null,"N","Y","",0]
["MBA13110150S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,22140.9,22140.9,0,0,0,0,22140.9,22140.9,null,null,"N","N",10,1]
["MBA13110150S","손료","RENT000000000002",null,"노무할증 10%감+20%감","노무비의 70%","식",1,0,0,154986.70000000001,154986.70000000001,0,0,154986.70000000001,154986.70000000001,null,null,"N","N",70,1]
[null,null,null,null,"[합 계]",null,null,0,0,22140,0,154986,0,0,0,177126,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13110160S",null,null,null,"강관 용접 배관","D400, 옥외배관, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA13110160S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.90700000000000003,0,0,229482,208140.1,0,0,229482,208140.1,null,null,"N","Y","",0]
["MBA13110160S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.32700000000000001,0,0,165545,54133.2,0,0,165545,54133.2,null,null,"N","Y","",0]
["MBA13110160S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,26227.3,26227.3,0,0,0,0,26227.3,26227.3,null,null,"N","N",10,1]
["MBA13110160S","손료","RENT000000000002",null,"노무할증 10%감+20%감","노무비의 70%","식",1,0,0,183591.3,183591.3,0,0,183591.3,183591.3,null,null,"N","N",70,1]
[null,null,null,null,"[합 계]",null,null,0,0,26227,0,183591,0,0,0,209818,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA20010010S",null,null,null,"나사식 접합 및 배관","D15, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA20010010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",3.3000000000000002E-2,0,0,229482,7572.9,0,0,229482,7572.9,null,null,"N","N","",1]
["MBA20010010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.9000000000000001E-2,0,0,165545,4800.8,0,0,165545,4800.8,null,null,"N","N","",1]
["MBA20010010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,247.4,247.4,0,0,0,0,247.4,247.4,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,247,0,12373,0,0,0,12620,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA20010020S",null,null,null,"나사식 접합 및 배관","D20, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA20010020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",3.7999999999999999E-2,0,0,229482,8720.2999999999993,0,0,229482,8720.2999999999993,null,null,"N","N","",1]
["MBA20010020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.03,0,0,165545,4966.3,0,0,165545,4966.3,null,null,"N","N","",1]
["MBA20010020S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,273.7,273.7,0,0,0,0,273.7,273.7,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,273,0,13686,0,0,0,13959,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA20010030S",null,null,null,"나사식 접합 및 배관","D25, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA20010030S","노무","L001010101000039",null,"배관공","일반공사 직종","인",5.0999999999999997E-2,0,0,229482,11703.5,0,0,229482,11703.5,null,null,"N","N","",1]
["MBA20010030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.4000000000000002E-2,0,0,165545,5628.5,0,0,165545,5628.5,null,null,"N","N","",1]
["MBA20010030S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,346.6,346.6,0,0,0,0,346.6,346.6,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,346,0,17332,0,0,0,17678,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA20010040S",null,null,null,"나사식 접합 및 배관","D32, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA20010040S","노무","L001010101000039",null,"배관공","일반공사 직종","인",6.2E-2,0,0,229482,14227.8,0,0,229482,14227.8,null,null,"N","N","",1]
["MBA20010040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.6999999999999998E-2,0,0,165545,6125.1,0,0,165545,6125.1,null,null,"N","N","",1]
["MBA20010040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,407,407,0,0,0,0,407,407,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,407,0,20352,0,0,0,20759,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA20010050S",null,null,null,"나사식 접합 및 배관","D40, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA20010050S","노무","L001010101000039",null,"배관공","일반공사 직종","인",6.9000000000000006E-2,0,0,229482,15834.2,0,0,229482,15834.2,null,null,"N","N","",1]
["MBA20010050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.9E-2,0,0,165545,6456.2,0,0,165545,6456.2,null,null,"N","N","",1]
["MBA20010050S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,445.8,445.8,0,0,0,0,445.8,445.8,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,445,0,22290,0,0,0,22735,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA20010060S",null,null,null,"나사식 접합 및 배관","D50, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA20010060S","노무","L001010101000039",null,"배관공","일반공사 직종","인",9.1999999999999998E-2,0,0,229482,21112.3,0,0,229482,21112.3,null,null,"N","N","",1]
["MBA20010060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.5999999999999999E-2,0,0,165545,7615,0,0,165545,7615,null,null,"N","N","",1]
["MBA20010060S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,574.5,574.5,0,0,0,0,574.5,574.5,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,574,0,28727,0,0,0,29301,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA20110010S",null,null,null,"나사식 접합 및 배관","D15, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA20110010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",3.3000000000000002E-2,0,0,229482,7572.9,0,0,229482,7572.9,null,null,"N","Y","",0]
["MBA20110010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.9000000000000001E-2,0,0,165545,4800.8,0,0,165545,4800.8,null,null,"N","Y","",0]
["MBA20110010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1237.3,1237.3,0,0,0,0,1237.3,1237.3,null,null,"N","N",10,1]
["MBA20110010S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,9898.9,9898.9,0,0,9898.9,9898.9,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,1237,0,9898,0,0,0,11135,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA20110020S",null,null,null,"나사식 접합 및 배관","D20, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA20110020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",3.7999999999999999E-2,0,0,229482,8720.2999999999993,0,0,229482,8720.2999999999993,null,null,"N","Y","",0]
["MBA20110020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.03,0,0,165545,4966.3,0,0,165545,4966.3,null,null,"N","Y","",0]
["MBA20110020S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1368.6,1368.6,0,0,0,0,1368.6,1368.6,null,null,"N","N",10,1]
["MBA20110020S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,10949.2,10949.2,0,0,10949.2,10949.2,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,1368,0,10949,0,0,0,12317,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA20110030S",null,null,null,"나사식 접합 및 배관","D25, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA20110030S","노무","L001010101000039",null,"배관공","일반공사 직종","인",5.0999999999999997E-2,0,0,229482,11703.5,0,0,229482,11703.5,null,null,"N","Y","",0]
["MBA20110030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.4000000000000002E-2,0,0,165545,5628.5,0,0,165545,5628.5,null,null,"N","Y","",0]
["MBA20110030S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1733.2,1733.2,0,0,0,0,1733.2,1733.2,null,null,"N","N",10,1]
["MBA20110030S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,13865.6,13865.6,0,0,13865.6,13865.6,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,1733,0,13865,0,0,0,15598,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA20110040S",null,null,null,"나사식 접합 및 배관","D32, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA20110040S","노무","L001010101000039",null,"배관공","일반공사 직종","인",6.2E-2,0,0,229482,14227.8,0,0,229482,14227.8,null,null,"N","Y","",0]
["MBA20110040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.6999999999999998E-2,0,0,165545,6125.1,0,0,165545,6125.1,null,null,"N","Y","",0]
["MBA20110040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,2035.2,2035.2,0,0,0,0,2035.2,2035.2,null,null,"N","N",10,1]
["MBA20110040S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,16282.3,16282.3,0,0,16282.3,16282.3,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,2035,0,16282,0,0,0,18317,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA20110050S",null,null,null,"나사식 접합 및 배관","D40, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA20110050S","노무","L001010101000039",null,"배관공","일반공사 직종","인",6.9000000000000006E-2,0,0,229482,15834.2,0,0,229482,15834.2,null,null,"N","Y","",0]
["MBA20110050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.9E-2,0,0,165545,6456.2,0,0,165545,6456.2,null,null,"N","Y","",0]
["MBA20110050S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,2229,2229,0,0,0,0,2229,2229,null,null,"N","N",10,1]
["MBA20110050S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,17832.3,17832.3,0,0,17832.3,17832.3,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,2229,0,17832,0,0,0,20061,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA20110060S",null,null,null,"나사식 접합 및 배관","D50, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA20110060S","노무","L001010101000039",null,"배관공","일반공사 직종","인",9.1999999999999998E-2,0,0,229482,21112.3,0,0,229482,21112.3,null,null,"N","Y","",0]
["MBA20110060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.5999999999999999E-2,0,0,165545,7615,0,0,165545,7615,null,null,"N","Y","",0]
["MBA20110060S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,2872.7,2872.7,0,0,0,0,2872.7,2872.7,null,null,"N","N",10,1]
["MBA20110060S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,22981.8,22981.8,0,0,22981.8,22981.8,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,2872,0,22981,0,0,0,25853,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA21010010S",null,null,null,"나사식 접합 및 배관","D15, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA21010010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",3.3000000000000002E-2,0,0,229482,7572.9,0,0,229482,7572.9,null,null,"N","Y","",0]
["MBA21010010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.9000000000000001E-2,0,0,165545,4800.8,0,0,165545,4800.8,null,null,"N","Y","",0]
["MBA21010010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,247.4,247.4,0,0,0,0,247.4,247.4,null,null,"N","N",2,1]
["MBA21010010S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,16085.8,16085.8,0,0,16085.8,16085.8,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,247,0,16085,0,0,0,16332,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA21010020S",null,null,null,"나사식 접합 및 배관","D20, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA21010020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",3.7999999999999999E-2,0,0,229482,8720.2999999999993,0,0,229482,8720.2999999999993,null,null,"N","Y","",0]
["MBA21010020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.03,0,0,165545,4966.3,0,0,165545,4966.3,null,null,"N","Y","",0]
["MBA21010020S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,273.7,273.7,0,0,0,0,273.7,273.7,null,null,"N","N",2,1]
["MBA21010020S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,17792.5,17792.5,0,0,17792.5,17792.5,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,273,0,17792,0,0,0,18065,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA21010030S",null,null,null,"나사식 접합 및 배관","D25, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA21010030S","노무","L001010101000039",null,"배관공","일반공사 직종","인",5.0999999999999997E-2,0,0,229482,11703.5,0,0,229482,11703.5,null,null,"N","Y","",0]
["MBA21010030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.4000000000000002E-2,0,0,165545,5628.5,0,0,165545,5628.5,null,null,"N","Y","",0]
["MBA21010030S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,346.6,346.6,0,0,0,0,346.6,346.6,null,null,"N","N",2,1]
["MBA21010030S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,22531.599999999999,22531.599999999999,0,0,22531.599999999999,22531.599999999999,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,346,0,22531,0,0,0,22877,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA21010040S",null,null,null,"나사식 접합 및 배관","D32, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA21010040S","노무","L001010101000039",null,"배관공","일반공사 직종","인",6.2E-2,0,0,229482,14227.8,0,0,229482,14227.8,null,null,"N","Y","",0]
["MBA21010040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.6999999999999998E-2,0,0,165545,6125.1,0,0,165545,6125.1,null,null,"N","Y","",0]
["MBA21010040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,407,407,0,0,0,0,407,407,null,null,"N","N",2,1]
["MBA21010040S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,26458.7,26458.7,0,0,26458.7,26458.7,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,407,0,26458,0,0,0,26865,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA21010050S",null,null,null,"나사식 접합 및 배관","D40, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA21010050S","노무","L001010101000039",null,"배관공","일반공사 직종","인",6.9000000000000006E-2,0,0,229482,15834.2,0,0,229482,15834.2,null,null,"N","Y","",0]
["MBA21010050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.9E-2,0,0,165545,6456.2,0,0,165545,6456.2,null,null,"N","Y","",0]
["MBA21010050S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,445.8,445.8,0,0,0,0,445.8,445.8,null,null,"N","N",2,1]
["MBA21010050S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,28977.5,28977.5,0,0,28977.5,28977.5,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,445,0,28977,0,0,0,29422,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA21010060S",null,null,null,"나사식 접합 및 배관","D50, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA21010060S","노무","L001010101000039",null,"배관공","일반공사 직종","인",9.1999999999999998E-2,0,0,229482,21112.3,0,0,229482,21112.3,null,null,"N","Y","",0]
["MBA21010060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.5999999999999999E-2,0,0,165545,7615,0,0,165545,7615,null,null,"N","Y","",0]
["MBA21010060S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,574.5,574.5,0,0,0,0,574.5,574.5,null,null,"N","N",2,1]
["MBA21010060S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,37345.4,37345.4,0,0,37345.4,37345.4,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,574,0,37345,0,0,0,37919,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA21110010S",null,null,null,"나사식 접합 및 배관","D15, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA21110010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",3.3000000000000002E-2,0,0,229482,7572.9,0,0,229482,7572.9,null,null,"N","Y","",0]
["MBA21110010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.9000000000000001E-2,0,0,165545,4800.8,0,0,165545,4800.8,null,null,"N","Y","",0]
["MBA21110010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1237.3,1237.3,0,0,0,0,1237.3,1237.3,null,null,"N","N",10,1]
["MBA21110010S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,13611,13611,0,0,13611,13611,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,1237,0,13611,0,0,0,14848,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA21110020S",null,null,null,"나사식 접합 및 배관","D20, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA21110020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",3.7999999999999999E-2,0,0,229482,8720.2999999999993,0,0,229482,8720.2999999999993,null,null,"N","Y","",0]
["MBA21110020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.03,0,0,165545,4966.3,0,0,165545,4966.3,null,null,"N","Y","",0]
["MBA21110020S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1368.6,1368.6,0,0,0,0,1368.6,1368.6,null,null,"N","N",10,1]
["MBA21110020S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,15055.2,15055.2,0,0,15055.2,15055.2,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,1368,0,15055,0,0,0,16423,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA21110030S",null,null,null,"나사식 접합 및 배관","D25, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA21110030S","노무","L001010101000039",null,"배관공","일반공사 직종","인",5.0999999999999997E-2,0,0,229482,11703.5,0,0,229482,11703.5,null,null,"N","Y","",0]
["MBA21110030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.4000000000000002E-2,0,0,165545,5628.5,0,0,165545,5628.5,null,null,"N","Y","",0]
["MBA21110030S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1733.2,1733.2,0,0,0,0,1733.2,1733.2,null,null,"N","N",10,1]
["MBA21110030S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,19065.2,19065.2,0,0,19065.2,19065.2,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,1733,0,19065,0,0,0,20798,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA21110040S",null,null,null,"나사식 접합 및 배관","D32, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA21110040S","노무","L001010101000039",null,"배관공","일반공사 직종","인",6.2E-2,0,0,229482,14227.8,0,0,229482,14227.8,null,null,"N","Y","",0]
["MBA21110040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.6999999999999998E-2,0,0,165545,6125.1,0,0,165545,6125.1,null,null,"N","Y","",0]
["MBA21110040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,2035.2,2035.2,0,0,0,0,2035.2,2035.2,null,null,"N","N",10,1]
["MBA21110040S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,22388.1,22388.1,0,0,22388.1,22388.1,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,2035,0,22388,0,0,0,24423,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA21110050S",null,null,null,"나사식 접합 및 배관","D40, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA21110050S","노무","L001010101000039",null,"배관공","일반공사 직종","인",6.9000000000000006E-2,0,0,229482,15834.2,0,0,229482,15834.2,null,null,"N","Y","",0]
["MBA21110050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.9E-2,0,0,165545,6456.2,0,0,165545,6456.2,null,null,"N","Y","",0]
["MBA21110050S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,2229,2229,0,0,0,0,2229,2229,null,null,"N","N",10,1]
["MBA21110050S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,24519.4,24519.4,0,0,24519.4,24519.4,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,2229,0,24519,0,0,0,26748,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA21110060S",null,null,null,"나사식 접합 및 배관","D50, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA21110060S","노무","L001010101000039",null,"배관공","일반공사 직종","인",9.1999999999999998E-2,0,0,229482,21112.3,0,0,229482,21112.3,null,null,"N","Y","",0]
["MBA21110060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.5999999999999999E-2,0,0,165545,7615,0,0,165545,7615,null,null,"N","Y","",0]
["MBA21110060S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,2872.7,2872.7,0,0,0,0,2872.7,2872.7,null,null,"N","N",10,1]
["MBA21110060S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,31600,31600,0,0,31600,31600,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,2872,0,31600,0,0,0,34472,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA22010010S",null,null,null,"나사식 접합 및 배관","D15, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA22010010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",3.3000000000000002E-2,0,0,229482,7572.9,0,0,229482,7572.9,null,null,"N","Y","",0]
["MBA22010010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.9000000000000001E-2,0,0,165545,4800.8,0,0,165545,4800.8,null,null,"N","Y","",0]
["MBA22010010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,247.4,247.4,0,0,0,0,247.4,247.4,null,null,"N","N",2,1]
["MBA22010010S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,14848.4,14848.4,0,0,14848.4,14848.4,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,247,0,14848,0,0,0,15095,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA22010020S",null,null,null,"나사식 접합 및 배관","D20, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA22010020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",3.7999999999999999E-2,0,0,229482,8720.2999999999993,0,0,229482,8720.2999999999993,null,null,"N","Y","",0]
["MBA22010020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.03,0,0,165545,4966.3,0,0,165545,4966.3,null,null,"N","Y","",0]
["MBA22010020S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,273.7,273.7,0,0,0,0,273.7,273.7,null,null,"N","N",2,1]
["MBA22010020S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,16423.900000000001,16423.900000000001,0,0,16423.900000000001,16423.900000000001,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,273,0,16423,0,0,0,16696,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA22010030S",null,null,null,"나사식 접합 및 배관","D25, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA22010030S","노무","L001010101000039",null,"배관공","일반공사 직종","인",5.0999999999999997E-2,0,0,229482,11703.5,0,0,229482,11703.5,null,null,"N","Y","",0]
["MBA22010030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.4000000000000002E-2,0,0,165545,5628.5,0,0,165545,5628.5,null,null,"N","Y","",0]
["MBA22010030S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,346.6,346.6,0,0,0,0,346.6,346.6,null,null,"N","N",2,1]
["MBA22010030S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,20798.400000000001,20798.400000000001,0,0,20798.400000000001,20798.400000000001,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,346,0,20798,0,0,0,21144,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA22010040S",null,null,null,"나사식 접합 및 배관","D32, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA22010040S","노무","L001010101000039",null,"배관공","일반공사 직종","인",6.2E-2,0,0,229482,14227.8,0,0,229482,14227.8,null,null,"N","Y","",0]
["MBA22010040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.6999999999999998E-2,0,0,165545,6125.1,0,0,165545,6125.1,null,null,"N","Y","",0]
["MBA22010040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,407,407,0,0,0,0,407,407,null,null,"N","N",2,1]
["MBA22010040S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,24423.4,24423.4,0,0,24423.4,24423.4,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,407,0,24423,0,0,0,24830,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA22010050S",null,null,null,"나사식 접합 및 배관","D40, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA22010050S","노무","L001010101000039",null,"배관공","일반공사 직종","인",6.9000000000000006E-2,0,0,229482,15834.2,0,0,229482,15834.2,null,null,"N","Y","",0]
["MBA22010050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.9E-2,0,0,165545,6456.2,0,0,165545,6456.2,null,null,"N","Y","",0]
["MBA22010050S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,445.8,445.8,0,0,0,0,445.8,445.8,null,null,"N","N",2,1]
["MBA22010050S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,26748.400000000001,26748.400000000001,0,0,26748.400000000001,26748.400000000001,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,445,0,26748,0,0,0,27193,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA22010060S",null,null,null,"나사식 접합 및 배관","D50, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA22010060S","노무","L001010101000039",null,"배관공","일반공사 직종","인",9.1999999999999998E-2,0,0,229482,21112.3,0,0,229482,21112.3,null,null,"N","Y","",0]
["MBA22010060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.5999999999999999E-2,0,0,165545,7615,0,0,165545,7615,null,null,"N","Y","",0]
["MBA22010060S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,574.5,574.5,0,0,0,0,574.5,574.5,null,null,"N","N",2,1]
["MBA22010060S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,34472.699999999997,34472.699999999997,0,0,34472.699999999997,34472.699999999997,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,574,0,34472,0,0,0,35046,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA22110010S",null,null,null,"나사식 접합 및 배관","D15, 화장실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA22110010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",3.3000000000000002E-2,0,0,229482,7572.9,0,0,229482,7572.9,null,null,"N","Y","",0]
["MBA22110010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.9000000000000001E-2,0,0,165545,4800.8,0,0,165545,4800.8,null,null,"N","Y","",0]
["MBA22110010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1237.3,1237.3,0,0,0,0,1237.3,1237.3,null,null,"N","N",10,1]
["MBA22110010S","손료","RENT000000000002",null,"노무할증 20%증+20%감","노무비의 100%","식",1,0,0,12373.7,12373.7,0,0,12373.7,12373.7,null,null,"N","N",100,1]
[null,null,null,null,"[합 계]",null,null,0,0,1237,0,12373,0,0,0,13610,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA22110020S",null,null,null,"나사식 접합 및 배관","D20, 화장실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA22110020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",3.7999999999999999E-2,0,0,229482,8720.2999999999993,0,0,229482,8720.2999999999993,null,null,"N","Y","",0]
["MBA22110020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.03,0,0,165545,4966.3,0,0,165545,4966.3,null,null,"N","Y","",0]
["MBA22110020S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1368.6,1368.6,0,0,0,0,1368.6,1368.6,null,null,"N","N",10,1]
["MBA22110020S","손료","RENT000000000002",null,"노무할증 20%증+20%감","노무비의 100%","식",1,0,0,13686.6,13686.6,0,0,13686.6,13686.6,null,null,"N","N",100,1]
[null,null,null,null,"[합 계]",null,null,0,0,1368,0,13686,0,0,0,15054,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA22110030S",null,null,null,"나사식 접합 및 배관","D25, 화장실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA22110030S","노무","L001010101000039",null,"배관공","일반공사 직종","인",5.0999999999999997E-2,0,0,229482,11703.5,0,0,229482,11703.5,null,null,"N","Y","",0]
["MBA22110030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.4000000000000002E-2,0,0,165545,5628.5,0,0,165545,5628.5,null,null,"N","Y","",0]
["MBA22110030S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1733.2,1733.2,0,0,0,0,1733.2,1733.2,null,null,"N","N",10,1]
["MBA22110030S","손료","RENT000000000002",null,"노무할증 20%증+20%감","노무비의 100%","식",1,0,0,17332,17332,0,0,17332,17332,null,null,"N","N",100,1]
[null,null,null,null,"[합 계]",null,null,0,0,1733,0,17332,0,0,0,19065,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA22110040S",null,null,null,"나사식 접합 및 배관","D32, 화장실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA22110040S","노무","L001010101000039",null,"배관공","일반공사 직종","인",6.2E-2,0,0,229482,14227.8,0,0,229482,14227.8,null,null,"N","Y","",0]
["MBA22110040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.6999999999999998E-2,0,0,165545,6125.1,0,0,165545,6125.1,null,null,"N","Y","",0]
["MBA22110040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,2035.2,2035.2,0,0,0,0,2035.2,2035.2,null,null,"N","N",10,1]
["MBA22110040S","손료","RENT000000000002",null,"노무할증 20%증+20%감","노무비의 100%","식",1,0,0,20352.900000000001,20352.900000000001,0,0,20352.900000000001,20352.900000000001,null,null,"N","N",100,1]
[null,null,null,null,"[합 계]",null,null,0,0,2035,0,20352,0,0,0,22387,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA22110050S",null,null,null,"나사식 접합 및 배관","D40, 화장실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA22110050S","노무","L001010101000039",null,"배관공","일반공사 직종","인",6.9000000000000006E-2,0,0,229482,15834.2,0,0,229482,15834.2,null,null,"N","Y","",0]
["MBA22110050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.9E-2,0,0,165545,6456.2,0,0,165545,6456.2,null,null,"N","Y","",0]
["MBA22110050S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,2229,2229,0,0,0,0,2229,2229,null,null,"N","N",10,1]
["MBA22110050S","손료","RENT000000000002",null,"노무할증 20%증+20%감","노무비의 100%","식",1,0,0,22290.400000000001,22290.400000000001,0,0,22290.400000000001,22290.400000000001,null,null,"N","N",100,1]
[null,null,null,null,"[합 계]",null,null,0,0,2229,0,22290,0,0,0,24519,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA22110060S",null,null,null,"나사식 접합 및 배관","D50, 화장실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA22110060S","노무","L001010101000039",null,"배관공","일반공사 직종","인",9.1999999999999998E-2,0,0,229482,21112.3,0,0,229482,21112.3,null,null,"N","Y","",0]
["MBA22110060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.5999999999999999E-2,0,0,165545,7615,0,0,165545,7615,null,null,"N","Y","",0]
["MBA22110060S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,2872.7,2872.7,0,0,0,0,2872.7,2872.7,null,null,"N","N",10,1]
["MBA22110060S","손료","RENT000000000002",null,"노무할증 20%증+20%감","노무비의 100%","식",1,0,0,28727.3,28727.3,0,0,28727.3,28727.3,null,null,"N","N",100,1]
[null,null,null,null,"[합 계]",null,null,0,0,2872,0,28727,0,0,0,31599,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA23010010S",null,null,null,"나사식 접합 및 배관","D15, 옥외배관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA23010010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",3.3000000000000002E-2,0,0,229482,7572.9,0,0,229482,7572.9,null,null,"N","Y","",0]
["MBA23010010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.9000000000000001E-2,0,0,165545,4800.8,0,0,165545,4800.8,null,null,"N","Y","",0]
["MBA23010010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,247.4,247.4,0,0,0,0,247.4,247.4,null,null,"N","N",2,1]
["MBA23010010S","손료","RENT000000000002",null,"노무할증 10%감","노무비의 90%","식",1,0,0,11136.3,11136.3,0,0,11136.3,11136.3,null,null,"N","N",90,1]
[null,null,null,null,"[합 계]",null,null,0,0,247,0,11136,0,0,0,11383,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA23010020S",null,null,null,"나사식 접합 및 배관","D20, 옥외배관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA23010020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",3.7999999999999999E-2,0,0,229482,8720.2999999999993,0,0,229482,8720.2999999999993,null,null,"N","Y","",0]
["MBA23010020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.03,0,0,165545,4966.3,0,0,165545,4966.3,null,null,"N","Y","",0]
["MBA23010020S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,273.7,273.7,0,0,0,0,273.7,273.7,null,null,"N","N",2,1]
["MBA23010020S","손료","RENT000000000002",null,"노무할증 10%감","노무비의 90%","식",1,0,0,12317.9,12317.9,0,0,12317.9,12317.9,null,null,"N","N",90,1]
[null,null,null,null,"[합 계]",null,null,0,0,273,0,12317,0,0,0,12590,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA23010030S",null,null,null,"나사식 접합 및 배관","D25, 옥외배관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA23010030S","노무","L001010101000039",null,"배관공","일반공사 직종","인",5.0999999999999997E-2,0,0,229482,11703.5,0,0,229482,11703.5,null,null,"N","Y","",0]
["MBA23010030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.4000000000000002E-2,0,0,165545,5628.5,0,0,165545,5628.5,null,null,"N","Y","",0]
["MBA23010030S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,346.6,346.6,0,0,0,0,346.6,346.6,null,null,"N","N",2,1]
["MBA23010030S","손료","RENT000000000002",null,"노무할증 10%감","노무비의 90%","식",1,0,0,15598.8,15598.8,0,0,15598.8,15598.8,null,null,"N","N",90,1]
[null,null,null,null,"[합 계]",null,null,0,0,346,0,15598,0,0,0,15944,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA23010040S",null,null,null,"나사식 접합 및 배관","D32, 옥외배관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA23010040S","노무","L001010101000039",null,"배관공","일반공사 직종","인",6.2E-2,0,0,229482,14227.8,0,0,229482,14227.8,null,null,"N","Y","",0]
["MBA23010040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.6999999999999998E-2,0,0,165545,6125.1,0,0,165545,6125.1,null,null,"N","Y","",0]
["MBA23010040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,407,407,0,0,0,0,407,407,null,null,"N","N",2,1]
["MBA23010040S","손료","RENT000000000002",null,"노무할증 10%감","노무비의 90%","식",1,0,0,18317.599999999999,18317.599999999999,0,0,18317.599999999999,18317.599999999999,null,null,"N","N",90,1]
[null,null,null,null,"[합 계]",null,null,0,0,407,0,18317,0,0,0,18724,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA23010050S",null,null,null,"나사식 접합 및 배관","D40, 옥외배관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA23010050S","노무","L001010101000039",null,"배관공","일반공사 직종","인",6.9000000000000006E-2,0,0,229482,15834.2,0,0,229482,15834.2,null,null,"N","Y","",0]
["MBA23010050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.9E-2,0,0,165545,6456.2,0,0,165545,6456.2,null,null,"N","Y","",0]
["MBA23010050S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,445.8,445.8,0,0,0,0,445.8,445.8,null,null,"N","N",2,1]
["MBA23010050S","손료","RENT000000000002",null,"노무할증 10%감","노무비의 90%","식",1,0,0,20061.3,20061.3,0,0,20061.3,20061.3,null,null,"N","N",90,1]
[null,null,null,null,"[합 계]",null,null,0,0,445,0,20061,0,0,0,20506,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA23010060S",null,null,null,"나사식 접합 및 배관","D50, 옥외배관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA23010060S","노무","L001010101000039",null,"배관공","일반공사 직종","인",9.1999999999999998E-2,0,0,229482,21112.3,0,0,229482,21112.3,null,null,"N","Y","",0]
["MBA23010060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.5999999999999999E-2,0,0,165545,7615,0,0,165545,7615,null,null,"N","Y","",0]
["MBA23010060S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,574.5,574.5,0,0,0,0,574.5,574.5,null,null,"N","N",2,1]
["MBA23010060S","손료","RENT000000000002",null,"노무할증 10%감","노무비의 90%","식",1,0,0,25854.5,25854.5,0,0,25854.5,25854.5,null,null,"N","N",90,1]
[null,null,null,null,"[합 계]",null,null,0,0,574,0,25854,0,0,0,26428,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA23110010S",null,null,null,"나사식 접합 및 배관","D15, 옥외배관, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA23110010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",3.3000000000000002E-2,0,0,229482,7572.9,0,0,229482,7572.9,null,null,"N","Y","",0]
["MBA23110010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.9000000000000001E-2,0,0,165545,4800.8,0,0,165545,4800.8,null,null,"N","Y","",0]
["MBA23110010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1237.3,1237.3,0,0,0,0,1237.3,1237.3,null,null,"N","N",10,1]
["MBA23110010S","손료","RENT000000000002",null,"노무할증 10%감+20%감","노무비의 70%","식",1,0,0,8661.5,8661.5,0,0,8661.5,8661.5,null,null,"N","N",70,1]
[null,null,null,null,"[합 계]",null,null,0,0,1237,0,8661,0,0,0,9898,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA23110020S",null,null,null,"나사식 접합 및 배관","D20, 옥외배관, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA23110020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",3.7999999999999999E-2,0,0,229482,8720.2999999999993,0,0,229482,8720.2999999999993,null,null,"N","Y","",0]
["MBA23110020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.03,0,0,165545,4966.3,0,0,165545,4966.3,null,null,"N","Y","",0]
["MBA23110020S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1368.6,1368.6,0,0,0,0,1368.6,1368.6,null,null,"N","N",10,1]
["MBA23110020S","손료","RENT000000000002",null,"노무할증 10%감+20%감","노무비의 70%","식",1,0,0,9580.6,9580.6,0,0,9580.6,9580.6,null,null,"N","N",70,1]
[null,null,null,null,"[합 계]",null,null,0,0,1368,0,9580,0,0,0,10948,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA23110030S",null,null,null,"나사식 접합 및 배관","D25, 옥외배관, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA23110030S","노무","L001010101000039",null,"배관공","일반공사 직종","인",5.0999999999999997E-2,0,0,229482,11703.5,0,0,229482,11703.5,null,null,"N","Y","",0]
["MBA23110030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.4000000000000002E-2,0,0,165545,5628.5,0,0,165545,5628.5,null,null,"N","Y","",0]
["MBA23110030S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1733.2,1733.2,0,0,0,0,1733.2,1733.2,null,null,"N","N",10,1]
["MBA23110030S","손료","RENT000000000002",null,"노무할증 10%감+20%감","노무비의 70%","식",1,0,0,12132.4,12132.4,0,0,12132.4,12132.4,null,null,"N","N",70,1]
[null,null,null,null,"[합 계]",null,null,0,0,1733,0,12132,0,0,0,13865,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA23110040S",null,null,null,"나사식 접합 및 배관","D32, 옥외배관, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA23110040S","노무","L001010101000039",null,"배관공","일반공사 직종","인",6.2E-2,0,0,229482,14227.8,0,0,229482,14227.8,null,null,"N","Y","",0]
["MBA23110040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.6999999999999998E-2,0,0,165545,6125.1,0,0,165545,6125.1,null,null,"N","Y","",0]
["MBA23110040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,2035.2,2035.2,0,0,0,0,2035.2,2035.2,null,null,"N","N",10,1]
["MBA23110040S","손료","RENT000000000002",null,"노무할증 10%감+20%감","노무비의 70%","식",1,0,0,14247,14247,0,0,14247,14247,null,null,"N","N",70,1]
[null,null,null,null,"[합 계]",null,null,0,0,2035,0,14247,0,0,0,16282,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA23110050S",null,null,null,"나사식 접합 및 배관","D40, 옥외배관, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA23110050S","노무","L001010101000039",null,"배관공","일반공사 직종","인",6.9000000000000006E-2,0,0,229482,15834.2,0,0,229482,15834.2,null,null,"N","Y","",0]
["MBA23110050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.9E-2,0,0,165545,6456.2,0,0,165545,6456.2,null,null,"N","Y","",0]
["MBA23110050S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,2229,2229,0,0,0,0,2229,2229,null,null,"N","N",10,1]
["MBA23110050S","손료","RENT000000000002",null,"노무할증 10%감+20%감","노무비의 70%","식",1,0,0,15603.2,15603.2,0,0,15603.2,15603.2,null,null,"N","N",70,1]
[null,null,null,null,"[합 계]",null,null,0,0,2229,0,15603,0,0,0,17832,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA23110060S",null,null,null,"나사식 접합 및 배관","D50, 옥외배관, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA23110060S","노무","L001010101000039",null,"배관공","일반공사 직종","인",9.1999999999999998E-2,0,0,229482,21112.3,0,0,229482,21112.3,null,null,"N","Y","",0]
["MBA23110060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.5999999999999999E-2,0,0,165545,7615,0,0,165545,7615,null,null,"N","Y","",0]
["MBA23110060S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,2872.7,2872.7,0,0,0,0,2872.7,2872.7,null,null,"N","N",10,1]
["MBA23110060S","손료","RENT000000000002",null,"노무할증 10%감+20%감","노무비의 70%","식",1,0,0,20109.099999999999,20109.099999999999,0,0,20109.099999999999,20109.099999999999,null,null,"N","N",70,1]
[null,null,null,null,"[합 계]",null,null,0,0,2872,0,20109,0,0,0,22981,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30010010S",null,null,null,"그루브조인트식 접합 및 배관","D25, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30010010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",4.9000000000000002E-2,0,0,229482,11244.6,0,0,229482,11244.6,null,null,"N","N","",1]
["MBA30010010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5999999999999999E-2,0,0,165545,4304.1000000000004,0,0,165545,4304.1000000000004,null,null,"N","N","",1]
["MBA30010010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,310.89999999999998,310.89999999999998,0,0,0,0,310.89999999999998,310.89999999999998,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,310,0,15548,0,0,0,15858,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30010020S",null,null,null,"그루브조인트식 접합 및 배관","D32, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30010020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",6.0999999999999999E-2,0,0,229482,13998.4,0,0,229482,13998.4,null,null,"N","N","",1]
["MBA30010020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.03,0,0,165545,4966.3,0,0,165545,4966.3,null,null,"N","N","",1]
["MBA30010020S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,379.2,379.2,0,0,0,0,379.2,379.2,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,379,0,18964,0,0,0,19343,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30010030S",null,null,null,"그루브조인트식 접합 및 배관","D40, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30010030S","노무","L001010101000039",null,"배관공","일반공사 직종","인",6.9000000000000006E-2,0,0,229482,15834.2,0,0,229482,15834.2,null,null,"N","N","",1]
["MBA30010030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.2000000000000001E-2,0,0,165545,5297.4,0,0,165545,5297.4,null,null,"N","N","",1]
["MBA30010030S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,422.6,422.6,0,0,0,0,422.6,422.6,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,422,0,21131,0,0,0,21553,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30010040S",null,null,null,"그루브조인트식 접합 및 배관","D50, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30010040S","노무","L001010101000039",null,"배관공","일반공사 직종","인",9.2999999999999999E-2,0,0,229482,21341.8,0,0,229482,21341.8,null,null,"N","N","",1]
["MBA30010040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.04,0,0,165545,6621.8,0,0,165545,6621.8,null,null,"N","N","",1]
["MBA30010040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,559.20000000000005,559.20000000000005,0,0,0,0,559.20000000000005,559.20000000000005,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,559,0,27963,0,0,0,28522,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30010050S",null,null,null,"그루브조인트식 접합 및 배관","D65, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30010050S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.112,0,0,229482,25701.9,0,0,229482,25701.9,null,null,"N","N","",1]
["MBA30010050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.4999999999999998E-2,0,0,165545,7449.5,0,0,165545,7449.5,null,null,"N","N","",1]
["MBA30010050S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,663,663,0,0,0,0,663,663,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,663,0,33151,0,0,0,33814,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30010060S",null,null,null,"그루브조인트식 접합 및 배관","D80, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30010060S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.14499999999999999,0,0,229482,33274.800000000003,0,0,229482,33274.800000000003,null,null,"N","N","",1]
["MBA30010060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.3999999999999999E-2,0,0,165545,8939.4,0,0,165545,8939.4,null,null,"N","N","",1]
["MBA30010060S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,844.2,844.2,0,0,0,0,844.2,844.2,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,844,0,42214,0,0,0,43058,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30010070S",null,null,null,"그루브조인트식 접합 및 배관","D100, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30010070S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.219,0,0,229482,50256.5,0,0,229482,50256.5,null,null,"N","N","",1]
["MBA30010070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.7000000000000004E-2,0,0,165545,11091.5,0,0,165545,11091.5,null,null,"N","N","",1]
["MBA30010070S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,1226.9000000000001,1226.9000000000001,0,0,0,0,1226.9000000000001,1226.9000000000001,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,1226,0,61348,0,0,0,62574,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30010080S",null,null,null,"그루브조인트식 접합 및 배관","D125, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30010080S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.26,0,0,229482,59665.3,0,0,229482,59665.3,null,null,"N","N","",1]
["MBA30010080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.9000000000000001E-2,0,0,165545,13078,0,0,165545,13078,null,null,"N","N","",1]
["MBA30010080S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,1454.8,1454.8,0,0,0,0,1454.8,1454.8,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,1454,0,72743,0,0,0,74197,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30010090S",null,null,null,"그루브조인트식 접합 및 배관","D150, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30010090S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.32200000000000001,0,0,229482,73893.2,0,0,229482,73893.2,null,null,"N","N","",1]
["MBA30010090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",8.7999999999999995E-2,0,0,165545,14567.9,0,0,165545,14567.9,null,null,"N","N","",1]
["MBA30010090S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,1769.2,1769.2,0,0,0,0,1769.2,1769.2,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,1769,0,88461,0,0,0,90230,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30010100S",null,null,null,"그루브조인트식 접합 및 배관","D200, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30010100S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.44400000000000001,0,0,229482,101890,0,0,229482,101890,null,null,"N","N","",1]
["MBA30010100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.11600000000000001,0,0,165545,19203.2,0,0,165545,19203.2,null,null,"N","N","",1]
["MBA30010100S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,2421.8000000000002,2421.8000000000002,0,0,0,0,2421.8000000000002,2421.8000000000002,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,2421,0,121093,0,0,0,123514,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30010110S",null,null,null,"그루브조인트식 접합 및 배관","D250, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30010110S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.58199999999999996,0,0,229482,133558.5,0,0,229482,133558.5,null,null,"N","N","",1]
["MBA30010110S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.13900000000000001,0,0,165545,23010.7,0,0,165545,23010.7,null,null,"N","N","",1]
["MBA30010110S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,3131.3,3131.3,0,0,0,0,3131.3,3131.3,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,3131,0,156569,0,0,0,159700,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30010120S",null,null,null,"그루브조인트식 접합 및 배관","D300, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30010120S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.74199999999999999,0,0,229482,170275.6,0,0,229482,170275.6,null,null,"N","N","",1]
["MBA30010120S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.154,0,0,165545,25493.9,0,0,165545,25493.9,null,null,"N","N","",1]
["MBA30010120S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,3915.3,3915.3,0,0,0,0,3915.3,3915.3,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,3915,0,195769,0,0,0,199684,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30010130S",null,null,null,"그루브조인트식 접합 및 배관","D350, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30010130S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.89300000000000002,0,0,229482,204927.4,0,0,229482,204927.4,null,null,"N","N","",1]
["MBA30010130S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.17799999999999999,0,0,165545,29467,0,0,165545,29467,null,null,"N","N","",1]
["MBA30010130S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,4687.8,4687.8,0,0,0,0,4687.8,4687.8,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,4687,0,234394,0,0,0,239081,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30010140S",null,null,null,"그루브조인트식 접합 및 배관","D400, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30010140S","노무","L001010101000039",null,"배관공","일반공사 직종","인",1.056,0,0,229482,242332.9,0,0,229482,242332.9,null,null,"N","N","",1]
["MBA30010140S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.20399999999999999,0,0,165545,33771.1,0,0,165545,33771.1,null,null,"N","N","",1]
["MBA30010140S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,5522,5522,0,0,0,0,5522,5522,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,5522,0,276104,0,0,0,281626,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30010150S",null,null,null,"그루브조인트식 접합 및 배관","D450, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30010150S","노무","L001010101000039",null,"배관공","일반공사 직종","인",1.1870000000000001,0,0,229482,272395.09999999998,0,0,229482,272395.09999999998,null,null,"N","N","",1]
["MBA30010150S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.22500000000000001,0,0,165545,37247.599999999999,0,0,165545,37247.599999999999,null,null,"N","N","",1]
["MBA30010150S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,6192.8,6192.8,0,0,0,0,6192.8,6192.8,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,6192,0,309642,0,0,0,315834,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30010160S",null,null,null,"그루브조인트식 접합 및 배관","D500, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30010160S","노무","L001010101000039",null,"배관공","일반공사 직종","인",1.3180000000000001,0,0,229482,302457.2,0,0,229482,302457.2,null,null,"N","N","",1]
["MBA30010160S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.246,0,0,165545,40724,0,0,165545,40724,null,null,"N","N","",1]
["MBA30010160S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,6863.6,6863.6,0,0,0,0,6863.6,6863.6,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,6863,0,343181,0,0,0,350044,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30010170S",null,null,null,"그루브조인트식 접합 및 배관","D550, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30010170S","노무","L001010101000039",null,"배관공","일반공사 직종","인",1.444,0,0,229482,331372,0,0,229482,331372,null,null,"N","N","",1]
["MBA30010170S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.26600000000000001,0,0,165545,44034.9,0,0,165545,44034.9,null,null,"N","N","",1]
["MBA30010170S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,7508.1,7508.1,0,0,0,0,7508.1,7508.1,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,7508,0,375406,0,0,0,382914,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30010180S",null,null,null,"그루브조인트식 접합 및 배관","D600, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30010180S","노무","L001010101000039",null,"배관공","일반공사 직종","인",1.5760000000000001,0,0,229482,361663.6,0,0,229482,361663.6,null,null,"N","N","",1]
["MBA30010180S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.28699999999999998,0,0,165545,47511.4,0,0,165545,47511.4,null,null,"N","N","",1]
["MBA30010180S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,8183.5,8183.5,0,0,0,0,8183.5,8183.5,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,8183,0,409175,0,0,0,417358,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30110010S",null,null,null,"그루브조인트식 접합 및 배관","D25, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30110010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",4.9000000000000002E-2,0,0,229482,11244.6,0,0,229482,11244.6,null,null,"N","Y","",0]
["MBA30110010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5999999999999999E-2,0,0,165545,4304.1000000000004,0,0,165545,4304.1000000000004,null,null,"N","Y","",0]
["MBA30110010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1554.8,1554.8,0,0,0,0,1554.8,1554.8,null,null,"N","N",10,1]
["MBA30110010S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,12438.9,12438.9,0,0,12438.9,12438.9,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,1554,0,12438,0,0,0,13992,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30110020S",null,null,null,"그루브조인트식 접합 및 배관","D32, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30110020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",6.0999999999999999E-2,0,0,229482,13998.4,0,0,229482,13998.4,null,null,"N","Y","",0]
["MBA30110020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.03,0,0,165545,4966.3,0,0,165545,4966.3,null,null,"N","Y","",0]
["MBA30110020S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1896.4,1896.4,0,0,0,0,1896.4,1896.4,null,null,"N","N",10,1]
["MBA30110020S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,15171.7,15171.7,0,0,15171.7,15171.7,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,1896,0,15171,0,0,0,17067,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30110030S",null,null,null,"그루브조인트식 접합 및 배관","D40, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30110030S","노무","L001010101000039",null,"배관공","일반공사 직종","인",6.9000000000000006E-2,0,0,229482,15834.2,0,0,229482,15834.2,null,null,"N","Y","",0]
["MBA30110030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.2000000000000001E-2,0,0,165545,5297.4,0,0,165545,5297.4,null,null,"N","Y","",0]
["MBA30110030S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,2113.1,2113.1,0,0,0,0,2113.1,2113.1,null,null,"N","N",10,1]
["MBA30110030S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,16905.2,16905.2,0,0,16905.2,16905.2,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,2113,0,16905,0,0,0,19018,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30110040S",null,null,null,"그루브조인트식 접합 및 배관","D50, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30110040S","노무","L001010101000039",null,"배관공","일반공사 직종","인",9.2999999999999999E-2,0,0,229482,21341.8,0,0,229482,21341.8,null,null,"N","Y","",0]
["MBA30110040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.04,0,0,165545,6621.8,0,0,165545,6621.8,null,null,"N","Y","",0]
["MBA30110040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,2796.3,2796.3,0,0,0,0,2796.3,2796.3,null,null,"N","N",10,1]
["MBA30110040S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,22370.799999999999,22370.799999999999,0,0,22370.799999999999,22370.799999999999,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,2796,0,22370,0,0,0,25166,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30110050S",null,null,null,"그루브조인트식 접합 및 배관","D65, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30110050S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.112,0,0,229482,25701.9,0,0,229482,25701.9,null,null,"N","Y","",0]
["MBA30110050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.4999999999999998E-2,0,0,165545,7449.5,0,0,165545,7449.5,null,null,"N","Y","",0]
["MBA30110050S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,3315.1,3315.1,0,0,0,0,3315.1,3315.1,null,null,"N","N",10,1]
["MBA30110050S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,26521.1,26521.1,0,0,26521.1,26521.1,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,3315,0,26521,0,0,0,29836,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30110060S",null,null,null,"그루브조인트식 접합 및 배관","D80, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30110060S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.14499999999999999,0,0,229482,33274.800000000003,0,0,229482,33274.800000000003,null,null,"N","Y","",0]
["MBA30110060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.3999999999999999E-2,0,0,165545,8939.4,0,0,165545,8939.4,null,null,"N","Y","",0]
["MBA30110060S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,4221.3999999999996,4221.3999999999996,0,0,0,0,4221.3999999999996,4221.3999999999996,null,null,"N","N",10,1]
["MBA30110060S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,33771.300000000003,33771.300000000003,0,0,33771.300000000003,33771.300000000003,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,4221,0,33771,0,0,0,37992,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30110070S",null,null,null,"그루브조인트식 접합 및 배관","D100, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30110070S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.219,0,0,229482,50256.5,0,0,229482,50256.5,null,null,"N","Y","",0]
["MBA30110070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.7000000000000004E-2,0,0,165545,11091.5,0,0,165545,11091.5,null,null,"N","Y","",0]
["MBA30110070S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,6134.8,6134.8,0,0,0,0,6134.8,6134.8,null,null,"N","N",10,1]
["MBA30110070S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,49078.400000000001,49078.400000000001,0,0,49078.400000000001,49078.400000000001,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,6134,0,49078,0,0,0,55212,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30110080S",null,null,null,"그루브조인트식 접합 및 배관","D125, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30110080S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.26,0,0,229482,59665.3,0,0,229482,59665.3,null,null,"N","Y","",0]
["MBA30110080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.9000000000000001E-2,0,0,165545,13078,0,0,165545,13078,null,null,"N","Y","",0]
["MBA30110080S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,7274.3,7274.3,0,0,0,0,7274.3,7274.3,null,null,"N","N",10,1]
["MBA30110080S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,58194.6,58194.6,0,0,58194.6,58194.6,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,7274,0,58194,0,0,0,65468,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30110090S",null,null,null,"그루브조인트식 접합 및 배관","D150, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30110090S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.32200000000000001,0,0,229482,73893.2,0,0,229482,73893.2,null,null,"N","Y","",0]
["MBA30110090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",8.7999999999999995E-2,0,0,165545,14567.9,0,0,165545,14567.9,null,null,"N","Y","",0]
["MBA30110090S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,8846.1,8846.1,0,0,0,0,8846.1,8846.1,null,null,"N","N",10,1]
["MBA30110090S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,70768.800000000003,70768.800000000003,0,0,70768.800000000003,70768.800000000003,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,8846,0,70768,0,0,0,79614,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30110100S",null,null,null,"그루브조인트식 접합 및 배관","D200, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30110100S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.44400000000000001,0,0,229482,101890,0,0,229482,101890,null,null,"N","Y","",0]
["MBA30110100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.11600000000000001,0,0,165545,19203.2,0,0,165545,19203.2,null,null,"N","Y","",0]
["MBA30110100S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,12109.3,12109.3,0,0,0,0,12109.3,12109.3,null,null,"N","N",10,1]
["MBA30110100S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,96874.5,96874.5,0,0,96874.5,96874.5,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,12109,0,96874,0,0,0,108983,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30110110S",null,null,null,"그루브조인트식 접합 및 배관","D250, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30110110S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.58199999999999996,0,0,229482,133558.5,0,0,229482,133558.5,null,null,"N","Y","",0]
["MBA30110110S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.13900000000000001,0,0,165545,23010.7,0,0,165545,23010.7,null,null,"N","Y","",0]
["MBA30110110S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,15656.9,15656.9,0,0,0,0,15656.9,15656.9,null,null,"N","N",10,1]
["MBA30110110S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,125255.3,125255.3,0,0,125255.3,125255.3,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,15656,0,125255,0,0,0,140911,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30110120S",null,null,null,"그루브조인트식 접합 및 배관","D300, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30110120S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.74199999999999999,0,0,229482,170275.6,0,0,229482,170275.6,null,null,"N","Y","",0]
["MBA30110120S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.154,0,0,165545,25493.9,0,0,165545,25493.9,null,null,"N","Y","",0]
["MBA30110120S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,19576.900000000001,19576.900000000001,0,0,0,0,19576.900000000001,19576.900000000001,null,null,"N","N",10,1]
["MBA30110120S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,156615.6,156615.6,0,0,156615.6,156615.6,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,19576,0,156615,0,0,0,176191,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30110130S",null,null,null,"그루브조인트식 접합 및 배관","D350, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30110130S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.89300000000000002,0,0,229482,204927.4,0,0,229482,204927.4,null,null,"N","Y","",0]
["MBA30110130S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.17799999999999999,0,0,165545,29467,0,0,165545,29467,null,null,"N","Y","",0]
["MBA30110130S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,23439.4,23439.4,0,0,0,0,23439.4,23439.4,null,null,"N","N",10,1]
["MBA30110130S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,187515.5,187515.5,0,0,187515.5,187515.5,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,23439,0,187515,0,0,0,210954,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30110140S",null,null,null,"그루브조인트식 접합 및 배관","D400, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30110140S","노무","L001010101000039",null,"배관공","일반공사 직종","인",1.056,0,0,229482,242332.9,0,0,229482,242332.9,null,null,"N","Y","",0]
["MBA30110140S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.20399999999999999,0,0,165545,33771.1,0,0,165545,33771.1,null,null,"N","Y","",0]
["MBA30110140S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,27610.400000000001,27610.400000000001,0,0,0,0,27610.400000000001,27610.400000000001,null,null,"N","N",10,1]
["MBA30110140S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,220883.20000000001,220883.20000000001,0,0,220883.20000000001,220883.20000000001,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,27610,0,220883,0,0,0,248493,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30110150S",null,null,null,"그루브조인트식 접합 및 배관","D450, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30110150S","노무","L001010101000039",null,"배관공","일반공사 직종","인",1.1870000000000001,0,0,229482,272395.09999999998,0,0,229482,272395.09999999998,null,null,"N","Y","",0]
["MBA30110150S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.22500000000000001,0,0,165545,37247.599999999999,0,0,165545,37247.599999999999,null,null,"N","Y","",0]
["MBA30110150S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,30964.2,30964.2,0,0,0,0,30964.2,30964.2,null,null,"N","N",10,1]
["MBA30110150S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,247714.1,247714.1,0,0,247714.1,247714.1,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,30964,0,247714,0,0,0,278678,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30110160S",null,null,null,"그루브조인트식 접합 및 배관","D500, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30110160S","노무","L001010101000039",null,"배관공","일반공사 직종","인",1.3180000000000001,0,0,229482,302457.2,0,0,229482,302457.2,null,null,"N","Y","",0]
["MBA30110160S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.246,0,0,165545,40724,0,0,165545,40724,null,null,"N","Y","",0]
["MBA30110160S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,34318.1,34318.1,0,0,0,0,34318.1,34318.1,null,null,"N","N",10,1]
["MBA30110160S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,274544.90000000002,274544.90000000002,0,0,274544.90000000002,274544.90000000002,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,34318,0,274544,0,0,0,308862,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30110170S",null,null,null,"그루브조인트식 접합 및 배관","D550, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30110170S","노무","L001010101000039",null,"배관공","일반공사 직종","인",1.444,0,0,229482,331372,0,0,229482,331372,null,null,"N","Y","",0]
["MBA30110170S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.26600000000000001,0,0,165545,44034.9,0,0,165545,44034.9,null,null,"N","Y","",0]
["MBA30110170S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,37540.6,37540.6,0,0,0,0,37540.6,37540.6,null,null,"N","N",10,1]
["MBA30110170S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,300325.5,300325.5,0,0,300325.5,300325.5,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,37540,0,300325,0,0,0,337865,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30110180S",null,null,null,"그루브조인트식 접합 및 배관","D600, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA30110180S","노무","L001010101000039",null,"배관공","일반공사 직종","인",1.5760000000000001,0,0,229482,361663.6,0,0,229482,361663.6,null,null,"N","Y","",0]
["MBA30110180S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.28699999999999998,0,0,165545,47511.4,0,0,165545,47511.4,null,null,"N","Y","",0]
["MBA30110180S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,40917.5,40917.5,0,0,0,0,40917.5,40917.5,null,null,"N","N",10,1]
["MBA30110180S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,327340,327340,0,0,327340,327340,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,40917,0,327340,0,0,0,368257,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31010010S",null,null,null,"그루브조인트식 접합 및 배관","D25, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31010010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",4.9000000000000002E-2,0,0,229482,11244.6,0,0,229482,11244.6,null,null,"N","Y","",0]
["MBA31010010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5999999999999999E-2,0,0,165545,4304.1000000000004,0,0,165545,4304.1000000000004,null,null,"N","Y","",0]
["MBA31010010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,310.89999999999998,310.89999999999998,0,0,0,0,310.89999999999998,310.89999999999998,null,null,"N","N",2,1]
["MBA31010010S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,20213.3,20213.3,0,0,20213.3,20213.3,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,310,0,20213,0,0,0,20523,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31010020S",null,null,null,"그루브조인트식 접합 및 배관","D32, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31010020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",6.0999999999999999E-2,0,0,229482,13998.4,0,0,229482,13998.4,null,null,"N","Y","",0]
["MBA31010020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.03,0,0,165545,4966.3,0,0,165545,4966.3,null,null,"N","Y","",0]
["MBA31010020S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,379.2,379.2,0,0,0,0,379.2,379.2,null,null,"N","N",2,1]
["MBA31010020S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,24654.1,24654.1,0,0,24654.1,24654.1,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,379,0,24654,0,0,0,25033,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31010030S",null,null,null,"그루브조인트식 접합 및 배관","D40, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31010030S","노무","L001010101000039",null,"배관공","일반공사 직종","인",6.9000000000000006E-2,0,0,229482,15834.2,0,0,229482,15834.2,null,null,"N","Y","",0]
["MBA31010030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.2000000000000001E-2,0,0,165545,5297.4,0,0,165545,5297.4,null,null,"N","Y","",0]
["MBA31010030S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,422.6,422.6,0,0,0,0,422.6,422.6,null,null,"N","N",2,1]
["MBA31010030S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,27471,27471,0,0,27471,27471,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,422,0,27471,0,0,0,27893,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31010040S",null,null,null,"그루브조인트식 접합 및 배관","D50, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31010040S","노무","L001010101000039",null,"배관공","일반공사 직종","인",9.2999999999999999E-2,0,0,229482,21341.8,0,0,229482,21341.8,null,null,"N","Y","",0]
["MBA31010040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.04,0,0,165545,6621.8,0,0,165545,6621.8,null,null,"N","Y","",0]
["MBA31010040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,559.20000000000005,559.20000000000005,0,0,0,0,559.20000000000005,559.20000000000005,null,null,"N","N",2,1]
["MBA31010040S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,36352.6,36352.6,0,0,36352.6,36352.6,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,559,0,36352,0,0,0,36911,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31010050S",null,null,null,"그루브조인트식 접합 및 배관","D65, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31010050S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.112,0,0,229482,25701.9,0,0,229482,25701.9,null,null,"N","Y","",0]
["MBA31010050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.4999999999999998E-2,0,0,165545,7449.5,0,0,165545,7449.5,null,null,"N","Y","",0]
["MBA31010050S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,663,663,0,0,0,0,663,663,null,null,"N","N",2,1]
["MBA31010050S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,43096.800000000003,43096.800000000003,0,0,43096.800000000003,43096.800000000003,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,663,0,43096,0,0,0,43759,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31010060S",null,null,null,"그루브조인트식 접합 및 배관","D80, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31010060S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.14499999999999999,0,0,229482,33274.800000000003,0,0,229482,33274.800000000003,null,null,"N","Y","",0]
["MBA31010060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.3999999999999999E-2,0,0,165545,8939.4,0,0,165545,8939.4,null,null,"N","Y","",0]
["MBA31010060S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,844.2,844.2,0,0,0,0,844.2,844.2,null,null,"N","N",2,1]
["MBA31010060S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,54878.400000000001,54878.400000000001,0,0,54878.400000000001,54878.400000000001,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,844,0,54878,0,0,0,55722,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31010070S",null,null,null,"그루브조인트식 접합 및 배관","D100, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31010070S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.219,0,0,229482,50256.5,0,0,229482,50256.5,null,null,"N","Y","",0]
["MBA31010070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.7000000000000004E-2,0,0,165545,11091.5,0,0,165545,11091.5,null,null,"N","Y","",0]
["MBA31010070S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,1226.9000000000001,1226.9000000000001,0,0,0,0,1226.9000000000001,1226.9000000000001,null,null,"N","N",2,1]
["MBA31010070S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,79752.399999999994,79752.399999999994,0,0,79752.399999999994,79752.399999999994,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,1226,0,79752,0,0,0,80978,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31010080S",null,null,null,"그루브조인트식 접합 및 배관","D125, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31010080S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.26,0,0,229482,59665.3,0,0,229482,59665.3,null,null,"N","Y","",0]
["MBA31010080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.9000000000000001E-2,0,0,165545,13078,0,0,165545,13078,null,null,"N","Y","",0]
["MBA31010080S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,1454.8,1454.8,0,0,0,0,1454.8,1454.8,null,null,"N","N",2,1]
["MBA31010080S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,94566.2,94566.2,0,0,94566.2,94566.2,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,1454,0,94566,0,0,0,96020,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31010090S",null,null,null,"그루브조인트식 접합 및 배관","D150, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31010090S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.32200000000000001,0,0,229482,73893.2,0,0,229482,73893.2,null,null,"N","Y","",0]
["MBA31010090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",8.7999999999999995E-2,0,0,165545,14567.9,0,0,165545,14567.9,null,null,"N","Y","",0]
["MBA31010090S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,1769.2,1769.2,0,0,0,0,1769.2,1769.2,null,null,"N","N",2,1]
["MBA31010090S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,114999.4,114999.4,0,0,114999.4,114999.4,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,1769,0,114999,0,0,0,116768,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31010100S",null,null,null,"그루브조인트식 접합 및 배관","D200, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31010100S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.44400000000000001,0,0,229482,101890,0,0,229482,101890,null,null,"N","Y","",0]
["MBA31010100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.11600000000000001,0,0,165545,19203.2,0,0,165545,19203.2,null,null,"N","Y","",0]
["MBA31010100S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,2421.8000000000002,2421.8000000000002,0,0,0,0,2421.8000000000002,2421.8000000000002,null,null,"N","N",2,1]
["MBA31010100S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,157421.1,157421.1,0,0,157421.1,157421.1,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,2421,0,157421,0,0,0,159842,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31010110S",null,null,null,"그루브조인트식 접합 및 배관","D250, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31010110S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.58199999999999996,0,0,229482,133558.5,0,0,229482,133558.5,null,null,"N","Y","",0]
["MBA31010110S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.13900000000000001,0,0,165545,23010.7,0,0,165545,23010.7,null,null,"N","Y","",0]
["MBA31010110S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,3131.3,3131.3,0,0,0,0,3131.3,3131.3,null,null,"N","N",2,1]
["MBA31010110S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,203539.9,203539.9,0,0,203539.9,203539.9,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,3131,0,203539,0,0,0,206670,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31010120S",null,null,null,"그루브조인트식 접합 및 배관","D300, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31010120S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.74199999999999999,0,0,229482,170275.6,0,0,229482,170275.6,null,null,"N","Y","",0]
["MBA31010120S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.154,0,0,165545,25493.9,0,0,165545,25493.9,null,null,"N","Y","",0]
["MBA31010120S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,3915.3,3915.3,0,0,0,0,3915.3,3915.3,null,null,"N","N",2,1]
["MBA31010120S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,254500.3,254500.3,0,0,254500.3,254500.3,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,3915,0,254500,0,0,0,258415,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31010130S",null,null,null,"그루브조인트식 접합 및 배관","D350, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31010130S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.89300000000000002,0,0,229482,204927.4,0,0,229482,204927.4,null,null,"N","Y","",0]
["MBA31010130S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.17799999999999999,0,0,165545,29467,0,0,165545,29467,null,null,"N","Y","",0]
["MBA31010130S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,4687.8,4687.8,0,0,0,0,4687.8,4687.8,null,null,"N","N",2,1]
["MBA31010130S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,304712.7,304712.7,0,0,304712.7,304712.7,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,4687,0,304712,0,0,0,309399,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31010140S",null,null,null,"그루브조인트식 접합 및 배관","D400, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31010140S","노무","L001010101000039",null,"배관공","일반공사 직종","인",1.056,0,0,229482,242332.9,0,0,229482,242332.9,null,null,"N","Y","",0]
["MBA31010140S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.20399999999999999,0,0,165545,33771.1,0,0,165545,33771.1,null,null,"N","Y","",0]
["MBA31010140S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,5522,5522,0,0,0,0,5522,5522,null,null,"N","N",2,1]
["MBA31010140S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,358935.2,358935.2,0,0,358935.2,358935.2,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,5522,0,358935,0,0,0,364457,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31010150S",null,null,null,"그루브조인트식 접합 및 배관","D450, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31010150S","노무","L001010101000039",null,"배관공","일반공사 직종","인",1.1870000000000001,0,0,229482,272395.09999999998,0,0,229482,272395.09999999998,null,null,"N","Y","",0]
["MBA31010150S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.22500000000000001,0,0,165545,37247.599999999999,0,0,165545,37247.599999999999,null,null,"N","Y","",0]
["MBA31010150S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,6192.8,6192.8,0,0,0,0,6192.8,6192.8,null,null,"N","N",2,1]
["MBA31010150S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,402535.5,402535.5,0,0,402535.5,402535.5,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,6192,0,402535,0,0,0,408727,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31010160S",null,null,null,"그루브조인트식 접합 및 배관","D500, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31010160S","노무","L001010101000039",null,"배관공","일반공사 직종","인",1.3180000000000001,0,0,229482,302457.2,0,0,229482,302457.2,null,null,"N","Y","",0]
["MBA31010160S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.246,0,0,165545,40724,0,0,165545,40724,null,null,"N","Y","",0]
["MBA31010160S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,6863.6,6863.6,0,0,0,0,6863.6,6863.6,null,null,"N","N",2,1]
["MBA31010160S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,446135.5,446135.5,0,0,446135.5,446135.5,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,6863,0,446135,0,0,0,452998,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31010170S",null,null,null,"그루브조인트식 접합 및 배관","D550, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31010170S","노무","L001010101000039",null,"배관공","일반공사 직종","인",1.444,0,0,229482,331372,0,0,229482,331372,null,null,"N","Y","",0]
["MBA31010170S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.26600000000000001,0,0,165545,44034.9,0,0,165545,44034.9,null,null,"N","Y","",0]
["MBA31010170S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,7508.1,7508.1,0,0,0,0,7508.1,7508.1,null,null,"N","N",2,1]
["MBA31010170S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,488028.9,488028.9,0,0,488028.9,488028.9,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,7508,0,488028,0,0,0,495536,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31010180S",null,null,null,"그루브조인트식 접합 및 배관","D600, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31010180S","노무","L001010101000039",null,"배관공","일반공사 직종","인",1.5760000000000001,0,0,229482,361663.6,0,0,229482,361663.6,null,null,"N","Y","",0]
["MBA31010180S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.28699999999999998,0,0,165545,47511.4,0,0,165545,47511.4,null,null,"N","Y","",0]
["MBA31010180S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,8183.5,8183.5,0,0,0,0,8183.5,8183.5,null,null,"N","N",2,1]
["MBA31010180S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,531927.5,531927.5,0,0,531927.5,531927.5,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,8183,0,531927,0,0,0,540110,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31110010S",null,null,null,"그루브조인트식 접합 및 배관","D25, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31110010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",4.9000000000000002E-2,0,0,229482,11244.6,0,0,229482,11244.6,null,null,"N","Y","",0]
["MBA31110010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5999999999999999E-2,0,0,165545,4304.1000000000004,0,0,165545,4304.1000000000004,null,null,"N","Y","",0]
["MBA31110010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1554.8,1554.8,0,0,0,0,1554.8,1554.8,null,null,"N","N",10,1]
["MBA31110010S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,17103.5,17103.5,0,0,17103.5,17103.5,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,1554,0,17103,0,0,0,18657,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31110020S",null,null,null,"그루브조인트식 접합 및 배관","D32, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31110020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",6.0999999999999999E-2,0,0,229482,13998.4,0,0,229482,13998.4,null,null,"N","Y","",0]
["MBA31110020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.03,0,0,165545,4966.3,0,0,165545,4966.3,null,null,"N","Y","",0]
["MBA31110020S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1896.4,1896.4,0,0,0,0,1896.4,1896.4,null,null,"N","N",10,1]
["MBA31110020S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,20861.099999999999,20861.099999999999,0,0,20861.099999999999,20861.099999999999,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,1896,0,20861,0,0,0,22757,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31110030S",null,null,null,"그루브조인트식 접합 및 배관","D40, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31110030S","노무","L001010101000039",null,"배관공","일반공사 직종","인",6.9000000000000006E-2,0,0,229482,15834.2,0,0,229482,15834.2,null,null,"N","Y","",0]
["MBA31110030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.2000000000000001E-2,0,0,165545,5297.4,0,0,165545,5297.4,null,null,"N","Y","",0]
["MBA31110030S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,2113.1,2113.1,0,0,0,0,2113.1,2113.1,null,null,"N","N",10,1]
["MBA31110030S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,23244.7,23244.7,0,0,23244.7,23244.7,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,2113,0,23244,0,0,0,25357,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31110040S",null,null,null,"그루브조인트식 접합 및 배관","D50, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31110040S","노무","L001010101000039",null,"배관공","일반공사 직종","인",9.2999999999999999E-2,0,0,229482,21341.8,0,0,229482,21341.8,null,null,"N","Y","",0]
["MBA31110040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.04,0,0,165545,6621.8,0,0,165545,6621.8,null,null,"N","Y","",0]
["MBA31110040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,2796.3,2796.3,0,0,0,0,2796.3,2796.3,null,null,"N","N",10,1]
["MBA31110040S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,30759.9,30759.9,0,0,30759.9,30759.9,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,2796,0,30759,0,0,0,33555,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31110050S",null,null,null,"그루브조인트식 접합 및 배관","D65, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31110050S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.112,0,0,229482,25701.9,0,0,229482,25701.9,null,null,"N","Y","",0]
["MBA31110050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.4999999999999998E-2,0,0,165545,7449.5,0,0,165545,7449.5,null,null,"N","Y","",0]
["MBA31110050S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,3315.1,3315.1,0,0,0,0,3315.1,3315.1,null,null,"N","N",10,1]
["MBA31110050S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,36466.5,36466.5,0,0,36466.5,36466.5,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,3315,0,36466,0,0,0,39781,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31110060S",null,null,null,"그루브조인트식 접합 및 배관","D80, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31110060S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.14499999999999999,0,0,229482,33274.800000000003,0,0,229482,33274.800000000003,null,null,"N","Y","",0]
["MBA31110060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.3999999999999999E-2,0,0,165545,8939.4,0,0,165545,8939.4,null,null,"N","Y","",0]
["MBA31110060S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,4221.3999999999996,4221.3999999999996,0,0,0,0,4221.3999999999996,4221.3999999999996,null,null,"N","N",10,1]
["MBA31110060S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,46435.6,46435.6,0,0,46435.6,46435.6,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,4221,0,46435,0,0,0,50656,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31110070S",null,null,null,"그루브조인트식 접합 및 배관","D100, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31110070S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.219,0,0,229482,50256.5,0,0,229482,50256.5,null,null,"N","Y","",0]
["MBA31110070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.7000000000000004E-2,0,0,165545,11091.5,0,0,165545,11091.5,null,null,"N","Y","",0]
["MBA31110070S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,6134.8,6134.8,0,0,0,0,6134.8,6134.8,null,null,"N","N",10,1]
["MBA31110070S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,67482.8,67482.8,0,0,67482.8,67482.8,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,6134,0,67482,0,0,0,73616,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31110080S",null,null,null,"그루브조인트식 접합 및 배관","D125, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31110080S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.26,0,0,229482,59665.3,0,0,229482,59665.3,null,null,"N","Y","",0]
["MBA31110080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.9000000000000001E-2,0,0,165545,13078,0,0,165545,13078,null,null,"N","Y","",0]
["MBA31110080S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,7274.3,7274.3,0,0,0,0,7274.3,7274.3,null,null,"N","N",10,1]
["MBA31110080S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,80017.600000000006,80017.600000000006,0,0,80017.600000000006,80017.600000000006,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,7274,0,80017,0,0,0,87291,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31110090S",null,null,null,"그루브조인트식 접합 및 배관","D150, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31110090S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.32200000000000001,0,0,229482,73893.2,0,0,229482,73893.2,null,null,"N","Y","",0]
["MBA31110090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",8.7999999999999995E-2,0,0,165545,14567.9,0,0,165545,14567.9,null,null,"N","Y","",0]
["MBA31110090S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,8846.1,8846.1,0,0,0,0,8846.1,8846.1,null,null,"N","N",10,1]
["MBA31110090S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,97307.199999999997,97307.199999999997,0,0,97307.199999999997,97307.199999999997,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,8846,0,97307,0,0,0,106153,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31110100S",null,null,null,"그루브조인트식 접합 및 배관","D200, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31110100S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.44400000000000001,0,0,229482,101890,0,0,229482,101890,null,null,"N","Y","",0]
["MBA31110100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.11600000000000001,0,0,165545,19203.2,0,0,165545,19203.2,null,null,"N","Y","",0]
["MBA31110100S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,12109.3,12109.3,0,0,0,0,12109.3,12109.3,null,null,"N","N",10,1]
["MBA31110100S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,133202.5,133202.5,0,0,133202.5,133202.5,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,12109,0,133202,0,0,0,145311,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31110110S",null,null,null,"그루브조인트식 접합 및 배관","D250, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31110110S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.58199999999999996,0,0,229482,133558.5,0,0,229482,133558.5,null,null,"N","Y","",0]
["MBA31110110S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.13900000000000001,0,0,165545,23010.7,0,0,165545,23010.7,null,null,"N","Y","",0]
["MBA31110110S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,15656.9,15656.9,0,0,0,0,15656.9,15656.9,null,null,"N","N",10,1]
["MBA31110110S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,172226.1,172226.1,0,0,172226.1,172226.1,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,15656,0,172226,0,0,0,187882,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31110120S",null,null,null,"그루브조인트식 접합 및 배관","D300, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31110120S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.74199999999999999,0,0,229482,170275.6,0,0,229482,170275.6,null,null,"N","Y","",0]
["MBA31110120S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.154,0,0,165545,25493.9,0,0,165545,25493.9,null,null,"N","Y","",0]
["MBA31110120S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,19576.900000000001,19576.900000000001,0,0,0,0,19576.900000000001,19576.900000000001,null,null,"N","N",10,1]
["MBA31110120S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,215346.4,215346.4,0,0,215346.4,215346.4,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,19576,0,215346,0,0,0,234922,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31110130S",null,null,null,"그루브조인트식 접합 및 배관","D350, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31110130S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.89300000000000002,0,0,229482,204927.4,0,0,229482,204927.4,null,null,"N","Y","",0]
["MBA31110130S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.17799999999999999,0,0,165545,29467,0,0,165545,29467,null,null,"N","Y","",0]
["MBA31110130S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,23439.4,23439.4,0,0,0,0,23439.4,23439.4,null,null,"N","N",10,1]
["MBA31110130S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,257833.8,257833.8,0,0,257833.8,257833.8,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,23439,0,257833,0,0,0,281272,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31110140S",null,null,null,"그루브조인트식 접합 및 배관","D400, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31110140S","노무","L001010101000039",null,"배관공","일반공사 직종","인",1.056,0,0,229482,242332.9,0,0,229482,242332.9,null,null,"N","Y","",0]
["MBA31110140S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.20399999999999999,0,0,165545,33771.1,0,0,165545,33771.1,null,null,"N","Y","",0]
["MBA31110140S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,27610.400000000001,27610.400000000001,0,0,0,0,27610.400000000001,27610.400000000001,null,null,"N","N",10,1]
["MBA31110140S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,303714.40000000002,303714.40000000002,0,0,303714.40000000002,303714.40000000002,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,27610,0,303714,0,0,0,331324,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31110150S",null,null,null,"그루브조인트식 접합 및 배관","D450, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31110150S","노무","L001010101000039",null,"배관공","일반공사 직종","인",1.1870000000000001,0,0,229482,272395.09999999998,0,0,229482,272395.09999999998,null,null,"N","Y","",0]
["MBA31110150S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.22500000000000001,0,0,165545,37247.599999999999,0,0,165545,37247.599999999999,null,null,"N","Y","",0]
["MBA31110150S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,30964.2,30964.2,0,0,0,0,30964.2,30964.2,null,null,"N","N",10,1]
["MBA31110150S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,340606.9,340606.9,0,0,340606.9,340606.9,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,30964,0,340606,0,0,0,371570,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31110160S",null,null,null,"그루브조인트식 접합 및 배관","D500, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31110160S","노무","L001010101000039",null,"배관공","일반공사 직종","인",1.3180000000000001,0,0,229482,302457.2,0,0,229482,302457.2,null,null,"N","Y","",0]
["MBA31110160S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.246,0,0,165545,40724,0,0,165545,40724,null,null,"N","Y","",0]
["MBA31110160S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,34318.1,34318.1,0,0,0,0,34318.1,34318.1,null,null,"N","N",10,1]
["MBA31110160S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,377499.3,377499.3,0,0,377499.3,377499.3,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,34318,0,377499,0,0,0,411817,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31110170S",null,null,null,"그루브조인트식 접합 및 배관","D550, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31110170S","노무","L001010101000039",null,"배관공","일반공사 직종","인",1.444,0,0,229482,331372,0,0,229482,331372,null,null,"N","Y","",0]
["MBA31110170S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.26600000000000001,0,0,165545,44034.9,0,0,165545,44034.9,null,null,"N","Y","",0]
["MBA31110170S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,37540.6,37540.6,0,0,0,0,37540.6,37540.6,null,null,"N","N",10,1]
["MBA31110170S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,412947.5,412947.5,0,0,412947.5,412947.5,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,37540,0,412947,0,0,0,450487,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31110180S",null,null,null,"그루브조인트식 접합 및 배관","D600, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA31110180S","노무","L001010101000039",null,"배관공","일반공사 직종","인",1.5760000000000001,0,0,229482,361663.6,0,0,229482,361663.6,null,null,"N","Y","",0]
["MBA31110180S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.28699999999999998,0,0,165545,47511.4,0,0,165545,47511.4,null,null,"N","Y","",0]
["MBA31110180S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,40917.5,40917.5,0,0,0,0,40917.5,40917.5,null,null,"N","N",10,1]
["MBA31110180S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,450092.5,450092.5,0,0,450092.5,450092.5,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,40917,0,450092,0,0,0,491009,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32010010S",null,null,null,"그루브조인트식 접합 및 배관","D25, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32010010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",4.9000000000000002E-2,0,0,229482,11244.6,0,0,229482,11244.6,null,null,"N","Y","",0]
["MBA32010010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5999999999999999E-2,0,0,165545,4304.1000000000004,0,0,165545,4304.1000000000004,null,null,"N","Y","",0]
["MBA32010010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,310.89999999999998,310.89999999999998,0,0,0,0,310.89999999999998,310.89999999999998,null,null,"N","N",2,1]
["MBA32010010S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,18658.400000000001,18658.400000000001,0,0,18658.400000000001,18658.400000000001,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,310,0,18658,0,0,0,18968,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32010020S",null,null,null,"그루브조인트식 접합 및 배관","D32, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32010020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",6.0999999999999999E-2,0,0,229482,13998.4,0,0,229482,13998.4,null,null,"N","Y","",0]
["MBA32010020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.03,0,0,165545,4966.3,0,0,165545,4966.3,null,null,"N","Y","",0]
["MBA32010020S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,379.2,379.2,0,0,0,0,379.2,379.2,null,null,"N","N",2,1]
["MBA32010020S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,22757.599999999999,22757.599999999999,0,0,22757.599999999999,22757.599999999999,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,379,0,22757,0,0,0,23136,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32010030S",null,null,null,"그루브조인트식 접합 및 배관","D40, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32010030S","노무","L001010101000039",null,"배관공","일반공사 직종","인",6.9000000000000006E-2,0,0,229482,15834.2,0,0,229482,15834.2,null,null,"N","Y","",0]
["MBA32010030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.2000000000000001E-2,0,0,165545,5297.4,0,0,165545,5297.4,null,null,"N","Y","",0]
["MBA32010030S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,422.6,422.6,0,0,0,0,422.6,422.6,null,null,"N","N",2,1]
["MBA32010030S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,25357.9,25357.9,0,0,25357.9,25357.9,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,422,0,25357,0,0,0,25779,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32010040S",null,null,null,"그루브조인트식 접합 및 배관","D50, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32010040S","노무","L001010101000039",null,"배관공","일반공사 직종","인",9.2999999999999999E-2,0,0,229482,21341.8,0,0,229482,21341.8,null,null,"N","Y","",0]
["MBA32010040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.04,0,0,165545,6621.8,0,0,165545,6621.8,null,null,"N","Y","",0]
["MBA32010040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,559.20000000000005,559.20000000000005,0,0,0,0,559.20000000000005,559.20000000000005,null,null,"N","N",2,1]
["MBA32010040S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,33556.300000000003,33556.300000000003,0,0,33556.300000000003,33556.300000000003,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,559,0,33556,0,0,0,34115,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32010050S",null,null,null,"그루브조인트식 접합 및 배관","D65, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32010050S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.112,0,0,229482,25701.9,0,0,229482,25701.9,null,null,"N","Y","",0]
["MBA32010050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.4999999999999998E-2,0,0,165545,7449.5,0,0,165545,7449.5,null,null,"N","Y","",0]
["MBA32010050S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,663,663,0,0,0,0,663,663,null,null,"N","N",2,1]
["MBA32010050S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,39781.599999999999,39781.599999999999,0,0,39781.599999999999,39781.599999999999,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,663,0,39781,0,0,0,40444,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32010060S",null,null,null,"그루브조인트식 접합 및 배관","D80, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32010060S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.14499999999999999,0,0,229482,33274.800000000003,0,0,229482,33274.800000000003,null,null,"N","Y","",0]
["MBA32010060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.3999999999999999E-2,0,0,165545,8939.4,0,0,165545,8939.4,null,null,"N","Y","",0]
["MBA32010060S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,844.2,844.2,0,0,0,0,844.2,844.2,null,null,"N","N",2,1]
["MBA32010060S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,50657,50657,0,0,50657,50657,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,844,0,50657,0,0,0,51501,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32010070S",null,null,null,"그루브조인트식 접합 및 배관","D100, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32010070S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.219,0,0,229482,50256.5,0,0,229482,50256.5,null,null,"N","Y","",0]
["MBA32010070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.7000000000000004E-2,0,0,165545,11091.5,0,0,165545,11091.5,null,null,"N","Y","",0]
["MBA32010070S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,1226.9000000000001,1226.9000000000001,0,0,0,0,1226.9000000000001,1226.9000000000001,null,null,"N","N",2,1]
["MBA32010070S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,73617.600000000006,73617.600000000006,0,0,73617.600000000006,73617.600000000006,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,1226,0,73617,0,0,0,74843,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32010080S",null,null,null,"그루브조인트식 접합 및 배관","D125, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32010080S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.26,0,0,229482,59665.3,0,0,229482,59665.3,null,null,"N","Y","",0]
["MBA32010080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.9000000000000001E-2,0,0,165545,13078,0,0,165545,13078,null,null,"N","Y","",0]
["MBA32010080S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,1454.8,1454.8,0,0,0,0,1454.8,1454.8,null,null,"N","N",2,1]
["MBA32010080S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,87291.9,87291.9,0,0,87291.9,87291.9,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,1454,0,87291,0,0,0,88745,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32010090S",null,null,null,"그루브조인트식 접합 및 배관","D150, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32010090S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.32200000000000001,0,0,229482,73893.2,0,0,229482,73893.2,null,null,"N","Y","",0]
["MBA32010090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",8.7999999999999995E-2,0,0,165545,14567.9,0,0,165545,14567.9,null,null,"N","Y","",0]
["MBA32010090S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,1769.2,1769.2,0,0,0,0,1769.2,1769.2,null,null,"N","N",2,1]
["MBA32010090S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,106153.3,106153.3,0,0,106153.3,106153.3,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,1769,0,106153,0,0,0,107922,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32010100S",null,null,null,"그루브조인트식 접합 및 배관","D200, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32010100S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.44400000000000001,0,0,229482,101890,0,0,229482,101890,null,null,"N","Y","",0]
["MBA32010100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.11600000000000001,0,0,165545,19203.2,0,0,165545,19203.2,null,null,"N","Y","",0]
["MBA32010100S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,2421.8000000000002,2421.8000000000002,0,0,0,0,2421.8000000000002,2421.8000000000002,null,null,"N","N",2,1]
["MBA32010100S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,145311.79999999999,145311.79999999999,0,0,145311.79999999999,145311.79999999999,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,2421,0,145311,0,0,0,147732,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32010110S",null,null,null,"그루브조인트식 접합 및 배관","D250, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32010110S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.58199999999999996,0,0,229482,133558.5,0,0,229482,133558.5,null,null,"N","Y","",0]
["MBA32010110S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.13900000000000001,0,0,165545,23010.7,0,0,165545,23010.7,null,null,"N","Y","",0]
["MBA32010110S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,3131.3,3131.3,0,0,0,0,3131.3,3131.3,null,null,"N","N",2,1]
["MBA32010110S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,187883,187883,0,0,187883,187883,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,3131,0,187883,0,0,0,191014,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32010120S",null,null,null,"그루브조인트식 접합 및 배관","D300, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32010120S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.74199999999999999,0,0,229482,170275.6,0,0,229482,170275.6,null,null,"N","Y","",0]
["MBA32010120S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.154,0,0,165545,25493.9,0,0,165545,25493.9,null,null,"N","Y","",0]
["MBA32010120S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,3915.3,3915.3,0,0,0,0,3915.3,3915.3,null,null,"N","N",2,1]
["MBA32010120S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,234923.4,234923.4,0,0,234923.4,234923.4,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,3915,0,234923,0,0,0,238838,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32010130S",null,null,null,"그루브조인트식 접합 및 배관","D350, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32010130S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.89300000000000002,0,0,229482,204927.4,0,0,229482,204927.4,null,null,"N","Y","",0]
["MBA32010130S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.17799999999999999,0,0,165545,29467,0,0,165545,29467,null,null,"N","Y","",0]
["MBA32010130S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,4687.8,4687.8,0,0,0,0,4687.8,4687.8,null,null,"N","N",2,1]
["MBA32010130S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,281273.2,281273.2,0,0,281273.2,281273.2,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,4687,0,281273,0,0,0,285960,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32010140S",null,null,null,"그루브조인트식 접합 및 배관","D400, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32010140S","노무","L001010101000039",null,"배관공","일반공사 직종","인",1.056,0,0,229482,242332.9,0,0,229482,242332.9,null,null,"N","Y","",0]
["MBA32010140S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.20399999999999999,0,0,165545,33771.1,0,0,165545,33771.1,null,null,"N","Y","",0]
["MBA32010140S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,5522,5522,0,0,0,0,5522,5522,null,null,"N","N",2,1]
["MBA32010140S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,331324.79999999999,331324.79999999999,0,0,331324.79999999999,331324.79999999999,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,5522,0,331324,0,0,0,336846,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32010150S",null,null,null,"그루브조인트식 접합 및 배관","D450, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32010150S","노무","L001010101000039",null,"배관공","일반공사 직종","인",1.1870000000000001,0,0,229482,272395.09999999998,0,0,229482,272395.09999999998,null,null,"N","Y","",0]
["MBA32010150S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.22500000000000001,0,0,165545,37247.599999999999,0,0,165545,37247.599999999999,null,null,"N","Y","",0]
["MBA32010150S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,6192.8,6192.8,0,0,0,0,6192.8,6192.8,null,null,"N","N",2,1]
["MBA32010150S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,371571.20000000001,371571.20000000001,0,0,371571.20000000001,371571.20000000001,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,6192,0,371571,0,0,0,377763,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32010160S",null,null,null,"그루브조인트식 접합 및 배관","D500, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32010160S","노무","L001010101000039",null,"배관공","일반공사 직종","인",1.3180000000000001,0,0,229482,302457.2,0,0,229482,302457.2,null,null,"N","Y","",0]
["MBA32010160S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.246,0,0,165545,40724,0,0,165545,40724,null,null,"N","Y","",0]
["MBA32010160S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,6863.6,6863.6,0,0,0,0,6863.6,6863.6,null,null,"N","N",2,1]
["MBA32010160S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,411817.4,411817.4,0,0,411817.4,411817.4,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,6863,0,411817,0,0,0,418680,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32010170S",null,null,null,"그루브조인트식 접합 및 배관","D550, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32010170S","노무","L001010101000039",null,"배관공","일반공사 직종","인",1.444,0,0,229482,331372,0,0,229482,331372,null,null,"N","Y","",0]
["MBA32010170S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.26600000000000001,0,0,165545,44034.9,0,0,165545,44034.9,null,null,"N","Y","",0]
["MBA32010170S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,7508.1,7508.1,0,0,0,0,7508.1,7508.1,null,null,"N","N",2,1]
["MBA32010170S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,450488.2,450488.2,0,0,450488.2,450488.2,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,7508,0,450488,0,0,0,457996,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32010180S",null,null,null,"그루브조인트식 접합 및 배관","D600, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32010180S","노무","L001010101000039",null,"배관공","일반공사 직종","인",1.5760000000000001,0,0,229482,361663.6,0,0,229482,361663.6,null,null,"N","Y","",0]
["MBA32010180S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.28699999999999998,0,0,165545,47511.4,0,0,165545,47511.4,null,null,"N","Y","",0]
["MBA32010180S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,8183.5,8183.5,0,0,0,0,8183.5,8183.5,null,null,"N","N",2,1]
["MBA32010180S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,491010,491010,0,0,491010,491010,null,null,"N","N",120,1]
["MBA32110010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5999999999999999E-2,0,0,165545,4304.1000000000004,0,0,165545,4304.1000000000004,null,null,"N","Y","",0]
["MBA32110020S",null,null,null,"그루브조인트식 접합 및 배관","D32, 화장실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32110030S","노무","L001010101000039",null,"배관공","일반공사 직종","인",6.9000000000000006E-2,0,0,229482,15834.2,0,0,229482,15834.2,null,null,"N","Y","",0]
["MBA32110040S",null,null,null,"그루브조인트식 접합 및 배관","D50, 화장실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32110050S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.112,0,0,229482,25701.9,0,0,229482,25701.9,null,null,"N","Y","",0]
[null,null,null,null,"[합 계]",null,null,0,0,4221,0,42214,0,0,0,46435,null,null,null,null,"",1]
["MBA32110070S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.219,0,0,229482,50256.5,0,0,229482,50256.5,null,null,"N","Y","",0]
["MBA32110080S",null,null,null,"그루브조인트식 접합 및 배관","D125, 화장실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA32110090S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.32200000000000001,0,0,229482,73893.2,0,0,229482,73893.2,null,null,"N","Y","",0]
["MBA32110100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.11600000000000001,0,0,165545,19203.2,0,0,165545,19203.2,null,null,"N","Y","",0]
["MBA32110110S","손료","RENT000000000002",null,"노무할증 20%증+20%감","노무비의 100%","식",1,0,0,156569.20000000001,156569.20000000001,0,0,156569.20000000001,156569.20000000001,null,null,"N","N",100,1]
["MBA32110120S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.154,0,0,165545,25493.9,0,0,165545,25493.9,null,null,"N","Y","",0]
["MBA32110130S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,23439.4,23439.4,0,0,0,0,23439.4,23439.4,null,null,"N","N",10,1]
["MBA32110150S","노무","L001010101000039",null,"배관공","일반공사 직종","인",1.1870000000000001,0,0,229482,272395.09999999998,0,0,229482,272395.09999999998,null,null,"N","Y","",0]
["MBA32110150S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,30964.2,30964.2,0,0,0,0,30964.2,30964.2,null,null,"N","N",10,1]
["MBA32110160S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,34318.1,34318.1,0,0,0,0,34318.1,34318.1,null,null,"N","N",10,1]
["MBA32110180S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,40917.5,40917.5,0,0,0,0,40917.5,40917.5,null,null,"N","N",10,1]
["MBA32110180S","손료","RENT000000000002",null,"노무할증 20%증+20%감","노무비의 100%","식",1,0,0,409175,409175,0,0,409175,409175,null,null,"N","N",100,1]
["MBA33010020S",null,null,null,"그루브조인트식 접합 및 배관","D32, 옥외배관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA33010030S","손료","RENT000000000002",null,"노무할증 10%감","노무비의 90%","식",1,0,0,19018.400000000001,19018.400000000001,0,0,19018.400000000001,19018.400000000001,null,null,"N","N",90,1]
[null,null,null,null,"[합 계]",null,null,0,0,422,0,19018,0,0,0,19440,null,null,null,null,"",1]
["MBA33010050S","손료","RENT000000000002",null,"노무할증 10%감","노무비의 90%","식",1,0,0,29836.2,29836.2,0,0,29836.2,29836.2,null,null,"N","N",90,1]
[null,null,null,null,"[합 계]",null,null,0,0,844,0,37992,0,0,0,38836,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,1454,0,65468,0,0,0,66922,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA33010100S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,2421.8000000000002,2421.8000000000002,0,0,0,0,2421.8000000000002,2421.8000000000002,null,null,"N","N",2,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA33010130S",null,null,null,"그루브조인트식 접합 및 배관","D350, 옥외배관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA33010140S",null,null,null,"그루브조인트식 접합 및 배관","D400, 옥외배관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA33010150S",null,null,null,"그루브조인트식 접합 및 배관","D450, 옥외배관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA33010150S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.22500000000000001,0,0,165545,37247.599999999999,0,0,165545,37247.599999999999,null,null,"N","Y","",0]
["MBA33010170S",null,null,null,"그루브조인트식 접합 및 배관","D550, 옥외배관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA33010180S","노무","L001010101000039",null,"배관공","일반공사 직종","인",1.5760000000000001,0,0,229482,361663.6,0,0,229482,361663.6,null,null,"N","Y","",0]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA33110020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",6.0999999999999999E-2,0,0,229482,13998.4,0,0,229482,13998.4,null,null,"N","Y","",0]
["MBA33110030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.2000000000000001E-2,0,0,165545,5297.4,0,0,165545,5297.4,null,null,"N","Y","",0]
["MBA33110040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,2796.3,2796.3,0,0,0,0,2796.3,2796.3,null,null,"N","N",10,1]
["MBA33110050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.4999999999999998E-2,0,0,165545,7449.5,0,0,165545,7449.5,null,null,"N","Y","",0]
[null,null,null,null,"[합 계]",null,null,0,0,3315,0,23205,0,0,0,26520,null,null,null,null,"",1]
["MBA33110070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.7000000000000004E-2,0,0,165545,11091.5,0,0,165545,11091.5,null,null,"N","Y","",0]
["MBA33110080S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,7274.3,7274.3,0,0,0,0,7274.3,7274.3,null,null,"N","N",10,1]
["MBA33110090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",8.7999999999999995E-2,0,0,165545,14567.9,0,0,165545,14567.9,null,null,"N","Y","",0]
["MBA33110100S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,12109.3,12109.3,0,0,0,0,12109.3,12109.3,null,null,"N","N",10,1]
["MBA33110110S","손료","RENT000000000002",null,"노무할증 10%감+20%감","노무비의 70%","식",1,0,0,109598.39999999999,109598.39999999999,0,0,109598.39999999999,109598.39999999999,null,null,"N","N",70,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBA33110130S","손료","RENT000000000002",null,"노무할증 10%감+20%감","노무비의 70%","식",1,0,0,164076,164076,0,0,164076,164076,null,null,"N","N",70,1]
["MBA33110140S","노무","L001010101000039",null,"배관공","일반공사 직종","인",1.056,0,0,229482,242332.9,0,0,229482,242332.9,null,null,"N","Y","",0]
["MBA33110150S","손료","RENT000000000002",null,"노무할증 10%감+20%감","노무비의 70%","식",1,0,0,216749.8,216749.8,0,0,216749.8,216749.8,null,null,"N","N",70,1]
[null,null,null,null,"[합 계]",null,null,0,0,34318,0,240226,0,0,0,274544,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,37540,0,262784,0,0,0,300324,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,40917,0,286422,0,0,0,327339,null,null,null,null,"",1]
["MBC00010020S","노무","L001010101000012",null,"용접공","일반공사 직종","인",1.7999999999999999E-2,0,0,267021,4806.3,0,0,267021,4806.3,null,null,"N","N","",1]
["MBC00010040S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.03,0,0,267021,8010.6,0,0,267021,8010.6,null,null,"N","N","",1]
["MBC00010050S",null,null,null,"동관 용접 접합","D25","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBC00010060S",null,null,null,"동관 용접 접합","D32","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBC00010090S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,712.9,712.9,0,0,0,0,712.9,712.9,null,null,"N","N",3,1]
["MBC00010110S",null,null,null,"동관 용접 접합","D100","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBC00010120S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.16900000000000001,0,0,267021,45126.5,0,0,267021,45126.5,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBC00110010S",null,null,null,"동관 용접 접합","D8, 고소작업대 사용","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBC00110010S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,2990.5,2990.5,0,0,2990.5,2990.5,null,null,"N","N",80,1]
["MBC00110020S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,3845,3845,0,0,3845,3845,null,null,"N","N",80,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBC00110050S","노무","L001010101000012",null,"용접공","일반공사 직종","인",3.7999999999999999E-2,0,0,267021,10146.700000000001,0,0,267021,10146.700000000001,null,null,"N","Y","",0]
[null,null,null,null,"[합 계]",null,null,0,0,1562,0,9612,0,0,0,11174,null,null,null,null,"",1]
["MBC00110070S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,11321.6,11321.6,0,0,11321.6,11321.6,null,null,"N","N",80,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBC00110110S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.13700000000000001,0,0,267021,36581.800000000003,0,0,267021,36581.800000000003,null,null,"N","Y","",0]
["MBC00110120S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 13%","식",1,5866.4,5866.4,0,0,0,0,5866.4,5866.4,null,null,"N","N",13,1]
[null,null,null,null,"[합 계]",null,null,0,0,9198,0,56608,0,0,0,65806,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBC10010010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,129.4,129.4,0,0,0,0,129.4,129.4,null,null,"N","N",2,1]
["MBC10010030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.6E-2,0,0,165545,2648.7,0,0,165545,2648.7,null,null,"N","N","",1]
["MBC10010040S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.03,0,0,229482,6884.4,0,0,229482,6884.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,247,0,12399,0,0,0,12646,null,null,null,null,"",1]
["MBC10010070S",null,null,null,"동관 용접 배관","D40, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBC10010070S","노무","L001010101000039",null,"배관공","일반공사 직종","인",5.1999999999999998E-2,0,0,229482,11933,0,0,229482,11933,null,null,"N","N","",1]
["MBC10010090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.7E-2,0,0,165545,7780.6,0,0,165545,7780.6,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,672,0,33633,0,0,0,34305,null,null,null,null,"",1]
["MBC10010110S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.6999999999999999E-2,0,0,165545,12746.9,0,0,165545,12746.9,null,null,"N","N","",1]
["MBC10010130S",null,null,null,"동관 용접 배관","D150, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBC10010150S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,2674.2,2674.2,0,0,0,0,2674.2,2674.2,null,null,"N","N",2,1]
["MBC10110010S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,5179.6000000000004,5179.6000000000004,0,0,5179.6000000000004,5179.6000000000004,null,null,"N","N",80,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBC10110030S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,6892.1,6892.1,0,0,6892.1,6892.1,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,1019,0,8156,0,0,0,9175,null,null,null,null,"",1]
["MBC10110050S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1239.9000000000001,1239.9000000000001,0,0,0,0,1239.9000000000001,1239.9000000000001,null,null,"N","N",10,1]
[null,null,null,null,"[합 계]",null,null,0,0,1489,0,11918,0,0,0,13407,null,null,null,null,"",1]
["MBC10110070S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1739.5,1739.5,0,0,0,0,1739.5,1739.5,null,null,"N","N",10,1]
["MBC10110090S",null,null,null,"동관 용접 배관","D65, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBC10110100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.8999999999999997E-2,0,0,165545,9767.1,0,0,165545,9767.1,null,null,"N","Y","",0]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBC10110120S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,45361.8,45361.8,0,0,45361.8,45361.8,null,null,"N","N",80,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBC10110150S",null,null,null,"동관 용접 배관","D250, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,13371,0,106969,0,0,0,120340,null,null,null,null,"",1]
["MBC11010020S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,148.6,148.6,0,0,0,0,148.6,148.6,null,null,"N","N",2,1]
["MBC11010030S","노무","L001010101000039",null,"배관공","일반공사 직종","인",2.5999999999999999E-2,0,0,229482,5966.5,0,0,229482,5966.5,null,null,"N","Y","",0]
[null,null,null,null,"[합 계]",null,null,0,0,172,0,11199,0,0,0,11371,null,null,null,null,"",1]
["MBC11010050S","노무","L001010101000039",null,"배관공","일반공사 직종","인",3.5999999999999997E-2,0,0,229482,8261.2999999999993,0,0,229482,8261.2999999999993,null,null,"N","Y","",0]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBC11010070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.3000000000000002E-2,0,0,165545,5462.9,0,0,165545,5462.9,null,null,"N","Y","",0]
["MBC11010080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.2000000000000003E-2,0,0,165545,6952.8,0,0,165545,6952.8,null,null,"N","Y","",0]
["MBC11010090S",null,null,null,"동관 용접 배관","D65, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBC11010120S",null,null,null,"동관 용접 배관","D125, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBC11010120S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.18,0,0,229482,41306.699999999997,0,0,229482,41306.699999999997,null,null,"N","Y","",0]
["MBC11010130S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,1361.4,1361.4,0,0,0,0,1361.4,1361.4,null,null,"N","N",2,1]
["MBC11010150S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.442,0,0,229482,101431,0,0,229482,101431,null,null,"N","Y","",0]
[null,null,null,null,"[합 계]",null,null,0,0,2674,0,173825,0,0,0,176499,null,null,null,null,"",1]
["MBC11110010S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,7121.9,7121.9,0,0,7121.9,7121.9,null,null,"N","N",110,1]
["MBC11110030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.6E-2,0,0,165545,2648.7,0,0,165545,2648.7,null,null,"N","Y","",0]
["MBC11110040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.02,0,0,165545,3310.9,0,0,165545,3310.9,null,null,"N","Y","",0]
["MBC11110050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5000000000000001E-2,0,0,165545,4138.6000000000004,0,0,165545,4138.6000000000004,null,null,"N","Y","",0]
["MBC11110050S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,13639.8,13639.8,0,0,13639.8,13639.8,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,1489,0,16387,0,0,0,17876,null,null,null,null,"",1]
["MBC11110080S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,2278.6999999999998,2278.6999999999998,0,0,0,0,2278.6999999999998,2278.6999999999998,null,null,"N","N",10,1]
["MBC11110090S","노무","L001010101000039",null,"배관공","일반공사 직종","인",8.3000000000000004E-2,0,0,229482,19047,0,0,229482,19047,null,null,"N","Y","",0]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBC11110110S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,50119,50119,0,0,50119,50119,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,5670,0,62372,0,0,0,68042,null,null,null,null,"",1]
["MBC11110130S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,74878.5,74878.5,0,0,74878.5,74878.5,null,null,"N","N",110,1]
["MBC11110140S",null,null,null,"동관 용접 배관","D200, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBC12010010S",null,null,null,"동관 용접 배관","D8, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,129,0,7769,0,0,0,7898,null,null,null,null,"",1]
["MBC12010020S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,8916,8916,0,0,8916,8916,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,172,0,10338,0,0,0,10510,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBC12010060S","노무","L001010101000039",null,"배관공","일반공사 직종","인",4.3999999999999997E-2,0,0,229482,10097.200000000001,0,0,229482,10097.200000000001,null,null,"N","Y","",0]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBC12010070S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,347.9,347.9,0,0,0,0,347.9,347.9,null,null,"N","N",2,1]
["MBC12010090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.7E-2,0,0,165545,7780.6,0,0,165545,7780.6,null,null,"N","Y","",0]
["MBC12010100S",null,null,null,"동관 용접 배관","D80, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBC12010110S",null,null,null,"동관 용접 배관","D100, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBC12010120S",null,null,null,"동관 용접 배관","D125, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBC12010130S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.218,0,0,229482,50027,0,0,229482,50027,null,null,"N","Y","",0]
["MBC12010140S","손료","RENT000000000002",null,"노무할증 20%증","노무비의 120%","식",1,0,0,121467.4,121467.4,0,0,121467.4,121467.4,null,null,"N","N",120,1]
["MBC12010150S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.442,0,0,229482,101431,0,0,229482,101431,null,null,"N","Y","",0]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBC12110020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",2.3E-2,0,0,229482,5278,0,0,229482,5278,null,null,"N","Y","",0]
["MBC12110030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.6E-2,0,0,165545,2648.7,0,0,165545,2648.7,null,null,"N","Y","",0]
["MBC12110040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1019.5,1019.5,0,0,0,0,1019.5,1019.5,null,null,"N","N",10,1]
["MBC12110050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5000000000000001E-2,0,0,165545,4138.6000000000004,0,0,165545,4138.6000000000004,null,null,"N","Y","",0]
["MBC12110060S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1489.8,1489.8,0,0,0,0,1489.8,1489.8,null,null,"N","N",10,1]
["MBC12110080S",null,null,null,"동관 용접 배관","D50, 화장실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBC12110080S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,2278.6999999999998,2278.6999999999998,0,0,0,0,2278.6999999999998,2278.6999999999998,null,null,"N","N",10,1]
["MBC12110090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.7E-2,0,0,165545,7780.6,0,0,165545,7780.6,null,null,"N","Y","",0]
["MBC12110100S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,3363.3,3363.3,0,0,0,0,3363.3,3363.3,null,null,"N","N",10,1]
["MBC12110110S","손료","RENT000000000002",null,"노무할증 20%증+20%감","노무비의 100%","식",1,0,0,45562.8,45562.8,0,0,45562.8,45562.8,null,null,"N","N",100,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBC12110130S","손료","RENT000000000002",null,"노무할증 20%증+20%감","노무비의 100%","식",1,0,0,68071.399999999994,68071.399999999994,0,0,68071.399999999994,68071.399999999994,null,null,"N","N",100,1]
[null,null,null,null,"[합 계]",null,null,0,0,10122,0,101222,0,0,0,111344,null,null,null,null,"",1]
["MBC13010010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,129.4,129.4,0,0,0,0,129.4,129.4,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,129,0,5827,0,0,0,5956,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,148,0,6687,0,0,0,6835,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,203,0,9175,0,0,0,9378,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBC13010060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.9000000000000001E-2,0,0,165545,4800.8,0,0,165545,4800.8,null,null,"N","Y","",0]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBC13010080S",null,null,null,"동관 용접 배관","D50, 옥외배관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBC13010110S",null,null,null,"동관 용접 배관","D100, 옥외배관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBC13010110S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.14299999999999999,0,0,229482,32815.9,0,0,229482,32815.9,null,null,"N","Y","",0]
["MBC13010130S",null,null,null,"동관 용접 배관","D150, 옥외배관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBC13010140S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.33,0,0,229482,75729,0,0,229482,75729,null,null,"N","Y","",0]
[null,null,null,null,"[합 계]",null,null,0,0,2024,0,91100,0,0,0,93124,null,null,null,null,"",1]
["MBC13110010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",2.1000000000000001E-2,0,0,229482,4819.1000000000004,0,0,229482,4819.1000000000004,null,null,"N","Y","",0]
["MBC13110020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.2999999999999999E-2,0,0,165545,2152,0,0,165545,2152,null,null,"N","Y","",0]
["MBC13110030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.6E-2,0,0,165545,2648.7,0,0,165545,2648.7,null,null,"N","Y","",0]
["MBC13110040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.02,0,0,165545,3310.9,0,0,165545,3310.9,null,null,"N","Y","",0]
["MBC13110040S","손료","RENT000000000002",null,"노무할증 10%감+20%감","노무비의 70%","식",1,0,0,7136.7,7136.7,0,0,7136.7,7136.7,null,null,"N","N",70,1]
["MBC13110060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.9000000000000001E-2,0,0,165545,4800.8,0,0,165545,4800.8,null,null,"N","Y","",0]
["MBC13110070S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1739.5,1739.5,0,0,0,0,1739.5,1739.5,null,null,"N","N",10,1]
["MBC13110080S","노무","L001010101000039",null,"배관공","일반공사 직종","인",6.9000000000000006E-2,0,0,229482,15834.2,0,0,229482,15834.2,null,null,"N","Y","",0]
["MBC13110090S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,2682.7,2682.7,0,0,0,0,2682.7,2682.7,null,null,"N","N",10,1]
["MBC13110100S","손료","RENT000000000002",null,"노무할증 10%감+20%감","노무비의 70%","식",1,0,0,23543.200000000001,23543.200000000001,0,0,23543.200000000001,23543.200000000001,null,null,"N","N",70,1]
[null,null,null,null,"[합 계]",null,null,0,0,4556,0,31893,0,0,0,36449,null,null,null,null,"",1]
["MBC13110120S","손료","RENT000000000002",null,"노무할증 10%감+20%감","노무비의 70%","식",1,0,0,39691.599999999999,39691.599999999999,0,0,39691.599999999999,39691.599999999999,null,null,"N","N",70,1]
["MBC13110130S",null,null,null,"동관 용접 배관","D150, 옥외배관, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBC13110140S","손료","RENT000000000002",null,"노무할증 10%감+20%감","노무비의 70%","식",1,0,0,70856,70856,0,0,70856,70856,null,null,"N","N",70,1]
[null,null,null,null,"[합 계]",null,null,0,0,13371,0,93598,0,0,0,106969,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE00010030S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 4%","식",1,480.6,480.6,0,0,0,0,480.6,480.6,null,null,"N","N",4,1]
["MBE00010050S",null,null,null,"스텐관 용접 접합","D20","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,897,0,22429,0,0,0,23326,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,1271,0,31775,0,0,0,33046,null,null,null,null,"",1]
["MBE00010120S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.151,0,0,267021,40320.1,0,0,267021,40320.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,1783,0,44592,0,0,0,46375,null,null,null,null,"",1]
["MBE00010150S",null,null,null,"스텐관 용접 접합","D150","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,3150,0,78771,0,0,0,81921,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,4517,0,112949,0,0,0,117466,null,null,null,null,"",1]
["MBE00110010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 13%","식",1,1249.5999999999999,1249.5999999999999,0,0,0,0,1249.5999999999999,1249.5999999999999,null,null,"N","N",13,1]
["MBE00110020S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.04,0,0,267021,10680.8,0,0,267021,10680.8,null,null,"N","Y","",0]
[null,null,null,null,"[합 계]",null,null,0,0,1562,0,9612,0,0,0,11174,null,null,null,null,"",1]
["MBE00110050S",null,null,null,"스텐관 용접 접합","D20, 고소작업대 사용","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE00110060S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 13%","식",1,2291,2291,0,0,0,0,2291,2291,null,null,"N","N",13,1]
["MBE00110070S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 13%","식",1,2672.8,2672.8,0,0,0,0,2672.8,2672.8,null,null,"N","N",13,1]
[null,null,null,null,"[합 계]",null,null,0,0,2915,0,17943,0,0,0,20858,null,null,null,null,"",1]
["MBE00110100S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,25420.3,25420.3,0,0,25420.3,25420.3,null,null,"N","N",80,1]
["MBE00110110S",null,null,null,"스텐관 용접 접합","D80, 고소작업대 사용","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE00110120S",null,null,null,"스텐관 용접 접합","D90, 고소작업대 사용","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE00110130S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 13%","식",1,5797,5797,0,0,0,0,5797,5797,null,null,"N","N",13,1]
[null,null,null,null,"[합 계]",null,null,0,0,6907,0,42509,0,0,0,49416,null,null,null,null,"",1]
["MBE00110160S","노무","L001010101000012",null,"용접공","일반공사 직종","인",0.29499999999999998,0,0,267021,78771.100000000006,0,0,267021,78771.100000000006,null,null,"N","Y","",0]
["MBE00110170S",null,null,null,"스텐관 용접 접합","D250, 고소작업대 사용","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE00110180S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 13%","식",1,14683.4,14683.4,0,0,0,0,14683.4,14683.4,null,null,"N","N",13,1]
["MBE10010020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.2999999999999999E-2,0,0,165545,2152,0,0,165545,2152,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,139,0,6971,0,0,0,7110,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE10010060S","노무","L001010101000039",null,"배관공","일반공사 직종","인",4.8000000000000001E-2,0,0,229482,11015.1,0,0,229482,11015.1,null,null,"N","N","",1]
["MBE10010060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.1999999999999999E-2,0,0,165545,3641.9,0,0,165545,3641.9,null,null,"N","N","",1]
["MBE10010080S",null,null,null,"스텐관 용접 배관","D40, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,577,0,28881,0,0,0,29458,null,null,null,null,"",1]
["MBE10010120S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.14399999999999999,0,0,229482,33045.4,0,0,229482,33045.4,null,null,"N","N","",1]
["MBE10010130S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,943.6,943.6,0,0,0,0,943.6,943.6,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,943,0,47184,0,0,0,48127,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE10010170S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.45800000000000002,0,0,229482,105102.7,0,0,229482,105102.7,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE10110010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,674.1,674.1,0,0,0,0,674.1,674.1,null,null,"N","N",10,1]
["MBE10110020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",2.1000000000000001E-2,0,0,229482,4819.1000000000004,0,0,229482,4819.1000000000004,null,null,"N","Y","",0]
["MBE10110030S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,6627.2,6627.2,0,0,6627.2,6627.2,null,null,"N","N",80,1]
["MBE10110040S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,7126.8,7126.8,0,0,7126.8,7126.8,null,null,"N","N",80,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE10110060S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,11725.6,11725.6,0,0,11725.6,11725.6,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,1767,0,14142,0,0,0,15909,null,null,null,null,"",1]
["MBE10110080S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1938.6,1938.6,0,0,0,0,1938.6,1938.6,null,null,"N","N",10,1]
[null,null,null,null,"[합 계]",null,null,0,0,2342,0,18741,0,0,0,21083,null,null,null,null,"",1]
["MBE10110100S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,2888.1,2888.1,0,0,0,0,2888.1,2888.1,null,null,"N","N",10,1]
["MBE10110120S",null,null,null,"스텐관 용접 배관","D90, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE10110130S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.6000000000000003E-2,0,0,165545,10925.9,0,0,165545,10925.9,null,null,"N","Y","",0]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE10110150S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,57436.4,57436.4,0,0,57436.4,57436.4,null,null,"N","N",80,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE10110180S",null,null,null,"스텐관 용접 배관","D300, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,18006,0,144048,0,0,0,162054,null,null,null,null,"",1]
["MBE11010020S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,139.4,139.4,0,0,0,0,139.4,139.4,null,null,"N","N",2,1]
["MBE11010030S","노무","L001010101000039",null,"배관공","일반공사 직종","인",2.5999999999999999E-2,0,0,229482,5966.5,0,0,229482,5966.5,null,null,"N","Y","",0]
[null,null,null,null,"[합 계]",null,null,0,0,165,0,10769,0,0,0,10934,null,null,null,null,"",1]
["MBE11010050S","노무","L001010101000039",null,"배관공","일반공사 직종","인",3.3000000000000002E-2,0,0,229482,7572.9,0,0,229482,7572.9,null,null,"N","Y","",0]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE11010070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5000000000000001E-2,0,0,165545,4138.6000000000004,0,0,165545,4138.6000000000004,null,null,"N","Y","",0]
["MBE11010080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.7E-2,0,0,165545,4469.7,0,0,165545,4469.7,null,null,"N","Y","",0]
[null,null,null,null,"[합 계]",null,null,0,0,468,0,30454,0,0,0,30922,null,null,null,null,"",1]
["MBE11010100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.04,0,0,165545,6621.8,0,0,165545,6621.8,null,null,"N","Y","",0]
["MBE11010120S",null,null,null,"스텐관 용접 배관","D90, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE11010120S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.14399999999999999,0,0,229482,33045.4,0,0,229482,33045.4,null,null,"N","Y","",0]
["MBE11010130S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,943.6,943.6,0,0,0,0,943.6,943.6,null,null,"N","N",2,1]
["MBE11010150S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.24,0,0,229482,55075.6,0,0,229482,55075.6,null,null,"N","Y","",0]
[null,null,null,null,"[합 계]",null,null,0,0,1435,0,93334,0,0,0,94769,null,null,null,null,"",1]
["MBE11010160S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,130782.3,130782.3,0,0,130782.3,130782.3,null,null,"N","N",130,1]
["MBE11010180S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.61799999999999999,0,0,229482,141819.79999999999,0,0,229482,141819.79999999999,null,null,"N","Y","",0]
["MBE11010180S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,234078.7,234078.7,0,0,234078.7,234078.7,null,null,"N","N",130,1]
["MBE11110020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.2999999999999999E-2,0,0,165545,2152,0,0,165545,2152,null,null,"N","Y","",0]
["MBE11110020S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,7668.2,7668.2,0,0,7668.2,7668.2,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,828,0,9112,0,0,0,9940,null,null,null,null,"",1]
["MBE11110050S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1038.7,1038.7,0,0,0,0,1038.7,1038.7,null,null,"N","N",10,1]
["MBE11110060S","노무","L001010101000039",null,"배관공","일반공사 직종","인",4.8000000000000001E-2,0,0,229482,11015.1,0,0,229482,11015.1,null,null,"N","Y","",0]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE11110080S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,21324.6,21324.6,0,0,21324.6,21324.6,null,null,"N","N",110,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE11110100S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,31769.599999999999,31769.599999999999,0,0,31769.599999999999,31769.599999999999,null,null,"N","N",110,1]
["MBE11110110S",null,null,null,"스텐관 용접 배관","D80, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE11110130S",null,null,null,"스텐관 용접 배관","D100, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,4718,0,51902,0,0,0,56620,null,null,null,null,"",1]
["MBE11110140S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,69287.399999999994,69287.399999999994,0,0,69287.399999999994,69287.399999999994,null,null,"N","N",110,1]
[null,null,null,null,"[합 계]",null,null,0,0,7179,0,78975,0,0,0,86154,null,null,null,null,"",1]
["MBE11110170S",null,null,null,"스텐관 용접 배관","D250, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE11110180S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.61799999999999999,0,0,229482,141819.79999999999,0,0,229482,141819.79999999999,null,null,"N","Y","",0]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE12010010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,134.80000000000001,134.80000000000001,0,0,0,0,134.80000000000001,134.80000000000001,null,null,"N","N",2,1]
["MBE12010030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.4E-2,0,0,165545,2317.6,0,0,165545,2317.6,null,null,"N","Y","",0]
["MBE12010040S",null,null,null,"스텐관 용접 배관","D15, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE12010050S",null,null,null,"스텐관 용접 배관","D20, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE12010060S",null,null,null,"스텐관 용접 배관","D25, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE12010070S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,353.5,353.5,0,0,0,0,353.5,353.5,null,null,"N","N",2,1]
["MBE12010080S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,387.7,387.7,0,0,0,0,387.7,387.7,null,null,"N","N",2,1]
["MBE12010090S","노무","L001010101000039",null,"배관공","일반공사 직종","인",7.9000000000000001E-2,0,0,229482,18129,0,0,229482,18129,null,null,"N","Y","",0]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE12010110S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.11,0,0,229482,25243,0,0,229482,25243,null,null,"N","Y","",0]
["MBE12010120S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.06,0,0,165545,9932.7000000000007,0,0,165545,9932.7000000000007,null,null,"N","Y","",0]
["MBE12010130S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,943.6,943.6,0,0,0,0,943.6,943.6,null,null,"N","N",2,1]
["MBE12010140S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",8.7999999999999995E-2,0,0,165545,14567.9,0,0,165545,14567.9,null,null,"N","Y","",0]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,2012,0,120722,0,0,0,122734,null,null,null,null,"",1]
["MBE12010170S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,2721.1,2721.1,0,0,0,0,2721.1,2721.1,null,null,"N","N",2,1]
["MBE12010180S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.23100000000000001,0,0,165545,38240.800000000003,0,0,165545,38240.800000000003,null,null,"N","Y","",0]
["MBE12110010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,674.1,674.1,0,0,0,0,674.1,674.1,null,null,"N","N",10,1]
["MBE12110020S","손료","RENT000000000002",null,"노무할증 20%증+20%감","노무비의 100%","식",1,0,0,6971.1,6971.1,0,0,6971.1,6971.1,null,null,"N","N",100,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE12110040S","손료","RENT000000000002",null,"노무할증 20%증+20%감","노무비의 100%","식",1,0,0,8908.5,8908.5,0,0,8908.5,8908.5,null,null,"N","N",100,1]
["MBE12110060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.1999999999999999E-2,0,0,165545,3641.9,0,0,165545,3641.9,null,null,"N","Y","",0]
["MBE12110070S",null,null,null,"스텐관 용접 배관","D32, 화장실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,1767,0,17678,0,0,0,19445,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,1938,0,19386,0,0,0,21324,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,2888,0,28881,0,0,0,31769,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE12110120S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.06,0,0,165545,9932.7000000000007,0,0,165545,9932.7000000000007,null,null,"N","Y","",0]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,6298,0,62988,0,0,0,69286,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE12110170S",null,null,null,"스텐관 용접 배관","D250, 화장실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE12110170S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.45800000000000002,0,0,229482,105102.7,0,0,229482,105102.7,null,null,"N","Y","",0]
["MBE13010010S",null,null,null,"스텐관 용접 배관","D6, 옥외배관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE13010020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",2.1000000000000001E-2,0,0,229482,4819.1000000000004,0,0,229482,4819.1000000000004,null,null,"N","Y","",0]
[null,null,null,null,"[합 계]",null,null,0,0,139,0,6273,0,0,0,6412,null,null,null,null,"",1]
["MBE13010040S","노무","L001010101000039",null,"배관공","일반공사 직종","인",2.8000000000000001E-2,0,0,229482,6425.4,0,0,229482,6425.4,null,null,"N","Y","",0]
["MBE13010050S","노무","L001010101000039",null,"배관공","일반공사 직종","인",3.3000000000000002E-2,0,0,229482,7572.9,0,0,229482,7572.9,null,null,"N","Y","",0]
["MBE13010060S","노무","L001010101000039",null,"배관공","일반공사 직종","인",4.8000000000000001E-2,0,0,229482,11015.1,0,0,229482,11015.1,null,null,"N","Y","",0]
["MBE13010070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5000000000000001E-2,0,0,165545,4138.6000000000004,0,0,165545,4138.6000000000004,null,null,"N","Y","",0]
["MBE13010070S","손료","RENT000000000002",null,"노무할증 10%감","노무비의 90%","식",1,0,0,15910.2,15910.2,0,0,15910.2,15910.2,null,null,"N","N",90,1]
["MBE13010090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.2000000000000001E-2,0,0,165545,5297.4,0,0,165545,5297.4,null,null,"N","Y","",0]
["MBE13010100S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,577.6,577.6,0,0,0,0,577.6,577.6,null,null,"N","N",2,1]
["MBE13010110S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.11,0,0,229482,25243,0,0,229482,25243,null,null,"N","Y","",0]
["MBE13010120S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,859.5,859.5,0,0,0,0,859.5,859.5,null,null,"N","N",2,1]
["MBE13010130S","손료","RENT000000000002",null,"노무할증 10%감","노무비의 90%","식",1,0,0,42465.599999999999,42465.599999999999,0,0,42465.599999999999,42465.599999999999,null,null,"N","N",90,1]
["MBE13010140S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,1259.7,1259.7,0,0,0,0,1259.7,1259.7,null,null,"N","N",2,1]
["MBE13010150S","손료","RENT000000000002",null,"노무할증 10%감","노무비의 90%","식",1,0,0,64616,64616,0,0,64616,64616,null,null,"N","N",90,1]
["MBE13010160S",null,null,null,"스텐관 용접 배관","D200, 옥외배관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE13010170S","손료","RENT000000000002",null,"노무할증 10%감","노무비의 90%","식",1,0,0,122453.6,122453.6,0,0,122453.6,122453.6,null,null,"N","N",90,1]
[null,null,null,null,"[합 계]",null,null,0,0,3601,0,162054,0,0,0,165655,null,null,null,null,"",1]
["MBE13110010S","손료","RENT000000000002",null,"노무할증 10%감+20%감","노무비의 70%","식",1,0,0,4719.1000000000004,4719.1000000000004,0,0,4719.1000000000004,4719.1000000000004,null,null,"N","N",70,1]
[null,null,null,null,"[합 계]",null,null,0,0,697,0,4879,0,0,0,5576,null,null,null,null,"",1]
["MBE13110040S",null,null,null,"스텐관 용접 배관","D15, 옥외배관, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,890,0,6235,0,0,0,7125,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE13110060S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1465.7,1465.7,0,0,0,0,1465.7,1465.7,null,null,"N","N",10,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE13110090S",null,null,null,"스텐관 용접 배관","D50, 옥외배관, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE13110100S",null,null,null,"스텐관 용접 배관","D65, 옥외배관, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE13110110S",null,null,null,"스텐관 용접 배관","D80, 옥외배관, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE13110120S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,4297.8,4297.8,0,0,0,0,4297.8,4297.8,null,null,"N","N",10,1]
["MBE13110130S",null,null,null,"스텐관 용접 배관","D100, 옥외배관, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE13110140S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.21099999999999999,0,0,229482,48420.7,0,0,229482,48420.7,null,null,"N","Y","",0]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE13110160S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.34100000000000003,0,0,229482,78253.3,0,0,229482,78253.3,null,null,"N","Y","",0]
["MBE13110170S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.187,0,0,165545,30956.9,0,0,165545,30956.9,null,null,"N","Y","",0]
["MBE13110180S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,18006,18006,0,0,0,0,18006,18006,null,null,"N","N",10,1]
["MBE20010010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.7000000000000001E-2,0,0,165545,2814.2,0,0,165545,2814.2,null,null,"N","N","",1]
["MBE20010030S","노무","L001010101000039",null,"배관공","일반공사 직종","인",5.2999999999999999E-2,0,0,229482,12162.5,0,0,229482,12162.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,332,0,16632,0,0,0,16964,null,null,null,null,"",1]
["MBE20010050S",null,null,null,"프레스식 접합 및 배관","D40, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE20010060S",null,null,null,"프레스식 접합 및 배관","D50, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE20010070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.7000000000000002E-2,0,0,165545,9436,0,0,165545,9436,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,796,0,39840,0,0,0,40636,null,null,null,null,"",1]
["MBE20010100S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.192,0,0,229482,44060.5,0,0,229482,44060.5,null,null,"N","N","",1]
["MBE20110010S",null,null,null,"프레스식 접합 및 배관","D13, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,1413,0,11307,0,0,0,12720,null,null,null,null,"",1]
["MBE20110040S",null,null,null,"프레스식 접합 및 배관","D30, 옥내일반, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE20110040S","노무","L001010101000039",null,"배관공","일반공사 직종","인",6.7000000000000004E-2,0,0,229482,15375.2,0,0,229482,15375.2,null,null,"N","Y","",0]
["MBE20110050S","노무","L001010101000039",null,"배관공","일반공사 직종","인",7.8E-2,0,0,229482,17899.5,0,0,229482,17899.5,null,null,"N","Y","",0]
["MBE20110070S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.109,0,0,229482,25013.5,0,0,229482,25013.5,null,null,"N","Y","",0]
["MBE20110070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.7000000000000002E-2,0,0,165545,9436,0,0,165545,9436,null,null,"N","Y","",0]
[null,null,null,null,"[합 계]",null,null,0,0,3984,0,31872,0,0,0,35856,null,null,null,null,"",1]
["MBE20110100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.10199999999999999,0,0,165545,16885.5,0,0,165545,16885.5,null,null,"N","Y","",0]
["MBE21010010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",3.4000000000000002E-2,0,0,229482,7802.3,0,0,229482,7802.3,null,null,"N","Y","",0]
["MBE21010020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.3E-2,0,0,165545,3807.5,0,0,165545,3807.5,null,null,"N","Y","",0]
["MBE21010030S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,332.6,332.6,0,0,0,0,332.6,332.6,null,null,"N","N",2,1]
["MBE21010030S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,21621.8,21621.8,0,0,21621.8,21621.8,null,null,"N","N",130,1]
["MBE21010050S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,490.4,490.4,0,0,0,0,490.4,490.4,null,null,"N","N",2,1]
["MBE21010060S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,34313.199999999997,34313.199999999997,0,0,34313.199999999997,34313.199999999997,null,null,"N","N",130,1]
["MBE21010070S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.109,0,0,229482,25013.5,0,0,229482,25013.5,null,null,"N","Y","",0]
["MBE21010080S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,51792.7,51792.7,0,0,51792.7,51792.7,null,null,"N","N",130,1]
["MBE21010090S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,67946.899999999994,67946.899999999994,0,0,67946.899999999994,67946.899999999994,null,null,"N","N",130,1]
["MBE21010100S","손료","RENT000000000002",null,"노무할증 30%증","노무비의 130%","식",1,0,0,79229.8,79229.8,0,0,79229.8,79229.8,null,null,"N","N",130,1]
[null,null,null,null,"[합 계]",null,null,0,0,1061,0,11678,0,0,0,12739,null,null,null,null,"",1]
["MBE21110020S",null,null,null,"프레스식 접합 및 배관","D20, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,1663,0,18295,0,0,0,19958,null,null,null,null,"",1]
["MBE21110040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,2100.3000000000002,2100.3000000000002,0,0,0,0,2100.3000000000002,2100.3000000000002,null,null,"N","N",10,1]
["MBE21110050S","손료","RENT000000000002",null,"노무할증 30%증+20%감","노무비의 110%","식",1,0,0,26973.4,26973.4,0,0,26973.4,26973.4,null,null,"N","N",110,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE21110080S",null,null,null,"프레스식 접합 및 배관","D75, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE21110100S",null,null,null,"프레스식 접합 및 배관","D100, 기계실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE21110100S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,6094.6,6094.6,0,0,0,0,6094.6,6094.6,null,null,"N","N",10,1]
["MBE22010020S",null,null,null,"프레스식 접합 및 배관","D20, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,282,0,16960,0,0,0,17242,null,null,null,null,"",1]
["MBE22010040S",null,null,null,"프레스식 접합 및 배관","D30, 화장실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE22010050S","노무","L001010101000039",null,"배관공","일반공사 직종","인",7.8E-2,0,0,229482,17899.5,0,0,229482,17899.5,null,null,"N","Y","",0]
["MBE22010060S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,527.79999999999995,527.79999999999995,0,0,0,0,527.79999999999995,527.79999999999995,null,null,"N","N",2,1]
["MBE22010070S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.109,0,0,229482,25013.5,0,0,229482,25013.5,null,null,"N","Y","",0]
["MBE22010080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.6000000000000003E-2,0,0,165545,10925.9,0,0,165545,10925.9,null,null,"N","Y","",0]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE22010100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.10199999999999999,0,0,165545,16885.5,0,0,165545,16885.5,null,null,"N","Y","",0]
["MBE22110010S",null,null,null,"프레스식 접합 및 배관","D13, 화장실, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE22110020S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1413.4,1413.4,0,0,0,0,1413.4,1413.4,null,null,"N","N",10,1]
["MBE22110030S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1663.2,1663.2,0,0,0,0,1663.2,1663.2,null,null,"N","N",10,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE22110050S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,2452.1,2452.1,0,0,0,0,2452.1,2452.1,null,null,"N","N",10,1]
["MBE22110070S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.109,0,0,229482,25013.5,0,0,229482,25013.5,null,null,"N","Y","",0]
["MBE22110070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.7000000000000002E-2,0,0,165545,9436,0,0,165545,9436,null,null,"N","Y","",0]
["MBE22110080S","손료","RENT000000000002",null,"노무할증 20%증+20%감","노무비의 100%","식",1,0,0,39840.6,39840.6,0,0,39840.6,39840.6,null,null,"N","N",100,1]
["MBE22110100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.10199999999999999,0,0,165545,16885.5,0,0,165545,16885.5,null,null,"N","Y","",0]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,212,0,9554,0,0,0,9766,null,null,null,null,"",1]
["MBE23010030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.7E-2,0,0,165545,4469.7,0,0,165545,4469.7,null,null,"N","Y","",0]
[null,null,null,null,"[합 계]",null,null,0,0,332,0,14968,0,0,0,15300,null,null,null,null,"",1]
["MBE23010050S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,490.4,490.4,0,0,0,0,490.4,490.4,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,490,0,22069,0,0,0,22559,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE23010080S","손료","RENT000000000002",null,"노무할증 10%감","노무비의 90%","식",1,0,0,35856.5,35856.5,0,0,35856.5,35856.5,null,null,"N","N",90,1]
["MBE23010090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",8.6999999999999994E-2,0,0,165545,14402.4,0,0,165545,14402.4,null,null,"N","Y","",0]
["MBE23010100S",null,null,null,"프레스식 접합 및 배관","D100, 옥외배관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,1061,0,7431,0,0,0,8492,null,null,null,null,"",1]
["MBE23110030S",null,null,null,"프레스식 접합 및 배관","D25, 옥외배관, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,1663,0,11642,0,0,0,13305,null,null,null,null,"",1]
["MBE23110040S","노무","L001010101000039",null,"배관공","일반공사 직종","인",6.7000000000000004E-2,0,0,229482,15375.2,0,0,229482,15375.2,null,null,"N","Y","",0]
["MBE23110060S","노무","L001010101000039",null,"배관공","일반공사 직종","인",8.4000000000000005E-2,0,0,229482,19276.400000000001,0,0,229482,19276.400000000001,null,null,"N","Y","",0]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,3444,0,24114,0,0,0,27558,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBE23110100S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.192,0,0,229482,44060.5,0,0,229482,44060.5,null,null,"N","Y","",0]
["MBE30010010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.7E-2,0,0,165545,4469.7,0,0,165545,4469.7,null,null,"N","N","",1]
["MBE30010020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",3.9E-2,0,0,229482,8949.7000000000007,0,0,229482,8949.7000000000007,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,1408,0,11265,0,0,0,12673,null,null,null,null,"",1]
["MBG00010010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,965.8,965.8,0,0,0,0,965.8,965.8,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,1180,0,59023,0,0,0,60203,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBG00010050S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,2012.8,2012.8,0,0,0,0,2012.8,2012.8,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,2261,0,113084,0,0,0,115345,null,null,null,null,"",1]
["MBG00010070S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,2910.2,2910.2,0,0,0,0,2910.2,2910.2,null,null,"N","N",2,1]
["MBG00110010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",8.1000000000000003E-2,0,0,165545,13409.1,0,0,165545,13409.1,null,null,"N","Y","",0]
["MBG00110020S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,47218.8,47218.8,0,0,47218.8,47218.8,null,null,"N","N",80,1]
[null,null,null,null,"[합 계]",null,null,0,0,6581,0,52654,0,0,0,59235,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,10064,0,80514,0,0,0,90578,null,null,null,null,"",1]
["MBG00110070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.154,0,0,165545,25493.9,0,0,165545,25493.9,null,null,"N","Y","",0]
["MBG10010010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.14299999999999999,0,0,229482,32815.9,0,0,229482,32815.9,null,null,"N","N","",1]
["MBG10010020S",null,null,null," 수밀밴드접합 및 배관","D65","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBG10010030S",null,null,null," 수밀밴드접합 및 배관","D75","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBG10010040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.122,0,0,165545,20196.400000000001,0,0,165545,20196.400000000001,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,1873,0,93676,0,0,0,95549,null,null,null,null,"",1]
["MBG10010070S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.434,0,0,229482,99595.1,0,0,229482,99595.1,null,null,"N","N","",1]
["MBG10110010S",null,null,null," 수밀밴드접합 및 배관","D50, 고소작업대 사용","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,5389,0,43119,0,0,0,48508,null,null,null,null,"",1]
["MBG10110030S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,6053.9,6053.9,0,0,0,0,6053.9,6053.9,null,null,"N","N",10,1]
["MBG10110040S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.248,0,0,229482,56911.5,0,0,229482,56911.5,null,null,"N","Y","",0]
["MBG10110050S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.3,0,0,229482,68844.600000000006,0,0,229482,68844.600000000006,null,null,"N","Y","",0]
["MBG10110070S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.434,0,0,229482,99595.1,0,0,229482,99595.1,null,null,"N","Y","",0]
["MBG10110070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.22,0,0,165545,36419.9,0,0,165545,36419.9,null,null,"N","Y","",0]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,411,0,20556,0,0,0,20967,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,449,0,22493,0,0,0,22942,null,null,null,null,"",1]
["MBI00010060S",null,null,null,"PVC관 접착제 접합 및 배관","D65","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBI00010070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.3E-2,0,0,165545,10429.299999999999,0,0,165545,10429.299999999999,null,null,"N","N","",1]
["MBI00010070S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,745.5,745.5,0,0,0,0,745.5,745.5,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,1098,0,54919,0,0,0,56017,null,null,null,null,"",1]
["MBI00010110S",null,null,null,"PVC관 접착제 접합 및 배관","D200","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,1591,0,79583,0,0,0,81174,null,null,null,null,"",1]
["MBI00110020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",5.3999999999999999E-2,0,0,229482,12392,0,0,229482,12392,null,null,"N","Y","",0]
["MBI00110030S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.06,0,0,229482,13768.9,0,0,229482,13768.9,null,null,"N","Y","",0]
["MBI00110040S","노무","L001010101000039",null,"배관공","일반공사 직종","인",6.7000000000000004E-2,0,0,229482,15375.2,0,0,229482,15375.2,null,null,"N","Y","",0]
["MBI00110050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.7E-2,0,0,165545,7780.6,0,0,165545,7780.6,null,null,"N","Y","",0]
["MBI00110050S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,22012.799999999999,22012.799999999999,0,0,22012.799999999999,22012.799999999999,null,null,"N","N",80,1]
["MBI00110070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.3E-2,0,0,165545,10429.299999999999,0,0,165545,10429.299999999999,null,null,"N","Y","",0]
["MBI00110080S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,4598.3999999999996,4598.3999999999996,0,0,0,0,4598.3999999999996,4598.3999999999996,null,null,"N","N",10,1]
["MBI00110090S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.17799999999999999,0,0,229482,40847.699999999997,0,0,229482,40847.699999999997,null,null,"N","Y","",0]
["MBI00110100S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,6289.8,6289.8,0,0,0,0,6289.8,6289.8,null,null,"N","N",10,1]
["MBI00110110S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,63666.5,63666.5,0,0,63666.5,63666.5,null,null,"N","N",80,1]
["MBI10010010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,132.80000000000001,132.80000000000001,0,0,0,0,132.80000000000001,132.80000000000001,null,null,"N","N",2,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBI10010030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.2E-2,0,0,165545,1986.5,0,0,165545,1986.5,null,null,"N","N","",1]
["MBI10010050S","노무","L001010101000039",null,"배관공","일반공사 직종","인",2.5000000000000001E-2,0,0,229482,5737,0,0,229482,5737,null,null,"N","N","",1]
["MBI10010060S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,165.6,165.6,0,0,0,0,165.6,165.6,null,null,"N","N",2,1]
["MBI10010070S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,173.5,173.5,0,0,0,0,173.5,173.5,null,null,"N","N",2,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBI10010100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.1000000000000001E-2,0,0,165545,3476.4,0,0,165545,3476.4,null,null,"N","N","",1]
["MBI10010110S","노무","L001010101000039",null,"배관공","일반공사 직종","인",4.9000000000000002E-2,0,0,229482,11244.6,0,0,229482,11244.6,null,null,"N","N","",1]
["MBI10010111S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,406.3,406.3,0,0,0,0,406.3,406.3,null,null,"N","N",2,1]
["MBI10010112S","노무","L001010101000039",null,"배관공","일반공사 직종","인",7.4999999999999997E-2,0,0,229482,17211.099999999999,0,0,229482,17211.099999999999,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBI10110010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",2.1000000000000001E-2,0,0,229482,4819.1000000000004,0,0,229482,4819.1000000000004,null,null,"N","Y","",0]
["MBI10110020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",2.1000000000000001E-2,0,0,229482,4819.1000000000004,0,0,229482,4819.1000000000004,null,null,"N","Y","",0]
["MBI10110030S","노무","L001010101000039",null,"배관공","일반공사 직종","인",2.1999999999999999E-2,0,0,229482,5048.6000000000004,0,0,229482,5048.6000000000004,null,null,"N","Y","",0]
["MBI10110040S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,5944,5944,0,0,5944,5944,null,null,"N","N",80,1]
["MBI10110050S","노무","L001010101000039",null,"배관공","일반공사 직종","인",2.5000000000000001E-2,0,0,229482,5737,0,0,229482,5737,null,null,"N","Y","",0]
["MBI10110060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.4E-2,0,0,165545,2317.6,0,0,165545,2317.6,null,null,"N","Y","",0]
["MBI10110070S",null,null,null,"PVC관 소켓 접합 및 배관","D35, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBI10110080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.6E-2,0,0,165545,2648.7,0,0,165545,2648.7,null,null,"N","Y","",0]
["MBI10110090S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1078.2,1078.2,0,0,0,0,1078.2,1078.2,null,null,"N","N",10,1]
["MBI10110100S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,9757.2999999999993,9757.2999999999993,0,0,9757.2999999999993,9757.2999999999993,null,null,"N","N",80,1]
["MBI10110110S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,1554.8,1554.8,0,0,0,0,1554.8,1554.8,null,null,"N","N",10,1]
["MBI10110130S",null,null,null,"PVC관 소켓 접합 및 배관","D125, 고소작업대 사용","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBI10110130S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,2399.8000000000002,2399.8000000000002,0,0,0,0,2399.8000000000002,2399.8000000000002,null,null,"N","N",10,1]
["MBI10110140S","손료","RENT000000000002",null,"노무할증 20%감","노무비의 80%","식",1,0,0,24011.200000000001,24011.200000000001,0,0,24011.200000000001,24011.200000000001,null,null,"N","N",80,1]
["MBI10110150S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,3767.3,3767.3,0,0,0,0,3767.3,3767.3,null,null,"N","N",10,1]
[null,null,null,null,"[합 계]",null,null,0,0,112,0,11203,0,0,0,11315,null,null,null,null,"",1]
["MBK10010010S",null,null,null,"PB 이중관 접합 및 배관","D16","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MBK10010020S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 1%","식",1,159.69999999999999,159.69999999999999,0,0,0,0,159.69999999999999,159.69999999999999,null,null,"N","N",1,1]
["MBK20010010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.4E-2,0,0,165545,2317.6,0,0,165545,2317.6,null,null,"N","N","",1]
["MCA10000000S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1,0,0,165545,165545,0,0,165545,165545,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MCA10010020S",null,null,null,"아연도금강판 스파이럴덕트 설치","D160, t 0.5mm ","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MCA10010030S","노무","L001010101000043",null,"덕트공","일반공사 직종","인",0.13600000000000001,0,0,207048,28158.5,0,0,207048,28158.5,null,null,"N","N","",1]
["MCA10010050S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,876.9,876.9,0,0,0,0,876.9,876.9,null,null,"N","N",2,1]
["MCA10010060S",null,null,null,"아연도금강판 스파이럴덕트 설치","D250, t 0.6mm ","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MCA10010090S","노무","L001010101000043",null,"덕트공","일반공사 직종","인",0.25,0,0,207048,51762,0,0,207048,51762,null,null,"N","N","",1]
["MCA10010100S","노무","L001010101000043",null,"덕트공","일반공사 직종","인",0.25,0,0,207048,51762,0,0,207048,51762,null,null,"N","N","",1]
["MCA10010110S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,1730.7,1730.7,0,0,0,0,1730.7,1730.7,null,null,"N","N",2,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MCA10010130S",null,null,null,"아연도금강판 스파이럴덕트 설치","D550, t 0.6mm ","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MCA10010150S","노무","L001010101000043",null,"덕트공","일반공사 직종","인",0.5,0,0,207048,103524,0,0,207048,103524,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MCA10010170S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,2633.3,2633.3,0,0,0,0,2633.3,2633.3,null,null,"N","N",2,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MCA10010200S",null,null,null,"아연도금강판 스파이럴덕트 설치","D900, t 1.0mm ","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MCA10010210S","노무","L001010101000043",null,"덕트공","일반공사 직종","인",0.6,0,0,207048,124228.8,0,0,207048,124228.8,null,null,"N","N","",1]
["MCA10010220S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,3146.7,3146.7,0,0,0,0,3146.7,3146.7,null,null,"N","N",2,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,3167,0,31674,0,0,0,34841,null,null,null,null,"",1]
["MCA10110040S","노무","L001010101000043",null,"덕트공","일반공사 직종","인",0.121,0,0,207048,25052.799999999999,0,0,207048,25052.799999999999,null,null,"N","N","",1]
["MCA10110050S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,3854.7,3854.7,0,0,0,0,3854.7,3854.7,null,null,"N","N",10,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MCA10110090S","노무","L001010101000043",null,"덕트공","일반공사 직종","인",0.221,0,0,207048,45757.599999999999,0,0,207048,45757.599999999999,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,5800,0,58007,0,0,0,63807,null,null,null,null,"",1]
["MCA10110110S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,7730.2,7730.2,0,0,0,0,7730.2,7730.2,null,null,"N","N",10,1]
["MCA10110120S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,7730.2,7730.2,0,0,0,0,7730.2,7730.2,null,null,"N","N",10,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MCA10110150S","노무","L001010101000043",null,"덕트공","일반공사 직종","인",0.44,0,0,207048,91101.1,0,0,207048,91101.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,11593,0,115932,0,0,0,127525,null,null,null,null,"",1]
["MCA10110170S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,11593.2,11593.2,0,0,0,0,11593.2,11593.2,null,null,"N","N",10,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MCA10110190S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 10%","식",1,13953.3,13953.3,0,0,0,0,13953.3,13953.3,null,null,"N","N",10,1]
["MCA10110210S","노무","L001010101000043",null,"덕트공","일반공사 직종","인",0.53,0,0,207048,109735.4,0,0,207048,109735.4,null,null,"N","N","",1]
["MCA10110220S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.18,0,0,165545,29798.1,0,0,165545,29798.1,null,null,"N","N","",1]
["MCA30000000S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,15733.7,15733.7,0,0,0,0,15733.7,15733.7,null,null,"N","N",2,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MCA40010010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,115.9,115.9,0,0,0,0,115.9,115.9,null,null,"N","N",2,1]
["MCA50010010S","노무","L001010101000043",null,"덕트공","일반공사 직종","인",0.05,0,0,207048,10352.4,0,0,207048,10352.4,null,null,"N","N","",1]
["MCA50010040S","노무","L001010101000043",null,"덕트공","일반공사 직종","인",0.09,0,0,207048,18634.3,0,0,207048,18634.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,18634,0,0,0,18634,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MCA50010100S","노무","L001010101000043",null,"덕트공","일반공사 직종","인",0.21,0,0,207048,43480,0,0,207048,43480,null,null,"N","N","",1]
["MCB00010010S","노무","L001010101000043",null,"덕트공","일반공사 직종","인",0.36799999999999999,0,0,207048,76193.600000000006,0,0,207048,76193.600000000006,null,null,"N","N","",1]
["MCB00010040S",null,null,null,"취출구 설치","아네모디퓨저, 목지름400mm 이하","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MCB00110020S","노무","L001010101000043",null,"덕트공","일반공사 직종","인",0.32200000000000001,0,0,207048,66669.399999999994,0,0,207048,66669.399999999994,null,null,"N","N","",1]
["MCB00110040S","노무","L001010101000043",null,"덕트공","일반공사 직종","인",0.36499999999999999,0,0,207048,75572.5,0,0,207048,75572.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,87995,0,0,0,87995,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,115946,0,0,0,115946,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MCB00310010S",null,null,null,"취출구 설치","슬릿형, 변길이1m 미만","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MCB00310020S","노무","L001010101000043",null,"덕트공","일반공사 직종","인",1.1020000000000001,0,0,207048,228166.8,0,0,207048,228166.8,null,null,"N","N","",1]
["MCB10010010S",null,null,null,"흡입구 설치","도어그릴, 장변길이1m 미만","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,165638,0,0,0,165638,null,null,null,null,"",1]
["MCB10310010S","노무","L001010101000043",null,"덕트공","일반공사 직종","인",0.96,0,0,207048,198766,0,0,207048,198766,null,null,"N","N","",1]
["MCB20010010S",null,null,null,"덕트 플렉시블조인트","송풍기규격 032(#2)","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MCB20010020S",null,null,null,"덕트 플렉시블조인트","송풍기규격 036(#2⅓)","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MCB20010050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",9.7000000000000003E-2,0,0,165545,16057.8,0,0,165545,16057.8,null,null,"N","N","",1]
["MCB20010060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.111,0,0,165545,18375.400000000001,0,0,165545,18375.400000000001,null,null,"N","N","",1]
["MCB20010070S","노무","L001010101000043",null,"덕트공","일반공사 직종","인",0.42099999999999999,0,0,207048,87167.2,0,0,207048,87167.2,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,175474,0,0,0,175474,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,242964,0,0,0,242964,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,288137,0,0,0,288137,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,429659,0,0,0,429659,null,null,null,null,"",1]
["MCB30010010S",null,null,null,"일반댐퍼(사각) 설치"," 방화댐퍼, 0.1㎡이하","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MCB30010020S","노무","L001010101000043",null,"덕트공","일반공사 직종","인",0.125,0,0,207048,25881,0,0,207048,25881,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,77643,0,0,0,77643,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MCB40110030S",null,null,null,"일반댐퍼(원형) 설치","풍량조절댐퍼(수동식), D300 이하","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MCB50010010S","노무","L001010101000043",null,"덕트공","일반공사 직종","인",2.0409999999999999,0,0,207048,422584.9,0,0,207048,422584.9,null,null,"N","N","",1]
["MDA00000000S",null,null,null,"일반마감 배관보온","보온재 재질, 두께, 마감방식, 시공위치 등에 따른 시공량(m)  참조","인/일",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA00010010S","노무","L001010101000044",null,"보온공","일반공사 직종","인",2.3E-2,0,0,204285,4698.5,0,0,204285,4698.5,null,null,"N","N","",1]
["MDA00010020S","노무","L001010101000044",null,"보온공","일반공사 직종","인",2.5999999999999999E-2,0,0,204285,5311.4,0,0,204285,5311.4,null,null,"N","N","",1]
["MDA00010030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.4999999999999999E-2,0,0,165545,2483.1,0,0,165545,2483.1,null,null,"N","N","",1]
["MDA00010050S",null,null,null,"관보온/고무발포보온재","D40, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA00010080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.3000000000000002E-2,0,0,165545,5462.9,0,0,165545,5462.9,null,null,"N","N","",1]
["MDA00010090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.9E-2,0,0,165545,6456.2,0,0,165545,6456.2,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA00110010S","노무","L001010101000044",null,"보온공","일반공사 직종","인",2.5999999999999999E-2,0,0,204285,5311.4,0,0,204285,5311.4,null,null,"N","N","",1]
["MDA00110040S",null,null,null,"관보온/고무발포보온재","D32, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,10908,0,0,0,10908,null,null,null,null,"",1]
["MDA00110060S",null,null,null,"관보온/고무발포보온재","D50, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA00110080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.6999999999999998E-2,0,0,165545,6125.1,0,0,165545,6125.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,24891,0,0,0,24891,null,null,null,null,"",1]
["MDA00110110S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.125,0,0,204285,25535.599999999999,0,0,204285,25535.599999999999,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA00110130S",null,null,null,"관보온/고무발포보온재","D250, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,8611,0,0,0,8611,null,null,null,null,"",1]
["MDA00210020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.7000000000000001E-2,0,0,165545,2814.2,0,0,165545,2814.2,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,10703,0,0,0,10703,null,null,null,null,"",1]
["MDA00210060S",null,null,null,"관보온/고무발포보온재","D50, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA00210070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.5000000000000003E-2,0,0,165545,5794,0,0,165545,5794,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA00210100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.06,0,0,165545,9932.7000000000007,0,0,165545,9932.7000000000007,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA00210130S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.23,0,0,204285,46985.5,0,0,204285,46985.5,null,null,"N","N","",1]
["MDA00210140S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.26,0,0,204285,53114.1,0,0,204285,53114.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,12260,0,0,0,12260,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,13000,0,0,0,13000,null,null,null,null,"",1]
["MDA00310050S","노무","L001010101000044",null,"보온공","일반공사 직종","인",6.2E-2,0,0,204285,12665.6,0,0,204285,12665.6,null,null,"N","N","",1]
["MDA00310060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.5999999999999997E-2,0,0,165545,5959.6,0,0,165545,5959.6,null,null,"N","N","",1]
["MDA00310080S",null,null,null,"관보온/고무발포보온재","D80, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,25835,0,0,0,25835,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA00310120S",null,null,null,"관보온/고무발포보온재","D200, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,57411,0,0,0,57411,null,null,null,null,"",1]
["MDA00410010S","노무","L001010101000044",null,"보온공","일반공사 직종","인",4.2999999999999997E-2,0,0,204285,8784.2000000000007,0,0,204285,8784.2000000000007,null,null,"N","N","",1]
["MDA00410030S",null,null,null,"관보온/고무발포보온재","D25, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA00410040S",null,null,null,"관보온/고무발포보온재","D32, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,19724,0,0,0,19724,null,null,null,null,"",1]
["MDA00410060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.04,0,0,165545,6621.8,0,0,165545,6621.8,null,null,"N","N","",1]
["MDA00410080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.05,0,0,165545,8277.2000000000007,0,0,165545,8277.2000000000007,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA00410110S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.154,0,0,204285,31459.8,0,0,204285,31459.8,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,13982,0,0,0,13982,null,null,null,null,"",1]
["MDA00510030S","노무","L001010101000044",null,"보온공","일반공사 직종","인",5.7000000000000002E-2,0,0,204285,11644.2,0,0,204285,11644.2,null,null,"N","N","",1]
["MDA00510040S","노무","L001010101000044",null,"보온공","일반공사 직종","인",6.8000000000000005E-2,0,0,204285,13891.3,0,0,204285,13891.3,null,null,"N","N","",1]
["MDA00510060S",null,null,null,"관보온/고무발포보온재","D50, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,28705,0,0,0,28705,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA00510100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.6999999999999999E-2,0,0,165545,12746.9,0,0,165545,12746.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,59454,0,0,0,59454,null,null,null,null,"",1]
["MDA00510130S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.26,0,0,204285,53114.1,0,0,204285,53114.1,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA01010020S",null,null,null,"관보온/고무발포보온재","D20, 보온두께 25mm 이하, 일반접합, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,9759,0,0,0,9759,null,null,null,null,"",1]
["MDA01010050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.4E-2,0,0,165545,3973,0,0,165545,3973,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA01010080S",null,null,null,"관보온/고무발포보온재","D80, 보온두께 25mm 이하, 일반접합, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA01010100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.6000000000000001E-2,0,0,165545,9270.5,0,0,165545,9270.5,null,null,"N","N","",1]
["MDA01010120S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.17699999999999999,0,0,204285,36158.400000000001,0,0,204285,36158.400000000001,null,null,"N","N","",1]
["MDA01010120S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",8.8999999999999996E-2,0,0,165545,14733.5,0,0,165545,14733.5,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,10129,0,0,0,10129,null,null,null,null,"",1]
["MDA01110030S","노무","L001010101000044",null,"보온공","일반공사 직종","인",3.9E-2,0,0,204285,7967.1,0,0,204285,7967.1,null,null,"N","N","",1]
["MDA01110050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.7E-2,0,0,165545,4469.7,0,0,165545,4469.7,null,null,"N","N","",1]
["MDA01110070S",null,null,null,"관보온/고무발포보온재","D65, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA01110080S","노무","L001010101000044",null,"보온공","일반공사 직종","인",8.8999999999999996E-2,0,0,204285,18181.3,0,0,204285,18181.3,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA01110110S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.4999999999999997E-2,0,0,165545,12415.8,0,0,165545,12415.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,43262,0,0,0,43262,null,null,null,null,"",1]
["MDA01110140S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.27,0,0,204285,55156.9,0,0,204285,55156.9,null,null,"N","N","",1]
["MDA01210010S",null,null,null,"관보온/고무발포보온재","D15, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA01210030S",null,null,null,"관보온/고무발포보온재","D25, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,15501,0,0,0,15501,null,null,null,null,"",1]
["MDA01210060S",null,null,null,"관보온/고무발포보온재","D50, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA01210070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.2999999999999997E-2,0,0,165545,7118.4,0,0,165545,7118.4,null,null,"N","N","",1]
["MDA01210090S",null,null,null,"관보온/고무발포보온재","D100, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA01210090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.2E-2,0,0,165545,10263.700000000001,0,0,165545,10263.700000000001,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,91858,0,0,0,91858,null,null,null,null,"",1]
["MDA01310020S","노무","L001010101000044",null,"보온공","일반공사 직종","인",5.0999999999999997E-2,0,0,204285,10418.5,0,0,204285,10418.5,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA01310050S",null,null,null,"관보온/고무발포보온재","D40, 보온두께 50mm 이하, 일반접합, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,24482,0,0,0,24482,null,null,null,null,"",1]
["MDA01310070S","노무","L001010101000044",null,"보온공","일반공사 직종","인",9.2999999999999999E-2,0,0,204285,18998.5,0,0,204285,18998.5,null,null,"N","N","",1]
["MDA01310090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.8999999999999997E-2,0,0,165545,9767.1,0,0,165545,9767.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,40762,0,0,0,40762,null,null,null,null,"",1]
["MDA01310120S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.193,0,0,204285,39427,0,0,204285,39427,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,14722,0,0,0,14722,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,16445,0,0,0,16445,null,null,null,null,"",1]
["MDA01410040S","노무","L001010101000044",null,"보온공","일반공사 직종","인",7.0999999999999994E-2,0,0,204285,14504.2,0,0,204285,14504.2,null,null,"N","N","",1]
["MDA01410050S",null,null,null,"관보온/고무발포보온재","D40, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA01410070S",null,null,null,"관보온/고무발포보온재","D65, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA01410080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.06,0,0,165545,9932.7000000000007,0,0,165545,9932.7000000000007,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA01410110S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",9.2999999999999999E-2,0,0,165545,15395.6,0,0,165545,15395.6,null,null,"N","N","",1]
["MDA01410130S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.13,0,0,165545,21520.799999999999,0,0,165545,21520.799999999999,null,null,"N","N","",1]
["MDA01410140S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.3,0,0,204285,61285.5,0,0,204285,61285.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,19519,0,0,0,19519,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,24112,0,0,0,24112,null,null,null,null,"",1]
["MDA01510060S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.114,0,0,204285,23288.400000000001,0,0,204285,23288.400000000001,null,null,"N","N","",1]
["MDA01510070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.2E-2,0,0,165545,10263.700000000001,0,0,165545,10263.700000000001,null,null,"N","N","",1]
["MDA01510090S",null,null,null,"관보온/고무발포보온재","D100, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA01510110S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.22,0,0,204285,44942.7,0,0,204285,44942.7,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA01510140S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.36,0,0,204285,73542.600000000006,0,0,204285,73542.600000000006,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,103340,0,0,0,103340,null,null,null,null,"",1]
["MDA10010020S","노무","L001010101000044",null,"보온공","일반공사 직종","인",2.9000000000000001E-2,0,0,204285,5924.2,0,0,204285,5924.2,null,null,"N","N","",1]
["MDA10010040S",null,null,null,"관보온/고무발포보온재","D32, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA10010060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5999999999999999E-2,0,0,165545,4304.1000000000004,0,0,165545,4304.1000000000004,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,14926,0,0,0,14926,null,null,null,null,"",1]
["MDA10010090S",null,null,null,"관보온/고무발포보온재","D100, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA10010120S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",8.2000000000000003E-2,0,0,165545,13574.6,0,0,165545,13574.6,null,null,"N","N","",1]
["MDA10110010S","노무","L001010101000044",null,"보온공","일반공사 직종","인",2.9000000000000001E-2,0,0,204285,5924.2,0,0,204285,5924.2,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA10110040S",null,null,null,"관보온/고무발포보온재","D32, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA10110050S",null,null,null,"관보온/고무발포보온재","D40, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA10110080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.1000000000000002E-2,0,0,165545,6787.3,0,0,165545,6787.3,null,null,"N","N","",1]
["MDA10110090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.8000000000000001E-2,0,0,165545,7946.1,0,0,165545,7946.1,null,null,"N","N","",1]
["MDA10110100S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.11600000000000001,0,0,204285,23697,0,0,204285,23697,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,63152,0,0,0,63152,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,9555,0,0,0,9555,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,10908,0,0,0,10908,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,13778,0,0,0,13778,null,null,null,null,"",1]
["MDA10210060S",null,null,null,"관보온/고무발포보온재","D50, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA10210070S",null,null,null,"관보온/고무발포보온재","D65, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA10210080S",null,null,null,"관보온/고무발포보온재","D80, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA10210110S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.08,0,0,165545,13243.6,0,0,165545,13243.6,null,null,"N","N","",1]
["MDA10210130S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.26,0,0,204285,53114.1,0,0,204285,53114.1,null,null,"N","N","",1]
["MDA10210140S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.28000000000000003,0,0,204285,57199.8,0,0,204285,57199.8,null,null,"N","N","",1]
["MDA10310020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.3E-2,0,0,165545,3807.5,0,0,165545,3807.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,14148,0,0,0,14148,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,16649,0,0,0,16649,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA10310070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.2999999999999997E-2,0,0,165545,7118.4,0,0,165545,7118.4,null,null,"N","N","",1]
["MDA10310090S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.109,0,0,204285,22267,0,0,204285,22267,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA10310140S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.25,0,0,204285,51071.199999999997,0,0,204285,51071.199999999997,null,null,"N","N","",1]
["MDA10410010S","노무","L001010101000044",null,"보온공","일반공사 직종","인",4.7E-2,0,0,204285,9601.2999999999993,0,0,204285,9601.2999999999993,null,null,"N","N","",1]
["MDA10410020S","노무","L001010101000044",null,"보온공","일반공사 직종","인",5.1999999999999998E-2,0,0,204285,10622.8,0,0,204285,10622.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,15705,0,0,0,15705,null,null,null,null,"",1]
["MDA10410060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.3999999999999997E-2,0,0,165545,7283.9,0,0,165545,7283.9,null,null,"N","N","",1]
["MDA10410070S",null,null,null,"관보온/고무발포보온재","D65, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA10410080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.5E-2,0,0,165545,9104.9,0,0,165545,9104.9,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA10410120S",null,null,null,"관보온/고무발포보온재","D200, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,68893,0,0,0,68893,null,null,null,null,"",1]
["MDA10510010S","노무","L001010101000044",null,"보온공","일반공사 직종","인",5.5E-2,0,0,204285,11235.6,0,0,204285,11235.6,null,null,"N","N","",1]
["MDA10510010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.7E-2,0,0,165545,4469.7,0,0,165545,4469.7,null,null,"N","N","",1]
["MDA10510040S",null,null,null,"관보온/고무발포보온재","D32, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA10510060S",null,null,null,"관보온/고무발포보온재","D50, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA10510080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.4000000000000001E-2,0,0,165545,10594.8,0,0,165545,10594.8,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA10510110S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.19700000000000001,0,0,204285,40244.1,0,0,204285,40244.1,null,null,"N","N","",1]
["MDA10510130S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.28000000000000003,0,0,204285,57199.8,0,0,204285,57199.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,91858,0,0,0,91858,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,8815,0,0,0,8815,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,9964,0,0,0,9964,null,null,null,null,"",1]
["MDA11010040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.1999999999999999E-2,0,0,165545,3641.9,0,0,165545,3641.9,null,null,"N","N","",1]
["MDA11010060S",null,null,null,"관보온/고무발포보온재","D50, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,20463,0,0,0,20463,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA11010110S",null,null,null,"관보온/고무발포보온재","D150, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA11010120S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.19600000000000001,0,0,204285,40039.800000000003,0,0,204285,40039.800000000003,null,null,"N","N","",1]
["MDA11010130S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.24,0,0,204285,49028.4,0,0,204285,49028.4,null,null,"N","N","",1]
["MDA11010140S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.13,0,0,165545,21520.799999999999,0,0,165545,21520.799999999999,null,null,"N","N","",1]
["MDA11110020S",null,null,null,"관보온/고무발포보온재","D20, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,12630,0,0,0,12630,null,null,null,null,"",1]
["MDA11110050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.03,0,0,165545,4966.3,0,0,165545,4966.3,null,null,"N","N","",1]
["MDA11110060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.5999999999999997E-2,0,0,165545,5959.6,0,0,165545,5959.6,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA11110120S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.23,0,0,204285,46985.5,0,0,204285,46985.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,78333,0,0,0,78333,null,null,null,null,"",1]
["MDA11210010S","노무","L001010101000044",null,"보온공","일반공사 직종","인",4.2999999999999997E-2,0,0,204285,8784.2000000000007,0,0,204285,8784.2000000000007,null,null,"N","N","",1]
["MDA11210030S","노무","L001010101000044",null,"보온공","일반공사 직종","인",5.2999999999999999E-2,0,0,204285,10827.1,0,0,204285,10827.1,null,null,"N","N","",1]
["MDA11210040S",null,null,null,"관보온/고무발포보온재","D32, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,24686,0,0,0,24686,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA11210080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.0999999999999999E-2,0,0,165545,10098.200000000001,0,0,165545,10098.200000000001,null,null,"N","N","",1]
["MDA11210100S",null,null,null,"관보온/고무발포보온재","D125, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA11210110S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.2,0,0,204285,40857,0,0,204285,40857,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA11310010S",null,null,null,"관보온/고무발포보온재","D15, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,14352,0,0,0,14352,null,null,null,null,"",1]
["MDA11310040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.5000000000000003E-2,0,0,165545,5794,0,0,165545,5794,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA11310060S",null,null,null,"관보온/고무발포보온재","D50, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA11310100S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.157,0,0,204285,32072.7,0,0,204285,32072.7,null,null,"N","N","",1]
["MDA11310100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.8E-2,0,0,165545,12912.5,0,0,165545,12912.5,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,84074,0,0,0,84074,null,null,null,null,"",1]
["MDA11410020S","노무","L001010101000044",null,"보온공","일반공사 직종","인",6.4000000000000001E-2,0,0,204285,13074.2,0,0,204285,13074.2,null,null,"N","N","",1]
["MDA11410030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.4000000000000002E-2,0,0,165545,5628.5,0,0,165545,5628.5,null,null,"N","N","",1]
["MDA11410050S",null,null,null,"관보온/고무발포보온재","D40, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,26779,0,0,0,26779,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA11410090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.4999999999999997E-2,0,0,165545,12415.8,0,0,165545,12415.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,51670,0,0,0,51670,null,null,null,null,"",1]
["MDA11410120S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.25,0,0,204285,51071.199999999997,0,0,204285,51071.199999999997,null,null,"N","N","",1]
["MDA11410140S",null,null,null,"관보온/고무발포보온재","D300, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA11510010S",null,null,null,"관보온/고무발포보온재","D15, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,22390,0,0,0,22390,null,null,null,null,"",1]
["MDA11510030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.1000000000000002E-2,0,0,165545,6787.3,0,0,165545,6787.3,null,null,"N","N","",1]
["MDA11510050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.7000000000000002E-2,0,0,165545,9436,0,0,165545,9436,null,null,"N","N","",1]
["MDA11510070S",null,null,null,"관보온/고무발포보온재","D65, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA11510080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",8.2000000000000003E-2,0,0,165545,13574.6,0,0,165545,13574.6,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,86117,0,0,0,86117,null,null,null,null,"",1]
["MDA11510140S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.41,0,0,204285,83756.800000000003,0,0,204285,83756.800000000003,null,null,"N","N","",1]
["MDA20010010S","노무","L001010101000044",null,"보온공","일반공사 직종","인",1.6E-2,0,0,204285,3268.5,0,0,204285,3268.5,null,null,"N","N","",1]
["MDA20010030S",null,null,null,"관보온/발포폴리에틸렌보온재","D25, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,7093,0,0,0,7093,null,null,null,null,"",1]
["MDA20010060S","노무","L001010101000044",null,"보온공","일반공사 직종","인",3.3000000000000002E-2,0,0,204285,6741.4,0,0,204285,6741.4,null,null,"N","N","",1]
["MDA20010070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.02,0,0,165545,3310.9,0,0,165545,3310.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,16075,0,0,0,16075,null,null,null,null,"",1]
["MDA20010100S","노무","L001010101000044",null,"보온공","일반공사 직종","인",6.9000000000000006E-2,0,0,204285,14095.6,0,0,204285,14095.6,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA20010130S",null,null,null,"관보온/발포폴리에틸렌보온재","D250, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,43058,0,0,0,43058,null,null,null,null,"",1]
["MDA20110020S","노무","L001010101000044",null,"보온공","일반공사 직종","인",2.1000000000000001E-2,0,0,204285,4289.8999999999996,0,0,204285,4289.8999999999996,null,null,"N","N","",1]
["MDA20110040S",null,null,null,"관보온/발포폴리에틸렌보온재","D32, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA20110050S",null,null,null,"관보온/발포폴리에틸렌보온재","D40, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA20110070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.1999999999999999E-2,0,0,165545,3641.9,0,0,165545,3641.9,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA20110090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.1E-2,0,0,165545,5131.8,0,0,165545,5131.8,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA20110120S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.11799999999999999,0,0,204285,24105.599999999999,0,0,204285,24105.599999999999,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,6889,0,0,0,6889,null,null,null,null,"",1]
["MDA20210050S","노무","L001010101000044",null,"보온공","일반공사 직종","인",3.5999999999999997E-2,0,0,204285,7354.2,0,0,204285,7354.2,null,null,"N","N","",1]
["MDA20210050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.7999999999999999E-2,0,0,165545,2979.8,0,0,165545,2979.8,null,null,"N","N","",1]
["MDA20210070S",null,null,null,"관보온/발포폴리에틸렌보온재","D65, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,17223,0,0,0,17223,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA20210110S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.1999999999999998E-2,0,0,165545,8608.2999999999993,0,0,165545,8608.2999999999993,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,47077,0,0,0,47077,null,null,null,null,"",1]
["MDA20210140S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.192,0,0,204285,39222.699999999997,0,0,204285,39222.699999999997,null,null,"N","N","",1]
["MDA20310030S",null,null,null,"관보온/발포폴리에틸렌보온재","D25, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA20310040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.9E-2,0,0,165545,3145.3,0,0,165545,3145.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,10908,0,0,0,10908,null,null,null,null,"",1]
["MDA20310060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5999999999999999E-2,0,0,165545,4304.1000000000004,0,0,165545,4304.1000000000004,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA20310090S",null,null,null,"관보온/발포폴리에틸렌보온재","D100, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA20310110S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.05,0,0,165545,8277.2000000000007,0,0,165545,8277.2000000000007,null,null,"N","N","",1]
["MDA20310130S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.13900000000000001,0,0,204285,28395.599999999999,0,0,204285,28395.599999999999,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA20410020S",null,null,null,"관보온/발포폴리에틸렌보온재","D20, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,10334,0,0,0,10334,null,null,null,null,"",1]
["MDA20410040S","노무","L001010101000044",null,"보온공","일반공사 직종","인",4.2000000000000003E-2,0,0,204285,8579.9,0,0,204285,8579.9,null,null,"N","N","",1]
["MDA20410060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.9000000000000001E-2,0,0,165545,4800.8,0,0,165545,4800.8,null,null,"N","N","",1]
["MDA20410070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.03,0,0,165545,4966.3,0,0,165545,4966.3,null,null,"N","N","",1]
["MDA20410090S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.08,0,0,204285,16342.8,0,0,204285,16342.8,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,38261,0,0,0,38261,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,44206,0,0,0,44206,null,null,null,null,"",1]
["MDA20510010S","노무","L001010101000044",null,"보온공","일반공사 직종","인",3.5000000000000003E-2,0,0,204285,7149.9,0,0,204285,7149.9,null,null,"N","N","",1]
["MDA20510020S",null,null,null,"관보온/발포폴리에틸렌보온재","D20, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA20510040S",null,null,null,"관보온/발포폴리에틸렌보온재","D32, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA20510050S",null,null,null,"관보온/발포폴리에틸렌보온재","D40, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA20510070S",null,null,null,"관보온/발포폴리에틸렌보온재","D65, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA20510080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.04,0,0,165545,6621.8,0,0,165545,6621.8,null,null,"N","N","",1]
["MDA20510100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.5E-2,0,0,165545,9104.9,0,0,165545,9104.9,null,null,"N","N","",1]
["MDA20510110S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.128,0,0,204285,26148.400000000001,0,0,204285,26148.400000000001,null,null,"N","N","",1]
["MDA20510120S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.153,0,0,204285,31255.599999999999,0,0,204285,31255.599999999999,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,5536,0,0,0,5536,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,6315,0,0,0,6315,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA21010060S",null,null,null,"관보온/발포폴리에틸렌보온재","D50, 보온두께 25mm 이하, 일반접합, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA21010080S","노무","L001010101000044",null,"보온공","일반공사 직종","인",5.6000000000000001E-2,0,0,204285,11439.9,0,0,204285,11439.9,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,27761,0,0,0,27761,null,null,null,null,"",1]
["MDA21010130S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.152,0,0,204285,31051.3,0,0,204285,31051.3,null,null,"N","N","",1]
["MDA21010140S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.17699999999999999,0,0,204285,36158.400000000001,0,0,204285,36158.400000000001,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,7259,0,0,0,7259,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,8037,0,0,0,8037,null,null,null,null,"",1]
["MDA21110060S",null,null,null,"관보온/발포폴리에틸렌보온재","D50, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA21110060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.1999999999999999E-2,0,0,165545,3641.9,0,0,165545,3641.9,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA21110090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.7999999999999999E-2,0,0,165545,6290.7,0,0,165545,6290.7,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA21110130S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.17199999999999999,0,0,204285,35137,0,0,204285,35137,null,null,"N","N","",1]
["MDA21110140S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.1,0,0,165545,16554.5,0,0,165545,16554.5,null,null,"N","N","",1]
["MDA21210020S",null,null,null,"관보온/발포폴리에틸렌보온재","D20, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA21210040S",null,null,null,"관보온/발포폴리에틸렌보온재","D32, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA21210060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5999999999999999E-2,0,0,165545,4304.1000000000004,0,0,165545,4304.1000000000004,null,null,"N","N","",1]
["MDA21210070S","노무","L001010101000044",null,"보온공","일반공사 직종","인",6.3E-2,0,0,204285,12869.9,0,0,204285,12869.9,null,null,"N","N","",1]
["MDA21210080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.7999999999999999E-2,0,0,165545,6290.7,0,0,165545,6290.7,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA21210120S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.16800000000000001,0,0,204285,34319.800000000003,0,0,204285,34319.800000000003,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,57411,0,0,0,57411,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,9185,0,0,0,9185,null,null,null,null,"",1]
["MDA21310030S",null,null,null,"관보온/발포폴리에틸렌보온재","D25, 보온두께 50mm 이하, 일반접합, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA21310040S",null,null,null,"관보온/발포폴리에틸렌보온재","D32, 보온두께 50mm 이하, 일반접합, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA21310050S",null,null,null,"관보온/발포폴리에틸렌보온재","D40, 보온두께 50mm 이하, 일반접합, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA21310080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.6999999999999998E-2,0,0,165545,6125.1,0,0,165545,6125.1,null,null,"N","N","",1]
["MDA21310100S",null,null,null,"관보온/발포폴리에틸렌보온재","D125, 보온두께 50mm 이하, 일반접합, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA21310110S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.11799999999999999,0,0,204285,24105.599999999999,0,0,204285,24105.599999999999,null,null,"N","N","",1]
["MDA21310130S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",8.2000000000000003E-2,0,0,165545,13574.6,0,0,165545,13574.6,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,50891,0,0,0,50891,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,10538,0,0,0,10538,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA21410040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5000000000000001E-2,0,0,165545,4138.6000000000004,0,0,165545,4138.6000000000004,null,null,"N","N","",1]
["MDA21410060S",null,null,null,"관보온/발포폴리에틸렌보온재","D50, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA21410110S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.13400000000000001,0,0,204285,27374.1,0,0,204285,27374.1,null,null,"N","N","",1]
["MDA21410120S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.161,0,0,204285,32889.800000000003,0,0,204285,32889.800000000003,null,null,"N","N","",1]
["MDA21410130S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.185,0,0,204285,37792.699999999997,0,0,204285,37792.699999999997,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,57411,0,0,0,57411,null,null,null,null,"",1]
["MDA21510020S",null,null,null,"관보온/발포폴리에틸렌보온재","D20, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,14722,0,0,0,14722,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,20093,0,0,0,20093,null,null,null,null,"",1]
["MDA21510060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.1000000000000002E-2,0,0,165545,6787.3,0,0,165545,6787.3,null,null,"N","N","",1]
["MDA21510090S",null,null,null,"관보온/발포폴리에틸렌보온재","D100, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA21510090S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.114,0,0,204285,23288.400000000001,0,0,204285,23288.400000000001,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA21510120S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",9.5000000000000001E-2,0,0,165545,15726.7,0,0,165545,15726.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,63152,0,0,0,63152,null,null,null,null,"",1]
["MDA30010010S","노무","L001010101000044",null,"보온공","일반공사 직종","인",1.7999999999999999E-2,0,0,204285,3677.1,0,0,204285,3677.1,null,null,"N","N","",1]
["MDA30010030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.0999999999999999E-2,0,0,165545,1820.9,0,0,165545,1820.9,null,null,"N","N","",1]
["MDA30010040S",null,null,null,"관보온/발포폴리에틸렌보온재","D32, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA30010080S","노무","L001010101000044",null,"보온공","일반공사 직종","인",5.1999999999999998E-2,0,0,204285,10622.8,0,0,204285,10622.8,null,null,"N","N","",1]
["MDA30010080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5999999999999999E-2,0,0,165545,4304.1000000000004,0,0,165545,4304.1000000000004,null,null,"N","N","",1]
["MDA30010100S","노무","L001010101000044",null,"보온공","일반공사 직종","인",7.4999999999999997E-2,0,0,204285,15321.3,0,0,204285,15321.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,33094,0,0,0,33094,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA30110010S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.02,0,0,204285,4085.7,0,0,204285,4085.7,null,null,"N","N","",1]
["MDA30110030S",null,null,null,"관보온/발포폴리에틸렌보온재","D25, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,8611,0,0,0,8611,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA30110070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.4E-2,0,0,165545,3973,0,0,165545,3973,null,null,"N","N","",1]
["MDA30110080S",null,null,null,"관보온/발포폴리에틸렌보온재","D80, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA30110100S","노무","L001010101000044",null,"보온공","일반공사 직종","인",8.5000000000000006E-2,0,0,204285,17364.2,0,0,204285,17364.2,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA30110130S",null,null,null,"관보온/발포폴리에틸렌보온재","D250, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,52614,0,0,0,52614,null,null,null,null,"",1]
["MDA30210020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.2999999999999999E-2,0,0,165545,2152,0,0,165545,2152,null,null,"N","N","",1]
["MDA30210030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.4999999999999999E-2,0,0,165545,2483.1,0,0,165545,2483.1,null,null,"N","N","",1]
["MDA30210050S",null,null,null,"관보온/발포폴리에틸렌보온재","D40, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA30210090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.04,0,0,165545,6621.8,0,0,165545,6621.8,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA30210120S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.151,0,0,204285,30847,0,0,204285,30847,null,null,"N","N","",1]
["MDA30210140S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.21,0,0,204285,42899.8,0,0,204285,42899.8,null,null,"N","N","",1]
["MDA30310010S",null,null,null,"관보온/발포폴리에틸렌보온재","D15, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,9759,0,0,0,9759,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,10129,0,0,0,10129,null,null,null,null,"",1]
["MDA30310050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.4E-2,0,0,165545,3973,0,0,165545,3973,null,null,"N","N","",1]
["MDA30310070S",null,null,null,"관보온/발포폴리에틸렌보온재","D65, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,19519,0,0,0,19519,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA30310120S",null,null,null,"관보온/발포폴리에틸렌보온재","D200, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,37521,0,0,0,37521,null,null,null,null,"",1]
["MDA30310140S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.16300000000000001,0,0,204285,33298.400000000001,0,0,204285,33298.400000000001,null,null,"N","N","",1]
["MDA30410010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.7000000000000001E-2,0,0,165545,2814.2,0,0,165545,2814.2,null,null,"N","N","",1]
["MDA30410030S",null,null,null,"관보온/발포폴리에틸렌보온재","D25, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,13204,0,0,0,13204,null,null,null,null,"",1]
["MDA30410060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.1E-2,0,0,165545,5131.8,0,0,165545,5131.8,null,null,"N","N","",1]
["MDA30410070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.3000000000000002E-2,0,0,165545,5462.9,0,0,165545,5462.9,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA30410100S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.105,0,0,204285,21449.9,0,0,204285,21449.9,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA30410130S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.16900000000000001,0,0,204285,34524.1,0,0,204285,34524.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,52614,0,0,0,52614,null,null,null,null,"",1]
["MDA30510020S","노무","L001010101000044",null,"보온공","일반공사 직종","인",4.3999999999999997E-2,0,0,204285,8988.5,0,0,204285,8988.5,null,null,"N","N","",1]
["MDA30510040S","노무","L001010101000044",null,"보온공","일반공사 직종","인",5.2999999999999999E-2,0,0,204285,10827.1,0,0,204285,10827.1,null,null,"N","N","",1]
["MDA30510050S",null,null,null,"관보온/발포폴리에틸렌보온재","D40, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,22390,0,0,0,22390,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA30510090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.0999999999999997E-2,0,0,165545,8442.7000000000007,0,0,165545,8442.7000000000007,null,null,"N","N","",1]
["MDA30510110S",null,null,null,"관보온/발포폴리에틸렌보온재","D150, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA30510120S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.17100000000000001,0,0,204285,34932.699999999997,0,0,204285,34932.699999999997,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA31010020S",null,null,null,"관보온/발포폴리에틸렌보온재","D20, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,7093,0,0,0,7093,null,null,null,null,"",1]
["MDA31010050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.9E-2,0,0,165545,3145.3,0,0,165545,3145.3,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA31010070S",null,null,null,"관보온/발포폴리에틸렌보온재","D65, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA31010110S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.107,0,0,204285,21858.400000000001,0,0,204285,21858.400000000001,null,null,"N","N","",1]
["MDA31010120S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.13800000000000001,0,0,204285,28191.3,0,0,204285,28191.3,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,7093,0,0,0,7093,null,null,null,null,"",1]
["MDA31110030S","노무","L001010101000044",null,"보온공","일반공사 직종","인",3.1E-2,0,0,204285,6332.8,0,0,204285,6332.8,null,null,"N","N","",1]
["MDA31110040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.9E-2,0,0,165545,3145.3,0,0,165545,3145.3,null,null,"N","N","",1]
["MDA31110060S",null,null,null,"관보온/발포폴리에틸렌보온재","D50, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,14352,0,0,0,14352,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,35225,0,0,0,35225,null,null,null,null,"",1]
["MDA31110130S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.193,0,0,204285,39427,0,0,204285,39427,null,null,"N","N","",1]
["MDA31210010S",null,null,null,"관보온/발포폴리에틸렌보온재","D15, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA31210020S",null,null,null,"관보온/발포폴리에틸렌보온재","D20, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,10908,0,0,0,10908,null,null,null,null,"",1]
["MDA31210040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.1999999999999999E-2,0,0,165545,3641.9,0,0,165545,3641.9,null,null,"N","N","",1]
["MDA31210060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.03,0,0,165545,4966.3,0,0,165545,4966.3,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA31210090S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.10199999999999999,0,0,204285,20837,0,0,204285,20837,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,66850,0,0,0,66850,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,78333,0,0,0,78333,null,null,null,null,"",1]
["MDA31310020S","노무","L001010101000044",null,"보온공","일반공사 직종","인",4.1000000000000002E-2,0,0,204285,8375.6,0,0,204285,8375.6,null,null,"N","N","",1]
["MDA31310040S",null,null,null,"관보온/발포폴리에틸렌보온재","D32, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,16445,0,0,0,16445,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA31310080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.1000000000000002E-2,0,0,165545,6787.3,0,0,165545,6787.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,32150,0,0,0,32150,null,null,null,null,"",1]
["MDA31310110S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.13100000000000001,0,0,204285,26761.3,0,0,204285,26761.3,null,null,"N","N","",1]
["MDA31310120S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.157,0,0,204285,32072.7,0,0,204285,32072.7,null,null,"N","N","",1]
["MDA31310140S",null,null,null,"관보온/발포폴리에틸렌보온재","D300, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,11686,0,0,0,11686,null,null,null,null,"",1]
["MDA31410030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.4E-2,0,0,165545,3973,0,0,165545,3973,null,null,"N","N","",1]
["MDA31410040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.8000000000000001E-2,0,0,165545,4635.2,0,0,165545,4635.2,null,null,"N","N","",1]
["MDA31410060S",null,null,null,"관보온/발포폴리에틸렌보온재","D50, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA31410080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.7E-2,0,0,165545,7780.6,0,0,165545,7780.6,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA31410110S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.15,0,0,204285,30642.7,0,0,204285,30642.7,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA31410130S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.21,0,0,204285,42899.8,0,0,204285,42899.8,null,null,"N","N","",1]
["MDA31510010S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.05,0,0,204285,10214.200000000001,0,0,204285,10214.200000000001,null,null,"N","N","",1]
["MDA31510020S",null,null,null,"관보온/발포폴리에틸렌보온재","D20, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA31510040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.4000000000000002E-2,0,0,165545,5628.5,0,0,165545,5628.5,null,null,"N","N","",1]
["MDA31510060S","노무","L001010101000044",null,"보온공","일반공사 직종","인",9.4E-2,0,0,204285,19202.7,0,0,204285,19202.7,null,null,"N","N","",1]
["MDA31510060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.7E-2,0,0,165545,7780.6,0,0,165545,7780.6,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,37687,0,0,0,37687,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA31510130S",null,null,null,"관보온/발포폴리에틸렌보온재","D250, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA40010010S",null,null,null,"관보온/유리솜보온재","D15, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA40010020S",null,null,null,"관보온/유리솜보온재","D20, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA40010040S",null,null,null,"관보온/유리솜보온재","D32, 보온두께 25mm 이하, 일반접합, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA40010050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.7999999999999999E-2,0,0,165545,2979.8,0,0,165545,2979.8,null,null,"N","N","",1]
["MDA40010060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.1000000000000001E-2,0,0,165545,3476.4,0,0,165545,3476.4,null,null,"N","N","",1]
["MDA40010070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5000000000000001E-2,0,0,165545,4138.6000000000004,0,0,165545,4138.6000000000004,null,null,"N","N","",1]
["MDA40010090S","노무","L001010101000044",null,"보온공","일반공사 직종","인",6.9000000000000006E-2,0,0,204285,14095.6,0,0,204285,14095.6,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,39818,0,0,0,39818,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,47077,0,0,0,47077,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA40110030S",null,null,null,"관보온/유리솜보온재","D25, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA40110040S",null,null,null,"관보온/유리솜보온재","D32, 보온두께 25mm 이하, 일반접합, 옥내일반, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA40110050S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.04,0,0,204285,8171.4,0,0,204285,8171.4,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,19149,0,0,0,19149,null,null,null,null,"",1]
["MDA40110100S","노무","L001010101000044",null,"보온공","일반공사 직종","인",9.5000000000000001E-2,0,0,204285,19407,0,0,204285,19407,null,null,"N","N","",1]
["MDA40110110S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.111,0,0,204285,22675.599999999999,0,0,204285,22675.599999999999,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,52244,0,0,0,52244,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,57411,0,0,0,57411,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,7833,0,0,0,7833,null,null,null,null,"",1]
["MDA40210030S",null,null,null,"관보온/유리솜보온재","D25, 보온두께 25mm 이하, 일반접합, 옥내일반, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA40210040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.9E-2,0,0,165545,3145.3,0,0,165545,3145.3,null,null,"N","N","",1]
["MDA40210060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.7E-2,0,0,165545,4469.7,0,0,165545,4469.7,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA40210110S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.4000000000000001E-2,0,0,165545,10594.8,0,0,165545,10594.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,36743,0,0,0,36743,null,null,null,null,"",1]
["MDA40210130S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.21,0,0,204285,42899.8,0,0,204285,42899.8,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA40310020S",null,null,null,"관보온/유리솜보온재","D20, 보온두께 50mm 이하, 일반접합, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA40310040S","노무","L001010101000044",null,"보온공","일반공사 직종","인",4.7E-2,0,0,204285,9601.2999999999993,0,0,204285,9601.2999999999993,null,null,"N","N","",1]
["MDA40310050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.8000000000000001E-2,0,0,165545,4635.2,0,0,165545,4635.2,null,null,"N","N","",1]
["MDA40310060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.2000000000000001E-2,0,0,165545,5297.4,0,0,165545,5297.4,null,null,"N","N","",1]
["MDA40310090S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.09,0,0,204285,18385.599999999999,0,0,204285,18385.599999999999,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,30428,0,0,0,30428,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,43058,0,0,0,43058,null,null,null,null,"",1]
["MDA40410010S",null,null,null,"관보온/유리솜보온재","D15, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA40410020S",null,null,null,"관보온/유리솜보온재","D20, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA40410030S",null,null,null,"관보온/유리솜보온재","D25, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA40410050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.1E-2,0,0,165545,5131.8,0,0,165545,5131.8,null,null,"N","N","",1]
["MDA40410070S",null,null,null,"관보온/유리솜보온재","D65, 보온두께 50mm 이하, 일반접합, 옥내일반, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA40410080S","노무","L001010101000044",null,"보온공","일반공사 직종","인",9.0999999999999998E-2,0,0,204285,18589.900000000001,0,0,204285,18589.900000000001,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA40410100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.8999999999999997E-2,0,0,165545,9767.1,0,0,165545,9767.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,47855,0,0,0,47855,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA40510010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.1999999999999999E-2,0,0,165545,3641.9,0,0,165545,3641.9,null,null,"N","N","",1]
["MDA40510030S",null,null,null,"관보온/유리솜보온재","D25, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA40510070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.3999999999999997E-2,0,0,165545,7283.9,0,0,165545,7283.9,null,null,"N","N","",1]
["MDA40510080S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.104,0,0,204285,21245.599999999999,0,0,204285,21245.599999999999,null,null,"N","N","",1]
["MDA40510100S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.13500000000000001,0,0,204285,27578.400000000001,0,0,204285,27578.400000000001,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,47077,0,0,0,47077,null,null,null,null,"",1]
["MDA40510130S",null,null,null,"관보온/유리솜보온재","D250, 보온두께 50mm 이하, 일반접합, 옥내일반, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,74634,0,0,0,74634,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,8037,0,0,0,8037,null,null,null,null,"",1]
["MDA41010030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.4999999999999999E-2,0,0,165545,2483.1,0,0,165545,2483.1,null,null,"N","N","",1]
["MDA41010050S",null,null,null,"관보온/유리솜보온재","D40, 보온두께 25mm 이하, 일반접합, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA41010060S",null,null,null,"관보온/유리솜보온재","D50, 보온두께 25mm 이하, 일반접합, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA41010090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.1000000000000002E-2,0,0,165545,6787.3,0,0,165545,6787.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,29075,0,0,0,29075,null,null,null,null,"",1]
["MDA41010120S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.16400000000000001,0,0,204285,33502.699999999997,0,0,204285,33502.699999999997,null,null,"N","N","",1]
["MDA41010140S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.11,0,0,165545,18209.900000000001,0,0,165545,18209.900000000001,null,null,"N","N","",1]
["MDA41110010S",null,null,null,"관보온/유리솜보온재","D15, 보온두께 25mm 이하, 일반접합, 기계실, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,9185,0,0,0,9185,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA41110050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.4E-2,0,0,165545,3973,0,0,165545,3973,null,null,"N","N","",1]
["MDA41110070S","노무","L001010101000044",null,"보온공","일반공사 직종","인",6.7000000000000004E-2,0,0,204285,13687,0,0,204285,13687,null,null,"N","N","",1]
["MDA41110080S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.08,0,0,204285,16342.8,0,0,204285,16342.8,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA41110120S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.185,0,0,204285,37792.699999999997,0,0,204285,37792.699999999997,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,53188,0,0,0,53188,null,null,null,null,"",1]
["MDA41110140S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.24,0,0,204285,49028.4,0,0,204285,49028.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,9759,0,0,0,9759,null,null,null,null,"",1]
["MDA41210030S",null,null,null,"관보온/유리솜보온재","D25, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA41210050S",null,null,null,"관보온/유리솜보온재","D40, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA41210070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.04,0,0,165545,6621.8,0,0,165545,6621.8,null,null,"N","N","",1]
["MDA41210100S",null,null,null,"관보온/유리솜보온재","D125, 보온두께 25mm 이하, 일반접합, 기계실, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA41210100S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.13600000000000001,0,0,204285,27782.7,0,0,204285,27782.7,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA41210130S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.13,0,0,165545,21520.799999999999,0,0,165545,21520.799999999999,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,82418,0,0,0,82418,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA41310050S",null,null,null,"관보온/유리솜보온재","D40, 보온두께 50mm 이하, 일반접합, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA41310090S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.106,0,0,204285,21654.2,0,0,204285,21654.2,null,null,"N","N","",1]
["MDA41310090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.2999999999999999E-2,0,0,165545,8773.7999999999993,0,0,165545,8773.7999999999993,null,null,"N","N","",1]
["MDA41310110S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.152,0,0,204285,31051.3,0,0,204285,31051.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,61109,0,0,0,61109,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,68893,0,0,0,68893,null,null,null,null,"",1]
["MDA41410020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5999999999999999E-2,0,0,165545,4304.1000000000004,0,0,165545,4304.1000000000004,null,null,"N","N","",1]
["MDA41410040S",null,null,null,"관보온/유리솜보온재","D32, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,21612,0,0,0,21612,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA41410080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.5E-2,0,0,165545,9104.9,0,0,165545,9104.9,null,null,"N","N","",1]
["MDA41410090S",null,null,null,"관보온/유리솜보온재","D100, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA41410110S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.17199999999999999,0,0,204285,35137,0,0,204285,35137,null,null,"N","N","",1]
["MDA41410120S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.1,0,0,165545,16554.5,0,0,165545,16554.5,null,null,"N","N","",1]
["MDA41410140S",null,null,null,"관보온/유리솜보온재","D300, 보온두께 50mm 이하, 일반접합, 기계실, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,15705,0,0,0,15705,null,null,null,null,"",1]
["MDA41510030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.2000000000000001E-2,0,0,165545,5297.4,0,0,165545,5297.4,null,null,"N","N","",1]
["MDA41510040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.7999999999999999E-2,0,0,165545,6290.7,0,0,165545,6290.7,null,null,"N","N","",1]
["MDA41510060S",null,null,null,"관보온/유리솜보온재","D50, 보온두께 50mm 이하, 일반접합, 기계실, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA41510100S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.16800000000000001,0,0,204285,34319.800000000003,0,0,204285,34319.800000000003,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,57411,0,0,0,57411,null,null,null,null,"",1]
["MDA41510130S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.28999999999999998,0,0,204285,59242.6,0,0,204285,59242.6,null,null,"N","N","",1]
["MDA50010010S","노무","L001010101000044",null,"보온공","일반공사 직종","인",2.3E-2,0,0,204285,4698.5,0,0,204285,4698.5,null,null,"N","N","",1]
["MDA50010020S",null,null,null,"관보온/유리솜보온재","D20, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA50010030S",null,null,null,"관보온/유리솜보온재","D25, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,9555,0,0,0,9555,null,null,null,null,"",1]
["MDA50010060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.3E-2,0,0,165545,3807.5,0,0,165545,3807.5,null,null,"N","N","",1]
["MDA50010080S",null,null,null,"관보온/유리솜보온재","D80, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA50010090S","노무","L001010101000044",null,"보온공","일반공사 직종","인",7.4999999999999997E-2,0,0,204285,15321.3,0,0,204285,15321.3,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA50010130S",null,null,null,"관보온/유리솜보온재","D250, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,51096,0,0,0,51096,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,56263,0,0,0,56263,null,null,null,null,"",1]
["MDA50110020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.4E-2,0,0,165545,2317.6,0,0,165545,2317.6,null,null,"N","N","",1]
["MDA50110040S",null,null,null,"관보온/유리솜보온재","D32, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA50110080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.6999999999999998E-2,0,0,165545,6125.1,0,0,165545,6125.1,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA50110110S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.122,0,0,204285,24922.7,0,0,204285,24922.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,57411,0,0,0,57411,null,null,null,null,"",1]
["MDA50110140S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.22,0,0,204285,44942.7,0,0,204285,44942.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,8611,0,0,0,8611,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,10703,0,0,0,10703,null,null,null,null,"",1]
["MDA50210040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.1999999999999999E-2,0,0,165545,3641.9,0,0,165545,3641.9,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,24482,0,0,0,24482,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA50210110S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.14199999999999999,0,0,204285,29008.400000000001,0,0,204285,29008.400000000001,null,null,"N","N","",1]
["MDA50210120S",null,null,null,"관보온/유리솜보온재","D200, 보온두께 25mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA50210130S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.23,0,0,204285,46985.5,0,0,204285,46985.5,null,null,"N","N","",1]
["MDA50310010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.9E-2,0,0,165545,3145.3,0,0,165545,3145.3,null,null,"N","N","",1]
["MDA50310030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.1999999999999999E-2,0,0,165545,3641.9,0,0,165545,3641.9,null,null,"N","N","",1]
["MDA50310040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5999999999999999E-2,0,0,165545,4304.1000000000004,0,0,165545,4304.1000000000004,null,null,"N","N","",1]
["MDA50310060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.5000000000000003E-2,0,0,165545,5794,0,0,165545,5794,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,40188,0,0,0,40188,null,null,null,null,"",1]
["MDA50310130S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.19600000000000001,0,0,204285,40039.800000000003,0,0,204285,40039.800000000003,null,null,"N","N","",1]
["MDA50410010S",null,null,null,"관보온/유리솜보온재","D15, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA50410020S",null,null,null,"관보온/유리솜보온재","D20, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA50410040S","노무","L001010101000044",null,"보온공","일반공사 직종","인",5.8000000000000003E-2,0,0,204285,11848.5,0,0,204285,11848.5,null,null,"N","N","",1]
["MDA50410050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.4000000000000002E-2,0,0,165545,5628.5,0,0,165545,5628.5,null,null,"N","N","",1]
["MDA50410060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.9E-2,0,0,165545,6456.2,0,0,165545,6456.2,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,24317,0,0,0,24317,null,null,null,null,"",1]
["MDA50410090S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.11,0,0,204285,22471.3,0,0,204285,22471.3,null,null,"N","N","",1]
["MDA50410110S",null,null,null,"관보온/유리솜보온재","D150, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,52614,0,0,0,52614,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,63152,0,0,0,63152,null,null,null,null,"",1]
["MDA50510020S",null,null,null,"관보온/유리솜보온재","D20, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA50510030S",null,null,null,"관보온/유리솜보온재","D25, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA50510040S",null,null,null,"관보온/유리솜보온재","D32, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA50510050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.04,0,0,165545,6621.8,0,0,165545,6621.8,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA50510100S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.151,0,0,204285,30847,0,0,204285,30847,null,null,"N","N","",1]
["MDA50510110S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.183,0,0,204285,37384.1,0,0,204285,37384.1,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA50510140S",null,null,null,"관보온/유리솜보온재","D300, 보온두께 50mm 이하, 그루브조인트접합, 옥내일반, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,8037,0,0,0,8037,null,null,null,null,"",1]
["MDA51010030S","노무","L001010101000044",null,"보온공","일반공사 직종","인",3.4000000000000002E-2,0,0,204285,6945.6,0,0,204285,6945.6,null,null,"N","N","",1]
["MDA51010040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.02,0,0,165545,3310.9,0,0,165545,3310.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,16075,0,0,0,16075,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,37521,0,0,0,37521,null,null,null,null,"",1]
["MDA51010130S",null,null,null,"관보온/유리솜보온재","D250, 보온두께 25mm 이하, 그루브조인트접합, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA51010130S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.21,0,0,204285,42899.8,0,0,204285,42899.8,null,null,"N","N","",1]
["MDA51110010S",null,null,null,"관보온/유리솜보온재","D15, 보온두께 25mm 이하, 그루브조인트접합, 기계실, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA51110021S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.02,0,0,165545,3310.9,0,0,165545,3310.9,null,null,"N","N","",1]
["MDA51110022S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.3E-2,0,0,165545,3807.5,0,0,165545,3807.5,null,null,"N","N","",1]
["MDA51110023S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.7E-2,0,0,165545,4469.7,0,0,165545,4469.7,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA51110027S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.1999999999999998E-2,0,0,165545,8608.2999999999993,0,0,165545,8608.2999999999993,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,36947,0,0,0,36947,null,null,null,null,"",1]
["MDA51110030S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.21,0,0,204285,42899.8,0,0,204285,42899.8,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA51210010S",null,null,null,"관보온/유리솜보온재","D15, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA51210020S","노무","L001010101000044",null,"보온공","일반공사 직종","인",4.2999999999999997E-2,0,0,204285,8784.2000000000007,0,0,204285,8784.2000000000007,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA51210050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.3000000000000002E-2,0,0,165545,5462.9,0,0,165545,5462.9,null,null,"N","N","",1]
["MDA51210070S","노무","L001010101000044",null,"보온공","일반공사 직종","인",9.0999999999999998E-2,0,0,204285,18589.900000000001,0,0,204285,18589.900000000001,null,null,"N","N","",1]
["MDA51210080S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.109,0,0,204285,22267,0,0,204285,22267,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,44780,0,0,0,44780,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,72592,0,0,0,72592,null,null,null,null,"",1]
["MDA51210140S",null,null,null,"관보온/유리솜보온재","D300, 보온두께 25mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA51310010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.3E-2,0,0,165545,3807.5,0,0,165545,3807.5,null,null,"N","N","",1]
["MDA51310030S",null,null,null,"관보온/유리솜보온재","D25, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA51310050S",null,null,null,"관보온/유리솜보온재","D40, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA51310070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.4999999999999998E-2,0,0,165545,7449.5,0,0,165545,7449.5,null,null,"N","N","",1]
["MDA51310080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.2999999999999999E-2,0,0,165545,8773.7999999999993,0,0,165545,8773.7999999999993,null,null,"N","N","",1]
["MDA51310100S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.13800000000000001,0,0,204285,28191.3,0,0,204285,28191.3,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA51310130S",null,null,null,"관보온/유리솜보온재","D250, 보온두께 50mm 이하, 그루브조인트접합, 기계실","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,74634,0,0,0,74634,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA51410030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.1E-2,0,0,165545,5131.8,0,0,165545,5131.8,null,null,"N","N","",1]
["MDA51410050S",null,null,null,"관보온/유리솜보온재","D40, 보온두께 50mm 이하, 그루브조인트접합, 기계실, 매직","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA51410060S","노무","L001010101000044",null,"보온공","일반공사 직종","인",9.7000000000000003E-2,0,0,204285,19815.599999999999,0,0,204285,19815.599999999999,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,38835,0,0,0,38835,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,45559,0,0,0,45559,null,null,null,null,"",1]
["MDA51410120S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.23,0,0,204285,46985.5,0,0,204285,46985.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,86117,0,0,0,86117,null,null,null,null,"",1]
["MDA51510010S",null,null,null,"관보온/유리솜보온재","D15, 보온두께 50mm 이하, 그루브조인트접합, 기계실, P.P시트","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA51510020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.5000000000000003E-2,0,0,165545,5794,0,0,165545,5794,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA51510050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.0999999999999997E-2,0,0,165545,8442.7000000000007,0,0,165545,8442.7000000000007,null,null,"N","N","",1]
["MDA51510070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.3E-2,0,0,165545,10429.299999999999,0,0,165545,10429.299999999999,null,null,"N","N","",1]
["MDA51510080S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.14899999999999999,0,0,204285,30438.400000000001,0,0,204285,30438.400000000001,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA51510120S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.14000000000000001,0,0,165545,23176.3,0,0,165545,23176.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,78333,0,0,0,78333,null,null,null,null,"",1]
["MDA51510140S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.36,0,0,204285,73542.600000000006,0,0,204285,73542.600000000006,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA60010020S",null,null,null,"관보온/칼라함석마감"," D20, 보온두께 25mm","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA60010040S","노무","L001010101000044",null,"보온공","일반공사 직종","인",7.0999999999999994E-2,0,0,204285,14504.2,0,0,204285,14504.2,null,null,"N","N","",1]
["MDA60010060S","노무","L001010101000044",null,"보온공","일반공사 직종","인",8.3000000000000004E-2,0,0,204285,16955.599999999999,0,0,204285,16955.599999999999,null,null,"N","N","",1]
["MDA60010060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.2000000000000003E-2,0,0,165545,6952.8,0,0,165545,6952.8,null,null,"N","N","",1]
["MDA60110030S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.13300000000000001,0,0,204285,27169.9,0,0,204285,27169.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,40966,0,0,0,40966,null,null,null,null,"",1]
["MDA60110050S",null,null,null,"관보온/칼라함석마감"," D150, 보온두께 40mm","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDA60210020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.11,0,0,165545,18209.900000000001,0,0,165545,18209.900000000001,null,null,"N","N","",1]
["MDC00010010S",null,null,null,"밸브보온/고무발포보온재","D15, 보온두께 25mm 이하, 일반밸브, 옥내일반","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC00010020S",null,null,null,"밸브보온/고무발포보온재","D20, 보온두께 25mm 이하, 일반밸브, 옥내일반","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC00010050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.5999999999999998E-2,0,0,165545,12581.4,0,0,165545,12581.4,null,null,"N","N","",1]
["MDC00010070S",null,null,null,"밸브보온/고무발포보온재","D65, 보온두께 25mm 이하, 일반밸브, 옥내일반","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC00010080S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.28799999999999998,0,0,204285,58834,0,0,204285,58834,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC00010110S",null,null,null,"밸브보온/고무발포보온재","D150, 보온두께 25mm 이하, 일반밸브, 옥내일반","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,108236,0,0,0,108236,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC00110010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.111,0,0,165545,18375.400000000001,0,0,165545,18375.400000000001,null,null,"N","N","",1]
["MDC00110030S",null,null,null,"밸브보온/고무발포보온재","D25, 보온두께 50mm 이하, 일반밸브, 옥내일반","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,106270,0,0,0,106270,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,122043,0,0,0,122043,null,null,null,null,"",1]
["MDC00110100S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.59199999999999997,0,0,204285,120936.7,0,0,204285,120936.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,165263,0,0,0,165263,null,null,null,null,"",1]
["MDC00110130S",null,null,null,"밸브보온/고무발포보온재","D250, 보온두께 50mm 이하, 일반밸브, 옥내일반","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,200661,0,0,0,200661,null,null,null,null,"",1]
["MDC01010020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.8000000000000005E-2,0,0,165545,11257,0,0,165545,11257,null,null,"N","Y","",0]
["MDC01010030S",null,null,null,"밸브보온/고무발포보온재","D25, 보온두께 25mm 이하, 일반밸브, 기계실","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC01010050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.5999999999999998E-2,0,0,165545,12581.4,0,0,165545,12581.4,null,null,"N","Y","",0]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,75660,0,0,0,75660,null,null,null,null,"",1]
["MDC01010080S",null,null,null,"밸브보온/고무발포보온재","D80, 보온두께 25mm 이하, 일반밸브, 기계실","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC01010090S",null,null,null,"밸브보온/고무발포보온재","D100, 보온두께 25mm 이하, 일반밸브, 기계실","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC01010100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.12,0,0,165545,19865.400000000001,0,0,165545,19865.400000000001,null,null,"N","Y","",0]
["MDC01010120S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.41799999999999998,0,0,204285,85391.1,0,0,204285,85391.1,null,null,"N","Y","",0]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,129883,0,0,0,129883,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,136865,0,0,0,136865,null,null,null,null,"",1]
["MDC01110010S",null,null,null,"밸브보온/고무발포보온재","D15, 보온두께 50mm 이하, 일반밸브, 기계실","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC01110020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.114,0,0,165545,18872.099999999999,0,0,165545,18872.099999999999,null,null,"N","Y","",0]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,115382,0,0,0,115382,null,null,null,null,"",1]
["MDC01110060S",null,null,null,"밸브보온/고무발포보온재","D50, 보온두께 50mm 이하, 일반밸브, 기계실","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC01110080S",null,null,null,"밸브보온/고무발포보온재","D80, 보온두께 50mm 이하, 일반밸브, 기계실","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC01110080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.156,0,0,165545,25825,0,0,165545,25825,null,null,"N","Y","",0]
["MDC01110090S","손료","RENT000000000001",null,"노무할증  20%증","노무비의 120%","식",1,0,0,165133.4,165133.4,0,0,165133.4,165133.4,null,null,"N","N",120,1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,184060,0,0,0,184060,null,null,null,null,"",1]
["MDC01110120S",null,null,null,"밸브보온/고무발포보온재","D200, 보온두께 50mm 이하, 일반밸브, 기계실","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,231453,0,0,0,231453,null,null,null,null,"",1]
["MDC01110140S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.25700000000000001,0,0,165545,42545,0,0,165545,42545,null,null,"N","Y","",0]
["MDC10010020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.8000000000000005E-2,0,0,165545,11257,0,0,165545,11257,null,null,"N","Y","",0]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC10010040S",null,null,null,"밸브보온/고무발포보온재","D32, 보온두께 25mm 이하, 각종부속부착, 옥내일반","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC10010050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.5999999999999998E-2,0,0,165545,12581.4,0,0,165545,12581.4,null,null,"N","Y","",0]
["MDC10010070S","손료","RENT000000000001",null,"노무할증  25%증","노무비의 125%","식",1,0,0,83677.8,83677.8,0,0,83677.8,83677.8,null,null,"N","N",125,1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,83677,0,0,0,83677,null,null,null,null,"",1]
["MDC10010090S","손료","RENT000000000001",null,"노무할증  25%증","노무비의 125%","식",1,0,0,110714.8,110714.8,0,0,110714.8,110714.8,null,null,"N","N",125,1]
["MDC10010110S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.38300000000000001,0,0,204285,78241.100000000006,0,0,204285,78241.100000000006,null,null,"N","Y","",0]
["MDC10010120S",null,null,null,"밸브보온/고무발포보온재","D200, 보온두께 25mm 이하, 각종부속부착, 옥내일반","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,142568,0,0,0,142568,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC10110010S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.33300000000000002,0,0,204285,68026.899999999994,0,0,204285,68026.899999999994,null,null,"N","Y","",0]
["MDC10110030S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.35499999999999998,0,0,204285,72521.100000000006,0,0,204285,72521.100000000006,null,null,"N","Y","",0]
["MDC10110040S",null,null,null,"밸브보온/고무발포보온재","D32, 보온두께 50mm 이하, 각종부속부착, 옥내일반","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC10110050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.129,0,0,165545,21355.3,0,0,165545,21355.3,null,null,"N","Y","",0]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,142568,0,0,0,142568,null,null,null,null,"",1]
["MDC10110090S","손료","RENT000000000001",null,"노무할증  25%증","노무비의 125%","식",1,0,0,172014,172014,0,0,172014,172014,null,null,"N","N",125,1]
["MDC10110100S","손료","RENT000000000001",null,"노무할증  25%증","노무비의 125%","식",1,0,0,191729.3,191729.3,0,0,191729.3,191729.3,null,null,"N","N",125,1]
["MDC10110110S",null,null,null,"밸브보온/고무발포보온재","D150, 보온두께 50mm 이하, 각종부속부착, 옥내일반","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,241097,0,0,0,241097,null,null,null,null,"",1]
["MDC11010010S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.19800000000000001,0,0,204285,40448.400000000001,0,0,204285,40448.400000000001,null,null,"N","Y","",0]
["MDC11010020S","손료","RENT000000000001",null,"노무할증  25%증+20%증","노무비의 145%","식",1,0,0,76750,76750,0,0,76750,76750,null,null,"N","N",145,1]
["MDC11010030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.0000000000000007E-2,0,0,165545,11588.1,0,0,165545,11588.1,null,null,"N","Y","",0]
["MDC11010050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.5999999999999998E-2,0,0,165545,12581.4,0,0,165545,12581.4,null,null,"N","Y","",0]
["MDC11010060S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.24299999999999999,0,0,204285,49641.2,0,0,204285,49641.2,null,null,"N","Y","",0]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC11010080S","손료","RENT000000000001",null,"노무할증  25%증+20%증","노무비의 145%","식",1,0,0,108353.1,108353.1,0,0,108353.1,108353.1,null,null,"N","N",145,1]
["MDC11010090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.113,0,0,165545,18706.5,0,0,165545,18706.5,null,null,"N","Y","",0]
["MDC11010110S",null,null,null,"밸브보온/고무발포보온재","D150, 보온두께 25mm 이하, 각종부속부착, 기계실","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC11010120S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.41799999999999998,0,0,204285,85391.1,0,0,204285,85391.1,null,null,"N","Y","",0]
["MDC11010130S",null,null,null,"밸브보온/고무발포보온재","D250, 보온두께 25mm 이하, 각종부속부착, 기계실","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC11110010S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.33300000000000002,0,0,204285,68026.899999999994,0,0,204285,68026.899999999994,null,null,"N","Y","",0]
["MDC11110010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.111,0,0,165545,18375.400000000001,0,0,165545,18375.400000000001,null,null,"N","Y","",0]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,129261,0,0,0,129261,null,null,null,null,"",1]
["MDC11110040S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.371,0,0,204285,75789.7,0,0,204285,75789.7,null,null,"N","Y","",0]
["MDC11110050S",null,null,null,"밸브보온/고무발포보온재","D40, 보온두께 50mm 이하, 각종부속부착, 기계실","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,176962,0,0,0,176962,null,null,null,null,"",1]
["MDC11110110S",null,null,null,"밸브보온/고무발포보온재","D150, 보온두께 50mm 이하, 각종부속부착, 기계실","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC11110120S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.65300000000000002,0,0,204285,133398.1,0,0,204285,133398.1,null,null,"N","Y","",0]
["MDC11110120S","손료","RENT000000000001",null,"노무할증  25%증+20%증","노무비의 145%","식",1,0,0,245275.9,245275.9,0,0,245275.9,245275.9,null,null,"N","N",145,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC20010020S",null,null,null,"밸브보온/발포폴리에틸렌보온재","D20, 보온두께 25mm 이하, 일반밸브, 옥내일반","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC20010030S",null,null,null,"밸브보온/발포폴리에틸렌보온재","D25, 보온두께 25mm 이하, 일반밸브, 옥내일반","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC20010060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.0999999999999999E-2,0,0,165545,10098.200000000001,0,0,165545,10098.200000000001,null,null,"N","N","",1]
["MDC20010080S",null,null,null,"밸브보온/발포폴리에틸렌보온재","D80, 보온두께 25mm 이하, 일반밸브, 옥내일반","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC20010090S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.25700000000000001,0,0,204285,52501.2,0,0,204285,52501.2,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC20010110S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.28799999999999998,0,0,204285,58834,0,0,204285,58834,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,85828,0,0,0,85828,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC20110020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",8.5999999999999993E-2,0,0,165545,14236.8,0,0,165545,14236.8,null,null,"N","N","",1]
["MDC20110040S",null,null,null,"밸브보온/발포폴리에틸렌보온재","D32, 보온두께 50mm 이하, 일반밸브, 옥내일반","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,85828,0,0,0,85828,null,null,null,null,"",1]
["MDC20110100S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.44500000000000001,0,0,204285,90906.8,0,0,204285,90906.8,null,null,"N","N","",1]
["MDC20110110S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.47899999999999998,0,0,204285,97852.5,0,0,204285,97852.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,127287,0,0,0,127287,null,null,null,null,"",1]
["MDC20110140S",null,null,null,"밸브보온/발포폴리에틸렌보온재","D300, 보온두께 50mm 이하, 일반밸브, 옥내일반","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC21010010S","손료","RENT000000000001",null,"노무할증  20%증","노무비의 120%","식",1,0,0,46260.1,46260.1,0,0,46260.1,46260.1,null,null,"N","N",120,1]
["MDC21010030S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.158,0,0,204285,32277,0,0,204285,32277,null,null,"N","Y","",0]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,51374,0,0,0,51374,null,null,null,null,"",1]
["MDC21010060S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.183,0,0,204285,37384.1,0,0,204285,37384.1,null,null,"N","Y","",0]
["MDC21010070S","손료","RENT000000000001",null,"노무할증  20%증","노무비의 120%","식",1,0,0,60271.199999999997,60271.199999999997,0,0,60271.199999999997,60271.199999999997,null,null,"N","N",120,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC21010110S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.28799999999999998,0,0,204285,58834,0,0,204285,58834,null,null,"N","Y","",0]
["MDC21010130S",null,null,null,"밸브보온/발포폴리에틸렌보온재","D250, 보온두께 25mm 이하, 일반밸브, 기계실","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC21010130S","손료","RENT000000000001",null,"노무할증  20%증","노무비의 120%","식",1,0,0,102993.8,102993.8,0,0,102993.8,102993.8,null,null,"N","N",120,1]
["MDC21010140S","손료","RENT000000000001",null,"노무할증  20%증","노무비의 120%","식",1,0,0,120741.3,120741.3,0,0,120741.3,120741.3,null,null,"N","N",120,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC21110030S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.26700000000000002,0,0,204285,54544,0,0,204285,54544,null,null,"N","Y","",0]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,86670,0,0,0,86670,null,null,null,null,"",1]
["MDC21110050S","손료","RENT000000000001",null,"노무할증  20%증","노무비의 120%","식",1,0,0,90850.8,90850.8,0,0,90850.8,90850.8,null,null,"N","N",120,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC21110090S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.4,0,0,204285,81714,0,0,204285,81714,null,null,"N","Y","",0]
["MDC21110100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.14799999999999999,0,0,165545,24500.6,0,0,165545,24500.6,null,null,"N","Y","",0]
["MDC21110110S","손료","RENT000000000001",null,"노무할증  20%증","노무비의 120%","식",1,0,0,149008.9,149008.9,0,0,149008.9,149008.9,null,null,"N","N",120,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC21110140S","손료","RENT000000000001",null,"노무할증  20%증","노무비의 120%","식",1,0,0,181012.6,181012.6,0,0,181012.6,181012.6,null,null,"N","N",120,1]
["MDC30010010S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.14899999999999999,0,0,204285,30438.400000000001,0,0,204285,30438.400000000001,null,null,"N","Y","",0]
["MDC30010020S","손료","RENT000000000001",null,"노무할증  25%증","노무비의 125%","식",1,0,0,49622.8,49622.8,0,0,49622.8,49622.8,null,null,"N","N",125,1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,53514,0,0,0,53514,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC30010060S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.183,0,0,204285,37384.1,0,0,204285,37384.1,null,null,"N","Y","",0]
["MDC30010080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.1999999999999995E-2,0,0,165545,11919.2,0,0,165545,11919.2,null,null,"N","Y","",0]
["MDC30010080S","손료","RENT000000000001",null,"노무할증  25%증","노무비의 125%","식",1,0,0,70311.199999999997,70311.199999999997,0,0,70311.199999999997,70311.199999999997,null,null,"N","N",125,1]
["MDC30010100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.09,0,0,165545,14899,0,0,165545,14899,null,null,"N","Y","",0]
["MDC30010120S",null,null,null,"밸브보온/발포폴리에틸렌보온재","D200, 보온두께 25mm 이하, 각종부속부착, 옥내일반","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC30010120S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.314,0,0,204285,64145.4,0,0,204285,64145.4,null,null,"N","Y","",0]
["MDC30010140S","손료","RENT000000000001",null,"노무할증  25%증","노무비의 125%","식",1,0,0,125772.2,125772.2,0,0,125772.2,125772.2,null,null,"N","N",125,1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,81269,0,0,0,81269,null,null,null,null,"",1]
["MDC30110020S",null,null,null,"밸브보온/발포폴리에틸렌보온재","D20, 보온두께 50mm 이하, 각종부속부착, 옥내일반","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC30110040S",null,null,null,"밸브보온/발포폴리에틸렌보온재","D32, 보온두께 50mm 이하, 각종부속부착, 옥내일반","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC30110050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",9.7000000000000003E-2,0,0,165545,16057.8,0,0,165545,16057.8,null,null,"N","Y","",0]
["MDC30110060S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.308,0,0,204285,62919.7,0,0,204285,62919.7,null,null,"N","Y","",0]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,107285,0,0,0,107285,null,null,null,null,"",1]
["MDC30110090S",null,null,null,"밸브보온/발포폴리에틸렌보온재","D100, 보온두께 50mm 이하, 각종부속부착, 옥내일반","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC30110100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.14799999999999999,0,0,165545,24500.6,0,0,165545,24500.6,null,null,"N","Y","",0]
["MDC30110110S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.159,0,0,165545,26321.599999999999,0,0,165545,26321.599999999999,null,null,"N","Y","",0]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,181026,0,0,0,181026,null,null,null,null,"",1]
["MDC31010010S",null,null,null,"밸브보온/발포폴리에틸렌보온재","D15, 보온두께 25mm 이하, 각종부속부착, 기계실","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC31010020S",null,null,null,"밸브보온/발포폴리에틸렌보온재","D20, 보온두께 25mm 이하, 각종부속부착, 기계실","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC31010030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.1999999999999998E-2,0,0,165545,8608.2999999999993,0,0,165545,8608.2999999999993,null,null,"N","Y","",0]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,62077,0,0,0,62077,null,null,null,null,"",1]
["MDC31010060S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.183,0,0,204285,37384.1,0,0,204285,37384.1,null,null,"N","Y","",0]
["MDC31010070S",null,null,null,"밸브보온/발포폴리에틸렌보온재","D65, 보온두께 25mm 이하, 각종부속부착, 기계실","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,72827,0,0,0,72827,null,null,null,null,"",1]
["MDC31010090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",8.5000000000000006E-2,0,0,165545,14071.3,0,0,165545,14071.3,null,null,"N","Y","",0]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,101877,0,0,0,101877,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC31010130S",null,null,null,"밸브보온/발포폴리에틸렌보온재","D250, 보온두께 25mm 이하, 각종부속부착, 기계실","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC31010140S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.129,0,0,165545,21355.3,0,0,165545,21355.3,null,null,"N","Y","",0]
["MDC31110020S",null,null,null,"밸브보온/발포폴리에틸렌보온재","D20, 보온두께 50mm 이하, 각종부속부착, 기계실","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,97362,0,0,0,97362,null,null,null,null,"",1]
["MDC31110030S","손료","RENT000000000001",null,"노무할증  25%증+20%증","노무비의 145%","식",1,0,0,100452.3,100452.3,0,0,100452.3,100452.3,null,null,"N","N",145,1]
["MDC31110050S",null,null,null,"밸브보온/발포폴리에틸렌보온재","D40, 보온두께 50mm 이하, 각종부속부착, 기계실","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC31110060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.10199999999999999,0,0,165545,16885.5,0,0,165545,16885.5,null,null,"N","Y","",0]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,124450,0,0,0,124450,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,132943,0,0,0,132943,null,null,null,null,"",1]
["MDC31110100S",null,null,null,"밸브보온/발포폴리에틸렌보온재","D125, 보온두께 50mm 이하, 각종부속부착, 기계실","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC31110120S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.16300000000000001,0,0,165545,26983.8,0,0,165545,26983.8,null,null,"N","Y","",0]
["MDC31110130S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.185,0,0,165545,30625.8,0,0,165545,30625.8,null,null,"N","Y","",0]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,218723,0,0,0,218723,null,null,null,null,"",1]
["MDC40010020S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.23100000000000001,0,0,204285,47189.8,0,0,204285,47189.8,null,null,"N","N","",1]
["MDC40010040S",null,null,null,"밸브보온/함석마감","D100","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC40010050S",null,null,null,"밸브보온/함석마감","D125","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,85187,0,0,0,85187,null,null,null,null,"",1]
["MDC40010090S",null,null,null,"밸브보온/함석마감","D300","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDC40010090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",9.7000000000000003E-2,0,0,165545,16057.8,0,0,165545,16057.8,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDE00110010S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.24,0,0,204285,49028.4,0,0,204285,49028.4,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,82418,0,0,0,82418,null,null,null,null,"",1]
["MDE10110010S",null,null,null,"원형덕트보온/고무발포보온재","보온두께 50mm 이하","㎡",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MDE11110010S",null,null,null,"원형덕트보온/발포폴리에틸렌","보온두께 50mm 이하","㎡",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,72592,0,0,0,72592,null,null,null,null,"",1]
["MDG00110010S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",1.7000000000000001E-2,0,0,233722,3973.2,0,0,233722,3973.2,null,null,"N","N","",1]
["MDG00110010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.0000000000000001E-3,0,0,165545,993.2,0,0,165545,993.2,null,null,"N","N","",1]
["MEA00010010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,6632.3,6632.3,0,0,0,0,6632.3,6632.3,null,null,"N","N",3,1]
["MEA00010030S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",0.97699999999999998,0,0,233722,228346.3,0,0,233722,228346.3,null,null,"N","N","",1]
["MEA00010040S",null,null,null,"일반펌프 설치","3.7 kw 이하","대",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,11704,0,390156,0,0,0,401860,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MEA00010070S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",2.1440000000000001,0,0,233722,501099.9,0,0,233722,501099.9,null,null,"N","N","",1]
["MEA00010090S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",3.677,0,0,233722,859395.7,0,0,233722,859395.7,null,null,"N","N","",1]
["MEA00010100S",null,null,null,"일반펌프 설치","37 kw 이하","대",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MEA00010110S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5299999999999998,0,0,165545,418828.79999999999,0,0,165545,418828.79999999999,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,11629,0,387653,0,0,0,399282,null,null,null,null,"",1]
["MEA10010030S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,14569.5,14569.5,0,0,0,0,14569.5,14569.5,null,null,"N","N",3,1]
["MEA10010040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,17599.3,17599.3,0,0,0,0,17599.3,17599.3,null,null,"N","N",3,1]
["MEA10010050S",null,null,null,"배수펌프 설치","5.5 kw 이하","대",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,204855,0,0,0,204855,null,null,null,null,"",1]
["MEA20010050S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",0.83,0,0,233722,193989.2,0,0,233722,193989.2,null,null,"N","N","",1]
["MEA20010060S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",0.89100000000000001,0,0,233722,208246.3,0,0,233722,208246.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,292597,0,0,0,292597,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,386475,0,0,0,386475,null,null,null,null,"",1]
["MEA20010100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.499,0,0,165545,82606.899999999994,0,0,165545,82606.899999999994,null,null,"N","N","",1]
["MEA20010120S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.75800000000000001,0,0,165545,125483.1,0,0,165545,125483.1,null,null,"N","N","",1]
["MEB00010010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.309,0,0,165545,51153.4,0,0,165545,51153.4,null,null,"N","N","",1]
["MEB00010030S",null,null,null,"송풍기 설치","호칭번호 040(#2⅔), 편흡입","대",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MEB00010040S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",1.3129999999999999,0,0,233722,306876.90000000002,0,0,233722,306876.90000000002,null,null,"N","N","",1]
["MEB00010050S",null,null,null,"송풍기 설치","호칭번호 050(#3⅓), 편흡입","대",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MEB00010070S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",1.843,0,0,233722,430749.6,0,0,233722,430749.6,null,null,"N","N","",1]
["MEB00010070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.54700000000000004,0,0,165545,90553.1,0,0,165545,90553.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,18177,0,605919,0,0,0,624096,null,null,null,null,"",1]
["MEB00010100S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",3.0139999999999998,0,0,233722,704438.1,0,0,233722,704438.1,null,null,"N","N","",1]
["MEB00010110S",null,null,null,"송풍기 설치","호칭번호 100(#6⅔), 편흡입","대",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,57371,0,1912375,0,0,0,1969746,null,null,null,null,"",1]
["MEB00010160S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",7.6820000000000004,0,0,233722,1795452.4,0,0,233722,1795452.4,null,null,"N","N","",1]
["MEB00110020S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",1.4690000000000001,0,0,233722,343337.6,0,0,233722,343337.6,null,null,"N","N","",1]
["MEB00110020S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,12465.4,12465.4,0,0,0,0,12465.4,12465.4,null,null,"N","N",3,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,18092,0,603085,0,0,0,621177,null,null,null,null,"",1]
["MEB00110080S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",2.83,0,0,233722,661433.19999999995,0,0,233722,661433.19999999995,null,null,"N","N","",1]
["MEB00110090S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,28326.5,28326.5,0,0,0,0,28326.5,28326.5,null,null,"N","N",3,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MEB00110120S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.639,0,0,165545,271328.2,0,0,165545,271328.2,null,null,"N","N","",1]
["MEB00110130S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,51647.1,51647.1,0,0,0,0,51647.1,51647.1,null,null,"N","N",3,1]
["MEB00110150S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,75810.8,75810.8,0,0,0,0,75810.8,75810.8,null,null,"N","N",3,1]
["MEB00110160S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,86136.9,86136.9,0,0,0,0,86136.9,86136.9,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,8840,0,500975,0,0,0,509815,null,null,null,null,"",1]
["MEB01010030S",null,null,null,"송풍기 설치","호칭번호 040(#2⅔), 편흡입, 천장행거형","대",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MEB01010040S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",1.3129999999999999,0,0,233722,306876.90000000002,0,0,233722,306876.90000000002,null,null,"N","Y","",0]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MEB01010050S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,12222.3,12222.3,0,0,0,0,12222.3,12222.3,null,null,"N","N",3,1]
["MEB01010070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.54700000000000004,0,0,165545,90553.1,0,0,165545,90553.1,null,null,"N","Y","",0]
["MEB01010080S",null,null,null,"송풍기 설치","호칭번호 071(#4⅔), 편흡입, 천장행거형","대",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MEB01010090S",null,null,null,"송풍기 설치","호칭번호 080(#5⅓), 편흡입, 천장행거형","대",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MEB01010100S",null,null,null,"송풍기 설치","호칭번호 090(#6), 편흡입, 천장행거형","대",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MEB01010110S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,30255.9,30255.9,0,0,0,0,30255.9,30255.9,null,null,"N","N",3,1]
["MEB01010120S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,35445.9,35445.9,0,0,0,0,35445.9,35445.9,null,null,"N","N",3,1]
["MEB01010130S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",4.6059999999999999,0,0,233722,1076523.5,0,0,233722,1076523.5,null,null,"N","Y","",0]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MEB01010150S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",6.76,0,0,233722,1579960.7,0,0,233722,1579960.7,null,null,"N","Y","",0]
["MEB01010160S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.2810000000000001,0,0,165545,377608.1,0,0,165545,377608.1,null,null,"N","Y","",0]
["MEB01110010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,11686.2,11686.2,0,0,0,0,11686.2,11686.2,null,null,"N","N",3,1]
["MEB01110020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.436,0,0,165545,72177.600000000006,0,0,165545,72177.600000000006,null,null,"N","Y","",0]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,14722,0,834297,0,0,0,849019,null,null,null,null,"",1]
["MEB01110050S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,16149.1,16149.1,0,0,0,0,16149.1,16149.1,null,null,"N","N",3,1]
["MEB01110060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.63300000000000001,0,0,165545,104789.9,0,0,165545,104789.9,null,null,"N","Y","",0]
["MEB01110070S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,20664,20664,0,0,0,0,20664,20664,null,null,"N","N",3,1]
["MEB01110080S","손료","RENT000000000003",null,"노무할증 70%증","노무비의 170%","식",1,0,0,1360834.7,1360834.7,0,0,1360834.7,1360834.7,null,null,"N","N",170,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MEB01110100S","손료","RENT000000000003",null,"노무할증 70%증","노무비의 170%","식",1,0,0,1915085.1,1915085.1,0,0,1915085.1,1915085.1,null,null,"N","N",170,1]
["MEB01110120S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.639,0,0,165545,271328.2,0,0,165545,271328.2,null,null,"N","Y","",0]
["MEB01110130S",null,null,null,"송풍기 설치","호칭번호 125(#8⅓), 양흡입, 천장행거형","대",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,51647,0,2926672,0,0,0,2978319,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,57914,0,3281813,0,0,0,3339727,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,75810,0,4295949,0,0,0,4371759,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MEB10010030S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",0.5,0,0,233722,116861,0,0,233722,116861,null,null,"N","N","",1]
["MEB10010040S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",0.8,0,0,233722,186977.6,0,0,233722,186977.6,null,null,"N","N","",1]
["MEB30010010S",null,null,null,"무덕트 유인팬 설치","풍량 1,600㎥/h 이하","대",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,87624,0,0,0,87624,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MEB40010020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.5999999999999999E-2,0,0,165545,7615,0,0,165545,7615,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,339,0,16981,0,0,0,17320,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,921,0,46097,0,0,0,47018,null,null,null,null,"",1]
["MFA00010060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.121,0,0,165545,20030.900000000001,0,0,165545,20030.900000000001,null,null,"N","N","",1]
["MFA00010070S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,2060.9,2060.9,0,0,0,0,2060.9,2060.9,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,2784,0,139208,0,0,0,141992,null,null,null,null,"",1]
["MFA00010100S",null,null,null,"일반밸브 및 콕류 설치","D300","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MFA00010100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.26100000000000001,0,0,165545,43207.199999999997,0,0,165545,43207.199999999997,null,null,"N","N","",1]
["MFA10010020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.29499999999999998,0,0,165545,48835.7,0,0,165545,48835.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,14720,0,736041,0,0,0,750761,null,null,null,null,"",1]
["MFA10010040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,17531.5,17531.5,0,0,0,0,17531.5,17531.5,null,null,"N","N",2,1]
["MFA10010060S",null,null,null,"감압밸브장치 설치","D50","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MFA10010070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.0469999999999999,0,0,165545,173325.6,0,0,165545,173325.6,null,null,"N","N","",1]
["MFA10010080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.2969999999999999,0,0,165545,214711.8,0,0,165545,214711.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,38537,0,1926863,0,0,0,1965400,null,null,null,null,"",1]
["MFA10010100S","노무","L001010101000039",null,"배관공","일반공사 직종","인",8.4649999999999999,0,0,229482,1942565.1,0,0,229482,1942565.1,null,null,"N","N","",1]
["MFA10010120S",null,null,null,"감압밸브장치 설치","D200","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MFB00010010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.23499999999999999,0,0,165545,38903,0,0,165545,38903,null,null,"N","N","",1]
["MFB00010020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.31900000000000001,0,0,165545,52808.800000000003,0,0,165545,52808.800000000003,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,6292,0,314619,0,0,0,320911,null,null,null,null,"",1]
["MFB00010050S","노무","L001010101000039",null,"배관공","일반공사 직종","인",1.756,0,0,229482,402970.3,0,0,229482,402970.3,null,null,"N","N","",1]
["MFB00010060S",null,null,null,"스팀트랩 장치 설치","D50","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MFC00010010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.14199999999999999,0,0,165545,23507.3,0,0,165545,23507.3,null,null,"N","N","",1]
["MFC00010020S",null,null,null,"익스팬션조인트","D32, 복식","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,2914,0,145725,0,0,0,148639,null,null,null,null,"",1]
["MFC00010050S",null,null,null,"익스팬션조인트","D65, 복식","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MFC00010060S","노무","L001010101000039",null,"배관공","일반공사 직종","인",1.119,0,0,229482,256790.3,0,0,229482,256790.3,null,null,"N","N","",1]
["MFC00010070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.57699999999999996,0,0,165545,95519.4,0,0,165545,95519.4,null,null,"N","N","",1]
["MFC00010090S",null,null,null,"익스팬션조인트","D150, 복식","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,14314,0,715719,0,0,0,730033,null,null,null,null,"",1]
["MFC00110010S",null,null,null,"익스팬션조인트","D20∼25, 단식","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MFC00110030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.20899999999999999,0,0,165545,34598.9,0,0,165545,34598.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,3350,0,167548,0,0,0,170898,null,null,null,null,"",1]
["MFC00110060S",null,null,null,"익스팬션조인트","D80, 단식","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MFC00110070S",null,null,null,"익스팬션조인트","D100, 단식","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MFC00110090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.72299999999999998,0,0,165545,119689,0,0,165545,119689,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,17967,0,898392,0,0,0,916359,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,238,0,11940,0,0,0,12178,null,null,null,null,"",1]
["MFC10010030S",null,null,null,"플랙시블커넥터 설치","D65","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MFC10010040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.114,0,0,165545,18872.099999999999,0,0,165545,18872.099999999999,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,3209,0,160460,0,0,0,163669,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,5485,0,274285,0,0,0,279770,null,null,null,null,"",1]
["MFC10010090S",null,null,null,"플랙시블커넥터 설치","D250","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MFC10010100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.46100000000000002,0,0,165545,76316.2,0,0,165545,76316.2,null,null,"N","N","",1]
["MFD00010010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,128.5,128.5,0,0,0,0,128.5,128.5,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,257,0,12850,0,0,0,13107,null,null,null,null,"",1]
["MFD00010040S",null,null,null,"수격방지기","D80","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,773,0,38659,0,0,0,39432,null,null,null,null,"",1]
["MFD00010060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.06,0,0,165545,9932.7000000000007,0,0,165545,9932.7000000000007,null,null,"N","N","",1]
["MFD00010080S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,1797.9,1797.9,0,0,0,0,1797.9,1797.9,null,null,"N","N",2,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MGA00010020S",null,null,null,"직독식 유량계 설치","D20∼32","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MGA00010030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.14299999999999999,0,0,165545,23672.9,0,0,165545,23672.9,null,null,"N","N","",1]
["MGA00010050S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 1%","식",1,2105.4,2105.4,0,0,0,0,2105.4,2105.4,null,null,"N","N",1,1]
[null,null,null,null,"[합 계]",null,null,0,0,2105,0,210549,0,0,0,212654,null,null,null,null,"",1]
["MGA00110010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 1%","식",1,584.6,584.6,0,0,0,0,584.6,584.6,null,null,"N","N",1,1]
["MGA00110030S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.253,0,0,229482,58058.9,0,0,229482,58058.9,null,null,"N","N","",1]
["MGA10010010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.112,0,0,165545,18541,0,0,165545,18541,null,null,"N","N","",1]
["MGA10010020S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 1%","식",1,521.4,521.4,0,0,0,0,521.4,521.4,null,null,"N","N",1,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MGB00010020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.14199999999999999,0,0,229482,32586.400000000001,0,0,229482,32586.400000000001,null,null,"N","N","",1]
["MGB10010020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.47799999999999998,0,0,229482,109692.3,0,0,229482,109692.3,null,null,"N","N","",1]
["MGB10010030S",null,null,null,"적산열량계 건물용","D80","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MGB10010040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.52100000000000002,0,0,165545,86248.9,0,0,165545,86248.9,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MGB20010020S",null,null,null,"적산열량계 산업용","D50","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MGB20010040S",null,null,null,"적산열량계 산업용","D150","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MGB20010040S","노무","L001010101000084",null,"계장공","일반공사 직종","인",0.95,0,0,302065,286961.7,0,0,302065,286961.7,null,null,"N","N","",1]
["MHA00010020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.253,0,0,165545,41882.800000000003,0,0,165545,41882.800000000003,null,null,"N","N","",1]
["MHA00010030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.24099999999999999,0,0,165545,39896.300000000003,0,0,165545,39896.300000000003,null,null,"N","N","",1]
["MHA00010050S","노무","L001010101000042",null,"위생공","일반공사 직종","인",0.90700000000000003,0,0,213253,193420.4,0,0,213253,193420.4,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,250870,0,0,0,250870,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,157822,0,0,0,157822,null,null,null,null,"",1]
["MHA10010030S","노무","L001010101000042",null,"위생공","일반공사 직종","인",0.66900000000000004,0,0,213253,142666.20000000001,0,0,213253,142666.20000000001,null,null,"N","N","",1]
["MHA20010010S",null,null,null,"도기세면기 설치","벽붙임 도기세면기","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MHA40010010S",null,null,null,"카운터형세면기 설치","카운터분리형","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MHA50010010S",null,null,null,"욕조 설치","욕조","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MHB00010010S",null,null,null,"매립형 욕조수전 설치","욕조혼합수전","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MHB10010010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.7999999999999999E-2,0,0,165545,2979.8,0,0,165545,2979.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,15140,0,0,0,15140,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,21112,0,0,0,21112,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,34277,0,0,0,34277,null,null,null,null,"",1]
["MHB30010010S",null,null,null,"씽크수전 설치","대붙임 혼합수전","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,14957,0,0,0,14957,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MHC10010010S",null,null,null,"욕실금구류 설치","수건걸이, BAR형","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,31987,0,0,0,31987,null,null,null,null,"",1]
["MHC20010010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.9E-2,0,0,165545,6456.2,0,0,165545,6456.2,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MHC20010030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.5E-2,0,0,165545,9104.9,0,0,165545,9104.9,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,1055638,0,0,0,1055638,null,null,null,null,"",1]
["MIA00010030S","노무","L001010101000006",null,"비계공","일반공사 직종","인",5,0,0,280472,1402360,0,0,280472,1402360,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,2045026,0,0,0,2045026,null,null,null,null,"",1]
["MIA00010060S",null,null,null,"냉동기 반입 ","지하1층 1회, 냉동U.S. 100톤","식",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,5211940,0,0,0,5211940,null,null,null,null,"",1]
["MIA00010080S",null,null,null,"냉동기 반입 ","지하1층 1회, 냉동U.S. 200톤","식",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MIA00010100S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",30,0,0,214222,6426660,0,0,214222,6426660,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,25397200,0,0,0,25397200,null,null,null,null,"",1]
["MIA01010010S","노무","L001010101000006",null,"비계공","일반공사 직종","인",3,0,0,280472,841416,0,0,280472,841416,null,null,"N","N","",1]
["MIA01010030S",null,null,null,"냉동기 반입 ","지하2층 1회, 냉동U.S. 30톤","식",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,2820192,0,0,0,2820192,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,4865218,0,0,0,4865218,null,null,null,null,"",1]
["MIA01010060S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",8,0,0,214222,1713776,0,0,214222,1713776,null,null,"N","N","",1]
["MIA01010090S",null,null,null,"냉동기 반입 ","지하2층 1회, 냉동U.S. 300톤","식",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MIA01010100S",null,null,null,"냉동기 반입 ","지하2층 1회, 냉동U.S. 400톤","식",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MIA01010110S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",50,0,0,214222,10711100,0,0,214222,10711100,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MIA01110040S","노무","L001010101000006",null,"비계공","일반공사 직종","인",14,0,0,280472,3926608,0,0,280472,3926608,null,null,"N","N","",1]
["MIA01110050S","노무","L001010101000006",null,"비계공","일반공사 직종","인",23,0,0,280472,6450856,0,0,280472,6450856,null,null,"N","N","",1]
["MIA01110060S","노무","L001010101000006",null,"비계공","일반공사 직종","인",30,0,0,280472,8414160,0,0,280472,8414160,null,null,"N","N","",1]
["MIA01110080S",null,null,null,"냉동기 반입 ","지하2층 2회, 냉동U.S. 200톤","식",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,31006640,0,0,0,31006640,null,null,null,null,"",1]
["MIA01110110S","노무","L001010101000006",null,"비계공","일반공사 직종","인",120,0,0,280472,33656640,0,0,280472,33656640,null,null,"N","N","",1]
["MIA01110120S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",100,0,0,214222,21422200,0,0,214222,21422200,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,2045026,0,0,0,2045026,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MIA02010060S",null,null,null,"냉동기 반입 ","지하3층 1회, 냉동U.S. 100톤","식",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,11693740,0,0,0,11693740,null,null,null,null,"",1]
["MIA02010090S","노무","L001010101000006",null,"비계공","일반공사 직종","인",56,0,0,280472,15706432,0,0,280472,15706432,null,null,"N","N","",1]
["MIA02010110S",null,null,null,"냉동기 반입 ","지하3층 1회, 냉동U.S. 500톤","식",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MIA02010120S",null,null,null,"냉동기 반입 ","지하3층 1회, 냉동U.S. 600톤","식",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MIA02110020S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",4,0,0,214222,856888,0,0,214222,856888,null,null,"N","N","",1]
["MIA02110030S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",7,0,0,214222,1499554,0,0,214222,1499554,null,null,"N","N","",1]
["MIA02110040S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",8,0,0,214222,1713776,0,0,214222,1713776,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MIA02110070S","노무","L001010101000006",null,"비계공","일반공사 직종","인",57,0,0,280472,15986904,0,0,280472,15986904,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,60688280,0,0,0,60688280,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,560944,0,0,0,560944,null,null,null,null,"",1]
["MIA03010040S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",1,0,0,214222,214222,0,0,214222,214222,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,775166,0,0,0,775166,null,null,null,null,"",1]
["MIA03010060S","노무","L001010101000006",null,"비계공","일반공사 직종","인",4,0,0,280472,1121888,0,0,280472,1121888,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MIA03010090S",null,null,null,"냉동기 소운반","10m 거리내, 냉동U.S. 300톤","식",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MIA03010110S","노무","L001010101000006",null,"비계공","일반공사 직종","인",20,0,0,280472,5609440,0,0,280472,5609440,null,null,"N","N","",1]
["MIA03110010S","노무","L001010101000006",null,"비계공","일반공사 직종","인",2,0,0,280472,560944,0,0,280472,560944,null,null,"N","N","",1]
["MIA03110030S",null,null,null,"냉동기 가조립 ","설치기초상, 냉동U.S. 30톤","식",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MIA03110040S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",2,0,0,214222,428444,0,0,214222,428444,null,null,"N","N","",1]
["MIA03110060S",null,null,null,"냉동기 가조립 ","설치기초상, 냉동U.S. 100톤","식",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MIA03110060S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",4,0,0,214222,856888,0,0,214222,856888,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MIA03110100S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",14,0,0,214222,2999108,0,0,214222,2999108,null,null,"N","N","",1]
["MIA03110110S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",20,0,0,214222,4284440,0,0,214222,4284440,null,null,"N","N","",1]
["MIA10010010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",2.19,0,0,229482,502565.5,0,0,229482,502565.5,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MIA10010040S",null,null,null,"냉동기 설치","왕복동식냉동기 20 냉동톤","대",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,1575418,0,0,0,1575418,null,null,null,null,"",1]
["MIA10010060S","노무","L001010101000039",null,"배관공","일반공사 직종","인",5.91,0,0,229482,1356238.6,0,0,229482,1356238.6,null,null,"N","N","",1]
["MID00010010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.6,0,0,165545,99327,0,0,165545,99327,null,null,"N","N","",1]
["MID00010030S",null,null,null,"공기가열기, 공기냉각기, 공기여과기 설치","유효길이 914㎜","대",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MID00010040S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",3.5,0,0,233722,818027,0,0,233722,818027,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,1416927,0,0,0,1416927,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,1550343,0,0,0,1550343,null,null,null,null,"",1]
["MID00010100S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",6.5,0,0,233722,1519193,0,0,233722,1519193,null,null,"N","N","",1]
["MID00010110S",null,null,null,"공기가열기, 공기냉각기, 공기여과기 설치","유효길이 2,134㎜","대",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MID00010130S",null,null,null,"공기가열기, 공기냉각기, 공기여과기 설치","유효길이 2,438㎜","대",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,2400499,0,0,0,2400499,null,null,null,null,"",1]
["MID00010160S",null,null,null,"공기가열기, 공기냉각기, 공기여과기 설치","유효길이 3,048㎜","대",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MID20010010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.5,0,0,165545,82772.5,0,0,165545,82772.5,null,null,"N","N","",1]
["MID20010030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1,0,0,165545,165545,0,0,165545,165545,null,null,"N","N","",1]
["MID20010040S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",1.3,0,0,233722,303838.59999999998,0,0,233722,303838.59999999998,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,1397434,0,0,0,1397434,null,null,null,null,"",1]
["MID20110020S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",1.3,0,0,233722,303838.59999999998,0,0,233722,303838.59999999998,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MID20210020S",null,null,null,"공조기(A.H.U)","15㎾이하, 핸들링 유닛","대",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MID20310010S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",1,0,0,233722,233722,0,0,233722,233722,null,null,"N","N","",1]
["MID20310020S",null,null,null,"공조기(A.H.U)","팬코일유닛(상치형) 풍량 680㎥/hr 이상","대",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,433355,0,0,0,433355,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MID20510020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.5,0,0,165545,82772.5,0,0,165545,82772.5,null,null,"N","N","",1]
["MID30010010S",null,null,null,"천장형 에어컨 설치 ","실내기, 냉방능력 16kW 이하","대",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MID30110010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,6329.8,6329.8,0,0,0,0,6329.8,6329.8,null,null,"N","N",2,1]
["MID30110020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.67,0,0,165545,110915.1,0,0,165545,110915.1,null,null,"N","N","",1]
["MID40010020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.16,0,0,165545,26487.200000000001,0,0,165545,26487.200000000001,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,1838,0,91929,0,0,0,93767,null,null,null,null,"",1]
["MIE00010010S",null,null,null,"보일러 설치","주철제, 1호(20∼60 미만) 1,000Kcal/hr","절",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MIE00010020S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.3,0,0,214222,64266.6,0,0,214222,64266.6,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MIE00010050S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.7,0,0,214222,149955.4,0,0,214222,149955.4,null,null,"N","N","",1]
["MIE00110010S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.8,0,0,214222,171377.6,0,0,214222,171377.6,null,null,"N","N","",1]
["MIE00210010S","노무","L001010101000041",null,"보일러공","일반공사 직종","인",6,0,0,220312,1321872,0,0,220312,1321872,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MIE20010030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.19900000000000001,0,0,165545,32943.4,0,0,165545,32943.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,259424,0,0,0,259424,null,null,null,null,"",1]
["MIE20010050S","노무","L001010101000041",null,"보일러공","일반공사 직종","인",1.218,0,0,220312,268340,0,0,220312,268340,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,756250,0,0,0,756250,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,1178103,0,0,0,1178103,null,null,null,null,"",1]
["MIE50010010S",null,null,null,"방열기 설치","주철제 바닥설치 20절 이하","조",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MIE50010020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.1,0,0,165545,16554.5,0,0,165545,16554.5,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MIE50010050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.1,0,0,165545,16554.5,0,0,165545,16554.5,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MIE50210010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",1.9,0,0,229482,436015.8,0,0,229482,436015.8,null,null,"N","N","",1]
["MIE50210020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",2.4,0,0,229482,550756.80000000005,0,0,229482,550756.80000000005,null,null,"N","N","",1]
["MIE50310020S",null,null,null,"방열기 설치","강판제/알루미늄제 방열기 1m 이상","조",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,631,0,21034,0,0,0,21665,null,null,null,null,"",1]
["MIF10010010S","노무","L001010101000041",null,"보일러공","일반공사 직종","인",0.17,0,0,220312,37453,0,0,220312,37453,null,null,"N","N","",1]
["MIF10010020S","노무","L001010101000041",null,"보일러공","일반공사 직종","인",0.18,0,0,220312,39656.1,0,0,220312,39656.1,null,null,"N","N","",1]
["MIF10010030S","손료","RENT000000000001",null,"공구손료","노무비의 2%","식",1,1311.4,1311.4,0,0,0,0,1311.4,1311.4,null,null,"N","N",2,1]
["MIF20010010S",null,null,null,"온수분배기 설치","공급 및 환수 헤더, 2구","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MIF20010050S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.47099999999999997,0,0,229482,108086,0,0,229482,108086,null,null,"N","N","",1]
["MIF20010060S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,3113.6,3113.6,0,0,0,0,3113.6,3113.6,null,null,"N","N",2,1]
["MJA00010020S",null,null,null,"입상관 방진가대 설치","D65","조",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MJA00010040S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.125,0,0,229482,28685.200000000001,0,0,229482,28685.200000000001,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MJA00010060S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,2085.3000000000002,2085.3000000000002,0,0,0,0,2085.3000000000002,2085.3000000000002,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,2323,0,77454,0,0,0,79777,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MJA00010100S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.28100000000000003,0,0,229482,64484.4,0,0,229482,64484.4,null,null,"N","N","",1]
["MJA10010010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 5%","식",1,59853.8,59853.8,0,0,0,0,59853.8,59853.8,null,null,"N","N",5,1]
["MJA10010020S",null,null,null,"잡철물 제작 및 설치","규격철물설치, 일반철재","톤",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MJA10010020S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 5%","식",1,147870.6,147870.6,0,0,0,0,147870.6,147870.6,null,null,"N","N",5,1]
["MJA10010030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.25,0,0,165545,372476.2,0,0,165545,372476.2,null,null,"N","N","",1]
["MJA10110010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.68,0,0,165545,112570.6,0,0,165545,112570.6,null,null,"N","N","",1]
["MJA10110020S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",2.5,0,0,214222,535555,0,0,214222,535555,null,null,"N","N","",1]
["MJA10110030S",null,null,null,"잡철물 제작 및 설치","현장제작설치, 경량철재","톤",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,85,0,4258,0,0,0,4343,null,null,null,null,"",1]
["MJB10010030S","노무","L001010101000029",null,"도장공","일반공사 직종","인",2.4E-2,0,0,250776,6018.6,0,0,250776,6018.6,null,null,"N","N","",1]
["MJB20010010S","노무","L001010101000029",null,"도장공","일반공사 직종","인",8.0000000000000002E-3,0,0,250776,2006.2,0,0,250776,2006.2,null,null,"N","N","",1]
["MJB20010010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,43.4,43.4,0,0,0,0,43.4,43.4,null,null,"N","N",2,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MJB20010040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.0000000000000001E-3,0,0,165545,827.7,0,0,165545,827.7,null,null,"N","N","",1]
["MJC00010010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",4.2999999999999997E-2,0,0,229482,9867.7000000000007,0,0,229482,9867.7000000000007,null,null,"N","N","",1]
["MJC00010030S","노무","L001010101000039",null,"배관공","일반공사 직종","인",6.6000000000000003E-2,0,0,229482,15145.8,0,0,229482,15145.8,null,null,"N","N","",1]
["MJC00010040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 1%","식",1,244.5,244.5,0,0,0,0,244.5,244.5,null,null,"N","N",1,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MJC00110020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.7999999999999999E-2,0,0,165545,2979.8,0,0,165545,2979.8,null,null,"N","N","",1]
["MJC00110030S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 1%","식",1,243,243,0,0,0,0,243,243,null,null,"N","N",1,1]
["MJC00110050S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.124,0,0,229482,28455.7,0,0,229482,28455.7,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MJC01010020S","손료","RENT000000000002",null,"노무할증  20%증","노무비의 120%","식",1,0,0,20906.7,20906.7,0,0,20906.7,20906.7,null,null,"N","N",120,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MJC01010050S",null,null,null,"슬리브 설치","D300∼400, 단열재 설치구간, 바닥","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,282,0,33845,0,0,0,34127,null,null,null,null,"",1]
["MJC01110010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.2E-2,0,0,165545,1986.5,0,0,165545,1986.5,null,null,"N","Y","",0]
["MJC01110030S","노무","L001010101000039",null,"배관공","일반공사 직종","인",8.5000000000000006E-2,0,0,229482,19505.900000000001,0,0,229482,19505.900000000001,null,null,"N","Y","",0]
[null,null,null,null,"[합 계]",null,null,0,0,243,0,29168,0,0,0,29411,null,null,null,null,"",1]
["MJC01110050S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.124,0,0,229482,28455.7,0,0,229482,28455.7,null,null,"N","Y","",0]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MJC10010020S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,894.1,894.1,0,0,0,0,894.1,894.1,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,1066,0,53348,0,0,0,54414,null,null,null,null,"",1]
["MJC10010040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,1239.7,1239.7,0,0,0,0,1239.7,1239.7,null,null,"N","N",2,1]
["MJC10010050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.21,0,0,165545,34764.400000000001,0,0,165545,34764.400000000001,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MJC10010080S","노무","L001010101000015",null,"착암공","일반공사 직종","인",0.33900000000000002,0,0,210152,71241.5,0,0,210152,71241.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,2885,0,144267,0,0,0,147152,null,null,null,null,"",1]
["MJC10010100S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,3200.9,3200.9,0,0,0,0,3200.9,3200.9,null,null,"N","N",2,1]
["MJC10110020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.152,0,0,165545,25162.799999999999,0,0,165545,25162.799999999999,null,null,"N","N","",1]
["MJC10110030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.18099999999999999,0,0,165545,29963.599999999999,0,0,165545,29963.599999999999,null,null,"N","N","",1]
["MJC10110040S","노무","L001010101000015",null,"착암공","일반공사 직종","인",0.21099999999999999,0,0,210152,44342,0,0,210152,44342,null,null,"N","N","",1]
["MJC10110050S","노무","L001010101000015",null,"착암공","일반공사 직종","인",0.26800000000000002,0,0,210152,56320.7,0,0,210152,56320.7,null,null,"N","N","",1]
["MJC10110060S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,2419.4,2419.4,0,0,0,0,2419.4,2419.4,null,null,"N","N",2,1]
["MJC10110080S",null,null,null,"배관을 위한 구멍뚫기","300mm, 콘크리트 두께 150mm, 벽체","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MJC10110090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.49099999999999999,0,0,165545,81282.5,0,0,165545,81282.5,null,null,"N","N","",1]
["MJC10110100S","노무","L001010101000015",null,"착암공","일반공사 직종","인",0.54400000000000004,0,0,210152,114322.6,0,0,210152,114322.6,null,null,"N","N","",1]
["MJC11010020S","노무","L001010101000015",null,"착암공","일반공사 직종","인",0.20799999999999999,0,0,210152,43711.6,0,0,210152,43711.6,null,null,"N","N","",1]
["MJC11010030S",null,null,null,"배관을 위한 구멍뚫기","75mm, 콘크리트 두께 300mm, 바닥","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MJC11010050S",null,null,null,"배관을 위한 구멍뚫기","150mm, 콘크리트 두께 300mm, 바닥","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MJC11010060S","노무","L001010101000015",null,"착암공","일반공사 직종","인",0.44600000000000001,0,0,210152,93727.7,0,0,210152,93727.7,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MJC11010090S",null,null,null,"배관을 위한 구멍뚫기","350mm, 콘크리트 두께 300mm, 바닥","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MJC11110020S",null,null,null,"배관을 위한 구멍뚫기","50mm, 콘크리트 두께 300mm, 벽체","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MJC11110030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.317,0,0,165545,52477.7,0,0,165545,52477.7,null,null,"N","N","",1]
["MJC11110030S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,2381.9,2381.9,0,0,0,0,2381.9,2381.9,null,null,"N","N",2,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MJC11110070S",null,null,null,"배관을 위한 구멍뚫기","250mm, 콘크리트 두께 300mm, 벽체","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,5041,0,252092,0,0,0,257133,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,5800,0,290038,0,0,0,295838,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,7326,0,366304,0,0,0,373630,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MJD10010010S",null,null,null,"시험점화","단독주택","호당",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MJD10010020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.05,0,0,165545,8277.2000000000007,0,0,165545,8277.2000000000007,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,395,0,19751,0,0,0,20146,null,null,null,null,"",1]
["MKA10010010S",null,null,null,"소화용구 격납상자 설치","소화용구 격납상자","조",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MKB00010010S",null,null,null,"알람밸브 설치","D65","조",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MKB00010030S","노무","L001010101000039",null,"배관공","일반공사 직종","인",1.66,0,0,229482,380940.1,0,0,229482,380940.1,null,null,"N","N","",1]
["MKB00010050S",null,null,null,"알람밸브 설치","D150","조",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MKB10010030S","노무","L001010101000039",null,"배관공","일반공사 직종","인",2.19,0,0,229482,502565.5,0,0,229482,502565.5,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,484207,0,0,0,484207,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MKC00010020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.6,0,0,229482,137689.20000000001,0,0,229482,137689.20000000001,null,null,"N","N","",1]
["MKC10010020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",1.5,0,0,229482,344223,0,0,229482,344223,null,null,"N","N","",1]
["MKD00010020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.6,0,0,229482,137689.20000000001,0,0,229482,137689.20000000001,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,275378,0,0,0,275378,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,527798,0,0,0,527798,null,null,null,null,"",1]
["MKG00010010S",null,null,null,"스프링클러 헤드설치","스프링클러 헤드","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,592063,0,0,0,592063,null,null,null,null,"",1]
["MKG10010030S","노무","L001010101000039",null,"배관공","일반공사 직종","인",3.4,0,0,229482,780238.8,0,0,229482,780238.8,null,null,"N","N","",1]
["MKH00010010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.52,0,0,229482,119330.6,0,0,229482,119330.6,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MKH00010080S",null,null,null,"소화약제 소화설비 설치","선택밸브, D125 이하","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MKH00110010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.21,0,0,229482,48191.199999999997,0,0,229482,48191.199999999997,null,null,"N","N","",1]
["MKH00210010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",1.03,0,0,229482,236366.4,0,0,229482,236366.4,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,94087,0,0,0,94087,null,null,null,null,"",1]
["MKH00610010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.31,0,0,229482,71139.399999999994,0,0,229482,71139.399999999994,null,null,"N","N","",1]
["MKH01010010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",2.06,0,0,229482,472732.9,0,0,229482,472732.9,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MKH01410010S",null,null,null,"소화약제 소화설비 설치","벨","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MKH10010010S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",0.21199999999999999,0,0,233722,49549,0,0,233722,49549,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MLA00010030S","노무","L001010101000058",null,"플랜트용접공","일반공사 직종","인",5.8000000000000003E-2,0,0,286083,16592.8,0,0,286083,16592.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,497,0,16592,0,0,0,17089,null,null,null,null,"",1]
["MLA00010050S","노무","L001010101000058",null,"플랜트용접공","일반공사 직종","인",7.5999999999999998E-2,0,0,286083,21742.3,0,0,286083,21742.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,781,0,26033,0,0,0,26814,null,null,null,null,"",1]
["MLA00010080S",null,null,null,"가스용 강관 용접 접합(알곤용접)","D80","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MLA00010100S",null,null,null,"가스용 강관 용접 접합(알곤용접)","D125","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MLA00010120S","노무","L001010101000058",null,"플랜트용접공","일반공사 직종","인",0.28699999999999998,0,0,286083,82105.8,0,0,286083,82105.8,null,null,"N","N","",1]
["MLA00010120S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,2463.1,2463.1,0,0,0,0,2463.1,2463.1,null,null,"N","N",3,1]
["MLA00010150S",null,null,null,"가스용 강관 용접 접합(알곤용접)","D350","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,4514,0,150479,0,0,0,154993,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MLA00110020S","노무","L001010101000058",null,"플랜트용접공","일반공사 직종","인",4.9000000000000002E-2,0,0,286083,14018,0,0,286083,14018,null,null,"N","Y","",0]
["MLA00110040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,592.1,592.1,0,0,0,0,592.1,592.1,null,null,"N","N",3,1]
["MLA00110050S",null,null,null,"가스용 강관 용접 접합(아크용접)","D40","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,781,0,24731,0,0,0,25512,null,null,null,null,"",1]
["MLA00110080S",null,null,null,"가스용 강관 용접 접합(아크용접)","D80","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MLA00110090S","노무","L001010101000058",null,"플랜트용접공","일반공사 직종","인",0.159,0,0,286083,45487.1,0,0,286083,45487.1,null,null,"N","Y","",0]
["MLA00110100S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,1639.2,1639.2,0,0,0,0,1639.2,1639.2,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,1913,0,60606,0,0,0,62519,null,null,null,null,"",1]
["MLA00110120S",null,null,null,"가스용 강관 용접 접합(아크용접)","D200","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MLA00110140S",null,null,null,"가스용 강관 용접 접합(아크용접)","D300","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MLA00110160S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,4514.3,4514.3,0,0,0,0,4514.3,4514.3,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,58,0,5876,0,0,0,5934,null,null,null,null,"",1]
["MLA10010030S",null,null,null,"가스용 강관 용접식 부설","D25, 인력시공","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MLA10010040S",null,null,null,"가스용 강관 용접식 부설","D32, 인력시공","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MLA10010050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.01,0,0,165545,1655.4,0,0,165545,1655.4,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,160,0,16086,0,0,0,16246,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,193,0,19336,0,0,0,19529,null,null,null,null,"",1]
["MLA10010100S",null,null,null,"가스용 강관 용접식 부설","D125, 인력시공","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MLA10010110S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.1E-2,0,0,165545,5131.8,0,0,165545,5131.8,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,711,0,71140,0,0,0,71851,null,null,null,null,"",1]
["MLA10010150S",null,null,null,"가스용 강관 용접식 부설","D350, 인력시공","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,1094,0,109419,0,0,0,110513,null,null,null,null,"",1]
["MLA10110010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.2E-2,0,0,165545,1986.5,0,0,165545,1986.5,null,null,"N","N","",1]
["MLA10110020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.7999999999999999E-2,0,0,165545,2979.8,0,0,165545,2979.8,null,null,"N","N","",1]
["MLA10110030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.3E-2,0,0,165545,3807.5,0,0,165545,3807.5,null,null,"N","N","",1]
["MLA10110040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,1011.4,1011.4,0,0,0,0,1011.4,1011.4,null,null,"N","N",3,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MLA10110060S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,1461.5,1461.5,0,0,0,0,1461.5,1461.5,null,null,"N","N",3,1]
["MLA20010010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",6.0999999999999999E-2,0,0,229482,13998.4,0,0,229482,13998.4,null,null,"N","N","",1]
["MLA20010020S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 5%","식",1,1196.8,1196.8,0,0,0,0,1196.8,1196.8,null,null,"N","N",5,1]
["MLA20010040S",null,null,null,"가스용 강관 나사식 접합 및 배관","D40","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MLA20010050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.5999999999999999E-2,0,0,165545,7615,0,0,165545,7615,null,null,"N","N","",1]
["MLB00010010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.9E-2,0,0,165545,3145.3,0,0,165545,3145.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,1260,0,25213,0,0,0,26473,null,null,null,null,"",1]
["MLB00010040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 5%","식",1,1890.9,1890.9,0,0,0,0,1890.9,1890.9,null,null,"N","N",5,1]
["MLB00010050S",null,null,null,"가스용 PE관 버트융착식 접합 및 부설","D63","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MLB00010070S",null,null,null,"가스용 PE관 버트융착식 접합 및 부설","D90","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MLB00010070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.7000000000000002E-2,0,0,165545,9436,0,0,165545,9436,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,3859,0,77182,0,0,0,81041,null,null,null,null,"",1]
["MLB00010100S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.35499999999999998,0,0,229482,81466.100000000006,0,0,229482,81466.100000000006,null,null,"N","N","",1]
["MLB00010110S",null,null,null,"가스용 PE관 버트융착식 접합 및 부설","D160","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MLB00010130S",null,null,null,"가스용 PE관 버트융착식 접합 및 부설","D200","개소",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MLB00010140S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.127,0,0,165545,21024.2,0,0,165545,21024.2,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,7304,0,146091,0,0,0,153395,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,8944,0,178889,0,0,0,187833,null,null,null,null,"",1]
["MLB00010170S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.745,0,0,229482,170964,0,0,229482,170964,null,null,"N","N","",1]
["MLB00010180S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.19500000000000001,0,0,165545,32281.200000000001,0,0,165545,32281.200000000001,null,null,"N","N","",1]
["MLC00010010S",null,null,null,"분기공 설치","D20∼25","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MLC00010020S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 1%","식",1,2090.6,2090.6,0,0,0,0,2090.6,2090.6,null,null,"N","N",1,1]
["MLC00010030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.219,0,0,165545,36254.300000000003,0,0,165545,36254.300000000003,null,null,"N","N","",1]
["MLC00010040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 1%","식",1,2812.2,2812.2,0,0,0,0,2812.2,2812.2,null,null,"N","N",1,1]
[null,null,null,null,"[합 계]",null,null,0,0,3291,0,329172,0,0,0,332463,null,null,null,null,"",1]
["MLC00010060S","노무","L001010101000058",null,"플랜트용접공","일반공사 직종","인",0.755,0,0,286083,215992.6,0,0,286083,215992.6,null,null,"N","N","",1]
["MLC00010070S",null,null,null,"분기공 설치","D150","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MLC00010090S","노무","L001010101000058",null,"플랜트용접공","일반공사 직종","인",1.337,0,0,286083,382492.9,0,0,286083,382492.9,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MLC00010110S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 1%","식",1,9287.5,9287.5,0,0,0,0,9287.5,9287.5,null,null,"N","N",1,1]
["MLC10010010S",null,null,null,"가스용 밸브설치","D15∼25","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MLC10010020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.308,0,0,229482,70680.399999999994,0,0,229482,70680.399999999994,null,null,"N","N","",1]
["MLC10010030S",null,null,null,"가스용 밸브설치","D65","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MLC10010050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.17199999999999999,0,0,165545,28473.7,0,0,165545,28473.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,3635,0,181760,0,0,0,185395,null,null,null,null,"",1]
["MLC10010080S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.97599999999999998,0,0,229482,223974.39999999999,0,0,229482,223974.39999999999,null,null,"N","N","",1]
["MLC10010090S",null,null,null,"가스용 밸브설치","D250","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,10576,0,528827,0,0,0,539403,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MLC30010010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.7000000000000002E-2,0,0,165545,9436,0,0,165545,9436,null,null,"N","N","",1]
["MQA00010010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",1.2E-2,0,0,229482,2753.7,0,0,229482,2753.7,null,null,"N","N","",1]
["MQA00010020S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,89.4,89.4,0,0,0,0,89.4,89.4,null,null,"N","N",2,1]
["MQA00010030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.0999999999999999E-2,0,0,165545,1820.9,0,0,165545,1820.9,null,null,"N","N","",1]
["MQA00010050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.4E-2,0,0,165545,2317.6,0,0,165545,2317.6,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,142,0,7136,0,0,0,7278,null,null,null,null,"",1]
["MQA00010070S",null,null,null,"배관 해체/강관","D65mm이하, 강관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA00010080S","노무","L001010101000039",null,"배관공","일반공사 직종","인",3.9E-2,0,0,229482,8949.7000000000007,0,0,229482,8949.7000000000007,null,null,"N","N","",1]
["MQA00010090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.5000000000000003E-2,0,0,165545,5794,0,0,165545,5794,null,null,"N","N","",1]
["MQA00010110S",null,null,null,"배관 해체/강관","D150mm이하, 강관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA00010120S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.121,0,0,229482,27767.3,0,0,229482,27767.3,null,null,"N","N","",1]
["MQA00010130S",null,null,null,"배관 해체/강관","D250mm이하, 강관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA00010150S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.25,0,0,229482,57370.5,0,0,229482,57370.5,null,null,"N","N","",1]
["MQA00010160S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,2010.7,2010.7,0,0,0,0,2010.7,2010.7,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,2010,0,100538,0,0,0,102548,null,null,null,null,"",1]
["MQA01010020S",null,null,null,"배관 해체/동관","D20mm이하, 동관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA01010040S","노무","L001010101000039",null,"배관공","일반공사 직종","인",1.7999999999999999E-2,0,0,229482,4130.6000000000004,0,0,229482,4130.6000000000004,null,null,"N","N","",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA01010090S",null,null,null,"배관 해체/동관","D100mm이하, 동관","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA01010100S","노무","L001010101000039",null,"배관공","일반공사 직종","인",6.6000000000000003E-2,0,0,229482,15145.8,0,0,229482,15145.8,null,null,"N","N","",1]
["MQA01010110S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,530.1,530.1,0,0,0,0,530.1,530.1,null,null,"N","N",2,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,"[합 계]",null,null,0,0,407,0,20369,0,0,0,20776,null,null,null,null,"",1]
["MQA10010030S","노무","L001010101000043",null,"덕트공","일반공사 직종","인",6.3E-2,0,0,207048,13044,0,0,207048,13044,null,null,"N","N","",1]
["MQA10010040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,487.7,487.7,0,0,0,0,487.7,487.7,null,null,"N","N",2,1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA20010010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.4E-2,0,0,165545,3973,0,0,165545,3973,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,235,0,11799,0,0,0,12034,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA20010030S",null,null,null,"스파이럴덕트 해체","D180이하, t 0.5mm ","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA20010030S","노무","L001010101000043",null,"덕트공","일반공사 직종","인",4.1000000000000002E-2,0,0,207048,8488.9,0,0,207048,8488.9,null,null,"N","N","",1]
["MQA20010030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.8000000000000001E-2,0,0,165545,4635.2,0,0,165545,4635.2,null,null,"N","N","",1]
["MQA20010030S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,262.39999999999998,262.39999999999998,0,0,0,0,262.39999999999998,262.39999999999998,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,262,0,13124,0,0,0,13386,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA20010040S",null,null,null,"스파이럴덕트 해체","D200이하, t 0.5mm ","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA20010040S","노무","L001010101000043",null,"덕트공","일반공사 직종","인",4.4999999999999998E-2,0,0,207048,9317.1,0,0,207048,9317.1,null,null,"N","N","",1]
["MQA20010040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.03,0,0,165545,4966.3,0,0,165545,4966.3,null,null,"N","N","",1]
["MQA20010040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,285.60000000000002,285.60000000000002,0,0,0,0,285.60000000000002,285.60000000000002,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,285,0,14283,0,0,0,14568,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA20010050S",null,null,null,"스파이럴덕트 해체","D225이하, t 0.6mm ","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA20010050S","노무","L001010101000043",null,"덕트공","일반공사 직종","인",0.05,0,0,207048,10352.4,0,0,207048,10352.4,null,null,"N","N","",1]
["MQA20010050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.3000000000000002E-2,0,0,165545,5462.9,0,0,165545,5462.9,null,null,"N","N","",1]
["MQA20010050S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,316.3,316.3,0,0,0,0,316.3,316.3,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,316,0,15815,0,0,0,16131,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA20010060S",null,null,null,"스파이럴덕트 해체","D250이하, t 0.6mm ","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA20010060S","노무","L001010101000043",null,"덕트공","일반공사 직종","인",5.5E-2,0,0,207048,11387.6,0,0,207048,11387.6,null,null,"N","N","",1]
["MQA20010060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.5999999999999997E-2,0,0,165545,5959.6,0,0,165545,5959.6,null,null,"N","N","",1]
["MQA20010060S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,346.9,346.9,0,0,0,0,346.9,346.9,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,346,0,17347,0,0,0,17693,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA20010070S",null,null,null,"스파이럴덕트 해체","D275이하, t 0.6mm ","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA20010070S","노무","L001010101000043",null,"덕트공","일반공사 직종","인",5.8999999999999997E-2,0,0,207048,12215.8,0,0,207048,12215.8,null,null,"N","N","",1]
["MQA20010070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.04,0,0,165545,6621.8,0,0,165545,6621.8,null,null,"N","N","",1]
["MQA20010070S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,376.7,376.7,0,0,0,0,376.7,376.7,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,376,0,18837,0,0,0,19213,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA20010080S",null,null,null,"스파이럴덕트 해체","D300이하, t 0.6mm ","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA20010080S","노무","L001010101000043",null,"덕트공","일반공사 직종","인",6.4000000000000001E-2,0,0,207048,13251,0,0,207048,13251,null,null,"N","N","",1]
["MQA20010080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.2999999999999997E-2,0,0,165545,7118.4,0,0,165545,7118.4,null,null,"N","N","",1]
["MQA20010080S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,407.3,407.3,0,0,0,0,407.3,407.3,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,407,0,20369,0,0,0,20776,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA20010090S",null,null,null,"스파이럴덕트 해체","D350이하, t 0.6mm ","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA20010090S","노무","L001010101000043",null,"덕트공","일반공사 직종","인",7.3999999999999996E-2,0,0,207048,15321.5,0,0,207048,15321.5,null,null,"N","N","",1]
["MQA20010090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.9000000000000002E-2,0,0,165545,8111.7,0,0,165545,8111.7,null,null,"N","N","",1]
["MQA20010090S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,468.6,468.6,0,0,0,0,468.6,468.6,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,468,0,23433,0,0,0,23901,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA20010100S",null,null,null,"스파이럴덕트 해체","D400이하, t 0.6mm ","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA20010100S","노무","L001010101000043",null,"덕트공","일반공사 직종","인",8.4000000000000005E-2,0,0,207048,17392,0,0,207048,17392,null,null,"N","N","",1]
["MQA20010100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.6000000000000001E-2,0,0,165545,9270.5,0,0,165545,9270.5,null,null,"N","N","",1]
["MQA20010100S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,533.20000000000005,533.20000000000005,0,0,0,0,533.20000000000005,533.20000000000005,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,533,0,26662,0,0,0,27195,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA20010110S",null,null,null,"스파이럴덕트 해체","D450이하, t 0.6mm ","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA20010110S","노무","L001010101000043",null,"덕트공","일반공사 직종","인",0.104,0,0,207048,21532.9,0,0,207048,21532.9,null,null,"N","N","",1]
["MQA20010110S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.9000000000000006E-2,0,0,165545,11422.6,0,0,165545,11422.6,null,null,"N","N","",1]
["MQA20010110S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,659.1,659.1,0,0,0,0,659.1,659.1,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,659,0,32955,0,0,0,33614,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA20010120S",null,null,null,"스파이럴덕트 해체","D500이하, t 0.6mm ","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA20010120S","노무","L001010101000043",null,"덕트공","일반공사 직종","인",0.114,0,0,207048,23603.4,0,0,207048,23603.4,null,null,"N","N","",1]
["MQA20010120S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.5999999999999998E-2,0,0,165545,12581.4,0,0,165545,12581.4,null,null,"N","N","",1]
["MQA20010120S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,723.6,723.6,0,0,0,0,723.6,723.6,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,723,0,36184,0,0,0,36907,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA20010130S",null,null,null,"스파이럴덕트 해체","D550이하, t 0.6mm ","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA20010130S","노무","L001010101000043",null,"덕트공","일반공사 직종","인",0.123,0,0,207048,25466.9,0,0,207048,25466.9,null,null,"N","N","",1]
["MQA20010130S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",8.2000000000000003E-2,0,0,165545,13574.6,0,0,165545,13574.6,null,null,"N","N","",1]
["MQA20010130S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,780.8,780.8,0,0,0,0,780.8,780.8,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,780,0,39041,0,0,0,39821,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA20010140S",null,null,null,"스파이럴덕트 해체","D600이하, t 0.6mm ","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA20010140S","노무","L001010101000043",null,"덕트공","일반공사 직종","인",0.13200000000000001,0,0,207048,27330.3,0,0,207048,27330.3,null,null,"N","N","",1]
["MQA20010140S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",8.7999999999999995E-2,0,0,165545,14567.9,0,0,165545,14567.9,null,null,"N","N","",1]
["MQA20010140S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,837.9,837.9,0,0,0,0,837.9,837.9,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,837,0,41898,0,0,0,42735,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA30010010S",null,null,null,"배관보온 해체/고무발포보온재","D15, 보온두께 50mm 이하, 고무발포보온재","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA30010010S","노무","L001010101000044",null,"보온공","일반공사 직종","인",1.4E-2,0,0,204285,2859.9,0,0,204285,2859.9,null,null,"N","N","",1]
["MQA30010010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.01,0,0,165545,1655.4,0,0,165545,1655.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,4515,0,0,0,4515,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA30010020S",null,null,null,"배관보온 해체/고무발포보온재","D20, 보온두께 50mm 이하, 고무발포보온재","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA30010020S","노무","L001010101000044",null,"보온공","일반공사 직종","인",1.6E-2,0,0,204285,3268.5,0,0,204285,3268.5,null,null,"N","N","",1]
["MQA30010020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.0999999999999999E-2,0,0,165545,1820.9,0,0,165545,1820.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,5089,0,0,0,5089,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA30010030S",null,null,null,"배관보온 해체/고무발포보온재","D25, 보온두께 50mm 이하, 고무발포보온재","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA30010030S","노무","L001010101000044",null,"보온공","일반공사 직종","인",1.7000000000000001E-2,0,0,204285,3472.8,0,0,204285,3472.8,null,null,"N","N","",1]
["MQA30010030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.0999999999999999E-2,0,0,165545,1820.9,0,0,165545,1820.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,5293,0,0,0,5293,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA30010040S",null,null,null,"배관보온 해체/고무발포보온재","D32, 보온두께 50mm 이하, 고무발포보온재","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA30010040S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.02,0,0,204285,4085.7,0,0,204285,4085.7,null,null,"N","N","",1]
["MQA30010040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.2999999999999999E-2,0,0,165545,2152,0,0,165545,2152,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,6237,0,0,0,6237,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA30010050S",null,null,null,"배관보온 해체/고무발포보온재","D40, 보온두께 50mm 이하, 고무발포보온재","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA30010050S","노무","L001010101000044",null,"보온공","일반공사 직종","인",2.3E-2,0,0,204285,4698.5,0,0,204285,4698.5,null,null,"N","N","",1]
["MQA30010050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.6E-2,0,0,165545,2648.7,0,0,165545,2648.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,7347,0,0,0,7347,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA30010060S",null,null,null,"배관보온 해체/고무발포보온재","D50, 보온두께 50mm 이하, 고무발포보온재","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA30010060S","노무","L001010101000044",null,"보온공","일반공사 직종","인",2.7E-2,0,0,204285,5515.6,0,0,204285,5515.6,null,null,"N","N","",1]
["MQA30010060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.7999999999999999E-2,0,0,165545,2979.8,0,0,165545,2979.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,8495,0,0,0,8495,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA30010070S",null,null,null,"배관보온 해체/고무발포보온재","D65, 보온두께 50mm 이하, 고무발포보온재","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA30010070S","노무","L001010101000044",null,"보온공","일반공사 직종","인",2.9000000000000001E-2,0,0,204285,5924.2,0,0,204285,5924.2,null,null,"N","N","",1]
["MQA30010070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.02,0,0,165545,3310.9,0,0,165545,3310.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,9235,0,0,0,9235,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA30010080S",null,null,null,"배관보온 해체/고무발포보온재","D80, 보온두께 50mm 이하, 고무발포보온재","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA30010080S","노무","L001010101000044",null,"보온공","일반공사 직종","인",3.3000000000000002E-2,0,0,204285,6741.4,0,0,204285,6741.4,null,null,"N","N","",1]
["MQA30010080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.1999999999999999E-2,0,0,165545,3641.9,0,0,165545,3641.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,10383,0,0,0,10383,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA30010090S",null,null,null,"배관보온 해체/고무발포보온재","D100, 보온두께 50mm 이하, 고무발포보온재","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA30010090S","노무","L001010101000044",null,"보온공","일반공사 직종","인",3.7999999999999999E-2,0,0,204285,7762.8,0,0,204285,7762.8,null,null,"N","N","",1]
["MQA30010090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5000000000000001E-2,0,0,165545,4138.6000000000004,0,0,165545,4138.6000000000004,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,11901,0,0,0,11901,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA30010100S",null,null,null,"배관보온 해체/고무발포보온재","D125, 보온두께 50mm 이하, 고무발포보온재","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA30010100S","노무","L001010101000044",null,"보온공","일반공사 직종","인",4.5999999999999999E-2,0,0,204285,9397.1,0,0,204285,9397.1,null,null,"N","N","",1]
["MQA30010100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.03,0,0,165545,4966.3,0,0,165545,4966.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,14363,0,0,0,14363,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA30010110S",null,null,null,"배관보온 해체/고무발포보온재","D150, 보온두께 50mm 이하, 고무발포보온재","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA30010110S","노무","L001010101000044",null,"보온공","일반공사 직종","인",5.2999999999999999E-2,0,0,204285,10827.1,0,0,204285,10827.1,null,null,"N","N","",1]
["MQA30010110S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.5000000000000003E-2,0,0,165545,5794,0,0,165545,5794,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,16621,0,0,0,16621,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA30010120S",null,null,null,"배관보온 해체/고무발포보온재","D200, 보온두께 50mm 이하, 고무발포보온재","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA30010120S","노무","L001010101000044",null,"보온공","일반공사 직종","인",6.4000000000000001E-2,0,0,204285,13074.2,0,0,204285,13074.2,null,null,"N","N","",1]
["MQA30010120S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.2000000000000003E-2,0,0,165545,6952.8,0,0,165545,6952.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,20027,0,0,0,20027,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA30010130S",null,null,null,"배관보온 해체/고무발포보온재","D250, 보온두께 50mm 이하, 고무발포보온재","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA30010130S","노무","L001010101000044",null,"보온공","일반공사 직종","인",7.2999999999999995E-2,0,0,204285,14912.8,0,0,204285,14912.8,null,null,"N","N","",1]
["MQA30010130S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.9000000000000002E-2,0,0,165545,8111.7,0,0,165545,8111.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,23024,0,0,0,23024,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA30010140S",null,null,null,"배관보온 해체/고무발포보온재","D300, 보온두께 50mm 이하, 고무발포보온재","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA30010140S","노무","L001010101000044",null,"보온공","일반공사 직종","인",8.3000000000000004E-2,0,0,204285,16955.599999999999,0,0,204285,16955.599999999999,null,null,"N","N","",1]
["MQA30010140S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.5E-2,0,0,165545,9104.9,0,0,165545,9104.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,26060,0,0,0,26060,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA31010010S",null,null,null,"배관보온 해체/발포폴리에틸렌보온재","D15, 보온두께 50mm 이하, 발포폴리에틸렌보온재","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA31010010S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.01,0,0,204285,2042.8,0,0,204285,2042.8,null,null,"N","N","",1]
["MQA31010010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",7.0000000000000001E-3,0,0,165545,1158.8,0,0,165545,1158.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,3201,0,0,0,3201,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA31010020S",null,null,null,"배관보온 해체/발포폴리에틸렌보온재","D20, 보온두께 50mm 이하, 발포폴리에틸렌보온재","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA31010020S","노무","L001010101000044",null,"보온공","일반공사 직종","인",1.2E-2,0,0,204285,2451.4,0,0,204285,2451.4,null,null,"N","N","",1]
["MQA31010020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",8.0000000000000002E-3,0,0,165545,1324.3,0,0,165545,1324.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,3775,0,0,0,3775,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA31010030S",null,null,null,"배관보온 해체/발포폴리에틸렌보온재","D25, 보온두께 50mm 이하, 발포폴리에틸렌보온재","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA31010030S","노무","L001010101000044",null,"보온공","일반공사 직종","인",1.2E-2,0,0,204285,2451.4,0,0,204285,2451.4,null,null,"N","N","",1]
["MQA31010030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",8.0000000000000002E-3,0,0,165545,1324.3,0,0,165545,1324.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,3775,0,0,0,3775,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA31010040S",null,null,null,"배관보온 해체/발포폴리에틸렌보온재","D32, 보온두께 50mm 이하, 발포폴리에틸렌보온재","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA31010040S","노무","L001010101000044",null,"보온공","일반공사 직종","인",1.4E-2,0,0,204285,2859.9,0,0,204285,2859.9,null,null,"N","N","",1]
["MQA31010040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.01,0,0,165545,1655.4,0,0,165545,1655.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,4515,0,0,0,4515,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA31010050S",null,null,null,"배관보온 해체/발포폴리에틸렌보온재","D40, 보온두께 50mm 이하, 발포폴리에틸렌보온재","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA31010050S","노무","L001010101000044",null,"보온공","일반공사 직종","인",1.7000000000000001E-2,0,0,204285,3472.8,0,0,204285,3472.8,null,null,"N","N","",1]
["MQA31010050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.0999999999999999E-2,0,0,165545,1820.9,0,0,165545,1820.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,5293,0,0,0,5293,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA31010060S",null,null,null,"배관보온 해체/발포폴리에틸렌보온재","D50, 보온두께 50mm 이하, 발포폴리에틸렌보온재","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA31010060S","노무","L001010101000044",null,"보온공","일반공사 직종","인",1.9E-2,0,0,204285,3881.4,0,0,204285,3881.4,null,null,"N","N","",1]
["MQA31010060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.2999999999999999E-2,0,0,165545,2152,0,0,165545,2152,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,6033,0,0,0,6033,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA31010070S",null,null,null,"배관보온 해체/발포폴리에틸렌보온재","D65, 보온두께 50mm 이하, 발포폴리에틸렌보온재","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA31010070S","노무","L001010101000044",null,"보온공","일반공사 직종","인",2.1000000000000001E-2,0,0,204285,4289.8999999999996,0,0,204285,4289.8999999999996,null,null,"N","N","",1]
["MQA31010070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.4E-2,0,0,165545,2317.6,0,0,165545,2317.6,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,6607,0,0,0,6607,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA31010080S",null,null,null,"배관보온 해체/발포폴리에틸렌보온재","D80, 보온두께 50mm 이하, 발포폴리에틸렌보온재","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA31010080S","노무","L001010101000044",null,"보온공","일반공사 직종","인",2.4E-2,0,0,204285,4902.8,0,0,204285,4902.8,null,null,"N","N","",1]
["MQA31010080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.6E-2,0,0,165545,2648.7,0,0,165545,2648.7,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,7551,0,0,0,7551,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA31010090S",null,null,null,"배관보온 해체/발포폴리에틸렌보온재","D100, 보온두께 50mm 이하, 발포폴리에틸렌보온재","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA31010090S","노무","L001010101000044",null,"보온공","일반공사 직종","인",2.7E-2,0,0,204285,5515.6,0,0,204285,5515.6,null,null,"N","N","",1]
["MQA31010090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.7999999999999999E-2,0,0,165545,2979.8,0,0,165545,2979.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,8495,0,0,0,8495,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA31010100S",null,null,null,"배관보온 해체/발포폴리에틸렌보온재","D125, 보온두께 50mm 이하, 발포폴리에틸렌보온재","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA31010100S","노무","L001010101000044",null,"보온공","일반공사 직종","인",3.3000000000000002E-2,0,0,204285,6741.4,0,0,204285,6741.4,null,null,"N","N","",1]
["MQA31010100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.1999999999999999E-2,0,0,165545,3641.9,0,0,165545,3641.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,10383,0,0,0,10383,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA31010110S",null,null,null,"배관보온 해체/발포폴리에틸렌보온재","D150, 보온두께 50mm 이하, 발포폴리에틸렌보온재","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA31010110S","노무","L001010101000044",null,"보온공","일반공사 직종","인",3.7999999999999999E-2,0,0,204285,7762.8,0,0,204285,7762.8,null,null,"N","N","",1]
["MQA31010110S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5000000000000001E-2,0,0,165545,4138.6000000000004,0,0,165545,4138.6000000000004,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,11901,0,0,0,11901,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA31010120S",null,null,null,"배관보온 해체/발포폴리에틸렌보온재","D200, 보온두께 50mm 이하, 발포폴리에틸렌보온재","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA31010120S","노무","L001010101000044",null,"보온공","일반공사 직종","인",4.4999999999999998E-2,0,0,204285,9192.7999999999993,0,0,204285,9192.7999999999993,null,null,"N","N","",1]
["MQA31010120S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.03,0,0,165545,4966.3,0,0,165545,4966.3,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,14159,0,0,0,14159,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA31010130S",null,null,null,"배관보온 해체/발포폴리에틸렌보온재","D250, 보온두께 50mm 이하, 발포폴리에틸렌보온재","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA31010130S","노무","L001010101000044",null,"보온공","일반공사 직종","인",5.1999999999999998E-2,0,0,204285,10622.8,0,0,204285,10622.8,null,null,"N","N","",1]
["MQA31010130S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.5000000000000003E-2,0,0,165545,5794,0,0,165545,5794,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,16416,0,0,0,16416,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA31010140S",null,null,null,"배관보온 해체/발포폴리에틸렌보온재","D300, 보온두께 50mm 이하, 발포폴리에틸렌보온재","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA31010140S","노무","L001010101000044",null,"보온공","일반공사 직종","인",5.8999999999999997E-2,0,0,204285,12052.8,0,0,204285,12052.8,null,null,"N","N","",1]
["MQA31010140S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.9E-2,0,0,165545,6456.2,0,0,165545,6456.2,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,18509,0,0,0,18509,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA32010010S",null,null,null,"배관보온 해체/유리면보온재(글라스울)","D15, 보온두께 50mm 이하, 유리면보온재(글라스울)","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA32010010S","노무","L001010101000044",null,"보온공","일반공사 직종","인",1.6E-2,0,0,204285,3268.5,0,0,204285,3268.5,null,null,"N","N","",1]
["MQA32010010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.0999999999999999E-2,0,0,165545,1820.9,0,0,165545,1820.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,5089,0,0,0,5089,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA32010020S",null,null,null,"배관보온 해체/유리면보온재(글라스울)","D20, 보온두께 50mm 이하, 유리면보온재(글라스울)","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA32010020S","노무","L001010101000044",null,"보온공","일반공사 직종","인",1.7999999999999999E-2,0,0,204285,3677.1,0,0,204285,3677.1,null,null,"N","N","",1]
["MQA32010020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.2E-2,0,0,165545,1986.5,0,0,165545,1986.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,5663,0,0,0,5663,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA32010030S",null,null,null,"배관보온 해체/유리면보온재(글라스울)","D25, 보온두께 50mm 이하, 유리면보온재(글라스울)","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA32010030S","노무","L001010101000044",null,"보온공","일반공사 직종","인",1.9E-2,0,0,204285,3881.4,0,0,204285,3881.4,null,null,"N","N","",1]
["MQA32010030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.2999999999999999E-2,0,0,165545,2152,0,0,165545,2152,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,6033,0,0,0,6033,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA32010040S",null,null,null,"배관보온 해체/유리면보온재(글라스울)","D32, 보온두께 50mm 이하, 유리면보온재(글라스울)","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA32010040S","노무","L001010101000044",null,"보온공","일반공사 직종","인",2.3E-2,0,0,204285,4698.5,0,0,204285,4698.5,null,null,"N","N","",1]
["MQA32010040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.4999999999999999E-2,0,0,165545,2483.1,0,0,165545,2483.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,7181,0,0,0,7181,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA32010050S",null,null,null,"배관보온 해체/유리면보온재(글라스울)","D40, 보온두께 50mm 이하, 유리면보온재(글라스울)","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA32010050S","노무","L001010101000044",null,"보온공","일반공사 직종","인",2.5999999999999999E-2,0,0,204285,5311.4,0,0,204285,5311.4,null,null,"N","N","",1]
["MQA32010050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.7000000000000001E-2,0,0,165545,2814.2,0,0,165545,2814.2,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,8125,0,0,0,8125,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA32010060S",null,null,null,"배관보온 해체/유리면보온재(글라스울)","D50, 보온두께 50mm 이하, 유리면보온재(글라스울)","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA32010060S","노무","L001010101000044",null,"보온공","일반공사 직종","인",3.1E-2,0,0,204285,6332.8,0,0,204285,6332.8,null,null,"N","N","",1]
["MQA32010060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.02,0,0,165545,3310.9,0,0,165545,3310.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,9643,0,0,0,9643,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA32010070S",null,null,null,"배관보온 해체/유리면보온재(글라스울)","D65, 보온두께 50mm 이하, 유리면보온재(글라스울)","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA32010070S","노무","L001010101000044",null,"보온공","일반공사 직종","인",3.3000000000000002E-2,0,0,204285,6741.4,0,0,204285,6741.4,null,null,"N","N","",1]
["MQA32010070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.1999999999999999E-2,0,0,165545,3641.9,0,0,165545,3641.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,10383,0,0,0,10383,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA32010080S",null,null,null,"배관보온 해체/유리면보온재(글라스울)","D80, 보온두께 50mm 이하, 유리면보온재(글라스울)","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA32010080S","노무","L001010101000044",null,"보온공","일반공사 직종","인",3.7999999999999999E-2,0,0,204285,7762.8,0,0,204285,7762.8,null,null,"N","N","",1]
["MQA32010080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.5000000000000001E-2,0,0,165545,4138.6000000000004,0,0,165545,4138.6000000000004,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,11901,0,0,0,11901,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA32010090S",null,null,null,"배관보온 해체/유리면보온재(글라스울)","D100, 보온두께 50mm 이하, 유리면보온재(글라스울)","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA32010090S","노무","L001010101000044",null,"보온공","일반공사 직종","인",4.2999999999999997E-2,0,0,204285,8784.2000000000007,0,0,204285,8784.2000000000007,null,null,"N","N","",1]
["MQA32010090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",2.8000000000000001E-2,0,0,165545,4635.2,0,0,165545,4635.2,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,13419,0,0,0,13419,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA32010100S",null,null,null,"배관보온 해체/유리면보온재(글라스울)","D125, 보온두께 50mm 이하, 유리면보온재(글라스울)","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA32010100S","노무","L001010101000044",null,"보온공","일반공사 직종","인",5.0999999999999997E-2,0,0,204285,10418.5,0,0,204285,10418.5,null,null,"N","N","",1]
["MQA32010100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",3.4000000000000002E-2,0,0,165545,5628.5,0,0,165545,5628.5,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,16047,0,0,0,16047,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA32010110S",null,null,null,"배관보온 해체/유리면보온재(글라스울)","D150, 보온두께 50mm 이하, 유리면보온재(글라스울)","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA32010110S","노무","L001010101000044",null,"보온공","일반공사 직종","인",0.06,0,0,204285,12257.1,0,0,204285,12257.1,null,null,"N","N","",1]
["MQA32010110S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.04,0,0,165545,6621.8,0,0,165545,6621.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,18878,0,0,0,18878,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA32010120S",null,null,null,"배관보온 해체/유리면보온재(글라스울)","D200, 보온두께 50mm 이하, 유리면보온재(글라스울)","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA32010120S","노무","L001010101000044",null,"보온공","일반공사 직종","인",7.1999999999999995E-2,0,0,204285,14708.5,0,0,204285,14708.5,null,null,"N","N","",1]
["MQA32010120S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",4.8000000000000001E-2,0,0,165545,7946.1,0,0,165545,7946.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,22654,0,0,0,22654,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA32010130S",null,null,null,"배관보온 해체/유리면보온재(글라스울)","D250, 보온두께 50mm 이하, 유리면보온재(글라스울)","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA32010130S","노무","L001010101000044",null,"보온공","일반공사 직종","인",8.2000000000000003E-2,0,0,204285,16751.3,0,0,204285,16751.3,null,null,"N","N","",1]
["MQA32010130S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.5E-2,0,0,165545,9104.9,0,0,165545,9104.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,25856,0,0,0,25856,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA32010140S",null,null,null,"배관보온 해체/유리면보온재(글라스울)","D300, 보온두께 50mm 이하, 유리면보온재(글라스울)","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA32010140S","노무","L001010101000044",null,"보온공","일반공사 직종","인",9.2999999999999999E-2,0,0,204285,18998.5,0,0,204285,18998.5,null,null,"N","N","",1]
["MQA32010140S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.2E-2,0,0,165545,10263.700000000001,0,0,165545,10263.700000000001,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,29262,0,0,0,29262,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA40010010S",null,null,null,"덕트보온 해체/고무발포보온재","고무발포보온재","㎡",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA40010010S","노무","L001010101000044",null,"보온공","일반공사 직종","인",8.1000000000000003E-2,0,0,204285,16547,0,0,204285,16547,null,null,"N","N","",1]
["MQA40010010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.3999999999999999E-2,0,0,165545,8939.4,0,0,165545,8939.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,25486,0,0,0,25486,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA41010010S",null,null,null,"덕트보온 해체/발포폴리에틸렌보온재","발포폴리에틸렌보온재","㎡",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA41010010S","노무","L001010101000044",null,"보온공","일반공사 직종","인",8.1000000000000003E-2,0,0,204285,16547,0,0,204285,16547,null,null,"N","N","",1]
["MQA41010010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",5.3999999999999999E-2,0,0,165545,8939.4,0,0,165545,8939.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,25486,0,0,0,25486,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA42010010S",null,null,null,"덕트보온 해체/유리면보온재(글라스울)","유리면보온재(글라스울)","㎡",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA42010010S","노무","L001010101000044",null,"보온공","일반공사 직종","인",9.6000000000000002E-2,0,0,204285,19611.3,0,0,204285,19611.3,null,null,"N","N","",1]
["MQA42010010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",6.4000000000000001E-2,0,0,165545,10594.8,0,0,165545,10594.8,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,30206,0,0,0,30206,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA50010010S",null,null,null,"펌프 해체","0.75kW 이하, 일반펌프","대",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA50010010S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",0.245,0,0,233722,57261.8,0,0,233722,57261.8,null,null,"N","N","",1]
["MQA50010010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.16300000000000001,0,0,165545,26983.8,0,0,165545,26983.8,null,null,"N","N","",1]
["MQA50010010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,1684.9,1684.9,0,0,0,0,1684.9,1684.9,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,1684,0,84245,0,0,0,85929,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA50010020S",null,null,null,"펌프 해체","1.5kW 이하, 일반펌프","대",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA50010020S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",0.27100000000000002,0,0,233722,63338.6,0,0,233722,63338.6,null,null,"N","N","",1]
["MQA50010020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.18099999999999999,0,0,165545,29963.599999999999,0,0,165545,29963.599999999999,null,null,"N","N","",1]
["MQA50010020S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,1866,1866,0,0,0,0,1866,1866,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,1866,0,93302,0,0,0,95168,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA50010030S",null,null,null,"펌프 해체","2.2kW 이하, 일반펌프","대",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA50010030S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",0.312,0,0,233722,72921.2,0,0,233722,72921.2,null,null,"N","N","",1]
["MQA50010030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.20799999999999999,0,0,165545,34433.300000000003,0,0,165545,34433.300000000003,null,null,"N","N","",1]
["MQA50010030S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,2147,2147,0,0,0,0,2147,2147,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,2147,0,107354,0,0,0,109501,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA50010040S",null,null,null,"펌프 해체","3.7kW 이하, 일반펌프","대",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA50010040S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",0.35899999999999999,0,0,233722,83906.1,0,0,233722,83906.1,null,null,"N","N","",1]
["MQA50010040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.23899999999999999,0,0,165545,39565.199999999997,0,0,165545,39565.199999999997,null,null,"N","N","",1]
["MQA50010040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,2469.4,2469.4,0,0,0,0,2469.4,2469.4,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,2469,0,123471,0,0,0,125940,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA50010050S",null,null,null,"펌프 해체","5.5kW 이하, 일반펌프","대",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA50010050S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",0.432,0,0,233722,100967.9,0,0,233722,100967.9,null,null,"N","N","",1]
["MQA50010050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.28799999999999998,0,0,165545,47676.9,0,0,165545,47676.9,null,null,"N","N","",1]
["MQA50010050S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,2972.8,2972.8,0,0,0,0,2972.8,2972.8,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,2972,0,148644,0,0,0,151616,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA50010060S",null,null,null,"펌프 해체","7.5kW 이하, 일반펌프","대",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA50010060S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",0.54500000000000004,0,0,233722,127378.4,0,0,233722,127378.4,null,null,"N","N","",1]
["MQA50010060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.36299999999999999,0,0,165545,60092.800000000003,0,0,165545,60092.800000000003,null,null,"N","N","",1]
["MQA50010060S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,3749.4,3749.4,0,0,0,0,3749.4,3749.4,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,3749,0,187471,0,0,0,191220,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA50010070S",null,null,null,"펌프 해체","11kW 이하, 일반펌프","대",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA50010070S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",0.68500000000000005,0,0,233722,160099.5,0,0,233722,160099.5,null,null,"N","N","",1]
["MQA50010070S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.45700000000000002,0,0,165545,75654,0,0,165545,75654,null,null,"N","N","",1]
["MQA50010070S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,4715,4715,0,0,0,0,4715,4715,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,4715,0,235753,0,0,0,240468,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA50010080S",null,null,null,"펌프 해체","15kW 이하, 일반펌프","대",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA50010080S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",0.72699999999999998,0,0,233722,169915.8,0,0,233722,169915.8,null,null,"N","N","",1]
["MQA50010080S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.48499999999999999,0,0,165545,80289.3,0,0,165545,80289.3,null,null,"N","N","",1]
["MQA50010080S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,5004.1000000000004,5004.1000000000004,0,0,0,0,5004.1000000000004,5004.1000000000004,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,5004,0,250205,0,0,0,255209,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA50010090S",null,null,null,"펌프 해체","22kW 이하, 일반펌프","대",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA50010090S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",1.175,0,0,233722,274623.3,0,0,233722,274623.3,null,null,"N","N","",1]
["MQA50010090S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.78300000000000003,0,0,165545,129621.7,0,0,165545,129621.7,null,null,"N","N","",1]
["MQA50010090S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,8084.9,8084.9,0,0,0,0,8084.9,8084.9,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,8084,0,404245,0,0,0,412329,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA50010100S",null,null,null,"펌프 해체","37kW 이하, 일반펌프","대",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA50010100S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",1.5169999999999999,0,0,233722,354556.2,0,0,233722,354556.2,null,null,"N","N","",1]
["MQA50010100S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.0109999999999999,0,0,165545,167365.9,0,0,165545,167365.9,null,null,"N","N","",1]
["MQA50010100S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,10438.4,10438.4,0,0,0,0,10438.4,10438.4,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,10438,0,521922,0,0,0,532360,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA50010110S",null,null,null,"펌프 해체","55kW 이하, 일반펌프","대",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA50010110S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",2.44,0,0,233722,570281.6,0,0,233722,570281.6,null,null,"N","N","",1]
["MQA50010110S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.627,0,0,165545,269341.7,0,0,165545,269341.7,null,null,"N","N","",1]
["MQA50010110S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,16792.400000000001,16792.400000000001,0,0,0,0,16792.400000000001,16792.400000000001,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,16792,0,839623,0,0,0,856415,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA50010120S",null,null,null,"펌프 해체","75kW 이하, 일반펌프","대",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQA50010120S","노무","L001010101000051",null,"기계설비공","일반공사 직종","인",2.9889999999999999,0,0,233722,698595,0,0,233722,698595,null,null,"N","N","",1]
["MQA50010120S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1.9930000000000001,0,0,165545,329931.09999999998,0,0,165545,329931.09999999998,null,null,"N","N","",1]
["MQA50010120S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 2%","식",1,20570.5,20570.5,0,0,0,0,20570.5,20570.5,null,null,"N","N",2,1]
[null,null,null,null,"[합 계]",null,null,0,0,20570,0,1028526,0,0,0,1049096,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC00010010S",null,null,null,"유량계 교체/보호통","ø13~15mm, 급수급탕난방용","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC00010010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.17,0,0,229482,39011.9,0,0,229482,39011.9,null,null,"N","N","",1]
["MQC00010010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.17,0,0,165545,28142.6,0,0,165545,28142.6,null,null,"N","N","",1]
["MQC00010010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 1%","식",1,671.5,671.5,0,0,0,0,671.5,671.5,null,null,"N","N",1,1]
[null,null,null,null,"[합 계]",null,null,0,0,671,0,67154,0,0,0,67825,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC00010020S",null,null,null,"유량계 교체/보호통","ø20~32mm, 급수급탕난방용","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC00010020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.2,0,0,229482,45896.4,0,0,229482,45896.4,null,null,"N","N","",1]
["MQC00010020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.2,0,0,165545,33109,0,0,165545,33109,null,null,"N","N","",1]
["MQC00010020S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 1%","식",1,790,790,0,0,0,0,790,790,null,null,"N","N",1,1]
[null,null,null,null,"[합 계]",null,null,0,0,790,0,79005,0,0,0,79795,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC00010030S",null,null,null,"유량계 교체/보호통","ø40~50mm, 급수급탕난방용","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC00010030S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.25,0,0,229482,57370.5,0,0,229482,57370.5,null,null,"N","N","",1]
["MQC00010030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.25,0,0,165545,41386.199999999997,0,0,165545,41386.199999999997,null,null,"N","N","",1]
["MQC00010030S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 1%","식",1,987.5,987.5,0,0,0,0,987.5,987.5,null,null,"N","N",1,1]
[null,null,null,null,"[합 계]",null,null,0,0,987,0,98756,0,0,0,99743,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC01010010S",null,null,null,"유량계 교체/유량계","ø13~15mm, 급수급탕난방용","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC01010010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.13,0,0,229482,29832.6,0,0,229482,29832.6,null,null,"N","N","",1]
["MQC01010010S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.13,0,0,165545,21520.799999999999,0,0,165545,21520.799999999999,null,null,"N","N","",1]
["MQC01010010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 1%","식",1,513.5,513.5,0,0,0,0,513.5,513.5,null,null,"N","N",1,1]
[null,null,null,null,"[합 계]",null,null,0,0,513,0,51353,0,0,0,51866,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC01010020S",null,null,null,"유량계 교체/유량계","ø20~32mm, 급수급탕난방용","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC01010020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.14000000000000001,0,0,229482,32127.4,0,0,229482,32127.4,null,null,"N","N","",1]
["MQC01010020S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.14000000000000001,0,0,165545,23176.3,0,0,165545,23176.3,null,null,"N","N","",1]
["MQC01010020S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 1%","식",1,553,553,0,0,0,0,553,553,null,null,"N","N",1,1]
[null,null,null,null,"[합 계]",null,null,0,0,553,0,55303,0,0,0,55856,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC01010030S",null,null,null,"유량계 교체/유량계","ø40~50mm, 급수급탕난방용","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC01010030S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.17,0,0,229482,39011.9,0,0,229482,39011.9,null,null,"N","N","",1]
["MQC01010030S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.17,0,0,165545,28142.6,0,0,165545,28142.6,null,null,"N","N","",1]
["MQC01010030S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 1%","식",1,671.5,671.5,0,0,0,0,671.5,671.5,null,null,"N","N",1,1]
[null,null,null,null,"[합 계]",null,null,0,0,671,0,67154,0,0,0,67825,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC01010040S",null,null,null,"유량계 교체/유량계","ø65~80mm, 급수급탕난방용","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC01010040S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.5,0,0,229482,114741,0,0,229482,114741,null,null,"N","N","",1]
["MQC01010040S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.5,0,0,165545,82772.5,0,0,165545,82772.5,null,null,"N","N","",1]
["MQC01010040S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 1%","식",1,1975.1,1975.1,0,0,0,0,1975.1,1975.1,null,null,"N","N",1,1]
[null,null,null,null,"[합 계]",null,null,0,0,1975,0,197513,0,0,0,199488,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC01010050S",null,null,null,"유량계 교체/유량계","ø100~150mm, 급수급탕난방용","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC01010050S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.67,0,0,229482,153752.9,0,0,229482,153752.9,null,null,"N","N","",1]
["MQC01010050S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",0.67,0,0,165545,110915.1,0,0,165545,110915.1,null,null,"N","N","",1]
["MQC01010050S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 1%","식",1,2646.6,2646.6,0,0,0,0,2646.6,2646.6,null,null,"N","N",1,1]
[null,null,null,null,"[합 계]",null,null,0,0,2646,0,264668,0,0,0,267314,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC01010060S",null,null,null,"유량계 교체/유량계","ø200~300mm, 급수급탕난방용","개",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC01010060S","노무","L001010101000039",null,"배관공","일반공사 직종","인",1,0,0,229482,229482,0,0,229482,229482,null,null,"N","N","",1]
["MQC01010060S","노무","L001010101000002",null,"보통인부","일반공사 직종","인",1,0,0,165545,165545,0,0,165545,165545,null,null,"N","N","",1]
["MQC01010060S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 1%","식",1,3950.2,3950.2,0,0,0,0,3950.2,3950.2,null,null,"N","N",1,1]
[null,null,null,null,"[합 계]",null,null,0,0,3950,0,395027,0,0,0,398977,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC10010010S",null,null,null,"관갱생공","D15mm","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC10010010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",7.1999999999999995E-2,0,0,229482,16522.7,0,0,229482,16522.7,null,null,"N","N","",1]
["MQC10010010S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",3.5999999999999997E-2,0,0,214222,7711.9,0,0,214222,7711.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,24234,0,0,0,24234,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC10010020S",null,null,null,"관갱생공","D20mm","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC10010020S","노무","L001010101000039",null,"배관공","일반공사 직종","인",7.1999999999999995E-2,0,0,229482,16522.7,0,0,229482,16522.7,null,null,"N","N","",1]
["MQC10010020S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",3.5999999999999997E-2,0,0,214222,7711.9,0,0,214222,7711.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,24234,0,0,0,24234,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC10010030S",null,null,null,"관갱생공","D25mm","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC10010030S","노무","L001010101000039",null,"배관공","일반공사 직종","인",7.1999999999999995E-2,0,0,229482,16522.7,0,0,229482,16522.7,null,null,"N","N","",1]
["MQC10010030S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",3.5999999999999997E-2,0,0,214222,7711.9,0,0,214222,7711.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,24234,0,0,0,24234,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC10010040S",null,null,null,"관갱생공","D32mm","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC10010040S","노무","L001010101000039",null,"배관공","일반공사 직종","인",7.1999999999999995E-2,0,0,229482,16522.7,0,0,229482,16522.7,null,null,"N","N","",1]
["MQC10010040S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",3.5999999999999997E-2,0,0,214222,7711.9,0,0,214222,7711.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,24234,0,0,0,24234,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC10010050S",null,null,null,"관갱생공","D40mm","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC10010050S","노무","L001010101000039",null,"배관공","일반공사 직종","인",7.1999999999999995E-2,0,0,229482,16522.7,0,0,229482,16522.7,null,null,"N","N","",1]
["MQC10010050S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",3.5999999999999997E-2,0,0,214222,7711.9,0,0,214222,7711.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,24234,0,0,0,24234,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC10010060S",null,null,null,"관갱생공","D50mm","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC10010060S","노무","L001010101000039",null,"배관공","일반공사 직종","인",7.1999999999999995E-2,0,0,229482,16522.7,0,0,229482,16522.7,null,null,"N","N","",1]
["MQC10010060S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",3.5999999999999997E-2,0,0,214222,7711.9,0,0,214222,7711.9,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,24234,0,0,0,24234,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC10010070S",null,null,null,"관갱생공","D65mm","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC10010070S","노무","L001010101000039",null,"배관공","일반공사 직종","인",8.1000000000000003E-2,0,0,229482,18588,0,0,229482,18588,null,null,"N","N","",1]
["MQC10010070S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",3.9E-2,0,0,214222,8354.6,0,0,214222,8354.6,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,26942,0,0,0,26942,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC10010080S",null,null,null,"관갱생공","D80mm","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC10010080S","노무","L001010101000039",null,"배관공","일반공사 직종","인",8.1000000000000003E-2,0,0,229482,18588,0,0,229482,18588,null,null,"N","N","",1]
["MQC10010080S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",3.9E-2,0,0,214222,8354.6,0,0,214222,8354.6,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,26942,0,0,0,26942,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC10010090S",null,null,null,"관갱생공","D100mm","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC10010090S","노무","L001010101000039",null,"배관공","일반공사 직종","인",8.1000000000000003E-2,0,0,229482,18588,0,0,229482,18588,null,null,"N","N","",1]
["MQC10010090S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",3.9E-2,0,0,214222,8354.6,0,0,214222,8354.6,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,26942,0,0,0,26942,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC10010100S",null,null,null,"관갱생공","D125mm","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC10010100S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.10100000000000001,0,0,229482,23177.599999999999,0,0,229482,23177.599999999999,null,null,"N","N","",1]
["MQC10010100S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.05,0,0,214222,10711.1,0,0,214222,10711.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,33888,0,0,0,33888,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC10010110S",null,null,null,"관갱생공","D150mm","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC10010110S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.10100000000000001,0,0,229482,23177.599999999999,0,0,229482,23177.599999999999,null,null,"N","N","",1]
["MQC10010110S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.05,0,0,214222,10711.1,0,0,214222,10711.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,33888,0,0,0,33888,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC10010120S",null,null,null,"관갱생공","D200mm","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC10010120S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.10100000000000001,0,0,229482,23177.599999999999,0,0,229482,23177.599999999999,null,null,"N","N","",1]
["MQC10010120S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",0.05,0,0,214222,10711.1,0,0,214222,10711.1,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,33888,0,0,0,33888,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC10010130S",null,null,null,"관갱생공","D250mm","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC10010130S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.111,0,0,229482,25472.5,0,0,229482,25472.5,null,null,"N","N","",1]
["MQC10010130S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",5.6000000000000001E-2,0,0,214222,11996.4,0,0,214222,11996.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,37468,0,0,0,37468,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC10010140S",null,null,null,"관갱생공","D300mm","m",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC10010140S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.111,0,0,229482,25472.5,0,0,229482,25472.5,null,null,"N","N","",1]
["MQC10010140S","노무","L001010101000003",null,"특별인부","일반공사 직종","인",5.6000000000000001E-2,0,0,214222,11996.4,0,0,214222,11996.4,null,null,"N","N","",1]
[null,null,null,null,"[합 계]",null,null,0,0,0,0,37468,0,0,0,37468,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC20010010S",null,null,null,"배관누수 검사","급수급탕난방용 옥내배관(D50mm이하)","회",0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]
["MQC20010010S","노무","L001010101000039",null,"배관공","일반공사 직종","인",0.71,0,0,229482,162932.20000000001,0,0,229482,162932.20000000001,null,null,"N","N","",1]
["MQC20010010S","손료","RENT000000000001",null,"공구손료및기계경비","노무비의 3%","식",1,4887.8999999999996,4887.8999999999996,0,0,0,0,4887.8999999999996,4887.8999999999996,null,null,"N","N",3,1]
[null,null,null,null,"[합 계]",null,null,0,0,4887,0,162932,0,0,0,167819,null,null,null,null,"",1]
[null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,null,null,null,null,"",1]