{"text_format":"1","workbook":"xlsx","n_sheets":25,"sheets":["Pipes","Data pipe acc ASA","Data pipe acc. DIN","Data SS pipe","Data Castiron pipe","WN Flanges","Data WN flanges","Blind & Slip-on fl.","Data Slip-on & Bl.fl.","Lapjoint fl.","Data Lapjoint fl.","Data Stub-Collar","Orifice fl.","Data Orifice fl.","Fittings","Data fittings","Red. fittings","Data red. fittings","Swage nipples","Data swage nipples","Weldolets","Data weldolets","Tolerences","Details & facing","Attributes"],"not_rendered":{"charts":0,"images":85,"macros":1,"external_links":1,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Pipes","index":0,"n_rows":193,"n_cols":40,"rows_kept":193,"cut":false,"hidden":true,"merged":[[0,0,0,8]]}
["PIPE DIMENSIONS CS & SS"]
[]
["Dimensions acc. ANSI",null,null,null,null,"Nominal Pipe Size:"]
["do","Pipe ø outside",{"$f":"INDEX($D$88:$D$123,A88)","v":660.4},"mm"]
["di","Pipe ø inside",{"$f":"C4-(2*C6)","v":"#VALUE!"},"mm"]
["s","Pipe wallthkn.",{"$f":"INDEX(B87:V123,MATCH(C4,D87:D123, ),MATCH(H6,B87:V87, ))","v":"-"},"mm",null,"Pipe schedule:",null,"80"]
["A","Pipe section",{"$f":"(PI()/4*(C4^2-C5^2))/100","v":"#VALUE!"},"cm²",null,"Capacity","v = (m/s)"]
["O","Circumference",{"$f":"PI()*C4","v":2074.707788},"mm",null,"C1",0.5,{"$f":"($C$5/1000)^2*PI()/4*0.5*3600","v":"#VALUE!"},"m³/h"]
["S","Surface",{"$f":"C8/1000","v":2.074707788},"m²/m¹",null,"C2",1.0,{"$f":"($C$5/1000)^2*PI()/4*1*3600","v":"#VALUE!"},"m³/h"]
["W1","Weight",{"$f":"C7/10*7.85","v":"#VALUE!"},"kg/m¹",null,"C3",1.5,{"$f":"($C$5/1000)^2*PI()/4*1.5*3600","v":"#VALUE!"},"m³/h"]
["W2","Weight full of water",{"$f":"((PI()/4*(C5/1000)^2)*1000)+C10","v":"#VALUE!"},"kg/m¹",null,"C4  Choose",1.5,{"$f":"H9*G11","v":"#VALUE!"},"m³/h"]
[]
[]
[]
["Dim. acc. DIN 2448 (seaml.)",null,null,null,null,"Diameter Nominal:"]
["do","Pipe ø outside",{"$f":"INDEX($D$128:$D$158,A128)","v":10.2},"mm"]
["di","Pipe ø inside",{"$f":"C16-(2*C18)","v":6.6},"mm"]
["s","Pipe wallthkn.",{"$f":"INDEX(B127:AN158,MATCH(C16,D127:D158, ),MATCH(H18,B127:AN127, ))","v":1.8},"mm",null,"Wallthickness (mm)",null,1.8]
["A","Pipe section",{"$f":"(PI()/4*(C16^2-C17^2))/100","v":0.4750088092},"cm²",null,"Capacity","v = (m/s)"]
["O","Circumference",{"$f":"PI()*C16","v":32.04424507},"mm",null,"C1",0.5,{"$f":"($C$17/1000)^2*PI()/4*0.5*3600","v":0.0615814992},"m³/h"]
["S","Surface",{"$f":"C20/1000","v":0.03204424507},"m²/m¹",null,"C2",1.0,{"$f":"($C$17/1000)^2*PI()/4*0.8*3600","v":0.09853039871},"m³/h"]
["W1","Weight",{"$f":"C19/10*7.85","v":0.3728819152},"kg/m¹",null,"C3",1.5,{"$f":"($C$17/1000)^2*PI()/4*3600","v":0.1231629984},"m³/h"]
["W2","Weight full of water",{"$f":"((PI()/4*(C17/1000)^2)*1000)+C22","v":0.4070938592},"kg/m¹",null,"C4  Choose",1.5,{"$f":"H21*G23","v":0.1477955981},"m³/h"]
[]
[]
[]
["Dim. acc. DIN 2458 (welded)",null,null,null,null,"Diameter Nominal:"]
["do","Pipe ø outside",{"$f":"INDEX($D$163:$D$193,A163)","v":13.5},"mm"]
["di","Pipe ø inside",{"$f":"C28-(2*C30)","v":6.3},"mm"]
["s","Pipe wallthkn.",{"$f":"INDEX(B162:AN193,MATCH(C28,D162:D193, ),MATCH(H30,B162:AN162, ))","v":3.6},"mm",null,"Wallthickness (mm)",null,3.6]
["A","Pipe section",{"$f":"(PI()/4*(C28^2-C29^2))/100","v":1.119663622},"cm²",null,"Capacity","v = (m/s)"]
["O","Circumference",{"$f":"PI()*C28","v":42.41150082},"mm",null,"C1",0.5,{"$f":"($C$29/1000)^2*PI()/4*0.5*3600","v":0.05611041559},"m³/h"]
["S","Surface",{"$f":"C32/1000","v":0.04241150082},"m²/m¹",null,"C2",1.0,{"$f":"($C$29/1000)^2*PI()/4*0.8*3600","v":0.08977666494},"m³/h"]
["W1","Weight",{"$f":"C31/10*7.85","v":0.8789359431},"kg/m¹",null,"C3",1.5,{"$f":"($C$29/1000)^2*PI()/4*3600","v":0.1122208312},"m³/h"]
["W2","Weight full of water",{"$f":"((PI()/4*(C29/1000)^2)*1000)+C34","v":0.9101083962},"kg/m¹",null,"C4  Choose",2.8,{"$f":"H33*G35","v":0.2513746618},"m³/h"]
[]
[]
["Dim. Stainless steel pipes",null,null,null,null,"Pipe dimensions (mm)"]
["do","Pipe ø outside",{"$f":"INDEX('Data SS pipe'!$C$3:$C$604,'Data SS pipe'!$A$3,'Data SS pipe'!$C$3)","v":1.59},"mm"]
["di","Pipe ø inside",{"$f":"INDEX('Data SS pipe'!$F$3:$F$604,'Data SS pipe'!$A$3,'Data SS pipe'!$F$3)","v":"#VALUE!"},"mm"]
["s","Pipe wallthkn.",{"$f":"INDEX('Data SS pipe'!$D$3:$D$604,'Data SS pipe'!$A$3,'Data SS pipe'!$D$3)","v":"#VALUE!"},"mm"]
["A","Pipe section",{"$f":"(PI()/4*(C39^2-C40^2))/100","v":"#VALUE!"},"cm²",null,"Capacity","v = (m/s)"]
["O","Circumference",{"$f":"PI()*C39","v":4.995132319},"mm",null,"C1",0.5,{"$f":"($C$40/1000)^2*PI()/4*0.5*3600","v":"#VALUE!"},"m³/h"]
["S","Surface",{"$f":"C43/1000","v":0.004995132319},"m²/m¹",null,"C2",1.0,{"$f":"($C$40/1000)^2*PI()/4*0.8*3600","v":"#VALUE!"},"m³/h"]
["W1","Weight",{"$f":"C42/10*7.85","v":"#VALUE!"},"kg/m¹",null,"C3",1.5,{"$f":"($C$40/1000)^2*PI()/4*3600","v":"#VALUE!"},"m³/h"]
["W2","Weight full of water",{"$f":"((PI()/4*(C40/1000)^2)*1000)+C45","v":"#VALUE!"},"kg/m¹",null,"C4  Choose",1.5,{"$f":"H44*G46","v":"#VALUE!"},"m³/h"]
[null,null,null,null,null,null,1.0]
[]
["Dim. Cast iron pipes",null,null,null,null,"Nominal Pipe Size:"]
["do","Pipe ø outside",{"$f":"INDEX('Data Castiron pipe'!I3:I115,'Data Castiron pipe'!A3)","v":96.52},"mm"]
["di","Pipe ø inside",{"$f":"INDEX('Data Castiron pipe'!L$3:L$115,'Data Castiron pipe'!$A$3)","v":76.708},"mm"]
["s","Pipe wallthkn.",{"$f":"INDEX('Data Castiron pipe'!K$3:K$115,'Data Castiron pipe'!$A$3)","v":9.906},"mm"]
["A","Pipe section",{"$f":"(PI()/4*(C50^2-C51^2))/100","v":26.95481106},"cm²",null,"Capacity","v = (m/s)"]
["O","Circumference",{"$f":"PI()*C50","v":303.2265229},"mm",null,"C1",0.5,{"$f":"($C$51/1000)^2*PI()/4*0.5*3600","v":8.318474806},"m³/h"]
["S","Surface",{"$f":"C54/1000","v":0.3032265229},"m²/m¹",null,"C2",1.0,{"$f":"($C$40/1000)^2*PI()/4*0.8*3600","v":"#VALUE!"},"m³/h"]
["W1","Weight",{"$f":"C53/10*7.85","v":21.15952668},"kg/m¹",null,"C3",1.5,{"$f":"($C$40/1000)^2*PI()/4*3600","v":"#VALUE!"},"m³/h"]
["W2","Weight full of water",{"$f":"((PI()/4*(C51/1000)^2)*1000)+C56","v":25.78090157},"kg/m¹",null,"C4  Choose",2.0,{"$f":"H56*G57","v":"#VALUE!"},"m³/h"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"PIPE   DATA acc ANSI B 16.5"]
[null,"NPS","DN","OD","5S","5","10S","10","20","30","40S","Std.",40.0,"60","80S","XS","80","100","120","140","160","XXS"]
[25.0,"1/8\"",6.0,10.29,"-","-","-","-","-","-",1.73,1.73,1.73,"-",2.41,2.41,2.41,"-","-","-","-","-"]
[null,"1/4\"",10.0,13.72,"-","-","-","-","-","-",2.24,2.24,2.24,"-",3.02,3.02,3.02,"-","-","-","-","-"]
[null,"3/8\"","-",17.15,"-","-","-","-","-","-",2.31,2.31,2.31,"-",3.2,3.2,3.2,"-","-","-","-","-"]
[null,"1/2\"",15.0,21.34,1.65,1.65,2.11,2.11,"-","-",2.77,2.77,2.77,"-",3.73,3.73,3.73,"-","-","-",4.75,7.47]
[null,"3/4\"",20.0,26.67,1.65,1.65,2.11,2.11,"-","-",2.87,2.87,2.87,"-",3.91,3.91,3.91,"-","-","-",5.54,7.82]
[null,"1\"",25.0,33.4,1.65,1.65,2.77,2.77,"-","-",3.38,3.38,3.38,"-",4.55,4.55,4.55,"-","-","-",6.35,9.09]
[null,"1¼\"",32.0,42.16,1.65,1.65,2.77,2.77,"-","-",3.56,3.56,3.56,"-",4.85,4.85,4.85,"-","-","-",6.35,9.7]
[null,"1½\"",40.0,48.26,1.65,1.65,2.77,2.77,"-","-",3.68,3.68,3.68,"-",5.08,5.08,5.08,"-","-","-",7.14,10.16]
[null,"2\"",50.0,60.33,1.65,1.65,2.77,2.77,"-","-",3.91,3.91,3.91,"-",5.54,5.54,5.54,"-","-","-",8.71,11.07]
[null,"2½\"",65.0,73.03,2.11,2.11,3.05,3.05,"-","-",5.16,5.16,5.16,"-",7.01,7.01,7.01,"-","-","-",9.53,14.02]
[null,"3\"",80.0,88.9,2.11,2.11,3.05,3.05,"-","-",5.49,5.49,5.49,"-",7.62,7.62,7.62,"-","-","-",11.13,15.24]
[null,"3½\"","-",101.6,2.11,2.11,3.05,3.05,"-","-",5.74,5.74,5.74,"-",8.08,8.08,8.08,"-","-","-","-",16.15]
[null,"4\"",100.0,114.3,2.11,2.11,3.05,3.05,"-","-",6.02,6.02,6.02,"-",8.56,8.56,8.56,"-",11.13,"-",13.49,17.12]
[null,"5\"",125.0,141.3,2.77,2.77,3.4,3.4,"-","-",6.55,6.55,6.55,"-",9.53,9.53,9.53,"-",12.7,"-",15.88,19.05]
[null,"6\"",150.0,168.28,2.77,2.77,3.4,3.4,"-","-",7.11,7.11,7.11,"-",10.97,10.97,10.97,"-",14.27,"-",18.24,21.95]
[null,"8\"",200.0,219.08,2.77,2.77,3.76,3.76,6.35,7.04,8.18,8.18,8.18,10.31,12.7,12.7,12.7,15.06,18.24,20.62,23.01,22.23]
[null,"10\"",250.0,273.05,3.4,3.4,4.19,4.19,6.35,7.8,9.27,9.27,9.27,12.7,12.7,12.7,15.06,18.24,21.41,25.4,28.58,25.4]
[null,"12\"",300.0,323.85,3.96,4.19,4.57,4.57,6.35,8.38,9.53,9.53,10.31,14.27,12.7,12.7,17.45,21.41,25.4,28.58,33.32,25.4]
[null,"14\"",350.0,355.6,3.96,"-",4.78,6.35,7.92,9.53,"-",9.53,11.13,15.06,"-",12.7,19.05,23.8,27.76,31.75,35.71,"-"]
[null,"16\"",400.0,406.4,4.19,"-",4.78,6.35,7.92,9.53,"-",9.53,12.7,16.66,"-",12.7,21.41,26.19,30.94,36.53,40.46,"-"]
[null,"18\"",450.0,457.2,4.19,"-",4.78,6.35,7.92,11.13,"-",9.53,14.27,19.05,"-",12.7,23.8,29.36,34.93,39.67,45.24,"-"]
[null,"20\"",500.0,508.0,4.78,"-",5.54,6.35,9.35,12.7,"-",9.53,15.06,20.62,"-",12.7,26.19,32.54,38.1,44.45,49.99,"-"]
[null,"22\"",550.0,558.8,4.78,"-",5.54,6.35,9.35,12.7,"-",9.53,15.88,22.23,"-",12.7,28.57,34.92,41.27,47.62,53.97,"-"]
[null,"24\"",600.0,609.6,5.54,"-",6.35,6.35,9.35,14.27,"-",9.53,17.45,24.59,"-",12.7,30.94,38.89,46.02,52.37,59.51,"-"]
[null,"26\"",650.0,660.4,"-","-","-",7.92,12.7,"-","-",9.53,"-","-","-",12.7,"-","-","-","-","-","-"]
[null,"28\"",700.0,711.2,"-","-","-",7.92,12.7,15.87,"-",9.53,"-","-","-",12.7,"-","-","-","-","-","-"]
[null,"30\"",750.0,762.0,"-","-","-",7.92,12.7,15.87,"-",9.53,"-","-","-",12.7,"-","-","-","-","-","-"]
[null,"32\"",800.0,812.8,"-","-","-",7.92,12.7,15.87,"-",9.53,17.45,"-","-",12.7,"-","-","-","-","-","-"]
[null,"34\"",850.0,863.6,"-","-","-",7.92,12.7,15.87,"-",9.53,17.45,"-","-",12.7,"-","-","-","-","-","-"]
[null,"36\"",900.0,914.4,"-","-","-",7.92,12.7,15.87,"-",9.53,19.05,"-","-",12.7,"-","-","-","-","-","-"]
[null,"38\"",950.0,965.2,"-","-","-","-","-","-","-",9.53,"-","-","-",12.7,"-","-","-","-","-","-"]
[null,"40\"",1000.0,1016.0,"-","-","-","-","-","-","-",9.53,"-","-","-",12.7,"-","-","-","-","-","-"]
[null,"42\"",1050.0,1066.8,"-","-","-","-","-","-","-",9.53,"-","-","-",12.7,"-","-","-","-","-","-"]
[null,"44\"",1100.0,1117.6,"-","-","-","-","-","-","-",9.53,"-","-","-",12.7,"-","-","-","-","-","-"]
[null,"46\"",1150.0,1168.4,"-","-","-","-","-","-","-",9.53,"-","-","-",12.7,"-","-","-","-","-","-"]
[null,"48\"",1200.0,1219.2,"-","-","-","-","-","-","-",9.53,"-","-","-",12.7,"-","-","-","-","-","-"]
[]
[]
[null,null,null,null,null,null,null,null,null,"WALLTHICKNESS  OF  SEAMLESS  PIPE  acc.  DIN 2448"]
[null,"NPS","DN","OD",1.4,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,40.0,45.0,50.0,55.0,60.0,65.0]
[1.0,"1/8\"","-",10.2,"-",1.6,1.8,2.0,2.3,2.6,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"1/4\"",10.0,13.5,"-","-",1.8,2.0,2.3,2.6,2.9,3.2,3.6,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"3/8\"","-",17.2,"-","-",1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"1/2\"",15.0,21.3,"-","-","-",2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"3/4\"",20.0,26.9,"-","-","-",2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"1\"",25.0,33.7,"-","-","-","-",2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"1¼\"",32.0,42.4,"-","-","-","-","-",2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"1½\"",40.0,48.3,"-","-","-","-","-",2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"2\"",50.0,60.3,"-","-","-","-","-","-",2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"2½\"",65.0,73.0,"-","-","-","-","-","-",2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,"-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"3\"",80.0,88.9,"-","-","-","-","-","-","-",3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,"-","-","-","-","-","-","-","-","-","-"]
[null,"3½\"","-",101.6,"-","-","-","-","-","-","-","-",3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,"-","-","-","-","-","-","-","-","-"]
[null,"4\"",100.0,114.3,"-","-","-","-","-","-","-","-",3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,"-","-","-","-","-","-","-"]
[null,"5\"",125.0,139.7,"-","-","-","-","-","-","-","-","-",4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,"-","-","-","-","-","-"]
[null,"6\"",150.0,168.3,"-","-","-","-","-","-","-","-","-","-",4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,40.0,45.0,50.0,"-","-","-"]
[null,"8\"",200.0,219.1,"-","-","-","-","-","-","-","-","-","-","-","-","-",6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,40.0,45.0,50.0,55.0,60.0,"-"]
[null,"10\"",250.0,273.0,"-","-","-","-","-","-","-","-","-","-","-","-","-",6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,40.0,45.0,50.0,55.0,60.0,65.0]
[null,"12\"",300.0,323.9,"-","-","-","-","-","-","-","-","-","-","-","-","-","-",7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,40.0,45.0,50.0,55.0,60.0,65.0]
[null,"14\"",350.0,355.6,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,40.0,45.0,50.0,55.0,60.0,65.0]
[null,"16\"",400.0,406.4,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,40.0,45.0,50.0,55.0,60.0,65.0]
[null,"18\"",450.0,457.0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,40.0,45.0,50.0,55.0,60.0,65.0]
[null,"20\"",500.0,508.0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,40.0,45.0,50.0,55.0,60.0,65.0]
[null,"22\"",550.0,559.0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,40.0,45.0,50.0,55.0,60.0,65.0]
[null,"24\"",600.0,610.0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,40.0,45.0,50.0,55.0,60.0,65.0]
[null,"28\"",700.0,711.0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"32\"",800.0,813.0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"36\"",900.0,914.0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"40\"",1000.0,1016.0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"48\"",1200.0,1220.0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"56\"",1400.0,1420.0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"64\"",1600.0,1620.0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[]
[]
[null,null,null,null,null,null,null,null,null,"WALLTHICKNESS  OF  WELDED  PIPE  acc.  DIN 2458"]
[null,"NPS","DN","OD",1.4,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,40.0,45.0,50.0,55.0,60.0,65.0]
[2.0,"1/8\"","-",10.2,1.4,1.6,1.8,2.0,2.3,2.6,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"1/4\"",10.0,13.5,1.4,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"3/8\"","-",17.2,1.4,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"1/2\"",15.0,21.3,1.4,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"3/4\"",20.0,26.9,1.4,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"1\"",25.0,33.7,1.4,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"1¼\"",32.0,42.4,1.4,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"1½\"",40.0,48.3,1.4,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"2\"",50.0,60.3,1.4,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"2½\"",65.0,73.0,"-",1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"3\"",80.0,88.9,"-",1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"3½\"","-",101.6,"-","-","-",2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"4\"",100.0,114.3,"-","-","-",2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"5\"",125.0,139.7,"-","-","-",2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"6\"",150.0,168.3,"-","-","-","-","-","-",2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"8\"",200.0,219.1,"-","-","-","-","-","-","-",3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"10\"",250.0,273.0,"-","-","-","-","-","-","-",3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"12\"",300.0,323.9,"-","-","-","-","-","-","-",3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"14\"",350.0,355.6,"-","-","-","-","-","-","-",3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"16\"",400.0,406.4,"-","-","-","-","-","-","-","-",3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"18\"",450.0,457.0,"-","-","-","-","-","-","-","-",3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"20\"",500.0,508.0,"-","-","-","-","-","-","-","-",3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"22\"",550.0,559.0,"-","-","-","-","-","-","-","-","-","-",4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,"-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"24\"",600.0,610.0,"-","-","-","-","-","-","-","-","-","-",4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,"-","-","-","-","-","-","-","-","-"]
[null,"28\"",700.0,711.0,"-","-","-","-","-","-","-","-","-","-","-",5.0,"-","-",7.1,"-","-","-","-",12.5,"-","-","-",20.0,"-","-","-","-",32.0,"-","-","-","-","-","-","-"]
[null,"32\"",800.0,813.0,"-","-","-","-","-","-","-","-","-","-","-","-",5.6,"-","-",8.0,"-","-","-",12.5,"-","-","-","-",22.2,"-","-","-","-",36.0,"-","-","-","-","-","-"]
[null,"36\"",900.0,914.0,"-","-","-","-","-","-","-","-","-","-","-","-","-",6.3,"-","-","-",10.0,6.0,12.5,"-","-","-","-","-",25.0,"-","-","-","-",40.0,"-","-","-","-","-"]
[null,"40\"",1000.0,1016.0,"-","-","-","-","-","-","-","-","-","-","-","-","-",6.3,"-","-","-",10.0,"-",12.5,"-","-","-","-","-","-",28.0,"-","-","-","-",45.0,"-","-","-","-"]
[null,"48\"",1200.0,1220.0,"-","-","-","-","-","-","-","-","-","-","-","-","-",6.3,"-","-","-",10.0,"-",12.5,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"56\"",1400.0,1420.0,"-","-","-","-","-","-","-","-","-","-","-","-","-",6.3,"-","-","-",10.0,"-",12.5,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"64\"",1600.0,1620.0,"-","-","-","-","-","-","-","-","-","-","-","-","-",6.3,"-","-","-",10.0,"-",12.5,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]

{"sheet":"Data pipe acc ASA","index":1,"n_rows":38,"n_cols":22,"rows_kept":38,"cut":false,"hidden":true,"merged":[[0,1,0,21]]}
[null,"PIPE   DATA acc ANSI B 16.5"]
[null,"NPS","DN","OD","5S","5","10S","10","20","30","40S","Std.",40.0,"60","80S","XS","80","100","120","140","160","XXS"]
[1.0,"1/8\"",6.0,10.29,"-","-","-","-","-","-",1.73,1.73,1.73,"-",2.41,2.41,2.41,"-","-","-","-","-"]
[null,"1/4\"",10.0,13.72,"-","-","-","-","-","-",2.24,2.24,2.24,"-",3.02,3.02,3.02,"-","-","-","-","-"]
[null,"3/8\"","-",17.15,"-","-","-","-","-","-",2.31,2.31,2.31,"-",3.2,3.2,3.2,"-","-","-","-","-"]
[null,"1/2\"",15.0,21.34,1.65,1.65,2.11,2.11,"-","-",2.77,2.77,2.77,"-",3.73,3.73,3.73,"-","-","-",4.75,7.47]
[null,"3/4\"",20.0,26.67,1.65,1.65,2.11,2.11,"-","-",2.87,2.87,2.87,"-",3.91,3.91,3.91,"-","-","-",5.54,7.82]
[null,"1\"",25.0,33.4,1.65,1.65,2.77,2.77,"-","-",3.38,3.38,3.38,"-",4.55,4.55,4.55,"-","-","-",6.35,9.09]
[null,"1¼\"",32.0,42.16,1.65,1.65,2.77,2.77,"-","-",3.56,3.56,3.56,"-",4.85,4.85,4.85,"-","-","-",6.35,9.7]
[null,"1½\"",40.0,48.26,1.65,1.65,2.77,2.77,"-","-",3.68,3.68,3.68,"-",5.08,5.08,5.08,"-","-","-",7.14,10.16]
[null,"2\"",50.0,60.33,1.65,1.65,2.77,2.77,"-","-",3.91,3.91,3.91,"-",5.54,5.54,5.54,"-","-","-",8.71,11.07]
[null,"2½\"",65.0,73.03,2.11,2.11,3.05,3.05,"-","-",5.16,5.16,5.16,"-",7.01,7.01,7.01,"-","-","-",9.53,14.02]
[null,"3\"",80.0,88.9,2.11,2.11,3.05,3.05,"-","-",5.49,5.49,5.49,"-",7.62,7.62,7.62,"-","-","-",11.13,15.24]
[null,"3½\"","-",101.6,2.11,2.11,3.05,3.05,"-","-",5.74,5.74,5.74,"-",8.08,8.08,8.08,"-","-","-","-",16.15]
[null,"4\"",100.0,114.3,2.11,2.11,3.05,3.05,"-","-",6.02,6.02,6.02,"-",8.56,8.56,8.56,"-",11.13,"-",13.49,17.12]
[null,"5\"",125.0,141.3,2.77,2.77,3.4,3.4,"-","-",6.55,6.55,6.55,"-",9.53,9.53,9.53,"-",12.7,"-",15.88,19.05]
[null,"6\"",150.0,168.28,2.77,2.77,3.4,3.4,"-","-",7.11,7.11,7.11,"-",10.97,10.97,10.97,"-",14.27,"-",18.24,21.95]
[null,"8\"",200.0,219.08,2.77,2.77,3.76,3.76,6.35,7.04,8.18,8.18,8.18,10.31,12.7,12.7,12.7,15.06,18.24,20.62,23.01,22.23]
[null,"10\"",250.0,273.05,3.4,3.4,4.19,4.19,6.35,7.8,9.27,9.27,9.27,12.7,12.7,12.7,15.06,18.24,21.41,25.4,28.58,25.4]
[null,"12\"",300.0,323.85,3.96,4.19,4.57,4.57,6.35,8.38,9.53,9.53,10.31,14.27,12.7,12.7,17.45,21.41,25.4,28.58,33.32,25.4]
[null,"14\"",350.0,355.6,3.96,"-",4.78,6.35,7.92,9.53,"-",9.53,11.13,15.06,"-",12.7,19.05,23.8,27.76,31.75,35.71,"-"]
[null,"16\"",400.0,406.4,4.19,"-",4.78,6.35,7.92,9.53,"-",9.53,12.7,16.66,"-",12.7,21.41,26.19,30.94,36.53,40.46,"-"]
[null,"18\"",450.0,457.2,4.19,"-",4.78,6.35,7.92,11.13,"-",9.53,14.27,19.05,"-",12.7,23.8,29.36,34.93,39.67,45.24,"-"]
[null,"20\"",500.0,508.0,4.78,"-",5.54,6.35,9.35,12.7,"-",9.53,15.06,20.62,"-",12.7,26.19,32.54,38.1,44.45,49.99,"-"]
[null,"22\"",550.0,558.8,4.78,"-",5.54,6.35,9.35,12.7,"-",9.53,15.88,22.23,"-",12.7,28.57,34.92,41.27,47.62,53.97,"-"]
[null,"24\"",600.0,609.6,5.54,"-",6.35,6.35,9.35,14.27,"-",9.53,17.45,24.59,"-",12.7,30.94,38.89,46.02,52.37,59.51,"-"]
[null,"26\"",650.0,660.4,"-","-","-",7.92,12.7,"-","-",9.53,"-","-","-",12.7,"-","-","-","-","-","-"]
[null,"28\"",700.0,711.2,"-","-","-",7.92,12.7,15.87,"-",9.53,"-","-","-",12.7,"-","-","-","-","-","-"]
[null,"30\"",750.0,762.0,"-","-","-",7.92,12.7,15.87,"-",9.53,"-","-","-",12.7,"-","-","-","-","-","-"]
[null,"32\"",800.0,812.8,"-","-","-",7.92,12.7,15.87,"-",9.53,17.45,"-","-",12.7,"-","-","-","-","-","-"]
[null,"34\"",850.0,863.6,"-","-","-",7.92,12.7,15.87,"-",9.53,17.45,"-","-",12.7,"-","-","-","-","-","-"]
[null,"36\"",900.0,914.4,"-","-","-",7.92,12.7,15.87,"-",9.53,19.05,"-","-",12.7,"-","-","-","-","-","-"]
[null,"38\"",950.0,965.2,"-","-","-","-","-","-","-",9.53,"-","-","-",12.7,"-","-","-","-","-","-"]
[null,"40\"",1000.0,1016.0,"-","-","-","-","-","-","-",9.53,"-","-","-",12.7,"-","-","-","-","-","-"]
[null,"42\"",1050.0,1066.8,"-","-","-","-","-","-","-",9.53,"-","-","-",12.7,"-","-","-","-","-","-"]
[null,"44\"",1100.0,1117.6,"-","-","-","-","-","-","-",9.53,"-","-","-",12.7,"-","-","-","-","-","-"]
[null,"46\"",1150.0,1168.4,"-","-","-","-","-","-","-",9.53,"-","-","-",12.7,"-","-","-","-","-","-"]
[null,"48\"",1200.0,1219.2,"-","-","-","-","-","-","-",9.53,"-","-","-",12.7,"-","-","-","-","-","-"]

{"sheet":"Data pipe acc. DIN","index":2,"n_rows":33,"n_cols":89,"rows_kept":33,"cut":false,"hidden":true,"merged":[[0,3,0,39],[0,44,0,66],[0,70,0,88]]}
[null,null,null,"WALLTHICKNESS  OF  SEAMLESS  AND  WELDED  PIPE  acc.  DIN 2448  /   DIN 2458",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SEAMLESS PIPE acc. DIN 2448",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WELDED PIPE acc. DIN 2458"]
[null,"NPS","DN","OD",1.4,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,40.0,45.0,50.0,55.0,60.0,65.0,null,null,"NPS","DN","OD",null,null,null,null,null,null,null,null,null,null,"WALLTHICKNESS",null,null,null,null,null,null,null,null,null,null,null,null,"NPS","DN","OD",null,null,null,null,null,null,null,null,"WALLTHICKNESS"]
[1.0,"1/8\"","-",10.2,1.4,1.6,1.8,2.0,2.3,2.6,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,null,"1/8\"","-",10.2,1.6,1.8,2.0,2.3,2.6,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,"1/8\"","-",10.2,1.4,1.6,1.8,2.0,2.3,2.6,"-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"1/4\"",10.0,13.5,1.4,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,null,"1/4\"",10.0,13.5,1.8,2.0,2.3,2.6,2.9,3.2,3.6,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,"1/4\"",10.0,13.5,1.4,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,"-","-","-","-","-","-","-","-","-"]
[null,"3/8\"","-",17.2,1.4,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,null,"3/8\"","-",17.2,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,"-","-","-","-","-","-","-","-","-","-","-","-","-",null,"3/8\"","-",17.2,1.4,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,"-","-","-","-","-","-","-","-"]
[null,"1/2\"",15.0,21.3,1.4,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,null,"1/2\"",15.0,21.3,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,"-","-","-","-","-","-","-","-","-","-","-","-","-",null,"1/2\"",15.0,21.3,1.4,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,"-","-","-","-","-","-","-"]
[null,"3/4\"",20.0,26.9,1.4,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,null,"3/4\"",20.0,26.9,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,"-","-","-","-","-","-","-","-","-","-",null,"3/4\"",20.0,26.9,1.4,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,"-","-","-","-","-","-"]
[null,"1\"",25.0,33.7,1.4,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,null,"1\"",25.0,33.7,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,"-","-","-","-","-","-","-","-","-",null,"1\"",25.0,33.7,1.4,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,"-","-"]
[null,"1¼\"",32.0,42.4,1.4,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,null,"1¼\"",32.0,42.4,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,"-","-","-","-","-","-","-","-","-",null,"1¼\"",32.0,42.4,1.4,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,"-"]
[null,"1½\"",40.0,48.3,1.4,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,null,"1½\"",40.0,48.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,"-","-","-","-","-","-","-",null,"1½\"",40.0,48.3,1.4,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,"-"]
[null,"2\"",50.0,60.3,1.4,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,null,"2\"",50.0,60.3,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,"-","-","-","-","-","-",null,"2\"",50.0,60.3,1.4,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0]
[null,"2½\"",65.0,73.0,"-",1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,"-","-","-","-","-","-","-","-","-","-","-","-","-",null,null,"2½\"",65.0,73.0,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,"-","-","-","-","-",null,"2½\"",65.0,73.0,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,"-"]
[null,"3\"",80.0,88.9,"-",1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,"-","-","-","-","-","-","-","-","-","-",null,null,"3\"",80.0,88.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,"-","-","-",null,"3\"",80.0,88.9,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,"-"]
[null,"3½\"","-",101.6,"-","-","-",2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,"-","-","-","-","-","-","-","-","-",null,null,"3½\"","-",101.6,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,"-","-","-",null,"3½\"","-",101.6,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,"-","-","-"]
[null,"4\"",100.0,114.3,"-","-","-",2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,"-","-","-","-","-","-","-",null,null,"4\"",100.0,114.3,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,"-",null,"4\"",100.0,114.3,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,"-","-"]
[null,"5\"",125.0,139.7,"-","-","-",2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,"-","-","-","-","-","-",null,null,"5\"",125.0,139.7,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,"-",null,"5\"",125.0,139.7,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,"-","-"]
[null,"6\"",150.0,168.3,"-","-","-","-","-","-",2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,40.0,45.0,50.0,"-","-","-",null,null,"6\"",150.0,168.3,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,40.0,45.0,null,"6\"",150.0,168.3,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,"-","-","-","-","-"]
[null,"8\"",200.0,219.1,"-","-","-","-","-","-","-",3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,40.0,45.0,50.0,55.0,60.0,"-",null,null,"8\"",200.0,219.1,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,40.0,45.0,50.0,55.0,60.0,"-",null,"8\"",200.0,219.1,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,"-","-","-","-","-"]
[null,"10\"",250.0,273.0,"-","-","-","-","-","-","-",3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,40.0,45.0,50.0,55.0,60.0,65.0,null,null,"10\"",250.0,273.0,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,40.0,45.0,50.0,55.0,60.0,65.0,null,"10\"",250.0,273.0,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,"-","-","-","-","-"]
[null,"12\"",300.0,323.9,"-","-","-","-","-","-","-",3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,40.0,45.0,50.0,55.0,60.0,65.0,null,null,"12\"",300.0,323.9,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,40.0,45.0,50.0,55.0,60.0,65.0,"-",null,"12\"",300.0,323.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,"-","-","-","-","-"]
[null,"14\"",350.0,355.6,"-","-","-","-","-","-","-",3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,40.0,45.0,50.0,55.0,60.0,65.0,null,null,"14\"",350.0,355.6,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,40.0,45.0,50.0,55.0,60.0,65.0,"-","-",null,"14\"",350.0,355.6,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,"-","-","-","-","-"]
[null,"16\"",400.0,406.4,"-","-","-","-","-","-","-","-",3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,40.0,45.0,50.0,55.0,60.0,65.0,null,null,"16\"",400.0,406.4,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,40.0,45.0,50.0,55.0,60.0,65.0,"-","-","-",null,"16\"",400.0,406.4,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,"-","-","-","-","-","-"]
[null,"18\"",450.0,457.0,"-","-","-","-","-","-","-","-",3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,40.0,45.0,50.0,55.0,60.0,65.0,null,null,"18\"",450.0,457.0,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,40.0,45.0,50.0,55.0,60.0,65.0,"-","-","-","-",null,"18\"",450.0,457.0,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,"-","-","-","-","-","-"]
[null,"20\"",500.0,508.0,"-","-","-","-","-","-","-","-",3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,40.0,45.0,50.0,55.0,60.0,65.0,null,null,"20\"",500.0,508.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,40.0,45.0,50.0,55.0,60.0,65.0,"-","-","-","-","-",null,"20\"",500.0,508.0,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,"-","-","-","-"]
[null,"22\"",550.0,559.0,"-","-","-","-","-","-","-","-","-","-",4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,40.0,45.0,50.0,55.0,60.0,65.0,null,null,"22\"",550.0,559.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,40.0,45.0,50.0,55.0,60.0,65.0,"-","-","-","-","-","-",null,"22\"",550.0,559.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,"-","-","-","-"]
[null,"24\"",600.0,610.0,"-","-","-","-","-","-","-","-","-","-",4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,40.0,45.0,50.0,55.0,60.0,65.0,null,null,"24\"",600.0,610.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,40.0,45.0,50.0,55.0,60.0,65.0,"-","-","-","-","-","-",null,"24\"",600.0,610.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,"-"]
[null,"28\"",700.0,711.0,"-","-","-","-","-","-","-","-","-","-","-",5.0,"-","-",7.1,"-","-","-","-",12.5,"-","-","-",20.0,"-","-","-","-",32.0,"-","-","-","-","-","-","-"]
[null,"32\"",800.0,813.0,"-","-","-","-","-","-","-","-","-","-","-","-",5.6,"-","-",8.0,"-","-","-",12.5,"-","-","-","-",22.2,"-","-","-","-",36.0,"-","-","-","-","-","-"]
[null,"36\"",900.0,914.0,"-","-","-","-","-","-","-","-","-","-","-","-","-",6.3,"-","-","-",10.0,"-",12.5,"-","-","-","-","-",25.0,"-","-","-","-",40.0,"-","-","-","-","-"]
[null,"40\"",1000.0,1016.0,"-","-","-","-","-","-","-","-","-","-","-","-","-",6.3,"-","-","-",10.0,"-",12.5,"-","-","-","-","-","-",28.0,"-","-","-","-",45.0,"-","-","-","-"]
[null,"48\"",1200.0,1220.0,"-","-","-","-","-","-","-","-","-","-","-","-","-",6.3,"-","-","-",10.0,"-",12.5,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"56\"",1400.0,1420.0,"-","-","-","-","-","-","-","-","-","-","-","-","-",6.3,"-","-","-",10.0,"-",12.5,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"64\"",1600.0,1620.0,"-","-","-","-","-","-","-","-","-","-","-","-","-",6.3,"-","-","-",10.0,"-",12.5,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]

{"sheet":"Data SS pipe","index":3,"n_rows":604,"n_cols":6,"rows_kept":604,"cut":false,"hidden":true,"merged":[]}
["Data Stainless steel pipes",null,"Diameter","Wall","Size and schedule","Diameter"]
[null,"  x  ","outside","thickness",null,"inside"]
[1.0,{"$f":"CONCATENATE(C3,$B$2,D3,E3)","v":"1.59  x  0,51   (1/18\" OD)"},1.59,"0,51","   (1/18\" OD)",{"$f":"C3-D3*2","v":"#VALUE!"}]
[null,"3,00  x  1,00","3,00","1,00",null,"#VALUE!"]
[null,"3.18  x  0.51   (1/8\" OD)",3.18,0.51,"   (1/8\" OD)",2.16]
[null,"3.18  x  0.71   (1/8\" OD)",3.18,0.71,"   (1/8\" OD)",1.76]
[null,"3.18  x  0.89   (1/8\" OD)",3.18,0.89,"   (1/8\" OD)",1.4]
[null,"4,00  x  0,50","4,00","0,50",null,"#VALUE!"]
[null,"4,00  x  1,00","4,00","1,00",null,"#VALUE!"]
[null,"4.76  x  0,71   (3/16\" OD)",4.76,"0,71","   (3/16\" OD)","#VALUE!"]
[null,"4.76  x  0.89   (3/16\" OD)",4.76,0.89,"   (3/16\" OD)",2.98]
[null,"4.76  x  1,24   (3/16\" OD)",4.76,"1,24","   (3/16\" OD)","#VALUE!"]
[null,"5,00  x  0,50","5,00","0,50",null,"#VALUE!"]
[null,"5,00  x  1,00","5,00","1,00",null,"#VALUE!"]
[null,"6,00  x  0,50","6,00","0,50",null,"#VALUE!"]
[null,"6,00  x  1,00","6,00","1,00",null,"#VALUE!"]
[null,"6,00  x  1,50","6,00","1,50",null,"#VALUE!"]
[null,"6,00  x  2,00","6,00","2,00",null,"#VALUE!"]
[null,"6,35  x  0,51   (1/4\" OD)","6,35","0,51","   (1/4\" OD)","#VALUE!"]
[null,"6.35  x  0.71   (1/4\" OD)",6.35,0.71,"   (1/4\" OD)",4.93]
[null,"6.35  x  0.89   (1/4\" OD)",6.35,0.89,"   (1/4\" OD)",4.57]
[null,"6.35  x  1.24   (1/4\" OD)",6.35,1.24,"   (1/4\" OD)",3.87]
[null,"6.35  x  1.65   (1/4\" OD)",6.35,1.65,"   (1/4\" OD)",3.05]
[null,"6.35  x  2,03   (1/4\" OD)",6.35,"2,03","   (1/4\" OD)","#VALUE!"]
[null,"8,00  x  0,50","8,00","0,50",null,"#VALUE!"]
[null,"8,00  x  1,00","8,00","1,00",null,"#VALUE!"]
[null,"8,00  x  1,50","8,00","1,50",null,"#VALUE!"]
[null,"8,00  x  2,00","8,00","2,00",null,"#VALUE!"]
[null,"8,00  x  2,50","8,00","2,50",null,"#VALUE!"]
[null,"9,00  x  1,00","9,00","1,00",null,"#VALUE!"]
[null,"9.53  x  0.71   (3/8\" OD)",9.53,0.71,"   (3/8\" OD)",8.11]
[null,"9.53  x  0.89   (3/8\" OD)",9.53,0.89,"   (3/8\" OD)",7.75]
[null,"9.53  x  1.24   (3/8\" OD)",9.53,1.24,"   (3/8\" OD)",7.05]
[null,"9.53  x  1.65   (3/8\" OD)",9.53,1.65,"   (3/8\" OD)",6.23]
[null,"10,00  x  0,50","10,00","0,50",null,"#VALUE!"]
[null,"10,00  x  0,60","10,00","0,60",null,"#VALUE!"]
[null,"10,00  x  1,00","10,00","1,00",null,"#VALUE!"]
[null,"10,00  x  1,50","10,00","1,50",null,"#VALUE!"]
[null,"10,00  x  2,00","10,00","2,00",null,"#VALUE!"]
[null,"10,00  x  2,50","10,00","2,50",null,"#VALUE!"]
[null,"10,20  x  1,60","10,20","1,60",null,"#VALUE!"]
[null,"10,20  x  2,00   ISO 1/8\" Gas","10,20","2,00","   ISO 1/8\" Gas","#VALUE!"]
[null,"10,20  x  2,00   ISO","10,20","2,00","   ISO","#VALUE!"]
[null,"10,29  x  1,24   1/8\" sched 10S","10,29","1,24","   1/8\" sched 10S","#VALUE!"]
[null,"10,29  x  1,73   1/8\" sched 40S","10,29","1,73","   1/8\" sched 40S","#VALUE!"]
[null,"10,29  x  2,41   1/8\" sched 80S","10,29","2,41","   1/8\" sched 80S","#VALUE!"]
[null,"11,00  x  1,00","11,00","1,00",null,"#VALUE!"]
[null,"11,00  x  1,50","11,00","1,50",null,"#VALUE!"]
[null,"11,00  x  2,00","11,00","2,00",null,"#VALUE!"]
[null,"12,00  x  0,60","12,00","0,60",null,"#VALUE!"]
[null,"12,00  x  1,00","12,00","1,00",null,"#VALUE!"]
[null,"12,00  x  1,50","12,00","1,50",null,"#VALUE!"]
[null,"12,00  x  2,00","12,00","2,00",null,"#VALUE!"]
[null,"12,00  x  2,50","12,00","2,50",null,"#VALUE!"]
[null,"12,00  x  3,00","12,00","3,00",null,"#VALUE!"]
[null,"12,00  x  4,00","12,00","4,00",null,"#VALUE!"]
[null,"12,70  x  0,71   (1/2\" OD)","12,70","0,71","   (1/2\" OD)","#VALUE!"]
[null,"12,70  x  0,89   (1/2\" OD)","12,70","0,89","   (1/2\" OD)","#VALUE!"]
[null,"12,70  x  1,24   (1/2\" OD)","12,70","1,24","   (1/2\" OD)","#VALUE!"]
[null,"12,70  x  1,65   (1/2\" OD)","12,70","1,65","   (1/2\" OD)","#VALUE!"]
[null,"12,70  x  2,03   (1/2\" OD)","12,70","2,03","   (1/2\" OD)","#VALUE!"]
[null,"12,70  x  2,11   (1/2\" OD)","12,70","2,11","   (1/2\" OD)","#VALUE!"]
[null,"13,00  x  1,00","13,00","1,00",null,"#VALUE!"]
[null,"13,00  x  1,50","13,00","1,50",null,"#VALUE!"]
[null,"13,50  x  1,60   ISO","13,50","1,60","   ISO","#VALUE!"]
[null,"13,50  x  2,00   ISO","13,50","2,00","   ISO","#VALUE!"]
[null,"13,50  x  2,35   ISO 1/4\" Gas","13,50","2,35","   ISO 1/4\" Gas","#VALUE!"]
[null,"13,72  x  1,65   1/4\" sched 10S","13,72","1,65","   1/4\" sched 10S","#VALUE!"]
[null,"13,72  x  2,24   1/4\" sched 40S","13,72","2,24","   1/4\" sched 40S","#VALUE!"]
[null,"13,72  x  3,02   1/4\" sched 80S","13,72","3,02","   1/4\" sched 80S","#VALUE!"]
[null,"14,00  x  1,00","14,00","1,00",null,"#VALUE!"]
[null,"14,00  x  1,50","14,00","1,50",null,"#VALUE!"]
[null,"14,00  x  2,00","14,00","2,00",null,"#VALUE!"]
[null,"14,00  x  2,50","14,00","2,50",null,"#VALUE!"]
[null,"14,00  x  3,00","14,00","3,00",null,"#VALUE!"]
[null,"15,00  x  0,60","15,00","0,60",null,"#VALUE!"]
[null,"15,00  x  1,00","15,00","1,00",null,"#VALUE!"]
[null,"15,00  x  1,50","15,00","1,50",null,"#VALUE!"]
[null,"15,00  x  2,00","15,00","2,00",null,"#VALUE!"]
[null,"15,00  x  2,50","15,00","2,50",null,"#VALUE!"]
[null,"15,00  x  3,00","15,00","3,00",null,"#VALUE!"]
[null,"15,00  x  4,00","15,00","4,00",null,"#VALUE!"]
[null,"15,88  x  0,89   (5/8\" OD)","15,88","0,89","   (5/8\" OD)","#VALUE!"]
[null,"15,88  x  1,24   (5/8\" OD)","15,88","1,24","   (5/8\" OD)","#VALUE!"]
[null,"15,88  x  1,65   (5/8\" OD)","15,88","1,65","   (5/8\" OD)","#VALUE!"]
[null,"15,88  x  2,11   (5/8\" OD)","15,88","2,11","   (5/8\" OD)","#VALUE!"]
[null,"16,00  x  1,00","16,00","1,00",null,"#VALUE!"]
[null,"16,00  x  1,50","16,00","1,50",null,"#VALUE!"]
[null,"16,00  x  2,00","16,00","2,00",null,"#VALUE!"]
[null,"16,00  x  2,50","16,00","2,50",null,"#VALUE!"]
[null,"16,00  x  3,00","16,00","3,00",null,"#VALUE!"]
[null,"16,00  x  4,00","16,00","4,00",null,"#VALUE!"]
[null,"17,00  x  1,00","17,00","1,00",null,"#VALUE!"]
[null,"17,00  x  1,50","17,00","1,50",null,"#VALUE!"]
[null,"17,00  x  3,00","17,00","3,00",null,"#VALUE!"]
[null,"17,15  x  1,65   3/8\" sched 10S","17,15","1,65","   3/8\" sched 10S","#VALUE!"]
[null,"17,15  x  2,31   3/8\" sched 40S","17,15","2,31","   3/8\" sched 40S","#VALUE!"]
[null,"17,15  x  3,20   3/8\" sched 80S","17,15","3,20","   3/8\" sched 80S","#VALUE!"]
[null,"17,20  x  1,50","17,20","1,50",null,"#VALUE!"]
[null,"17,20  x  1,60   ISO","17,20","1,60","   ISO","#VALUE!"]
[null,"17,20  x  2,00","17,20","2,00",null,"#VALUE!"]
[null,"17,20  x  2,30","17,20","2,30",null,"#VALUE!"]
[null,"17,20  x  2,90","17,20","2,90",null,"#VALUE!"]
[null,"17,20  x  3,20","17,20","3,20",null,"#VALUE!"]
[null,"18,00  x  0,70","18,00","0,70",null,"#VALUE!"]
[null,"18,00  x  1,00   ISO","18,00","1,00","   ISO","#VALUE!"]
[null,"18,00  x  1,50   ISO 3/8\" Gas","18,00","1,50","   ISO 3/8\" Gas","#VALUE!"]
[null,"18,00  x  2,00","18,00","2,00",null,"#VALUE!"]
[null,"18,00  x  2,50","18,00","2,50",null,"#VALUE!"]
[null,"18,00  x  3,00","18,00","3,00",null,"#VALUE!"]
[null,"18,00  x  4,00","18,00","4,00",null,"#VALUE!"]
[null,"19,00  x  1,50","19,00","1,50",null,"#VALUE!"]
[null,"19,05  x  0,89   (3/4\" OD)","19,05","0,89","   (3/4\" OD)","#VALUE!"]
[null,"19,05  x  1,24   (3/4\" OD)","19,05","1,24","   (3/4\" OD)","#VALUE!"]
[null,"19,05  x  1,65   (3/4\" OD)","19,05","1,65","   (3/4\" OD)","#VALUE!"]
[null,"19,05  x  2,11   (3/4\" OD)","19,05","2,11","   (3/4\" OD)","#VALUE!"]
[null,"20,00  x  1,00","20,00","1,00",null,"#VALUE!"]
[null,"20,00  x  1,50","20,00","1,50",null,"#VALUE!"]
[null,"20,00  x  2,00","20,00","2,00",null,"#VALUE!"]
[null,"20,00  x  2,50","20,00","2,50",null,"#VALUE!"]
[null,"20,00  x  3,00","20,00","3,00",null,"#VALUE!"]
[null,"20,00  x  3,50","20,00","3,50",null,"#VALUE!"]
[null,"20,00  x  4,00","20,00","4,00",null,"#VALUE!"]
[null,"20,00  x  5,00","20,00","5,00",null,"#VALUE!"]
[null,"21,30  x  1,20","21,30","1,20",null,"#VALUE!"]
[null,"21,30  x  1,50","21,30","1,50",null,"#VALUE!"]
[null,"21,30  x  1,60   ISO","21,30","1,60","   ISO","#VALUE!"]
[null,"21,30  x  2,00   ISO","21,30","2,00","   ISO","#VALUE!"]
[null,"21,30  x  2,60   ISO 1/2\" Gas","21,30","2,60","   ISO 1/2\" Gas","#VALUE!"]
[null,"21,30  x  2,90","21,30","2,90",null,"#VALUE!"]
[null,"21,30  x  3,20   ISO","21,30","3,20","   ISO","#VALUE!"]
[null,"21,34  x  1,65   1/2\" sched 5S","21,34","1,65","   1/2\" sched 5S","#VALUE!"]
[null,"21,34  x  2,11   1/2\" sched 10S","21,34","2,11","   1/2\" sched 10S","#VALUE!"]
[null,"21,34  x  2,77   1/2\" sched 40S","21,34","2,77","   1/2\" sched 40S","#VALUE!"]
[null,"21,34  x  3,73   1/2\" sched 80S","21,34","3,73","   1/2\" sched 80S","#VALUE!"]
[null,"21,34  x  4,75   1/2\" sched 160","21,34","4,75","   1/2\" sched 160","#VALUE!"]
[null,"21,34  x  7,47   1/2\" sched XXS","21,34","7,47","   1/2\" sched XXS","#VALUE!"]
[null,"22,00  x  0,70","22,00","0,70",null,"#VALUE!"]
[null,"22,00  x  1,00","22,00","1,00",null,"#VALUE!"]
[null,"22,00  x  1,20","22,00","1,20",null,"#VALUE!"]
[null,"22,00  x  1,50","22,00","1,50",null,"#VALUE!"]
[null,"22,00  x  2,00","22,00","2,00",null,"#VALUE!"]
[null,"22,00  x  2,50","22,00","2,50",null,"#VALUE!"]
[null,"22,00  x  3,00","22,00","3,00",null,"#VALUE!"]
[null,"22,00  x  4,00","22,00","4,00",null,"#VALUE!"]
[null,"23,00  x  1,50","23,00","1,50",null,"#VALUE!"]
[null,"24,00  x  2,00","24,00","2,00",null,"#VALUE!"]
[null,"24,00  x  3,50","24,00","3,50",null,"#VALUE!"]
[null,"24,00  x  4,00","24,00","4,00",null,"#VALUE!"]
[null,"24,00  x  7,00","24,00","7,00",null,"#VALUE!"]
[null,"25,00  x  1,00","25,00","1,00",null,"#VALUE!"]
[null,"25,00  x  1,50","25,00","1,50",null,"#VALUE!"]
[null,"25,00  x  2,00","25,00","2,00",null,"#VALUE!"]
[null,"25,00  x  2,50","25,00","2,50",null,"#VALUE!"]
[null,"25,00  x  3,00","25,00","3,00",null,"#VALUE!"]
[null,"25,00  x  3,50","25,00","3,50",null,"#VALUE!"]
[null,"25,00  x  4,00","25,00","4,00",null,"#VALUE!"]
[null,"25,00  x  5,00","25,00","5,00",null,"#VALUE!"]
[null,"25,40  x  1,25   (1\" OD)","25,40","1,25","   (1\" OD)","#VALUE!"]
[null,"25,40  x  1,65   (1\" OD)","25,40","1,65","   (1\" OD)","#VALUE!"]
[null,"25,40  x  2,11   (1\" OD)","25,40","2,11","   (1\" OD)","#VALUE!"]
[null,"25,40  x  3,40   (1\" OD)","25,40","3,40","   (1\" OD)","#VALUE!"]
[null,"26,67  x  1,65   3/4\" sched 5S","26,67","1,65","   3/4\" sched 5S","#VALUE!"]
[null,"26,67  x  2,11   3/4\" sched 10S","26,67","2,11","   3/4\" sched 10S","#VALUE!"]
[null,"26,67  x  2,87   3/4\" sched 40S","26,67","2,87","   3/4\" sched 40S","#VALUE!"]
[null,"26,67  x  3,91   3/4\" sched 80S","26,67","3,91","   3/4\" sched 80S","#VALUE!"]
[null,"26,67  x  5,54   3/4\" sched 160","26,67","5,54","   3/4\" sched 160","#VALUE!"]
[null,"26,67  x  7,82   3/4\" sched XXS","26,67","7,82","   3/4\" sched XXS","#VALUE!"]
[null,"26,90  x  1,20","26,90","1,20",null,"#VALUE!"]
[null,"26,90  x  1,50","26,90","1,50",null,"#VALUE!"]
[null,"26,90  x  1,60   ISO","26,90","1,60","   ISO","#VALUE!"]
[null,"26,90  x  2,00   ISO","26,90","2,00","   ISO","#VALUE!"]
[null,"26,90  x  2,30   ISO","26,90","2,30","   ISO","#VALUE!"]
[null,"26,90  x  2,60   ISO 3/4\" Gas","26,90","2,60","   ISO 3/4\" Gas","#VALUE!"]
[null,"26,90  x  3,20   ISO","26,90","3,20","   ISO","#VALUE!"]
[null,"26,90  x  4,00   ISO","26,90","4,00","   ISO","#VALUE!"]
[null,"28,00  x  0,80","28,00","0,80",null,"#VALUE!"]
[null,"28,00  x  1,00","28,00","1,00",null,"#VALUE!"]
[null,"28,00  x  1,50","28,00","1,50",null,"#VALUE!"]
[null,"28,00  x  2,00","28,00","2,00",null,"#VALUE!"]
[null,"28,00  x  3,00","28,00","3,00",null,"#VALUE!"]
[null,"28,00  x  3,50","28,00","3,50",null,"#VALUE!"]
[null,"28,00  x  4,00","28,00","4,00",null,"#VALUE!"]
[null,"28,00  x  5,00","28,00","5,00",null,"#VALUE!"]
[null,"30,00  x  1,00","30,00","1,00",null,"#VALUE!"]
[null,"30,00  x  1,50","30,00","1,50",null,"#VALUE!"]
[null,"30,00  x  2,00","30,00","2,00",null,"#VALUE!"]
[null,"30,00  x  2,50","30,00","2,50",null,"#VALUE!"]
[null,"30,00  x  2,60","30,00","2,60",null,"#VALUE!"]
[null,"30,00  x  3,00","30,00","3,00",null,"#VALUE!"]
[null,"30,00  x  3,50","30,00","3,50",null,"#VALUE!"]
[null,"30,00  x  4,00","30,00","4,00",null,"#VALUE!"]
[null,"30,00  x  5,00","30,00","5,00",null,"#VALUE!"]
[null,"31,75  x  1,65   (1¼\" OD)","31,75","1,65","   (1¼\" OD)","#VALUE!"]
[null,"31,80  x  1,25","31,80","1,25",null,"#VALUE!"]
[null,"32,00  x  1,20","32,00","1,20",null,"#VALUE!"]
[null,"32,00  x  1,50","32,00","1,50",null,"#VALUE!"]
[null,"32,00  x  2,00","32,00","2,00",null,"#VALUE!"]
[null,"32,00  x  2,50","32,00","2,50",null,"#VALUE!"]
[null,"32,00  x  3,00","32,00","3,00",null,"#VALUE!"]
[null,"33,00  x  1,50","33,00","1,50",null,"#VALUE!"]
[null,"33,40  x  1,65   1\" sched 5S","33,40","1,65","   1\" sched 5S","#VALUE!"]
[null,"33,40  x  2,77   1\" sched 10S","33,40","2,77","   1\" sched 10S","#VALUE!"]
[null,"33,40  x  3,38   1\" sched 40S","33,40","3,38","   1\" sched 40S","#VALUE!"]
[null,"33,40  x  4,55   1\" sched 80S","33,40","4,55","   1\" sched 80S","#VALUE!"]
[null,"33,40  x  6,35   1\" sched 160","33,40","6,35","   1\" sched 160","#VALUE!"]
[null,"33,40  x  9,09   1\" sched XXS","33,40","9,09","   1\" sched XXS","#VALUE!"]
[null,"33,70  x  1,20","33,70","1,20",null,"#VALUE!"]
[null,"33,70  x  1,50","33,70","1,50",null,"#VALUE!"]
[null,"33,70  x  1,60   ISO","33,70","1,60","   ISO","#VALUE!"]
[null,"33,70  x  2,00   ISO","33,70","2,00","   ISO","#VALUE!"]
[null,"33,70  x  2,60   ISO","33,70","2,60","   ISO","#VALUE!"]
[null,"33,70  x  2,90","33,70","2,90",null,"#VALUE!"]
[null,"33,70  x  3,00","33,70","3,00",null,"#VALUE!"]
[null,"33,70  x  3,20   ISO 1\" Gas","33,70","3,20","   ISO 1\" Gas","#VALUE!"]
[null,"33,70  x  3,25","33,70","3,25",null,"#VALUE!"]
[null,"33,70  x  3,60","33,70","3,60",null,"#VALUE!"]
[null,"33,70  x  4,05   ISO","33,70","4,05","   ISO","#VALUE!"]
[null,"34,00  x  1,00","34,00","1,00",null,"#VALUE!"]
[null,"34,00  x  1,50","34,00","1,50",null,"#VALUE!"]
[null,"34,00  x  2,00","34,00","2,00",null,"#VALUE!"]
[null,"34,00  x  3,50","34,00","3,50",null,"#VALUE!"]
[null,"34,00  x  4,00","34,00","4,00",null,"#VALUE!"]
[null,"34,00  x  5,00","34,00","5,00",null,"#VALUE!"]
[null,"34,00  x  5,50","34,00","5,50",null,"#VALUE!"]
[null,"35,00  x  1,00","35,00","1,00",null,"#VALUE!"]
[null,"35,00  x  1,50","35,00","1,50",null,"#VALUE!"]
[null,"35,00  x  2,00","35,00","2,00",null,"#VALUE!"]
[null,"35,00  x  2,50","35,00","2,50",null,"#VALUE!"]
[null,"35,00  x  3,00","35,00","3,00",null,"#VALUE!"]
[null,"35,00  x  4,00","35,00","4,00",null,"#VALUE!"]
[null,"35,00  x  5,00","35,00","5,00",null,"#VALUE!"]
[null,"36,00  x  2,00","36,00","2,00",null,"#VALUE!"]
[null,"36,00  x  3,00","36,00","3,00",null,"#VALUE!"]
[null,"38,00  x  1,00","38,00","1,00",null,"#VALUE!"]
[null,"38,00  x  1,50","38,00","1,50",null,"#VALUE!"]
[null,"38,00  x  2,00","38,00","2,00",null,"#VALUE!"]
[null,"38,00  x  2,50","38,00","2,50",null,"#VALUE!"]
[null,"38,00  x  2,60","38,00","2,60",null,"#VALUE!"]
[null,"38,00  x  3,00","38,00","3,00",null,"#VALUE!"]
[null,"38,00  x  3,60","38,00","3,60",null,"#VALUE!"]
[null,"38,00  x  4,00","38,00","4,00",null,"#VALUE!"]
[null,"38,00  x  5,00","38,00","5,00",null,"#VALUE!"]
[null,"38,00  x  6,00","38,00","6,00",null,"#VALUE!"]
[null,"38,10  x  1,24   (1½\" OD)","38,10","1,24","   (1½\" OD)","#VALUE!"]
[null,"38,10  x  1,50","38,10","1,50",null,"#VALUE!"]
[null,"38,10  x  1,65   (1½\" OD)","38,10","1,65","   (1½\" OD)","#VALUE!"]
[null,"38,10  x  3,40   (1½\" OD)","38,10","3,40","   (1½\" OD)","#VALUE!"]
[null,"40,00  x  1,00","40,00","1,00",null,"#VALUE!"]
[null,"40,00  x  1,50","40,00","1,50",null,"#VALUE!"]
[null,"40,00  x  2,00","40,00","2,00",null,"#VALUE!"]
[null,"40,00  x  2,50","40,00","2,50",null,"#VALUE!"]
[null,"40,00  x  3,00","40,00","3,00",null,"#VALUE!"]
[null,"40,00  x  4,00","40,00","4,00",null,"#VALUE!"]
[null,"40,00  x  5,00","40,00","5,00",null,"#VALUE!"]
[null,"41,00  x  4,00","41,00","4,00",null,"#VALUE!"]
[null,"42,00  x  1,20","42,00","1,20",null,"#VALUE!"]
[null,"42,00  x  2,00","42,00","2,00",null,"#VALUE!"]
[null,"42,00  x  3,00","42,00","3,00",null,"#VALUE!"]
[null,"42,00  x  6,00","42,00","6,00",null,"#VALUE!"]
[null,"42,16  x  1,65   1¼\" sched 5S","42,16","1,65","   1¼\" sched 5S","#VALUE!"]
[null,"42,16  x  2,77   1¼\" sched 10S","42,16","2,77","   1¼\" sched 10S","#VALUE!"]
[null,"42,16  x  3,56   1¼\" sched 40S","42,16","3,56","   1¼\" sched 40S","#VALUE!"]
[null,"42,16  x  4,85   1¼\" sched 80S","42,16","4,85","   1¼\" sched 80S","#VALUE!"]
[null,"42,16  x  6,35   1¼\" sched 160","42,16","6,35","   1¼\" sched 160","#VALUE!"]
[null,"42,40  x  1,20","42,40","1,20",null,"#VALUE!"]
[null,"42,40  x  1,50","42,40","1,50",null,"#VALUE!"]
[null,"42,40  x  1,60","42,40","1,60",null,"#VALUE!"]
[null,"42,40  x  2,00   ISO","42,40","2,00","   ISO","#VALUE!"]
[null,"42,40  x  2,60   ISO","42,40","2,60","   ISO","#VALUE!"]
[null,"42,40  x  3,00","42,40","3,00",null,"#VALUE!"]
[null,"42,40  x  3,20   ISO 1¼\" Gas","42,40","3,20","   ISO 1¼\" Gas","#VALUE!"]
[null,"42,40  x  4,05   ISO","42,40","4,05","   ISO","#VALUE!"]
[null,"43,00  x  1,50","43,00","1,50",null,"#VALUE!"]
[null,"43,00  x  5,50","43,00","5,50",null,"#VALUE!"]
[null,"44,50  x  1,50","44,50","1,50",null,"#VALUE!"]
[null,"44,50  x  2,00","44,50","2,00",null,"#VALUE!"]
[null,"44,50  x  2,50","44,50","2,50",null,"#VALUE!"]
[null,"44,50  x  2,60","44,50","2,60",null,"#VALUE!"]
[null,"44,50  x  2,90","44,50","2,90",null,"#VALUE!"]
[null,"44,50  x  3,00","44,50","3,00",null,"#VALUE!"]
[null,"44,50  x  4,00","44,50","4,00",null,"#VALUE!"]
[null,"45,00  x  1,50","45,00","1,50",null,"#VALUE!"]
[null,"45,00  x  2,00","45,00","2,00",null,"#VALUE!"]
[null,"45,00  x  3,50","45,00","3,50",null,"#VALUE!"]
[null,"45,00  x  5,00","45,00","5,00",null,"#VALUE!"]
[null,"48,26  x  1,65   1½\" sched 5S","48,26","1,65","   1½\" sched 5S","#VALUE!"]
[null,"48,26  x  2,77   1½\" sched 10S","48,26","2,77","   1½\" sched 10S","#VALUE!"]
[null,"48,26  x  3,68   1½\" sched 40S","48,26","3,68","   1½\" sched 40S","#VALUE!"]
[null,"48,26  x  5,08   1½\" sched 80S","48,26","5,08","   1½\" sched 80S","#VALUE!"]
[null,"48,26  x  7,14   1½\" sched 160","48,26","7,14","   1½\" sched 160","#VALUE!"]
[null,"48,30  x  1,20","48,30","1,20",null,"#VALUE!"]
[null,"48,30  x  1,50","48,30","1,50",null,"#VALUE!"]
[null,"48,30  x  1,60   ISO","48,30","1,60","   ISO","#VALUE!"]
[null,"48,30  x  2,00   ISO","48,30","2,00","   ISO","#VALUE!"]
[null,"48,30  x  2,60   ISO","48,30","2,60","   ISO","#VALUE!"]
[null,"48,30  x  2,90   ISO","48,30","2,90","   ISO","#VALUE!"]
[null,"48,30  x  3,20   ISO 1½\" Gas","48,30","3,20","   ISO 1½\" Gas","#VALUE!"]
[null,"48,30  x  4,05   ISO","48,30","4,05","   ISO","#VALUE!"]
[null,"50,00  x  1,00","50,00","1,00",null,"#VALUE!"]
[null,"50,00  x  1,50","50,00","1,50",null,"#VALUE!"]
[null,"50,00  x  2,00","50,00","2,00",null,"#VALUE!"]
[null,"50,00  x  3,00","50,00","3,00",null,"#VALUE!"]
[null,"50,00  x  4,00","50,00","4,00",null,"#VALUE!"]
[null,"50,00  x  5,00","50,00","5,00",null,"#VALUE!"]
[null,"50,00  x  6,00","50,00","6,00",null,"#VALUE!"]
[null,"50,80  x  1,24   (2\" OD)","50,80","1,24","   (2\" OD)","#VALUE!"]
[null,"50,80  x  1,50","50,80","1,50",null,"#VALUE!"]
[null,"50,80  x  1,65   (2\" OD)","50,80","1,65","   (2\" OD)","#VALUE!"]
[null,"50,80  x  2,00","50,80","2,00",null,"#VALUE!"]
[null,"50,80  x  2,50","50,80","2,50",null,"#VALUE!"]
[null,"50,80  x  3,40   (2\" OD)","50,80","3,40","   (2\" OD)","#VALUE!"]
[null,"51,00  x  2,50","51,00","2,50",null,"#VALUE!"]
[null,"51,00  x  2,60","51,00","2,60",null,"#VALUE!"]
[null,"51,00  x  2,60","51,00","2,60",null,"#VALUE!"]
[null,"51,00  x  2,90","51,00","2,90",null,"#VALUE!"]
[null,"52,00  x  1,00","52,00","1,00",null,"#VALUE!"]
[null,"52,00  x  1,50","52,00","1,50",null,"#VALUE!"]
[null,"53,00  x  1,50","53,00","1,50",null,"#VALUE!"]
[null,"54,00  x  1,20","54,00","1,20",null,"#VALUE!"]
[null,"54,00  x  2,00","54,00","2,00",null,"#VALUE!"]
[null,"55,00  x  5,50","55,00","5,50",null,"#VALUE!"]
[null,"57,00  x  1,50","57,00","1,50",null,"#VALUE!"]
[null,"57,00  x  2,00","57,00","2,00",null,"#VALUE!"]
[null,"57,00  x  2,50","57,00","2,50",null,"#VALUE!"]
[null,"57,00  x  2,60","57,00","2,60",null,"#VALUE!"]
[null,"57,00  x  2,90","57,00","2,90",null,"#VALUE!"]
[null,"57,00  x  3,00","57,00","3,00",null,"#VALUE!"]
[null,"57,00  x  3,50","57,00","3,50",null,"#VALUE!"]
[null,"57,00  x  4,00","57,00","4,00",null,"#VALUE!"]
[null,"57,00  x  4,50","57,00","4,50",null,"#VALUE!"]
[null,"57,00  x  5,00","57,00","5,00",null,"#VALUE!"]
[null,"57,00  x  6,50","57,00","6,50",null,"#VALUE!"]
[null,"60,00  x  5,00","60,00","5,00",null,"#VALUE!"]
[null,"60,30  x  1,20","60,30","1,20",null,"#VALUE!"]
[null,"60,30  x  1,50","60,30","1,50",null,"#VALUE!"]
[null,"60,30  x  1,60   ISO","60,30","1,60","   ISO","#VALUE!"]
[null,"60,30  x  2,00   ISO","60,30","2,00","   ISO","#VALUE!"]
[null,"60,30  x  2,60   ISO","60,30","2,60","   ISO","#VALUE!"]
[null,"60,30  x  2,90   ISO","60,30","2,90","   ISO","#VALUE!"]
[null,"60,30  x  3,20","60,30","3,20",null,"#VALUE!"]
[null,"60,30  x  3,60   ISO 2\" Gas","60,30","3,60","   ISO 2\" Gas","#VALUE!"]
[null,"60,30  x  4,50   ISO","60,30","4,50","   ISO","#VALUE!"]
[null,"60,33  x  1,65   2\" sched 5S","60,33","1,65","   2\" sched 5S","#VALUE!"]
[null,"60,33  x  2,77   2\" sched 10S","60,33","2,77","   2\" sched 10S","#VALUE!"]
[null,"60,33  x  3,91   2\" sched 40S","60,33","3,91","   2\" sched 40S","#VALUE!"]
[null,"60,33  x  5,54   2\" sched 80S","60,33","5,54","   2\" sched 80S","#VALUE!"]
[null,"60,33  x  8,71   2\" sched 160","60,33","8,71","   2\" sched 160","#VALUE!"]
[null,"63,00  x  1,50","63,00","1,50",null,"#VALUE!"]
[null,"63,50  x  1,50   ISO","63,50","1,50","   ISO","#VALUE!"]
[null,"63,50  x  2,00   ISO","63,50","2,00","   ISO","#VALUE!"]
[null,"63,50  x  2,50","63,50","2,50",null,"#VALUE!"]
[null,"63,50  x  2,60   ISO","63,50","2,60","   ISO","#VALUE!"]
[null,"63,50  x  3,00","63,50","3,00",null,"#VALUE!"]
[null,"64,00  x  2,00","64,00","2,00",null,"#VALUE!"]
[null,"65,00  x  2,50","65,00","2,50",null,"#VALUE!"]
[null,"65,00  x  3,00","65,00","3,00",null,"#VALUE!"]
[null,"65,00  x  3,50","65,00","3,50",null,"#VALUE!"]
[null,"69,00  x  2,00","69,00","2,00",null,"#VALUE!"]
[null,"70,00  x  1,50","70,00","1,50",null,"#VALUE!"]
[null,"70,00  x  2,00","70,00","2,00",null,"#VALUE!"]
[null,"70,00  x  2,50","70,00","2,50",null,"#VALUE!"]
[null,"70,00  x  2,90","70,00","2,90",null,"#VALUE!"]
[null,"70,00  x  3,00","70,00","3,00",null,"#VALUE!"]
[null,"70,00  x  4,00","70,00","4,00",null,"#VALUE!"]
[null,"70,00  x  4,50","70,00","4,50",null,"#VALUE!"]
[null,"70,00  x  5,00","70,00","5,00",null,"#VALUE!"]
[null,"70,00  x  7,00","70,00","7,00",null,"#VALUE!"]
[null,"73,03  x  2,11   2½\" sched 5S","73,03","2,11","   2½\" sched 5S","#VALUE!"]
[null,"73,03  x  3,05   2½\" sched 10S","73,03","3,05","   2½\" sched 10S","#VALUE!"]
[null,"73,03  x  5,16   2½\" sched 40S","73,03","5,16","   2½\" sched 40S","#VALUE!"]
[null,"73,03  x  7,01   2½\" sched 80S","73,03","7,01","   2½\" sched 80S","#VALUE!"]
[null,"75,00  x  2,50","75,00","2,50",null,"#VALUE!"]
[null,"76,00  x  5,00","76,00","5,00",null,"#VALUE!"]
[null,"76,00  x  6,00","76,00","6,00",null,"#VALUE!"]
[null,"76,10  x  1,50   ISO","76,10","1,50","   ISO","#VALUE!"]
[null,"76,10  x  1,60","76,10","1,60",null,"#VALUE!"]
[null,"76,10  x  2,00   ISO","76,10","2,00","   ISO","#VALUE!"]
[null,"76,10  x  2,60   ISO","76,10","2,60","   ISO","#VALUE!"]
[null,"76,10  x  2,90   ISO","76,10","2,90","   ISO","#VALUE!"]
[null,"76,10  x  3,60   ISO 2½\" Gas","76,10","3,60","   ISO 2½\" Gas","#VALUE!"]
[null,"76,10  x  4,00","76,10","4,00",null,"#VALUE!"]
[null,"76,10  x  4,50   ISO","76,10","4,50","   ISO","#VALUE!"]
[null,"76,10  x  5,00   ISO","76,10","5,00","   ISO","#VALUE!"]
[null,"76,10  x  6,30","76,10","6,30",null,"#VALUE!"]
[null,"80,00  x  2,00","80,00","2,00",null,"#VALUE!"]
[null,"80,00  x  3,00","80,00","3,00",null,"#VALUE!"]
[null,"80,00  x  4,00","80,00","4,00",null,"#VALUE!"]
[null,"80,00  x  5,00","80,00","5,00",null,"#VALUE!"]
[null,"83,00  x  1,50","83,00","1,50",null,"#VALUE!"]
[null,"84,00  x  2,00","84,00","2,00",null,"#VALUE!"]
[null,"85,00  x  2,50","85,00","2,50",null,"#VALUE!"]
[null,"86,00  x  3,00","86,00","3,00",null,"#VALUE!"]
[null,"88,90  x  1,50","88,90","1,50",null,"#VALUE!"]
[null,"88,90  x  1,60","88,90","1,60",null,"#VALUE!"]
[null,"88,90  x  2,00   ISO","88,90","2,00","   ISO","#VALUE!"]
[null,"88,90  x  2,11   3\" sched 5S","88,90","2,11","   3\" sched 5S","#VALUE!"]
[null,"88,90  x  2,30   ISO","88,90","2,30","   ISO","#VALUE!"]
[null,"88,90  x  2,60   ISO","88,90","2,60","   ISO","#VALUE!"]
[null,"88,90  x  2,90   ISO","88,90","2,90","   ISO","#VALUE!"]
[null,"88,90  x  3,05   3\" sched 10S","88,90","3,05","   3\" sched 10S","#VALUE!"]
[null,"88,90  x  3,20   ISO","88,90","3,20","   ISO","#VALUE!"]
[null,"88,90  x  3,60","88,90","3,60",null,"#VALUE!"]
[null,"88,90  x  4,00","88,90","4,00",null,"#VALUE!"]
[null,"88,90  x  4,05   ISO 3\" Gas","88,90","4,05","   ISO 3\" Gas","#VALUE!"]
[null,"88,90  x  4,50   ISO","88,90","4,50","   ISO","#VALUE!"]
[null,"88,90  x  5,00   ISO","88,90","5,00","   ISO","#VALUE!"]
[null,"88,90  x  5,49   3\" sched 40S","88,90","5,49","   3\" sched 40S","#VALUE!"]
[null,"88,90  x  7,62   3\" sched 80S","88,90","7,62","   3\" sched 80S","#VALUE!"]
[null,"88,90  x  11,13   3\" sched 160","88,90","11,13","   3\" sched 160","#VALUE!"]
[null,"88,90  x  15,24   3\" sched XXS","88,90","15,24","   3\" sched XXS","#VALUE!"]
[null,"90,00  x  5,00","90,00","5,00",null,"#VALUE!"]
[null,"97,00  x  4,00","97,00","4,00",null,"#VALUE!"]
[null,"101,60  x  1,50   ISO","101,60","1,50","   ISO","#VALUE!"]
[null,"101,60  x  2,00","101,60","2,00",null,"#VALUE!"]
[null,"101,60  x  2,11   3½\" sched 5S","101,60","2,11","   3½\" sched 5S","#VALUE!"]
[null,"101,60  x  2,00","101,60","2,00",null,"#VALUE!"]
[null,"101,60  x  3,05   3½\" sched 10S","101,60","3,05","   3½\" sched 10S","#VALUE!"]
[null,"101,60  x  3,60","101,60","3,60",null,"#VALUE!"]
[null,"101,60  x  4,00   ISO 3½\" Gas","101,60","4,00","   ISO 3½\" Gas","#VALUE!"]
[null,"101,60  x  5,00   ISO","101,60","5,00","   ISO","#VALUE!"]
[null,"101,60  x  5,74   3½\" sched 40S","101,60","5,74","   3½\" sched 40S","#VALUE!"]
[null,"101,60  x  8,08   3½\" sched 80S","101,60","8,08","   3½\" sched 80S","#VALUE!"]
[null,"102,00  x  6,50","102,00","6,50",null,"#VALUE!"]
[null,"103,00  x  1,50","103,00","1,50",null,"#VALUE!"]
[null,"104,00  x  2,00","104,00","2,00",null,"#VALUE!"]
[null,"105,00  x  2,50","105,00","2,50",null,"#VALUE!"]
[null,"106,00  x  2,70","106,00","2,70",null,"#VALUE!"]
[null,"106,00  x  3,00","106,00","3,00",null,"#VALUE!"]
[null,"108,00  x  2,00","108,00","2,00",null,"#VALUE!"]
[null,"108,00  x  2,90","108,00","2,90",null,"#VALUE!"]
[null,"108,00  x  3,00","108,00","3,00",null,"#VALUE!"]
[null,"108,00  x  3,60","108,00","3,60",null,"#VALUE!"]
[null,"108,00  x  4,00","108,00","4,00",null,"#VALUE!"]
[null,"108,00  x  4,50","108,00","4,50",null,"#VALUE!"]
[null,"108,00  x  5,00","108,00","5,00",null,"#VALUE!"]
[null,"108,00  x  6,30","108,00","6,30",null,"#VALUE!"]
[null,"114,30  x  1,50","114,30","1,50",null,"#VALUE!"]
[null,"114,30  x  1,60","114,30","1,60",null,"#VALUE!"]
[null,"114,30  x  2,00   ISO","114,30","2,00","   ISO","#VALUE!"]
[null,"114,30  x  2,11   4\" sched 5S","114,30","2,11","   4\" sched 5S","#VALUE!"]
[null,"114,30  x  2,60","114,30","2,60",null,"#VALUE!"]
[null,"114,30  x  2,90   ISO","114,30","2,90","   ISO","#VALUE!"]
[null,"114,30  x  3,05   4\" sched 10S","114,30","3,05","   4\" sched 10S","#VALUE!"]
[null,"114,30  x  3,20","114,30","3,20",null,"#VALUE!"]
[null,"114,30  x  3,60   ISO","114,30","3,60","   ISO","#VALUE!"]
[null,"114,30  x  4,00","114,30","4,00",null,"#VALUE!"]
[null,"114,30  x  4,50   ISO 4\" Gas","114,30","4,50","   ISO 4\" Gas","#VALUE!"]
[null,"114,30  x  5,40   ISO","114,30","5,40","   ISO","#VALUE!"]
[null,"114,30  x  6,02   4\" sched 40S","114,30","6,02","   4\" sched 40S","#VALUE!"]
[null,"114,30  x  6,30","114,30","6,30",null,"#VALUE!"]
[null,"114,30  x  8,56   4\" sched 80S","114,30","8,56","   4\" sched 80S","#VALUE!"]
[null,"114,30  x  13,49   4\" sched 160","114,30","13,49","   4\" sched 160","#VALUE!"]
[null,"114,30  x  17,12   4\" sched XXS","114,30","17,12","   4\" sched XXS","#VALUE!"]
[null,"121,00  x  4,00","121,00","4,00",null,"#VALUE!"]
[null,"127,00  x  4,00","127,00","4,00",null,"#VALUE!"]
[null,"128,00  x  1,50","128,00","1,50",null,"#VALUE!"]
[null,"129,00  x  2,00","129,00","2,00",null,"#VALUE!"]
[null,"130,00  x  2,50","130,00","2,50",null,"#VALUE!"]
[null,"131,00  x  3,00","131,00","3,00",null,"#VALUE!"]
[null,"133,00  x  3,00","133,00","3,00",null,"#VALUE!"]
[null,"133,00  x  4,00","133,00","4,00",null,"#VALUE!"]
[null,"133,00  x  5,00","133,00","5,00",null,"#VALUE!"]
[null,"133,00  x  6,30","133,00","6,30",null,"#VALUE!"]
[null,"139,70  x  2,00   ISO","139,70","2,00","   ISO","#VALUE!"]
[null,"139,70  x  2,50   ISO","139,70","2,50","   ISO","#VALUE!"]
[null,"139,70  x  2,60","139,70","2,60",null,"#VALUE!"]
[null,"139,70  x  2,90","139,70","2,90",null,"#VALUE!"]
[null,"139,70  x  3,00   ISO","139,70","3,00","   ISO","#VALUE!"]
[null,"139,70  x  4,00   ISO","139,70","4,00","   ISO","#VALUE!"]
[null,"139,70  x  5,00","139,70","5,00",null,"#VALUE!"]
[null,"141,30  x  2,77   5\" sched 5S","141,30","2,77","   5\" sched 5S","#VALUE!"]
[null,"141,30  x  3,40   5\" sched 10S","141,30","3,40","   5\" sched 10S","#VALUE!"]
[null,"141,30  x  6,35   5\" sched 40S","141,30","6,35","   5\" sched 40S","#VALUE!"]
[null,"141,30  x  6,55","141,30","6,55",null,"#VALUE!"]
[null,"141,30  x  9,53   5\" sched 80S","141,30","9,53","   5\" sched 80S","#VALUE!"]
[null,"141,30  x  15,88   5\" sched 160","141,30","15,88","   5\" sched 160","#VALUE!"]
[null,"153,00  x  1,50","153,00","1,50",null,"#VALUE!"]
[null,"154,00  x  2,00","154,00","2,00",null,"#VALUE!"]
[null,"155,00  x  2,50","155,00","2,50",null,"#VALUE!"]
[null,"156,00  x  3,00","156,00","3,00",null,"#VALUE!"]
[null,"158,00  x  4,00","158,00","4,00",null,"#VALUE!"]
[null,"159,00  x  2,00","159,00","2,00",null,"#VALUE!"]
[null,"159,00  x  3,00","159,00","3,00",null,"#VALUE!"]
[null,"159,00  x  4,00","159,00","4,00",null,"#VALUE!"]
[null,"159,00  x  4,50","159,00","4,50",null,"#VALUE!"]
[null,"159,00  x  5,00","159,00","5,00",null,"#VALUE!"]
[null,"159,00  x  6,30","159,00","6,30",null,"#VALUE!"]
[null,"168,28  x  2,77   6\" sched 5S","168,28","2,77","   6\" sched 5S","#VALUE!"]
[null,"168,28  x  3,40   6\" sched 10S","168,28","3,40","   6\" sched 10S","#VALUE!"]
[null,"168,28  x  7,11   6\" sched 40S","168,28","7,11","   6\" sched 40S","#VALUE!"]
[null,"168,28  x  10,97   6\" sched 80S","168,28","10,97","   6\" sched 80S","#VALUE!"]
[null,"168,28  x  18,26   6\" sched XXS","168,28","18,26","   6\" sched XXS","#VALUE!"]
[null,"168,30  x  2,00   ISO","168,30","2,00","   ISO","#VALUE!"]
[null,"168,30  x  2,50   ISO","168,30","2,50","   ISO","#VALUE!"]
[null,"168,30  x  2,60","168,30","2,60",null,"#VALUE!"]
[null,"168,30  x  2,90","168,30","2,90",null,"#VALUE!"]
[null,"168,30  x  3,00   ISO","168,30","3,00","   ISO","#VALUE!"]
[null,"168,30  x  4,00   ISO","168,30","4,00","   ISO","#VALUE!"]
[null,"168,30  x  4,50","168,30","4,50",null,"#VALUE!"]
[null,"168,30  x  5,00   ISO","168,30","5,00","   ISO","#VALUE!"]
[null,"168,30  x  6,30","168,30","6,30",null,"#VALUE!"]
[null,"179,00  x  2,00","179,00","2,00",null,"#VALUE!"]
[null,"204,00  x  2,00","204,00","2,00",null,"#VALUE!"]
[null,"205,00  x  2,50","205,00","2,50",null,"#VALUE!"]
[null,"206,00  x  3,00","206,00","3,00",null,"#VALUE!"]
[null,"208,00  x  4,00","208,00","4,00",null,"#VALUE!"]
[null,"219,08  x  2,77   8\" sched 5S","219,08","2,77","   8\" sched 5S","#VALUE!"]
[null,"219,08  x  3,76   8\" sched 10S","219,08","3,76","   8\" sched 10S","#VALUE!"]
[null,"219,08  x  6,35   8\" sched 20","219,08","6,35","   8\" sched 20","#VALUE!"]
[null,"219,08  x  8,18   8\" sched 40S","219,08","8,18","   8\" sched 40S","#VALUE!"]
[null,"219,08  x  12,70   8\" sched 80S","219,08","12,70","   8\" sched 80S","#VALUE!"]
[null,"219,08  x  23,01   8\" sched 160","219,08","23,01","   8\" sched 160","#VALUE!"]
[null,"219,10  x  2,00   ISO","219,10","2,00","   ISO","#VALUE!"]
[null,"219,10  x  2,60","219,10","2,60",null,"#VALUE!"]
[null,"219,10  x  2,90","219,10","2,90",null,"#VALUE!"]
[null,"219,10  x  3,00   ISO","219,10","3,00","   ISO","#VALUE!"]
[null,"219,10  x  4,00","219,10","4,00",null,"#VALUE!"]
[null,"219,10  x  6,50","219,10","6,50",null,"#VALUE!"]
[null,"254,00  x  2,00   ISO","254,00","2,00","   ISO","#VALUE!"]
[null,"255,00  x  2,50","255,00","2,50",null,"#VALUE!"]
[null,"256,00  x  3,00","256,00","3,00",null,"#VALUE!"]
[null,"258,00  x  4,00","258,00","4,00",null,"#VALUE!"]
[null,"273,00  x  2,00","273,00","2,00",null,"#VALUE!"]
[null,"273,00  x  2,50","273,00","2,50",null,"#VALUE!"]
[null,"273,00  x  2,60","273,00","2,60",null,"#VALUE!"]
[null,"273,00  x  2,90","273,00","2,90",null,"#VALUE!"]
[null,"273,00  x  3,00","273,00","3,00",null,"#VALUE!"]
[null,"273,00  x  4,00","273,00","4,00",null,"#VALUE!"]
[null,"273,05  x  3,40   10\" sched 5S","273,05","3,40","   10\" sched 5S","#VALUE!"]
[null,"273,05  x  4,19   10\" sched 10S","273,05","4,19","   10\" sched 10S","#VALUE!"]
[null,"273,05  x  6,35   10\" sched 20","273,05","6,35","   10\" sched 20","#VALUE!"]
[null,"273,05  x  9,27   10\" sched 40S","273,05","9,27","   10\" sched 40S","#VALUE!"]
[null,"273,05  x  12,70   10\" sched 80S","273,05","12,70","   10\" sched 80S","#VALUE!"]
[null,"304,00  x  2,00","304,00","2,00",null,"#VALUE!"]
[null,"305,00  x  2,50","305,00","2,50",null,"#VALUE!"]
[null,"306,00  x  3,00","306,00","3,00",null,"#VALUE!"]
[null,"308,00  x  4,00","308,00","4,00",null,"#VALUE!"]
[null,"323,85  x  3,96   12\" sched 5S","323,85","3,96","   12\" sched 5S","#VALUE!"]
[null,"323,85  x  4,57   12\" sched 10S","323,85","4,57","   12\" sched 10S","#VALUE!"]
[null,"323,85  x  6,35   12\" sched 20","323,85","6,35","   12\" sched 20","#VALUE!"]
[null,"323,85  x  9,53   12\" sched 40S","323,85","9,53","   12\" sched 40S","#VALUE!"]
[null,"323,85  x  12,70   12\" sched 80S","323,85","12,70","   12\" sched 80S","#VALUE!"]
[null,"323,90  x  2,00   ISO","323,90","2,00","   ISO","#VALUE!"]
[null,"323,90  x  2,50   ISO","323,90","2,50","   ISO","#VALUE!"]
[null,"323,90  x  2,90","323,90","2,90",null,"#VALUE!"]
[null,"323,90  x  3,00   ISO","323,90","3,00","   ISO","#VALUE!"]
[null,"323,90  x  3,60","323,90","3,60",null,"#VALUE!"]
[null,"323,90  x  4,00   ISO","323,90","4,00","   ISO","#VALUE!"]
[null,"323,90  x  10,00","323,90","10,00",null,"#VALUE!"]
[null,"355,00  x  2,50","355,00","2,50",null,"#VALUE!"]
[null,"355,60  x  2,90","355,60","2,90",null,"#VALUE!"]
[null,"355,60  x  3,96   14\" sched 5S","355,60","3,96","   14\" sched 5S","#VALUE!"]
[null,"355,60  x  4,00","355,60","4,00",null,"#VALUE!"]
[null,"355,60  x  4,78   14\" sched 10S","355,60","4,78","   14\" sched 10S","#VALUE!"]
[null,"355,60  x  6,35   14\" sched 10","355,60","6,35","   14\" sched 10","#VALUE!"]
[null,"355,60  x  7,92   14\" sched 20","355,60","7,92","   14\" sched 20","#VALUE!"]
[null,"355,60  x  9,53   14\" sched 40S","355,60","9,53","   14\" sched 40S","#VALUE!"]
[null,"355,60  x  12,70   14\" sched 80S","355,60","12,70","   14\" sched 80S","#VALUE!"]
[null,"356,00  x  3,00","356,00","3,00",null,"#VALUE!"]
[null,"358,00  x  4,00","358,00","4,00",null,"#VALUE!"]
[null,"406,00  x  3,00","406,00","3,00",null,"#VALUE!"]
[null,"406,40  x  4,19   16\" sched 5S","406,40","4,19","   16\" sched 5S","#VALUE!"]
[null,"406,40  x  4,78   16\" sched 10S","406,40","4,78","   16\" sched 10S","#VALUE!"]
[null,"406,40  x  6,35   16\" sched 10","406,40","6,35","   16\" sched 10","#VALUE!"]
[null,"406,40  x  7,92   16\" sched 20","406,40","7,92","   16\" sched 20","#VALUE!"]
[null,"406,40  x  9,53   16\" sched 40S","406,40","9,53","   16\" sched 40S","#VALUE!"]
[null,"406,40  x  12,70   16\" sched 80S","406,40","12,70","   16\" sched 80S","#VALUE!"]
[null,"408,00  x  4,00","408,00","4,00",null,"#VALUE!"]
[null,"456,00  x  3,00","456,00","3,00",null,"#VALUE!"]
[null,"457,20  x  3,00","457,20","3,00",null,"#VALUE!"]
[null,"457,20  x  4,19   18\" sched 5S","457,20","4,19","   18\" sched 5S","#VALUE!"]
[null,"457,20  x  4,78   18\" sched 10S","457,20","4,78","   18\" sched 10S","#VALUE!"]
[null,"457,20  x  5,00","457,20","5,00",null,"#VALUE!"]
[null,"457,20  x  5,54   18\" sched 20","457,20","5,54","   18\" sched 20","#VALUE!"]
[null,"457,20  x  6,35   18\" sched 10","457,20","6,35","   18\" sched 10","#VALUE!"]
[null,"457,20  x  9,53   18\" sched 40S","457,20","9,53","   18\" sched 40S","#VALUE!"]
[null,"457,20  x  12,70   18\" sched 80S","457,20","12,70","   18\" sched 80S","#VALUE!"]
[null,"458,00  x  4,00","458,00","4,00",null,"#VALUE!"]
[null,"506,00  x  3,00","506,00","3,00",null,"#VALUE!"]
[null,"508,00  x  3,00","508,00","3,00",null,"#VALUE!"]
[null,"508,00  x  4,00","508,00","4,00",null,"#VALUE!"]
[null,"508,00  x  4,78   20\" sched 5S","508,00","4,78","   20\" sched 5S","#VALUE!"]
[null,"508,00  x  5,54   20\" sched 10S","508,00","5,54","   20\" sched 10S","#VALUE!"]
[null,"508,00  x  5,60","508,00","5,60",null,"#VALUE!"]
[null,"508,00  x  6,35   20\" sched 10","508,00","6,35","   20\" sched 10","#VALUE!"]
[null,"508,00  x  9,53   20\" sched 40S","508,00","9,53","   20\" sched 40S","#VALUE!"]
[null,"508,00  x  12,70   20\" sched 80S","508,00","12,70","   20\" sched 80S","#VALUE!"]
[null,"558,80  x  4,78   22\" sched 5S","558,80","4,78","   22\" sched 5S","#VALUE!"]
[null,"558,80  x  5,54   22\" sched 10S","558,80","5,54","   22\" sched 10S","#VALUE!"]
[null,"558,80  x  9,53   22\" sched 40S","558,80","9,53","   22\" sched 40S","#VALUE!"]
[null,"558,80  x  12,70   22\" sched 80S","558,80","12,70","   22\" sched 80S","#VALUE!"]
[null,"606,00  x  3,00","606,00","3,00",null,"#VALUE!"]
[null,"608,00  x  4,00","608,00","4,00",null,"#VALUE!"]
[null,"609,60  x  3,00","609,60","3,00",null,"#VALUE!"]
[null,"609,60  x  5,54   24\" sched 5S","609,60","5,54","   24\" sched 5S","#VALUE!"]
[null,"609,60  x  6,35   24\" sched 10S","609,60","6,35","   24\" sched 10S","#VALUE!"]
[null,"609,60  x  9,53   24\" sched 40S","609,60","9,53","   24\" sched 40S","#VALUE!"]
[null,"609,60  x  12,70   24\" sched 80S","609,60","12,70","   24\" sched 80S","#VALUE!"]
[null,"711,20  x  4,00","711,20","4,00",null,"#VALUE!"]
[null,"711,20  x  7,10","711,20","7,10",null,"#VALUE!"]
[null,"812,80  x  4,00","812,80","4,00",null,"#VALUE!"]
[null,"812,80  x  8,00","812,80","8,00",null,"#VALUE!"]
[null,"914,40  x  4,00","914,40","4,00",null,"#VALUE!"]

{"sheet":"Data Castiron pipe","index":4,"n_rows":115,"n_cols":12,"rows_kept":115,"cut":false,"hidden":true,"merged":[[0,3,0,4]]}
["Cast iron pipe",null,"Class","Rating",null,"Size","Size","OD","OD","Wallth.","Wallth.","Di"]
["\" ",null," ",null,null,"NPS","DN","Inch","mm","Inch","mm"]
[1.0,{"$f":"CONCATENATE($A$1,$C$2,$C$1,$C$2,D3,$C$2,E3,$C$2,$F$1,$C$2,F3,$A$2)","v":"Cast iron pipe Class 100 ft (43# ) Size 3\" "},"A","100 ft","(43# )","3","80",3.8,{"$f":"H3*25.4","v":96.52},0.39,{"$f":"J3*25.4","v":9.906},{"$f":"I3-(2*K3)","v":76.708}]
[null,"Cast iron pipe Class 100 ft (43# ) Size 4\" ","A","100 ft","(43# )","4","100",4.8,121.92,0.42,10.668,100.584]
[null,"Cast iron pipe Class 100 ft (43# ) Size 6\" ","A","100 ft","(43# )","6","150",6.9,175.26,0.44,11.176,152.908]
[null,"Cast iron pipe Class 100 ft (43# ) Size 8\" ","A","100 ft","(43# )","8","200",9.05,229.87,0.46,11.684,206.502]
[null,"Cast iron pipe Class 100 ft (43# ) Size 10\" ","A","100 ft","(43# )","10","250",11.1,281.94,0.5,12.7,256.54]
[null,"Cast iron pipe Class 100 ft (43# ) Size 12\" ","A","100 ft","(43# )","12","300",13.2,335.28,0.54,13.716,307.848]
[null,"Cast iron pipe Class 100 ft (43# ) Size 14\" ","A","100 ft","(43# )","14","350",15.3,388.62,0.57,14.478,359.664]
[null,"Cast iron pipe Class 100 ft (43# ) Size 16\" ","A","100 ft","(43# )","16","400",17.4,441.96,0.6,15.24,411.48]
[null,"Cast iron pipe Class 100 ft (43# ) Size 18\" ","A","100 ft","(43# )","18","450",19.5,495.3,0.64,16.256,462.788]
[null,"Cast iron pipe Class 100 ft (43# ) Size 20\" ","A","100 ft","(43# )","20","500",21.6,548.64,0.67,17.018,514.604]
[null,"Cast iron pipe Class 100 ft (43# ) Size 24\" ","A","100 ft","(43# )","24","600",25.8,655.32,0.76,19.304,616.712]
[null,"Cast iron pipe Class 100 ft (43# ) Size 30\" ","A","100 ft","(43# )","30","750",31.74,806.196,0.88,22.352,761.492]
[null,"Cast iron pipe Class 100 ft (43# ) Size 36\" ","A","100 ft","(43# )","36","900",37.96,964.184,0.99,25.146,913.892]
[null,"Cast iron pipe Class 100 ft (43# ) Size 42\" ","A","100 ft","(43# )","42","1050",44.2,1122.68,1.1,27.94,1066.8]
[null,"Cast iron pipe Class 100 ft (43# ) Size 48\" ","A","100 ft","(43# )","48","1200",50.5,1282.7,1.26,32.004,1218.692]
[null,"Cast iron pipe Class 100 ft (43# ) Size 54\" ","A","100 ft","(43# )","54","1350",56.66,1439.164,1.35,34.29,1370.584]
[null,"Cast iron pipe Class 100 ft (43# ) Size 60\" ","A","100 ft","(43# )","60","1500",62.8,1595.12,1.39,35.306,1524.508]
[null,"Cast iron pipe Class 100 ft (43# ) Size 72\" ","A","100 ft","(43# )","72","1800",75.34,1913.636,1.62,41.148,1831.34]
[null,"Cast iron pipe Class 100 ft (43# ) Size 84\" ","A","100 ft","(43# )","84","2100",87.54,2223.516,1.72,43.688,2136.14]
[null,"Cast iron pipe Class 200 ft (86# ) Size 3\" ","B","200 ft","(86# )","3","80",3.96,100.584,0.42,10.668,79.248]
[null,"Cast iron pipe Class 200 ft (86# ) Size 4\" ","B","200 ft","(86# )","4","100",5.0,127,0.45,11.43,104.14]
[null,"Cast iron pipe Class 200 ft (86# ) Size 6\" ","B","200 ft","(86# )","6","150",7.1,180.34,0.48,12.192,155.956]
[null,"Cast iron pipe Class 200 ft (86# ) Size 8\" ","B","200 ft","(86# )","8","200",9.05,229.87,0.51,12.954,203.962]
[null,"Cast iron pipe Class 200 ft (86# ) Size 10\" ","B","200 ft","(86# )","10","250",11.1,281.94,0.57,14.478,252.984]
[null,"Cast iron pipe Class 200 ft (86# ) Size 12\" ","B","200 ft","(86# )","12","300",13.2,335.28,0.62,15.748,303.784]
[null,"Cast iron pipe Class 200 ft (86# ) Size 14\" ","B","200 ft","(86# )","14","350",15.3,388.62,0.66,16.764,355.092]
[null,"Cast iron pipe Class 200 ft (86# ) Size 16\" ","B","200 ft","(86# )","16","400",17.4,441.96,0.7,17.78,406.4]
[null,"Cast iron pipe Class 200 ft (86# ) Size 18\" ","B","200 ft","(86# )","18","450",19.5,495.3,0.75,19.05,457.2]
[null,"Cast iron pipe Class 200 ft (86# ) Size 20\" ","B","200 ft","(86# )","20","500",21.6,548.64,0.8,20.32,508]
[null,"Cast iron pipe Class 200 ft (86# ) Size 24\" ","B","200 ft","(86# )","24","600",25.8,655.32,0.89,22.606,610.108]
[null,"Cast iron pipe Class 200 ft (86# ) Size 30\" ","B","200 ft","(86# )","30","750",32.0,812.8,1.03,26.162,760.476]
[null,"Cast iron pipe Class 200 ft (86# ) Size 36\" ","B","200 ft","(86# )","36","900",38.3,972.82,1.15,29.21,914.4]
[null,"Cast iron pipe Class 200 ft (86# ) Size 42\" ","B","200 ft","(86# )","42","1050",44.5,1130.3,1.28,32.512,1065.276]
[null,"Cast iron pipe Class 200 ft (86# ) Size 48\" ","B","200 ft","(86# )","48","1200",50.8,1290.32,1.42,36.068,1218.184]
[null,"Cast iron pipe Class 200 ft (86# ) Size 54\" ","B","200 ft","(86# )","54","1350",57.1,1450.34,1.55,39.37,1371.6]
[null,"Cast iron pipe Class 200 ft (86# ) Size 60\" ","B","200 ft","(86# )","60","1500",63.4,1610.36,1.67,42.418,1525.524]
[null,"Cast iron pipe Class 200 ft (86# ) Size 72\" ","B","200 ft","(86# )","72","1800",76.0,1930.4,1.95,49.53,1831.34]
[null,"Cast iron pipe Class 200 ft (86# ) Size 84\" ","B","200 ft","(86# )","84","2100",88.54,2248.916,2.22,56.388,2136.14]
[null,"Cast iron pipe Class 300 ft (130# ) Size 3\" ","C","300 ft","(130# )","3","80",3.96,100.584,0.45,11.43,77.724]
[null,"Cast iron pipe Class 300 ft (130# ) Size 4\" ","C","300 ft","(130# )","4","100",5.0,127,0.48,12.192,102.616]
[null,"Cast iron pipe Class 300 ft (130# ) Size 6\" ","C","300 ft","(130# )","6","150",7.1,180.34,0.51,12.954,154.432]
[null,"Cast iron pipe Class 300 ft (130# ) Size 8\" ","C","300 ft","(130# )","8","200",9.3,236.22,0.56,14.224,207.772]
[null,"Cast iron pipe Class 300 ft (130# ) Size 10\" ","C","300 ft","(130# )","10","250",11.4,289.56,0.62,15.748,258.064]
[null,"Cast iron pipe Class 300 ft (130# ) Size 12\" ","C","300 ft","(130# )","12","300",13.5,342.9,0.68,17.272,308.356]
[null,"Cast iron pipe Class 300 ft (130# ) Size 14\" ","C","300 ft","(130# )","14","350",15.65,397.51,0.74,18.796,359.918]
[null,"Cast iron pipe Class 300 ft (130# ) Size 16\" ","C","300 ft","(130# )","16","400",17.8,452.12,0.8,20.32,411.48]
[null,"Cast iron pipe Class 300 ft (130# ) Size 18\" ","C","300 ft","(130# )","18","450",19.92,505.968,0.87,22.098,461.772]
[null,"Cast iron pipe Class 300 ft (130# ) Size 20\" ","C","300 ft","(130# )","20","500",22.06,560.324,0.92,23.368,513.588]
[null,"Cast iron pipe Class 300 ft (130# ) Size 24\" ","C","300 ft","(130# )","24","600",26.32,668.528,1.04,26.416,615.696]
[null,"Cast iron pipe Class 300 ft (130# ) Size 30\" ","C","300 ft","(130# )","30","750",32.4,822.96,1.2,30.48,762]
[null,"Cast iron pipe Class 300 ft (130# ) Size 36\" ","C","300 ft","(130# )","36","900",38.7,982.98,1.36,34.544,913.892]
[null,"Cast iron pipe Class 300 ft (130# ) Size 42\" ","C","300 ft","(130# )","42","1050",45.1,1145.54,1.54,39.116,1067.308]
[null,"Cast iron pipe Class 300 ft (130# ) Size 48\" ","C","300 ft","(130# )","48","1200",51.4,1305.56,1.71,43.434,1218.692]
[null,"Cast iron pipe Class 300 ft (130# ) Size 54\" ","C","300 ft","(130# )","54","1350",57.8,1468.12,1.9,48.26,1371.6]
[null,"Cast iron pipe Class 300 ft (130# ) Size 60\" ","C","300 ft","(130# )","60","1500",64.2,1630.68,2.0,50.8,1529.08]
[null,"Cast iron pipe Class 300 ft (130# ) Size 72\" ","C","300 ft","(130# )","72","1800",76.88,1952.752,2.39,60.706,1831.34]
[null,"Cast iron pipe Class 400 ft (173# ) Size 3\" ","D","400 ft","(173# )","3","80",3.96,100.584,0.48,12.192,76.2]
[null,"Cast iron pipe Class 400 ft (173# ) Size 4\" ","D","400 ft","(173# )","4","100",5.0,127,0.52,13.208,100.584]
[null,"Cast iron pipe Class 400 ft (173# ) Size 6\" ","D","400 ft","(173# )","6","150",7.1,180.34,0.55,13.97,152.4]
[null,"Cast iron pipe Class 400 ft (173# ) Size 8\" ","D","400 ft","(173# )","8","200",9.3,236.22,0.6,15.24,205.74]
[null,"Cast iron pipe Class 400 ft (173# ) Size 10\" ","D","400 ft","(173# )","10","250",11.4,289.56,0.68,17.272,255.016]
[null,"Cast iron pipe Class 400 ft (173# ) Size 12\" ","D","400 ft","(173# )","12","300",13.5,342.9,0.75,19.05,304.8]
[null,"Cast iron pipe Class 400 ft (173# ) Size 14\" ","D","400 ft","(173# )","14","350",15.65,397.51,0.82,20.828,355.854]
[null,"Cast iron pipe Class 400 ft (173# ) Size 16\" ","D","400 ft","(173# )","16","400",17.8,452.12,0.89,22.606,406.908]
[null,"Cast iron pipe Class 400 ft (173# ) Size 18\" ","D","400 ft","(173# )","18","450",19.92,505.968,0.96,24.384,457.2]
[null,"Cast iron pipe Class 400 ft (173# ) Size 20\" ","D","400 ft","(173# )","20","500",22.06,560.324,1.03,26.162,508]
[null,"Cast iron pipe Class 400 ft (173# ) Size 24\" ","D","400 ft","(173# )","24","600",26.32,668.528,1.16,29.464,609.6]
[null,"Cast iron pipe Class 400 ft (173# ) Size 30\" ","D","400 ft","(173# )","30","750",32.74,831.596,1.37,34.798,762]
[null,"Cast iron pipe Class 400 ft (173# ) Size 36\" ","D","400 ft","(173# )","36","900",39.16,994.664,1.58,40.132,914.4]
[null,"Cast iron pipe Class 400 ft (173# ) Size 42\" ","D","400 ft","(173# )","42","1050",45.58,1157.732,1.78,45.212,1067.308]
[null,"Cast iron pipe Class 400 ft (173# ) Size 48\" ","D","400 ft","(173# )","48","1200",51.98,1320.292,1.96,49.784,1220.724]
[null,"Cast iron pipe Class 400 ft (173# ) Size 54\" ","D","400 ft","(173# )","54","1350",58.4,1483.36,2.23,56.642,1370.076]
[null,"Cast iron pipe Class 400 ft (173# ) Size 60\" ","D","400 ft","(173# )","60","1500",64.82,1646.428,2.38,60.452,1525.524]
[null,"Cast iron pipe Class 500 ft (217# ) Size 4\" ","E","500 ft","(217# )","4","100",7.22,183.388,0.58,14.732,153.924]
[null,"Cast iron pipe Class 500 ft (217# ) Size 6\" ","E","500 ft","(217# )","6","150",9.42,239.268,0.66,16.764,205.74]
[null,"Cast iron pipe Class 500 ft (217# ) Size 8\" ","E","500 ft","(217# )","8","200",11.6,294.64,0.74,18.796,257.048]
[null,"Cast iron pipe Class 500 ft (217# ) Size 10\" ","E","500 ft","(217# )","10","250",13.78,350.012,0.82,20.828,308.356]
[null,"Cast iron pipe Class 500 ft (217# ) Size 12\" ","E","500 ft","(217# )","12","300",15.98,405.892,0.9,22.86,360.172]
[null,"Cast iron pipe Class 500 ft (217# ) Size 14\" ","E","500 ft","(217# )","14","350",18.16,461.264,0.98,24.892,411.48]
[null,"Cast iron pipe Class 500 ft (217# ) Size 16\" ","E","500 ft","(217# )","16","400",20.34,516.636,1.07,27.178,462.28]
[null,"Cast iron pipe Class 500 ft (217# ) Size 18\" ","E","500 ft","(217# )","18","450",22.54,572.516,1.15,29.21,514.096]
[null,"Cast iron pipe Class 500 ft (217# ) Size 20\" ","E","500 ft","(217# )","20","500",26.9,683.26,1.31,33.274,616.712]
[null,"Cast iron pipe Class 500 ft (217# ) Size 24\" ","E","500 ft","(217# )","24","600",33.1,840.74,1.55,39.37,762]
[null,"Cast iron pipe Class 500 ft (217# ) Size 30\" ","E","500 ft","(217# )","30","750",39.6,1005.84,1.8,45.72,914.4]
[null,"Cast iron pipe Class 600 ft (260# ) Size 4\" ","F","600 ft","(260# )","4","100",7.22,183.388,0.61,15.494,152.4]
[null,"Cast iron pipe Class 600 ft (260# ) Size 6\" ","F","600 ft","(260# )","6","150",9.42,239.268,0.71,18.034,203.2]
[null,"Cast iron pipe Class 600 ft (260# ) Size 8\" ","F","600 ft","(260# )","8","200",11.6,294.64,0.8,20.32,254]
[null,"Cast iron pipe Class 600 ft (260# ) Size 10\" ","F","600 ft","(260# )","10","250",13.78,350.012,0.89,22.606,304.8]
[null,"Cast iron pipe Class 600 ft (260# ) Size 12\" ","F","600 ft","(260# )","12","300",15.98,405.892,0.99,25.146,355.6]
[null,"Cast iron pipe Class 600 ft (260# ) Size 14\" ","F","600 ft","(260# )","14","350",18.16,461.264,1.08,27.432,406.4]
[null,"Cast iron pipe Class 600 ft (260# ) Size 16\" ","F","600 ft","(260# )","16","400",20.34,516.636,1.17,29.718,457.2]
[null,"Cast iron pipe Class 600 ft (260# ) Size 18\" ","F","600 ft","(260# )","18","450",22.54,572.516,1.27,32.258,508]
[null,"Cast iron pipe Class 600 ft (260# ) Size 20\" ","F","600 ft","(260# )","20","500",26.9,683.26,1.45,36.83,609.6]
[null,"Cast iron pipe Class 600 ft (260# ) Size 24\" ","F","600 ft","(260# )","24","600",33.46,849.884,1.73,43.942,762]
[null,"Cast iron pipe Class 600 ft (260# ) Size 30\" ","F","600 ft","(260# )","30","750",40.04,1017.016,2.02,51.308,914.4]
[null,"Cast iron pipe Class 700 ft (304# ) Size 4\" ","G","700 ft","(304# )","4","100",7.38,187.452,0.65,16.51,154.432]
[null,"Cast iron pipe Class 700 ft (304# ) Size 6\" ","G","700 ft","(304# )","6","150",9.6,243.84,0.75,19.05,205.74]
[null,"Cast iron pipe Class 700 ft (304# ) Size 8\" ","G","700 ft","(304# )","8","200",11.84,300.736,0.86,21.844,257.048]
[null,"Cast iron pipe Class 700 ft (304# ) Size 10\" ","G","700 ft","(304# )","10","250",14.08,357.632,0.97,24.638,308.356]
[null,"Cast iron pipe Class 700 ft (304# ) Size 12\" ","G","700 ft","(304# )","12","300",16.32,414.528,1.07,27.178,360.172]
[null,"Cast iron pipe Class 700 ft (304# ) Size 14\" ","G","700 ft","(304# )","14","350",18.54,470.916,1.18,29.972,410.972]
[null,"Cast iron pipe Class 700 ft (304# ) Size 16\" ","G","700 ft","(304# )","16","400",20.78,527.812,1.28,32.512,462.788]
[null,"Cast iron pipe Class 700 ft (304# ) Size 18\" ","G","700 ft","(304# )","18","450",23.02,584.708,1.39,35.306,514.096]
[null,"Cast iron pipe Class 700 ft (304# ) Size 20\" ","G","700 ft","(304# )","20","500",27.76,705.104,1.75,44.45,616.204]
[null,"Cast iron pipe Class 800 ft (347# ) Size 4\" ","H","800 ft","(347# )","4","100",7.38,187.452,0.69,17.526,152.4]
[null,"Cast iron pipe Class 800 ft (347# ) Size 6\" ","H","800 ft","(347# )","6","150",9.6,243.84,0.8,20.32,203.2]
[null,"Cast iron pipe Class 800 ft (347# ) Size 8\" ","H","800 ft","(347# )","8","200",11.84,300.736,0.92,23.368,254]
[null,"Cast iron pipe Class 800 ft (347# ) Size 10\" ","H","800 ft","(347# )","10","250",14.08,357.632,1.04,26.416,304.8]
[null,"Cast iron pipe Class 800 ft (347# ) Size 12\" ","H","800 ft","(347# )","12","300",16.32,414.528,1.16,29.464,355.6]
[null,"Cast iron pipe Class 800 ft (347# ) Size 14\" ","H","800 ft","(347# )","14","350",18.54,470.916,1.27,32.258,406.4]
[null,"Cast iron pipe Class 800 ft (347# ) Size 16\" ","H","800 ft","(347# )","16","400",20.78,527.812,1.39,35.306,457.2]
[null,"Cast iron pipe Class 800 ft (347# ) Size 18\" ","H","800 ft","(347# )","18","450",23.02,584.708,1.51,38.354,508]
[null,"Cast iron pipe Class 800 ft (347# ) Size 20\" ","H","800 ft","(347# )","20","500",27.76,705.104,1.88,47.752,609.6]

{"sheet":"WN Flanges","index":5,"n_rows":42,"n_cols":8,"rows_kept":42,"cut":false,"hidden":false,"merged":[[0,0,0,8],[25,17,25,27],[52,10,52,27]]}
["WELDING NECK FLANGE & PIPE DIMENSIONS"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Flange dimensions"]
["D","Flange diam.",{"$f":"INDEX('Data WN flanges'!H$3:H$1755,'Data WN flanges'!$A$3)","v":1073.1},"mm"]
["H","Flange length",{"$f":"INDEX('Data WN flanges'!I$3:I$1755,'Data WN flanges'!$A$3)","v":93.7},"mm"]
["b","Flange thkn. incl. RF",{"$f":"INDEX('Data WN flanges'!J$3:J$1755,'Data WN flanges'!$A$3)","v":60.5},"mm",null,"Include data of following WN flanges:"]
["d1","Diam. raced face",{"$f":"INDEX('Data WN flanges'!K$3:K$1755,'Data WN flanges'!$A$3)","v":1000.3},"mm",null,"ANSI B 16.5",null,"125-2500#"]
["k","Pitch circle",{"$f":"INDEX('Data WN flanges'!L$3:L$1755,'Data WN flanges'!$A$3)","v":1025.7},"mm",null,"ANSI B 16.5 Long WN fl.",null,"150-2500#"]
["n","Number of bolts",{"$f":"INDEX('Data WN flanges'!M$3:M$1755,'Data WN flanges'!$A$3)","v":36},"pce",null,"ANSI B 16.31 Cast iron",null,"25-800#"]
["d2","Diam. boltholes",{"$f":"INDEX('Data WN flanges'!N$3:N$1755,'Data WN flanges'!$A$3)","v":25.4},"mm",null,"ANSI B 16.47 - API Std. 605",null,"75-900#"]
["d3","Diameter hub",{"$f":"INDEX('Data WN flanges'!O$3:O$1755,'Data WN flanges'!$A$3)","v":962.2},"mm",null,"ANSI B 16.47 - MSS SP-44",null,"150-900#"]
["f","Raced face height",{"$f":"INDEX('Data WN flanges'!P$3:P$1755,'Data WN flanges'!$A$3)","v":1.6},"mm",null,"BS 10 tables A-T",null,"43-1400#"]
["r","Round off",{"$f":"INDEX('Data WN flanges'!Q$3:Q$1755,'Data WN flanges'!$A$3)","v":"-"},"mm",null,"BS 10 Cast iron",null,"200#"]
["g","Thickness of gasket",{"$f":"INDEX('Data WN flanges'!R$3:R$1755,'Data WN flanges'!$A$3)","v":7},"mm",null,"BS 3293",null,"150-600#"]
["L","Required stud length",{"$f":"INDEX('Data WN flanges'!S$3:S$1755,'Data WN flanges'!$A$3)","v":182},"mm 1)",null,"BS 4772 Cast iron",null,"PN 10 -12"]
["bt","Bolt",{"$f":"INDEX('Data WN flanges'!T$3:T$1755,'Data WN flanges'!$A$3)","v":"M24"},null,null,"BS 4504",null,"PN 6 - 100"]
["m","Nut height",{"$f":"INDEX('Data WN flanges'!U$3:U$1755,'Data WN flanges'!$A$3)","v":19},"mm",null,"DIN 2630-2638",null,"PN 1-160"]
["W","Weight",{"$f":"INDEX('Data WN flanges'!V$3:V$1755,'Data WN flanges'!$A$3)","v":"-"},"kg",null,"DIN 2627-2629",null,"PN 250-400"]
[null,null,null,null,null,"DIN Cast iron 2532-33",null,"PN 10-16"]
["Surface finish",null,null,null,null,"DIN Cast iron 28604-07",null,"PN 10-40"]
[null,"Stock DN < 24\"","6,3-12,5","µm",null,"NEN 5831-5835",null,"PN 6 - 40"]
[null,"Stock DN > 24\"","12,5-25,0","µm",null,"JIS B 2210-2213",null,"PN 5-40"]
[null,"Smooth","3,2-6,3","µm",null,"Pressure vessels DIN 28034",null,"-"]
[]
["1)","for flange / flange connection"]

{"sheet":"Data WN flanges","index":6,"n_rows":1755,"n_cols":22,"rows_kept":1755,"cut":false,"hidden":true,"merged":[]}
["Data WN fanges",null," ",null,null,"Size","Size","Fl. diam.","Fl. height","Fl. thickn.","Diam. RF","Pitch circle","No. of bolts","Bolt hole","Diam. Hub","RF height","Round of","Gasket th.","Stud length","Bolt","Nut height","Weight"]
[null,"Type / Size / Rating","Type","Rating","Norm","NPS","DN","D","H","b","d1","k","n","d2","d3","f","r","g","L","bt","m","W"]
[48.0,{"$f":"CONCATENATE(C3,D3,$C$1,E3,$C$1,$F$1,$C$1,F3)","v":"WNRF 125# ANSI B16.5 Size 26\""},"WNRF"," 125#","ANSI B16.5","26\"",650.0,870.0,125.4,50.8,749.3,806.5,24.0,35.1,723.9,1.6,"-",7.0,{"$f":"(J3+U3+8)*2+R3","v":176.6},"M33",26.0,"-"]
[null,"WNRF 125# ANSI B16.5 Size 28\"","WNRF"," 125#","ANSI B16.5","28\"",700.0,927.1,126.9,52.3,800.1,863.6,28.0,35.1,781.1,1.6,"-",7.0,179.6,"M33",26.0,"-"]
[null,"WNRF 125# ANSI B16.5 Size 30\"","WNRF"," 125#","ANSI B16.5","30\"",750.0,984.3,128.7,54.1,857.3,914.4,28.0,35.1,831.9,1.6,"-",7.0,183.2,"M33",26.0,"-"]
[null,"WNRF 125# ANSI B16.5 Size 32\"","WNRF"," 125#","ANSI B16.5","32\"",800.0,1060.5,131.8,57.2,914.4,977.9,28.0,41.4,889.0,1.6,"-",7.0,189.4,"M36",26.0,"-"]
[null,"WNRF 125# ANSI B16.5 Size 34\"","WNRF"," 125#","ANSI B16.5","34\"",850.0,1111.3,133.3,58.7,965.2,1028.7,32.0,41.4,939.8,1.6,"-",7.0,192.4,"M36",26.0,"-"]
[null,"WNRF 125# ANSI B16.5 Size 36\"","WNRF"," 125#","ANSI B16.5","36\"",900.0,1168.4,135.1,60.5,1022.4,1086.0,32.0,41.4,997.0,1.6,"-",7.0,196,"M36",26.0,"-"]
[null,"WNRF 125# ANSI B16.5 Size 38\"","WNRF"," 125#","ANSI B16.5","38\"",950.0,1238.3,135.1,60.5,1073.2,1149.4,32.0,41.4,1060.5,1.6,"-",7.0,196,"M36",26.0,"-"]
[null,"WNRF 125# ANSI B16.5 Size 40\"","WNRF"," 125#","ANSI B16.5","40\"",1000.0,1289.1,138.1,63.5,1124.0,1200.2,36.0,41.4,1111.3,1.6,"-",7.0,208,"M36",29.0,"-"]
[null,"WNRF 125# ANSI B16.5 Size 42\"","WNRF"," 125#","ANSI B16.5","42\"",1050.0,1346.2,141.4,66.8,1193.8,1257.3,36.0,41.4,1168.4,1.6,"-",7.0,214.6,"M36",29.0,"-"]
[null,"WNRF 125# ANSI B16.5 Size 44\"","WNRF"," 125#","ANSI B16.5","44\"",1100.0,1403.4,141.4,66.8,1244.6,1314.5,40.0,41.4,1219.2,1.6,"-",7.0,214.6,"M36",29.0,"-"]
[null,"WNRF 125# ANSI B16.5 Size 46\"","WNRF"," 125#","ANSI B16.5","46\"",1150.0,1454.2,142.7,68.1,1295.4,1365.3,40.0,41.4,1270.0,1.6,"-",7.0,217.2,"M36",29.0,"-"]
[null,"WNRF 125# ANSI B16.5 Size 48\"","WNRF"," 125#","ANSI B16.5","48\"",1200.0,1511.3,144.5,69.85,1358.9,1422.4,44.0,41.4,1327.2,1.6,"-",7.0,220.7,"M36",29.0,"-"]
[null,"WNRF 125# ANSI B16.5 Size 50\"","WNRF"," 125#","ANSI B16.5","50\"",1250.0,1568.5,144.5,69.9,1409.7,1479.6,44.0,47.8,1378.0,1.6,"-",7.0,226.8,"M39",32.0,"-"]
[null,"WNRF 125# ANSI B16.5 Size 52\"","WNRF"," 125#","ANSI B16.5","52\"",1300.0,1625.6,147.8,73.2,1460.5,1536.7,44.0,47.8,1435.1,1.6,"-",7.0,233.4,"M39",32.0,"-"]
[null,"WNRF 125# ANSI B16.5 Size 54\"","WNRF"," 125#","ANSI B16.5","54\"",1350.0,1682.8,150.8,76.2,1517.7,1593.9,44.0,47.8,1492.3,1.6,"-",7.0,239.4,"M39",32.0,"-"]
[null,"WNRF 125# ANSI B16.5 Size 60\"","WNRF"," 125#","ANSI B16.5","60\"",1500.0,1854.2,154.1,79.5,1676.4,1759.0,52.0,47.8,1657.4,1.6,"-",7.0,246,"M39",32.0,"-"]
[null,"WNRF 150# ANSI B16.5 Size 1/2\"","WNRF"," 150#","ANSI B16.5","1/2\"",15.0,88.9,47.8,11.2,35.1,60.5,4.0,15.7,30.2,1.6,3.0,3.0,61.4,"M12",10.0,0.48]
[null,"WNRF 150# ANSI B16.5 Size 3/4\"","WNRF"," 150#","ANSI B16.5","3/4\"",20.0,98.6,52.3,12.7,42.9,69.9,4.0,15.7,38.1,1.6,3.0,3.0,64.4,"M12",10.0,0.71]
[null,"WNRF 150# ANSI B16.5 Size 1\"","WNRF"," 150#","ANSI B16.5","1\"",25.0,108.0,55.6,14.2,50.8,79.2,4.0,15.7,49.3,1.6,3.0,3.0,67.4,"M12",10.0,1.01]
[null,"WNRF 150# ANSI B16.5 Size 1¼\"","WNRF"," 150#","ANSI B16.5","1¼\"",32.0,117.3,57.2,15.7,63.5,88.9,4.0,15.7,58.7,1.6,4.8,3.0,70.4,"M12",10.0,1.33]
[null,"WNRF 150# ANSI B16.5 Size 1½\"","WNRF"," 150#","ANSI B16.5","1½\"",40.0,127.0,62.0,17.5,73.2,98.6,4.0,15.7,65.0,1.6,6.35,3.0,74,"M12",10.0,1.72]
[null,"WNRF 150# ANSI B16.5 Size 2\"","WNRF"," 150#","ANSI B16.5","2\"",50.0,152.4,63.5,19.1,91.9,120.7,4.0,19.1,77.7,1.6,7.87,4.0,84.2,"M16",13.0,2.58]
[null,"WNRF 150# ANSI B16.5 Size 2½\"","WNRF"," 150#","ANSI B16.5","2½\"",65.0,117.8,69.9,22.4,104.6,139.7,4.0,19.1,90.4,1.6,7.87,4.0,90.8,"M16",13.0,4.11]
[null,"WNRF 150# ANSI B16.5 Size 3\"","WNRF"," 150#","ANSI B16.5","3\"",80.0,190.5,69.9,23.9,127.0,152.4,4.0,19.1,108.0,1.6,9.65,4.0,93.8,"M16",13.0,4.92]
[null,"WNRF 150# ANSI B16.5 Size 3½\"","WNRF"," 150#","ANSI B16.5","3½\"","-",215.9,71.4,23.9,139.7,177.8,8.0,19.1,122.2,1.6,9.65,4.0,93.8,"M16",13.0,6.08]
[null,"WNRF 150# ANSI B16.5 Size 4\"","WNRF"," 150#","ANSI B16.5","4\"",100.0,228.6,76.2,23.9,157.2,190.5,8.0,19.1,134.9,1.6,11.18,5.0,94.8,"M16",13.0,6.84]
[null,"WNRF 150# ANSI B16.5 Size 5\"","WNRF"," 150#","ANSI B16.5","5\"",125.0,254.0,88.9,23.9,185.7,215.9,8.0,22.4,163.6,1.6,11.18,5.0,100.8,"M20",16.0,8.56]
[null,"WNRF 150# ANSI B16.5 Size 6\"","WNRF"," 150#","ANSI B16.5","6\"",150.0,279.4,88.9,25.4,215.9,241.3,8.0,22.4,192.0,1.6,12.7,6.0,104.8,"M20",16.0,10.6]
[null,"WNRF 150# ANSI B16.5 Size 8\"","WNRF"," 150#","ANSI B16.5","8\"",200.0,342.9,101.6,28.4,269.7,298.5,8.0,22.4,246.1,1.6,12.7,6.0,110.8,"M20",16.0,17.6]
[null,"WNRF 150# ANSI B16.5 Size 10\"","WNRF"," 150#","ANSI B16.5","10\"",250.0,406.4,101.6,30.2,323.9,362.0,12.0,25.4,304.8,1.6,12.7,6.0,120.4,"M24",19.0,24.0]
[null,"WNRF 150# ANSI B16.5 Size 12\"","WNRF"," 150#","ANSI B16.5","12\"",300.0,482.6,114.3,31.8,381.0,431.8,12.0,25.4,365.3,1.6,12.7,6.0,123.6,"M24",19.0,36.5]
[null,"WNRF 150# ANSI B16.5 Size 14\"","WNRF"," 150#","ANSI B16.5","14\"",350.0,533.4,127.0,35.1,412.8,476.3,12.0,28.4,400.1,1.6,12.7,7.0,137.2,"M27",22.0,48.4]
[null,"WNRF 150# ANSI B16.5 Size 16\"","WNRF"," 150#","ANSI B16.5","16\"",400.0,596.9,127.0,36.6,469.9,539.8,16.0,28.4,457.2,1.6,12.7,7.0,140.2,"M27",22.0,60.6]
[null,"WNRF 150# ANSI B16.5 Size 18\"","WNRF"," 150#","ANSI B16.5","18\"",450.0,635.0,139.7,39.6,533.4,577.9,16.0,31.8,505.0,1.6,12.7,7.0,150.2,"M30",24.0,68.3]
[null,"WNRF 150# ANSI B16.5 Size 20\"","WNRF"," 150#","ANSI B16.5","20\"",500.0,698.5,144.5,42.9,584.2,635.0,20.0,31.8,558.8,1.6,12.7,7.0,156.8,"M30",24.0,84.5]
[null,"WNRF 150# ANSI B16.5 Size 22\"","WNRF"," 150#","ANSI B16.5","22\"",550.0,749.3,149.2,46.0,641.2,692.1,20.0,34.9,609.6,1.6,12.7,7.0,167,"M33",26.0,102.0]
[null,"WNRF 150# ANSI B16.5 Size 24\"","WNRF"," 150#","ANSI B16.5","24\"",600.0,812.8,152.4,47.8,692.2,749.3,20.0,35.1,663.4,1.6,12.7,7.0,170.6,"M33",26.0,115.0]
[null,"WNRF 150# ANSI B16.5 Size 26\"","WNRF"," 150#","ANSI B16.5","26\"",650.0,869.9,127.0,50.8,742.9,806.4,24.0,34.9,723.9,1.6,12.7,7.0,176.6,"M33",26.0,118.0]
[null,"WNRF 150# ANSI B16.5 Size 30\"","WNRF"," 150#","ANSI B16.5","30\"",750.0,984.2,130.2,54.0,857.2,914.4,28.0,34.9,831.8,1.6,12.7,7.0,183,"M33",26.0,153.0]
[null,"WNRF 150# ANSI B16.5 Size 34\"","WNRF"," 150#","ANSI B16.5","34\"",850.0,1111.2,150.8,58.8,958.8,1028.7,32.0,41.3,911.2,1.6,12.7,7.0,202.6,"M39",31.0,212.0]
[null,"WNRF 150# ANSI B16.5 Size 36\"","WNRF"," 150#","ANSI B16.5","36\"",900.0,1168.4,161.9,60.3,1022.3,1085.8,32.0,41.3,966.8,1.6,12.7,7.0,205.6,"M39",31.0,242.0]
[null,"WNRF 150# ANSI B16.5 Size 42\"","WNRF"," 150#","ANSI B16.5","42\"",1050.0,1344.2,193.7,64.7,1193.8,1257.3,36.0,41.3,1131.9,1.6,12.7,7.0,214.4,"M39",31.0,358.0]
[null,"WNRF 175# ANSI B16.5 Size 26\"","WNRF"," 175#","ANSI B16.5","26\"",650.0,800.1,84.3,46.0,736.6,759.0,28.0,22.4,701.8,1.6,"-",7.0,147,"M20",16.0,"-"]
[null,"WNRF 175# ANSI B16.5 Size 28\"","WNRF"," 175#","ANSI B16.5","28\"",700.0,850.9,84.3,47.8,787.4,809.8,28.0,22.4,752.6,1.6,"-",7.0,150.6,"M20",16.0,"-"]
[null,"WNRF 175# ANSI B16.5 Size 30\"","WNRF"," 175#","ANSI B16.5","30\"",750.0,908.0,90.6,50.8,844.5,866.9,36.0,22.4,809.8,1.6,"-",7.0,156.6,"M20",16.0,"-"]
[null,"WNRF 175# ANSI B16.5 Size 32\"","WNRF"," 175#","ANSI B16.5","32\"",800.0,958.8,90.6,53.8,895.3,917.7,36.0,22.4,860.6,1.6,"-",7.0,162.6,"M20",16.0,"-"]
[null,"WNRF 175# ANSI B16.5 Size 34\"","WNRF"," 175#","ANSI B16.5","34\"",850.0,1022.3,93.7,57.1,949.5,974.9,36.0,25.4,911.4,1.6,"-",7.0,175.2,"M24",19.0,"-"]
[null,"WNRF 175# ANSI B16.5 Size 36\"","WNRF"," 175#","ANSI B16.5","36\"",900.0,1073.1,93.7,60.5,1000.3,1025.7,36.0,25.4,962.2,1.6,"-",7.0,182,"M24",19.0,"-"]
[null,"WNRF 175# ANSI B16.5 Size 38\"","WNRF"," 175#","ANSI B16.5","38\"",950.0,1124.0,103.3,63.5,1051.1,1076.5,36.0,25.4,1013.0,1.6,"-",7.0,188,"M24",19.0,"-"]
[null,"WNRF 175# ANSI B16.5 Size 40\"","WNRF"," 175#","ANSI B16.5","40\"",1000.0,1174.8,103.3,66.5,1101.9,1127.3,40.0,25.4,1063.8,1.6,"-",7.0,194,"M24",19.0,"-"]
[null,"WNRF 175# ANSI B16.5 Size 42\"","WNRF"," 175#","ANSI B16.5","42\"",1050.0,1244.6,112.7,69.8,1162.1,1190.8,40.0,28.7,1120.9,1.6,"-",7.0,206.6,"M27",22.0,"-"]
[null,"WNRF 175# ANSI B16.5 Size 44\"","WNRF"," 175#","ANSI B16.5","44\"",1100.0,1295.4,112.7,73.2,1212.8,1241.6,40.0,28.7,1171.7,1.6,"-",7.0,213.4,"M27",22.0,"-"]
[null,"WNRF 175# ANSI B16.5 Size 46\"","WNRF"," 175#","ANSI B16.5","46\"",1150.0,1346.2,112.7,76.2,1263.6,1292.4,40.0,28.7,1222.5,1.6,"-",7.0,219.4,"M27",22.0,"-"]
[null,"WNRF 175# ANSI B16.5 Size 48\"","WNRF"," 175#","ANSI B16.5","48\"",1200.0,1397.0,122.4,79.2,1314.4,1343.2,44.0,28.7,1273.3,1.6,"-",7.0,225.4,"M27",22.0,"-"]
[null,"WNRF 175# ANSI B16.5 Size 50\"","WNRF"," 175#","ANSI B16.5","50\"",1250.0,1447.8,122.4,82.5,1365.3,1394.3,44.0,28.7,1324.1,1.6,"-",7.0,232,"M27",22.0,"-"]
[null,"WNRF 175# ANSI B16.5 Size 52\"","WNRF"," 175#","ANSI B16.5","52\"",1300.0,1511.3,135.1,85.9,1422.4,1454.1,44.0,31.8,1377.9,1.6,"-",7.0,242.8,"M30",24.0,"-"]
[null,"WNRF 175# ANSI B16.5 Size 54\"","WNRF"," 175#","ANSI B16.5","54\"",1350.0,1562.1,135.1,88.9,1473.2,1504.9,44.0,31.8,1428.8,1.6,"-",7.0,248.8,"M30",24.0,"-"]
[null,"WNRF 175# ANSI B16.5 Size 60\"","WNRF"," 175#","ANSI B16.5","60\"",1500.0,1714.5,144.4,98.6,1625.6,1657.3,48.0,31.8,1581.1,1.6,"-",7.0,268.2,"M30",24.0,"-"]
[null,"WNRF 175# ANSI B16.5 Size 66\"","WNRF"," 175#","ANSI B16.5","66\"",1650.0,1866.9,154.1,107.9,1778.0,1809.9,56.0,31.8,1739.9,1.6,"-",7.0,286.8,"M30",24.0,"-"]
[null,"WNRF 175# ANSI B16.5 Size 72\"","WNRF"," 175#","ANSI B16.5","72\"",1800.0,2032.0,166.8,114.3,1943.1,1974.8,64.0,31.8,1892.3,1.6,"-",7.0,299.6,"M30",24.0,"-"]
[null,"WNRF 300# ANSI B16.5 Size 1/2\"","WNRF"," 300#","ANSI B16.5","1/2\"",15.0,95.2,52.4,14.3,35.0,66.5,4.0,15.7,38.1,1.6,3.0,3.0,67.6,"M12",10.0,0.75]
[null,"WNRF 300# ANSI B16.5 Size 3/4\"","WNRF"," 300#","ANSI B16.5","3/4\"",20.0,117.5,57.1,15.9,42.9,82.5,4.0,19.0,47.7,1.6,3.0,3.0,76.8,"M16",13.0,1.26]
[null,"WNRF 300# ANSI B16.5 Size 1\"","WNRF"," 300#","ANSI B16.5","1\"",25.0,123.8,61.9,17.5,50.8,88.9,4.0,19.0,53.8,1.6,3.0,3.0,80,"M16",13.0,1.52]
[null,"WNRF 300# ANSI B16.5 Size 1¼\"","WNRF"," 300#","ANSI B16.5","1¼\"",32.0,133.3,65.1,19.0,63.5,98.5,4.0,19.0,63.5,1.6,4.8,3.0,83,"M16",13.0,2.03]
[null,"WNRF 300# ANSI B16.5 Size 1½\"","WNRF"," 300#","ANSI B16.5","1½\"",40.0,155.6,68.3,20.6,73.1,114.3,4.0,22.3,69.8,1.6,6.35,3.0,92.2,"M20",16.0,2.89]
[null,"WNRF 300# ANSI B16.5 Size 2\"","WNRF"," 300#","ANSI B16.5","2\"",50.0,165.1,69.8,22.3,91.9,127.0,8.0,19.0,84.0,1.6,7.87,4.0,90.6,"M16",13.0,3.4]
[null,"WNRF 300# ANSI B16.5 Size 2½\"","WNRF"," 300#","ANSI B16.5","2½\"",65.0,190.5,76.2,25.4,104.6,149.3,8.0,22.3,100.0,1.6,7.87,4.0,102.8,"M20",16.0,5.17]
[null,"WNRF 300# ANSI B16.5 Size 3\"","WNRF"," 300#","ANSI B16.5","3\"",80.0,209.5,79.4,28.4,127.0,168.1,8.0,22.3,117.3,1.6,9.65,4.0,108.8,"M20",16.0,6.93]
[null,"WNRF 300# ANSI B16.5 Size 3½\"","WNRF"," 300#","ANSI B16.5","3½\"","-",228.6,81.0,30.2,139.7,184.1,8.0,22.3,133.3,1.6,9.65,4.0,112.4,"M20",16.0,8.67]
[null,"WNRF 300# ANSI B16.5 Size 4\"","WNRF"," 300#","ANSI B16.5","4\"",100.0,254.0,85.7,31.7,157.2,200.1,8.0,22.3,146.0,1.6,11.18,5.0,116.4,"M20",16.0,11.2]
[null,"WNRF 300# ANSI B16.5 Size 5\"","WNRF"," 300#","ANSI B16.5","5\"",125.0,279.4,98.4,35.0,185.6,234.9,8.0,22.3,177.8,1.6,11.18,5.0,123,"M20",16.0,15.1]
[null,"WNRF 300# ANSI B16.5 Size 6\"","WNRF"," 300#","ANSI B16.5","6\"",150.0,317.5,98.4,36.5,215.9,269.7,12.0,22.3,206.2,1.6,12.7,6.0,127,"M20",16.0,19.1]
[null,"WNRF 300# ANSI B16.5 Size 8\"","WNRF"," 300#","ANSI B16.5","8\"",200.0,381.0,111.1,41.1,269.7,330.2,12.0,25.4,260.3,1.6,12.7,6.0,142.2,"M24",19.0,29.9]
[null,"WNRF 300# ANSI B16.5 Size 10\"","WNRF"," 300#","ANSI B16.5","10\"",250.0,444.5,117.5,47.7,323.8,387.3,16.0,28.4,320.5,1.6,12.7,6.0,161.4,"M27",22.0,42.7]
[null,"WNRF 300# ANSI B16.5 Size 12\"","WNRF"," 300#","ANSI B16.5","12\"",300.0,520.7,130.2,50.8,381.0,450.8,16.0,31.7,374.6,1.6,12.7,6.0,171.6,"M30",24.0,61.8]
[null,"WNRF 300# ANSI B16.5 Size 14\"","WNRF"," 300#","ANSI B16.5","14\"",350.0,584.2,142.9,53.8,412.7,514.3,20.0,31.7,425.4,1.6,12.7,7.0,178.6,"M30",24.0,85.8]
[null,"WNRF 300# ANSI B16.5 Size 16\"","WNRF"," 300#","ANSI B16.5","16\"",400.0,647.7,146.0,57.1,469.9,571.5,20.0,35.0,482.6,1.6,12.7,7.0,189.2,"M33",26.0,106.0]
[null,"WNRF 300# ANSI B16.5 Size 18\"","WNRF"," 300#","ANSI B16.5","18\"",450.0,711.2,158.7,60.4,533.4,628.6,24.0,35.0,533.4,1.6,12.7,7.0,195.8,"M33",26.0,131.0]
[null,"WNRF 300# ANSI B16.5 Size 20\"","WNRF"," 300#","ANSI B16.5","20\"",500.0,774.7,161.9,63.5,584.2,685.8,24.0,35.0,587.2,1.6,12.7,7.0,202,"M33",26.0,158.0]
[null,"WNRF 300# ANSI B16.5 Size 22\"","WNRF"," 300#","ANSI B16.5","22\"",550.0,838.2,165.1,66.7,641.2,742.9,24.0,41.3,641.2,1.6,12.7,7.0,218.4,"M39",31.0,195.0]
[null,"WNRF 300# ANSI B16.5 Size 24\"","WNRF"," 300#","ANSI B16.5","24\"",600.0,914.4,168.3,69.8,692.1,812.8,24.0,41.1,701.5,1.6,12.7,7.0,224.6,"M39",31.0,230.0]
[null,"WNRF 300# ANSI B16.5 Size 26\"","WNRF"," 300#","ANSI B16.5","26\"",650.0,971.5,184.1,79.4,749.3,876.3,28.0,44.4,720.7,1.6,12.7,7.0,249.8,"M42",34.0,279.0]
[null,"WNRF 300# ANSI B16.5 Size 30\"","WNRF"," 300#","ANSI B16.5","30\"",750.0,1092.2,209.5,92.1,857.2,996.9,28.0,47.6,827.1,1.6,12.7,7.0,279.2,"M45",36.0,390.0]
[null,"WNRF 300# ANSI B16.5 Size 34\"","WNRF"," 300#","ANSI B16.5","34\"",850.0,1206.5,231.8,1016.0,965.2,1104.9,28.0,50.8,936.6,1.6,12.7,7.0,2131,"M48",38.0,504.0]
[null,"WNRF 300# ANSI B16.5 Size 36\"","WNRF"," 300#","ANSI B16.5","36\"",900.0,1270.0,241.3,104.8,1022.3,1168.4,32.0,54.0,990.6,1.6,12.7,7.0,316.6,"M52",42.0,560.0]
[null,"WNRF 300# ANSI B16.5 Size 42\"","WNRF"," 300#","ANSI B16.5","42\"",1050.0,1447.8,276.2,117.5,1193.8,1339.8,36.0,54.0,1154.1,1.6,12.7,7.0,342,"M52",42.0,790.0]
[null,"WNRF 350# ANSI B16.5 Size 26\"","WNRF"," 350#","ANSI B16.5","26\"",650.0,831.8,125.4,63.5,749.3,777.7,28.0,28.4,708.2,1.6,"-",7.0,194,"M27",22.0,"-"]
[null,"WNRF 350# ANSI B16.5 Size 28\"","WNRF"," 350#","ANSI B16.5","28\"",700.0,882.6,125.4,63.5,800.1,828.5,28.0,28.4,759.0,1.6,"-",7.0,194,"M27",22.0,"-"]
[null,"WNRF 350# ANSI B16.5 Size 30\"","WNRF"," 350#","ANSI B16.5","30\"",750.0,939.8,131.7,66.5,857.3,886.0,32.0,28.4,815.8,1.6,"-",7.0,200,"M27",22.0,"-"]
[null,"WNRF 350# ANSI B16.5 Size 32\"","WNRF"," 350#","ANSI B16.5","32\"",800.0,990.6,138.1,69.8,908.0,936.8,36.0,28.4,866.6,1.6,"-",7.0,206.6,"M27",22.0,"-"]
[null,"WNRF 350# ANSI B16.5 Size 34\"","WNRF"," 350#","ANSI B16.5","34\"",850.0,1041.4,144.4,73.2,958.8,987.6,40.0,28.4,917.4,1.6,"-",7.0,213.4,"M27",22.0,"-"]
[null,"WNRF 350# ANSI B16.5 Size 36\"","WNRF"," 350#","ANSI B16.5","36\"",900.0,1111.3,153.8,79.2,1022.3,1054.1,40.0,31.8,977.9,1.6,"-",7.0,229.4,"M30",24.0,"-"]
[null,"WNRF 350# ANSI B16.5 Size 38\"","WNRF"," 350#","ANSI B16.5","38\"",950.0,1162.1,153.8,79.2,1073.1,1104.9,40.0,31.8,1028.7,1.6,"-",7.0,229.4,"M30",24.0,"-"]
[null,"WNRF 350# ANSI B16.5 Size 40\"","WNRF"," 350#","ANSI B16.5","40\"",1000.0,1212.8,157.2,82.5,1124.0,1155.7,44.0,31.8,1079.5,1.6,"-",7.0,236,"M30",24.0,"-"]
[null,"WNRF 350# ANSI B16.5 Size 42\"","WNRF"," 350#","ANSI B16.5","42\"",1050.0,1270.0,163.5,88.9,1181.1,1212.8,48.0,31.8,1136.6,1.6,"-",7.0,248.8,"M30",24.0,"-"]
[null,"WNRF 350# ANSI B16.5 Size 44\"","WNRF"," 350#","ANSI B16.5","44\"",1100.0,1339.8,169.36,95.3,1241.6,1276.3,44.0,35.1,1187.5,1.6,"-",7.0,265.6,"M33",26.0,"-"]
[null,"WNRF 350# ANSI B16.5 Size 46\"","WNRF"," 350#","ANSI B16.5","46\"",1150.0,1390.6,182.5,107.9,1292.4,1327.1,48.0,35.1,1238.3,1.6,"-",7.0,290.8,"M33",26.0,"-"]
[null,"WNRF 350# ANSI B16.5 Size 48\"","WNRF"," 350#","ANSI B16.5","48\"",1200.0,1441.4,182.5,107.9,1343.2,1377.9,48.0,35.1,1289.1,1.6,"-",7.0,290.8,"M33",26.0,"-"]
[null,"WNRF 400# ANSI B16.5 Size 1/2\"","WNRF"," 400#","ANSI B16.5","1/2\"",15.0,95.3,58.7,20.6,35.1,66.5,4.0,15.7,38.1,6.4,3.0,3.0,80.2,"M12",10.0,0.87]
[null,"WNRF 400# ANSI B16.5 Size 3/4\"","WNRF"," 400#","ANSI B16.5","3/4\"",20.0,117.3,63.6,22.1,42.9,82.6,4.0,19.1,47.8,6.4,3.0,3.0,89.2,"M16",13.0,1.45]
[null,"WNRF 400# ANSI B16.5 Size 1\"","WNRF"," 400#","ANSI B16.5","1\"",25.0,124.0,68.4,23.9,50.8,88.9,4.0,19.1,53.8,6.4,3.0,3.0,92.8,"M16",13.0,1.76]
[null,"WNRF 400# ANSI B16.5 Size 1¼\"","WNRF"," 400#","ANSI B16.5","1¼\"",32.0,133.4,72.9,27.0,63.5,98.6,4.0,19.1,63.5,6.4,4.8,3.0,99,"M16",13.0,2.49]
[null,"WNRF 400# ANSI B16.5 Size 1½\"","WNRF"," 400#","ANSI B16.5","1½\"",40.0,155.4,76.3,28.4,73.2,114.3,4.0,22.4,69.9,6.4,6.35,3.0,107.8,"M20",16.0,3.49]
[null,"WNRF 400# ANSI B16.5 Size 2\"","WNRF"," 400#","ANSI B16.5","2\"",50.0,165.1,79.6,31.8,91.9,127.0,8.0,19.1,84.1,6.4,7.87,4.0,109.6,"M16",13.0,4.36]
[null,"WNRF 400# ANSI B16.5 Size 2½\"","WNRF"," 400#","ANSI B16.5","2½\"",65.0,190.5,85.6,34.8,104.6,149.4,8.0,22.4,100.1,6.4,7.87,4.0,121.6,"M20",16.0,6.43]
[null,"WNRF 400# ANSI B16.5 Size 3\"","WNRF"," 400#","ANSI B16.5","3\"",80.0,209.6,89.0,38.4,127.0,168.1,8.0,22.4,117.3,6.4,9.65,4.0,128.8,"M20",16.0,8.53]
[null,"WNRF 400# ANSI B16.5 Size 3½\"","WNRF"," 400#","ANSI B16.5","3½\"","-",228.6,92.3,41.5,139.7,184.2,8.0,25.4,133.4,6.4,9.65,4.0,141,"M24",19.0,10.7]
[null,"WNRF 400# ANSI B16.5 Size 4\"","WNRF"," 400#","ANSI B16.5","4\"",100.0,254.0,95.3,41.5,157.2,200.2,8.0,25.4,146.1,6.4,11.18,5.0,142,"M24",19.0,12.8]
[null,"WNRF 400# ANSI B16.5 Size 5\"","WNRF"," 400#","ANSI B16.5","5\"",125.0,279.4,108.0,44.5,185.7,235.0,8.0,25.4,177.8,6.4,11.18,5.0,148,"M24",19.0,16.9]
[null,"WNRF 400# ANSI B16.5 Size 6\"","WNRF"," 400#","ANSI B16.5","6\"",150.0,317.5,109.5,47.5,215.9,269.7,12.0,25.4,206.2,6.4,12.7,6.0,155,"M24",19.0,22.0]
[null,"WNRF 400# ANSI B16.5 Size 8\"","WNRF"," 400#","ANSI B16.5","8\"",200.0,381.0,123.7,54.4,269.7,330.2,12.0,28.4,260.4,6.4,12.7,6.0,174.8,"M27",22.0,34.7]
[null,"WNRF 400# ANSI B16.5 Size 10\"","WNRF"," 400#","ANSI B16.5","10\"",250.0,444.5,130.4,60.2,323.9,387.4,16.0,31.8,320.5,6.4,12.7,6.0,190.4,"M30",24.0,48.5]
[null,"WNRF 400# ANSI B16.5 Size 12\"","WNRF"," 400#","ANSI B16.5","12\"",300.0,520.7,143.1,63.6,381.0,450.9,16.0,35.1,374.7,6.4,12.7,6.0,201.2,"M33",26.0,69.6]
[null,"WNRF 400# ANSI B16.5 Size 14\"","WNRF"," 400#","ANSI B16.5","14\"",350.0,584.2,155.8,66.9,412.8,514.4,20.0,35.1,425.5,6.4,12.7,7.0,208.8,"M33",26.0,95.5]
[null,"WNRF 400# ANSI B16.5 Size 16\"","WNRF"," 400#","ANSI B16.5","16\"",400.0,647.7,158.8,69.9,469.9,571.5,20.0,38.1,482.6,6.4,12.7,7.0,220.8,"M36",29.0,118.0]
[null,"WNRF 400# ANSI B16.5 Size 18\"","WNRF"," 400#","ANSI B16.5","18\"",450.0,711.2,171.5,72.9,533.4,628.7,24.0,38.1,533.4,6.4,12.7,7.0,226.8,"M36",29.0,145.0]
[null,"WNRF 400# ANSI B16.5 Size 20\"","WNRF"," 400#","ANSI B16.5","20\"",500.0,774.7,174.5,76.3,584.2,685.8,24.0,41.1,587.2,6.4,12.7,7.0,237.6,"M39",31.0,173.0]
[null,"WNRF 400# ANSI B16.5 Size 24\"","WNRF"," 400#","ANSI B16.5","24\"",600.0,914.4,181.2,82.6,692.2,812.8,24.0,47.8,701.5,6.4,12.7,7.0,260.2,"M45",36.0,249.0]
[null,"WNRF 600# ANSI B16.5 Size 1/2\"","WNRF"," 600#","ANSI B16.5","1/2\"",15.0,95.3,58.7,20.6,35.1,66.5,4.0,15.7,38.1,6.4,3.0,3.0,80.2,"M12",10.0,0.87]
[null,"WNRF 600# ANSI B16.5 Size 3/4\"","WNRF"," 600#","ANSI B16.5","3/4\"",20.0,117.3,63.6,22.1,42.9,82.6,4.0,19.1,47.8,6.4,3.0,3.0,89.2,"M16",13.0,1.45]
[null,"WNRF 600# ANSI B16.5 Size 1\"","WNRF"," 600#","ANSI B16.5","1\"",25.0,124.0,68.4,23.9,50.8,88.9,4.0,19.1,53.8,6.4,3.0,3.0,92.8,"M16",13.0,1.76]
[null,"WNRF 600# ANSI B16.5 Size 1¼\"","WNRF"," 600#","ANSI B16.5","1¼\"",32.0,133.4,72.9,27.0,63.5,98.6,4.0,19.1,63.5,6.4,4.8,3.0,99,"M16",13.0,2.49]
[null,"WNRF 600# ANSI B16.5 Size 1½\"","WNRF"," 600#","ANSI B16.5","1½\"",40.0,155.4,76.3,28.4,73.2,114.3,4.0,22.3,69.9,6.4,6.35,3.0,107.8,"M20",16.0,3.49]
[null,"WNRF 600# ANSI B16.5 Size 2\"","WNRF"," 600#","ANSI B16.5","2\"",50.0,165.1,79.6,31.8,91.9,127.0,8.0,19.1,84.1,6.4,7.87,4.0,109.6,"M16",13.0,4.36]
[null,"WNRF 600# ANSI B16.5 Size 2½\"","WNRF"," 600#","ANSI B16.5","2½\"",65.0,190.5,85.6,34.8,104.6,149.4,8.0,22.4,100.1,6.4,7.87,4.0,121.6,"M20",16.0,6.43]
[null,"WNRF 600# ANSI B16.5 Size 3\"","WNRF"," 600#","ANSI B16.5","3\"",80.0,209.6,89.0,38.4,127.0,168.1,8.0,22.4,117.3,6.4,9.65,4.0,128.8,"M20",16.0,8.53]
[null,"WNRF 600# ANSI B16.5 Size 3½\"","WNRF"," 600#","ANSI B16.5","3½\"","-",228.6,92.3,41.5,139.7,184.2,8.0,25.4,133.4,6.4,9.65,4.0,141,"M24",19.0,10.7]
[null,"WNRF 600# ANSI B16.5 Size 4\"","WNRF"," 600#","ANSI B16.5","4\"",100.0,273.1,108.0,44.5,157.2,215.9,8.0,25.4,152.4,6.4,11.18,5.0,148,"M24",19.0,17.4]
[null,"WNRF 600# ANSI B16.5 Size 5\"","WNRF"," 600#","ANSI B16.5","5\"",125.0,330.2,120.7,50.9,185.7,266.7,8.0,28.4,189.0,6.4,11.18,5.0,166.8,"M27",22.0,29.2]
[null,"WNRF 600# ANSI B16.5 Size 6\"","WNRF"," 600#","ANSI B16.5","6\"",150.0,355.6,133.7,54.2,215.9,292.1,12.0,28.4,222.3,6.4,12.7,6.0,174.4,"M27",22.0,34.9]
[null,"WNRF 600# ANSI B16.5 Size 8\"","WNRF"," 600#","ANSI B16.5","8\"",200.0,419.1,139.8,62.0,269.7,349.3,12.0,31.8,273.1,6.4,12.7,6.0,194,"M30",24.0,53.9]
[null,"WNRF 600# ANSI B16.5 Size 10\"","WNRF"," 600#","ANSI B16.5","10\"",250.0,508.0,158.8,69.9,323.9,431.8,16.0,35.1,342.9,6.4,12.7,6.0,213.8,"M33",26.0,86.5]
[null,"WNRF 600# ANSI B16.5 Size 12\"","WNRF"," 600#","ANSI B16.5","12\"",300.0,558.8,161.8,72.9,381.0,489.0,20.0,35.1,400.1,6.4,12.7,6.0,219.8,"M33",26.0,103.0]
[null,"WNRF 600# ANSI B16.5 Size 14\"","WNRF"," 600#","ANSI B16.5","14\"",350.0,603.3,171.5,76.3,412.8,527.1,20.0,38.1,431.8,6.4,12.7,7.0,233.6,"M36",29.0,158.0]
[null,"WNRF 600# ANSI B16.5 Size 16\"","WNRF"," 600#","ANSI B16.5","16\"",400.0,685.8,184.2,82.6,469.9,603.3,20.0,41.1,495.3,6.4,12.7,7.0,250.2,"M39",31.0,219.0]
[null,"WNRF 600# ANSI B16.5 Size 18\"","WNRF"," 600#","ANSI B16.5","18\"",450.0,743.0,190.6,89.0,533.4,654.1,20.0,44.5,546.1,6.4,12.7,7.0,269,"M42",34.0,252.0]
[null,"WNRF 600# ANSI B16.5 Size 20\"","WNRF"," 600#","ANSI B16.5","20\"",500.0,812.8,196.9,95.3,584.2,723.9,24.0,44.5,609.6,6.4,12.7,7.0,281.6,"M42",34.0,313.0]
[null,"WNRF 600# ANSI B16.5 Size 22\"","WNRF"," 600#","ANSI B16.5","22\"",550.0,869.9,203.2,99.6,641.2,777.9,24.0,47.6,666.7,6.4,12.7,7.0,294.2,"M45",36.0,380.0]
[null,"WNRF 600# ANSI B16.5 Size 24\"","WNRF"," 600#","ANSI B16.5","24\"",600.0,939.8,209.6,108.0,692.2,838.2,24.0,50.8,717.6,6.4,12.7,7.0,315,"M48",38.0,444.0]
[null,"WNRF 600# ANSI B16.5 Size 26\"","WNRF"," 600#","ANSI B16.5","26\"",650.0,1016.0,228.6,114.3,749.3,914.4,28.0,50.8,747.7,6.4,12.7,8.0,328.6,"M48",38.0,487.0]
[null,"WNRF 600# ANSI B16.5 Size 30\"","WNRF"," 600#","ANSI B16.5","30\"",750.0,1130.3,254.0,120.7,857.2,1022.3,28.0,54.0,862.0,6.4,12.7,9.0,350.4,"M52",42.0,559.0]
[null,"WNRF 600# ANSI B16.5 Size 34\"","WNRF"," 600#","ANSI B16.5","34\"",850.0,1244.6,276.3,127.0,965.2,1130.3,28.0,60.3,973.1,6.4,12.7,10.0,370,"M56",45.0,689.0]
[null,"WNRF 600# ANSI B16.5 Size 36\"","WNRF"," 600#","ANSI B16.5","36\"",900.0,1314.4,289.0,130.2,1022.3,1193.8,28.0,66.7,1031.9,6.4,12.7,11.0,389.4,"M64",51.0,780.0]
[null,"WNRF 600# ANSI B16.5 Size 42\"","WNRF"," 600#","ANSI B16.5","42\"",1050.0,1492.2,330.2,146.1,1193.8,1365.2,28.0,73.0,1201.7,6.4,12.7,12.0,430.2,"M68",55.0,1096.0]
[null,"WNRF 900# ANSI B16.5 Size 1/2\"","WNRF"," 900#","ANSI B16.5","1/2\"",15.0,120.6,66.8,28.7,35.0,82.5,4.0,22.3,38.1,6.4,3.0,3.0,108.4,"M20",16.0,1.87]
[null,"WNRF 900# ANSI B16.5 Size 3/4\"","WNRF"," 900#","ANSI B16.5","3/4\"",20.0,130.0,76.2,31.8,42.9,88.9,4.0,22.3,44.4,6.4,3.0,3.0,114.6,"M20",16.0,2.56]
[null,"WNRF 900# ANSI B16.5 Size 1\"","WNRF"," 900#","ANSI B16.5","1\"",25.0,149.3,79.5,34.8,50.8,101.6,4.0,25.4,52.3,6.4,3.0,3.0,126.6,"M24",19.0,3.74]
[null,"WNRF 900# ANSI B16.5 Size 1¼\"","WNRF"," 900#","ANSI B16.5","1¼\"",32.0,158.7,79.5,34.8,63.5,111.2,4.0,25.4,63.5,6.4,4.8,3.0,126.6,"M24",19.0,4.33]
[null,"WNRF 900# ANSI B16.5 Size 1½\"","WNRF"," 900#","ANSI B16.5","1½\"",40.0,177.8,88.9,38.1,73.1,123.9,4.0,28.4,69.8,6.4,6.35,3.0,139.2,"M27",22.0,5.94]
[null,"WNRF 900# ANSI B16.5 Size 2\"","WNRF"," 900#","ANSI B16.5","2\"",50.0,215.9,108.0,44.5,91.9,165.1,8.0,25.4,104.6,6.4,7.87,4.0,147,"M24",19.0,10.8]
[null,"WNRF 900# ANSI B16.5 Size 2½\"","WNRF"," 900#","ANSI B16.5","2½\"",65.0,244.3,111.0,47.5,104.6,190.5,8.0,28.4,123.9,6.4,7.87,4.0,159,"M27",22.0,15.0]
[null,"WNRF 900# ANSI B16.5 Size 3\"","WNRF"," 900#","ANSI B16.5","3\"",80.0,241.3,108.0,44.5,127.0,190.5,8.0,25.4,127.0,6.4,9.65,4.0,141,"M20",16.0,13.7]
[null,"WNRF 900# ANSI B16.5 Size 4\"","WNRF"," 900#","ANSI B16.5","4\"",100.0,292.1,120.7,50.8,157.2,234.9,8.0,31.7,158.7,6.4,11.18,5.0,166.6,"M27",22.0,22.5]
[null,"WNRF 900# ANSI B16.5 Size 5\"","WNRF"," 900#","ANSI B16.5","5\"",125.0,349.2,133.4,57.2,185.6,279.4,8.0,35.0,190.5,6.4,11.18,5.0,187.4,"M33",26.0,37.4]
[null,"WNRF 900# ANSI B16.5 Size 6\"","WNRF"," 900#","ANSI B16.5","6\"",150.0,381.0,146.1,62.0,215.9,317.5,12.0,31.7,234.9,6.4,12.7,6.0,190,"M27",22.0,47.7]
[null,"WNRF 900# ANSI B16.5 Size 8\"","WNRF"," 900#","ANSI B16.5","8\"",200.0,469.9,168.4,69.9,269.7,393.7,12.0,38.1,298.4,6.4,12.7,6.0,219.8,"M36",29.0,81.3]
[null,"WNRF 900# ANSI B16.5 Size 10\"","WNRF"," 900#","ANSI B16.5","10\"",250.0,546.1,190.5,76.2,323.8,169.9,16.0,38.1,368.3,6.4,12.7,6.0,232.4,"M36",29.0,119.0]
[null,"WNRF 900# ANSI B16.5 Size 12\"","WNRF"," 900#","ANSI B16.5","12\"",300.0,609.6,206.5,85.6,381.0,533.4,20.0,38.1,419.1,6.4,12.7,6.0,251.2,"M36",29.0,157.0]
[null,"WNRF 900# ANSI B16.5 Size 14\"","WNRF"," 900#","ANSI B16.5","14\"",350.0,641.3,219.2,92.2,412.7,558.8,20.0,41.1,450.8,6.4,12.7,7.0,265.4,"M39",29.0,180.0]
[null,"WNRF 900# ANSI B16.5 Size 16\"","WNRF"," 900#","ANSI B16.5","16\"",400.0,704.8,222.3,95.3,469.9,615.9,20.0,44.4,508.0,6.4,12.7,7.0,281.6,"M42",34.0,217.0]
[null,"WNRF 900# ANSI B16.5 Size 18\"","WNRF"," 900#","ANSI B16.5","18\"",450.0,787.4,235.0,108.0,533.4,685.8,20.0,50.8,565.1,6.4,12.7,7.0,315,"M48",38.0,292.0]
[null,"WNRF 900# ANSI B16.5 Size 20\"","WNRF"," 900#","ANSI B16.5","20\"",500.0,857.2,254.0,114.3,584.2,749.3,20.0,53.8,622.3,6.4,12.7,7.0,335.6,"M52",42.0,362.0]
[null,"WNRF 900# ANSI B16.5 Size 24\"","WNRF"," 900#","ANSI B16.5","24\"",600.0,1041.4,298.5,146.1,692.1,901.7,20.0,66.5,749.3,6.4,12.7,7.0,417.2,"M64",51.0,665.0]
[null,"WNRF 1500# ANSI B16.5 Size 1/2\"","WNRF"," 1500#","ANSI B16.5","1/2\"",15.0,120.6,66.8,28.7,35.0,82.5,4.0,22.3,38.1,6.4,3.0,3.0,108.4,"M20",16.0,1.87]
[null,"WNRF 1500# ANSI B16.5 Size 3/4\"","WNRF"," 1500#","ANSI B16.5","3/4\"",20.0,130.0,76.2,31.8,42.9,88.9,4.0,22.3,44.4,6.4,3.0,3.0,114.6,"M20",16.0,2.56]
[null,"WNRF 1500# ANSI B16.5 Size 1\"","WNRF"," 1500#","ANSI B16.5","1\"",25.0,149.3,79.5,34.8,50.8,101.6,4.0,25.4,52.3,6.4,3.0,3.0,126.6,"M24",19.0,3.74]
[null,"WNRF 1500# ANSI B16.5 Size 1¼\"","WNRF"," 1500#","ANSI B16.5","1¼\"",32.0,158.7,79.5,34.8,63.5,111.2,4.0,25.4,63.5,6.4,4.8,3.0,126.6,"M24",19.0,4.33]
[null,"WNRF 1500# ANSI B16.5 Size 1½\"","WNRF"," 1500#","ANSI B16.5","1½\"",40.0,177.8,88.9,38.1,73.1,123.9,4.0,28.4,69.8,6.4,6.35,3.0,139.2,"M27",22.0,5.94]
[null,"WNRF 1500# ANSI B16.5 Size 2\"","WNRF"," 1500#","ANSI B16.5","2\"",50.0,215.9,108.0,44.5,91.9,165.1,8.0,25.4,104.6,6.4,7.87,4.0,147,"M24",19.0,10.8]
[null,"WNRF 1500# ANSI B16.5 Size 2½\"","WNRF"," 1500#","ANSI B16.5","2½\"",65.0,244.3,111.0,47.5,104.6,190.5,8.0,28.4,123.9,6.4,7.87,4.0,159,"M27",22.0,15.0]
[null,"WNRF 1500# ANSI B16.5 Size 3\"","WNRF"," 1500#","ANSI B16.5","3\"",80.0,266.7,123.7,54.1,127.0,203.2,8.0,31.7,133.3,6.4,9.65,4.0,176.2,"M30",24.0,19.9]
[null,"WNRF 1500# ANSI B16.5 Size 4\"","WNRF"," 1500#","ANSI B16.5","4\"",100.0,311.1,130.3,60.2,157.2,241.3,8.0,35.0,162.0,6.4,11.18,5.0,193.4,"M33",26.0,29.9]
[null,"WNRF 1500# ANSI B16.5 Size 5\"","WNRF"," 1500#","ANSI B16.5","5\"",125.0,374.6,161.8,79.5,185.6,292.1,8.0,41.1,196.8,6.4,11.18,5.0,242,"M39",31.0,55.4]
[null,"WNRF 1500# ANSI B16.5 Size 6\"","WNRF"," 1500#","ANSI B16.5","6\"",150.0,393.7,177.8,86.9,215.9,317.5,12.0,38.1,228.6,6.4,12.7,6.0,253.8,"M36",29.0,68.4]
[null,"WNRF 1500# ANSI B16.5 Size 8\"","WNRF"," 1500#","ANSI B16.5","8\"",200.0,482.6,219.2,98.3,269.7,393.7,12.0,44.4,292.1,6.4,12.7,6.0,286.6,"M42",34.0,117.0]
[null,"WNRF 1500# ANSI B16.5 Size 10\"","WNRF"," 1500#","ANSI B16.5","10\"",250.0,584.2,260.4,114.3,323.8,485.6,12.0,50.8,368.3,6.4,12.7,6.0,326.6,"M48",38.0,194.0]
[null,"WNRF 1500# ANSI B16.5 Size 12\"","WNRF"," 1500#","ANSI B16.5","12\"",300.0,673.1,288.8,130.3,381.0,571.5,16.0,53.8,450.8,6.4,12.7,6.0,366.6,"M52",42.0,288.0]
[null,"WNRF 1500# ANSI B16.5 Size 14\"","WNRF"," 1500#","ANSI B16.5","14\"",350.0,749.3,304.8,139.7,412.7,635.0,16.0,60.4,495.3,6.4,12.7,7.0,392.4,"M56",45.0,380.0]
[null,"WNRF 1500# ANSI B16.5 Size 16\"","WNRF"," 1500#","ANSI B16.5","16\"",400.0,825.5,317.5,152.4,469.9,704.8,16.0,66.5,552.4,6.4,12.7,7.0,423.8,"M60",48.0,485.0]
[null,"WNRF 1500# ANSI B16.5 Size 18\"","WNRF"," 1500#","ANSI B16.5","18\"",450.0,914.4,333.5,168.4,533.4,774.7,16.0,73.1,596.9,6.4,12.7,7.0,467.8,"M68",54.0,644.0]
[null,"WNRF 1500# ANSI B16.5 Size 20\"","WNRF"," 1500#","ANSI B16.5","20\"",500.0,984.2,362.0,184.2,584.2,831.8,16.0,79.2,641.3,6.4,12.7,7.0,513.4,"M76",61.0,775.0]
[null,"WNRF 1500# ANSI B16.5 Size 24\"","WNRF"," 1500#","ANSI B16.5","24\"",600.0,1168.4,412.8,209.6,692.1,990.6,16.0,91.9,762.0,6.4,12.7,7.0,570.2,"M80",64.0,1232.0]
[null,"WNRF 2500# ANSI B16.5 Size 1/2\"","WNRF"," 2500#","ANSI B16.5","1/2\"",15.0,133.4,79.6,36.6,35.1,88.9,4.0,22.4,42.9,6.4,3.0,3.0,124.2,"M20",16.0,3.12]
[null,"WNRF 2500# ANSI B16.5 Size 3/4\"","WNRF"," 2500#","ANSI B16.5","3/4\"",20.0,139.7,85.6,38.2,42.9,95.3,4.0,22.4,50.8,6.4,3.0,3.0,127.4,"M20",16.0,3.7]
[null,"WNRF 2500# ANSI B16.5 Size 1\"","WNRF"," 2500#","ANSI B16.5","1\"",25.0,158.8,95.3,41.5,50.8,108.0,4.0,25.4,57.2,6.4,3.0,3.0,140,"M24",19.0,5.24]
[null,"WNRF 2500# ANSI B16.5 Size 1¼\"","WNRF"," 2500#","ANSI B16.5","1¼\"",32.0,184.2,101.7,44.5,63.5,130.0,4.0,28.4,73.2,6.4,4.8,3.0,152,"M27",22.0,7.474]
[null,"WNRF 2500# ANSI B16.5 Size 1½\"","WNRF"," 2500#","ANSI B16.5","1½\"",40.0,203.2,117.7,50.9,73.1,146.1,4.0,31.8,79.2,6.4,6.35,3.0,168.8,"M30",24.0,10.9]
[null,"WNRF 2500# ANSI B16.5 Size 2\"","WNRF"," 2500#","ANSI B16.5","2\"",50.0,235.0,133.4,57.2,91.9,171.5,8.0,28.4,95.3,6.4,7.87,4.0,178.4,"M27",22.0,16.2]
[null,"WNRF 2500# ANSI B16.5 Size 2½\"","WNRF"," 2500#","ANSI B16.5","2½\"",65.0,266.7,149.1,63.6,104.6,196.9,8.0,31.8,114.3,6.4,7.87,4.0,195.2,"M30",24.0,23.7]
[null,"WNRF 2500# ANSI B16.5 Size 3\"","WNRF"," 2500#","ANSI B16.5","3\"",80.0,304.8,174.5,72.9,127.0,228.6,8.0,35.1,133.4,6.4,9.7,4.0,217.8,"M33",26.0,36.2]
[null,"WNRF 2500# ANSI B16.5 Size 4\"","WNRF"," 2500#","ANSI B16.5","4\"",100.0,355.6,196.9,82.6,157.2,273.1,8.0,41.1,165.1,6.4,11.18,5.0,248.2,"M39",31.0,55.3]
[null,"WNRF 2500# ANSI B16.5 Size 5\"","WNRF"," 2500#","ANSI B16.5","5\"",125.0,419.1,235.0,98.3,185.6,323.9,8.0,47.8,203.2,6.4,11.18,5.0,289.6,"M45",36.0,92.5]
[null,"WNRF 2500# ANSI B16.5 Size 6\"","WNRF"," 2500#","ANSI B16.5","6\"",150.0,482.6,279.5,114.4,215.9,368.3,8.0,53.8,235.0,6.4,12.7,6.0,326.8,"M48",38.0,143.0]
[null,"WNRF 2500# ANSI B16.5 Size 8\"","WNRF"," 2500#","ANSI B16.5","8\"",200.0,552.5,323.9,133.4,269.7,438.2,12.0,53.8,304.8,6.4,12.7,6.0,364.8,"M48",38.0,215.0]
[null,"WNRF 2500# ANSI B16.5 Size 10\"","WNRF"," 2500#","ANSI B16.5","10\"",250.0,673.1,125.5,171.5,323.8,539.8,12.0,66.5,374.7,6.4,12.7,6.0,461,"M60",48.0,406.0]
[null,"WNRF 2500# ANSI B16.5 Size 12\"","WNRF"," 2500#","ANSI B16.5","12\"",300.0,762.0,470.0,190.6,381.0,619.3,12.0,73.2,441.5,6.4,12.7,6.0,505.2,"M64",51.0,572.0]
[null,"Smls Lg WNRF 150# ANSI B16.5 Size 1/2\"","Smls Lg WNRF"," 150#","ANSI B16.5","1/2\"",15.0,88.9,228.6,11.2,35.1,60.5,4.0,15.7,30.23,1.6,"-",3.0,61.4,"M12",10.0,"-"]
[null,"Smls Lg WNRF 150# ANSI B16.5 Size 3/4\"","Smls Lg WNRF"," 150#","ANSI B16.5","3/4\"",20.0,98.6,228.6,12.7,42.9,69.9,4.0,15.7,38.1,1.6,"-",3.0,64.4,"M12",10.0,"-"]
[null,"Smls Lg WNRF 150# ANSI B16.5 Size 1\"","Smls Lg WNRF"," 150#","ANSI B16.5","1\"",25.0,108.0,228.6,14.2,50.8,79.2,4.0,15.7,50.8,1.6,"-",3.0,67.4,"M12",10.0,3.6]
[null,"Smls Lg WNRF 150# ANSI B16.5 Size 1¼\"","Smls Lg WNRF"," 150#","ANSI B16.5","1¼\"",32.0,117.3,228.6,15.7,63.5,88.9,4.0,15.7,60.3,1.6,"-",3.0,70.4,"M12",10.0,4.5]
[null,"Smls Lg WNRF 150# ANSI B16.5 Size 1½\"","Smls Lg WNRF"," 150#","ANSI B16.5","1½\"",40.0,127.0,228.6,17.5,73.2,98.6,4.0,15.7,66.7,1.6,"-",3.0,74,"M12",10.0,5.5]
[null,"Smls Lg WNRF 150# ANSI B16.5 Size 2\"","Smls Lg WNRF"," 150#","ANSI B16.5","2\"",50.0,152.4,228.6,19.1,91.9,120.7,4.0,19.1,82.5,1.6,"-",4.0,84.2,"M16",13.0,7.3]
[null,"Smls Lg WNRF 150# ANSI B16.5 Size 2½\"","Smls Lg WNRF"," 150#","ANSI B16.5","2½\"",65.0,117.8,228.6,22.4,104.6,139.7,4.0,19.1,95.2,1.6,"-",4.0,90.8,"M16",13.0,9.5]
[null,"Smls Lg WNRF 150# ANSI B16.5 Size 3\"","Smls Lg WNRF"," 150#","ANSI B16.5","3\"",80.0,190.5,228.6,23.9,127.0,152.4,4.0,19.1,107.9,1.6,"-",4.0,93.8,"M16",13.0,10.9]
[null,"Smls Lg WNRF 150# ANSI B16.5 Size 3½","Smls Lg WNRF"," 150#","ANSI B16.5","3½",90.0,215.9,228.6,23.9,139.7,177.8,8.0,19.1,123.8,1.6,"-",4.0,93.8,"M16",13.0,14.1]
[null,"Smls Lg WNRF 150# ANSI B16.5 Size 4\"","Smls Lg WNRF"," 150#","ANSI B16.5","4\"",100.0,228.6,304.8,23.9,157.2,190.5,8.0,19.1,139.7,1.6,"-",5.0,94.8,"M16",13.0,21.3]
[null,"Smls Lg WNRF 150# ANSI B16.5 Size 5\"","Smls Lg WNRF"," 150#","ANSI B16.5","5\"",125.0,254.0,304.8,23.9,185.7,215.9,8.0,22.4,165.1,1.6,"-",5.0,100.8,"M20",16.0,25.9]
[null,"Smls Lg WNRF 150# ANSI B16.5 Size 6\"","Smls Lg WNRF"," 150#","ANSI B16.5","6\"",150.0,279.4,304.8,25.4,215.9,241.3,8.0,22.4,196.8,1.6,"-",6.0,104.8,"M20",16.0,35.0]
[null,"Smls Lg WNRF 150# ANSI B16.5 Size 8\"","Smls Lg WNRF"," 150#","ANSI B16.5","8\"",200.0,342.9,304.8,28.4,269.7,298.5,8.0,22.4,247.6,1.6,"-",6.0,110.8,"M20",16.0,46.8]
[null,"Smls Lg WNRF 150# ANSI B16.5 Size 10\"","Smls Lg WNRF"," 150#","ANSI B16.5","10\"",250.0,406.4,304.8,30.2,323.9,362.0,12.0,25.4,304.8,1.6,"-",6.0,120.4,"M24",19.0,68.1]
[null,"Smls Lg WNRF 150# ANSI B16.5 Size 12\"","Smls Lg WNRF"," 150#","ANSI B16.5","12\"",300.0,482.6,304.8,31.8,381.0,431.8,12.0,25.4,365.1,1.6,"-",6.0,123.6,"M24",19.0,97.6]
[null,"Smls Lg WNRF 150# ANSI B16.5 Size 14\"","Smls Lg WNRF"," 150#","ANSI B16.5","14\"",350.0,533.4,304.8,35.1,412.8,476.3,12.0,28.4,406.4,1.6,"-",7.0,137.2,"M27",22.0,100.0]
[null,"Smls Lg WNRF 150# ANSI B16.5 Size 16\"","Smls Lg WNRF"," 150#","ANSI B16.5","16\"",400.0,596.9,304.8,36.6,469.9,539.8,16.0,28.4,457.2,1.6,"-",7.0,140.2,"M27",22.0,115.0]
[null,"Smls Lg WNRF 150# ANSI B16.5 Size 18\"","Smls Lg WNRF"," 150#","ANSI B16.5","18\"",450.0,635.0,304.8,39.6,533.4,577.9,16.0,31.8,508.0,1.6,"-",7.0,150.2,"M30",24.0,126.0]
[null,"Smls Lg WNRF 150# ANSI B16.5 Size 20\"","Smls Lg WNRF"," 150#","ANSI B16.5","20\"",500.0,698.5,304.8,42.9,584.2,635.0,20.0,31.8,558.8,1.6,"-",7.0,156.8,"M30",24.0,147.0]
[null,"Smls Lg WNRF 150# ANSI B16.5 Size 24\"","Smls Lg WNRF"," 150#","ANSI B16.5","24\"",600.0,812.8,304.8,47.8,692.2,749.3,20.0,35.1,666.7,1.6,"-",7.0,170.6,"M33",26.0,199.0]
[null,"Smls Lg WNRF 300# ANSI B16.5 Size 1/2\"","Smls Lg WNRF"," 300#","ANSI B16.5","1/2\"",15.0,95.2,228.6,14.3,35.0,66.5,4.0,15.7,38.1,1.6,"-",3.0,67.6,"M12",10.0,"-"]
[null,"Smls Lg WNRF 300# ANSI B16.5 Size 3/4\"","Smls Lg WNRF"," 300#","ANSI B16.5","3/4\"",20.0,117.5,228.6,15.9,42.9,82.5,4.0,19.0,47.8,1.6,"-",3.0,76.8,"M16",13.0,"-"]
[null,"Smls Lg WNRF 300# ANSI B16.5 Size 1\"","Smls Lg WNRF"," 300#","ANSI B16.5","1\"",25.0,123.8,228.6,17.5,50.8,88.9,4.0,19.0,54.0,1.6,"-",3.0,80,"M16",13.0,4.5]
[null,"Smls Lg WNRF 300# ANSI B16.5 Size 1¼\"","Smls Lg WNRF"," 300#","ANSI B16.5","1¼\"",32.0,133.3,228.6,19.0,63.5,98.5,4.0,19.0,63.5,1.6,"-",3.0,83,"M16",13.0,6.4]
[null,"Smls Lg WNRF 300# ANSI B16.5 Size 1½\"","Smls Lg WNRF"," 300#","ANSI B16.5","1½\"",40.0,155.6,228.6,20.6,73.1,114.3,4.0,22.3,73.0,1.6,"-",3.0,92.2,"M20",16.0,7.7]
[null,"Smls Lg WNRF 300# ANSI B16.5 Size 2\"","Smls Lg WNRF"," 300#","ANSI B16.5","2\"",50.0,165.1,228.6,22.3,91.9,127.0,8.0,19.0,92.1,1.6,"-",4.0,90.6,"M16",13.0,8.6]
[null,"Smls Lg WNRF 300# ANSI B16.5 Size 2½\"","Smls Lg WNRF"," 300#","ANSI B16.5","2½\"",65.0,190.5,228.6,25.4,104.6,149.3,8.0,22.3,104.8,1.6,"-",4.0,102.8,"M20",16.0,12.7]
[null,"Smls Lg WNRF 300# ANSI B16.5 Size 3\"","Smls Lg WNRF"," 300#","ANSI B16.5","3\"",80.0,209.5,228.6,28.4,127.0,168.1,8.0,22.3,127.0,1.6,"-",4.0,108.8,"M20",16.0,16.3]
[null,"Smls Lg WNRF 300# ANSI B16.5 Size 3½","Smls Lg WNRF"," 300#","ANSI B16.5","3½",90.0,228.6,228.6,30.2,139.7,184.1,8.0,22.3,139.7,1.6,"-",4.0,112.4,"M20",16.0,20.4]
[null,"Smls Lg WNRF 300# ANSI B16.5 Size 4\"","Smls Lg WNRF"," 300#","ANSI B16.5","4\"",100.0,254.0,304.8,31.7,157.2,200.1,8.0,22.3,157.2,1.6,"-",5.0,116.4,"M20",16.0,24.5]
[null,"Smls Lg WNRF 300# ANSI B16.5 Size 5\"","Smls Lg WNRF"," 300#","ANSI B16.5","5\"",125.0,279.4,304.8,35.0,185.6,234.9,8.0,22.3,185.7,1.6,"-",5.0,123,"M20",16.0,39.0]
[null,"Smls Lg WNRF 300# ANSI B16.5 Size 6\"","Smls Lg WNRF"," 300#","ANSI B16.5","6\"",150.0,317.5,304.8,36.5,215.9,269.7,12.0,22.3,215.9,1.6,"-",6.0,127,"M20",16.0,49.0]
[null,"Smls Lg WNRF 300# ANSI B16.5 Size 8\"","Smls Lg WNRF"," 300#","ANSI B16.5","8\"",200.0,381.0,304.8,41.1,269.7,330.2,12.0,25.4,269.9,1.6,"-",6.0,142.2,"M24",19.0,68.1]
[null,"Smls Lg WNRF 300# ANSI B16.5 Size 10\"","Smls Lg WNRF"," 300#","ANSI B16.5","10\"",250.0,444.5,304.8,47.7,323.8,387.3,16.0,28.4,323.8,1.6,"-",6.0,161.4,"M27",22.0,99.0]
[null,"Smls Lg WNRF 300# ANSI B16.5 Size 12\"","Smls Lg WNRF"," 300#","ANSI B16.5","12\"",300.0,520.7,304.8,50.8,381.0,450.8,16.0,31.7,381.0,1.6,"-",6.0,171.6,"M30",24.0,131.0]
[null,"Smls Lg WNRF 300# ANSI B16.5 Size 14\"","Smls Lg WNRF"," 300#","ANSI B16.5","14\"",350.0,584.2,304.8,53.8,412.7,514.3,20.0,31.7,412.7,1.6,"-",7.0,178.6,"M30",24.0,155.0]
[null,"Smls Lg WNRF 300# ANSI B16.5 Size 16\"","Smls Lg WNRF"," 300#","ANSI B16.5","16\"",400.0,647.7,304.8,57.1,469.9,571.5,20.0,35.0,469.9,1.6,"-",7.0,189.2,"M33",26.0,193.0]
[null,"Smls Lg WNRF 300# ANSI B16.5 Size 18\"","Smls Lg WNRF"," 300#","ANSI B16.5","18\"",450.0,711.2,304.8,60.4,533.4,628.6,24.0,35.0,533.4,1.6,"-",7.0,195.8,"M33",26.0,224.0]
[null,"Smls Lg WNRF 300# ANSI B16.5 Size 20\"","Smls Lg WNRF"," 300#","ANSI B16.5","20\"",500.0,774.7,304.8,63.5,584.2,685.8,24.0,35.0,584.2,1.6,"-",7.0,202,"M33",26.0,261.0]
[null,"Smls Lg WNRF 300# ANSI B16.5 Size 24\"","Smls Lg WNRF"," 300#","ANSI B16.5","24\"",600.0,914.4,304.8,69.8,692.1,812.8,24.0,41.1,692.1,1.6,"-",7.0,224.6,"M39",31.0,374.0]
[null,"Smls Lg WNRF 400# ANSI B16.5 Size 1\"","Smls Lg WNRF"," 400#","ANSI B16.5","1\"",25.0,124.0,228.6,23.9,50.8,88.9,4.0,19.1,54.0,6.4,"-",3.0,92.8,"M16",13.0,5.0]
[null,"Smls Lg WNRF 400# ANSI B16.5 Size 1¼\"","Smls Lg WNRF"," 400#","ANSI B16.5","1¼\"",32.0,133.4,228.6,27.0,63.5,98.6,4.0,19.1,63.5,6.4,"-",3.0,99,"M16",13.0,6.4]
[null,"Smls Lg WNRF 400# ANSI B16.5 Size 1½\"","Smls Lg WNRF"," 400#","ANSI B16.5","1½\"",40.0,155.4,228.6,28.4,73.2,114.3,4.0,22.4,69.8,6.4,"-",3.0,107.8,"M20",16.0,7.7]
[null,"Smls Lg WNRF 400# ANSI B16.5 Size 2\"","Smls Lg WNRF"," 400#","ANSI B16.5","2\"",50.0,165.1,228.6,31.8,91.9,127.0,8.0,19.1,82.5,6.4,"-",4.0,109.6,"M16",13.0,9.5]
[null,"Smls Lg WNRF 400# ANSI B16.5 Size 2½\"","Smls Lg WNRF"," 400#","ANSI B16.5","2½\"",65.0,190.5,228.6,34.8,104.6,149.4,8.0,22.4,100.0,6.4,"-",4.0,121.6,"M20",16.0,13.2]
[null,"Smls Lg WNRF 400# ANSI B16.5 Size 3\"","Smls Lg WNRF"," 400#","ANSI B16.5","3\"",80.0,209.6,228.6,38.4,127.0,168.1,8.0,22.4,117.5,6.4,"-",4.0,128.8,"M20",16.0,17.3]
[null,"Smls Lg WNRF 400# ANSI B16.5 Size 3½","Smls Lg WNRF"," 400#","ANSI B16.5","3½",90.0,228.6,228.6,41.5,139.7,184.2,8.0,25.4,133.3,6.4,"-",4.0,141,"M24",19.0,21.8]
[null,"Smls Lg WNRF 400# ANSI B16.5 Size 4\"","Smls Lg WNRF"," 400#","ANSI B16.5","4\"",100.0,254.0,304.8,41.5,157.2,200.2,8.0,25.4,146.0,6.4,"-",5.0,142,"M24",19.0,30.4]
[null,"Smls Lg WNRF 400# ANSI B16.5 Size 5\"","Smls Lg WNRF"," 400#","ANSI B16.5","5\"",125.0,279.4,304.8,44.5,185.7,235.0,8.0,25.4,177.8,6.4,"-",5.0,148,"M24",19.0,40.9]
[null,"Smls Lg WNRF 400# ANSI B16.5 Size 6\"","Smls Lg WNRF"," 400#","ANSI B16.5","6\"",150.0,317.5,304.8,47.5,215.9,269.7,12.0,25.4,206.4,6.4,"-",6.0,155,"M24",19.0,52.2]
[null,"Smls Lg WNRF 400# ANSI B16.5 Size 8\"","Smls Lg WNRF"," 400#","ANSI B16.5","8\"",200.0,381.0,304.8,54.4,269.7,330.2,12.0,28.4,260.3,6.4,"-",6.0,174.8,"M27",22.0,63.6]
[null,"Smls Lg WNRF 400# ANSI B16.5 Size 10\"","Smls Lg WNRF"," 400#","ANSI B16.5","10\"",250.0,444.5,304.8,60.2,323.9,387.4,16.0,31.8,320.7,6.4,"-",6.0,190.4,"M30",24.0,104.0]
[null,"Smls Lg WNRF 400# ANSI B16.5 Size 12\"","Smls Lg WNRF"," 400#","ANSI B16.5","12\"",300.0,520.7,304.8,63.6,381.0,450.9,16.0,35.1,374.6,6.4,"-",6.0,201.2,"M33",26.0,127.0]
[null,"Smls Lg WNRF 400# ANSI B16.5 Size 14\"","Smls Lg WNRF"," 400#","ANSI B16.5","14\"",350.0,284.2,"specify",66.9,412.8,514.4,20.0,35.1,425.4,6.4,"-",7.0,208.8,"M33",26.0,153.0]
[null,"Smls Lg WNRF 400# ANSI B16.5 Size 16\"","Smls Lg WNRF"," 400#","ANSI B16.5","16\"",400.0,647.7,"specify",69.9,469.9,571.5,20.0,38.1,482.6,6.4,"-",7.0,220.8,"M36",29.0,189.0]
[null,"Smls Lg WNRF 400# ANSI B16.5 Size 18\"","Smls Lg WNRF"," 400#","ANSI B16.5","18\"",450.0,711.2,"specify",72.9,533.4,628.7,24.0,38.1,533.4,6.4,"-",7.0,226.8,"M36",29.0,218.0]
[null,"Smls Lg WNRF 400# ANSI B16.5 Size 20\"","Smls Lg WNRF"," 400#","ANSI B16.5","20\"",500.0,774.7,"specify",76.3,584.2,685.8,24.0,41.1,587.4,6.4,"-",7.0,237.6,"M39",31.0,256.0]
[null,"Smls Lg WNRF 400# ANSI B16.5 Size 24\"","Smls Lg WNRF"," 400#","ANSI B16.5","24\"",600.0,914.4,"specify",82.6,692.2,812.8,24.0,47.8,701.7,6.4,"-",7.0,260.2,"M45",36.0,363.0]
[null,"Smls Lg WNRF 600# ANSI B16.5 Size 1\"","Smls Lg WNRF"," 600#","ANSI B16.5","1\"",25.0,124.0,228.6,23.9,50.8,88.9,4.0,19.1,54.0,6.4,"-",3.0,92.8,"M16",13.0,5.0]
[null,"Smls Lg WNRF 600# ANSI B16.5 Size 1¼\"","Smls Lg WNRF"," 600#","ANSI B16.5","1¼\"",32.0,133.4,228.6,27.0,63.5,98.6,4.0,19.1,63.5,6.4,"-",3.0,99,"M16",13.0,6.4]
[null,"Smls Lg WNRF 600# ANSI B16.5 Size 1½\"","Smls Lg WNRF"," 600#","ANSI B16.5","1½\"",40.0,155.4,228.6,28.4,73.2,114.3,4.0,22.3,69.8,6.4,"-",3.0,107.8,"M20",16.0,7.7]
[null,"Smls Lg WNRF 600# ANSI B16.5 Size 2\"","Smls Lg WNRF"," 600#","ANSI B16.5","2\"",50.0,165.1,228.6,31.8,91.9,127.0,8.0,19.1,82.5,6.4,"-",4.0,109.6,"M16",13.0,9.5]
[null,"Smls Lg WNRF 600# ANSI B16.5 Size 2½\"","Smls Lg WNRF"," 600#","ANSI B16.5","2½\"",65.0,190.5,228.6,34.8,104.6,149.4,8.0,22.4,100.0,6.4,"-",4.0,121.6,"M20",16.0,13.2]
[null,"Smls Lg WNRF 600# ANSI B16.5 Size 3\"","Smls Lg WNRF"," 600#","ANSI B16.5","3\"",80.0,209.6,228.6,38.4,127.0,168.1,8.0,22.4,117.5,6.4,"-",4.0,128.8,"M20",16.0,17.3]
[null,"Smls Lg WNRF 600# ANSI B16.5 Size 3½","Smls Lg WNRF"," 600#","ANSI B16.5","3½",90.0,228.6,228.6,41.5,139.7,184.2,8.0,25.4,133.3,6.4,"-",4.0,141,"M24",19.0,21.8]
[null,"Smls Lg WNRF 600# ANSI B16.5 Size 4\"","Smls Lg WNRF"," 600#","ANSI B16.5","4\"",100.0,273.1,304.8,44.5,157.2,215.9,8.0,25.4,152.4,6.4,"-",5.0,148,"M24",19.0,36.3]
[null,"Smls Lg WNRF 600# ANSI B16.5 Size 5\"","Smls Lg WNRF"," 600#","ANSI B16.5","5\"",125.0,330.2,304.8,50.9,185.7,266.7,8.0,28.4,190.5,6.4,"-",5.0,166.8,"M27",22.0,58.1]
[null,"Smls Lg WNRF 600# ANSI B16.5 Size 6\"","Smls Lg WNRF"," 600#","ANSI B16.5","6\"",150.0,355.6,304.8,54.2,215.9,292.1,12.0,28.4,222.2,6.4,"-",6.0,174.4,"M27",22.0,71.1]
[null,"Smls Lg WNRF 600# ANSI B16.5 Size 8\"","Smls Lg WNRF"," 600#","ANSI B16.5","8\"",200.0,419.1,304.8,62.0,269.7,349.3,12.0,31.8,273.0,6.4,"-",6.0,194,"M30",24.0,97.6]
[null,"Smls Lg WNRF 600# ANSI B16.5 Size 10\"","Smls Lg WNRF"," 600#","ANSI B16.5","10\"",250.0,508.0,304.8,69.9,323.9,431.8,16.0,35.1,342.9,6.4,"-",6.0,213.8,"M33",26.0,147.0]
[null,"Smls Lg WNRF 600# ANSI B16.5 Size 12\"","Smls Lg WNRF"," 600#","ANSI B16.5","12\"",300.0,558.8,304.8,72.9,381.0,489.0,20.0,35.1,400.0,6.4,"-",6.0,219.8,"M33",26.0,227.0]
[null,"Smls Lg WNRF 600# ANSI B16.5 Size 14\"","Smls Lg WNRF"," 600#","ANSI B16.5","14\"",350.0,603.3,"specify",76.3,412.8,527.1,20.0,38.1,431.0,6.4,"-",7.0,233.6,"M36",29.0,189.0]
[null,"Smls Lg WNRF 600# ANSI B16.5 Size 16\"","Smls Lg WNRF"," 600#","ANSI B16.5","16\"",400.0,685.8,"specify",82.6,469.9,603.3,20.0,41.1,495.3,6.4,"-",7.0,250.2,"M39",31.0,256.0]
[null,"Smls Lg WNRF 600# ANSI B16.5 Size 18\"","Smls Lg WNRF"," 600#","ANSI B16.5","18\"",450.0,743.0,"specify",89.0,533.4,654.1,20.0,44.5,546.1,6.4,"-",7.0,269,"M42",34.0,297.0]
[null,"Smls Lg WNRF 600# ANSI B16.5 Size 20\"","Smls Lg WNRF"," 600#","ANSI B16.5","20\"",500.0,812.8,"specify",95.3,584.2,723.9,24.0,44.5,609.6,6.4,"-",7.0,281.6,"M42",34.0,381.0]
[null,"Smls Lg WNRF 600# ANSI B16.5 Size 24\"","Smls Lg WNRF"," 600#","ANSI B16.5","24\"",600.0,939.8,"specify",108.0,692.2,838.2,24.0,50.8,717.5,6.4,"-",7.0,315,"M48",38.0,499.0]
[null,"Smls Lg WNRF 900# ANSI B16.5 Size 1\"","Smls Lg WNRF"," 900#","ANSI B16.5","1\"",25.0,149.3,228.6,34.8,50.8,101.6,4.0,25.4,52.4,6.4,"-",3.0,126.6,"M24",19.0,6.8]
[null,"Smls Lg WNRF 900# ANSI B16.5 Size 1¼\"","Smls Lg WNRF"," 900#","ANSI B16.5","1¼\"",32.0,158.7,228.6,34.8,63.5,111.2,4.0,25.4,63.5,6.4,"-",3.0,126.6,"M24",19.0,8.2]
[null,"Smls Lg WNRF 900# ANSI B16.5 Size 1½\"","Smls Lg WNRF"," 900#","ANSI B16.5","1½\"",40.0,177.8,228.6,38.1,73.1,123.9,4.0,28.4,69.8,6.4,"-",3.0,139.2,"M27",22.0,10.4]
[null,"Smls Lg WNRF 900# ANSI B16.5 Size 2\"","Smls Lg WNRF"," 900#","ANSI B16.5","2\"",50.0,215.9,228.6,44.5,91.9,165.1,8.0,25.4,104.8,6.4,"-",4.0,147,"M24",19.0,20.0]
[null,"Smls Lg WNRF 900# ANSI B16.5 Size 2½\"","Smls Lg WNRF"," 900#","ANSI B16.5","2½\"",65.0,244.3,304.8,47.5,104.6,190.5,8.0,28.4,123.8,6.4,"-",4.0,159,"M27",22.0,32.7]
[null,"Smls Lg WNRF 900# ANSI B16.5 Size 3\"","Smls Lg WNRF"," 900#","ANSI B16.5","3\"",80.0,241.3,304.8,44.5,127.0,190.5,8.0,25.4,127.0,6.4,"-",4.0,141,"M20",16.0,29.5]
[null,"Smls Lg WNRF 900# ANSI B16.5 Size 4\"","Smls Lg WNRF"," 900#","ANSI B16.5","4\"",100.0,292.1,304.8,50.8,157.2,234.9,8.0,31.7,158.7,6.4,"-",5.0,166.6,"M27",22.0,44.5]
[null,"Smls Lg WNRF 900# ANSI B16.5 Size 5\"","Smls Lg WNRF"," 900#","ANSI B16.5","5\"",125.0,349.2,304.8,57.2,185.6,279.4,8.0,35.0,190.5,6.4,"-",5.0,187.4,"M33",26.0,64.9]
[null,"Smls Lg WNRF 900# ANSI B16.5 Size 6\"","Smls Lg WNRF"," 900#","ANSI B16.5","6\"",150.0,381.0,304.8,62.0,215.9,317.5,12.0,31.7,234.9,6.4,"-",6.0,190,"M27",22.0,90.4]
[null,"Smls Lg WNRF 900# ANSI B16.5 Size 8\"","Smls Lg WNRF"," 900#","ANSI B16.5","8\"",200.0,469.9,304.8,69.9,269.7,393.7,12.0,38.1,298.4,6.4,"-",6.0,219.8,"M36",29.0,141.0]
[null,"Smls Lg WNRF 900# ANSI B16.5 Size 10\"","Smls Lg WNRF"," 900#","ANSI B16.5","10\"",250.0,546.1,406.4,76.2,323.8,169.9,16.0,38.1,368.3,6.4,"-",6.0,232.4,"M36",29.0,175.0]
[null,"Smls Lg WNRF 900# ANSI B16.5 Size 12\"","Smls Lg WNRF"," 900#","ANSI B16.5","12\"",300.0,609.6,406.4,85.6,381.0,533.4,20.0,38.1,419.1,6.4,"-",6.0,251.2,"M36",29.0,303.0]
[null,"Smls Lg WNRF 900# ANSI B16.5 Size 14\"","Smls Lg WNRF"," 900#","ANSI B16.5","14\"",350.0,641.3,"specify",92.2,412.7,558.8,20.0,41.1,450.8,6.4,"-",7.0,265.4,"M39",29.0,253.0]
[null,"Smls Lg WNRF 900# ANSI B16.5 Size 16\"","Smls Lg WNRF"," 900#","ANSI B16.5","16\"",400.0,704.8,"specify",95.3,469.9,615.9,20.0,44.4,508.0,6.4,"-",7.0,281.6,"M42",34.0,304.0]
[null,"Smls Lg WNRF 900# ANSI B16.5 Size 18\"","Smls Lg WNRF"," 900#","ANSI B16.5","18\"",450.0,787.4,"specify",108.0,533.4,685.8,20.0,50.8,565.1,6.4,"-",7.0,315,"M48",38.0,431.0]
[null,"Smls Lg WNRF 900# ANSI B16.5 Size 20\"","Smls Lg WNRF"," 900#","ANSI B16.5","20\"",500.0,857.2,"specify",114.3,584.2,749.3,20.0,53.8,622.3,6.4,"-",7.0,335.6,"M52",42.0,472.0]
[null,"Smls Lg WNRF 900# ANSI B16.5 Size 24\"","Smls Lg WNRF"," 900#","ANSI B16.5","24\"",600.0,1041.4,"specify",146.1,692.1,901.7,20.0,66.5,749.3,6.4,"-",7.0,417.2,"M64",51.0,806.0]
[null,"Smls Lg WNRF 1500# ANSI B16.5 Size 1\"","Smls Lg WNRF"," 1500#","ANSI B16.5","1\"",25.0,149.3,228.6,34.8,50.8,101.6,4.0,25.4,50.8,6.4,"-",3.0,126.6,"M24",19.0,6.8]
[null,"Smls Lg WNRF 1500# ANSI B16.5 Size 1¼\"","Smls Lg WNRF"," 1500#","ANSI B16.5","1¼\"",32.0,158.7,228.6,34.8,63.5,111.2,4.0,25.4,63.5,6.4,"-",3.0,126.6,"M24",19.0,8.2]
[null,"Smls Lg WNRF 1500# ANSI B16.5 Size 1½\"","Smls Lg WNRF"," 1500#","ANSI B16.5","1½\"",40.0,177.8,228.6,38.1,73.1,123.9,4.0,28.4,73.0,6.4,"-",3.0,139.2,"M27",22.0,10.4]
[null,"Smls Lg WNRF 1500# ANSI B16.5 Size 2\"","Smls Lg WNRF"," 1500#","ANSI B16.5","2\"",50.0,215.9,228.6,44.5,91.9,165.1,8.0,25.4,92.1,6.4,"-",4.0,147,"M24",19.0,20.0]
[null,"Smls Lg WNRF 1500# ANSI B16.5 Size 2½\"","Smls Lg WNRF"," 1500#","ANSI B16.5","2½\"",65.0,244.3,304.8,47.5,104.6,190.5,8.0,28.4,104.8,6.4,"-",4.0,159,"M27",22.0,32.7]
[null,"Smls Lg WNRF 1500# ANSI B16.5 Size 3\"","Smls Lg WNRF"," 1500#","ANSI B16.5","3\"",80.0,266.7,304.8,54.1,127.0,203.2,8.0,31.7,127.0,6.4,"-",4.0,176.2,"M30",24.0,38.1]
[null,"Smls Lg WNRF 1500# ANSI B16.5 Size 4\"","Smls Lg WNRF"," 1500#","ANSI B16.5","4\"",100.0,311.1,304.8,60.2,157.2,241.3,8.0,35.0,157.2,6.4,"-",5.0,193.4,"M33",26.0,53.6]
[null,"Smls Lg WNRF 1500# ANSI B16.5 Size 5\"","Smls Lg WNRF"," 1500#","ANSI B16.5","5\"",125.0,374.6,304.8,79.5,185.6,292.1,8.0,41.1,185.7,6.4,"-",5.0,242,"M39",31.0,88.5]
[null,"Smls Lg WNRF 1500# ANSI B16.5 Size 6\"","Smls Lg WNRF"," 1500#","ANSI B16.5","6\"",150.0,393.7,304.8,86.9,215.9,317.5,12.0,38.1,215.9,6.4,"-",6.0,253.8,"M36",29.0,107.0]
[null,"Smls Lg WNRF 1500# ANSI B16.5 Size 8\"","Smls Lg WNRF"," 1500#","ANSI B16.5","8\"",200.0,482.6,304.8,98.3,269.7,393.7,12.0,44.4,269.9,6.4,"-",6.0,286.6,"M42",34.0,166.0]
[null,"Smls Lg WNRF 1500# ANSI B16.5 Size 10\"","Smls Lg WNRF"," 1500#","ANSI B16.5","10\"",250.0,584.2,406.4,114.3,323.8,485.6,12.0,50.8,323.8,6.4,"-",6.0,326.6,"M48",38.0,277.0]
[null,"Smls Lg WNRF 1500# ANSI B16.5 Size 12\"","Smls Lg WNRF"," 1500#","ANSI B16.5","12\"",300.0,673.1,406.4,130.3,381.0,571.5,16.0,53.8,381.0,6.4,"-",6.0,366.6,"M52",42.0,467.0]
[null,"Smls Lg WNRF 1500# ANSI B16.5 Size 14\"","Smls Lg WNRF"," 1500#","ANSI B16.5","14\"",350.0,749.3,"specify",139.7,412.7,635.0,16.0,60.4,412.7,6.4,"-",7.0,392.4,"M56",45.0,468.0]
[null,"Smls Lg WNRF 1500# ANSI B16.5 Size 16\"","Smls Lg WNRF"," 1500#","ANSI B16.5","16\"",400.0,825.5,"specify",152.4,469.9,704.8,16.0,66.5,469.9,6.4,"-",7.0,423.8,"M60",48.0,606.0]
[null,"Smls Lg WNRF 1500# ANSI B16.5 Size 18\"","Smls Lg WNRF"," 1500#","ANSI B16.5","18\"",450.0,914.4,"specify",168.4,533.4,774.7,16.0,73.1,533.4,6.4,"-",7.0,467.8,"M68",54.0,795.0]
[null,"Smls Lg WNRF 1500# ANSI B16.5 Size 20\"","Smls Lg WNRF"," 1500#","ANSI B16.5","20\"",500.0,984.2,"specify",184.2,584.2,831.8,16.0,79.2,584.2,6.4,"-",7.0,513.4,"M76",61.0,967.0]
[null,"Smls Lg WNRF 1500# ANSI B16.5 Size 24\"","Smls Lg WNRF"," 1500#","ANSI B16.5","24\"",600.0,1168.4,"specify",209.6,692.1,990.6,16.0,91.9,692.1,6.4,"-",7.0,570.2,"M80",64.0,1444.0]
[null,"Smls Lg WNRF 2500# ANSI B16.5 Size 1\"","Smls Lg WNRF"," 2500#","ANSI B16.5","1\"",25.0,158.8,228.6,41.5,50.8,108.0,4.0,25.4,50.8,6.4,"-",3.0,140,"M24",19.0,9.1]
[null,"Smls Lg WNRF 2500# ANSI B16.5 Size 1¼\"","Smls Lg WNRF"," 2500#","ANSI B16.5","1¼\"",32.0,184.2,228.6,44.5,63.5,130.0,4.0,28.4,63.5,6.4,"-",3.0,152,"M27",22.0,13.6]
[null,"Smls Lg WNRF 2500# ANSI B16.5 Size 1½\"","Smls Lg WNRF"," 2500#","ANSI B16.5","1½\"",40.0,203.2,228.6,50.9,73.1,146.1,4.0,31.8,73.0,6.4,"-",3.0,168.8,"M30",24.0,17.3]
[null,"Smls Lg WNRF 2500# ANSI B16.5 Size 2\"","Smls Lg WNRF"," 2500#","ANSI B16.5","2\"",50.0,235.0,228.6,57.2,91.9,171.5,8.0,28.4,92.1,6.4,"-",4.0,178.4,"M27",22.0,25.0]
[null,"Smls Lg WNRF 2500# ANSI B16.5 Size 2½\"","Smls Lg WNRF"," 2500#","ANSI B16.5","2½\"",65.0,266.7,304.8,63.6,104.6,196.9,8.0,31.8,104.8,6.4,"-",4.0,195.2,"M30",24.0,38.6]
[null,"Smls Lg WNRF 2500# ANSI B16.5 Size 3\"","Smls Lg WNRF"," 2500#","ANSI B16.5","3\"",80.0,304.8,304.8,72.9,127.0,228.6,8.0,35.1,127.0,6.4,"-",4.0,217.8,"M33",26.0,56.8]
[null,"Smls Lg WNRF 2500# ANSI B16.5 Size 4\"","Smls Lg WNRF"," 2500#","ANSI B16.5","4\"",100.0,355.6,304.8,82.6,157.2,273.1,8.0,41.1,157.2,6.4,"-",5.0,248.2,"M39",31.0,84.0]
[null,"Smls Lg WNRF 2500# ANSI B16.5 Size 5\"","Smls Lg WNRF"," 2500#","ANSI B16.5","5\"",125.0,419.1,304.8,98.3,185.6,323.9,8.0,47.8,185.7,6.4,"-",5.0,289.6,"M45",36.0,136.0]
[null,"Smls Lg WNRF 2500# ANSI B16.5 Size 6\"","Smls Lg WNRF"," 2500#","ANSI B16.5","6\"",150.0,482.6,304.8,114.4,215.9,368.3,8.0,53.8,215.7,6.4,"-",6.0,326.8,"M48",38.0,204.0]
[null,"Smls Lg WNRF 2500# ANSI B16.5 Size 8\"","Smls Lg WNRF"," 2500#","ANSI B16.5","8\"",200.0,552.5,304.8,133.4,269.7,438.2,12.0,53.8,269.9,6.4,"-",6.0,364.8,"M48",38.0,272.0]
[null,"Smls Lg WNRF 2500# ANSI B16.5 Size 10\"","Smls Lg WNRF"," 2500#","ANSI B16.5","10\"",250.0,673.1,406.4,171.5,323.8,539.8,12.0,66.5,323.8,6.4,"-",6.0,461,"M60",48.0,522.0]
[null,"Smls Lg WNRF 2500# ANSI B16.5 Size 12\"","Smls Lg WNRF"," 2500#","ANSI B16.5","12\"",300.0,762.0,406.4,190.6,381.0,619.3,12.0,73.2,381.0,6.4,"-",6.0,505.2,"M64",51.0,708.0]
[null,"Cast Iron WNRF 25# ANSI B16.1 Size 4\"","Cast Iron WNRF"," 25#","ANSI B16.1","4\"",100.0,228.6,"-",19.05,"-",190.5,8.0,19.1,"-","-","-",5.0,"-","M16",13.0,"-"]
[null,"Cast Iron WNRF 25# ANSI B16.1 Size 5\"","Cast Iron WNRF"," 25#","ANSI B16.1","5\"",125.0,254.0,"-",19.05,"-",215.9,8.0,19.1,"-","-","-",5.0,"-","M16",13.0,"-"]
[null,"Cast Iron WNRF 25# ANSI B16.1 Size 6\"","Cast Iron WNRF"," 25#","ANSI B16.1","6\"",150.0,279.0,"-",19.05,"-",241.3,8.0,19.1,"-","-","-",6.0,"-","M16",13.0,"-"]
[null,"Cast Iron WNRF 25# ANSI B16.1 Size 8\"","Cast Iron WNRF"," 25#","ANSI B16.1","8\"",200.0,343.0,"-",19.05,"-",298.45,8.0,19.1,"-","-","-",6.0,"-","M16",13.0,"-"]
[null,"Cast Iron WNRF 25# ANSI B16.1 Size 10\"","Cast Iron WNRF"," 25#","ANSI B16.1","10\"",250.0,406.0,"-",22.23,"-",361.95,12.0,19.1,"-","-","-",6.0,"-","M16",13.0,"-"]
[null,"Cast Iron WNRF 25# ANSI B16.1 Size 12\"","Cast Iron WNRF"," 25#","ANSI B16.1","12\"",300.0,483.0,"-",25.4,"-",431.8,12.0,19.1,"-","-","-",6.0,"-","M16",13.0,"-"]
[null,"Cast Iron WNRF 25# ANSI B16.1 Size 14\"","Cast Iron WNRF"," 25#","ANSI B16.1","14\"",350.0,533.0,"-",28.575,"-",476.25,12.0,22.3,"-","-","-",7.0,"-","M20",16.0,"-"]
[null,"Cast Iron WNRF 25# ANSI B16.1 Size 16\"","Cast Iron WNRF"," 25#","ANSI B16.1","16\"",400.0,597.0,"-",28.575,"-",539.75,16.0,22.3,"-","-","-",7.0,"-","M20",16.0,"-"]
[null,"Cast Iron WNRF 25# ANSI B16.1 Size 18\"","Cast Iron WNRF"," 25#","ANSI B16.1","18\"",450.0,635.0,"-",31.75,"-",577.85,16.0,22.3,"-","-","-",7.0,"-","M20",16.0,"-"]
[null,"Cast Iron WNRF 25# ANSI B16.1 Size 20\"","Cast Iron WNRF"," 25#","ANSI B16.1","20\"",500.0,699.0,"-",31.75,"-",635.0,20.0,22.3,"-","-","-",7.0,"-","M20",16.0,"-"]
[null,"Cast Iron WNRF 25# ANSI B16.1 Size 24\"","Cast Iron WNRF"," 25#","ANSI B16.1","24\"",600.0,813.0,"-",34.925,"-",749.3,20.0,22.3,"-","-","-",7.0,"-","M20",16.0,"-"]
[null,"Cast Iron WNRF 125# ANSI B16.1 Size 1\"","Cast Iron WNRF"," 125#","ANSI B16.1","1\"",25.0,108.0,"-",11.2,"-",79.0,4.0,15.7,"-","-","-",3.0,"-","M12",10.0,"-"]
[null,"Cast Iron WNRF 125# ANSI B16.1 Size 1¼\"","Cast Iron WNRF"," 125#","ANSI B16.1","1¼\"",32.0,117.0,"-",12.7,"-",89.0,4.0,15.7,"-","-","-",3.0,"-","M12",10.0,"-"]
[null,"Cast Iron WNRF 125# ANSI B16.1 Size 1½\"","Cast Iron WNRF"," 125#","ANSI B16.1","1½\"",40.0,127.0,"-",14.3,"-",98.0,4.0,15.7,"-","-","-",3.0,"-","M12",10.0,"-"]
[null,"Cast Iron WNRF 125# ANSI B16.1 Size 2\"","Cast Iron WNRF"," 125#","ANSI B16.1","2\"",50.0,152.0,"-",16.0,"-",121.0,4.0,19.1,"-","-","-",4.0,{"$f":"(J335+U335+8)*2+R335","v":78},"M16",13.0,"-"]
[null,"Cast Iron WNRF 125# ANSI B16.1 Size 2½\"","Cast Iron WNRF"," 125#","ANSI B16.1","2½\"",65.0,178.0,"-",18.0,"-",140.0,4.0,19.1,"-","-","-",4.0,82,"M16",13.0,"-"]
[null,"Cast Iron WNRF 125# ANSI B16.1 Size 3\"","Cast Iron WNRF"," 125#","ANSI B16.1","3\"",80.0,191.0,"-",19.0,"-",152.0,4.0,19.1,"-","-","-",4.0,84,"M16",13.0,"-"]
[null,"Cast Iron WNRF 125# ANSI B16.1 Size 3½\"","Cast Iron WNRF"," 125#","ANSI B16.1","3½\"","-",216.0,"-",21.0,"-",178.0,8.0,19.1,"-","-","-",4.0,88,"M16",13.0,"-"]
[null,"Cast Iron WNRF 125# ANSI B16.1 Size 4\"","Cast Iron WNRF"," 125#","ANSI B16.1","4\"",100.0,229.0,"-",24.0,"-",191.0,8.0,19.1,"-","-","-",5.0,95,"M16",13.0,"-"]
[null,"Cast Iron WNRF 125# ANSI B16.1 Size 5\"","Cast Iron WNRF"," 125#","ANSI B16.1","5\"",125.0,254.0,"-",24.0,"-",216.0,8.0,22.3,"-","-","-",5.0,101,"M20",16.0,"-"]
[null,"Cast Iron WNRF 125# ANSI B16.1 Size 6\"","Cast Iron WNRF"," 125#","ANSI B16.1","6\"",150.0,279.0,"-",25.0,"-",241.0,8.0,22.3,"-","-","-",6.0,104,"M20",16.0,"-"]
[null,"Cast Iron WNRF 125# ANSI B16.1 Size 8\"","Cast Iron WNRF"," 125#","ANSI B16.1","8\"",200.0,343.0,"-",28.0,"-",298.0,8.0,22.3,"-","-","-",6.0,110,"M20",16.0,"-"]
[null,"Cast Iron WNRF 125# ANSI B16.1 Size 10\"","Cast Iron WNRF"," 125#","ANSI B16.1","10\"",250.0,406.0,"-",30.0,"-",362.0,12.0,25.4,"-","-","-",6.0,120,"M24",19.0,"-"]
[null,"Cast Iron WNRF 125# ANSI B16.1 Size 12\"","Cast Iron WNRF"," 125#","ANSI B16.1","12\"",300.0,483.0,"-",32.0,"-",432.0,12.0,25.4,"-","-","-",6.0,124,"M24",19.0,"-"]
[null,"Cast Iron WNRF 125# ANSI B16.1 Size 14\"","Cast Iron WNRF"," 125#","ANSI B16.1","14\"",350.0,533.0,"-",35.0,"-",476.0,12.0,28.4,"-","-","-",7.0,137,"M27",22.0,"-"]
[null,"Cast Iron WNRF 125# ANSI B16.1 Size 16\"","Cast Iron WNRF"," 125#","ANSI B16.1","16\"",400.0,597.0,"-",36.0,"-",540.0,16.0,28.4,"-","-","-",7.0,139,"M27",22.0,"-"]
[null,"Cast Iron WNRF 125# ANSI B16.1 Size 18\"","Cast Iron WNRF"," 125#","ANSI B16.1","18\"",450.0,635.0,"-",39.7,"-",578.0,16.0,31.7,"-","-","-",7.0,150.4,"M30",24.0,"-"]
[null,"Cast Iron WNRF 125# ANSI B16.1 Size 20\"","Cast Iron WNRF"," 125#","ANSI B16.1","20\"",500.0,699.0,"-",42.9,"-",635.0,20.0,31.7,"-","-","-",7.0,156.8,"M30",24.0,"-"]
[null,"Cast Iron WNRF 125# ANSI B16.1 Size 24\"","Cast Iron WNRF"," 125#","ANSI B16.1","24\"",600.0,813.0,"-",47.7,"-",749.0,20.0,35.0,"-","-","-",7.0,170.4,"M33",26.0,"-"]
[null,"Cast Iron WNRF 125# ANSI B16.1 Size 26\"","Cast Iron WNRF"," 125#","ANSI B16.1","26\"",650.0,870.0,"-",50.8,"-",806.5,24.0,35.1,"-",1.6,"-",7.0,176.6,"M33",26.0,"-"]
[null,"Cast Iron WNRF 125# ANSI B16.1 Size 28\"","Cast Iron WNRF"," 125#","ANSI B16.1","28\"",700.0,927.1,"-",52.3,"-",863.6,28.0,35.1,"-",1.6,"-",7.0,179.6,"M33",26.0,"-"]
[null,"Cast Iron WNRF 125# ANSI B16.1 Size 30\"","Cast Iron WNRF"," 125#","ANSI B16.1","30\"",750.0,984.3,"-",54.1,"-",914.4,28.0,35.1,"-",1.6,"-",7.0,183.2,"M33",26.0,"-"]
[null,"Cast Iron WNRF 125# ANSI B16.1 Size 32\"","Cast Iron WNRF"," 125#","ANSI B16.1","32\"",800.0,1060.5,"-",57.2,"-",977.9,28.0,41.4,"-",1.6,"-",7.0,189.4,"M36",26.0,"-"]
[null,"Cast Iron WNRF 125# ANSI B16.1 Size 34\"","Cast Iron WNRF"," 125#","ANSI B16.1","34\"",850.0,1111.3,"-",58.7,"-",1028.7,32.0,41.4,"-",1.6,"-",7.0,192.4,"M36",26.0,"-"]
[null,"Cast Iron WNRF 125# ANSI B16.1 Size 36\"","Cast Iron WNRF"," 125#","ANSI B16.1","36\"",900.0,1168.4,"-",60.5,"-",1086.0,32.0,41.4,"-",1.6,"-",7.0,196,"M36",26.0,"-"]
[null,"Cast Iron WNRF 125# ANSI B16.1 Size 38\"","Cast Iron WNRF"," 125#","ANSI B16.1","38\"",950.0,1238.3,"-",60.5,"-",1149.4,32.0,41.4,"-",1.6,"-",7.0,196,"M36",26.0,"-"]
[null,"Cast Iron WNRF 125# ANSI B16.1 Size 40\"","Cast Iron WNRF"," 125#","ANSI B16.1","40\"",1000.0,1289.1,"-",63.5,"-",1200.2,36.0,41.4,"-",1.6,"-",7.0,208,"M36",29.0,"-"]
[null,"Cast Iron WNRF 125# ANSI B16.1 Size 42\"","Cast Iron WNRF"," 125#","ANSI B16.1","42\"",1050.0,1346.2,"-",66.8,"-",1257.3,36.0,41.4,"-",1.6,"-",7.0,214.6,"M36",29.0,"-"]
[null,"Cast Iron WNRF 125# ANSI B16.1 Size 44\"","Cast Iron WNRF"," 125#","ANSI B16.1","44\"",1100.0,1403.4,"-",66.8,"-",1314.5,40.0,41.4,"-",1.6,"-",7.0,214.6,"M36",29.0,"-"]
[null,"Cast Iron WNRF 125# ANSI B16.1 Size 46\"","Cast Iron WNRF"," 125#","ANSI B16.1","46\"",1150.0,1454.2,"-",68.1,"-",1365.3,40.0,41.4,"-",1.6,"-",7.0,217.2,"M36",29.0,"-"]
[null,"Cast Iron WNRF 125# ANSI B16.1 Size 48\"","Cast Iron WNRF"," 125#","ANSI B16.1","48\"",1200.0,1511.3,"-",69.85,"-",1422.4,44.0,41.4,"-",1.6,"-",7.0,220.7,"M36",29.0,"-"]
[null,"Cast Iron WNRF 125# ANSI B16.1 Size 50\"","Cast Iron WNRF"," 125#","ANSI B16.1","50\"",1250.0,1568.5,"-",69.9,"-",1479.6,44.0,47.8,"-",1.6,"-",7.0,226.8,"M39",32.0,"-"]
[null,"Cast Iron WNRF 125# ANSI B16.1 Size 52\"","Cast Iron WNRF"," 125#","ANSI B16.1","52\"",1300.0,1625.6,"-",73.2,"-",1536.7,44.0,47.8,"-",1.6,"-",7.0,233.4,"M39",32.0,"-"]
[null,"Cast Iron WNRF 125# ANSI B16.1 Size 54\"","Cast Iron WNRF"," 125#","ANSI B16.1","54\"",1350.0,1682.8,"-",76.2,"-",1593.9,44.0,47.8,"-",1.6,"-",7.0,239.4,"M39",32.0,"-"]
[null,"Cast Iron WNRF 125# ANSI B16.1 Size 60\"","Cast Iron WNRF"," 125#","ANSI B16.1","60\"",1500.0,1854.2,"-",79.5,"-",1759.0,52.0,47.8,"-",1.6,"-",7.0,246,"M39",32.0,"-"]
[null,"Cast Iron WNRF 250# ANSI B16.1 Size 1\"","Cast Iron WNRF"," 250#","ANSI B16.1","1\"",25.0,124.0,"-",17.5,68.0,89.0,4.0,19.1,"-",1.6,"-",3.0,80,"M16",13.0,"-"]
[null,"Cast Iron WNRF 250# ANSI B16.1 Size 1¼\"","Cast Iron WNRF"," 250#","ANSI B16.1","1¼\"",32.0,133.0,"-",19.1,78.0,98.0,4.0,19.1,"-",1.6,"-",3.0,83.2,"M16",13.0,"-"]
[null,"Cast Iron WNRF 250# ANSI B16.1 Size 1½\"","Cast Iron WNRF"," 250#","ANSI B16.1","1½\"",40.0,156.0,"-",20.6,91.0,114.0,4.0,22.3,"-",1.6,"-",3.0,92.2,"M20",16.0,"-"]
[null,"Cast Iron WNRF 250# ANSI B16.1 Size 2\"","Cast Iron WNRF"," 250#","ANSI B16.1","2\"",50.0,165.0,"-",22.2,106.0,127.0,8.0,19.1,"-",1.6,"-",4.0,90.4,"M16",13.0,"-"]
[null,"Cast Iron WNRF 250# ANSI B16.1 Size 2½\"","Cast Iron WNRF"," 250#","ANSI B16.1","2½\"",65.0,191.0,"-",25.4,125.0,149.0,8.0,22.3,"-",1.6,"-",4.0,102.8,"M20",16.0,"-"]
[null,"Cast Iron WNRF 250# ANSI B16.1 Size 3\"","Cast Iron WNRF"," 250#","ANSI B16.1","3\"",80.0,210.0,"-",28.6,144.0,168.0,8.0,22.3,"-",1.6,"-",4.0,109.2,"M20",16.0,"-"]
[null,"Cast Iron WNRF 250# ANSI B16.1 Size 3½\"","Cast Iron WNRF"," 250#","ANSI B16.1","3½\"","-",229.0,"-",30.2,160.0,184.0,8.0,22.3,"-",1.6,"-",4.0,112.4,"M20",16.0,"-"]
[null,"Cast Iron WNRF 250# ANSI B16.1 Size 4\"","Cast Iron WNRF"," 250#","ANSI B16.1","4\"",100.0,254.0,"-",31.8,176.0,200.0,8.0,22.3,"-",1.6,"-",5.0,116.6,"M20",16.0,"-"]
[null,"Cast Iron WNRF 250# ANSI B16.1 Size 5\"","Cast Iron WNRF"," 250#","ANSI B16.1","5\"",125.0,279.0,"-",34.9,211.0,235.0,8.0,22.3,"-",1.6,"-",5.0,122.8,"M20",16.0,"-"]
[null,"Cast Iron WNRF 250# ANSI B16.1 Size 6\"","Cast Iron WNRF"," 250#","ANSI B16.1","6\"",150.0,318.0,"-",36.5,246.0,270.0,12.0,22.3,"-",1.6,"-",6.0,127,"M20",16.0,"-"]
[null,"Cast Iron WNRF 250# ANSI B16.1 Size 8\"","Cast Iron WNRF"," 250#","ANSI B16.1","8\"",200.0,381.0,"-",41.3,303.0,330.0,12.0,25.4,"-",1.6,"-",6.0,142.6,"M24",19.0,"-"]
[null,"Cast Iron WNRF 250# ANSI B16.1 Size 10\"","Cast Iron WNRF"," 250#","ANSI B16.1","10\"",250.0,445.0,"-",47.6,357.0,387.0,16.0,29.0,"-",1.6,"-",6.0,161.2,"M27",22.0,"-"]
[null,"Cast Iron WNRF 250# ANSI B16.1 Size 12\"","Cast Iron WNRF"," 250#","ANSI B16.1","12\"",300.0,521.0,"-",50.8,418.0,451.0,16.0,32.0,"-",1.6,"-",6.0,171.6,"M30",24.0,"-"]
[null,"Cast Iron WNRF 250# ANSI B16.1 Size 14\"","Cast Iron WNRF"," 250#","ANSI B16.1","14\"",350.0,584.0,"-",54.0,481.0,514.0,20.0,32.0,"-",1.6,"-",7.0,179,"M30",24.0,"-"]
[null,"Cast Iron WNRF 250# ANSI B16.1 Size 16\"","Cast Iron WNRF"," 250#","ANSI B16.1","16\"",400.0,648.0,"-",57.2,535.0,572.0,20.0,35.0,"-",1.6,"-",7.0,189.4,"M33",26.0,"-"]
[null,"Cast Iron WNRF 250# ANSI B16.1 Size 18\"","Cast Iron WNRF"," 250#","ANSI B16.1","18\"",450.0,711.0,"-",60.3,592.0,629.0,24.0,35.0,"-",1.6,"-",7.0,195.6,"M33",26.0,"-"]
[null,"Cast Iron WNRF 250# ANSI B16.1 Size 20\"","Cast Iron WNRF"," 250#","ANSI B16.1","20\"",500.0,775.0,"-",63.5,649.0,686.0,24.0,35.0,"-",1.6,"-",7.0,202,"M33",26.0,"-"]
[null,"Cast Iron WNRF 250# ANSI B16.1 Size 24\"","Cast Iron WNRF"," 250#","ANSI B16.1","24\"",600.0,914.0,"-",69.9,770.0,813.0,24.0,41.0,"-",1.6,"-",7.0,224.8,"M39",31.0,"-"]
[null,"Cast Iron WNRF 250# ANSI B16.1 Size 30\"","Cast Iron WNRF"," 250#","ANSI B16.1","30\"",750.0,1092.0,"-","-",945.0,997.0,28.0,51.0,"-",1.6,"-",7.0,"-","M48",38.0,"-"]
[null,"Cast Iron WNRF 250# ANSI B16.1 Size 36\"","Cast Iron WNRF"," 250#","ANSI B16.1","36\"",900.0,1270.0,"-","-",1110.0,1168.0,32.0,57.0,"-",1.6,"-",7.0,"-","M52",42.0,"-"]
[null,"Cast Iron WNRF 250# ANSI B16.1 Size 42\"","Cast Iron WNRF"," 250#","ANSI B16.1","42\"",1000.0,1448.0,"-","-",1281.0,1340.0,36.0,57.0,"-",1.6,"-",7.0,"-","M52",42.0,"-"]
[null,"Cast Iron WNRF 250# ANSI B16.1 Size 48\"","Cast Iron WNRF"," 250#","ANSI B16.1","48\"",1200.0,1651.0,"-","-",1484.0,1543.0,40.0,57.0,"-",1.6,"-",7.0,"-","M52",42.0,"-"]
[null,"Cast Iron WNRF 800# ANSI B16.1 Size 2\"","Cast Iron WNRF"," 800#","ANSI B16.1","2\"",50.0,165.1,"-",31.8,"-",127.0,8.0,19.05,"-",1.6,"-",4.0,{"$f":"(J388+U388+8)*2+R388","v":109.6},"M16",13.0,"-"]
[null,"Cast Iron WNRF 800# ANSI B16.1 Size 2½\"","Cast Iron WNRF"," 800#","ANSI B16.1","2½\"",65.0,190.5,"-",34.9,"-",149.2,8.0,22.23,"-",1.6,"-",4.0,121.8,"M20",16.0,"-"]
[null,"Cast Iron WNRF 800# ANSI B16.1 Size 3\"","Cast Iron WNRF"," 800#","ANSI B16.1","3\"",80.0,209.6,"-",38.1,"-",168.3,8.0,22.23,"-",1.6,"-",4.0,128.2,"M20",16.0,"-"]
[null,"Cast Iron WNRF 800# ANSI B16.1 Size 3½\"","Cast Iron WNRF"," 800#","ANSI B16.1","3½\"","-",228.6,"-",41.3,"-",184.2,8.0,25.4,"-",1.6,"-",4.0,138.6,"M22",18.0,"-"]
[null,"Cast Iron WNRF 800# ANSI B16.1 Size 4\"","Cast Iron WNRF"," 800#","ANSI B16.1","4\"",100.0,273.1,"-",47.6,"-",215.9,8.0,25.4,"-",1.6,"-",5.0,152.2,"M22",18.0,"-"]
[null,"Cast Iron WNRF 800# ANSI B16.1 Size 5\"","Cast Iron WNRF"," 800#","ANSI B16.1","5\"",125.0,330.2,"-",54.0,"-",266.7,8.0,28.58,"-",1.6,"-",5.0,167,"M24",19.0,"-"]
[null,"Cast Iron WNRF 800# ANSI B16.1 Size 6\"","Cast Iron WNRF"," 800#","ANSI B16.1","6\"",150.0,355.6,"-",57.2,"-",292.1,12.0,28.58,"-",1.6,"-",6.0,174.4,"M24",19.0,"-"]
[null,"Cast Iron WNRF 800# ANSI B16.1 Size 8\"","Cast Iron WNRF"," 800#","ANSI B16.1","8\"",200.0,419.1,"-",63.5,"-",349.3,12.0,31.75,"-",1.6,"-",6.0,193,"M27",22.0,"-"]
[null,"Cast Iron WNRF 800# ANSI B16.1 Size 10\"","Cast Iron WNRF"," 800#","ANSI B16.1","10\"",250.0,508.0,"-",73.0,"-",431.8,16.0,34.93,"-",1.6,"-",6.0,216,"M30",24.0,"-"]
[null,"Cast Iron WNRF 800# ANSI B16.1 Size 12\"","Cast Iron WNRF"," 800#","ANSI B16.1","12\"",300.0,558.8,"-",76.2,"-",489.0,20.0,34.93,"-",1.6,"-",6.0,222.4,"M30",24.0,"-"]
[null,"WNRF 75# ANSI B16.47-API 605 Size 26\"","WNRF"," 75#","ANSI B16.47-API 605","26\"",650.0,762.0,58.7,33.3,704.9,723.9,36.0,19.1,676.1,1.6,7.9,7.0,115.6,"M16",13.0,40.0]
[null,"WNRF 75# ANSI B16.47-API 605 Size 28\"","WNRF"," 75#","ANSI B16.47-API 605","28\"",700.0,812.8,62.0,33.3,755.7,774.7,40.0,19.1,726.9,1.6,7.9,7.0,115.6,"M16",13.0,44.0]
[null,"WNRF 75# ANSI B16.47-API 605 Size 30\"","WNRF"," 75#","ANSI B16.47-API 605","30\"",750.0,863.6,65.0,33.3,806.5,825.5,44.0,19.1,777.7,1.6,7.9,7.0,115.6,"M16",13.0,48.0]
[null,"WNRF 75# ANSI B16.47-API 605 Size 32\"","WNRF"," 75#","ANSI B16.47-API 605","32\"",800.0,914.4,69.9,35.1,857.3,876.3,48.0,19.1,828.5,1.6,7.9,7.0,119.2,"M16",13.0,54.0]
[null,"WNRF 75# ANSI B16.47-API 605 Size 34\"","WNRF"," 75#","ANSI B16.47-API 605","34\"",850.0,965.2,73.2,35.1,908.1,927.1,52.0,19.1,879.3,1.6,7.9,7.0,119.2,"M16",13.0,59.0]
[null,"WNRF 75# ANSI B16.47-API 605 Size 36\"","WNRF"," 75#","ANSI B16.47-API 605","36\"",900.0,1033.5,85.9,36.6,965.2,992.1,40.0,22.4,935.0,1.6,9.7,7.0,128.2,"M20",16.0,78.0]
[null,"WNRF 75# ANSI B16.47-API 605 Size 38\"","WNRF"," 75#","ANSI B16.47-API 605","38\"",950.0,1084.3,88.9,38.1,1016.0,1042.9,40.0,22.4,985.8,1.6,9.7,7.0,131.2,"M20",16.0,85.0]
[null,"WNRF 75# ANSI B16.47-API 605 Size 40\"","WNRF"," 75#","ANSI B16.47-API 605","40\"",1000.0,1135.1,91.9,38.1,1066.8,1093.7,44.0,22.4,1036.6,1.6,9.7,7.0,131.2,"M20",16.0,93.0]
[null,"WNRF 75# ANSI B16.47-API 605 Size 42\"","WNRF"," 75#","ANSI B16.47-API 605","42\"",1050.0,1185.9,95.3,39.6,1117.6,1144.5,48.0,22.4,1087.4,1.6,9.7,7.0,134.2,"M20",16.0,100.0]
[null,"WNRF 75# ANSI B16.47-API 605 Size 44\"","WNRF"," 75#","ANSI B16.47-API 605","44\"",1100.0,1251.0,101.9,42.9,1174.8,1203.5,36.0,25.4,1140.0,1.6,9.7,7.0,144.8,"M22",18.0,113.0]
[null,"WNRF 75# ANSI B16.47-API 605 Size 46\"","WNRF"," 75#","ANSI B16.47-API 605","46\"",1150.0,1301.8,108.0,44.5,1225.6,1254.3,40.0,25.4,1190.8,1.6,9.7,7.0,148,"M22",18.0,127.0]
[null,"WNRF 75# ANSI B16.47-API 605 Size 48\"","WNRF"," 75#","ANSI B16.47-API 605","48\"",1200.0,1352.6,111.3,46.0,1276.4,1305.1,44.0,25.4,1241.6,1.6,9.7,7.0,151,"M22",18.0,141.0]
[null,"WNRF 75# ANSI B16.47-API 605 Size 50\"","WNRF"," 75#","ANSI B16.47-API 605","50\"",1250.0,1403.4,115.6,47.8,1327.2,1355.9,44.0,25.4,1293.9,1.6,9.7,7.0,154.6,"M22",18.0,153.0]
[null,"WNRF 75# ANSI B16.47-API 605 Size 52\"","WNRF"," 75#","ANSI B16.47-API 605","52\"",1300.0,1457.5,120.7,47.8,1378.0,1409.7,48.0,25.4,1344.7,1.6,9.7,7.0,154.6,"M22",18.0,160.0]
[null,"WNRF 75# ANSI B16.47-API 605 Size 54\"","WNRF"," 75#","ANSI B16.47-API 605","54\"",1350.0,1508.3,125.5,49.3,1428.8,1460.5,48.0,25.4,1397.0,1.6,9.7,7.0,157.6,"M22",18.0,177.0]
[null,"WNRF 75# ANSI B16.47-API 605 Size 56\"","WNRF"," 75#","ANSI B16.47-API 605","56\"",1400.0,1574.8,166.6,50.8,1485.9,1521.0,40.0,28.4,1450.8,1.6,11.2,7.0,162.6,"M24",19.0,198.0]
[null,"WNRF 75# ANSI B16.47-API 605 Size 58\"","WNRF"," 75#","ANSI B16.47-API 605","58\"",1450.0,1625.6,138.2,52.3,1536.7,1571.8,44.0,28.4,1501.6,1.6,11.2,7.0,165.6,"M24",19.0,218.0]
[null,"WNRF 75# ANSI B16.47-API 605 Size 60\"","WNRF"," 75#","ANSI B16.47-API 605","60\"",1500.0,1676.4,144.5,55.6,1587.5,1622.6,44.0,28.4,1552.4,1.6,11.2,7.0,172.2,"M24",19.0,245.0]
[null,"WNRF 150# ANSI B16.47-API 605 Size 26\"","WNRF"," 150#","ANSI B16.47-API 605","26\"",650.0,785.9,88.9,41.1,711.2,744.5,36.0,22.4,684.3,1.6,9.7,7.0,137.2,"M20",16.0,63.0]
[null,"WNRF 150# ANSI B16.47-API 605 Size 28\"","WNRF"," 150#","ANSI B16.47-API 605","28\"",700.0,836.7,95.3,44.5,762.0,795.3,40.0,22.4,735.1,1.6,9.7,7.0,144,"M20",16.0,74.0]
[null,"WNRF 150# ANSI B16.47-API 605 Size 30\"","WNRF"," 150#","ANSI B16.47-API 605","30\"",750.0,887.5,100.1,44.5,812.8,846.1,44.0,22.4,787.4,1.6,9.7,7.0,144,"M20",16.0,80.0]
[null,"WNRF 150# ANSI B16.47-API 605 Size 32\"","WNRF"," 150#","ANSI B16.47-API 605","32\"",800.0,941.3,108.0,46.0,863.6,900.2,48.0,22.4,839.7,1.6,9.7,7.0,147,"M20",16.0,92.0]
[null,"WNRF 150# ANSI B16.47-API 605 Size 34\"","WNRF"," 150#","ANSI B16.47-API 605","34\"",850.0,1004.8,110.2,49.3,920.8,957.3,40.0,25.4,892.0,1.6,9.7,7.0,157.6,"M22",18.0,113.0]
[null,"WNRF 150# ANSI B16.47-API 605 Size 36\"","WNRF"," 150#","ANSI B16.47-API 605","36\"",900.0,1057.1,117.3,52.3,971.6,1009.7,44.0,25.4,944.6,1.6,9.7,7.0,163.6,"M22",18.0,129.0]
[null,"WNRF 150# ANSI B16.47-API 605 Size 38\"","WNRF"," 150#","ANSI B16.47-API 605","38\"",950.0,1124.0,124.0,53.8,1022.4,1069.8,40.0,28.4,997.0,1.6,9.7,7.0,168.6,"M24",19.0,150.0]
[null,"WNRF 150# ANSI B16.47-API 605 Size 40\"","WNRF"," 150#","ANSI B16.47-API 605","40\"",1000.0,1174.8,128.5,55.6,1120.6,1120.6,44.0,28.4,1049.3,1.6,9.7,7.0,172.2,"M24",19.0,162.0]
[null,"WNRF 150# ANSI B16.47-API 605 Size 42\"","WNRF"," 150#","ANSI B16.47-API 605","42\"",1050.0,1225.6,133.4,58.7,1130.3,1171.4,48.0,28.4,1101.9,1.6,11.2,7.0,178.4,"M24",19.0,184.0]
[null,"WNRF 150# ANSI B16.47-API 605 Size 44\"","WNRF"," 150#","ANSI B16.47-API 605","44\"",1100.0,1276.4,136.7,60.5,1435.1,1222.2,52.0,28.4,1152.7,1.6,11.2,7.0,182,"M24",19.0,192.0]
[null,"WNRF 150# ANSI B16.47-API 605 Size 46\"","WNRF"," 150#","ANSI B16.47-API 605","46\"",1150.0,1341.4,144.5,62.0,1234.9,1284.2,40.0,31.8,1205.0,1.6,11.2,7.0,191,"M27",22.0,224.0]
[null,"WNRF 150# ANSI B16.47-API 605 Size 48\"","WNRF"," 150#","ANSI B16.47-API 605","48\"",1200.0,1392.2,149.4,65.0,1289.1,1335.0,44.0,31.8,1257.3,1.6,11.2,7.0,197,"M27",22.0,231.0]
[null,"WNRF 150# ANSI B16.47-API 605 Size 50\"","WNRF"," 150#","ANSI B16.47-API 605","50\"",1250.0,1435.4,153.9,68.3,1339.9,1385.8,48.0,31.8,1308.1,1.6,11.2,7.0,203.6,"M27",22.0,263.0]
[null,"WNRF 150# ANSI B16.47-API 605 Size 52\"","WNRF"," 150#","ANSI B16.47-API 605","52\"",1300.0,1493.8,157.2,69.9,1390.7,1436.6,52.0,31.8,1360.4,1.6,11.2,7.0,206.8,"M27",22.0,285.0]
[null,"WNRF 150# ANSI B16.47-API 605 Size 54\"","WNRF"," 150#","ANSI B16.47-API 605","54\"",1350.0,1549.4,162.1,71.4,1441.5,1492.3,56.0,31.8,1412.7,1.6,11.2,7.0,209.8,"M27",22.0,287.0]
[null,"WNRF 150# ANSI B16.47-API 605 Size 56\"","WNRF"," 150#","ANSI B16.47-API 605","56\"",1400.0,1600.2,166.6,73.2,1492.3,1543.1,60.0,31.8,1465.3,1.6,14.2,7.0,213.4,"M27",22.0,323.0]
[null,"WNRF 150# ANSI B16.47-API 605 Size 58\"","WNRF"," 150#","ANSI B16.47-API 605","58\"",1450.0,1674.9,174.8,74.7,1543.1,1611.4,48.0,35.1,1516.1,1.6,14.2,7.0,224.4,"M33",26.0,384.0]
[null,"WNRF 150# ANSI B16.47-API 605 Size 60\"","WNRF"," 150#","ANSI B16.47-API 605","60\"",1500.0,1725.7,179.3,76.2,1600.2,1662.2,52.0,35.1,1570.0,1.6,14.2,7.0,227.4,"M33",26.0,388.0]
[null,"WNRF 300# ANSI B16.47-API 605 Size 26\"","WNRF"," 300#","ANSI B16.47-API 605","26\"",650.0,866.6,144.5,88.9,736.6,803.1,32.0,35.1,701.5,1.6,14.2,7.0,252.8,"M33",26.0,181.0]
[null,"WNRF 300# ANSI B16.47-API 605 Size 28\"","WNRF"," 300#","ANSI B16.47-API 605","28\"",700.0,920.8,149.4,88.9,787.4,857.3,36.0,35.1,755.7,1.6,14.2,7.0,252.8,"M33",26.0,203.0]
[null,"WNRF 300# ANSI B16.47-API 605 Size 30\"","WNRF"," 300#","ANSI B16.47-API 605","30\"",750.0,990.6,158.0,93.7,844.6,920.8,36.0,38.1,812.8,1.6,14.2,7.0,262.4,"M36",26.0,268.0]
[null,"WNRF 300# ANSI B16.47-API 605 Size 32\"","WNRF"," 300#","ANSI B16.47-API 605","32\"",800.0,1054.1,168.1,103.1,901.7,977.9,32.0,41.1,863.6,1.6,15.7,7.0,291.2,"M39",31.0,330.0]
[null,"WNRF 300# ANSI B16.47-API 605 Size 34\"","WNRF"," 300#","ANSI B16.47-API 605","34\"",850.0,1107.9,173.0,103.1,952.5,1031.7,36.0,41.1,917.4,1.6,15.7,7.0,291.2,"M39",31.0,357.0]
[null,"WNRF 300# ANSI B16.47-API 605 Size 36\"","WNRF"," 300#","ANSI B16.47-API 605","36\"",900.0,1171.4,180.8,103.1,1009.7,1089.2,32.0,44.5,965.2,1.6,15.7,7.0,297.2,"M42",34.0,405.0]
[null,"WNRF 300# ANSI B16.47-API 605 Size 38\"","WNRF"," 300#","ANSI B16.47-API 605","38\"",950.0,1222.2,192.0,111.3,1060.5,1140.0,36.0,44.5,1016.0,1.6,15.7,7.0,313.6,"M42",34.0,416.0]
[null,"WNRF 300# ANSI B16.47-API 605 Size 40\"","WNRF"," 300#","ANSI B16.47-API 605","40\"",1000.0,1273.0,198.4,115.8,1114.6,1190.8,40.0,44.5,1066.8,1.6,15.7,7.0,322.6,"M42",34.0,450.0]
[null,"WNRF 300# ANSI B16.47-API 605 Size 42\"","WNRF"," 300#","ANSI B16.47-API 605","42\"",1050.0,1333.5,204.7,119.1,1168.4,1244.6,36.0,47.8,1117.6,1.6,15.7,7.0,333.2,"M45",36.0,502.0]
[null,"WNRF 300# ANSI B16.47-API 605 Size 44\"","WNRF"," 300#","ANSI B16.47-API 605","44\"",1100.0,1384.3,214.4,127.0,1219.2,1295.4,40.0,47.8,1173.2,1.6,15.7,7.0,349,"M45",36.0,552.0]
[null,"WNRF 300# ANSI B16.47-API 605 Size 46\"","WNRF"," 300#","ANSI B16.47-API 605","46\"",1150.0,1460.5,222.3,128.5,1270.0,1365.3,36.0,50.8,1228.9,1.6,15.7,7.0,356,"M48",38.0,650.0]
[null,"WNRF 300# ANSI B16.47-API 605 Size 48\"","WNRF"," 300#","ANSI B16.47-API 605","48\"",1200.0,1511.3,223.8,128.5,1327.2,1416.1,40.0,50.8,1277.9,1.6,15.7,7.0,356,"M48",38.0,731.0]
[null,"WNRF 300# ANSI B16.47-API 605 Size 50\"","WNRF"," 300#","ANSI B16.47-API 605","50\"",1250.0,1562.1,235.0,138.2,1378.0,1466.9,44.0,50.8,1330.5,1.6,15.7,7.0,375.4,"M48",38.0,760.0]
[null,"WNRF 300# ANSI B16.47-API 605 Size 52\"","WNRF"," 300#","ANSI B16.47-API 605","52\"",1300.0,1612.9,242.8,142.7,1428.8,1517.7,48.0,50.8,1382.8,1.6,15.7,7.0,384.4,"M48",38.0,800.0]
[null,"WNRF 300# ANSI B16.47-API 605 Size 54\"","WNRF"," 300#","ANSI B16.47-API 605","54\"",1350.0,1673.4,239.8,136.7,1479.6,1577.8,48.0,50.8,1435.1,1.6,15.7,7.0,372.4,"M48",38.0,898.0]
[null,"WNRF 300# ANSI B16.47-API 605 Size 56\"","WNRF"," 300#","ANSI B16.47-API 605","56\"",1400.0,1765.3,268.2,153.9,1536.7,1651.0,36.0,60.5,1493.8,1.6,17.5,7.0,420.8,"M56",45.0,1143.0]
[null,"WNRF 300# ANSI B16.47-API 605 Size 58\"","WNRF"," 300#","ANSI B16.47-API 605","58\"",1450.0,1827.3,274.6,153.9,1593.9,1713.0,40.0,60.5,1547.9,1.6,17.5,7.0,420.8,"M56",45.0,1217.0]
[null,"WNRF 300# ANSI B16.47-API 605 Size 60\"","WNRF"," 300#","ANSI B16.47-API 605","60\"",1500.0,1878.1,271.5,150.9,1651.0,1763.8,40.0,60.5,1598.7,1.6,17.5,7.0,414.8,"M56",45.0,1311.0]
[null,"WNRF 400# ANSI B16.47-API 605 Size 26\"","WNRF"," 400#","ANSI B16.47-API 605","26\"",650.0,850.9,155.8,95.3,711.2,781.1,28.0,38.1,688.8,6.4,11.2,7.0,271.6,"M36",29.0,176.0]
[null,"WNRF 400# ANSI B16.47-API 605 Size 28\"","WNRF"," 400#","ANSI B16.47-API 605","28\"",700.0,914.4,165.2,101.7,762.0,838.2,24.0,41.1,739.6,6.4,12.7,7.0,288.4,"M39",31.0,216.0]
[null,"WNRF 400# ANSI B16.47-API 605 Size 30\"","WNRF"," 400#","ANSI B16.47-API 605","30\"",750.0,971.6,183.9,108.0,819.2,895.4,28.0,41.1,793.8,6.4,12.7,7.0,301,"M39",31.0,253.0]
[null,"WNRF 400# ANSI B16.47-API 605 Size 32\"","WNRF"," 400#","ANSI B16.47-API 605","32\"",800.0,1035.1,185.7,114.4,873.3,952.5,28.0,44.5,844.6,6.4,12.7,7.0,319.8,"M42",34.0,300.0]
[null,"WNRF 400# ANSI B16.47-API 605 Size 34\"","WNRF"," 400#","ANSI B16.47-API 605","34\"",850.0,1085.9,193.9,117.7,927.1,1003.3,32.0,44.5,898.7,6.4,14.2,7.0,326.4,"M42",34.0,327.0]
[null,"WNRF 400# ANSI B16.47-API 605 Size 36\"","WNRF"," 400#","ANSI B16.47-API 605","36\"",900.0,1155.7,206.6,125.5,980.9,1066.8,28.0,47.8,952.5,6.4,14.2,7.0,346,"M45",36.0,402.0]
[null,"WNRF 400# ANSI B16.47-API 605 Size 38\"","WNRF"," 400#","ANSI B16.47-API 605","38\"",950.0,1206.5,212.6,130.4,1035.1,1117.6,32.0,47.8,1003.3,6.4,14.2,7.0,355.8,"M45",36.0,433.0]
[null,"WNRF 400# ANSI B16.47-API 605 Size 40\"","WNRF"," 400#","ANSI B16.47-API 605","40\"",1000.0,1270.0,222.3,136.4,1092.2,1174.8,32.0,50.8,1054.1,6.4,14.2,7.0,371.8,"M48",38.0,505.0]
[null,"WNRF 400# ANSI B16.47-API 605 Size 42\"","WNRF"," 400#","ANSI B16.47-API 605","42\"",1050.0,1320.8,230.2,139.8,1143.0,1225.6,32.0,50.8,1107.9,6.4,14.2,7.0,378.6,"M48",38.0,542.0]
[null,"WNRF 400# ANSI B16.47-API 605 Size 44\"","WNRF"," 400#","ANSI B16.47-API 605","44\"",1100.0,1384.3,239.8,146.1,1200.2,1282.7,32.0,53.8,1158.7,6.4,14.2,7.0,391.2,"M48",38.0,613.0]
[null,"WNRF 400# ANSI B16.47-API 605 Size 46\"","WNRF"," 400#","ANSI B16.47-API 605","46\"",1150.0,1441.5,250.7,152.5,1257.3,1339.9,36.0,53.8,1212.9,6.4,14.2,7.0,404,"M48",38.0,678.0]
[null,"WNRF 400# ANSI B16.47-API 605 Size 48\"","WNRF"," 400#","ANSI B16.47-API 605","48\"",1200.0,1511.3,263.4,158.8,1308.1,1403.4,28.0,60.5,1267.0,6.4,14.2,7.0,430.6,"M56",45.0,802.0]
[null,"WNRF 400# ANSI B16.47-API 605 Size 50\"","WNRF"," 400#","ANSI B16.47-API 605","50\"",1250.0,1568.5,274.6,163.6,1361.9,1460.5,32.0,60.5,1320.8,6.4,14.2,7.0,440.2,"M56",45.0,885.0]
[null,"WNRF 400# ANSI B16.47-API 605 Size 52\"","WNRF"," 400#","ANSI B16.47-API 605","52\"",1300.0,1619.3,282.8,168.5,1412.7,1511.3,32.0,60.5,1371.6,6.4,14.2,7.0,450,"M56",45.0,1020.0]
[null,"WNRF 400# ANSI B16.47-API 605 Size 54\"","WNRF"," 400#","ANSI B16.47-API 605","54\"",1350.0,1701.8,295.5,176.3,1470.2,1581.2,28.0,66.5,1425.4,6.4,14.2,7.0,471.6,"M60",48.0,1194.0]
[null,"WNRF 400# ANSI B16.47-API 605 Size 56\"","WNRF"," 400#","ANSI B16.47-API 605","56\"",1400.0,1752.6,304.9,181.2,1527.0,1632.0,32.0,66.5,1479.6,6.4,14.2,7.0,481.4,"M60",48.0,1262.0]
[null,"WNRF 400# ANSI B16.47-API 605 Size 58\"","WNRF"," 400#","ANSI B16.47-API 605","58\"",1450.0,1803.4,312.7,184.2,1577.8,1682.8,32.0,66.5,1530.4,6.4,14.2,7.0,487.4,"M60",48.0,1322.0]
[null,"WNRF 400# ANSI B16.47-API 605 Size 60\"","WNRF"," 400#","ANSI B16.47-API 605","60\"",1500.0,1886.0,325.4,192.1,1635.3,1752.6,32.0,73.2,1524.0,6.4,14.2,7.0,515.2,"M68",54.0,1550.0]
[null,"WNRF 600# ANSI B16.47-API 605 Size 26\"","WNRF"," 600#","ANSI B16.47-API 605","26\"",650.0,889.0,187.2,117.7,726.9,806.5,28.0,44.5,698.5,6.4,12.7,7.0,326.4,"M42",34.0,267.0]
[null,"WNRF 600# ANSI B16.47-API 605 Size 28\"","WNRF"," 600#","ANSI B16.47-API 605","28\"",700.0,952.5,196.9,122.2,784.4,863.6,28.0,47.8,752.3,6.4,12.7,7.0,339.4,"M45",36.0,326.0]
[null,"WNRF 600# ANSI B16.47-API 605 Size 30\"","WNRF"," 600#","ANSI B16.47-API 605","30\"",750.0,1022.4,211.1,131.9,841.2,927.1,28.0,50.8,806.5,6.4,12.7,7.0,362.8,"M48",38.0,402.0]
[null,"WNRF 600# ANSI B16.47-API 605 Size 32\"","WNRF"," 600#","ANSI B16.47-API 605","32\"",800.0,1085.9,222.3,136.4,895.4,984.3,28.0,53.8,860.6,6.4,12.7,7.0,371.8,"M48",38.0,462.0]
[null,"WNRF 600# ANSI B16.47-API 605 Size 34\"","WNRF"," 600#","ANSI B16.47-API 605","34\"",850.0,1162.1,239.8,147.6,952.5,1054.1,24.0,60.5,914.4,6.4,14.2,7.0,408.2,"M56",45.0,582.0]
[null,"WNRF 600# ANSI B16.47-API 605 Size 36\"","WNRF"," 600#","ANSI B16.47-API 605","36\"",900.0,1212.9,249.2,152.5,1009.7,1104.9,28.0,60.5,968.2,6.4,14.2,7.0,418,"M56",45.0,627.0]
[null,"WNRF 600# ANSI B16.47-API 605 Size 38\"","WNRF"," 600#","ANSI B16.47-API 605","38\"",950.0,1270.0,260.4,158.8,1054.1,1162.1,28.0,60.5,1022.4,6.4,14.2,7.0,430.6,"M56",45.0,707.0]
[null,"WNRF 600# ANSI B16.47-API 605 Size 40\"","WNRF"," 600#","ANSI B16.47-API 605","40\"",1000.0,1320.8,270.1,165.2,111.3,1212.9,32.0,60.5,1073.2,6.4,14.2,7.0,443.4,"M56",45.0,762.0]
[null,"WNRF 600# ANSI B16.47-API 605 Size 42\"","WNRF"," 600#","ANSI B16.47-API 605","42\"",1050.0,1403.4,285.8,174.5,1168.4,1282.7,28.0,66.5,1127.3,6.4,14.2,7.0,468,"M60",48.0,928.0]
[null,"WNRF 600# ANSI B16.47-API 605 Size 44\"","WNRF"," 600#","ANSI B16.47-API 605","44\"",1100.0,1454.2,295.5,179.4,1225.6,1333.5,32.0,66.5,1181.1,6.4,14.2,7.0,477.8,"M60",48.0,992.0]
[null,"WNRF 600# ANSI B16.47-API 605 Size 46\"","WNRF"," 600#","ANSI B16.47-API 605","46\"",1150.0,1511.3,306.4,185.7,1276.4,1390.7,32.0,66.5,1234.9,6.4,14.2,7.0,490.4,"M60",48.0,1100.0]
[null,"WNRF 600# ANSI B16.47-API 605 Size 48\"","WNRF"," 600#","ANSI B16.47-API 605","48\"",1200.0,1593.9,322.4,195.4,1333.5,1460.5,32.0,73.2,1289.1,6.4,14.2,7.0,521.8,"M68",54.0,1299.0]
[null,"WNRF 600# ANSI B16.47-API 605 Size 50\"","WNRF"," 600#","ANSI B16.47-API 605","50\"",1250.0,1671.1,335.1,203.3,1384.3,1524.0,28.0,79.2,1343.2,6.4,14.2,7.0,545.6,"M72",58.0,1524.0]
[null,"WNRF 600# ANSI B16.47-API 605 Size 52\"","WNRF"," 600#","ANSI B16.47-API 605","52\"",1300.0,1720.9,343.0,209.6,1435.1,1574.8,32.0,79.2,1394.0,6.4,14.2,7.0,558.2,"M72",58.0,1585.0]
[null,"WNRF 600# ANSI B16.47-API 605 Size 54\"","WNRF"," 600#","ANSI B16.47-API 605","54\"",1350.0,1778.0,355.7,216.0,1492.3,1632.0,32.0,79.2,1447.8,6.4,14.2,7.0,571,"M72",58.0,1735.0]
[null,"WNRF 600# ANSI B16.47-API 605 Size 56\"","WNRF"," 600#","ANSI B16.47-API 605","56\"",1400.0,1854.2,368.4,223.8,1543.1,1695.5,32.0,85.9,1501.6,6.4,15.7,7.0,598.6,"M80",64.0,1952.0]
[null,"WNRF 600# ANSI B16.47-API 605 Size 58\"","WNRF"," 600#","ANSI B16.47-API 605","58\"",1450.0,1905.0,376.2,228.7,1600.2,1746.3,32.0,85.9,1552.4,6.4,15.7,7.0,608.4,"M80",64.0,2069.0]
[null,"WNRF 600# ANSI B16.47-API 605 Size 60\"","WNRF"," 600#","ANSI B16.47-API 605","60\"",1500.0,1993.9,395.3,239.8,1657.4,1822.5,28.0,91.9,1609.9,6.4,17.5,7.0,638.6,"M85",68.0,2474.0]
[null,"WNRF 900# ANSI B16.47-API 605 Size 26\"","WNRF"," 900#","ANSI B16.47-API 605","26\"",650.0,1022.4,265.2,141.3,762.0,901.7,20.0,66.5,743.0,6.4,11.2,7.0,401.6,"M60",48.0,564.0]
[null,"WNRF 900# ANSI B16.47-API 605 Size 28\"","WNRF"," 900#","ANSI B16.47-API 605","28\"",700.0,1104.9,267.5,154.0,819.2,971.6,20.0,73.2,797.1,6.4,12.7,7.0,439,"M68",54.0,706.0]
[null,"WNRF 900# ANSI B16.47-API 605 Size 30\"","WNRF"," 900#","ANSI B16.47-API 605","30\"",750.0,1181.1,295.5,161.8,876.3,1035.1,20.0,79.2,850.9,6.4,12.7,7.0,462.6,"M72",58.0,833.0]
[null,"WNRF 900# ANSI B16.47-API 605 Size 32\"","WNRF"," 900#","ANSI B16.47-API 605","32\"",800.0,1238.3,309.7,166.7,927.1,1092.2,20.0,79.2,908.1,6.4,12.7,7.0,472.4,"M72",58.0,919.0]
[null,"WNRF 900# ANSI B16.47-API 605 Size 34\"","WNRF"," 900#","ANSI B16.47-API 605","34\"",850.0,1314.5,325.4,177.9,990.6,1155.7,20.0,85.9,962.2,6.4,14.2,7.0,506.8,"M80",64.0,1105.0]
[null,"WNRF 900# ANSI B16.47-API 605 Size 36\"","WNRF"," 900#","ANSI B16.47-API 605","36\"",900.0,1346.2,331.8,179.4,1028.7,1200.2,24.0,79.2,1016.0,6.4,14.2,7.0,497.8,"M72",58.0,1124.0]
[null,"WNRF 900# ANSI B16.47-API 605 Size 38\"","WNRF"," 900#","ANSI B16.47-API 605","38\"",950.0,1460.5,359.0,196.9,1098.6,1289.1,20.0,91.9,1022.4,6.4,19.1,7.0,552.8,"M85",68.0,1495.0]
[null,"WNRF 900# ANSI B16.47-API 605 Size 40\"","WNRF"," 900#","ANSI B16.47-API 605","40\"",1000.0,1511.3,369.9,203.3,1162.1,1339.9,24.0,91.9,1127.3,6.4,20.6,7.0,565.6,"M85",68.0,1584.0]
[null,"WNRF 900# ANSI B16.47-API 605 Size 42\"","WNRF"," 900#","ANSI B16.47-API 605","42\"",1050.0,1562.1,377.7,212.6,1212.9,1390.7,24.0,91.9,1176.3,6.4,20.6,7.0,584.2,"M85",68.0,1718.0]
[null,"WNRF 900# ANSI B16.47-API 605 Size 44\"","WNRF"," 900#","ANSI B16.47-API 605","44\"",1100.0,1648.0,397.1,220.8,1270.0,1463.5,24.0,98.6,1234.9,6.4,22.4,7.0,608.6,"M90",72.0,2006.0]
[null,"WNRF 900# ANSI B16.47-API 605 Size 46\"","WNRF"," 900#","ANSI B16.47-API 605","46\"",1150.0,1733.6,417.6,232.0,1333.5,1536.7,24.0,104.6,1292.4,6.4,22.4,7.0,639,"M95",76.0,2337.0]
[null,"WNRF 900# ANSI B16.47-API 605 Size 48\"","WNRF"," 900#","ANSI B16.47-API 605","48\"",1200.0,1784.4,425.5,239.8,1384.3,1587.5,24.0,104.6,1343.2,6.4,23.9,7.0,654.6,"M95",76.0,2509.0]
[null,"WNRF 150# ANSI B16.47-MSS SP-44 Size 12\"","WNRF"," 150#","ANSI B16.47-MSS SP-44","12\"",300.0,482.6,114.3,31.8,381.0,431.8,12.0,25.4,365.3,1.6,9.7,6.0,121.6,"M22",18.0,43.0]
[null,"WNRF 150# ANSI B16.47-MSS SP-44 Size 14\"","WNRF"," 150#","ANSI B16.47-MSS SP-44","14\"",350.0,533.4,127.0,35.1,412.8,476.3,12.0,28.4,400.1,1.6,9.7,7.0,131.2,"M24",19.0,58.0]
[null,"WNRF 150# ANSI B16.47-MSS SP-44 Size 16\"","WNRF"," 150#","ANSI B16.47-MSS SP-44","16\"",400.0,596.9,127.0,36.6,469.9,539.8,16.0,28.4,457.2,1.6,9.7,7.0,134.2,"M24",19.0,76.0]
[null,"WNRF 150# ANSI B16.47-MSS SP-44 Size 18\"","WNRF"," 150#","ANSI B16.47-MSS SP-44","18\"",450.0,635.0,139.7,39.6,533.4,577.9,16.0,31.8,505.0,1.6,9.7,7.0,146.2,"M27",22.0,94.0]
[null,"WNRF 150# ANSI B16.47-MSS SP-44 Size 20\"","WNRF"," 150#","ANSI B16.47-MSS SP-44","20\"",500.0,698.5,144.5,42.9,584.2,635.0,20.0,31.8,558.8,1.6,9.7,7.0,152.8,"M27",22.0,122.0]
[null,"WNRF 150# ANSI B16.47-MSS SP-44 Size 22\"","WNRF"," 150#","ANSI B16.47-MSS SP-44","22\"",550.0,749.3,179.4,46.0,641.4,692.2,20.0,35.1,609.6,1.6,9.7,7.0,167,"M33",26.0,154.0]
[null,"WNRF 150# ANSI B16.47-MSS SP-44 Size 24\"","WNRF"," 150#","ANSI B16.47-MSS SP-44","24\"",600.0,812.8,152.4,47.8,692.2,749.3,20.0,35.1,663.4,1.6,9.7,7.0,170.6,"M33",26.0,185.0]
[null,"WNRF 150# ANSI B16.47-MSS SP-44 Size 26\"","WNRF"," 150#","ANSI B16.47-MSS SP-44","26\"",650.0,870.0,120.7,68.3,749.3,806.5,24.0,35.1,676.1,1.6,9.7,7.0,211.6,"M33",26.0,306.0]
[null,"WNRF 150# ANSI B16.47-MSS SP-44 Size 28\"","WNRF"," 150#","ANSI B16.47-MSS SP-44","28\"",700.0,927.1,125.5,71.4,800.1,863.6,28.0,35.1,726.9,1.6,11.2,7.0,217.8,"M33",26.0,363.0]
[null,"WNRF 150# ANSI B16.47-MSS SP-44 Size 30\"","WNRF"," 150#","ANSI B16.47-MSS SP-44","30\"",750.0,684.2,136.7,74.7,857.3,914.4,28.0,35.1,781.1,1.6,11.2,7.0,220.4,"M33",24.0,430.0]
[null,"WNRF 150# ANSI B16.47-MSS SP-44 Size 32\"","WNRF"," 150#","ANSI B16.47-MSS SP-44","32\"",800.0,1060.4,144.5,80.8,914.4,977.9,28.0,41.1,831.9,1.6,11.2,7.0,246.6,"M39",31.0,537.0]
[null,"WNRF 150# ANSI B16.47-MSS SP-44 Size 34\"","WNRF"," 150#","ANSI B16.47-MSS SP-44","34\"",850.0,1111.2,149.4,82.6,965.2,1028.7,32.0,41.1,882.7,1.6,12.7,7.0,250.2,"M39",31.0,600.0]
[null,"WNRF 150# ANSI B16.47-MSS SP-44 Size 36\"","WNRF"," 150#","ANSI B16.47-MSS SP-44","36\"",900.0,1168.4,157.2,90.4,1022.4,1085.9,32.0,41.1,933.5,1.6,12.7,7.0,265.8,"M39",31.0,730.0]
[null,"WNRF 150# ANSI B16.47-MSS SP-44 Size 38\"","WNRF"," 150#","ANSI B16.47-MSS SP-44","38\"",950.0,1238.2,157.2,87.4,1073.2,1149.4,32.0,41.1,990.6,1.6,12.7,7.0,259.8,"M39",31.0,792.0]
[null,"WNRF 150# ANSI B16.47-MSS SP-44 Size 40\"","WNRF"," 150#","ANSI B16.47-MSS SP-44","40\"",1000.0,1289.0,163.6,90.4,1124.0,1200.2,36.0,41.1,1041.4,1.6,12.7,7.0,265.8,"M39",31.0,893.0]
[null,"WNRF 150# ANSI B16.47-MSS SP-44 Size 42\"","WNRF"," 150#","ANSI B16.47-MSS SP-44","42\"",1050.0,1346.2,171.5,96.8,1193.8,1257.3,36.0,41.1,1092.2,1.6,12.7,7.0,278.6,"M39",31.0,1044.0]
[null,"WNRF 150# ANSI B16.47-MSS SP-44 Size 44\"","WNRF"," 150#","ANSI B16.47-MSS SP-44","44\"",1100.0,1403.3,177.8,101.6,1244.6,1314.5,40.0,41.1,1143.0,1.6,12.7,7.0,288.2,"M39",31.0,1190.0]
[null,"WNRF 150# ANSI B16.47-MSS SP-44 Size 46\"","WNRF"," 150#","ANSI B16.47-MSS SP-44","46\"",1150.0,1454.1,185.7,103.1,1295.4,1365.3,40.0,41.1,1196.8,1.6,12.7,7.0,291.2,"M39",31.0,1299.0]
[null,"WNRF 150# ANSI B16.47-MSS SP-44 Size 48\"","WNRF"," 150#","ANSI B16.47-MSS SP-44","48\"",1200.0,1511.3,191.3,108.0,1325.9,1422.4,44.0,41.1,1247.6,1.6,12.7,7.0,301,"M39",31.0,1470.0]
[null,"WNRF 150# ANSI B16.47-MSS SP-44 Size 50\"","WNRF"," 150#","ANSI B16.47-MSS SP-44","50\"",1250.0,1568.4,203.2,111.3,1409.7,1479.6,44.0,47.8,1301.8,1.6,12.7,7.0,317.6,"M45",36.0,1615.0]
[null,"WNRF 150# ANSI B16.47-MSS SP-44 Size 52\"","WNRF"," 150#","ANSI B16.47-MSS SP-44","52\"",1300.0,1625.6,209.6,115.8,1460.5,1536.7,44.0,47.8,1352.6,1.6,12.7,7.0,326.6,"M45",36.0,1817.0]
[null,"WNRF 150# ANSI B16.47-MSS SP-44 Size 54\"","WNRF"," 150#","ANSI B16.47-MSS SP-44","54\"",1350.0,1682.7,215.9,120.7,1511.3,1593.9,44.0,47.8,1403.4,1.6,12.7,7.0,336.4,"M45",36.0,2031.0]
[null,"WNRF 150# ANSI B16.47-MSS SP-44 Size 56\"","WNRF"," 150#","ANSI B16.47-MSS SP-44","56\"",1400.0,1746.2,228.6,124.0,1574.8,1651.0,48.0,47.8,1457.5,1.6,12.7,7.0,343,"M45",36.0,2244.0]
[null,"WNRF 150# ANSI B16.47-MSS SP-44 Size 58\"","WNRF"," 150#","ANSI B16.47-MSS SP-44","58\"",1450.0,1803.4,235.0,128.5,1625.6,1708.2,48.0,47.8,1508.3,1.6,12.7,7.0,352,"M45",36.0,2491.0]
[null,"WNRF 150# ANSI B16.47-MSS SP-44 Size 60\"","WNRF"," 150#","ANSI B16.47-MSS SP-44","60\"",1500.0,1854.2,239.8,131.8,1676.4,1759.0,52.0,47.8,1559.1,1.6,12.7,7.0,358.6,"M45",36.0,2697.0]
[null,"WNRF 300# ANSI B16.47-MSS SP-44 Size 12\"","WNRF"," 300#","ANSI B16.47-MSS SP-44","12\"",300.0,520.7,130.0,50.8,"-",450.9,16.0,31.8,374.7,1.6,9.65,6.0,167.6,"M27",22.0,62.0]
[null,"WNRF 300# ANSI B16.47-MSS SP-44 Size 14\"","WNRF"," 300#","ANSI B16.47-MSS SP-44","14\"",350.0,584.2,142.7,53.8,"-",514.4,20.0,31.8,425.5,1.6,9.65,7.0,174.6,"M27",22.0,86.0]
[null,"WNRF 300# ANSI B16.47-MSS SP-44 Size 16\"","WNRF"," 300#","ANSI B16.47-MSS SP-44","16\"",400.0,647.7,146.1,57.2,"-",571.5,20.0,35.1,482.6,1.6,9.65,7.0,189.4,"M33",26.0,106.0]
[null,"WNRF 300# ANSI B16.47-MSS SP-44 Size 18\"","WNRF"," 300#","ANSI B16.47-MSS SP-44","18\"",450.0,711.2,158.8,60.5,"-",628.7,24.0,35.1,533.4,1.6,9.65,7.0,196,"M33",26.0,131.0]
[null,"WNRF 300# ANSI B16.47-MSS SP-44 Size 20\"","WNRF"," 300#","ANSI B16.47-MSS SP-44","20\"",500.0,774.7,162.1,63.5,"-",685.8,24.0,35.1,587.2,1.6,9.65,7.0,202,"M33",26.0,158.0]
[null,"WNRF 300# ANSI B16.47-MSS SP-44 Size 22\"","WNRF"," 300#","ANSI B16.47-MSS SP-44","22\"",550.0,838.2,165.1,66.5,"-",743.0,24.0,41.1,641.4,1.6,9.65,7.0,218,"M39",31.0,194.0]
[null,"WNRF 300# ANSI B16.47-MSS SP-44 Size 24\"","WNRF"," 300#","ANSI B16.47-MSS SP-44","24\"",600.0,914.4,168.1,69.9,"-",812.8,24.0,41.1,701.5,1.6,9.65,7.0,224.8,"M39",31.0,230.0]
[null,"WNRF 300# ANSI B16.47-MSS SP-44 Size 26\"","WNRF"," 300#","ANSI B16.47-MSS SP-44","26\"",650.0,971.6,184.2,79.2,749.3,876.3,28.0,44.5,720.9,1.6,9.65,7.0,249.4,"M42",34.0,275.0]
[null,"WNRF 300# ANSI B16.47-MSS SP-44 Size 28\"","WNRF"," 300#","ANSI B16.47-MSS SP-44","28\"",700.0,1035.1,196.9,85.9,800.1,939.8,28.0,44.5,774.7,1.6,11.2,7.0,262.8,"M42",34.0,340.0]
[null,"WNRF 300# ANSI B16.47-MSS SP-44 Size 30\"","WNRF"," 300#","ANSI B16.47-MSS SP-44","30\"",750.0,1092.2,209.6,91.9,857.2,997.0,28.0,47.8,827.0,1.6,11.2,7.0,278.8,"M45",36.0,389.0]
[null,"WNRF 300# ANSI B16.47-MSS SP-44 Size 32\"","WNRF"," 300#","ANSI B16.47-MSS SP-44","32\"",800.0,1149.4,222.3,98.6,914.4,1054.1,28.0,50.8,881.1,1.6,11.2,7.0,296.2,"M48",38.0,438.0]
[null,"WNRF 300# ANSI B16.47-MSS SP-44 Size 34\"","WNRF"," 300#","ANSI B16.47-MSS SP-44","34\"",850.0,1206.5,231.6,101.6,965.2,1104.9,28.0,50.8,936.8,1.6,12.7,7.0,302.2,"M48",38.0,498.0]
[null,"WNRF 300# ANSI B16.47-MSS SP-44 Size 36\"","WNRF"," 300#","ANSI B16.47-MSS SP-44","36\"",900.0,1270.0,241.3,104.6,1022.3,1168.4,32.0,53.8,990.6,1.6,12.7,7.0,308.2,"M48",38.0,563.0]
[null,"WNRF 300# ANSI B16.47-MSS SP-44 Size 38\"","WNRF"," 300#","ANSI B16.47-MSS SP-44","38\"",950.0,1168.4,180.8,108.0,1028.7,1092.2,32.0,41.1,993.6,1.6,12.7,7.0,301,"M39",31.0,307.0]
[null,"WNRF 300# ANSI B16.47-MSS SP-44 Size 40\"","WNRF"," 300#","ANSI B16.47-MSS SP-44","40\"",1000.0,1238.3,193.5,114.3,1085.8,1155.7,32.0,44.5,1047.8,1.6,12.7,7.0,319.6,"M42",34.0,372.0]
[null,"WNRF 300# ANSI B16.47-MSS SP-44 Size 42\"","WNRF"," 300#","ANSI B16.47-MSS SP-44","42\"",1050.0,1289.1,200.2,119.1,1136.6,1206.5,32.0,44.5,1098.6,1.6,12.7,7.0,329.2,"M42",34.0,409.0]
[null,"WNRF 300# ANSI B16.47-MSS SP-44 Size 44\"","WNRF"," 300#","ANSI B16.47-MSS SP-44","44\"",1100.0,1352.6,206.2,124.0,1193.8,1263.7,32.0,47.8,1149.4,1.6,12.7,7.0,343,"M45",36.0,464.0]
[null,"WNRF 300# ANSI B16.47-MSS SP-44 Size 46\"","WNRF"," 300#","ANSI B16.47-MSS SP-44","46\"",1150.0,1416.1,215.9,128.0,1244.6,1320.8,28.0,50.8,1203.5,1.6,12.7,7.0,355,"M48",38.0,544.0]
[null,"WNRF 300# ANSI B16.47-MSS SP-44 Size 48\"","WNRF"," 300#","ANSI B16.47-MSS SP-44","48\"",1200.0,1466.9,222.9,133.4,1301.7,1371.6,32.0,50.8,1254.3,1.6,12.7,7.0,365.8,"M48",38.0,567.0]
[null,"WNRF 300# ANSI B16.47-MSS SP-44 Size 50\"","WNRF"," 300#","ANSI B16.47-MSS SP-44","50\"",1250.0,1530.4,231.6,139.7,1358.9,1428.8,32.0,53.8,1305.1,1.6,12.7,7.0,378.4,"M48",38.0,643.0]
[null,"WNRF 300# ANSI B16.47-MSS SP-44 Size 52\"","WNRF"," 300#","ANSI B16.47-MSS SP-44","52\"",1300.0,1581.2,238.3,144.5,1409.7,1479.6,32.0,53.8,1355.9,1.6,12.7,7.0,388,"M48",38.0,694.0]
[null,"WNRF 300# ANSI B16.47-MSS SP-44 Size 54\"","WNRF"," 300#","ANSI B16.47-MSS SP-44","54\"",1350.0,1657.4,252.5,152.4,1466.8,1549.4,28.0,60.5,1409.7,1.6,12.7,7.0,417.8,"M56",45.0,832.0]
[null,"WNRF 300# ANSI B16.47-MSS SP-44 Size 56\"","WNRF"," 300#","ANSI B16.47-MSS SP-44","56\"",1400.0,1708.2,260.4,153.9,1517.6,1600.2,28.0,60.5,1463.5,1.6,12.7,7.0,420.8,"M56",45.0,882.0]
[null,"WNRF 300# ANSI B16.47-MSS SP-44 Size 58\"","WNRF"," 300#","ANSI B16.47-MSS SP-44","58\"",1450.0,1759.0,266.7,158.8,1574.8,1651.0,32.0,60.5,1514.3,1.6,12.7,7.0,430.6,"M56",45.0,928.0]
[null,"WNRF 300# ANSI B16.47-MSS SP-44 Size 60\"","WNRF"," 300#","ANSI B16.47-MSS SP-44","60\"",1500.0,1809.8,273.1,163.6,1625.6,1701.8,32.0,60.5,1565.1,1.6,12.7,7.0,440.2,"M56",45.0,989.0]
[null,"WNRF 400# ANSI B16.47-MSS SP-44 Size 12\"","WNRF"," 400#","ANSI B16.47-MSS SP-44","12\"",300.0,323.8,143.1,63.6,"-",450.9,16.0,35.1,374.7,6.4,9.65,6.0,201.2,"M33",26.0,70.0]
[null,"WNRF 400# ANSI B16.47-MSS SP-44 Size 14\"","WNRF"," 400#","ANSI B16.47-MSS SP-44","14\"",350.0,355.6,155.8,66.9,"-",514.4,20.0,35.1,425.5,6.4,9.65,7.0,208.8,"M33",26.0,96.0]
[null,"WNRF 400# ANSI B16.47-MSS SP-44 Size 16\"","WNRF"," 400#","ANSI B16.47-MSS SP-44","16\"",400.0,406.4,158.8,69.9,"-",571.5,20.0,38.1,482.6,6.4,9.65,7.0,220.8,"M36",29.0,118.0]
[null,"WNRF 400# ANSI B16.47-MSS SP-44 Size 18\"","WNRF"," 400#","ANSI B16.47-MSS SP-44","18\"",450.0,457.2,171.5,72.9,"-",628.7,24.0,38.1,533.4,6.4,9.65,7.0,226.8,"M36",29.0,145.0]
[null,"WNRF 400# ANSI B16.47-MSS SP-44 Size 20\"","WNRF"," 400#","ANSI B16.47-MSS SP-44","20\"",500.0,508.0,174.5,76.3,"-",685.8,24.0,41.1,587.2,6.4,9.65,7.0,237.6,"M39",31.0,173.0]
[null,"WNRF 400# ANSI B16.47-MSS SP-44 Size 22\"","WNRF"," 400#","ANSI B16.47-MSS SP-44","22\"",550.0,558.8,177.9,79.6,"-",743.0,24.0,44.5,641.4,6.4,9.65,7.0,250.2,"M42",34.0,211.0]
[null,"WNRF 400# ANSI B16.47-MSS SP-44 Size 24\"","WNRF"," 400#","ANSI B16.47-MSS SP-44","24\"",600.0,609.6,181.2,82.6,"-",812.8,24.0,47.8,701.5,6.4,9.65,7.0,260.2,"M45",36.0,249.0]
[null,"WNRF 400# ANSI B16.47-MSS SP-44 Size 26\"","WNRF"," 400#","ANSI B16.47-MSS SP-44","26\"",650.0,660.4,199.9,95.3,749.3,876.3,28.0,47.8,726.9,6.4,9.65,7.0,285.6,"M45",36.0,304.0]
[null,"WNRF 400# ANSI B16.47-MSS SP-44 Size 28\"","WNRF"," 400#","ANSI B16.47-MSS SP-44","28\"",700.0,711.2,212.6,101.7,800.1,939.8,28.0,50.8,782.6,6.4,11.2,7.0,302.4,"M48",38.0,362.0]
[null,"WNRF 400# ANSI B16.47-MSS SP-44 Size 30\"","WNRF"," 400#","ANSI B16.47-MSS SP-44","30\"",750.0,762.0,225.3,108.0,857.2,997.0,28.0,53.8,836.7,6.4,11.2,7.0,315,"M48",38.0,415.0]
[null,"WNRF 400# ANSI B16.47-MSS SP-44 Size 32\"","WNRF"," 400#","ANSI B16.47-MSS SP-44","32\"",800.0,812.8,238.0,114.4,914.4,1054.1,28.0,53.8,889.0,6.4,11.2,7.0,327.8,"M48",38.0,478.0]
[null,"WNRF 400# ANSI B16.47-MSS SP-44 Size 34\"","WNRF"," 400#","ANSI B16.47-MSS SP-44","34\"",850.0,863.6,247.7,117.7,965.2,1104.9,28.0,53.8,944.6,6.4,12.7,7.0,334.4,"M48",38.0,538.0]
[null,"WNRF 400# ANSI B16.47-MSS SP-44 Size 36\"","WNRF"," 400#","ANSI B16.47-MSS SP-44","36\"",900.0,914.4,257.4,120.7,1022.3,1168.4,32.0,53.8,1000.3,6.4,12.7,7.0,340.4,"M48",38.0,604.0]
[null,"WNRF 400# ANSI B16.47-MSS SP-44 Size 38\"","WNRF"," 400#","ANSI B16.47-MSS SP-44","38\"",950.0,965.2,212.6,130.4,1035.0,1117.6,32.0,47.8,1000.3,6.4,12.7,7.0,355.8,"M45",36.0,406.0]
[null,"WNRF 400# ANSI B16.47-MSS SP-44 Size 40\"","WNRF"," 400#","ANSI B16.47-MSS SP-44","40\"",1000.0,1016.0,222.3,136.4,1092.2,1174.8,32.0,50.8,1054.1,6.4,12.7,7.0,371.8,"M48",38.0,473.0]
[null,"WNRF 400# ANSI B16.47-MSS SP-44 Size 42\"","WNRF"," 400#","ANSI B16.47-MSS SP-44","42\"",1050.0,1066.8,230.2,139.8,1143.0,1225.6,32.0,50.8,1107.9,6.4,12.7,7.0,378.6,"M48",38.0,513.0]
[null,"WNRF 400# ANSI B16.47-MSS SP-44 Size 44\"","WNRF"," 400#","ANSI B16.47-MSS SP-44","44\"",1100.0,1117.6,239.8,146.1,1200.1,1282.7,32.0,53.8,1158.7,6.4,12.7,7.0,391.2,"M48",38.0,586.0]
[null,"WNRF 400# ANSI B16.47-MSS SP-44 Size 46\"","WNRF"," 400#","ANSI B16.47-MSS SP-44","46\"",1150.0,1168.4,250.7,152.5,1257.3,1339.9,36.0,53.8,1212.9,6.4,12.7,7.0,404,"M48",38.0,648.0]
[null,"WNRF 400# ANSI B16.47-MSS SP-44 Size 48\"","WNRF"," 400#","ANSI B16.47-MSS SP-44","48\"",1200.0,1219.2,262.4,158.8,1308.1,1403.4,28.0,60.5,1267.0,6.4,12.7,7.0,430.6,"M56",45.0,768.0]
[null,"WNRF 400# ANSI B16.47-MSS SP-44 Size 50\"","WNRF"," 400#","ANSI B16.47-MSS SP-44","50\"",1250.0,1270.0,274.6,163.6,1362.0,1460.5,32.0,60.5,1320.8,6.4,12.7,7.0,440.2,"M56",45.0,832.0]
[null,"WNRF 400# ANSI B16.47-MSS SP-44 Size 52\"","WNRF"," 400#","ANSI B16.47-MSS SP-44","52\"",1300.0,1320.8,282.8,168.5,1412.8,1511.3,32.0,60.5,1371.6,6.4,12.7,7.0,450,"M56",45.0,897.0]
[null,"WNRF 400# ANSI B16.47-MSS SP-44 Size 54\"","WNRF"," 400#","ANSI B16.47-MSS SP-44","54\"",1350.0,1371.6,295.5,176.3,1470.0,1581.2,28.0,66.5,1425.4,6.4,12.7,7.0,477.6,"M64",51.0,1086.0]
[null,"WNRF 400# ANSI B16.47-MSS SP-44 Size 56\"","WNRF"," 400#","ANSI B16.47-MSS SP-44","56\"",1400.0,1422.4,304.9,181.2,1527.1,1632.0,32.0,66.5,1479.6,6.4,12.7,7.0,487.4,"M64",51.0,1139.0]
[null,"WNRF 400# ANSI B16.47-MSS SP-44 Size 58\"","WNRF"," 400#","ANSI B16.47-MSS SP-44","58\"",1450.0,1473.2,312.7,184.2,1577.9,1682.8,32.0,66.5,1530.4,6.4,12.7,7.0,493.4,"M64",51.0,1208.0]
[null,"WNRF 400# ANSI B16.47-MSS SP-44 Size 60\"","WNRF"," 400#","ANSI B16.47-MSS SP-44","60\"",1500.0,1524.0,325.4,192.1,1635.1,1752.6,32.0,73.2,1584.5,6.4,12.7,7.0,515.2,"M68",54.0,1408.0]
[null,"WNRF 600# ANSI B16.47-MSS SP-44 Size 12\"","WNRF"," 600#","ANSI B16.47-MSS SP-44","12\"",300.0,558.8,161.8,72.9,"-",489.0,20.0,35.1,400.1,6.4,9.7,6.0,219.8,"M33",26.0,103.0]
[null,"WNRF 600# ANSI B16.47-MSS SP-44 Size 14\"","WNRF"," 600#","ANSI B16.47-MSS SP-44","14\"",350.0,603.3,171.5,76.3,"-",527.1,20.0,38.1,431.8,6.4,9.7,7.0,233.6,"M36",29.0,122.0]
[null,"WNRF 600# ANSI B16.47-MSS SP-44 Size 16\"","WNRF"," 600#","ANSI B16.47-MSS SP-44","16\"",400.0,685.8,184.2,82.6,"-",603.3,20.0,41.1,495.3,6.4,9.7,7.0,250.2,"M39",31.0,170.0]
[null,"WNRF 600# ANSI B16.47-MSS SP-44 Size 18\"","WNRF"," 600#","ANSI B16.47-MSS SP-44","18\"",450.0,743.0,190.6,89.0,"-",654.1,20.0,44.5,546.1,6.4,9.7,7.0,269,"M42",34.0,204.0]
[null,"WNRF 600# ANSI B16.47-MSS SP-44 Size 20\"","WNRF"," 600#","ANSI B16.47-MSS SP-44","20\"",500.0,812.8,196.9,95.3,"-",723.9,24.0,44.5,609.6,6.4,9.7,7.0,281.6,"M42",34.0,254.0]
[null,"WNRF 600# ANSI B16.47-MSS SP-44 Size 22\"","WNRF"," 600#","ANSI B16.47-MSS SP-44","22\"",550.0,870.0,203.3,101.7,"-",777.7,24.0,47.8,666.8,6.4,9.7,7.0,298.4,"M45",36.0,306.0]
[null,"WNRF 600# ANSI B16.47-MSS SP-44 Size 24\"","WNRF"," 600#","ANSI B16.47-MSS SP-44","24\"",600.0,936.453333333334,213.726666666667,107.04,"-",837.653333333333,24.5333333333333,50.4599999999999,716.72,6.4,9.7,7.33333333333333,314.3466667,"M33",38.4666666666666,358.0]
[null,"WNRF 600# ANSI B16.47-MSS SP-44 Size 26\"","WNRF"," 600#","ANSI B16.47-MSS SP-44","26\"",650.0,1016.0,228.7,114.4,749.3,914.4,28.0,50.8,747.8,6.4,12.7,7.0,327.8,"M48",38.0,427.0]
[null,"WNRF 600# ANSI B16.47-MSS SP-44 Size 28\"","WNRF"," 600#","ANSI B16.47-MSS SP-44","28\"",700.0,1073.2,241.4,117.7,800.1,965.2,28.0,53.8,803.1,6.4,12.7,7.0,334.4,"M48",38.0,479.0]
[null,"WNRF 600# ANSI B16.47-MSS SP-44 Size 30\"","WNRF"," 600#","ANSI B16.47-MSS SP-44","30\"",750.0,1130.3,254.1,120.7,857.2,1022.4,28.0,53.8,862.1,6.4,12.7,7.0,340.4,"M48",38.0,545.0]
[null,"WNRF 600# ANSI B16.47-MSS SP-44 Size 32\"","WNRF"," 600#","ANSI B16.47-MSS SP-44","32\"",800.0,1193.8,266.8,123.7,914.4,1079.5,28.0,60.5,917.4,6.4,12.7,7.0,360.4,"M56",45.0,610.0]
[null,"WNRF 600# ANSI B16.47-MSS SP-44 Size 34\"","WNRF"," 600#","ANSI B16.47-MSS SP-44","34\"",850.0,1244.6,276.1,127.1,965.2,1130.3,28.0,60.5,973.1,6.4,14.2,7.0,367.2,"M56",45.0,666.0]
[null,"WNRF 600# ANSI B16.47-MSS SP-44 Size 36\"","WNRF"," 600#","ANSI B16.47-MSS SP-44","36\"",900.0,1314.5,288.8,130.4,1022.3,1193.8,28.0,66.5,1031.7,6.4,14.2,7.0,379.8,"M60",48.0,755.0]
[null,"WNRF 600# ANSI B16.47-MSS SP-44 Size 38\"","WNRF"," 600#","ANSI B16.47-MSS SP-44","38\"",950.0,1270.0,260.4,158.8,1054.1,1162.1,28.0,60.5,1022.4,6.4,14.2,7.0,430.6,"M56",45.0,640.0]
[null,"WNRF 600# ANSI B16.47-MSS SP-44 Size 40\"","WNRF"," 600#","ANSI B16.47-MSS SP-44","40\"",1000.0,1320.8,270.1,165.0,1111.2,1212.9,32.0,60.5,1073.2,6.4,14.2,7.0,443,"M56",45.0,683.0]
[null,"WNRF 600# ANSI B16.47-MSS SP-44 Size 42\"","WNRF"," 600#","ANSI B16.47-MSS SP-44","42\"",1050.0,1403.4,285.8,174.5,1168.4,1282.7,28.0,66.5,1127.3,6.4,14.2,7.0,468,"M60",48.0,754.0]
[null,"WNRF 600# ANSI B16.47-MSS SP-44 Size 44\"","WNRF"," 600#","ANSI B16.47-MSS SP-44","44\"",1100.0,1454.2,295.5,179.4,1225.5,1333.5,32.0,66.5,1181.1,6.4,14.2,7.0,477.8,"M60",48.0,903.0]
[null,"WNRF 600# ANSI B16.47-MSS SP-44 Size 46\"","WNRF"," 600#","ANSI B16.47-MSS SP-44","46\"",1150.0,1511.3,306.4,185.7,1273.3,1390.7,32.0,66.5,1234.9,6.4,14.2,7.0,490.4,"M60",48.0,1054.0]
[null,"WNRF 600# ANSI B16.47-MSS SP-44 Size 48\"","WNRF"," 600#","ANSI B16.47-MSS SP-44","48\"",1200.0,1593.9,321.1,195.4,1333.5,1460.5,32.0,73.2,1289.1,6.4,14.2,7.0,523.8,"M68",55.0,1200.0]
[null,"WNRF 600# ANSI B16.47-MSS SP-44 Size 50\"","WNRF"," 600#","ANSI B16.47-MSS SP-44","50\"",1250.0,1670.1,335.1,203.3,1384.3,1524.0,28.0,79.2,1343.2,6.4,14.2,7.0,549.6,"M75",60.0,1363.0]
[null,"WNRF 600# ANSI B16.47-MSS SP-44 Size 52\"","WNRF"," 600#","ANSI B16.47-MSS SP-44","52\"",1300.0,1720.9,343.0,209.6,1435.1,1574.8,32.0,79.2,1394.0,6.4,14.2,7.0,562.2,"M75",60.0,1466.0]
[null,"WNRF 600# ANSI B16.47-MSS SP-44 Size 54\"","WNRF"," 600#","ANSI B16.47-MSS SP-44","54\"",1350.0,1778.0,355.7,216.0,1492.2,1632.0,32.0,79.2,1447.8,6.4,14.2,7.0,575,"M75",60.0,1605.0]
[null,"WNRF 600# ANSI B16.47-MSS SP-44 Size 56\"","WNRF"," 600#","ANSI B16.47-MSS SP-44","56\"",1400.0,1854.2,368.4,223.8,1543.0,1695.5,32.0,85.9,1501.6,6.4,17.5,7.0,598.6,"M80",64.0,1709.0]
[null,"WNRF 600# ANSI B16.47-MSS SP-44 Size 58\"","WNRF"," 600#","ANSI B16.47-MSS SP-44","58\"",1450.0,1905.0,376.2,228.7,1600.2,1746.3,32.0,85.9,1552.4,6.4,17.5,7.0,608.4,"M80",64.0,1916.0]
[null,"WNRF 600# ANSI B16.47-MSS SP-44 Size 60\"","WNRF"," 600#","ANSI B16.47-MSS SP-44","60\"",1500.0,1993.9,395.3,239.8,1657.3,1822.5,28.0,91.9,1609.9,6.4,17.5,7.0,638.6,"M85",68.0,2300.0]
[null,"WNRF 900# ANSI B16.47-MSS SP-44 Size 12\"","WNRF"," 900#","ANSI B16.47-MSS SP-44","12\"",300.0,609.6,206.6,85.6,"-",533.4,20.0,38.1,419.1,6.4,11.2,7.0,252.2,"M36",29.0,157.0]
[null,"WNRF 900# ANSI B16.47-MSS SP-44 Size 14\"","WNRF"," 900#","ANSI B16.47-MSS SP-44","14\"",350.0,641.4,219.3,92.3,"-",558.8,20.0,41.1,450.9,6.4,11.2,7.0,269.6,"M39",31.0,180.0]
[null,"WNRF 900# ANSI B16.47-MSS SP-44 Size 16\"","WNRF"," 900#","ANSI B16.47-MSS SP-44","16\"",400.0,704.9,222.3,95.3,"-",616.0,20.0,44.5,508.0,6.4,11.2,7.0,281.6,"M42",34.0,217.0]
[null,"WNRF 900# ANSI B16.47-MSS SP-44 Size 18\"","WNRF"," 900#","ANSI B16.47-MSS SP-44","18\"",450.0,787.4,235.0,108.0,"-",685.8,20.0,50.8,585.2,6.4,11.2,7.0,315,"M48",38.0,292.0]
[null,"WNRF 900# ANSI B16.47-MSS SP-44 Size 20\"","WNRF"," 900#","ANSI B16.47-MSS SP-44","20\"",500.0,857.3,254.1,114.4,"-",749.3,20.0,53.8,622.3,6.4,11.2,7.0,327.8,"M48",38.0,362.0]
[null,"WNRF 900# ANSI B16.47-MSS SP-44 Size 24\"","WNRF"," 900#","ANSI B16.47-MSS SP-44","24\"",600.0,1041.4,298.5,146.1,"-",901.7,20.0,66.5,749.3,6.4,11.2,7.0,417.2,"M64",51.0,665.0]
[null,"WNRF 900# ANSI B16.47-MSS SP-44 Size 26\"","WNRF"," 900#","ANSI B16.47-MSS SP-44","26\"",650.0,1085.9,292.2,146.1,749.3,952.5,20.0,73.2,774.7,6.4,11.2,7.0,425.2,"M68",55.0,692.0]
[null,"WNRF 900# ANSI B16.47-MSS SP-44 Size 28\"","WNRF"," 900#","ANSI B16.47-MSS SP-44","28\"",700.0,1168.4,304.9,149.1,800.1,1022.4,20.0,79.2,831.9,6.4,12.7,7.0,443.2,"M76",61.0,822.0]
[null,"WNRF 900# ANSI B16.47-MSS SP-44 Size 30\"","WNRF"," 900#","ANSI B16.47-MSS SP-44","30\"",750.0,1231.9,317.6,155.8,857.2,1085.9,20.0,79.2,889.0,6.4,12.7,7.0,456.6,"M76",61.0,962.0]
[null,"WNRF 900# ANSI B16.47-MSS SP-44 Size 32\"","WNRF"," 900#","ANSI B16.47-MSS SP-44","32\"",800.0,1314.5,336.6,165.2,914.4,1155.7,20.0,85.9,946.2,6.4,12.7,7.0,481.4,"M80",64.0,1155.0]
[null,"WNRF 900# ANSI B16.47-MSS SP-44 Size 34\"","WNRF"," 900#","ANSI B16.47-MSS SP-44","34\"",850.0,1397.0,355.7,171.5,965.2,1225.6,20.0,91.9,1006.3,6.4,14.2,7.0,502,"M85",68.0,1348.0]
[null,"WNRF 900# ANSI B16.47-MSS SP-44 Size 36\"","WNRF"," 900#","ANSI B16.47-MSS SP-44","36\"",900.0,1460.5,368.4,177.9,1022.3,1289.1,20.0,91.9,1063.8,6.4,14.2,7.0,514.8,"M85",68.0,1541.0]
[null,"WNRF 900# ANSI B16.47-MSS SP-44 Size 38\"","WNRF"," 900#","ANSI B16.47-MSS SP-44","38\"",950.0,1460.5,359.0,196.9,1098.5,1289.1,20.0,91.9,1073.2,6.4,19.1,7.0,552.8,"M85",68.0,1537.0]
[null,"WNRF 900# ANSI B16.47-MSS SP-44 Size 40\"","WNRF"," 900#","ANSI B16.47-MSS SP-44","40\"",1000.0,1511.3,369.9,203.3,1162.0,1339.9,24.0,91.9,1127.3,6.4,20.6,7.0,565.6,"M85",68.0,1643.0]
[null,"WNRF 900# ANSI B16.47-MSS SP-44 Size 42\"","WNRF"," 900#","ANSI B16.47-MSS SP-44","42\"",1050.0,1562.1,377.7,212.6,1212.8,1390.7,24.0,91.9,1176.3,6.4,20.6,7.0,584.2,"M85",68.0,1798.0]
[null,"WNRF 900# ANSI B16.47-MSS SP-44 Size 44\"","WNRF"," 900#","ANSI B16.47-MSS SP-44","44\"",1100.0,1648.0,397.1,220.8,1270.0,1463.5,24.0,98.6,1234.9,6.4,22.4,7.0,616.6,"M95",76.0,1952.0]
[null,"WNRF 900# ANSI B16.47-MSS SP-44 Size 46\"","WNRF"," 900#","ANSI B16.47-MSS SP-44","46\"",1150.0,1733.6,417.4,232.0,1333.5,1536.7,24.0,104.6,1292.4,6.4,22.4,7.0,647,"M100",80.0,2107.0]
[null,"WNRF 900# ANSI B16.47-MSS SP-44 Size 48\"","WNRF"," 900#","ANSI B16.47-MSS SP-44","48\"",1200.0,1784.4,423.9,239.8,1384.3,1587.5,24.0,104.6,1343.2,6.4,23.8,7.0,662.6,"M100",80.0,2260.0]
[null,"WNRF 150# BS 3293 Size 26\"","WNRF"," 150#","BS 3293","26\"",650.0,870.0,127.0,50.8,743.0,806.5,24.0,34.9,723.9,1.6,"-",7.0,172.6,"M30",24.0,118.0]
[null,"WNRF 150# BS 3293 Size 28\"","WNRF"," 150#","BS 3293","28\"",700.0,927.1,128.6,52.4,793.8,863.6,28.0,34.9,781.1,1.6,"-",7.0,175.8,"M30",24.0,134.0]
[null,"WNRF 150# BS 3293 Size 30\"","WNRF"," 150#","BS 3293","30\"",750.0,984.3,130.2,54.0,857.3,914.4,28.0,34.9,831.9,1.6,"-",7.0,179,"M30",24.0,153.0]
[null,"WNRF 150# BS 3293 Size 32\"","WNRF"," 150#","BS 3293","32\"",800.0,1060.5,133.4,57.2,908.1,977.9,28.0,41.3,889.0,1.6,"-",7.0,195.4,"M39",29.0,190.0]
[null,"WNRF 150# BS 3293 Size 34\"","WNRF"," 150#","BS 3293","34\"",850.0,1111.3,135.0,58.8,958.8,1028.7,32.0,41.3,939.8,1.6,"-",7.0,198.6,"M39",29.0,212.0]
[null,"WNRF 150# BS 3293 Size 36\"","WNRF"," 150#","BS 3293","36\"",900.0,1168.4,136.5,60.3,1022.4,1085.9,32.0,41.3,997.0,1.6,"-",7.0,201.6,"M39",29.0,242.0]
[null,"WNRF 150# BS 3293 Size 38\"","WNRF"," 150#","BS 3293","38\"",950.0,1238.3,136.5,60.3,1073.2,1149.4,32.0,41.3,1060.5,1.6,"-",7.0,201.6,"M39",29.0,284.0]
[null,"WNRF 150# BS 3293 Size 40\"","WNRF"," 150#","BS 3293","40\"",1000.0,1289.1,139.7,63.5,1124.0,1200.2,36.0,41.3,1111.3,1.6,"-",7.0,208,"M39",29.0,311.0]
[null,"WNRF 150# BS 3293 Size 42\"","WNRF"," 150#","BS 3293","42\"",1050.0,1346.2,142.9,66.7,1193.8,1257.3,36.0,41.3,1168.4,1.6,"-",7.0,214.4,"M39",29.0,358.0]
[null,"WNRF 150# BS 3293 Size 44\"","WNRF"," 150#","BS 3293","44\"",1100.0,1403.4,142.9,66.7,1244.6,1314.5,40.0,41.3,1219.2,1.6,"-",7.0,214.4,"M39",29.0,376.0]
[null,"WNRF 150# BS 3293 Size 46\"","WNRF"," 150#","BS 3293","46\"",1150.0,1454.2,144.5,68.3,1295.4,1365.3,40.0,41.3,1270.0,1.6,"-",7.0,217.6,"M39",29.0,399.0]
[null,"WNRF 150# BS 3293 Size 48\"","WNRF"," 150#","BS 3293","48\"",1200.0,1511.3,146.1,69.9,1358.9,1422.4,44.0,41.3,1327.2,1.6,"-",7.0,220.8,"M39",29.0,440.0]
[null,"WNRF 300# BS 3293 Size 26\"","WNRF"," 300#","BS 3293","26\"",650.0,971.6,184.2,79.4,749.3,876.3,28.0,44.5,720.7,1.6,"-",7.0,249.8,"M42",34.0,279.0]
[null,"WNRF 300# BS 3293 Size 28\"","WNRF"," 300#","BS 3293","28\"",700.0,1035.1,196.9,85.7,800.1,939.8,28.0,44.5,774.7,1.6,"-",7.0,262.4,"M42",34.0,340.0]
[null,"WNRF 300# BS 3293 Size 30\"","WNRF"," 300#","BS 3293","30\"",750.0,1092.2,209.6,92.1,857.3,997.0,28.0,47.6,827.1,1.6,"-",7.0,279.2,"M45",36.0,390.0]
[null,"WNRF 300# BS 3293 Size 32\"","WNRF"," 300#","BS 3293","32\"",800.0,1149.4,222.3,98.4,914.4,1054.1,28.0,50.8,881.1,1.6,"-",7.0,295.8,"M48",38.0,435.0]
[null,"WNRF 300# BS 3293 Size 34\"","WNRF"," 300#","BS 3293","34\"",850.0,1206.5,231.8,101.6,965.2,1104.9,28.0,50.8,936.6,1.6,"-",7.0,302.2,"M48",38.0,504.0]
[null,"WNRF 300# BS 3293 Size 36\"","WNRF"," 300#","BS 3293","36\"",900.0,1270.0,241.3,104.8,1022.4,1168.4,32.0,54.0,990.6,1.6,"-",7.0,316.6,"M52",42.0,560.0]
[null,"WNRF 400# BS 3293 Size 26\"","WNRF"," 400#","BS 3293","26\"",650.0,971.6,200.1,95.3,749.3,876.3,28.0,47.6,727.1,6.4,"-",7.0,285.6,"M45",36.0,340.0]
[null,"WNRF 400# BS 3293 Size 28\"","WNRF"," 400#","BS 3293","28\"",700.0,1035.1,212.8,101.7,800.1,939.8,28.0,50.8,782.6,6.4,"-",7.0,302.4,"M48",38.0,399.0]
[null,"WNRF 400# BS 3293 Size 30\"","WNRF"," 400#","BS 3293","30\"",750.0,1092.2,225.5,108.0,857.3,997.0,28.0,54.0,836.6,6.4,"-",7.0,323,"M52",42.0,454.0]
[null,"WNRF 400# BS 3293 Size 32\"","WNRF"," 400#","BS 3293","32\"",800.0,1149.4,238.2,114.4,914.4,1054.1,28.0,54.0,889.0,6.4,"-",7.0,335.8,"M52",42.0,522.0]
[null,"WNRF 400# BS 3293 Size 34\"","WNRF"," 400#","BS 3293","34\"",850.0,1206.5,247.7,117.5,965.2,1104.9,28.0,54.0,944.6,6.4,"-",7.0,342,"M52",42.0,590.0]
[null,"WNRF 400# BS 3293 Size 36\"","WNRF"," 400#","BS 3293","36\"",900.0,1270.0,257.3,120.7,1022.4,1168.4,32.0,54.0,1000.1,6.4,"-",7.0,348.4,"M52",42.0,669.0]
[null,"WNRF 600# BS 3293 Size 26\"","WNRF"," 600#","BS 3293","26\"",650.0,1016.0,228.7,114.4,749.3,914.4,28.0,50.8,747.7,6.4,"-",7.0,327.8,"M48",38.0,437.0]
[null,"WNRF 600# BS 3293 Size 28\"","WNRF"," 600#","BS 3293","28\"",700.0,1073.2,241.4,117.5,800.1,965.2,28.0,54.0,803.3,6.4,"-",7.0,342,"M52",42.0,508.0]
[null,"WNRF 600# BS 3293 Size 30\"","WNRF"," 600#","BS 3293","30\"",750.0,1130.3,254.1,120.7,857.3,1022.4,28.0,54.0,862.0,6.4,"-",7.0,348.4,"M52",42.0,559.0]
[null,"WNRF 600# BS 3293 Size 32\"","WNRF"," 600#","BS 3293","32\"",800.0,1193.8,266.8,123.9,914.4,1079.5,28.0,60.3,917.6,6.4,"-",7.0,360.8,"M56",45.0,680.0]
[null,"WNRF 600# BS 3293 Size 34\"","WNRF"," 600#","BS 3293","34\"",850.0,1244.6,276.3,127.1,965.2,1130.3,28.0,60.3,973.1,6.4,"-",7.0,367.2,"M56",45.0,717.0]
[null,"WNRF 600# BS 3293 Size 36\"","WNRF"," 600#","BS 3293","36\"",900.0,1314.5,289.0,130.2,1022.4,1193.8,28.0,66.7,1031.9,6.4,"-",7.0,385.4,"M64",51.0,780.0]
[null,{"$f":"CONCATENATE(C648,$C$1,D648,$C$1,E648,$C$1,$F$1,$C$1,$G$2,$C$1,G648)","v":"WNRF PN 6 BS 4504 Size DN 10"},"WNRF","PN 6","BS 4504","1/4\"",10.0,75.0,28.0,12.0,35.0,50.0,4.0,11.0,26.0,2.0,4.0,3.0,59,"M10",8.0,0.3]
[null,"WNRF PN 6 BS 4504 Size DN 15","WNRF","PN 6","BS 4504","1/2\"",15.0,80.0,30.0,12.0,40.0,55.0,4.0,11.0,30.0,2.0,4.0,3.0,59,"M10",8.0,0.39]
[null,"WNRF PN 6 BS 4504 Size DN 20","WNRF","PN 6","BS 4504","3/4\"",20.0,90.0,32.0,14.0,50.0,65.0,4.0,11.0,38.0,2.0,4.0,3.0,63,"M10",8.0,0.59]
[null,"WNRF PN 6 BS 4504 Size DN 25","WNRF","PN 6","BS 4504","1\"",25.0,100.0,35.0,14.0,60.0,75.0,4.0,11.0,42.0,2.0,4.0,3.0,63,"M10",8.0,0.75]
[null,"WNRF PN 6 BS 4504 Size DN 32","WNRF","PN 6","BS 4504","1¼\"",32.0,120.0,35.0,14.0,70.0,90.0,4.0,14.0,55.0,2.0,6.0,3.0,67,"M12",10.0,1.05]
[null,"WNRF PN 6 BS 4504 Size DN 40","WNRF","PN 6","BS 4504","1½\"",40.0,130.0,38.0,14.0,80.0,100.0,4.0,14.0,62.0,3.0,6.0,3.0,67,"M12",10.0,1.18]
[null,"WNRF PN 6 BS 4504 Size DN 50","WNRF","PN 6","BS 4504","2\"",50.0,140.0,38.0,14.0,90.0,110.0,4.0,14.0,74.0,3.0,6.0,4.0,68,"M12",10.0,1.34]
[null,"WNRF PN 6 BS 4504 Size DN 65","WNRF","PN 6","BS 4504","2½\"",65.0,160.0,38.0,14.0,110.0,130.0,4.0,14.0,88.0,3.0,6.0,4.0,68,"M12",10.0,1.67]
[null,"WNRF PN 6 BS 4504 Size DN 80","WNRF","PN 6","BS 4504","3\"",80.0,190.0,42.0,16.0,128.0,150.0,4.0,18.0,102.0,3.0,8.0,4.0,78,"M16",13.0,2.71]
[null,"WNRF PN 6 BS 4504 Size DN 100","WNRF","PN 6","BS 4504","4\"",100.0,210.0,45.0,16.0,148.0,170.0,4.0,18.0,130.0,3.0,8.0,5.0,79,"M16",13.0,3.24]
[null,"WNRF PN 6 BS 4504 Size DN 125","WNRF","PN 6","BS 4504","5\"",125.0,240.0,48.0,18.0,178.0,200.0,8.0,18.0,155.0,3.0,8.0,5.0,83,"M16",13.0,4.49]
[null,"WNRF PN 6 BS 4504 Size DN 150","WNRF","PN 6","BS 4504","6\"",150.0,265.0,48.0,18.0,202.0,225.0,8.0,18.0,184.0,3.0,10.0,6.0,84,"M16",13.0,5.15]
[null,"WNRF PN 6 BS 4504 Size DN 200","WNRF","PN 6","BS 4504","8\"",200.0,320.0,55.0,20.0,258.0,280.0,8.0,18.0,236.0,3.0,10.0,6.0,88,"M16",13.0,7.78]
[null,"WNRF PN 6 BS 4504 Size DN 250","WNRF","PN 6","BS 4504","10\"",250.0,375.0,60.0,22.0,312.0,335.0,12.0,18.0,290.0,3.0,12.0,6.0,92,"M16",13.0,10.8]
[null,"WNRF PN 6 BS 4504 Size DN 300","WNRF","PN 6","BS 4504","12\"",300.0,440.0,62.0,22.0,365.0,395.0,12.0,22.0,342.0,4.0,12.0,6.0,98,"M20",16.0,14.0]
[null,"WNRF PN 6 BS 4504 Size DN 350","WNRF","PN 6","BS 4504","14\"",350.0,490.0,62.0,22.0,415.0,445.0,12.0,22.0,385.0,4.0,12.0,7.0,99,"M20",16.0,18.5]
[null,"WNRF PN 6 BS 4504 Size DN 400","WNRF","PN 6","BS 4504","16\"",400.0,540.0,65.0,22.0,465.0,495.0,16.0,22.0,438.0,4.0,12.0,7.0,99,"M20",16.0,21.2]
[null,"WNRF PN 6 BS 4504 Size DN 450","WNRF","PN 6","BS 4504","18\"",450.0,595.0,65.0,24.0,520.0,550.0,16.0,22.0,492.0,4.0,12.0,7.0,103,"M20",16.0,24.8]
[null,"WNRF PN 6 BS 4504 Size DN 500","WNRF","PN 6","BS 4504","20\"",500.0,645.0,68.0,24.0,570.0,600.0,20.0,22.0,538.0,4.0,12.0,7.0,103,"M20",16.0,28.6]
[null,"WNRF PN 6 BS 4504 Size DN 600","WNRF","PN 6","BS 4504","24\"",600.0,755.0,70.0,24.0,670.0,705.0,20.0,26.0,640.0,5.0,12.0,7.0,109,"M24",19.0,31.5]
[null,"WNRF PN 6 BS 4504 Size DN 700","WNRF","PN 6","BS 4504","28\"",700.0,860.0,70.0,24.0,775.0,810.0,24.0,26.0,740.0,5.0,12.0,7.0,109,"M24",19.0,37.4]
[null,"WNRF PN 6 BS 4504 Size DN 800","WNRF","PN 6","BS 4504","32\"",800.0,975.0,70.0,24.0,880.0,920.0,24.0,30.0,842.0,5.0,12.0,7.0,115,"M27",22.0,46.1]
[null,"WNRF PN 6 BS 4504 Size DN 900","WNRF","PN 6","BS 4504","36\"",900.0,1075.0,70.0,26.0,980.0,1020.0,24.0,30.0,942.0,5.0,12.0,7.0,119,"M27",22.0,55.6]
[null,"WNRF PN 6 BS 4504 Size DN 1000","WNRF","PN 6","BS 4504","40\"",1000.0,1175.0,70.0,26.0,1080.0,1120.0,28.0,30.0,1045.0,5.0,16.0,7.0,119,"M27",22.0,61.9]
[null,"WNRF PN 6 BS 4504 Size DN 1200","WNRF","PN 6","BS 4504","48\"",1200.0,1405.0,90.0,28.0,1295.0,1340.0,32.0,33.0,1248.0,5.0,16.0,7.0,127,"M30",24.0,100.0]
[null,"WNRF PN 6 BS 4504 Size DN 1400","WNRF","PN 6","BS 4504","56\"",1400.0,1630.0,90.0,32.0,1510.0,1560.0,36.0,36.0,1452.0,5.0,16.0,7.0,139,"M33",26.0,149.0]
[null,"WNRF PN 6 BS 4504 Size DN 1600","WNRF","PN 6","BS 4504","64\"",1600.0,1830.0,90.0,34.0,1710.0,1760.0,40.0,36.0,1655.0,5.0,16.0,7.0,143,"M33",26.0,180.0]
[null,"WNRF PN 6 BS 4504 Size DN 1800","WNRF","PN 6","BS 4504","72\"",1800.0,2045.0,100.0,36.0,1920.0,1970.0,44.0,39.0,1855.0,5.0,16.0,7.0,153,"M36",29.0,225.0]
[null,"WNRF PN 6 BS 4504 Size DN 2000","WNRF","PN 6","BS 4504","80\"",2000.0,2265.0,110.0,38.0,2125.0,2180.0,48.0,42.0,2058.0,5.0,16.0,7.0,161,"M39",31.0,295.0]
[null,"WNRF PN 10 BS 4504 Size DN 10","WNRF","PN 10","BS 4504","1/4\"",10.0,75.0,28.0,12.0,35.0,50.0,4.0,11.0,26.0,2.0,4.0,3.0,59,"M10",8.0,0.58]
[null,"WNRF PN 10 BS 4504 Size DN 15","WNRF","PN 10","BS 4504","1/2\"",15.0,95.0,35.0,14.0,45.0,65.0,4.0,14.0,32.0,2.0,4.0,3.0,67,"M12",10.0,0.648]
[null,"WNRF PN 10 BS 4504 Size DN 20","WNRF","PN 10","BS 4504","3/4\"",20.0,105.0,38.0,16.0,58.0,75.0,4.0,14.0,40.0,2.0,4.0,3.0,71,"M12",10.0,0.952]
[null,"WNRF PN 10 BS 4504 Size DN 25","WNRF","PN 10","BS 4504","1\"",25.0,115.0,38.0,16.0,68.0,85.0,4.0,14.0,45.0,2.0,4.0,3.0,71,"M12",10.0,1.14]
[null,"WNRF PN 10 BS 4504 Size DN 32","WNRF","PN 10","BS 4504","1¼\"",32.0,140.0,40.0,16.0,78.0,100.0,4.0,18.0,56.0,2.0,6.0,3.0,77,"M16",13.0,1.69]
[null,"WNRF PN 10 BS 4504 Size DN 40","WNRF","PN 10","BS 4504","1½\"",40.0,150.0,42.0,16.0,88.0,110.0,4.0,18.0,64.0,3.0,6.0,3.0,77,"M16",13.0,1.86]
[null,"WNRF PN 10 BS 4504 Size DN 50","WNRF","PN 10","BS 4504","2\"",50.0,165.0,45.0,18.0,102.0,125.0,4.0,18.0,75.0,3.0,6.0,4.0,82,"M16",13.0,2.53]
[null,"WNRF PN 10 BS 4504 Size DN 65","WNRF","PN 10","BS 4504","2½\"",65.0,185.0,45.0,18.0,122.0,145.0,4.0,18.0,90.0,3.0,6.0,4.0,82,"M16",13.0,3.06]
[null,"WNRF PN 10 BS 4504 Size DN 80","WNRF","PN 10","BS 4504","3\"",80.0,200.0,50.0,20.0,138.0,160.0,8.0,18.0,105.0,3.0,8.0,4.0,86,"M16",13.0,3.7]
[null,"WNRF PN 10 BS 4504 Size DN 100","WNRF","PN 10","BS 4504","4\"",100.0,220.0,52.0,20.0,158.0,180.0,8.0,18.0,131.0,3.0,8.0,5.0,87,"M16",13.0,4.62]
[null,"WNRF PN 10 BS 4504 Size DN 125","WNRF","PN 10","BS 4504","5\"",125.0,250.0,55.0,22.0,188.0,210.0,8.0,18.0,156.0,3.0,8.0,5.0,91,"M16",13.0,6.3]
[null,"WNRF PN 10 BS 4504 Size DN 150","WNRF","PN 10","BS 4504","6\"",150.0,285.0,55.0,22.0,212.0,240.0,8.0,22.0,184.0,3.0,10.0,6.0,98,"M20",16.0,7.75]
[null,"WNRF PN 10 BS 4504 Size DN 200","WNRF","PN 10","BS 4504","8\"",200.0,340.0,62.0,24.0,268.0,295.0,8.0,22.0,235.0,3.0,10.0,6.0,102,"M20",16.0,11.3]
[null,"WNRF PN 10 BS 4504 Size DN 250","WNRF","PN 10","BS 4504","10\"",250.0,395.0,68.0,26.0,320.0,350.0,12.0,22.0,292.0,3.0,12.0,6.0,106,"M20",16.0,14.7]
[null,"WNRF PN 10 BS 4504 Size DN 300","WNRF","PN 10","BS 4504","12\"",300.0,445.0,68.0,26.0,370.0,400.0,12.0,22.0,344.0,4.0,12.0,6.0,106,"M20",16.0,17.4]
[null,"WNRF PN 10 BS 4504 Size DN 350","WNRF","PN 10","BS 4504","14\"",350.0,505.0,68.0,26.0,430.0,460.0,16.0,22.0,385.0,4.0,12.0,7.0,107,"M20",16.0,23.6]
[null,"WNRF PN 10 BS 4504 Size DN 400","WNRF","PN 10","BS 4504","16\"",400.0,565.0,72.0,26.0,482.0,515.0,16.0,26.0,440.0,4.0,12.0,7.0,113,"M24",19.0,28.6]
[null,"WNRF PN 10 BS 4504 Size DN 450","WNRF","PN 10","BS 4504","18\"",450.0,615.0,72.0,28.0,532.0,565.0,20.0,26.0,492.0,4.0,12.0,7.0,117,"M24",19.0,33.4]
[null,"WNRF PN 10 BS 4504 Size DN 500","WNRF","PN 10","BS 4504","20\"",500.0,670.0,75.0,28.0,585.0,620.0,20.0,26.0,542.0,4.0,12.0,7.0,117,"M24",19.0,38.1]
[null,"WNRF PN 10 BS 4504 Size DN 600","WNRF","PN 10","BS 4504","24\"",600.0,780.0,80.0,28.0,685.0,725.0,20.0,30.0,642.0,5.0,12.0,7.0,123,"M27",22.0,44.6]
[null,"WNRF PN 10 BS 4504 Size DN 700","WNRF","PN 10","BS 4504","28\"",700.0,895.0,80.0,30.0,800.0,840.0,24.0,30.0,745.0,5.0,12.0,7.0,127,"M27",22.0,62.4]
[null,"WNRF PN 10 BS 4504 Size DN 800","WNRF","PN 10","BS 4504","32\"",800.0,1015.0,90.0,32.0,905.0,950.0,24.0,33.0,850.0,5.0,12.0,7.0,135,"M30",24.0,84.1]
[null,"WNRF PN 10 BS 4504 Size DN 900","WNRF","PN 10","BS 4504","36\"",900.0,1115.0,95.0,34.0,1005.0,1050.0,28.0,33.0,950.0,5.0,12.0,7.0,139,"M30",24.0,98.5]
[null,"WNRF PN 10 BS 4504 Size DN 1000","WNRF","PN 10","BS 4504","40\"",1000.0,1230.0,95.0,34.0,1110.0,1160.0,28.0,36.0,1052.0,5.0,16.0,7.0,143,"M33",26.0,115.0]
[null,"WNRF PN 10 BS 4504 Size DN 1200","WNRF","PN 10","BS 4504","48\"",1200.0,1455.0,115.0,38.0,1330.0,1380.0,32.0,39.0,1255.0,5.0,16.0,7.0,157,"M36",29.0,182.0]
[null,"WNRF PN 10 BS 4504 Size DN 1400","WNRF","PN 10","BS 4504","56\"",1400.0,1675.0,120.0,42.0,1535.0,1590.0,36.0,42.0,1460.0,5.0,16.0,7.0,169,"M39",31.0,248.0]
[null,"WNRF PN 10 BS 4504 Size DN 1600","WNRF","PN 10","BS 4504","64\"",1600.0,1915.0,130.0,46.0,1760.0,1820.0,40.0,48.0,1665.0,5.0,16.0,7.0,187,"M45",36.0,347.0]
[null,"WNRF PN 10 BS 4504 Size DN 1800","WNRF","PN 10","BS 4504","72\"",1800.0,2115.0,140.0,50.0,1960.0,2020.0,44.0,48.0,1868.0,5.0,16.0,7.0,195,"M45",36.0,430.0]
[null,"WNRF PN 10 BS 4504 Size DN 2000","WNRF","PN 10","BS 4504","80\"",2000.0,2325.0,150.0,54.0,2170.0,2230.0,48.0,48.0,2072.0,5.0,16.0,7.0,203,"M45",36.0,539.0]
[null,"WNRF PN 16 BS 4504 Size DN 10","WNRF","PN 16","BS 4504","1/4\"",10.0,90.0,35.0,14.0,40.0,60.0,4.0,14.0,28.0,2.0,4.0,3.0,67,"M12",10.0,0.58]
[null,"WNRF PN 16 BS 4504 Size DN 15","WNRF","PN 16","BS 4504","1/2\"",15.0,95.0,35.0,14.0,45.0,65.0,4.0,14.0,32.0,2.0,4.0,3.0,67,"M12",10.0,0.648]
[null,"WNRF PN 16 BS 4504 Size DN 20","WNRF","PN 16","BS 4504","3/4\"",20.0,105.0,38.0,16.0,58.0,75.0,4.0,14.0,40.0,2.0,4.0,3.0,71,"M12",10.0,0.952]
[null,"WNRF PN 16 BS 4504 Size DN 25","WNRF","PN 16","BS 4504","1\"",25.0,115.0,38.0,16.0,68.0,85.0,4.0,14.0,45.0,2.0,4.0,3.0,71,"M12",10.0,1.14]
[null,"WNRF PN 16 BS 4504 Size DN 32","WNRF","PN 16","BS 4504","1¼\"",32.0,140.0,40.0,16.0,78.0,100.0,4.0,18.0,56.0,2.0,6.0,3.0,77,"M16",13.0,1.69]
[null,"WNRF PN 16 BS 4504 Size DN 40","WNRF","PN 16","BS 4504","1½\"",40.0,150.0,42.0,16.0,88.0,110.0,4.0,18.0,64.0,3.0,6.0,3.0,77,"M16",13.0,1.86]
[null,"WNRF PN 16 BS 4504 Size DN 50","WNRF","PN 16","BS 4504","2\"",50.0,165.0,45.0,18.0,102.0,125.0,4.0,18.0,75.0,3.0,6.0,4.0,82,"M16",13.0,2.53]
[null,"WNRF PN 16 BS 4504 Size DN 65","WNRF","PN 16","BS 4504","2½\"",65.0,185.0,45.0,18.0,122.0,145.0,4.0,18.0,90.0,3.0,6.0,4.0,82,"M16",13.0,3.06]
[null,"WNRF PN 16 BS 4504 Size DN 80","WNRF","PN 16","BS 4504","3\"",80.0,200.0,50.0,20.0,138.0,160.0,8.0,18.0,105.0,3.0,8.0,4.0,86,"M16",13.0,3.7]
[null,"WNRF PN 16 BS 4504 Size DN 100","WNRF","PN 16","BS 4504","4\"",100.0,220.0,52.0,20.0,158.0,180.0,8.0,18.0,131.0,3.0,8.0,5.0,87,"M16",13.0,4.62]
[null,"WNRF PN 16 BS 4504 Size DN 125","WNRF","PN 16","BS 4504","5\"",125.0,250.0,55.0,22.0,188.0,210.0,8.0,18.0,156.0,3.0,8.0,5.0,91,"M16",13.0,6.3]
[null,"WNRF PN 16 BS 4504 Size DN 150","WNRF","PN 16","BS 4504","6\"",150.0,285.0,55.0,22.0,212.0,240.0,8.0,22.0,184.0,3.0,10.0,6.0,98,"M20",16.0,7.75]
[null,"WNRF PN 16 BS 4504 Size DN 200","WNRF","PN 16","BS 4504","8\"",200.0,315.0,60.0,24.0,242.0,270.0,8.0,22.0,210.0,3.0,10.0,6.0,102,"M20",16.0,9.85]
[null,"WNRF PN 16 BS 4504 Size DN 250","WNRF","PN 16","BS 4504","10\"",250.0,340.0,62.0,24.0,268.0,295.0,12.0,22.0,235.0,3.0,10.0,6.0,102,"M20",16.0,11.0]
[null,"WNRF PN 16 BS 4504 Size DN 300","WNRF","PN 16","BS 4504","12\"",300.0,405.0,70.0,26.0,320.0,355.0,12.0,26.0,292.0,3.0,12.0,6.0,112,"M24",19.0,15.6]
[null,"WNRF PN 16 BS 4504 Size DN 350","WNRF","PN 16","BS 4504","14\"",350.0,460.0,78.0,28.0,378.0,410.0,12.0,26.0,344.0,4.0,12.0,6.0,116,"M24",19.0,22.0]
[null,"WNRF PN 16 BS 4504 Size DN 400","WNRF","PN 16","BS 4504","16\"",400.0,520.0,82.0,30.0,438.0,470.0,16.0,26.0,390.0,4.0,12.0,7.0,121,"M24",19.0,31.2]
[null,"WNRF PN 16 BS 4504 Size DN 450","WNRF","PN 16","BS 4504","18\"",450.0,580.0,85.0,32.0,490.0,525.0,16.0,30.0,445.0,4.0,12.0,7.0,131,"M27",22.0,39.3]
[null,"WNRF PN 16 BS 4504 Size DN 500","WNRF","PN 16","BS 4504","20\"",500.0,715.0,90.0,34.0,610.0,650.0,20.0,33.0,548.0,4.0,12.0,7.0,139,"M30",24.0,61.0]
[null,"WNRF PN 16 BS 4504 Size DN 600","WNRF","PN 16","BS 4504","24\"",600.0,840.0,95.0,36.0,725.0,770.0,20.0,36.0,652.0,5.0,12.0,7.0,147,"M33",26.0,75.4]
[null,"WNRF PN 16 BS 4504 Size DN 700","WNRF","PN 16","BS 4504","28\"",700.0,910.0,100.0,36.0,795.0,840.0,24.0,36.0,755.0,5.0,12.0,7.0,147,"M33",26.0,77.0]
[null,"WNRF PN 16 BS 4504 Size DN 800","WNRF","PN 16","BS 4504","32\"",800.0,1025.0,105.0,38.0,900.0,950.0,24.0,39.0,855.0,5.0,12.0,7.0,157,"M36",29.0,101.0]
[null,"WNRF PN 16 BS 4504 Size DN 900","WNRF","PN 16","BS 4504","36\"",900.0,1125.0,110.0,40.0,1000.0,1050.0,28.0,39.0,955.0,5.0,12.0,7.0,161,"M36",29.0,122.0]
[null,"WNRF PN 16 BS 4504 Size DN 1000","WNRF","PN 16","BS 4504","40\"",1000.0,1255.0,120.0,42.0,1115.0,1170.0,28.0,42.0,1058.0,5.0,16.0,7.0,169,"M39",31.0,162.0]
[null,"WNRF PN 16 BS 4504 Size DN 1200","WNRF","PN 16","BS 4504","48\"",1200.0,1485.0,130.0,48.0,1330.0,1390.0,32.0,48.0,1262.0,5.0,16.0,7.0,191,"M45",36.0,243.0]
[null,"WNRF PN 16 BS 4504 Size DN 1400","WNRF","PN 16","BS 4504","56\"",1400.0,1685.0,145.0,52.0,1530.0,1590.0,36.0,48.0,1465.0,5.0,16.0,7.0,199,"M45",36.0,323.0]
[null,"WNRF PN 16 BS 4504 Size DN 1600","WNRF","PN 16","BS 4504","64\"",1600.0,1930.0,160.0,58.0,1750.0,1820.0,40.0,56.0,1668.0,5.0,16.0,7.0,223,"M52",42.0,479.0]
[null,"WNRF PN 16 BS 4504 Size DN 1800","WNRF","PN 16","BS 4504","72\"",1800.0,2130.0,170.0,62.0,1950.0,2020.0,44.0,56.0,1870.0,5.0,16.0,7.0,231,"M52",42.0,599.0]
[null,"WNRF PN 16 BS 4504 Size DN 2000","WNRF","PN 16","BS 4504","80\"",2000.0,2345.0,180.0,66.0,2150.0,2230.0,48.0,62.0,2072.0,5.0,16.0,7.0,245,"M56",45.0,719.0]
[null,"WNRF PN 25 BS 4504 Size DN 10","WNRF","PN 25","BS 4504","1/4\"",10.0,90.0,35.0,16.0,40.0,60.0,4.0,14.0,28.0,2.0,4.0,3.0,71,"M12",10.0,0.661]
[null,"WNRF PN 25 BS 4504 Size DN 15","WNRF","PN 25","BS 4504","1/2\"",15.0,95.0,38.0,16.0,45.0,65.0,4.0,14.0,32.0,2.0,4.0,3.0,71,"M12",10.0,0.746]
[null,"WNRF PN 25 BS 4504 Size DN 20","WNRF","PN 25","BS 4504","3/4\"",20.0,105.0,40.0,18.0,58.0,75.0,4.0,14.0,40.0,2.0,4.0,3.0,75,"M12",10.0,1.06]
[null,"WNRF PN 25 BS 4504 Size DN 25","WNRF","PN 25","BS 4504","1\"",25.0,115.0,40.0,18.0,68.0,85.0,4.0,14.0,46.0,2.0,4.0,3.0,75,"M12",10.0,1.29]
[null,"WNRF PN 25 BS 4504 Size DN 32","WNRF","PN 25","BS 4504","1¼\"",32.0,140.0,42.0,18.0,78.0,100.0,4.0,18.0,56.0,2.0,6.0,3.0,81,"M16",13.0,1.88]
[null,"WNRF PN 25 BS 4504 Size DN 40","WNRF","PN 25","BS 4504","1½\"",40.0,150.0,45.0,18.0,88.0,110.0,4.0,18.0,64.0,3.0,6.0,3.0,81,"M16",13.0,2.33]
[null,"WNRF PN 25 BS 4504 Size DN 50","WNRF","PN 25","BS 4504","2\"",50.0,165.0,48.0,20.0,102.0,125.0,4.0,18.0,75.0,3.0,6.0,4.0,86,"M16",13.0,2.82]
[null,"WNRF PN 25 BS 4504 Size DN 65","WNRF","PN 25","BS 4504","2½\"",65.0,185.0,52.0,22.0,122.0,145.0,8.0,18.0,90.0,3.0,6.0,4.0,90,"M16",13.0,3.74]
[null,"WNRF PN 25 BS 4504 Size DN 80","WNRF","PN 25","BS 4504","3\"",80.0,200.0,58.0,24.0,138.0,160.0,8.0,18.0,105.0,3.0,8.0,4.0,94,"M16",13.0,4.75]
[null,"WNRF PN 25 BS 4504 Size DN 100","WNRF","PN 25","BS 4504","4\"",100.0,235.0,65.0,24.0,162.0,190.0,8.0,22.0,134.0,3.0,8.0,5.0,101,"M20",16.0,6.52]
[null,"WNRF PN 25 BS 4504 Size DN 125","WNRF","PN 25","BS 4504","5\"",125.0,270.0,68.0,26.0,188.0,220.0,8.0,26.0,162.0,3.0,8.0,5.0,111,"M24",19.0,9.07]
[null,"WNRF PN 25 BS 4504 Size DN 150","WNRF","PN 25","BS 4504","6\"",150.0,300.0,75.0,28.0,218.0,250.0,8.0,26.0,192.0,3.0,10.0,6.0,116,"M24",19.0,11.8]
[null,"WNRF PN 25 BS 4504 Size DN 200","WNRF","PN 25","BS 4504","8\"",200.0,360.0,80.0,30.0,278.0,310.0,12.0,26.0,244.0,3.0,10.0,6.0,120,"M24",19.0,17.0]
[null,"WNRF PN 25 BS 4504 Size DN 250","WNRF","PN 25","BS 4504","10\"",250.0,425.0,88.0,32.0,335.0,370.0,12.0,30.0,298.0,3.0,12.0,6.0,130,"M27",22.0,24.4]
[null,"WNRF PN 25 BS 4504 Size DN 300","WNRF","PN 25","BS 4504","12\"",300.0,485.0,92.0,34.0,395.0,430.0,16.0,30.0,352.0,4.0,12.0,6.0,134,"M27",22.0,31.2]
[null,"WNRF PN 25 BS 4504 Size DN 350","WNRF","PN 25","BS 4504","14\"",350.0,555.0,100.0,38.0,450.0,490.0,16.0,33.0,398.0,4.0,12.0,7.0,147,"M30",24.0,47.2]
[null,"WNRF PN 25 BS 4504 Size DN 400","WNRF","PN 25","BS 4504","16\"",400.0,620.0,110.0,40.0,505.0,550.0,16.0,36.0,452.0,4.0,12.0,7.0,155,"M33",26.0,61.7]
[null,"WNRF PN 25 BS 4504 Size DN 500","WNRF","PN 25","BS 4504","20\"",500.0,730.0,125.0,44.0,615.0,660.0,20.0,36.0,558.0,4.0,12.0,7.0,163,"M33",26.0,89.6]
[null,"WNRF PN 25 BS 4504 Size DN 600","WNRF","PN 25","BS 4504","24\"",600.0,845.0,125.0,46.0,720.0,770.0,20.0,39.0,660.0,5.0,12.0,7.0,173,"M36",29.0,104.0]
[null,"WNRF PN 25 BS 4504 Size DN 700","WNRF","PN 25","BS 4504","28\"",700.0,960.0,125.0,46.0,820.0,875.0,24.0,42.0,760.0,5.0,12.0,7.0,177,"M39",31.0,136.0]
[null,"WNRF PN 25 BS 4504 Size DN 800","WNRF","PN 25","BS 4504","32\"",800.0,1085.0,135.0,50.0,930.0,990.0,24.0,48.0,865.0,5.0,12.0,7.0,195,"M45",36.0,186.0]
[null,"WNRF PN 25 BS 4504 Size DN 900","WNRF","PN 25","BS 4504","36\"",900.0,1185.0,145.0,54.0,1030.0,1090.0,28.0,48.0,968.0,5.0,12.0,7.0,203,"M45",36.0,236.0]
[null,"WNRF PN 25 BS 4504 Size DN 1000","WNRF","PN 25","BS 4504","40\"",1000.0,1320.0,155.0,58.0,1140.0,1210.0,28.0,56.0,1070.0,5.0,16.0,7.0,223,"M52",42.0,307.0]
[null,"WNRF PN 40 BS 4504 Size DN 10","WNRF","PN 40","BS 4504","1/4\"",10.0,90.0,35.0,16.0,40.0,60.0,4.0,14.0,28.0,2.0,4.0,3.0,71,"M12",10.0,0.661]
[null,"WNRF PN 40 BS 4504 Size DN 15","WNRF","PN 40","BS 4504","1/2\"",15.0,95.0,38.0,16.0,45.0,65.0,4.0,14.0,32.0,2.0,4.0,3.0,71,"M12",10.0,0.746]
[null,"WNRF PN 40 BS 4504 Size DN 20","WNRF","PN 40","BS 4504","3/4\"",20.0,105.0,40.0,18.0,58.0,75.0,4.0,14.0,40.0,2.0,4.0,3.0,75,"M12",10.0,1.06]
[null,"WNRF PN 40 BS 4504 Size DN 25","WNRF","PN 40","BS 4504","1\"",25.0,115.0,40.0,18.0,68.0,85.0,4.0,14.0,46.0,2.0,4.0,3.0,75,"M12",10.0,1.29]
[null,"WNRF PN 40 BS 4504 Size DN 32","WNRF","PN 40","BS 4504","1¼\"",32.0,140.0,42.0,18.0,78.0,100.0,4.0,18.0,56.0,2.0,6.0,3.0,81,"M16",13.0,1.88]
[null,"WNRF PN 40 BS 4504 Size DN 40","WNRF","PN 40","BS 4504","1½\"",40.0,150.0,45.0,18.0,88.0,110.0,4.0,18.0,64.0,3.0,6.0,3.0,81,"M16",13.0,2.33]
[null,"WNRF PN 40 BS 4504 Size DN 50","WNRF","PN 40","BS 4504","2\"",50.0,165.0,48.0,20.0,102.0,125.0,4.0,18.0,75.0,3.0,6.0,4.0,86,"M16",13.0,2.82]
[null,"WNRF PN 40 BS 4504 Size DN 65","WNRF","PN 40","BS 4504","2½\"",65.0,185.0,52.0,22.0,122.0,145.0,8.0,18.0,90.0,3.0,6.0,4.0,90,"M16",13.0,3.74]
[null,"WNRF PN 40 BS 4504 Size DN 80","WNRF","PN 40","BS 4504","3\"",80.0,200.0,58.0,24.0,138.0,160.0,8.0,18.0,105.0,3.0,8.0,4.0,94,"M16",13.0,4.75]
[null,"WNRF PN 40 BS 4504 Size DN 100","WNRF","PN 40","BS 4504","4\"",100.0,235.0,65.0,24.0,162.0,190.0,8.0,22.0,134.0,3.0,8.0,5.0,101,"M20",16.0,6.52]
[null,"WNRF PN 40 BS 4504 Size DN 125","WNRF","PN 40","BS 4504","5\"",125.0,270.0,68.0,26.0,188.0,220.0,8.0,26.0,162.0,3.0,8.0,5.0,111,"M24",19.0,9.07]
[null,"WNRF PN 40 BS 4504 Size DN 150","WNRF","PN 40","BS 4504","6\"",150.0,300.0,75.0,28.0,218.0,250.0,8.0,26.0,192.0,3.0,10.0,6.0,116,"M24",19.0,11.8]
[null,"WNRF PN 40 BS 4504 Size DN 200","WNRF","PN 40","BS 4504","8\"",200.0,375.0,88.0,34.0,285.0,320.0,12.0,30.0,244.0,3.0,10.0,6.0,134,"M27",22.0,21.5]
[null,"WNRF PN 40 BS 4504 Size DN 250","WNRF","PN 40","BS 4504","10\"",250.0,450.0,105.0,38.0,345.0,385.0,12.0,33.0,306.0,3.0,12.0,6.0,146,"M30",24.0,34.9]
[null,"WNRF PN 40 BS 4504 Size DN 300","WNRF","PN 40","BS 4504","12\"",300.0,515.0,115.0,42.0,410.0,450.0,16.0,33.0,362.0,4.0,12.0,6.0,154,"M30",24.0,49.7]
[null,"WNRF PN 40 BS 4504 Size DN 350","WNRF","PN 40","BS 4504","14\"",350.0,580.0,125.0,46.0,465.0,510.0,16.0,36.0,408.0,4.0,12.0,7.0,167,"M33",26.0,68.1]
[null,"WNRF PN 40 BS 4504 Size DN 400","WNRF","PN 40","BS 4504","16\"",400.0,660.0,135.0,50.0,535.0,585.0,16.0,39.0,462.0,4.0,12.0,7.0,181,"M36",29.0,96.5]
[null,"WNRF PN 40 BS 4504 Size DN 450","WNRF","PN 40","BS 4504","18\"",450.0,685.0,135.0,50.0,560.0,610.0,20.0,39.0,500.0,4.0,12.0,7.0,181,"M36",29.0,108.0]
[null,"WNRF PN 40 BS 4504 Size DN 500","WNRF","PN 40","BS 4504","20\"",500.0,755.0,140.0,52.0,615.0,670.0,20.0,42.0,562.0,4.0,12.0,7.0,189,"M39",31.0,117.0]
[null,"WNRF PN 40 BS 4504 Size DN 600","WNRF","PN 40","BS 4504","24\"",600.0,890.0,"-",60.0,735.0,795.0,20.0,48.0,"-",5.0,12.0,7.0,215,"M45",36.0,"-"]
[null,"WNRF PN 64 BS 4504 Size DN 10","WNRF","PN 64","BS 4504","1/4\"",10.0,100.0,45.0,20.0,40.0,70.0,4.0,14.0,32.0,2.0,4.0,3.0,79,"M12",10.0,1.09]
[null,"WNRF PN 64 BS 4504 Size DN 15","WNRF","PN 64","BS 4504","1/2\"",15.0,105.0,45.0,20.0,45.0,75.0,4.0,14.0,34.0,2.0,4.0,3.0,79,"M12",10.0,1.19]
[null,"WNRF PN 64 BS 4504 Size DN 20","WNRF","PN 64","BS 4504","3/4\"",20.0,130.0,"-",22.0,58.0,90.0,4.0,18.0,"-",2.0,4.0,3.0,89,"M16",13.0,"-"]
[null,"WNRF PN 64 BS 4504 Size DN 25","WNRF","PN 64","BS 4504","1\"",25.0,140.0,58.0,24.0,68.0,100.0,4.0,18.0,52.0,2.0,4.0,3.0,93,"M16",13.0,2.66]
[null,"WNRF PN 64 BS 4504 Size DN 32","WNRF","PN 64","BS 4504","1¼\"",32.0,155.0,"-",26.0,78.0,110.0,4.0,22.0,"-",2.0,4.0,3.0,103,"M20",16.0,"-"]
[null,"WNRF PN 64 BS 4504 Size DN 40","WNRF","PN 64","BS 4504","1½\"",40.0,170.0,62.0,26.0,88.0,125.0,4.0,22.0,70.0,3.0,6.0,3.0,103,"M20",16.0,4.09]
[null,"WNRF PN 64 BS 4504 Size DN 50","WNRF","PN 64","BS 4504","2\"",50.0,180.0,62.0,26.0,102.0,135.0,4.0,22.0,82.0,3.0,6.0,4.0,104,"M20",16.0,4.55]
[null,"WNRF PN 64 BS 4504 Size DN 65","WNRF","PN 64","BS 4504","2½\"",65.0,205.0,68.0,26.0,122.0,160.0,8.0,22.0,98.0,3.0,6.0,4.0,104,"M20",16.0,5.73]
[null,"WNRF PN 64 BS 4504 Size DN 80","WNRF","PN 64","BS 4504","3\"",80.0,215.0,72.0,28.0,138.0,170.0,8.0,22.0,112.0,3.0,8.0,4.0,108,"M20",16.0,6.69]
[null,"WNRF PN 64 BS 4504 Size DN 100","WNRF","PN 64","BS 4504","4\"",100.0,250.0,78.0,30.0,162.0,200.0,8.0,26.0,138.0,3.0,8.0,5.0,119,"M24",19.0,9.66]
[null,"WNRF PN 64 BS 4504 Size DN 125","WNRF","PN 64","BS 4504","5\"",125.0,295.0,88.0,34.0,188.0,240.0,8.0,30.0,168.0,3.0,8.0,5.0,133,"M27",22.0,15.1]
[null,"WNRF PN 64 BS 4504 Size DN 150","WNRF","PN 64","BS 4504","6\"",150.0,345.0,95.0,36.0,218.0,280.0,8.0,33.0,202.0,3.0,10.0,6.0,142,"M30",24.0,21.9]
[null,"WNRF PN 64 BS 4504 Size DN 175","WNRF","PN 64","BS 4504","7\"",175.0,375.0,105.0,40.0,260.0,310.0,12.0,33.0,228.0,3.0,10.0,6.0,150,"M30",24.0,23.7]
[null,"WNRF PN 64 BS 4504 Size DN 200","WNRF","PN 64","BS 4504","8\"",200.0,415.0,110.0,42.0,285.0,345.0,12.0,36.0,256.0,3.0,10.0,6.0,158,"M33",26.0,34.9]
[null,"WNRF PN 64 BS 4504 Size DN 250","WNRF","PN 64","BS 4504","10\"",250.0,470.0,125.0,46.0,345.0,400.0,12.0,36.0,316.0,3.0,12.0,6.0,166,"M33",26.0,49.6]
[null,"WNRF PN 64 BS 4504 Size DN 300","WNRF","PN 64","BS 4504","12\"",300.0,530.0,140.0,52.0,410.0,460.0,16.0,36.0,372.0,4.0,12.0,6.0,178,"M33",26.0,68.7]
[null,"WNRF PN 64 BS 4504 Size DN 350","WNRF","PN 64","BS 4504","14\"",350.0,600.0,150.0,56.0,465.0,525.0,16.0,39.0,420.0,4.0,12.0,7.0,193,"M36",29.0,94.6]
[null,"WNRF PN 64 BS 4504 Size DN 400","WNRF","PN 64","BS 4504","16\"",400.0,670.0,160.0,60.0,535.0,585.0,16.0,42.0,475.0,4.0,12.0,7.0,205,"M39",31.0,124.0]
[null,"WNRF PN 64 BS 4504 Size DN 500","WNRF","PN 64","BS 4504","20\"",500.0,800.0,"-",68.0,615.0,705.0,20.0,48.0,"-",4.0,12.0,7.0,231,"M45",36.0,"-"]
[null,"WNRF PN 64 BS 4504 Size DN 600","WNRF","PN 64","BS 4504","24\"",600.0,930.0,"-",76.0,735.0,820.0,20.0,56.0,"-",4.0,12.0,7.0,259,"M52",42.0,"-"]
[null,"WNRF PN 100 BS 4504 Size DN 10","WNRF","PN 100","BS 4504","1/4\"",10.0,100.0,45.0,20.0,40.0,70.0,4.0,14.0,32.0,2.0,4.0,3.0,79,"M12",10.0,1.09]
[null,"WNRF PN 100 BS 4504 Size DN 15","WNRF","PN 100","BS 4504","1/2\"",15.0,105.0,45.0,20.0,45.0,75.0,4.0,14.0,34.0,2.0,4.0,3.0,79,"M12",10.0,1.2]
[null,"WNRF PN 100 BS 4504 Size DN 20","WNRF","PN 100","BS 4504","3/4\"",20.0,130.0,"-",22.0,58.0,90.0,4.0,18.0,"-",2.0,4.0,3.0,89,"M16",13.0,"-"]
[null,"WNRF PN 100 BS 4504 Size DN 25","WNRF","PN 100","BS 4504","1\"",25.0,140.0,58.0,24.0,68.0,100.0,4.0,18.0,52.0,2.0,4.0,3.0,93,"M16",13.0,2.66]
[null,"WNRF PN 100 BS 4504 Size DN 32","WNRF","PN 100","BS 4504","1¼\"",32.0,155.0,"-",26.0,78.0,110.0,4.0,22.0,"-",2.0,4.0,3.0,103,"M20",16.0,"-"]
[null,"WNRF PN 100 BS 4504 Size DN 40","WNRF","PN 100","BS 4504","1½\"",40.0,170.0,62.0,26.0,88.0,125.0,4.0,22.0,70.0,3.0,6.0,3.0,103,"M20",16.0,4.3]
[null,"WNRF PN 100 BS 4504 Size DN 50","WNRF","PN 100","BS 4504","2\"",50.0,195.0,68.0,28.0,102.0,145.0,4.0,26.0,90.0,3.0,6.0,4.0,114,"M24",19.0,6.25]
[null,"WNRF PN 100 BS 4504 Size DN 65","WNRF","PN 100","BS 4504","2½\"",65.0,220.0,76.0,30.0,122.0,170.0,8.0,26.0,108.0,3.0,6.0,4.0,118,"M24",19.0,7.91]
[null,"WNRF PN 100 BS 4504 Size DN 80","WNRF","PN 100","BS 4504","3\"",80.0,230.0,78.0,32.0,138.0,180.0,8.0,26.0,120.0,3.0,8.0,4.0,122,"M24",19.0,8.95]
[null,"WNRF PN 100 BS 4504 Size DN 100","WNRF","PN 100","BS 4504","4\"",100.0,265.0,90.0,36.0,162.0,210.0,8.0,30.0,150.0,3.0,8.0,5.0,137,"M27",22.0,13.7]
[null,"WNRF PN 100 BS 4504 Size DN 125","WNRF","PN 100","BS 4504","5\"",125.0,315.0,105.0,40.0,188.0,250.0,8.0,33.0,180.0,3.0,8.0,5.0,149,"M30",24.0,22.7]
[null,"WNRF PN 100 BS 4504 Size DN 150","WNRF","PN 100","BS 4504","6\"",150.0,355.0,115.0,44.0,218.0,290.0,12.0,33.0,210.0,3.0,10.0,6.0,158,"M30",24.0,30.2]
[null,"WNRF PN 100 BS 4504 Size DN 175","WNRF","PN 100","BS 4504","7\"",175.0,390.0,127.0,48.0,260.0,320.0,12.0,33.0,245.0,3.0,10.0,7.0,167,"M30",24.0,38.9]
[null,"WNRF PN 100 BS 4504 Size DN 200","WNRF","PN 100","BS 4504","8\"",200.0,430.0,130.0,52.0,285.0,360.0,12.0,36.0,278.0,3.0,10.0,7.0,181,"M33",27.0,52.8]
[null,"WNRF PN 100 BS 4504 Size DN 250","WNRF","PN 100","BS 4504","10\"",250.0,505.0,157.0,60.0,345.0,430.0,12.0,39.0,340.0,3.0,12.0,7.0,201,"M36",29.0,81.4]
[null,"WNRF PN 100 BS 4504 Size DN 300","WNRF","PN 100","BS 4504","12\"",300.0,585.0,170.0,68.0,410.0,500.0,16.0,42.0,400.0,4.0,12.0,7.0,221,"M39",31.0,122.0]
[null,"WNRF PN 100 BS 4504 Size DN 350","WNRF","PN 100","BS 4504","14\"",350.0,655.0,189.0,74.0,465.0,560.0,16.0,48.0,460.0,4.0,12.0,7.0,243,"M45",36.0,165.0]
[null,"WNRF PN 100 BS 4504 Size DN 400","WNRF","PN 100","BS 4504","16\"",400.0,715.0,"-",78.0,535.0,620.0,16.0,48.0,"-",4.0,12.0,7.0,251,"M45",36.0,"-"]
[null,"WNRF PN 100 BS 4504 Size DN 500","WNRF","PN 100","BS 4504","20\"",500.0,870.0,"-",94.0,615.0,760.0,20.0,56.0,"-",4.0,12.0,7.0,295,"M52",42.0,"-"]
[null,"WNRF PN 100 BS 4504 Size DN 600","WNRF","PN 100","BS 4504","24\"",600.0,990.0,"-",104.0,735.0,875.0,20.0,62.0,"-",4.0,12.0,7.0,321,"M56",45.0,"-"]
[null,{"$f":"CONCATENATE(C818,D818,$C$1,E818,$C$1,$F$1,$C$1,$C$1,F818)","v":"WN 100 ft-43,4# BS 10 Table A Size  1/2\""},"WN 100 ft-","43,4#","BS 10 Table A","1/2\"",15.0,95.25,"-",12.7,"-",66.68,4.0,14.29,"-","-","-",3.0,64.4,"M12",10.0,"-"]
[null,"WN 100 ft-43,4# BS 10 Table A Size  3/4\"","WN 100 ft-","43,4#","BS 10 Table A","3/4\"",20.0,101.6,"-",12.7,"-",73.03,4.0,14.29,"-","-","-",3.0,64.4,"M12",10.0,"-"]
[null,"WN 100 ft-43,4# BS 10 Table A Size  1\"","WN 100 ft-","43,4#","BS 10 Table A","1\"",25.0,114.3,"-",12.7,"-",82.55,4.0,14.29,"-","-","-",3.0,64.4,"M12",10.0,"-"]
[null,"WN 100 ft-43,4# BS 10 Table A Size  1¼\"","WN 100 ft-","43,4#","BS 10 Table A","1¼\"",32.0,120.65,"-",15.88,"-",87.31,4.0,14.29,"-","-","-",3.0,70.76,"M12",10.0,"-"]
[null,"WN 100 ft-43,4# BS 10 Table A Size  1½\"","WN 100 ft-","43,4#","BS 10 Table A","1½\"",40.0,133.35,"-",15.88,"-",98.43,4.0,14.29,"-","-","-",3.0,70.76,"M12",10.0,"-"]
[null,"WN 100 ft-43,4# BS 10 Table A Size  2\"","WN 100 ft-","43,4#","BS 10 Table A","2\"",50.0,152.4,"-",15.88,"-",114.3,4.0,17.46,"-","-","-",4.0,77.76,"M16",13.0,"-"]
[null,"WN 100 ft-43,4# BS 10 Table A Size  2½\"","WN 100 ft-","43,4#","BS 10 Table A","2½\"",65.0,165.1,"-",17.46,"-",127.0,4.0,17.46,"-","-","-",4.0,80.92,"M16",13.0,"-"]
[null,"WN 100 ft-43,4# BS 10 Table A Size  3\"","WN 100 ft-","43,4#","BS 10 Table A","3\"",80.0,184.15,"-",17.46,"-",146.05,4.0,17.46,"-","-","-",4.0,80.92,"M16",13.0,"-"]
[null,"WN 100 ft-43,4# BS 10 Table A Size  3½\"","WN 100 ft-","43,4#","BS 10 Table A","3½\"","-",203.2,"-",19.05,"-",165.1,4.0,17.46,"-","-","-",4.0,84.1,"M16",13.0,"-"]
[null,"WN 100 ft-43,4# BS 10 Table A Size  4\"","WN 100 ft-","43,4#","BS 10 Table A","4\"",100.0,215.9,"-",19.1,"-",177.8,4.0,17.46,"-","-","-",5.0,85.2,"M16",13.0,"-"]
[null,"WN 100 ft-43,4# BS 10 Table A Size  5\"","WN 100 ft-","43,4#","BS 10 Table A","5\"",125.0,254.0,"-",19.1,"-",209.55,4.0,17.46,"-","-","-",5.0,85.2,"M16",13.0,"-"]
[null,"WN 100 ft-43,4# BS 10 Table A Size  6\"","WN 100 ft-","43,4#","BS 10 Table A","6\"",150.0,279.4,"-",20.63,"-",234.95,4.0,17.46,"-","-","-",6.0,89.26,"M16",13.0,"-"]
[null,"WN 100 ft-43,4# BS 10 Table A Size  7\"","WN 100 ft-","43,4#","BS 10 Table A","7\"",175.0,304.8,"-",20.63,"-",260.35,8.0,17.46,"-","-","-",6.0,89.26,"M16",13.0,"-"]
[null,"WN 100 ft-43,4# BS 10 Table A Size  8\"","WN 100 ft-","43,4#","BS 10 Table A","8\"",200.0,336.55,"-",22.23,"-",292.1,8.0,17.46,"-","-","-",6.0,92.46,"M16",13.0,"-"]
[null,"WN 100 ft-43,4# BS 10 Table A Size  9\"","WN 100 ft-","43,4#","BS 10 Table A","9\"",225.0,368.3,"-",22.23,"-",323.85,8.0,17.46,"-","-","-",6.0,92.46,"M16",13.0,"-"]
[null,"WN 100 ft-43,4# BS 10 Table A Size  10\"","WN 100 ft-","43,4#","BS 10 Table A","10\"",250.0,406.4,"-",23.81,"-",355.6,8.0,22.23,"-","-","-",6.0,101.62,"M20",16.0,"-"]
[null,"WN 100 ft-43,4# BS 10 Table A Size  12\"","WN 100 ft-","43,4#","BS 10 Table A","12\"",300.0,457.2,"-",23.81,"-",406.4,8.0,22.23,"-","-","-",6.0,101.62,"M20",16.0,"-"]
[null,"WN 100 ft-43,4# BS 10 Table A Size  14\"","WN 100 ft-","43,4#","BS 10 Table A","14\"",350.0,514.35,"-","-","-",469.9,8.0,25.4,"-","-","-",7.0,"-","M22",18.0,"-"]
[null,"WN 100 ft-43,4# BS 10 Table A Size  16\"","WN 100 ft-","43,4#","BS 10 Table A","16\"",400.0,577.85,"-","-","-",520.7,12.0,25.4,"-","-","-",7.0,"-","M22",18.0,"-"]
[null,"WN 100 ft-43,4# BS 10 Table A Size  18\"","WN 100 ft-","43,4#","BS 10 Table A","18\"",450.0,641.35,"-","-","-",584.0,12.0,25.4,"-","-","-",7.0,"-","M22",18.0,"-"]
[null,"WN 100 ft-43,4# BS 10 Table A Size  20\"","WN 100 ft-","43,4#","BS 10 Table A","20\"",500.0,704.85,"-","-","-",641.35,12.0,25.4,"-","-","-",7.0,"-","M22",18.0,"-"]
[null,"WN 100 ft-43,4# BS 10 Table A Size  22\"","WN 100 ft-","43,4#","BS 10 Table A","22\"",550.0,736.6,"-","-","-",698.5,12.0,28.58,"-","-","-",7.0,"-","M24",19.0,"-"]
[null,"WN 100 ft-43,4# BS 10 Table A Size  24\"","WN 100 ft-","43,4#","BS 10 Table A","24\"",600.0,825.5,"-","-","-",755.65,12.0,28.58,"-","-","-",7.0,"-","M24",19.0,"-"]
[null,{"$f":"CONCATENATE(C841,$C$1,D841,$C$1,E841,$C$1,$F$1,$C$1,$C$1,F841)","v":"WN 50# BS 10 Table D Size  1/2\""},"WN","50#","BS 10 Table D","1/2\"",15.0,95.25,"-",9.53,"-",60.33,4.0,14.29,"-","-","-",3.0,{"$f":"(J841+U841+8)*2+R841","v":58.06},"M12",10.0,"-"]
[null,"WN 50# BS 10 Table D Size  3/4\"","WN","50#","BS 10 Table D","3/4\"",20.0,101.6,"-",9.53,"-",73.03,4.0,14.29,"-","-","-",3.0,58.06,"M12",10.0,"-"]
[null,"WN 50# BS 10 Table D Size  1\"","WN","50#","BS 10 Table D","1\"",25.0,114.3,"-",9.5,"-",82.55,4.0,14.29,"-","-","-",3.0,58,"M12",10.0,"-"]
[null,"WN 50# BS 10 Table D Size  1¼\"","WN","50#","BS 10 Table D","1¼\"",32.0,120.65,"-",12.7,"-",87.31,4.0,14.3,"-","-","-",3.0,64.4,"M12",10.0,"-"]
[null,"WN 50# BS 10 Table D Size  1½\"","WN","50#","BS 10 Table D","1½\"",40.0,133.4,"-",12.7,"-",98.4,4.0,14.3,"-","-","-",3.0,64.4,"M12",10.0,"-"]
[null,"WN 50# BS 10 Table D Size  2\"","WN","50#","BS 10 Table D","2\"",50.0,152.4,"-",14.29,"-",114.3,4.0,17.46,"-","-","-",4.0,74.58,"M16",13.0,"-"]
[null,"WN 50# BS 10 Table D Size  2½\"","WN","50#","BS 10 Table D","2½\"",65.0,165.1,"-",14.29,"-",127.0,4.0,17.46,"-","-","-",4.0,74.58,"M16",13.0,"-"]
[null,"WN 50# BS 10 Table D Size  3\"","WN","50#","BS 10 Table D","3\"",80.0,184.2,"-",14.29,"-",146.1,4.0,17.46,"-","-","-",4.0,74.58,"M16",13.0,"-"]
[null,"WN 50# BS 10 Table D Size  3½\"","WN","50#","BS 10 Table D","3½\"","-",203.2,"-",14.28,"-",165.1,4.0,17.46,"-","-","-",4.0,74.56,"M16",13.0,"-"]
[null,"WN 50# BS 10 Table D Size  4\"","WN","50#","BS 10 Table D","4\"",100.0,215.9,"-",17.46,"-",177.8,4.0,17.46,"-","-","-",5.0,81.92,"M16",13.0,"-"]
[null,"WN 50# BS 10 Table D Size  5\"","WN","50#","BS 10 Table D","5\"",125.0,254.0,"-",17.46,"-",209.6,8.0,17.46,"-","-","-",5.0,81.92,"M16",13.0,"-"]
[null,"WN 50# BS 10 Table D Size  6\"","WN","50#","BS 10 Table D","6\"",150.0,279.4,"-",17.46,"-",235.0,8.0,17.46,"-","-","-",6.0,82.92,"M16",13.0,"-"]
[null,"WN 50# BS 10 Table D Size  7\"","WN","50#","BS 10 Table D","7\"",175.0,304.8,"-",19.05,"-",260.35,8.0,17.46,"-","-","-",6.0,86.1,"M16",13.0,"-"]
[null,"WN 50# BS 10 Table D Size  8\"","WN","50#","BS 10 Table D","8\"",200.0,336.6,"-",19.05,"-",292.1,8.0,17.46,"-","-","-",6.0,86.1,"M16",13.0,"-"]
[null,"WN 50# BS 10 Table D Size  9\"","WN","50#","BS 10 Table D","9\"",225.0,368.3,"-",19.05,"-",323.85,8.0,17.46,"-","-","-",6.0,86.1,"M16",13.0,"-"]
[null,"WN 50# BS 10 Table D Size  10\"","WN","50#","BS 10 Table D","10\"",250.0,406.4,"-",19.05,"-",355.6,8.0,22.2,"-","-","-",6.0,92.1,"M20",16.0,"-"]
[null,"WN 50# BS 10 Table D Size  12\"","WN","50#","BS 10 Table D","12\"",300.0,457.2,"-",22.23,"-",406.4,12.0,22.2,"-","-","-",6.0,98.46,"M20",16.0,"-"]
[null,"WN 50# BS 10 Table D Size  14\"","WN","50#","BS 10 Table D","14\"",350.0,527.1,"-","-","-",469.9,12.0,25.4,"-","-","-",7.0,"-","M22",18.0,"-"]
[null,"WN 50# BS 10 Table D Size  16\"","WN","50#","BS 10 Table D","16\"",400.0,577.9,"-","-","-",520.7,12.0,25.4,"-","-","-",7.0,"-","M22",18.0,"-"]
[null,"WN 50# BS 10 Table D Size  18\"","WN","50#","BS 10 Table D","18\"",450.0,641.4,"-","-","-",584.2,12.0,25.4,"-","-","-",7.0,"-","M22",18.0,"-"]
[null,"WN 50# BS 10 Table D Size  20\"","WN","50#","BS 10 Table D","20\"",500.0,704.9,"-","-","-",641.4,16.0,25.4,"-","-","-",7.0,"-","M22",18.0,"-"]
[null,"WN 50# BS 10 Table D Size  24\"","WN","50#","BS 10 Table D","24\"",600.0,825.5,"-","-","-",755.7,16.0,28.5,"-","-","-",7.0,"-","M24",19.0,"-"]
[null,"WN 100# BS 10 Table E Size  1/2\"","WN","100#","BS 10 Table E","1/2\"",15.0,95.25,"-",9.53,null,66.68,4.0,14.29,"-","-","-",3.0,{"$f":"(J863+U863+8)*2+R863","v":58.06},"M12",10.0]
[null,"WN 100# BS 10 Table E Size  3/4\"","WN","100#","BS 10 Table E","3/4\"",20.0,101.6,"-",9.53,null,73.03,4.0,14.29,"-","-","-",3.0,58.06,"M12",10.0]
[null,"WN 100# BS 10 Table E Size  1\"","WN","100#","BS 10 Table E","1\"",25.0,114.3,"-",9.53,"-",82.55,4.0,14.29,"-","-","-",3.0,58.06,"M12",10.0,"-"]
[null,"WN 100# BS 10 Table E Size  1¼\"","WN","100#","BS 10 Table E","1¼\"",32.0,120.65,"-",12.7,"-",87.31,4.0,14.3,"-","-","-",3.0,64.4,"M12",10.0,"-"]
[null,"WN 100# BS 10 Table E Size  1½\"","WN","100#","BS 10 Table E","1½\"",40.0,133.4,"-",12.7,"-",98.4,4.0,15.9,"-","-","-",3.0,64.4,"M12",10.0,"-"]
[null,"WN 100# BS 10 Table E Size  2\"","WN","100#","BS 10 Table E","2\"",50.0,152.4,"-",14.29,"-",114.3,4.0,17.46,"-","-","-",4.0,74.58,"M16",13.0,"-"]
[null,"WN 100# BS 10 Table E Size  2½\"","WN","100#","BS 10 Table E","2½\"",65.0,165.1,"-",14.29,"-",127.0,4.0,17.46,"-","-","-",4.0,74.58,"M16",13.0,"-"]
[null,"WN 100# BS 10 Table E Size  3\"","WN","100#","BS 10 Table E","3\"",80.0,184.2,"-",14.29,"-",146.1,4.0,17.46,"-","-","-",4.0,74.58,"M16",13.0,"-"]
[null,"WN 100# BS 10 Table E Size  3½\"","WN","100#","BS 10 Table E","3½\"","-",203.2,"-",14.29,null,165.1,8.0,17.46,"-","-","-",4.0,74.58,"M16",13.0]
[null,"WN 100# BS 10 Table E Size  4\"","WN","100#","BS 10 Table E","4\"",100.0,215.9,"-",17.46,"-",177.8,8.0,17.46,"-","-","-",5.0,81.92,"M16",13.0,"-"]
[null,"WN 100# BS 10 Table E Size  5\"","WN","100#","BS 10 Table E","5\"",125.0,254.0,"-",17.46,"-",209.6,8.0,17.46,"-","-","-",5.0,81.92,"M16",13.0,"-"]
[null,"WN 100# BS 10 Table E Size  6\"","WN","100#","BS 10 Table E","6\"",150.0,279.4,"-",17.46,"-",235.0,8.0,22.2,"-","-","-",6.0,88.92,"M20",16.0,"-"]
[null,"WN 100# BS 10 Table E Size  7\"","WN","100#","BS 10 Table E","7\"",175.0,304.8,"-",19.05,"-",260.35,8.0,22.2,"-","-","-",6.0,92.1,"M20",16.0,"-"]
[null,"WN 100# BS 10 Table E Size  8\"","WN","100#","BS 10 Table E","8\"",200.0,336.6,"-",19.05,"-",292.1,8.0,22.2,"-","-","-",6.0,92.1,"M20",16.0,"-"]
[null,"WN 100# BS 10 Table E Size  9\"","WN","100#","BS 10 Table E","9\"",225.0,368.3,"-",20.63,null,323.85,12.0,22.23,"-","-","-",6.0,95.26,"M20",16.0]
[null,"WN 100# BS 10 Table E Size  10\"","WN","100#","BS 10 Table E","10\"",250.0,406.4,"-",22.23,"-",355.6,12.0,22.2,"-","-","-",6.0,98.46,"M20",16.0,"-"]
[null,"WN 100# BS 10 Table E Size  12\"","WN","100#","BS 10 Table E","12\"",300.0,457.2,"-",25.4,"-",406.4,12.0,25.4,"-","-","-",6.0,108.8,"M22",18.0,"-"]
[null,"WN 100# BS 10 Table E Size  14\"","WN","100#","BS 10 Table E","14\"",350.0,527.1,"-","-","-",469.9,12.0,25.4,"-","-","-",7.0,"-","M22",18.0,"-"]
[null,"WN 100# BS 10 Table E Size  16\"","WN","100#","BS 10 Table E","16\"",400.0,577.9,"-","-","-",520.7,12.0,25.4,"-","-","-",7.0,"-","M22",18.0,"-"]
[null,"WN 100# BS 10 Table E Size  18\"","WN","100#","BS 10 Table E","18\"",450.0,641.4,"-","-","-",584.2,16.0,25.4,"-","-","-",7.0,"-","M22",18.0,"-"]
[null,"WN 100# BS 10 Table E Size  20\"","WN","100#","BS 10 Table E","20\"",500.0,704.9,"-","-","-",641.4,16.0,25.4,"-","-","-",7.0,"-","M22",18.0,"-"]
[null,"WN 100# BS 10 Table E Size  24\"","WN","100#","BS 10 Table E","24\"",600.0,825.5,"-","-","-",755.7,16.0,31.7,"-","-","-",7.0,"-","M27",22.0,"-"]
[null,"WN 150# BS 10 Table F Size  1/2\"","WN","150#","BS 10 Table F","1/2\"",15.0,95.25,"-",9.53,"-",66.68,4.0,14.29,"-","-","-",3.0,{"$f":"(J885+U885+8)*2+R885","v":58.06},"M12",10.0,"-"]
[null,"WN 150# BS 10 Table F Size  3/4\"","WN","150#","BS 10 Table F","3/4\"",20.0,114.3,"-",9.53,"-",73.03,4.0,17.46,"-","-","-",3.0,64.06,"M16",13.0,"-"]
[null,"WN 150# BS 10 Table F Size  1\"","WN","150#","BS 10 Table F","1\"",25.0,120.65,"-",9.53,"-",87.0,4.0,17.46,"-","-","-",3.0,64.06,"M16",13.0,"-"]
[null,"WN 150# BS 10 Table F Size  1¼","WN","150#","BS 10 Table F","1¼",32.0,133.35,"-",12.7,"-",98.43,4.0,17.46,"-","-","-",3.0,70.4,"M16",13.0,"-"]
[null,"WN 150# BS 10 Table F Size  1½","WN","150#","BS 10 Table F","1½",40.0,139.7,"-",12.7,"-",104.78,4.0,17.46,"-","-","-",3.0,70.4,"M16",13.0,"-"]
[null,"WN 150# BS 10 Table F Size  2\"","WN","150#","BS 10 Table F","2\"",50.0,165.1,"-",15.88,"-",127.0,4.0,17.46,"-","-","-",4.0,77.76,"M16",13.0,"-"]
[null,"WN 150# BS 10 Table F Size  2½\"","WN","150#","BS 10 Table F","2½\"",65.0,184.15,"-",15.88,"-",146.05,8.0,17.46,"-","-","-",4.0,77.76,"M16",13.0,"-"]
[null,"WN 150# BS 10 Table F Size  3\"","WN","150#","BS 10 Table F","3\"",80.0,203.2,"-",15.88,"-",165.1,8.0,17.46,"-","-","-",5.0,78.76,"M16",13.0,"-"]
[null,"WN 150# BS 10 Table F Size  3½\"","WN","150#","BS 10 Table F","3½\"","-",215.9,"-",19.1,"-",177.8,8.0,17.46,"-","-","-",5.0,85.2,"M16",13.0,"-"]
[null,"WN 150# BS 10 Table F Size  4\"","WN","150#","BS 10 Table F","4\"",100.0,228.6,"-",19.05,"-",190.5,8.0,17.46,"-","-","-",6.0,86.1,"M16",13.0,"-"]
[null,"WN 150# BS 10 Table F Size  5\"","WN","150#","BS 10 Table F","5\"",125.0,279.4,"-",22.23,"-",241.3,8.0,22.23,"-","-","-",6.0,92.46,"M20",13.0,"-"]
[null,"WN 150# BS 10 Table F Size  6\"","WN","150#","BS 10 Table F","6\"",150.0,304.8,"-",22.23,"-",260.35,12.0,22.23,"-","-","-",6.0,98.46,"M20",16.0,"-"]
[null,"WN 150# BS 10 Table F Size  7\"","WN","150#","BS 10 Table F","7\"",175.0,336.55,"-",22.23,"-",292.1,12.0,22.23,"-","-","-",6.0,98.46,"M20",16.0,"-"]
[null,"WN 150# BS 10 Table F Size  8\"","WN","150#","BS 10 Table F","8\"",200.0,368.3,"-",25.4,"-",323.85,12.0,22.23,"-","-","-",6.0,104.8,"M20",16.0,"-"]
[null,"WN 150# BS 10 Table F Size  9\"","WN","150#","BS 10 Table F","9\"",225.0,406.4,"-",25.4,"-",355.6,12.0,25.4,"-","-","-",6.0,108.8,"M22",18.0]
[null,"WN 150# BS 10 Table F Size  10\"","WN","150#","BS 10 Table F","10\"",250.0,431.8,"-",25.4,"-",381.0,12.0,25.4,"-","-","-",6.0,108.8,"M22",18.0,"-"]
[null,"WN 150# BS 10 Table F Size  12\"","WN","150#","BS 10 Table F","12\"",300.0,488.95,"-",31.75,"-",444.5,16.0,25.4,"-","-","-",6.0,123.5,"M24",19.0,"-"]
[null,"WN 250# BS 10 Table H Size  1/2\"","WN","250#","BS 10 Table H","1/2\"",15.0,114.3,"-",12.7,"-",82.55,4.0,17.4,"-","-","-",3.0,70.4,"M16",13.0,"-"]
[null,"WN 250# BS 10 Table H Size  3/4\"","WN","250#","BS 10 Table H","3/4\"",20.0,114.3,"-",12.7,"-",82.55,4.0,17.4,"-","-","-",3.0,70.4,"M16",13.0,"-"]
[null,"WN 250# BS 10 Table H Size  1\"","WN","250#","BS 10 Table H","1\"",25.0,120.65,"-",14.29,"-",87.31,4.0,17.4,"-","-","-",3.0,73.58,"M16",13.0,"-"]
[null,"WN 250# BS 10 Table H Size  1¼","WN","250#","BS 10 Table H","1¼",32.0,133.35,"-",17.46,"-",98.43,4.0,17.4,"-","-","-",3.0,79.92,"M16",13.0,"-"]
[null,"WN 250# BS 10 Table H Size  1½","WN","250#","BS 10 Table H","1½",40.0,139.7,"-",17.46,"-",104.78,4.0,17.4,"-","-","-",3.0,79.92,"M16",13.0,"-"]
[null,"WN 250# BS 10 Table H Size  2\"","WN","250#","BS 10 Table H","2\"",50.0,165.1,"-",19.05,"-",127.0,4.0,17.4,"-","-","-",4.0,84.1,"M16",13.0,"-"]
[null,"WN 250# BS 10 Table H Size  2½\"","WN","250#","BS 10 Table H","2½\"",65.0,190.5,"-",19.05,"-",146.05,8.0,17.4,"-","-","-",4.0,84.1,"M16",13.0,"-"]
[null,"WN 250# BS 10 Table H Size  3\"","WN","250#","BS 10 Table H","3\"",80.0,203.2,"-",22.23,"-",165.1,8.0,17.4,"-","-","-",4.0,90.46,"M16",13.0,"-"]
[null,"WN 250# BS 10 Table H Size  3½\"","WN","250#","BS 10 Table H","3½\"","-",215.9,"-",22.23,"-",177.8,8.0,17.4,"-","-","-",4.0,90.46,"M16",13.0,"-"]
[null,"WN 250# BS 10 Table H Size  4\"","WN","250#","BS 10 Table H","4\"",100.0,228.6,"-",25.4,"-",190.5,8.0,17.4,"-","-","-",5.0,97.8,"M16",13.0,"-"]
[null,"WN 250# BS 10 Table H Size  5\"","WN","250#","BS 10 Table H","5\"",125.0,279.4,"-",28.58,"-",234.95,8.0,22.23,"-","-","-",5.0,110.16,"M20",16.0,"-"]
[null,"WN 250# BS 10 Table H Size  6\"","WN","250#","BS 10 Table H","6\"",150.0,304.8,"-",31.75,"-",260.35,12.0,22.23,"-","-","-",6.0,117.5,"M20",16.0,"-"]
[null,"WN 250# BS 10 Table H Size  7\"","WN","250#","BS 10 Table H","7\"",175.0,336.55,"-",31.75,"-",292.1,12.0,22.23,"-","-","-",6.0,117.5,"M20",16.0,"-"]
[null,"WN 250# BS 10 Table H Size  8\"","WN","250#","BS 10 Table H","8\"",200.0,368.3,"-",31.75,"-",323.85,12.0,22.23,"-","-","-",6.0,117.5,"M20",16.0,"-"]
[null,"WN 250# BS 10 Table H Size  9\"","WN","250#","BS 10 Table H","9\"",225.0,406.4,"-",34.93,"-",355.6,12.0,25.4,"-","-","-",6.0,127.86,"M22",18.0,"-"]
[null,"WN 250# BS 10 Table H Size  10\"","WN","250#","BS 10 Table H","10\"",250.0,431.8,"-",34.93,"-",381.0,12.0,25.4,"-","-","-",6.0,127.86,"M22",18.0,"-"]
[null,"WN 250# BS 10 Table H Size  12\"","WN","250#","BS 10 Table H","12\"",300.0,488.95,"-",38.1,"-",431.8,16.0,25.4,"-","-","-",6.0,134.2,"M22",18.0,"-"]
[null,"WN 350# BS 10 Table H Size  1/2\"","WN","350#","BS 10 Table H","1/2\"",15.0,114.3,"-",15.88,"-",82.55,4.0,17.4,"-","-","-",3.0,76.76,"M16",13.0,"-"]
[null,"WN 350# BS 10 Table H Size  3/4\"","WN","350#","BS 10 Table H","3/4\"",20.0,114.3,"-",15.88,"-",82.55,4.0,17.4,"-","-","-",3.0,76.76,"M16",13.0,"-"]
[null,"WN 350# BS 10 Table H Size  1\"","WN","350#","BS 10 Table H","1\"",25.0,120.65,"-",19.05,"-",87.31,4.0,17.4,"-","-","-",3.0,83.1,"M16",13.0,"-"]
[null,"WN 350# BS 10 Table H Size  1¼","WN","350#","BS 10 Table H","1¼",32.0,133.35,"-",19.05,"-",98.43,4.0,17.4,"-","-","-",3.0,83.1,"M16",13.0,"-"]
[null,"WN 350# BS 10 Table H Size  1½","WN","350#","BS 10 Table H","1½",40.0,139.7,"-",22.23,"-",104.78,4.0,17.4,"-","-","-",3.0,89.46,"M16",13.0,"-"]
[null,"WN 350# BS 10 Table H Size  2\"","WN","350#","BS 10 Table H","2\"",50.0,165.1,"-",25.4,"-",127.0,4.0,22.23,"-","-","-",4.0,102.8,"M20",16.0,"-"]
[null,"WN 350# BS 10 Table H Size  2½\"","WN","350#","BS 10 Table H","2½\"",65.0,184.15,"-",25.4,"-",146.05,8.0,22.23,"-","-","-",4.0,102.8,"M20",16.0,"-"]
[null,"WN 350# BS 10 Table H Size  3\"","WN","350#","BS 10 Table H","3\"",80.0,203.2,"-",31.75,"-",165.1,8.0,22.23,"-","-","-",4.0,115.5,"M20",16.0,"-"]
[null,"WN 350# BS 10 Table H Size  3½\"","WN","350#","BS 10 Table H","3½\"","-",215.9,"-",31.75,"-",177.8,8.0,22.23,"-","-","-",4.0,115.5,"M20",16.0,"-"]
[null,"WN 350# BS 10 Table H Size  4\"","WN","350#","BS 10 Table H","4\"",100.0,228.6,"-",34.93,"-",190.5,8.0,22.23,"-","-","-",5.0,122.86,"M20",16.0,"-"]
[null,"WN 350# BS 10 Table H Size  5\"","WN","350#","BS 10 Table H","5\"",125.0,279.4,"-",38.1,"-",234.95,8.0,25.4,"-","-","-",5.0,133.2,"M22",18.0,"-"]
[null,"WN 350# BS 10 Table H Size  6\"","WN","350#","BS 10 Table H","6\"",150.0,304.8,"-",38.1,"-",260.35,12.0,25.4,"-","-","-",6.0,134.2,"M22",18.0,"-"]
[null,"WN 350# BS 10 Table H Size  7\"","WN","350#","BS 10 Table H","7\"",175.0,336.55,"-",41.28,"-",285.75,12.0,25.4,"-","-","-",6.0,140.56,"M22",18.0,"-"]
[null,"WN 350# BS 10 Table H Size  8\"","WN","350#","BS 10 Table H","8\"",200.0,368.3,"-",41.28,"-",323.85,12.0,25.4,"-","-","-",6.0,140.56,"M22",18.0,"-"]
[null,"WN 350# BS 10 Table H Size  9\"","WN","350#","BS 10 Table H","9\"",225.0,406.4,"-",44.45,"-",355.6,12.0,28.58,"-","-","-",6.0,148.9,"M24",19.0,"-"]
[null,"WN 350# BS 10 Table H Size  10\"","WN","350#","BS 10 Table H","10\"",250.0,431.8,"-",47.63,"-",381.0,12.0,28.58,"-","-","-",6.0,155.26,"M24",19.0,"-"]
[null,"WN 350# BS 10 Table H Size  12\"","WN","350#","BS 10 Table H","12\"",300.0,488.95,"-",50.8,"-",438.15,16.0,28.58,"-","-","-",6.0,161.6,"M24",19.0,"-"]
[null,"WN 450# BS 10 Table K Size  1/2\"","WN","450#","BS 10 Table K","1/2\"",15.0,114.3,"-",19.05,"-",88.9,4.0,17.46,"-","-","-",3.0,83.1,"M16",13.0,"-"]
[null,"WN 450# BS 10 Table K Size  3/4\"","WN","450#","BS 10 Table K","3/4\"",20.0,114.3,"-",19.05,"-",88.9,4.0,17.46,"-","-","-",3.0,83.1,"M16",13.0,"-"]
[null,"WN 450# BS 10 Table K Size  1\"","WN","450#","BS 10 Table K","1\"",25.0,120.65,"-",22.23,"-",95.25,4.0,17.46,"-","-","-",3.0,89.46,"M16",13.0,"-"]
[null,"WN 450# BS 10 Table K Size  1¼","WN","450#","BS 10 Table K","1¼",32.0,133.35,"-",22.23,"-",98.43,4.0,17.46,"-","-","-",3.0,89.46,"M16",13.0,"-"]
[null,"WN 450# BS 10 Table K Size  1½","WN","450#","BS 10 Table K","1½",40.0,139.7,"-",25.4,"-",114.3,4.0,22.23,"-","-","-",3.0,101.8,"M20",16.0,"-"]
[null,"WN 450# BS 10 Table K Size  2\"","WN","450#","BS 10 Table K","2\"",50.0,165.1,"-",25.4,"-",127.0,8.0,17.46,"-","-","-",4.0,96.8,"M16",13.0,"-"]
[null,"WN 450# BS 10 Table K Size  2½\"","WN","450#","BS 10 Table K","2½\"",65.0,184.15,"-",28.28,"-",146.05,8.0,22.23,"-","-","-",4.0,108.56,"M20",16.0,"-"]
[null,"WN 450# BS 10 Table K Size  3\"","WN","450#","BS 10 Table K","3\"",80.0,203.2,"-",31.75,"-",165.1,8.0,22.23,"-","-","-",4.0,115.5,"M20",16.0,"-"]
[null,"WN 450# BS 10 Table K Size  3½\"","WN","450#","BS 10 Table K","3½\"","-",228.6,"-",31.75,"-",184.15,8.0,25.4,"-","-","-",4.0,119.5,"M22",18.0,"-"]
[null,"WN 450# BS 10 Table K Size  4\"","WN","450#","BS 10 Table K","4\"",100.0,241.3,"-",34.93,"-",196.85,8.0,25.4,"-","-","-",5.0,126.86,"M22",18.0,"-"]
[null,"WN 450# BS 10 Table K Size  5\"","WN","450#","BS 10 Table K","5\"",125.0,279.4,"-",41.28,"-",234.95,12.0,25.4,"-","-","-",5.0,139.56,"M22",18.0,"-"]
[null,"WN 450# BS 10 Table K Size  6\"","WN","450#","BS 10 Table K","6\"",150.0,304.8,"-",41.28,"-",260.35,12.0,25.4,"-","-","-",6.0,140.56,"M22",18.0,"-"]
[null,"WN 450# BS 10 Table K Size  7\"","WN","450#","BS 10 Table K","7\"",175.0,342.9,"-",44.45,"-",292.1,12.0,28.58,"-","-","-",6.0,148.9,"M24",19.0,"-"]
[null,"WN 450# BS 10 Table K Size  8\"","WN","450#","BS 10 Table K","8\"",200.0,368.3,"-",47.63,"-",317.5,12.0,28.58,"-","-","-",6.0,155.26,"M24",19.0,"-"]
[null,"WN 450# BS 10 Table K Size  9\"","WN","450#","BS 10 Table K","9\"",225.0,406.4,"-",50.8,"-",355.6,16.0,28.58,"-","-","-",6.0,161.6,"M24",19.0,"-"]
[null,"WN 450# BS 10 Table K Size  10\"","WN","450#","BS 10 Table K","10\"",250.0,431.8,"-",50.8,"-",381.0,16.0,28.58,"-","-","-",6.0,161.6,"M24",19.0,"-"]
[null,"WN 450# BS 10 Table K Size  12\"","WN","450#","BS 10 Table K","12\"",300.0,501.65,"-",57.15,"-",431.8,16.0,31.75,"-","-","-",6.0,180.3,"M27",22.0,"-"]
[null,"WNRF 600# BS 10 Table R Size  1/2\"","WNRF","600#","BS 10 Table R","1/2\"",15.0,114.3,"-",19.05,57.15,82.55,4.0,17.46,"-",1.59,"-",3.0,83.1,"M16",13.0,"-"]
[null,"WNRF 600# BS 10 Table R Size  3/4\"","WNRF","600#","BS 10 Table R","3/4\"",20.0,114.3,"-",19.05,57.15,82.55,4.0,17.46,"-",1.59,"-",3.0,83.1,"M16",13.0,"-"]
[null,"WNRF 600# BS 10 Table R Size  1\"","WNRF","600#","BS 10 Table R","1\"",25.0,127.0,"-",22.23,63.5,95.25,4.0,17.46,"-",1.59,"-",3.0,89.46,"M16",13.0,"-"]
[null,"WNRF 600# BS 10 Table R Size  1¼","WNRF","600#","BS 10 Table R","1¼",32.0,133.35,"-",22.23,69.85,98.43,4.0,17.46,"-",1.59,"-",3.0,89.46,"M16",13.0,"-"]
[null,"WNRF 600# BS 10 Table R Size  1½","WNRF","600#","BS 10 Table R","1½",40.0,152.4,"-",25.4,76.2,114.3,4.0,22.23,"-",1.59,"-",3.0,101.8,"M20",16.0,"-"]
[null,"WNRF 600# BS 10 Table R Size  2\"","WNRF","600#","BS 10 Table R","2\"",50.0,165.1,"-",25.4,88.9,127.0,8.0,17.46,"-",1.59,"-",4.0,96.8,"M16",13.0,"-"]
[null,"WNRF 600# BS 10 Table R Size  2½\"","WNRF","600#","BS 10 Table R","2½\"",65.0,184.15,"-",28.58,101.6,146.05,8.0,22.23,"-",1.59,"-",4.0,109.16,"M20",16.0,"-"]
[null,"WNRF 600# BS 10 Table R Size  3\"","WNRF","600#","BS 10 Table R","3\"",80.0,203.2,"-",31.75,114.3,165.1,8.0,22.23,"-",1.59,"-",4.0,115.5,"M20",16.0,"-"]
[null,"WNRF 600# BS 10 Table R Size  3½\"","WNRF","600#","BS 10 Table R","3½\"","-",228.6,"-",31.75,127.0,184.15,8.0,25.4,"-",1.59,"-",4.0,119.5,"M22",18.0,"-"]
[null,"WNRF 600# BS 10 Table R Size  4\"","WNRF","600#","BS 10 Table R","4\"",100.0,241.3,"-",34.93,139.7,196.85,8.0,25.4,"-",1.59,"-",5.0,126.86,"M22",18.0,"-"]
[null,"WNRF 600# BS 10 Table R Size  5\"","WNRF","600#","BS 10 Table R","5\"",125.0,279.4,"-",41.28,165.1,234.95,12.0,25.4,"-",1.59,"-",5.0,139.56,"M22",18.0,"-"]
[null,"WNRF 600# BS 10 Table R Size  6\"","WNRF","600#","BS 10 Table R","6\"",150.0,304.8,"-",44.45,190.5,260.35,12.0,25.4,"-",1.59,"-",6.0,146.9,"M22",18.0,"-"]
[null,"WNRF 600# BS 10 Table R Size  7\"","WNRF","600#","BS 10 Table R","7\"",175.0,342.9,"-",47.63,222.25,292.1,12.0,28.58,"-",1.59,"-",6.0,155.26,"M24",19.0,"-"]
[null,"WNRF 600# BS 10 Table R Size  8\"","WNRF","600#","BS 10 Table R","8\"",200.0,361.95,"-",50.8,247.65,323.85,12.0,28.58,"-",1.59,"-",6.0,161.6,"M24",19.0,"-"]
[null,"WNRF 600# BS 10 Table R Size  9\"","WNRF","600#","BS 10 Table R","9\"",225.0,406.4,"-",57.15,273.05,355.6,16.0,28.58,"-",1.59,"-",6.0,174.3,"M24",19.0,"-"]
[null,"WNRF 600# BS 10 Table R Size  10\"","WNRF","600#","BS 10 Table R","10\"",250.0,431.8,"-",57.15,298.45,387.35,16.0,28.58,"-",1.59,"-",6.0,174.3,"M24",19.0,"-"]
[null,"WNRF 600# BS 10 Table R Size  12\"","WNRF","600#","BS 10 Table R","12\"",300.0,508.0,"-",63.5,349.25,457.2,16.0,31.75,"-",1.59,"-",6.0,193,"M27",22.0,"-"]
[null,"WNRF 900# BS 10 Table S Size  1/2\"","WNRF","900#","BS 10 Table S","1/2\"",15.0,127.0,"-",22.23,50.8,88.9,4.0,22.23,"-",1.59,"-",3.0,95.46,"M20",16.0,"-"]
[null,"WNRF 900# BS 10 Table S Size  3/4\"","WNRF","900#","BS 10 Table S","3/4\"",20.0,127.0,"-",22.23,50.8,88.9,4.0,22.23,"-",1.59,"-",3.0,95.46,"M20",16.0,"-"]
[null,"WNRF 900# BS 10 Table S Size  1\"","WNRF","900#","BS 10 Table S","1\"",25.0,139.7,"-",25.4,60.96,101.6,4.0,22.23,"-",1.59,"-",3.0,101.8,"M20",16.0,"-"]
[null,"WNRF 900# BS 10 Table S Size  1¼","WNRF","900#","BS 10 Table S","1¼",32.0,146.05,"-",28.58,63.5,107.95,4.0,22.23,"-",1.59,"-",3.0,108.16,"M20",16.0,"-"]
[null,"WNRF 900# BS 10 Table S Size  1½","WNRF","900#","BS 10 Table S","1½",40.0,158.75,"-",28.58,69.85,120.65,4.0,22.23,"-",1.59,"-",3.0,108.16,"M20",16.0,"-"]
[null,"WNRF 900# BS 10 Table S Size  2\"","WNRF","900#","BS 10 Table S","2\"",50.0,171.45,"-",31.75,82.55,133.35,8.0,22.23,"-",1.59,"-",4.0,115.5,"M20",16.0,"-"]
[null,"WNRF 900# BS 10 Table S Size  2½\"","WNRF","900#","BS 10 Table S","2½\"",65.0,184.15,"-",31.75,95.25,146.05,8.0,22.23,"-",1.59,"-",4.0,115.5,"M20",16.0,"-"]
[null,"WNRF 900# BS 10 Table S Size  3\"","WNRF","900#","BS 10 Table S","3\"",80.0,203.2,"-",34.93,114.3,165.1,8.0,25.4,"-",1.59,"-",4.0,125.86,"M22",18.0,"-"]
[null,"WNRF 900# BS 10 Table S Size  3½\"","WNRF","900#","BS 10 Table S","3½\"","-",234.95,"-",38.1,120.65,190.5,8.0,25.4,"-",1.59,"-",4.0,132.2,"M22",18.0,"-"]
[null,"WNRF 900# BS 10 Table S Size  4\"","WNRF","900#","BS 10 Table S","4\"",100.0,247.65,"-",41.28,133.35,203.2,8.0,28.58,"-",1.59,"-",5.0,141.56,"M24",19.0,"-"]
[null,"WNRF 900# BS 10 Table S Size  5\"","WNRF","900#","BS 10 Table S","5\"",125.0,285.75,"-",44.45,158.75,234.95,12.0,25.4,"-",1.59,"-",5.0,145.9,"M22",18.0,"-"]
[null,"WNRF 900# BS 10 Table S Size  6\"","WNRF","900#","BS 10 Table S","6\"",150.0,323.85,"-",50.8,184.15,273.05,12.0,28.58,"-",1.59,"-",6.0,161.6,"M24",19.0,"-"]
[null,"WNRF 900# BS 10 Table S Size  7\"","WNRF","900#","BS 10 Table S","7\"",175.0,374.65,"-",57.15,215.9,317.5,12.0,31.75,"-",1.59,"-",6.0,180.3,"M27",22.0,"-"]
[null,"WNRF 900# BS 10 Table S Size  8\"","WNRF","900#","BS 10 Table S","8\"",200.0,412.75,"-",63.5,241.3,355.6,12.0,34.93,"-",1.59,"-",6.0,197,"M30",24.0,"-"]
[null,"WNRF 900# BS 10 Table S Size  9\"","WNRF","900#","BS 10 Table S","9\"",225.0,438.15,"-",66.68,266.7,387.35,16.0,31.93,"-",1.59,"-",6.0,199.36,"M27",22.0,"-"]
[null,"WNRF 900# BS 10 Table S Size  10\"","WNRF","900#","BS 10 Table S","10\"",250.0,482.6,"-",73.03,292.1,425.45,16.0,34.93,"-",1.59,"-",6.0,216.06,"M30",24.0,"-"]
[null,"WNRF 1400# BS 10 Table T Size  1/2\"","WNRF","1400#","BS 10 Table T","1/2\"",15.0,139.7,"-",25.4,57.15,101.6,4.0,22.23,"-",1.59,"-",3.0,101.8,"M20",16.0,"-"]
[null,"WNRF 1400# BS 10 Table T Size  3/4\"","WNRF","1400#","BS 10 Table T","3/4\"",20.0,139.7,"-",25.4,57.15,101.6,4.0,22.23,"-",1.59,"-",3.0,101.8,"M20",16.0,"-"]
[null,"WNRF 1400# BS 10 Table T Size  1\"","WNRF","1400#","BS 10 Table T","1\"",25.0,146.05,"-",31.75,63.5,107.95,4.0,22.23,"-",1.59,"-",3.0,114.5,"M20",16.0,"-"]
[null,"WNRF 1400# BS 10 Table T Size  1¼","WNRF","1400#","BS 10 Table T","1¼",32.0,158.75,"-",31.75,69.85,120.65,4.0,22.23,"-",1.59,"-",3.0,118.5,"M22",18.0,"-"]
[null,"WNRF 1400# BS 10 Table T Size  1½","WNRF","1400#","BS 10 Table T","1½",40.0,171.45,"-",34.93,76.2,133.35,8.0,25.4,"-",1.59,"-",3.0,120.86,"M20",16.0,"-"]
[null,"WNRF 1400# BS 10 Table T Size  2\"","WNRF","1400#","BS 10 Table T","2\"",50.0,184.15,"-",34.93,88.9,146.05,8.0,22.23,"-",1.59,"-",4.0,121.86,"M20",16.0,"-"]
[null,"WNRF 1400# BS 10 Table T Size  2½\"","WNRF","1400#","BS 10 Table T","2½\"",65.0,203.2,"-",47.63,114.3,165.1,8.0,22.23,"-",1.59,"-",4.0,151.26,"M22",18.0,"-"]
[null,"WNRF 1400# BS 10 Table T Size  3\"","WNRF","1400#","BS 10 Table T","3\"",80.0,234.95,"-",53.98,127.0,190.5,8.0,25.4,"-",1.59,"-",4.0,165.96,"M24",19.0,"-"]
[null,"WNRF 1400# BS 10 Table T Size  3½\"","WNRF","1400#","BS 10 Table T","3½\"","-",266.7,"-",57.15,139.7,215.9,8.0,28.58,"-",1.59,"-",4.0,178.3,"M27",22.0,"-"]
[null,"WNRF 1400# BS 10 Table T Size  4\"","WNRF","1400#","BS 10 Table T","4\"",100.0,285.75,"-",60.33,152.4,241.3,8.0,31.75,"-",1.59,"-",5.0,185.66,"M27",22.0,"-"]
[null,"WNRF 1400# BS 10 Table T Size  5\"","WNRF","1400#","BS 10 Table T","5\"",125.0,323.85,"-",66.68,177.8,273.05,12.0,31.75,"-",1.59,"-",5.0,198.36,"M27",22.0,"-"]
[null,"WNRF 1400# BS 10 Table T Size  6\"","WNRF","1400#","BS 10 Table T","6\"",150.0,374.65,"-",73.03,203.2,317.5,12.0,34.93,"-",1.59,"-",6.0,216.06,"M30",24.0,"-"]
[null,"WNRF 1400# BS 10 Table T Size  7\"","WNRF","1400#","BS 10 Table T","7\"",175.0,431.8,"-",82.55,234.95,368.3,12.0,38.1,"-",1.59,"-",6.0,239.1,"M33",26.0,"-"]
[null,"WNRF 1400# BS 10 Table T Size  8\"","WNRF","1400#","BS 10 Table T","8\"",200.0,476.25,"-",88.9,266.7,406.4,12.0,34.93,"-",1.59,"-",6.0,247.8,"M30",24.0,"-"]
[null,"WNRF 1400# BS 10 Table T Size  9\"","WNRF","1400#","BS 10 Table T","9\"",225.0,508.0,"-",95.25,298.45,444.5,16.0,38.1,"-",1.59,"-",6.0,264.5,"M33",26.0,"-"]
[null,"WNRF 1400# BS 10 Table T Size  10\"","WNRF","1400#","BS 10 Table T","10\"",250.0,558.8,"-",107.95,323.85,488.95,16.0,41.28,"-",1.59,"-",6.0,295.9,"M36",29.0,"-"]
[null,"Cast Iron WNRF PN 10 BS 4772 Size  3\"","Cast Iron WNRF","PN 10","BS 4772","3\"",80.0,200.0,"-",19.0,132.0,160.0,8.0,19.0,"-",3.0,"-",4.0,84,"M16",13.0,"-"]
[null,"Cast Iron WNRF PN 10 BS 4773 Size  4\"","Cast Iron WNRF","PN 10","BS 4773","4\"",100.0,220.0,"-",19.0,156.0,180.0,8.0,19.0,"-",3.0,"-",5.0,85,"M16",13.0,"-"]
[null,"Cast Iron WNRF PN 10 BS 4774 Size  6\"","Cast Iron WNRF","PN 10","BS 4774","6\"",150.0,285.0,"-",19.0,211.0,240.0,8.0,23.0,"-",3.0,"-",6.0,92,"M20",16.0,"-"]
[null,"Cast Iron WNRF PN 10 BS 4775 Size  8\"","Cast Iron WNRF","PN 10","BS 4775","8\"",200.0,340.0,"-",2.0,266.0,295.0,8.0,23.0,"-",3.0,"-",6.0,58,"M20",16.0,"-"]
[null,"Cast Iron WNRF PN 10 BS 4776 Size  10\"","Cast Iron WNRF","PN 10","BS 4776","10\"",250.0,400.0,"-",22.0,319.0,350.0,12.0,23.0,"-",3.0,"-",6.0,98,"M20",16.0,"-"]
[null,"Cast Iron WNRF PN 10 BS 4777 Size  12\"","Cast Iron WNRF","PN 10","BS 4777","12\"",300.0,455.0,"-",24.5,370.0,400.0,12.0,23.0,"-",4.0,"-",6.0,103,"M20",16.0,"-"]
[null,"Cast Iron WNRF PN 12 BS 4778 Size  3\"","Cast Iron WNRF","PN 12","BS 4778","3\"",80.0,200.0,"-",19.0,132.0,160.0,8.0,19.0,"-",3.0,"-",4.0,84,"M16",13.0,"-"]
[null,"Cast Iron WNRF PN 12 BS 4779 Size  4\"","Cast Iron WNRF","PN 12","BS 4779","4\"",100.0,220.0,"-",19.0,156.0,180.0,8.0,19.0,"-",3.0,"-",5.0,85,"M16",13.0,"-"]
[null,"Cast Iron WNRF PN 12 BS 4780 Size  6\"","Cast Iron WNRF","PN 12","BS 4780","6\"",150.0,285.0,"-",19.0,211.0,240.0,8.0,23.0,"-",3.0,"-",6.0,92,"M20",16.0,"-"]
[null,"Cast Iron WNRF PN 12 BS 4781 Size  8\"","Cast Iron WNRF","PN 12","BS 4781","8\"",200.0,340.0,"-",2.0,266.0,295.0,12.0,23.0,"-",3.0,"-",6.0,58,"M20",16.0,"-"]
[null,"Cast Iron WNRF PN 12 BS 4782 Size  10\"","Cast Iron WNRF","PN 12","BS 4782","10\"",250.0,400.0,"-",22.0,319.0,355.0,12.0,28.0,"-",3.0,"-",6.0,98,"M24",16.0,"-"]
[null,"Cast Iron WNRF PN 12 BS 4783 Size  12\"","Cast Iron WNRF","PN 12","BS 4783","12\"",300.0,455.0,"-",24.5,370.0,410.0,12.0,28.0,"-",4.0,"-",6.0,109,"M24",19.0,"-"]
[null,"Cast Iron WN 200# BS 10 Size  3\"","Cast Iron WN","200#","BS 10","3\"",80.0,184.15,"-",14.28,"-",146.05,4.0,19.05,"-","-","-",4.0,74.56,"M16",13.0,"-"]
[null,"Cast Iron WN 200# BS 10 Size  4\"","Cast Iron WN","200#","BS 10","4\"",100.0,215.9,"-",17.46,"-",177.8,8.0,19.05,"-","-","-",5.0,81.92,"M16",13.0,"-"]
[null,"Cast Iron WN 200# BS 10 Size  6\"","Cast Iron WN","200#","BS 10","6\"",150.0,279.4,"-",17.46,"-",234.95,8.0,22.23,"-","-","-",6.0,88.92,"M20",16.0,"-"]
[null,"Cast Iron WN 200# BS 10 Size  8\"","Cast Iron WN","200#","BS 10","8\"",200.0,336.55,"-",19.05,"-",292.1,8.0,22.23,"-","-","-",6.0,92.1,"M20",16.0,"-"]
[null,"Cast Iron WN 200# BS 10 Size  10\"","Cast Iron WN","200#","BS 10","10\"",250.0,406.4,"-",22.23,"-",355.6,12.0,22.23,"-","-","-",6.0,98.46,"M20",16.0,"-"]
[null,"Cast Iron WN 200# BS 10 Size  12\"","Cast Iron WN","200#","BS 10","12\"",300.0,457.2,"-",25.4,"-",406.4,12.0,25.4,"-","-","-",6.0,108.8,"M22",18.0,"-"]
[null,{"$f":"CONCATENATE(C1020,$C$1,D1020,$C$1,E1020,$C$1,$F$1,$C$1,$C$1,$G$2,$C$1,G1020)","v":"WNRF PN 1/2,5 DIN 2630 Size  DN 10"},"WNRF","PN 1/2,5","DIN 2630","1/4\"",10.0,75.0,28.0,12.0,35.0,50.0,4.0,11.0,26.0,2.0,4.0,3.0,59,"M10",8.0,0.34]
[null,"WNRF PN 1/2,5 DIN 2630 Size  DN 15","WNRF","PN 1/2,5","DIN 2630","1/2\"",15.0,80.0,30.0,12.0,40.0,55.0,4.0,11.0,30.0,2.0,4.0,3.0,59,"M10",8.0,0.39]
[null,"WNRF PN 1/2,5 DIN 2630 Size  DN 20","WNRF","PN 1/2,5","DIN 2630","3/4\"",20.0,90.0,32.0,14.0,50.0,65.0,4.0,11.0,38.0,2.0,4.0,3.0,63,"M10",8.0,0.59]
[null,"WNRF PN 1/2,5 DIN 2630 Size  DN 25","WNRF","PN 1/2,5","DIN 2630","1\"",25.0,100.0,35.0,14.0,60.0,75.0,4.0,11.0,42.0,2.0,4.0,3.0,63,"M10",8.0,0.75]
[null,"WNRF PN 1/2,5 DIN 2630 Size  DN 32","WNRF","PN 1/2,5","DIN 2630","1¼\"",32.0,120.0,35.0,14.0,70.0,90.0,4.0,14.0,55.0,2.0,6.0,3.0,67,"M12",10.0,1.05]
[null,"WNRF PN 1/2,5 DIN 2630 Size  DN 40","WNRF","PN 1/2,5","DIN 2630","1½\"",40.0,130.0,38.0,14.0,80.0,100.0,4.0,14.0,62.0,3.0,6.0,3.0,67,"M12",10.0,1.18]
[null,"WNRF PN 1/2,5 DIN 2630 Size  DN 50","WNRF","PN 1/2,5","DIN 2630","2\"",50.0,140.0,38.0,14.0,90.0,110.0,4.0,14.0,74.0,3.0,6.0,4.0,68,"M12",10.0,1.34]
[null,"WNRF PN 1/2,5 DIN 2630 Size  DN 65","WNRF","PN 1/2,5","DIN 2630","2½\"",65.0,160.0,38.0,14.0,110.0,130.0,4.0,14.0,88.0,3.0,6.0,4.0,68,"M12",10.0,1.67]
[null,"WNRF PN 1/2,5 DIN 2630 Size  DN 80","WNRF","PN 1/2,5","DIN 2630","3\"",80.0,190.0,42.0,16.0,128.0,150.0,4.0,18.0,102.0,3.0,8.0,4.0,78,"M16",13.0,2.71]
[null,"WNRF PN 1/2,5 DIN 2630 Size  DN 100","WNRF","PN 1/2,5","DIN 2630","4\"",100.0,210.0,45.0,16.0,148.0,170.0,4.0,18.0,130.0,3.0,8.0,5.0,79,"M16",13.0,3.24]
[null,"WNRF PN 1/2,5 DIN 2630 Size  DN 125","WNRF","PN 1/2,5","DIN 2630","5\"",125.0,240.0,48.0,18.0,178.0,200.0,8.0,18.0,155.0,3.0,8.0,5.0,83,"M16",13.0,4.49]
[null,"WNRF PN 1/2,5 DIN 2630 Size  DN 150","WNRF","PN 1/2,5","DIN 2630","6\"",150.0,265.0,48.0,18.0,202.0,225.0,8.0,18.0,184.0,3.0,10.0,6.0,84,"M16",13.0,5.15]
[null,"WNRF PN 1/2,5 DIN 2630 Size  DN 200","WNRF","PN 1/2,5","DIN 2630","8\"",200.0,320.0,55.0,20.0,258.0,280.0,8.0,18.0,236.0,3.0,10.0,6.0,88,"M16",13.0,7.78]
[null,"WNRF PN 1/2,5 DIN 2630 Size  DN 250","WNRF","PN 1/2,5","DIN 2630","10\"",250.0,375.0,60.0,22.0,312.0,335.0,12.0,18.0,290.0,3.0,12.0,6.0,92,"M16",13.0,10.8]
[null,"WNRF PN 1/2,5 DIN 2630 Size  DN 300","WNRF","PN 1/2,5","DIN 2630","12\"",300.0,440.0,62.0,22.0,365.0,395.0,12.0,22.0,342.0,4.0,12.0,6.0,98,"M20",16.0,14.0]
[null,"WNRF PN 1/2,5 DIN 2630 Size  DN 350","WNRF","PN 1/2,5","DIN 2630","14\"",350.0,490.0,62.0,22.0,415.0,445.0,12.0,22.0,385.0,4.0,12.0,7.0,99,"M20",16.0,18.5]
[null,"WNRF PN 1/2,5 DIN 2630 Size  DN 400","WNRF","PN 1/2,5","DIN 2630","16\"",400.0,540.0,65.0,22.0,465.0,495.0,16.0,22.0,438.0,4.0,12.0,7.0,99,"M20",16.0,21.2]
[null,"WNRF PN 1/2,5 DIN 2630 Size  DN 500","WNRF","PN 1/2,5","DIN 2630","20\"",500.0,645.0,68.0,24.0,570.0,600.0,20.0,22.0,538.0,4.0,12.0,7.0,103,"M20",16.0,28.6]
[null,"WNRF PN 1/2,5 DIN 2630 Size  DN 600","WNRF","PN 1/2,5","DIN 2630","24\"",600.0,755.0,70.0,24.0,670.0,705.0,20.0,26.0,640.0,5.0,12.0,7.0,109,"M24",19.0,31.5]
[null,"WNRF PN 1/2,5 DIN 2630 Size  DN 700","WNRF","PN 1/2,5","DIN 2630","28\"",700.0,860.0,70.0,24.0,775.0,810.0,24.0,26.0,740.0,5.0,12.0,7.0,109,"M24",19.0,37.4]
[null,"WNRF PN 1/2,5 DIN 2630 Size  DN 800","WNRF","PN 1/2,5","DIN 2630","32\"",800.0,975.0,70.0,24.0,880.0,920.0,24.0,30.0,842.0,5.0,12.0,7.0,115,"M27",22.0,46.1]
[null,"WNRF PN 1/2,5 DIN 2630 Size  DN 900","WNRF","PN 1/2,5","DIN 2630","36\"",900.0,1075.0,70.0,26.0,980.0,1020.0,24.0,30.0,942.0,5.0,12.0,7.0,119,"M27",22.0,55.6]
[null,"WNRF PN 1/2,5 DIN 2630 Size  DN 1000","WNRF","PN 1/2,5","DIN 2630","40\"",1000.0,1175.0,70.0,26.0,1080.0,1120.0,28.0,30.0,1045.0,5.0,16.0,7.0,119,"M27",22.0,61.9]
[null,"WNRF PN 1/2,5 DIN 2630 Size  DN 1200","WNRF","PN 1/2,5","DIN 2630","48\"",1200.0,1375.0,70.0,26.0,1280.0,1320.0,32.0,30.0,1245.0,5.0,16.0,7.0,119,"M27",22.0,73.9]
[null,"WNRF PN 1/2,5 DIN 2630 Size  DN 1400","WNRF","PN 1/2,5","DIN 2630","56\"",1400.0,1575.0,70.0,26.0,1480.0,1520.0,36.0,30.0,1445.0,5.0,16.0,7.0,119,"M27",22.0,85.4]
[null,"WNRF PN 1/2,5 DIN 2630 Size  DN 1600","WNRF","PN 1/2,5","DIN 2630","64\"",1600.0,1790.0,80.0,26.0,1690.0,1730.0,40.0,30.0,1645.0,5.0,16.0,7.0,119,"M27",22.0,108.0]
[null,"WNRF PN 1/2,5 DIN 2630 Size  DN 1800","WNRF","PN 1/2,5","DIN 2630","72\"",1800.0,1990.0,80.0,26.0,1890.0,1930.0,44.0,30.0,1845.0,5.0,16.0,7.0,119,"M27",22.0,125.0]
[null,"WNRF PN 1/2,5 DIN 2630 Size  DN 2000","WNRF","PN 1/2,5","DIN 2630","80\"",2000.0,2190.0,80.0,26.0,2090.0,2130.0,48.0,30.0,2045.0,5.0,16.0,7.0,119,"M27",22.0,138.0]
[null,"WNRF PN 1/2,5 DIN 2630 Size  DN 2200","WNRF","PN 1/2,5","DIN 2630","88\"",2200.0,2405.0,90.0,28.0,2295.0,2340.0,52.0,33.0,2248.0,6.0,18.0,7.0,127,"M30",24.0,172.0]
[null,"WNRF PN 1/2,5 DIN 2630 Size  DN 2400","WNRF","PN 1/2,5","DIN 2630","96\"",2400.0,2605.0,90.0,28.0,2495.0,2540.0,56.0,33.0,2448.0,6.0,18.0,7.0,127,"M30",24.0,196.0]
[null,"WNRF PN 1/2,5 DIN 2630 Size  DN 2600","WNRF","PN 1/2,5","DIN 2630","104\"",2600.0,2805.0,90.0,28.0,2695.0,2740.0,60.0,33.0,2648.0,6.0,18.0,7.0,127,"M30",24.0,203.0]
[null,"WNRF PN 1/2,5 DIN 2630 Size  DN 2800","WNRF","PN 1/2,5","DIN 2630","112\"",2800.0,3030.0,90.0,30.0,2910.0,2960.0,64.0,36.0,2848.0,6.0,18.0,7.0,135,"M33",26.0,259.0]
[null,"WNRF PN 1/2,5 DIN 2630 Size  DN 3000","WNRF","PN 1/2,5","DIN 2630","120\"",3000.0,3230.0,90.0,30.0,3110.0,3160.0,68.0,36.0,3050.0,6.0,18.0,7.0,135,"M33",26.0,292.0]
[null,"WNRF PN 1/2,5 DIN 2630 Size  DN 3200","WNRF","PN 1/2,5","DIN 2630","128\"",3200.0,3430.0,90.0,30.0,3310.0,3360.0,72.0,36.0,3250.0,6.0,20.0,7.0,135,"M33",26.0,294.0]
[null,"WNRF PN 1/2,5 DIN 2630 Size  DN 3400","WNRF","PN 1/2,5","DIN 2630","136\"",3400.0,3630.0,95.0,32.0,3510.0,3560.0,76.0,36.0,3450.0,6.0,20.0,7.0,139,"M33",26.0,331.0]
[null,"WNRF PN 1/2,5 DIN 2630 Size  DN 3600","WNRF","PN 1/2,5","DIN 2630","144\"",3600.0,3840.0,100.0,32.0,3720.0,3770.0,80.0,36.0,3652.0,6.0,20.0,7.0,139,"M33",26.0,402.0]
[null,"WNRF PN 1/2,5 DIN 2630 Size  DN 3800","WNRF","PN 1/2,5","DIN 2630","152\"",3800.0,4045.0,100.0,34.0,3920.0,3970.0,80.0,39.0,3852.0,6.0,20.0,7.0,149,"M36",29.0,416.0]
[null,"WNRF PN 1/2,5 DIN 2630 Size  DN 4000","WNRF","PN 1/2,5","DIN 2630","160\"",4000.0,4245.0,100.0,34.0,4120.0,4170.0,84.0,39.0,4052.0,6.0,20.0,7.0,149,"M36",29.0,437.0]
[null,"WNRF PN 6 DIN 2631 Size  DN 10","WNRF","PN 6","DIN 2631","1/4\"",10.0,75.0,28.0,12.0,35.0,50.0,4.0,11.0,26.0,2.0,4.0,3.0,59,"M10",8.0,0.34]
[null,"WNRF PN 6 DIN 2631 Size  DN 15","WNRF","PN 6","DIN 2631","1/2\"",15.0,80.0,30.0,12.0,40.0,55.0,4.0,11.0,30.0,2.0,4.0,3.0,59,"M10",8.0,0.39]
[null,"WNRF PN 6 DIN 2631 Size  DN 20","WNRF","PN 6","DIN 2631","3/4\"",20.0,90.0,32.0,14.0,50.0,65.0,4.0,11.0,38.0,2.0,4.0,3.0,63,"M10",8.0,0.59]
[null,"WNRF PN 6 DIN 2631 Size  DN 25","WNRF","PN 6","DIN 2631","1\"",25.0,100.0,35.0,14.0,60.0,75.0,4.0,11.0,42.0,2.0,4.0,3.0,63,"M10",8.0,0.75]
[null,"WNRF PN 6 DIN 2631 Size  DN 32","WNRF","PN 6","DIN 2631","1¼\"",32.0,120.0,35.0,14.0,70.0,90.0,4.0,14.0,55.0,2.0,6.0,3.0,67,"M12",10.0,1.05]
[null,"WNRF PN 6 DIN 2631 Size  DN 40","WNRF","PN 6","DIN 2631","1½\"",40.0,130.0,38.0,14.0,80.0,100.0,4.0,14.0,62.0,3.0,6.0,3.0,67,"M12",10.0,1.18]
[null,"WNRF PN 6 DIN 2631 Size  DN 50","WNRF","PN 6","DIN 2631","2\"",50.0,140.0,38.0,14.0,90.0,110.0,4.0,14.0,74.0,3.0,6.0,4.0,68,"M12",10.0,1.34]
[null,"WNRF PN 6 DIN 2631 Size  DN 65","WNRF","PN 6","DIN 2631","2½\"",65.0,160.0,38.0,14.0,110.0,130.0,4.0,14.0,88.0,3.0,6.0,4.0,68,"M12",10.0,1.67]
[null,"WNRF PN 6 DIN 2631 Size  DN 80","WNRF","PN 6","DIN 2631","3\"",80.0,190.0,42.0,16.0,128.0,150.0,4.0,18.0,102.0,3.0,8.0,4.0,78,"M16",13.0,2.71]
[null,"WNRF PN 6 DIN 2631 Size  DN 100","WNRF","PN 6","DIN 2631","4\"",100.0,210.0,45.0,16.0,148.0,170.0,4.0,18.0,130.0,3.0,8.0,5.0,79,"M16",13.0,3.24]
[null,"WNRF PN 6 DIN 2631 Size  DN 125","WNRF","PN 6","DIN 2631","5\"",125.0,240.0,48.0,18.0,178.0,200.0,8.0,18.0,155.0,3.0,8.0,5.0,83,"M16",13.0,4.49]
[null,"WNRF PN 6 DIN 2631 Size  DN 150","WNRF","PN 6","DIN 2631","6\"",150.0,265.0,48.0,18.0,202.0,225.0,8.0,18.0,184.0,3.0,10.0,6.0,84,"M16",13.0,5.15]
[null,"WNRF PN 6 DIN 2631 Size  DN 200","WNRF","PN 6","DIN 2631","8\"",200.0,320.0,55.0,20.0,258.0,280.0,8.0,18.0,236.0,3.0,10.0,6.0,88,"M16",13.0,7.78]
[null,"WNRF PN 6 DIN 2631 Size  DN 250","WNRF","PN 6","DIN 2631","10\"",250.0,375.0,60.0,22.0,312.0,335.0,12.0,18.0,290.0,3.0,12.0,6.0,92,"M16",13.0,10.8]
[null,"WNRF PN 6 DIN 2631 Size  DN 300","WNRF","PN 6","DIN 2631","12\"",300.0,440.0,62.0,22.0,365.0,395.0,12.0,22.0,342.0,4.0,12.0,6.0,98,"M20",16.0,14.0]
[null,"WNRF PN 6 DIN 2631 Size  DN 350","WNRF","PN 6","DIN 2631","14\"",350.0,490.0,62.0,22.0,415.0,445.0,12.0,22.0,385.0,4.0,12.0,7.0,99,"M20",16.0,18.5]
[null,"WNRF PN 6 DIN 2631 Size  DN 400","WNRF","PN 6","DIN 2631","16\"",400.0,540.0,65.0,22.0,465.0,495.0,16.0,22.0,438.0,4.0,12.0,7.0,99,"M20",16.0,21.2]
[null,"WNRF PN 6 DIN 2631 Size  DN 500","WNRF","PN 6","DIN 2631","20\"",500.0,645.0,68.0,24.0,570.0,600.0,20.0,22.0,538.0,4.0,12.0,7.0,103,"M20",16.0,28.6]
[null,"WNRF PN 6 DIN 2631 Size  DN 600","WNRF","PN 6","DIN 2631","24\"",600.0,755.0,70.0,24.0,670.0,705.0,20.0,26.0,640.0,5.0,12.0,7.0,109,"M24",19.0,31.5]
[null,"WNRF PN 6 DIN 2631 Size  DN 700","WNRF","PN 6","DIN 2631","28\"",700.0,860.0,70.0,24.0,775.0,810.0,24.0,26.0,740.0,5.0,12.0,7.0,109,"M24",19.0,37.4]
[null,"WNRF PN 6 DIN 2631 Size  DN 800","WNRF","PN 6","DIN 2631","32\"",800.0,975.0,70.0,24.0,880.0,920.0,24.0,30.0,842.0,5.0,12.0,7.0,115,"M27",22.0,46.1]
[null,"WNRF PN 6 DIN 2631 Size  DN 900","WNRF","PN 6","DIN 2631","36\"",900.0,1075.0,70.0,26.0,980.0,1020.0,24.0,30.0,942.0,5.0,12.0,7.0,119,"M27",22.0,55.6]
[null,"WNRF PN 6 DIN 2631 Size  DN 1000","WNRF","PN 6","DIN 2631","40\"",1000.0,1175.0,70.0,26.0,1080.0,1120.0,28.0,30.0,1045.0,5.0,16.0,7.0,119,"M27",22.0,61.9]
[null,"WNRF PN 6 DIN 2631 Size  DN 1200","WNRF","PN 6","DIN 2631","48\"",1200.0,1405.0,90.0,28.0,1295.0,1340.0,32.0,33.0,1248.0,5.0,16.0,7.0,127,"M30",24.0,100.0]
[null,"WNRF PN 6 DIN 2631 Size  DN 1400","WNRF","PN 6","DIN 2631","56\"",1400.0,1630.0,90.0,32.0,1510.0,1560.0,36.0,36.0,1452.0,5.0,16.0,7.0,139,"M33",26.0,149.0]
[null,"WNRF PN 6 DIN 2631 Size  DN 1600","WNRF","PN 6","DIN 2631","64\"",1600.0,1830.0,90.0,34.0,1710.0,1760.0,40.0,36.0,1655.0,5.0,16.0,7.0,143,"M33",26.0,180.0]
[null,"WNRF PN 6 DIN 2631 Size  DN 1800","WNRF","PN 6","DIN 2631","72\"",1800.0,2045.0,100.0,36.0,1920.0,1970.0,44.0,39.0,1855.0,5.0,16.0,7.0,153,"M36",29.0,225.0]
[null,"WNRF PN 6 DIN 2631 Size  DN 2000","WNRF","PN 6","DIN 2631","80\"",2000.0,2265.0,110.0,38.0,2125.0,2180.0,48.0,42.0,2058.0,5.0,16.0,7.0,161,"M39",31.0,295.0]
[null,"WNRF PN 6 DIN 2631 Size  DN 2200","WNRF","PN 6","DIN 2631","88\"",2200.0,2475.0,115.0,42.0,2335.0,2390.0,52.0,42.0,2260.0,6.0,18.0,7.0,169,"M39",31.0,361.0]
[null,"WNRF PN 6 DIN 2631 Size  DN 2400","WNRF","PN 6","DIN 2631","96\"",2400.0,2685.0,125.0,44.0,2545.0,2600.0,56.0,42.0,2462.0,6.0,18.0,7.0,173,"M39",31.0,415.0]
[null,"WNRF PN 6 DIN 2631 Size  DN 2600","WNRF","PN 6","DIN 2631","104\"",2600.0,2905.0,130.0,46.0,2750.0,2810.0,60.0,48.0,2665.0,6.0,18.0,7.0,187,"M45",36.0,530.0]
[null,"WNRF PN 6 DIN 2631 Size  DN 2800","WNRF","PN 6","DIN 2631","112\"",2800.0,3115.0,135.0,48.0,2960.0,3020.0,64.0,48.0,2865.0,6.0,18.0,7.0,191,"M45",36.0,643.0]
[null,"WNRF PN 6 DIN 2631 Size  DN 3000","WNRF","PN 6","DIN 2631","120\"",3000.0,3315.0,140.0,50.0,3160.0,3220.0,68.0,48.0,3068.0,6.0,18.0,7.0,195,"M45",36.0,777.0]
[null,"WNRF PN 6 DIN 2631 Size  DN 3200","WNRF","PN 6","DIN 2631","128\"",3200.0,3525.0,150.0,54.0,3370.0,3430.0,72.0,48.0,3272.0,6.0,20.0,7.0,203,"M45",36.0,851.0]
[null,"WNRF PN 6 DIN 2631 Size  DN 3400","WNRF","PN 6","DIN 2631","136\"",3400.0,3735.0,160.0,56.0,3580.0,3640.0,76.0,48.0,3475.0,6.0,20.0,7.0,207,"M45",36.0,993.0]
[null,"WNRF PN 6 DIN 2631 Size  DN 3600","WNRF","PN 6","DIN 2631","144\"",3600.0,3970.0,165.0,60.0,3790.0,3860.0,80.0,56.0,3678.0,6.0,20.0,7.0,227,"M52",42.0,1001.0]
[null,"WNRF PN 10 DIN 2632 Size  DN 10","WNRF","PN 10","DIN 2632","1/4\"",10.0,90.0,35.0,14.0,40.0,60.0,4.0,14.0,28.0,2.0,4.0,3.0,67,"M12",10.0,0.58]
[null,"WNRF PN 10 DIN 2632 Size  DN 15","WNRF","PN 10","DIN 2632","1/2\"",15.0,95.0,35.0,14.0,45.0,65.0,4.0,14.0,32.0,2.0,4.0,3.0,67,"M12",10.0,0.648]
[null,"WNRF PN 10 DIN 2632 Size  DN 20","WNRF","PN 10","DIN 2632","3/4\"",20.0,105.0,38.0,16.0,58.0,75.0,4.0,14.0,40.0,2.0,4.0,3.0,71,"M12",10.0,0.952]
[null,"WNRF PN 10 DIN 2632 Size  DN 25","WNRF","PN 10","DIN 2632","1\"",25.0,115.0,38.0,16.0,68.0,85.0,4.0,14.0,45.0,2.0,4.0,3.0,71,"M12",10.0,1.14]
[null,"WNRF PN 10 DIN 2632 Size  DN 32","WNRF","PN 10","DIN 2632","1¼\"",32.0,140.0,40.0,16.0,78.0,100.0,4.0,18.0,56.0,2.0,6.0,3.0,77,"M16",13.0,1.69]
[null,"WNRF PN 10 DIN 2632 Size  DN 40","WNRF","PN 10","DIN 2632","1½\"",40.0,150.0,42.0,16.0,88.0,110.0,4.0,18.0,64.0,3.0,6.0,3.0,77,"M16",13.0,1.86]
[null,"WNRF PN 10 DIN 2632 Size  DN 50","WNRF","PN 10","DIN 2632","2\"",50.0,165.0,45.0,18.0,102.0,125.0,4.0,18.0,75.0,3.0,6.0,4.0,82,"M16",13.0,2.53]
[null,"WNRF PN 10 DIN 2632 Size  DN 65","WNRF","PN 10","DIN 2632","2½\"",65.0,185.0,45.0,18.0,122.0,145.0,4.0,18.0,90.0,3.0,6.0,4.0,82,"M16",13.0,3.06]
[null,"WNRF PN 10 DIN 2632 Size  DN 80","WNRF","PN 10","DIN 2632","3\"",80.0,200.0,50.0,20.0,138.0,160.0,8.0,18.0,105.0,3.0,8.0,4.0,86,"M16",13.0,3.7]
[null,"WNRF PN 10 DIN 2632 Size  DN 100","WNRF","PN 10","DIN 2632","4\"",100.0,220.0,52.0,20.0,158.0,180.0,8.0,18.0,131.0,3.0,8.0,5.0,87,"M16",13.0,4.62]
[null,"WNRF PN 10 DIN 2632 Size  DN 125","WNRF","PN 10","DIN 2632","5\"",125.0,250.0,55.0,22.0,188.0,210.0,8.0,18.0,156.0,3.0,8.0,5.0,91,"M16",13.0,6.3]
[null,"WNRF PN 10 DIN 2632 Size  DN 150","WNRF","PN 10","DIN 2632","6\"",150.0,285.0,55.0,22.0,212.0,240.0,8.0,22.0,184.0,3.0,10.0,6.0,98,"M20",16.0,7.75]
[null,"WNRF PN 10 DIN 2632 Size  DN 200","WNRF","PN 10","DIN 2632","8\"",200.0,340.0,62.0,24.0,268.0,295.0,8.0,22.0,235.0,3.0,10.0,6.0,102,"M20",16.0,11.3]
[null,"WNRF PN 10 DIN 2632 Size  DN 250","WNRF","PN 10","DIN 2632","10\"",250.0,395.0,68.0,26.0,320.0,350.0,12.0,22.0,292.0,3.0,12.0,6.0,106,"M20",16.0,14.7]
[null,"WNRF PN 10 DIN 2632 Size  DN 300","WNRF","PN 10","DIN 2632","12\"",300.0,445.0,68.0,26.0,370.0,400.0,12.0,22.0,344.0,4.0,12.0,6.0,106,"M20",16.0,17.4]
[null,"WNRF PN 10 DIN 2632 Size  DN 350","WNRF","PN 10","DIN 2632","14\"",350.0,505.0,68.0,26.0,430.0,460.0,16.0,22.0,385.0,4.0,12.0,7.0,107,"M20",16.0,23.6]
[null,"WNRF PN 10 DIN 2632 Size  DN 400","WNRF","PN 10","DIN 2632","16\"",400.0,565.0,72.0,26.0,482.0,515.0,16.0,26.0,440.0,4.0,12.0,7.0,113,"M24",19.0,28.6]
[null,"WNRF PN 10 DIN 2632 Size  DN 500","WNRF","PN 10","DIN 2632","20\"",500.0,670.0,75.0,28.0,585.0,620.0,20.0,26.0,542.0,4.0,12.0,7.0,117,"M24",19.0,38.1]
[null,"WNRF PN 10 DIN 2632 Size  DN 600","WNRF","PN 10","DIN 2632","24\"",600.0,780.0,80.0,28.0,685.0,725.0,20.0,30.0,642.0,5.0,12.0,7.0,123,"M27",22.0,44.6]
[null,"WNRF PN 10 DIN 2632 Size  DN 700","WNRF","PN 10","DIN 2632","28\"",700.0,895.0,80.0,30.0,800.0,840.0,24.0,30.0,745.0,5.0,12.0,7.0,127,"M27",22.0,62.4]
[null,"WNRF PN 10 DIN 2632 Size  DN 800","WNRF","PN 10","DIN 2632","32\"",800.0,1015.0,90.0,32.0,905.0,950.0,24.0,33.0,850.0,5.0,12.0,7.0,135,"M30",24.0,84.1]
[null,"WNRF PN 10 DIN 2632 Size  DN 900","WNRF","PN 10","DIN 2632","36\"",900.0,1115.0,95.0,34.0,1005.0,1050.0,28.0,33.0,950.0,5.0,12.0,7.0,139,"M30",24.0,98.5]
[null,"WNRF PN 10 DIN 2632 Size  DN 1000","WNRF","PN 10","DIN 2632","40\"",1000.0,1230.0,95.0,34.0,1110.0,1160.0,28.0,36.0,1052.0,5.0,16.0,7.0,143,"M33",26.0,115.0]
[null,"WNRF PN 10 DIN 2632 Size  DN 1200","WNRF","PN 10","DIN 2632","48\"",1200.0,1455.0,115.0,38.0,1330.0,1380.0,32.0,39.0,1255.0,5.0,16.0,7.0,157,"M36",29.0,182.0]
[null,"WNRF PN 10 DIN 2632 Size  DN 1400","WNRF","PN 10","DIN 2632","56\"",1400.0,1675.0,120.0,42.0,1535.0,1590.0,36.0,42.0,1460.0,5.0,16.0,7.0,169,"M39",31.0,248.0]
[null,"WNRF PN 10 DIN 2632 Size  DN 1600","WNRF","PN 10","DIN 2632","64\"",1600.0,1915.0,130.0,46.0,1760.0,1820.0,40.0,48.0,1665.0,5.0,16.0,7.0,187,"M45",36.0,347.0]
[null,"WNRF PN 10 DIN 2632 Size  DN 1800","WNRF","PN 10","DIN 2632","72\"",1800.0,2115.0,140.0,50.0,1960.0,2020.0,44.0,48.0,1868.0,5.0,16.0,7.0,195,"M45",36.0,430.0]
[null,"WNRF PN 10 DIN 2632 Size  DN 2000","WNRF","PN 10","DIN 2632","80\"",2000.0,2325.0,150.0,54.0,2170.0,2230.0,48.0,48.0,2072.0,5.0,16.0,7.0,203,"M45",36.0,539.0]
[null,"WNRF PN 10 DIN 2632 Size  DN 2200","WNRF","PN 10","DIN 2632","88\"",2200.0,2550.0,160.0,58.0,2370.0,2440.0,52.0,56.0,2275.0,6.0,18.0,7.0,223,"M52",42.0,658.0]
[null,"WNRF PN 10 DIN 2632 Size  DN 2400","WNRF","PN 10","DIN 2632","96\"",2400.0,2760.0,170.0,62.0,2570.0,2650.0,56.0,56.0,2478.0,6.0,18.0,7.0,231,"M52",42.0,825.0]
[null,"WNRF PN 10 DIN 2632 Size  DN 2600","WNRF","PN 10","DIN 2632","104\"",2600.0,2960.0,180.0,66.0,2780.0,2850.0,60.0,56.0,2680.0,6.0,18.0,7.0,239,"M52",42.0,979.0]
[null,"WNRF PN 10 DIN 2632 Size  DN 2800","WNRF","PN 10","DIN 2632","112\"",2800.0,3180.0,190.0,70.0,3000.0,3070.0,64.0,56.0,2882.0,6.0,18.0,7.0,247,"M52",42.0,1156.0]
[null,"WNRF PN 10 DIN 2632 Size  DN 3000","WNRF","PN 10","DIN 2632","120\"",3000.0,3405.0,200.0,75.0,3210.0,3290.0,68.0,62.0,3085.0,6.0,18.0,7.0,263,"M56",45.0,1402.0]
[null,"WNRF PN 16 DIN 2633 Size  DN 10","WNRF","PN 16","DIN 2633","1/4\"",10.0,90.0,35.0,14.0,40.0,60.0,4.0,14.0,28.0,2.0,4.0,3.0,67,"M12",10.0,0.58]
[null,"WNRF PN 16 DIN 2633 Size  DN 15","WNRF","PN 16","DIN 2633","1/2\"",15.0,95.0,35.0,14.0,45.0,65.0,4.0,14.0,32.0,2.0,4.0,3.0,67,"M12",10.0,0.648]
[null,"WNRF PN 16 DIN 2633 Size  DN 20","WNRF","PN 16","DIN 2633","3/4\"",20.0,105.0,38.0,16.0,58.0,75.0,4.0,14.0,40.0,2.0,4.0,3.0,71,"M12",10.0,0.952]
[null,"WNRF PN 16 DIN 2633 Size  DN 25","WNRF","PN 16","DIN 2633","1\"",25.0,115.0,38.0,16.0,68.0,85.0,4.0,14.0,45.0,2.0,4.0,3.0,71,"M12",10.0,1.14]
[null,"WNRF PN 16 DIN 2633 Size  DN 32","WNRF","PN 16","DIN 2633","1¼\"",32.0,140.0,40.0,16.0,78.0,100.0,4.0,18.0,56.0,2.0,6.0,3.0,77,"M16",13.0,1.69]
[null,"WNRF PN 16 DIN 2633 Size  DN 40","WNRF","PN 16","DIN 2633","1½\"",40.0,150.0,42.0,16.0,88.0,110.0,4.0,18.0,64.0,3.0,6.0,3.0,77,"M16",13.0,1.86]
[null,"WNRF PN 16 DIN 2633 Size  DN 50","WNRF","PN 16","DIN 2633","2\"",50.0,165.0,45.0,18.0,102.0,125.0,4.0,18.0,75.0,3.0,6.0,4.0,82,"M16",13.0,2.53]
[null,"WNRF PN 16 DIN 2633 Size  DN 65","WNRF","PN 16","DIN 2633","2½\"",65.0,185.0,45.0,18.0,122.0,145.0,4.0,18.0,90.0,3.0,6.0,4.0,82,"M16",13.0,3.06]
[null,"WNRF PN 16 DIN 2633 Size  DN 80","WNRF","PN 16","DIN 2633","3\"",80.0,200.0,50.0,20.0,138.0,160.0,8.0,18.0,105.0,3.0,8.0,4.0,86,"M16",13.0,3.7]
[null,"WNRF PN 16 DIN 2633 Size  DN 100","WNRF","PN 16","DIN 2633","4\"",100.0,220.0,52.0,20.0,158.0,180.0,8.0,18.0,131.0,3.0,8.0,5.0,87,"M16",13.0,4.62]
[null,"WNRF PN 16 DIN 2633 Size  DN 125","WNRF","PN 16","DIN 2633","5\"",125.0,250.0,55.0,22.0,188.0,210.0,8.0,18.0,156.0,3.0,8.0,5.0,91,"M16",13.0,6.3]
[null,"WNRF PN 16 DIN 2633 Size  DN 150","WNRF","PN 16","DIN 2633","6\"",150.0,285.0,55.0,22.0,212.0,240.0,8.0,22.0,184.0,3.0,10.0,6.0,98,"M20",16.0,7.75]
[null,"WNRF PN 16 DIN 2633 Size  DN 175","WNRF","PN 16","DIN 2633","-",175.0,315.0,60.0,24.0,242.0,270.0,8.0,22.0,210.0,3.0,10.0,6.0,102,"M20",16.0,9.85]
[null,"WNRF PN 16 DIN 2633 Size  DN 200","WNRF","PN 16","DIN 2633","8\"",200.0,340.0,62.0,24.0,268.0,295.0,12.0,22.0,235.0,3.0,10.0,6.0,102,"M20",16.0,11.0]
[null,"WNRF PN 16 DIN 2633 Size  DN 250","WNRF","PN 16","DIN 2633","10\"",250.0,405.0,70.0,26.0,320.0,355.0,12.0,26.0,292.0,3.0,12.0,6.0,112,"M24",19.0,15.6]
[null,"WNRF PN 16 DIN 2633 Size  DN 300","WNRF","PN 16","DIN 2633","12\"",300.0,460.0,78.0,28.0,378.0,410.0,12.0,26.0,344.0,4.0,12.0,6.0,116,"M24",19.0,22.0]
[null,"WNRF PN 16 DIN 2633 Size  DN 350","WNRF","PN 16","DIN 2633","14\"",350.0,520.0,82.0,30.0,438.0,470.0,16.0,26.0,390.0,4.0,12.0,7.0,121,"M24",19.0,31.2]
[null,"WNRF PN 16 DIN 2633 Size  DN 400","WNRF","PN 16","DIN 2633","16\"",400.0,580.0,85.0,32.0,490.0,525.0,16.0,30.0,445.0,4.0,12.0,7.0,131,"M27",22.0,39.3]
[null,"WNRF PN 16 DIN 2633 Size  DN 500","WNRF","PN 16","DIN 2633","20\"",500.0,715.0,90.0,34.0,610.0,650.0,20.0,33.0,548.0,4.0,12.0,7.0,139,"M30",24.0,61.0]
[null,"WNRF PN 16 DIN 2633 Size  DN 600","WNRF","PN 16","DIN 2633","24\"",600.0,840.0,95.0,36.0,725.0,770.0,20.0,36.0,652.0,5.0,12.0,7.0,147,"M33",26.0,75.4]
[null,"WNRF PN 16 DIN 2633 Size  DN 700","WNRF","PN 16","DIN 2633","28\"",700.0,910.0,100.0,36.0,795.0,840.0,24.0,36.0,755.0,5.0,12.0,7.0,147,"M33",26.0,77.0]
[null,"WNRF PN 16 DIN 2633 Size  DN 800","WNRF","PN 16","DIN 2633","32\"",800.0,1025.0,105.0,38.0,900.0,950.0,24.0,39.0,855.0,5.0,12.0,7.0,157,"M36",29.0,101.0]
[null,"WNRF PN 16 DIN 2633 Size  DN 900","WNRF","PN 16","DIN 2633","36\"",900.0,1125.0,110.0,40.0,1000.0,1050.0,28.0,39.0,955.0,5.0,12.0,7.0,161,"M36",29.0,122.0]
[null,"WNRF PN 16 DIN 2633 Size  DN 1000","WNRF","PN 16","DIN 2633","40\"",1000.0,1255.0,120.0,42.0,1115.0,1170.0,28.0,42.0,1058.0,5.0,16.0,7.0,169,"M39",31.0,162.0]
[null,"WNRF PN 16 DIN 2633 Size  DN 1200","WNRF","PN 16","DIN 2633","48\"",1200.0,1485.0,130.0,48.0,1330.0,1390.0,32.0,48.0,1262.0,5.0,16.0,7.0,191,"M45",36.0,243.0]
[null,"WNRF PN 16 DIN 2633 Size  DN 1400","WNRF","PN 16","DIN 2633","56\"",1400.0,1685.0,145.0,52.0,1530.0,1590.0,36.0,48.0,1465.0,5.0,16.0,7.0,199,"M45",36.0,323.0]
[null,"WNRF PN 16 DIN 2633 Size  DN 1600","WNRF","PN 16","DIN 2633","64\"",1600.0,1930.0,160.0,58.0,1750.0,1820.0,40.0,56.0,1668.0,5.0,16.0,7.0,223,"M52",42.0,479.0]
[null,"WNRF PN 16 DIN 2633 Size  DN 1800","WNRF","PN 16","DIN 2633","72\"",1800.0,2130.0,170.0,62.0,1950.0,2020.0,44.0,56.0,1870.0,5.0,16.0,7.0,231,"M52",42.0,599.0]
[null,"WNRF PN 16 DIN 2633 Size  DN 2000","WNRF","PN 16","DIN 2633","80\"",2000.0,2345.0,180.0,66.0,2150.0,2230.0,48.0,62.0,2072.0,5.0,16.0,7.0,245,"M56",45.0,719.0]
[null,"WNRF PN 25 DIN 2634 Size  DN 10","WNRF","PN 25","DIN 2634","1/4\"",10.0,90.0,35.0,16.0,40.0,60.0,4.0,14.0,28.0,2.0,4.0,3.0,71,"M12",10.0,0.661]
[null,"WNRF PN 25 DIN 2634 Size  DN 15","WNRF","PN 25","DIN 2634","1/2\"",15.0,95.0,38.0,16.0,45.0,65.0,4.0,14.0,32.0,2.0,4.0,3.0,71,"M12",10.0,0.746]
[null,"WNRF PN 25 DIN 2634 Size  DN 20","WNRF","PN 25","DIN 2634","3/4\"",20.0,105.0,40.0,18.0,58.0,75.0,4.0,14.0,40.0,2.0,4.0,3.0,75,"M12",10.0,1.06]
[null,"WNRF PN 25 DIN 2634 Size  DN 25","WNRF","PN 25","DIN 2634","1\"",25.0,115.0,40.0,18.0,68.0,85.0,4.0,14.0,46.0,2.0,4.0,3.0,75,"M12",10.0,1.29]
[null,"WNRF PN 25 DIN 2634 Size  DN 32","WNRF","PN 25","DIN 2634","1¼\"",32.0,140.0,42.0,18.0,78.0,100.0,4.0,18.0,56.0,2.0,6.0,3.0,81,"M16",13.0,1.88]
[null,"WNRF PN 25 DIN 2634 Size  DN 40","WNRF","PN 25","DIN 2634","1½\"",40.0,150.0,45.0,18.0,88.0,110.0,4.0,18.0,64.0,3.0,6.0,3.0,81,"M16",13.0,2.33]
[null,"WNRF PN 25 DIN 2634 Size  DN 50","WNRF","PN 25","DIN 2634","2\"",50.0,165.0,48.0,20.0,102.0,125.0,4.0,18.0,75.0,3.0,6.0,4.0,86,"M16",13.0,2.82]
[null,"WNRF PN 25 DIN 2634 Size  DN 65","WNRF","PN 25","DIN 2634","2½\"",65.0,185.0,52.0,22.0,122.0,145.0,8.0,18.0,90.0,3.0,6.0,4.0,90,"M16",13.0,3.74]
[null,"WNRF PN 25 DIN 2634 Size  DN 80","WNRF","PN 25","DIN 2634","3\"",80.0,200.0,58.0,24.0,138.0,160.0,8.0,18.0,105.0,3.0,8.0,4.0,94,"M16",13.0,4.75]
[null,"WNRF PN 25 DIN 2634 Size  DN 100","WNRF","PN 25","DIN 2634","4\"",100.0,235.0,65.0,24.0,162.0,190.0,8.0,22.0,134.0,3.0,8.0,5.0,101,"M20",16.0,6.52]
[null,"WNRF PN 25 DIN 2634 Size  DN 125","WNRF","PN 25","DIN 2634","5\"",125.0,270.0,68.0,26.0,188.0,220.0,8.0,26.0,162.0,3.0,8.0,5.0,111,"M24",19.0,9.07]
[null,"WNRF PN 25 DIN 2634 Size  DN 150","WNRF","PN 25","DIN 2634","6\"",150.0,300.0,75.0,28.0,218.0,250.0,8.0,26.0,192.0,3.0,10.0,6.0,116,"M24",19.0,11.8]
[null,"WNRF PN 25 DIN 2634 Size  DN 175","WNRF","PN 25","DIN 2634","-",175.0,330.0,75.0,28.0,248.0,280.0,12.0,26.0,218.0,3.0,10.0,6.0,116,"M24",19.0,13.4]
[null,"WNRF PN 25 DIN 2634 Size  DN 200","WNRF","PN 25","DIN 2634","8\"",200.0,360.0,80.0,30.0,278.0,310.0,12.0,26.0,244.0,3.0,10.0,6.0,120,"M24",19.0,17.0]
[null,"WNRF PN 25 DIN 2634 Size  DN 250","WNRF","PN 25","DIN 2634","10\"",250.0,425.0,88.0,32.0,335.0,370.0,12.0,30.0,298.0,3.0,12.0,6.0,130,"M27",22.0,24.4]
[null,"WNRF PN 25 DIN 2634 Size  DN 300","WNRF","PN 25","DIN 2634","12\"",300.0,485.0,92.0,34.0,395.0,430.0,16.0,30.0,352.0,4.0,12.0,6.0,134,"M27",22.0,31.2]
[null,"WNRF PN 25 DIN 2634 Size  DN 350","WNRF","PN 25","DIN 2634","14\"",350.0,555.0,100.0,38.0,450.0,490.0,16.0,33.0,398.0,4.0,12.0,7.0,147,"M30",24.0,47.2]
[null,"WNRF PN 25 DIN 2634 Size  DN 400","WNRF","PN 25","DIN 2634","16\"",400.0,620.0,110.0,40.0,505.0,550.0,16.0,36.0,452.0,4.0,12.0,7.0,155,"M33",26.0,61.7]
[null,"WNRF PN 25 DIN 2634 Size  DN 500","WNRF","PN 25","DIN 2634","20\"",500.0,730.0,125.0,44.0,615.0,660.0,20.0,36.0,558.0,4.0,12.0,7.0,163,"M33",26.0,89.6]
[null,"WNRF PN 25 DIN 2634 Size  DN 600","WNRF","PN 25","DIN 2634","24\"",600.0,845.0,125.0,46.0,720.0,770.0,20.0,39.0,660.0,5.0,12.0,7.0,173,"M36",29.0,104.0]
[null,"WNRF PN 25 DIN 2634 Size  DN 700","WNRF","PN 25","DIN 2634","28\"",700.0,960.0,125.0,46.0,820.0,875.0,24.0,42.0,760.0,5.0,12.0,7.0,177,"M39",31.0,136.0]
[null,"WNRF PN 25 DIN 2634 Size  DN 800","WNRF","PN 25","DIN 2634","32\"",800.0,1085.0,135.0,50.0,930.0,990.0,24.0,48.0,865.0,5.0,12.0,7.0,195,"M45",36.0,186.0]
[null,"WNRF PN 25 DIN 2634 Size  DN 900","WNRF","PN 25","DIN 2634","36\"",900.0,1185.0,145.0,54.0,1030.0,1090.0,28.0,48.0,968.0,5.0,12.0,7.0,203,"M45",36.0,236.0]
[null,"WNRF PN 25 DIN 2634 Size  DN 1000","WNRF","PN 25","DIN 2634","40\"",1000.0,1320.0,155.0,58.0,1140.0,1210.0,28.0,56.0,1070.0,5.0,16.0,7.0,223,"M52",42.0,307.0]
[null,"WNRF PN 40 DIN 2635 Size  DN 10","WNRF","PN 40","DIN 2635","1/4\"",10.0,90.0,35.0,16.0,40.0,60.0,4.0,14.0,28.0,2.0,4.0,3.0,71,"M12",10.0,0.661]
[null,"WNRF PN 40 DIN 2635 Size  DN 15","WNRF","PN 40","DIN 2635","1/2\"",15.0,95.0,38.0,16.0,45.0,65.0,4.0,14.0,32.0,2.0,4.0,3.0,71,"M12",10.0,0.746]
[null,"WNRF PN 40 DIN 2635 Size  DN 20","WNRF","PN 40","DIN 2635","3/4\"",20.0,105.0,40.0,18.0,58.0,75.0,4.0,14.0,40.0,2.0,4.0,3.0,75,"M12",10.0,1.06]
[null,"WNRF PN 40 DIN 2635 Size  DN 25","WNRF","PN 40","DIN 2635","1\"",25.0,115.0,40.0,18.0,68.0,85.0,4.0,14.0,46.0,2.0,4.0,3.0,75,"M12",10.0,1.29]
[null,"WNRF PN 40 DIN 2635 Size  DN 32","WNRF","PN 40","DIN 2635","1¼\"",32.0,140.0,42.0,18.0,78.0,100.0,4.0,18.0,56.0,2.0,6.0,3.0,81,"M16",13.0,1.88]
[null,"WNRF PN 40 DIN 2635 Size  DN 40","WNRF","PN 40","DIN 2635","1½\"",40.0,150.0,45.0,18.0,88.0,110.0,4.0,18.0,64.0,3.0,6.0,3.0,81,"M16",13.0,2.33]
[null,"WNRF PN 40 DIN 2635 Size  DN 50","WNRF","PN 40","DIN 2635","2\"",50.0,165.0,48.0,20.0,102.0,125.0,4.0,18.0,75.0,3.0,6.0,4.0,86,"M16",13.0,2.82]
[null,"WNRF PN 40 DIN 2635 Size  DN 65","WNRF","PN 40","DIN 2635","2½\"",65.0,185.0,52.0,22.0,122.0,145.0,8.0,18.0,90.0,3.0,6.0,4.0,90,"M16",13.0,3.74]
[null,"WNRF PN 40 DIN 2635 Size  DN 80","WNRF","PN 40","DIN 2635","3\"",80.0,200.0,58.0,24.0,138.0,160.0,8.0,18.0,105.0,3.0,8.0,4.0,94,"M16",13.0,4.75]
[null,"WNRF PN 40 DIN 2635 Size  DN 100","WNRF","PN 40","DIN 2635","4\"",100.0,235.0,65.0,24.0,162.0,190.0,8.0,22.0,134.0,3.0,8.0,5.0,101,"M20",16.0,6.52]
[null,"WNRF PN 40 DIN 2635 Size  DN 125","WNRF","PN 40","DIN 2635","5\"",125.0,270.0,68.0,26.0,188.0,220.0,8.0,26.0,162.0,3.0,8.0,5.0,111,"M24",19.0,9.07]
[null,"WNRF PN 40 DIN 2635 Size  DN 150","WNRF","PN 40","DIN 2635","6\"",150.0,300.0,75.0,28.0,218.0,250.0,8.0,26.0,192.0,3.0,10.0,6.0,116,"M24",19.0,11.8]
[null,"WNRF PN 40 DIN 2635 Size  DN 175","WNRF","PN 40","DIN 2635","-",175.0,350.0,82.0,32.0,260.0,295.0,12.0,30.0,218.0,3.0,10.0,6.0,130,"M27",22.0,18.2]
[null,"WNRF PN 40 DIN 2635 Size  DN 200","WNRF","PN 40","DIN 2635","8\"",200.0,375.0,88.0,34.0,285.0,320.0,12.0,30.0,244.0,3.0,10.0,6.0,134,"M27",22.0,21.5]
[null,"WNRF PN 40 DIN 2635 Size  DN 250","WNRF","PN 40","DIN 2635","10\"",250.0,450.0,105.0,38.0,345.0,385.0,12.0,33.0,306.0,3.0,12.0,6.0,146,"M30",24.0,34.9]
[null,"WNRF PN 40 DIN 2635 Size  DN 300","WNRF","PN 40","DIN 2635","12\"",300.0,515.0,115.0,42.0,410.0,450.0,16.0,33.0,362.0,4.0,12.0,6.0,154,"M30",24.0,49.7]
[null,"WNRF PN 40 DIN 2635 Size  DN 350","WNRF","PN 40","DIN 2635","14\"",350.0,580.0,125.0,46.0,465.0,510.0,16.0,36.0,408.0,4.0,12.0,7.0,167,"M33",26.0,68.1]
[null,"WNRF PN 40 DIN 2635 Size  DN 400","WNRF","PN 40","DIN 2635","16\"",400.0,660.0,135.0,50.0,535.0,585.0,16.0,39.0,462.0,4.0,12.0,7.0,181,"M36",29.0,96.5]
[null,"WNRF PN 40 DIN 2635 Size  DN 500","WNRF","PN 40","DIN 2635","20\"",500.0,755.0,140.0,52.0,615.0,670.0,20.0,42.0,562.0,4.0,12.0,7.0,189,"M39",31.0,117.0]
[null,"WNRF PN 64 DIN 2636 Size  DN 10","WNRF","PN 64","DIN 2636","1/4\"",10.0,100.0,45.0,20.0,40.0,70.0,4.0,14.0,32.0,2.0,4.0,3.0,79,"M12",10.0,1.09]
[null,"WNRF PN 64 DIN 2636 Size  DN 15","WNRF","PN 64","DIN 2636","1/2\"",15.0,105.0,45.0,20.0,45.0,75.0,4.0,14.0,34.0,2.0,4.0,3.0,79,"M12",10.0,1.19]
[null,"WNRF PN 64 DIN 2636 Size  DN 25","WNRF","PN 64","DIN 2636","1\"",25.0,140.0,58.0,24.0,68.0,100.0,4.0,18.0,52.0,2.0,4.0,3.0,93,"M16",13.0,2.66]
[null,"WNRF PN 64 DIN 2636 Size  DN 40","WNRF","PN 64","DIN 2636","1½\"",40.0,170.0,62.0,26.0,88.0,125.0,4.0,22.0,70.0,3.0,6.0,3.0,103,"M20",16.0,4.09]
[null,"WNRF PN 64 DIN 2636 Size  DN 50","WNRF","PN 64","DIN 2636","2\"",50.0,180.0,62.0,26.0,102.0,135.0,4.0,22.0,82.0,3.0,6.0,4.0,104,"M20",16.0,4.55]
[null,"WNRF PN 64 DIN 2636 Size  DN 65","WNRF","PN 64","DIN 2636","2½\"",65.0,205.0,68.0,26.0,122.0,160.0,8.0,22.0,98.0,3.0,6.0,4.0,104,"M20",16.0,5.73]
[null,"WNRF PN 64 DIN 2636 Size  DN 80","WNRF","PN 64","DIN 2636","3\"",80.0,215.0,72.0,28.0,138.0,170.0,8.0,22.0,112.0,3.0,8.0,4.0,108,"M20",16.0,6.69]
[null,"WNRF PN 64 DIN 2636 Size  DN 100","WNRF","PN 64","DIN 2636","4\"",100.0,250.0,78.0,30.0,162.0,200.0,8.0,26.0,138.0,3.0,8.0,5.0,119,"M24",19.0,9.66]
[null,"WNRF PN 64 DIN 2636 Size  DN 125","WNRF","PN 64","DIN 2636","5\"",125.0,295.0,88.0,34.0,188.0,240.0,8.0,30.0,168.0,3.0,8.0,5.0,133,"M27",22.0,15.1]
[null,"WNRF PN 64 DIN 2636 Size  DN 150","WNRF","PN 64","DIN 2636","6\"",150.0,345.0,95.0,36.0,218.0,280.0,8.0,33.0,202.0,3.0,10.0,6.0,142,"M30",24.0,21.9]
[null,"WNRF PN 64 DIN 2636 Size  DN 175","WNRF","PN 64","DIN 2636","7\"",175.0,375.0,105.0,40.0,260.0,310.0,12.0,33.0,228.0,3.0,10.0,6.0,150,"M30",24.0,23.7]
[null,"WNRF PN 64 DIN 2636 Size  DN 200","WNRF","PN 64","DIN 2636","8\"",200.0,415.0,110.0,42.0,285.0,345.0,12.0,36.0,256.0,3.0,10.0,6.0,158,"M33",26.0,34.9]
[null,"WNRF PN 64 DIN 2636 Size  DN 250","WNRF","PN 64","DIN 2636","10\"",250.0,470.0,125.0,46.0,345.0,400.0,12.0,36.0,316.0,3.0,12.0,6.0,166,"M33",26.0,49.6]
[null,"WNRF PN 64 DIN 2636 Size  DN 300","WNRF","PN 64","DIN 2636","12\"",300.0,530.0,140.0,52.0,410.0,460.0,16.0,36.0,372.0,4.0,12.0,6.0,178,"M33",26.0,68.7]
[null,"WNRF PN 64 DIN 2636 Size  DN 350","WNRF","PN 64","DIN 2636","14\"",350.0,600.0,150.0,56.0,465.0,525.0,16.0,39.0,420.0,4.0,12.0,7.0,193,"M36",29.0,94.6]
[null,"WNRF PN 64 DIN 2636 Size  DN 400","WNRF","PN 64","DIN 2636","16\"",400.0,670.0,160.0,60.0,535.0,585.0,16.0,42.0,475.0,4.0,12.0,7.0,205,"M39",31.0,124.0]
[null,"WNRF PN 100 DIN 2637 Size  DN 10","WNRF","PN 100","DIN 2637","1/4\"",10.0,100.0,45.0,20.0,40.0,70.0,4.0,14.0,32.0,2.0,4.0,3.0,79,"M12",10.0,1.09]
[null,"WNRF PN 100 DIN 2637 Size  DN 15","WNRF","PN 100","DIN 2637","1/2\"",15.0,105.0,45.0,20.0,45.0,75.0,4.0,14.0,34.0,2.0,4.0,3.0,79,"M12",10.0,1.19]
[null,"WNRF PN 100 DIN 2637 Size  DN 25","WNRF","PN 100","DIN 2637","1\"",25.0,140.0,58.0,24.0,68.0,100.0,4.0,18.0,52.0,2.0,4.0,3.0,93,"M16",13.0,2.66]
[null,"WNRF PN 100 DIN 2637 Size  DN 40","WNRF","PN 100","DIN 2637","1½\"",40.0,170.0,62.0,26.0,88.0,125.0,4.0,22.0,70.0,3.0,6.0,3.0,103,"M20",16.0,4.09]
[null,"WNRF PN 100 DIN 2637 Size  DN 50","WNRF","PN 100","DIN 2637","2\"",50.0,195.0,68.0,28.0,102.0,145.0,4.0,26.0,90.0,3.0,6.0,4.0,114,"M24",19.0,5.98]
[null,"WNRF PN 100 DIN 2637 Size  DN 65","WNRF","PN 100","DIN 2637","2½\"",65.0,220.0,76.0,30.0,122.0,170.0,8.0,26.0,108.0,3.0,6.0,4.0,118,"M24",19.0,7.91]
[null,"WNRF PN 100 DIN 2637 Size  DN 80","WNRF","PN 100","DIN 2637","3\"",80.0,230.0,78.0,32.0,138.0,180.0,8.0,26.0,120.0,3.0,8.0,4.0,122,"M24",19.0,8.95]
[null,"WNRF PN 100 DIN 2637 Size  DN 100","WNRF","PN 100","DIN 2637","4\"",100.0,265.0,90.0,36.0,162.0,210.0,8.0,30.0,150.0,3.0,8.0,5.0,137,"M27",22.0,13.7]
[null,"WNRF PN 100 DIN 2637 Size  DN 125","WNRF","PN 100","DIN 2637","5\"",125.0,315.0,105.0,40.0,188.0,250.0,8.0,33.0,180.0,3.0,8.0,5.0,149,"M30",24.0,22.7]
[null,"WNRF PN 100 DIN 2637 Size  DN 150","WNRF","PN 100","DIN 2637","6\"",150.0,355.0,115.0,44.0,218.0,290.0,12.0,33.0,210.0,3.0,10.0,6.0,158,"M30",24.0,30.2]
[null,"WNRF PN 100 DIN 2637 Size  DN 175","WNRF","PN 100","DIN 2637","-",175.0,385.0,127.0,48.0,260.0,320.0,12.0,33.0,245.0,3.0,10.0,6.0,166,"M30",24.0,38.9]
[null,"WNRF PN 100 DIN 2637 Size  DN 200","WNRF","PN 100","DIN 2637","8\"",200.0,430.0,130.0,52.0,285.0,360.0,12.0,36.0,278.0,3.0,10.0,6.0,178,"M33",26.0,52.8]
[null,"WNRF PN 100 DIN 2637 Size  DN 250","WNRF","PN 100","DIN 2637","10\"",250.0,505.0,157.0,60.0,345.0,430.0,12.0,39.0,340.0,3.0,12.0,6.0,200,"M36",29.0,81.4]
[null,"WNRF PN 100 DIN 2637 Size  DN 300","WNRF","PN 100","DIN 2637","12\"",300.0,585.0,170.0,68.0,410.0,500.0,16.0,42.0,400.0,4.0,12.0,6.0,220,"M39",31.0,122.0]
[null,"WNRF PN 100 DIN 2637 Size  DN 350","WNRF","PN 100","DIN 2637","14\"",350.0,655.0,189.0,74.0,465.0,560.0,16.0,48.0,460.0,4.0,12.0,7.0,243,"M45",36.0,165.0]
[null,"WNRF PN 160 DIN 2638 Size  DN 10","WNRF","PN 160","DIN 2638","1/4\"",10.0,100.0,45.0,20.0,40.0,70.0,4.0,14.0,32.0,2.0,4.0,3.0,79,"M12",10.0,1.09]
[null,"WNRF PN 160 DIN 2638 Size  DN 15","WNRF","PN 160","DIN 2638","1/2\"",15.0,105.0,45.0,20.0,45.0,75.0,4.0,14.0,34.0,2.0,4.0,3.0,79,"M12",10.0,1.19]
[null,"WNRF PN 160 DIN 2638 Size  DN 25","WNRF","PN 160","DIN 2638","1\"",25.0,140.0,58.0,24.0,68.0,100.0,4.0,18.0,52.0,2.0,4.0,3.0,93,"M16",13.0,2.66]
[null,"WNRF PN 160 DIN 2638 Size  DN 40","WNRF","PN 160","DIN 2638","1½\"",40.0,170.0,64.0,28.0,88.0,125.0,4.0,22.0,70.0,3.0,6.0,3.0,107,"M20",16.0,4.3]
[null,"WNRF PN 160 DIN 2638 Size  DN 50","WNRF","PN 160","DIN 2638","2\"",50.0,195.0,75.0,30.0,102.0,145.0,4.0,26.0,90.0,3.0,6.0,4.0,118,"M24",19.0,6.25]
[null,"WNRF PN 160 DIN 2638 Size  DN 65","WNRF","PN 160","DIN 2638","2½\"",65.0,220.0,82.0,34.0,122.0,170.0,8.0,26.0,108.0,3.0,6.0,4.0,126,"M24",19.0,8.35]
[null,"WNRF PN 160 DIN 2638 Size  DN 80","WNRF","PN 160","DIN 2638","3\"",80.0,230.0,86.0,36.0,138.0,180.0,8.0,26.0,120.0,3.0,8.0,4.0,130,"M24",19.0,9.75]
[null,"WNRF PN 160 DIN 2638 Size  DN 100","WNRF","PN 160","DIN 2638","4\"",100.0,265.0,100.0,40.0,162.0,210.0,8.0,30.0,150.0,3.0,8.0,5.0,145,"M27",22.0,14.8]
[null,"WNRF PN 160 DIN 2638 Size  DN 125","WNRF","PN 160","DIN 2638","5\"",125.0,315.0,115.0,44.0,188.0,250.0,8.0,33.0,180.0,3.0,8.0,5.0,157,"M30",24.0,23.0]
[null,"WNRF PN 160 DIN 2638 Size  DN 150","WNRF","PN 160","DIN 2638","6\"",150.0,355.0,128.0,50.0,218.0,290.0,12.0,33.0,210.0,3.0,10.0,6.0,170,"M30",24.0,32.5]
[null,"WNRF PN 160 DIN 2638 Size  DN 175","WNRF","PN 160","DIN 2638","-",175.0,390.0,138.0,54.0,260.0,320.0,12.0,36.0,245.0,3.0,10.0,6.0,182,"M33",26.0,43.5]
[null,"WNRF PN 160 DIN 2638 Size  DN 200","WNRF","PN 160","DIN 2638","8\"",200.0,430.0,140.0,60.0,285.0,360.0,12.0,36.0,278.0,3.0,10.0,6.0,194,"M33",26.0,59.4]
[null,"WNRF PN 160 DIN 2638 Size  DN 250","WNRF","PN 160","DIN 2638","10\"",250.0,515.0,155.0,68.0,345.0,430.0,12.0,42.0,340.0,3.0,12.0,6.0,220,"M39",31.0,94.5]
[null,"WNRF PN 160 DIN 2638 Size  DN 300","WNRF","PN 160","DIN 2638","12\"",300.0,585.0,175.0,78.0,410.0,500.0,16.0,42.0,400.0,4.0,12.0,6.0,240,"M39",31.0,136.0]
[null,"WNRF PN 250 DIN 2628 Size  DN 10","WNRF","PN 250","DIN 2628","1/4\"",10.0,125.0,58.0,24.0,40.0,85.0,4.0,18.0,44.0,2.0,4.0,3.0,93,"M16",13.0,2.08]
[null,"WNRF PN 250 DIN 2628 Size  DN 15","WNRF","PN 250","DIN 2628","1/2\"",15.0,130.0,60.0,26.0,45.0,90.0,4.0,18.0,48.0,2.0,4.0,3.0,97,"M16",13.0,2.47]
[null,"WNRF PN 250 DIN 2628 Size  DN 25","WNRF","PN 250","DIN 2628","1\"",25.0,150.0,65.0,28.0,68.0,105.0,4.0,22.0,60.0,2.0,4.0,3.0,107,"M20",16.0,2.51]
[null,"WNRF PN 250 DIN 2628 Size  DN 40","WNRF","PN 250","DIN 2628","1½\"",40.0,185.0,80.0,34.0,88.0,135.0,4.0,26.0,84.0,3.0,6.0,3.0,125,"M24",19.0,6.45]
[null,"WNRF PN 250 DIN 2628 Size  DN 50","WNRF","PN 250","DIN 2628","2\"",50.0,200.0,85.0,38.0,102.0,150.0,8.0,26.0,95.0,3.0,6.0,4.0,134,"M24",19.0,7.85]
[null,"WNRF PN 250 DIN 2628 Size  DN 65","WNRF","PN 250","DIN 2628","2½\"",65.0,230.0,95.0,42.0,122.0,180.0,8.0,26.0,124.0,3.0,6.0,4.0,142,"M24",19.0,12.2]
[null,"WNRF PN 250 DIN 2628 Size  DN 80","WNRF","PN 250","DIN 2628","3\"",80.0,255.0,102.0,46.0,138.0,200.0,8.0,30.0,136.0,3.0,8.0,4.0,156,"M27",22.0,16.0]
[null,"WNRF PN 250 DIN 2628 Size  DN 100","WNRF","PN 250","DIN 2628","4\"",100.0,300.0,120.0,54.0,162.0,235.0,8.0,33.0,164.0,3.0,8.0,5.0,177,"M30",24.0,26.3]
[null,"WNRF PN 250 DIN 2628 Size  DN 125","WNRF","PN 250","DIN 2628","5\"",125.0,340.0,140.0,60.0,188.0,275.0,12.0,33.0,200.0,3.0,8.0,5.0,189,"M30",24.0,37.8]
[null,"WNRF PN 250 DIN 2628 Size  DN 150","WNRF","PN 250","DIN 2628","6\"",150.0,390.0,160.0,68.0,218.0,320.0,12.0,36.0,240.0,3.0,10.0,6.0,210,"M33",26.0,58.0]
[null,"WNRF PN 250 DIN 2628 Size  DN 200","WNRF","PN 250","DIN 2628","8\"",200.0,485.0,190.0,82.0,285.0,400.0,12.0,42.0,305.0,3.0,10.0,6.0,248,"M39",31.0,105.0]
[null,"WNRF PN 250 DIN 2628 Size  DN 250","WNRF","PN 250","DIN 2628","10\"",250.0,585.0,215.0,100.0,345.0,490.0,16.0,48.0,385.0,3.0,12.0,6.0,294,"M45",36.0,182.0]
[null,"WNRF PN 320 DIN 2629 Size  DN 10","WNRF","PN 320","DIN 2629","1/4\"",10.0,125.0,58.0,24.0,40.0,85.0,4.0,18.0,44.0,2.0,4.0,3.0,93,"M16",13.0,2.08]
[null,"WNRF PN 320 DIN 2629 Size  DN 15","WNRF","PN 320","DIN 2629","1/2\"",15.0,130.0,60.0,26.0,45.0,90.0,4.0,18.0,48.0,2.0,4.0,3.0,97,"M16",13.0,2.47]
[null,"WNRF PN 320 DIN 2629 Size  DN 25","WNRF","PN 320","DIN 2629","1\"",25.0,160.0,78.0,34.0,68.0,115.0,4.0,22.0,68.0,2.0,4.0,3.0,119,"M20",16.0,5.0]
[null,"WNRF PN 320 DIN 2629 Size  DN 40","WNRF","PN 320","DIN 2629","1½\"",40.0,195.0,88.0,38.0,88.0,145.0,4.0,26.0,92.0,3.0,6.0,3.0,133,"M24",19.0,8.25]
[null,"WNRF PN 320 DIN 2629 Size  DN 50","WNRF","PN 320","DIN 2629","2\"",50.0,210.0,100.0,42.0,102.0,160.0,8.0,26.0,106.0,3.0,6.0,4.0,142,"M24",19.0,10.3]
[null,"WNRF PN 320 DIN 2629 Size  DN 65","WNRF","PN 320","DIN 2629","2½\"",65.0,255.0,120.0,51.0,122.0,200.0,8.0,30.0,138.0,3.0,6.0,4.0,166,"M27",22.0,19.1]
[null,"WNRF PN 320 DIN 2629 Size  DN 80","WNRF","PN 320","DIN 2629","3\"",80.0,275.0,130.0,55.0,138.0,220.0,8.0,30.0,156.0,3.0,8.0,4.0,174,"M27",22.0,24.8]
[null,"WNRF PN 320 DIN 2629 Size  DN 100","WNRF","PN 320","DIN 2629","4\"",100.0,335.0,145.0,65.0,162.0,265.0,8.0,36.0,186.0,3.0,8.0,5.0,203,"M33",26.0,42.0]
[null,"WNRF PN 320 DIN 2629 Size  DN 125","WNRF","PN 320","DIN 2629","5\"",125.0,380.0,175.0,75.0,188.0,310.0,12.0,36.0,230.0,3.0,8.0,5.0,223,"M33",26.0,64.5]
[null,"WNRF PN 320 DIN 2629 Size  DN 150","WNRF","PN 320","DIN 2629","6\"",150.0,425.0,195.0,84.0,218.0,350.0,12.0,39.0,265.0,3.0,10.0,6.0,248,"M36",29.0,89.5]
[null,"WNRF PN 320 DIN 2629 Size  DN 175","WNRF","PN 320","DIN 2629","-",175.0,485.0,215.0,95.0,260.0,400.0,12.0,42.0,308.0,3.0,10.0,6.0,274,"M39",31.0,134.0]
[null,"WNRF PN 320 DIN 2629 Size  DN 200","WNRF","PN 320","DIN 2629","8\"",200.0,525.0,235.0,103.0,285.0,440.0,16.0,42.0,345.0,3.0,10.0,6.0,290,"M39",31.0,170.0]
[null,"WNRF PN 320 DIN 2629 Size  DN 250","WNRF","PN 320","DIN 2629","10\"",250.0,640.0,300.0,125.0,345.0,540.0,16.0,52.0,428.0,3.0,12.0,6.0,348,"M48",38.0,308.0]
[null,"WNRF PN 400 DIN 2627 Size  DN 10","WNRF","PN 400","DIN 2627","1/4\"",10.0,125.0,65.0,28.0,40.0,85.0,4.0,18.0,48.0,2.0,4.0,3.0,101,"M16",13.0,2.52]
[null,"WNRF PN 400 DIN 2627 Size  DN 15","WNRF","PN 400","DIN 2627","1/2\"",15.0,145.0,68.0,30.0,45.0,100.0,4.0,22.0,56.0,2.0,4.0,3.0,111,"M20",16.0,3.59]
[null,"WNRF PN 400 DIN 2627 Size  DN 25","WNRF","PN 400","DIN 2627","1\"",25.0,180.0,90.0,38.0,68.0,130.0,4.0,26.0,82.0,2.0,4.0,3.0,133,"M24",19.0,7.43]
[null,"WNRF PN 400 DIN 2627 Size  DN 40","WNRF","PN 400","DIN 2627","1½\"",40.0,220.0,110.0,48.0,88.0,165.0,4.0,30.0,106.0,3.0,6.0,3.0,159,"M27",22.0,14.0]
[null,"WNRF PN 400 DIN 2627 Size  DN 50","WNRF","PN 400","DIN 2627","2\"",50.0,235.0,120.0,52.0,102.0,180.0,8.0,30.0,120.0,3.0,6.0,4.0,168,"M27",22.0,16.7]
[null,"WNRF PN 400 DIN 2627 Size  DN 65","WNRF","PN 400","DIN 2627","2½\"",65.0,290.0,135.0,64.0,122.0,225.0,8.0,33.0,158.0,3.0,6.0,4.0,196,"M30",24.0,31.6]
[null,"WNRF PN 400 DIN 2627 Size  DN 80","WNRF","PN 400","DIN 2627","3\"",80.0,305.0,150.0,68.0,138.0,240.0,8.0,33.0,174.0,3.0,8.0,4.0,204,"M30",24.0,38.4]
[null,"WNRF PN 400 DIN 2627 Size  DN 100","WNRF","PN 400","DIN 2627","4\"",100.0,370.0,175.0,80.0,162.0,295.0,8.0,39.0,216.0,3.0,8.0,5.0,239,"M36",29.0,67.3]
[null,"WNRF PN 400 DIN 2627 Size  DN 125","WNRF","PN 400","DIN 2627","5\"",125.0,415.0,200.0,92.0,188.0,340.0,12.0,39.0,258.0,3.0,8.0,5.0,263,"M36",29.0,96.0]
[null,"WNRF PN 400 DIN 2627 Size  DN 150","WNRF","PN 400","DIN 2627","6\"",150.0,475.0,225.0,105.0,218.0,390.0,12.0,42.0,302.0,3.0,10.0,6.0,294,"M39",31.0,146.0]
[null,"WNRF PN 400 DIN 2627 Size  DN 200","WNRF","PN 400","DIN 2627","8\"",200.0,585.0,280.0,130.0,285.0,490.0,16.0,48.0,388.0,3.0,10.0,6.0,354,"M45",36.0,296.0]
[null,"Cast Iron WNRF PN 10 DIN 2532 Size  DN 40","Cast Iron WNRF","PN 10","DIN 2532","1½\"",40.0,150.0,"-","-","-",110.0,4.0,18.0,"-","-","-",3.0,"-","M16",13.0,"-"]
[null,"Cast Iron WNRF PN 10 DIN 2532 Size  DN 50","Cast Iron WNRF","PN 10","DIN 2532","2\"",50.0,165.0,"-","-","-",125.0,4.0,19.0,"-","-","-",4.0,"-","M16",13.0,"-"]
[null,"Cast Iron WNRF PN 10 DIN 2532 Size  DN 65","Cast Iron WNRF","PN 10","DIN 2532","2½\"",65.0,185.0,"-","-","-",145.0,4.0,19.0,"-","-","-",4.0,"-","M16",13.0,"-"]
[null,"Cast Iron WNRF PN 10 DIN 2532 Size  DN 80","Cast Iron WNRF","PN 10","DIN 2532","3\"",80.0,200.0,"-","-","-",160.0,8.0,19.0,"-","-","-",4.0,"-","M16",13.0,"-"]
[null,"Cast Iron WNRF PN 10 DIN 2532 Size  DN 100","Cast Iron WNRF","PN 10","DIN 2532","4\"",100.0,220.0,"-","-","-",180.0,8.0,19.0,"-","-","-",5.0,"-","M16",13.0,"-"]
[null,"Cast Iron WNRF PN 10 DIN 2532 Size  DN 125","Cast Iron WNRF","PN 10","DIN 2532","5\"",125.0,250.0,"-","-","-",210.0,8.0,19.0,"-","-","-",5.0,"-","M16",13.0,"-"]
[null,"Cast Iron WNRF PN 10 DIN 2532 Size  DN 150","Cast Iron WNRF","PN 10","DIN 2532","6\"",150.0,285.0,"-","-","-",240.0,8.0,22.0,"-","-","-",6.0,"-","M20",16.0,"-"]
[null,"Cast Iron WNRF PN 10 DIN 2532 Size  DN 200","Cast Iron WNRF","PN 10","DIN 2532","8\"",200.0,340.0,"-",26.0,268.0,295.0,8.0,22.0,240.0,3.0,8.0,6.0,{"$f":"(J1287+U1287+8)*2+R1287","v":106},"M20",16.0,9.66]
[null,"Cast Iron WNRF PN 10 DIN 2532 Size  DN 250","Cast Iron WNRF","PN 10","DIN 2532","10\"",250.0,395.0,"-",28.0,320.0,350.0,12.0,22.0,292.0,3.0,8.0,6.0,110,"M20",16.0,12.5]
[null,"Cast Iron WNRF PN 10 DIN 2532 Size  DN 300","Cast Iron WNRF","PN 10","DIN 2532","12\"",300.0,445.0,"-",28.0,370.0,400.0,12.0,22.0,342.0,4.0,8.0,6.0,110,"M20",16.0,13.7]
[null,"Cast Iron WNRF PN 10 DIN 2532 Size  DN 350","Cast Iron WNRF","PN 10","DIN 2532","14\"",350.0,505.0,"-",30.0,430.0,460.0,16.0,22.0,396.0,4.0,8.0,7.0,115,"M20",16.0,18.3]
[null,"Cast Iron WNRF PN 10 DIN 2532 Size  DN 400","Cast Iron WNRF","PN 10","DIN 2532","16\"",400.0,565.0,"-",32.0,482.0,515.0,16.0,26.0,448.0,4.0,10.0,7.0,125,"M24",19.0,23.7]
[null,"Cast Iron WNRF PN 10 DIN 2532 Size  DN 450","Cast Iron WNRF","PN 10","DIN 2532","18\"",450.0,615.0,"-",32.0,532.0,565.0,20.0,26.0,498.0,4.0,10.0,7.0,125,"M24",19.0,25.0]
[null,"Cast Iron WNRF PN 10 DIN 2532 Size  DN 500","Cast Iron WNRF","PN 10","DIN 2532","20\"",500.0,670.0,"-",34.0,585.0,620.0,20.0,26.0,552.0,4.0,10.0,7.0,129,"M24",19.0,30.6]
[null,"Cast Iron WNRF PN 10 DIN 2532 Size  DN 600","Cast Iron WNRF","PN 10","DIN 2532","24\"",600.0,780.0,"-",36.0,685.0,725.0,20.0,30.0,654.0,5.0,10.0,7.0,139,"M27",22.0,39.0]
[null,"Cast Iron WNRF PN 10 DIN 2532 Size  DN 700","Cast Iron WNRF","PN 10","DIN 2532","28\"",700.0,895.0,"-",40.0,800.0,840.0,24.0,30.0,760.0,5.0,10.0,7.0,147,"M27",22.0,54.8]
[null,"Cast Iron WNRF PN 10 DIN 2532 Size  DN 750","Cast Iron WNRF","PN 10","DIN 2532","30\"",750.0,965.0,"-","-","-",900.0,24.0,33.0,"-",5.0,"-",7.0,"-","M30",24.0,"-"]
[null,"Cast Iron WNRF PN 10 DIN 2532 Size  DN 800","Cast Iron WNRF","PN 10","DIN 2532","32\"",800.0,1015.0,"-",44.0,905.0,950.0,24.0,33.0,866.0,5.0,12.0,7.0,{"$f":"(J1297+U1297+8)*2+R1297","v":159},"M30",24.0,76.0]
[null,"Cast Iron WNRF PN 10 DIN 2532 Size  DN 900","Cast Iron WNRF","PN 10","DIN 2532","36\"",900.0,1115.0,"-",46.0,1005.0,1050.0,28.0,33.0,970.0,5.0,12.0,7.0,163,"M30",24.0,85.8]
[null,"Cast Iron WNRF PN 10 DIN 2532 Size  DN 1000","Cast Iron WNRF","PN 10","DIN 2532","40\"",1000.0,1230.0,"-",50.0,1110.0,1160.0,28.0,36.0,1076.0,5.0,12.0,7.0,175,"M33",26.0,113.0]
[null,"Cast Iron WNRF PN 10 DIN 2532 Size  DN 1100","Cast Iron WNRF","PN 10","DIN 2532","44\"",1100.0,1340.0,"-","-","-",1270.0,32.0,36.0,"-",5.0,"-",7.0,"-","M33",26.0,"-"]
[null,"Cast Iron WNRF PN 10 DIN 2532 Size  DN 1200","Cast Iron WNRF","PN 10","DIN 2532","48\"",1200.0,1455.0,"-",56.0,1330.0,1380.0,32.0,39.0,1284.0,5.0,15.0,7.0,{"$f":"(J1301+U1301+8)*2+R1301","v":193},"M36",29.0,163.0]
[null,"Cast Iron WNRF PN 10 DIN 2532 Size  DN 1400","Cast Iron WNRF","PN 10","DIN 2532","56\"",1400.0,1675.0,"-",62.0,1535.0,1590.0,36.0,42.0,1494.0,5.0,18.0,7.0,209,"M39",31.0,225.0]
[null,"Cast Iron WNRF PN 10 DIN 2532 Size  DN 1600","Cast Iron WNRF","PN 10","DIN 2532","64\"",1600.0,1915.0,"-",68.0,1760.0,1820.0,40.0,48.0,1702.0,5.0,18.0,7.0,231,"M45",36.0,317.0]
[null,"Cast Iron WNRF PN 10 DIN 2532 Size  DN 1800","Cast Iron WNRF","PN 10","DIN 2532","72\"",1800.0,2115.0,"-",70.0,1960.0,2020.0,44.0,48.0,1906.0,5.0,18.0,7.0,235,"M45",36.0,345.0]
[null,"Cast Iron WNRF PN 10 DIN 2532 Size  DN 2000","Cast Iron WNRF","PN 10","DIN 2532","80\"",2000.0,2325.0,"-",74.0,2170.0,2230.0,48.0,48.0,2112.0,5.0,18.0,7.0,243,"M45",36.0,410.0]
[null,"Cast Iron WNRF PN 10 DIN 2532 Size  DN 2200","Cast Iron WNRF","PN 10","DIN 2532","88\"",2200.0,2550.0,"-",80.0,2370.0,2440.0,52.0,56.0,2320.0,6.0,20.0,7.0,267,"M52",42.0,499.0]
[null,"Cast Iron WNRF PN 10 DIN 2532 Size  DN 2400","Cast Iron WNRF","PN 10","DIN 2532","96\"",2400.0,2760.0,"-",82.0,2570.0,2650.0,56.0,56.0,2524.0,6.0,20.0,7.0,271,"M52",42.0,560.0]
[null,"Cast Iron WNRF PN 10 DIN 2532 Size  DN 2600","Cast Iron WNRF","PN 10","DIN 2532","104\"",2600.0,2960.0,"-",88.0,2780.0,2850.0,60.0,56.0,2732.0,6.0,20.0,7.0,283,"M52",42.0,628.0]
[null,"Cast Iron WNRF PN 10 DIN 2532 Size  DN 2800","Cast Iron WNRF","PN 10","DIN 2532","112\"",2800.0,3180.0,"-",94.0,3000.0,3070.0,64.0,56.0,2940.0,6.0,20.0,7.0,295,"M52",42.0,772.0]
[null,"Cast Iron WNRF PN 10 DIN 2532 Size  DN 3000","Cast Iron WNRF","PN 10","DIN 2532","120\"",3000.0,3405.0,"-",100.0,3210.0,3290.0,68.0,62.0,3150.0,6.0,20.0,7.0,313,"M56",45.0,919.0]
[null,"Cast Iron WNRF PN 16 DIN 2533 Size  DN 40","Cast Iron WNRF","PN 16","DIN 2533","1½\"",40.0,150.0,"-","-","-",110.0,4.0,16.0,"-","-","-",3.0,"-","M16",13.0,"-"]
[null,"Cast Iron WNRF PN 16 DIN 2533 Size  DN 50","Cast Iron WNRF","PN 16","DIN 2533","2\"",50.0,165.0,"-","-",102.0,125.0,4.0,18.0,"-","-","-",4.0,"-","M16",13.0,"-"]
[null,"Cast Iron WNRF PN 16 DIN 2533 Size  DN 65","Cast Iron WNRF","PN 16","DIN 2533","2½\"",65.0,185.0,"-","-","-",145.0,4.0,18.0,"-","-","-",4.0,"-","M16",13.0,"-"]
[null,"Cast Iron WNRF PN 16 DIN 2533 Size  DN 80","Cast Iron WNRF","PN 16","DIN 2533","3\"",80.0,200.0,"-","-",138.0,160.0,8.0,18.0,"-","-","-",4.0,"-","M16",13.0,"-"]
[null,"Cast Iron WNRF PN 16 DIN 2533 Size  DN 100","Cast Iron WNRF","PN 16","DIN 2533","4\"",100.0,220.0,"-","-",162.0,180.0,8.0,18.0,"-","-","-",5.0,"-","M16",13.0,"-"]
[null,"Cast Iron WNRF PN 16 DIN 2533 Size  DN 125","Cast Iron WNRF","PN 16","DIN 2533","5\"",125.0,250.0,"-","-",188.0,210.0,8.0,18.0,"-","-","-",5.0,"-","M16",13.0,"-"]
[null,"Cast Iron WNRF PN 16 DIN 2533 Size  DN 150","Cast Iron WNRF","PN 16","DIN 2533","6\"",150.0,285.0,"-","-",212.0,240.0,8.0,23.0,"-","-","-",6.0,"-","M20",16.0,"-"]
[null,"Cast Iron WNRF PN 16 DIN 2533 Size  DN 200","Cast Iron WNRF","PN 16","DIN 2533","8\"",200.0,340.0,"-","-",268.0,295.0,12.0,23.0,"-","-","-",6.0,"-","M20",16.0,"-"]
[null,"Cast Iron WNRF PN 16 DIN 2533 Size  DN 250","Cast Iron WNRF","PN 16","DIN 2533","10\"",250.0,400.0,"-","-",320.0,355.0,12.0,28.0,"-","-","-",6.0,"-","M24",19.0,"-"]
[null,"Cast Iron WNRF PN 16 DIN 2533 Size  DN 300","Cast Iron WNRF","PN 16","DIN 2533","12\"",300.0,455.0,"-","-",370.0,410.0,12.0,28.0,"-","-","-",6.0,"-","M24",19.0,"-"]
[null,"Cast Iron WNRF PN 16 DIN 2533 Size  DN 350","Cast Iron WNRF","PN 16","DIN 2533","14\"",350.0,520.0,"-","-",438.0,470.0,16.0,28.0,"-","-","-",7.0,"-","M24",19.0,"-"]
[null,"Cast Iron WNRF PN 16 DIN 2533 Size  DN 400","Cast Iron WNRF","PN 16","DIN 2533","16\"",400.0,580.0,"-","-",490.0,525.0,16.0,31.0,"-","-","-",7.0,"-","M27",22.0,"-"]
[null,"Cast Iron WNRF PN 16 DIN 2533 Size  DN 450","Cast Iron WNRF","PN 16","DIN 2533","18\"",450.0,640.0,"-","-",560.0,585.0,20.0,31.0,"-","-","-",7.0,"-","M27",22.0,"-"]
[null,"Cast Iron WNRF PN 16 DIN 2533 Size  DN 500","Cast Iron WNRF","PN 16","DIN 2533","20\"",500.0,715.0,"-","-",610.0,650.0,20.0,34.0,"-","-","-",7.0,"-","M30",24.0,"-"]
[null,"Cast Iron WNRF PN 16 DIN 2533 Size  DN 600","Cast Iron WNRF","PN 16","DIN 2533","24\"",600.0,840.0,"-","-",725.0,770.0,20.0,37.0,"-","-","-",7.0,"-","M33",27.0,"-"]
[null,"Cast Iron WNRF PN 16 DIN 2533 Size  DN 700","Cast Iron WNRF","PN 16","DIN 2533","28\"",700.0,910.0,"-","-",795.0,840.0,24.0,37.0,"-","-","-",7.0,"-","M33",27.0,"-"]
[null,"Cast Iron WNRF PN 16 DIN 2533 Size  DN 750","Cast Iron WNRF","PN 16","DIN 2533","30\"",750.0,970.0,"-","-","-",900.0,24.0,37.0,"-","-","-",7.0,"-","M33",27.0,"-"]
[null,"Cast Iron WNRF PN 16 DIN 2533 Size  DN 800","Cast Iron WNRF","PN 16","DIN 2533","32\"",800.0,1025.0,"-","-",900.0,950.0,24.0,40.0,"-","-","-",7.0,"-","M36",29.0,"-"]
[null,"Cast Iron WNRF PN 16 DIN 2533 Size  DN 900","Cast Iron WNRF","PN 16","DIN 2533","36\"",900.0,1125.0,"-","-",1000.0,1050.0,28.0,40.0,"-","-","-",7.0,"-","M36",29.0,"-"]
[null,"Cast Iron WNRF PN 16 DIN 2533 Size  DN 1000","Cast Iron WNRF","PN 16","DIN 2533","40\"",1000.0,1255.0,"-","-",1115.0,1170.0,28.0,43.0,"-","-","-",7.0,"-","M39",31.0,"-"]
[null,"Cast Iron WNRF PN 16 DIN 2533 Size  DN 1100","Cast Iron WNRF","PN 16","DIN 2533","44\"",1100.0,1355.0,"-","-","-",1270.0,32.0,43.0,"-","-","-",7.0,"-","M39",31.0,"-"]
[null,"Cast Iron WNRF PN 16 DIN 2533 Size  DN 1200","Cast Iron WNRF","PN 16","DIN 2533","48\"",1200.0,1485.0,"-","-",1330.0,1390.0,32.0,49.0,"-","-","-",7.0,"-","M45",36.0,"-"]
[null,"Cast Iron WNRF PN 16 DIN 2533 Size  DN 1400","Cast Iron WNRF","PN 16","DIN 2533","56\"",1400.0,1685.0,"-","-","-",1590.0,36.0,49.0,"-","-","-",7.0,"-","M45",36.0,"-"]
[null,"Cast Iron WNRF PN 16 DIN 2533 Size  DN 1600","Cast Iron WNRF","PN 16","DIN 2533","64\"",1600.0,1930.0,"-","-","-",1820.0,40.0,56.0,"-","-","-",7.0,"-","M52",42.0,"-"]
[null,"Cast Iron WNRF PN 16 DIN 2533 Size  DN 1800","Cast Iron WNRF","PN 16","DIN 2533","72\"",1800.0,2130.0,"-","-","-",2020.0,44.0,56.0,"-","-","-",7.0,"-","M52",42.0,"-"]
[null,"Cast Iron WNRF PN 16 DIN 2533 Size  DN 2000","Cast Iron WNRF","PN 16","DIN 2533","80\"",2000.0,2345.0,"-","-","-",2230.0,48.0,62.0,"-","-","-",7.0,"-","M56",45.0,"-"]
[null,"Cast Iron WNRF PN 10 DIN 28604 Size  DN 40","Cast Iron WNRF","PN 10","DIN 28604","1½\"",40.0,150.0,39.0,19.0,83.0,110.0,4.0,19.0,73.0,3.0,5.0,3.0,{"$f":"(J1337+U1337+8)*2+R1337","v":83},"M16",13.0,1.7]
[null,"Cast Iron WNRF PN 10 DIN 28604 Size  DN 50","Cast Iron WNRF","PN 10","DIN 28604","2\"",50.0,165.0,40.0,19.0,98.0,125.0,4.0,19.0,83.0,3.0,5.0,4.0,84,"M16",13.0,2.1]
[null,"Cast Iron WNRF PN 10 DIN 28604 Size  DN 65","Cast Iron WNRF","PN 10","DIN 28604","2½\"",65.0,185.0,41.5,19.0,118.0,145.0,4.0,19.0,99.0,3.0,5.0,4.0,84,"M16",13.0,2.6]
[null,"Cast Iron WNRF PN 10 DIN 28604 Size  DN 80","Cast Iron WNRF","PN 10","DIN 28604","3\"",80.0,200.0,43.0,19.0,133.0,160.0,4.0,19.0,115.0,3.0,6.0,4.0,84,"M16",13.0,3.0]
[null,"Cast Iron WNRF PN 10 DIN 28604 Size  DN 100","Cast Iron WNRF","PN 10","DIN 28604","4\"",100.0,220.0,45.0,19.0,153.0,180.0,8.0,19.0,134.0,3.0,6.0,5.0,85,"M16",13.0,3.3]
[null,"Cast Iron WNRF PN 10 DIN 28604 Size  DN 125","Cast Iron WNRF","PN 10","DIN 28604","5\"",125.0,250.0,47.5,19.0,183.0,210.0,8.0,19.0,160.0,3.0,6.0,5.0,85,"M16",13.0,4.0]
[null,"Cast Iron WNRF PN 10 DIN 28604 Size  DN 150","Cast Iron WNRF","PN 10","DIN 28604","6\"",150.0,285.0,50.0,19.0,209.0,240.0,8.0,23.0,185.0,3.0,6.0,6.0,92,"M20",16.0,5.0]
[null,"Cast Iron WNRF PN 10 DIN 28604 Size  DN 200","Cast Iron WNRF","PN 10","DIN 28604","8\"",200.0,340.0,55.0,20.0,264.0,295.0,8.0,23.0,237.0,3.0,8.0,6.0,94,"M20",16.0,6.9]
[null,"Cast Iron WNRF PN 10 DIN 28604 Size  DN 250","Cast Iron WNRF","PN 10","DIN 28604","10\"",250.0,400.0,60.0,22.0,319.0,350.0,12.0,23.0,291.0,3.0,8.0,6.0,98,"M20",16.0,9.8]
[null,"Cast Iron WNRF PN 10 DIN 28604 Size  DN 300","Cast Iron WNRF","PN 10","DIN 28604","12\"",300.0,455.0,65.0,24.5,367.0,400.0,12.0,23.0,346.0,4.0,8.0,6.0,103,"M20",16.0,13.0]
[null,"Cast Iron WNRF PN 10 DIN 28604 Size  DN 350","Cast Iron WNRF","PN 10","DIN 28604","14\"",350.0,505.0,70.0,24.5,427.0,460.0,16.0,23.0,397.0,4.0,10.0,7.0,104,"M20",16.0,14.7]
[null,"Cast Iron WNRF PN 10 DIN 28604 Size  DN 400","Cast Iron WNRF","PN 10","DIN 28604","16\"",400.0,565.0,75.0,24.5,477.0,515.0,16.0,28.0,447.0,4.0,10.0,7.0,110,"M24",19.0,17.2]
[null,"Cast Iron WNRF PN 10 DIN 28604 Size  DN 500","Cast Iron WNRF","PN 10","DIN 28604","20\"",500.0,670.0,85.0,26.5,582.0,620.0,20.0,28.0,551.0,4.0,10.0,7.0,114,"M24",19.0,23.2]
[null,"Cast Iron WNRF PN 10 DIN 28604 Size  DN 600","Cast Iron WNRF","PN 10","DIN 28604","24\"",600.0,780.0,95.0,30.0,862.0,725.0,20.0,31.0,657.0,5.0,10.0,7.0,127,"M27",22.0,32.8]
[null,"Cast Iron WNRF PN 10 DIN 28604 Size  DN 700","Cast Iron WNRF","PN 10","DIN 28604","28\"",700.0,895.0,105.0,32.5,797.0,840.0,24.0,31.0,755.0,5.0,10.0,7.0,132,"M27",22.0,44.3]
[null,"Cast Iron WNRF PN 10 DIN 28604 Size  DN 800","Cast Iron WNRF","PN 10","DIN 28604","32\"",800.0,1015.0,115.0,35.0,904.0,950.0,24.0,34.0,860.0,5.0,12.0,7.0,141,"M30",24.0,58.8]
[null,"Cast Iron WNRF PN 10 DIN 28604 Size  DN 900","Cast Iron WNRF","PN 10","DIN 28604","36\"",900.0,1115.0,125.0,37.5,1004.0,1050.0,28.0,34.0,964.0,5.0,12.0,7.0,146,"M30",24.0,69.6]
[null,"Cast Iron WNRF PN 10 DIN 28604 Size  DN 1000","Cast Iron WNRF","PN 10","DIN 28604","40\"",1000.0,1230.0,135.0,40.0,1111.0,1160.0,28.0,37.0,1068.0,5.0,12.0,7.0,157,"M33",27.0,87.6]
[null,"Cast Iron WNRF PN 10 DIN 28604 Size  DN 1200","Cast Iron WNRF","PN 10","DIN 28604","48\"",1200.0,1455.0,155.0,45.0,1329.0,1380.0,32.0,40.0,1281.0,5.0,15.0,7.0,171,"M36",29.0,136.5]
[null,"Cast Iron WNRF PN 16 DIN 28605 Size  DN 40","Cast Iron WNRF","PN 16","DIN 28605","1½\"",40.0,150.0,39.0,19.0,83.0,110.0,4.0,19.0,73.0,3.0,5.0,3.0,83,"M16",13.0,1.7]
[null,"Cast Iron WNRF PN 16 DIN 28605 Size  DN 50","Cast Iron WNRF","PN 16","DIN 28605","2\"",50.0,165.0,40.0,19.0,98.0,125.0,4.0,19.0,83.0,3.0,5.0,4.0,84,"M16",13.0,2.1]
[null,"Cast Iron WNRF PN 16 DIN 28605 Size  DN 65","Cast Iron WNRF","PN 16","DIN 28605","2½\"",65.0,185.0,41.5,19.0,118.0,145.0,4.0,19.0,99.0,3.0,5.0,4.0,84,"M16",13.0,2.6]
[null,"Cast Iron WNRF PN 16 DIN 28605 Size  DN 80","Cast Iron WNRF","PN 16","DIN 28605","3\"",80.0,200.0,43.0,19.0,133.0,160.0,8.0,19.0,115.0,3.0,6.0,4.0,84,"M16",13.0,2.8]
[null,"Cast Iron WNRF PN 16 DIN 28605 Size  DN 100","Cast Iron WNRF","PN 16","DIN 28605","4\"",100.0,220.0,45.0,19.0,153.0,180.0,8.0,19.0,134.0,3.0,6.0,5.0,85,"M16",13.0,3.3]
[null,"Cast Iron WNRF PN 16 DIN 28605 Size  DN 125","Cast Iron WNRF","PN 16","DIN 28605","5\"",125.0,250.0,47.5,19.0,183.0,210.0,8.0,19.0,160.0,3.0,6.0,5.0,85,"M16",13.0,4.0]
[null,"Cast Iron WNRF PN 16 DIN 28605 Size  DN 150","Cast Iron WNRF","PN 16","DIN 28605","6\"",150.0,285.0,50.0,19.0,209.0,240.0,8.0,23.0,185.0,3.0,6.0,6.0,92,"M20",16.0,5.0]
[null,"Cast Iron WNRF PN 16 DIN 28605 Size  DN 200","Cast Iron WNRF","PN 16","DIN 28605","8\"",200.0,340.0,55.0,20.0,264.0,295.0,12.0,23.0,237.0,3.0,8.0,6.0,94,"M20",16.0,6.7]
[null,"Cast Iron WNRF PN 16 DIN 28605 Size  DN 250","Cast Iron WNRF","PN 16","DIN 28605","10\"",250.0,400.0,60.0,22.0,319.0,355.0,12.0,28.0,291.0,3.0,8.0,6.0,104,"M24",19.0,9.4]
[null,"Cast Iron WNRF PN 16 DIN 28605 Size  DN 300","Cast Iron WNRF","PN 16","DIN 28605","12\"",300.0,455.0,65.0,24.5,372.0,410.0,12.0,28.0,346.0,4.0,8.0,6.0,109,"M24",19.0,12.6]
[null,"Cast Iron WNRF PN 16 DIN 28605 Size  DN 350","Cast Iron WNRF","PN 16","DIN 28605","14\"",350.0,520.0,70.0,26.5,432.0,470.0,16.0,28.0,400.0,4.0,10.0,7.0,114,"M24",19.0,17.5]
[null,"Cast Iron WNRF PN 16 DIN 28605 Size  DN 400","Cast Iron WNRF","PN 16","DIN 28605","16\"",400.0,580.0,75.0,28.0,484.0,525.0,16.0,31.0,452.0,4.0,10.0,7.0,123,"M27",22.0,22.1]
[null,"Cast Iron WNRF PN 16 DIN 28605 Size  DN 500","Cast Iron WNRF","PN 16","DIN 28605","20\"",500.0,715.0,85.0,31.5,606.0,650.0,20.0,34.0,559.0,4.0,12.0,7.0,134,"M30",24.0,37.4]
[null,"Cast Iron WNRF PN 16 DIN 28605 Size  DN 600","Cast Iron WNRF","PN 16","DIN 28605","24\"",600.0,840.0,95.0,36.0,721.0,770.0,20.0,37.0,666.0,5.0,12.0,7.0,149,"M33",27.0,57.6]
[null,"Cast Iron WNRF PN 16 DIN 28605 Size  DN 700","Cast Iron WNRF","PN 16","DIN 28605","28\"",700.0,910.0,105.0,39.5,791.0,840.0,24.0,37.0,765.0,5.0,12.0,7.0,156,"M33",27.0,67.4]
[null,"Cast Iron WNRF PN 16 DIN 28605 Size  DN 800","Cast Iron WNRF","PN 16","DIN 28605","32\"",800.0,1025.0,115.0,43.0,898.0,950.0,24.0,40.0,871.0,5.0,12.0,7.0,167,"M36",29.0,76.8]
[null,"Cast Iron WNRF PN 16 DIN 28605 Size  DN 900","Cast Iron WNRF","PN 16","DIN 28605","36\"",900.0,1125.0,125.0,46.5,998.0,1050.0,28.0,40.0,977.0,5.0,12.0,7.0,174,"M36",29.0,91.4]
[null,"Cast Iron WNRF PN 16 DIN 28605 Size  DN 1000","Cast Iron WNRF","PN 16","DIN 28605","40\"",1000.0,1255.0,135.0,50.0,1115.0,1170.0,28.0,43.0,1082.0,5.0,12.0,7.0,185,"M39",31.0,127.0]
[null,"Cast Iron WNRF PN 16 DIN 28605 Size  DN 1200","Cast Iron WNRF","PN 16","DIN 28605","48\"",1200.0,1455.0,155.0,57.0,1330.0,1390.0,32.0,48.0,1298.0,5.0,15.0,7.0,209,"M45",36.0,198.0]
[null,"Cast Iron WNRF PN 25 DIN 28606 Size  DN 40","Cast Iron WNRF","PN 25","DIN 28606","1½\"",40.0,15.0,39.0,19.0,83.0,110.0,4.0,19.0,73.0,3.0,5.0,3.0,83,"M16",13.0,1.7]
[null,"Cast Iron WNRF PN 25 DIN 28606 Size  DN 50","Cast Iron WNRF","PN 25","DIN 28606","2\"",50.0,165.0,40.0,19.0,98.0,125.0,4.0,19.0,83.0,3.0,5.0,4.0,84,"M16",13.0,2.1]
[null,"Cast Iron WNRF PN 25 DIN 28606 Size  DN 65","Cast Iron WNRF","PN 25","DIN 28606","2½\"",65.0,185.0,41.5,19.0,118.0,145.0,8.0,19.0,99.0,3.0,5.0,4.0,84,"M16",13.0,2.4]
[null,"Cast Iron WNRF PN 25 DIN 28606 Size  DN 80","Cast Iron WNRF","PN 25","DIN 28606","3\"",80.0,200.0,43.0,19.0,133.0,160.0,8.0,19.0,115.0,3.0,6.0,4.0,84,"M16",13.0,2.8]
[null,"Cast Iron WNRF PN 25 DIN 28606 Size  DN 100","Cast Iron WNRF","PN 25","DIN 28606","4\"",100.0,235.0,45.0,19.0,159.0,190.0,8.0,23.0,134.0,3.0,6.0,5.0,91,"M20",16.0,3.8]
[null,"Cast Iron WNRF PN 25 DIN 28606 Size  DN 125","Cast Iron WNRF","PN 25","DIN 28606","5\"",125.0,270.0,47.5,19.0,184.0,220.0,8.0,28.0,160.0,3.0,6.0,5.0,97,"M24",19.0,4.7]
[null,"Cast Iron WNRF PN 25 DIN 28606 Size  DN 150","Cast Iron WNRF","PN 25","DIN 28606","6\"",150.0,300.0,50.0,20.0,214.0,250.0,8.0,28.0,187.0,3.0,6.0,6.0,100,"M24",19.0,6.0]
[null,"Cast Iron WNRF PN 25 DIN 28606 Size  DN 200","Cast Iron WNRF","PN 25","DIN 28606","8\"",200.0,360.0,55.0,22.0,274.0,310.0,12.0,28.0,241.0,3.0,8.0,6.0,104,"M24",19.0,8.7]
[null,"Cast Iron WNRF PN 25 DIN 28606 Size  DN 250","Cast Iron WNRF","PN 25","DIN 28606","10\"",250.0,425.0,60.0,24.5,331.0,370.0,12.0,31.0,295.0,3.0,8.0,6.0,115,"M27",22.0,13.0]
[null,"Cast Iron WNRF PN 25 DIN 28606 Size  DN 300","Cast Iron WNRF","PN 25","DIN 28606","12\"",300.0,485.0,65.0,27.5,389.0,430.0,16.0,31.0,351.0,4.0,8.0,6.0,121,"M27",22.0,17.7]
[null,"Cast Iron WNRF PN 25 DIN 28606 Size  DN 350","Cast Iron WNRF","PN 25","DIN 28606","14\"",350.0,555.0,70.0,30.0,446.0,490.0,16.0,34.0,412.0,4.0,10.0,7.0,131,"M30",24.0,25.4]
[null,"Cast Iron WNRF PN 25 DIN 28606 Size  DN 400","Cast Iron WNRF","PN 25","DIN 28606","16\"",400.0,620.0,75.0,32.0,503.0,550.0,16.0,37.0,465.0,4.0,10.0,7.0,141,"M33",27.0,33.2]
[null,"Cast Iron WNRF PN 25 DIN 28606 Size  DN 500","Cast Iron WNRF","PN 25","DIN 28606","20\"",500.0,730.0,85.0,36.5,613.0,660.0,20.0,37.0,574.0,4.0,12.0,7.0,150,"M33",27.0,47.2]
[null,"Cast Iron WNRF PN 25 DIN 28606 Size  DN 600","Cast Iron WNRF","PN 25","DIN 28606","24\"",600.0,845.0,95.0,42.0,718.0,770.0,20.0,40.0,684.0,5.0,12.0,7.0,165,"M36",29.0,68.0]
[null,"Cast Iron WNRF PN 40 DIN 28607 Size  DN 40","Cast Iron WNRF","PN 40","DIN 28607","1½\"",40.0,150.0,39.0,19.0,83.0,110.0,4.0,19.0,73.0,3.0,5.0,3.0,83,"M16",13.0,1.7]
[null,"Cast Iron WNRF PN 40 DIN 28607 Size  DN 50","Cast Iron WNRF","PN 40","DIN 28607","2\"",50.0,165.0,40.0,19.0,98.0,125.0,4.0,19.0,83.0,3.0,5.0,4.0,84,"M16",13.0,2.1]
[null,"Cast Iron WNRF PN 40 DIN 28607 Size  DN 65","Cast Iron WNRF","PN 40","DIN 28607","2½\"",65.0,185.0,41.5,19.0,118.0,145.0,8.0,19.0,99.0,3.0,5.0,4.0,84,"M16",13.0,2.4]
[null,"Cast Iron WNRF PN 40 DIN 28607 Size  DN 80","Cast Iron WNRF","PN 40","DIN 28607","3\"",80.0,200.0,43.0,19.0,133.0,160.0,8.0,19.0,115.0,3.0,6.0,4.0,84,"M16",13.0,2.8]
[null,"Cast Iron WNRF PN 40 DIN 28607 Size  DN 100","Cast Iron WNRF","PN 40","DIN 28607","4\"",100.0,235.0,45.0,19.0,159.0,190.0,8.0,23.0,134.0,3.0,6.0,5.0,91,"M20",16.0,3.8]
[null,"Cast Iron WNRF PN 40 DIN 28607 Size  DN 125","Cast Iron WNRF","PN 40","DIN 28607","5\"",125.0,270.0,47.5,23.5,184.0,220.0,8.0,28.0,167.0,3.0,6.0,5.0,106,"M24",19.0,5.9]
[null,"Cast Iron WNRF PN 40 DIN 28607 Size  DN 150","Cast Iron WNRF","PN 40","DIN 28607","6\"",150.0,300.0,50.0,26.0,214.0,250.0,8.0,28.0,196.0,3.0,6.0,6.0,112,"M24",19.0,7.9]
[null,"Cast Iron WNRF PN 40 DIN 28607 Size  DN 200","Cast Iron WNRF","PN 40","DIN 28607","8\"",200.0,375.0,55.0,30.0,281.0,320.0,12.0,31.0,253.0,3.0,8.0,6.0,126,"M27",22.0,13.4]
[null,"Cast Iron WNRF PN 40 DIN 28607 Size  DN 250","Cast Iron WNRF","PN 40","DIN 28607","10\"",250.0,450.0,60.0,34.0,343.0,385.0,12.0,34.0,310.0,3.0,8.0,6.0,138,"M30",24.0,21.7]
[null,"Cast Iron WNRF PN 40 DIN 28607 Size  DN 300","Cast Iron WNRF","PN 40","DIN 28607","12\"",300.0,515.0,65.0,39.5,406.0,450.0,16.0,34.0,370.0,4.0,8.0,6.0,149,"M30",24.0,31.1]
[null,"Cast Iron WNRF PN 40 DIN 28607 Size  DN 350","Cast Iron WNRF","PN 40","DIN 28607","14\"",350.0,580.0,70.0,44.0,463.0,510.0,16.0,37.0,428.0,4.0,10.0,7.0,165,"M33",27.0,42.54]
[null,"Cast Iron WNRF PN 40 DIN 28607 Size  DN 400","Cast Iron WNRF","PN 40","DIN 28607","16\"",400.0,660.0,75.0,48.0,535.0,585.0,16.0,40.0,484.0,4.0,10.0,7.0,177,"M36",29.0,61.2]
[null,{"$f":"CONCATENATE(C1401,$C$1,$C$1,E1401,$C$1,$F$1,$C$1,$C$1,$G$2,$C$1,G1401,D1401)","v":"WN for Pr.Vessels  DIN 28034 Size  DN 300 / 20"},"WN for Pr.Vessels"," / 20","DIN 28034","12\"",300.0,415.0,49.0,20.0,"-",375.0,12.0,18.0,336.0,"-",6.0,6.0,88,"M16",13.0,10.5]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 300 / 25","WN for Pr.Vessels"," / 25","DIN 28034","12\"",300.0,430.0,54.0,25.0,"-",385.0,12.0,23.0,336.0,"-",6.0,6.0,104,"M20",16.0,14.5]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 300 / 30","WN for Pr.Vessels"," / 30","DIN 28034","12\"",300.0,445.0,59.0,30.0,"-",395.0,12.0,27.0,336.0,"-",6.0,6.0,120,"M24",19.0,18.9]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 350 / 20","WN for Pr.Vessels"," / 20","DIN 28034","14\"",350.0,460.0,49.0,20.0,"-",420.0,16.0,18.0,380.0,"-",6.0,7.0,89,"M16",13.0,11.8]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 350 / 25","WN for Pr.Vessels"," / 25","DIN 28034","14\"",350.0,475.0,54.0,25.0,"-",430.0,16.0,23.0,380.0,"-",6.0,7.0,105,"M20",16.0,16.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 350 / 35","WN for Pr.Vessels"," / 35","DIN 28034","14\"",350.0,490.0,64.0,35.0,"-",440.0,16.0,27.0,384.0,"-",8.0,7.0,131,"M24",19.0,24.1]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 400 / 20","WN for Pr.Vessels"," / 20","DIN 28034","16\"",400.0,510.0,49.0,20.0,"-",470.0,16.0,18.0,431.0,"-",6.0,7.0,89,"M16",13.0,13.4]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 400 / 25","WN for Pr.Vessels"," / 25","DIN 28034","16\"",400.0,525.0,54.0,25.0,"-",480.0,16.0,23.0,431.0,"-",6.0,7.0,105,"M20",16.0,19.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 400 / 35","WN for Pr.Vessels"," / 35","DIN 28034","16\"",400.0,545.0,67.0,35.0,"-",495.0,16.0,27.0,435.0,"-",8.0,7.0,131,"M24",19.0,30.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 450 / 20","WN for Pr.Vessels"," / 20","DIN 28034","18\"",450.0,550.0,49.0,20.0,"-",510.0,20.0,18.0,469.0,"-",6.0,7.0,89,"M16",13.0,14.6]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 450 / 25","WN for Pr.Vessels"," / 25","DIN 28034","18\"",450.0,565.0,54.0,25.0,"-",520.0,20.0,23.0,473.0,"-",6.0,7.0,105,"M20",16.0,21.1]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 450 / 35","WN for Pr.Vessels"," / 35","DIN 28034","18\"",450.0,580.0,67.0,35.0,"-",530.0,20.0,27.0,473.0,"-",8.0,7.0,131,"M24",19.0,31.3]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 500 / 25","WN for Pr.Vessels"," / 25","DIN 28034","20\"",500.0,600.0,54.0,25.0,"-",560.0,20.0,18.0,520.0,"-",6.0,7.0,99,"M16",13.0,19.5]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 500 / 30","WN for Pr.Vessels"," / 30","DIN 28034","20\"",500.0,615.0,59.0,30.0,"-",570.0,20.0,23.0,524.0,"-",6.0,7.0,115,"M20",16.0,25.6]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 500 / 35","WN for Pr.Vessels"," / 35","DIN 28034","20\"",500.0,635.0,67.0,35.0,"-",585.0,20.0,27.0,524.0,"-",8.0,7.0,131,"M24",19.0,35.6]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 500 / 45","WN for Pr.Vessels"," / 45","DIN 28034","20\"",500.0,645.0,82.0,45.0,"-",590.0,20.0,30.0,532.0,"-",8.0,7.0,157,"M27",22.0,48.6]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 600 / 30","WN for Pr.Vessels"," / 30","DIN 28034","24\"",600.0,710.0,59.0,30.0,"-",665.0,24.0,23.0,612.0,"-",6.0,7.0,115,"M20",16.0,30.7]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 600 / 40","WN for Pr.Vessels"," / 40","DIN 28034","24\"",600.0,730.0,72.0,40.0,"-",680.0,24.0,27.0,620.0,"-",8.0,7.0,141,"M24",19.0,48.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 600 / 45","WN for Pr.Vessels"," / 45","DIN 28034","24\"",600.0,745.0,82.0,45.0,"-",690.0,24.0,30.0,624.0,"-",8.0,7.0,157,"M27",22.0,59.7]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 600 / 50","WN for Pr.Vessels"," / 50","DIN 28034","24\"",600.0,760.0,95.0,50.0,"-",695.0,24.0,33.0,624.0,"-",10.0,7.0,171,"M30",24.0,75.3]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 700 / 30","WN for Pr.Vessels"," / 30","DIN 28034","28\"",700.0,810.0,59.0,30.0,"-",765.0,28.0,23.0,716.0,"-",6.0,7.0,115,"M20",16.0,34.9]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 700 / 40","WN for Pr.Vessels"," / 40","DIN 28034","28\"",700.0,830.0,72.0,40.0,"-",780.0,28.0,27.0,720.0,"-",8.0,7.0,141,"M24",19.0,55.3]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 700 / 50","WN for Pr.Vessels"," / 50","DIN 28034","28\"",700.0,845.0,92.0,50.0,"-",790.0,28.0,30.0,724.0,"-",10.0,7.0,167,"M27",22.0,76.7]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 700 / 55","WN for Pr.Vessels"," / 55","DIN 28034","28\"",700.0,865.0,105.0,55.0,"-",800.0,28.0,33.0,728.0,"-",10.0,7.0,181,"M30",24.0,99.3]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 800 / 35","WN for Pr.Vessels"," / 35","DIN 28034","32\"",800.0,915.0,64.0,35.0,"-",870.0,32.0,23.0,816.0,"-",8.0,7.0,125,"M20",16.0,47.9]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 800 / 45","WN for Pr.Vessels"," / 45","DIN 28034","32\"",800.0,930.0,82.0,45.0,"-",880.0,32.0,27.0,824.0,"-",8.0,7.0,151,"M24",19.0,72.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 800 / 50","WN for Pr.Vessels"," / 50","DIN 28034","32\"",800.0,945.0,95.0,50.0,"-",890.0,32.0,30.0,824.0,"-",10.0,7.0,167,"M27",22.0,91.6]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 800 / 55","WN for Pr.Vessels"," / 55","DIN 28034","32\"",800.0,965.0,108.0,55.0,"-",900.0,32.0,33.0,828.0,"-",10.0,7.0,181,"M30",24.0,117.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 900 / 35","WN for Pr.Vessels"," / 35","DIN 28034","36\"",900.0,1015.0,64.0,35.0,"-",970.0,36.0,23.0,916.0,"-",8.0,7.0,125,"M20",16.0,53.5]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 900 / 45","WN for Pr.Vessels"," / 45","DIN 28034","36\"",900.0,1030.0,82.0,45.0,"-",980.0,36.0,27.0,924.0,"-",8.0,7.0,151,"M24",19.0,80.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 900 / 50","WN for Pr.Vessels"," / 50","DIN 28034","36\"",900.0,1045.0,95.0,50.0,"-",990.0,36.0,30.0,924.0,"-",8.0,7.0,167,"M27",22.0,101.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 900 / 55","WN for Pr.Vessels"," / 55","DIN 28034","36\"",900.0,1065.0,108.0,55.0,"-",1000.0,36.0,33.0,928.0,"-",10.0,7.0,181,"M30",24.0,131.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1000 / 35","WN for Pr.Vessels"," / 35","DIN 28034","40\"",1000.0,1115.0,64.0,35.0,"-",1070.0,40.0,23.0,1016.0,"-",8.0,7.0,125,"M20",16.0,58.8]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1000 / 45","WN for Pr.Vessels"," / 45","DIN 28034","40\"",1000.0,1130.0,82.0,45.0,"-",1080.0,40.0,27.0,1024.0,"-",8.0,7.0,151,"M24",19.0,88.6]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1000 / 55","WN for Pr.Vessels"," / 55","DIN 28034","40\"",1000.0,1150.0,105.0,55.0,"-",1095.0,40.0,30.0,1028.0,"-",10.0,7.0,177,"M27",22.0,128.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1000 / 60","WN for Pr.Vessels"," / 60","DIN 28034","40\"",1000.0,1170.0,118.0,60.0,"-",1105.0,40.0,33.0,1032.0,"-",10.0,7.0,191,"M30",24.0,163.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1100 / 35","WN for Pr.Vessels"," / 35","DIN 28034","44\"",1100.0,1215.0,64.0,35.0,"-",1170.0,44.0,23.0,1116.0,"-",8.0,7.0,125,"M20",16.0,64.8]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1100 / 45","WN for Pr.Vessels"," / 45","DIN 28034","44\"",1100.0,1230.0,82.0,45.0,"-",1180.0,44.0,27.0,1124.0,"-",8.0,7.0,151,"M24",19.0,96.3]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1100 / 55","WN for Pr.Vessels"," / 55","DIN 28034","44\"",1100.0,1250.0,105.0,55.0,"-",1195.0,44.0,30.0,1128.0,"-",10.0,7.0,177,"M27",22.0,141.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1100 / 60","WN for Pr.Vessels"," / 60","DIN 28034","44\"",1100.0,1270.0,118.0,60.0,"-",1205.0,44.0,33.0,1132.0,"-",10.0,7.0,191,"M30",24.0,179.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1200 / 35","WN for Pr.Vessels"," / 35","DIN 28034","48\"",1200.0,1315.0,67.0,35.0,"-",1270.0,48.0,23.0,1216.0,"-",8.0,7.0,125,"M20",16.0,75.1]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1200 / 45","WN for Pr.Vessels"," / 45","DIN 28034","48\"",1200.0,1330.0,82.0,45.0,"-",1280.0,48.0,27.0,1224.0,"-",8.0,7.0,151,"M24",19.0,105.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1200 / 55","WN for Pr.Vessels"," / 55","DIN 28034","48\"",1200.0,1350.0,105.0,55.0,"-",1295.0,48.0,30.0,1228.0,"-",10.0,7.0,177,"M27",22.0,153.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1200 / 60","WN for Pr.Vessels"," / 60","DIN 28034","48\"",1200.0,1370.0,118.0,60.0,"-",1305.0,48.0,33.0,1232.0,"-",10.0,7.0,191,"M30",24.0,197.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1300 / 35","WN for Pr.Vessels"," / 35","DIN 28034","52\"",1300.0,1415.0,67.0,35.0,"-",1370.0,52.0,23.0,1316.0,"-",8.0,7.0,125,"M20",16.0,80.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1300 / 50","WN for Pr.Vessels"," / 50","DIN 28034","52\"",1300.0,1335.0,92.0,50.0,"-",1385.0,52.0,27.0,1324.0,"-",10.0,7.0,161,"M24",19.0,131.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1300 / 55","WN for Pr.Vessels"," / 55","DIN 28034","52\"",1300.0,1450.0,105.0,55.0,"-",1395.0,52.0,30.0,1328.0,"-",10.0,7.0,177,"M27",22.0,165.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1300 / 60","WN for Pr.Vessels"," / 60","DIN 28034","52\"",1300.0,1470.0,118.0,60.0,"-",1405.0,52.0,33.0,1332.0,"-",10.0,7.0,191,"M30",24.0,210.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1400 / 35","WN for Pr.Vessels"," / 35","DIN 28034","56\"",1400.0,1515.0,67.0,35.0,"-",1470.0,56.0,23.0,1416.0,"-",8.0,7.0,125,"M20",16.0,86.4]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1400 / 50","WN for Pr.Vessels"," / 50","DIN 28034","56\"",1400.0,1535.0,92.0,50.0,"-",1485.0,56.0,27.0,1424.0,"-",10.0,7.0,161,"M24",19.0,141.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1400 / 55","WN for Pr.Vessels"," / 55","DIN 28034","56\"",1400.0,1550.0,105.0,55.0,"-",1495.0,56.0,30.0,1428.0,"-",10.0,7.0,177,"M27",22.0,178.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1400 / 60","WN for Pr.Vessels"," / 60","DIN 28034","56\"",1400.0,1570.0,118.0,60.0,"-",1505.0,56.0,33.0,1432.0,"-",10.0,7.0,191,"M30",24.0,224.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1500 / 35","WN for Pr.Vessels"," / 35","DIN 28034","60\"",1500.0,1615.0,67.0,35.0,"-",1570.0,60.0,23.0,1516.0,"-",8.0,7.0,125,"M20",16.0,92.6]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1500 / 50","WN for Pr.Vessels"," / 50","DIN 28034","60\"",1500.0,1635.0,92.0,50.0,"-",1585.0,60.0,27.0,1524.0,"-",10.0,7.0,161,"M24",19.0,151.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1500 / 60","WN for Pr.Vessels"," / 60","DIN 28034","60\"",1500.0,1655.0,115.0,60.0,"-",1600.0,60.0,30.0,1532.0,"-",10.0,7.0,187,"M27",22.0,215.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1500 / 65","WN for Pr.Vessels"," / 65","DIN 28034","60\"",1500.0,1675.0,128.0,65.0,"-",1610.0,60.0,33.0,1536.0,"-",10.0,7.0,201,"M30",24.0,268.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1600 / 35","WN for Pr.Vessels"," / 35","DIN 28034","64\"",1600.0,1715.0,67.0,35.0,"-",1670.0,64.0,23.0,1616.0,"-",8.0,7.0,125,"M20",16.0,99.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1600 / 50","WN for Pr.Vessels"," / 50","DIN 28034","64\"",1600.0,1735.0,92.0,50.0,"-",1685.0,64.0,27.0,1624.0,"-",10.0,7.0,161,"M24",19.0,161.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1600 / 60","WN for Pr.Vessels"," / 60","DIN 28034","64\"",1600.0,1755.0,115.0,60.0,"-",1700.0,64.0,30.0,1632.0,"-",10.0,7.0,187,"M27",22.0,229.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1600 / 65","WN for Pr.Vessels"," / 65","DIN 28034","64\"",1600.0,175.0,128.0,65.0,"-",1710.0,64.0,33.0,1636.0,"-",10.0,7.0,201,"M30",24.0,282.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1700 / 40","WN for Pr.Vessels"," / 40","DIN 28034","68\"",1700.0,1815.0,72.0,40.0,"-",1770.0,68.0,23.0,1720.0,"-",8.0,7.0,135,"M20",16.0,118.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1700 / 50","WN for Pr.Vessels"," / 50","DIN 28034","68\"",1700.0,1835.0,92.0,50.0,"-",1785.0,68.0,27.0,1724.0,"-",10.0,7.0,161,"M24",19.0,170.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1700 / 60","WN for Pr.Vessels"," / 60","DIN 28034","68\"",1700.0,1855.0,115.0,60.0,"-",1800.0,68.0,30.0,1732.0,"-",10.0,7.0,187,"M27",22.0,242.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1700 / 65","WN for Pr.Vessels"," / 65","DIN 28034","68\"",1700.0,1875.0,128.0,65.0,"-",1810.0,68.0,33.0,1736.0,"-",10.0,7.0,201,"M30",24.0,302.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1800 / 40","WN for Pr.Vessels"," / 40","DIN 28034","72\"",1800.0,1915.0,72.0,40.0,"-",1870.0,72.0,23.0,1820.0,"-",8.0,7.0,135,"M20",16.0,125.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1800 / 55","WN for Pr.Vessels"," / 55","DIN 28034","72\"",1800.0,1940.0,102.0,55.0,"-",1890.0,72.0,27.0,1828.0,"-",10.0,7.0,171,"M24",19.0,207.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1800 / 60","WN for Pr.Vessels"," / 60","DIN 28034","72\"",1800.0,1955.0,115.0,60.0,"-",1900.0,72.0,30.0,1832.0,"-",10.0,7.0,187,"M27",22.0,255.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1800 / 65","WN for Pr.Vessels"," / 65","DIN 28034","72\"",1800.0,1975.0,128.0,65.0,"-",1910.0,72.0,33.0,1832.0,"-",10.0,7.0,201,"M30",24.0,319.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1900 / 40","WN for Pr.Vessels"," / 40","DIN 28034","76\"",1900.0,2015.0,72.0,40.0,"-",1970.0,76.0,23.0,1920.0,"-",8.0,7.0,135,"M20",16.0,132.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1900 / 55","WN for Pr.Vessels"," / 55","DIN 28034","76\"",1900.0,2040.0,102.0,55.0,"-",1990.0,76.0,27.0,1928.0,"-",10.0,7.0,171,"M24",19.0,217.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1900 / 65","WN for Pr.Vessels"," / 65","DIN 28034","76\"",1900.0,2060.0,125.0,65.0,"-",2005.0,76.0,30.0,1936.0,"-",10.0,7.0,197,"M27",22.0,304.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 1900 / 70","WN for Pr.Vessels"," / 70","DIN 28034","76\"",1900.0,2080.0,138.0,70.0,"-",2015.0,76.0,33.0,1940.0,"-",10.0,7.0,211,"M30",24.0,374.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 2000 / 40","WN for Pr.Vessels"," / 40","DIN 28034","80\"",2000.0,2115.0,72.0,40.0,"-",2070.0,80.0,23.0,2020.0,"-",8.0,7.0,135,"M20",16.0,139.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 2000 / 55","WN for Pr.Vessels"," / 55","DIN 28034","80\"",2000.0,2140.0,102.0,55.0,"-",2090.0,80.0,27.0,2028.0,"-",10.0,7.0,171,"M24",19.0,226.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 2000 / 65","WN for Pr.Vessels"," / 65","DIN 28034","80\"",2000.0,2160.0,125.0,65.0,"-",2105.0,80.0,30.0,2036.0,"-",10.0,7.0,197,"M27",22.0,319.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 2000 / 70","WN for Pr.Vessels"," / 70","DIN 28034","80\"",2000.0,2180.0,138.0,70.0,"-",2115.0,80.0,33.0,2040.0,"-",12.0,7.0,211,"M30",24.0,393.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 2100 / 40","WN for Pr.Vessels"," / 40","DIN 28034","84\"",2100.0,2215.0,72.0,40.0,"-",2170.0,84.0,23.0,2120.0,"-",8.0,7.0,135,"M20",16.0,146.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 2100 / 55","WN for Pr.Vessels"," / 55","DIN 28034","84\"",2100.0,2240.0,102.0,55.0,"-",2190.0,84.0,27.0,2128.0,"-",10.0,7.0,171,"M24",19.0,240.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 2100 / 65","WN for Pr.Vessels"," / 65","DIN 28034","84\"",2100.0,2260.0,125.0,65.0,"-",2205.0,84.0,30.0,2136.0,"-",10.0,7.0,197,"M27",22.0,327.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 2100 / 70","WN for Pr.Vessels"," / 70","DIN 28034","84\"",2100.0,2285.0,148.0,75.0,"-",2220.0,84.0,33.0,2144.0,"-",12.0,7.0,221,"M30",24.0,457.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 2200 / 40","WN for Pr.Vessels"," / 40","DIN 28034","88\"",2200.0,2315.0,72.0,40.0,"-",2270.0,86.0,23.0,2220.0,"-",8.0,7.0,135,"M20",16.0,153.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 2200 / 55","WN for Pr.Vessels"," / 55","DIN 28034","88\"",2200.0,2340.0,102.0,55.0,"-",2290.0,86.0,27.0,2228.0,"-",10.0,7.0,171,"M24",19.0,251.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 2200 / 65","WN for Pr.Vessels"," / 65","DIN 28034","88\"",2200.0,2360.0,125.0,65.0,"-",2305.0,86.0,30.0,2236.0,"-",10.0,7.0,197,"M27",22.0,350.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 2200 / 75","WN for Pr.Vessels"," / 75","DIN 28034","88\"",2200.0,2385.0,148.0,75.0,"-",2320.0,86.0,33.0,2244.0,"-",12.0,7.0,221,"M30",24.0,475.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 2300 / 40","WN for Pr.Vessels"," / 40","DIN 28034","92\"",2300.0,2415.0,72.0,40.0,"-",2370.0,92.0,23.0,2320.0,"-",8.0,7.0,135,"M20",16.0,160.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 2300 / 55","WN for Pr.Vessels"," / 55","DIN 28034","92\"",2300.0,2440.0,102.0,55.0,"-",2390.0,92.0,27.0,2328.0,"-",10.0,7.0,171,"M24",19.0,262.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 2300 / 65","WN for Pr.Vessels"," / 65","DIN 28034","92\"",2300.0,2460.0,125.0,65.0,"-",2405.0,92.0,30.0,2336.0,"-",10.0,7.0,197,"M27",22.0,365.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 2300 / 75","WN for Pr.Vessels"," / 75","DIN 28034","92\"",2300.0,2485.0,148.0,75.0,"-",2420.0,92.0,33.0,2344.0,"-",12.0,7.0,221,"M30",24.0,496.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 2400 / 45","WN for Pr.Vessels"," / 45","DIN 28034","96\"",2400.0,2520.0,82.0,45.0,"-",2475.0,96.0,23.0,2424.0,"-",8.0,7.0,145,"M20",16.0,198.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 2400 / 55","WN for Pr.Vessels"," / 55","DIN 28034","96\"",2400.0,2540.0,102.0,55.0,"-",2490.0,96.0,27.0,2428.0,"-",10.0,7.0,171,"M24",19.0,273.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 2400 / 70","WN for Pr.Vessels"," / 70","DIN 28034","96\"",2400.0,2565.0,135.0,70.0,"-",2510.0,96.0,30.0,2440.0,"-",12.0,7.0,207,"M27",22.0,427.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 2400 / 75","WN for Pr.Vessels"," / 75","DIN 28034","96\"",2400.0,2585.0,148.0,75.0,"-",2520.0,96.0,33.0,2444.0,"-",12.0,7.0,221,"M30",24.0,519.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 2600 / 45","WN for Pr.Vessels"," / 45","DIN 28034","104\"",2600.0,2720.0,82.0,45.0,"-",2675.0,104.0,23.0,2624.0,"-",8.0,7.0,145,"M20",16.0,213.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 2600 / 60","WN for Pr.Vessels"," / 60","DIN 28034","104\"",2600.0,2745.0,112.0,60.0,"-",2695.0,104.0,27.0,2632.0,"-",10.0,7.0,181,"M24",19.0,334.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 2600 / 70","WN for Pr.Vessels"," / 70","DIN 28034","104\"",2600.0,2765.0,135.0,70.0,"-",2710.0,104.0,30.0,2640.0,"-",12.0,7.0,207,"M27",22.0,458.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 2600 / 85","WN for Pr.Vessels"," / 85","DIN 28034","104\"",2600.0,2785.0,168.0,85.0,"-",2720.0,104.0,33.0,2644.0,"-",12.0,7.0,241,"M30",24.0,640.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 2800 / 45","WN for Pr.Vessels"," / 45","DIN 28034","112\"",2800.0,2920.0,82.0,45.0,"-",2875.0,112.0,23.0,2824.0,"-",8.0,7.0,145,"M20",16.0,229.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 2800 / 65","WN for Pr.Vessels"," / 65","DIN 28034","112\"",2800.0,2950.0,122.0,65.0,"-",2900.0,112.0,27.0,2836.0,"-",10.0,7.0,191,"M24",19.0,410.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 2800 / 70","WN for Pr.Vessels"," / 70","DIN 28034","112\"",2800.0,2965.0,135.0,70.0,"-",2910.0,112.0,30.0,2840.0,"-",12.0,7.0,207,"M27",22.0,491.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 2800 / 85","WN for Pr.Vessels"," / 85","DIN 28034","112\"",2800.0,2985.0,168.0,85.0,"-",2920.0,112.0,33.0,2844.0,"-",12.0,7.0,241,"M30",24.0,682.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 3000 / 45","WN for Pr.Vessels"," / 45","DIN 28034","120\"",3000.0,3120.0,82.0,45.0,"-",3075.0,120.0,23.0,3024.0,"-",8.0,7.0,145,"M20",16.0,245.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 3000 / 65","WN for Pr.Vessels"," / 65","DIN 28034","120\"",3000.0,3150.0,122.0,65.0,"-",3100.0,120.0,27.0,3036.0,"-",10.0,7.0,191,"M24",19.0,436.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 3000 / 75","WN for Pr.Vessels"," / 75","DIN 28034","120\"",3000.0,3170.0,145.0,75.0,"-",3115.0,120.0,30.0,3044.0,"-",12.0,7.0,217,"M27",22.0,584.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 3000 / 85","WN for Pr.Vessels"," / 85","DIN 28034","120\"",3000.0,3185.0,168.0,85.0,"-",3120.0,120.0,33.0,3044.0,"-",12.0,7.0,241,"M30",24.0,733.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 3200 / 45","WN for Pr.Vessels"," / 45","DIN 28034","128\"",3200.0,3320.0,82.0,45.0,"-",3275.0,128.0,23.0,3224.0,"-",8.0,7.0,145,"M20",16.0,260.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 3200 / 65","WN for Pr.Vessels"," / 65","DIN 28034","128\"",3200.0,3350.0,122.0,65.0,"-",3300.0,128.0,27.0,3236.0,"-",10.0,7.0,191,"M24",19.0,462.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 3200 / 80","WN for Pr.Vessels"," / 80","DIN 28034","128\"",3200.0,3370.0,155.0,80.0,"-",3315.0,128.0,30.0,3244.0,"-",12.0,7.0,227,"M27",22.0,645.0]
[null,"WN for Pr.Vessels  DIN 28034 Size  DN 3200 / 85","WN for Pr.Vessels"," / 85","DIN 28034","128\"",3200.0,3385.0,168.0,85.0,"-",3320.0,128.0,33.0,3244.0,"-",12.0,7.0,241,"M30",24.0,780.0]
[null,{"$f":"CONCATENATE(C1509,$C$1,D1509,$C$1,E1509,$C$1,$F$1,$C$1,$C$1,$G$2,$C$1,G1509)","v":"WNRF PN 6 NEN 5831 Size  DN 10"},"WNRF","PN 6","NEN 5831","1/4\"",10.0,75.0,28.0,12.0,35.0,50.0,4.0,11.5,26.0,2.0,4.0,7.0,63,"M10",8.0,0.34]
[null,"WNRF PN 6 NEN 5831 Size  DN 15","WNRF","PN 6","NEN 5831","1/2\"",15.0,80.0,30.0,12.0,40.0,55.0,4.0,11.5,30.0,2.0,4.0,3.0,59,"M10",8.0,0.39]
[null,"WNRF PN 6 NEN 5831 Size  DN 20","WNRF","PN 6","NEN 5831","3/4\"",20.0,90.0,32.0,14.0,50.0,65.0,4.0,11.5,38.0,2.0,4.0,3.0,63,"M10",8.0,0.59]
[null,"WNRF PN 6 NEN 5831 Size  DN 25","WNRF","PN 6","NEN 5831",1.0,25.0,100.0,35.0,14.0,60.0,75.0,4.0,11.5,42.0,2.0,4.0,3.0,63,"M10",8.0,0.75]
[null,"WNRF PN 6 NEN 5831 Size  DN 32","WNRF","PN 6","NEN 5831","1¼\"",32.0,120.0,35.0,14.0,70.0,90.0,4.0,14.0,55.0,2.0,6.0,3.0,67,"M12",10.0,1.05]
[null,"WNRF PN 6 NEN 5831 Size  DN 40","WNRF","PN 6","NEN 5831","1½\"",40.0,130.0,38.0,14.0,80.0,100.0,4.0,14.0,62.0,3.0,6.0,3.0,67,"M12",10.0,1.18]
[null,"WNRF PN 6 NEN 5831 Size  DN 50","WNRF","PN 6","NEN 5831","2\"",50.0,140.0,38.0,14.0,90.0,110.0,4.0,14.0,74.0,3.0,6.0,4.0,68,"M12",10.0,1.34]
[null,"WNRF PN 6 NEN 5831 Size  DN 65","WNRF","PN 6","NEN 5831","2½\"",65.0,160.0,38.0,14.0,110.0,130.0,4.0,14.0,88.0,3.0,6.0,4.0,68,"M12",10.0,1.67]
[null,"WNRF PN 6 NEN 5831 Size  DN 80","WNRF","PN 6","NEN 5831","3\"",80.0,190.0,42.0,16.0,128.0,150.0,4.0,18.0,102.0,3.0,8.0,4.0,78,"M16",13.0,2.71]
[null,"WNRF PN 6 NEN 5831 Size  DN 100","WNRF","PN 6","NEN 5831","4\"",100.0,210.0,45.0,16.0,148.0,170.0,4.0,18.0,130.0,3.0,8.0,5.0,79,"M16",13.0,3.24]
[null,"WNRF PN 6 NEN 5831 Size  DN 125","WNRF","PN 6","NEN 5831","5\"",125.0,240.0,48.0,18.0,178.0,200.0,8.0,18.0,155.0,3.0,8.0,5.0,83,"M16",13.0,4.49]
[null,"WNRF PN 6 NEN 5831 Size  DN 150","WNRF","PN 6","NEN 5831","6\"",150.0,265.0,48.0,18.0,202.0,225.0,8.0,18.0,184.0,3.0,10.0,6.0,84,"M16",13.0,5.15]
[null,"WNRF PN 6 NEN 5831 Size  DN 200","WNRF","PN 6","NEN 5831","8\"",200.0,320.0,55.0,20.0,258.0,280.0,8.0,18.0,236.0,3.0,10.0,6.0,88,"M16",13.0,7.78]
[null,"WNRF PN 6 NEN 5831 Size  DN 250","WNRF","PN 6","NEN 5831","10\"",250.0,375.0,60.0,22.0,312.0,335.0,12.0,18.0,290.0,3.0,12.0,6.0,92,"M16",13.0,10.8]
[null,"WNRF PN 6 NEN 5831 Size  DN 300","WNRF","PN 6","NEN 5831","12\"",300.0,440.0,62.0,22.0,365.0,395.0,12.0,23.0,342.0,4.0,12.0,6.0,98,"M20",16.0,14.0]
[null,"WNRF PN 6 NEN 5831 Size  DN 350","WNRF","PN 6","NEN 5831","14\"",350.0,490.0,62.0,22.0,415.0,445.0,12.0,23.0,385.0,4.0,12.0,7.0,99,"M20",16.0,16.1]
[null,"WNRF PN 6 NEN 5831 Size  DN 400","WNRF","PN 6","NEN 5831","16\"",400.0,540.0,65.0,22.0,465.0,495.0,16.0,23.0,438.0,4.0,12.0,7.0,99,"M20",16.0,18.3]
[null,"WNRF PN 6 NEN 5831 Size  DN 500","WNRF","PN 6","NEN 5831","20\"",500.0,645.0,68.0,24.0,570.0,600.0,20.0,23.0,538.0,4.0,12.0,7.0,103,"M20",16.0,24.6]
[null,"WNRF PN 6 NEN 5831 Size  DN 600","WNRF","PN 6","NEN 5831","24\"",600.0,755.0,70.0,24.0,670.0,705.0,20.0,27.0,640.0,5.0,12.0,7.0,109,"M24",19.0,31.5]
[null,"WNRF PN 6 NEN 5831 Size  DN 700","WNRF","PN 6","NEN 5831","28\"",700.0,860.0,70.0,24.0,775.0,810.0,24.0,27.0,740.0,5.0,12.0,7.0,109,"M24",19.0,37.4]
[null,"WNRF PN 6 NEN 5831 Size  DN 800","WNRF","PN 6","NEN 5831","32\"",800.0,975.0,70.0,24.0,880.0,920.0,24.0,30.0,842.0,5.0,12.0,7.0,115,"M27",22.0,46.1]
[null,"WNRF PN 6 NEN 5831 Size  DN 900","WNRF","PN 6","NEN 5831","36\"",900.0,1075.0,70.0,26.0,980.0,1020.0,24.0,30.0,942.0,5.0,12.0,7.0,119,"M27",22.0,55.6]
[null,"WNRF PN 6 NEN 5831 Size  DN 1000","WNRF","PN 6","NEN 5831","40\"",1000.0,1175.0,70.0,26.0,1080.0,1120.0,28.0,30.0,1045.0,5.0,16.0,7.0,119,"M27",22.0,61.9]
[null,"WNRF PN 6 NEN 5831 Size  DN 1200","WNRF","PN 6","NEN 5831","48\"",1200.0,1405.0,90.0,28.0,1295.0,1340.0,32.0,33.0,1248.0,5.0,16.0,7.0,127,"M30",24.0,100.0]
[null,"WNRF PN 6 NEN 5831 Size  DN 1400","WNRF","PN 6","NEN 5831","56\"",1400.0,1630.0,90.0,32.0,1510.0,1560.0,36.0,36.0,1452.0,5.0,16.0,7.0,139,"M33",26.0,149.0]
[null,"WNRF PN 6 NEN 5831 Size  DN 1600","WNRF","PN 6","NEN 5831","64\"",1600.0,1830.0,90.0,34.0,1710.0,1760.0,40.0,36.0,1655.0,5.0,16.0,7.0,143,"M33",26.0,180.0]
[null,"WNRF PN 6 NEN 5831 Size  DN 1800","WNRF","PN 6","NEN 5831","72\"",1800.0,2045.0,100.0,36.0,1920.0,1970.0,44.0,39.0,1855.0,5.0,16.0,7.0,153,"M36",29.0,225.0]
[null,"WNRF PN 6 NEN 5831 Size  DN 2000","WNRF","PN 6","NEN 5831","80\"",2000.0,2265.0,110.0,38.0,2125.0,2180.0,48.0,42.0,2058.0,5.0,16.0,7.0,161,"M39",31.0,295.0]
[null,"WNRF PN 6 NEN 5831 Size  DN 2200","WNRF","PN 6","NEN 5831","88\"",2200.0,2475.0,115.0,42.0,2335.0,2390.0,52.0,42.0,2260.0,6.0,18.0,7.0,169,"M39",31.0,361.0]
[null,"WNRF PN 6 NEN 5831 Size  DN 2400","WNRF","PN 6","NEN 5831","96\"",2400.0,2685.0,125.0,44.0,2545.0,2600.0,56.0,42.0,2462.0,6.0,18.0,7.0,173,"M39",31.0,415.0]
[null,"WNRF PN 6 NEN 5831 Size  DN 2600","WNRF","PN 6","NEN 5831","104\"",2600.0,2905.0,130.0,46.0,2750.0,2810.0,60.0,48.0,2665.0,6.0,18.0,7.0,187,"M45",36.0,530.0]
[null,"WNRF PN 6 NEN 5831 Size  DN 2800","WNRF","PN 6","NEN 5831","112\"",2800.0,3115.0,135.0,48.0,2960.0,3020.0,64.0,48.0,2865.0,6.0,18.0,7.0,191,"M45",36.0,643.0]
[null,"WNRF PN 6 NEN 5831 Size  DN 3000","WNRF","PN 6","NEN 5831","120\"",3000.0,3315.0,140.0,50.0,3160.0,3220.0,68.0,48.0,3068.0,6.0,18.0,7.0,195,"M45",36.0,777.0]
[null,"WNRF PN 6 NEN 5831 Size  DN 3200","WNRF","PN 6","NEN 5831","128\"",3200.0,3525.0,150.0,54.0,3370.0,3430.0,72.0,48.0,3272.0,6.0,20.0,7.0,203,"M45",36.0,851.0]
[null,"WNRF PN 6 NEN 5831 Size  DN 3400","WNRF","PN 6","NEN 5831","136\"",3400.0,3735.0,160.0,56.0,3580.0,3640.0,76.0,48.0,3475.0,6.0,20.0,7.0,207,"M45",36.0,993.0]
[null,"WNRF PN 6 NEN 5831 Size  DN 3600","WNRF","PN 6","NEN 5831","144\"",3600.0,3970.0,165.0,60.0,3790.0,3860.0,80.0,56.0,3678.0,6.0,20.0,7.0,227,"M52",42.0,1001.0]
[null,"WNRF PN 10 NEN 5832 Size  DN 10","WNRF","PN 10","NEN 5832","1/4\"",10.0,90.0,35.0,14.0,40.0,60.0,4.0,14.0,28.0,2.0,4.0,3.0,67,"M12",10.0,0.58]
[null,"WNRF PN 10 NEN 5832 Size  DN 15","WNRF","PN 10","NEN 5832","1/2\"",15.0,95.0,35.0,14.0,45.0,65.0,4.0,14.0,32.0,2.0,4.0,3.0,67,"M12",10.0,0.65]
[null,"WNRF PN 10 NEN 5832 Size  DN 20","WNRF","PN 10","NEN 5832","3/4\"",20.0,105.0,38.0,16.0,58.0,75.0,4.0,14.0,40.0,2.0,4.0,3.0,71,"M12",10.0,0.95]
[null,"WNRF PN 10 NEN 5832 Size  DN 25","WNRF","PN 10","NEN 5832",1.0,25.0,115.0,38.0,16.0,68.0,85.0,4.0,14.0,45.0,2.0,4.0,3.0,71,"M12",10.0,1.14]
[null,"WNRF PN 10 NEN 5832 Size  DN 32","WNRF","PN 10","NEN 5832","1¼\"",32.0,140.0,40.0,16.0,78.0,100.0,4.0,18.0,56.0,2.0,6.0,3.0,77,"M16",13.0,1.69]
[null,"WNRF PN 10 NEN 5832 Size  DN 40","WNRF","PN 10","NEN 5832","1½\"",40.0,150.0,42.0,16.0,88.0,110.0,4.0,18.0,64.0,3.0,6.0,3.0,77,"M16",13.0,1.86]
[null,"WNRF PN 10 NEN 5832 Size  DN 50","WNRF","PN 10","NEN 5832","2\"",50.0,165.0,45.0,18.0,102.0,125.0,4.0,18.0,75.0,3.0,6.0,4.0,82,"M16",13.0,2.53]
[null,"WNRF PN 10 NEN 5832 Size  DN 65","WNRF","PN 10","NEN 5832","2½\"",65.0,185.0,45.0,18.0,122.0,145.0,4.0,18.0,90.0,3.0,6.0,4.0,82,"M16",13.0,3.06]
[null,"WNRF PN 10 NEN 5832 Size  DN 80","WNRF","PN 10","NEN 5832","3\"",80.0,200.0,50.0,20.0,138.0,160.0,4.0,18.0,105.0,3.0,8.0,4.0,86,"M16",13.0,3.7]
[null,"WNRF PN 10 NEN 5832 Size  DN 100","WNRF","PN 10","NEN 5832","4\"",100.0,220.0,52.0,20.0,158.0,180.0,8.0,18.0,131.0,3.0,8.0,5.0,87,"M16",13.0,4.62]
[null,"WNRF PN 10 NEN 5832 Size  DN 125","WNRF","PN 10","NEN 5832","5\"",125.0,250.0,55.0,22.0,188.0,210.0,8.0,18.0,156.0,3.0,8.0,5.0,91,"M16",13.0,6.3]
[null,"WNRF PN 10 NEN 5832 Size  DN 150","WNRF","PN 10","NEN 5832","6\"",150.0,285.0,55.0,22.0,212.0,240.0,8.0,23.0,184.0,3.0,10.0,6.0,98,"M20",16.0,7.75]
[null,"WNRF PN 10 NEN 5832 Size  DN 175","WNRF","PN 10","NEN 5832","7\"",175.0,315.0,60.0,24.0,242.0,270.0,8.0,23.0,210.0,3.0,10.0,6.0,102,"M20",16.0,10.0]
[null,"WNRF PN 10 NEN 5832 Size  DN 200","WNRF","PN 10","NEN 5832","8\"",200.0,340.0,62.0,24.0,268.0,295.0,8.0,23.0,235.0,3.0,10.0,6.0,102,"M20",16.0,11.3]
[null,"WNRF PN 10 NEN 5832 Size  DN 250","WNRF","PN 10","NEN 5832","10\"",250.0,395.0,68.0,26.0,320.0,350.0,12.0,23.0,292.0,3.0,12.0,6.0,106,"M20",16.0,14.7]
[null,"WNRF PN 10 NEN 5832 Size  DN 300","WNRF","PN 10","NEN 5832","12\"",300.0,445.0,68.0,26.0,370.0,400.0,12.0,23.0,344.0,4.0,12.0,6.0,106,"M20",16.0,17.6]
[null,"WNRF PN 10 NEN 5832 Size  DN 350","WNRF","PN 10","NEN 5832","14\"",350.0,505.0,68.0,26.0,430.0,460.0,16.0,23.0,385.0,4.0,12.0,7.0,107,"M20",16.0,21.4]
[null,"WNRF PN 10 NEN 5832 Size  DN 400","WNRF","PN 10","NEN 5832","16\"",400.0,565.0,72.0,26.0,482.0,515.0,16.0,27.0,440.0,4.0,12.0,7.0,113,"M24",19.0,26.1]
[null,"WNRF PN 10 NEN 5832 Size  DN 500","WNRF","PN 10","NEN 5832","20\"",500.0,670.0,75.0,28.0,585.0,620.0,20.0,27.0,542.0,4.0,12.0,7.0,117,"M24",19.0,34.7]
[null,"WNRF PN 10 NEN 5832 Size  DN 600","WNRF","PN 10","NEN 5832","24\"",600.0,780.0,80.0,28.0,685.0,725.0,20.0,30.0,642.0,5.0,12.0,7.0,123,"M27",22.0,42.2]
[null,"WNRF PN 10 NEN 5832 Size  DN 700","WNRF","PN 10","NEN 5832","28\"",700.0,895.0,80.0,30.0,800.0,840.0,24.0,30.0,745.0,5.0,12.0,7.0,127,"M27",22.0,58.7]
[null,"WNRF PN 10 NEN 5832 Size  DN 800","WNRF","PN 10","NEN 5832","32\"",800.0,1015.0,90.0,32.0,905.0,950.0,24.0,33.0,850.0,5.0,12.0,7.0,135,"M30",24.0,80.0]
[null,"WNRF PN 10 NEN 5832 Size  DN 900","WNRF","PN 10","NEN 5832","36\"",900.0,1115.0,95.0,34.0,1005.0,1050.0,28.0,33.0,950.0,5.0,12.0,7.0,139,"M30",24.0,95.6]
[null,"WNRF PN 10 NEN 5832 Size  DN 1000","WNRF","PN 10","NEN 5832","40\"",1000.0,1230.0,95.0,34.0,1110.0,1160.0,28.0,36.0,1052.0,5.0,16.0,7.0,143,"M33",26.0,114.0]
[null,"WNRF PN 10 NEN 5832 Size  DN 1200","WNRF","PN 10","NEN 5832","48\"",1200.0,1455.0,115.0,38.0,1330.0,1380.0,32.0,39.0,1255.0,5.0,16.0,7.0,157,"M36",29.0,182.0]
[null,"WNRF PN 10 NEN 5832 Size  DN 1400","WNRF","PN 10","NEN 5832","56\"",1400.0,1675.0,120.0,42.0,1535.0,1590.0,36.0,42.0,1460.0,5.0,16.0,7.0,169,"M39",31.0,248.0]
[null,"WNRF PN 10 NEN 5832 Size  DN 1600","WNRF","PN 10","NEN 5832","64\"",1600.0,1915.0,130.0,46.0,1760.0,1820.0,40.0,48.0,1665.0,5.0,16.0,7.0,187,"M45",36.0,347.0]
[null,"WNRF PN 10 NEN 5832 Size  DN 1800","WNRF","PN 10","NEN 5832","72\"",1800.0,2115.0,140.0,50.0,1960.0,2020.0,44.0,48.0,1868.0,5.0,16.0,7.0,195,"M45",36.0,430.0]
[null,"WNRF PN 10 NEN 5832 Size  DN 2000","WNRF","PN 10","NEN 5832","80\"",2000.0,2325.0,150.0,54.0,2170.0,2230.0,48.0,48.0,2072.0,5.0,16.0,7.0,203,"M45",36.0,539.0]
[null,"WNRF PN 10 NEN 5832 Size  DN 2200","WNRF","PN 10","NEN 5832","88\"",2200.0,2550.0,160.0,58.0,2370.0,2440.0,52.0,56.0,2275.0,6.0,18.0,7.0,223,"M52",42.0,658.0]
[null,"WNRF PN 10 NEN 5832 Size  DN 2400","WNRF","PN 10","NEN 5832","96\"",2400.0,2760.0,170.0,62.0,2570.0,2650.0,56.0,56.0,2478.0,6.0,18.0,7.0,231,"M52",42.0,825.0]
[null,"WNRF PN 10 NEN 5832 Size  DN 2600","WNRF","PN 10","NEN 5832","104'",2600.0,2960.0,180.0,66.0,2780.0,2850.0,60.0,56.0,2680.0,6.0,18.0,7.0,239,"M52",42.0,979.0]
[null,"WNRF PN 10 NEN 5832 Size  DN 2800","WNRF","PN 10","NEN 5832","112\"",2800.0,3180.0,190.0,70.0,3000.0,3070.0,64.0,56.0,2882.0,6.0,18.0,7.0,247,"M52",42.0,1156.0]
[null,"WNRF PN 10 NEN 5832 Size  DN 3000","WNRF","PN 10","NEN 5832","120\"",3000.0,3405.0,200.0,74.0,3210.0,3290.0,68.0,62.0,3085.0,6.0,18.0,7.0,261,"M56",45.0,1402.0]
[null,"WNRF PN 16 NEN 5833 Size  DN 10","WNRF","PN 16","NEN 5833","1/4\"",10.0,90.0,35.0,14.0,40.0,60.0,4.0,14.0,28.0,2.0,4.0,3.0,67,"M12",10.0,0.58]
[null,"WNRF PN 16 NEN 5833 Size  DN 15","WNRF","PN 16","NEN 5833","1/2\"",15.0,95.0,35.0,14.0,45.0,65.0,4.0,14.0,32.0,2.0,4.0,3.0,67,"M12",10.0,0.65]
[null,"WNRF PN 16 NEN 5833 Size  DN 20","WNRF","PN 16","NEN 5833","3/4\"",20.0,105.0,38.0,16.0,58.0,75.0,4.0,14.0,40.0,2.0,4.0,3.0,71,"M12",10.0,0.95]
[null,"WNRF PN 16 NEN 5833 Size  DN 25","WNRF","PN 16","NEN 5833",1.0,25.0,115.0,38.0,16.0,68.0,85.0,4.0,14.0,45.0,2.0,4.0,3.0,71,"M12",10.0,1.14]
[null,"WNRF PN 16 NEN 5833 Size  DN 32","WNRF","PN 16","NEN 5833","1¼\"",32.0,140.0,40.0,16.0,78.0,100.0,4.0,18.0,56.0,2.0,6.0,3.0,77,"M16",13.0,1.69]
[null,"WNRF PN 16 NEN 5833 Size  DN 40","WNRF","PN 16","NEN 5833","1½\"",40.0,150.0,42.0,16.0,88.0,110.0,4.0,18.0,64.0,3.0,6.0,3.0,77,"M16",13.0,1.86]
[null,"WNRF PN 16 NEN 5833 Size  DN 50","WNRF","PN 16","NEN 5833","2\"",50.0,165.0,45.0,18.0,102.0,125.0,4.0,18.0,75.0,3.0,6.0,4.0,82,"M16",13.0,2.53]
[null,"WNRF PN 16 NEN 5833 Size  DN 65","WNRF","PN 16","NEN 5833","2½\"",65.0,185.0,45.0,18.0,122.0,145.0,4.0,18.0,90.0,3.0,6.0,4.0,82,"M16",13.0,3.06]
[null,"WNRF PN 16 NEN 5833 Size  DN 80","WNRF","PN 16","NEN 5833","3\"",80.0,200.0,50.0,20.0,138.0,160.0,8.0,18.0,105.0,3.0,8.0,4.0,86,"M16",13.0,3.7]
[null,"WNRF PN 16 NEN 5833 Size  DN 100","WNRF","PN 16","NEN 5833","4\"",100.0,220.0,52.0,20.0,158.0,180.0,8.0,18.0,131.0,3.0,8.0,5.0,87,"M16",13.0,4.62]
[null,"WNRF PN 16 NEN 5833 Size  DN 125","WNRF","PN 16","NEN 5833","5\"",125.0,250.0,55.0,22.0,188.0,210.0,8.0,18.0,156.0,3.0,8.0,5.0,91,"M16",13.0,6.3]
[null,"WNRF PN 16 NEN 5833 Size  DN 150","WNRF","PN 16","NEN 5833","6\"",150.0,285.0,55.0,22.0,212.0,240.0,8.0,23.0,184.0,3.0,10.0,6.0,98,"M20",16.0,7.75]
[null,"WNRF PN 16 NEN 5833 Size  DN 175","WNRF","PN 16","NEN 5833","7\"",175.0,315.0,60.0,24.0,242.0,270.0,8.0,23.0,210.0,3.0,10.0,6.0,102,"M20",16.0,10.0]
[null,"WNRF PN 16 NEN 5833 Size  DN 200","WNRF","PN 16","NEN 5833","8\"",200.0,340.0,62.0,24.0,268.0,295.0,12.0,23.0,235.0,3.0,10.0,6.0,102,"M20",16.0,11.0]
[null,"WNRF PN 16 NEN 5833 Size  DN 250","WNRF","PN 16","NEN 5833","10\"",250.0,405.0,70.0,26.0,320.0,355.0,12.0,27.0,292.0,3.0,12.0,6.0,112,"M24",19.0,15.6]
[null,"WNRF PN 16 NEN 5833 Size  DN 300","WNRF","PN 16","NEN 5833","12\"",300.0,460.0,78.0,28.0,378.0,410.0,12.0,27.0,344.0,4.0,12.0,6.0,116,"M24",19.0,22.0]
[null,"WNRF PN 16 NEN 5833 Size  DN 350","WNRF","PN 16","NEN 5833","14\"",350.0,520.0,82.0,30.0,438.0,470.0,16.0,27.0,390.0,4.0,12.0,7.0,121,"M24",19.0,28.7]
[null,"WNRF PN 16 NEN 5833 Size  DN 400","WNRF","PN 16","NEN 5833","16\"",400.0,580.0,85.0,32.0,490.0,525.0,16.0,30.0,445.0,4.0,12.0,7.0,131,"M27",22.0,36.3]
[null,"WNRF PN 16 NEN 5833 Size  DN 500","WNRF","PN 16","NEN 5833","20\"",500.0,715.0,90.0,34.0,610.0,650.0,20.0,33.0,548.0,4.0,12.0,7.0,139,"M30",24.0,59.3]
[null,"WNRF PN 16 NEN 5833 Size  DN 600","WNRF","PN 16","NEN 5833","24\"",600.0,840.0,95.0,36.0,725.0,770.0,20.0,36.0,652.0,5.0,12.0,7.0,147,"M33",26.0,73.4]
[null,"WNRF PN 16 NEN 5833 Size  DN 700","WNRF","PN 16","NEN 5833","28\"",700.0,910.0,100.0,36.0,795.0,840.0,24.0,36.0,755.0,5.0,12.0,7.0,147,"M33",26.0,75.0]
[null,"WNRF PN 16 NEN 5833 Size  DN 800","WNRF","PN 16","NEN 5833","32\"",800.0,1025.0,105.0,38.0,900.0,950.0,24.0,39.0,855.0,5.0,12.0,7.0,157,"M36",29.0,99.0]
[null,"WNRF PN 16 NEN 5833 Size  DN 900","WNRF","PN 16","NEN 5833","36\"",900.0,1125.0,110.0,40.0,1000.0,1050.0,28.0,39.0,955.0,5.0,12.0,7.0,161,"M36",29.0,119.0]
[null,"WNRF PN 16 NEN 5833 Size  DN 1000","WNRF","PN 16","NEN 5833","40\"",1000.0,1255.0,120.0,42.0,1115.0,1170.0,28.0,42.0,1058.0,5.0,16.0,7.0,169,"M39",31.0,159.0]
[null,"WNRF PN 16 NEN 5833 Size  DN 1200","WNRF","PN 16","NEN 5833","48\"",1200.0,1485.0,130.0,48.0,1330.0,1390.0,32.0,48.0,1262.0,5.0,16.0,7.0,191,"M45",36.0,243.0]
[null,"WNRF PN 16 NEN 5833 Size  DN 1400","WNRF","PN 16","NEN 5833","56\"",1400.0,1685.0,145.0,52.0,1530.0,1590.0,36.0,48.0,1465.0,5.0,16.0,7.0,199,"M45",36.0,323.0]
[null,"WNRF PN 16 NEN 5833 Size  DN 1600","WNRF","PN 16","NEN 5833","64\"",1600.0,1930.0,160.0,58.0,1750.0,1820.0,40.0,56.0,1668.0,5.0,16.0,7.0,223,"M52",42.0,479.0]
[null,"WNRF PN 16 NEN 5833 Size  DN 1800","WNRF","PN 16","NEN 5833","72\"",1800.0,2130.0,170.0,62.0,1950.0,2020.0,44.0,56.0,1870.0,5.0,16.0,7.0,231,"M52",42.0,599.0]
[null,"WNRF PN 16 NEN 5833 Size  DN 2000","WNRF","PN 16","NEN 5833","80\"",2000.0,2345.0,180.0,66.0,2150.0,2230.0,48.0,62.0,2072.0,5.0,16.0,7.0,245,"M56",45.0,719.0]
[null,"WNRF PN 25 NEN 5834 Size  DN 10","WNRF","PN 25","NEN 5834","1/4\"",10.0,90.0,35.0,16.0,40.0,60.0,4.0,14.0,28.0,2.0,4.0,3.0,71,"M12",10.0,0.661]
[null,"WNRF PN 25 NEN 5834 Size  DN 15","WNRF","PN 25","NEN 5834","1/2\"",15.0,95.0,38.0,16.0,45.0,65.0,4.0,14.0,32.0,2.0,4.0,3.0,71,"M12",10.0,0.746]
[null,"WNRF PN 25 NEN 5834 Size  DN 20","WNRF","PN 25","NEN 5834","3/4\"",20.0,105.0,40.0,18.0,58.0,75.0,4.0,14.0,40.0,2.0,4.0,3.0,75,"M12",10.0,1.06]
[null,"WNRF PN 25 NEN 5834 Size  DN 25","WNRF","PN 25","NEN 5834",1.0,25.0,115.0,40.0,18.0,68.0,85.0,4.0,14.0,46.0,2.0,4.0,3.0,75,"M12",10.0,1.29]
[null,"WNRF PN 25 NEN 5834 Size  DN 32","WNRF","PN 25","NEN 5834","1¼\"",32.0,140.0,42.0,18.0,78.0,100.0,4.0,18.0,56.0,2.0,6.0,3.0,81,"M16",13.0,1.88]
[null,"WNRF PN 25 NEN 5834 Size  DN 40","WNRF","PN 25","NEN 5834","1½\"",40.0,150.0,45.0,18.0,88.0,110.0,4.0,18.0,64.0,3.0,6.0,3.0,81,"M16",13.0,2.33]
[null,"WNRF PN 25 NEN 5834 Size  DN 50","WNRF","PN 25","NEN 5834","2\"",50.0,165.0,48.0,20.0,102.0,125.0,4.0,18.0,75.0,3.0,6.0,4.0,86,"M16",13.0,2.82]
[null,"WNRF PN 25 NEN 5834 Size  DN 65","WNRF","PN 25","NEN 5834","2½\"",65.0,185.0,52.0,22.0,122.0,145.0,8.0,18.0,90.0,3.0,6.0,4.0,90,"M16",13.0,3.74]
[null,"WNRF PN 25 NEN 5834 Size  DN 80","WNRF","PN 25","NEN 5834","3\"",80.0,200.0,58.0,24.0,138.0,160.0,8.0,18.0,105.0,3.0,8.0,4.0,94,"M16",13.0,4.75]
[null,"WNRF PN 25 NEN 5834 Size  DN 100","WNRF","PN 25","NEN 5834","4\"",100.0,235.0,65.0,24.0,162.0,190.0,8.0,23.0,134.0,3.0,8.0,5.0,101,"M20",16.0,6.52]
[null,"WNRF PN 25 NEN 5834 Size  DN 125","WNRF","PN 25","NEN 5834","5\"",125.0,270.0,68.0,26.0,188.0,220.0,8.0,27.0,162.0,3.0,8.0,5.0,111,"M24",19.0,9.07]
[null,"WNRF PN 25 NEN 5834 Size  DN 150","WNRF","PN 25","NEN 5834","6\"",150.0,300.0,75.0,28.0,218.0,250.0,8.0,27.0,192.0,3.0,10.0,6.0,116,"M24",19.0,11.8]
[null,"WNRF PN 25 NEN 5834 Size  DN 175","WNRF","PN 25","NEN 5834","7\"",175.0,320.0,75.0,28.0,248.0,280.0,12.0,27.0,218.0,3.0,10.0,6.0,116,"M24",19.0,13.4]
[null,"WNRF PN 25 NEN 5834 Size  DN 200","WNRF","PN 25","NEN 5834","8\"",200.0,360.0,80.0,30.0,278.0,310.0,12.0,27.0,244.0,3.0,10.0,6.0,120,"M24",19.0,17.0]
[null,"WNRF PN 25 NEN 5834 Size  DN 250","WNRF","PN 25","NEN 5834","10\"",250.0,425.0,88.0,32.0,335.0,370.0,12.0,30.0,298.0,3.0,12.0,6.0,130,"M27",22.0,24.4]
[null,"WNRF PN 25 NEN 5834 Size  DN 300","WNRF","PN 25","NEN 5834","12\"",300.0,485.0,92.0,34.0,395.0,430.0,16.0,30.0,352.0,4.0,12.0,6.0,134,"M27",22.0,31.2]
[null,"WNRF PN 25 NEN 5834 Size  DN 350","WNRF","PN 25","NEN 5834","14\"",350.0,555.0,100.0,38.0,450.0,490.0,16.0,33.0,398.0,4.0,12.0,7.0,147,"M30",24.0,45.0]
[null,"WNRF PN 25 NEN 5834 Size  DN 400","WNRF","PN 25","NEN 5834","16\"",400.0,620.0,110.0,40.0,505.0,550.0,16.0,36.0,452.0,4.0,12.0,7.0,155,"M33",26.0,58.7]
[null,"WNRF PN 25 NEN 5834 Size  DN 500","WNRF","PN 25","NEN 5834","20\"",500.0,730.0,125.0,44.0,615.0,660.0,20.0,36.0,558.0,4.0,12.0,7.0,163,"M33",26.0,86.1]
[null,"WNRF PN 25 NEN 5834 Size  DN 600","WNRF","PN 25","NEN 5834","24\"",600.0,845.0,125.0,46.0,720.0,770.0,20.0,39.0,660.0,5.0,12.0,7.0,173,"M36",29.0,101.0]
[null,"WNRF PN 25 NEN 5834 Size  DN 700","WNRF","PN 25","NEN 5834","28\"",700.0,960.0,125.0,46.0,820.0,875.0,24.0,42.0,760.0,5.0,12.0,7.0,177,"M39",31.0,134.0]
[null,"WNRF PN 25 NEN 5834 Size  DN 800","WNRF","PN 25","NEN 5834","32\"",800.0,1085.0,135.0,50.0,930.0,990.0,24.0,48.0,865.0,5.0,12.0,7.0,195,"M45",36.0,183.0]
[null,"WNRF PN 25 NEN 5834 Size  DN 900","WNRF","PN 25","NEN 5834","36\"",900.0,1185.0,145.0,54.0,1030.0,1090.0,28.0,48.0,968.0,5.0,12.0,7.0,203,"M45",36.0,232.0]
[null,"WNRF PN 25 NEN 5834 Size  DN 1000","WNRF","PN 25","NEN 5834","40\"",1000.0,1320.0,155.0,58.0,1140.0,1210.0,28.0,56.0,1070.0,5.0,16.0,7.0,223,"M52",42.0,302.0]
[null,"WNRF PN 40 NEN 5835 Size  DN 10","WNRF","PN 40","NEN 5835","1/4\"",10.0,90.0,35.0,16.0,40.0,60.0,4.0,14.0,28.0,2.0,4.0,3.0,71,"M12",10.0,0.661]
[null,"WNRF PN 40 NEN 5835 Size  DN 15","WNRF","PN 40","NEN 5835","1/2\"",15.0,95.0,38.0,16.0,45.0,65.0,4.0,14.0,32.0,2.0,4.0,3.0,71,"M12",10.0,0.746]
[null,"WNRF PN 40 NEN 5835 Size  DN 20","WNRF","PN 40","NEN 5835","3/4\"",20.0,105.0,40.0,18.0,58.0,75.0,4.0,14.0,40.0,2.0,4.0,3.0,75,"M12",10.0,1.06]
[null,"WNRF PN 40 NEN 5835 Size  DN 25","WNRF","PN 40","NEN 5835",1.0,25.0,115.0,40.0,18.0,68.0,85.0,4.0,14.0,46.0,2.0,4.0,3.0,75,"M12",10.0,1.29]
[null,"WNRF PN 40 NEN 5835 Size  DN 32","WNRF","PN 40","NEN 5835","1¼\"",32.0,140.0,42.0,18.0,78.0,100.0,4.0,18.0,56.0,2.0,6.0,3.0,81,"M16",13.0,1.88]
[null,"WNRF PN 40 NEN 5835 Size  DN 40","WNRF","PN 40","NEN 5835","1½\"",40.0,150.0,45.0,18.0,88.0,110.0,4.0,18.0,64.0,3.0,6.0,3.0,81,"M16",13.0,2.33]
[null,"WNRF PN 40 NEN 5835 Size  DN 50","WNRF","PN 40","NEN 5835","2\"",50.0,165.0,48.0,20.0,102.0,125.0,4.0,18.0,75.0,3.0,6.0,4.0,86,"M16",13.0,2.82]
[null,"WNRF PN 40 NEN 5835 Size  DN 65","WNRF","PN 40","NEN 5835","2½\"",65.0,185.0,52.0,22.0,122.0,145.0,8.0,18.0,90.0,3.0,6.0,4.0,90,"M16",13.0,3.74]
[null,"WNRF PN 40 NEN 5835 Size  DN 80","WNRF","PN 40","NEN 5835","3\"",80.0,200.0,58.0,24.0,138.0,160.0,8.0,18.0,105.0,3.0,8.0,4.0,94,"M16",13.0,4.75]
[null,"WNRF PN 40 NEN 5835 Size  DN 100","WNRF","PN 40","NEN 5835","4\"",100.0,235.0,65.0,24.0,162.0,190.0,8.0,23.0,134.0,3.0,8.0,5.0,101,"M20",16.0,6.52]
[null,"WNRF PN 40 NEN 5835 Size  DN 125","WNRF","PN 40","NEN 5835","5\"",125.0,270.0,68.0,26.0,188.0,220.0,8.0,27.0,162.0,3.0,8.0,5.0,111,"M24",19.0,9.07]
[null,"WNRF PN 40 NEN 5835 Size  DN 150","WNRF","PN 40","NEN 5835","6\"",150.0,300.0,75.0,28.0,218.0,250.0,8.0,27.0,192.0,3.0,10.0,6.0,116,"M24",19.0,11.8]
[null,"WNRF PN 40 NEN 5835 Size  DN 175","WNRF","PN 40","NEN 5835","7\"",175.0,350.0,82.0,32.0,260.0,295.0,12.0,30.0,218.0,3.0,10.0,6.0,130,"M27",22.0,18.2]
[null,"WNRF PN 40 NEN 5835 Size  DN 200","WNRF","PN 40","NEN 5835","8\"",200.0,375.0,88.0,34.0,285.0,320.0,12.0,30.0,244.0,3.0,10.0,6.0,134,"M27",22.0,21.5]
[null,"WNRF PN 40 NEN 5835 Size  DN 250","WNRF","PN 40","NEN 5835","10\"",250.0,450.0,105.0,38.0,345.0,385.0,12.0,33.0,306.0,3.0,12.0,6.0,146,"M30",24.0,34.9]
[null,"WNRF PN 40 NEN 5835 Size  DN 300","WNRF","PN 40","NEN 5835","12\"",300.0,515.0,115.0,42.0,410.0,450.0,16.0,33.0,362.0,4.0,12.0,6.0,154,"M30",24.0,49.7]
[null,"WNRF PN 40 NEN 5835 Size  DN 350","WNRF","PN 40","NEN 5835","14\"",350.0,580.0,125.0,46.0,465.0,510.0,16.0,36.0,408.0,4.0,12.0,7.0,167,"M33",26.0,68.1]
[null,"WNRF PN 40 NEN 5835 Size  DN 400","WNRF","PN 40","NEN 5835","16\"",400.0,660.0,135.0,50.0,535.0,585.0,16.0,39.0,462.0,4.0,12.0,7.0,181,"M36",29.0,96.5]
[null,"WNRF PN 40 NEN 5835 Size  DN 500","WNRF","PN 40","NEN 5835","20\"",500.0,755.0,140.0,52.0,615.0,670.0,20.0,42.0,562.0,4.0,12.0,7.0,189,"M39",31.0,117.0]
[null,"WNRF 5K (PN 5) JIS B 2211 Size  DN 10","WNRF","5K (PN 5)","JIS B 2211","1/4\"",10.0,75.0,"-","-",39.0,55.0,4.0,12.0,"-","-","-",3.0,"-","M10",8.0,"-"]
[null,"WNRF 5K (PN 5) JIS B 2211 Size  DN 15","WNRF","5K (PN 5)","JIS B 2211","1/2\"",15.0,80.0,"-","-",44.0,60.0,4.0,12.0,"-","-","-",3.0,"-","M10",8.0,"-"]
[null,"WNRF 5K (PN 5) JIS B 2211 Size  DN 20","WNRF","5K (PN 5)","JIS B 2211","3/4\"",20.0,85.0,"-","-",49.0,65.0,4.0,12.0,"-","-","-",3.0,"-","M10",8.0,"-"]
[null,"WNRF 5K (PN 5) JIS B 2211 Size  DN 25","WNRF","5K (PN 5)","JIS B 2211","1\"",25.0,95.0,"-","-",59.0,75.0,4.0,12.0,"-","-","-",3.0,"-","M10",8.0,"-"]
[null,"WNRF 5K (PN 5) JIS B 2211 Size  DN 32","WNRF","5K (PN 5)","JIS B 2211","1¼\"",32.0,115.0,"-","-",70.0,90.0,4.0,15.0,"-","-","-",3.0,"-","M12",10.0,"-"]
[null,"WNRF 5K (PN 5) JIS B 2211 Size  DN 40","WNRF","5K (PN 5)","JIS B 2211","1½\"",40.0,120.0,"-","-",75.0,95.0,4.0,15.0,"-","-","-",3.0,"-","M12",10.0,"-"]
[null,"WNRF 5K (PN 5) JIS B 2211 Size  DN 50","WNRF","5K (PN 5)","JIS B 2211","2\"",50.0,130.0,"-","-",85.0,105.0,4.0,15.0,"-","-","-",4.0,"-","M12",10.0,"-"]
[null,"WNRF 5K (PN 5) JIS B 2211 Size  DN 65","WNRF","5K (PN 5)","JIS B 2211","2½\"",65.0,155.0,"-","-",110.0,130.0,4.0,15.0,"-","-","-",4.0,"-","M12",10.0,"-"]
[null,"WNRF 5K (PN 5) JIS B 2211 Size  DN 80","WNRF","5K (PN 5)","JIS B 2211","3\"",80.0,180.0,"-","-",121.0,145.0,4.0,19.0,"-","-","-",4.0,"-","M16",13.0,"-"]
[null,"WNRF 5K (PN 5) JIS B 2211 Size  DN 100","WNRF","5K (PN 5)","JIS B 2211","4\"",100.0,200.0,"-","-",141.0,165.0,8.0,19.0,"-","-","-",5.0,"-","M16",13.0,"-"]
[null,"WNRF 5K (PN 5) JIS B 2211 Size  DN 125","WNRF","5K (PN 5)","JIS B 2211","5\"",125.0,235.0,"-","-",176.0,200.0,8.0,19.0,"-","-","-",5.0,"-","M16",13.0,"-"]
[null,"WNRF 5K (PN 5) JIS B 2211 Size  DN 150","WNRF","5K (PN 5)","JIS B 2211","6\"",150.0,265.0,"-","-",206.0,230.0,8.0,19.0,"-","-","-",6.0,"-","M16",13.0,"-"]
[null,"WNRF 5K (PN 5) JIS B 2211 Size  DN 200","WNRF","5K (PN 5)","JIS B 2211","8\"",200.0,320.0,"-","-",252.0,280.0,8.0,23.0,"-","-","-",6.0,"-","M20",16.0,"-"]
[null,"WNRF 5K (PN 5) JIS B 2211 Size  DN 250","WNRF","5K (PN 5)","JIS B 2211","10\"",250.0,385.0,"-","-",317.0,345.0,12.0,23.0,"-","-","-",6.0,"-","M20",16.0,"-"]
[null,"WNRF 5K (PN 5) JIS B 2211 Size  DN 300","WNRF","5K (PN 5)","JIS B 2211","12\"",300.0,430.0,"-","-",360.0,390.0,12.0,23.0,"-","-","-",6.0,"-","M20",16.0,"-"]
[null,"WNRF 5K (PN 5) JIS B 2211 Size  DN 350","WNRF","5K (PN 5)","JIS B 2211","14\"",350.0,480.0,"-","-","-",435.0,12.0,25.0,"-","-","-",7.0,"-","M22",18.0,"-"]
[null,"WNRF 5K (PN 5) JIS B 2211 Size  DN 400","WNRF","5K (PN 5)","JIS B 2211","16\"",400.0,540.0,"-","-","-",495.0,16.0,25.0,"-","-","-",7.0,"-","M22",18.0,"-"]
[null,"WNRF 5K (PN 5) JIS B 2211 Size  DN 450","WNRF","5K (PN 5)","JIS B 2211","18\"",450.0,605.0,"-","-","-",555.0,16.0,25.0,"-","-","-",7.0,"-","M22",18.0,"-"]
[null,"WNRF 5K (PN 5) JIS B 2211 Size  DN 500","WNRF","5K (PN 5)","JIS B 2211","20\"",500.0,655.0,"-","-","-",605.0,20.0,25.0,"-","-","-",7.0,"-","M22",18.0,"-"]
[null,"WNRF 5K (PN 5) JIS B 2211 Size  DN 600","WNRF","5K (PN 5)","JIS B 2211","24\"",600.0,770.0,"-","-","-",715.0,20.0,27.0,"-","-","-",7.0,"-","M24",19.0,"-"]
[null,"WNRF 10K (PN 10) JIS B 2212 Size  DN 10","WNRF","10K (PN 10)","JIS B 2212","1/4\"",10.0,90.0,"-","-",46.0,65.0,4.0,15.0,"-","-","-",3.0,"-","M12",10.0,"-"]
[null,"WNRF 10K (PN 10) JIS B 2212 Size  DN 15","WNRF","10K (PN 10)","JIS B 2212","1/2\"",15.0,95.0,"-","-",51.0,70.0,4.0,15.0,"-","-","-",3.0,"-","M12",10.0,"-"]
[null,"WNRF 10K (PN 10) JIS B 2212 Size  DN 20","WNRF","10K (PN 10)","JIS B 2212","3/4\"",20.0,100.0,"-","-",56.0,75.0,4.0,15.0,"-","-","-",3.0,"-","M12",10.0,"-"]
[null,"WNRF 10K (PN 10) JIS B 2212 Size  DN 25","WNRF","10K (PN 10)","JIS B 2212","1\"",25.0,125.0,"-","-",67.0,90.0,4.0,19.0,"-","-","-",3.0,"-","M16",13.0,"-"]
[null,"WNRF 10K (PN 10) JIS B 2212 Size  DN 32","WNRF","10K (PN 10)","JIS B 2212","1¼\"",32.0,135.0,"-","-",76.0,100.0,4.0,19.0,"-","-","-",3.0,"-","M16",13.0,"-"]
[null,"WNRF 10K (PN 10) JIS B 2212 Size  DN 40","WNRF","10K (PN 10)","JIS B 2212","1½\"",40.0,140.0,"-","-",81.0,105.0,4.0,19.0,"-","-","-",3.0,"-","M16",13.0,"-"]
[null,"WNRF 10K (PN 10) JIS B 2212 Size  DN 50","WNRF","10K (PN 10)","JIS B 2212","2\"",50.0,155.0,"-","-",96.0,120.0,4.0,19.0,"-","-","-",4.0,"-","M16",13.0,"-"]
[null,"WNRF 10K (PN 10) JIS B 2212 Size  DN 65","WNRF","10K (PN 10)","JIS B 2212","2½\"",65.0,175.0,"-","-",116.0,140.0,4.0,19.0,"-","-","-",4.0,"-","M16",13.0,"-"]
[null,"WNRF 10K (PN 10) JIS B 2212 Size  DN 80","WNRF","10K (PN 10)","JIS B 2212","3\"",80.0,185.0,"-","-",126.0,150.0,8.0,19.0,"-","-","-",4.0,"-","M16",13.0,"-"]
[null,"WNRF 10K (PN 10) JIS B 2212 Size  DN 100","WNRF","10K (PN 10)","JIS B 2212","4\"",100.0,210.0,"-","-",151.0,175.0,8.0,19.0,"-","-","-",5.0,"-","M16",13.0,"-"]
[null,"WNRF 10K (PN 10) JIS B 2212 Size  DN 125","WNRF","10K (PN 10)","JIS B 2212","5\"",125.0,250.0,"-","-",182.0,210.0,8.0,23.0,"-","-","-",5.0,"-","M20",16.0,"-"]
[null,"WNRF 10K (PN 10) JIS B 2212 Size  DN 150","WNRF","10K (PN 10)","JIS B 2212","6\"",150.0,280.0,"-","-",212.0,240.0,8.0,23.0,"-","-","-",6.0,"-","M20",16.0,"-"]
[null,"WNRF 10K (PN 10) JIS B 2212 Size  DN 200","WNRF","10K (PN 10)","JIS B 2212","8\"",200.0,330.0,"-","-",262.0,290.0,12.0,23.0,"-","-","-",6.0,"-","M20",16.0,"-"]
[null,"WNRF 10K (PN 10) JIS B 2212 Size  DN 250","WNRF","10K (PN 10)","JIS B 2212","10\"",250.0,400.0,"-","-",324.0,355.0,12.0,25.0,"-","-","-",6.0,"-","M22",18.0,"-"]
[null,"WNRF 10K (PN 10) JIS B 2212 Size  DN 300","WNRF","10K (PN 10)","JIS B 2212","12\"",300.0,445.0,"-","-",368.0,400.0,16.0,25.0,"-","-","-",6.0,"-","M22",18.0,"-"]
[null,"WNRF 10K (PN 10) JIS B 2212 Size  DN 350","WNRF","10K (PN 10)","JIS B 2212","14\"",350.0,490.0,"-","-","-",445.0,16.0,25.0,"-","-","-",7.0,"-","M22",18.0,"-"]
[null,"WNRF 10K (PN 10) JIS B 2212 Size  DN 400","WNRF","10K (PN 10)","JIS B 2212","16\"",400.0,560.0,"-","-","-",510.0,16.0,27.0,"-","-","-",7.0,"-","M24",19.0,"-"]
[null,"WNRF 10K (PN 10) JIS B 2212 Size  DN 450","WNRF","10K (PN 10)","JIS B 2212","18\"",450.0,620.0,"-","-","-",565.0,20.0,27.0,"-","-","-",7.0,"-","M24",19.0,"-"]
[null,"WNRF 10K (PN 10) JIS B 2212 Size  DN 500","WNRF","10K (PN 10)","JIS B 2212","20\"",500.0,675.0,"-","-","-",620.0,20.0,27.0,"-","-","-",7.0,"-","M24",19.0,"-"]
[null,"WNRF 10K (PN 10) JIS B 2212 Size  DN 600","WNRF","10K (PN 10)","JIS B 2212","24\"",600.0,795.0,"-","-","-",730.0,24.0,33.0,"-","-","-",7.0,"-","M30",24.0,"-"]
[null,"WNRF 16K (PN 16) JIS B 2213 Size  DN 10","WNRF","16K (PN 16)","JIS B 2213","1/4\"",10.0,90.0,"-","-",46.0,65.0,4.0,15.0,"-","-","-",3.0,"-","M12",10.0,"-"]
[null,"WNRF 16K (PN 16) JIS B 2213 Size  DN 15","WNRF","16K (PN 16)","JIS B 2213","1/2\"",15.0,95.0,"-","-",51.0,70.0,4.0,15.0,"-","-","-",3.0,"-","M12",10.0,"-"]
[null,"WNRF 16K (PN 16) JIS B 2213 Size  DN 20","WNRF","16K (PN 16)","JIS B 2213","3/4\"",20.0,100.0,"-","-",56.0,75.0,4.0,15.0,"-","-","-",3.0,"-","M12",10.0,"-"]
[null,"WNRF 16K (PN 16) JIS B 2213 Size  DN 25","WNRF","16K (PN 16)","JIS B 2213","1\"",25.0,125.0,"-","-",67.0,90.0,4.0,19.0,"-","-","-",3.0,"-","M16",13.0,"-"]
[null,"WNRF 16K (PN 16) JIS B 2213 Size  DN 32","WNRF","16K (PN 16)","JIS B 2213","1¼\"",32.0,135.0,"-","-",76.0,100.0,4.0,19.0,"-","-","-",3.0,"-","M16",13.0,"-"]
[null,"WNRF 16K (PN 16) JIS B 2213 Size  DN 40","WNRF","16K (PN 16)","JIS B 2213","1½\"",40.0,140.0,"-","-",81.0,102.0,4.0,19.0,"-","-","-",3.0,"-","M16",13.0,"-"]
[null,"WNRF 16K (PN 16) JIS B 2213 Size  DN 50","WNRF","16K (PN 16)","JIS B 2213","2\"",50.0,155.0,"-","-",96.0,120.0,8.0,19.0,"-","-","-",4.0,"-","M16",13.0,"-"]
[null,"WNRF 16K (PN 16) JIS B 2213 Size  DN 65","WNRF","16K (PN 16)","JIS B 2213","2½\"",65.0,175.0,"-","-",116.0,140.0,8.0,19.0,"-","-","-",4.0,"-","M16",13.0,"-"]
[null,"WNRF 16K (PN 16) JIS B 2213 Size  DN 80","WNRF","16K (PN 16)","JIS B 2213","3\"",80.0,200.0,"-","-",132.0,160.0,8.0,23.0,"-","-","-",4.0,"-","M20",16.0,"-"]
[null,"WNRF 16K (PN 16) JIS B 2213 Size  DN 100","WNRF","16K (PN 16)","JIS B 2213","4\"",100.0,225.0,"-","-",160.0,185.0,8.0,23.0,"-","-","-",5.0,"-","M20",16.0,"-"]
[null,"WNRF 16K (PN 16) JIS B 2213 Size  DN 125","WNRF","16K (PN 16)","JIS B 2213","5\"",125.0,270.0,"-","-",195.0,225.0,8.0,25.0,"-","-","-",5.0,"-","M22",18.0,"-"]
[null,"WNRF 16K (PN 16) JIS B 2213 Size  DN 150","WNRF","16K (PN 16)","JIS B 2213","6\"",150.0,305.0,"-","-",230.0,260.0,12.0,25.0,"-","-","-",6.0,"-","M22",18.0,"-"]
[null,"WNRF 16K (PN 16) JIS B 2213 Size  DN 200","WNRF","16K (PN 16)","JIS B 2213","8\"",200.0,350.0,"-","-",275.0,305.0,12.0,25.0,"-","-","-",6.0,"-","M22",18.0,"-"]
[null,"WNRF 16K (PN 16) JIS B 2213 Size  DN 250","WNRF","16K (PN 16)","JIS B 2213","10\"",250.0,430.0,"-","-",345.0,380.0,12.0,27.0,"-","-","-",6.0,"-","M24",19.0,"-"]
[null,"WNRF 16K (PN 16) JIS B 2213 Size  DN 300","WNRF","16K (PN 16)","JIS B 2213","12\"",300.0,480.0,"-","-",395.0,430.0,16.0,27.0,"-","-","-",6.0,"-","M24",19.0,"-"]
[null,"WNRF 16K (PN 16) JIS B 2213 Size  DN 350","WNRF","16K (PN 16)","JIS B 2213","14\"",350.0,540.0,"-","-","-",480.0,16.0,33.0,"-","-","-",7.0,"-","M30",24.0,"-"]
[null,"WNRF 16K (PN 16) JIS B 2213 Size  DN 400","WNRF","16K (PN 16)","JIS B 2213","16\"",400.0,605.0,"-","-","-",540.0,16.0,33.0,"-","-","-",7.0,"-","M30",24.0,"-"]
[null,"WNRF 16K (PN 16) JIS B 2213 Size  DN 450","WNRF","16K (PN 16)","JIS B 2213","18\"",450.0,675.0,"-","-","-",605.0,20.0,33.0,"-","-","-",7.0,"-","M30",24.0,"-"]
[null,"WNRF 16K (PN 16) JIS B 2213 Size  DN 500","WNRF","16K (PN 16)","JIS B 2213","20\"",500.0,730.0,"-","-","-",660.0,20.0,33.0,"-","-","-",7.0,"-","M30",24.0,"-"]
[null,"WNRF 16K (PN 16) JIS B 2213 Size  DN 600","WNRF","16K (PN 16)","JIS B 2213","24\"",600.0,845.0,"-","-","-",770.0,24.0,39.0,"-","-","-",7.0,"-","M36",29.0,"-"]
[null,"WNRF 20K (PN 20) JIS B 2210 Size  DN 10","WNRF","20K (PN 20)","JIS B 2210","1/4\"",10.0,90.0,"-","-",46.0,65.0,4.0,15.0,"-","-","-",3.0,"-","M12",10.0,"-"]
[null,"WNRF 20K (PN 20) JIS B 2210 Size  DN 15","WNRF","20K (PN 20)","JIS B 2210","1/2\"",15.0,95.0,"-","-",51.0,70.0,4.0,15.0,"-","-","-",3.0,"-","M12",10.0,"-"]
[null,"WNRF 20K (PN 20) JIS B 2210 Size  DN 20","WNRF","20K (PN 20)","JIS B 2210","3/4\"",20.0,100.0,"-","-",56.0,75.0,4.0,15.0,"-","-","-",3.0,"-","M12",10.0,"-"]
[null,"WNRF 20K (PN 20) JIS B 2210 Size  DN 25","WNRF","20K (PN 20)","JIS B 2210","1\"",25.0,125.0,"-","-",67.0,90.0,4.0,19.0,"-","-","-",3.0,"-","M16",13.0,"-"]
[null,"WNRF 20K (PN 20) JIS B 2210 Size  DN 32","WNRF","20K (PN 20)","JIS B 2210","1¼\"",32.0,135.0,"-","-",76.0,100.0,4.0,19.0,"-","-","-",3.0,"-","M16",13.0,"-"]
[null,"WNRF 20K (PN 20) JIS B 2210 Size  DN 40","WNRF","20K (PN 20)","JIS B 2210","1½\"",40.0,140.0,"-","-",81.0,105.0,4.0,19.0,"-","-","-",3.0,"-","M16",13.0,"-"]
[null,"WNRF 20K (PN 20) JIS B 2210 Size  DN 50","WNRF","20K (PN 20)","JIS B 2210","2\"",50.0,155.0,"-","-",96.0,120.0,8.0,19.0,"-","-","-",4.0,"-","M16",13.0,"-"]
[null,"WNRF 20K (PN 20) JIS B 2210 Size  DN 65","WNRF","20K (PN 20)","JIS B 2210","2½\"",65.0,175.0,"-","-",116.0,140.0,8.0,19.0,"-","-","-",4.0,"-","M16",13.0,"-"]
[null,"WNRF 20K (PN 20) JIS B 2210 Size  DN 80","WNRF","20K (PN 20)","JIS B 2210","3\"",80.0,200.0,"-","-",132.0,160.0,8.0,23.0,"-","-","-",4.0,"-","M20",16.0,"-"]
[null,"WNRF 20K (PN 20) JIS B 2210 Size  DN 100","WNRF","20K (PN 20)","JIS B 2210","4\"",100.0,225.0,"-","-",160.0,185.0,8.0,23.0,"-","-","-",5.0,"-","M20",16.0,"-"]
[null,"WNRF 20K (PN 20) JIS B 2210 Size  DN 125","WNRF","20K (PN 20)","JIS B 2210","5\"",125.0,270.0,"-","-",195.0,225.0,8.0,25.0,"-","-","-",5.0,"-","M22",18.0,"-"]
[null,"WNRF 20K (PN 20) JIS B 2210 Size  DN 150","WNRF","20K (PN 20)","JIS B 2210","6\"",150.0,305.0,"-","-",230.0,280.0,12.0,25.0,"-","-","-",6.0,"-","M22",18.0,"-"]
[null,"WNRF 20K (PN 20) JIS B 2210 Size  DN 200","WNRF","20K (PN 20)","JIS B 2210","8\"",200.0,350.0,"-","-",275.0,305.0,12.0,25.0,"-","-","-",6.0,"-","M22",18.0,"-"]
[null,"WNRF 20K (PN 20) JIS B 2210 Size  DN 250","WNRF","20K (PN 20)","JIS B 2210","10\"",250.0,430.0,"-","-",345.0,380.0,12.0,27.0,"-","-","-",6.0,"-","M24",19.0,"-"]
[null,"WNRF 20K (PN 20) JIS B 2210 Size  DN 300","WNRF","20K (PN 20)","JIS B 2210","12\"",300.0,480.0,"-","-",395.0,430.0,16.0,27.0,"-","-","-",6.0,"-","M24",19.0,"-"]
[null,"WNRF 30K (PN 30) JIS B 2210 Size  DN 10","WNRF","30K (PN 30)","JIS B 2210","1/4\"",10.0,110.0,"-","-",52.0,75.0,4.0,19.0,"-","-","-",3.0,"-","M16",13.0,"-"]
[null,"WNRF 30K (PN 30) JIS B 2210 Size  DN 15","WNRF","30K (PN 30)","JIS B 2210","1/2\"",15.0,115.0,"-","-",55.0,80.0,4.0,19.0,"-","-","-",3.0,"-","M16",13.0,"-"]
[null,"WNRF 30K (PN 30) JIS B 2210 Size  DN 20","WNRF","30K (PN 30)","JIS B 2210","3/4\"",20.0,120.0,"-","-",60.0,85.0,4.0,19.0,"-","-","-",3.0,"-","M16",13.0,"-"]
[null,"WNRF 30K (PN 30) JIS B 2210 Size  DN 25","WNRF","30K (PN 30)","JIS B 2210","1\"",25.0,130.0,"-","-",70.0,95.0,4.0,19.0,"-","-","-",3.0,"-","M16",13.0,"-"]
[null,"WNRF 30K (PN 30) JIS B 2210 Size  DN 32","WNRF","30K (PN 30)","JIS B 2210","1¼\"",32.0,140.0,"-","-",80.0,105.0,4.0,19.0,"-","-","-",3.0,"-","M16",13.0,"-"]
[null,"WNRF 30K (PN 30) JIS B 2210 Size  DN 40","WNRF","30K (PN 30)","JIS B 2210","1½\"",40.0,160.0,"-","-",90.0,120.0,4.0,23.0,"-","-","-",3.0,"-","M20",16.0,"-"]
[null,"WNRF 30K (PN 30) JIS B 2210 Size  DN 50","WNRF","30K (PN 30)","JIS B 2210","2\"",50.0,165.0,"-","-",105.0,130.0,8.0,19.0,"-","-","-",4.0,"-","M16",13.0,"-"]
[null,"WNRF 30K (PN 30) JIS B 2210 Size  DN 65","WNRF","30K (PN 30)","JIS B 2210","2½\"",65.0,200.0,"-","-",130.0,160.0,8.0,23.0,"-","-","-",4.0,"-","M20",16.0,"-"]
[null,"WNRF 30K (PN 30) JIS B 2210 Size  DN 80","WNRF","30K (PN 30)","JIS B 2210","3\"",80.0,210.0,"-","-",140.0,170.0,8.0,23.0,"-","-","-",4.0,"-","M20",16.0,"-"]
[null,"WNRF 30K (PN 30) JIS B 2210 Size  DN 100","WNRF","30K (PN 30)","JIS B 2210","4\"",100.0,240.0,"-","-",160.0,195.0,8.0,25.0,"-","-","-",5.0,"-","M22",18.0,"-"]
[null,"WNRF 30K (PN 30) JIS B 2210 Size  DN 125","WNRF","30K (PN 30)","JIS B 2210","5\"",125.0,275.0,"-","-",195.0,230.0,8.0,25.0,"-","-","-",5.0,"-","M22",18.0,"-"]
[null,"WNRF 30K (PN 30) JIS B 2210 Size  DN 150","WNRF","30K (PN 30)","JIS B 2210","6\"",150.0,325.0,"-","-",235.0,275.0,12.0,27.0,"-","-","-",6.0,"-","M24",19.0,"-"]
[null,"WNRF 30K (PN 30) JIS B 2210 Size  DN 200","WNRF","30K (PN 30)","JIS B 2210","8\"",200.0,370.0,"-","-",280.0,320.0,12.0,27.0,"-","-","-",6.0,"-","M24",19.0,"-"]
[null,"WNRF 30K (PN 30) JIS B 2210 Size  DN 250","WNRF","30K (PN 30)","JIS B 2210","10\"",250.0,450.0,"-","-",345.0,390.0,12.0,33.0,"-","-","-",6.0,"-","M30",24.0,"-"]
[null,"WNRF 30K (PN 30) JIS B 2210 Size  DN 300","WNRF","30K (PN 30)","JIS B 2210","12\"",300.0,515.0,"-","-",405.0,450.0,16.0,33.0,"-","-","-",6.0,"-","M30",24.0,"-"]
[null,"WNRF 40K (PN 40) JIS B 2210 Size  DN 10","WNRF","40K (PN 40)","JIS B 2210","1/4\"",10.0,110.0,"-","-",52.0,75.0,4.0,19.0,"-","-","-",3.0,"-","M16",13.0,"-"]
[null,"WNRF 40K (PN 40) JIS B 2210 Size  DN 15","WNRF","40K (PN 40)","JIS B 2210","1/2\"",15.0,115.0,"-","-",55.0,80.0,4.0,19.0,"-","-","-",3.0,"-","M16",13.0,"-"]
[null,"WNRF 40K (PN 40) JIS B 2210 Size  DN 20","WNRF","40K (PN 40)","JIS B 2210","3/4\"",20.0,120.0,"-","-",60.0,85.0,4.0,19.0,"-","-","-",3.0,"-","M16",13.0,"-"]
[null,"WNRF 40K (PN 40) JIS B 2210 Size  DN 25","WNRF","40K (PN 40)","JIS B 2210","1\"",25.0,130.0,"-","-",70.0,95.0,4.0,19.0,"-","-","-",3.0,"-","M16",13.0,"-"]
[null,"WNRF 40K (PN 40) JIS B 2210 Size  DN 32","WNRF","40K (PN 40)","JIS B 2210","1¼\"",32.0,140.0,"-","-",80.0,105.0,4.0,19.0,"-","-","-",3.0,"-","M16",13.0,"-"]
[null,"WNRF 40K (PN 40) JIS B 2210 Size  DN 40","WNRF","40K (PN 40)","JIS B 2210","1½\"",40.0,160.0,"-","-",90.0,120.0,4.0,23.0,"-","-","-",3.0,"-","M20",16.0,"-"]
[null,"WNRF 40K (PN 40) JIS B 2210 Size  DN 50","WNRF","40K (PN 40)","JIS B 2210","2\"",50.0,165.0,"-","-",105.0,130.0,8.0,19.0,"-","-","-",4.0,"-","M16",13.0,"-"]
[null,"WNRF 40K (PN 40) JIS B 2210 Size  DN 65","WNRF","40K (PN 40)","JIS B 2210","2½\"",65.0,200.0,"-","-",130.0,160.0,8.0,23.0,"-","-","-",4.0,"-","M20",16.0,"-"]
[null,"WNRF 40K (PN 40) JIS B 2210 Size  DN 80","WNRF","40K (PN 40)","JIS B 2210","3\"",80.0,210.0,"-","-",140.0,170.0,8.0,23.0,"-","-","-",4.0,"-","M20",16.0,"-"]
[null,"WNRF 40K (PN 40) JIS B 2210 Size  DN 100","WNRF","40K (PN 40)","JIS B 2210","4\"",100.0,250.0,"-","-",165.0,205.0,8.0,25.0,"-","-","-",5.0,"-","M22",18.0,"-"]
[null,"WNRF 40K (PN 40) JIS B 2210 Size  DN 125","WNRF","40K (PN 40)","JIS B 2210","5\"",125.0,300.0,"-","-",200.0,250.0,8.0,27.0,"-","-","-",5.0,"-","M24",19.0,"-"]
[null,"WNRF 40K (PN 40) JIS B 2210 Size  DN 150","WNRF","40K (PN 40)","JIS B 2210","6\"",150.0,355.0,"-","-",240.0,295.0,12.0,33.0,"-","-","-",6.0,"-","M30",24.0,"-"]
[null,"WNRF 40K (PN 40) JIS B 2210 Size  DN 200","WNRF","40K (PN 40)","JIS B 2210","8\"",200.0,405.0,"-","-",290.0,345.0,12.0,33.0,"-","-","-",6.0,"-","M30",24.0,"-"]
[null,"WNRF 40K (PN 40) JIS B 2210 Size  DN 250","WNRF","40K (PN 40)","JIS B 2210","10\"",250.0,475.0,"-","-",355.0,410.0,12.0,33.0,"-","-","-",6.0,"-","M30",24.0,"-"]
[null,"WNRF 40K (PN 40) JIS B 2210 Size  DN 300","WNRF","40K (PN 40)","JIS B 2210","12\"",300.0,540.0,"-","-",410.0,470.0,16.0,39.0,"-","-","-",6.0,"-","M36",29.0,"-"]

{"sheet":"Blind & Slip-on fl.","index":7,"n_rows":55,"n_cols":9,"rows_kept":55,"cut":false,"hidden":true,"merged":[[0,0,0,8],[42,5,42,7]]}
["BLIND & SLIP ON FLANGES"]
[]
["Blind flange acc.:"]
["ANSI B 16.5, MSS-SP44"]
["BS 3293, DIN 2527"]
[]
[]
[]
[]
[]
[]
[]
["Slip-on flange acc.:"]
["DIN 1882, NEN 5818/19"]
["DIN 2573/76"]
[]
[]
[]
[]
[]
[]
[]
["Slip-on flange acc.:"]
["ANSI B 16.5, MSS-SP44"]
["BS 3293, DIN 86029/30"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Flange dimensions"]
["D","Flange diameter",null,{"$f":"INDEX('Data Slip-on & Bl.fl.'!H$3:H$1121,'Data Slip-on & Bl.fl.'!$A$3)","v":209.6},"mm"]
["h","Flange height",null,{"$f":"INDEX('Data Slip-on & Bl.fl.'!I$3:I$1121,'Data Slip-on & Bl.fl.'!$A$3)","v":52.4},"mm"]
["b / b1","Flange thickness",null,{"$f":"INDEX('Data Slip-on & Bl.fl.'!J$3:J$1121,'Data Slip-on & Bl.fl.'!$A$3)","v":38.2},"mm","Include data of following flanges:"]
["d1","Diameter RF",null,{"$f":"INDEX('Data Slip-on & Bl.fl.'!K$3:K$1121,'Data Slip-on & Bl.fl.'!$A$3)","v":127},"mm","SO/BL RF ANSI B 16.5",null,null,"125-1500#"]
["k","Pitch circle bolts",null,{"$f":"INDEX('Data Slip-on & Bl.fl.'!L$3:L$1121,'Data Slip-on & Bl.fl.'!$A$3)","v":168.1},"mm","SO/BL RF ANSI B 16.47-MSS SP-44",null,null,"150-900#"]
["n","Number of bolts",null,{"$f":"INDEX('Data Slip-on & Bl.fl.'!M$3:M$1121,'Data Slip-on & Bl.fl.'!$A$3)","v":8},"pce","SO/BL RF ANSI B 16.47-API 650",null,null,"75-900#"]
["d2","Diameter boltholes",null,{"$f":"INDEX('Data Slip-on & Bl.fl.'!N$3:N$1121,'Data Slip-on & Bl.fl.'!$A$3)","v":22.4},"mm","SORF BS 3293",null,null,"150-600#"]
["d3","Diameter hub",null,{"$f":"INDEX('Data Slip-on & Bl.fl.'!O$3:O$1121,'Data Slip-on & Bl.fl.'!$A$3)","v":117.3},"mm","SO    DIN 2573",null,null,"PN 6"]
["f","Heigt of RF",null,{"$f":"INDEX('Data Slip-on & Bl.fl.'!P$3:P$1121,'Data Slip-on & Bl.fl.'!$A$3)","v":6.4},"mm","SO    DIN 2576",null,null,"PN 10"]
["d4","Diameter pipe hole",null,{"$f":"INDEX('Data Slip-on & Bl.fl.'!Q$3:Q$1121,'Data Slip-on & Bl.fl.'!$A$3)","v":90.7},"mm","SO    DIN 2641-42",null,null,"PN 6-10"]
["g","Thickness of gasket",null,{"$f":"INDEX('Data Slip-on & Bl.fl.'!R$3:R$1121,'Data Slip-on & Bl.fl.'!$A$3)","v":4},"mm","SO    DIN 2655-56",null,null,"PN 16-25"]
["L","Required stud length",null,{"$f":"INDEX('Data Slip-on & Bl.fl.'!S$3:S$1121,'Data Slip-on & Bl.fl.'!$A$3)","v":122.4},"mm 1)","BL    DIN 2527",null,null,"PN 6-100"]
["bt","Bolt",null,{"$f":"INDEX('Data Slip-on & Bl.fl.'!T$3:T$1121,'Data Slip-on & Bl.fl.'!$A$3)","v":"M20"},null,"SORF DIN 86029-30",null,null,"PN 10-16"]
["m","Nut height",null,{"$f":"INDEX('Data Slip-on & Bl.fl.'!U$3:U$1121,'Data Slip-on & Bl.fl.'!$A$3)","v":16},"mm","SO    DIN 1882",null,null,"PN 10"]
["W","Weight",null,{"$f":"INDEX('Data Slip-on & Bl.fl.'!V$3:V$1121,'Data Slip-on & Bl.fl.'!$A$3)","v":7},"kg","SO    NEN 5818-19",null,null,"PN 6-10"]
["1)","for flange / flange connection",null,null,null,"Pressure vessels DIN 28031-32-36"]

{"sheet":"Data Slip-on & Bl.fl.","index":8,"n_rows":1121,"n_cols":22,"rows_kept":1121,"cut":false,"hidden":true,"merged":[]}
["Data Slip-on & Blind flanges",null,"Type","Rating","Norm","Size","Size","Outside","Height","Fl thickn.","Diam. RF","Pitch circle","No. Of bolts","D bolthole","Diam hub","RF thickn.","D pipehole","Gasket","Studlength","Bolt","Nut height","Weight"]
[" / ","Type / Size / Rating"," ",null,null,"NPS","DN","D","h","b-b1","d1","k","n","d2","d3","f","d4","g","L","bt","m","W"]
[110.0,{"$f":"CONCATENATE(C3,$C$2,D3,$C$2,E3,$C$2,$F$1,$C$2,F3)","v":"SORF 125# ANSI B16.5 Size 26\""},"SORF","125#","ANSI B16.5","26\"",650.0,870.0,85.9,50.8,749.3,806.5,24.0,35.1,723.9,1.6,"specify",7.0,{"$f":"(J3+U3+5)*2+R3","v":170.6},"M33",26.0,"-"]
[null,"SORF 125# ANSI B16.5 Size 28\"","SORF","125#","ANSI B16.5","28\"",700.0,927.1,87.4,52.3,800.1,863.6,28.0,35.1,781.1,1.6,"specify",7.0,173.6,"M33",26.0,"-"]
[null,"SORF 125# ANSI B16.5 Size 30\"","SORF","125#","ANSI B16.5","30\"",750.0,984.3,88.9,54.1,857.3,914.4,28.0,35.1,831.9,1.6,"specify",7.0,177.2,"M33",26.0,"-"]
[null,"SORF 125# ANSI B16.5 Size 32\"","SORF","125#","ANSI B16.5","32\"",800.0,1060.5,92.2,57.2,914.4,977.9,28.0,41.4,889.0,1.6,"specify",7.0,183.4,"M36",26.0,"-"]
[null,"SORF 125# ANSI B16.5 Size 34\"","SORF","125#","ANSI B16.5","34\"",850.0,1111.3,93.5,58.7,965.2,1028.7,32.0,41.4,939.8,1.6,"specify",7.0,186.4,"M36",26.0,"-"]
[null,"SORF 125# ANSI B16.5 Size 36\"","SORF","125#","ANSI B16.5","36\"",900.0,1168.4,95.3,60.5,1022.4,1086.0,32.0,41.4,997.0,1.6,"specify",7.0,190,"M36",26.0,"-"]
[null,"SORF 125# ANSI B16.5 Size 38\"","SORF","125#","ANSI B16.5","38\"",950.0,1238.3,95.3,60.5,1073.2,1149.4,32.0,41.4,1060.5,1.6,"specify",7.0,190,"M36",26.0,"-"]
[null,"SORF 125# ANSI B16.5 Size 40\"","SORF","125#","ANSI B16.5","40\"",1000.0,1289.1,98.6,63.5,1124.0,1200.2,36.0,41.4,1111.3,1.6,"specify",7.0,202,"M36",29.0,"-"]
[null,"SORF 125# ANSI B16.5 Size 42\"","SORF","125#","ANSI B16.5","42\"",1050.0,1346.2,101.6,66.8,1193.8,1257.3,36.0,41.4,1168.4,1.6,"specify",7.0,208.6,"M36",29.0,"-"]
[null,"SORF 125# ANSI B16.5 Size 44\"","SORF","125#","ANSI B16.5","44\"",1100.0,1403.4,101.6,66.8,1244.6,1314.5,40.0,41.4,1219.2,1.6,"specify",7.0,208.6,"M36",29.0,"-"]
[null,"SORF 125# ANSI B16.5 Size 46\"","SORF","125#","ANSI B16.5","46\"",1150.0,1454.2,103.1,68.1,1295.4,1365.3,40.0,41.4,1270.0,1.6,"specify",7.0,211.2,"M36",29.0,"-"]
[null,"SORF 125# ANSI B16.5 Size 48\"","SORF","125#","ANSI B16.5","48\"",1200.0,1511.3,104.9,69.85,1358.9,1422.4,44.0,41.4,1327.2,1.6,"specify",7.0,214.7,"M36",29.0,"-"]
[null,"SORF 125# ANSI B16.5 Size 50\"","SORF","125#","ANSI B16.5","50\"",1250.0,1568.5,104.9,69.9,1409.7,1479.6,44.0,47.8,1378.0,1.6,"specify",7.0,220.8,"M39",32.0,"-"]
[null,"SORF 125# ANSI B16.5 Size 52\"","SORF","125#","ANSI B16.5","52\"",1300.0,1625.6,108.0,73.2,1460.5,1536.7,44.0,47.8,1435.1,1.6,"specify",7.0,227.4,"M39",32.0,"-"]
[null,"SORF 125# ANSI B16.5 Size 54\"","SORF","125#","ANSI B16.5","54\"",1350.0,1682.8,111.3,76.2,1517.7,1593.9,44.0,47.8,1492.3,1.6,"specify",7.0,233.4,"M39",32.0,"-"]
[null,"SORF 125# ANSI B16.5 Size 60\"","SORF","125#","ANSI B16.5","60\"",1500.0,1854.2,114.3,79.5,1676.4,1759.0,52.0,47.8,1657.4,1.6,"specify",7.0,240,"M39",32.0,"-"]
[null,"SORF 125# ANSI B16.5 Size 66\"","SORF","125#","ANSI B16.5","66\"",1650.0,2032.0,124.0,85.9,1854.2,1930.4,52.0,47.8,1816.1,1.6,"specify",7.0,252.8,"M39",32.0,"-"]
[null,"SORF 125# ANSI B16.5 Size 72\"","SORF","125#","ANSI B16.5","72\"",1800.0,2197.1,127.0,88.9,2019.3,2095.5,60.0,47.8,1993.9,1.6,"specify",7.0,258.8,"M39",32.0,"-"]
[null,"SORF 125# ANSI B16.5 Size 84\"","SORF","125#","ANSI B16.5","84\"",2100.0,2533.7,136.7,98.6,2349.5,2525.7,64.0,54.1,2298.7,1.6,"specify",7.0,298.2,"M52",42.0,"-"]
[null,"SORF 125# ANSI B16.5 Size 96\"","SORF","125#","ANSI B16.5","96\"",2400.0,2876.6,146.1,108.0,2679.7,2755.9,66.0,60.5,2609.9,1.6,"specify",7.0,323,"M56",45.0,"-"]
[null,"SORF 150# ANSI B16.5 Size 1/2\"","SORF","150#","ANSI B16.5","1/2\"",15.0,88.9,15.9,11.1,35.1,60.5,4.0,15.7,30.2,1.6,22.3,3.0,55.2,"M12",10.0,0.8]
[null,"SORF 150# ANSI B16.5 Size 3/4\"","SORF","150#","ANSI B16.5","3/4\"",20.0,98.6,15.9,12.7,42.9,69.9,4.0,15.7,38.1,1.6,27.7,3.0,58.4,"M12",10.0,0.9]
[null,"SORF 150# ANSI B16.5 Size 1\"","SORF","150#","ANSI B16.5","1\"",25.0,108.0,17.5,14.3,50.8,79.2,4.0,15.7,49.3,1.6,34.5,3.0,61.6,"M12",10.0,1.0]
[null,"SORF 150# ANSI B16.5 Size 1¼\"","SORF","150#","ANSI B16.5","1¼\"",32.0,117.3,20.6,15.9,63.5,88.9,4.0,15.7,58.7,1.6,43.2,3.0,64.8,"M12",10.0,1.3]
[null,"SORF 150# ANSI B16.5 Size 1½\"","SORF","150#","ANSI B16.5","1½\"",40.0,127.0,22.2,17.5,73.2,98.6,4.0,15.7,65.0,1.6,49.5,3.0,68,"M12",10.0,1.4]
[null,"SORF 150# ANSI B16.5 Size 2\"","SORF","150#","ANSI B16.5","2\"",50.0,152.4,25.4,19.0,91.9,120.7,4.0,19.1,77.7,1.6,62.0,4.0,78,"M16",13.0,2.3]
[null,"SORF 150# ANSI B16.5 Size 2½\"","SORF","150#","ANSI B16.5","2½\"",65.0,117.8,28.6,22.2,104.6,139.7,4.0,19.1,90.4,1.6,74.7,4.0,84.4,"M16",13.0,3.2]
[null,"SORF 150# ANSI B16.5 Size 3\"","SORF","150#","ANSI B16.5","3\"",80.0,190.5,30.2,23.8,127.0,152.4,4.0,19.1,108.0,1.6,90.7,4.0,87.6,"M16",13.0,3.6]
[null,"SORF 150# ANSI B16.5 Size 3½\"","SORF","150#","ANSI B16.5","3½\"","-",215.9,31.7,23.8,139.7,177.8,8.0,19.1,122.2,1.6,101.4,4.0,87.6,"M16",13.0,5.0]
[null,"SORF 150# ANSI B16.5 Size 4\"","SORF","150#","ANSI B16.5","4\"",100.0,228.6,33.3,23.8,157.2,190.5,8.0,19.1,134.9,1.6,116.1,5.0,88.6,"M16",13.0,5.9]
[null,"SORF 150# ANSI B16.5 Size 5\"","SORF","150#","ANSI B16.5","5\"",125.0,254.0,36.5,23.8,185.7,215.9,8.0,22.4,163.6,1.6,143.8,5.0,94.6,"M20",16.0,6.8]
[null,"SORF 150# ANSI B16.5 Size 6\"","SORF","150#","ANSI B16.5","6\"",150.0,279.4,39.7,25.4,215.9,241.3,8.0,22.4,192.0,1.6,170.7,6.0,98.8,"M20",16.0,8.6]
[null,"SORF 150# ANSI B16.5 Size 8\"","SORF","150#","ANSI B16.5","8\"",200.0,342.9,44.4,28.6,269.7,298.5,8.0,22.4,246.1,1.6,221.5,6.0,105.2,"M20",16.0,13.6]
[null,"SORF 150# ANSI B16.5 Size 10\"","SORF","150#","ANSI B16.5","10\"",250.0,406.4,49.2,30.2,323.9,362.0,12.0,25.4,304.8,1.6,276.3,6.0,114.4,"M24",19.0,19.5]
[null,"SORF 150# ANSI B16.5 Size 12\"","SORF","150#","ANSI B16.5","12\"",300.0,482.6,55.6,31.7,381.0,431.8,12.0,25.4,365.3,1.6,327.1,6.0,117.4,"M24",19.0,29.1]
[null,"SORF 150# ANSI B16.5 Size 14\"","SORF","150#","ANSI B16.5","14\"",350.0,533.4,57.1,34.9,412.8,476.3,12.0,28.4,400.1,1.6,359.1,7.0,130.8,"M27",22.0,38.6]
[null,"SORF 150# ANSI B16.5 Size 16\"","SORF","150#","ANSI B16.5","16\"",400.0,596.9,63.5,36.5,469.9,539.8,16.0,28.4,457.2,1.6,410.5,7.0,134,"M27",22.0,42.2]
[null,"SORF 150# ANSI B16.5 Size 18\"","SORF","150#","ANSI B16.5","18\"",450.0,635.0,68.3,39.7,533.4,577.9,16.0,31.8,505.0,1.6,461.8,7.0,144.4,"M30",24.0,54.5]
[null,"SORF 150# ANSI B16.5 Size 20\"","SORF","150#","ANSI B16.5","20\"",500.0,698.5,73.0,42.9,584.2,635.0,20.0,31.8,558.8,1.6,513.1,7.0,150.8,"M30",24.0,70.0]
[null,"SORF 150# ANSI B16.5 Size 22\"","SORF","150#","ANSI B16.5","22\"",550.0,749.3,79.4,46.0,641.2,692.1,20.0,34.9,609.6,1.6,564.4,7.0,161,"M33",26.0,72.0]
[null,"SORF 150# ANSI B16.5 Size 24\"","SORF","150#","ANSI B16.5","24\"",600.0,812.8,82.5,47.6,692.2,749.3,20.0,35.1,663.4,1.6,615.9,7.0,164.2,"M33",26.0,95.0]
[null,"SORF 150# ANSI B16.5 Size 26\"","SORF","150#","ANSI B16.5","26\"",650.0,869.9,85.7,50.8,742.9,806.4,24.0,34.9,723.9,1.6,717.5,7.0,170.6,"M33",26.0,123.0]
[null,"SORF 150# ANSI B16.5 Size 30\"","SORF","150#","ANSI B16.5","30\"",750.0,984.2,88.9,54.0,857.2,914.4,28.0,34.9,831.8,1.6,768.3,7.0,177,"M33",26.0,138.0]
[null,"SORF 150# ANSI B16.5 Size 34\"","SORF","150#","ANSI B16.5","34\"",850.0,1111.2,150.8,58.8,958.8,1028.7,32.0,41.3,911.2,1.6,869.9,7.0,196.6,"M39",31.0,186.0]
[null,"SORF 150# ANSI B16.5 Size 36\"","SORF","150#","ANSI B16.5","36\"",900.0,1168.4,161.9,60.3,1022.3,1085.8,32.0,41.3,966.8,1.6,920.7,7.0,199.6,"M39",31.0,211.0]
[null,"SORF 150# ANSI B16.5 Size 42\"","SORF","150#","ANSI B16.5","42\"",1050.0,1344.2,193.7,66.7,1193.8,1257.3,36.0,41.3,1131.9,1.6,1073.1,7.0,212.4,"M39",31.0,313.0]
[null,"SORF 175# ANSI B16.5 Size 26\"","SORF","175#","ANSI B16.5","26\"",650.0,812.8,69.8,46.0,736.6,759.0,28.0,22.4,701.8,1.6,"specify",7.0,141,"M20",16.0,"-"]
[null,"SORF 175# ANSI B16.5 Size 28\"","SORF","175#","ANSI B16.5","28\"",700.0,863.6,69.8,49.3,787.4,809.8,28.0,22.4,752.6,1.6,"specify",8.0,148.6,"M20",16.0,"-"]
[null,"SORF 175# ANSI B16.5 Size 30\"","SORF","175#","ANSI B16.5","30\"",750.0,927.1,69.8,53.8,844.5,866.9,36.0,22.4,809.8,1.6,"specify",9.0,158.6,"M20",16.0,"-"]
[null,"SORF 175# ANSI B16.5 Size 32\"","SORF","175#","ANSI B16.5","32\"",800.0,977.9,69.8,57.1,895.3,917.7,36.0,22.4,860.6,1.6,"specify",10.0,166.2,"M20",16.0,"-"]
[null,"SORF 175# ANSI B16.5 Size 34\"","SORF","175#","ANSI B16.5","34\"",850.0,1041.4,85.9,60.5,949.5,974.9,36.0,25.4,911.4,1.6,"specify",11.0,180,"M24",19.0,"-"]
[null,"SORF 175# ANSI B16.5 Size 36\"","SORF","175#","ANSI B16.5","36\"",900.0,1092.2,85.9,63.5,1000.3,1025.7,36.0,25.4,962.2,1.6,"specify",12.0,187,"M24",19.0,"-"]
[null,"SORF 175# ANSI B16.5 Size 38\"","SORF","175#","ANSI B16.5","38\"",950.0,1149.3,95.3,66.5,1051.1,1076.5,36.0,25.4,1013.0,1.6,"specify",13.0,194,"M24",19.0,"-"]
[null,"SORF 175# ANSI B16.5 Size 40\"","SORF","175#","ANSI B16.5","40\"",1000.0,1200.1,101.6,69.8,1101.9,1127.3,40.0,25.4,1063.8,1.6,"specify",14.0,201.6,"M24",19.0,"-"]
[null,"SORF 175# ANSI B16.5 Size 42\"","SORF","175#","ANSI B16.5","42\"",1050.0,1263.6,111.3,73.2,1162.1,1190.8,40.0,28.7,1120.9,1.6,"specify",15.0,215.4,"M27",22.0,"-"]
[null,"SORF 175# ANSI B16.5 Size 44\"","SORF","175#","ANSI B16.5","44\"",1100.0,1314.4,111.3,76.2,1212.8,1241.6,40.0,28.7,1171.7,1.6,"specify",16.0,222.4,"M27",22.0,"-"]
[null,"SORF 175# ANSI B16.5 Size 46\"","SORF","175#","ANSI B16.5","46\"",1150.0,1371.6,117.3,79.2,1263.6,1292.4,40.0,28.7,1222.5,1.6,"specify",17.0,229.4,"M27",22.0,"-"]
[null,"SORF 175# ANSI B16.5 Size 48\"","SORF","175#","ANSI B16.5","48\"",1200.0,1422.4,124.0,82.5,1314.4,1343.2,44.0,28.7,1273.3,1.6,"specify",18.0,237,"M27",22.0,"-"]
[null,"SORF 175# ANSI B16.5 Size 50\"","SORF","175#","ANSI B16.5","50\"",1250.0,1479.6,124.0,85.9,1365.3,1394.3,44.0,28.7,1324.1,1.6,"specify",19.0,244.8,"M27",22.0,"-"]
[null,"SORF 175# ANSI B16.5 Size 52\"","SORF","175#","ANSI B16.5","52\"",1300.0,1543.1,136.7,88.9,1422.4,1454.1,44.0,31.8,1377.9,1.6,"specify",20.0,255.8,"M30",24.0,"-"]
[null,"SORF 175# ANSI B16.5 Size 54\"","SORF","175#","ANSI B16.5","54\"",1350.0,1600.2,136.7,91.9,1473.2,1504.9,44.0,31.8,1428.8,1.6,"specify",21.0,262.8,"M30",24.0,"-"]
[null,"SORF 175# ANSI B16.5 Size 60\"","SORF","175#","ANSI B16.5","60\"",1500.0,1752.6,149.4,101.6,1625.6,1657.3,48.0,31.8,1581.1,1.6,"specify",22.0,283.2,"M30",24.0,"-"]
[null,"SORF 175# ANSI B16.5 Size 66\"","SORF","175#","ANSI B16.5","66\"",1650.0,1905.0,174.8,111.3,1778.0,1809.9,56.0,31.8,1739.9,1.6,"specify",23.0,303.6,"M30",24.0,"-"]
[null,"SORF 175# ANSI B16.5 Size 72\"","SORF","175#","ANSI B16.5","72\"",1800.0,2057.4,203.2,127.0,1943.1,1974.8,64.0,31.8,1892.3,1.6,"specify",24.0,336,"M30",24.0,"-"]
[null,"SORF 300# ANSI B16.5 Size 1/2\"","SORF","300#","ANSI B16.5","1/2\"",15.0,95.2,22.2,14.3,35.0,66.5,4.0,15.7,38.1,1.6,22.3,3.0,61.6,"M12",10.0,1.2]
[null,"SORF 300# ANSI B16.5 Size 3/4\"","SORF","300#","ANSI B16.5","3/4\"",20.0,117.5,25.4,15.9,42.9,82.5,4.0,19.0,47.7,1.6,27.7,3.0,70.8,"M16",13.0,1.3]
[null,"SORF 300# ANSI B16.5 Size 1\"","SORF","300#","ANSI B16.5","1\"",25.0,123.8,27.0,17.5,50.8,88.9,4.0,19.0,53.8,1.6,34.5,3.0,74,"M16",13.0,1.4]
[null,"SORF 300# ANSI B16.5 Size 1¼\"","SORF","300#","ANSI B16.5","1¼\"",32.0,133.3,27.0,19.0,63.5,98.5,4.0,19.0,63.5,1.6,43.2,3.0,77,"M16",13.0,1.8]
[null,"SORF 300# ANSI B16.5 Size 1½\"","SORF","300#","ANSI B16.5","1½\"",40.0,155.6,3.2,20.6,73.1,114.3,4.0,22.3,69.8,1.6,49.5,3.0,86.2,"M20",16.0,2.7]
[null,"SORF 300# ANSI B16.5 Size 2\"","SORF","300#","ANSI B16.5","2\"",50.0,165.1,33.3,22.2,91.9,127.0,8.0,19.0,84.0,1.6,62.0,4.0,84.4,"M16",13.0,3.2]
[null,"SORF 300# ANSI B16.5 Size 2½\"","SORF","300#","ANSI B16.5","2½\"",65.0,190.5,38.1,25.4,104.6,149.3,8.0,22.3,100.0,1.6,74.7,4.0,96.8,"M20",16.0,4.5]
[null,"SORF 300# ANSI B16.5 Size 3\"","SORF","300#","ANSI B16.5","3\"",80.0,209.5,42.9,28.6,127.0,168.1,8.0,22.3,117.3,1.6,90.7,4.0,103.2,"M20",16.0,5.9]
[null,"SORF 300# ANSI B16.5 Size 3½\"","SORF","300#","ANSI B16.5","3½\"","-",228.6,44.4,30.2,139.7,184.1,8.0,22.3,133.3,1.6,101.4,4.0,106.4,"M20",16.0,7.7]
[null,"SORF 300# ANSI B16.5 Size 4\"","SORF","300#","ANSI B16.5","4\"",100.0,254.0,47.6,31.7,157.2,200.1,8.0,22.3,146.0,1.6,116.1,5.0,110.4,"M20",16.0,10.0]
[null,"SORF 300# ANSI B16.5 Size 5\"","SORF","300#","ANSI B16.5","5\"",125.0,279.4,50.8,34.9,185.6,234.9,8.0,22.3,177.8,1.6,143.8,5.0,116.8,"M20",16.0,12.7]
[null,"SORF 300# ANSI B16.5 Size 6\"","SORF","300#","ANSI B16.5","6\"",150.0,317.5,52.4,36.5,215.9,269.7,12.0,22.3,206.2,1.6,170.7,6.0,121,"M20",16.0,17.7]
[null,"SORF 300# ANSI B16.5 Size 8\"","SORF","300#","ANSI B16.5","8\"",200.0,381.0,61.9,41.3,269.7,330.2,12.0,25.4,260.3,1.6,221.5,6.0,136.6,"M24",19.0,26.3]
[null,"SORF 300# ANSI B16.5 Size 10\"","SORF","300#","ANSI B16.5","10\"",250.0,444.5,66.7,47.6,323.8,387.3,16.0,28.4,320.5,1.6,276.3,6.0,155.2,"M27",22.0,36.8]
[null,"SORF 300# ANSI B16.5 Size 12\"","SORF","300#","ANSI B16.5","12\"",300.0,520.7,73.0,50.8,381.0,450.8,16.0,31.7,374.6,1.6,327.1,6.0,165.6,"M30",24.0,52.0]
[null,"SORF 300# ANSI B16.5 Size 14\"","SORF","300#","ANSI B16.5","14\"",350.0,584.2,76.2,54.0,412.7,514.3,20.0,31.7,425.4,1.6,359.1,7.0,173,"M30",24.0,74.0]
[null,"SORF 300# ANSI B16.5 Size 16\"","SORF","300#","ANSI B16.5","16\"",400.0,647.7,82.5,27.1,469.9,571.5,20.0,35.0,482.6,1.6,410.5,7.0,123.2,"M33",26.0,100.0]
[null,"SORF 300# ANSI B16.5 Size 18\"","SORF","300#","ANSI B16.5","18\"",450.0,711.2,88.9,60.3,533.4,628.6,24.0,35.0,533.4,1.6,461.8,7.0,189.6,"M33",26.0,127.0]
[null,"SORF 300# ANSI B16.5 Size 20\"","SORF","300#","ANSI B16.5","20\"",500.0,774.7,95.2,63.5,584.2,685.8,24.0,35.0,587.2,1.6,513.1,7.0,196,"M33",26.0,148.0]
[null,"SORF 300# ANSI B16.5 Size 22\"","SORF","300#","ANSI B16.5","22\"",550.0,838.2,101.6,64.7,641.2,742.9,24.0,41.3,641.2,1.6,564.4,7.0,208.4,"M39",31.0,197.0]
[null,"SORF 300# ANSI B16.5 Size 24\"","SORF","300#","ANSI B16.5","24\"",600.0,914.4,106.4,69.8,692.1,812.8,24.0,41.1,701.5,1.6,615.9,7.0,218.6,"M39",31.0,222.0]
[null,"SORF 300# ANSI B16.5 Size 26\"","SORF","300#","ANSI B16.5","26\"",650.0,971.5,184.1,79.6,749.3,876.3,28.0,44.4,720.7,1.6,717.5,7.0,244.2,"M42",34.0,251.0]
[null,"SORF 300# ANSI B16.5 Size 30\"","SORF","300#","ANSI B16.5","30\"",750.0,1092.2,29.5,92.1,857.2,996.9,28.0,47.6,827.1,1.6,768.3,7.0,273.2,"M45",36.0,354.0]
[null,"SORF 300# ANSI B16.5 Size 34\"","SORF","300#","ANSI B16.5","34\"",850.0,1206.5,231.8,101.6,965.2,1104.9,28.0,50.8,936.6,1.6,869.9,7.0,296.2,"M48",38.0,460.0]
[null,"SORF 300# ANSI B16.5 Size 36\"","SORF","300#","ANSI B16.5","36\"",900.0,1270.0,241.3,104.8,1022.3,1168.4,32.0,54.0,990.6,1.6,920.7,7.0,310.6,"M52",42.0,513.0]
[null,"SORF 300# ANSI B16.5 Size 42\"","SORF","300#","ANSI B16.5","42\"",1050.0,1447.8,276.2,117.3,1193.8,1339.8,36.0,54.0,1154.1,1.6,1073.1,7.0,335.6,"M52",42.0,731.0]
[null,"SORF 350# ANSI B16.5 Size 26\"","SORF","350#","ANSI B16.5","26\"",650.0,850.9,114.3,63.5,749.3,777.7,28.0,28.4,null,1.6,"specify",7.0,188,"M27",22.0,"-"]
[null,"SORF 350# ANSI B16.5 Size 28\"","SORF","350#","ANSI B16.5","28\"",700.0,901.7,114.3,63.5,800.1,828.5,28.0,28.4,null,1.6,"specify",7.0,188,"M27",22.0,"-"]
[null,"SORF 350# ANSI B16.5 Size 30\"","SORF","350#","ANSI B16.5","30\"",750.0,958.8,120.6,66.5,857.3,886.0,32.0,28.4,null,1.6,"specify",7.0,194,"M27",22.0,"-"]
[null,"SORF 350# ANSI B16.5 Size 32\"","SORF","350#","ANSI B16.5","32\"",800.0,1009.7,127.0,69.8,908.0,936.8,36.0,28.4,null,1.6,"specify",7.0,200.6,"M27",22.0,"-"]
[null,"SORF 350# ANSI B16.5 Size 34\"","SORF","350#","ANSI B16.5","34\"",850.0,1073.1,130.0,73.2,958.8,987.6,40.0,28.4,null,1.6,"specify",7.0,207.4,"M27",22.0,"-"]
[null,"SORF 350# ANSI B16.5 Size 36\"","SORF","350#","ANSI B16.5","36\"",900.0,1136.6,142.7,79.2,1022.3,1054.1,40.0,31.8,null,1.6,"specify",7.0,223.4,"M30",24.0,"-"]
[null,"SORF 350# ANSI B16.5 Size 38\"","SORF","350#","ANSI B16.5","38\"",950.0,1187.5,142.7,79.2,1073.1,1104.9,40.0,31.8,null,1.6,"specify",7.0,223.4,"M30",24.0,"-"]
[null,"SORF 350# ANSI B16.5 Size 40\"","SORF","350#","ANSI B16.5","40\"",1000.0,1238.3,149.4,82.5,1124.0,1155.7,44.0,31.8,null,1.6,"specify",7.0,230,"M30",24.0,"-"]
[null,"SORF 350# ANSI B16.5 Size 42\"","SORF","350#","ANSI B16.5","42\"",1050.0,1301.8,155.4,88.9,1181.1,1212.8,48.0,31.8,null,1.6,"specify",7.0,242.8,"M30",24.0,"-"]
[null,"SORF 350# ANSI B16.5 Size 44\"","SORF","350#","ANSI B16.5","44\"",1100.0,1371.6,171.4,95.3,1241.6,1276.3,44.0,35.1,null,1.6,"specify",7.0,259.6,"M33",26.0,"-"]
[null,"SORF 350# ANSI B16.5 Size 46\"","SORF","350#","ANSI B16.5","46\"",1150.0,1422.4,184.1,107.9,1292.4,1327.1,48.0,35.1,null,1.6,"specify",7.0,284.8,"M33",26.0,"-"]
[null,"SORF 350# ANSI B16.5 Size 48\"","SORF","350#","ANSI B16.5","48\"",1200.0,1479.6,184.1,107.9,1343.2,1377.9,48.0,35.1,null,1.6,"specify",7.0,284.8,"M33",26.0,"-"]
[null,"SORF 400# ANSI B16.5 Size 1/2\"","SORF","400#","ANSI B16.5","1/2\"",15.0,95.3,28.8,20.6,35.1,66.5,4.0,15.7,38.1,6.4,22.3,3.0,74.2,"M12",10.0,0.74]
[null,"SORF 400# ANSI B16.5 Size 3/4\"","SORF","400#","ANSI B16.5","3/4\"",20.0,117.3,31.8,22.1,42.9,82.6,4.0,19.1,47.8,6.4,27.7,3.0,83.2,"M16",13.0,1.27]
[null,"SORF 400# ANSI B16.5 Size 1\"","SORF","400#","ANSI B16.5","1\"",25.0,124.0,33.3,23.9,50.8,88.9,4.0,19.1,53.8,6.4,34.5,3.0,86.8,"M16",13.0,1.52]
[null,"SORF 400# ANSI B16.5 Size 1¼\"","SORF","400#","ANSI B16.5","1¼\"",32.0,133.4,34.8,27.0,63.5,98.6,4.0,19.1,63.5,6.4,43.2,3.0,93,"M16",13.0,2.03]
[null,"SORF 400# ANSI B16.5 Size 1½\"","SORF","400#","ANSI B16.5","1½\"",40.0,155.4,38.2,28.8,73.2,114.3,4.0,22.4,69.9,6.4,49.5,3.0,102.6,"M20",16.0,2.96]
[null,"SORF 400# ANSI B16.5 Size 2\"","SORF","400#","ANSI B16.5","2\"",50.0,165.1,43.0,31.8,91.9,127.0,8.0,19.1,84.1,6.4,62.0,4.0,103.6,"M16",13.0,3.62]
[null,"SORF 400# ANSI B16.5 Size 2½\"","SORF","400#","ANSI B16.5","2½\"",65.0,190.5,47.5,34.8,104.6,149.4,8.0,22.4,100.1,6.4,74.7,4.0,115.6,"M20",16.0,5.28]
[null,"SORF 400# ANSI B16.5 Size 3\"","SORF","400#","ANSI B16.5","3\"",80.0,209.6,52.4,38.2,127.0,168.1,8.0,22.4,117.3,6.4,90.7,4.0,122.4,"M20",16.0,7.0]
[null,"SORF 400# ANSI B16.5 Size 3½\"","SORF","400#","ANSI B16.5","3½\"","-",228.6,55.7,41.5,139.7,184.2,8.0,25.4,133.4,6.4,101.4,4.0,135,"M24",19.0,8.84]
[null,"SORF 400# ANSI B16.5 Size 4\"","SORF","400#","ANSI B16.5","4\"",100.0,254.0,57.2,41.5,157.2,200.2,8.0,25.4,146.1,6.4,116.1,5.0,136,"M24",19.0,11.1]
[null,"SORF 400# ANSI B16.5 Size 5\"","SORF","400#","ANSI B16.5","5\"",125.0,279.4,60.2,44.5,185.7,235.0,8.0,25.4,177.8,6.4,143.8,5.0,142,"M24",19.0,13.9]
[null,"SORF 400# ANSI B16.5 Size 6\"","SORF","400#","ANSI B16.5","6\"",150.0,317.5,63.6,47.5,215.9,269.7,12.0,25.4,206.2,6.4,170.7,6.0,149,"M24",19.0,18.3]
[null,"SORF 400# ANSI B16.5 Size 8\"","SORF","400#","ANSI B16.5","8\"",200.0,381.0,74.7,54.2,269.7,330.2,12.0,28.4,260.4,6.4,221.5,6.0,168.4,"M27",22.0,28.6]
[null,"SORF 400# ANSI B16.5 Size 10\"","SORF","400#","ANSI B16.5","10\"",250.0,444.5,79.6,60.2,323.9,387.4,16.0,31.8,320.5,6.4,276.3,6.0,184.4,"M30",24.0,39.2]
[null,"SORF 400# ANSI B16.5 Size 12\"","SORF","400#","ANSI B16.5","12\"",300.0,520.7,85.6,63.6,381.0,450.9,16.0,35.1,374.7,6.4,327.1,6.0,195.2,"M33",26.0,57.0]
[null,"SORF 400# ANSI B16.5 Size 14\"","SORF","400#","ANSI B16.5","14\"",350.0,584.2,90.5,66.9,412.8,514.4,20.0,35.1,425.5,6.4,359.1,7.0,202.8,"M33",26.0,79.1]
[null,"SORF 400# ANSI B16.5 Size 16\"","SORF","400#","ANSI B16.5","16\"",400.0,647.7,100.1,69.9,469.9,571.5,20.0,38.1,482.6,6.4,410.5,7.0,214.8,"M36",29.0,101.0]
[null,"SORF 400# ANSI B16.5 Size 18\"","SORF","400#","ANSI B16.5","18\"",450.0,711.2,105.0,72.9,533.4,628.7,24.0,38.1,533.4,6.4,461.8,7.0,220.8,"M36",29.0,123.0]
[null,"SORF 400# ANSI B16.5 Size 20\"","SORF","400#","ANSI B16.5","20\"",500.0,774.7,108.0,76.3,584.2,685.8,24.0,41.1,587.2,6.4,513.1,7.0,231.6,"M39",31.0,146.0]
[null,"SORF 400# ANSI B16.5 Size 24\"","SORF","400#","ANSI B16.5","24\"",600.0,914.4,120.7,82.6,692.2,812.8,24.0,47.8,701.5,6.4,616.0,7.0,254.2,"M45",36.0,219.0]
[null,"SORF 600# ANSI B16.5 Size 1/2\"","SORF","600#","ANSI B16.5","1/2\"",15.0,95.3,28.8,20.6,35.1,66.5,4.0,15.7,38.1,6.4,22.3,3.0,74.2,"M12",10.0,0.74]
[null,"SORF 600# ANSI B16.5 Size 3/4\"","SORF","600#","ANSI B16.5","3/4\"",20.0,117.3,31.8,22.1,42.9,82.6,4.0,19.1,47.8,6.4,27.7,3.0,83.2,"M16",13.0,1.27]
[null,"SORF 600# ANSI B16.5 Size 1\"","SORF","600#","ANSI B16.5","1\"",25.0,124.0,33.3,23.9,50.8,88.9,4.0,19.1,53.8,6.4,34.5,3.0,86.8,"M16",13.0,1.52]
[null,"SORF 600# ANSI B16.5 Size 1¼\"","SORF","600#","ANSI B16.5","1¼\"",32.0,133.4,34.8,27.0,63.5,98.6,4.0,19.1,63.5,6.4,43.2,3.0,93,"M16",13.0,2.03]
[null,"SORF 600# ANSI B16.5 Size 1½\"","SORF","600#","ANSI B16.5","1½\"",40.0,155.4,38.2,28.8,73.2,114.3,4.0,22.3,69.9,6.4,49.5,3.0,102.6,"M20",16.0,2.96]
[null,"SORF 600# ANSI B16.5 Size 2\"","SORF","600#","ANSI B16.5","2\"",50.0,165.1,43.0,31.8,91.9,127.0,8.0,19.1,84.1,6.4,62.0,4.0,103.6,"M16",13.0,3.62]
[null,"SORF 600# ANSI B16.5 Size 2½\"","SORF","600#","ANSI B16.5","2½\"",65.0,190.5,47.5,34.8,104.6,149.4,8.0,22.4,100.1,6.4,74.7,4.0,115.6,"M20",16.0,5.28]
[null,"SORF 600# ANSI B16.5 Size 3\"","SORF","600#","ANSI B16.5","3\"",80.0,209.6,52.4,38.2,127.0,168.1,8.0,22.4,117.3,6.4,90.7,4.0,122.4,"M20",16.0,7.0]
[null,"SORF 600# ANSI B16.5 Size 3½\"","SORF","600#","ANSI B16.5","3½\"","-",228.6,55.7,41.5,139.7,184.2,8.0,25.4,133.4,6.4,101.4,4.0,135,"M24",19.0,8.84]
[null,"SORF 600# ANSI B16.5 Size 4\"","SORF","600#","ANSI B16.5","4\"",100.0,273.1,60.2,44.5,157.2,215.9,8.0,25.4,152.4,6.4,116.1,5.0,142,"M24",19.0,14.5]
[null,"SORF 600# ANSI B16.5 Size 5\"","SORF","600#","ANSI B16.5","5\"",125.0,330.2,66.9,50.9,185.7,266.7,8.0,28.4,189.0,6.4,143.8,5.0,160.8,"M27",22.0,24.4]
[null,"SORF 600# ANSI B16.5 Size 6\"","SORF","600#","ANSI B16.5","6\"",150.0,355.6,72.9,54.2,215.9,292.1,12.0,28.4,222.3,6.4,170.7,6.0,168.4,"M27",22.0,28.7]
[null,"SORF 600# ANSI B16.5 Size 8\"","SORF","600#","ANSI B16.5","8\"",200.0,419.1,82.6,62.0,269.7,349.3,12.0,31.8,273.1,6.4,221.5,6.0,188,"M30",24.0,43.4]
[null,"SORF 600# ANSI B16.5 Size 10\"","SORF","600#","ANSI B16.5","10\"",250.0,508.0,92.3,69.9,323.9,431.8,16.0,35.1,342.9,6.4,276.3,6.0,207.8,"M33",26.0,70.3]
[null,"SORF 600# ANSI B16.5 Size 12\"","SORF","600#","ANSI B16.5","12\"",300.0,558.8,98.3,72.9,381.0,489.0,20.0,35.1,400.1,6.4,327.1,6.0,213.8,"M33",26.0,84.2]
[null,"SORF 600# ANSI B16.5 Size 14\"","SORF","600#","ANSI B16.5","14\"",350.0,603.3,100.1,76.3,412.8,527.1,20.0,38.1,431.8,6.4,359.1,7.0,227.6,"M36",29.0,98.7]
[null,"SORF 600# ANSI B16.5 Size 16\"","SORF","600#","ANSI B16.5","16\"",400.0,685.8,112.8,82.6,469.9,603.3,20.0,41.1,495.3,6.4,410.5,7.0,244.2,"M39",31.0,142.0]
[null,"SORF 600# ANSI B16.5 Size 18\"","SORF","600#","ANSI B16.5","18\"",450.0,743.0,123.7,89.0,533.4,654.1,20.0,44.5,546.1,6.4,461.8,7.0,263,"M42",34.0,173.0]
[null,"SORF 600# ANSI B16.5 Size 20\"","SORF","600#","ANSI B16.5","20\"",500.0,812.8,133.4,95.3,584.2,723.9,24.0,44.5,609.6,6.4,513.1,7.0,275.6,"M42",34.0,220.0]
[null,"SORF 600# ANSI B16.5 Size 22\"","SORF","600#","ANSI B16.5","22\"",550.0,869.9,139.7,101.6,641.2,777.9,24.0,47.6,666.7,6.4,564.4,7.0,292.2,"M45",36.0,292.0]
[null,"SORF 600# ANSI B16.5 Size 24\"","SORF","600#","ANSI B16.5","24\"",600.0,939.8,146.1,108.0,692.2,838.2,24.0,50.8,717.6,6.4,615.9,7.0,309,"M48",38.0,398.0]
[null,"SORF 600# ANSI B16.5 Size 26\"","SORF","600#","ANSI B16.5","26\"",650.0,1016.0,228.6,114.3,749.3,914.4,28.0,50.8,747.7,6.4,717.5,7.0,321.6,"M48",38.0,408.0]
[null,"SORF 600# ANSI B16.5 Size 30\"","SORF","600#","ANSI B16.5","30\"",750.0,1130.3,254.0,120.7,857.2,1022.3,28.0,54.0,862.0,6.4,768.3,7.0,342.4,"M52",42.0,576.0]
[null,"SORF 600# ANSI B16.5 Size 34\"","SORF","600#","ANSI B16.5","34\"",850.0,1244.6,276.3,127.0,965.2,1130.3,28.0,60.3,973.1,6.4,869.9,7.0,361,"M56",45.0,652.0]
[null,"SORF 600# ANSI B16.5 Size 36\"","SORF","600#","ANSI B16.5","36\"",900.0,1314.4,287.0,130.2,1022.3,1193.8,28.0,66.7,1031.9,6.4,920.7,7.0,379.4,"M64",51.0,744.0]
[null,"SORF 600# ANSI B16.5 Size 42\"","SORF","600#","ANSI B16.5","42\"",1050.0,1492.2,330.2,146.1,1193.8,1365.2,28.0,73.0,1201.7,6.4,1073.1,7.0,419.2,"M68",55.0,1058.0]
[null,"SORF 900# ANSI B16.5 Size 1/2\"","SORF","900#","ANSI B16.5","1/2\"",15.0,120.6,38.1,28.7,35.0,82.5,4.0,22.3,38.1,6.4,22.3,3.0,102.4,"M20",16.0,1.74]
[null,"SORF 900# ANSI B16.5 Size 3/4\"","SORF","900#","ANSI B16.5","3/4\"",20.0,130.0,41.4,31.8,42.9,88.9,4.0,22.3,44.4,6.4,27.7,3.0,108.6,"M20",16.0,2.34]
[null,"SORF 900# ANSI B16.5 Size 1\"","SORF","900#","ANSI B16.5","1\"",25.0,149.3,47.5,35.0,50.8,101.6,4.0,25.4,52.3,6.4,34.5,3.0,121,"M24",19.0,3.44]
[null,"SORF 900# ANSI B16.5 Size 1¼\"","SORF","900#","ANSI B16.5","1¼\"",32.0,158.7,47.5,35.0,63.5,111.2,4.0,25.4,63.5,6.4,43.2,3.0,121,"M24",19.0,3.91]
[null,"SORF 900# ANSI B16.5 Size 1½\"","SORF","900#","ANSI B16.5","1½\"",40.0,177.8,50.9,38.1,73.1,123.9,4.0,28.4,69.8,6.4,49.5,3.0,133.2,"M27",22.0,5.36]
[null,"SORF 900# ANSI B16.5 Size 2\"","SORF","900#","ANSI B16.5","2\"",50.0,215.9,63.5,44.5,91.9,165.1,8.0,25.4,104.6,6.4,62.0,4.0,141,"M24",19.0,9.85]
[null,"SORF 900# ANSI B16.5 Size 2½\"","SORF","900#","ANSI B16.5","2½\"",65.0,244.3,69.9,47.5,104.6,190.5,8.0,28.4,123.9,6.4,74.7,4.0,153,"M27",22.0,13.7]
[null,"SORF 900# ANSI B16.5 Size 3\"","SORF","900#","ANSI B16.5","3\"",80.0,241.3,60.2,44.5,127.0,190.5,8.0,25.4,127.0,6.4,90.7,4.0,135,"M20",16.0,11.6]
[null,"SORF 900# ANSI B16.5 Size 4\"","SORF","900#","ANSI B16.5","4\"",100.0,292.1,76.2,50.8,157.2,234.9,8.0,31.7,158.7,6.4,116.1,5.0,160.6,"M27",22.0,19.7]
[null,"SORF 900# ANSI B16.5 Size 5\"","SORF","900#","ANSI B16.5","5\"",125.0,349.2,85.6,57.2,185.6,279.4,8.0,35.0,190.5,6.4,143.8,5.0,181.4,"M33",26.0,31.9]
[null,"SORF 900# ANSI B16.5 Size 6\"","SORF","900#","ANSI B16.5","6\"",150.0,381.0,92.2,62.0,215.9,317.5,12.0,31.7,234.9,6.4,170.7,6.0,184,"M27",22.0,41.1]
[null,"SORF 900# ANSI B16.5 Size 8\"","SORF","900#","ANSI B16.5","8\"",200.0,469.9,108.0,69.9,269.7,393.7,12.0,38.1,298.4,6.4,221.5,6.0,213.8,"M36",29.0,70.7]
[null,"SORF 900# ANSI B16.5 Size 10\"","SORF","900#","ANSI B16.5","10\"",250.0,546.1,114.3,76.2,323.8,169.9,16.0,38.1,368.3,6.4,276.3,6.0,226.4,"M36",29.0,101.0]
[null,"SORF 900# ANSI B16.5 Size 12\"","SORF","900#","ANSI B16.5","12\"",300.0,609.6,123.7,85.6,381.0,533.4,20.0,38.1,419.1,6.4,327.1,6.0,245.2,"M36",29.0,133.0]
[null,"SORF 900# ANSI B16.5 Size 14\"","SORF","900#","ANSI B16.5","14\"",350.0,641.3,136.4,92.2,412.7,558.8,20.0,41.1,450.8,6.4,359.1,7.0,259.4,"M39",29.0,153.0]
[null,"SORF 900# ANSI B16.5 Size 16\"","SORF","900#","ANSI B16.5","16\"",400.0,704.8,139.7,95.3,469.9,615.9,20.0,44.4,508.0,6.4,410.5,7.0,275.6,"M42",34.0,185.0]
[null,"SORF 900# ANSI B16.5 Size 18\"","SORF","900#","ANSI B16.5","18\"",450.0,787.4,158.8,108.0,533.4,685.8,20.0,50.8,565.1,6.4,461.8,7.0,309,"M48",38.0,258.0]
[null,"SORF 900# ANSI B16.5 Size 20\"","SORF","900#","ANSI B16.5","20\"",500.0,857.2,165.1,114.3,584.2,749.3,20.0,53.8,622.3,6.4,513.1,7.0,329.6,"M52",42.0,317.0]
[null,"SORF 900# ANSI B16.5 Size 24\"","SORF","900#","ANSI B16.5","24\"",600.0,1041.4,209.6,146.1,692.1,901.7,20.0,66.5,749.3,6.4,615.9,7.0,411.2,"M64",51.0,606.0]
[null,"SORF 1500# ANSI B16.5 Size 1/2\"","SORF","1500#","ANSI B16.5","1/2\"",15.0,120.6,38.1,28.7,35.0,82.5,4.0,22.3,38.1,6.4,22.3,3.0,102.4,"M20",16.0,3.2]
[null,"SORF 1500# ANSI B16.5 Size 3/4\"","SORF","1500#","ANSI B16.5","3/4\"",20.0,130.0,41.4,31.8,42.9,88.9,4.0,22.3,44.4,6.4,27.7,3.0,108.6,"M20",16.0,3.6]
[null,"SORF 1500# ANSI B16.5 Size 1\"","SORF","1500#","ANSI B16.5","1\"",25.0,149.3,47.5,35.0,50.8,101.6,4.0,25.4,52.3,6.4,34.5,3.0,121,"M24",19.0,4.1]
[null,"SORF 1500# ANSI B16.5 Size 1¼\"","SORF","1500#","ANSI B16.5","1¼\"",32.0,158.7,47.5,35.0,63.5,111.2,4.0,25.4,63.5,6.4,43.2,3.0,121,"M24",19.0,4.5]
[null,"SORF 1500# ANSI B16.5 Size 1½\"","SORF","1500#","ANSI B16.5","1½\"",40.0,177.8,50.9,38.1,73.1,123.9,4.0,28.4,69.8,6.4,49.5,3.0,133.2,"M27",22.0,6.4]
[null,"SORF 1500# ANSI B16.5 Size 2\"","SORF","1500#","ANSI B16.5","2\"",50.0,215.9,63.5,44.5,91.9,165.1,8.0,25.4,104.6,6.4,62.0,4.0,141,"M24",19.0,11.3]
[null,"SORF 1500# ANSI B16.5 Size 2½\"","SORF","1500#","ANSI B16.5","2½\"",65.0,244.3,69.9,47.5,104.6,190.5,8.0,28.4,123.9,6.4,74.7,4.0,153,"M27",22.0,16.3]
[null,"SORF 1500# ANSI B16.5 Size 3\"","SORF","1500#","ANSI B16.5","3\"",80.0,266.7,79.4,54.0,127.0,203.2,8.0,31.7,133.3,6.4,90.7,4.0,170,"M30",24.0,21.8]
[null,"SORF 1500# ANSI B16.5 Size 4\"","SORF","1500#","ANSI B16.5","4\"",100.0,311.1,96.9,60.4,157.2,241.3,8.0,35.0,162.0,6.4,116.1,5.0,187.8,"M33",26.0,33.0]
[null,"SORF 1500# ANSI B16.5 Size 5\"","SORF","1500#","ANSI B16.5","5\"",125.0,374.6,111.2,79.4,185.6,292.1,8.0,41.1,196.8,6.4,143.8,5.0,235.8,"M39",31.0,60.0]
[null,"SORF 1500# ANSI B16.5 Size 6\"","SORF","1500#","ANSI B16.5","6\"",150.0,393.7,125.5,88.9,215.9,317.5,12.0,38.1,228.6,6.4,170.7,6.0,251.8,"M36",29.0,74.0]
[null,"SORF 1500# ANSI B16.5 Size 8\"","SORF","1500#","ANSI B16.5","8\"",200.0,482.6,149.3,98.5,269.7,393.7,12.0,44.4,292.1,6.4,221.5,6.0,281,"M42",34.0,117.0]
[null,"SORF 1500# ANSI B16.5 Size 10\"","SORF","1500#","ANSI B16.5","10\"",250.0,584.2,165.1,114.3,323.8,485.6,12.0,50.8,368.3,6.4,276.3,6.0,320.6,"M48",38.0,198.0]
[null,"SORF 1500# ANSI B16.5 Size 12\"","SORF","1500#","ANSI B16.5","12\"",300.0,673.1,187.4,130.2,381.0,571.5,16.0,53.8,450.8,6.4,327.1,6.0,360.4,"M52",42.0,303.0]
[null,"SORF 1500# ANSI B16.5 Size 14\"","SORF","1500#","ANSI B16.5","14\"",350.0,749.3,"-",139.7,412.7,635.0,16.0,60.4,495.3,6.4,359.1,7.0,386.4,"M56",45.0,"-"]
[null,"SORF 1500# ANSI B16.5 Size 16\"","SORF","1500#","ANSI B16.5","16\"",400.0,825.5,"-",152.4,469.9,704.8,16.0,66.5,552.4,6.4,410.5,7.0,417.8,"M60",48.0,"-"]
[null,"SORF 1500# ANSI B16.5 Size 18\"","SORF","1500#","ANSI B16.5","18\"",450.0,914.4,"-",176.3,533.4,774.7,16.0,73.1,596.9,6.4,461.8,7.0,477.6,"M68",54.0,"-"]
[null,"SORF 1500# ANSI B16.5 Size 20\"","SORF","1500#","ANSI B16.5","20\"",500.0,984.2,"-",184.2,584.2,831.8,16.0,79.2,641.3,6.4,513.1,7.0,507.4,"M76",61.0,"-"]
[null,"SORF 1500# ANSI B16.5 Size 24\"","SORF","1500#","ANSI B16.5","24\"",600.0,1168.4,"-",209.6,692.1,990.6,16.0,91.9,762.0,6.4,615.9,7.0,564.2,"M80",64.0,"-"]
[null,"BLRF 125# ANSI B16.5 Size 26\"","BLRF","125#","ANSI B16.5","26\"",650.0,870.0,"-",50.8,749.3,806.5,24.0,35.1,"-",1.6,"-",7.0,170.6,"M33",26.0,"-"]
[null,"BLRF 125# ANSI B16.5 Size 28\"","BLRF","125#","ANSI B16.5","28\"",700.0,927.1,"-",52.3,800.1,863.6,28.0,35.1,"-",1.6,"-",7.0,173.6,"M33",26.0,"-"]
[null,"BLRF 125# ANSI B16.5 Size 30\"","BLRF","125#","ANSI B16.5","30\"",750.0,984.3,"-",54.1,857.3,914.4,28.0,35.1,"-",1.6,"-",7.0,177.2,"M33",26.0,"-"]
[null,"BLRF 125# ANSI B16.5 Size 32\"","BLRF","125#","ANSI B16.5","32\"",800.0,1060.5,"-",57.2,914.4,977.9,28.0,41.4,"-",1.6,"-",7.0,183.4,"M36",26.0,"-"]
[null,"BLRF 125# ANSI B16.5 Size 34\"","BLRF","125#","ANSI B16.5","34\"",850.0,1111.3,"-",58.7,965.2,1028.7,32.0,41.4,"-",1.6,"-",7.0,186.4,"M36",26.0,"-"]
[null,"BLRF 125# ANSI B16.5 Size 36\"","BLRF","125#","ANSI B16.5","36\"",900.0,1168.4,"-",60.5,1022.4,1086.0,32.0,41.4,"-",1.6,"-",7.0,190,"M36",26.0,"-"]
[null,"BLRF 125# ANSI B16.5 Size 38\"","BLRF","125#","ANSI B16.5","38\"",950.0,1238.3,"-",60.5,1073.2,1149.4,32.0,41.4,"-",1.6,"-",7.0,190,"M36",26.0,"-"]
[null,"BLRF 125# ANSI B16.5 Size 40\"","BLRF","125#","ANSI B16.5","40\"",1000.0,1289.1,"-",63.5,1124.0,1200.2,36.0,41.4,"-",1.6,"-",7.0,202,"M36",29.0,"-"]
[null,"BLRF 125# ANSI B16.5 Size 42\"","BLRF","125#","ANSI B16.5","42\"",1050.0,1346.2,"-",66.8,1193.8,1257.3,36.0,41.4,"-",1.6,"-",7.0,208.6,"M36",29.0,"-"]
[null,"BLRF 125# ANSI B16.5 Size 44\"","BLRF","125#","ANSI B16.5","44\"",1100.0,1403.4,"-",66.8,1244.6,1314.5,40.0,41.4,"-",1.6,"-",7.0,208.6,"M36",29.0,"-"]
[null,"BLRF 125# ANSI B16.5 Size 46\"","BLRF","125#","ANSI B16.5","46\"",1150.0,1454.2,"-",68.1,1295.4,1365.3,40.0,41.4,"-",1.6,"-",7.0,211.2,"M36",29.0,"-"]
[null,"BLRF 125# ANSI B16.5 Size 48\"","BLRF","125#","ANSI B16.5","48\"",1200.0,1511.3,"-",69.85,1358.9,1422.4,44.0,41.4,"-",1.6,"-",7.0,214.7,"M36",29.0,"-"]
[null,"BLRF 125# ANSI B16.5 Size 50\"","BLRF","125#","ANSI B16.5","50\"",1250.0,1568.5,"-",69.9,1409.7,1479.6,44.0,47.8,"-",1.6,"-",7.0,220.8,"M39",32.0,"-"]
[null,"BLRF 125# ANSI B16.5 Size 52\"","BLRF","125#","ANSI B16.5","52\"",1300.0,1625.6,"-",73.2,1460.5,1536.7,44.0,47.8,"-",1.6,"-",7.0,227.4,"M39",32.0,"-"]
[null,"BLRF 125# ANSI B16.5 Size 54\"","BLRF","125#","ANSI B16.5","54\"",1350.0,1682.8,"-",76.2,1517.7,1593.9,44.0,47.8,"-",1.6,"-",7.0,233.4,"M39",32.0,"-"]
[null,"BLRF 125# ANSI B16.5 Size 60\"","BLRF","125#","ANSI B16.5","60\"",1500.0,1854.2,"-",79.5,1676.4,1759.0,52.0,47.8,"-",1.6,"-",7.0,240,"M39",32.0,"-"]
[null,"BLRF 125# ANSI B16.5 Size 66\"","BLRF","125#","ANSI B16.5","66\"",1650.0,2032.0,"-",85.9,1854.2,1930.4,52.0,47.8,"-",1.6,"-",7.0,252.8,"M39",32.0,"-"]
[null,"BLRF 125# ANSI B16.5 Size 72\"","BLRF","125#","ANSI B16.5","72\"",1800.0,2197.1,"-",88.9,2019.3,2095.5,60.0,47.8,"-",1.6,"-",7.0,258.8,"M39",32.0,"-"]
[null,"BLRF 125# ANSI B16.5 Size 84\"","BLRF","125#","ANSI B16.5","84\"",2100.0,2533.7,"-",98.6,2349.5,2525.7,64.0,54.1,"-",1.6,"-",7.0,298.2,"M52",42.0,"-"]
[null,"BLRF 125# ANSI B16.5 Size 96\"","BLRF","125#","ANSI B16.5","96\"",2400.0,2876.6,"-",108.0,2679.7,2755.9,66.0,60.5,"-",1.6,"-",7.0,323,"M56",45.0,"-"]
[null,"BLRF 150# ANSI B16.5 Size 1/2\"","BLRF","150#","ANSI B16.5","1/2\"",15.0,88.9,"-",11.1,35.1,60.5,4.0,15.7,"-",1.6,"-",3.0,55.2,"M12",10.0,0.8]
[null,"BLRF 150# ANSI B16.5 Size 3/4\"","BLRF","150#","ANSI B16.5","3/4\"",20.0,98.6,"-",12.7,42.9,69.9,4.0,15.7,"-",1.6,"-",3.0,58.4,"M12",10.0,0.9]
[null,"BLRF 150# ANSI B16.5 Size 1\"","BLRF","150#","ANSI B16.5","1\"",25.0,108.0,"-",14.3,50.8,79.2,4.0,15.7,"-",1.6,"-",3.0,61.6,"M12",10.0,1.0]
[null,"BLRF 150# ANSI B16.5 Size 1¼\"","BLRF","150#","ANSI B16.5","1¼\"",32.0,117.3,"-",15.9,63.5,88.9,4.0,15.7,"-",1.6,"-",3.0,64.8,"M12",10.0,1.3]
[null,"BLRF 150# ANSI B16.5 Size 1½\"","BLRF","150#","ANSI B16.5","1½\"",40.0,127.0,"-",17.5,73.2,98.6,4.0,15.7,"-",1.6,"-",3.0,68,"M12",10.0,1.4]
[null,"BLRF 150# ANSI B16.5 Size 2\"","BLRF","150#","ANSI B16.5","2\"",50.0,152.4,"-",19.0,91.9,120.7,4.0,19.1,"-",1.6,"-",4.0,78,"M16",13.0,1.6]
[null,"BLRF 150# ANSI B16.5 Size 2½\"","BLRF","150#","ANSI B16.5","2½\"",65.0,117.8,"-",22.2,104.6,139.7,4.0,19.1,"-",1.6,"-",4.0,84.4,"M16",13.0,3.2]
[null,"BLRF 150# ANSI B16.5 Size 3\"","BLRF","150#","ANSI B16.5","3\"",80.0,190.5,"-",23.8,127.0,152.4,4.0,19.1,"-",1.6,"-",4.0,87.6,"M16",13.0,4.1]
[null,"BLRF 150# ANSI B16.5 Size 3½\"","BLRF","150#","ANSI B16.5","3½\"","-",215.9,"-",23.8,139.7,177.8,8.0,19.1,"-",1.6,"-",4.0,87.6,"M16",13.0,5.9]
[null,"BLRF 150# ANSI B16.5 Size 4\"","BLRF","150#","ANSI B16.5","4\"",100.0,228.6,"-",23.8,157.2,190.5,8.0,19.1,"-",1.6,"-",5.0,88.6,"M16",13.0,7.7]
[null,"BLRF 150# ANSI B16.5 Size 5\"","BLRF","150#","ANSI B16.5","5\"",125.0,254.0,"-",23.8,185.7,215.9,8.0,22.4,"-",1.6,"-",5.0,94.6,"M20",16.0,9.1]
[null,"BLRF 150# ANSI B16.5 Size 6\"","BLRF","150#","ANSI B16.5","6\"",150.0,279.4,"-",25.4,215.9,241.3,8.0,22.4,"-",1.6,"-",6.0,98.8,"M20",16.0,11.8]
[null,"BLRF 150# ANSI B16.5 Size 8\"","BLRF","150#","ANSI B16.5","8\"",200.0,342.9,"-",28.6,269.7,298.5,8.0,22.4,"-",1.6,"-",6.0,105.2,"M20",16.0,20.4]
[null,"BLRF 150# ANSI B16.5 Size 10\"","BLRF","150#","ANSI B16.5","10\"",250.0,406.4,"-",30.2,323.9,362.0,12.0,25.4,"-",1.6,"-",6.0,114.4,"M24",19.0,31.8]
[null,"BLRF 150# ANSI B16.5 Size 12\"","BLRF","150#","ANSI B16.5","12\"",300.0,482.6,"-",31.7,381.0,431.8,12.0,25.4,"-",1.6,"-",6.0,117.4,"M24",19.0,50.0]
[null,"BLRF 150# ANSI B16.5 Size 14\"","BLRF","150#","ANSI B16.5","14\"",350.0,533.4,"-",34.9,412.8,476.3,12.0,28.4,"-",1.6,"-",7.0,130.8,"M27",22.0,60.0]
[null,"BLRF 150# ANSI B16.5 Size 16\"","BLRF","150#","ANSI B16.5","16\"",400.0,596.9,"-",36.5,469.9,539.8,16.0,28.4,"-",1.6,"-",7.0,134,"M27",22.0,77.0]
[null,"BLRF 150# ANSI B16.5 Size 18\"","BLRF","150#","ANSI B16.5","18\"",450.0,635.0,"-",39.7,533.4,577.9,16.0,31.8,"-",1.6,"-",7.0,144.4,"M30",24.0,95.0]
[null,"BLRF 150# ANSI B16.5 Size 20\"","BLRF","150#","ANSI B16.5","20\"",500.0,698.5,"-",42.9,584.2,635.0,20.0,31.8,"-",1.6,"-",7.0,150.8,"M30",24.0,123.0]
[null,"BLRF 150# ANSI B16.5 Size 22\"","BLRF","150#","ANSI B16.5","22\"",550.0,749.3,"-",46.0,641.2,692.1,20.0,34.9,"-",1.6,"-",7.0,161,"M33",26.0,151.0]
[null,"BLRF 150# ANSI B16.5 Size 24\"","BLRF","150#","ANSI B16.5","24\"",600.0,812.8,"-",47.6,692.2,749.3,20.0,35.1,"-",1.6,"-",7.0,164.2,"M33",26.0,187.0]
[null,"BLRF 150# ANSI B16.5 Size 26\"","BLRF","150#","ANSI B16.5","26\"",650.0,869.9,"-",50.8,742.9,806.4,24.0,34.9,"-",1.6,"-",7.0,170.6,"M33",26.0,226.0]
[null,"BLRF 150# ANSI B16.5 Size 30\"","BLRF","150#","ANSI B16.5","30\"",750.0,984.2,"-",54.0,857.2,914.4,28.0,34.9,"-",1.6,"-",7.0,177,"M33",26.0,309.0]
[null,"BLRF 150# ANSI B16.5 Size 34\"","BLRF","150#","ANSI B16.5","34\"",850.0,1111.2,"-",58.8,958.8,1028.7,32.0,41.3,"-",1.6,"-",7.0,196.6,"M39",31.0,425.0]
[null,"BLRF 150# ANSI B16.5 Size 36\"","BLRF","150#","ANSI B16.5","36\"",900.0,1168.4,"-",60.3,1022.3,1085.8,32.0,41.3,"-",1.6,"-",7.0,199.6,"M39",31.0,485.0]
[null,"BLRF 150# ANSI B16.5 Size 42\"","BLRF","150#","ANSI B16.5","42\"",1050.0,1344.2,"-",66.7,1193.8,1257.3,36.0,41.3,"-",1.6,"-",7.0,212.4,"M39",31.0,716.0]
[null,"BLRF 175# ANSI B16.5 Size 26\"","BLRF","175#","ANSI B16.5","26\"",650.0,812.8,"-",46.0,736.6,759.0,28.0,22.4,"-",1.6,"-",7.0,141,"M20",16.0,"-"]
[null,"BLRF 175# ANSI B16.5 Size 28\"","BLRF","175#","ANSI B16.5","28\"",700.0,863.6,"-",49.3,787.4,809.8,28.0,22.4,"-",1.6,"-",8.0,148.6,"M20",16.0,"-"]
[null,"BLRF 175# ANSI B16.5 Size 30\"","BLRF","175#","ANSI B16.5","30\"",750.0,927.1,"-",53.8,844.5,866.9,36.0,22.4,"-",1.6,"-",9.0,158.6,"M20",16.0,"-"]
[null,"BLRF 175# ANSI B16.5 Size 32\"","BLRF","175#","ANSI B16.5","32\"",800.0,977.9,"-",57.1,895.3,917.7,36.0,22.4,"-",1.6,"-",10.0,166.2,"M20",16.0,"-"]
[null,"BLRF 175# ANSI B16.5 Size 34\"","BLRF","175#","ANSI B16.5","34\"",850.0,1041.4,"-",60.5,949.5,974.9,36.0,25.4,"-",1.6,"-",11.0,180,"M24",19.0,"-"]
[null,"BLRF 175# ANSI B16.5 Size 36\"","BLRF","175#","ANSI B16.5","36\"",900.0,1092.2,"-",63.5,1000.3,1025.7,36.0,25.4,"-",1.6,"-",12.0,187,"M24",19.0,"-"]
[null,"BLRF 175# ANSI B16.5 Size 38\"","BLRF","175#","ANSI B16.5","38\"",950.0,1149.3,"-",66.5,1051.1,1076.5,36.0,25.4,"-",1.6,"-",13.0,194,"M24",19.0,"-"]
[null,"BLRF 175# ANSI B16.5 Size 40\"","BLRF","175#","ANSI B16.5","40\"",1000.0,1200.1,"-",69.8,1101.9,1127.3,40.0,25.4,"-",1.6,"-",14.0,201.6,"M24",19.0,"-"]
[null,"BLRF 175# ANSI B16.5 Size 42\"","BLRF","175#","ANSI B16.5","42\"",1050.0,1263.6,"-",73.2,1162.1,1190.8,40.0,28.7,"-",1.6,"-",15.0,215.4,"M27",22.0,"-"]
[null,"BLRF 175# ANSI B16.5 Size 44\"","BLRF","175#","ANSI B16.5","44\"",1100.0,1314.4,"-",76.2,1212.8,1241.6,40.0,28.7,"-",1.6,"-",16.0,222.4,"M27",22.0,"-"]
[null,"BLRF 175# ANSI B16.5 Size 46\"","BLRF","175#","ANSI B16.5","46\"",1150.0,1371.6,"-",79.2,1263.6,1292.4,40.0,28.7,"-",1.6,"-",17.0,229.4,"M27",22.0,"-"]
[null,"BLRF 175# ANSI B16.5 Size 48\"","BLRF","175#","ANSI B16.5","48\"",1200.0,1422.4,"-",82.5,1314.4,1343.2,44.0,28.7,"-",1.6,"-",18.0,237,"M27",22.0,"-"]
[null,"BLRF 175# ANSI B16.5 Size 50\"","BLRF","175#","ANSI B16.5","50\"",1250.0,1479.6,"-",85.9,1365.3,1394.3,44.0,28.7,"-",1.6,"-",19.0,244.8,"M27",22.0,"-"]
[null,"BLRF 175# ANSI B16.5 Size 52\"","BLRF","175#","ANSI B16.5","52\"",1300.0,1543.1,"-",88.9,1422.4,1454.1,44.0,31.8,"-",1.6,"-",20.0,255.8,"M30",24.0,"-"]
[null,"BLRF 175# ANSI B16.5 Size 54\"","BLRF","175#","ANSI B16.5","54\"",1350.0,1600.2,"-",91.9,1473.2,1504.9,44.0,31.8,"-",1.6,"-",21.0,262.8,"M30",24.0,"-"]
[null,"BLRF 175# ANSI B16.5 Size 60\"","BLRF","175#","ANSI B16.5","60\"",1500.0,1752.6,"-",101.6,1625.6,1657.3,48.0,31.8,"-",1.6,"-",22.0,283.2,"M30",24.0,"-"]
[null,"BLRF 175# ANSI B16.5 Size 66\"","BLRF","175#","ANSI B16.5","66\"",1650.0,1905.0,"-",111.3,1778.0,1809.9,56.0,31.8,"-",1.6,"-",23.0,303.6,"M30",24.0,"-"]
[null,"BLRF 175# ANSI B16.5 Size 72\"","BLRF","175#","ANSI B16.5","72\"",1800.0,2057.4,"-",127.0,1943.1,1974.8,64.0,31.8,"-",1.6,"-",24.0,336,"M30",24.0,"-"]
[null,"BLRF 300# ANSI B16.5 Size 1/2\"","BLRF","300#","ANSI B16.5","1/2\"",15.0,95.2,"-",14.3,35.0,66.5,4.0,15.7,"-",1.6,"-",3.0,61.6,"M12",10.0,1.0]
[null,"BLRF 300# ANSI B16.5 Size 3/4\"","BLRF","300#","ANSI B16.5","3/4\"",20.0,117.5,"-",15.9,42.9,82.5,4.0,19.0,"-",1.6,"-",3.0,70.8,"M16",13.0,1.4]
[null,"BLRF 300# ANSI B16.5 Size 1\"","BLRF","300#","ANSI B16.5","1\"",25.0,123.8,"-",17.5,50.8,88.9,4.0,19.0,"-",1.6,"-",3.0,74,"M16",13.0,1.8]
[null,"BLRF 300# ANSI B16.5 Size 1¼\"","BLRF","300#","ANSI B16.5","1¼\"",32.0,133.3,"-",19.0,63.5,98.5,4.0,19.0,"-",1.6,"-",3.0,77,"M16",13.0,2.7]
[null,"BLRF 300# ANSI B16.5 Size 1½\"","BLRF","300#","ANSI B16.5","1½\"",40.0,155.6,"-",20.6,73.1,114.3,4.0,22.3,"-",1.6,"-",3.0,86.2,"M20",16.0,3.2]
[null,"BLRF 300# ANSI B16.5 Size 2\"","BLRF","300#","ANSI B16.5","2\"",50.0,165.1,"-",22.2,91.9,127.0,8.0,19.0,"-",1.6,"-",4.0,84.4,"M16",13.0,3.6]
[null,"BLRF 300# ANSI B16.5 Size 2½\"","BLRF","300#","ANSI B16.5","2½\"",65.0,190.5,"-",25.4,104.6,149.3,8.0,22.3,"-",1.6,"-",4.0,96.8,"M20",16.0,5.4]
[null,"BLRF 300# ANSI B16.5 Size 3\"","BLRF","300#","ANSI B16.5","3\"",80.0,209.5,"-",28.6,127.0,168.1,8.0,22.3,"-",1.6,"-",4.0,103.2,"M20",16.0,7.3]
[null,"BLRF 300# ANSI B16.5 Size 3½\"","BLRF","300#","ANSI B16.5","3½\"","-",228.6,"-",30.2,139.7,184.1,8.0,22.3,"-",1.6,"-",4.0,106.4,"M20",16.0,9.5]
[null,"BLRF 300# ANSI B16.5 Size 4\"","BLRF","300#","ANSI B16.5","4\"",100.0,254.0,"-",31.7,157.2,200.1,8.0,22.3,"-",1.6,"-",5.0,110.4,"M20",16.0,12.2]
[null,"BLRF 300# ANSI B16.5 Size 5\"","BLRF","300#","ANSI B16.5","5\"",125.0,279.4,"-",34.9,185.6,234.9,8.0,22.3,"-",1.6,"-",5.0,116.8,"M20",16.0,15.9]
[null,"BLRF 300# ANSI B16.5 Size 6\"","BLRF","300#","ANSI B16.5","6\"",150.0,317.5,"-",36.5,215.9,269.7,12.0,22.3,"-",1.6,"-",6.0,121,"M20",16.0,22.7]
[null,"BLRF 300# ANSI B16.5 Size 8\"","BLRF","300#","ANSI B16.5","8\"",200.0,381.0,"-",41.3,269.7,330.2,12.0,25.4,"-",1.6,"-",6.0,136.6,"M24",19.0,37.0]
[null,"BLRF 300# ANSI B16.5 Size 10\"","BLRF","300#","ANSI B16.5","10\"",250.0,444.5,"-",47.6,323.8,387.3,16.0,28.4,"-",1.6,"-",6.0,155.2,"M27",22.0,50.0]
[null,"BLRF 300# ANSI B16.5 Size 12\"","BLRF","300#","ANSI B16.5","12\"",300.0,520.7,"-",50.8,381.0,450.8,16.0,31.7,"-",1.6,"-",6.0,165.6,"M30",24.0,84.0]
[null,"BLRF 300# ANSI B16.5 Size 14\"","BLRF","300#","ANSI B16.5","14\"",350.0,584.2,"-",54.0,412.7,514.3,20.0,31.7,"-",1.6,"-",7.0,173,"M30",24.0,107.0]
[null,"BLRF 300# ANSI B16.5 Size 16\"","BLRF","300#","ANSI B16.5","16\"",400.0,647.7,"-",27.1,469.9,571.5,20.0,35.0,"-",1.6,"-",7.0,123.2,"M33",26.0,139.0]
[null,"BLRF 300# ANSI B16.5 Size 18\"","BLRF","300#","ANSI B16.5","18\"",450.0,711.2,"-",60.3,533.4,628.6,24.0,35.0,"-",1.6,"-",7.0,189.6,"M33",26.0,177.0]
[null,"BLRF 300# ANSI B16.5 Size 20\"","BLRF","300#","ANSI B16.5","20\"",500.0,774.7,"-",63.5,584.2,685.8,24.0,35.0,"-",1.6,"-",7.0,196,"M33",26.0,223.0]
[null,"BLRF 300# ANSI B16.5 Size 22\"","BLRF","300#","ANSI B16.5","22\"",550.0,838.2,"-",64.7,641.2,742.9,24.0,41.3,"-",1.6,"-",7.0,208.4,"M39",31.0,270.0]
[null,"BLRF 300# ANSI B16.5 Size 24\"","BLRF","300#","ANSI B16.5","24\"",600.0,914.4,"-",69.8,692.1,812.8,24.0,41.1,"-",1.6,"-",7.0,218.6,"M39",31.0,342.0]
[null,"BLRF 300# ANSI B16.5 Size 26\"","BLRF","300#","ANSI B16.5","26\"",650.0,971.5,"-",79.6,749.3,876.3,28.0,44.4,"-",1.6,"-",7.0,244.2,"M42",34.0,431.0]
[null,"BLRF 300# ANSI B16.5 Size 30\"","BLRF","300#","ANSI B16.5","30\"",750.0,1092.2,"-",92.1,857.2,996.9,28.0,47.6,"-",1.6,"-",7.0,273.2,"M45",36.0,637.0]
[null,"BLRF 300# ANSI B16.5 Size 34\"","BLRF","300#","ANSI B16.5","34\"",850.0,1206.5,"-",101.6,965.2,1104.9,28.0,50.8,"-",1.6,"-",7.0,296.2,"M48",38.0,862.0]
[null,"BLRF 300# ANSI B16.5 Size 36\"","BLRF","300#","ANSI B16.5","36\"",900.0,1270.0,"-",104.8,1022.3,1168.4,32.0,54.0,"-",1.6,"-",7.0,310.6,"M52",42.0,977.0]
[null,"BLRF 300# ANSI B16.5 Size 42\"","BLRF","300#","ANSI B16.5","42\"",1050.0,1447.8,"-",117.3,1193.8,1339.8,36.0,54.0,"-",1.6,"-",7.0,335.6,"M52",42.0,1436.0]
[null,"BLRF 350# ANSI B16.5 Size 26\"","BLRF","350#","ANSI B16.5","26\"",650.0,850.9,"-",63.5,749.3,777.7,28.0,28.4,"-",1.6,"-",7.0,188,"M27",22.0,"-"]
[null,"BLRF 350# ANSI B16.5 Size 28\"","BLRF","350#","ANSI B16.5","28\"",700.0,901.7,"-",63.5,800.1,828.5,28.0,28.4,"-",1.6,"-",7.0,188,"M27",22.0,"-"]
[null,"BLRF 350# ANSI B16.5 Size 30\"","BLRF","350#","ANSI B16.5","30\"",750.0,958.8,"-",66.5,857.3,886.0,32.0,28.4,"-",1.6,"-",7.0,194,"M27",22.0,"-"]
[null,"BLRF 350# ANSI B16.5 Size 32\"","BLRF","350#","ANSI B16.5","32\"",800.0,1009.7,"-",69.8,908.0,936.8,36.0,28.4,"-",1.6,"-",7.0,200.6,"M27",22.0,"-"]
[null,"BLRF 350# ANSI B16.5 Size 34\"","BLRF","350#","ANSI B16.5","34\"",850.0,1073.1,"-",73.2,958.8,987.6,40.0,28.4,"-",1.6,"-",7.0,207.4,"M27",22.0,"-"]
[null,"BLRF 350# ANSI B16.5 Size 36\"","BLRF","350#","ANSI B16.5","36\"",900.0,1136.6,"-",79.2,1022.3,1054.1,40.0,31.8,"-",1.6,"-",7.0,223.4,"M30",24.0,"-"]
[null,"BLRF 350# ANSI B16.5 Size 38\"","BLRF","350#","ANSI B16.5","38\"",950.0,1187.5,"-",79.2,1073.1,1104.9,40.0,31.8,"-",1.6,"-",7.0,223.4,"M30",24.0,"-"]
[null,"BLRF 350# ANSI B16.5 Size 40\"","BLRF","350#","ANSI B16.5","40\"",1000.0,1238.3,"-",82.5,1124.0,1155.7,44.0,31.8,"-",1.6,"-",7.0,230,"M30",24.0,"-"]
[null,"BLRF 350# ANSI B16.5 Size 42\"","BLRF","350#","ANSI B16.5","42\"",1050.0,1301.8,"-",88.9,1181.1,1212.8,48.0,31.8,"-",1.6,"-",7.0,242.8,"M30",24.0,"-"]
[null,"BLRF 350# ANSI B16.5 Size 44\"","BLRF","350#","ANSI B16.5","44\"",1100.0,1371.6,"-",95.3,1241.6,1276.3,44.0,35.1,"-",1.6,"-",7.0,259.6,"M33",26.0,"-"]
[null,"BLRF 350# ANSI B16.5 Size 46\"","BLRF","350#","ANSI B16.5","46\"",1150.0,1422.4,"-",107.9,1292.4,1327.1,48.0,35.1,"-",1.6,"-",7.0,284.8,"M33",26.0,"-"]
[null,"BLRF 350# ANSI B16.5 Size 48\"","BLRF","350#","ANSI B16.5","48\"",1200.0,1479.6,"-",107.9,1343.2,1377.9,48.0,35.1,"-",1.6,"-",7.0,284.8,"M33",26.0,"-"]
[null,"BLRF 400# ANSI B16.5 Size 1/2\"","BLRF","400#","ANSI B16.5","1/2\"",15.0,95.3,"-",20.6,35.1,66.5,4.0,15.7,"-",6.4,"-",3.0,74.2,"M12",10.0,1.77]
[null,"BLRF 400# ANSI B16.5 Size 3/4\"","BLRF","400#","ANSI B16.5","3/4\"",20.0,117.3,"-",22.1,42.9,82.6,4.0,19.1,"-",6.4,"-",3.0,83.2,"M16",13.0,2.42]
[null,"BLRF 400# ANSI B16.5 Size 1\"","BLRF","400#","ANSI B16.5","1\"",25.0,124.0,"-",23.9,50.8,88.9,4.0,19.1,"-",6.4,"-",3.0,86.8,"M16",13.0,3.57]
[null,"BLRF 400# ANSI B16.5 Size 1¼\"","BLRF","400#","ANSI B16.5","1¼\"",32.0,133.4,"-",27.0,63.5,98.6,4.0,19.1,"-",6.4,"-",3.0,93,"M16",13.0,4.14]
[null,"BLRF 400# ANSI B16.5 Size 1½\"","BLRF","400#","ANSI B16.5","1½\"",40.0,155.4,"-",28.4,73.2,114.3,4.0,22.4,"-",6.4,"-",3.0,101.8,"M20",16.0,5.75]
[null,"BLRF 400# ANSI B16.5 Size 2\"","BLRF","400#","ANSI B16.5","2\"",50.0,165.1,"-",31.8,91.9,127.0,8.0,19.1,"-",6.4,"-",4.0,103.6,"M16",13.0,10.1]
[null,"BLRF 400# ANSI B16.5 Size 2½\"","BLRF","400#","ANSI B16.5","2½\"",65.0,190.5,"-",34.8,104.6,149.4,8.0,22.4,"-",6.4,"-",4.0,115.6,"M20",16.0,14.0]
[null,"BLRF 400# ANSI B16.5 Size 3\"","BLRF","400#","ANSI B16.5","3\"",80.0,209.6,"-",38.4,127.0,168.1,8.0,22.4,"-",6.4,"-",4.0,122.8,"M20",16.0,13.1]
[null,"BLRF 400# ANSI B16.5 Size 3½\"","BLRF","400#","ANSI B16.5","3½\"","-",228.6,"-",41.5,139.7,184.2,8.0,25.4,"-",6.4,"-",4.0,135,"M24",19.0,"-"]
[null,"BLRF 400# ANSI B16.5 Size 4\"","BLRF","400#","ANSI B16.5","4\"",100.0,254.0,"-",41.5,157.2,200.2,8.0,25.4,"-",6.4,"-",5.0,136,"M24",19.0,26.9]
[null,"BLRF 400# ANSI B16.5 Size 5\"","BLRF","400#","ANSI B16.5","5\"",125.0,279.4,"-",44.5,185.7,235.0,8.0,25.4,"-",6.4,"-",5.0,142,"M24",19.0,36.5]
[null,"BLRF 400# ANSI B16.5 Size 6\"","BLRF","400#","ANSI B16.5","6\"",150.0,317.5,"-",47.5,215.9,269.7,12.0,25.4,"-",6.4,"-",6.0,149,"M24",19.0,47.4]
[null,"BLRF 400# ANSI B16.5 Size 8\"","BLRF","400#","ANSI B16.5","8\"",200.0,381.0,"-",54.4,269.7,330.2,12.0,28.4,"-",6.4,"-",6.0,168.8,"M27",22.0,82.5]
[null,"BLRF 400# ANSI B16.5 Size 10\"","BLRF","400#","ANSI B16.5","10\"",250.0,444.5,"-",60.2,323.9,387.4,16.0,31.8,"-",6.4,"-",6.0,184.4,"M30",24.0,122.0]
[null,"BLRF 400# ANSI B16.5 Size 12\"","BLRF","400#","ANSI B16.5","12\"",300.0,520.7,"-",63.6,381.0,450.9,16.0,35.1,"-",6.4,"-",6.0,195.2,"M33",26.0,173.0]
[null,"BLRF 400# ANSI B16.5 Size 14\"","BLRF","400#","ANSI B16.5","14\"",350.0,284.2,"-",66.9,412.8,514.4,20.0,35.1,"-",6.4,"-",7.0,202.8,"M33",26.0,206.0]
[null,"BLRF 400# ANSI B16.5 Size 16\"","BLRF","400#","ANSI B16.5","16\"",400.0,647.7,"-",69.9,469.9,571.5,20.0,38.1,"-",6.4,"-",7.0,214.8,"M36",29.0,259.0]
[null,"BLRF 400# ANSI B16.5 Size 18\"","BLRF","400#","ANSI B16.5","18\"",450.0,711.2,"-",72.9,533.4,628.7,24.0,38.1,"-",6.4,"-",7.0,220.8,"M36",29.0,367.0]
[null,"BLRF 400# ANSI B16.5 Size 20\"","BLRF","400#","ANSI B16.5","20\"",500.0,774.7,"-",76.3,584.2,685.8,24.0,41.1,"-",6.4,"-",7.0,231.6,"M39",31.0,463.0]
[null,"BLRF 400# ANSI B16.5 Size 24\"","BLRF","400#","ANSI B16.5","24\"",600.0,914.4,"-",82.6,692.2,812.8,24.0,47.8,"-",6.4,"-",7.0,254.2,"M45",36.0,876.0]
[null,"BLRF 600# ANSI B16.5 Size 1/2\"","BLRF","600#","ANSI B16.5","1/2\"",15.0,95.3,"-",20.6,35.1,66.5,4.0,15.7,"-",6.4,"-",3.0,74.2,"M12",10.0,0.76]
[null,"BLRF 600# ANSI B16.5 Size 3/4\"","BLRF","600#","ANSI B16.5","3/4\"",20.0,117.3,"-",22.1,42.9,82.6,4.0,19.1,"-",6.4,"-",3.0,83.2,"M16",13.0,1.28]
[null,"BLRF 600# ANSI B16.5 Size 1\"","BLRF","600#","ANSI B16.5","1\"",25.0,124.0,"-",23.9,50.8,88.9,4.0,19.1,"-",6.4,"-",3.0,86.8,"M16",13.0,1.6]
[null,"BLRF 600# ANSI B16.5 Size 1¼\"","BLRF","600#","ANSI B16.5","1¼\"",32.0,133.4,"-",27.0,63.5,98.6,4.0,19.1,"-",6.4,"-",3.0,93,"M16",13.0,2.23]
[null,"BLRF 600# ANSI B16.5 Size 1½\"","BLRF","600#","ANSI B16.5","1½\"",40.0,155.4,"-",28.4,73.2,114.3,4.0,22.3,"-",6.4,"-",3.0,101.8,"M20",16.0,3.25]
[null,"BLRF 600# ANSI B16.5 Size 2\"","BLRF","600#","ANSI B16.5","2\"",50.0,165.1,"-",31.8,91.9,127.0,8.0,19.1,"-",6.4,"-",4.0,103.6,"M16",13.0,1.15]
[null,"BLRF 600# ANSI B16.5 Size 2½\"","BLRF","600#","ANSI B16.5","2½\"",65.0,190.5,"-",34.8,104.6,149.4,8.0,22.4,"-",6.4,"-",4.0,115.6,"M20",16.0,6.13]
[null,"BLRF 600# ANSI B16.5 Size 3\"","BLRF","600#","ANSI B16.5","3\"",80.0,209.6,"-",38.4,127.0,168.1,8.0,22.4,"-",6.4,"-",4.0,122.8,"M20",16.0,8.44]
[null,"BLRF 600# ANSI B16.5 Size 3½\"","BLRF","600#","ANSI B16.5","3½\"","-",228.6,"-",41.5,139.7,184.2,8.0,25.4,"-",6.4,"-",4.0,135,"M24",19.0,11.0]
[null,"BLRF 600# ANSI B16.5 Size 4\"","BLRF","600#","ANSI B16.5","4\"",100.0,273.1,"-",44.5,157.2,215.9,8.0,25.4,"-",6.4,"-",5.0,142,"M24",19.0,17.3]
[null,"BLRF 600# ANSI B16.5 Size 5\"","BLRF","600#","ANSI B16.5","5\"",125.0,330.2,"-",50.9,185.7,266.7,8.0,28.4,"-",6.4,"-",5.0,160.8,"M27",22.0,29.4]
[null,"BLRF 600# ANSI B16.5 Size 6\"","BLRF","600#","ANSI B16.5","6\"",150.0,355.6,"-",54.2,215.9,292.1,12.0,28.4,"-",6.4,"-",6.0,168.4,"M27",22.0,36.1]
[null,"BLRF 600# ANSI B16.5 Size 8\"","BLRF","600#","ANSI B16.5","8\"",200.0,419.1,"-",62.0,269.7,349.3,12.0,31.8,"-",6.4,"-",6.0,188,"M30",24.0,58.9]
[null,"BLRF 600# ANSI B16.5 Size 10\"","BLRF","600#","ANSI B16.5","10\"",250.0,508.0,"-",69.9,323.9,431.8,16.0,35.1,"-",6.4,"-",6.0,207.8,"M33",26.0,97.5]
[null,"BLRF 600# ANSI B16.5 Size 12\"","BLRF","600#","ANSI B16.5","12\"",300.0,558.8,"-",72.9,381.0,489.0,20.0,35.1,"-",6.4,"-",6.0,213.8,"M33",26.0,124.0]
[null,"BLRF 600# ANSI B16.5 Size 14\"","BLRF","600#","ANSI B16.5","14\"",350.0,603.3,"-",76.3,412.8,527.1,20.0,38.1,"-",6.4,"-",7.0,227.6,"M36",29.0,151.0]
[null,"BLRF 600# ANSI B16.5 Size 16\"","BLRF","600#","ANSI B16.5","16\"",400.0,685.8,"-",82.6,469.9,603.3,20.0,41.1,"-",6.4,"-",7.0,244.2,"M39",31.0,214.0]
[null,"BLRF 600# ANSI B16.5 Size 18\"","BLRF","600#","ANSI B16.5","18\"",450.0,743.0,"-",89.0,533.4,654.1,20.0,44.5,"-",6.4,"-",7.0,263,"M42",34.0,272.0]
[null,"BLRF 600# ANSI B16.5 Size 20\"","BLRF","600#","ANSI B16.5","20\"",500.0,812.8,"-",95.3,584.2,723.9,24.0,44.5,"-",6.4,"-",7.0,275.6,"M42",34.0,349.0]
[null,"BLRF 600# ANSI B16.5 Size 22\"","BLRF","600#","ANSI B16.5","22\"",550.0,869.9,"-",99.6,641.2,777.9,24.0,47.6,"-",6.4,"-",7.0,288.2,"M45",36.0,437.0]
[null,"BLRF 600# ANSI B16.5 Size 24\"","BLRF","600#","ANSI B16.5","24\"",600.0,939.8,"-",108.0,692.2,838.2,24.0,50.8,"-",6.4,"-",7.0,309,"M48",38.0,533.0]
[null,"BLRF 600# ANSI B16.5 Size 26\"","BLRF","600#","ANSI B16.5","26\"",650.0,1130.3,"-",114.3,749.3,914.4,28.0,50.8,"-",6.4,"-",7.0,321.6,"M48",38.0,676.0]
[null,"BLRF 600# ANSI B16.5 Size 30\"","BLRF","600#","ANSI B16.5","30\"",750.0,1130.3,"-",120.7,857.2,1022.3,28.0,54.0,"-",6.4,"-",7.0,342.4,"M52",42.0,895.0]
[null,"BLRF 600# ANSI B16.5 Size 34\"","BLRF","600#","ANSI B16.5","34\"",850.0,1244.6,"-",127.0,965.2,1130.3,28.0,60.3,"-",6.4,"-",7.0,361,"M56",45.0,1185.0]
[null,"BLRF 600# ANSI B16.5 Size 36\"","BLRF","600#","ANSI B16.5","36\"",900.0,1314.4,"-",130.2,1022.3,1193.8,28.0,66.7,"-",6.4,"-",7.0,379.4,"M64",51.0,1368.0]
[null,"BLRF 600# ANSI B16.5 Size 42\"","BLRF","600#","ANSI B16.5","42\"",1050.0,1492.2,"-",146.1,1193.8,1365.2,28.0,73.0,"-",6.4,"-",7.0,419.2,"M68",55.0,2006.0]
[null,"BLRF 900# ANSI B16.5 Size 1/2\"","BLRF","900#","ANSI B16.5","1/2\"",15.0,120.6,"-",28.7,35.0,82.5,4.0,22.3,"-",6.4,"-",3.0,102.4,"M20",16.0,1.77]
[null,"BLRF 900# ANSI B16.5 Size 3/4\"","BLRF","900#","ANSI B16.5","3/4\"",20.0,130.0,"-",31.8,42.9,88.9,4.0,22.3,"-",6.4,"-",3.0,108.6,"M20",16.0,2.42]
[null,"BLRF 900# ANSI B16.5 Size 1\"","BLRF","900#","ANSI B16.5","1\"",25.0,149.3,"-",34.8,50.8,101.6,4.0,25.4,"-",6.4,"-",3.0,120.6,"M24",19.0,3.57]
[null,"BLRF 900# ANSI B16.5 Size 1¼\"","BLRF","900#","ANSI B16.5","1¼\"",32.0,158.7,"-",34.8,63.5,111.2,4.0,25.4,"-",6.4,"-",3.0,120.6,"M24",19.0,4.14]
[null,"BLRF 900# ANSI B16.5 Size 1½\"","BLRF","900#","ANSI B16.5","1½\"",40.0,177.8,"-",38.1,73.1,123.9,4.0,28.4,"-",6.4,"-",3.0,133.2,"M27",22.0,5.75]
[null,"BLRF 900# ANSI B16.5 Size 2\"","BLRF","900#","ANSI B16.5","2\"",50.0,215.9,"-",44.5,91.9,165.1,8.0,25.4,"-",6.4,"-",4.0,141,"M24",19.0,10.1]
[null,"BLRF 900# ANSI B16.5 Size 2½\"","BLRF","900#","ANSI B16.5","2½\"",65.0,244.3,"-",47.5,104.6,190.5,8.0,28.4,"-",6.4,"-",4.0,153,"M27",22.0,14.0]
[null,"BLRF 900# ANSI B16.5 Size 3\"","BLRF","900#","ANSI B16.5","3\"",80.0,241.3,"-",44.5,127.0,190.5,8.0,25.4,"-",6.4,"-",4.0,135,"M20",16.0,13.1]
[null,"BLRF 900# ANSI B16.5 Size 4\"","BLRF","900#","ANSI B16.5","4\"",100.0,292.1,"-",50.8,157.2,234.9,8.0,31.7,"-",6.4,"-",5.0,160.6,"M27",22.0,26.9]
[null,"BLRF 900# ANSI B16.5 Size 5\"","BLRF","900#","ANSI B16.5","5\"",125.0,349.2,"-",57.2,185.6,279.4,8.0,35.0,"-",6.4,"-",5.0,181.4,"M33",26.0,36.5]
[null,"BLRF 900# ANSI B16.5 Size 6\"","BLRF","900#","ANSI B16.5","6\"",150.0,381.0,"-",62.0,215.9,317.5,12.0,31.7,"-",6.4,"-",6.0,184,"M27",22.0,47.4]
[null,"BLRF 900# ANSI B16.5 Size 8\"","BLRF","900#","ANSI B16.5","8\"",200.0,469.9,"-",69.9,269.7,393.7,12.0,38.1,"-",6.4,"-",6.0,213.8,"M36",29.0,82.5]
[null,"BLRF 900# ANSI B16.5 Size 10\"","BLRF","900#","ANSI B16.5","10\"",250.0,546.1,"-",76.2,323.8,169.9,16.0,38.1,"-",6.4,"-",6.0,226.4,"M36",29.0,122.0]
[null,"BLRF 900# ANSI B16.5 Size 12\"","BLRF","900#","ANSI B16.5","12\"",300.0,609.6,"-",85.6,381.0,533.4,20.0,38.1,"-",6.4,"-",6.0,245.2,"M36",29.0,173.0]
[null,"BLRF 900# ANSI B16.5 Size 14\"","BLRF","900#","ANSI B16.5","14\"",350.0,641.3,"-",92.2,412.7,558.8,20.0,41.1,"-",6.4,"-",7.0,259.4,"M39",29.0,206.0]
[null,"BLRF 900# ANSI B16.5 Size 16\"","BLRF","900#","ANSI B16.5","16\"",400.0,704.8,"-",95.3,469.9,615.9,20.0,44.4,"-",6.4,"-",7.0,275.6,"M42",34.0,259.0]
[null,"BLRF 900# ANSI B16.5 Size 18\"","BLRF","900#","ANSI B16.5","18\"",450.0,787.4,"-",108.0,533.4,685.8,20.0,50.8,"-",6.4,"-",7.0,309,"M48",38.0,367.0]
[null,"BLRF 900# ANSI B16.5 Size 20\"","BLRF","900#","ANSI B16.5","20\"",500.0,857.2,"-",114.3,584.2,749.3,20.0,53.8,"-",6.4,"-",7.0,329.6,"M52",42.0,463.0]
[null,"BLRF 900# ANSI B16.5 Size 24\"","BLRF","900#","ANSI B16.5","24\"",600.0,1041.4,"-",146.1,692.1,901.7,20.0,66.5,"-",6.4,"-",7.0,411.2,"M64",51.0,876.0]
[null,"BLRF 1500# ANSI B16.5 Size 1/2\"","BLRF","1500#","ANSI B16.5","1/2\"",15.0,120.6,"-",28.7,35.0,82.5,4.0,22.3,"-",6.4,"-",3.0,102.4,"M20",16.0,1.77]
[null,"BLRF 1500# ANSI B16.5 Size 3/4\"","BLRF","1500#","ANSI B16.5","3/4\"",20.0,130.0,"-",31.8,42.9,88.9,4.0,22.3,"-",6.4,"-",3.0,108.6,"M20",16.0,2.42]
[null,"BLRF 1500# ANSI B16.5 Size 1\"","BLRF","1500#","ANSI B16.5","1\"",25.0,149.3,"-",34.8,50.8,101.6,4.0,25.4,"-",6.4,"-",3.0,120.6,"M24",19.0,3.57]
[null,"BLRF 1500# ANSI B16.5 Size 1¼\"","BLRF","1500#","ANSI B16.5","1¼\"",32.0,158.7,"-",34.8,63.5,111.2,4.0,25.4,"-",6.4,"-",3.0,120.6,"M24",19.0,4.14]
[null,"BLRF 1500# ANSI B16.5 Size 1½\"","BLRF","1500#","ANSI B16.5","1½\"",40.0,177.8,"-",38.1,73.1,123.9,4.0,28.4,"-",6.4,"-",3.0,133.2,"M27",22.0,5.75]
[null,"BLRF 1500# ANSI B16.5 Size 2\"","BLRF","1500#","ANSI B16.5","2\"",50.0,215.9,"-",44.5,91.9,165.1,8.0,25.4,"-",6.4,"-",4.0,141,"M24",19.0,10.1]
[null,"BLRF 1500# ANSI B16.5 Size 2½\"","BLRF","1500#","ANSI B16.5","2½\"",65.0,244.3,"-",47.5,104.6,190.5,8.0,28.4,"-",6.4,"-",4.0,153,"M27",22.0,14.0]
[null,"BLRF 1500# ANSI B16.5 Size 3\"","BLRF","1500#","ANSI B16.5","3\"",80.0,266.7,"-",54.1,127.0,203.2,8.0,31.7,"-",6.4,"-",4.0,170.2,"M30",24.0,19.1]
[null,"BLRF 1500# ANSI B16.5 Size 4\"","BLRF","1500#","ANSI B16.5","4\"",100.0,311.1,"-",60.2,157.2,241.3,8.0,35.0,"-",6.4,"-",5.0,187.4,"M33",26.0,29.9]
[null,"BLRF 1500# ANSI B16.5 Size 5\"","BLRF","1500#","ANSI B16.5","5\"",125.0,374.6,"-",79.5,185.6,292.1,8.0,41.1,"-",6.4,"-",5.0,236,"M39",31.0,58.4]
[null,"BLRF 1500# ANSI B16.5 Size 6\"","BLRF","1500#","ANSI B16.5","6\"",150.0,393.7,"-",86.9,215.9,317.5,12.0,38.1,"-",6.4,"-",6.0,247.8,"M36",29.0,71.8]
[null,"BLRF 1500# ANSI B16.5 Size 8\"","BLRF","1500#","ANSI B16.5","8\"",200.0,482.6,"-",98.3,269.7,393.7,12.0,44.4,"-",6.4,"-",6.0,280.6,"M42",34.0,122.0]
[null,"BLRF 1500# ANSI B16.5 Size 10\"","BLRF","1500#","ANSI B16.5","10\"",250.0,584.2,"-",114.3,323.8,485.6,12.0,50.8,"-",6.4,"-",6.0,320.6,"M48",38.0,210.0]
[null,"BLRF 1500# ANSI B16.5 Size 12\"","BLRF","1500#","ANSI B16.5","12\"",300.0,673.1,"-",130.3,381.0,571.5,16.0,53.8,"-",6.4,"-",6.0,360.6,"M52",42.0,316.0]
[null,"BLRF 1500# ANSI B16.5 Size 14\"","BLRF","1500#","ANSI B16.5","14\"",350.0,749.3,"-",139.7,412.7,635.0,16.0,60.4,"-",6.4,"-",7.0,386.4,"M56",45.0,420.0]
[null,"BLRF 1500# ANSI B16.5 Size 16\"","BLRF","1500#","ANSI B16.5","16\"",400.0,825.5,"-",152.4,469.9,704.8,16.0,66.5,"-",6.4,"-",7.0,417.8,"M60",48.0,558.0]
[null,"BLRF 1500# ANSI B16.5 Size 18\"","BLRF","1500#","ANSI B16.5","18\"",450.0,914.4,"-",168.4,533.4,774.7,16.0,73.1,"-",6.4,"-",7.0,461.8,"M68",54.0,760.0]
[null,"BLRF 1500# ANSI B16.5 Size 20\"","BLRF","1500#","ANSI B16.5","20\"",500.0,984.2,"-",184.2,584.2,831.8,16.0,79.2,"-",6.4,"-",7.0,507.4,"M76",61.0,965.0]
[null,"BLRF 1500# ANSI B16.5 Size 24\"","BLRF","1500#","ANSI B16.5","24\"",600.0,1168.4,"-",209.6,692.1,990.6,16.0,91.9,"-",6.4,"-",7.0,564.2,"M80",64.0,1558.0]
[null,"BLRF 2500# ANSI B16.5 Size 1/2\"","BLRF","2500#","ANSI B16.5","1/2\"",15.0,133.4,"-",36.6,35.1,88.9,4.0,22.4,"-",6.4,"-",3.0,118.2,"M20",16.0,2.99]
[null,"BLRF 2500# ANSI B16.5 Size 3/4\"","BLRF","2500#","ANSI B16.5","3/4\"",20.0,139.7,"-",38.2,42.9,95.3,4.0,22.4,"-",6.4,"-",3.0,121.4,"M20",16.0,3.5]
[null,"BLRF 2500# ANSI B16.5 Size 1\"","BLRF","2500#","ANSI B16.5","1\"",25.0,158.8,"-",41.5,50.8,108.0,4.0,25.4,"-",6.4,"-",3.0,134,"M24",19.0,4.96]
[null,"BLRF 2500# ANSI B16.5 Size 1¼\"","BLRF","2500#","ANSI B16.5","1¼\"",32.0,184.2,"-",44.5,63.5,130.0,4.0,28.4,"-",6.4,"-",3.0,146,"M27",22.0,7.35]
[null,"BLRF 2500# ANSI B16.5 Size 1½\"","BLRF","2500#","ANSI B16.5","1½\"",40.0,203.2,"-",50.9,73.1,146.1,4.0,31.8,"-",6.4,"-",3.0,162.8,"M30",24.0,10.4]
[null,"BLRF 2500# ANSI B16.5 Size 2\"","BLRF","2500#","ANSI B16.5","2\"",50.0,235.0,"-",57.2,91.9,171.5,8.0,28.4,"-",6.4,"-",4.0,172.4,"M27",22.0,15.6]
[null,"BLRF 2500# ANSI B16.5 Size 2½\"","BLRF","2500#","ANSI B16.5","2½\"",65.0,266.7,"-",63.6,104.6,196.9,8.0,31.8,"-",6.4,"-",4.0,189.2,"M30",24.0,22.6]
[null,"BLRF 2500# ANSI B16.5 Size 3\"","BLRF","2500#","ANSI B16.5","3\"",80.0,304.8,"-",72.9,127.0,228.6,8.0,35.1,"-",6.4,"-",4.0,211.8,"M33",26.0,34.8]
[null,"BLRF 2500# ANSI B16.5 Size 4\"","BLRF","2500#","ANSI B16.5","4\"",100.0,355.6,"-",82.6,157.2,273.1,8.0,41.1,"-",6.4,"-",5.0,242.2,"M39",31.0,53.9]
[null,"BLRF 2500# ANSI B16.5 Size 5\"","BLRF","2500#","ANSI B16.5","5\"",125.0,419.1,"-",98.3,185.6,323.9,8.0,47.8,"-",6.4,"-",5.0,283.6,"M45",36.0,90.8]
[null,"BLRF 2500# ANSI B16.5 Size 6\"","BLRF","2500#","ANSI B16.5","6\"",150.0,482.6,"-",114.4,215.9,368.3,8.0,53.8,"-",6.4,"-",6.0,320.8,"M48",38.0,141.0]
[null,"BLRF 2500# ANSI B16.5 Size 8\"","BLRF","2500#","ANSI B16.5","8\"",200.0,552.5,"-",133.4,269.7,438.2,12.0,53.8,"-",6.4,"-",6.0,358.8,"M48",38.0,214.0]
[null,"BLRF 2500# ANSI B16.5 Size 10\"","BLRF","2500#","ANSI B16.5","10\"",250.0,673.1,"-",171.5,323.8,539.8,12.0,66.5,"-",6.4,"-",6.0,455,"M60",48.0,411.0]
[null,"BLRF 2500# ANSI B16.5 Size 12\"","BLRF","2500#","ANSI B16.5","12\"",300.0,762.0,"-",190.6,381.0,619.3,12.0,73.2,"-",6.4,"-",6.0,499.2,"M64",51.0,592.0]
[null,"BLRF  75# ANSI B16.47-API 605 Size 26\"","BLRF"," 75#","ANSI B16.47-API 605","26\"",650.0,762.0,"-",33.3,704.9,723.9,36.0,19.1,"-",1.6,"-",7.0,{"$f":"(J389+U389+8)*2+R389","v":115.6},"M16",13.0,"-"]
[null,"BLRF  75# ANSI B16.47-API 605 Size 28\"","BLRF"," 75#","ANSI B16.47-API 605","28\"",700.0,812.8,"-",33.3,755.7,774.7,40.0,19.1,"-",1.6,"-",7.0,115.6,"M16",13.0,"-"]
[null,"BLRF  75# ANSI B16.47-API 605 Size 30\"","BLRF"," 75#","ANSI B16.47-API 605","30\"",750.0,863.6,"-",33.3,806.5,825.5,44.0,19.1,"-",1.6,"-",7.0,115.6,"M16",13.0,"-"]
[null,"BLRF  75# ANSI B16.47-API 605 Size 32\"","BLRF"," 75#","ANSI B16.47-API 605","32\"",800.0,914.4,"-",35.1,857.3,876.3,48.0,19.1,"-",1.6,"-",7.0,119.2,"M16",13.0,"-"]
[null,"BLRF  75# ANSI B16.47-API 605 Size 34\"","BLRF"," 75#","ANSI B16.47-API 605","34\"",850.0,965.2,"-",35.1,908.1,927.1,52.0,19.1,"-",1.6,"-",7.0,119.2,"M16",13.0,"-"]
[null,"BLRF  75# ANSI B16.47-API 605 Size 36\"","BLRF"," 75#","ANSI B16.47-API 605","36\"",900.0,1033.5,"-",36.6,965.2,992.1,40.0,22.4,"-",1.6,"-",7.0,128.2,"M20",16.0,"-"]
[null,"BLRF  75# ANSI B16.47-API 605 Size 38\"","BLRF"," 75#","ANSI B16.47-API 605","38\"",950.0,1084.3,"-",38.1,1016.0,1042.9,40.0,22.4,"-",1.6,"-",7.0,131.2,"M20",16.0,"-"]
[null,"BLRF  75# ANSI B16.47-API 605 Size 40\"","BLRF"," 75#","ANSI B16.47-API 605","40\"",1000.0,1135.1,"-",38.1,1066.8,1093.7,44.0,22.4,"-",1.6,"-",7.0,131.2,"M20",16.0,"-"]
[null,"BLRF  75# ANSI B16.47-API 605 Size 42\"","BLRF"," 75#","ANSI B16.47-API 605","42\"",1050.0,1185.9,"-",39.6,1117.6,1144.5,48.0,22.4,"-",1.6,"-",7.0,134.2,"M20",16.0,"-"]
[null,"BLRF  75# ANSI B16.47-API 605 Size 44\"","BLRF"," 75#","ANSI B16.47-API 605","44\"",1100.0,1251.0,"-",42.9,1174.8,1203.5,36.0,25.4,"-",1.6,"-",7.0,144.8,"M22",18.0,"-"]
[null,"BLRF  75# ANSI B16.47-API 605 Size 46\"","BLRF"," 75#","ANSI B16.47-API 605","46\"",1150.0,1301.8,"-",44.5,1225.6,1254.3,40.0,25.4,"-",1.6,"-",7.0,148,"M22",18.0,"-"]
[null,"BLRF  75# ANSI B16.47-API 605 Size 48\"","BLRF"," 75#","ANSI B16.47-API 605","48\"",1200.0,1352.6,"-",46.0,1276.4,1305.1,44.0,25.4,"-",1.6,"-",7.0,151,"M22",18.0,"-"]
[null,"BLRF  75# ANSI B16.47-API 605 Size 50\"","BLRF"," 75#","ANSI B16.47-API 605","50\"",1250.0,1403.4,"-",47.8,1327.2,1355.9,44.0,25.4,"-",1.6,"-",7.0,154.6,"M22",18.0,"-"]
[null,"BLRF  75# ANSI B16.47-API 605 Size 52\"","BLRF"," 75#","ANSI B16.47-API 605","52\"",1300.0,1457.5,"-",47.8,1378.0,1409.7,48.0,25.4,"-",1.6,"-",7.0,154.6,"M22",18.0,"-"]
[null,"BLRF  75# ANSI B16.47-API 605 Size 54\"","BLRF"," 75#","ANSI B16.47-API 605","54\"",1350.0,1508.3,"-",49.3,1428.8,1460.5,48.0,25.4,"-",1.6,"-",7.0,157.6,"M22",18.0,"-"]
[null,"BLRF  75# ANSI B16.47-API 605 Size 56\"","BLRF"," 75#","ANSI B16.47-API 605","56\"",1400.0,1574.8,"-",50.8,1485.9,1521.0,40.0,28.4,"-",1.6,"-",7.0,162.6,"M24",19.0,"-"]
[null,"BLRF  75# ANSI B16.47-API 605 Size 58\"","BLRF"," 75#","ANSI B16.47-API 605","58\"",1450.0,1625.6,"-",52.3,1536.7,1571.8,44.0,28.4,"-",1.6,"-",7.0,165.6,"M24",19.0,"-"]
[null,"BLRF  75# ANSI B16.47-API 605 Size 60\"","BLRF"," 75#","ANSI B16.47-API 605","60\"",1500.0,1676.4,"-",55.6,1587.5,1622.6,44.0,28.4,"-",1.6,"-",7.0,172.2,"M24",19.0,"-"]
[null,"BLRF  150# ANSI B16.47-API 605 Size 26\"","BLRF"," 150#","ANSI B16.47-API 605","26\"",650.0,785.9,"-",41.1,711.2,744.5,36.0,22.4,"-",1.6,"-",7.0,137.2,"M20",16.0,"-"]
[null,"BLRF  150# ANSI B16.47-API 605 Size 28\"","BLRF"," 150#","ANSI B16.47-API 605","28\"",700.0,836.7,"-",44.5,762.0,795.3,40.0,22.4,"-",1.6,"-",7.0,144,"M20",16.0,"-"]
[null,"BLRF  150# ANSI B16.47-API 605 Size 30\"","BLRF"," 150#","ANSI B16.47-API 605","30\"",750.0,887.5,"-",44.5,812.8,846.1,44.0,22.4,"-",1.6,"-",7.0,144,"M20",16.0,"-"]
[null,"BLRF  150# ANSI B16.47-API 605 Size 32\"","BLRF"," 150#","ANSI B16.47-API 605","32\"",800.0,941.3,"-",46.0,863.6,900.2,48.0,22.4,"-",1.6,"-",7.0,147,"M20",16.0,"-"]
[null,"BLRF  150# ANSI B16.47-API 605 Size 34\"","BLRF"," 150#","ANSI B16.47-API 605","34\"",850.0,1004.8,"-",49.3,920.8,957.3,40.0,25.4,"-",1.6,"-",7.0,157.6,"M22",18.0,"-"]
[null,"BLRF  150# ANSI B16.47-API 605 Size 36\"","BLRF"," 150#","ANSI B16.47-API 605","36\"",900.0,1057.1,"-",52.3,971.6,1009.7,44.0,25.4,"-",1.6,"-",7.0,163.6,"M22",18.0,"-"]
[null,"BLRF  150# ANSI B16.47-API 605 Size 38\"","BLRF"," 150#","ANSI B16.47-API 605","38\"",950.0,1124.0,"-",53.8,1022.4,1069.8,40.0,28.4,"-",1.6,"-",7.0,168.6,"M24",19.0,"-"]
[null,"BLRF  150# ANSI B16.47-API 605 Size 40\"","BLRF"," 150#","ANSI B16.47-API 605","40\"",1000.0,1174.8,"-",55.6,1120.6,1120.6,44.0,28.4,"-",1.6,"-",7.0,172.2,"M24",19.0,"-"]
[null,"BLRF  150# ANSI B16.47-API 605 Size 42\"","BLRF"," 150#","ANSI B16.47-API 605","42\"",1050.0,1225.6,"-",58.7,1130.3,1171.4,48.0,28.4,"-",1.6,"-",7.0,178.4,"M24",19.0,"-"]
[null,"BLRF  150# ANSI B16.47-API 605 Size 44\"","BLRF"," 150#","ANSI B16.47-API 605","44\"",1100.0,1276.4,"-",60.5,1435.1,1222.2,52.0,28.4,"-",1.6,"-",7.0,182,"M24",19.0,"-"]
[null,"BLRF  150# ANSI B16.47-API 605 Size 46\"","BLRF"," 150#","ANSI B16.47-API 605","46\"",1150.0,1341.4,"-",62.0,1234.9,1284.2,40.0,31.8,"-",1.6,"-",7.0,191,"M27",22.0,"-"]
[null,"BLRF  150# ANSI B16.47-API 605 Size 48\"","BLRF"," 150#","ANSI B16.47-API 605","48\"",1200.0,1392.2,"-",65.0,1289.1,1335.0,44.0,31.8,"-",1.6,"-",7.0,197,"M27",22.0,"-"]
[null,"BLRF  150# ANSI B16.47-API 605 Size 50\"","BLRF"," 150#","ANSI B16.47-API 605","50\"",1250.0,1435.4,"-",68.3,1339.9,1385.8,48.0,31.8,"-",1.6,"-",7.0,203.6,"M27",22.0,"-"]
[null,"BLRF  150# ANSI B16.47-API 605 Size 52\"","BLRF"," 150#","ANSI B16.47-API 605","52\"",1300.0,1493.8,"-",69.9,1390.7,1436.6,52.0,31.8,"-",1.6,"-",7.0,206.8,"M27",22.0,"-"]
[null,"BLRF  150# ANSI B16.47-API 605 Size 54\"","BLRF"," 150#","ANSI B16.47-API 605","54\"",1350.0,1549.4,"-",71.4,1441.5,1492.3,56.0,31.8,"-",1.6,"-",7.0,209.8,"M27",22.0,"-"]
[null,"BLRF  150# ANSI B16.47-API 605 Size 56\"","BLRF"," 150#","ANSI B16.47-API 605","56\"",1400.0,1600.2,"-",73.2,1492.3,1543.1,60.0,31.8,"-",1.6,"-",7.0,213.4,"M27",22.0,"-"]
[null,"BLRF  150# ANSI B16.47-API 605 Size 58\"","BLRF"," 150#","ANSI B16.47-API 605","58\"",1450.0,1674.9,"-",74.7,1543.1,1611.4,48.0,35.1,"-",1.6,"-",7.0,224.4,"M33",26.0,"-"]
[null,"BLRF  150# ANSI B16.47-API 605 Size 60\"","BLRF"," 150#","ANSI B16.47-API 605","60\"",1500.0,1725.7,"-",76.2,1600.2,1662.2,52.0,35.1,"-",1.6,"-",7.0,227.4,"M33",26.0,"-"]
[null,"BLRF  300# ANSI B16.47-API 605 Size 26\"","BLRF"," 300#","ANSI B16.47-API 605","26\"",650.0,866.6,"-",88.9,736.6,803.1,32.0,35.1,"-",1.6,"-",7.0,252.8,"M33",26.0,"-"]
[null,"BLRF  300# ANSI B16.47-API 605 Size 28\"","BLRF"," 300#","ANSI B16.47-API 605","28\"",700.0,920.8,"-",88.9,787.4,857.3,36.0,35.1,"-",1.6,"-",7.0,252.8,"M33",26.0,"-"]
[null,"BLRF  300# ANSI B16.47-API 605 Size 30\"","BLRF"," 300#","ANSI B16.47-API 605","30\"",750.0,990.6,"-",93.7,844.6,920.8,36.0,38.1,"-",1.6,"-",7.0,262.4,"M36",26.0,"-"]
[null,"BLRF  300# ANSI B16.47-API 605 Size 32\"","BLRF"," 300#","ANSI B16.47-API 605","32\"",800.0,1054.1,"-",103.1,901.7,977.9,32.0,41.1,"-",1.6,"-",7.0,291.2,"M39",31.0,"-"]
[null,"BLRF  300# ANSI B16.47-API 605 Size 34\"","BLRF"," 300#","ANSI B16.47-API 605","34\"",850.0,1107.9,"-",103.1,952.5,1031.7,36.0,41.1,"-",1.6,"-",7.0,291.2,"M39",31.0,"-"]
[null,"BLRF  300# ANSI B16.47-API 605 Size 36\"","BLRF"," 300#","ANSI B16.47-API 605","36\"",900.0,1171.4,"-",103.1,1009.7,1089.2,32.0,44.5,"-",1.6,"-",7.0,297.2,"M42",34.0,"-"]
[null,"BLRF  300# ANSI B16.47-API 605 Size 38\"","BLRF"," 300#","ANSI B16.47-API 605","38\"",950.0,1222.2,"-",111.3,1060.5,1140.0,36.0,44.5,"-",1.6,"-",7.0,313.6,"M42",34.0,"-"]
[null,"BLRF  300# ANSI B16.47-API 605 Size 40\"","BLRF"," 300#","ANSI B16.47-API 605","40\"",1000.0,1273.0,"-",115.8,1114.6,1190.8,40.0,44.5,"-",1.6,"-",7.0,322.6,"M42",34.0,"-"]
[null,"BLRF  300# ANSI B16.47-API 605 Size 42\"","BLRF"," 300#","ANSI B16.47-API 605","42\"",1050.0,1333.5,"-",119.1,1168.4,1244.6,36.0,47.8,"-",1.6,"-",7.0,333.2,"M45",36.0,"-"]
[null,"BLRF  300# ANSI B16.47-API 605 Size 44\"","BLRF"," 300#","ANSI B16.47-API 605","44\"",1100.0,1384.3,"-",127.0,1219.2,1295.4,40.0,47.8,"-",1.6,"-",7.0,349,"M45",36.0,"-"]
[null,"BLRF  300# ANSI B16.47-API 605 Size 46\"","BLRF"," 300#","ANSI B16.47-API 605","46\"",1150.0,1460.5,"-",128.5,1270.0,1365.3,36.0,50.8,"-",1.6,"-",7.0,356,"M48",38.0,"-"]
[null,"BLRF  300# ANSI B16.47-API 605 Size 48\"","BLRF"," 300#","ANSI B16.47-API 605","48\"",1200.0,1511.3,"-",128.5,1327.2,1416.1,40.0,50.8,"-",1.6,"-",7.0,356,"M48",38.0,"-"]
[null,"BLRF  300# ANSI B16.47-API 605 Size 50\"","BLRF"," 300#","ANSI B16.47-API 605","50\"",1250.0,1562.1,"-",138.2,1378.0,1466.9,44.0,50.8,"-",1.6,"-",7.0,375.4,"M48",38.0,"-"]
[null,"BLRF  300# ANSI B16.47-API 605 Size 52\"","BLRF"," 300#","ANSI B16.47-API 605","52\"",1300.0,1612.9,"-",142.7,1428.8,1517.7,48.0,50.8,"-",1.6,"-",7.0,384.4,"M48",38.0,"-"]
[null,"BLRF  300# ANSI B16.47-API 605 Size 54\"","BLRF"," 300#","ANSI B16.47-API 605","54\"",1350.0,1673.4,"-",136.7,1479.6,1577.8,48.0,50.8,"-",1.6,"-",7.0,372.4,"M48",38.0,"-"]
[null,"BLRF  300# ANSI B16.47-API 605 Size 56\"","BLRF"," 300#","ANSI B16.47-API 605","56\"",1400.0,1765.3,"-",153.9,1536.7,1651.0,36.0,60.5,"-",1.6,"-",7.0,420.8,"M56",45.0,"-"]
[null,"BLRF  300# ANSI B16.47-API 605 Size 58\"","BLRF"," 300#","ANSI B16.47-API 605","58\"",1450.0,1827.3,"-",153.9,1593.9,1713.0,40.0,60.5,"-",1.6,"-",7.0,420.8,"M56",45.0,"-"]
[null,"BLRF  300# ANSI B16.47-API 605 Size 60\"","BLRF"," 300#","ANSI B16.47-API 605","60\"",1500.0,1878.1,"-",150.9,1651.0,1763.8,40.0,60.5,"-",1.6,"-",7.0,414.8,"M56",45.0,"-"]
[null,"BLRF  400# ANSI B16.47-API 605 Size 26\"","BLRF"," 400#","ANSI B16.47-API 605","26\"",650.0,850.9,"-",95.3,711.2,781.1,28.0,38.1,"-",6.4,"-",7.0,271.6,"M36",29.0,"-"]
[null,"BLRF  400# ANSI B16.47-API 605 Size 28\"","BLRF"," 400#","ANSI B16.47-API 605","28\"",700.0,914.4,"-",101.7,762.0,838.2,24.0,41.1,"-",6.4,"-",7.0,288.4,"M39",31.0,"-"]
[null,"BLRF  400# ANSI B16.47-API 605 Size 30\"","BLRF"," 400#","ANSI B16.47-API 605","30\"",750.0,971.6,"-",108.0,819.2,895.4,28.0,41.1,"-",6.4,"-",7.0,301,"M39",31.0,"-"]
[null,"BLRF  400# ANSI B16.47-API 605 Size 32\"","BLRF"," 400#","ANSI B16.47-API 605","32\"",800.0,1035.1,"-",114.4,873.3,952.5,28.0,44.5,"-",6.4,"-",7.0,319.8,"M42",34.0,"-"]
[null,"BLRF  400# ANSI B16.47-API 605 Size 34\"","BLRF"," 400#","ANSI B16.47-API 605","34\"",850.0,1085.9,"-",117.7,927.1,1003.3,32.0,44.5,"-",6.4,"-",7.0,326.4,"M42",34.0,"-"]
[null,"BLRF  400# ANSI B16.47-API 605 Size 36\"","BLRF"," 400#","ANSI B16.47-API 605","36\"",900.0,1155.7,"-",125.5,980.9,1066.8,28.0,47.8,"-",6.4,"-",7.0,346,"M45",36.0,"-"]
[null,"BLRF  400# ANSI B16.47-API 605 Size 38\"","BLRF"," 400#","ANSI B16.47-API 605","38\"",950.0,1206.5,"-",130.4,1035.1,1117.6,32.0,47.8,"-",6.4,"-",7.0,355.8,"M45",36.0,"-"]
[null,"BLRF  400# ANSI B16.47-API 605 Size 40\"","BLRF"," 400#","ANSI B16.47-API 605","40\"",1000.0,1270.0,"-",136.4,1092.2,1174.8,32.0,50.8,"-",6.4,"-",7.0,371.8,"M48",38.0,"-"]
[null,"BLRF  400# ANSI B16.47-API 605 Size 42\"","BLRF"," 400#","ANSI B16.47-API 605","42\"",1050.0,1320.8,"-",139.8,1143.0,1225.6,32.0,50.8,"-",6.4,"-",7.0,378.6,"M48",38.0,"-"]
[null,"BLRF  400# ANSI B16.47-API 605 Size 44\"","BLRF"," 400#","ANSI B16.47-API 605","44\"",1100.0,1384.3,"-",146.1,1200.2,1282.7,32.0,53.8,"-",6.4,"-",7.0,391.2,"M48",38.0,"-"]
[null,"BLRF  400# ANSI B16.47-API 605 Size 46\"","BLRF"," 400#","ANSI B16.47-API 605","46\"",1150.0,1441.5,"-",152.5,1257.3,1339.9,36.0,53.8,"-",6.4,"-",7.0,404,"M48",38.0,"-"]
[null,"BLRF  400# ANSI B16.47-API 605 Size 48\"","BLRF"," 400#","ANSI B16.47-API 605","48\"",1200.0,1511.3,"-",158.8,1308.1,1403.4,28.0,60.5,"-",6.4,"-",7.0,430.6,"M56",45.0,"-"]
[null,"BLRF  400# ANSI B16.47-API 605 Size 50\"","BLRF"," 400#","ANSI B16.47-API 605","50\"",1250.0,1568.5,"-",163.6,1361.9,1460.5,32.0,60.5,"-",6.4,"-",7.0,440.2,"M56",45.0,"-"]
[null,"BLRF  400# ANSI B16.47-API 605 Size 52\"","BLRF"," 400#","ANSI B16.47-API 605","52\"",1300.0,1619.3,"-",168.5,1412.7,1511.3,32.0,60.5,"-",6.4,"-",7.0,450,"M56",45.0,"-"]
[null,"BLRF  400# ANSI B16.47-API 605 Size 54\"","BLRF"," 400#","ANSI B16.47-API 605","54\"",1350.0,1701.8,"-",176.3,1470.2,1581.2,28.0,66.5,"-",6.4,"-",7.0,471.6,"M60",48.0,"-"]
[null,"BLRF  400# ANSI B16.47-API 605 Size 56\"","BLRF"," 400#","ANSI B16.47-API 605","56\"",1400.0,1752.6,"-",181.2,1527.0,1632.0,32.0,66.5,"-",6.4,"-",7.0,481.4,"M60",48.0,"-"]
[null,"BLRF  400# ANSI B16.47-API 605 Size 58\"","BLRF"," 400#","ANSI B16.47-API 605","58\"",1450.0,1803.4,"-",184.2,1577.8,1682.8,32.0,66.5,"-",6.4,"-",7.0,487.4,"M60",48.0,"-"]
[null,"BLRF  400# ANSI B16.47-API 605 Size 60\"","BLRF"," 400#","ANSI B16.47-API 605","60\"",1500.0,1886.0,"-",192.1,1635.3,1752.6,32.0,73.2,"-",6.4,"-",7.0,515.2,"M68",54.0,"-"]
[null,"BLRF  600# ANSI B16.47-API 605 Size 26\"","BLRF"," 600#","ANSI B16.47-API 605","26\"",650.0,889.0,"-",117.7,726.9,806.5,28.0,44.5,"-",6.4,"-",7.0,326.4,"M42",34.0,"-"]
[null,"BLRF  600# ANSI B16.47-API 605 Size 28\"","BLRF"," 600#","ANSI B16.47-API 605","28\"",700.0,952.5,"-",122.2,784.4,863.6,28.0,47.8,"-",6.4,"-",7.0,339.4,"M45",36.0,"-"]
[null,"BLRF  600# ANSI B16.47-API 605 Size 30\"","BLRF"," 600#","ANSI B16.47-API 605","30\"",750.0,1022.4,"-",131.9,841.2,927.1,28.0,50.8,"-",6.4,"-",7.0,362.8,"M48",38.0,"-"]
[null,"BLRF  600# ANSI B16.47-API 605 Size 32\"","BLRF"," 600#","ANSI B16.47-API 605","32\"",800.0,1085.9,"-",136.4,895.4,984.3,28.0,53.8,"-",6.4,"-",7.0,371.8,"M48",38.0,"-"]
[null,"BLRF  600# ANSI B16.47-API 605 Size 34\"","BLRF"," 600#","ANSI B16.47-API 605","34\"",850.0,1162.1,"-",147.6,952.5,1054.1,24.0,60.5,"-",6.4,"-",7.0,408.2,"M56",45.0,"-"]
[null,"BLRF  600# ANSI B16.47-API 605 Size 36\"","BLRF"," 600#","ANSI B16.47-API 605","36\"",900.0,1212.9,"-",152.5,1009.7,1104.9,28.0,60.5,"-",6.4,"-",7.0,418,"M56",45.0,"-"]
[null,"BLRF  600# ANSI B16.47-API 605 Size 38\"","BLRF"," 600#","ANSI B16.47-API 605","38\"",950.0,1270.0,"-",158.8,1054.1,1162.1,28.0,60.5,"-",6.4,"-",7.0,430.6,"M56",45.0,"-"]
[null,"BLRF  600# ANSI B16.47-API 605 Size 40\"","BLRF"," 600#","ANSI B16.47-API 605","40\"",1000.0,1320.8,"-",165.2,111.3,1212.9,32.0,60.5,"-",6.4,"-",7.0,443.4,"M56",45.0,"-"]
[null,"BLRF  600# ANSI B16.47-API 605 Size 42\"","BLRF"," 600#","ANSI B16.47-API 605","42\"",1050.0,1403.4,"-",174.5,1168.4,1282.7,28.0,66.5,"-",6.4,"-",7.0,468,"M60",48.0,"-"]
[null,"BLRF  600# ANSI B16.47-API 605 Size 44\"","BLRF"," 600#","ANSI B16.47-API 605","44\"",1100.0,1454.2,"-",179.4,1225.6,1333.5,32.0,66.5,"-",6.4,"-",7.0,477.8,"M60",48.0,"-"]
[null,"BLRF  600# ANSI B16.47-API 605 Size 46\"","BLRF"," 600#","ANSI B16.47-API 605","46\"",1150.0,1511.3,"-",185.7,1276.4,1390.7,32.0,66.5,"-",6.4,"-",7.0,490.4,"M60",48.0,"-"]
[null,"BLRF  600# ANSI B16.47-API 605 Size 48\"","BLRF"," 600#","ANSI B16.47-API 605","48\"",1200.0,1593.9,"-",195.4,1333.5,1460.5,32.0,73.2,"-",6.4,"-",7.0,521.8,"M68",54.0,"-"]
[null,"BLRF  600# ANSI B16.47-API 605 Size 50\"","BLRF"," 600#","ANSI B16.47-API 605","50\"",1250.0,1671.1,"-",203.3,1384.3,1524.0,28.0,79.2,"-",6.4,"-",7.0,545.6,"M72",58.0,"-"]
[null,"BLRF  600# ANSI B16.47-API 605 Size 52\"","BLRF"," 600#","ANSI B16.47-API 605","52\"",1300.0,1720.9,"-",209.6,1435.1,1574.8,32.0,79.2,"-",6.4,"-",7.0,558.2,"M72",58.0,"-"]
[null,"BLRF  600# ANSI B16.47-API 605 Size 54\"","BLRF"," 600#","ANSI B16.47-API 605","54\"",1350.0,1778.0,"-",216.0,1492.3,1632.0,32.0,79.2,"-",6.4,"-",7.0,571,"M72",58.0,"-"]
[null,"BLRF  600# ANSI B16.47-API 605 Size 56\"","BLRF"," 600#","ANSI B16.47-API 605","56\"",1400.0,1854.2,"-",223.8,1543.1,1695.5,32.0,85.9,"-",6.4,"-",7.0,598.6,"M80",64.0,"-"]
[null,"BLRF  600# ANSI B16.47-API 605 Size 58\"","BLRF"," 600#","ANSI B16.47-API 605","58\"",1450.0,1905.0,"-",228.7,1600.2,1746.3,32.0,85.9,"-",6.4,"-",7.0,608.4,"M80",64.0,"-"]
[null,"BLRF  600# ANSI B16.47-API 605 Size 60\"","BLRF"," 600#","ANSI B16.47-API 605","60\"",1500.0,1993.9,"-",239.8,1657.4,1822.5,28.0,91.9,"-",6.4,"-",7.0,638.6,"M85",68.0,"-"]
[null,"BLRF  900# ANSI B16.47-API 605 Size 26\"","BLRF"," 900#","ANSI B16.47-API 605","26\"",650.0,1022.4,"-",141.3,762.0,901.7,20.0,66.5,"-",6.4,"-",7.0,401.6,"M60",48.0,"-"]
[null,"BLRF  900# ANSI B16.47-API 605 Size 28\"","BLRF"," 900#","ANSI B16.47-API 605","28\"",700.0,1104.9,"-",154.0,819.2,971.6,20.0,73.2,"-",6.4,"-",7.0,439,"M68",54.0,"-"]
[null,"BLRF  900# ANSI B16.47-API 605 Size 30\"","BLRF"," 900#","ANSI B16.47-API 605","30\"",750.0,1181.1,"-",161.8,876.3,1035.1,20.0,79.2,"-",6.4,"-",7.0,462.6,"M72",58.0,"-"]
[null,"BLRF  900# ANSI B16.47-API 605 Size 32\"","BLRF"," 900#","ANSI B16.47-API 605","32\"",800.0,1238.3,"-",166.7,927.1,1092.2,20.0,79.2,"-",6.4,"-",7.0,472.4,"M72",58.0,"-"]
[null,"BLRF  900# ANSI B16.47-API 605 Size 34\"","BLRF"," 900#","ANSI B16.47-API 605","34\"",850.0,1314.5,"-",177.9,990.6,1155.7,20.0,85.9,"-",6.4,"-",7.0,506.8,"M80",64.0,"-"]
[null,"BLRF  900# ANSI B16.47-API 605 Size 36\"","BLRF"," 900#","ANSI B16.47-API 605","36\"",900.0,1346.2,"-",179.4,1028.7,1200.2,24.0,79.2,"-",6.4,"-",7.0,497.8,"M72",58.0,"-"]
[null,"BLRF  900# ANSI B16.47-API 605 Size 38\"","BLRF"," 900#","ANSI B16.47-API 605","38\"",950.0,1460.5,"-",196.9,1098.6,1289.1,20.0,91.9,"-",6.4,"-",7.0,552.8,"M85",68.0,"-"]
[null,"BLRF  900# ANSI B16.47-API 605 Size 40\"","BLRF"," 900#","ANSI B16.47-API 605","40\"",1000.0,1511.3,"-",203.3,1162.1,1339.9,24.0,91.9,"-",6.4,"-",7.0,565.6,"M85",68.0,"-"]
[null,"BLRF  900# ANSI B16.47-API 605 Size 42\"","BLRF"," 900#","ANSI B16.47-API 605","42\"",1050.0,1562.1,"-",212.6,1212.9,1390.7,24.0,91.9,"-",6.4,"-",7.0,584.2,"M85",68.0,"-"]
[null,"BLRF  900# ANSI B16.47-API 605 Size 44\"","BLRF"," 900#","ANSI B16.47-API 605","44\"",1100.0,1648.0,"-",220.8,1270.0,1463.5,24.0,98.6,"-",6.4,"-",7.0,608.6,"M90",72.0,"-"]
[null,"BLRF  900# ANSI B16.47-API 605 Size 46\"","BLRF"," 900#","ANSI B16.47-API 605","46\"",1150.0,1733.6,"-",232.0,1333.5,1536.7,24.0,104.6,"-",6.4,"-",7.0,639,"M95",76.0,"-"]
[null,"BLRF  900# ANSI B16.47-API 605 Size 48\"","BLRF"," 900#","ANSI B16.47-API 605","48\"",1200.0,1784.4,"-",239.8,1384.3,1587.5,24.0,104.6,"-",6.4,"-",7.0,654.6,"M95",76.0,"-"]
[null,"BLRF 150# ANSI B16.47-MSS SP-44 Size 12\"","BLRF","150#","ANSI B16.47-MSS SP-44","12\"",300.0,482.6,"-",31.8,381.0,431.8,12.0,25.4,"-",1.6,"-",6.0,{"$f":"(J491+U491+5)*2+R491","v":117.6},"M24",19.0,43.0]
[null,"BLRF 150# ANSI B16.47-MSS SP-44 Size 14\"","BLRF","150#","ANSI B16.47-MSS SP-44","14\"",350.0,533.4,"-",35.1,412.8,476.3,12.0,28.4,"-",1.6,"-",7.0,131.2,"M27",22.0,58.0]
[null,"BLRF 150# ANSI B16.47-MSS SP-44 Size 16\"","BLRF","150#","ANSI B16.47-MSS SP-44","16\"",400.0,596.9,"-",36.6,469.9,539.8,16.0,28.4,"-",1.6,"-",7.0,134.2,"M27",22.0,76.0]
[null,"BLRF 150# ANSI B16.47-MSS SP-44 Size 18\"","BLRF","150#","ANSI B16.47-MSS SP-44","18\"",450.0,635.0,"-",39.6,533.4,577.9,16.0,31.8,"-",1.6,"-",7.0,144.2,"M30",24.0,94.0]
[null,"BLRF 150# ANSI B16.47-MSS SP-44 Size 20\"","BLRF","150#","ANSI B16.47-MSS SP-44","20\"",500.0,698.5,"-",42.9,584.2,635.0,20.0,31.8,"-",1.6,"-",7.0,150.8,"M30",24.0,122.0]
[null,"BLRF 150# ANSI B16.47-MSS SP-44 Size 22\"","BLRF","150#","ANSI B16.47-MSS SP-44","22\"",550.0,749.3,"-",46.0,641.4,692.2,20.0,35.1,"-",1.6,"-",7.0,161,"M33",26.0,154.0]
[null,"BLRF 150# ANSI B16.47-MSS SP-44 Size 24\"","BLRF","150#","ANSI B16.47-MSS SP-44","24\"",600.0,812.8,"-",47.8,692.2,749.3,20.0,35.1,"-",1.6,"-",7.0,164.6,"M33",26.0,185.0]
[null,"BLRF 150# ANSI B16.47-MSS SP-44 Size 26\"","BLRF","150#","ANSI B16.47-MSS SP-44","26\"",650.0,870.0,"-",68.3,749.3,806.5,24.0,35.1,"-",1.6,"-",7.0,205.6,"M33",26.0,306.0]
[null,"BLRF 150# ANSI B16.47-MSS SP-44 Size 28\"","BLRF","150#","ANSI B16.47-MSS SP-44","28\"",700.0,927.1,"-",71.4,800.1,863.6,28.0,35.1,"-",1.6,"-",7.0,211.8,"M33",26.0,363.0]
[null,"BLRF 150# ANSI B16.47-MSS SP-44 Size 30\"","BLRF","150#","ANSI B16.47-MSS SP-44","30\"",750.0,684.2,"-",74.7,857.3,914.4,28.0,35.1,"-",1.6,"-",7.0,214.4,"M33",24.0,430.0]
[null,"BLRF 150# ANSI B16.47-MSS SP-44 Size 32\"","BLRF","150#","ANSI B16.47-MSS SP-44","32\"",800.0,1060.4,"-",80.8,914.4,977.9,28.0,41.1,"-",1.6,"-",7.0,240.6,"M39",31.0,537.0]
[null,"BLRF 150# ANSI B16.47-MSS SP-44 Size 34\"","BLRF","150#","ANSI B16.47-MSS SP-44","34\"",850.0,1111.2,"-",82.6,965.2,1028.7,32.0,41.1,"-",1.6,"-",7.0,244.2,"M39",31.0,600.0]
[null,"BLRF 150# ANSI B16.47-MSS SP-44 Size 36\"","BLRF","150#","ANSI B16.47-MSS SP-44","36\"",900.0,1168.4,"-",90.4,1022.4,1085.9,32.0,41.1,"-",1.6,"-",7.0,259.8,"M39",31.0,730.0]
[null,"BLRF 150# ANSI B16.47-MSS SP-44 Size 38\"","BLRF","150#","ANSI B16.47-MSS SP-44","38\"",950.0,1238.2,"-",87.4,1073.2,1149.4,32.0,41.1,"-",1.6,"-",7.0,253.8,"M39",31.0,792.0]
[null,"BLRF 150# ANSI B16.47-MSS SP-44 Size 40\"","BLRF","150#","ANSI B16.47-MSS SP-44","40\"",1000.0,1289.0,"-",90.4,1124.0,1200.2,36.0,41.1,"-",1.6,"-",7.0,259.8,"M39",31.0,893.0]
[null,"BLRF 150# ANSI B16.47-MSS SP-44 Size 42\"","BLRF","150#","ANSI B16.47-MSS SP-44","42\"",1050.0,1346.2,"-",96.8,1193.8,1257.3,36.0,41.1,"-",1.6,"-",7.0,272.6,"M39",31.0,1044.0]
[null,"BLRF 150# ANSI B16.47-MSS SP-44 Size 44\"","BLRF","150#","ANSI B16.47-MSS SP-44","44\"",1100.0,1403.3,"-",101.6,1244.6,1314.5,40.0,41.1,"-",1.6,"-",7.0,282.2,"M39",31.0,1190.0]
[null,"BLRF 150# ANSI B16.47-MSS SP-44 Size 46\"","BLRF","150#","ANSI B16.47-MSS SP-44","46\"",1150.0,1454.1,"-",103.1,1295.4,1365.3,40.0,41.1,"-",1.6,"-",7.0,285.2,"M39",31.0,1299.0]
[null,"BLRF 150# ANSI B16.47-MSS SP-44 Size 48\"","BLRF","150#","ANSI B16.47-MSS SP-44","48\"",1200.0,1511.3,"-",108.0,1325.9,1422.4,44.0,41.1,"-",1.6,"-",7.0,295,"M39",31.0,1470.0]
[null,"BLRF 150# ANSI B16.47-MSS SP-44 Size 50\"","BLRF","150#","ANSI B16.47-MSS SP-44","50\"",1250.0,1568.4,"-",111.3,1409.7,1479.6,44.0,47.8,"-",1.6,"-",7.0,311.6,"M45",36.0,1615.0]
[null,"BLRF 150# ANSI B16.47-MSS SP-44 Size 52\"","BLRF","150#","ANSI B16.47-MSS SP-44","52\"",1300.0,1625.6,"-",115.8,1460.5,1536.7,44.0,47.8,"-",1.6,"-",7.0,320.6,"M45",36.0,1817.0]
[null,"BLRF 150# ANSI B16.47-MSS SP-44 Size 54\"","BLRF","150#","ANSI B16.47-MSS SP-44","54\"",1350.0,1682.7,"-",120.7,1511.3,1593.9,44.0,47.8,"-",1.6,"-",7.0,330.4,"M45",36.0,2031.0]
[null,"BLRF 150# ANSI B16.47-MSS SP-44 Size 56\"","BLRF","150#","ANSI B16.47-MSS SP-44","56\"",1400.0,1746.2,"-",124.0,1574.8,1651.0,48.0,47.8,"-",1.6,"-",7.0,337,"M45",36.0,2244.0]
[null,"BLRF 150# ANSI B16.47-MSS SP-44 Size 58\"","BLRF","150#","ANSI B16.47-MSS SP-44","58\"",1450.0,1803.4,"-",128.5,1625.6,1708.2,48.0,47.8,"-",1.6,"-",7.0,346,"M45",36.0,2491.0]
[null,"BLRF 150# ANSI B16.47-MSS SP-44 Size 60\"","BLRF","150#","ANSI B16.47-MSS SP-44","60\"",1500.0,1854.2,"-",131.8,1676.4,1759.0,52.0,47.8,"-",1.6,"-",7.0,352.6,"M45",36.0,2697.0]
[null,"BLRF 150# ANSI B16.47-MSS SP-44 Size 12\"","BLRF","150#","ANSI B16.47-MSS SP-44","12\"",300.0,520.7,"-",50.8,"-",450.9,16.0,31.8,"-",1.6,"-",6.0,165.6,"M30",24.0,79.0]
[null,"BLRF 150# ANSI B16.47-MSS SP-44 Size 14\"","BLRF","150#","ANSI B16.47-MSS SP-44","14\"",350.0,584.2,"-",53.8,"-",514.4,20.0,31.8,"-",1.6,"-",7.0,172.6,"M30",24.0,105.0]
[null,"BLRF 150# ANSI B16.47-MSS SP-44 Size 16\"","BLRF","150#","ANSI B16.47-MSS SP-44","16\"",400.0,647.7,"-",57.2,"-",571.5,20.0,35.1,"-",1.6,"-",7.0,183.4,"M33",26.0,137.0]
[null,"BLRF 150# ANSI B16.47-MSS SP-44 Size 18\"","BLRF","150#","ANSI B16.47-MSS SP-44","18\"",450.0,711.2,"-",60.5,"-",628.7,24.0,35.1,"-",1.6,"-",7.0,190,"M33",26.0,175.0]
[null,"BLRF 150# ANSI B16.47-MSS SP-44 Size 20\"","BLRF","150#","ANSI B16.47-MSS SP-44","20\"",500.0,774.7,"-",63.5,"-",685.8,24.0,35.1,"-",1.6,"-",7.0,196,"M33",26.0,221.0]
[null,"BLRF 150# ANSI B16.47-MSS SP-44 Size 22\"","BLRF","150#","ANSI B16.47-MSS SP-44","22\"",550.0,838.2,"-",66.5,"-",743.0,24.0,41.1,"-",1.6,"-",7.0,212,"M39",31.0,280.0]
[null,"BLRF 150# ANSI B16.47-MSS SP-44 Size 24\"","BLRF","150#","ANSI B16.47-MSS SP-44","24\"",600.0,914.4,"-",69.9,"-",812.8,24.0,41.1,"-",1.6,"-",7.0,218.8,"M39",31.0,339.0]
[null,"BLRF 300# ANSI B16.47-MSS SP-44 Size 26\"","BLRF","300#","ANSI B16.47-MSS SP-44","26\"",650.0,971.6,"-",84.1,749.3,876.3,28.0,44.5,"-",1.6,"-",7.0,253.2,"M42",34.0,460.0]
[null,"BLRF 300# ANSI B16.47-MSS SP-44 Size 28\"","BLRF","300#","ANSI B16.47-MSS SP-44","28\"",700.0,1035.1,"-",90.4,800.1,939.8,28.0,44.5,"-",1.6,"-",7.0,265.8,"M42",34.0,566.0]
[null,"BLRF 300# ANSI B16.47-MSS SP-44 Size 30\"","BLRF","300#","ANSI B16.47-MSS SP-44","30\"",750.0,1092.2,"-",95.3,857.2,997.0,28.0,47.8,"-",1.6,"-",7.0,279.6,"M45",36.0,663.0]
[null,"BLRF 300# ANSI B16.47-MSS SP-44 Size 32\"","BLRF","300#","ANSI B16.47-MSS SP-44","32\"",800.0,1149.4,"-",100.1,914.4,1054.1,28.0,50.8,"-",1.6,"-",7.0,293.2,"M48",38.0,770.0]
[null,"BLRF 300# ANSI B16.47-MSS SP-44 Size 34\"","BLRF","300#","ANSI B16.47-MSS SP-44","34\"",850.0,1206.5,"-",104.6,965.2,1104.9,28.0,50.8,"-",1.6,"-",7.0,302.2,"M48",38.0,894.0]
[null,"BLRF 300# ANSI B16.47-MSS SP-44 Size 36\"","BLRF","300#","ANSI B16.47-MSS SP-44","36\"",900.0,1270.0,"-",111.3,1022.3,1168.4,32.0,53.8,"-",1.6,"-",7.0,315.6,"M48",38.0,1040.0]
[null,"BLRF 300# ANSI B16.47-MSS SP-44 Size 38\"","BLRF","300#","ANSI B16.47-MSS SP-44","38\"",950.0,1168.4,"-",108.0,1028.7,1092.2,32.0,41.1,"-",1.6,"-",7.0,295,"M39",31.0,872.0]
[null,"BLRF 300# ANSI B16.47-MSS SP-44 Size 40\"","BLRF","300#","ANSI B16.47-MSS SP-44","40\"",1000.0,1238.3,"-",114.3,1085.8,1155.7,32.0,44.5,"-",1.6,"-",7.0,313.6,"M42",34.0,1035.0]
[null,"BLRF 300# ANSI B16.47-MSS SP-44 Size 42\"","BLRF","300#","ANSI B16.47-MSS SP-44","42\"",1050.0,1289.1,"-",119.1,1136.6,1206.5,32.0,44.5,"-",1.6,"-",7.0,323.2,"M42",34.0,1173.0]
[null,"BLRF 300# ANSI B16.47-MSS SP-44 Size 44\"","BLRF","300#","ANSI B16.47-MSS SP-44","44\"",1100.0,1352.6,"-",124.0,1193.8,1263.7,32.0,47.8,"-",1.6,"-",7.0,337,"M45",36.0,1340.0]
[null,"BLRF 300# ANSI B16.47-MSS SP-44 Size 46\"","BLRF","300#","ANSI B16.47-MSS SP-44","46\"",1150.0,1416.1,"-",128.5,1244.6,1320.8,28.0,50.8,"-",1.6,"-",7.0,350,"M48",38.0,1600.0]
[null,"BLRF 300# ANSI B16.47-MSS SP-44 Size 48\"","BLRF","300#","ANSI B16.47-MSS SP-44","48\"",1200.0,1466.9,"-",133.4,1301.7,1371.6,32.0,50.8,"-",1.6,"-",7.0,359.8,"M48",38.0,1700.0]
[null,"BLRF 300# ANSI B16.47-MSS SP-44 Size 50\"","BLRF","300#","ANSI B16.47-MSS SP-44","50\"",1250.0,1530.4,"-",139.7,1358.9,1428.8,32.0,53.8,"-",1.6,"-",7.0,372.4,"M48",38.0,1936.0]
[null,"BLRF 300# ANSI B16.47-MSS SP-44 Size 52\"","BLRF","300#","ANSI B16.47-MSS SP-44","52\"",1300.0,1581.2,"-",144.5,1409.7,1479.6,32.0,53.8,"-",1.6,"-",7.0,382,"M48",38.0,2143.0]
[null,"BLRF 300# ANSI B16.47-MSS SP-44 Size 54\"","BLRF","300#","ANSI B16.47-MSS SP-44","54\"",1350.0,1657.4,"-",152.4,1466.8,1549.4,28.0,60.5,"-",1.6,"-",7.0,411.8,"M56",45.0,2486.0]
[null,"BLRF 300# ANSI B16.47-MSS SP-44 Size 56\"","BLRF","300#","ANSI B16.47-MSS SP-44","56\"",1400.0,1708.2,"-",153.9,1517.6,1600.2,28.0,60.5,"-",1.6,"-",7.0,414.8,"M56",45.0,2674.0]
[null,"BLRF 300# ANSI B16.47-MSS SP-44 Size 58\"","BLRF","300#","ANSI B16.47-MSS SP-44","58\"",1450.0,1759.0,"-",158.8,1574.8,1651.0,32.0,60.5,"-",1.6,"-",7.0,424.6,"M56",45.0,2913.0]
[null,"BLRF 300# ANSI B16.47-MSS SP-44 Size 60\"","BLRF","300#","ANSI B16.47-MSS SP-44","60\"",1500.0,1809.8,"-",163.6,1625.6,1701.8,32.0,60.5,"-",1.6,"-",7.0,434.2,"M56",45.0,3184.0]
[null,"BLRF 400# ANSI B16.47-MSS SP-44 Size 12\"","BLRF","400#","ANSI B16.47-MSS SP-44","12\"",300.0,323.8,"-",63.6,"-",450.9,16.0,35.1,"-",6.4,"-",6.0,195.2,"M33",26.0,94.0]
[null,"BLRF 400# ANSI B16.47-MSS SP-44 Size 14\"","BLRF","400#","ANSI B16.47-MSS SP-44","14\"",350.0,355.6,"-",66.9,"-",514.4,20.0,35.1,"-",6.4,"-",7.0,202.8,"M33",26.0,124.0]
[null,"BLRF 400# ANSI B16.47-MSS SP-44 Size 16\"","BLRF","400#","ANSI B16.47-MSS SP-44","16\"",400.0,406.4,"-",69.9,"-",571.5,20.0,38.1,"-",6.4,"-",7.0,214.8,"M36",29.0,162.0]
[null,"BLRF 400# ANSI B16.47-MSS SP-44 Size 18\"","BLRF","400#","ANSI B16.47-MSS SP-44","18\"",450.0,457.2,"-",72.9,"-",628.7,24.0,38.1,"-",6.4,"-",7.0,220.8,"M36",29.0,205.0]
[null,"BLRF 400# ANSI B16.47-MSS SP-44 Size 20\"","BLRF","400#","ANSI B16.47-MSS SP-44","20\"",500.0,508.0,"-",76.3,"-",685.8,24.0,41.1,"-",6.4,"-",7.0,231.6,"M39",31.0,254.0]
[null,"BLRF 400# ANSI B16.47-MSS SP-44 Size 22\"","BLRF","400#","ANSI B16.47-MSS SP-44","22\"",550.0,558.8,"-",79.6,"-",743.0,24.0,44.5,"-",6.4,"-",7.0,244.2,"M42",34.0,320.0]
[null,"BLRF 400# ANSI B16.47-MSS SP-44 Size 24\"","BLRF","400#","ANSI B16.47-MSS SP-44","24\"",600.0,609.6,"-",82.6,"-",812.8,24.0,47.8,"-",6.4,"-",7.0,254.2,"M45",36.0,386.0]
[null,"BLRF 400# ANSI B16.47-MSS SP-44 Size 26\"","BLRF","400#","ANSI B16.47-MSS SP-44","26\"",650.0,660.4,"-",105.0,749.3,876.3,28.0,47.8,"-",6.4,"-",7.0,299,"M45",36.0,534.0]
[null,"BLRF 400# ANSI B16.47-MSS SP-44 Size 28\"","BLRF","400#","ANSI B16.47-MSS SP-44","28\"",700.0,711.2,"-",111.0,800.1,939.8,28.0,50.8,"-",6.4,"-",7.0,315,"M48",38.0,645.0]
[null,"BLRF 400# ANSI B16.47-MSS SP-44 Size 30\"","BLRF","400#","ANSI B16.47-MSS SP-44","30\"",750.0,762.0,"-",117.7,857.2,997.0,28.0,53.8,"-",6.4,"-",7.0,328.4,"M48",38.0,760.0]
[null,"BLRF 400# ANSI B16.47-MSS SP-44 Size 32\"","BLRF","400#","ANSI B16.47-MSS SP-44","32\"",800.0,812.8,"-",122.2,914.4,1054.1,28.0,53.8,"-",6.4,"-",7.0,337.4,"M48",38.0,885.0]
[null,"BLRF 400# ANSI B16.47-MSS SP-44 Size 34\"","BLRF","400#","ANSI B16.47-MSS SP-44","34\"",850.0,863.6,"-",128.6,965.2,1104.9,28.0,53.8,"-",6.4,"-",7.0,350.2,"M48",38.0,1035.0]
[null,"BLRF 400# ANSI B16.47-MSS SP-44 Size 36\"","BLRF","400#","ANSI B16.47-MSS SP-44","36\"",900.0,914.4,"-",134.9,1022.3,1168.4,32.0,53.8,"-",6.4,"-",7.0,362.8,"M48",38.0,1205.0]
[null,"BLRF 400# ANSI B16.47-MSS SP-44 Size 38\"","BLRF","400#","ANSI B16.47-MSS SP-44","38\"",950.0,965.2,"-",130.4,1035.0,1117.6,32.0,47.8,"-",6.4,"-",7.0,349.8,"M45",36.0,1055.0]
[null,"BLRF 400# ANSI B16.47-MSS SP-44 Size 40\"","BLRF","400#","ANSI B16.47-MSS SP-44","40\"",1000.0,1016.0,"-",136.4,1092.2,1174.8,32.0,50.8,"-",6.4,"-",7.0,365.8,"M48",38.0,1229.0]
[null,"BLRF 400# ANSI B16.47-MSS SP-44 Size 42\"","BLRF","400#","ANSI B16.47-MSS SP-44","42\"",1050.0,1066.8,"-",139.8,1143.0,1225.6,32.0,50.8,"-",6.4,"-",7.0,372.6,"M48",38.0,1366.0]
[null,"BLRF 400# ANSI B16.47-MSS SP-44 Size 44\"","BLRF","400#","ANSI B16.47-MSS SP-44","44\"",1100.0,1117.6,"-",146.1,1200.1,1282.7,32.0,53.8,"-",6.4,"-",7.0,385.2,"M48",38.0,1569.0]
[null,"BLRF 400# ANSI B16.47-MSS SP-44 Size 46\"","BLRF","400#","ANSI B16.47-MSS SP-44","46\"",1150.0,1168.4,"-",152.5,1257.3,1339.9,36.0,53.8,"-",6.4,"-",7.0,398,"M48",38.0,1776.0]
[null,"BLRF 400# ANSI B16.47-MSS SP-44 Size 48\"","BLRF","400#","ANSI B16.47-MSS SP-44","48\"",1200.0,1219.2,"-",158.8,1308.1,1403.4,28.0,60.5,"-",6.4,"-",7.0,424.6,"M56",45.0,2043.0]
[null,"BLRF 400# ANSI B16.47-MSS SP-44 Size 50\"","BLRF","400#","ANSI B16.47-MSS SP-44","50\"",1250.0,1270.0,"-",165.2,1362.0,1460.5,32.0,60.5,"-",6.4,"-",7.0,437.4,"M56",45.0,2294.0]
[null,"BLRF 400# ANSI B16.47-MSS SP-44 Size 52\"","BLRF","400#","ANSI B16.47-MSS SP-44","52\"",1300.0,1320.8,"-",170.0,1412.8,1511.3,32.0,60.5,"-",6.4,"-",7.0,447,"M56",45.0,2500.0]
[null,"BLRF 400# ANSI B16.47-MSS SP-44 Size 54\"","BLRF","400#","ANSI B16.47-MSS SP-44","54\"",1350.0,1371.6,"-",177.9,1470.0,1581.2,28.0,66.5,"-",6.4,"-",7.0,474.8,"M64",51.0,2900.0]
[null,"BLRF 400# ANSI B16.47-MSS SP-44 Size 56\"","BLRF","400#","ANSI B16.47-MSS SP-44","56\"",1400.0,1422.4,"-",184.7,1527.1,1632.0,32.0,66.5,"-",6.4,"-",7.0,488.4,"M64",51.0,3174.0]
[null,"BLRF 400# ANSI B16.47-MSS SP-44 Size 58\"","BLRF","400#","ANSI B16.47-MSS SP-44","58\"",1450.0,1473.2,"-",187.2,1577.9,1682.8,32.0,66.5,"-",6.4,"-",7.0,493.4,"M64",51.0,3462.0]
[null,"BLRF 400# ANSI B16.47-MSS SP-44 Size 60\"","BLRF","400#","ANSI B16.47-MSS SP-44","60\"",1500.0,1524.0,"-",195.4,1635.1,1752.6,32.0,73.2,"-",6.4,"-",7.0,515.8,"M68",54.0,3940.0]
[null,"BLRF 600# ANSI B16.47-MSS SP-44 Size 12\"","BLRF","600#","ANSI B16.47-MSS SP-44","12\"",300.0,558.8,"-",72.9,"-",489.0,20.0,35.1,"-",6.4,"-",6.0,213.8,"M33",26.0,124.0]
[null,"BLRF 600# ANSI B16.47-MSS SP-44 Size 14\"","BLRF","600#","ANSI B16.47-MSS SP-44","14\"",350.0,603.3,"-",76.3,"-",527.1,20.0,38.1,"-",6.4,"-",7.0,227.6,"M36",29.0,151.0]
[null,"BLRF 600# ANSI B16.47-MSS SP-44 Size 16\"","BLRF","600#","ANSI B16.47-MSS SP-44","16\"",400.0,685.8,"-",82.6,"-",603.3,20.0,41.1,"-",6.4,"-",7.0,244.2,"M39",31.0,214.0]
[null,"BLRF 600# ANSI B16.47-MSS SP-44 Size 18\"","BLRF","600#","ANSI B16.47-MSS SP-44","18\"",450.0,743.0,"-",89.0,"-",654.1,20.0,44.5,"-",6.4,"-",7.0,263,"M42",34.0,272.0]
[null,"BLRF 600# ANSI B16.47-MSS SP-44 Size 20\"","BLRF","600#","ANSI B16.47-MSS SP-44","20\"",500.0,812.8,"-",95.3,"-",723.9,24.0,44.5,"-",6.4,"-",7.0,275.6,"M42",34.0,349.0]
[null,"BLRF 600# ANSI B16.47-MSS SP-44 Size 22\"","BLRF","600#","ANSI B16.47-MSS SP-44","22\"",550.0,870.0,"-",101.7,"-",777.7,24.0,47.8,"-",6.4,"-",7.0,292.4,"M45",36.0,440.0]
[null,"BLRF 600# ANSI B16.47-MSS SP-44 Size 24\"","BLRF","600#","ANSI B16.47-MSS SP-44","24\"",600.0,936.453333333334,"-",107.04,"-",837.653333333333,24.5333333333333,50.4599999999999,"-",6.4,"-",7.33333333333333,308.3466667,"M33",38.4666666666666,533.0]
[null,"BLRF 600# ANSI B16.47-MSS SP-44 Size 26\"","BLRF","600#","ANSI B16.47-MSS SP-44","26\"",650.0,1016.0,"-",131.9,749.3,914.4,28.0,50.8,"-",6.4,"-",7.0,356.8,"M48",38.0,740.0]
[null,"BLRF 600# ANSI B16.47-MSS SP-44 Size 28\"","BLRF","600#","ANSI B16.47-MSS SP-44","28\"",700.0,1073.2,"-",138.2,800.1,965.2,28.0,53.8,"-",6.4,"-",7.0,369.4,"M48",38.0,869.0]
[null,"BLRF 600# ANSI B16.47-MSS SP-44 Size 30\"","BLRF","600#","ANSI B16.47-MSS SP-44","30\"",750.0,1130.3,"-",140.1,857.2,1022.4,28.0,53.8,"-",6.4,"-",7.0,373.2,"M48",38.0,1030.0]
[null,"BLRF 600# ANSI B16.47-MSS SP-44 Size 32\"","BLRF","600#","ANSI B16.47-MSS SP-44","32\"",800.0,1193.8,"-",154.0,914.4,1079.5,28.0,60.5,"-",6.4,"-",7.0,415,"M56",45.0,1204.0]
[null,"BLRF 600# ANSI B16.47-MSS SP-44 Size 34\"","BLRF","600#","ANSI B16.47-MSS SP-44","34\"",850.0,1244.6,"-",160.3,965.2,1130.3,28.0,60.5,"-",6.4,"-",7.0,427.6,"M56",45.0,1371.0]
[null,"BLRF 600# ANSI B16.47-MSS SP-44 Size 36\"","BLRF","600#","ANSI B16.47-MSS SP-44","36\"",900.0,1314.5,"-",168.5,1022.3,1193.8,28.0,66.5,"-",6.4,"-",7.0,450,"M60",48.0,1600.0]
[null,"BLRF 600# ANSI B16.47-MSS SP-44 Size 38\"","BLRF","600#","ANSI B16.47-MSS SP-44","38\"",950.0,1270.0,"-",161.8,1054.1,1162.1,28.0,60.5,"-",6.4,"-",7.0,430.6,"M56",45.0,1447.0]
[null,"BLRF 600# ANSI B16.47-MSS SP-44 Size 40\"","BLRF","600#","ANSI B16.47-MSS SP-44","40\"",1000.0,1320.8,"-",168.5,1111.2,1212.9,32.0,60.5,"-",6.4,"-",7.0,444,"M56",45.0,1620.0]
[null,"BLRF 600# ANSI B16.47-MSS SP-44 Size 42\"","BLRF","600#","ANSI B16.47-MSS SP-44","42\"",1050.0,1403.4,"-",177.9,1168.4,1282.7,28.0,66.5,"-",6.4,"-",7.0,468.8,"M60",48.0,1948.0]
[null,"BLRF 600# ANSI B16.47-MSS SP-44 Size 44\"","BLRF","600#","ANSI B16.47-MSS SP-44","44\"",1100.0,1454.2,"-",184.2,1225.5,1333.5,32.0,66.5,"-",6.4,"-",7.0,481.4,"M60",48.0,2100.0]
[null,"BLRF 600# ANSI B16.47-MSS SP-44 Size 46\"","BLRF","600#","ANSI B16.47-MSS SP-44","46\"",1150.0,1511.3,"-",192.1,1273.3,1390.7,32.0,66.5,"-",6.4,"-",7.0,497.2,"M60",48.0,2450.0]
[null,"BLRF 600# ANSI B16.47-MSS SP-44 Size 48\"","BLRF","600#","ANSI B16.47-MSS SP-44","48\"",1200.0,1593.9,"-",201.7,1333.5,1460.5,32.0,73.2,"-",6.4,"-",7.0,530.4,"M68",55.0,2850.0]
[null,"BLRF 600# ANSI B16.47-MSS SP-44 Size 50\"","BLRF","600#","ANSI B16.47-MSS SP-44","50\"",1250.0,1670.1,"-",209.6,1384.3,1524.0,28.0,79.2,"-",6.4,"-",7.0,556.2,"M75",60.0,3233.0]
[null,"BLRF 600# ANSI B16.47-MSS SP-44 Size 52\"","BLRF","600#","ANSI B16.47-MSS SP-44","52\"",1300.0,1720.9,"-",216.0,1435.1,1574.8,32.0,79.2,"-",6.4,"-",7.0,569,"M75",60.0,3570.0]
[null,"BLRF 600# ANSI B16.47-MSS SP-44 Size 54\"","BLRF","600#","ANSI B16.47-MSS SP-44","54\"",1350.0,1778.0,"-",223.8,1492.2,1632.0,32.0,79.2,"-",6.4,"-",7.0,584.6,"M75",60.0,3968.0]
[null,"BLRF 600# ANSI B16.47-MSS SP-44 Size 56\"","BLRF","600#","ANSI B16.47-MSS SP-44","56\"",1400.0,1854.2,"-",232.0,1543.0,1695.5,32.0,85.9,"-",6.4,"-",7.0,609,"M80",64.0,4450.0]
[null,"BLRF 600# ANSI B16.47-MSS SP-44 Size 58\"","BLRF","600#","ANSI B16.47-MSS SP-44","58\"",1450.0,1905.0,"-",238.0,1600.2,1746.3,32.0,85.9,"-",6.4,"-",7.0,621,"M80",64.0,4850.0]
[null,"BLRF 600# ANSI B16.47-MSS SP-44 Size 60\"","BLRF","600#","ANSI B16.47-MSS SP-44","60\"",1500.0,1993.9,"-",249.2,1657.3,1822.5,28.0,91.9,"-",6.4,"-",7.0,651.4,"M85",68.0,5588.0]
[null,"BLRF 900# ANSI B16.47-MSS SP-44 Size 12\"","BLRF","900#","ANSI B16.47-MSS SP-44","12\"",300.0,609.6,"-",85.6,"-",533.4,20.0,38.1,"-",6.4,"-",7.0,246.2,"M36",29.0,173.0]
[null,"BLRF 900# ANSI B16.47-MSS SP-44 Size 14\"","BLRF","900#","ANSI B16.47-MSS SP-44","14\"",350.0,641.4,"-",92.3,"-",558.8,20.0,41.1,"-",6.4,"-",7.0,263.6,"M39",31.0,206.0]
[null,"BLRF 900# ANSI B16.47-MSS SP-44 Size 16\"","BLRF","900#","ANSI B16.47-MSS SP-44","16\"",400.0,704.9,"-",95.3,"-",616.0,20.0,44.5,"-",6.4,"-",7.0,275.6,"M42",34.0,259.0]
[null,"BLRF 900# ANSI B16.47-MSS SP-44 Size 18\"","BLRF","900#","ANSI B16.47-MSS SP-44","18\"",450.0,787.4,"-",108.0,"-",685.8,20.0,50.8,"-",6.4,"-",7.0,309,"M48",38.0,367.0]
[null,"BLRF 900# ANSI B16.47-MSS SP-44 Size 20\"","BLRF","900#","ANSI B16.47-MSS SP-44","20\"",500.0,857.3,"-",114.4,"-",749.3,20.0,53.8,"-",6.4,"-",7.0,321.8,"M48",38.0,463.0]
[null,"BLRF 900# ANSI B16.47-MSS SP-44 Size 24\"","BLRF","900#","ANSI B16.47-MSS SP-44","24\"",600.0,1041.4,"-",146.1,"-",901.7,20.0,66.5,"-",6.4,"-",7.0,411.2,"M64",51.0,876.0]
[null,"BLRF 900# ANSI B16.47-MSS SP-44 Size 26\"","BLRF","900#","ANSI B16.47-MSS SP-44","26\"",650.0,1085.9,"-",166.7,749.3,952.5,20.0,73.2,"-",6.4,"-",7.0,460.4,"M68",55.0,1060.0]
[null,"BLRF 900# ANSI B16.47-MSS SP-44 Size 28\"","BLRF","900#","ANSI B16.47-MSS SP-44","28\"",700.0,1168.4,"-",177.9,800.1,1022.4,20.0,79.2,"-",6.4,"-",7.0,494.8,"M76",61.0,1306.0]
[null,"BLRF 900# ANSI B16.47-MSS SP-44 Size 30\"","BLRF","900#","ANSI B16.47-MSS SP-44","30\"",750.0,1231.9,"-",188.8,857.2,1085.9,20.0,79.2,"-",6.4,"-",7.0,516.6,"M76",61.0,1565.0]
[null,"BLRF 900# ANSI B16.47-MSS SP-44 Size 32\"","BLRF","900#","ANSI B16.47-MSS SP-44","32\"",800.0,1314.5,"-",199.9,914.4,1155.7,20.0,85.9,"-",6.4,"-",7.0,544.8,"M80",64.0,1885.0]
[null,"BLRF 900# ANSI B16.47-MSS SP-44 Size 34\"","BLRF","900#","ANSI B16.47-MSS SP-44","34\"",850.0,1397.0,"-",211.1,965.2,1225.6,20.0,91.9,"-",6.4,"-",7.0,575.2,"M85",68.0,2250.0]
[null,"BLRF 900# ANSI B16.47-MSS SP-44 Size 36\"","BLRF","900#","ANSI B16.47-MSS SP-44","36\"",900.0,1460.5,"-",220.8,1022.3,1289.1,20.0,91.9,"-",6.4,"-",7.0,594.6,"M85",68.0,2595.0]
[null,"BLRF 900# ANSI B16.47-MSS SP-44 Size 38\"","BLRF","900#","ANSI B16.47-MSS SP-44","38\"",950.0,1460.5,"-",222.3,1098.5,1289.1,20.0,91.9,"-",6.4,"-",7.0,597.6,"M85",68.0,2610.0]
[null,"BLRF 900# ANSI B16.47-MSS SP-44 Size 40\"","BLRF","900#","ANSI B16.47-MSS SP-44","40\"",1000.0,1511.3,"-",230.2,1162.0,1339.9,24.0,91.9,"-",6.4,"-",7.0,613.4,"M85",68.0,2870.0]
[null,"BLRF 900# ANSI B16.47-MSS SP-44 Size 42\"","BLRF","900#","ANSI B16.47-MSS SP-44","42\"",1050.0,1562.1,"-",238.0,1212.8,1390.7,24.0,91.9,"-",6.4,"-",7.0,629,"M85",68.0,3195.0]
[null,"BLRF 900# ANSI B16.47-MSS SP-44 Size 44\"","BLRF","900#","ANSI B16.47-MSS SP-44","44\"",1100.0,1648.0,"-",249.2,1270.0,1463.5,24.0,98.6,"-",6.4,"-",7.0,667.4,"M95",76.0,3720.0]
[null,"BLRF 900# ANSI B16.47-MSS SP-44 Size 46\"","BLRF","900#","ANSI B16.47-MSS SP-44","46\"",1150.0,1733.6,"-",261.9,1333.5,1536.7,24.0,104.6,"-",6.4,"-",7.0,700.8,"M100",80.0,4579.0]
[null,"BLRF 900# ANSI B16.47-MSS SP-44 Size 48\"","BLRF","900#","ANSI B16.47-MSS SP-44","48\"",1200.0,1784.4,"-",270.1,1384.3,1587.5,24.0,104.6,"-",6.4,"-",7.0,717.2,"M100",80.0,4730.0]
[null,"SORF 150# BS 3293 Size 26\"","SORF","150#","BS 3293","26\"",650.0,870.0,85.7,50.8,743.0,806.5,24.0,34.9,723.9,1.6,"-",7.0,166.6,"M30",24.0,107.0]
[null,"SORF 150# BS 3293 Size 28\"","SORF","150#","BS 3293","28\"",700.0,927.1,87.3,52.4,793.8,863.6,28.0,34.9,781.1,1.6,"-",7.0,169.8,"M30",24.0,122.0]
[null,"SORF 150# BS 3293 Size 30\"","SORF","150#","BS 3293","30\"",750.0,984.3,88.9,54.0,857.3,914.4,28.0,34.9,831.9,1.6,"-",7.0,173,"M30",24.0,138.0]
[null,"SORF 150# BS 3293 Size 32\"","SORF","150#","BS 3293","32\"",800.0,1060.5,92.1,57.2,908.1,977.9,28.0,41.3,889.0,1.6,"-",7.0,189.4,"M39",29.0,170.0]
[null,"SORF 150# BS 3293 Size 34\"","SORF","150#","BS 3293","34\"",850.0,1111.3,93.7,58.8,958.8,1028.7,32.0,41.3,939.8,1.6,"-",7.0,192.6,"M39",29.0,184.0]
[null,"SORF 150# BS 3293 Size 36\"","SORF","150#","BS 3293","36\"",900.0,1168.4,95.3,60.3,1022.4,1085.9,32.0,41.3,997.0,1.6,"-",7.0,195.6,"M39",29.0,211.0]
[null,"SORF 150# BS 3293 Size 38\"","SORF","150#","BS 3293","38\"",950.0,1238.3,95.3,60.3,1073.2,1149.4,32.0,41.3,1060.5,1.6,"-",7.0,195.6,"M39",29.0,249.0]
[null,"SORF 150# BS 3293 Size 40\"","SORF","150#","BS 3293","40\"",1000.0,1289.1,98.4,63.5,1124.0,1200.2,36.0,41.3,1111.3,1.6,"-",7.0,202,"M39",29.0,272.0]
[null,"SORF 150# BS 3293 Size 42\"","SORF","150#","BS 3293","42\"",1050.0,1346.2,101.6,66.7,1193.8,1257.3,36.0,41.3,1168.4,1.6,"-",7.0,208.4,"M39",29.0,313.0]
[null,"SORF 150# BS 3293 Size 44\"","SORF","150#","BS 3293","44\"",1100.0,1403.4,101.6,66.7,1244.6,1314.5,40.0,41.3,1219.2,1.6,"-",7.0,208.4,"M39",29.0,331.0]
[null,"SORF 150# BS 3293 Size 46\"","SORF","150#","BS 3293","46\"",1150.0,1454.2,103.3,68.3,1295.4,1365.3,40.0,41.3,1270.0,1.6,"-",7.0,211.6,"M39",29.0,349.0]
[null,"SORF 150# BS 3293 Size 48\"","SORF","150#","BS 3293","48\"",1200.0,1511.3,104.8,69.9,1358.9,1422.4,44.0,41.3,1327.2,1.6,"-",7.0,214.8,"M39",29.0,381.0]
[null,"SORF 300# BS 3293 Size 26\"","SORF","300#","BS 3293","26\"",650.0,971.6,184.2,79.4,749.3,876.3,28.0,44.5,720.7,1.6,"-",7.0,243.8,"M42",34.0,251.0]
[null,"SORF 300# BS 3293 Size 28\"","SORF","300#","BS 3293","28\"",700.0,1035.1,196.9,85.7,800.1,939.8,28.0,44.5,774.7,1.6,"-",7.0,256.4,"M42",34.0,313.0]
[null,"SORF 300# BS 3293 Size 30\"","SORF","300#","BS 3293","30\"",750.0,1092.2,209.6,92.1,857.3,997.0,28.0,47.6,827.1,1.6,"-",7.0,273.2,"M45",36.0,354.0]
[null,"SORF 300# BS 3293 Size 32\"","SORF","300#","BS 3293","32\"",800.0,1149.4,222.3,98.4,914.4,1054.1,28.0,50.8,881.1,1.6,"-",7.0,289.8,"M48",38.0,395.0]
[null,"SORF 300# BS 3293 Size 34\"","SORF","300#","BS 3293","34\"",850.0,1206.5,231.8,101.6,965.2,1104.9,28.0,50.8,936.6,1.6,"-",7.0,296.2,"M48",38.0,460.0]
[null,"SORF 300# BS 3293 Size 36\"","SORF","300#","BS 3293","36\"",900.0,1270.0,241.3,104.8,1022.4,1168.4,32.0,54.0,990.6,1.6,"-",7.0,310.6,"M52",42.0,513.0]
[null,"SORF 400# BS 3293 Size 26\"","SORF","400#","BS 3293","26\"",650.0,971.6,200.1,95.3,749.3,876.3,28.0,47.6,727.1,6.4,"-",7.0,279.6,"M45",36.0,295.0]
[null,"SORF 400# BS 3293 Size 28\"","SORF","400#","BS 3293","28\"",700.0,1035.1,212.8,101.7,800.1,939.8,28.0,50.8,782.7,6.4,"-",7.0,296.4,"M48",38.0,354.0]
[null,"SORF 400# BS 3293 Size 30\"","SORF","400#","BS 3293","30\"",750.0,1092.2,225.5,108.0,857.3,997.0,28.0,54.0,836.6,6.4,"-",7.0,317,"M52",42.0,408.0]
[null,"SORF 400# BS 3293 Size 32\"","SORF","400#","BS 3293","32\"",800.0,1149.4,238.2,114.4,914.4,1054.1,28.0,54.0,889.0,6.4,"-",7.0,329.8,"M52",42.0,465.0]
[null,"SORF 400# BS 3293 Size 34\"","SORF","400#","BS 3293","34\"",850.0,1206.5,248.1,117.5,965.2,1104.9,28.0,54.0,944.6,6.4,"-",7.0,336,"M52",42.0,522.0]
[null,"SORF 400# BS 3293 Size 36\"","SORF","400#","BS 3293","36\"",900.0,1270.0,257.2,120.8,1022.4,1168.4,32.0,54.0,1000.1,6.4,"-",7.0,342.6,"M52",42.0,601.0]
[null,"SORF 600# BS 3293 Size 26\"","SORF","600#","BS 3293","26\"",650.0,1016.0,228.7,114.4,749.3,914.4,28.0,50.8,747.7,6.4,"-",7.0,321.8,"M48",38.0,408.0]
[null,"SORF 600# BS 3293 Size 28\"","SORF","600#","BS 3293","28\"",700.0,1073.2,241.4,117.5,800.1,965.2,28.0,54.0,803.3,6.4,"-",7.0,336,"M52",42.0,472.0]
[null,"SORF 600# BS 3293 Size 30\"","SORF","600#","BS 3293","30\"",750.0,1130.3,254.0,120.7,857.3,1022.4,28.0,54.0,862.0,6.4,"-",7.0,342.4,"M52",42.0,526.0]
[null,"SORF 600# BS 3293 Size 32\"","SORF","600#","BS 3293","32\"",800.0,1193.8,266.8,123.9,914.4,1079.5,28.0,60.3,917.6,6.4,"-",7.0,354.8,"M56",45.0,605.0]
[null,"SORF 600# BS 3293 Size 34\"","SORF","600#","BS 3293","34\"",850.0,1244.6,276.3,127.1,965.2,1130.3,28.0,60.3,973.1,6.4,"-",7.0,361.2,"M56",45.0,652.0]
[null,"SORF 600# BS 3293 Size 36\"","SORF","600#","BS 3293","36\"",900.0,1314.5,289.0,130.2,1022.4,1193.8,28.0,66.7,1031.9,6.4,"-",7.0,379.4,"M64",51.0,744.0]
[null,{"$f":"CONCATENATE(C639,$C$2,D639,$C$2,E639,$C$2,$F$1,$C$2,G639)","v":"SO PN 6 DIN 2573 Size 10"},"SO","PN 6","DIN 2573","1/4\"",10.0,75.0,"-",12.0,"-",50.0,4.0,11.0,"-","-",17.7,3.0,53,"M10",8.0,0.36]
[null,{"$f":"CONCATENATE(C640,$C$2,D640,$C$2,E640,$C$2,$F$1,$C$2,$G$2,$C$2,G640)","v":"SO PN 6 DIN 2573 Size DN 15"},"SO","PN 6","DIN 2573","1/2\"",15.0,80.0,"-",12.0,"-",55.0,4.0,11.0,"-","-",22.0,3.0,53,"M10",8.0,0.41]
[null,"SO PN 6 DIN 2573 Size DN 20","SO","PN 6","DIN 2573","3/4\"",20.0,90.0,"-",14.0,"-",65.0,4.0,11.0,"-","-",27.6,3.0,57,"M10",8.0,0.6]
[null,"SO PN 6 DIN 2573 Size DN 25","SO","PN 6","DIN 2573","1\"",25.0,100.0,"-",14.0,"-",75.0,4.0,11.0,"-","-",34.4,3.0,57,"M10",8.0,0.74]
[null,"SO PN 6 DIN 2573 Size DN 32","SO","PN 6","DIN 2573","1¼\"",32.0,120.0,"-",16.0,"-",90.0,4.0,14.0,"-","-",43.1,3.0,65,"M12",10.0,1.19]
[null,"SO PN 6 DIN 2573 Size DN 40","SO","PN 6","DIN 2573","1½\"",40.0,130.0,"-",16.0,"-",100.0,4.0,14.0,"-","-",49.0,3.0,65,"M12",10.0,1.39]
[null,"SO PN 6 DIN 2573 Size DN 50","SO","PN 6","DIN 2573","2\"",50.0,140.0,"-",16.0,"-",110.0,4.0,14.0,"-","-",61.1,4.0,66,"M12",10.0,1.53]
[null,"SO PN 6 DIN 2573 Size DN 65","SO","PN 6","DIN 2573","2½\"",65.0,160.0,"-",16.0,"-",130.0,4.0,14.0,"-","-",77.1,4.0,66,"M12",10.0,1.89]
[null,"SO PN 6 DIN 2573 Size DN 80","SO","PN 6","DIN 2573","3\"",80.0,190.0,"-",18.0,"-",150.0,4.0,18.0,"-","-",90.3,4.0,76,"M16",13.0,2.98]
[null,"SO PN 6 DIN 2573 Size DN 100","SO","PN 6","DIN 2573","4\"",100.0,210.0,"-",18.0,"-",170.0,4.0,18.0,"-","-",115.9,5.0,77,"M16",13.0,3.46]
[null,"SO PN 6 DIN 2573 Size DN 125","SO","PN 6","DIN 2573","5\"",125.0,240.0,"-",20.0,"-",200.0,8.0,18.0,"-","-",141.6,5.0,81,"M16",13.0,4.6]
[null,"SO PN 6 DIN 2573 Size DN 150","SO","PN 6","DIN 2573","6\"",150.0,265.0,"-",20.0,"-",225.0,8.0,18.0,"-","-",170.5,6.0,82,"M16",13.0,5.22]
[null,"SO PN 6 DIN 2573 Size DN 200","SO","PN 6","DIN 2573","8\"",200.0,320.0,"-",22.0,"-",280.0,8.0,18.0,"-","-",221.8,6.0,86,"M16",13.0,7.15]
[null,"SO PN 6 DIN 2573 Size DN 250","SO","PN 6","DIN 2573","10\"",250.0,375.0,"-",24.0,"-",335.0,12.0,18.0,"-","-",276.2,6.0,90,"M16",13.0,9.61]
[null,"SO PN 6 DIN 2573 Size DN 300","SO","PN 6","DIN 2573","12\"",300.0,440.0,"-",24.0,"-",395.0,12.0,22.0,"-","-",327.6,6.0,96,"M20",16.0,12.6]
[null,"SO PN 6 DIN 2573 Size DN 350","SO","PN 6","DIN 2573","14\"",350.0,490.0,"-",26.0,"-",445.0,12.0,22.0,"-","-",372.2,7.0,101,"M20",16.0,15.6]
[null,"SO PN 6 DIN 2573 Size DN 400","SO","PN 6","DIN 2573","16\"",400.0,540.0,"-",28.0,"-",495.0,16.0,22.0,"-","-",423.7,7.0,105,"M20",16.0,18.4]
[null,"SO PN 6 DIN 2573 Size DN 450","SO","PN 6","DIN 2573","18\"",450.0,595.0,"-",30.0,"-",550.0,16.0,22.0,"-","-",462.3,7.0,109,"M20",16.0,21.4]
[null,"SO PN 6 DIN 2573 Size DN 500","SO","PN 6","DIN 2573","20\"",500.0,645.0,"-",30.0,"-",600.0,20.0,22.0,"-","-",513.6,7.0,109,"M20",16.0,24.6]
[null,"SO PN 10 DIN 2576 Size DN 10","SO","PN 10","DIN 2576","1/4\"",10.0,90.0,"-",14.0,"-",60.0,4.0,14.0,"-","-",17.7,3.0,61,"M12",10.0,0.6]
[null,"SO PN 10 DIN 2576 Size DN 15","SO","PN 10","DIN 2576","1/2\"",15.0,95.0,"-",14.0,"-",65.0,4.0,14.0,"-","-",22.0,3.0,61,"M12",10.0,0.67]
[null,"SO PN 10 DIN 2576 Size DN 20","SO","PN 10","DIN 2576","3/4\"",20.0,105.0,"-",16.0,"-",75.0,4.0,14.0,"-","-",27.6,3.0,65,"M12",10.0,0.94]
[null,"SO PN 10 DIN 2576 Size DN 25","SO","PN 10","DIN 2576","1\"",25.0,115.0,"-",16.0,"-",85.0,4.0,14.0,"-","-",34.4,3.0,65,"M12",10.0,1.11]
[null,"SO PN 10 DIN 2576 Size DN 32","SO","PN 10","DIN 2576","1¼\"",32.0,140.0,"-",16.0,"-",100.0,4.0,18.0,"-","-",43.1,3.0,71,"M16",13.0,1.62]
[null,"SO PN 10 DIN 2576 Size DN 40","SO","PN 10","DIN 2576","1½\"",40.0,150.0,"-",16.0,"-",110.0,4.0,18.0,"-","-",49.0,3.0,71,"M16",13.0,1.86]
[null,"SO PN 10 DIN 2576 Size DN 50","SO","PN 10","DIN 2576","2\"",50.0,165.0,"-",18.0,"-",125.0,4.0,18.0,"-","-",61.1,4.0,76,"M16",13.0,2.47]
[null,"SO PN 10 DIN 2576 Size DN 65","SO","PN 10","DIN 2576","2½\"",65.0,185.0,"-",18.0,"-",145.0,4.0,18.0,"-","-",77.1,4.0,76,"M16",13.0,3.0]
[null,"SO PN 10 DIN 2576 Size DN 80","SO","PN 10","DIN 2576","3\"",80.0,200.0,"-",20.0,"-",160.0,8.0,18.0,"-","-",90.3,4.0,80,"M16",13.0,3.79]
[null,"SO PN 10 DIN 2576 Size DN 100","SO","PN 10","DIN 2576","4\"",100.0,220.0,"-",20.0,"-",180.0,8.0,18.0,"-","-",115.9,5.0,81,"M16",13.0,4.03]
[null,"SO PN 10 DIN 2576 Size DN 125","SO","PN 10","DIN 2576","5\"",125.0,250.0,"-",22.0,"-",210.0,8.0,18.0,"-","-",141.6,5.0,85,"M16",13.0,5.46]
[null,"SO PN 10 DIN 2576 Size DN 150","SO","PN 10","DIN 2576","6\"",150.0,285.0,"-",22.0,"-",240.0,8.0,22.0,"-","-",170.5,6.0,92,"M20",16.0,6.57]
[null,"SO PN 10 DIN 2576 Size DN 175","SO","PN 10","DIN 2576","7\"",175.0,315.0,"-",24.0,"-",270.0,8.0,22.0,"-","-",196.1,6.0,96,"M20",16.0,8.45]
[null,"SO PN 10 DIN 2576 Size DN 200","SO","PN 10","DIN 2576","8\"",200.0,340.0,"-",24.0,"-",295.0,8.0,22.0,"-","-",221.8,6.0,96,"M20",16.0,9.31]
[null,"SO PN 10 DIN 2576 Size DN 250","SO","PN 10","DIN 2576","10\"",250.0,395.0,"-",26.0,"-",350.0,12.0,22.0,"-","-",276.2,6.0,100,"M20",16.0,11.9]
[null,"SO PN 10 DIN 2576 Size DN 300","SO","PN 10","DIN 2576","12\"",300.0,445.0,"-",26.0,"-",400.0,12.0,22.0,"-","-",327.6,6.0,100,"M20",16.0,13.8]
[null,"SO PN 10 DIN 2576 Size DN 350","SO","PN 10","DIN 2576","14\"",350.0,505.0,"-",28.0,"-",460.0,16.0,22.0,"-","-",372.2,7.0,105,"M20",16.0,19.0]
[null,"SO PN 10 DIN 2576 Size DN 400","SO","PN 10","DIN 2576","16\"",400.0,565.0,"-",32.0,"-",515.0,16.0,26.0,"-","-",423.7,7.0,119,"M24",19.0,25.9]
[null,"SO PN 10 DIN 2576 Size DN 450","SO","PN 10","DIN 2576","18\"",450.0,615.0,"-",38.0,"-",565.0,20.0,26.0,"-","-",462.3,7.0,131,"M24",19.0,35.6]
[null,"SO PN 10 DIN 2576 Size DN 500","SO","PN 10","DIN 2576","20\"",500.0,670.0,"-",38.0,"-",620.0,20.0,26.0,"-","-",513.6,7.0,131,"M24",19.0,41.1]
[null,"SO PN 6 DIN 2641 Size DN 15","SO","PN 6","DIN 2641","1/2\"",15.0,80.0,"-",10.0,"-",55.0,4.0,11.5,"-","-",24.0,3.0,49,"M10",8.0,"-"]
[null,"SO PN 6 DIN 2641 Size DN 20","SO","PN 6","DIN 2641","3/4\"",20.0,90.0,"-",10.0,"-",65.0,4.0,11.5,"-","-",30.0,3.0,49,"M10",8.0,"-"]
[null,"SO PN 6 DIN 2641 Size DN 25","SO","PN 6","DIN 2641","1\"",25.0,100.0,"-",12.0,"-",75.0,4.0,11.5,"-","-",36.0,3.0,53,"M10",8.0,"-"]
[null,"SO PN 6 DIN 2641 Size DN 32","SO","PN 6","DIN 2641","1¼\"",32.0,120.0,"-",12.0,"-",90.0,4.0,14.0,"-","-",46.0,3.0,57,"M12",10.0,"-"]
[null,"SO PN 6 DIN 2641 Size DN 40","SO","PN 6","DIN 2641","1½\"",40.0,130.0,"-",12.0,"-",100.0,4.0,14.0,"-","-",54.0,3.0,57,"M12",10.0,"-"]
[null,"SO PN 6 DIN 2641 Size DN 50","SO","PN 6","DIN 2641","2\"",50.0,140.0,"-",12.0,"-",110.0,4.0,14.0,"-","-",65.0,4.0,58,"M12",10.0,"-"]
[null,"SO PN 6 DIN 2641 Size DN 65","SO","PN 6","DIN 2641","2½\"",65.0,160.0,"-",12.0,"-",130.0,4.0,14.0,"-","-",81.0,4.0,58,"M12",10.0,"-"]
[null,"SO PN 6 DIN 2641 Size DN 80","SO","PN 6","DIN 2641","3\"",80.0,190.0,"-",14.0,"-",150.0,4.0,18.0,"-","-",94.0,4.0,68,"M16",13.0,"-"]
[null,"SO PN 6 DIN 2641 Size DN 100","SO","PN 6","DIN 2641","4\"",100.0,210.0,"-",14.0,"-",170.0,4.0,18.0,"-","-",119.0,5.0,69,"M16",13.0,"-"]
[null,"SO PN 6 DIN 2641 Size DN 125","SO","PN 6","DIN 2641","5\"",125.0,240.0,"-",14.0,"-",200.0,8.0,18.0,"-","-",145.0,5.0,69,"M16",13.0,"-"]
[null,"SO PN 6 DIN 2641 Size DN 150","SO","PN 6","DIN 2641","6\"",150.0,265.0,"-",14.0,"-",225.0,8.0,18.0,"-","-",173.0,6.0,70,"M16",13.0,"-"]
[null,"SO PN 6 DIN 2641 Size DN 200","SO","PN 6","DIN 2641","8\"",200.0,320.0,"-",16.0,"-",280.0,8.0,18.0,"-","-",225.0,6.0,74,"M16",13.0,"-"]
[null,"SO PN 6 DIN 2641 Size DN 250","SO","PN 6","DIN 2641","10\"",250.0,375.0,"-",20.0,"-",335.0,12.0,18.0,"-","-",279.0,6.0,82,"M16",13.0,"-"]
[null,"SO PN 6 DIN 2641 Size DN 300","SO","PN 6","DIN 2641","12\"",300.0,440.0,"-",24.0,"-",395.0,12.0,23.0,"-","-",329.0,6.0,96,"M20",16.0,"-"]
[null,"SO PN 6 DIN 2641 Size DN 350","SO","PN 6","DIN 2641","14\"",350.0,490.0,"-",26.0,"-",445.0,12.0,23.0,"-","-",362.0,7.0,101,"M20",16.0,"-"]
[null,"SO PN 6 DIN 2641 Size DN 400","SO","PN 6","DIN 2641","16\"",400.0,540.0,"-",28.0,"-",495.0,16.0,23.0,"-","-",413.0,7.0,105,"M20",16.0,"-"]
[null,"SO PN 6 DIN 2641 Size DN 500","SO","PN 6","DIN 2641","20\"",500.0,645.0,"-",32.0,"-",600.0,20.0,23.0,"-","-",517.0,7.0,113,"M20",16.0,"-"]
[null,"SO PN 6 DIN 2641 Size DN 600","SO","PN 6","DIN 2641","24\"",600.0,755.0,"-",36.0,"-",705.0,20.0,27.0,"-","-",618.0,7.0,127,"M24",19.0,"-"]
[null,"SO PN 6 DIN 2641 Size DN 700","SO","PN 6","DIN 2641","28\"",700.0,860.0,"-",40.0,"-",810.0,24.0,27.0,"-","-",721.0,7.0,135,"M24",19.0,"-"]
[null,"SO PN 6 DIN 2641 Size DN 800","SO","PN 6","DIN 2641","32\"",800.0,975.0,"-",44.0,"-",920.0,24.0,30.0,"-","-",824.0,7.0,149,"M27",22.0,"-"]
[null,"SO PN 6 DIN 2641 Size DN 900","SO","PN 6","DIN 2641","36\"",900.0,1075.0,"-",48.0,"-",1020.0,24.0,30.0,"-","-",926.0,7.0,157,"M27",22.0,"-"]
[null,"SO PN 6 DIN 2641 Size DN 1050","SO","PN 6","DIN 2641","42\"",1050.0,1175.0,"-",52.0,"-",1120.0,28.0,30.0,"-","-",1028.0,7.0,165,"M27",22.0,"-"]
[null,"SO PN 10 DIN 2642 Size DN 15","SO","PN 10","DIN 2642","1/2\"",15.0,95.0,"-",14.0,"-",65.0,4.0,14.0,"-","-",24.0,3.0,61,"M12",10.0,"-"]
[null,"SO PN 10 DIN 2642 Size DN 20","SO","PN 10","DIN 2642","3/4\"",20.0,105.0,"-",14.0,"-",75.0,4.0,14.0,"-","-",30.0,3.0,61,"M12",10.0,"-"]
[null,"SO PN 10 DIN 2642 Size DN 25","SO","PN 10","DIN 2642","1\"",25.0,115.0,"-",16.0,"-",85.0,4.0,14.0,"-","-",36.0,3.0,65,"M12",10.0,"-"]
[null,"SO PN 10 DIN 2642 Size DN 32","SO","PN 10","DIN 2642","1¼\"",32.0,140.0,"-",16.0,"-",100.0,4.0,18.0,"-","-",46.0,3.0,71,"M16",13.0,"-"]
[null,"SO PN 10 DIN 2642 Size DN 40","SO","PN 10","DIN 2642","1½\"",40.0,150.0,"-",16.0,"-",110.0,4.0,18.0,"-","-",54.0,3.0,71,"M16",13.0,"-"]
[null,"SO PN 10 DIN 2642 Size DN 50","SO","PN 10","DIN 2642","2\"",50.0,165.0,"-",16.0,"-",125.0,4.0,18.0,"-","-",65.0,4.0,72,"M16",13.0,"-"]
[null,"SO PN 10 DIN 2642 Size DN 65","SO","PN 10","DIN 2642","2½\"",65.0,185.0,"-",16.0,"-",145.0,4.0,18.0,"-","-",81.0,4.0,72,"M16",13.0,"-"]
[null,"SO PN 10 DIN 2642 Size DN 80","SO","PN 10","DIN 2642","3\"",80.0,200.0,"-",18.0,"-",160.0,4.0,18.0,"-","-",94.0,4.0,76,"M16",13.0,"-"]
[null,"SO PN 10 DIN 2642 Size DN 100","SO","PN 10","DIN 2642","4\"",100.0,220.0,"-",18.0,"-",180.0,8.0,18.0,"-","-",119.0,5.0,77,"M16",13.0,"-"]
[null,"SO PN 10 DIN 2642 Size DN 125","SO","PN 10","DIN 2642","5\"",125.0,250.0,"-",18.0,"-",210.0,8.0,18.0,"-","-",145.0,5.0,77,"M16",13.0,"-"]
[null,"SO PN 10 DIN 2642 Size DN 150","SO","PN 10","DIN 2642","6\"",150.0,285.0,"-",18.0,"-",240.0,8.0,23.0,"-","-",173.0,6.0,84,"M20",16.0,"-"]
[null,"SO PN 10 DIN 2642 Size DN 200","SO","PN 10","DIN 2642","8\"",200.0,340.0,"-",20.0,"-",295.0,8.0,23.0,"-","-",225.0,6.0,88,"M20",16.0,"-"]
[null,"SO PN 10 DIN 2642 Size DN 250","SO","PN 10","DIN 2642","10\"",250.0,395.0,"-",22.0,"-",350.0,12.0,23.0,"-","-",279.0,6.0,92,"M20",16.0,"-"]
[null,"SO PN 10 DIN 2642 Size DN 300","SO","PN 10","DIN 2642","12\"",300.0,445.0,"-",26.0,"-",400.0,12.0,23.0,"-","-",329.0,6.0,100,"M20",16.0,"-"]
[null,"SO PN 10 DIN 2642 Size DN 350","SO","PN 10","DIN 2642","14\"",350.0,505.0,"-",28.0,"-",460.0,16.0,23.0,"-","-",362.0,7.0,105,"M20",16.0,"-"]
[null,"SO PN 10 DIN 2642 Size DN 400","SO","PN 10","DIN 2642","16\"",400.0,565.0,"-",32.0,"-",515.0,16.0,27.0,"-","-",413.0,7.0,119,"M24",19.0,"-"]
[null,"SO PN 10 DIN 2642 Size DN 500","SO","PN 10","DIN 2642","20\"",500.0,670.0,"-",38.0,"-",620.0,20.0,27.0,"-","-",517.0,7.0,131,"M24",19.0,"-"]
[null,"SO PN 10 DIN 2642 Size DN 600","SO","PN 10","DIN 2642","24\"",600.0,780.0,"-",44.0,"-",725.0,20.0,30.0,"-","-",618.0,7.0,149,"M27",22.0,"-"]
[null,"SO PN 10 DIN 2642 Size DN 700","SO","PN 10","DIN 2642","28\"",700.0,895.0,"-",50.0,"-",840.0,24.0,30.0,"-","-",721.0,7.0,161,"M27",22.0,"-"]
[null,"SO PN 10 DIN 2642 Size DN 800","SO","PN 10","DIN 2642","32\"",800.0,1015.0,"-",56.0,"-",950.0,24.0,33.0,"-","-",824.0,7.0,177,"M30",24.0,"-"]
[null,"SO PN 25 DIN 2655 Size DN 15","SO","PN 25","DIN 2655","1/2\"",15.0,95.0,"-",16.0,"-",65.0,4.0,14.0,"-","-",24.0,3.0,65,"M12",10.0,"-"]
[null,"SO PN 25 DIN 2655 Size DN 20","SO","PN 25","DIN 2655","3/4\"",20.0,105.0,"-",16.0,"-",75.0,4.0,14.0,"-","-",30.0,3.0,65,"M12",10.0,"-"]
[null,"SO PN 25 DIN 2655 Size DN 25","SO","PN 25","DIN 2655","1\"",25.0,115.0,"-",18.0,"-",85.0,4.0,14.0,"-","-",36.0,3.0,69,"M12",10.0,"-"]
[null,"SO PN 25 DIN 2655 Size DN 32","SO","PN 25","DIN 2655","1¼\"",32.0,140.0,"-",18.0,"-",100.0,4.0,18.0,"-","-",46.0,3.0,75,"M16",13.0,"-"]
[null,"SO PN 25 DIN 2655 Size DN 40","SO","PN 25","DIN 2655","1½\"",40.0,150.0,"-",18.0,"-",110.0,4.0,18.0,"-","-",54.0,3.0,75,"M16",13.0,"-"]
[null,"SO PN 25 DIN 2655 Size DN 50","SO","PN 25","DIN 2655","2\"",50.0,165.0,"-",20.0,"-",125.0,4.0,18.0,"-","-",65.0,4.0,80,"M16",13.0,"-"]
[null,"SO PN 25 DIN 2655 Size DN 65","SO","PN 25","DIN 2655","2½\"",65.0,185.0,"-",20.0,"-",145.0,8.0,18.0,"-","-",81.0,4.0,80,"M16",13.0,"-"]
[null,"SO PN 25 DIN 2655 Size DN 80","SO","PN 25","DIN 2655","3\"",80.0,200.0,"-",22.0,"-",160.0,8.0,18.0,"-","-",94.0,4.0,84,"M16",13.0,"-"]
[null,"SO PN 25 DIN 2655 Size DN 100","SO","PN 25","DIN 2655","4\"",100.0,235.0,"-",22.0,"-",190.0,8.0,23.0,"-","-",119.0,5.0,91,"M20",16.0,"-"]
[null,"SO PN 25 DIN 2655 Size DN 125","SO","PN 25","DIN 2655","5\"",125.0,270.0,"-",24.0,"-",220.0,8.0,27.0,"-","-",145.0,5.0,101,"M24",19.0,"-"]
[null,"SO PN 25 DIN 2655 Size DN 150","SO","PN 25","DIN 2655","6\"",150.0,300.0,"-",24.0,"-",250.0,8.0,27.0,"-","-",173.0,6.0,102,"M24",19.0,"-"]
[null,"SO PN 25 DIN 2655 Size DN 200","SO","PN 25","DIN 2655","8\"",200.0,360.0,"-",26.0,"-",310.0,12.0,27.0,"-","-",225.0,6.0,106,"M24",19.0,"-"]
[null,"SO PN 25 DIN 2655 Size DN 250","SO","PN 25","DIN 2655","10\"",250.0,425.0,"-",30.0,"-",370.0,12.0,30.0,"-","-",279.0,6.0,120,"M27",22.0,"-"]
[null,"SO PN 25 DIN 2655 Size DN 300","SO","PN 25","DIN 2655","12\"",300.0,485.0,"-",34.0,"-",430.0,16.0,30.0,"-","-",329.0,6.0,128,"M27",22.0,"-"]
[null,"SO PN 25 DIN 2655 Size DN 350","SO","PN 25","DIN 2655","14\"",350.0,555.0,"-",38.0,"-",490.0,16.0,33.0,"-","-",362.0,7.0,141,"M30",24.0,"-"]
[null,"SO PN 25 DIN 2655 Size DN 400","SO","PN 25","DIN 2655","16\"",400.0,620.0,"-",42.0,"-",550.0,16.0,36.0,"-","-",413.0,7.0,155,"M33",27.0,"-"]
[null,"SO PN 25 DIN 2655 Size DN 500","SO","PN 25","DIN 2655","20\"",500.0,730.0,"-",50.0,"-",660.0,20.0,36.0,"-","-",517.0,7.0,171,"M33",27.0,"-"]
[null,"SO PN 40 DIN 2656 Size DN 15","SO","PN 40","DIN 2656","1/2\"",15.0,95.0,"-",16.0,"-",65.0,4.0,14.0,"-","-",24.0,3.0,65,"M12",10.0,"-"]
[null,"SO PN 40 DIN 2656 Size DN 20","SO","PN 40","DIN 2656","3/4\"",20.0,105.0,"-",16.0,"-",75.0,4.0,14.0,"-","-",30.0,3.0,65,"M12",10.0,"-"]
[null,"SO PN 40 DIN 2656 Size DN 25","SO","PN 40","DIN 2656","1\"",25.0,115.0,"-",18.0,"-",85.0,4.0,14.0,"-","-",36.0,3.0,69,"M12",10.0,"-"]
[null,"SO PN 40 DIN 2656 Size DN 32","SO","PN 40","DIN 2656","1¼\"",32.0,140.0,"-",18.0,"-",100.0,4.0,18.0,"-","-",46.0,3.0,75,"M16",13.0,"-"]
[null,"SO PN 40 DIN 2656 Size DN 40","SO","PN 40","DIN 2656","1½\"",40.0,150.0,"-",18.0,"-",110.0,4.0,18.0,"-","-",54.0,3.0,75,"M16",13.0,"-"]
[null,"SO PN 40 DIN 2656 Size DN 50","SO","PN 40","DIN 2656","2\"",50.0,165.0,"-",20.0,"-",125.0,4.0,18.0,"-","-",65.0,4.0,80,"M16",13.0,"-"]
[null,"SO PN 40 DIN 2656 Size DN 65","SO","PN 40","DIN 2656","2½\"",65.0,185.0,"-",20.0,"-",145.0,8.0,18.0,"-","-",81.0,4.0,80,"M16",13.0,"-"]
[null,"SO PN 40 DIN 2656 Size DN 80","SO","PN 40","DIN 2656","3\"",80.0,200.0,"-",22.0,"-",160.0,8.0,18.0,"-","-",94.0,4.0,84,"M16",13.0,"-"]
[null,"SO PN 40 DIN 2656 Size DN 100","SO","PN 40","DIN 2656","4\"",100.0,235.0,"-",22.0,"-",190.0,8.0,23.0,"-","-",119.0,5.0,91,"M20",16.0,"-"]
[null,"SO PN 40 DIN 2656 Size DN 125","SO","PN 40","DIN 2656","5\"",125.0,270.0,"-",24.0,"-",220.0,8.0,27.0,"-","-",145.0,5.0,101,"M24",19.0,"-"]
[null,"SO PN 40 DIN 2656 Size DN 150","SO","PN 40","DIN 2656","6\"",150.0,300.0,"-",24.0,"-",250.0,8.0,27.0,"-","-",173.0,6.0,102,"M24",19.0,"-"]
[null,"SO PN 40 DIN 2656 Size DN 200","SO","PN 40","DIN 2656","8\"",200.0,375.0,"-",30.0,"-",320.0,12.0,30.0,"-","-",225.0,6.0,120,"M27",22.0,"-"]
[null,"SO PN 40 DIN 2656 Size DN 250","SO","PN 40","DIN 2656","10\"",250.0,450.0,"-",36.0,"-",385.0,12.0,33.0,"-","-",279.0,6.0,136,"M30",24.0,"-"]
[null,"SO PN 40 DIN 2656 Size DN 300","SO","PN 40","DIN 2656","12\"",300.0,515.0,"-",40.0,"-",450.0,16.0,33.0,"-","-",329.0,6.0,144,"M30",24.0,"-"]
[null,"SO PN 40 DIN 2656 Size DN 350","SO","PN 40","DIN 2656","14\"",350.0,580.0,"-",46.0,"-",510.0,16.0,36.0,"-","-",362.0,7.0,163,"M33",27.0,"-"]
[null,"SO PN 40 DIN 2656 Size DN 400","SO","PN 40","DIN 2656","16\"",400.0,660.0,"-",50.0,"-",585.0,16.0,39.0,"-","-",413.0,7.0,175,"M36",29.0,"-"]
[null,"BL PN 6 DIN 2527 Size DN 10","BL","PN 6","DIN 2527","1/4\"",10.0,75.0,"-",12.0,"-",50.0,4.0,11.0,"-","-","-",3.0,53,"M10",8.0,0.38]
[null,"BL PN 6 DIN 2527 Size DN 15","BL","PN 6","DIN 2527","1/2\"",15.0,80.0,"-",12.0,"-",55.0,4.0,11.0,"-","-","-",3.0,53,"M10",8.0,0.44]
[null,"BL PN 6 DIN 2527 Size DN 20","BL","PN 6","DIN 2527","3/4\"",20.0,90.0,"-",14.0,"-",65.0,4.0,11.0,"-","-","-",3.0,57,"M10",8.0,0.65]
[null,"BL PN 6 DIN 2527 Size DN 25","BL","PN 6","DIN 2527","1\"",25.0,100.0,"-",14.0,"-",75.0,4.0,11.0,"-","-","-",3.0,57,"M10",8.0,0.82]
[null,"BL PN 6 DIN 2527 Size DN 32","BL","PN 6","DIN 2527","1¼\"",32.0,120.0,"-",14.0,"-",90.0,4.0,14.0,"-","-","-",3.0,61,"M12",10.0,1.17]
[null,"BL PN 6 DIN 2527 Size DN 40","BL","PN 6","DIN 2527","1½\"",40.0,130.0,"-",14.0,"-",100.0,4.0,14.0,"-","-","-",3.0,61,"M12",10.0,1.39]
[null,"BL PN 6 DIN 2527 Size DN 50","BL","PN 6","DIN 2527","2\"",50.0,140.0,"-",14.0,"-",110.0,4.0,14.0,"-","-","-",4.0,62,"M12",10.0,1.62]
[null,"BLRF PN 6 DIN 2527 Size DN 65","BLRF","PN 6","DIN 2527","2½\"",65.0,160.0,"-",14.0,55.0,130.0,4.0,14.0,"-",2.0,"-",4.0,62,"M12",10.0,2.48]
[null,"BLRF PN 6 DIN 2527 Size DN 80","BLRF","PN 6","DIN 2527","3\"",80.0,190.0,"-",16.0,70.0,150.0,4.0,18.0,"-",2.0,"-",4.0,72,"M16",13.0,3.49]
[null,"BLRF PN 6 DIN 2527 Size DN 100","BLRF","PN 6","DIN 2527","4\"",100.0,210.0,"-",16.0,90.0,170.0,4.0,18.0,"-",2.0,"-",5.0,73,"M16",13.0,4.86]
[null,"BLRF PN 6 DIN 2527 Size DN 125","BLRF","PN 6","DIN 2527","5\"",125.0,240.0,"-",18.0,115.0,200.0,8.0,18.0,"-",2.0,"-",5.0,77,"M16",13.0,6.28]
[null,"BLRF PN 6 DIN 2527 Size DN 150","BLRF","PN 6","DIN 2527","6\"",150.0,265.0,"-",18.0,140.0,225.0,8.0,18.0,"-",2.0,"-",6.0,78,"M16",13.0,7.75]
[null,"BLRF PN 6 DIN 2527 Size DN 175","BLRF","PN 6","DIN 2527","7\"",175.0,295.0,"-",20.0,165.0,255.0,8.0,18.0,"-",2.0,"-",6.0,82,"M16",13.0,10.7]
[null,"BLRF PN 6 DIN 2527 Size DN 200","BLRF","PN 6","DIN 2527","8\"",200.0,320.0,"-",20.0,190.0,280.0,8.0,18.0,"-",2.0,"-",6.0,82,"M16",13.0,12.7]
[null,"BLRF PN 6 DIN 2527 Size DN 250","BLRF","PN 6","DIN 2527","10\"",250.0,375.0,"-",22.0,235.0,335.0,12.0,18.0,"-",2.0,"-",6.0,86,"M16",13.0,19.0]
[null,"BLRF PN 6 DIN 2527 Size DN 300","BLRF","PN 6","DIN 2527","12\"",300.0,440.0,"-",22.0,285.0,395.0,12.0,22.0,"-",2.0,"-",6.0,92,"M20",16.0,26.3]
[null,"BLRF PN 6 DIN 2527 Size DN 350","BLRF","PN 6","DIN 2527","14\"",350.0,490.0,"-",22.0,330.0,445.0,12.0,22.0,"-",2.0,"-",7.0,93,"M20",16.0,32.9]
[null,"BLRF PN 6 DIN 2527 Size DN 400","BLRF","PN 6","DIN 2527","16\"",400.0,540.0,"-",22.0,380.0,495.0,16.0,22.0,"-",2.0,"-",7.0,93,"M20",16.0,40.2]
[null,"BLRF PN 6 DIN 2527 Size DN 500","BLRF","PN 6","DIN 2527","20\"",500.0,645.0,"-",24.0,475.0,600.0,20.0,22.0,"-",2.0,"-",7.0,97,"M20",16.0,63.2]
[null,"BL PN 10 DIN 2527 Size DN 10","BL","PN 10","DIN 2527","1/4\"",10.0,90.0,"-",14.0,"-",60.0,4.0,14.0,"-","-","-",3.0,61,"M12",10.0,0.63]
[null,"BL PN 10 DIN 2527 Size DN 15","BL","PN 10","DIN 2527","1/2\"",15.0,95.0,"-",14.0,"-",65.0,4.0,14.0,"-","-","-",3.0,61,"M12",10.0,0.72]
[null,"BL PN 10 DIN 2527 Size DN 20","BL","PN 10","DIN 2527","3/4\"",20.0,105.0,"-",16.0,"-",75.0,4.0,14.0,"-","-","-",3.0,65,"M12",10.0,1.01]
[null,"BL PN 10 DIN 2527 Size DN 25","BL","PN 10","DIN 2527","1\"",25.0,115.0,"-",16.0,"-",85.0,4.0,14.0,"-","-","-",3.0,65,"M12",10.0,1.23]
[null,"BL PN 10 DIN 2527 Size DN 32","BL","PN 10","DIN 2527","1¼\"",32.0,140.0,"-",16.0,"-",100.0,4.0,18.0,"-","-","-",3.0,71,"M16",13.0,1.8]
[null,"BL PN 10 DIN 2527 Size DN 40","BL","PN 10","DIN 2527","1½\"",40.0,150.0,"-",16.0,"-",110.0,4.0,18.0,"-","-","-",3.0,71,"M16",13.0,2.09]
[null,"BL PN 10 DIN 2527 Size DN 50","BL","PN 10","DIN 2527","2\"",50.0,165.0,"-",18.0,"-",125.0,4.0,18.0,"-","-","-",4.0,76,"M16",13.0,2.88]
[null,"BL PN 10 DIN 2527 Size DN 65","BL","PN 10","DIN 2527","2½\"",65.0,185.0,"-",18.0,55.0,145.0,4.0,18.0,"-",2.0,"-",4.0,76,"M16",13.0,3.7]
[null,"BL PN 10 DIN 2527 Size DN 80","BL","PN 10","DIN 2527","3\"",80.0,200.0,"-",20.0,70.0,160.0,8.0,18.0,"-",2.0,"-",4.0,80,"M16",13.0,4.83]
[null,"BL PN 10 DIN 2527 Size DN 100","BL","PN 10","DIN 2527","4\"",100.0,220.0,"-",20.0,90.0,180.0,8.0,18.0,"-",2.0,"-",5.0,81,"M16",13.0,5.75]
[null,"BL PN 10 DIN 2527 Size DN 125","BL","PN 10","DIN 2527","5\"",125.0,250.0,"-",22.0,115.0,210.0,8.0,18.0,"-",2.0,"-",5.0,85,"M16",13.0,8.59]
[null,"BL PN 10 DIN 2527 Size DN 150","BL","PN 10","DIN 2527","6\"",150.0,285.0,"-",22.0,140.0,240.0,8.0,22.0,"-",2.0,"-",6.0,92,"M20",16.0,10.6]
[null,"BL PN 10 DIN 2527 Size DN 175","BL","PN 10","DIN 2527","7\"",175.0,315.0,"-",24.0,165.0,270.0,8.0,22.0,"-",2.0,"-",6.0,96,"M20",16.0,14.3]
[null,"BL PN 10 DIN 2527 Size DN 200","BL","PN 10","DIN 2527","8\"",200.0,340.0,"-",24.0,190.0,295.0,8.0,22.0,"-",2.0,"-",6.0,96,"M20",16.0,16.9]
[null,"BL PN 10 DIN 2527 Size DN 250","BL","PN 10","DIN 2527","10\"",250.0,395.0,"-",26.0,235.0,350.0,12.0,22.0,"-",2.0,"-",6.0,100,"M20",16.0,24.7]
[null,"BL PN 10 DIN 2527 Size DN 300","BL","PN 10","DIN 2527","12\"",300.0,445.0,"-",26.0,285.0,400.0,12.0,22.0,"-",2.0,"-",6.0,100,"M20",16.0,31.9]
[null,"BL PN 10 DIN 2527 Size DN 350","BL","PN 10","DIN 2527","14\"",350.0,505.0,"-",26.0,330.0,460.0,16.0,22.0,"-",2.0,"-",7.0,101,"M20",16.0,41.9]
[null,"BL PN 10 DIN 2527 Size DN 400","BL","PN 10","DIN 2527","16\"",400.0,565.0,"-",26.0,380.0,515.0,16.0,26.0,"-",2.0,"-",7.0,107,"M24",19.0,51.2]
[null,"BL PN 10 DIN 2527 Size DN 500","BL","PN 10","DIN 2527","20\"",500.0,670.0,"-",28.0,475.0,620.0,20.0,26.0,"-",2.0,"-",7.0,111,"M24",19.0,77.8]
[null,"BL PN 16 DIN 2527 Size DN 10","BL","PN 16","DIN 2527","1/4\"",10.0,90.0,"-",14.0,"-",60.0,4.0,14.0,"-","-","-",3.0,61,"M12",10.0,0.63]
[null,"BL PN 16 DIN 2527 Size DN 15","BL","PN 16","DIN 2527","1/2\"",15.0,95.0,"-",14.0,"-",65.0,4.0,14.0,"-","-","-",3.0,61,"M12",10.0,0.72]
[null,"BL PN 16 DIN 2527 Size DN 20","BL","PN 16","DIN 2527","3/4\"",20.0,105.0,"-",16.0,"-",75.0,4.0,14.0,"-","-","-",3.0,65,"M12",10.0,1.01]
[null,"BL PN 16 DIN 2527 Size DN 25","BL","PN 16","DIN 2527","1\"",25.0,115.0,"-",16.0,"-",85.0,4.0,14.0,"-","-","-",3.0,65,"M12",10.0,1.23]
[null,"BL PN 16 DIN 2527 Size DN 32","BL","PN 16","DIN 2527","1¼\"",32.0,140.0,"-",16.0,"-",100.0,4.0,18.0,"-","-","-",3.0,71,"M16",13.0,1.8]
[null,"BL PN 16 DIN 2527 Size DN 40","BL","PN 16","DIN 2527","1½\"",40.0,150.0,"-",16.0,"-",110.0,4.0,18.0,"-","-","-",3.0,71,"M16",13.0,2.09]
[null,"BL PN 16 DIN 2527 Size DN 50","BL","PN 16","DIN 2527","2\"",50.0,165.0,"-",18.0,"-",125.0,4.0,18.0,"-","-","-",4.0,76,"M16",13.0,2.88]
[null,"BLRF PN 16 DIN 2527 Size DN 65","BLRF","PN 16","DIN 2527","2½\"",65.0,185.0,"-",18.0,55.0,145.0,4.0,18.0,"-",2.0,"-",4.0,76,"M16",13.0,3.7]
[null,"BLRF PN 16 DIN 2527 Size DN 80","BLRF","PN 16","DIN 2527","3\"",80.0,200.0,"-",20.0,70.0,160.0,8.0,18.0,"-",2.0,"-",4.0,80,"M16",13.0,4.83]
[null,"BLRF PN 16 DIN 2527 Size DN 100","BLRF","PN 16","DIN 2527","4\"",100.0,220.0,"-",20.0,90.0,180.0,8.0,18.0,"-",2.0,"-",5.0,81,"M16",13.0,5.75]
[null,"BLRF PN 16 DIN 2527 Size DN 125","BLRF","PN 16","DIN 2527","5\"",125.0,250.0,"-",22.0,115.0,210.0,8.0,18.0,"-",2.0,"-",5.0,85,"M16",13.0,8.59]
[null,"BLRF PN 16 DIN 2527 Size DN 150","BLRF","PN 16","DIN 2527","6\"",150.0,285.0,"-",22.0,140.0,240.0,8.0,22.0,"-",2.0,"-",6.0,92,"M20",16.0,10.6]
[null,"BLRF PN 16 DIN 2527 Size DN 175","BLRF","PN 16","DIN 2527","7\"",175.0,315.0,"-",24.0,165.0,270.0,8.0,22.0,"-",2.0,"-",6.0,96,"M20",16.0,14.3]
[null,"BLRF PN 16 DIN 2527 Size DN 200","BLRF","PN 16","DIN 2527","8\"",200.0,340.0,"-",24.0,190.0,295.0,12.0,26.0,"-",2.0,"-",6.0,102,"M24",19.0,16.5]
[null,"BLRF PN 16 DIN 2527 Size DN 250","BLRF","PN 16","DIN 2527","10\"",250.0,405.0,"-",26.0,235.0,355.0,12.0,26.0,"-",2.0,"-",6.0,106,"M24",19.0,25.6]
[null,"BLRF PN 16 DIN 2527 Size DN 300","BLRF","PN 16","DIN 2527","12\"",300.0,460.0,"-",28.0,285.0,410.0,12.0,26.0,"-",2.0,"-",6.0,110,"M24",19.0,36.1]
[null,"BLRF PN 16 DIN 2527 Size DN 350","BLRF","PN 16","DIN 2527","14\"",350.0,520.0,"-",30.0,330.0,470.0,16.0,26.0,"-",2.0,"-",7.0,115,"M24",19.0,49.1]
[null,"BLRF PN 16 DIN 2527 Size DN 400","BLRF","PN 16","DIN 2527","16\"",400.0,580.0,"-",32.0,380.0,525.0,16.0,30.0,"-",2.0,"-",7.0,125,"M27",22.0,65.3]
[null,"BLRF PN 16 DIN 2527 Size DN 500","BLRF","PN 16","DIN 2527","20\"",500.0,715.0,"-",36.0,475.0,650.0,20.0,33.0,"-",2.0,"-",7.0,137,"M30",24.0,105.0]
[null,"BL PN 25 DIN 2527 Size DN 10","BL","PN 25","DIN 2527","1/4\"",10.0,90.0,"-",16.0,"-",60.0,4.0,14.0,"-",2.0,"-",3.0,65,"M12",10.0,0.72]
[null,"BL PN 25 DIN 2527 Size DN 15","BL","PN 25","DIN 2527","1/2\"",15.0,95.0,"-",16.0,"-",65.0,4.0,14.0,"-",2.0,"-",3.0,65,"M12",10.0,0.81]
[null,"BL PN 25 DIN 2527 Size DN 20","BL","PN 25","DIN 2527","3/4\"",20.0,105.0,"-",18.0,"-",75.0,4.0,14.0,"-",2.0,"-",3.0,69,"M12",10.0,0.124]
[null,"BL PN 25 DIN 2527 Size DN 25","BL","PN 25","DIN 2527","1\"",25.0,115.0,"-",18.0,"-",85.0,4.0,14.0,"-",2.0,"-",3.0,69,"M12",10.0,1.38]
[null,"BL PN 25 DIN 2527 Size DN 32","BL","PN 25","DIN 2527","1¼\"",32.0,140.0,"-",18.0,"-",100.0,4.0,18.0,"-",2.0,"-",3.0,75,"M16",13.0,2.03]
[null,"BL PN 25 DIN 2527 Size DN 40","BL","PN 25","DIN 2527","1½\"",40.0,150.0,"-",18.0,"-",110.0,4.0,18.0,"-",2.0,"-",3.0,75,"M16",13.0,2.35]
[null,"BL PN 25 DIN 2527 Size DN 50","BL","PN 25","DIN 2527","2\"",50.0,165.0,"-",20.0,"-",125.0,4.0,18.0,"-",2.0,"-",4.0,80,"M16",13.0,3.2]
[null,"BL PN 25 DIN 2527 Size DN 65","BL","PN 25","DIN 2527","2½\"",65.0,185.0,"-",22.0,55.0,145.0,8.0,18.0,"-",2.0,"-",4.0,84,"M16",13.0,4.33]
[null,"BL PN 25 DIN 2527 Size DN 80","BL","PN 25","DIN 2527","3\"",80.0,200.0,"-",24.0,70.0,160.0,8.0,18.0,"-",2.0,"-",4.0,88,"M16",13.0,5.94]
[null,"BL PN 25 DIN 2527 Size DN 100","BL","PN 25","DIN 2527","4\"",100.0,235.0,"-",24.0,90.0,190.0,8.0,22.0,"-",2.0,"-",5.0,95,"M20",16.0,7.64]
[null,"BL PN 25 DIN 2527 Size DN 125","BL","PN 25","DIN 2527","5\"",125.0,270.0,"-",26.0,115.0,220.0,8.0,26.0,"-",2.0,"-",5.0,105,"M24",19.0,11.0]
[null,"BL PN 25 DIN 2527 Size DN 150","BL","PN 25","DIN 2527","6\"",150.0,300.0,"-",28.0,140.0,250.0,8.0,26.0,"-",2.0,"-",5.0,109,"M24",19.0,14.7]
[null,"BL PN 25 DIN 2527 Size DN 175","BL","PN 25","DIN 2527","7\"",175.0,330.0,"-",28.0,165.0,280.0,12.0,26.0,"-",2.0,"-",6.0,110,"M24",19.0,17.6]
[null,"BL PN 25 DIN 2527 Size DN 200","BL","PN 25","DIN 2527","8\"",200.0,360.0,"-",30.0,190.0,310.0,12.0,26.0,"-",2.0,"-",6.0,114,"M24",19.0,22.7]
[null,"BL PN 25 DIN 2527 Size DN 250","BL","PN 25","DIN 2527","10\"",250.0,425.0,"-",32.0,237.0,370.0,12.0,30.0,"-",2.0,"-",6.0,124,"M27",22.0,34.2]
[null,"BL PN 25 DIN 2527 Size DN 300","BL","PN 25","DIN 2527","12\"",300.0,485.0,"-",34.0,285.0,430.0,16.0,30.0,"-",2.0,"-",6.0,128,"M27",22.0,47.3]
[null,"BL PN 25 DIN 2527 Size DN 350","BL","PN 25","DIN 2527","14\"",350.0,555.0,"-",38.0,330.0,490.0,16.0,33.0,"-",2.0,"-",7.0,141,"M30",24.0,69.3]
[null,"BL PN 25 DIN 2527 Size DN 400","BL","PN 25","DIN 2527","16\"",400.0,620.0,"-",40.0,380.0,550.0,16.0,36.0,"-",2.0,"-",7.0,151,"M33",27.0,91.5]
[null,"BL PN 25 DIN 2527 Size DN 500","BL","PN 25","DIN 2527","20\"",500.0,730.0,"-",45.0,475.0,660.0,20.0,36.0,"-",2.0,"-",7.0,161,"M33",27.0,141.0]
[null,"BL PN 40 DIN 2527 Size DN 10","BL","PN 40","DIN 2527","1/4\"",10.0,90.0,"-",16.0,"-",60.0,4.0,14.0,"-",2.0,"-",3.0,65,"M12",10.0,0.72]
[null,"BL PN 40 DIN 2527 Size DN 15","BL","PN 40","DIN 2527","1/2\"",15.0,95.0,"-",16.0,"-",65.0,4.0,14.0,"-",2.0,"-",3.0,65,"M12",10.0,0.81]
[null,"BL PN 40 DIN 2527 Size DN 20","BL","PN 40","DIN 2527","3/4\"",20.0,105.0,"-",18.0,"-",75.0,4.0,14.0,"-",2.0,"-",3.0,69,"M12",10.0,0.124]
[null,"BL PN 40 DIN 2527 Size DN 25","BL","PN 40","DIN 2527","1\"",25.0,115.0,"-",18.0,"-",85.0,4.0,14.0,"-",2.0,"-",3.0,69,"M12",10.0,1.38]
[null,"BL PN 40 DIN 2527 Size DN 32","BL","PN 40","DIN 2527","1¼\"",32.0,140.0,"-",18.0,"-",100.0,4.0,18.0,"-",2.0,"-",3.0,69,"M16",10.0,2.03]
[null,"BL PN 40 DIN 2527 Size DN 40","BL","PN 40","DIN 2527","1½\"",40.0,150.0,"-",18.0,"-",110.0,4.0,18.0,"-",2.0,"-",3.0,75,"M16",13.0,2.35]
[null,"BL PN 40 DIN 2527 Size DN 50","BL","PN 40","DIN 2527","2\"",50.0,165.0,"-",20.0,"-",125.0,4.0,18.0,"-",2.0,"-",4.0,80,"M16",13.0,3.2]
[null,"BL PN 40 DIN 2527 Size DN 65","BL","PN 40","DIN 2527","2½\"",65.0,185.0,"-",22.0,55.0,145.0,8.0,18.0,"-",2.0,"-",4.0,84,"M16",13.0,4.33]
[null,"BL PN 40 DIN 2527 Size DN 80","BL","PN 40","DIN 2527","3\"",80.0,200.0,"-",24.0,70.0,160.0,8.0,18.0,"-",2.0,"-",4.0,88,"M16",13.0,5.94]
[null,"BL PN 40 DIN 2527 Size DN 100","BL","PN 40","DIN 2527","4\"",100.0,235.0,"-",24.0,90.0,190.0,8.0,22.0,"-",2.0,"-",5.0,95,"M20",16.0,7.64]
[null,"BL PN 40 DIN 2527 Size DN 125","BL","PN 40","DIN 2527","5\"",125.0,270.0,"-",26.0,115.0,220.0,8.0,26.0,"-",2.0,"-",5.0,105,"M24",19.0,11.0]
[null,"BL PN 40 DIN 2527 Size DN 150","BL","PN 40","DIN 2527","6\"",150.0,300.0,"-",28.0,140.0,250.0,8.0,26.0,"-",2.0,"-",6.0,110,"M24",19.0,14.7]
[null,"BL PN 40 DIN 2527 Size DN 175","BL","PN 40","DIN 2527","7\"",175.0,350.0,"-",32.0,165.0,295.0,12.0,30.0,"-",2.0,"-",6.0,124,"M27",22.0,22.4]
[null,"BL PN 40 DIN 2527 Size DN 200","BL","PN 40","DIN 2527","8\"",200.0,375.0,"-",34.0,190.0,320.0,12.0,30.0,"-",2.0,"-",6.0,128,"M27",22.0,27.6]
[null,"BL PN 40 DIN 2527 Size DN 250","BL","PN 40","DIN 2527","10\"",250.0,450.0,"-",38.0,235.0,385.0,12.0,33.0,"-",2.0,"-",6.0,140,"M30",24.0,44.5]
[null,"BL PN 40 DIN 2527 Size DN 300","BL","PN 40","DIN 2527","12\"",300.0,515.0,"-",42.0,285.0,450.0,16.0,33.0,"-",2.0,"-",6.0,148,"M30",24.0,64.3]
[null,"BL PN 40 DIN 2527 Size DN 350","BL","PN 40","DIN 2527","14\"",350.0,580.0,"-",46.0,330.0,510.0,16.0,36.0,"-",2.0,"-",7.0,163,"M33",27.0,90.8]
[null,"BL PN 40 DIN 2527 Size DN 400","BL","PN 40","DIN 2527","16\"",400.0,660.0,"-",50.0,380.0,585.0,16.0,39.0,"-",2.0,"-",7.0,175,"M36",29.0,129.0]
[null,"BL PN 40 DIN 2527 Size DN 500","BL","PN 40","DIN 2527","20\"",500.0,755.0,"-",56.0,475.0,670.0,20.0,42.0,"-",2.0,"-",7.0,191,"M39",31.0,175.0]
[null,"BLRF PN 64 DIN 2527 Size DN 10","BLRF","PN 64","DIN 2527","1/4\"",10.0,100.0,"-",20.0,40.0,70.0,4.0,14.0,"-",2.0,"-",3.0,73,"M12",10.0,1.0]
[null,"BLRF PN 64 DIN 2527 Size DN 15","BLRF","PN 64","DIN 2527","1/2\"",15.0,105.0,"-",20.0,45.0,75.0,4.0,14.0,"-",2.0,"-",3.0,73,"M12",10.0,1.22]
[null,"BLRF PN 64 DIN 2527 Size DN 25","BLRF","PN 64","DIN 2527","1\"",25.0,140.0,"-",24.0,68.0,100.0,4.0,18.0,"-",2.0,"-",3.0,87,"M16",13.0,2.65]
[null,"BLRF PN 64 DIN 2527 Size DN 32","BLRF","PN 64","DIN 2527","1¼\"",32.0,155.0,"-",24.0,78.0,110.0,4.0,22.0,"-",2.0,"-",3.0,93,"M20",16.0,3.24]
[null,"BLRF PN 64 DIN 2527 Size DN 40","BLRF","PN 64","DIN 2527","1½\"",40.0,170.0,"-",26.0,88.0,125.0,4.0,22.0,"-",2.0,"-",3.0,97,"M20",16.0,4.09]
[null,"BLRF PN 64 DIN 2527 Size DN 50","BLRF","PN 64","DIN 2527","2\"",50.0,180.0,"-",26.0,102.0,135.0,4.0,22.0,"-",2.0,"-",4.0,98,"M20",16.0,4.51]
[null,"BLRF PN 64 DIN 2527 Size DN 65","BLRF","PN 64","DIN 2527","2½\"",65.0,205.0,"-",26.0,122.0,160.0,8.0,22.0,"-",2.0,"-",4.0,98,"M20",16.0,5.71]
[null,"BLRF PN 64 DIN 2527 Size DN 80","BLRF","PN 64","DIN 2527","3\"",80.0,215.0,"-",28.0,138.0,170.0,8.0,22.0,"-",2.0,"-",4.0,102,"M20",16.0,6.92]
[null,"BLRF PN 64 DIN 2527 Size DN 100","BLRF","PN 64","DIN 2527","4\"",100.0,250.0,"-",30.0,162.0,200.0,8.0,26.0,"-",2.0,"-",5.0,113,"M24",19.0,10.1]
[null,"BLRF PN 64 DIN 2527 Size DN 125","BLRF","PN 64","DIN 2527","5\"",125.0,295.0,"-",34.0,188.0,240.0,8.0,30.0,"-",2.0,"-",5.0,127,"M27",22.0,16.0]
[null,"BLRF PN 64 DIN 2527 Size DN 150","BLRF","PN 64","DIN 2527","6\"",150.0,345.0,"-",36.0,218.0,280.0,8.0,33.0,"-",2.0,"-",6.0,136,"M30",24.0,23.5]
[null,"BLRF PN 64 DIN 2527 Size DN 175","BLRF","PN 64","DIN 2527","7\"",175.0,375.0,"-",40.0,260.0,310.0,12.0,33.0,"-",2.0,"-",6.0,144,"M30",24.0,30.8]
[null,"BLRF PN 64 DIN 2527 Size DN 200","BLRF","PN 64","DIN 2527","8\"",200.0,415.0,"-",42.0,285.0,345.0,12.0,36.0,"-",2.0,"-",6.0,154,"M33",27.0,39.7]
[null,"BLRF PN 64 DIN 2527 Size DN 250","BLRF","PN 64","DIN 2527","10\"",250.0,470.0,"-",46.0,345.0,400.0,12.0,36.0,"-",2.0,"-",6.0,162,"M33",27.0,57.4]
[null,"BLRF PN 64 DIN 2527 Size DN 300","BLRF","PN 64","DIN 2527","12\"",300.0,530.0,"-",52.0,410.0,460.0,16.0,36.0,"-",2.0,"-",6.0,174,"M33",27.0,81.0]
[null,"BLRF PN 64 DIN 2527 Size DN 350","BLRF","PN 64","DIN 2527","14\"",350.0,600.0,"-",56.0,465.0,525.0,16.0,39.0,"-",2.0,"-",7.0,187,"M36",29.0,114.0]
[null,"BLRF PN 64 DIN 2527 Size DN 400","BLRF","PN 64","DIN 2527","16\"",400.0,670.0,"-",60.0,535.0,585.0,16.0,42.0,"-",2.0,"-",7.0,201,"M39",32.0,153.0]
[null,"BLRF PN 100 DIN 2527 Size DN 10","BLRF","PN 100","DIN 2527","1/4\"",10.0,100.0,"-",20.0,40.0,70.0,4.0,14.0,"-",2.0,"-",3.0,73,"M12",10.0,1.0]
[null,"BLRF PN 100 DIN 2527 Size DN 15","BLRF","PN 100","DIN 2527","1/2\"",15.0,105.0,"-",20.0,45.0,75.0,4.0,14.0,"-",2.0,"-",3.0,73,"M12",10.0,1.22]
[null,"BLRF PN 100 DIN 2527 Size DN 25","BLRF","PN 100","DIN 2527","1\"",25.0,140.0,"-",24.0,68.0,100.0,4.0,18.0,"-",2.0,"-",3.0,87,"M16",13.0,2.65]
[null,"BLRF PN 100 DIN 2527 Size DN 32","BLRF","PN 100","DIN 2527","1¼\"",32.0,155.0,"-",24.0,78.0,110.0,4.0,22.0,"-",2.0,"-",3.0,93,"M20",16.0,3.24]
[null,"BLRF PN 100 DIN 2527 Size DN 40","BLRF","PN 100","DIN 2527","1½\"",40.0,170.0,"-",26.0,88.0,125.0,4.0,22.0,"-",2.0,"-",3.0,97,"M20",16.0,4.09]
[null,"BLRF PN 100 DIN 2527 Size DN 50","BLRF","PN 100","DIN 2527","2\"",50.0,195.0,"-",28.0,102.0,145.0,4.0,26.0,"-",2.0,"-",4.0,108,"M24",19.0,5.84]
[null,"BLRF PN 100 DIN 2527 Size DN 65","BLRF","PN 100","DIN 2527","2½\"",65.0,220.0,"-",30.0,122.0,170.0,8.0,26.0,"-",2.0,"-",4.0,112,"M24",19.0,8.03]
[null,"BLRF PN 100 DIN 2527 Size DN 80","BLRF","PN 100","DIN 2527","3\"",80.0,230.0,"-",32.0,138.0,180.0,8.0,26.0,"-",2.0,"-",4.0,116,"M24",19.0,9.43]
[null,"BLRF PN 100 DIN 2527 Size DN 100","BLRF","PN 100","DIN 2527","4\"",100.0,265.0,"-",36.0,162.0,210.0,8.0,30.0,"-",2.0,"-",5.0,131,"M27",22.0,14.3]
[null,"BLRF PN 100 DIN 2527 Size DN 125","BLRF","PN 100","DIN 2527","5\"",125.0,315.0,"-",40.0,188.0,250.0,8.0,33.0,"-",2.0,"-",5.0,143,"M30",24.0,22.6]
[null,"BLRF PN 100 DIN 2527 Size DN 150","BLRF","PN 100","DIN 2527","6\"",150.0,355.0,"-",44.0,218.0,290.0,12.0,33.0,"-",2.0,"-",6.0,152,"M30",24.0,31.8]
[null,"BLRF PN 100 DIN 2527 Size DN 175","BLRF","PN 100","DIN 2527","7\"",175.0,385.0,"-",48.0,260.0,320.0,12.0,33.0,"-",2.0,"-",6.0,160,"M30",24.0,41.3]
[null,"BLRF PN 100 DIN 2527 Size DN 200","BLRF","PN 100","DIN 2527","8\"",200.0,430.0,"-",52.0,285.0,360.0,12.0,36.0,"-",2.0,"-",6.0,174,"M33",27.0,56.1]
[null,"BLRF PN 100 DIN 2527 Size DN 250","BLRF","PN 100","DIN 2527","10\"",250.0,505.0,"-",60.0,345.0,430.0,12.0,39.0,"-",2.0,"-",6.0,194,"M36",29.0,89.6]
[null,"BLRF PN 100 DIN 2527 Size DN 300","BLRF","PN 100","DIN 2527","12\"",300.0,585.0,"-",68.0,410.0,500.0,16.0,42.0,"-",2.0,"-",6.0,216,"M39",32.0,119.0]
[null,"BLRF PN 100 DIN 2527 Size DN 350","BLRF","PN 100","DIN 2527","14\"",350.0,655.0,"-",74.0,465.0,560.0,16.0,48.0,"-",2.0,"-",7.0,237,"M45",36.0,175.0]
[null,"SORF PN 10 DIN 86029 Size DN 10","SORF","PN 10","DIN 86029","1/4\"",10.0,90.0,20.0,14.0,40.0,60.0,4.0,14.0,30.0,2.0,17.7,3.0,61,"M12",10.0,0.56]
[null,"SORF PN 10 DIN 86029 Size DN 15","SORF","PN 10","DIN 86029","1/2\"",15.0,95.0,20.0,14.0,45.0,65.0,4.0,14.0,35.0,2.0,22.0,3.0,61,"M12",10.0,0.64]
[null,"SORF PN 10 DIN 86029 Size DN 20","SORF","PN 10","DIN 86029","3/4\"",20.0,105.0,24.0,16.0,58.0,75.0,4.0,14.0,45.0,2.0,27.6,3.0,65,"M12",10.0,0.98]
[null,"SORF PN 10 DIN 86029 Size DN 25","SORF","PN 10","DIN 86029","1\"",25.0,115.0,24.0,16.0,68.0,85.0,4.0,14.0,52.0,2.0,34.4,3.0,65,"M12",10.0,1.12]
[null,"SORF PN 10 DIN 86029 Size DN 32","SORF","PN 10","DIN 86029","1¼\"",32.0,140.0,26.0,16.0,78.0,100.0,4.0,18.0,60.0,2.0,43.1,3.0,71,"M16",13.0,1.58]
[null,"SORF PN 10 DIN 86029 Size DN 40","SORF","PN 10","DIN 86029","1½\"",40.0,150.0,26.0,16.0,88.0,110.0,4.0,18.0,70.0,3.0,49.0,3.0,71,"M16",13.0,1.77]
[null,"SORF PN 10 DIN 86029 Size DN 50","SORF","PN 10","DIN 86029","2\"",50.0,165.0,28.0,18.0,102.0,125.0,4.0,18.0,85.0,3.0,61.1,4.0,76,"M16",13.0,2.4]
[null,"SORF PN 10 DIN 86029 Size DN 65","SORF","PN 10","DIN 86029","2½\"",65.0,185.0,32.0,18.0,122.0,145.0,4.0,18.0,105.0,3.0,77.1,4.0,76,"M16",13.0,3.1]
[null,"SORF PN 10 DIN 86029 Size DN 80","SORF","PN 10","DIN 86029","3\"",80.0,200.0,34.0,20.0,138.0,160.0,8.0,18.0,118.0,3.0,90.3,4.0,80,"M16",13.0,3.8]
[null,"SORF PN 10 DIN 86029 Size DN 100","SORF","PN 10","DIN 86029","4\"",100.0,220.0,38.0,20.0,158.0,180.0,8.0,18.0,140.0,3.0,115.9,5.0,81,"M16",13.0,4.3]
[null,"SORF PN 10 DIN 86029 Size DN 125","SORF","PN 10","DIN 86029","5\"",125.0,250.0,40.0,22.0,188.0,210.0,8.0,18.0,168.0,3.0,141.6,5.0,85,"M16",13.0,5.8]
[null,"SORF PN 10 DIN 86029 Size DN 150","SORF","PN 10","DIN 86029","6\"",150.0,285.0,44.0,22.0,212.0,240.0,8.0,22.0,195.0,3.0,170.5,6.0,92,"M20",16.0,7.1]
[null,"SORF PN 10 DIN 86029 Size DN 175","SORF","PN 10","DIN 86029","7\"",175.0,315.0,44.0,24.0,242.0,270.0,8.0,22.0,224.0,3.0,196.1,6.0,96,"M20",16.0,9.1]
[null,"SORF PN 10 DIN 86029 Size DN 200","SORF","PN 10","DIN 86029","8\"",200.0,340.0,44.0,24.0,268.0,295.0,8.0,22.0,247.0,3.0,222.0,6.0,96,"M20",16.0,9.9]
[null,"SORF PN 10 DIN 86029 Size DN 250","SORF","PN 10","DIN 86029","10\"",250.0,395.0,46.0,26.0,320.0,350.0,12.0,22.0,300.0,3.0,276.0,6.0,100,"M20",16.0,12.7]
[null,"SORF PN 10 DIN 86029 Size DN 300","SORF","PN 10","DIN 86029","12\"",300.0,445.0,46.0,26.0,370.0,400.0,12.0,22.0,352.0,4.0,327.0,6.0,100,"M20",16.0,14.4]
[null,"SORF PN 10 DIN 86029 Size DN 350","SORF","PN 10","DIN 86029","14\"",350.0,505.0,53.0,26.0,430.0,460.0,16.0,22.0,398.0,4.0,359.0,7.0,101,"M20",16.0,22.3]
[null,"SORF PN 10 DIN 86029 Size DN 400","SORF","PN 10","DIN 86029","16\"",400.0,565.0,57.0,26.0,482.0,515.0,16.0,26.0,448.0,4.0,410.0,7.0,107,"M24",19.0,26.7]
[null,"SORF PN 10 DIN 86029 Size DN 450","SORF","PN 10","DIN 86029","18\"",450.0,615.0,62.0,28.0,532.0,565.0,20.0,26.0,502.0,4.0,461.0,7.0,111,"M24",19.0,32.3]
[null,"SORF PN 10 DIN 86029 Size DN 500","SORF","PN 10","DIN 86029","20\"",500.0,670.0,67.0,28.0,585.0,620.0,20.0,26.0,552.0,4.0,512.0,7.0,111,"M24",19.0,37.3]
[null,"SORF PN 10 DIN 86029 Size DN 600","SORF","PN 10","DIN 86029","24\"",600.0,780.0,75.0,28.0,685.0,725.0,20.0,30.0,658.0,5.0,614.0,7.0,117,"M27",22.0,48.3]
[null,"SORF PN 10 DIN 86029 Size DN 700","SORF","PN 10","DIN 86029","28\"",700.0,895.0,77.0,30.0,800.0,840.0,24.0,30.0,760.0,5.0,716.0,7.0,121,"M27",22.0,62.7]
[null,"SORF PN 10 DIN 86029 Size DN 800","SORF","PN 10","DIN 86029","32\"",800.0,1015.0,84.0,32.0,905.0,950.0,24.0,33.0,864.0,5.0,818.0,7.0,129,"M30",24.0,83.4]
[null,"SORF PN 10 DIN 86029 Size DN 900","SORF","PN 10","DIN 86029","36\"",900.0,1115.0,88.0,34.0,1005.0,1050.0,28.0,33.0,969.0,5.0,920.0,7.0,133,"M30",24.0,99.2]
[null,"SORF PN 10 DIN 86029 Size DN 1000","SORF","PN 10","DIN 86029","40\"",1000.0,1230.0,92.0,34.0,1110.0,1160.0,28.0,36.0,1071.0,5.0,1022.0,7.0,139,"M33",27.0,116.8]
[null,"SORF PN 16 DIN 86030 Size DN 10","SORF","PN 16","DIN 86030","1/4\"",10.0,90.0,20.0,14.0,40.0,60.0,4.0,14.0,30.0,2.0,17.7,3.0,61,"M12",10.0,0.56]
[null,"SORF PN 16 DIN 86030 Size DN 15","SORF","PN 16","DIN 86030","1/2\"",15.0,95.0,20.0,14.0,45.0,65.0,4.0,14.0,35.0,2.0,22.0,3.0,61,"M12",10.0,0.64]
[null,"SORF PN 16 DIN 86030 Size DN 20","SORF","PN 16","DIN 86030","3/4\"",20.0,105.0,24.0,16.0,58.0,75.0,4.0,14.0,45.0,2.0,27.6,3.0,65,"M12",10.0,0.98]
[null,"SORF PN 16 DIN 86030 Size DN 25","SORF","PN 16","DIN 86030","1\"",25.0,115.0,24.0,16.0,68.0,85.0,4.0,14.0,52.0,2.0,34.4,3.0,65,"M12",10.0,1.12]
[null,"SORF PN 16 DIN 86030 Size DN 32","SORF","PN 16","DIN 86030","1¼\"",32.0,140.0,26.0,16.0,78.0,100.0,4.0,18.0,60.0,2.0,43.1,3.0,71,"M16",13.0,1.58]
[null,"SORF PN 16 DIN 86030 Size DN 40","SORF","PN 16","DIN 86030","1½\"",40.0,150.0,26.0,16.0,88.0,110.0,4.0,18.0,70.0,3.0,49.0,3.0,71,"M16",13.0,1.77]
[null,"SORF PN 16 DIN 86030 Size DN 50","SORF","PN 16","DIN 86030","2\"",50.0,165.0,28.0,18.0,102.0,125.0,4.0,18.0,85.0,3.0,61.1,4.0,76,"M16",13.0,2.4]
[null,"SORF PN 16 DIN 86030 Size DN 65","SORF","PN 16","DIN 86030","2½\"",65.0,185.0,32.0,18.0,122.0,145.0,4.0,18.0,105.0,3.0,77.1,4.0,76,"M16",13.0,3.1]
[null,"SORF PN 16 DIN 86030 Size DN 80","SORF","PN 16","DIN 86030","3\"",80.0,200.0,34.0,20.0,138.0,160.0,8.0,18.0,118.0,3.0,90.3,4.0,80,"M16",13.0,3.8]
[null,"SORF PN 16 DIN 86030 Size DN 100","SORF","PN 16","DIN 86030","4\"",100.0,220.0,38.0,20.0,158.0,180.0,8.0,18.0,140.0,3.0,115.9,5.0,81,"M16",13.0,4.3]
[null,"SORF PN 16 DIN 86030 Size DN 125","SORF","PN 16","DIN 86030","5\"",125.0,250.0,40.0,22.0,188.0,210.0,8.0,18.0,168.0,3.0,141.6,5.0,85,"M16",13.0,5.8]
[null,"SORF PN 16 DIN 86030 Size DN 150","SORF","PN 16","DIN 86030","6\"",150.0,285.0,44.0,22.0,212.0,240.0,8.0,22.0,195.0,3.0,170.5,6.0,92,"M20",16.0,7.1]
[null,"SORF PN 16 DIN 86030 Size DN 175","SORF","PN 16","DIN 86030","7\"",175.0,315.0,44.0,24.0,242.0,270.0,8.0,22.0,224.0,3.0,196.1,6.0,96,"M20",16.0,9.1]
[null,"SORF PN 16 DIN 86030 Size DN 200","SORF","PN 16","DIN 86030","8\"",200.0,340.0,44.0,24.0,268.0,295.0,12.0,22.0,247.0,3.0,222.0,6.0,96,"M20",16.0,9.7]
[null,"SORF PN 16 DIN 86030 Size DN 250","SORF","PN 16","DIN 86030","10\"",250.0,405.0,46.0,26.0,320.0,355.0,12.0,26.0,300.0,3.0,276.0,6.0,106,"M24",19.0,13.4]
[null,"SORF PN 16 DIN 86030 Size DN 300","SORF","PN 16","DIN 86030","12\"",300.0,460.0,46.0,28.0,378.0,410.0,12.0,26.0,355.0,4.0,327.0,6.0,110,"M24",19.0,17.3]
[null,"SORF PN 16 DIN 86030 Size DN 350","SORF","PN 16","DIN 86030","14\"",350.0,520.0,57.0,30.0,436.0,470.0,16.0,26.0,400.0,4.0,359.0,7.0,115,"M24",19.0,27.6]
[null,"SORF PN 16 DIN 86030 Size DN 400","SORF","PN 16","DIN 86030","16\"",400.0,580.0,63.0,32.0,490.0,525.0,16.0,30.0,457.0,4.0,410.0,7.0,125,"M27",22.0,36.0]
[null,"SORF PN 16 DIN 86030 Size DN 450","SORF","PN 16","DIN 86030","18\"",450.0,640.0,68.0,34.0,550.0,585.0,20.0,30.0,505.0,4.0,461.0,7.0,129,"M27",22.0,44.0]
[null,"SORF PN 16 DIN 86030 Size DN 500","SORF","PN 16","DIN 86030","20\"",500.0,715.0,73.0,34.0,610.0,650.0,20.0,33.0,559.0,4.0,512.0,7.0,133,"M30",24.0,56.4]
[null,"SORF PN 16 DIN 86030 Size DN 600","SORF","PN 16","DIN 86030","24\"",600.0,840.0,83.0,36.0,725.0,770.0,20.0,36.0,664.0,5.0,614.0,7.0,143,"M33",27.0,79.9]
[null,"SORF PN 16 DIN 86030 Size DN 700","SORF","PN 16","DIN 86030","28\"",700.0,910.0,83.0,36.0,795.0,840.0,24.0,36.0,760.0,5.0,716.0,7.0,143,"M33",27.0,75.7]
[null,"SORF PN 16 DIN 86030 Size DN 800","SORF","PN 16","DIN 86030","32\"",800.0,1025.0,90.0,38.0,900.0,950.0,24.0,39.0,864.0,5.0,818.0,7.0,151,"M36",29.0,97.6]
[null,"SORF PN 16 DIN 86030 Size DN 900","SORF","PN 16","DIN 86030","36\"",900.0,1125.0,94.0,40.0,1000.0,1050.0,28.0,39.0,969.0,5.0,920.0,7.0,155,"M36",29.0,114.6]
[null,"SORF PN 16 DIN 86030 Size DN 1000","SORF","PN 16","DIN 86030","40\"",1000.0,1255.0,100.0,42.0,1115.0,1170.0,28.0,42.0,1073.0,5.0,1022.0,7.0,163,"M39",31.0,151.2]
[null,"SO PN 10 DIN 1882 Size DN 25","SO","PN 10","DIN 1882","1\"",25.0,115.0,"-",12.0,"-",85.0,4.0,15.0,"-","-",34.0,3.0,57,"M12",10.0,"-"]
[null,"SO PN 10 DIN 1882 Size DN 32","SO","PN 10","DIN 1882","1¼\"",32.0,140.0,"-",12.0,"-",110.0,4.0,15.0,"-","-",43.0,3.0,57,"M12",10.0,"-"]
[null,"SO PN 10 DIN 1882 Size DN 40","SO","PN 10","DIN 1882","1½\"",40.0,140.0,"-",12.0,"-",110.0,4.0,15.0,"-","-",50.0,3.0,57,"M12",10.0,"-"]
[null,"SO PN 10 DIN 1882 Size DN 50","SO","PN 10","DIN 1882","2\"",50.0,165.0,"-",13.0,102.0,125.0,4.0,18.0,"-","-",59.0,4.0,66,"M16",13.0,"-"]
[null,"SO PN 10 DIN 1882 Size DN 65","SO","PN 10","DIN 1882","2½\"",65.0,185.0,"-",14.0,"-",145.0,4.0,18.0,"-","-",72.0,4.0,68,"M16",13.0,"-"]
[null,"SO PN 10 DIN 1882 Size DN 70","SO","PN 10","DIN 1882","-",70.0,185.0,"-",14.0,"-",145.0,4.0,18.0,"-","-",78.0,4.0,68,"M16",13.0,"-"]
[null,"SO PN 10 DIN 1882 Size DN 80","SO","PN 10","DIN 1882","3\"",80.0,200.0,"-",15.0,138.0,160.0,4.0,18.0,"-","-",91.0,4.0,70,"M16",13.0,"-"]
[null,"SO PN 10 DIN 1882 Size DN 100","SO","PN 10","DIN 1882","4\"",100.0,230.0,"-",16.0,158.0,180.0,4.0,23.0,"-","-",110.0,5.0,79,"M20",16.0,"-"]
[null,"SO PN 10 DIN 1882 Size DN 125","SO","PN 10","DIN 1882","5\"",125.0,260.0,"-",17.0,188.0,210.0,4.0,23.0,"-","-",135.0,5.0,81,"M20",16.0,"-"]
[null,"SO PN 10 DIN 1882 Size DN 150","SO","PN 10","DIN 1882","6\"",150.0,290.0,"-",18.0,212.0,240.0,6.0,23.0,"-","-",161.0,6.0,84,"M20",16.0,"-"]
[null,"SO PN 10 DIN 1882 Size DN 200","SO","PN 10","DIN 1882","8\"",200.0,350.0,"-",20.0,268.0,300.0,6.0,23.0,"-","-",221.0,6.0,88,"M20",16.0,"-"]
[null,"SO PN 10 DIN 1882 Size DN 250","SO","PN 10","DIN 1882","10\"",250.0,400.0,"-",22.0,320.0,350.0,8.0,23.0,"-","-",275.0,6.0,92,"M20",16.0,"-"]
[null,"SO PN 10 DIN 1882 Size DN 300","SO","PN 10","DIN 1882","12\"",300.0,450.0,"-",24.0,370.0,400.0,8.0,23.0,"-","-",326.0,6.0,96,"M20",16.0,"-"]
[null,"SO PN 10 DIN 1882 Size DN 350","SO","PN 10","DIN 1882","14\"",350.0,520.0,"-",26.0,430.0,465.0,10.0,27.0,"-","-",358.0,7.0,107,"M24",19.0,"-"]
[null,"SO PN 10 DIN 1882 Size DN 400","SO","PN 10","DIN 1882","16\"",400.0,575.0,"-",26.0,482.0,520.0,10.0,27.0,"-","-",409.0,7.0,107,"M24",19.0,"-"]
[null,"SO PN 10 DIN 1882 Size DN 450","SO","PN 10","DIN 1882","18\"",450.0,630.0,"-",28.0,532.0,570.0,12.0,27.0,"-","-",459.0,7.0,111,"M24",19.0,"-"]
[null,"SO PN 10 DIN 1882 Size DN 500","SO","PN 10","DIN 1882","20\"",500.0,680.0,"-",30.0,585.0,625.0,12.0,27.0,"-","-",510.0,7.0,115,"M24",19.0,"-"]
[null,"SO PN 10 DIN 1882 Size DN 550","SO","PN 10","DIN 1882","22\"",550.0,550.0,"-",32.0,"-",675.0,14.0,30.0,"-","-",561.0,7.0,125,"M27",22.0,"-"]
[null,"SO PN 10 DIN 1882 Size DN 600","SO","PN 10","DIN 1882","24\"",600.0,790.0,"-",32.0,685.0,725.0,16.0,30.0,"-","-",612.0,7.0,125,"M27",22.0,"-"]
[null,"SO PN 10 DIN 1882 Size DN 700","SO","PN 10","DIN 1882","28\"",700.0,900.0,"-",38.0,800.0,830.0,18.0,30.0,"-","-",716.0,7.0,137,"M27",22.0,"-"]
[null,"SO PN 10 DIN 1882 Size DN 800","SO","PN 10","DIN 1882","32\"",800.0,1015.0,"-","-",905.0,940.0,20.0,33.0,"-","-","-",7.0,"-","M30",24.0,"-"]
[null,"SO PN 10 DIN 1882 Size DN 900","SO","PN 10","DIN 1882","36\"",900.0,1120.0,"-","-",1005.0,1040.0,22.0,33.0,"-","-","-",7.0,"-","M30",24.0,"-"]
[null,"SO PN 10 DIN 1882 Size DN 1000","SO","PN 10","DIN 1882","40\"",1000.0,1220.0,"-","-",1110.0,1140.0,24.0,33.0,"-","-","-",7.0,"-","M30",24.0,"-"]
[null,"SO PN 10 DIN 1882 Size DN 1200","SO","PN 10","DIN 1882","48\"",1200.0,1430.0,"-","-",1330.0,1350.0,28.0,33.0,"-","-","-",7.0,"-","M30",24.0,"-"]
[null,"SO Pr.less vessel DIN 28031 Size DN 300","SO","Pr.less vessel","DIN 28031","12\"",300.0,415.0,"-",20.0,"-",375.0,12.0,18.0,"-","-",326.0,6.0,{"$f":"(J955+U955+5)*2+R955","v":82},"M16",13.0,7.9]
[null,"SO Pr.less vessel DIN 28031 Size DN 350","SO","Pr.less vessel","DIN 28031","14\"",350.0,460.0,"-",20.0,"-",420.0,16.0,18.0,"-","-",357.0,7.0,83,"M16",13.0,8.7]
[null,"SO Pr.less vessel DIN 28031 Size DN 400","SO","Pr.less vessel","DIN 28031","16\"",400.0,510.0,"-",20.0,"-",470.0,16.0,18.0,"-","-",408.0,7.0,83,"M16",13.0,9.7]
[null,"SO Pr.less vessel DIN 28031 Size DN 500","SO","Pr.less vessel","DIN 28031","20\"",500.0,600.0,"-",20.0,"-",560.0,20.0,18.0,"-","-",510.0,7.0,83,"M16",13.0,11.5]
[null,"SO Pr.less vessel DIN 28031 Size DN 600","SO","Pr.less vessel","DIN 28031","24\"",600.0,700.0,"-",20.0,"-",660.0,24.0,18.0,"-","-",602.0,7.0,83,"M16",13.0,14.8]
[null,"SO Pr.less vessel DIN 28031 Size DN 700","SO","Pr.less vessel","DIN 28031","28\"",700.0,800.0,"-",20.0,"-",760.0,28.0,18.0,"-","-",702.0,7.0,83,"M16",13.0,17.0]
[null,"SO Pr.less vessel DIN 28031 Size DN 800","SO","Pr.less vessel","DIN 28031","32\"",800.0,900.0,"-",20.0,"-",860.0,32.0,18.0,"-","-",802.0,7.0,83,"M16",13.0,19.3]
[null,"SO Pr.less vessel DIN 28031 Size DN 900","SO","Pr.less vessel","DIN 28031","36\"",900.0,1000.0,"-",20.0,"-",960.0,36.0,18.0,"-","-",902.0,7.0,83,"M16",13.0,21.6]
[null,"SO Pr.less vessel DIN 28031 Size DN 1000","SO","Pr.less vessel","DIN 28031","40\"",1000.0,1100.0,"-",20.0,"-",1060.0,40.0,18.0,"-","-",1002.0,7.0,83,"M16",13.0,23.8]
[null,"SO Pr.less vessel DIN 28031 Size DN 1100","SO","Pr.less vessel","DIN 28031","44\"",1100.0,1200.0,"-",20.0,"-",1160.0,44.0,18.0,"-","-",1102.0,7.0,83,"M16",13.0,26.0]
[null,"SO Pr.less vessel DIN 28031 Size DN 1200","SO","Pr.less vessel","DIN 28031","48\"",1200.0,1320.0,"-",25.0,"-",1270.0,48.0,18.0,"-","-",1202.0,7.0,93,"M16",13.0,43.4]
[null,"SO Pr.less vessel DIN 28031 Size DN 1300","SO","Pr.less vessel","DIN 28031","52\"",1300.0,1420.0,"-",25.0,"-",1370.0,48.0,18.0,"-","-",1303.0,7.0,93,"M16",13.0,47.0]
[null,"SO Pr.less vessel DIN 28031 Size DN 1400","SO","Pr.less vessel","DIN 28031","56\"",1400.0,1520.0,"-",25.0,"-",1470.0,48.0,18.0,"-","-",1403.0,7.0,93,"M16",13.0,50.4]
[null,"SO Pr.less vessel DIN 28031 Size DN 1500","SO","Pr.less vessel","DIN 28031","60\"",1500.0,1620.0,"-",25.0,"-",1570.0,52.0,18.0,"-","-",1503.0,7.0,93,"M16",13.0,53.8]
[null,"SO Pr.less vessel DIN 28031 Size DN 1600","SO","Pr.less vessel","DIN 28031","64\"",1600.0,1720.0,"-",25.0,"-",1670.0,56.0,18.0,"-","-",1603.0,7.0,93,"M16",13.0,57.2]
[null,"SO Pr.less vessel DIN 28031 Size DN 1700","SO","Pr.less vessel","DIN 28031","68\"",1700.0,1820.0,"-",25.0,"-",1770.0,56.0,18.0,"-","-",1703.0,7.0,93,"M16",13.0,60.6]
[null,"SO Pr.less vessel DIN 28031 Size DN 1800","SO","Pr.less vessel","DIN 28031","72\"",1800.0,1920.0,"-",30.0,"-",1870.0,56.0,23.0,"-","-",1803.0,7.0,109,"M20",16.0,75.5]
[null,"SO Pr.less vessel DIN 28031 Size DN 2000","SO","Pr.less vessel","DIN 28031","80\"",2000.0,2120.0,"-",30.0,"-",2070.0,64.0,23.0,"-","-",2003.0,7.0,109,"M20",16.0,82.9]
[null,"SO Pr.less vessel DIN 28031 Size DN 2200","SO","Pr.less vessel","DIN 28031","88\"",2200.0,2320.0,"-",30.0,"-",2270.0,72.0,23.0,"-","-",2203.0,7.0,109,"M20",16.0,91.1]
[null,"SO Pr.less vessel DIN 28031 Size DN 2400","SO","Pr.less vessel","DIN 28031","96\"",2400.0,2520.0,"-",30.0,"-",2475.0,72.0,23.0,"-","-",2403.0,7.0,109,"M20",16.0,101.0]
[null,"SO Pr.less vessel DIN 28031 Size DN 2600","SO","Pr.less vessel","DIN 28031","108\"",2600.0,2720.0,"-",30.0,"-",2675.0,80.0,23.0,"-","-",2603.0,7.0,109,"M20",16.0,109.0]
[null,"SO Pr.less vessel DIN 28031 Size DN 2800","SO","Pr.less vessel","DIN 28031","116\"",2800.0,2920.0,"-",30.0,"-",2875.0,88.0,23.0,"-","-",2803.0,7.0,109,"M20",16.0,116.0]
[null,"SO Pr.less vessel DIN 28031 Size DN 3000","SO","Pr.less vessel","DIN 28031","120\"",3000.0,3120.0,"-",30.0,"-",3075.0,96.0,23.0,"-","-",3003.0,7.0,109,"M20",16.0,123.0]
[null,"SO Pr.less vessel DIN 28031 Size DN 3200","SO","Pr.less vessel","DIN 28031","128\"",3200.0,3320.0,"-",30.0,"-",3275.0,96.0,23.0,"-","-",3203.0,7.0,109,"M20",16.0,132.0]
[null,"SO Pr.less vessel DIN 28031 Size DN 3400","SO","Pr.less vessel","DIN 28031","136\"",3400.0,3540.0,"-",40.0,"-",3490.0,104.0,23.0,"-","-",3403.0,7.0,129,"M20",16.0,222.0]
[null,"SO Pr.less vessel DIN 28031 Size DN 3600","SO","Pr.less vessel","DIN 28031","144\"",3600.0,3740.0,"-",40.0,"-",3690.0,112.0,23.0,"-","-",3603.0,7.0,129,"M20",16.0,233.0]
[null,"SO Pr.less vessel DIN 28031 Size DN 3800","SO","Pr.less vessel","DIN 28031","152\"",3800.0,3940.0,"-",40.0,"-",3890.0,112.0,23.0,"-","-",3803.0,7.0,129,"M20",16.0,247.0]
[null,"SO Pr.less vessel DIN 28031 Size DN 4000","SO","Pr.less vessel","DIN 28031","160\"",4000.0,4140.0,"-",40.0,"-",4090.0,120.0,23.0,"-","-",4003.0,7.0,129,"M20",16.0,260.0]
[null,{"$f":"CONCATENATE(C983,$C$2,D983,$C$2,E983,$C$2,$C$2,$G$2,$C$2,G983,$A$2,J983)","v":"SO Cst. Pr.less vessel DIN 28032  DN 300 / 25"},"SO Cst.","Pr.less vessel","DIN 28032","12\"",300.0,415.0,"-",25.0,"-",375.0,12.0,18.0,"-","-",326.0,6.0,92,"M16",13.0,10.1]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 300 / 30","SO Cst.","Pr.less vessel","DIN 28032","12\"",300.0,430.0,"-",30.0,"-",385.0,12.0,23.0,"-","-",326.0,6.0,108,"M20",16.0,13.9]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 300 / 40","SO Cst.","Pr.less vessel","DIN 28032","12\"",300.0,445.0,"-",40.0,"-",395.0,12.0,27.0,"-","-",326.0,6.0,134,"M24",19.0,21.2]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 350 / 25","SO Cst.","Pr.less vessel","DIN 28032","14\"",350.0,460.0,"-",25.0,"-",420.0,16.0,18.0,"-","-",357.0,7.0,93,"M16",13.0,11.2]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 350 / 35","SO Cst.","Pr.less vessel","DIN 28032","14\"",350.0,475.0,"-",35.0,"-",430.0,16.0,23.0,"-","-",357.0,7.0,119,"M20",16.0,18.1]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 350 / 45","SO Cst.","Pr.less vessel","DIN 28032","14\"",350.0,490.0,"-",45.0,"-",440.0,16.0,27.0,"-","-",357.0,7.0,145,"M24",19.0,26.1]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 400 / 25","SO Cst.","Pr.less vessel","DIN 28032","16\"",400.0,510.0,"-",25.0,"-",470.0,16.0,18.0,"-","-",408.0,7.0,93,"M16",13.0,12.5]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 400 / 35","SO Cst.","Pr.less vessel","DIN 28032","16\"",400.0,525.0,"-",35.0,"-",480.0,16.0,23.0,"-","-",408.0,7.0,119,"M20",16.0,20.2]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 400 / 45","SO Cst.","Pr.less vessel","DIN 28032","16\"",400.0,545.0,"-",45.0,"-",495.0,16.0,27.0,"-","-",408.0,7.0,145,"M24",19.0,31.5]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 500 / 30","SO Cst.","Pr.less vessel","DIN 28032","20\"",500.0,600.0,"-",30.0,"-",560.0,20.0,18.0,"-","-",510.0,7.0,103,"M16",13.0,18.1]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 500 / 35","SO Cst.","Pr.less vessel","DIN 28032","20\"",500.0,615.0,"-",35.0,"-",570.0,20.0,23.0,"-","-",510.0,7.0,119,"M20",16.0,24.1]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 500 / 45","SO Cst.","Pr.less vessel","DIN 28032","20\"",500.0,635.0,"-",45.0,"-",585.0,20.0,27.0,"-","-",510.0,7.0,145,"M24",19.0,37.0]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 600 / 30","SO Cst.","Pr.less vessel","DIN 28032","24\"",600.0,700.0,"-",30.0,"-",660.0,24.0,18.0,"-","-",602.0,7.0,103,"M16",13.0,22.9]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 600 / 35","SO Cst.","Pr.less vessel","DIN 28032","24\"",600.0,710.0,"-",35.0,"-",665.0,24.0,23.0,"-","-",602.0,7.0,119,"M20",16.0,29.4]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 600 / 50","SO Cst.","Pr.less vessel","DIN 28032","24\"",600.0,730.0,"-",50.0,"-",680.0,24.0,27.0,"-","-",602.0,7.0,155,"M24",19.0,49.3]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 700 / 30","SO Cst.","Pr.less vessel","DIN 28032","28\"",700.0,800.0,"-",30.0,"-",760.0,28.0,18.0,"-","-",702.0,7.0,103,"M16",13.0,26.5]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 700 / 40","SO Cst.","Pr.less vessel","DIN 28032","28\"",700.0,810.0,"-",40.0,"-",765.0,28.0,23.0,"-","-",702.0,7.0,129,"M20",16.0,37.9]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 700 / 50","SO Cst.","Pr.less vessel","DIN 28032","28\"",700.0,830.0,"-",50.0,"-",780.0,28.0,27.0,"-","-",702.0,7.0,155,"M24",19.0,56.6]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 800 / 30","SO Cst.","Pr.less vessel","DIN 28032","32\"",800.0,900.0,"-",30.0,"-",860.0,32.0,18.0,"-","-",802.0,7.0,103,"M16",13.0,30.1]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 800 / 40","SO Cst.","Pr.less vessel","DIN 28032","32\"",800.0,915.0,"-",40.0,"-",870.0,32.0,23.0,"-","-",802.0,7.0,129,"M20",16.0,44.8]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 800 / 55","SO Cst.","Pr.less vessel","DIN 28032","32\"",800.0,930.0,"-",55.0,"-",880.0,32.0,27.0,"-","-",802.0,7.0,165,"M24",19.0,70.1]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 900 / 40","SO Cst.","Pr.less vessel","DIN 28032","36\"",900.0,1015.0,"-",40.0,"-",970.0,36.0,23.0,"-","-",902.0,7.0,129,"M20",16.0,50.1]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 900 / 60","SO Cst.","Pr.less vessel","DIN 28032","36\"",900.0,1030.0,"-",60.0,"-",980.0,36.0,27.0,"-","-",902.0,7.0,175,"M24",19.0,85.4]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 1000 / 45","SO Cst.","Pr.less vessel","DIN 28032","40\"",1000.0,1115.0,"-",45.0,"-",1070.0,40.0,23.0,"-","-",1002.0,7.0,139,"M20",16.0,62.8]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 1000 / 60","SO Cst.","Pr.less vessel","DIN 28032","40\"",1000.0,1130.0,"-",60.0,"-",1080.0,40.0,27.0,"-","-",1002.0,7.0,175,"M24",19.0,94.1]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 1100 / 45","SO Cst.","Pr.less vessel","DIN 28032","44\"",1100.0,1215.0,"-",45.0,"-",1170.0,44.0,23.0,"-","-",1102.0,7.0,139,"M20",16.0,68.5]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 1100 / 65","SO Cst.","Pr.less vessel","DIN 28032","44\"",1100.0,1230.0,"-",65.0,"-",1180.0,44.0,27.0,"-","-",1102.0,7.0,185,"M24",19.0,112.0]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 1200 / 45","SO Cst.","Pr.less vessel","DIN 28032","48\"",1200.0,1315.0,"-",45.0,"-",1270.0,48.0,23.0,"-","-",1202.0,7.0,139,"M20",16.0,75.5]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 1200 / 65","SO Cst.","Pr.less vessel","DIN 28032","48\"",1200.0,1330.0,"-",65.0,"-",1280.0,48.0,27.0,"-","-",1202.0,7.0,185,"M24",19.0,121.0]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 1300 / 45","SO Cst.","Pr.less vessel","DIN 28032","52\"",1300.0,1415.0,"-",45.0,"-",1370.0,52.0,23.0,"-","-",1303.0,7.0,139,"M20",16.0,80.9]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 1300 / 70","SO Cst.","Pr.less vessel","DIN 28032","52\"",1300.0,1435.0,"-",70.0,"-",1385.0,52.0,27.0,"-","-",1303.0,7.0,195,"M24",19.0,146.0]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 1400 / 45","SO Cst.","Pr.less vessel","DIN 28032","56\"",1400.0,1515.0,"-",45.0,"-",1470.0,56.0,23.0,"-","-",1403.0,7.0,139,"M20",16.0,86.8]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 1400 / 70","SO Cst.","Pr.less vessel","DIN 28032","56\"",1400.0,1535.0,"-",70.0,"-",1485.0,56.0,27.0,"-","-",1403.0,7.0,195,"M24",19.0,157.0]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 1500 / 50","SO Cst.","Pr.less vessel","DIN 28032","60\"",1500.0,1615.0,"-",50.0,"-",1570.0,60.0,23.0,"-","-",1503.0,7.0,149,"M20",16.0,103.0]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 1500 / 70","SO Cst.","Pr.less vessel","DIN 28032","60\"",1500.0,1635.0,"-",70.0,"-",1585.0,60.0,27.0,"-","-",1503.0,7.0,195,"M24",19.0,167.0]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 1600 / 55","SO Cst.","Pr.less vessel","DIN 28032","64\"",1600.0,1715.0,"-",55.0,"-",1670.0,64.0,23.0,"-","-",1603.0,7.0,159,"M20",16.0,120.0]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 1600 / 70","SO Cst.","Pr.less vessel","DIN 28032","64\"",1600.0,1735.0,"-",70.0,"-",1685.0,64.0,27.0,"-","-",1603.0,7.0,195,"M24",19.0,178.0]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 1700 / 55","SO Cst.","Pr.less vessel","DIN 28032","68\"",1700.0,1815.0,"-",55.0,"-",1770.0,68.0,23.0,"-","-",1703.0,7.0,159,"M20",16.0,128.0]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 1700 / 75","SO Cst.","Pr.less vessel","DIN 28032","68\"",1700.0,1835.0,"-",75.0,"-",1785.0,68.0,27.0,"-","-",1703.0,7.0,205,"M24",19.0,202.0]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 1800 / 55","SO Cst.","Pr.less vessel","DIN 28032","72\"",1800.0,1915.0,"-",55.0,"-",1870.0,72.0,23.0,"-","-",1803.0,7.0,159,"M20",16.0,134.0]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 1800 / 80","SO Cst.","Pr.less vessel","DIN 28032","72\"",1800.0,1940.0,"-",80.0,"-",1890.0,72.0,27.0,"-","-",1803.0,7.0,215,"M24",19.0,236.0]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 2000 / 55","SO Cst.","Pr.less vessel","DIN 28032","80\"",2000.0,2115.0,"-",55.0,"-",2070.0,80.0,23.0,"-","-",2003.0,7.0,159,"M20",16.0,150.0]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 2000 / 80","SO Cst.","Pr.less vessel","DIN 28032","80\"",2000.0,2140.0,"-",80.0,"-",2090.0,80.0,27.0,"-","-",2003.0,7.0,215,"M24",19.0,260.0]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 2200 / 60","SO Cst.","Pr.less vessel","DIN 28032","88\"",2200.0,2315.0,"-",60.0,"-",2270.0,88.0,23.0,"-","-",2203.0,7.0,169,"M20",16.0,178.0]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 2200 / 90","SO Cst.","Pr.less vessel","DIN 28032","88\"",2200.0,2340.0,"-",90.0,"-",2290.0,88.0,27.0,"-","-",2203.0,7.0,235,"M24",19.0,232.0]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 2400 / 60","SO Cst.","Pr.less vessel","DIN 28032","96\"",2400.0,2520.0,"-",60.0,"-",2475.0,96.0,23.0,"-","-",2403.0,7.0,169,"M20",16.0,203.0]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 2400 / 85","SO Cst.","Pr.less vessel","DIN 28032","96\"",2400.0,2540.0,"-",85.0,"-",2490.0,96.0,27.0,"-","-",2403.0,7.0,225,"M24",19.0,334.0]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 2600 / 60","SO Cst.","Pr.less vessel","DIN 28032","108\"",2600.0,2720.0,"-",60.0,"-",2675.0,104.0,23.0,"-","-",2603.0,7.0,169,"M20",16.0,220.0]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 2600 / 95","SO Cst.","Pr.less vessel","DIN 28032","108\"",2600.0,2745.0,"-",95.0,"-",2695.0,104.0,27.0,"-","-",2603.0,7.0,245,"M24",19.0,417.0]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 2800 / 65","SO Cst.","Pr.less vessel","DIN 28032","116\"",2800.0,2920.0,"-",65.0,"-",2875.0,112.0,23.0,"-","-",2803.0,7.0,179,"M20",16.0,255.0]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 2800 / 100","SO Cst.","Pr.less vessel","DIN 28032","116\"",2800.0,2950.0,"-",100.0,"-",2900.0,112.0,27.0,"-","-",2803.0,7.0,255,"M24",19.0,490.0]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 3000 / 70","SO Cst.","Pr.less vessel","DIN 28032","120\"",3000.0,3120.0,"-",70.0,"-",3075.0,120.0,23.0,"-","-",3003.0,7.0,189,"M20",16.0,297.0]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 3000 / 95","SO Cst.","Pr.less vessel","DIN 28032","120\"",3000.0,3150.0,"-",95.0,"-",3100.0,120.0,27.0,"-","-",3003.0,7.0,245,"M24",19.0,496.0]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 3200 / 75","SO Cst.","Pr.less vessel","DIN 28032","128\"",3200.0,3320.0,"-",75.0,"-",3275.0,128.0,23.0,"-","-",3203.0,7.0,199,"M20",16.0,336.0]
[null,"SO Cst. Pr.less vessel DIN 28032  DN 3200 / 100","SO Cst.","Pr.less vessel","DIN 28032","128\"",3200.0,3350.0,"-",100.0,"-",3300.0,128.0,27.0,"-","-",3203.0,7.0,255,"M24",19.0,558.0]
[null,"SO St.steel Pr.vessel DIN 28036  DN 300 / 25","SO","St.steel Pr.vessel","DIN 28036","12\"",300.0,415.0,"-",25.0,"-",375.0,12.0,18.0,"-","-",326.0,6.0,92,"M16",13.0,9.7]
[null,"SO St.steel Pr.vessel DIN 28036  DN 300 / 30","SO","St.steel Pr.vessel","DIN 28036","12\"",300.0,430.0,"-",30.0,"-",385.0,12.0,23.0,"-","-",326.0,6.0,108,"M20",16.0,13.5]
[null,"SO St.steel Pr.vessel DIN 28036  DN 300 / 40","SO","St.steel Pr.vessel","DIN 28036","12\"",300.0,445.0,"-",40.0,"-",395.0,12.0,27.0,"-","-",326.0,6.0,134,"M24",19.0,20.5]
[null,"SO St.steel Pr.vessel DIN 28036  DN 350 / 25","SO","St.steel Pr.vessel","DIN 28036","14\"",350.0,460.0,"-",25.0,"-",420.0,16.0,18.0,"-","-",370.0,7.0,93,"M16",13.0,10.7]
[null,"SO St.steel Pr.vessel DIN 28036  DN 350 / 35","SO","St.steel Pr.vessel","DIN 28036","14\"",350.0,475.0,"-",35.0,"-",430.0,16.0,23.0,"-","-",370.0,7.0,119,"M20",16.0,17.4]
[null,"SO St.steel Pr.vessel DIN 28036  DN 350 / 45","SO","St.steel Pr.vessel","DIN 28036","14\"",350.0,490.0,"-",45.0,"-",440.0,16.0,27.0,"-","-",370.0,7.0,145,"M24",19.0,25.3]
[null,"SO St.steel Pr.vessel DIN 28036  DN 400 / 25","SO","St.steel Pr.vessel","DIN 28036","16\"",400.0,510.0,"-",25.0,"-",470.0,16.0,18.0,"-","-",421.0,7.0,93,"M16",13.0,12.1]
[null,"SO St.steel Pr.vessel DIN 28036  DN 400 / 35","SO","St.steel Pr.vessel","DIN 28036","16\"",400.0,525.0,"-",35.0,"-",480.0,16.0,23.0,"-","-",421.0,7.0,119,"M20",16.0,19.4]
[null,"SO St.steel Pr.vessel DIN 28036  DN 400 / 45","SO","St.steel Pr.vessel","DIN 28036","16\"",400.0,545.0,"-",45.0,"-",495.0,16.0,27.0,"-","-",421.0,7.0,145,"M24",19.0,30.2]
[null,"SO St.steel Pr.vessel DIN 28036  DN 450 / 3","SO","St.steel Pr.vessel","DIN 28036","18\"",450.0,550.0,"-",3.0,"-",510.0,20.0,18.0,"-","-",459.0,7.0,49,"M16",13.0,15.6]
[null,"SO St.steel Pr.vessel DIN 28036  DN 400 / 35","SO","St.steel Pr.vessel","DIN 28036","18\"",400.0,565.0,"-",35.0,"-",520.0,20.0,23.0,"-","-",459.0,7.0,119,"M20",16.0,21.2]
[null,"SO St.steel Pr.vessel DIN 28036  DN 400 / 45","SO","St.steel Pr.vessel","DIN 28036","18\"",400.0,580.0,"-",45.0,"-",530.0,20.0,27.0,"-","-",459.0,7.0,145,"M24",19.0,31.0]
[null,"SO St.steel Pr.vessel DIN 28036  DN 500 / 30","SO","St.steel Pr.vessel","DIN 28036","20\"",500.0,600.0,"-",30.0,"-",560.0,20.0,18.0,"-","-",510.0,7.0,103,"M16",13.0,17.2]
[null,"SO St.steel Pr.vessel DIN 28036  DN 500 / 35","SO","St.steel Pr.vessel","DIN 28036","20\"",500.0,615.0,"-",35.0,"-",570.0,20.0,23.0,"-","-",510.0,7.0,119,"M20",16.0,23.2]
[null,"SO St.steel Pr.vessel DIN 28036  DN 500 / 40","SO","St.steel Pr.vessel","DIN 28036","20\"",500.0,635.0,"-",40.0,"-",585.0,20.0,27.0,"-","-",510.0,7.0,135,"M24",19.0,31.7]
[null,"SO St.steel Pr.vessel DIN 28036  DN 500 / 50","SO","St.steel Pr.vessel","DIN 28036","20\"",500.0,645.0,"-",50.0,"-",590.0,20.0,30.0,"-","-",510.0,7.0,161,"M27",22.0,42.6]
[null,"SO St.steel Pr.vessel DIN 28036  DN 600 / 30","SO","St.steel Pr.vessel","DIN 28036","24\"",600.0,700.0,"-",30.0,"-",660.0,24.0,18.0,"-","-",602.0,7.0,103,"M16",13.0,22.1]
[null,"SO St.steel Pr.vessel DIN 28036  DN 600 / 40","SO","St.steel Pr.vessel","DIN 28036","24\"",600.0,710.0,"-",40.0,"-",665.0,24.0,23.0,"-","-",602.0,7.0,129,"M20",16.0,31.9]
[null,"SO St.steel Pr.vessel DIN 28036  DN 600 / 45","SO","St.steel Pr.vessel","DIN 28036","24\"",600.0,730.0,"-",45.0,"-",680.0,24.0,27.0,"-","-",602.0,7.0,145,"M24",19.0,42.4]
[null,"SO St.steel Pr.vessel DIN 28036  DN 600 / 50","SO","St.steel Pr.vessel","DIN 28036","24\"",600.0,745.0,"-",50.0,"-",690.0,24.0,30.0,"-","-",602.0,7.0,161,"M27",22.0,52.3]
[null,"SO St.steel Pr.vessel DIN 28036  DN 600 / 55","SO","St.steel Pr.vessel","DIN 28036","24\"",600.0,760.0,"-",55.0,"-",695.0,24.0,33.0,"-","-",602.0,7.0,175,"M30",24.0,64.1]
[null,"SO St.steel Pr.vessel DIN 28036  DN 700 / 30","SO","St.steel Pr.vessel","DIN 28036","28\"",700.0,800.0,"-",30.0,"-",760.0,28.0,18.0,"-","-",702.0,7.0,103,"M16",13.0,25.5]
[null,"SO St.steel Pr.vessel DIN 28036  DN 700 / 40","SO","St.steel Pr.vessel","DIN 28036","28\"",700.0,810.0,"-",40.0,"-",765.0,28.0,23.0,"-","-",702.0,7.0,129,"M20",16.0,36.6]
[null,"SO St.steel Pr.vessel DIN 28036  DN 700 / 45","SO","St.steel Pr.vessel","DIN 28036","28\"",700.0,830.0,"-",45.0,"-",780.0,28.0,27.0,"-","-",702.0,7.0,145,"M24",19.0,48.5]
[null,"SO St.steel Pr.vessel DIN 28036  DN 700 / 55","SO","St.steel Pr.vessel","DIN 28036","28\"",700.0,845.0,"-",55.0,"-",790.0,28.0,30.0,"-","-",702.0,7.0,171,"M27",22.0,72.7]
[null,"SO St.steel Pr.vessel DIN 28036  DN 700 / 65","SO","St.steel Pr.vessel","DIN 28036","28\"",700.0,865.0,"-",65.0,"-",800.0,28.0,33.0,"-","-",702.0,7.0,195,"M30",24.0,89.7]
[null,"SO St.steel Pr.vessel DIN 28036  DN 800 / 30","SO","St.steel Pr.vessel","DIN 28036","32\"",800.0,900.0,"-",30.0,"-",860.0,32.0,18.0,"-","-",802.0,7.0,103,"M16",13.0,29.0]
[null,"SO St.steel Pr.vessel DIN 28036  DN 800 / 40","SO","St.steel Pr.vessel","DIN 28036","32\"",800.0,915.0,"-",40.0,"-",870.0,32.0,23.0,"-","-",802.0,7.0,129,"M20",16.0,43.6]
[null,"SO St.steel Pr.vessel DIN 28036  DN 800 / 50","SO","St.steel Pr.vessel","DIN 28036","32\"",800.0,930.0,"-",50.0,"-",880.0,32.0,27.0,"-","-",802.0,7.0,155,"M24",19.0,61.0]
[null,"SO St.steel Pr.vessel DIN 28036  DN 800 / 65","SO","St.steel Pr.vessel","DIN 28036","32\"",800.0,945.0,"-",65.0,"-",890.0,32.0,30.0,"-","-",802.0,7.0,191,"M27",22.0,88.4]
[null,"SO St.steel Pr.vessel DIN 28036  DN 800 / 75","SO","St.steel Pr.vessel","DIN 28036","32\"",800.0,965.0,"-",75.0,"-",900.0,32.0,33.0,"-","-",802.0,7.0,215,"M30",24.0,117.0]
[null,"SO St.steel Pr.vessel DIN 28036  DN 900 / 40","SO","St.steel Pr.vessel","DIN 28036","36\"",900.0,1015.0,"-",40.0,"-",970.0,36.0,23.0,"-","-",902.0,7.0,129,"M20",16.0,48.5]
[null,"SO St.steel Pr.vessel DIN 28036  DN 900 / 60","SO","St.steel Pr.vessel","DIN 28036","36\"",900.0,1030.0,"-",60.0,"-",980.0,36.0,27.0,"-","-",902.0,7.0,175,"M24",19.0,81.8]
[null,"SO St.steel Pr.vessel DIN 28036  DN 900 / 65","SO","St.steel Pr.vessel","DIN 28036","36\"",900.0,1045.0,"-",65.0,"-",990.0,36.0,30.0,"-","-",902.0,7.0,191,"M27",22.0,99.0]
[null,"SO St.steel Pr.vessel DIN 28036  DN 900 / 75","SO","St.steel Pr.vessel","DIN 28036","36\"",900.0,1065.0,"-",75.0,"-",1000.0,36.0,33.0,"-","-",902.0,7.0,215,"M30",24.0,130.0]
[null,"SO St.steel Pr.vessel DIN 28036  DN 1000 / 45","SO","St.steel Pr.vessel","DIN 28036","40\"",1000.0,1115.0,"-",45.0,"-",1070.0,40.0,23.0,"-","-",1002.0,7.0,139,"M20",16.0,60.6]
[null,"SO St.steel Pr.vessel DIN 28036  DN 1000 / 60","SO","St.steel Pr.vessel","DIN 28036","40\"",1000.0,1130.0,"-",60.0,"-",1080.0,40.0,27.0,"-","-",1002.0,7.0,175,"M24",19.0,90.2]
[null,"SO St.steel Pr.vessel DIN 28036  DN 1100 / 45","SO","St.steel Pr.vessel","DIN 28036","44\"",1100.0,1215.0,"-",45.0,"-",1170.0,44.0,23.0,"-","-",1102.0,7.0,139,"M20",16.0,66.1]
[null,"SO St.steel Pr.vessel DIN 28036  DN 1200 / 45","SO","St.steel Pr.vessel","DIN 28036","48\"",1200.0,1315.0,"-",45.0,"-",1270.0,48.0,23.0,"-","-",1202.0,7.0,139,"M20",16.0,71.5]
[null,"SO St.steel Pr.vessel DIN 28036  DN 1300 / 50","SO","St.steel Pr.vessel","DIN 28036","52\"",1300.0,1415.0,"-",50.0,"-",1370.0,52.0,23.0,"-","-",1303.0,7.0,149,"M20",16.0,85.5]
[null,"SO St.steel Pr.vessel DIN 28036  DN 1400 / 50","SO","St.steel Pr.vessel","DIN 28036","56\"",1400.0,1515.0,"-",50.0,"-",1470.0,56.0,23.0,"-","-",1403.0,7.0,149,"M20",16.0,91.2]
[null,"SO St.steel Pr.vessel DIN 28036  DN 1500 / 55","SO","St.steel Pr.vessel","DIN 28036","60\"",1500.0,1615.0,"-",55.0,"-",1570.0,60.0,23.0,"-","-",1503.0,7.0,159,"M20",16.0,107.0]
[null,"SO St.steel Pr.vessel DIN 28036  DN 1600 / 55","SO","St.steel Pr.vessel","DIN 28036","64\"",1600.0,1715.0,"-",55.0,"-",1670.0,64.0,23.0,"-","-",1603.0,7.0,159,"M20",16.0,115.0]
[null,"SO St.steel Pr.vessel DIN 28036  DN 1700 / 55","SO","St.steel Pr.vessel","DIN 28036","68\"",1700.0,1815.0,"-",55.0,"-",1770.0,68.0,23.0,"-","-",1703.0,7.0,159,"M20",16.0,122.0]
[null,"SO St.steel Pr.vessel DIN 28036  DN 1800 / 55","SO","St.steel Pr.vessel","DIN 28036","72\"",1800.0,1915.0,"-",55.0,"-",1870.0,72.0,23.0,"-","-",1803.0,7.0,159,"M20",16.0,128.0]
[null,"SO St.steel Pr.vessel DIN 28036  DN 1900 / 60","SO","St.steel Pr.vessel","DIN 28036","76\"",1900.0,2015.0,"-",60.0,"-",1970.0,76.0,23.0,"-","-",1903.0,7.0,169,"M20",16.0,147.0]
[null,"SO St.steel Pr.vessel DIN 28036  DN 2000 / 60","SO","St.steel Pr.vessel","DIN 28036","80\"",2000.0,2115.0,"-",60.0,"-",2070.0,80.0,23.0,"-","-",2003.0,7.0,169,"M20",16.0,155.0]
[null,{"$f":"CONCATENATE(C1085,$C$2,D1085,$C$2,E1085,$C$2,$C$2,$F$1,$C$2,$G$2,$C$2,G1085)","v":"SO PN 6 NEN 5818  Size DN 10"},"SO","PN 6","NEN 5818","1/4\"",10.0,75.0,"-",12.0,"-",50.0,4.0,11.5,"-","-",17.7,3.0,53,"M10",8.0,0.36]
[null,"SO PN 6 NEN 5818  Size DN 15","SO","PN 6","NEN 5818","1/2\"",15.0,80.0,"-",12.0,"-",55.0,4.0,11.5,"-","-",21.8,3.0,53,"M10",8.0,0.41]
[null,"SO PN 6 NEN 5818  Size DN 20","SO","PN 6","NEN 5818","3/4\"",20.0,90.0,"-",14.0,"-",65.0,4.0,11.5,"-","-",27.4,3.0,57,"M10",8.0,0.6]
[null,"SO PN 6 NEN 5818  Size DN 25","SO","PN 6","NEN 5818","1\"",25.0,100.0,"-",14.0,"-",75.0,4.0,11.5,"-","-",34.2,3.0,57,"M10",8.0,0.74]
[null,"SO PN 6 NEN 5818  Size DN 32","SO","PN 6","NEN 5818","1¼\"",32.0,120.0,"-",16.0,"-",90.0,4.0,14.0,"-","-",42.9,3.0,65,"M12",10.0,1.19]
[null,"SO PN 6 NEN 5818  Size DN 40","SO","PN 6","NEN 5818","1½\"",40.0,130.0,"-",16.0,"-",100.0,4.0,14.0,"-","-",48.8,3.0,65,"M12",10.0,1.39]
[null,"SO PN 6 NEN 5818  Size DN 50","SO","PN 6","NEN 5818","2\"",50.0,140.0,"-",16.0,"-",110.0,4.0,14.0,"-","-",60.8,4.0,66,"M12",10.0,1.53]
[null,"SO PN 6 NEN 5818  Size DN 65","SO","PN 6","NEN 5818","2½\"",65.0,160.0,"-",16.0,"-",130.0,4.0,14.0,"-","-",76.6,4.0,66,"M12",10.0,1.89]
[null,"SO PN 6 NEN 5818  Size DN 80","SO","PN 6","NEN 5818","3\"",80.0,190.0,"-",18.0,"-",150.0,4.0,18.0,"-","-",89.4,4.0,76,"M16",13.0,2.98]
[null,"SO PN 6 NEN 5818  Size DN 100","SO","PN 6","NEN 5818","4\"",100.0,210.0,"-",18.0,"-",170.0,4.0,18.0,"-","-",114.8,5.0,77,"M16",13.0,3.46]
[null,"SO PN 6 NEN 5818  Size DN 125","SO","PN 6","NEN 5818","5\"",125.0,240.0,"-",20.0,"-",200.0,8.0,18.0,"-","-",140.2,5.0,81,"M16",13.0,4.6]
[null,"SO PN 6 NEN 5818  Size DN 150","SO","PN 6","NEN 5818","6\"",150.0,265.0,"-",20.0,"-",225.0,8.0,18.0,"-","-",168.8,6.0,82,"M16",13.0,5.22]
[null,"SO PN 6 NEN 5818  Size DN 200","SO","PN 6","NEN 5818","8\"",200.0,320.0,"-",22.0,"-",280.0,8.0,18.0,"-","-",220.1,6.0,86,"M16",13.0,7.15]
[null,"SO PN 6 NEN 5818  Size DN 250","SO","PN 6","NEN 5818","10\"",250.0,375.0,"-",24.0,"-",335.0,12.0,18.0,"-","-",274.0,6.0,90,"M16",13.0,9.61]
[null,"SO PN 6 NEN 5818  Size DN 300","SO","PN 6","NEN 5818","12\"",300.0,440.0,"-",24.0,"-",395.0,12.0,23.0,"-","-",324.9,6.0,96,"M20",16.0,12.6]
[null,"SO PN 6 NEN 5818  Size DN 350","SO","PN 6","NEN 5818","14\"",350.0,490.0,"-",26.0,"-",445.0,12.0,23.0,"-","-",369.0,7.0,101,"M20",16.0,15.6]
[null,"SO PN 6 NEN 5818  Size DN 400","SO","PN 6","NEN 5818","16\"",400.0,540.0,"-",28.0,"-",495.0,16.0,23.0,"-","-",420.0,7.0,105,"M20",16.0,18.4]
[null,"SO PN 6 NEN 5818  Size DN 500","SO","PN 6","NEN 5818","20\"",500.0,645.0,"-",30.0,"-",600.0,20.0,23.0,"-","-",522.0,7.0,109,"M20",16.0,24.6]
[null,"SO PN 10 NEN 5819  Size DN 10","SO","PN 10","NEN 5819","1/4\"",10.0,90.0,"-",14.0,"-",60.0,4.0,14.0,"-","-",17.7,3.0,61,"M12",10.0,0.61]
[null,"SO PN 10 NEN 5819  Size DN 15","SO","PN 10","NEN 5819","1/2\"",15.0,95.0,"-",14.0,"-",65.0,4.0,14.0,"-","-",21.8,3.0,61,"M12",10.0,0.67]
[null,"SO PN 10 NEN 5819  Size DN 20","SO","PN 10","NEN 5819","3/4\"",20.0,105.0,"-",16.0,"-",75.0,4.0,14.0,"-","-",27.4,3.0,65,"M12",10.0,0.95]
[null,"SO PN 10 NEN 5819  Size DN 25","SO","PN 10","NEN 5819","1\"",25.0,115.0,"-",16.0,"-",85.0,4.0,14.0,"-","-",34.2,3.0,65,"M12",10.0,1.11]
[null,"SO PN 10 NEN 5819  Size DN 32","SO","PN 10","NEN 5819","1¼\"",32.0,140.0,"-",16.0,"-",100.0,4.0,18.0,"-","-",42.9,3.0,71,"M16",13.0,1.62]
[null,"SO PN 10 NEN 5819  Size DN 40","SO","PN 10","NEN 5819","1½\"",40.0,150.0,"-",16.0,"-",110.0,4.0,18.0,"-","-",48.8,3.0,71,"M16",13.0,1.86]
[null,"SO PN 10 NEN 5819  Size DN 50","SO","PN 10","NEN 5819","2\"",50.0,165.0,"-",18.0,"-",125.0,4.0,18.0,"-","-",60.8,4.0,76,"M16",13.0,2.47]
[null,"SO PN 10 NEN 5819  Size DN 65","SO","PN 10","NEN 5819","2½\"",65.0,185.0,"-",18.0,"-",145.0,4.0,18.0,"-","-",76.6,4.0,76,"M16",13.0,3.0]
[null,"SO PN 10 NEN 5819  Size DN 80","SO","PN 10","NEN 5819","3\"",80.0,200.0,"-",20.0,"-",160.0,4.0,18.0,"-","-",89.4,4.0,80,"M16",13.0,3.79]
[null,"SO PN 10 NEN 5819  Size DN 100","SO","PN 10","NEN 5819","4\"",100.0,220.0,"-",20.0,"-",180.0,8.0,18.0,"-","-",114.8,5.0,81,"M16",13.0,4.03]
[null,"SO PN 10 NEN 5819  Size DN 125","SO","PN 10","NEN 5819","5\"",125.0,250.0,"-",22.0,"-",210.0,8.0,18.0,"-","-",140.2,5.0,85,"M16",13.0,5.46]
[null,"SO PN 10 NEN 5819  Size DN 150","SO","PN 10","NEN 5819","6\"",150.0,285.0,"-",22.0,"-",240.0,8.0,23.0,"-","-",168.8,6.0,92,"M20",16.0,6.57]
[null,"SO PN 10 NEN 5819  Size DN 175","SO","PN 10","NEN 5819","7\"",175.0,315.0,"-",24.0,"-",270.0,8.0,23.0,"-","-",194.7,6.0,96,"M20",16.0,8.45]
[null,"SO PN 10 NEN 5819  Size DN 200","SO","PN 10","NEN 5819","8\"",200.0,340.0,"-",24.0,"-",295.0,8.0,23.0,"-","-",220.1,6.0,96,"M20",16.0,9.31]
[null,"SO PN 10 NEN 5819  Size DN 250","SO","PN 10","NEN 5819","10\"",250.0,395.0,"-",26.0,"-",350.0,12.0,23.0,"-","-",274.0,6.0,100,"M20",16.0,11.9]
[null,"SO PN 10 NEN 5819  Size DN 300","SO","PN 10","NEN 5819","12\"",300.0,445.0,"-",26.0,"-",400.0,12.0,23.0,"-","-",324.9,6.0,100,"M20",16.0,13.8]
[null,"SO PN 10 NEN 5819  Size DN 350","SO","PN 10","NEN 5819","14\"",350.0,505.0,"-",28.0,"-",460.0,16.0,23.0,"-","-",369.0,7.0,105,"M20",16.0,19.0]
[null,"SO PN 10 NEN 5819  Size DN 400","SO","PN 10","NEN 5819","16\"",400.0,565.0,"-",32.0,"-",515.0,16.0,27.0,"-","-",420.0,7.0,119,"M24",19.0,25.9]
[null,"SO PN 10 NEN 5819  Size DN 500","SO","PN 10","NEN 5819","20\"",500.0,670.0,"-",38.0,"-",620.0,20.0,27.0,"-","-",522.0,7.0,131,"M24",19.0,37.9]

{"sheet":"Lapjoint fl.","index":9,"n_rows":54,"n_cols":48,"rows_kept":54,"cut":false,"hidden":true,"merged":[[0,0,0,8]]}
["LAPJOINT FLANGE & STUB-END DIMENSIONS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PIPE   DATA acc ANSI B 16.5",null,null,null,null,null,null,null,null,null,"ASA Stub end weights",null,null,null,null,null,null,null,null,null,"MSS Stub end weights"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NPS","DN","OD","5S","10S","40S","Std.","80S","XS",null,"NPS","DN","OD","5S","10S","40S","Std.","80S","XS",null,"NPS","DN","OD","5S","10S","40S","Std.","80S","XS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/2\"",15.0,21.34,1.65,2.11,2.77,2.77,3.73,3.73,null,"1/2\"",15.0,21.34,0.07076538671155265,0.09,0.11,"-",0.14,"-",null,"1/2\"",15.0,21.34,0.05,0.06,0.08,"-",0.1,"-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3/4\"",20.0,26.67,1.65,2.11,2.87,2.87,3.91,3.91,null,"3/4\"",20.0,26.67,0.09,0.12,0.15,"-",0.2,"-",null,"3/4\"",20.0,26.67,0.06,0.08,0.1,"-",0.14,"-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1\"",25.0,33.4,1.65,2.77,3.38,3.38,4.55,4.55,null,"1\"",25.0,33.4,0.150318890202087,0.24435930660811783,0.29285846428802187,"-",0.38051502209568466,"-",null,"1\"",25.0,33.4,0.08,0.13,0.16,"-",0.2,"-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1¼\"",32.0,42.16,1.65,2.77,3.56,3.56,4.85,4.85,null,"1¼\"",32.0,42.16,0.19596031049318205,0.32098156976347125,0.4052780939839664,"-",0.5360128136488691,"-",null,"1¼\"",32.0,42.16,0.11,0.17,0.22,"-",0.29,"-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1½\"",40.0,48.26,1.65,2.77,3.68,3.68,5.08,5.08,null,"1½\"",40.0,48.26,0.22991596732688327,0.3779859148721694,0.4935326484923352,"-",0.6629635246669923,"-",null,"1½\"",40.0,48.26,0.13,0.21,0.27,"-",0.37,"-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2\"",50.0,60.33,1.65,2.77,3.91,3.91,5.54,5.54,null,"2\"",50.0,60.33,0.42,0.7,0.97,"-",1.34,"-",null,"2\"",50.0,60.33,0.2,0.33,0.46,"-",0.64,"-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2½\"",65.0,73.03,2.11,3.05,5.16,5.16,7.01,7.01,null,"2½\"",65.0,73.03,0.65,0.93,1.5369792692182422,"-",2.0379024434821154,"-",null,"2½\"",65.0,73.03,0.31,0.44,0.72,"-",0.96,"-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3\"",80.0,88.9,2.11,3.05,5.49,5.49,7.62,7.62,null,"3\"",80.0,88.9,0.8178672406234618,1.1711436854387531,2.056282220412499,"-",2.791340575466913,"-",null,"3\"",80.0,88.9,0.39,0.56,0.99,"-",1.35,"-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3½\"","-",101.6,2.11,3.05,5.74,5.74,8.08,8.08,null,"3½\"","-",101.6,0.93,1.34,2.46,"-",3.39,"-",null,"3½\"","-",101.6,0.51,0.73,1.35,"-",1.87,"-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4\"",100.0,114.3,2.11,3.05,6.02,6.02,8.56,8.56,null,"4\"",100.0,114.3,1.07,1.54,2.96,"-",4.13,"-",null,"4\"",100.0,114.3,0.59,0.85,1.65,"-",2.3,"-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5\"",125.0,141.3,2.77,3.4,6.55,6.55,9.53,9.53,null,"5\"",125.0,141.3,2.23,2.73,5.15,"-",7.35,"-",null,"5\"",125.0,141.3,0.96,1.18,2.23,"-",3.19,"-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6\"",150.0,168.28,2.77,3.4,7.11,7.11,10.97,10.97,null,"6\"",150.0,168.28,2.68,3.28,6.73,"-",10.17,"-",null,"6\"",150.0,168.28,1.31,1.6,3.29,"-",4.99,"-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8\"",200.0,219.08,2.77,3.76,8.18,8.18,12.7,12.7,null,"8\"",200.0,219.08,3.52,4.76,10.17,"-",15.5,"-",null,"8\"",200.0,219.08,1.91,2.59,5.53,"-",8.45,"-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10\"",250.0,273.05,3.4,4.19,9.27,9.27,12.7,12.7,null,"10\"",250.0,273.05,6.56,8.06,17.53,"-",23.74,"-",null,"10\"",250.0,273.05,3.49,4.29,9.33,"-",12.65,"-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12\"",300.0,323.85,3.96,4.57,9.53,9.53,12.7,12.7,null,"12\"",300.0,323.85,9.17,10.57,21.73,"-",28.6983347152765,"-",null,"12\"",300.0,323.85,5.71,6.58,13.54,"-",17.89,"-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14\"",350.0,355.6,3.96,4.78,"-",9.53,"-",12.7,null,"14\"",350.0,355.6,11.868063650106436,14.561062059197416,"-",28.150930582981523,"-",37.2036646472435,null,"14\"",350.0,355.6,6.27,7.69,"-",14.88,"-",19.68]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16\"",400.0,406.4,4.19,4.78,"-",9.53,"-",12.7,null,"16\"",400.0,406.4,14.51,16.53,"-",32.6,"-",43.13,null,"16\"",400.0,406.4,7.72,8.8,"-",17.37,"-",23.0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18\"",450.0,457.2,4.19,4.78,"-",9.53,"-",12.7,null,"18\"",450.0,457.2,16.68,19.01,"-",37.54,"-",49.72,null,"18\"",450.0,457.2,9.03,10.29,"-",20.34,"-",26.95]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20\"",500.0,508.0,4.78,5.54,"-",9.53,"-",12.7,null,"20\"",500.0,508.0,21.12,24.44,"-",41.75,"-",55.33,null,"20\"",500.0,508.0,11.42,13.22,"-",22.6,"-",29.97]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"22\"",550.0,558.8,4.78,5.54,"-",9.53,"-",12.7,null,"22\"",550.0,558.8,23.48,27.18,"-",46.46,"-",61.6,null,"22\"",550.0,558.8,"-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24\"",600.0,609.6,5.54,6.35,"-",9.53,"-",12.7,null,"24\"",600.0,609.6,29.65,33.94,"-",50.7,"-",67.26,null,"24\"",600.0,609.6,16.15,18.49,"-",27.63,"-",36.68]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Flange dimensions"]
["D","Flange diameter",{"$f":"INDEX('Data Lapjoint fl.'!$I$4:$I$270,'Data Lapjoint fl.'!$A$4)","v":584.2},"mm"]
["h","Flange height",{"$f":"INDEX('Data Lapjoint fl.'!$J$4:$J$270,'Data Lapjoint fl.'!$A$4)","v":111.3},"mm"]
["b1","Flange thickness",{"$f":"INDEX('Data Lapjoint fl.'!$K$4:$K$270,'Data Lapjoint fl.'!$A$4)","v":53.8},"mm",null,"Include data of following LJ flanges:"]
["b2","Stub-end height ASA",{"$f":"INDEX('Data Lapjoint fl.'!$W$4:$W$270,'Data Lapjoint fl.'!$A$4)","v":304.8},"mm",null,"ANSI B 16.5",null,"150 #"]
["b2","Stub-end height MSS",{"$f":"INDEX('Data Lapjoint fl.'!$X$4:$X$270,'Data Lapjoint fl.'!$A$4)","v":152.4},"mm",null,"ANSI B 16.5",null,"300 #"]
["b2","Collar height",{"$f":"INDEX('Data Lapjoint fl.'!$Y$4:$Y$270,'Data Lapjoint fl.'!$A$4)","v":"-"},"mm",null,"MSS SP-44",null,"150 #"]
["k","Pitch circle",{"$f":"INDEX('Data Lapjoint fl.'!$N$4:$N$270,'Data Lapjoint fl.'!$A$4)","v":514.3},"mm",null,"MSS SP-44",null,"300 #"]
["n","Number of bolts",{"$f":"INDEX('Data Lapjoint fl.'!$P$4:$P$270,'Data Lapjoint fl.'!$A$4)","v":20},"pce",null,"DIN 2641 Carbon steel",null,"PN 6"]
["bt","Bolt",{"$f":"INDEX('Data Lapjoint fl.'!$Q$4:$Q$270,'Data Lapjoint fl.'!$A$4)","v":"M30"},"-",null,"DIN 2641 Aluminium",null,"PN 6"]
["L","Required bolt length",{"$f":"INDEX('Data Lapjoint fl.'!$S$4:$S$270,'Data Lapjoint fl.'!$A$4)","v":170.6},"mm",null,"DIN 2642 Carbon steel",null,"PN 10"]
["s","Thickn. Stubend fl.",null,"mm",null,"Din 2642 Aluminium",null,"PN 10"]
["s","Thickn. Collar flange",{"$f":"INDEX('Data Lapjoint fl.'!$Z$4:$Z$270,'Data Lapjoint fl.'!$A$4)","v":""},"mm"]
["g","Thickness of gasket",{"$f":"INDEX('Data Lapjoint fl.'!$T$4:$T$270,'Data Lapjoint fl.'!$A$4)","v":7},"mm"]
["m","Thickness of nut",{"$f":"INDEX('Data Lapjoint fl.'!$R$4:$R$270,'Data Lapjoint fl.'!$A$4)","v":24},"mm"]
["s1","Thickness pipe",{"$f":"INDEX('Data Lapjoint fl.'!$AA$4:$AA$270,'Data Lapjoint fl.'!$A$4)","v":""},"mm"]
["d1","Stub-end/collar diam.",{"$f":"INDEX('Data Lapjoint fl.'!$U$4:$U$270,'Data Lapjoint fl.'!$A$4)","v":355.6},"mm"]
["d2","Diam. boltholes",{"$f":"INDEX('Data Lapjoint fl.'!$O$4:$O$270,'Data Lapjoint fl.'!$A$4)","v":31.7},"mm",null,"W1","Weight flange",{"$f":"INDEX('Data Lapjoint fl.'!$AB$4:$AB$270,'Data Lapjoint fl.'!$A$4)","v":70.9},"kg"]
["d3","Diam. flangehole",{"$f":"INDEX('Data Lapjoint fl.'!$L$4:$L$270,'Data Lapjoint fl.'!$A$4)","v":360.2},"mm",null,"W2","Weight collar",{"$f":"INDEX('Data Lapjoint fl.'!$AE$4:$AE$270,'Data Lapjoint fl.'!$A$4)","v":"-"},"kg"]
["d4","Diameter rim",{"$f":"INDEX('Data Lapjoint fl.'!$V$4:$V$270,'Data Lapjoint fl.'!$A$4)","v":412.8},"mm",null,"W2","Weight stub / collar",null,"kg"]
["d5","Diameter hub",{"$f":"INDEX('Data Lapjoint fl.'!$M$4:$M$270,'Data Lapjoint fl.'!$A$4)","v":425.4},"mm",null,"W2","Weight stub MSS",null,"kg"]

{"sheet":"Data Lapjoint fl.","index":10,"n_rows":270,"n_cols":32,"rows_kept":270,"cut":false,"hidden":true,"merged":[[0,8,0,12],[0,13,0,18],[0,20,0,24],[0,27,0,30]]}
["Data Lap joint flanges:",null,null,null,null,null,null,null,"Flange ",null,null,null,null,"Studs",null,null,null,null,null,null,"Collar/Stub end",null,null,null,null,null,null,"Weight",null,null,null,"Ansi"]
[null,null,null,null,null,"Size  ","Size",null,"diam.","height","thickn.","pipehole","hubdiam.","pitch","bolthole","no.","boltsize","nut hght","length","gasket","Pipe ø","Flange ø","height","height","height","fl.height","Pipe th","Flange","Stub ASA","Stub MSS","Collar"," Sch."]
[null,"Type / Size / Rating","Type","Rating","Norm","NPS","DN ","  Mat. ","D","h","b1","d3","d5","k","d2","n","bt","m","L","g","d1","d4","b2-ASA","b2-MSS","b2 (C)","s","s1","kg"]
[100.0,{"$f":"CONCATENATE($C4,$D4,$E4,$F$2,$F4,$AF$2,AF4)","v":"LJ  150#  ANSI B16.5  Size  1/2\" Sch. 5S"},"LJ  ","150#  ","ANSI B16.5  ","1/2\"",15.0,"SS",88.9,15.7,11.2,22.9,30.2,60.5,15.7,4.0,"M12",10.0,{"$f":"(K4+R4+Z4+4)*2+T4","v":53.4},3.0,21.34,35.05,76.2,50.8,"-",{"$f":"AA4","v":""},{"$f":"'Lapjoint fl.'!$C$45","v":""},0.38,0.07076538671155265,0.04819219032956057,"-"," 5S"]
[null,"LJ  150#  ANSI B16.5  Size  1/2\" Sch. 10S","LJ  ","150#  ","ANSI B16.5  ","1/2\"",15.0,"SS",88.9,15.7,11.2,22.9,30.2,60.5,15.7,4.0,"M12",10.0,53.4,3.0,21.34,35.05,76.2,50.8,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},0.38,0.08861814661451187,0.06041936201800996,"-"," 10S"]
[null,"LJ  150#  ANSI B16.5  Size  1/2\" Sch. 40S","LJ  ","150#  ","ANSI B16.5  ","1/2\"",15.0,"SS",88.9,15.7,11.2,22.9,30.2,60.5,15.7,4.0,"M12",10.0,53.4,3.0,21.34,35.05,76.2,50.8,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},0.38,0.11280440528709768,0.07704252091180826,"-"," 40S"]
[null,"LJ  150#  ANSI B16.5  Size  1/2\" Sch. 80S","LJ  ","150#  ","ANSI B16.5  ","1/2\"",15.0,"SS",88.9,15.7,11.2,22.9,30.2,60.5,15.7,4.0,"M12",10.0,53.4,3.0,21.34,35.05,76.2,50.8,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},0.38,0.1449788534595513,0.09928570978942894,"-"," 80S"]
[null,"LJ  150#  ANSI B16.5  Size  3/4\" Sch. 5S","LJ  ","150#  ","ANSI B16.5  ","3/4\"",20.0,"SS",98.6,15.7,12.7,28.2,38.1,69.9,15.7,4.0,"M12",10.0,56.4,3.0,26.67,42.9,76.2,50.8,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},0.55,0.09167474174412238,0.0628487718048725,"-"," 5S"]
[null,"LJ  150#  ANSI B16.5  Size  3/4\" Sch. 10S","LJ  ","150#  ","ANSI B16.5  ","3/4\"",20.0,"SS",98.6,15.7,12.7,28.2,38.1,69.9,15.7,4.0,"M12",10.0,56.4,3.0,26.67,42.9,76.2,50.8,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},0.55,0.11535677638343436,0.07916202075310581,"-"," 10S"]
[null,"LJ  150#  ANSI B16.5  Size  3/4\" Sch. 40S","LJ  ","150#  ","ANSI B16.5  ","3/4\"",20.0,"SS",98.6,15.7,12.7,28.2,38.1,69.9,15.7,4.0,"M12",10.0,56.4,3.0,26.67,42.9,76.2,50.8,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},0.55,0.15269171849157295,0.10496014366550116,"-"," 40S"]
[null,"LJ  150#  ANSI B16.5  Size  3/4\" Sch. 80S","LJ  ","150#  ","ANSI B16.5  ","3/4\"",20.0,"SS",98.6,15.7,12.7,28.2,38.1,69.9,15.7,4.0,"M12",10.0,56.4,3.0,26.67,42.9,76.2,50.8,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},0.55,0.20016383022031475,0.13793252638923467,"-"," 80S"]
[null,"LJ  150#  ANSI B16.5  Size  1\" Sch. 5S","LJ  ","150#  ","ANSI B16.5  ","1\"",25.0,"SS",108.0,17.5,14.2,35.1,49.3,79.2,15.7,4.0,"M12",10.0,59.4,3.0,33.4,50.8,101.6,50.8,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},0.76,0.150318890202087,0.08002239014748243,"-"," 5S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 10S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.24435930660811783,0.1304786745455315,"-"," 10S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 40S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.29285846428802187,0.15664566596341897,"-"," 40S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 80S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.38051502209568466,0.20424234157296062,"-"," 80S"]
[null,"LJ  150#  ANSI B16.5  Size  1¼\" Sch. 5S","LJ  ","150#  ","ANSI B16.5  ","1¼\"",32.0,"SS",117.3,20.6,15.7,43.7,58.7,88.9,15.7,4.0,"M12",10.0,{"$f":"(K16+R16+Z16+4)*2+T16","v":62.4},3.0,42.16,63.5,101.6,50.8,"-",{"$f":"AA16","v":""},{"$f":"'Lapjoint fl.'!$C$45","v":""},1.01,0.19596031049318205,0.10604552651408965,"-"," 5S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 10S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.32098156976347125,0.17416600044583574,"-"," 10S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 40S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.4052780939839664,0.22033694735922876,"-"," 40S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 80S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.5360128136488691,0.29238989900948736,"-"," 80S"]
[null,"LJ  150#  ANSI B16.5  Size  1½\" Sch. 5S","LJ  ","150#  ","ANSI B16.5  ","1½\"",40.0,"SS",127.0,22.4,17.5,50.0,65.0,98.6,15.7,4.0,"M12",10.0,{"$f":"(K20+R20+Z20+4)*2+T20","v":66},3.0,48.26,73.15,101.6,50.8,"-",{"$f":"AA20","v":""},{"$f":"'Lapjoint fl.'!$C$45","v":""},1.3,0.22991596732688327,0.1263237640867143,"-"," 5S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 10S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.3779859148721694,0.2082088598859388,"-"," 10S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 40S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.4935326484923352,0.272440935604268,"-"," 40S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 80S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.6629635246669923,0.36723375063979596,"-"," 80S"]
[null,"LJ  150#  ANSI B16.5  Size  2\" Sch. 5S","LJ  ","150#  ","ANSI B16.5  ","2\"",50.0,"SS",152.4,25.4,19.1,62.5,77.7,120.7,19.1,4.0,"M16",13.0,{"$f":"(K24+R24+Z24+4)*2+T24","v":76.2},4.0,60.33,91.95,152.4,63.5,"-",{"$f":"AA24","v":""},{"$f":"'Lapjoint fl.'!$C$45","v":""},2.03,0.4244558714998417,0.19928889887548945,"-"," 5S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 10S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.7005800358302922,0.3297363577270344,"-"," 10S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 40S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.9716767374862928,0.4585042776270582,"-"," 40S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 80S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.3418457830580033,0.6355941773692938,"-"," 80S"]
[null,"LJ  150#  ANSI B16.5  Size  2½\" Sch. 5S","LJ  ","150#  ","ANSI B16.5  ","2½\"",65.0,"SS",117.8,28.4,22.4,75.4,90.4,139.7,19.1,4.0,"M16",13.0,{"$f":"(K28+R28+Z28+4)*2+T28","v":82.8},4.0,73.03,104.65,152.4,63.5,"-",{"$f":"AA28","v":""},{"$f":"'Lapjoint fl.'!$C$45","v":""},3.25,0.6533678306771649,0.30542631054228525,"-"," 5S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 10S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.9333601781704101,0.43703186770777025,"-"," 10S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 40S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.5369792692182422,0.7224305052913871,"-"," 40S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 80S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.0379024434821154,0.9612620563003152,"-"," 80S"]
[null,"LJ  150#  ANSI B16.5  Size  3\" Sch. 5S","LJ  ","150#  ","ANSI B16.5  ","3\"",80.0,"SS",190.5,30.2,23.9,91.4,108.0,152.4,19.1,4.0,"M16",13.0,{"$f":"(K32+R32+Z32+4)*2+T32","v":85.8},4.0,88.9,127.0,152.4,63.5,"-",{"$f":"AA32","v":""},{"$f":"'Lapjoint fl.'!$C$45","v":""},3.81,0.8178672406234618,0.39127834833595687,"-"," 5S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 10S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.1711436854387531,0.5611307848976743,"-"," 10S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 40S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.056282220412499,0.9891914460777878,"-"," 40S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 80S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.791340575466913,1.3477207913118394,"-"," 80S"]
[null,"LJ  150#  ANSI B16.5  Size  3½\" Sch. 5S","LJ  ","150#  ","ANSI B16.5  ","3½\"","-","SS",215.9,31.8,23.9,104.1,122.2,177.8,19.1,8.0,"M16",13.0,{"$f":"(K36+R36+Z36+4)*2+T36","v":85.8},4.0,101.6,139.7,152.4,76.2,"-",{"$f":"AA36","v":""},{"$f":"'Lapjoint fl.'!$C$45","v":""},4.76,0.9343893910257729,0.5108140068735323,"-"," 5S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 10S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.3395761777264537,0.7330270679694704,"-"," 10S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 40S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.4613577382263756,1.3507016484739454,"-"," 40S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 80S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.3916886412970504,1.8660318948216412,"-"," 80S"]
[null,"LJ  150#  ANSI B16.5  Size  4\" Sch. 5S","LJ  ","150#  ","ANSI B16.5  ","4\"",100.0,"SS",228.6,33.3,23.9,116.8,134.9,190.5,19.1,8.0,"M16",13.0,{"$f":"(K40+R40+Z40+4)*2+T40","v":86.8},5.0,114.3,157.2,152.4,76.2,"-",{"$f":"AA40","v":""},{"$f":"'Lapjoint fl.'!$C$45","v":""},5.25,1.070793056581357,0.5925686379407376,"-"," 5S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 10S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.5367473530556166,0.8512031934457629,"-"," 10S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 40S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.964079468622285,1.6466946683627446,"-"," 40S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 80S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.130666057807272,2.3008812480336207,"-"," 80S"]
[null,"LJ  150#  ANSI B16.5  Size  5\" Sch. 5S","LJ  ","150#  ","ANSI B16.5  ","5\"",125.0,"SS",254.0,36.6,23.9,144.5,163.6,215.9,22.4,8.0,"M20",16.0,{"$f":"(K44+R44+Z44+4)*2+T44","v":92.8},5.0,141.3,185.7,203.2,76.2,"-",{"$f":"AA44","v":""},{"$f":"'Lapjoint fl.'!$C$45","v":""},6.02,2.232568364938664,0.962885367434142,"-"," 5S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 10S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.72929766540264,1.177881334742825,"-"," 10S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 40S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5.151580560360563,2.2306279802130664,"-"," 40S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 80S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.348994676497363,3.1924501620074013,"-"," 80S"]
[null,"LJ  150#  ANSI B16.5  Size  6\" Sch. 5S","LJ  ","150#  ","ANSI B16.5  ","6\"",150.0,"SS",279.4,39.6,25.4,171.5,192.0,241.3,22.4,8.0,"M20",16.0,{"$f":"(K48+R48+Z48+4)*2+T48","v":96.8},6.0,168.28,215.9,203.2,88.9,"-",{"$f":"AA48","v":""},{"$f":"'Lapjoint fl.'!$C$45","v":""},7.4,2.684202129463946,1.3091890603152119,"-"," 5S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 10S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.283649578538363,1.6022806357497652,"-"," 10S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 40S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6.730749242103626,3.2931883727693685,"-"," 40S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 80S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10.166631044738047,4.988807106371507,"-"," 80S"]
[null,"LJ  150#  ANSI B16.5  Size  8\" Sch. 5S","LJ  ","150#  ","ANSI B16.5  ","8\"",200.0,"SS",342.9,44.5,28.4,222.3,246.1,298.5,22.4,8.0,"M20",16.0,{"$f":"(K52+R52+Z52+4)*2+T52","v":102.8},6.0,219.08,269.7,203.2,101.6,"-",{"$f":"AA52","v":""},{"$f":"'Lapjoint fl.'!$C$45","v":""},12.1,3.52259386500972,1.911589548106807,"-"," 5S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 10S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.7623877913504735,2.585525562083253,"-"," 10S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 40S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10.17439606577285,5.534878611186907,"-"," 40S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 80S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15.500598219343818,8.450355362343046,"-"," 80S"]
[null,"LJ  150#  ANSI B16.5  Size  10\" Sch. 5S","LJ  ","150#  ","ANSI B16.5  ","10\"",250.0,"SS",406.4,49.3,30.2,277.4,304.8,362.0,25.4,12.0,"M24",19.0,{"$f":"(K56+R56+Z56+4)*2+T56","v":112.4},6.0,273.05,323.9,254.0,127.0,"-",{"$f":"AA56","v":""},{"$f":"'Lapjoint fl.'!$C$45","v":""},16.4,6.559937826765604,3.485463959669181,"-"," 5S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 10S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8.062835117521624,4.285020526687177,"-"," 10S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 40S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17.534938518050676,9.333672447137126,"-"," 40S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 80S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,23.7424363733997,12.651667420485776,"-"," 80S"]
[null,"LJ  150#  ANSI B16.5  Size  12\" Sch. 5S","LJ  ","150#  ","ANSI B16.5  ","12\"",300.0,"SS",482.6,55.6,31.8,328.2,365.3,431.8,25.4,12.0,"M24",19.0,{"$f":"(K60+R60+Z60+4)*2+T60","v":115.6},6.0,323.85,381.0,254.0,152.4,"-",{"$f":"AA60","v":""},{"$f":"'Lapjoint fl.'!$C$45","v":""},26.1,9.171416202116891,5.707965483293002,"-"," 5S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 10S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10.566226586203566,6.576812199364878,"-"," 10S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 40S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,21.729662081334435,13.538359977621852,"-"," 40S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 80S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,28.6983347152765,17.891329751259235,"-"," 80S"]
[null,"LJ  150#  ANSI B16.5  Size  14\" Sch. 5S","LJ  ","150#  ","ANSI B16.5  ","14\"",350.0,"SS",533.4,79.2,35.1,360.2,400.1,476.3,28.4,12.0,"M27",22.0,{"$f":"(K64+R64+Z64+4)*2+T64","v":129.2},7.0,355.6,412.8,304.8,152.4,"-",{"$f":"AA64","v":""},{"$f":"'Lapjoint fl.'!$C$45","v":""},34.5,11.868063650106436,6.266494005706999,"-"," 5S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 10S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,14.561062059197416,7.689971600123838,"-"," 10S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. Std.","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,28.150930582981523,14.882495537875744,"-"," Std."]
[null,"LJ  150#  ANSI B16.5  Size   Sch. XS","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,37.2036646472435,19.682570214556655,"-"," XS"]
[null,"LJ  150#  ANSI B16.5  Size  16\" Sch. 5S","LJ  ","150#  ","ANSI B16.5  ","16\"",400.0,"SS",596.9,87.4,36.6,411.2,457.2,539.8,28.4,16.0,"M27",22.0,{"$f":"(K68+R68+Z68+4)*2+T68","v":132.2},7.0,406.4,469.9,304.8,152.4,"-",{"$f":"AA68","v":""},{"$f":"'Lapjoint fl.'!$C$45","v":""},44.6,14.505977364566638,7.721877755106224,"-"," 5S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 10S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16.526783991046823,8.798674640048391,"-"," 10S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. Std.","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,32.59990926986325,17.3730771700694,"-"," Std."]
[null,"LJ  150#  ANSI B16.5  Size   Sch. XS","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,43.132523967642044,23.001603449484207,"-"," XS"]
[null,"LJ  150#  ANSI B16.5  Size  18\" Sch. 5S","LJ  ","150#  ","ANSI B16.5  ","18\"",450.0,"SS",635.0,96.8,39.6,462.3,505.0,577.9,31.8,16.0,"M30",24.0,{"$f":"(K72+R72+Z72+4)*2+T72","v":142.2},7.0,457.2,533.4,304.8,152.4,"-",{"$f":"AA72","v":""},{"$f":"'Lapjoint fl.'!$C$45","v":""},48.7,16.678449716367066,9.02599459436555,"-"," 5S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 10S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19.005165337492187,10.286426070038747,"-"," 10S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. Std.","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,37.54111726811097,20.339242677979023,"-"," Std."]
[null,"LJ  150#  ANSI B16.5  Size   Sch. XS","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,49.717344699829546,26.954415826236847,"-"," XS"]
[null,"LJ  150#  ANSI B16.5  Size  20\" Sch. 5S","LJ  ","150#  ","ANSI B16.5  ","20\"",500.0,"SS",698.5,103.1,42.9,514.4,558.8,635.0,31.8,20.0,"M30",24.0,{"$f":"(K76+R76+Z76+4)*2+T76","v":148.8},7.0,508.0,584.2,304.8,152.4,"-",{"$f":"AA76","v":""},{"$f":"'Lapjoint fl.'!$C$45","v":""},61.6,21.116922224404117,11.419950969078974,"-"," 5S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 10S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,24.44187658988192,13.219951761530595,"-"," 10S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. Std.","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,41.75137733762374,22.59917830305298,"-"," Std."]
[null,"LJ  150#  ANSI B16.5  Size   Sch. XS","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55.32807952488837,29.96608239900059,"-"," XS"]
[null,"LJ  150#  ANSI B16.5  Size  22\" Sch. 5S","LJ  ","150#  ","ANSI B16.5  ","22\"",550.0,"SS",749.3,"-",46.0,"-","-",692.1,34.9,20.0,"M33",24.0,{"$f":"(K80+R80+Z80+4)*2+T80","v":155},7.0,558.8,641.4,304.8,"-","-",{"$f":"AA80","v":""},{"$f":"'Lapjoint fl.'!$C$45","v":""},"-",23.476875997999677,"-","-"," 5S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 10S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,27.177053139195525,"-","-"," 10S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. Std.","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,46.45647345945761,"-","-"," Std."]
[null,"LJ  150#  ANSI B16.5  Size   Sch. XS","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,61.598249592809616,"-","-"," XS"]
[null,"LJ  150#  ANSI B16.5  Size  24\" Sch. 5S","LJ  ","150#  ","ANSI B16.5  ","24\"",600.0,"SS",812.8,111.3,47.8,616.0,663.4,749.3,35.1,20.0,"M33",26.0,{"$f":"(K84+R84+Z84+4)*2+T84","v":162.6},7.0,609.6,692.2,304.8,152.4,"-",{"$f":"AA84","v":""},{"$f":"'Lapjoint fl.'!$C$45","v":""},86.6,29.646698810980666,16.146764517393546,"-"," 5S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. 10S","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,33.94156333647569,18.488364780797323,"-"," 10S"]
[null,"LJ  150#  ANSI B16.5  Size   Sch. Std.","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,50.70479895622873,27.63393020979923,"-"," Std."]
[null,"LJ  150#  ANSI B16.5  Size   Sch. XS","LJ  ","150#  ","ANSI B16.5  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,67.25971169238926,36.67556290431826,"-"," XS"]
[null,{"$f":"CONCATENATE($C88,$D88,$E88,$F$2,$F88)","v":"LJ  300#  ANSI B16.5  Size  1/2\""},"LJ  ","300#  ","ANSI B16.5  ","1/2\"",15.0,"SS",95.2,22.4,14.2,22.9,38.1,66.5,15.7,4.0,"M12",10.0,{"$f":"(K88+R88+Z88+4)*2+T88","v":59.4},3.0,21.34,35.05,76.2,50.8,"-",{"$f":"AA88","v":""},{"$f":"'Lapjoint fl.'!$C$45","v":""},0.62,null,null,"-"]
[null,"LJ  300#  ANSI B16.5  Size  3/4\"","LJ  ","300#  ","ANSI B16.5  ","3/4\"",20.0,"SS",117.5,25.4,15.7,28.2,47.7,82.5,19.0,4.0,"M16",13.0,68.4,3.0,26.67,42.9,76.2,50.8,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},1.1,null,null,"-"]
[null,"LJ  300#  ANSI B16.5  Size  1\"","LJ  ","300#  ","ANSI B16.5  ","1\"",25.0,"SS",123.8,26.9,17.5,35.1,53.8,88.9,19.0,4.0,"M16",13.0,72,3.0,33.4,50.8,101.6,50.8,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},1.33,null,null,"-"]
[null,"LJ  300#  ANSI B16.5  Size  1¼\"","LJ  ","300#  ","ANSI B16.5  ","1¼\"",32.0,"SS",133.3,26.9,19.1,43.7,63.5,98.5,19.0,4.0,"M16",13.0,75.2,3.0,42.16,63.5,101.6,50.8,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},1.65,null,null,"-"]
[null,"LJ  300#  ANSI B16.5  Size  1½\"","LJ  ","300#  ","ANSI B16.5  ","1½\"",40.0,"SS",155.6,30.2,20.6,50.0,69.8,114.3,22.3,4.0,"M20",16.0,84.2,3.0,48.26,73.15,101.6,50.8,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},2.44,null,null,"-"]
[null,"LJ  300#  ANSI B16.5  Size  2\"","LJ  ","300#  ","ANSI B16.5  ","2\"",50.0,"SS",165.1,33.3,22.4,62.5,84.0,127.0,19.0,8.0,"M16",13.0,82.8,4.0,60.33,91.95,152.4,63.5,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},2.83,null,null,"-"]
[null,"LJ  300#  ANSI B16.5  Size  2½\"","LJ  ","300#  ","ANSI B16.5  ","2½\"",65.0,"SS",190.5,38.1,25.4,75.4,100.0,149.3,22.3,8.0,"M20",16.0,94.8,4.0,73.03,104.65,152.4,63.5,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},4.25,null,null,"-"]
[null,"LJ  300#  ANSI B16.5  Size  3\"","LJ  ","300#  ","ANSI B16.5  ","3\"",80.0,"SS",209.5,42.9,28.4,91.4,117.3,168.1,22.3,8.0,"M20",16.0,100.8,4.0,88.9,127.0,152.4,63.5,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},5.78,null,null,"-"]
[null,"LJ  300#  ANSI B16.5  Size  3½\"","LJ  ","300#  ","ANSI B16.5  ","3½\"","-","SS",228.6,44.5,30.2,104.1,133.3,184.1,22.3,8.0,"M20",16.0,104.4,4.0,101.6,139.7,152.4,76.2,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},7.27,null,null,"-"]
[null,"LJ  300#  ANSI B16.5  Size  4\"","LJ  ","300#  ","ANSI B16.5  ","4\"",100.0,"SS",254.0,47.8,31.8,116.8,146.0,200.1,22.3,8.0,"M20",16.0,108.6,5.0,114.3,157.2,152.4,76.2,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},9.55,null,null,"-"]
[null,"LJ  300#  ANSI B16.5  Size  5\"","LJ  ","300#  ","ANSI B16.5  ","5\"",125.0,"SS",279.4,50.8,35.1,144.5,177.8,234.9,22.3,8.0,"M20",16.0,115.2,5.0,141.3,185.7,203.2,76.2,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},12.2,null,null,"-"]
[null,"LJ  300#  ANSI B16.5  Size  6\"","LJ  ","300#  ","ANSI B16.5  ","6\"",150.0,"SS",317.5,52.3,36.6,171.5,206.2,269.7,22.3,12.0,"M20",16.0,119.2,6.0,168.28,215.9,203.2,88.9,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},15.5,null,null,"-"]
[null,"LJ  300#  ANSI B16.5  Size  8\"","LJ  ","300#  ","ANSI B16.5  ","8\"",200.0,"SS",381.0,62.0,41.1,222.3,260.3,330.2,25.4,12.0,"M24",19.0,134.2,6.0,219.08,269.7,203.2,101.6,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},24.1,null,null,"-"]
[null,"LJ  300#  ANSI B16.5  Size  10\"","LJ  ","300#  ","ANSI B16.5  ","10\"",250.0,"SS",444.5,95.3,47.8,277.4,320.5,387.3,28.4,16.0,"M27",22.0,153.6,6.0,273.05,323.9,254.0,127.0,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},34.4,null,null,"-"]
[null,"LJ  300#  ANSI B16.5  Size  12\"","LJ  ","300#  ","ANSI B16.5  ","12\"",300.0,"SS",520.7,101.6,50.8,328.2,374.6,450.8,31.7,16.0,"M30",24.0,163.6,6.0,323.85,381.0,254.0,152.4,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},50.4,null,null,"-"]
[null,"LJ  300#  ANSI B16.5  Size  14\"","LJ  ","300#  ","ANSI B16.5  ","14\"",350.0,"SS",584.2,111.3,53.8,360.2,425.4,514.3,31.7,20.0,"M30",24.0,170.6,7.0,355.6,412.8,304.8,152.4,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},70.9,null,null,"-"]
[null,"LJ  300#  ANSI B16.5  Size  16\"","LJ  ","300#  ","ANSI B16.5  ","16\"",400.0,"SS",647.7,120.7,57.2,411.2,482.6,571.5,35.1,20.0,"M33",26.0,181.4,7.0,406.4,469.9,304.8,152.4,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},89.5,null,null,"-"]
[null,"LJ  300#  ANSI B16.5  Size  18\"","LJ  ","300#  ","ANSI B16.5  ","18\"",450.0,"SS",711.2,130.0,60.5,462.3,533.4,628.6,35.1,24.0,"M33",26.0,188,7.0,457.2,533.4,304.8,152.4,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},111.0,null,null,"-"]
[null,"LJ  300#  ANSI B16.5  Size  20\"","LJ  ","300#  ","ANSI B16.5  ","20\"",500.0,"SS",774.7,139.7,63.5,514.4,587.2,685.8,35.1,24.0,"M33",26.0,194,7.0,508.0,584.2,304.8,152.4,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},137.0,null,null,"-"]
[null,"LJ  300#  ANSI B16.5  Size  24\"","LJ  ","300#  ","ANSI B16.5  ","24\"",600.0,"SS",914.4,152.4,69.9,616.0,701.5,812.8,41.1,24.0,"M36",29.0,212.8,7.0,609.6,692.2,304.8,152.4,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},204.0,null,null,"-"]
[null,"LJ  400# ANSI B16.5  Size  1/2\"","LJ  ","400# ","ANSI B16.5  ","1/2\"",15.0,"SS",95.3,22.4,14.2,22.9,38.1,66.5,15.7,4.0,"M12",10.0,59.4,3.0,21.34,35.05,76.2,50.8,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},0.72,null,null,"-"]
[null,"LJ  400# ANSI B16.5  Size  3/4\"","LJ  ","400# ","ANSI B16.5  ","3/4\"",20.0,"SS",117.3,25.4,15.7,28.2,47.8,82.6,19.1,4.0,"M16",13.0,68.4,3.0,26.67,42.9,76.2,50.8,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},1.25,null,null,"-"]
[null,"LJ  400# ANSI B16.5  Size  1\"","LJ  ","400# ","ANSI B16.5  ","1\"",25.0,"SS",124.0,26.9,17.5,35.1,53.8,88.9,19.1,4.0,"M16",13.0,72,3.0,33.4,50.8,101.6,50.8,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},1.5,null,null,"-"]
[null,"LJ  400# ANSI B16.5  Size  1¼\"","LJ  ","400# ","ANSI B16.5  ","1¼\"",32.0,"SS",133.4,28.4,20.6,43.7,63.5,98.6,19.1,4.0,"M16",13.0,78.2,3.0,42.16,63.5,101.6,50.8,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},2.0,null,null,"-"]
[null,"LJ  400# ANSI B16.5  Size  1½\"","LJ  ","400# ","ANSI B16.5  ","1½\"",40.0,"SS",155.4,31.8,22.4,50.0,69.9,114.3,22.4,4.0,"M20",16.0,87.8,3.0,48.26,73.15,101.6,50.8,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},2.92,null,null,"-"]
[null,"LJ  400# ANSI B16.5  Size  2\"","LJ  ","400# ","ANSI B16.5  ","2\"",50.0,"SS",165.1,36.6,25.4,62.5,84.1,127.0,19.1,8.0,"M16",13.0,88.8,4.0,60.33,91.95,152.4,63.5,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},3.55,null,null,"-"]
[null,"LJ  400# ANSI B16.5  Size  2½\"","LJ  ","400# ","ANSI B16.5  ","2½\"",65.0,"SS",190.5,41.1,28.4,75.4,100.1,149.4,22.4,8.0,"M20",16.0,100.8,4.0,73.03,104.65,152.4,63.5,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},5.23,null,null,"-"]
[null,"LJ  400# ANSI B16.5  Size  3\"","LJ  ","400# ","ANSI B16.5  ","3\"",80.0,"SS",209.6,46.0,31.6,91.4,117.3,168.1,22.4,8.0,"M20",16.0,107.2,4.0,88.9,127.0,152.4,63.5,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},6.95,null,null,"-"]
[null,"LJ  400# ANSI B16.5  Size  3½\"","LJ  ","400# ","ANSI B16.5  ","3½\"","-","SS",228.6,49.3,35.1,104.1,133.4,184.2,25.4,8.0,"M24",19.0,120.2,4.0,101.6,139.7,152.4,76.2,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},8.78,null,null,"-"]
[null,"LJ  400# ANSI B16.5  Size  4\"","LJ  ","400# ","ANSI B16.5  ","4\"",100.0,"SS",254.0,50.8,35.1,116.8,146.1,200.2,25.4,8.0,"M24",19.0,121.2,5.0,114.3,157.2,152.4,76.2,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},10.9,null,null,"-"]
[null,"LJ  400# ANSI B16.5  Size  5\"","LJ  ","400# ","ANSI B16.5  ","5\"",125.0,"SS",279.4,53.8,38.1,144.5,177.8,235.0,25.4,8.0,"M24",19.0,127.2,5.0,141.3,185.7,203.2,76.2,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},13.7,null,null,"-"]
[null,"LJ  400# ANSI B16.5  Size  6\"","LJ  ","400# ","ANSI B16.5  ","6\"",150.0,"SS",317.5,57.2,41.1,171.5,206.2,269.7,25.4,12.0,"M24",19.0,134.2,6.0,168.28,215.9,203.2,88.9,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},18.0,null,null,"-"]
[null,"LJ  400# ANSI B16.5  Size  8\"","LJ  ","400# ","ANSI B16.5  ","8\"",200.0,"SS",381.0,68.3,47.8,222.3,260.4,330.2,28.4,12.0,"M27",22.0,153.6,6.0,219.08,269.7,203.2,101.6,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},28.3,null,null,"-"]
[null,"LJ  400# ANSI B16.5  Size  10\"","LJ  ","400# ","ANSI B16.5  ","10\"",250.0,"SS",444.5,101.6,53.8,277.4,320.5,387.4,31.8,16.0,"M30",24.0,169.6,6.0,273.05,323.9,254.0,127.0,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},38.8,null,null,"-"]
[null,"LJ  400# ANSI B16.5  Size  12\"","LJ  ","400# ","ANSI B16.5  ","12\"",300.0,"SS",520.7,108.0,57.2,328.2,374.7,450.9,35.1,16.0,"M33",26.0,180.4,6.0,323.85,381.0,254.0,152.4,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},56.6,null,null,"-"]
[null,"LJ  400# ANSI B16.5  Size  14\"","LJ  ","400# ","ANSI B16.5  ","14\"",350.0,"SS",584.2,117.3,60.5,360.2,425.5,514.4,35.1,20.0,"M33",26.0,188,7.0,355.6,412.8,304.8,152.4,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},78.6,null,null,"-"]
[null,"LJ  400# ANSI B16.5  Size  16\"","LJ  ","400# ","ANSI B16.5  ","16\"",400.0,"SS",647.7,127.0,63.5,411.2,482.6,571.5,38.1,20.0,"M36",29.0,200,7.0,406.4,469.9,304.8,152.4,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},100.0,null,null,"-"]
[null,"LJ  400# ANSI B16.5  Size  18\"","LJ  ","400# ","ANSI B16.5  ","18\"",450.0,"SS",711.2,136.7,66.5,462.3,533.4,628.7,38.1,24.0,"M36",29.0,206,7.0,457.2,533.4,304.8,152.4,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},122.0,null,null,"-"]
[null,"LJ  400# ANSI B16.5  Size  20\"","LJ  ","400# ","ANSI B16.5  ","20\"",500.0,"SS",774.7,146.1,69.9,514.4,587.2,685.8,41.1,24.0,"M39",31.0,216.8,7.0,508.0,584.2,304.8,152.4,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},145.0,null,null,"-"]
[null,"LJ  400# ANSI B16.5  Size  24\"","LJ  ","400# ","ANSI B16.5  ","24\"",600.0,"SS",914.4,158.8,76.2,616.0,701.5,812.8,47.8,24.0,"M45",36.0,239.4,7.0,609.6,692.2,304.8,152.4,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},217.0,null,null,"-"]
[null,"LJ  600# ANSI B16.5  Size  1/2\"","LJ  ","600# ","ANSI B16.5  ","1/2\"",15.0,"SS",95.3,22.4,14.2,22.9,38.1,66.5,15.7,4.0,"M12",10.0,59.4,3.0,21.34,35.05,76.2,50.8,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},0.72,null,null,"-"]
[null,"LJ  600# ANSI B16.5  Size  3/4\"","LJ  ","600# ","ANSI B16.5  ","3/4\"",20.0,"SS",117.3,25.4,15.7,28.2,47.8,82.6,19.1,4.0,"M16",13.0,68.4,3.0,26.67,42.9,76.2,50.8,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},1.25,null,null,"-"]
[null,"LJ  600# ANSI B16.5  Size  1\"","LJ  ","600# ","ANSI B16.5  ","1\"",25.0,"SS",124.0,26.9,17.5,35.1,53.8,88.9,19.1,4.0,"M16",13.0,72,3.0,33.4,50.8,101.6,50.8,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},1.5,null,null,"-"]
[null,"LJ  600# ANSI B16.5  Size  1¼\"","LJ  ","600# ","ANSI B16.5  ","1¼\"",32.0,"SS",133.4,28.4,20.6,43.7,63.5,98.6,19.1,4.0,"M16",13.0,78.2,3.0,42.16,63.5,101.6,50.8,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},2.0,null,null,"-"]
[null,"LJ  600# ANSI B16.5  Size  1½\"","LJ  ","600# ","ANSI B16.5  ","1½\"",40.0,"SS",155.4,31.8,22.4,50.0,69.9,114.3,22.3,4.0,"M20",16.0,87.8,3.0,48.26,73.15,101.6,50.8,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},2.92,null,null,"-"]
[null,"LJ  600# ANSI B16.5  Size  2\"","LJ  ","600# ","ANSI B16.5  ","2\"",50.0,"SS",165.1,36.6,25.4,62.5,84.1,127.0,19.1,8.0,"M16",13.0,88.8,4.0,60.33,91.95,152.4,63.5,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},3.55,null,null,"-"]
[null,"LJ  600# ANSI B16.5  Size  2½\"","LJ  ","600# ","ANSI B16.5  ","2½\"",65.0,"SS",190.5,41.1,28.4,75.4,100.1,149.4,22.4,8.0,"M20",16.0,100.8,4.0,73.03,104.65,152.4,63.5,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},5.23,null,null,"-"]
[null,"LJ  600# ANSI B16.5  Size  3\"","LJ  ","600# ","ANSI B16.5  ","3\"",80.0,"SS",209.6,46.0,31.8,91.4,117.3,168.1,22.4,8.0,"M20",16.0,107.6,4.0,88.9,127.0,152.4,63.5,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},6.95,null,null,"-"]
[null,"LJ  600# ANSI B16.5  Size  3½\"","LJ  ","600# ","ANSI B16.5  ","3½\"","-","SS",228.6,49.3,35.1,104.1,133.4,184.2,25.4,8.0,"M24",19.0,120.2,4.0,101.6,139.7,152.4,76.2,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},8.78,null,null,"-"]
[null,"LJ  600# ANSI B16.5  Size  4\"","LJ  ","600# ","ANSI B16.5  ","4\"",100.0,"SS",273.1,53.8,38.1,116.8,152.4,215.9,25.4,8.0,"M24",19.0,127.2,5.0,114.3,157.2,152.4,76.2,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},14.4,null,null,"-"]
[null,"LJ  600# ANSI B16.5  Size  5\"","LJ  ","600# ","ANSI B16.5  ","5\"",125.0,"SS",330.2,60.5,44.5,144.5,189.0,266.7,28.4,8.0,"M27",22.0,146,5.0,141.3,185.7,203.2,76.2,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},24.3,null,null,"-"]
[null,"LJ  600# ANSI B16.5  Size  6\"","LJ  ","600# ","ANSI B16.5  ","6\"",150.0,"SS",355.6,66.5,47.8,171.5,222.3,292.1,28.4,12.0,"M27",22.0,153.6,6.0,168.28,215.9,203.2,88.9,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},28.5,null,null,"-"]
[null,"LJ  600# ANSI B16.5  Size  8\"","LJ  ","600# ","ANSI B16.5  ","8\"",200.0,"SS",419.1,76.2,55.6,222.3,273.1,349.3,31.8,12.0,"M30",24.0,173.2,6.0,219.08,269.7,203.2,101.6,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},43.1,null,null,"-"]
[null,"LJ  600# ANSI B16.5  Size  10\"","LJ  ","600# ","ANSI B16.5  ","10\"",250.0,"SS",508.0,111.3,63.5,277.4,342.9,431.8,35.1,16.0,"M33",26.0,193,6.0,273.05,323.9,254.0,127.0,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},70.5,null,null,"-"]
[null,"LJ  600# ANSI B16.5  Size  12\"","LJ  ","600# ","ANSI B16.5  ","12\"",300.0,"SS",558.8,117.3,66.5,328.2,400.1,489.0,35.1,20.0,"M33",26.0,199,6.0,323.85,381.0,254.0,152.4,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},86.1,null,null,"-"]
[null,"LJ  600# ANSI B16.5  Size  14\"","LJ  ","600# ","ANSI B16.5  ","14\"",350.0,"SS",603.3,127.0,69.9,360.2,431.8,527.1,38.1,20.0,"M36",29.0,212.8,7.0,355.6,412.8,304.8,152.4,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},100.0,null,null,"-"]
[null,"LJ  600# ANSI B16.5  Size  16\"","LJ  ","600# ","ANSI B16.5  ","16\"",400.0,"SS",685.8,139.7,76.2,411.2,495.3,603.3,41.1,20.0,"M39",31.0,229.4,7.0,406.4,469.9,304.8,152.4,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},145.0,null,null,"-"]
[null,"LJ  600# ANSI B16.5  Size  18\"","LJ  ","600# ","ANSI B16.5  ","18\"",450.0,"SS",743.0,152.4,82.6,462.3,546.1,654.1,44.5,20.0,"M42",34.0,248.2,7.0,457.2,533.4,304.8,152.4,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},177.0,null,null,"-"]
[null,"LJ  600# ANSI B16.5  Size  20\"","LJ  ","600# ","ANSI B16.5  ","20\"",500.0,"SS",812.8,165.1,88.9,514.4,609.6,723.9,44.5,24.0,"M42",34.0,260.8,7.0,508.0,584.2,304.8,152.4,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},225.0,null,null,"-"]
[null,"LJ  600# ANSI B16.5  Size  24\"","LJ  ","600# ","ANSI B16.5  ","24\"",600.0,"SS",939.8,184.2,101.6,616.0,717.6,838.2,50.8,24.0,"M48",38.0,294.2,7.0,609.6,692.2,304.8,152.4,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},318.0,null,null,"-"]
[null,"LJ  900# ANSI B16.5  Size  1/2\"","LJ  ","900# ","ANSI B16.5  ","1/2\"",15.0,"SS",120.6,31.8,22.4,22.9,38.1,82.5,22.3,4.0,"M20",16.0,87.8,3.0,21.34,35.05,76.2,50.8,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},1.71,null,null,"-"]
[null,"LJ  900# ANSI B16.5  Size  3/4\"","LJ  ","900# ","ANSI B16.5  ","3/4\"",20.0,"SS",130.0,35.1,25.4,28.2,44.4,88.9,22.3,4.0,"M20",16.0,93.8,3.0,26.67,42.9,76.2,50.8,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},2.3,null,null,"-"]
[null,"LJ  900# ANSI B16.5  Size  1\"","LJ  ","900# ","ANSI B16.5  ","1\"",25.0,"SS",149.3,41.1,28.4,35.1,52.3,101.6,25.4,4.0,"M24",19.0,105.8,3.0,33.4,50.8,101.6,50.8,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},3.4,null,null,"-"]
[null,"LJ  900# ANSI B16.5  Size  1¼\"","LJ  ","900# ","ANSI B16.5  ","1¼\"",32.0,"SS",158.7,41.1,28.4,43.7,63.5,111.2,25.4,4.0,"M24",19.0,105.8,3.0,42.16,63.5,101.6,50.8,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},3.85,null,null,"-"]
[null,"LJ  900# ANSI B16.5  Size  1½\"","LJ  ","900# ","ANSI B16.5  ","1½\"",40.0,"SS",177.8,44.5,31.8,50.0,69.8,123.9,28.4,4.0,"M27",22.0,118.6,3.0,48.26,73.15,101.6,50.8,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},5.28,null,null,"-"]
[null,"LJ  900# ANSI B16.5  Size  2\"","LJ  ","900# ","ANSI B16.5  ","2\"",50.0,"SS",215.9,57.2,38.1,62.5,104.6,165.1,25.4,8.0,"M24",19.0,126.2,4.0,60.33,91.95,152.4,63.5,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},9.78,null,null,"-"]
[null,"LJ  900# ANSI B16.5  Size  2½\"","LJ  ","900# ","ANSI B16.5  ","2½\"",65.0,"SS",244.3,63.5,41.1,75.4,123.9,190.5,28.4,8.0,"M27",22.0,138.2,4.0,73.03,104.65,152.4,63.5,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},13.6,null,null,"-"]
[null,"LJ  900# ANSI B16.5  Size  3\"","LJ  ","900# ","ANSI B16.5  ","3\"",80.0,"SS",241.3,53.8,38.1,91.4,127.0,190.5,25.4,8.0,"M20",16.0,120.2,4.0,88.9,127.0,152.4,63.5,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},11.3,null,null,"-"]
[null,"LJ  900# ANSI B16.5  Size  4\"","LJ  ","900# ","ANSI B16.5  ","4\"",100.0,"SS",292.1,69.9,44.5,116.8,158.7,234.9,31.7,8.0,"M27",22.0,146,5.0,114.3,157.2,152.4,76.2,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},19.2,null,null,"-"]
[null,"LJ  900# ANSI B16.5  Size  5\"","LJ  ","900# ","ANSI B16.5  ","5\"",125.0,"SS",349.2,79.2,50.8,144.5,190.5,279.4,35.0,8.0,"M33",26.0,166.6,5.0,141.3,185.7,203.2,76.2,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},31.2,null,null,"-"]
[null,"LJ  900# ANSI B16.5  Size  6\"","LJ  ","900# ","ANSI B16.5  ","6\"",150.0,"SS",381.0,85.9,55.6,171.5,234.9,317.5,31.7,12.0,"M27",22.0,169.2,6.0,168.28,215.9,203.2,88.9,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},40.5,null,null,"-"]
[null,"LJ  900# ANSI B16.5  Size  8\"","LJ  ","900# ","ANSI B16.5  ","8\"",200.0,"SS",469.9,114.3,63.5,222.3,298.4,393.7,38.1,12.0,"M36",29.0,199,6.0,219.08,269.7,203.2,101.6,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},71.5,null,null,"-"]
[null,"LJ  900# ANSI B16.5  Size  10\"","LJ  ","900# ","ANSI B16.5  ","10\"",250.0,"SS",546.1,127.0,69.9,277.4,368.3,169.9,38.1,16.0,"M36",29.0,211.8,6.0,273.05,323.9,254.0,127.0,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},104.0,null,null,"-"]
[null,"LJ  900# ANSI B16.5  Size  12\"","LJ  ","900# ","ANSI B16.5  ","12\"",300.0,"SS",609.6,142.7,79.2,328.2,419.1,533.4,38.1,20.0,"M36",29.0,230.4,6.0,323.85,381.0,254.0,152.4,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},139.0,null,null,"-"]
[null,"LJ  900# ANSI B16.5  Size  14\"","LJ  ","900# ","ANSI B16.5  ","14\"",350.0,"SS",641.3,155.4,85.9,360.2,450.8,558.8,41.1,20.0,"M39",29.0,244.8,7.0,355.6,412.8,304.8,152.4,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},161.0,null,null,"-"]
[null,"LJ  900# ANSI B16.5  Size  16\"","LJ  ","900# ","ANSI B16.5  ","16\"",400.0,"SS",704.8,165.1,88.9,411.2,508.0,615.9,44.4,20.0,"M42",34.0,260.8,7.0,406.4,469.9,304.8,152.4,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},194.0,null,null,"-"]
[null,"LJ  900# ANSI B16.5  Size  18\"","LJ  ","900# ","ANSI B16.5  ","18\"",450.0,"SS",787.4,190.5,101.6,462.3,565.1,685.8,50.8,20.0,"M48",38.0,294.2,7.0,457.2,533.4,304.8,152.4,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},267.0,null,null,"-"]
[null,"LJ  900# ANSI B16.5  Size  20\"","LJ  ","900# ","ANSI B16.5  ","20\"",500.0,"SS",857.2,209.6,108.0,514.4,622.3,749.3,53.8,20.0,"M52",42.0,315,7.0,508.0,584.2,304.8,152.4,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},334.0,null,null,"-"]
[null,"LJ  900# ANSI B16.5  Size  24\"","LJ  ","900# ","ANSI B16.5  ","24\"",600.0,"SS",1041.4,266.7,139.7,616.0,749.3,901.7,66.5,20.0,"M64",51.0,396.4,7.0,609.6,692.2,304.8,152.4,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},618.0,null,null,"-"]
[null,"LJ  1500# ANSI B16.5  Size  1/2\"","LJ  ","1500# ","ANSI B16.5  ","1/2\"",15.0,"SS",120.6,31.8,22.4,22.9,38.1,82.5,22.3,4.0,"M20",16.0,87.8,3.0,21.34,35.05,76.2,50.8,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},1.71,null,null,"-"]
[null,"LJ  1500# ANSI B16.5  Size  3/4\"","LJ  ","1500# ","ANSI B16.5  ","3/4\"",20.0,"SS",130.0,35.1,25.4,28.2,44.4,88.9,22.3,4.0,"M20",16.0,93.8,3.0,26.67,42.9,76.2,50.8,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},2.3,null,null,"-"]
[null,"LJ  1500# ANSI B16.5  Size  1\"","LJ  ","1500# ","ANSI B16.5  ","1\"",25.0,"SS",149.3,41.1,28.4,35.1,52.3,101.6,25.4,4.0,"M24",19.0,105.8,3.0,33.4,50.8,101.6,50.8,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},3.4,null,null,"-"]
[null,"LJ  1500# ANSI B16.5  Size  1¼\"","LJ  ","1500# ","ANSI B16.5  ","1¼\"",32.0,"SS",158.7,41.1,28.4,43.7,63.5,111.2,25.4,4.0,"M24",19.0,105.8,3.0,42.16,63.5,101.6,50.8,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},3.85,null,null,"-"]
[null,"LJ  1500# ANSI B16.5  Size  1½\"","LJ  ","1500# ","ANSI B16.5  ","1½\"",40.0,"SS",177.8,44.5,31.8,50.0,69.8,123.9,28.4,4.0,"M27",22.0,118.6,3.0,48.26,73.15,101.6,50.8,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},5.28,null,null,"-"]
[null,"LJ  1500# ANSI B16.5  Size  2\"","LJ  ","1500# ","ANSI B16.5  ","2\"",50.0,"SS",215.9,57.2,38.1,62.5,104.6,165.1,25.4,8.0,"M24",19.0,126.2,4.0,60.33,91.95,152.4,63.5,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},9.78,null,null,"-"]
[null,"LJ  1500# ANSI B16.5  Size  2½\"","LJ  ","1500# ","ANSI B16.5  ","2½\"",65.0,"SS",244.3,63.5,41.1,75.4,123.9,190.5,28.4,8.0,"M27",22.0,138.2,4.0,73.03,104.65,152.4,63.5,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},13.6,null,null,"-"]
[null,"LJ  1500# ANSI B16.5  Size  3\"","LJ  ","1500# ","ANSI B16.5  ","3\"",80.0,"SS",266.7,73.2,47.8,91.4,133.3,203.2,31.7,8.0,"M30",24.0,155.6,4.0,88.9,127.0,152.4,63.5,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},17.8,null,null,"-"]
[null,"LJ  1500# ANSI B16.5  Size  4\"","LJ  ","1500# ","ANSI B16.5  ","4\"",100.0,"SS",311.1,90.4,53.8,116.8,162.0,241.3,35.0,8.0,"M33",26.0,172.6,5.0,114.3,157.2,152.4,76.2,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},27.5,null,null,"-"]
[null,"LJ  1500# ANSI B16.5  Size  5\"","LJ  ","1500# ","ANSI B16.5  ","5\"",125.0,"SS",374.6,104.6,73.2,144.5,196.8,292.1,41.1,8.0,"M39",31.0,221.4,5.0,141.3,185.7,203.2,76.2,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},51.5,null,null,"-"]
[null,"LJ  1500# ANSI B16.5  Size  6\"","LJ  ","1500# ","ANSI B16.5  ","6\"",150.0,"SS",393.7,119.1,82.6,171.5,228.6,317.5,38.1,12.0,"M36",29.0,237.2,6.0,168.28,215.9,203.2,88.9,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},62.0,null,null,"-"]
[null,"LJ  1500# ANSI B16.5  Size  8\"","LJ  ","1500# ","ANSI B16.5  ","8\"",200.0,"SS",482.6,142.7,91.9,222.3,292.1,393.7,44.4,12.0,"M42",34.0,265.8,6.0,219.08,269.7,203.2,101.6,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},105.0,null,null,"-"]
[null,"LJ  1500# ANSI B16.5  Size  10\"","LJ  ","1500# ","ANSI B16.5  ","10\"",250.0,"SS",584.2,177.8,108.0,277.4,368.3,485.6,50.8,12.0,"M48",38.0,306,6.0,273.05,323.9,254.0,127.0,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},179.0,null,null,"-"]
[null,"LJ  1500# ANSI B16.5  Size  12\"","LJ  ","1500# ","ANSI B16.5  ","12\"",300.0,"SS",673.1,218.9,124.0,328.2,450.8,571.5,53.8,16.0,"M52",42.0,346,6.0,323.85,381.0,254.0,152.4,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},269.0,null,null,"-"]
[null,"LJ  1500# ANSI B16.5  Size  14\"","LJ  ","1500# ","ANSI B16.5  ","14\"",350.0,"SS",749.3,241.3,133.4,360.2,495.3,635.0,60.4,16.0,"M56",45.0,371.8,7.0,355.6,412.8,304.8,152.4,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},365.0,null,null,"-"]
[null,"LJ  1500# ANSI B16.5  Size  16\"","LJ  ","1500# ","ANSI B16.5  ","16\"",400.0,"SS",825.5,260.4,146.1,411.2,552.4,704.8,66.5,16.0,"M60",48.0,403.2,7.0,406.4,469.9,304.8,152.4,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},459.0,null,null,"-"]
[null,"LJ  1500# ANSI B16.5  Size  18\"","LJ  ","1500# ","ANSI B16.5  ","18\"",450.0,"SS",914.4,276.4,162.1,462.3,596.9,774.7,73.1,16.0,"M68",54.0,447.2,7.0,457.2,533.4,304.8,152.4,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},598.0,null,null,"-"]
[null,"LJ  1500# ANSI B16.5  Size  20\"","LJ  ","1500# ","ANSI B16.5  ","20\"",500.0,"SS",984.2,292.1,177.8,514.4,641.3,831.8,79.2,16.0,"M76",61.0,492.6,7.0,508.0,584.2,304.8,152.4,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},712.0,null,null,"-"]
[null,"LJ  1500# ANSI B16.5  Size  24\"","LJ  ","1500# ","ANSI B16.5  ","24\"",600.0,"SS",1168.4,330.2,203.2,616.0,762.0,990.6,91.9,16.0,"M80",64.0,549.4,7.0,609.6,692.2,304.8,152.4,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},1090.0,null,null,"-"]
[null,"LJ  2500# ANSI B16.5  Size  1/2\"","LJ  ","2500# ","ANSI B16.5  ","1/2\"",15.0,"SS",133.4,39.6,30.2,22.9,42.9,88.9,22.4,4.0,"M20",16.0,103.4,3.0,21.34,35.05,76.2,50.8,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},2.92,null,null,"-"]
[null,"LJ  2500# ANSI B16.5  Size  3/4\"","LJ  ","2500# ","ANSI B16.5  ","3/4\"",20.0,"SS",139.7,42.9,31.8,28.2,50.8,95.3,22.4,4.0,"M20",16.0,106.6,3.0,26.67,42.9,76.2,50.8,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},3.4,null,null,"-"]
[null,"LJ  2500# ANSI B16.5  Size  1\"","LJ  ","2500# ","ANSI B16.5  ","1\"",25.0,"SS",158.8,47.8,35.1,35.1,57.2,108.0,25.4,4.0,"M24",19.0,119.2,3.0,33.4,50.8,101.6,50.8,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},4.77,null,null,"-"]
[null,"LJ  2500# ANSI B16.5  Size  1¼\"","LJ  ","2500# ","ANSI B16.5  ","1¼\"",32.0,"SS",184.2,52.3,38.1,43.7,73.2,130.0,28.4,4.0,"M27",22.0,131.2,3.0,42.16,63.5,101.6,50.8,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},7.08,null,null,"-"]
[null,"LJ  2500# ANSI B16.5  Size  1½\"","LJ  ","2500# ","ANSI B16.5  ","1½\"",40.0,"SS",203.2,60.5,44.5,50.0,79.2,146.1,31.8,4.0,"M30",24.0,148,3.0,48.26,73.15,101.6,50.8,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},9.93,null,null,"-"]
[null,"LJ  2500# ANSI B16.5  Size  2\"","LJ  ","2500# ","ANSI B16.5  ","2\"",50.0,"SS",235.0,69.9,50.8,62.5,95.3,171.5,28.4,8.0,"M27",22.0,157.6,4.0,60.33,91.95,152.4,63.5,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},14.7,null,null,"-"]
[null,"LJ  2500# ANSI B16.5  Size  2½\"","LJ  ","2500# ","ANSI B16.5  ","2½\"",65.0,"SS",266.7,79.2,57.2,75.4,114.3,196.9,31.8,8.0,"M30",24.0,174.4,4.0,73.03,104.65,152.4,63.5,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},21.3,null,null,"-"]
[null,"LJ  2500# ANSI B16.5  Size  3\"","LJ  ","2500# ","ANSI B16.5  ","3\"",80.0,"SS",304.8,91.9,66.5,91.4,133.4,228.6,35.1,8.0,"M33",26.0,197,4.0,88.9,127.0,152.4,63.5,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},32.3,null,null,"-"]
[null,"LJ  2500# ANSI B16.5  Size  4\"","LJ  ","2500# ","ANSI B16.5  ","4\"",100.0,"SS",355.6,108.0,76.2,116.8,165.1,273.1,41.1,8.0,"M39",31.0,227.4,5.0,114.3,157.2,152.4,76.2,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},52.5,null,null,"-"]
[null,"LJ  2500# ANSI B16.5  Size  5\"","LJ  ","2500# ","ANSI B16.5  ","5\"",125.0,"SS",419.1,130.0,91.9,144.5,203.2,323.9,47.8,8.0,"M45",36.0,268.8,5.0,141.3,185.7,203.2,76.2,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},82.6,null,null,"-"]
[null,"LJ  2500# ANSI B16.5  Size  6\"","LJ  ","2500# ","ANSI B16.5  ","6\"",150.0,"SS",482.6,152.4,108.0,171.5,235.0,368.3,53.8,8.0,"M48",38.0,306,6.0,168.28,215.9,203.2,88.9,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},127.0,null,null,"-"]
[null,"LJ  2500# ANSI B16.5  Size  8\"","LJ  ","2500# ","ANSI B16.5  ","8\"",200.0,"SS",552.5,177.8,127.0,222.3,304.8,438.2,53.8,12.0,"M48",38.0,344,6.0,219.08,269.7,203.2,101.6,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},186.0,null,null,"-"]
[null,"LJ  2500# ANSI B16.5  Size  10\"","LJ  ","2500# ","ANSI B16.5  ","10\"",250.0,"SS",673.1,228.6,165.1,277.4,374.7,539.8,66.5,12.0,"M60",48.0,440.2,6.0,273.05,323.9,254.0,127.0,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},352.0,null,null,"-"]
[null,"LJ  2500# ANSI B16.5  Size  12\"","LJ  ","2500# ","ANSI B16.5  ","12\"",300.0,"SS",762.0,254.0,184.2,328.2,441.5,619.3,73.2,12.0,"M64",51.0,484.4,6.0,323.85,381.0,254.0,152.4,"-","",{"$f":"'Lapjoint fl.'!$C$45","v":""},501.0,null,null,"-"]
[null,{"$f":"CONCATENATE($C200,$D200,$E200,$G$3,$G200,$H$3,$H200)","v":"LJ  PN  6  Din 2641 R1 DN 10  Mat. CSt."},"LJ  ","PN  6  ","Din 2641 R1 ","1/4\"",10.0,"CSt."]
[null,"LJ  PN  6  Din 2641 R2 DN 10  Mat. CSt.","LJ  ","PN  6  ","Din 2641 R2 ","1/4\"",10.0,"CSt."]
[null,"LJ  PN  6  Din 2641 R1 DN 15  Mat. CSt.","LJ  ","PN  6  ","Din 2641 R1 ","1/2\"",15.0,"CSt."]
[null,"LJ  PN  6  Din 2641 R2 DN 15  Mat. CSt.","LJ  ","PN  6  ","Din 2641 R2 ","1/2\"",15.0,"CSt."]
[null,"LJ  PN  6  Din 2641 R1 DN 20  Mat. CSt.","LJ  ","PN  6  ","Din 2641 R1 ","3/4\"",20.0,"CSt."]
[null,"LJ  PN  6  Din 2641 R2 DN 20  Mat. CSt.","LJ  ","PN  6  ","Din 2641 R2 ","3/4\"",20.0,"CSt."]
[null,"LJ  PN  6  Din 2641 R1 DN 25  Mat. CSt.","LJ  ","PN  6  ","Din 2641 R1 ","1\"",25.0,"CSt."]
[null,"LJ  PN  6  Din 2641 R2 DN 25  Mat. CSt.","LJ  ","PN  6  ","Din 2641 R2 ","1\"",25.0,"CSt."]
[null,"LJ  PN  6  Din 2642 R1 DN 32  Mat. CSt.","LJ  ","PN  6  ","Din 2642 R1 ","1¼\"",32.0,"CSt."]
[null,"LJ  PN  6  Din 2642 R2 DN 32  Mat. CSt.","LJ  ","PN  6  ","Din 2642 R2 ","1¼\"",32.0,"CSt."]
[null,"LJ  PN  6  Din 2642 R1 DN 40  Mat. CSt.","LJ  ","PN  6  ","Din 2642 R1 ","1½\"",40.0,"CSt."]
[null,"LJ  PN  6  Din 2642 R2 DN 40  Mat. CSt.","LJ  ","PN  6  ","Din 2642 R2 ","1½\"",40.0,"CSt."]
[null,"LJ  PN  6  Din 2642 R1 DN 50  Mat. CSt.","LJ  ","PN  6  ","Din 2642 R1 ","2\"",50.0,"CSt."]
[null,"LJ  PN  6  Din 2642 R2 DN 50  Mat. CSt.","LJ  ","PN  6  ","Din 2642 R2 ","2\"",50.0,"CSt."]
[null,"LJ  PN  6  Din 2642 R1 DN 65  Mat. CSt.","LJ  ","PN  6  ","Din 2642 R1 ","2½\"",65.0,"CSt."]
[null,"LJ  PN  6  Din 2642 R1 DN 80  Mat. CSt.","LJ  ","PN  6  ","Din 2642 R1 ","3\"",80.0,"CSt."]
[null,"LJ  PN  6  Din 2642 R1 DN 100  Mat. CSt.","LJ  ","PN  6  ","Din 2642 R1 ","4\"",100.0,"CSt."]
[null,"LJ  PN  6  Din 2642 R2 DN 100  Mat. CSt.","LJ  ","PN  6  ","Din 2642 R2 ","4\"",100.0,"CSt."]
[null,"LJ  PN  6  Din 2642 R1 DN 125  Mat. CSt.","LJ  ","PN  6  ","Din 2642 R1 ","5\"",125.0,"CSt."]
[null,"LJ  PN  6  Din 2642 R2 DN 125  Mat. CSt.","LJ  ","PN  6  ","Din 2642 R2 ","5\"",125.0,"CSt."]
[null,"LJ  PN  6  Din 2642 R1 DN 150  Mat. CSt.","LJ  ","PN  6  ","Din 2642 R1 ","6\"",150.0,"CSt."]
[null,"LJ  PN  6  Din 2642 R2 DN 150  Mat. CSt.","LJ  ","PN  6  ","Din 2642 R2 ","6\"",150.0,"CSt."]
[null,"LJ  PN  6  Din 2642 R1 DN 200  Mat. CSt.","LJ  ","PN  6  ","Din 2642 R1 ","8\"",200.0,"CSt."]
[null,"LJ  PN  6  Din 2642 R1 DN 250  Mat. CSt.","LJ  ","PN  6  ","Din 2642 R1 ","10\"",250.0,"CSt."]
[null,"LJ  PN  6  Din 2642 R2 DN 250  Mat. CSt.","LJ  ","PN  6  ","Din 2642 R2 ","10\"",250.0,"CSt."]
[null,"LJ  PN  6  Din 2642 R1 DN 300  Mat. CSt.","LJ  ","PN  6  ","Din 2642 R1 ","12\"",300.0,"CSt."]
[null,"LJ  PN  6  Din 2642 R1 DN 350  Mat. CSt.","LJ  ","PN  6  ","Din 2642 R1 ","14\"",350.0,"CSt."]
[null,"LJ  PN  6  Din 2642 R2 DN 350  Mat. CSt.","LJ  ","PN  6  ","Din 2642 R2 ","14\"",350.0,"CSt."]
[null,"LJ  PN  6  Din 2642 R1 DN 400  Mat. CSt.","LJ  ","PN  6  ","Din 2642 R1 ","16\"",400.0,"CSt."]
[null,"LJ  PN  6  Din 2642 R2 DN 400  Mat. CSt.","LJ  ","PN  6  ","Din 2642 R2 ","16\"",400.0,"CSt."]
[null,"LJ  PN  6  Din 2642 R1 DN 500  Mat. CSt.","LJ  ","PN  6  ","Din 2642 R1 ","20\"",500.0,"CSt."]
[null,"LJ  PN  6  Din 2642 R1 DN 600  Mat. CSt.","LJ  ","PN  6  ","Din 2642 R1 ","24\"",600.0,"CSt."]
[null,"LJ  PN  6  Din 2642 R1 DN 700  Mat. CSt.","LJ  ","PN  6  ","Din 2642 R1 ","28\"",700.0,"CSt."]
[null,"LJ  PN  6  Din 2642 R1 DN 800  Mat. CSt.","LJ  ","PN  6  ","Din 2642 R1 ","32\"",800.0,"CSt."]
[null,"LJ  PN  6  Din 2642 R1 DN 900  Mat. CSt.","LJ  ","PN  6  ","Din 2642 R1 ","36\"",900.0,"CSt."]
[null,"LJ  PN  6  Din 2642 R1 DN 1000  Mat. CSt.","LJ  ","PN  6  ","Din 2642 R1 ","40\"",1000.0,"CSt."]
[null,"LJ  PN  6  Din 2642 R1 DN 1200  Mat. CSt.","LJ  ","PN  6  ","Din 2642 R1 ","48\"",1200.0,"CSt."]
[null,"LJ  PN 10  Din 2642 R1 DN 10  Mat. CSt.","LJ  ","PN 10  ","Din 2642 R1 ","1/4\"",10.0,"CSt.",90.0,"-",16.0,19.0,"-",60.0,14.0,4.0,"M12",10.0,{"$f":"(K237+R237+Z237+4)*2+T237","v":69},3.0,17.2,40.0,"-","-",9.0,3.0,1.8,0.59,null,null,0.09]
[null,"LJ  PN 10  Din 2642 R2 DN 10  Mat. CSt.","LJ  ","PN 10  ","Din 2642 R2 ","1/4\"",10.0,"CSt.",91.0,"-",17.0,16.0,"-",60.0,14.0,4.0,"M12",10.0,71,3.0,14.0,40.0,"-","-",9.0,3.0,1.8,0.59,null,null,0.09]
[null,"LJ  PN 10  Din 2642 R1 DN 15  Mat. CSt.","LJ  ","PN 10  ","Din 2642 R1 ","1/2\"",15.0,"CSt.",95.0,"-",16.0,24.0,"-",65.0,14.0,4.0,"M12",10.0,69,3.0,21.3,45.0,"-","-",9.0,3.0,2.0,0.69,null,null,0.1]
[null,"LJ  PN 10  Din 2642 R2 DN 15  Mat. CSt.","LJ  ","PN 10  ","Din 2642 R2 ","1/2\"",15.0,"CSt.",96.0,"-",17.0,22.0,"-",65.0,14.0,4.0,"M12",10.0,71,3.0,20.0,45.0,"-","-",9.0,3.0,2.0,0.69,null,null,0.1]
[null,"LJ  PN 10  Din 2642 R1 DN 20  Mat. CSt.","LJ  ","PN 10  ","Din 2642 R1 ","3/4\"",20.0,"CSt.",105.0,"-",16.0,30.0,"-",75.0,14.0,4.0,"M12",10.0,69,3.0,26.9,58.0,"-","-",12.0,3.0,2.0,0.8,null,null,0.2]
[null,"LJ  PN 10  Din 2642 R2 DN 20  Mat. CSt.","LJ  ","PN 10  ","Din 2642 R2 ","3/4\"",20.0,"CSt.",106.0,"-",17.0,28.0,"-",75.0,14.0,4.0,"M12",10.0,71,3.0,25.0,58.0,"-","-",12.0,3.0,2.0,0.8,null,null,0.2]
[null,"LJ  PN 10  Din 2642 R1 DN 25  Mat. CSt.","LJ  ","PN 10  ","Din 2642 R1 ","1\"",25.0,"CSt.",115.0,"-",16.0,36.0,"-",85.0,14.0,4.0,"M12",10.0,69,3.0,33.7,68.0,"-","-",15.0,3.0,2.0,1.11,null,null,0.28]
[null,"LJ  PN 10  Din 2642 R2 DN 25  Mat. CSt.","LJ  ","PN 10  ","Din 2642 R2 ","1\"",25.0,"CSt.",116.0,"-",17.0,33.0,"-",85.0,14.0,4.0,"M12",10.0,71,3.0,30.0,68.0,"-","-",15.0,3.0,2.0,1.11,null,null,0.28]
[null,"LJ  PN 10  Din 2642 R1 DN 32  Mat. CSt.","LJ  ","PN 10  ","Din 2642 R1 ","1¼\"",32.0,"CSt.",140.0,"-",16.0,46.0,"-",100.0,18.0,4.0,"M16",13.0,76,3.0,42.4,78.0,"-","-",15.0,3.5,2.6,1.64,null,null,0.34]
[null,"LJ  PN 10  Din 2642 R2 DN 32  Mat. CSt.","LJ  ","PN 10  ","Din 2642 R2 ","1¼\"",32.0,"CSt.",141.0,"-",17.0,42.0,"-",100.0,18.0,4.0,"M16",13.0,78,3.0,38.0,78.0,"-","-",15.0,3.5,2.6,1.64,null,null,0.34]
[null,"LJ  PN 10  Din 2642 R1 DN 40  Mat. CSt.","LJ  ","PN 10  ","Din 2642 R1 ","1½\"",40.0,"CSt.",150.0,"-",16.0,54.0,"-",110.0,18.0,4.0,"M16",13.0,76,3.0,48.3,88.0,"-","-",17.0,3.5,2.6,1.86,null,null,0.43]
[null,"LJ  PN 10  Din 2642 R2 DN 40  Mat. CSt.","LJ  ","PN 10  ","Din 2642 R2 ","1½\"",40.0,"CSt.",151.0,"-",17.0,50.0,"-",110.0,18.0,4.0,"M16",13.0,78,3.0,44.5,88.0,"-","-",17.0,3.5,2.6,1.86,null,null,0.43]
[null,"LJ  PN 10  Din 2642 R1 DN 50  Mat. CSt.","LJ  ","PN 10  ","Din 2642 R1 ","2\"",50.0,"CSt.",165.0,"-",18.0,65.0,"-",125.0,18.0,4.0,"M16",13.0,81,4.0,60.3,102.0,"-","-",23.0,3.5,2.6,2.2,null,null,0.62]
[null,"LJ  PN 10  Din 2642 R2 DN 50  Mat. CSt.","LJ  ","PN 10  ","Din 2642 R2 ","2\"",50.0,"CSt.",166.0,"-",19.0,62.0,"-",125.0,18.0,4.0,"M16",13.0,83,4.0,57.0,102.0,"-","-",23.0,3.5,2.6,2.2,null,null,0.62]
[null,"LJ  PN 10  Din 2642 R1 DN 65  Mat. CSt.","LJ  ","PN 10  ","Din 2642 R1 ","2½\"",65.0,"CSt.",185.0,"-",18.0,81.0,"-",145.0,18.0,4.0,"M16",13.0,81,4.0,76.1,122.0,"-","-",23.0,3.5,2.6,2.62,null,null,0.79]
[null,"LJ  PN 10  Din 2642 R1 DN 80  Mat. CSt.","LJ  ","PN 10  ","Din 2642 R1 ","3\"",80.0,"CSt.",200.0,"-",20.0,94.0,"-",160.0,18.0,8.0,"M16",13.0,86,4.0,88.9,138.0,"-","-",23.0,4.0,3.2,3.32,null,null,1.1]
[null,"LJ  PN 10  Din 2642 R1 DN 100  Mat. CSt.","LJ  ","PN 10  ","Din 2642 R1 ","4\"",100.0,"CSt.",220.0,"-",20.0,119.0,"-",180.0,18.0,8.0,"M16",13.0,87,5.0,114.3,158.0,"-","-",28.0,4.0,3.2,3.67,null,null,1.3]
[null,"LJ  PN 10  Din 2642 R2 DN 100  Mat. CSt.","LJ  ","PN 10  ","Din 2642 R2 ","4\"",100.0,"CSt.",221.0,"-",21.0,113.0,"-",180.0,18.0,8.0,"M16",13.0,89,5.0,108.0,158.0,"-","-",28.0,4.0,3.2,3.67,null,null,1.3]
[null,"LJ  PN 10  Din 2642 R1 DN 125  Mat. CSt.","LJ  ","PN 10  ","Din 2642 R1 ","5\"",125.0,"CSt.",250.0,"-",22.0,145.0,"-",210.0,18.0,8.0,"M16",13.0,91,5.0,139.7,188.0,"-","-",30.0,4.0,3.2,4.54,null,null,2.0]
[null,"LJ  PN 10  Din 2642 R2 DN 125  Mat. CSt.","LJ  ","PN 10  ","Din 2642 R2 ","5\"",125.0,"CSt.",251.0,"-",23.0,138.0,"-",210.0,18.0,8.0,"M16",13.0,93,5.0,133.0,188.0,"-","-",30.0,4.0,3.2,4.54,null,null,2.0]
[null,"LJ  PN 10  Din 2642 R1 DN 150  Mat. CSt.","LJ  ","PN 10  ","Din 2642 R1 ","6\"",150.0,"CSt.",285.0,"-",22.0,173.0,"-",240.0,22.0,8.0,"M20",16.0,98,6.0,168.3,212.0,"-","-",30.0,4.0,3.2,5.6,null,null,2.2]
[null,"LJ  PN 10  Din 2642 R2 DN 150  Mat. CSt.","LJ  ","PN 10  ","Din 2642 R2 ","6\"",150.0,"CSt.",286.0,"-",23.0,164.0,"-",240.0,22.0,8.0,"M20",16.0,100,6.0,159.0,212.0,"-","-",30.0,4.0,3.2,5.6,null,null,2.2]
[null,"LJ  PN 10  Din 2642 R1 DN 200  Mat. CSt.","LJ  ","PN 10  ","Din 2642 R1 ","8\"",200.0,"CSt.",340.0,"-",24.0,225.0,"-",295.0,22.0,8.0,"M20",16.0,102,6.0,219.1,268.0,"-","-",30.0,4.0,3.2,7.46,null,null,3.1]
[null,"LJ  PN 10  Din 2642 R1 DN 250  Mat. CSt.","LJ  ","PN 10  ","Din 2642 R1 ","10\"",250.0,"CSt.",395.0,"-",26.0,279.0,"-",350.0,22.0,12.0,"M20",16.0,108,6.0,273.0,320.0,"-","-",30.0,5.0,4.0,10.3,null,null,4.2]
[null,"LJ  PN 10  Din 2642 R2 DN 250  Mat. CSt.","LJ  ","PN 10  ","Din 2642 R2 ","10\"",250.0,"CSt.",396.0,"-",27.0,273.0,"-",350.0,22.0,12.0,"M20",16.0,110,6.0,267.0,320.0,"-","-",30.0,5.0,4.0,10.3,null,null,4.2]
[null,"LJ  PN 10  Din 2642 R1 DN 300  Mat. CSt.","LJ  ","PN 10  ","Din 2642 R1 ","12\"",300.0,"CSt.",445.0,"-",26.0,329.0,"-",400.0,22.0,12.0,"M20",16.0,108,6.0,323.9,370.0,"-","-",35.0,5.0,4.0,14.0,null,null,4.9]
[null,"LJ  PN 10  Din 2642 R1 DN 350  Mat. CSt.","LJ  ","PN 10  ","Din 2642 R1 ","14\"",350.0,"CSt.",505.0,"-",26.0,362.0,"-",460.0,22.0,16.0,"M20",16.0,"-",7.0,355.6,430.0,"-","-","-","-","-",18.5,null,null,6.7]
[null,"LJ  PN 10  Din 2642 R2 DN 350  Mat. CSt.","LJ  ","PN 10  ","Din 2642 R2 ","14\"",350.0,"CSt.",506.0,"-",27.0,374.0,"-",460.0,22.0,16.0,"M20",16.0,"-",7.0,368.0,430.0,"-","-","-","-","-",18.5,null,null,6.7]
[null,"LJ  PN 10  Din 2642 R1 DN 400  Mat. CSt.","LJ  ","PN 10  ","Din 2642 R1 ","16\"",400.0,"CSt.",565.0,"-",32.0,413.0,"-",515.0,26.0,16.0,"M24",19.0,"-",7.0,406.4,482.0,"-","-","-","-","-",25.0,null,null,8.3]
[null,"LJ  PN 10  Din 2642 R2 DN 400  Mat. CSt.","LJ  ","PN 10  ","Din 2642 R2 ","16\"",400.0,"CSt.",566.0,"-",33.0,426.0,"-",515.0,26.0,16.0,"M24",19.0,"-",7.0,419.0,482.0,"-","-","-","-","-",25.0,null,null,8.3]
[null,"LJ  PN 10  Din 2642 R1 DN 500  Mat. CSt.","LJ  ","PN 10  ","Din 2642 R1 ","20\"",500.0,"CSt.",670.0,"-",34.0,517.0,"-",620.0,26.0,20.0,"m24",19.0,"-",7.0,508.0,585.0,"-","-","-","-","-",37.0,null,null,11.5]
[null,"LJ  PN 10  Din 2642 R1 DN 600  Mat. CSt.","LJ  ","PN 10  ","Din 2642 R1 ","24\"",600.0,"CSt.",780.0,"-",36.0,618.0,"-",725.0,30.0,20.0,"M27",22.0,"-",7.0,610.0,685.0,"-","-","-","-","-",56.3,null,null,15.6]
[null,"LJ  PN 10  Din 2642 R1 DN 700  Mat. CSt.","LJ  ","PN 10  ","Din 2642 R1 ","28\"",700.0,"CSt.",895.0,"-",40.0,721.0,"-",840.0,30.0,24.0,"M27",22.0,"-",7.0,711.0,800.0,"-","-","-","-","-",80.4,null,null,23.2]
[null,"LJ  PN 10  Din 2642 R1 DN 800  Mat. CSt.","LJ  ","PN 10  ","Din 2642 R1 ","32\"",800.0,"CSt.",1015.0,"-",44.0,824.0,"-",950.0,33.0,24.0,"M30",24.0,"-",7.0,813.0,905.0,"-","-","-","-","-",113.2,null,null,29.2]

{"sheet":"Data Stub-Collar","index":11,"n_rows":87,"n_cols":16,"rows_kept":87,"cut":false,"hidden":true,"merged":[[0,7,0,13],[0,14,0,15]]}
["Data Stub ends and Collars",null,null,null,null,null,null,"Collar/Stub end",null,null,null,null,null,null,"Weight"]
[null,null,null,"Size  ","Size",null,null,"Pipe ø","Flange ø","height","height","height","thickn.","thickn.","Stub ASA","Stub MSS"]
[null,"Norm / Size / Schedule","Norm","NPS","DN ","   Sch  ","  Mat. ","d1","d4","b2-ASA","b2-MSS","b2 (C)","s","s1","W2","W3"]
[1.0,{"$f":"CONCATENATE($C4,$D$2,$D4,$F$3,$F4)","v":"ANSI B16.5  Size  1/2\"   Sch  5S"},"ANSI B16.5  ","1/2\"",15.0,"5S","SS",21.3,35.05,76.2,50.8,"-",1.65,1.65,0.07076538671155265,0.04819219032956057]
[null,"ANSI B16.5  Size  1/2\"   Sch  10S","ANSI B16.5  ","1/2\"",15.0,"10S","SS",21.3,35.05,76.2,50.8,"-",2.11,2.11,0.08861814661451187,0.06041936201800996]
[null,"ANSI B16.5  Size  1/2\"   Sch  40S","ANSI B16.5  ","1/2\"",15.0,"40S","SS",21.3,35.05,76.2,50.8,"-",2.77,2.77,0.11280440528709768,0.07704252091180826]
[null,"ANSI B16.5  Size  1/2\"   Sch  80S","ANSI B16.5  ","1/2\"",15.0,"80S","SS",21.3,35.05,76.2,50.8,"-",3.73,3.73,0.1449788534595513,0.09928570978942894]
[null,"ANSI B16.5  Size  3/4\"   Sch  5S","ANSI B16.5  ","3/4\"",20.0,"5S","SS",26.7,42.9,76.2,50.8,"-",1.65,1.65,0.09167474174412238,0.0628487718048725]
[null,"ANSI B16.5  Size  3/4\"   Sch  10S","ANSI B16.5  ","3/4\"",20.0,"10S","SS",26.7,42.9,76.2,50.8,"-",2.11,2.11,0.11535677638343436,0.07916202075310581]
[null,"ANSI B16.5  Size  3/4\"   Sch  40S","ANSI B16.5  ","3/4\"",20.0,"40S","SS",26.7,42.9,76.2,50.8,"-",2.87,2.87,0.15269171849157295,0.10496014366550116]
[null,"ANSI B16.5  Size  3/4\"   Sch  80S","ANSI B16.5  ","3/4\"",20.0,"80S","SS",26.7,42.9,76.2,50.8,"-",3.91,3.91,0.20016383022031475,0.13793252638923467]
[null,"ANSI B16.5  Size  1\"   Sch  5S","ANSI B16.5  ","1\"",25.0,"5S","SS",33.4,50.8,101.6,50.8,"-",1.65,1.65,0.150318890202087,0.08002239014748243]
[null,"ANSI B16.5  Size  1\"   Sch  10S","ANSI B16.5  ","1\"",25.0,"10S","SS",33.4,50.8,101.6,50.8,"-",2.77,2.77,0.24435930660811783,0.1304786745455315]
[null,"ANSI B16.5  Size  1\"   Sch  40S","ANSI B16.5  ","1\"",25.0,"40S","SS",33.4,50.8,101.6,50.8,"-",3.38,3.38,0.29285846428802187,0.15664566596341897]
[null,"ANSI B16.5  Size  1\"   Sch  80S","ANSI B16.5  ","1\"",25.0,"80S","SS",33.4,50.8,101.6,50.8,"-",4.55,4.55,0.38051502209568466,0.20424234157296062]
[null,"ANSI B16.5  Size  1¼\"   Sch  5S","ANSI B16.5  ","1¼\"",32.0,"5S","SS",42.2,63.5,101.6,50.8,"-",1.65,1.65,0.19596031049318205,0.10604552651408965]
[null,"ANSI B16.5  Size  1¼\"   Sch  10S","ANSI B16.5  ","1¼\"",32.0,"10S","SS",42.2,63.5,101.6,50.8,"-",2.77,2.77,0.32098156976347125,0.17416600044583574]
[null,"ANSI B16.5  Size  1¼\"   Sch  40S","ANSI B16.5  ","1¼\"",32.0,"40S","SS",42.2,63.5,101.6,50.8,"-",3.56,3.56,0.4052780939839664,0.22033694735922876]
[null,"ANSI B16.5  Size  1¼\"   Sch  80S","ANSI B16.5  ","1¼\"",32.0,"80S","SS",42.2,63.5,101.6,50.8,"-",4.85,4.85,0.5360128136488691,0.29238989900948736]
[null,"ANSI B16.5  Size  1½\"   Sch  5S","ANSI B16.5  ","1½\"",40.0,"5S","SS",48.3,73.15,101.6,50.8,"-",1.65,1.65,0.22991596732688327,0.1263237640867143]
[null,"ANSI B16.5  Size  1½\"   Sch  10S","ANSI B16.5  ","1½\"",40.0,"10S","SS",48.3,73.15,101.6,50.8,"-",2.77,2.77,0.3779859148721694,0.2082088598859388]
[null,"ANSI B16.5  Size  1½\"   Sch  40S","ANSI B16.5  ","1½\"",40.0,"40S","SS",48.3,73.15,101.6,50.8,"-",3.68,3.68,0.4935326484923352,0.272440935604268]
[null,"ANSI B16.5  Size  1½\"   Sch  80S","ANSI B16.5  ","1½\"",40.0,"80S","SS",48.3,73.15,101.6,50.8,"-",5.08,5.08,0.6629635246669923,0.36723375063979596]
[null,"ANSI B16.5  Size  2\"   Sch  5S","ANSI B16.5  ","2\"",50.0,"5S","SS",60.3,91.95,152.4,63.5,"-",1.65,1.65,0.4244558714998417,0.19928889887548945]
[null,"ANSI B16.5  Size  2\"   Sch  10S","ANSI B16.5  ","2\"",50.0,"10S","SS",60.3,91.95,152.4,63.5,"-",2.77,2.77,0.7005800358302922,0.3297363577270344]
[null,"ANSI B16.5  Size  2\"   Sch  40S","ANSI B16.5  ","2\"",50.0,"40S","SS",60.3,91.95,152.4,63.5,"-",3.91,3.91,0.9716767374862928,0.4585042776270582]
[null,"ANSI B16.5  Size  2\"   Sch  80S","ANSI B16.5  ","2\"",50.0,"80S","SS",60.3,91.95,152.4,63.5,"-",5.54,5.54,1.3418457830580033,0.6355941773692938]
[null,"ANSI B16.5  Size  2½\"   Sch  5S","ANSI B16.5  ","2½\"",65.0,"5S","SS",73.0,104.65,152.4,63.5,"-",2.11,2.11,0.6533678306771649,0.30542631054228525]
[null,"ANSI B16.5  Size  2½\"   Sch  10S","ANSI B16.5  ","2½\"",65.0,"10S","SS",73.0,104.65,152.4,63.5,"-",3.05,3.05,0.9333601781704101,0.43703186770777025]
[null,"ANSI B16.5  Size  2½\"   Sch  40S","ANSI B16.5  ","2½\"",65.0,"40S","SS",73.0,104.65,152.4,63.5,"-",5.16,5.16,1.5369792692182422,0.7224305052913871]
[null,"ANSI B16.5  Size  2½\"   Sch  80S","ANSI B16.5  ","2½\"",65.0,"80S","SS",73.0,104.65,152.4,63.5,"-",7.01,7.01,2.0379024434821154,0.9612620563003152]
[null,"ANSI B16.5  Size  3\"   Sch  5S","ANSI B16.5  ","3\"",80.0,"5S","SS",88.9,127.0,152.4,63.5,"-",2.11,2.11,0.8178672406234618,0.39127834833595687]
[null,"ANSI B16.5  Size  3\"   Sch  10S","ANSI B16.5  ","3\"",80.0,"10S","SS",88.9,127.0,152.4,63.5,"-",3.05,3.05,1.1711436854387531,0.5611307848976743]
[null,"ANSI B16.5  Size  3\"   Sch  40S","ANSI B16.5  ","3\"",80.0,"40S","SS",88.9,127.0,152.4,63.5,"-",5.49,5.49,2.056282220412499,0.9891914460777878]
[null,"ANSI B16.5  Size  3\"   Sch  80S","ANSI B16.5  ","3\"",80.0,"80S","SS",88.9,127.0,152.4,63.5,"-",7.62,7.62,2.791340575466913,1.3477207913118394]
[null,"ANSI B16.5  Size  3½\"   Sch  5S","ANSI B16.5  ","3½\"","-","5S","SS",101.6,139.7,152.4,76.2,"-",2.11,2.11,0.9343893910257729,0.5108140068735323]
[null,"ANSI B16.5  Size  3½\"   Sch  10S","ANSI B16.5  ","3½\"","-","10S","SS",101.6,139.7,152.4,76.2,"-",3.05,3.05,1.3395761777264537,0.7330270679694704]
[null,"ANSI B16.5  Size  3½\"   Sch  40S","ANSI B16.5  ","3½\"","-","40S","SS",101.6,139.7,152.4,76.2,"-",5.74,5.74,2.4613577382263756,1.3507016484739454]
[null,"ANSI B16.5  Size  3½\"   Sch  80S","ANSI B16.5  ","3½\"","-","80S","SS",101.6,139.7,152.4,76.2,"-",8.08,8.08,3.3916886412970504,1.8660318948216412]
[null,"ANSI B16.5  Size  4\"   Sch  5S","ANSI B16.5  ","4\"",100.0,"5S","SS",114.3,157.2,152.4,76.2,"-",2.11,2.11,1.070793056581357,0.5925686379407376]
[null,"ANSI B16.5  Size  4\"   Sch  10S","ANSI B16.5  ","4\"",100.0,"10S","SS",114.3,157.2,152.4,76.2,"-",3.05,3.05,1.5367473530556166,0.8512031934457629]
[null,"ANSI B16.5  Size  4\"   Sch  40S","ANSI B16.5  ","4\"",100.0,"40S","SS",114.3,157.2,152.4,76.2,"-",6.02,6.02,2.964079468622285,1.6466946683627446]
[null,"ANSI B16.5  Size  4\"   Sch  80S","ANSI B16.5  ","4\"",100.0,"80S","SS",114.3,157.2,152.4,76.2,"-",8.56,8.56,4.130666057807272,2.3008812480336207]
[null,"ANSI B16.5  Size  5\"   Sch  5S","ANSI B16.5  ","5\"",125.0,"5S","SS",141.3,185.7,203.2,76.2,"-",2.77,2.77,2.232568364938664,0.962885367434142]
[null,"ANSI B16.5  Size  5\"   Sch  10S","ANSI B16.5  ","5\"",125.0,"10S","SS",141.3,185.7,203.2,76.2,"-",3.4,3.4,2.72929766540264,1.177881334742825]
[null,"ANSI B16.5  Size  5\"   Sch  40S","ANSI B16.5  ","5\"",125.0,"40S","SS",141.3,185.7,203.2,76.2,"-",6.55,6.55,5.151580560360563,2.2306279802130664]
[null,"ANSI B16.5  Size  5\"   Sch  80S","ANSI B16.5  ","5\"",125.0,"80S","SS",141.3,185.7,203.2,76.2,"-",9.53,9.53,7.348994676497363,3.1924501620074013]
[null,"ANSI B16.5  Size  6\"   Sch  5S","ANSI B16.5  ","6\"",150.0,"5S","SS",168.3,215.9,203.2,88.9,"-",2.77,2.77,2.684202129463946,1.3091890603152119]
[null,"ANSI B16.5  Size  6\"   Sch  10S","ANSI B16.5  ","6\"",150.0,"10S","SS",168.3,215.9,203.2,88.9,"-",3.4,3.4,3.283649578538363,1.6022806357497652]
[null,"ANSI B16.5  Size  6\"   Sch  40S","ANSI B16.5  ","6\"",150.0,"40S","SS",168.3,215.9,203.2,88.9,"-",7.11,7.11,6.730749242103626,3.2931883727693685]
[null,"ANSI B16.5  Size  6\"   Sch  80S","ANSI B16.5  ","6\"",150.0,"80S","SS",168.3,215.9,203.2,88.9,"-",10.97,10.97,10.166631044738047,4.988807106371507]
[null,"ANSI B16.5  Size  8\"   Sch  5S","ANSI B16.5  ","8\"",200.0,"5S","SS",219.1,269.7,203.2,101.6,"-",2.77,2.77,3.52259386500972,1.911589548106807]
[null,"ANSI B16.5  Size  8\"   Sch  10S","ANSI B16.5  ","8\"",200.0,"10S","SS",219.1,269.7,203.2,101.6,"-",3.76,3.76,4.7623877913504735,2.585525562083253]
[null,"ANSI B16.5  Size  8\"   Sch  40S","ANSI B16.5  ","8\"",200.0,"40S","SS",219.1,269.7,203.2,101.6,"-",8.18,8.18,10.17439606577285,5.534878611186907]
[null,"ANSI B16.5  Size  8\"   Sch  80S","ANSI B16.5  ","8\"",200.0,"80S","SS",219.1,269.7,203.2,101.6,"-",12.7,12.7,15.500598219343818,8.450355362343046]
[null,"ANSI B16.5  Size  10\"   Sch  5S","ANSI B16.5  ","10\"",250.0,"5S","SS",273.0,323.9,254.0,127.0,"-",3.4,3.4,6.559937826765604,3.485463959669181]
[null,"ANSI B16.5  Size  10\"   Sch  10S","ANSI B16.5  ","10\"",250.0,"10S","SS",273.0,323.9,254.0,127.0,"-",4.19,4.19,8.062835117521624,4.285020526687177]
[null,"ANSI B16.5  Size  10\"   Sch  40S","ANSI B16.5  ","10\"",250.0,"40S","SS",273.0,323.9,254.0,127.0,"-",9.27,9.27,17.534938518050676,9.333672447137126]
[null,"ANSI B16.5  Size  10\"   Sch  80S","ANSI B16.5  ","10\"",250.0,"80S","SS",273.0,323.9,254.0,127.0,"-",12.7,12.7,23.7424363733997,12.651667420485776]
[null,"ANSI B16.5  Size  12\"   Sch  5S","ANSI B16.5  ","12\"",300.0,"5S","SS",323.8,381.0,254.0,152.4,"-",3.96,3.96,9.171416202116891,5.707965483293002]
[null,"ANSI B16.5  Size  12\"   Sch  10S","ANSI B16.5  ","12\"",300.0,"10S","SS",323.8,381.0,254.0,152.4,"-",4.57,4.57,10.566226586203566,6.576812199364878]
[null,"ANSI B16.5  Size  12\"   Sch  40S","ANSI B16.5  ","12\"",300.0,"40S","SS",323.8,381.0,254.0,152.4,"-",9.53,9.53,21.729662081334435,13.538359977621852]
[null,"ANSI B16.5  Size  12\"   Sch  80S","ANSI B16.5  ","12\"",300.0,"80S","SS",323.8,381.0,254.0,152.4,"-",12.7,12.7,28.6983347152765,17.891329751259235]
[null,"ANSI B16.5  Size  14\"   Sch  5S","ANSI B16.5  ","14\"",350.0,"5S","SS",355.6,412.8,304.8,152.4,"-",3.96,3.96,11.868063650106436,6.266494005706999]
[null,"ANSI B16.5  Size  14\"   Sch  10S","ANSI B16.5  ","14\"",350.0,"10S","SS",355.6,412.8,304.8,152.4,"-",4.87,4.87,14.561062059197416,7.689971600123838]
[null,"ANSI B16.5  Size  14\"   Sch  Std","ANSI B16.5  ","14\"",350.0,"Std","SS",355.6,412.8,304.8,152.4,"-",9.53,9.53,28.150930582981523,14.882495537875744]
[null,"ANSI B16.5  Size  14\"   Sch  XS","ANSI B16.5  ","14\"",350.0,"XS","SS",355.6,412.8,304.8,152.4,"-",12.7,12.7,37.2036646472435,19.682570214556655]
[null,"ANSI B16.5  Size  16\"   Sch  5S","ANSI B16.5  ","16\"",400.0,"5S","SS",406.4,469.9,304.8,152.4,"-",4.19,4.19,14.505977364566638,7.721877755106224]
[null,"ANSI B16.5  Size  16\"   Sch  10S","ANSI B16.5  ","16\"",400.0,"10S","SS",406.4,469.9,304.8,152.4,"-",4.78,4.78,16.526783991046823,8.798674640048391]
[null,"ANSI B16.5  Size  16\"   Sch  Std","ANSI B16.5  ","16\"",400.0,"Std","SS",406.4,469.9,304.8,152.4,"-",9.53,9.53,32.59990926986325,17.3730771700694]
[null,"ANSI B16.5  Size  16\"   Sch  XS","ANSI B16.5  ","16\"",400.0,"XS","SS",406.4,469.9,304.8,152.4,"-",12.7,12.7,43.132523967642044,23.001603449484207]
[null,"ANSI B16.5  Size  18\"   Sch  5S","ANSI B16.5  ","18\"",450.0,"5S","SS",457.2,533.4,304.8,152.4,"-",4.19,4.19,16.678449716367066,9.02599459436555]
[null,"ANSI B16.5  Size  18\"   Sch  10S","ANSI B16.5  ","18\"",450.0,"10S","SS",457.2,533.4,304.8,152.4,"-",4.78,4.78,19.005165337492187,10.286426070038747]
[null,"ANSI B16.5  Size  18\"   Sch  Std","ANSI B16.5  ","18\"",450.0,"Std","SS",457.2,533.4,304.8,152.4,"-",9.53,9.53,37.54111726811097,20.339242677979023]
[null,"ANSI B16.5  Size  18\"   Sch  XS","ANSI B16.5  ","18\"",450.0,"XS","SS",457.2,533.4,304.8,152.4,"-",12.7,12.7,49.717344699829546,26.954415826236847]
[null,"ANSI B16.5  Size  20\"   Sch  5S","ANSI B16.5  ","20\"",500.0,"5S","SS",508.0,584.2,304.8,152.4,"-",4.78,4.78,21.116922224404117,11.419950969078974]
[null,"ANSI B16.5  Size  20\"   Sch  10S","ANSI B16.5  ","20\"",500.0,"10S","SS",508.0,584.2,304.8,152.4,"-",5.54,5.54,24.44187658988192,13.219951761530595]
[null,"ANSI B16.5  Size  20\"   Sch  Std","ANSI B16.5  ","20\"",500.0,"Std","SS",508.0,584.2,304.8,152.4,"-",9.53,9.53,41.75137733762374,22.59917830305298]
[null,"ANSI B16.5  Size  20\"   Sch  XS","ANSI B16.5  ","20\"",500.0,"XS","SS",508.0,584.2,304.8,152.4,"-",12.7,12.7,55.32807952488837,29.96608239900059]
[null,"ANSI B16.5  Size  22\"   Sch  5S","ANSI B16.5  ","22\"",550.0,"5S","SS",559.0,641.4,304.8,"-","-",4.78,4.78,23.476875997999677,"-"]
[null,"ANSI B16.5  Size  22\"   Sch  10S","ANSI B16.5  ","22\"",550.0,"10S","SS",559.0,641.4,304.8,"-","-",5.54,5.54,27.177053139195525,"-"]
[null,"ANSI B16.5  Size  22\"   Sch  Std","ANSI B16.5  ","22\"",550.0,"Std","SS",559.0,641.4,304.8,"-","-",9.53,9.53,46.45647345945761,"-"]
[null,"ANSI B16.5  Size  22\"   Sch  XS","ANSI B16.5  ","22\"",550.0,"XS","SS",559.0,641.4,304.8,"-","-",12.7,12.7,61.598249592809616,"-"]
[null,"ANSI B16.5  Size  24\"   Sch  5S","ANSI B16.5  ","24\"",600.0,"5S","SS",609.6,692.2,304.8,152.4,"-",5.54,5.54,29.646698810980666,16.146764517393546]
[null,"ANSI B16.5  Size  24\"   Sch  10S","ANSI B16.5  ","24\"",600.0,"10S","SS",609.6,692.2,304.8,152.4,"-",6.35,6.35,33.94156333647569,18.488364780797323]
[null,"ANSI B16.5  Size  24\"   Sch  Std","ANSI B16.5  ","24\"",600.0,"Std","SS",609.6,692.2,304.8,152.4,"-",9.53,9.53,50.70479895622873,27.63393020979923]
[null,"ANSI B16.5  Size  24\"   Sch  XS","ANSI B16.5  ","24\"",600.0,"XS","SS",609.6,692.2,304.8,152.4,"-",12.7,12.7,67.25971169238926,36.67556290431826]

{"sheet":"Orifice fl.","index":12,"n_rows":101,"n_cols":73,"rows_kept":101,"cut":false,"hidden":true,"merged":[[0,0,0,8],[46,17,46,35],[46,37,46,55],[46,57,46,73],[46,75,46,91],[68,36,68,72],[76,75,76,91]]}
["WN & SO ORIFICE FLANGES"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Flange dimensions"]
["D","Flange diam.",{"$f":"INDEX('Data Orifice fl.'!H$3:H$89,'Data Orifice fl.'!$A$3)","v":647.7},"mm"]
["H","Flange length",{"$f":"INDEX('Data Orifice fl.'!I$3:I$89,'Data Orifice fl.'!$A$3)","v":146.05},"mm"]
["b","Flange thkn. incl. RF",{"$f":"INDEX('Data Orifice fl.'!J$3:J$89,'Data Orifice fl.'!$A$3)","v":57.15},"mm",null,"Include data of following flanges:"]
["d1","Diam. raced face",{"$f":"INDEX('Data Orifice fl.'!K$3:K$89,'Data Orifice fl.'!$A$3)","v":469.9},"mm"]
["k","Pitch circle",{"$f":"INDEX('Data Orifice fl.'!L$3:L$89,'Data Orifice fl.'!$A$3)","v":571.5},"mm",null,"Ansi B 16.36 WN Orifice fl.",null,"300-2500#"]
["n","Number of bolts",{"$f":"INDEX('Data Orifice fl.'!M$3:M$89,'Data Orifice fl.'!$A$3)","v":20},"pce",null,"Ansi B 16.36 SO Orifice fl.",null,"300#"]
["d2","Diam. boltholes",{"$f":"INDEX('Data Orifice fl.'!N$3:N$89,'Data Orifice fl.'!$A$3)","v":35.05},"mm"]
["d3","Diameter hub",{"$f":"INDEX('Data Orifice fl.'!O$3:O$89,'Data Orifice fl.'!$A$3)","v":482.6},"mm"]
["e","Centre of tapping hole",{"$f":"INDEX('Data Orifice fl.'!W$3:W$89,'Data Orifice fl.'!$A$3)","v":23.88},"mm"]
["f","Raced face height",{"$f":"INDEX('Data Orifice fl.'!P$3:P$89,'Data Orifice fl.'!$A$3)","v":1.6},"mm"]
["r","Round off",{"$f":"INDEX('Data Orifice fl.'!Q$3:Q$89,'Data Orifice fl.'!$A$3)","v":12.7},"mm"]
["g","Thickness of gasket",{"$f":"INDEX('Data Orifice fl.'!R$3:R$89,'Data Orifice fl.'!$A$3)","v":7},"mm"]
["L","Required stud length",{"$f":"INDEX('Data Orifice fl.'!S$3:S$89,'Data Orifice fl.'!$A$3)","v":183.3},"mm 1)"]
["bt","Bolt",{"$f":"INDEX('Data Orifice fl.'!T$3:T$89,'Data Orifice fl.'!$A$3)","v":"M33"}]
["m","Nut height",{"$f":"INDEX('Data Orifice fl.'!U$3:U$89,'Data Orifice fl.'!$A$3)","v":26},"mm"]
["W","Weight",{"$f":"INDEX('Data Orifice fl.'!V$3:V$89,'Data Orifice fl.'!$A$3)","v":254.4},"kg"]
[]
["1)","for flange / flange connection"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WALLTHICKNESS  OF  SEAMLESS  AND  WELDED  PIPE  acc.  DIN 2448  /   DIN 2458"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NPS","DN","OD",1.4,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,40.0,45.0,50.0,55.0,60.0,65.0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22.0,"1/8\"",6.0,10.2,1.4,1.6,1.8,2.0,2.3,2.6,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/4\"",10.0,13.5,1.4,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3/8\"",12.0,17.2,1.4,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/2\"",15.0,21.3,1.4,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3/4\"",20.0,26.9,1.4,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1\"",25.0,33.7,1.4,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1¼\"",32.0,42.4,1.4,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1½\"",40.0,48.3,1.4,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2\"",50.0,60.3,1.4,1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,"-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2½\"",65.0,73.0,"-",1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,"-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3\"",80.0,88.9,"-",1.6,1.8,2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,"-","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3½\"",90.0,101.6,"-","-","-",2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,"-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4\"",100.0,114.3,"-","-","-",2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,"-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5\"",125.0,139.7,"-","-","-",2.0,2.3,2.6,2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,"-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6\"",150.0,168.3,"-","-","-","-","-","-",2.9,3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,40.0,45.0,50.0,"-","-","-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8\"",200.0,219.1,"-","-","-","-","-","-","-",3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,40.0,45.0,50.0,55.0,60.0,"-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10\"",250.0,273.0,"-","-","-","-","-","-","-",3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,40.0,45.0,50.0,55.0,60.0,65.0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12\"",300.0,323.9,"-","-","-","-","-","-","-",3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,40.0,45.0,50.0,55.0,60.0,65.0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14\"",350.0,355.6,"-","-","-","-","-","-","-",3.2,3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,40.0,45.0,50.0,55.0,60.0,65.0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16\"",400.0,406.4,"-","-","-","-","-","-","-","-",3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,40.0,45.0,50.0,55.0,60.0,65.0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18\"",450.0,457.0,"-","-","-","-","-","-","-","-",3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,40.0,45.0,50.0,55.0,60.0,65.0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20\"",500.0,508.0,"-","-","-","-","-","-","-","-",3.6,4.0,4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,40.0,45.0,50.0,55.0,60.0,65.0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"22\"",550.0,559.0,"-","-","-","-","-","-","-","-","-","-",4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,40.0,45.0,50.0,55.0,60.0,65.0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24\"",600.0,610.0,"-","-","-","-","-","-","-","-","-","-",4.5,5.0,5.6,6.3,7.1,8.0,8.8,10.0,11.0,12.5,14.2,16.0,17.5,20.0,22.2,25.0,28.0,30.0,32.0,36.0,40.0,45.0,50.0,55.0,60.0,65.0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"28\"",700.0,711.0,"-","-","-","-","-","-","-","-","-","-","-",5.0,"-","-",7.1,"-","-","-","-",12.5,"-","-","-",20.0,"-","-","-","-",32.0,"-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"32\"",800.0,813.0,"-","-","-","-","-","-","-","-","-","-","-","-",5.6,"-","-",8.0,"-","-","-",12.5,"-","-","-","-",22.2,"-","-","-","-",36.0,"-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36\"",900.0,914.0,"-","-","-","-","-","-","-","-","-","-","-","-","-",6.3,"-","-","-",10.0,"-",12.5,"-","-","-","-","-",25.0,"-","-","-","-",40.0,"-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"40\"",1000.0,1016.0,"-","-","-","-","-","-","-","-","-","-","-","-","-",6.3,"-","-","-",10.0,"-",12.5,"-","-","-","-","-","-",28.0,"-","-","-","-",45.0,"-","-","-","-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48\"",1200.0,1220.0,"-","-","-","-","-","-","-","-","-","-","-","-","-",6.3,"-","-","-",10.0,"-",12.5,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"56\"",1400.0,1420.0,"-","-","-","-","-","-","-","-","-","-","-","-","-",6.3,"-","-","-",10.0,"-",12.5,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"64\"",1600.0,1620.0,"-","-","-","-","-","-","-","-","-","-","-","-","-",6.3,"-","-","-",10.0,"-",12.5,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]

{"sheet":"Data Orifice fl.","index":13,"n_rows":89,"n_cols":23,"rows_kept":89,"cut":false,"hidden":true,"merged":[]}
["Data WN & SO Orifice flanges",null,null,null,null,null,null,"Fl. diam.","Fl. height","Fl. thickn.","Diam. RF","Pitch circle","No. of bolts","Bolt hole","Diam. Hub","RF height","Round of","Gasket th.","Stud length","Bolt","Nut height","Weight","e"]
[null,"Type / Size / Rating","Type","Rating","Norm","NPS","DN","D","H","b","d1","k","n","d2","d3","f","r","g","L","bt","m","W","Centre to face"]
[14.0,"WNRF 300# Ansi B16.36   Size 1\"","WNRF","300#","ANSI B16.36","1\"",25.0,123.95,82.55,38.1,50.8,88.9,4.0,17.5,53.85,1.6,3.0,3.0,{"$f":"(J3+U3+5)*2+R3","v":115.2},"M16",13.0,8.2,23.88]
[null,"WNRF 300# Ansi B16.36   Size 1¼\"","WNRF","300#","ANSI B16.36","1¼\"",32.0,133.35,84.1,38.1,63.5,98.4,4.0,17.5,63.5,1.6,3.0,3.0,115.2,"M16",13.0,9.5,23.88]
[null,"WNRF 300# Ansi B16.36   Size 1½\"","WNRF","300#","ANSI B16.36","1½\"",40.0,155.45,85.85,38.1,73.15,114.3,4.0,20.57,69.85,1.6,6.4,3.0,121.2,"M20",16.0,13.0,23.88]
[null,"WNRF 300# Ansi B16.36   Size 2\"","WNRF","300#","ANSI B16.36","2\"",50.0,165.1,85.85,38.1,91.95,127.0,8.0,17.5,84.07,1.6,7.9,4.0,116.2,"M16",13.0,15.0,23.88]
[null,"WNRF 300# Ansi B16.36   Size 2½\"","WNRF","300#","ANSI B16.36","2½\"",65.0,190.5,88.9,38.1,104.65,149.35,8.0,20.6,86.36,1.6,7.9,4.0,122.2,"M20",16.0,19.5,23.88]
[null,"WNRF 300# Ansi B16.36   Size 3\"","WNRF","300#","ANSI B16.36","3\"",80.0,209.55,88.9,38.1,127.0,168.15,8.0,20.6,117.35,1.6,9.7,4.0,122.2,"M20",16.0,22.0,23.88]
[null,"WNRF 300# Ansi B16.36   Size 4\"","WNRF","300#","ANSI B16.36","4\"",100.0,254.0,91.95,38.1,157.23,200.152,8.0,20.6,146.05,1.6,11.2,5.0,123.2,"M20",16.0,31.0,23.88]
[null,"WNRF 300# Ansi B16.36   Size 5\"","WNRF","300#","ANSI B16.36","5\"",125.0,279.4,101.6,38.1,185.7,234.9,8.0,22.3,177.8,1.6,11.2,2.0,120.2,"M20",16.0,35.0,23.88]
[null,"WNRF 300# Ansi B16.36   Size 6\"","WNRF","300#","ANSI B16.36","6\"",150.0,317.5,100.76,38.1,215.9,269.748,12.0,22.3,206.248,1.6,12.7,6.0,124.2,"M20",16.0,45.0,23.88]
[null,"WNRF 300# Ansi B16.36   Size 8\"","WNRF","300#","ANSI B16.36","8\"",200.0,381.0,111.25,41.15,269.75,330.2,12.0,25.4,260.35,1.6,12.7,6.0,136.3,"M24",19.0,70.0,23.88]
[null,"WNRF 300# Ansi B16.36   Size 10\"","WNRF","300#","ANSI B16.36","10\"",250.0,444.5,117.348,47.75,323.85,387.35,16.0,28.45,320.55,1.6,12.7,6.0,155.5,"M27",22.0,100.0,23.88]
[null,"WNRF 300# Ansi B16.36   Size 12\"","WNRF","300#","ANSI B16.36","12\"",300.0,520.7,130.048,50.8,381.0,438.15,16.0,31.75,374.65,1.6,12.7,6.0,165.6,"M30",24.0,150.0,23.88]
[null,"WNRF 300# Ansi B16.36   Size 14\"","WNRF","300#","ANSI B16.36","14\"",350.0,584.2,142.748,53.848,412.75,527.05,20.0,31.75,425.45,1.6,12.7,7.0,172.696,"M30",24.0,206.0,23.88]
[null,"WNRF 300# Ansi B16.36   Size 16\"","WNRF","300#","ANSI B16.36","16\"",400.0,647.7,146.05,57.15,469.9,571.5,20.0,35.05,482.6,1.6,12.7,7.0,183.3,"M33",26.0,254.4,23.88]
[null,"WNRF 300# Ansi B16.36   Size 18\"","WNRF","300#","ANSI B16.36","18\"",450.0,711.2,158.75,60.45,533.4,628.65,24.0,35.05,533.4,1.6,12.7,7.0,189.9,"M33",26.0,314.4,23.88]
[null,"WNRF 300# Ansi B16.36   Size 20\"","WNRF","300#","ANSI B16.36","20\"",500.0,774.7,162.052,63.5,584.2,685.8,24.0,35.05,587.25,1.6,12.7,7.0,196,"M33",26.0,379.2,23.88]
[null,"WNRF 300# Ansi B16.36   Size 24\"","WNRF","300#","ANSI B16.36","24\"",600.0,914.4,168.148,69.85,692.15,812.8,24.0,41.15,701.55,1.6,12.7,7.0,218.7,"M39",31.0,552.0,23.88]
[null,"WNRF 400# Ansi B16.36   Size 1\"","WNRF","400#","ANSI B16.36","1\"",25.0,123.95,82.55,38.1,50.8,88.9,4.0,17.5,53.85,6.4,3.0,3.0,115.2,"M16",13.0,8.2,23.88]
[null,"WNRF 400# Ansi B16.36   Size 1½\"","WNRF","400#","ANSI B16.36","1½\"",40.0,155.45,85.85,38.1,73.15,114.3,4.0,20.57,69.85,6.4,6.4,3.0,121.2,"M20",16.0,13.0,23.88]
[null,"WNRF 400# Ansi B16.36   Size 2\"","WNRF","400#","ANSI B16.36","2\"",50.0,165.1,85.85,38.1,91.95,127.0,8.0,17.5,84.07,6.4,7.9,4.0,116.2,"M16",13.0,15.0,23.88]
[null,"WNRF 400# Ansi B16.36   Size 2½\"","WNRF","400#","ANSI B16.36","2½\"",65.0,190.5,88.9,38.1,104.65,149.35,8.0,20.6,86.36,6.4,7.9,4.0,122.2,"M20",16.0,19.5,23.88]
[null,"WNRF 400# Ansi B16.36   Size 3\"","WNRF","400#","ANSI B16.36","3\"",80.0,209.55,88.9,38.1,127.0,168.15,8.0,20.6,117.35,6.4,9.7,4.0,122.2,"M20",16.0,22.0,23.88]
[null,"WNRF 400# Ansi B16.36   Size 4\"","WNRF","400#","ANSI B16.36","4\"",100.0,254.0,88.9,38.1,157.2,200.15,8.0,25.4,146.1,6.4,11.2,5.0,129.2,"M24",19.0,"-",23.88]
[null,"WNRF 400# Ansi B16.36   Size 6\"","WNRF","400#","ANSI B16.36","6\"",150.0,317.5,103.12,41.15,215.9,269.7,12.0,25.4,206.2,6.4,12.7,6.0,136.3,"M24",19.0,"-",23.88]
[null,"WNRF 400# Ansi B16.36   Size 8\"","WNRF","400#","ANSI B16.36","8\"",200.0,381.0,117.35,47.75,269.75,330.2,12.0,28.4,260.4,6.4,12.7,6.0,155.5,"M27",22.0,"-",23.88]
[null,"WNRF 400# Ansi B16.36   Size 10\"","WNRF","400#","ANSI B16.36","10\"",250.0,444.5,123.95,53.85,323.85,387.4,16.0,31.7,320.5,6.4,12.7,6.0,171.7,"M30",24.0,"-",23.88]
[null,"WNRF 400# Ansi B16.36   Size 12\"","WNRF","400#","ANSI B16.36","12\"",300.0,520.7,136.65,57.15,381.0,450.9,16.0,35.0,374.7,6.4,12.7,6.0,182.3,"M33",26.0,"-",23.88]
[null,"WNRF 400# Ansi B16.36   Size 14\"","WNRF","400#","ANSI B16.36","14\"",350.0,284.2,149.35,60.71,412.75,514.4,20.0,35.0,425.5,6.4,12.7,7.0,190.42,"M33",26.0,"-",23.88]
[null,"WNRF 400# Ansi B16.36   Size 16\"","WNRF","400#","ANSI B16.36","16\"",400.0,647.7,152.4,63.5,469.9,571.5,20.0,38.1,482.6,6.4,12.7,7.0,202,"M36",29.0,"-",23.88]
[null,"WNRF 400# Ansi B16.36   Size 18\"","WNRF","400#","ANSI B16.36","18\"",450.0,711.2,165.1,66.55,508.0,628.7,24.0,38.1,533.4,6.4,12.7,7.0,208.1,"M36",29.0,"-",23.88]
[null,"WNRF 400# Ansi B16.36   Size 20\"","WNRF","400#","ANSI B16.36","20\"",500.0,774.7,168.15,69.85,584.2,685.8,24.0,41.1,587.2,6.4,12.7,7.0,218.7,"M39",31.0,"-",23.88]
[null,"WNRF 400# Ansi B16.36   Size 24\"","WNRF","400#","ANSI B16.36","24\"",600.0,914.4,174.75,76.2,692.15,812.8,24.0,48.0,701.5,6.4,12.7,7.0,241.4,"M45",36.0,"-",23.88]
[null,"WNRF 600# Ansi B16.36   Size 1\"","WNRF","600#","ANSI B16.36","1\"",25.0,123.9,82.55,38.1,50.8,88.9,4.0,17.5,53.8,6.4,3.0,3.0,115.2,"M16",13.0,"-",23.88]
[null,"WNRF 600# Ansi B16.36   Size 1½\"","WNRF","600#","ANSI B16.36","1½\"",40.0,155.4,85.85,38.1,73.2,114.3,4.0,20.6,69.9,6.4,6.35,3.0,121.2,"M20",16.0,"-",23.88]
[null,"WNRF 600# Ansi B16.36   Size 2\"","WNRF","600#","ANSI B16.36","2\"",50.0,165.1,85.85,38.1,91.9,127.0,8.0,17.5,84.1,6.4,7.87,4.0,116.2,"M16",13.0,"-",23.88]
[null,"WNRF 600# Ansi B16.36   Size 2½\"","WNRF","600#","ANSI B16.36","2½\"",65.0,190.5,88.9,38.1,104.6,149.4,8.0,20.6,100.1,6.4,7.87,4.0,122.2,"M20",16.0,"-",23.88]
[null,"WNRF 600# Ansi B16.36   Size 3\"","WNRF","600#","ANSI B16.36","3\"",80.0,209.6,88.9,38.1,127.0,168.1,8.0,20.6,117.3,6.4,9.65,4.0,122.2,"M20",16.0,"-",23.88]
[null,"WNRF 600# Ansi B16.36   Size 4\"","WNRF","600#","ANSI B16.36","4\"",100.0,273.1,101.6,38.1,157.23,215.9,8.0,25.4,152.4,6.4,11.2,5.0,129.2,"M24",19.0,"-",23.88]
[null,"WNRF 600# Ansi B16.36   Size 6\"","WNRF","600#","ANSI B16.36","6\"",150.0,355.6,117.35,47.75,215.9,292.1,12.0,28.4,222.3,6.4,12.7,6.0,155.5,"M27",22.0,"-",23.88]
[null,"WNRF 600# Ansi B16.36   Size 8\"","WNRF","600#","ANSI B16.36","8\"",200.0,419.1,133.35,55.63,269.7,349.3,12.0,31.7,273.1,6.4,12.7,6.0,175.26,"M30",24.0,"-",23.88]
[null,"WNRF 600# Ansi B16.36   Size 10\"","WNRF","600#","ANSI B16.36","10\"",250.0,508.0,152.4,63.5,323.9,431.8,16.0,35.0,342.9,6.4,12.7,6.0,195,"M33",26.0,"-",23.88]
[null,"WNRF 600# Ansi B16.36   Size 12\"","WNRF","600#","ANSI B16.36","12\"",300.0,558.8,155.45,66.55,381.0,489.0,20.0,35.0,400.1,6.4,12.7,6.0,201.1,"M33",26.0,"-",23.88]
[null,"WNRF 600# Ansi B16.36   Size 14\"","WNRF","600#","ANSI B16.36","14\"",350.0,603.3,165.1,69.85,412.8,527.1,20.0,38.1,431.8,6.4,12.7,7.0,208.7,"M36",26.0,"-",23.88]
[null,"WNRF 600# Ansi B16.36   Size 16\"","WNRF","600#","ANSI B16.36","16\"",400.0,685.8,177.8,76.2,469.9,603.3,20.0,41.1,495.3,6.4,12.7,7.0,227.4,"M39",29.0,"-",23.88]
[null,"WNRF 600# Ansi B16.36   Size 18\"","WNRF","600#","ANSI B16.36","18\"",450.0,743.0,184.15,82.55,533.4,654.1,20.0,44.4,546.1,6.4,12.7,7.0,250.1,"M42",34.0,"-",23.88]
[null,"WNRF 600# Ansi B16.36   Size 20\"","WNRF","600#","ANSI B16.36","20\"",500.0,812.8,190.5,88.9,584.2,723.9,24.0,44.4,609.6,6.4,12.7,7.0,262.8,"M42",34.0,"-",23.88]
[null,"WNRF 600# Ansi B16.36   Size 24\"","WNRF","600#","ANSI B16.36","24\"",600.0,939.8,203.2,101.6,692.2,838.2,24.0,50.8,717.6,6.4,12.7,7.0,296.2,"M48",38.0,"-",23.88]
[null,"WNRF 900# Ansi B16.36   Size 1\"","WNRF","900#","ANSI B16.36","1\"",25.0,149.3,82.55,38.1,50.8,101.6,4.0,25.4,52.3,6.4,3.0,3.0,127.2,"M24",19.0,"-",23.88]
[null,"WNRF 900# Ansi B16.36   Size 1½\"","WNRF","900#","ANSI B16.36","1½\"",40.0,177.8,88.9,38.1,73.1,123.9,4.0,28.4,69.8,6.4,6.35,3.0,133.2,"M27",22.0,"-",23.88]
[null,"WNRF 900# Ansi B16.36   Size 2\"","WNRF","900#","ANSI B16.36","2\"",50.0,215.9,101.6,38.1,91.9,165.1,8.0,25.4,104.6,6.4,7.87,4.0,128.2,"M24",19.0,"-",23.88]
[null,"WNRF 900# Ansi B16.36   Size 2½\"","WNRF","900#","ANSI B16.36","2½\"",65.0,244.3,104.6,41.15,104.6,190.5,8.0,28.4,123.9,6.4,7.87,4.0,140.3,"M27",22.0,"-",23.88]
[null,"WNRF 900# Ansi B16.36   Size 3\"","WNRF","900#","ANSI B16.36","3\"",80.0,241.3,101.6,38.1,127.0,190.5,8.0,25.4,127.0,6.4,9.65,4.0,122.2,"M20",16.0,"-",23.88]
[null,"WNRF 900# Ansi B16.36   Size 4\"","WNRF","900#","ANSI B16.36","4\"",100.0,292.1,114.3,44.45,157.2,234.9,8.0,31.7,158.7,6.4,11.18,5.0,147.9,"M27",22.0,"-",23.88]
[null,"WNRF 900# Ansi B16.36   Size 6\"","WNRF","900#","ANSI B16.36","6\"",150.0,381.0,139.7,55.63,215.9,317.5,12.0,31.7,234.9,6.4,12.7,6.0,171.26,"M27",22.0,"-",23.88]
[null,"WNRF 900# Ansi B16.36   Size 8\"","WNRF","900#","ANSI B16.36","8\"",200.0,469.9,162.05,63.5,269.7,393.7,12.0,38.1,298.4,6.4,12.7,6.0,201,"M36",29.0,"-",23.88]
[null,"WNRF 900# Ansi B16.36   Size 10\"","WNRF","900#","ANSI B16.36","10\"",250.0,546.1,184.15,69.85,323.8,169.9,16.0,38.1,368.3,6.4,12.7,6.0,213.7,"M36",29.0,"-",23.88]
[null,"WNRF 900# Ansi B16.36   Size 12\"","WNRF","900#","ANSI B16.36","12\"",300.0,609.6,200.15,79.25,381.0,533.4,20.0,38.1,419.1,6.4,12.7,6.0,232.5,"M36",29.0,"-",23.88]
[null,"WNRF 900# Ansi B16.36   Size 14\"","WNRF","900#","ANSI B16.36","14\"",350.0,641.3,212.85,85.85,412.7,558.8,20.0,41.1,450.8,6.4,12.7,7.0,246.7,"M39",29.0,"-",23.88]
[null,"WNRF 900# Ansi B16.36   Size 16\"","WNRF","900#","ANSI B16.36","16\"",400.0,704.8,215.9,88.9,469.9,615.9,20.0,44.4,508.0,6.4,12.7,7.0,262.8,"M42",34.0,"-",23.88]
[null,"WNRF 900# Ansi B16.36   Size 18\"","WNRF","900#","ANSI B16.36","18\"",450.0,787.4,228.6,101.6,533.4,685.8,20.0,50.8,565.1,6.4,12.7,7.0,296.2,"M48",38.0,"-",23.88]
[null,"WNRF 900# Ansi B16.36   Size 20\"","WNRF","900#","ANSI B16.36","20\"",500.0,857.2,247.65,107.95,584.2,749.3,20.0,53.8,622.3,6.4,12.7,7.0,316.9,"M52",42.0,"-",23.88]
[null,"WNRF 900# Ansi B16.36   Size 24\"","WNRF","900#","ANSI B16.36","24\"",600.0,1041.4,292.1,139.7,692.1,901.7,20.0,66.5,749.3,6.4,12.7,7.0,398.4,"M64",51.0,"-",23.88]
[null,"WNRF 1500# Ansi B16.36   Size 1\"","WNRF","1500#","ANSI B16.36","1\"",25.0,149.3,82.55,38.1,50.8,101.6,4.0,25.4,52.3,6.4,3.0,3.0,127.2,"M24",19.0,"-",23.88]
[null,"WNRF 1500# Ansi B16.36   Size 1½\"","WNRF","1500#","ANSI B16.36","1½\"",40.0,177.8,88.9,38.1,73.1,123.9,4.0,28.4,69.8,6.4,6.35,3.0,133.2,"M27",22.0,"-",23.88]
[null,"WNRF 1500# Ansi B16.36   Size 2\"","WNRF","1500#","ANSI B16.36","2\"",50.0,215.9,101.6,38.1,91.9,165.1,8.0,25.4,104.6,6.4,7.87,4.0,128.2,"M24",19.0,"-",23.88]
[null,"WNRF 1500# Ansi B16.36   Size 2½\"","WNRF","1500#","ANSI B16.36","2½\"",65.0,244.3,104.6,41.15,104.6,190.5,8.0,28.4,123.9,6.4,7.87,4.0,140.3,"M27",22.0,"-",23.88]
[null,"WNRF 1500# Ansi B16.36   Size 3\"","WNRF","1500#","ANSI B16.36","3\"",80.0,266.7,117.35,47.75,127.0,203.2,8.0,31.7,133.3,6.4,9.65,4.0,157.5,"M30",24.0,"-",23.88]
[null,"WNRF 1500# Ansi B16.36   Size 4\"","WNRF","1500#","ANSI B16.36","4\"",100.0,311.1,123.95,53.85,157.2,241.3,8.0,35.0,162.0,6.4,11.18,5.0,174.7,"M33",26.0,"-",23.88]
[null,"WNRF 1500# Ansi B16.36   Size 6\"","WNRF","1500#","ANSI B16.36","6\"",150.0,393.7,171.45,82.55,215.9,317.5,12.0,38.1,228.6,6.4,12.7,6.0,239.1,"M36",29.0,"-",23.88]
[null,"WNRF 1500# Ansi B16.36   Size 8\"","WNRF","1500#","ANSI B16.36","8\"",200.0,482.6,212.85,91.95,269.7,393.7,12.0,44.4,292.1,6.4,12.7,6.0,267.9,"M42",34.0,"-",23.88]
[null,"WNRF 1500# Ansi B16.36   Size 10\"","WNRF","1500#","ANSI B16.36","10\"",250.0,584.2,254.0,107.95,323.8,485.6,12.0,50.8,368.3,6.4,12.7,6.0,307.9,"M48",38.0,"-",23.88]
[null,"WNRF 1500# Ansi B16.36   Size 12\"","WNRF","1500#","ANSI B16.36","12\"",300.0,673.1,282.45,123.95,381.0,571.5,16.0,53.8,450.8,6.4,12.7,6.0,347.9,"M52",42.0,"-",23.88]
[null,"WNRF 1500# Ansi B16.36   Size 14\"","WNRF","1500#","ANSI B16.36","14\"",350.0,749.3,298.45,133.35,412.7,635.0,16.0,60.4,495.3,6.4,12.7,7.0,373.7,"M56",45.0,"-",23.88]
[null,"WNRF 1500# Ansi B16.36   Size 16\"","WNRF","1500#","ANSI B16.36","16\"",400.0,825.5,311.15,146.05,469.9,704.8,16.0,66.5,552.4,6.4,12.7,7.0,405.1,"M60",48.0,"-",23.88]
[null,"WNRF 1500# Ansi B16.36   Size 18\"","WNRF","1500#","ANSI B16.36","18\"",450.0,914.4,327.15,162.05,533.4,774.7,16.0,73.1,596.9,6.4,12.7,7.0,449.1,"M68",54.0,"-",23.88]
[null,"WNRF 1500# Ansi B16.36   Size 20\"","WNRF","1500#","ANSI B16.36","20\"",500.0,984.2,355.6,177.8,584.2,831.8,16.0,79.2,641.3,6.4,12.7,7.0,494.6,"M76",61.0,"-",23.88]
[null,"WNRF 1500# Ansi B16.36   Size 24\"","WNRF","1500#","ANSI B16.36","24\"",600.0,1168.4,406.4,203.2,692.1,990.6,16.0,91.9,762.0,6.4,12.7,7.0,551.4,"M80",64.0,"-",23.88]
[null,"WNRF 2500# Ansi B16.36   Size 1\"","WNRF","2500#","ANSI B16.36","1\"",25.0,158.8,91.95,38.1,50.8,108.0,4.0,25.4,57.2,6.4,3.0,3.0,127.2,"M24",19.0,"-",23.88]
[null,"WNRF 2500# Ansi B16.36   Size 1½\"","WNRF","2500#","ANSI B16.36","1½\"",40.0,203.2,111.25,44.45,73.1,146.1,4.0,31.8,79.2,6.4,6.35,3.0,149.9,"M30",24.0,"-",23.88]
[null,"WNRF 2500# Ansi B16.36   Size 2\"","WNRF","2500#","ANSI B16.36","2\"",50.0,235.0,127.0,50.8,91.9,171.5,8.0,28.4,95.3,6.4,7.87,4.0,159.6,"M27",22.0,"-",23.88]
[null,"WNRF 2500# Ansi B16.36   Size 2½\"","WNRF","2500#","ANSI B16.36","2½\"",65.0,266.7,142.75,57.15,104.6,196.9,8.0,31.8,114.3,6.4,7.87,4.0,176.3,"M30",24.0,"-",23.88]
[null,"WNRF 2500# Ansi B16.36   Size 3\"","WNRF","2500#","ANSI B16.36","3\"",80.0,304.8,168.15,66.55,127.0,228.6,8.0,35.1,133.4,6.4,9.7,4.0,199.1,"M33",26.0,"-",23.88]
[null,"WNRF 2500# Ansi B16.36   Size 4\"","WNRF","2500#","ANSI B16.36","4\"",100.0,355.6,190.5,76.2,157.2,273.1,8.0,41.1,165.1,6.4,11.18,5.0,229.4,"M39",31.0,"-",23.88]
[null,"WNRF 2500# Ansi B16.36   Size 6\"","WNRF","2500#","ANSI B16.36","6\"",150.0,482.6,273.1,107.95,215.9,368.3,8.0,53.8,235.0,6.4,12.7,6.0,307.9,"M48",38.0,"-",23.88]
[null,"WNRF 2500# Ansi B16.36   Size 8\"","WNRF","2500#","ANSI B16.36","8\"",200.0,552.5,317.5,127.0,269.7,438.2,12.0,53.8,304.8,6.4,12.7,6.0,346,"M48",38.0,"-",23.88]
[null,"WNRF 2500# Ansi B16.36   Size 10\"","WNRF","2500#","ANSI B16.36","10\"",250.0,673.1,419.1,165.1,323.8,539.8,12.0,66.5,374.7,6.4,12.7,6.0,442.2,"M60",48.0,"-",23.88]
[null,"WNRF 2500# Ansi B16.36   Size 12\"","WNRF","2500#","ANSI B16.36","12\"",300.0,762.0,463.55,184.15,381.0,619.3,12.0,73.2,441.5,6.4,12.7,6.0,486.3,"M64",51.0,"-",23.88]

{"sheet":"Fittings","index":14,"n_rows":53,"n_cols":5,"rows_kept":53,"cut":false,"hidden":true,"merged":[[0,0,0,9],[62,23,62,24]]}
["DIMENSIONS of ELBOWS, TEES & CAPS"]
["Elbow 90º- LR (R=1,5D) acc. ANSI B 16.9"]
["Diam. outside","Do",{"$f":"INDEX('Data fittings'!$H$3:$H$38,'Data fittings'!$E$3)","v":33.4},"mm","Size"]
["Diam. Inside std.","Di",{"$f":"INDEX('Data fittings'!$I$3:$I$38,'Data fittings'!$E$3)","v":26.64},"mm"]
["Diam. Inside XS","Di",{"$f":"INDEX('Data fittings'!$J$3:$J$38,'Data fittings'!$E$3)","v":24.3},"mm"]
["Wallth. Std.","s",{"$f":"INDEX('Data fittings'!$Q$3:$Q$38,'Data fittings'!$E$3)","v":3.38},"mm"]
["Wallth. XS","s",{"$f":"INDEX('Data fittings'!$R$3:$R$38,'Data fittings'!$E$3)","v":4.55},"mm"]
["Center to end","R",{"$f":"INDEX('Data fittings'!$K$3:$K$38,'Data fittings'!$E$3)","v":38.1},"mm"]
["Weight Std.","W",{"$f":"INDEX('Data fittings'!$V$3:$V$38,'Data fittings'!$E$3)","v":0.15},"kg"]
["Weight XS","W",{"$f":"INDEX('Data fittings'!$W$3:$W$38,'Data fittings'!$E$3)","v":0.19},"kg"]
[]
["Elbow 90º- SR (R=D) acc. ANSI B 16.9"]
["Diam. outside","Do",{"$f":"INDEX('Data fittings'!$H$3:$H$38,'Data fittings'!$D$3)","v":33.4},"mm","Size"]
["Diam. Inside std.","Di",{"$f":"INDEX('Data fittings'!$I$3:$I$38,'Data fittings'!$D$3)","v":26.64},"mm"]
["Diam. Inside XS","Di",{"$f":"INDEX('Data fittings'!$J$3:$J$38,'Data fittings'!$D$3)","v":24.3},"mm"]
["Wallth. Std.","s",{"$f":"INDEX('Data fittings'!$Q$3:$Q$38,'Data fittings'!$D$3)","v":3.38},"mm"]
["Wallth. XS","s",{"$f":"INDEX('Data fittings'!$R$3:$R$38,'Data fittings'!$D$3)","v":4.55},"mm"]
["Center to end","R",{"$f":"INDEX('Data fittings'!$L$3:$L$38,'Data fittings'!$D$3)","v":25.4},"mm"]
["Weight Std.","W",{"$f":"INDEX('Data fittings'!$Z$3:$Z$38,'Data fittings'!$D$3)","v":0.1},"kg"]
["Weight XS","W",{"$f":"INDEX('Data fittings'!$AA$3:$AA$38,'Data fittings'!$D$3)","v":0.132},"kg"]
[]
["Elbow 45º- LR (R=1,5D) acc. ANSI B 16.9"]
["Diam. outside","Do",{"$f":"INDEX('Data fittings'!$H$3:$H$38,'Data fittings'!$C$3)","v":114.3},"mm","Size"]
["Diam. Inside std.","Di",{"$f":"INDEX('Data fittings'!$I$3:$I$38,'Data fittings'!$C$3)","v":102.26},"mm"]
["Diam. Inside XS","Di",{"$f":"INDEX('Data fittings'!$J$3:$J$38,'Data fittings'!$C$3)","v":97.18},"mm"]
["Wallth. Std.","s",{"$f":"INDEX('Data fittings'!$Q$3:$Q$38,'Data fittings'!$C$3)","v":6.02},"mm"]
["Wallth. XS","s",{"$f":"INDEX('Data fittings'!$R$3:$R$38,'Data fittings'!$C$3)","v":8.56},"mm"]
["Center to end","B",{"$f":"INDEX('Data fittings'!$M$3:$M$38,'Data fittings'!$C$3)","v":63.5},"mm"]
["Weight Std.","W",{"$f":"INDEX('Data fittings'!$X$3:$X$38,'Data fittings'!$C$3)","v":1.95},"kg"]
["Weight XS","W",{"$f":"INDEX('Data fittings'!$Y$3:$Y$38,'Data fittings'!$C$3)","v":2.66},"kg"]
[]
["Straight Tee acc. ANSI B 16.9"]
["Diam. outside","Do",{"$f":"INDEX('Data fittings'!$H$3:$H$38,'Data fittings'!$B$3)","v":33.4},"mm","Size"]
["Diam. Inside std.","Di",{"$f":"INDEX('Data fittings'!$I$3:$I$38,'Data fittings'!$B$3)","v":26.64},"mm"]
["Diam. Inside XS","Di",{"$f":"INDEX('Data fittings'!$J$3:$J$38,'Data fittings'!$B$3)","v":24.3},"mm"]
["Wallth. Std.","s",{"$f":"INDEX('Data fittings'!$Q$3:$Q$38,'Data fittings'!$B$3)","v":3.38},"mm"]
["Wallth. XS","s",{"$f":"INDEX('Data fittings'!$R$3:$R$38,'Data fittings'!$B$3)","v":4.55},"mm"]
["Center to end (run)","E",{"$f":"INDEX('Data fittings'!$O$3:$O$38,'Data fittings'!$B$3)","v":38.1},"mm"]
["Center to end (branch)","C",{"$f":"INDEX('Data fittings'!$N$3:$N$38,'Data fittings'!$B$3)","v":38.1},"mm"]
["End to end","F",{"$f":"INDEX('Data fittings'!$P$3:$P$38,'Data fittings'!$B$3)","v":76.2},"mm"]
["Weight Std.","W",{"$f":"INDEX('Data fittings'!$AB$3:$AB$38,'Data fittings'!$B$3)","v":0.34},"kg"]
["Weight XS","W",{"$f":"INDEX('Data fittings'!$AC$3:$AC$38,'Data fittings'!$B$3)","v":0.42},"kg"]
[]
["Cap acc. ANSI B 16.9"]
["Diam. outside","Do",{"$f":"INDEX('Data fittings'!$H$3:$H$38,'Data fittings'!$A$3)","v":33.4},"mm","Size"]
["Diam. Inside std.","Di",{"$f":"INDEX('Data fittings'!$I$3:$I$38,'Data fittings'!$A$3)","v":26.64},"mm"]
["Diam. Inside XS","Di",{"$f":"INDEX('Data fittings'!$J$3:$J$38,'Data fittings'!$A$3)","v":24.3},"mm"]
["Wallth. Std.","s",{"$f":"INDEX('Data fittings'!$Q$3:$Q$38,'Data fittings'!$A$3)","v":3.38},"mm"]
["Wallth. XS","s",{"$f":"INDEX('Data fittings'!$R$3:$R$38,'Data fittings'!$A$3)","v":4.55},"mm"]
["Cap length Std.","H",{"$f":"INDEX('Data fittings'!$S$3:$S$38,'Data fittings'!$A$3)","v":38.1},"mm"]
["Cap length XS","H",{"$f":"INDEX('Data fittings'!$T$3:$T$38,'Data fittings'!$A$3)","v":38.1},"mm"]
["Weight Std.","W",{"$f":"INDEX('Data fittings'!$AD$3:$AD$38,'Data fittings'!$A$3)","v":0.1},"kg"]
["Weight XS","W",{"$f":"INDEX('Data fittings'!$AE$3:$AE$38,'Data fittings'!$A$3)","v":0.13},"kg"]

{"sheet":"Data fittings","index":15,"n_rows":38,"n_cols":31,"rows_kept":38,"cut":false,"hidden":true,"merged":[[0,13,0,15]]}
["Fitting data : Elbows, Straight Tees and Caps",null,null,null,null,"NPS","DN","OD","ID","ID","Elbow LR","Elbow SR","Elbow 45º","Tee",null,null,"Wallth.","Wallth.","Cap",null,null,"Elbow 90º LR","Elbow 90º LR","Elbow 45º LR","Elbow 45º LR","Elbow 90º SR","Elbow 90º SR","Tee","Tee","Cap","Cap"]
[null,null,null,null,null,null,null,null,"Std.","XS","R = 1,5D","R = D","B","C","E","F","std.","XS","H","H1","D2","Weight std.","Weight XS","Weight std.","Weight XS","Weight std.","Weight XS","Weight std.","Weight XS","Weight std.","Weight XS"]
[6.0,6.0,13.0,6.0,6.0,"1/8\"",6.0,10.29,{"$f":"$H3-(2*$Q3)","v":6.83},{"$f":"$H3-(2*$R3)","v":5.47},"-","-","-","-","-","-",1.73,2.41,"-",null,"-","-","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,"1/4\"",10.0,13.72,9.24,7.68,"-","-","-","-","-","-",2.24,3.02,"-",null,"-","-","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,"3/8\"","-",17.15,12.53,10.75,"-","-","-","-","-","-",2.31,3.2,"-",null,"3/8\"","-","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,"1/2\"",15.0,21.34,15.8,13.88,38.1,"-",15.9,25.4,25.4,{"$f":"2*$O6","v":50.8},2.77,3.73,25.4,25.4,"1/2\"",0.08,0.1,0.04,0.05,"-","-",0.11,0.14,0.03,0.04]
[null,null,null,null,null,"3/4\"",20.0,26.67,20.93,18.85,38.1,"-",11.1,28.6,28.6,57.2,2.87,3.91,25.4,25.4,"3/4\"",0.08,0.1,0.04,0.05,"-","-",0.17,0.21,0.06,0.07]
[null,null,null,null,null,"1\"",25.0,33.4,26.64,24.3,38.1,25.4,22.2,38.1,38.1,76.2,3.38,4.55,38.1,38.1,"1\"",0.15,0.19,0.11,0.14,0.1,0.132,0.34,0.42,0.1,0.13]
[null,null,null,null,null,"1¼\"",32.0,42.16,35.04,32.46,47.6,31.8,25.4,47.6,47.6,95.2,3.56,4.85,38.1,38.1,"1¼\"",0.26,0.34,0.17,0.22,0.17,0.227,0.61,0.74,0.14,0.18]
[null,null,null,null,null,"1½\"",40.0,48.26,40.9,38.1,57.2,38.1,28.6,57.2,57.2,114.4,3.68,5.08,38.1,38.1,"1½\"",0.37,0.48,0.23,0.3,0.25,0.33,0.92,1.12,0.17,0.22]
[null,null,null,null,null,"2\"",50.0,60.33,52.51,49.25,76.2,50.8,34.9,63.5,63.5,127,3.91,5.54,38.1,44.0,"2\"",0.67,0.9,0.37,0.49,0.45,0.6,1.34,1.69,0.23,0.3]
[null,null,null,null,null,"2½\"",65.0,73.03,62.71,59.01,95.3,63.5,44.5,76.2,76.2,152.4,5.16,7.01,38.1,50.8,"2½\"",1.33,1.73,0.74,0.95,0.88,1.14,2.36,2.92,0.37,0.46]
[null,null,null,null,null,"3\"",80.0,88.9,77.92,73.66,114.3,76.2,50.8,85.7,85.7,171.4,5.49,7.62,50.8,63.5,"3\"",2.08,2.78,1.1,1.47,1.38,1.83,3.36,4.29,0.64,0.84]
[null,null,null,null,null,"3½\"","-",101.6,90.12,85.44,133.4,88.9,57.2,95.3,95.3,190.6,5.74,8.08,63.5,76.2,"3½\"",2.92,3.96,1.49,2.01,1.93,2.61,4.47,5.72,0.96,1.28]
[null,null,null,null,null,"4\"",100.0,114.3,102.26,97.18,152.4,101.6,63.5,104.8,104.8,209.6,6.02,8.56,63.5,76.2,"4\"",3.95,5.4,1.95,2.66,2.62,3.58,5.72,7.44,1.16,1.55]
[null,null,null,null,null,"5\"",125.0,141.3,128.2,122.24,190.5,127.0,79.4,123.8,123.8,247.6,6.55,9.53,76.2,89.0,"5\"",6.67,9.34,3.31,4.63,4.42,6.21,8.98,12.0,1.91,2.61]
[null,null,null,null,null,"6\"",150.0,168.28,154.06,146.34,228.6,152.4,95.3,142.9,142.9,285.8,7.11,10.97,88.9,102.0,"6\"",10.4,15.5,5.13,7.57,6.89,10.3,13.3,19.1,2.91,4.19]
[null,null,null,null,null,"8\"",200.0,219.08,202.72,193.68,304.8,203.2,127.0,177.8,177.8,355.6,8.18,12.7,101.6,127.0,"8\"",20.9,31.3,10.3,15.4,13.8,20.7,24.4,34.7,5.13,7.4]
[null,null,null,null,null,"10\"",250.0,273.05,254.51,247.65,381.0,254.0,158.8,215.9,215.9,431.8,9.27,12.7,127.0,152.0,"10\"",37.0,49.4,18.3,24.4,24.5,32.9,41.4,53.5,9.08,11.9]
[null,null,null,null,null,"12\"",300.0,323.85,304.79,298.45,457.2,304.8,190.5,254.0,254.0,508,9.53,12.7,152.4,178.0,"12\"",54.0,71.2,27.0,35.5,36.1,47.2,59.9,75.7,13.4,17.3]
[null,null,null,null,null,"14\"",350.0,355.6,336.54,330.2,533.4,355.6,222.3,279.4,279.4,558.8,9.53,12.7,165.1,191.0,"14\"",69.9,91.6,34.7,45.4,46.3,61.2,72.1,92.1,16.0,20.8]
[null,null,null,null,null,"16\"",400.0,406.4,387.34,381,609.6,406.4,254.0,304.8,304.8,609.6,9.53,12.7,177.8,203.0,"16\"",91.2,120.2,45.4,59.9,61.2,80.3,99.3,122.9,20.1,26.1]
[null,null,null,null,null,"18\"",450.0,457.2,438.14,431.8,685.8,457.2,285.8,342.9,342.9,685.8,9.53,12.7,203.2,229.0,"18\"",116.1,153.3,58.1,76.2,77.6,102.1,127.9,159.2,25.9,33.9]
[null,null,null,null,null,"20\"",500.0,508.0,488.94,482.6,762.0,508.0,317.5,381.0,381.0,762,9.53,12.7,228.6,254.0,"20\"",143.8,190.1,71.7,94.3,96.2,126.1,160.6,200.5,32.5,42.6]
[null,null,null,null,null,"22\"",550.0,558.8,539.74,533.4,838.2,558.8,342.9,419.1,419.1,838.2,9.53,12.7,254.0,254.0,"22\"",174.6,230.4,87.1,114.8,117.0,154.2,198.2,248.6,39.3,52.2]
[null,null,null,null,null,"24\"",600.0,609.6,590.54,584.2,914.4,609.6,381.0,431.8,431.8,863.6,9.53,12.7,266.7,305.0,"24\"",207.7,274.9,103.9,137.0,138.3,183.3,223.6,275.3,46.3,60.8]
[null,null,null,null,null,"26\"",650.0,660.4,641.34,635,990.6,660.4,406.2,495.3,495.3,990.6,9.53,12.7,266.7,"-","26\"",244.5,223.4,122.0,161.0,163.8,216.8,287.6,360.2,50.8,65.8]
[null,null,null,null,null,"28\"",700.0,711.2,692.14,685.8,1066.8,711.2,438.2,520.7,520.7,1041.4,9.53,12.7,266.7,"-","28\"",308.0,385.0,154.0,193.0,206.8,258.6,337.0,421.0,56.0,75.3]
[null,null,null,null,null,"30\"",750.0,762.0,742.94,736.6,1143.0,762.0,469.9,558.8,558.8,1117.6,9.53,12.7,266.7,"-","30\"",326.6,432.2,168.4,215.5,217.7,287.6,387.8,483.1,56.7,79.4]
[null,null,null,null,null,"32\"",800.0,812.8,793.74,787.4,1219.2,812.8,501.7,595.6,595.6,1191.2,9.53,12.7,266.7,"-","32\"",386.0,511.0,193.0,255.0,206.8,342.0,451.0,559.0,65.8,93.4]
[null,null,null,null,null,"34\"",850.0,863.6,844.54,838.2,1295.4,"-",633.4,635.0,635.0,1270,9.53,12.7,266.7,"-","34\"",420.0,557.9,210.0,279.0,"-","-",515.3,644.1,72.6,95.3]
[null,null,null,null,null,"36\"",900.0,914.4,895.34,889,1371.6,914.4,565.2,673.1,673.1,1346.2,9.53,12.7,266.7,"-","36\"",471.7,626.0,235.0,311.2,313.9,414.1,586.9,730.3,79.4,107.0]
[null,null,null,null,null,"38\"",950.0,965.2,946.14,939.8,1447.8,965.2,600.1,711.2,711.2,1422.4,9.53,12.7,304.8,"-","38\"",544.0,717.0,272.0,354.0,364.7,480.4,638.0,812.0,86.2,124.7]
[null,null,null,null,null,"40\"",1000.0,1016.0,996.94,990.6,1524.0,1016.0,631.8,749.3,749.3,1498.6,9.53,12.7,304.8,"-","40\"",590.0,794.0,295.0,397.0,395.1,532.1,690.0,895.0,95.3,129.3]
[null,null,null,null,null,"42\"",1050.0,1066.8,1047.74,1041.4,1600.2,1066.8,660.4,711.2,762.0,1524,9.53,12.7,304.8,"-","42\"",644.1,825.7,320.7,425.0,489.4,648.6,795.0,1045.0,104.0,136.0]
[null,null,null,null,null,"44\"",1100.0,1117.6,1098.54,1092.2,1676.4,1117.6,695.3,762.0,812.8,1625.6,9.53,12.7,342.9,"-","44\"",726.0,975.0,363.0,488.0,486.3,653.2,899.0,1194.0,120.2,167.8]
[null,null,null,null,null,"46\"",1150.0,1168.4,1149.34,1143,1752.6,1168.4,727.1,800.1,850.9,1701.8,9.53,12.7,342.9,"-","46\"",816.0,1055.0,408.0,530.0,547.1,706.7,1007.0,1346.0,136.0,186.0]
[null,null,null,null,null,"48\"",1200.0,1219.2,1200.14,1193.8,1828.8,1219.2,758.8,838.2,889.0,1778,9.53,12.7,342.9,"-",null,907.0,1134.0,454.0,567.0,607.8,759.8,1113.0,1499.0,159.0,215.5]

{"sheet":"Red. fittings","index":16,"n_rows":49,"n_cols":5,"rows_kept":49,"cut":false,"hidden":true,"merged":[[0,0,0,8]]}
["DIMENSIONS of REDUCERS & REDUCED TEES"]
["Conc. reducer acc. ANSI B16.9   run-size"]
["Diam. outside","D1",{"$f":"INDEX('Data red. fittings'!$E$207:$E$340,'Data red. fittings'!$C$207)","v":26.67},"mm","Size"]
["Diam. Inside Std.","Di",{"$f":"INDEX('Data red. fittings'!$G$207:$G$340,'Data red. fittings'!$C$207)","v":20.93},"mm"]
["Diam. Inside XS","Di",{"$f":"INDEX('Data red. fittings'!$I$207:$I$340,'Data red. fittings'!$C$207)","v":18.85},"mm"]
["Wallth. Std.","s1",{"$f":"INDEX('Data red. fittings'!$M$207:$M$340,'Data red. fittings'!$C$207)","v":2.87},"mm"]
["Wallth. XS","s1",{"$f":"INDEX('Data red. fittings'!$O$207:$O$340,'Data red. fittings'!$C$207)","v":3.91},"mm"]
["Length","L",{"$f":"INDEX('Data red. fittings'!$K$207:$K$340,'Data red. fittings'!$C$207)","v":38.1},"mm"]
[null,null,"red.-size"]
["Diam. outside","D2",{"$f":"INDEX('Data red. fittings'!$F$207:$F$340,'Data red. fittings'!$C$207)","v":17.15},"mm"]
["Diam. Inside Std.","Di",{"$f":"INDEX('Data red. fittings'!$H$207:$H$340,'Data red. fittings'!$C$207)","v":12.53},"mm"]
["Diam. Inside XS","Di",{"$f":"INDEX('Data red. fittings'!$J$207:$J$340,'Data red. fittings'!$C$207)","v":10.75},"mm"]
["Wallth. Std.","s2",{"$f":"INDEX('Data red. fittings'!$N$207:$N$340,'Data red. fittings'!$C$207)","v":2.31},"mm"]
["Wallth. XS","s2",{"$f":"INDEX('Data red. fittings'!$P$207:$P$340,'Data red. fittings'!$C$207)","v":3.2},"mm"]
["Weight Std.","W",{"$f":"INDEX('Data red. fittings'!$Q$207:$Q$340,'Data red. fittings'!$C$207)","v":0.09},"kg"]
["Weight XS","W",{"$f":"INDEX('Data red. fittings'!$R$207:$R$340,'Data red. fittings'!$C$207)","v":0.11},"kg"]
["Exc. reducer acc. ANSI B16.9    run-size"]
["Diam. outside","D1",{"$f":"INDEX('Data red. fittings'!$E$207:$E$340,'Data red. fittings'!$B$207)","v":26.67},"mm","Size"]
["Diam. Inside Std.","Di",{"$f":"INDEX('Data red. fittings'!$G$207:$G$340,'Data red. fittings'!$B$207)","v":20.93},"mm"]
["Diam. Inside XS","Di",{"$f":"INDEX('Data red. fittings'!$I$207:$I$340,'Data red. fittings'!$B$207)","v":18.85},"mm"]
["Wallth. Std.","s1",{"$f":"INDEX('Data red. fittings'!$M$207:$M$340,'Data red. fittings'!$B$207)","v":2.87},"mm"]
["Wallth. XS","s1",{"$f":"INDEX('Data red. fittings'!$O$207:$O$340,'Data red. fittings'!$B$207)","v":3.91},"mm"]
["Length","L",{"$f":"INDEX('Data red. fittings'!$K$207:$K$340,'Data red. fittings'!$B$207)","v":38.1},"mm"]
["Center to center","M",{"$f":"INDEX('Data red. fittings'!$L$207:$L$340,'Data red. fittings'!$B$207)","v":4.76},"mm"]
[null,null,"red.-size"]
["Diam. outside","D2",{"$f":"INDEX('Data red. fittings'!$F$207:$F$340,'Data red. fittings'!$B$207)","v":17.15},"mm"]
["Diam. Inside Std.","Di",{"$f":"INDEX('Data red. fittings'!$H$207:$H$340,'Data red. fittings'!$B$207)","v":12.53},"mm"]
["Diam. Inside XS","Di",{"$f":"INDEX('Data red. fittings'!$J$207:$J$340,'Data red. fittings'!$B$207)","v":10.75},"mm"]
["Wallth. Std.","s2",{"$f":"INDEX('Data red. fittings'!$N$207:$N$340,'Data red. fittings'!$B$207)","v":2.31},"mm"]
["Wallth. XS","s2",{"$f":"INDEX('Data red. fittings'!$P$207:$P$340,'Data red. fittings'!$B$207)","v":3.2},"mm"]
["Weight Std.","W",{"$f":"INDEX('Data red. fittings'!$Q$207:$Q$340,'Data red. fittings'!$B$207)","v":0.09},"kg"]
["Weight XS","W",{"$f":"INDEX('Data red. fittings'!$R$207:$R$340,'Data red. fittings'!$B$207)","v":0.11},"kg"]
["Reduced Tee acc. ANSI B16.9   run-size"]
["Diam. outside","D1",{"$f":"INDEX('Data red. fittings'!$E$3:$E$203,'Data red. fittings'!$C$3)","v":21.34},"mm","Size"]
["Diam. Inside Std.","Di",{"$f":"INDEX('Data red. fittings'!$G$3:$G$203,'Data red. fittings'!$C$3)","v":15.8},"mm"]
["Diam. Inside XS","Di",{"$f":"INDEX('Data red. fittings'!$I$3:$I$203,'Data red. fittings'!$C$3)","v":13.88},"mm"]
["Wallth. Std.","s1",{"$f":"INDEX('Data red. fittings'!$K$3:$K$203,'Data red. fittings'!$C$3)","v":2.77},"mm"]
["Wallth. XS","s1",{"$f":"INDEX('Data red. fittings'!$M$3:$M$203,'Data red. fittings'!$C$3)","v":3.73},"mm"]
["Center to end","E",{"$f":"INDEX('Data red. fittings'!$P$3:$P$203,'Data red. fittings'!$C$3)","v":25.4},"mm"]
["End to end (branch)","C",{"$f":"INDEX('Data red. fittings'!$O$3:$O$203,'Data red. fittings'!$C$3)","v":25.4},"mm"]
["End to end (run)","F",{"$f":"INDEX('Data red. fittings'!$Q$3:$Q$203,'Data red. fittings'!$C$3)","v":50.8},"mm"]
[null,null,"red.-size"]
["Diam. outside","D2",{"$f":"INDEX('Data red. fittings'!$F$3:$F$203,'Data red. fittings'!$C$3)","v":13.72},"mm"]
["Diam. Inside Std.","Di",{"$f":"INDEX('Data red. fittings'!$H$3:$H$203,'Data red. fittings'!$C$3)","v":9.24},"mm"]
["Diam. Inside XS","Di",{"$f":"INDEX('Data red. fittings'!$J$3:$J$203,'Data red. fittings'!$C$3)","v":7.68},"mm"]
["Wallth. Std.","s2",{"$f":"INDEX('Data red. fittings'!$L$3:$L$203,'Data red. fittings'!$C$3)","v":2.24},"mm"]
["Wallth. XS","s2",{"$f":"INDEX('Data red. fittings'!$N$3:$N$203,'Data red. fittings'!$C$3)","v":3.02},"mm"]
["Weight Std.","W",{"$f":"INDEX('Data red. fittings'!$R$3:$R$203,'Data red. fittings'!$C$3)","v":0.104},"kg"]
["Weight XS","W",{"$f":"INDEX('Data red. fittings'!$S$3:$S$203,'Data red. fittings'!$C$3)","v":0.122},"kg"]

{"sheet":"Data red. fittings","index":17,"n_rows":340,"n_cols":19,"rows_kept":340,"cut":false,"hidden":true,"merged":[[204,6,204,7],[204,8,204,9],[204,12,204,15],[204,16,204,17],[0,4,0,5],[0,6,0,7],[0,8,0,9],[0,10,0,13],[0,14,0,16],[0,17,0,18],[204,4,204,5]]}
["Fitting data:",null,null,"Reducing Tee","D outside",null,"D std. inside",null,"D XS inside",null,"Wallth.",null,null,null,"Dimensions Red. Tee",null,null,"Red. Tee"]
["Reduced Tees",null,null,"Std. - XS","D1","D2","d1","d2","d1","d2","s1 Std.","s2 Std.","s1 XS","s2 XS","C","E","F","Weight std.","Weight XS"]
[null,null,1.0,"1/2\"x1/2\"x1/4\"",21.34,13.72,{"$f":"E3-2*K3","v":15.8},9.24,{"$f":"E3-2*M3","v":13.88},7.68,2.77,2.24,3.73,3.02,25.4,25.4,{"$f":"2*P3","v":50.8},0.104,0.122]
[null,null,null,"1/2\"x1/2\"x3/8\"",21.34,17.15,{"$f":"E4-2*K4","v":15.8},12.53,{"$f":"E4-2*M4","v":13.88},10.75,2.77,2.31,3.73,3.2,25.4,25.4,50.8,0.104,0.127]
[null,null,null,"3/4\" x 3/4\" x 3/8\"",26.67,17.15,{"$f":"E5-2*K5","v":20.93},12.53,{"$f":"E5-2*M5","v":18.85},10.75,2.87,2.31,3.91,3.2,28.6,28.6,57.2,0.15,0.186]
[null,null,null,"3/4\" x 3/4\" x 1/2\"",26.67,21.34,{"$f":"E6-2*K6","v":20.93},15.8,{"$f":"E6-2*M6","v":18.85},13.88,2.87,2.77,3.91,3.73,28.6,28.6,57.2,0.154,0.191]
[null,null,null,"1\" x 1\" x 3/8\"",33.4,17.15,{"$f":"E7-2*K7","v":26.64},12.53,{"$f":"E7-2*M7","v":24.3},10.75,3.38,2.31,4.55,3.2,38.1,38.1,76.2,0.29,0.358]
[null,null,null,"1\" x 1\" x 1/2\"",33.4,21.34,{"$f":"E8-2*K8","v":26.64},15.8,{"$f":"E8-2*M8","v":24.3},13.88,3.38,2.77,4.55,3.73,38.1,38.1,76.2,0.29,0.358]
[null,null,null,"1\" x 1\" x 3/4\"",33.4,26.67,{"$f":"E9-2*K9","v":26.64},20.93,{"$f":"E9-2*M9","v":24.3},18.85,3.38,2.87,4.55,3.91,38.1,38.1,76.2,0.295,0.363]
[null,null,null,"1¼\" x 1¼\" x 1/2\"",42.16,21.34,{"$f":"E10-2*K10","v":35.04},15.8,{"$f":"E10-2*M10","v":32.46},13.88,3.56,2.77,4.85,3.73,47.6,47.6,95.2,0.499,0.621]
[null,null,null,"1¼\" x 1¼\" x 3/4\"",42.16,26.67,{"$f":"E11-2*K11","v":35.04},20.93,{"$f":"E11-2*M11","v":32.46},18.85,3.56,2.87,4.85,3.91,47.6,47.6,95.2,0.503,0.626]
[null,null,null,"1¼\" x 1¼\" x 1\"",42.16,33.4,{"$f":"E12-2*K12","v":35.04},26.64,{"$f":"E12-2*M12","v":32.46},24.3,3.56,3.38,4.85,4.55,47.6,47.6,95.2,0.531,0.658]
[null,null,null,"1½ x 1½\" x 1/2\"",48.26,21.34,{"$f":"E13-2*K13","v":40.9},15.8,{"$f":"E13-2*M13","v":38.1},13.88,3.68,2.77,5.08,3.73,57.2,57.2,114.4,0.73,0.918]
[null,null,null,"1½ x 1½\" x 3/4\"",48.26,26.67,{"$f":"E14-2*K14","v":40.9},20.93,{"$f":"E14-2*M14","v":38.1},18.85,3.68,2.87,5.08,3.91,57.2,57.2,114.4,0.73,0.921]
[null,null,null,"1½ x 1½\" x 1\"",48.26,33.4,{"$f":"E15-2*K15","v":40.9},26.64,{"$f":"E15-2*M15","v":38.1},24.3,3.68,3.38,5.08,4.55,57.2,57.2,114.4,0.762,0.948]
[null,null,null,"1½ x 1½\" x 1¼\"",48.26,42.16,{"$f":"E16-2*K16","v":40.9},35.04,{"$f":"E16-2*M16","v":38.1},32.46,3.68,3.56,5.08,4.85,57.2,57.2,114.4,0.798,0.998]
[null,null,null,"2\" x 2\" x 3/4\"",60.33,26.67,{"$f":"E17-2*K17","v":52.51},20.93,{"$f":"E17-2*M17","v":49.25},18.85,3.91,2.87,5.54,3.91,44.5,63.5,127,1.09,1.41]
[null,null,null,"2\" x 2\" x 1\"",60.33,33.4,{"$f":"E18-2*K18","v":52.51},26.64,{"$f":"E18-2*M18","v":49.25},24.3,3.91,3.38,5.54,4.55,50.8,63.5,127,1.12,1.44]
[null,null,null,"2\" x 2\" x 1¼\"",60.33,42.16,{"$f":"E19-2*K19","v":52.51},35.04,{"$f":"E19-2*M19","v":49.25},32.46,3.91,3.56,5.54,4.85,57.2,63.5,127,1.16,1.48]
[null,null,null,"2\" x 2\" x 1½\"",60.33,48.26,{"$f":"E20-2*K20","v":52.51},40.9,{"$f":"E20-2*M20","v":49.25},38.1,3.91,3.68,5.54,5.08,60.3,63.5,127,1.21,1.54]
[null,null,null,"2½\" x 2½\" x 1\"",73.03,33.4,{"$f":"E21-2*K21","v":62.71},26.64,{"$f":"E21-2*M21","v":59.01},24.3,5.16,3.38,7.01,4.55,57.2,76.2,152.4,1.96,2.48]
[null,null,null,"2½\" x 2½\" x 1¼\"",73.03,42.16,{"$f":"E22-2*K22","v":62.71},35.04,{"$f":"E22-2*M22","v":59.01},32.46,5.16,3.56,7.01,4.85,63.5,76.2,152.4,1.99,2.51]
[null,null,null,"2½\" x 2½\" x 1½\"",73.03,48.26,{"$f":"E23-2*K23","v":62.71},40.9,{"$f":"E23-2*M23","v":59.01},38.1,5.16,3.68,7.01,5.08,66.7,76.2,152.4,2.04,2.57]
[null,null,null,"2½\" x 2½\" x 2\"",73.03,60.33,{"$f":"E24-2*K24","v":62.71},52.51,{"$f":"E24-2*M24","v":59.01},49.25,5.16,3.91,7.01,5.54,69.9,76.2,152.4,2.08,2.61]
[null,null,null,"3\" x 3\" x 1\"",88.9,33.4,{"$f":"E25-2*K25","v":77.92},26.64,{"$f":"E25-2*M25","v":73.66},24.3,5.49,3.38,7.62,4.55,66.7,85.7,171.4,2.85,3.68]
[null,null,null,"3\" x 3\" x 1¼\"",88.9,42.16,{"$f":"E26-2*K26","v":77.92},35.04,{"$f":"E26-2*M26","v":73.66},32.46,5.49,3.56,7.62,4.85,69.9,85.7,171.4,2.88,3.71]
[null,null,null,"3\" x 3\" x 1½\"",88.9,48.26,{"$f":"E27-2*K27","v":77.92},40.9,{"$f":"E27-2*M27","v":73.66},38.1,5.49,3.68,7.62,5.08,73.0,85.7,171.4,2.92,3.76]
[null,null,null,"3\" x 3\" x 2\"",88.9,60.33,{"$f":"E28-2*K28","v":77.92},52.51,{"$f":"E28-2*M28","v":73.66},49.25,5.49,3.91,7.62,5.54,76.2,85.7,171.4,2.95,3.79]
[null,null,null,"3\" x 3\" x 2½\"",88.9,73.03,{"$f":"E29-2*K29","v":77.92},62.71,{"$f":"E29-2*M29","v":73.66},59.01,5.49,5.16,7.62,7.01,82.6,85.7,171.4,3.09,3.9]
[null,null,null,"3½\" x 3½\" x 1½\"",101.6,48.26,{"$f":"E30-2*K30","v":90.12},40.9,{"$f":"E30-2*M30","v":85.44},38.1,5.74,3.68,8.08,5.08,79.4,95.3,190.6,3.85,5.03]
[null,null,null,"3½\" x 3½\" x 2\"",101.6,60.33,{"$f":"E31-2*K31","v":90.12},52.51,{"$f":"E31-2*M31","v":85.44},49.25,5.74,3.91,8.08,5.54,82.6,95.3,190.6,3.85,5.08]
[null,null,null,"3½\" x 3½\" x 2½\"",101.6,73.03,{"$f":"E32-2*K32","v":90.12},62.71,{"$f":"E32-2*M32","v":85.44},59.01,5.74,5.16,8.08,7.01,88.9,95.3,190.6,3.99,5.22]
[null,null,null,"3½\" x 3½\" x 3\"",101.6,88.9,{"$f":"E33-2*K33","v":90.12},77.92,{"$f":"E33-2*M33","v":85.44},73.66,5.74,5.49,8.08,7.62,92.1,95.3,190.6,4.09,5.31]
[null,null,null,"4\" x 4\" x 1½\"",114.3,48.26,{"$f":"E34-2*K34","v":102.26},40.9,{"$f":"E34-2*M34","v":97.18},38.1,6.02,3.68,8.56,5.08,85.7,104.8,209.6,4.94,6.53]
[null,null,null,"4\" x 4\" x 2\"",114.3,60.33,{"$f":"E35-2*K35","v":102.26},52.51,{"$f":"E35-2*M35","v":97.18},49.25,6.02,3.91,8.56,5.54,88.9,104.8,209.6,4.99,6.58]
[null,null,null,"4\" x 4\" x 2½\"",114.3,73.03,{"$f":"E36-2*K36","v":102.26},62.71,{"$f":"E36-2*M36","v":97.18},59.01,6.02,5.16,8.56,7.01,95.3,104.8,209.6,5.13,6.67]
[null,null,null,"4\" x 4\" x 3\"",114.3,88.9,{"$f":"E37-2*K37","v":102.26},77.92,{"$f":"E37-2*M37","v":97.18},73.66,6.02,5.49,8.56,7.62,98.4,104.8,209.6,5.17,6.8]
[null,null,null,"4\" x 4\" x 3½\"",114.3,101.6,{"$f":"E38-2*K38","v":102.26},90.12,{"$f":"E38-2*M38","v":97.18},85.44,6.02,5.74,8.56,8.08,101.4,104.8,209.6,5.26,6.94]
[null,null,null,"5\" x 5\" x 2\"",141.3,60.33,{"$f":"E39-2*K39","v":128.2},52.51,{"$f":"E39-2*M39","v":122.24},49.25,6.55,3.91,9.53,5.54,104.8,123.8,247.6,7.8,10.6]
[null,null,null,"5\" x 5\" x 2½\"",141.3,73.03,{"$f":"E40-2*K40","v":128.2},62.71,{"$f":"E40-2*M40","v":122.24},59.01,6.55,5.16,9.53,7.01,108.0,123.8,247.6,7.89,10.7]
[null,null,null,"5\" x 5\" x 3\"",141.3,88.9,{"$f":"E41-2*K41","v":128.2},77.92,{"$f":"E41-2*M41","v":122.24},73.66,6.55,5.49,9.53,7.62,111.1,123.8,247.6,7.98,10.75]
[null,null,null,"5\" x 5\" x 3½\"",141.3,101.6,{"$f":"E42-2*K42","v":128.2},90.12,{"$f":"E42-2*M42","v":122.24},85.44,6.55,5.74,9.53,8.08,114.3,123.8,247.6,8.07,10.8]
[null,null,null,"5\" x 5\" x 4\"",141.3,114.3,{"$f":"E43-2*K43","v":128.2},102.26,{"$f":"E43-2*M43","v":122.24},97.18,6.55,6.02,9.53,8.56,117.5,123.8,247.6,8.21,11.0]
[null,null,null,"6\" x 6\" x 2½\"",168.28,73.03,{"$f":"E44-2*K44","v":154.06},62.71,{"$f":"E44-2*M44","v":146.34},59.01,7.11,5.16,10.97,7.01,120.7,142.9,285.8,11.7,16.7]
[null,null,null,"6\" x 6\" x 3\"",168.28,88.9,{"$f":"E45-2*K45","v":154.06},77.92,{"$f":"E45-2*M45","v":146.34},73.66,7.11,5.49,10.97,7.62,123.8,142.9,285.8,11.7,16.7]
[null,null,null,"6\" x 6\" x 3½\"",168.28,101.6,{"$f":"E46-2*K46","v":154.06},90.12,{"$f":"E46-2*M46","v":146.34},85.44,7.11,5.74,10.97,8.08,127.0,142.9,285.8,11.8,16.8]
[null,null,null,"6\" x 6\" x 4\"",168.28,114.3,{"$f":"E47-2*K47","v":154.06},102.26,{"$f":"E47-2*M47","v":146.34},97.18,7.11,6.02,10.97,8.56,130.2,142.9,285.8,11.9,16.9]
[null,null,null,"6\" x 6\" x 5\"",168.28,141.3,{"$f":"E48-2*K48","v":154.06},128.2,{"$f":"E48-2*M48","v":146.34},122.24,7.11,6.55,10.97,9.53,136.5,142.9,285.8,12.1,17.1]
[null,null,null,"8\" x 8\" x 3\"",219.08,88.9,{"$f":"E49-2*K49","v":202.72},77.92,{"$f":"E49-2*M49","v":197.14},73.66,8.18,5.49,10.97,7.62,152.4,177.8,355.6,21.6,31.3]
[null,null,null,"8\" x 8\" x 3½\"",219.08,101.6,{"$f":"E50-2*K50","v":202.72},90.12,{"$f":"E50-2*M50","v":193.68},85.44,8.18,5.74,12.7,8.08,152.4,177.8,355.6,21.64,31.3]
[null,null,null,"8\" x 8\" x 4\"",219.08,114.3,{"$f":"E51-2*K51","v":202.72},102.26,{"$f":"E51-2*M51","v":193.68},97.18,8.18,6.02,12.7,8.56,155.6,177.8,355.6,21.7,31.4]
[null,null,null,"8\" x 8\" x 5\"",219.08,141.3,{"$f":"E52-2*K52","v":202.72},128.2,{"$f":"E52-2*M52","v":193.68},122.24,8.18,6.55,12.7,9.53,161.9,177.8,355.6,21.8,31.5]
[null,null,null,"8\" x 8\" x 6\"",219.08,168.28,{"$f":"E53-2*K53","v":202.72},154.06,{"$f":"E53-2*M53","v":193.68},146.34,8.18,7.11,12.7,10.97,168.3,177.8,355.6,22.1,31.9]
[null,null,null,"10\" x 10\" x 4\"",273.05,114.3,{"$f":"E54-2*K54","v":254.51},102.26,{"$f":"E54-2*M54","v":247.65},97.18,9.27,6.02,12.7,8.56,184.2,215.9,431.8,36.8,48.1]
[null,null,null,"10\" x 10\" x 5\"",273.05,141.3,{"$f":"E55-2*K55","v":254.51},128.2,{"$f":"E55-2*M55","v":247.65},122.24,9.27,6.55,12.7,9.53,190.5,215.9,431.8,36.9,48.1]
[null,null,null,"10\" x 10\" x 6\"",273.05,168.28,{"$f":"E56-2*K56","v":254.51},154.06,{"$f":"E56-2*M56","v":247.65},146.34,9.27,7.11,12.7,10.97,193.7,215.9,431.8,37.1,49.0]
[null,null,null,"10\" x 10\" x 8\"",273.05,219.08,{"$f":"E57-2*K57","v":254.51},202.72,{"$f":"E57-2*M57","v":247.65},193.68,9.27,8.18,12.7,12.7,203.2,215.9,431.8,37.6,49.4]
[null,null,null,"12\" x 12\" x 5\"",323.85,141.3,{"$f":"E58-2*K58","v":304.79},128.2,{"$f":"E58-2*M58","v":298.45},122.24,9.53,6.55,12.7,9.53,215.9,254.0,508,53.1,68.5]
[null,null,null,"12\" x 12\" x 6\"",323.85,168.28,{"$f":"E59-2*K59","v":304.79},154.06,{"$f":"E59-2*M59","v":298.45},146.34,9.53,7.11,12.7,10.97,219.1,254.0,508,53.1,68.5]
[null,null,null,"12\" x 12\" x 8\"",323.85,219.08,{"$f":"E60-2*K60","v":304.79},202.72,{"$f":"E60-2*M60","v":298.45},193.68,9.53,8.18,12.7,12.7,228.6,254.0,508,53.5,69.4]
[null,null,null,"12\" x 12\" x 10\"",323.85,273.05,{"$f":"E61-2*K61","v":304.79},254.51,{"$f":"E61-2*M61","v":298.45},247.65,9.53,9.27,12.7,12.7,241.3,254.0,508,54.9,70.3]
[null,null,null,"14\" x 14\" x 6\"",355.6,168.28,{"$f":"E62-2*K62","v":336.54},154.06,{"$f":"E62-2*M62","v":330.2},146.34,9.53,7.11,12.7,10.97,238.1,279.4,558.8,64.4,83.0]
[null,null,null,"14\" x 14\" x 8\"",355.6,219.08,{"$f":"E63-2*K63","v":336.54},202.72,{"$f":"E63-2*M63","v":330.2},193.68,9.53,8.18,12.7,12.7,247.7,279.4,558.8,64.9,83.5]
[null,null,null,"14\" x 14\" x 10\"",355.6,273.05,{"$f":"E64-2*K64","v":336.54},254.51,{"$f":"E64-2*M64","v":330.2},247.65,9.53,9.27,12.7,12.7,257.2,279.4,558.8,65.3,83.9]
[null,null,null,"14\" x 14\" x 12\"",355.6,323.85,{"$f":"E65-2*K65","v":336.54},304.79,{"$f":"E65-2*M65","v":330.2},298.45,9.53,9.53,12.7,12.7,269.9,279.4,558.8,66.7,85.7]
[null,null,null,"16\" x 16\" x 6\"",406.4,168.28,{"$f":"E66-2*K66","v":387.34},154.06,{"$f":"E66-2*M66","v":381},146.34,9.53,7.11,12.7,10.97,263.6,304.8,609.6,79.8,101.2]
[null,null,null,"16\" x 16\" x 8\"",406.4,219.08,{"$f":"E67-2*K67","v":387.34},202.72,{"$f":"E67-2*M67","v":381},193.68,9.53,8.18,12.7,12.7,273.1,304.8,609.6,83.9,105.7]
[null,null,null,"16\" x 16\" x 10\"",406.4,273.05,{"$f":"E68-2*K68","v":387.34},254.51,{"$f":"E68-2*M68","v":381},247.65,9.53,9.27,12.7,12.7,282.6,304.8,609.6,88.5,110.7]
[null,null,null,"16\" x 16\" x 12\"",406.4,323.85,{"$f":"E69-2*K69","v":387.34},304.79,{"$f":"E69-2*M69","v":381},298.45,9.53,9.53,12.7,12.7,295.3,304.8,609.6,92.5,115.7]
[null,null,null,"16\" x 16\" x 14\"",406.4,355.6,{"$f":"E70-2*K70","v":387.34},336.54,{"$f":"E70-2*M70","v":381},330.2,9.53,9.53,12.7,12.7,304.8,304.8,609.6,95.3,118.4]
[null,null,null,"18\" x 18\" x 8\"",457.2,219.08,{"$f":"E71-2*K71","v":438.14},202.72,{"$f":"E71-2*M71","v":431.8},193.68,9.53,8.18,12.7,12.7,299.5,342.9,685.8,104.8,133.4]
[null,null,null,"18\" x 18\" x 10\"",457.2,273.05,{"$f":"E72-2*K72","v":438.14},254.51,{"$f":"E72-2*M72","v":431.8},247.65,9.53,9.27,12.7,12.7,308.0,342.9,685.8,110.7,139.3]
[null,null,null,"18\" x 18\" x 12\"",457.2,323.85,{"$f":"E73-2*K73","v":438.14},304.79,{"$f":"E73-2*M73","v":431.8},298.45,9.53,9.53,12.7,12.7,320.7,342.9,685.8,118.2,145.1]
[null,null,null,"18\" x 18\" x 14\"",457.2,355.6,{"$f":"E74-2*K74","v":438.14},336.54,{"$f":"E74-2*M74","v":431.8},330.2,9.53,9.53,12.7,12.7,330.2,342.9,685.8,118.2,148.8]
[null,null,null,"18\" x 18\" x 16\"",457.2,406.4,{"$f":"E75-2*K75","v":438.14},387.34,{"$f":"E75-2*M75","v":431.8},381,9.53,9.53,12.7,12.7,330.2,342.9,685.8,122.0,152.4]
[null,null,null,"20\" x 20\" x 8\"",508.0,219.08,{"$f":"E76-2*K76","v":488.94},202.72,{"$f":"E76-2*M76","v":482.6},193.68,9.53,8.18,12.7,12.7,323.9,381.0,762,127.9,163.7]
[null,null,null,"20\" x 20\" x 10\"",508.0,273.05,{"$f":"E77-2*K77","v":488.94},254.51,{"$f":"E77-2*M77","v":482.6},247.65,9.53,9.27,12.7,12.7,333.4,381.0,762,133.8,170.6]
[null,null,null,"20\" x 20\" x 12\"",508.0,323.85,{"$f":"E78-2*K78","v":488.94},304.79,{"$f":"E78-2*M78","v":482.6},298.45,9.53,9.53,12.7,12.7,348.1,381.0,762,139.7,175.9]
[null,null,null,"20\" x 20\" x 14\"",508.0,355.6,{"$f":"E79-2*K79","v":488.94},336.54,{"$f":"E79-2*M79","v":482.6},330.2,9.53,9.53,12.7,12.7,355.6,381.0,762,143.3,181.0]
[null,null,null,"20\" x 20\" x 16\"",508.0,406.4,{"$f":"E80-2*K80","v":488.94},387.34,{"$f":"E80-2*M80","v":482.6},381,9.53,9.53,12.7,12.7,355.6,381.0,762,149.2,187.3]
[null,null,null,"20\" x 20\" x 18\"",508.0,457.2,{"$f":"E81-2*K81","v":488.94},438.14,{"$f":"E81-2*M81","v":482.6},431.8,9.53,9.53,12.7,12.7,368.3,381.0,762,155.1,193.7]
[null,null,null,"22\" x 22\" x 12\"",558.8,323.85,{"$f":"E82-2*K82","v":539.74},304.79,{"$f":"E82-2*M82","v":533.4},298.45,9.53,9.53,12.7,12.7,371.5,419.1,838.2,171.0,212.2]
[null,null,null,"22\" x 22\" x 14\"",558.8,355.6,{"$f":"E83-2*K83","v":539.74},336.54,{"$f":"E83-2*M83","v":533.4},330.2,9.53,9.53,12.7,12.7,381.0,419.1,838.2,172.4,217.3]
[null,null,null,"22\" x 22\" x 16\"",558.8,406.4,{"$f":"E84-2*K84","v":539.74},387.34,{"$f":"E84-2*M84","v":533.4},381,9.53,9.53,12.7,12.7,381.0,419.1,838.2,178.7,225.4]
[null,null,null,"22\" x 22\" x 18\"",558.8,457.2,{"$f":"E85-2*K85","v":539.74},438.14,{"$f":"E85-2*M85","v":533.4},431.8,9.53,9.53,12.7,12.7,393.7,419.1,838.2,188.1,233.2]
[null,null,null,"22\" x 22\" x 20\"",558.8,508.0,{"$f":"E86-2*K86","v":539.74},488.94,{"$f":"E86-2*M86","v":533.4},482.6,9.53,9.53,12.7,12.7,406.4,419.1,838.2,191.9,241.3]
[null,null,null,"24\" x 24\" x 10\"",609.6,273.05,{"$f":"E87-2*K87","v":590.54},253.99,{"$f":"E87-2*M87","v":584.2},247.65,9.53,9.53,12.7,12.7,384.2,431.8,863.6,178.7,227.7]
[null,null,null,"24\" x 24\" x 12\"",609.6,323.85,{"$f":"E88-2*K88","v":590.54},304.79,{"$f":"E88-2*M88","v":584.2},298.45,9.53,9.53,12.7,12.7,396.9,431.8,863.6,188.8,235.0]
[null,null,null,"24\" x 24\" x 14\"",609.6,355.6,{"$f":"E89-2*K89","v":590.54},336.54,{"$f":"E89-2*M89","v":584.2},330.2,9.53,9.53,12.7,12.7,406.4,431.8,863.6,190.1,240.0]
[null,null,null,"24\" x 24\" x 16\"",609.6,406.4,{"$f":"E90-2*K90","v":590.54},387.34,{"$f":"E90-2*M90","v":584.2},381,9.53,9.53,12.7,12.7,406.4,431.8,863.6,196.4,246.8]
[null,null,null,"24\" x 24\" x 18\"",609.6,457.2,{"$f":"E91-2*K91","v":590.54},438.14,{"$f":"E91-2*M91","v":584.2},431.8,9.53,9.53,12.7,12.7,419.1,431.8,863.6,205.5,255.8]
[null,null,null,"24\" x 24\" x 20\"",609.6,508.0,{"$f":"E92-2*K92","v":590.54},488.94,{"$f":"E92-2*M92","v":584.2},482.6,9.53,9.53,12.7,12.7,431.8,431.8,863.6,205.5,260.8]
[null,null,null,"26\" x 26\" x 12\"",660.4,323.85,{"$f":"E93-2*K93","v":641.34},304.79,{"$f":"E93-2*M93","v":635},298.45,9.53,9.53,12.7,12.7,422.3,495.3,990.6,234.1,294.4]
[null,null,null,"26\" x 26\" x 14\"",660.4,355.6,{"$f":"E94-2*K94","v":641.34},336.54,{"$f":"E94-2*M94","v":635},330.2,9.53,9.53,12.7,12.7,431.8,495.3,990.6,239.0,300.3]
[null,null,null,"26\" x 26\" x 16\"",660.4,406.4,{"$f":"E95-2*K95","v":641.34},387.34,{"$f":"E95-2*M95","v":635},381,9.53,9.53,12.7,12.7,431.8,495.3,990.6,246.8,310.3]
[null,null,null,"26\" x 26\" x 18\"",660.4,457.2,{"$f":"E96-2*K96","v":641.34},438.14,{"$f":"E96-2*M96","v":635},431.8,9.53,9.53,12.7,12.7,444.5,495.3,990.6,254.9,320.2]
[null,null,null,"26\" x 26\" x 20\"",660.4,508.0,{"$f":"E97-2*K97","v":641.34},488.94,{"$f":"E97-2*M97","v":635},482.6,9.53,9.53,12.7,12.7,457.2,495.3,990.6,263.5,330.2]
[null,null,null,"26\" x 26\" x 22\"",660.4,558.8,{"$f":"E98-2*K98","v":641.34},539.74,{"$f":"E98-2*M98","v":635},533.4,9.53,9.53,12.7,12.7,469.9,495.3,990.6,271.2,339.7]
[null,null,null,"26\" x 26\" x 24\"",660.4,609.6,{"$f":"E99-2*K99","v":641.34},590.54,{"$f":"E99-2*M99","v":635},584.2,9.53,9.53,12.7,12.7,482.6,495.3,990.6,279.4,349.7]
[null,null,null,"28\" x 28\" x 14\"",711.2,355.6,{"$f":"E100-2*K100","v":692.14},336.54,{"$f":"E100-2*M100","v":685.8},330.2,9.53,9.53,12.7,12.7,457.2,520.7,1041.4,274.0,346.0]
[null,null,null,"28\" x 28\" x 16\"",711.2,406.4,{"$f":"E101-2*K101","v":692.14},387.34,{"$f":"E101-2*M101","v":685.8},381,9.53,9.53,12.7,12.7,457.2,520.7,1041.4,283.0,357.0]
[null,null,null,"28\" x 28\" x 18\"",711.2,457.2,{"$f":"E102-2*K102","v":692.14},438.14,{"$f":"E102-2*M102","v":685.8},431.8,9.53,9.53,12.7,12.7,469.9,520.7,1041.4,292.1,368.8]
[null,null,null,"28\" x 28\" x 20\"",711.2,508.0,{"$f":"E103-2*K103","v":692.14},488.94,{"$f":"E103-2*M103","v":685.8},482.6,9.53,9.53,12.7,12.7,482.6,520.7,1041.4,301.6,380.0]
[null,null,null,"28\" x 28\" x 22\"",711.2,558.8,{"$f":"E104-2*K104","v":692.14},539.74,{"$f":"E104-2*M104","v":685.8},533.4,9.53,9.53,12.7,12.7,495.3,520.7,1041.4,310.7,390.0]
[null,null,null,"28\" x 28\" x 24\"",711.2,609.6,{"$f":"E105-2*K105","v":692.14},590.54,{"$f":"E105-2*M105","v":685.8},584.2,9.53,9.53,12.7,12.7,508.0,520.7,1041.4,319.8,400.5]
[null,null,null,"28\" x 28\" x 26\"",711.2,660.4,{"$f":"E106-2*K106","v":692.14},641.34,{"$f":"E106-2*M106","v":685.8},635,9.53,9.53,12.7,12.7,520.7,520.7,1041.4,325.2,410.5]
[null,null,null,"30\" x 30\" x 14\"",762.0,355.6,{"$f":"E107-2*K107","v":742.94},336.54,{"$f":"E107-2*M107","v":736.6},330.2,9.53,9.53,12.7,12.7,482.6,520.7,1041.4,308.9,392.4]
[null,null,null,"30\" x 30\" x 16\"",762.0,406.4,{"$f":"E108-2*K108","v":742.94},387.34,{"$f":"E108-2*M108","v":736.6},381,9.53,9.53,12.7,12.7,482.6,558.8,1117.6,319.3,403.7]
[null,null,null,"30\" x 30\" x 18\"",762.0,457.2,{"$f":"E109-2*K109","v":742.94},438.14,{"$f":"E109-2*M109","v":736.6},431.8,9.53,9.53,12.7,12.7,495.3,558.8,1117.6,329.8,417.3]
[null,null,null,"30\" x 30\" x 20\"",762.0,508.0,{"$f":"E110-2*K110","v":742.94},488.94,{"$f":"E110-2*M110","v":736.6},482.6,9.53,9.53,12.7,12.7,508.0,558.8,1117.6,339.7,428.6]
[null,null,null,"30\" x 30\" x 22\"",762.0,558.8,{"$f":"E111-2*K111","v":742.94},539.74,{"$f":"E111-2*M111","v":736.6},533.4,9.53,9.53,12.7,12.7,520.7,558.8,1117.6,350.2,440.0]
[null,null,null,"30\" x 30\" x 24\"",762.0,609.6,{"$f":"E112-2*K112","v":742.94},590.54,{"$f":"E112-2*M112","v":736.6},584.2,9.53,9.53,12.7,12.7,533.4,558.8,1117.6,360.6,451.3]
[null,null,null,"30\" x 30\" x 26\"",762.0,660.4,{"$f":"E113-2*K113","v":742.94},641.34,{"$f":"E113-2*M113","v":736.6},635,9.53,9.53,12.7,12.7,546.1,558.8,1117.6,370.6,462.7]
[null,null,null,"30\" x 30\" x 28\"",762.0,711.2,{"$f":"E114-2*K114","v":742.94},692.14,{"$f":"E114-2*M114","v":736.6},685.8,9.53,9.53,12.7,12.7,546.1,558.8,1117.6,378.3,471.7]
[null,null,null,"32\" x 32\" x 16\"",812.8,406.4,{"$f":"E115-2*K115","v":793.74},387.34,{"$f":"E115-2*M115","v":787.4},381,9.53,9.53,12.7,12.7,508.0,596.9,1193.8,381.0,461.0]
[null,null,null,"32\" x 32\" x 18\"",812.8,457.2,{"$f":"E116-2*K116","v":793.74},438.14,{"$f":"E116-2*M116","v":787.4},431.8,9.53,9.53,12.7,12.7,520.7,596.9,1193.8,390.0,475.0]
[null,null,null,"32\" x 32\" x 20\"",812.8,508.0,{"$f":"E117-2*K117","v":793.74},488.94,{"$f":"E117-2*M117","v":787.4},482.6,9.53,9.53,12.7,12.7,533.4,596.9,1193.8,406.0,487.6]
[null,null,null,"32\" x 32\" x 24\"",812.8,609.6,{"$f":"E118-2*K118","v":793.74},590.54,{"$f":"E118-2*M118","v":787.4},584.2,9.53,9.53,12.7,12.7,558.8,596.9,1193.8,410.0,513.5]
[null,null,null,"32\" x 32\" x 26\"",812.8,660.4,{"$f":"E119-2*K119","v":793.74},641.34,{"$f":"E119-2*M119","v":787.4},635,9.53,9.53,12.7,12.7,571.5,596.9,1193.8,420.5,526.2]
[null,null,null,"32\" x 32\" x 28\"",812.8,711.2,{"$f":"E120-2*K120","v":793.74},692.14,{"$f":"E120-2*M120","v":787.4},685.8,9.53,9.53,12.7,12.7,571.5,596.9,1193.8,429.1,536.2]
[null,null,null,"32\" x 32\" x 30\"",812.8,762.0,{"$f":"E121-2*K121","v":793.74},742.94,{"$f":"E121-2*M121","v":787.4},736.6,9.53,9.53,12.7,12.7,584.2,596.9,1193.8,441.4,543.4]
[null,null,null,"34\" x 34\" x 16\"",863.6,406.4,{"$f":"E122-2*K122","v":844.54},387.34,{"$f":"E122-2*M122","v":838.2},381,9.53,9.53,12.7,12.7,533.4,635.0,1270,411.4,519.4]
[null,null,null,"34\" x 34\" x 18\"",863.6,457.2,{"$f":"E123-2*K123","v":844.54},438.14,{"$f":"E123-2*M123","v":838.2},431.8,9.53,9.53,12.7,12.7,546.1,635.0,1270,423.2,532.9]
[null,null,null,"34\" x 34\" x 20\"",863.6,508.0,{"$f":"E124-2*K124","v":844.54},488.94,{"$f":"E124-2*M124","v":838.2},482.6,9.53,9.53,12.7,12.7,558.8,635.0,1270,435.4,546.6]
[null,null,null,"34\" x 34\" x 22\"",863.6,558.8,{"$f":"E125-2*K125","v":844.54},539.74,{"$f":"E125-2*M125","v":838.2},533.4,9.53,9.53,12.7,12.7,571.5,635.0,1270,447.2,552.5]
[null,null,null,"34\" x 34\" x 24\"",863.6,609.6,{"$f":"E126-2*K126","v":844.54},590.54,{"$f":"E126-2*M126","v":838.2},584.2,9.53,9.53,12.7,12.7,584.2,635.0,1270,459.5,576.1]
[null,null,null,"34\" x 34\" x 26\"",863.6,660.4,{"$f":"E127-2*K127","v":844.54},641.34,{"$f":"E127-2*M127","v":838.2},635,9.53,9.53,12.7,12.7,596.9,635.0,1270,471.3,589.7]
[null,null,null,"34\" x 34\" x 28\"",863.6,711.2,{"$f":"E128-2*K128","v":844.54},692.14,{"$f":"E128-2*M128","v":838.2},685.8,9.53,9.53,12.7,12.7,596.9,635.0,1270,480.4,601.0]
[null,null,null,"34\" x 34\" x 30\"",863.6,762.0,{"$f":"E129-2*K129","v":844.54},742.94,{"$f":"E129-2*M129","v":838.2},736.6,9.53,9.53,12.7,12.7,609.6,635.0,1270,492.1,614.6]
[null,null,null,"34\" x 34\" x 32\"",863.6,812.8,{"$f":"E130-2*K130","v":844.54},793.74,{"$f":"E130-2*M130","v":838.2},787.4,9.53,9.53,12.7,12.7,622.3,635.0,1270,503.9,630.5]
[null,null,null,"36\" x 36\" x 16\"",914.4,406.4,{"$f":"E131-2*K131","v":895.34},387.34,{"$f":"E131-2*M131","v":889},381,9.53,9.53,12.7,12.7,558.8,673.1,1346.2,460.4,580.6]
[null,null,null,"36\" x 36\" x 18\"",914.4,457.2,{"$f":"E132-2*K132","v":895.34},438.14,{"$f":"E132-2*M132","v":889},431.8,9.53,9.53,12.7,12.7,571.5,673.1,1346.2,473.6,596.5]
[null,null,null,"36\" x 36\" x 20\"",914.4,508.0,{"$f":"E133-2*K133","v":895.34},488.94,{"$f":"E133-2*M133","v":889},482.6,9.53,9.53,12.7,12.7,584.2,673.1,1346.2,486.3,610.1]
[null,null,null,"36\" x 36\" x 22\"",914.4,558.8,{"$f":"E134-2*K134","v":895.34},539.74,{"$f":"E134-2*M134","v":889},533.4,9.53,9.53,12.7,12.7,596.9,673.1,1346.2,499.0,626.0]
[null,null,null,"36\" x 36\" x 24\"",914.4,609.6,{"$f":"E135-2*K135","v":895.34},590.54,{"$f":"E135-2*M135","v":889},584.2,9.53,9.53,12.7,12.7,609.6,673.1,1346.2,512.1,641.8]
[null,null,null,"36\" x 36\" x 26\"",914.4,660.4,{"$f":"E136-2*K136","v":895.34},641.34,{"$f":"E136-2*M136","v":889},635,9.53,9.53,12.7,12.7,622.3,673.1,1346.2,525.3,653.2]
[null,null,null,"36\" x 36\" x 28\"",914.4,711.2,{"$f":"E137-2*K137","v":895.34},692.14,{"$f":"E137-2*M137","v":889},685.8,9.53,9.53,12.7,12.7,622.3,673.1,1346.2,535.7,669.0]
[null,null,null,"36\" x 36\" x 30\"",914.4,762.0,{"$f":"E138-2*K138","v":895.34},742.94,{"$f":"E138-2*M138","v":889},736.6,9.53,9.53,12.7,12.7,635.0,673.1,1346.2,547.5,684.9]
[null,null,null,"36\" x 36\" x 32\"",914.4,812.8,{"$f":"E139-2*K139","v":895.34},793.74,{"$f":"E139-2*M139","v":889},787.4,9.53,9.53,12.7,12.7,647.7,673.1,1346.2,561.1,698.5]
[null,null,null,"36\" x 36\" x 34\"",914.4,863.6,{"$f":"E140-2*K140","v":895.34},844.54,{"$f":"E140-2*M140","v":889},838.2,9.53,9.53,12.7,12.7,650.4,673.1,1346.2,573.3,714.4]
[null,null,null,"38\" x 38\" x 18\"",965.2,457.2,{"$f":"E141-2*K141","v":946.14},438.14,{"$f":"E141-2*M141","v":939.8},431.8,9.53,9.53,12.7,12.7,596.9,711.2,1422.4,"On request","On request"]
[null,null,null,"38\" x 38\" x 20\"",965.2,508.0,{"$f":"E142-2*K142","v":946.14},488.94,{"$f":"E142-2*M142","v":939.8},482.6,9.53,9.53,12.7,12.7,609.6,711.2,1422.4,"On request","On request"]
[null,null,null,"38\" x 38\" x 24\"",965.2,609.6,{"$f":"E143-2*K143","v":946.14},590.54,{"$f":"E143-2*M143","v":939.8},584.2,9.53,9.53,12.7,12.7,635.0,711.2,1422.4,"On request","On request"]
[null,null,null,"38\" x 38\" x 26\"",965.2,660.4,{"$f":"E144-2*K144","v":946.14},641.34,{"$f":"E144-2*M144","v":939.8},635,9.53,9.53,12.7,12.7,647.7,711.2,1422.4,"On request","On request"]
[null,null,null,"38\" x 38\" x 28\"",965.2,711.2,{"$f":"E145-2*K145","v":946.14},692.14,{"$f":"E145-2*M145","v":939.8},685.8,9.53,9.53,12.7,12.7,647.7,711.2,1422.4,"On request","On request"]
[null,null,null,"38\" x 38\" x 30\"",965.2,762.0,{"$f":"E146-2*K146","v":946.14},742.94,{"$f":"E146-2*M146","v":939.8},736.6,9.53,9.53,12.7,12.7,673.1,711.2,1422.4,"On request","On request"]
[null,null,null,"38\" x 38\" x 32\"",965.2,812.8,{"$f":"E147-2*K147","v":946.14},793.74,{"$f":"E147-2*M147","v":939.8},787.4,9.53,9.53,12.7,12.7,685.8,711.2,1422.4,"On request","On request"]
[null,null,null,"38\" x 38\" x 34\"",965.2,863.6,{"$f":"E148-2*K148","v":946.14},844.54,{"$f":"E148-2*M148","v":939.8},838.2,9.53,9.53,12.7,12.7,698.5,711.2,1422.4,"On request","On request"]
[null,null,null,"38\" x 38\" x 36\"",965.2,914.4,{"$f":"E149-2*K149","v":946.14},895.34,{"$f":"E149-2*M149","v":939.8},889,9.53,9.53,12.7,12.7,711.2,711.2,1422.4,"On request","On request"]
[null,null,null,"40\" x 40\" x 20\"",1016.0,508.0,{"$f":"E150-2*K150","v":996.94},488.94,{"$f":"E150-2*M150","v":990.6},482.6,9.53,9.53,12.7,12.7,635.0,749.3,1498.6,"On request","On request"]
[null,null,null,"40\" x 40\" x 22\"",1016.0,558.8,{"$f":"E151-2*K151","v":996.94},539.74,{"$f":"E151-2*M151","v":990.6},533.4,9.53,9.53,12.7,12.7,647.7,749.3,1498.6,"On request","On request"]
[null,null,null,"40\" x 40\" x 24\"",1016.0,609.6,{"$f":"E152-2*K152","v":996.94},590.54,{"$f":"E152-2*M152","v":990.6},584.2,9.53,9.53,12.7,12.7,660.4,749.3,1498.6,"On request","On request"]
[null,null,null,"40\" x 40\" x 26\"",1016.0,660.4,{"$f":"E153-2*K153","v":996.94},641.34,{"$f":"E153-2*M153","v":990.6},635,9.53,9.53,12.7,12.7,673.1,749.3,1498.6,"On request","On request"]
[null,null,null,"40\" x 40\" x 28\"",1016.0,711.2,{"$f":"E154-2*K154","v":996.94},692.14,{"$f":"E154-2*M154","v":990.6},685.8,9.53,9.53,12.7,12.7,673.1,749.3,1498.6,"On request","On request"]
[null,null,null,"40\" x 40\" x 30\"",1016.0,762.0,{"$f":"E155-2*K155","v":996.94},742.94,{"$f":"E155-2*M155","v":990.6},736.6,9.53,9.53,12.7,12.7,698.5,749.3,1498.6,"On request","On request"]
[null,null,null,"40\" x 40\" x 32\"",1016.0,812.8,{"$f":"E156-2*K156","v":996.94},793.74,{"$f":"E156-2*M156","v":990.6},787.4,9.53,9.53,12.7,12.7,711.2,749.3,1498.6,"On request","On request"]
[null,null,null,"40\" x 40\" x 34\"",1016.0,863.6,{"$f":"E157-2*K157","v":996.94},844.54,{"$f":"E157-2*M157","v":990.6},838.2,9.53,9.53,12.7,12.7,723.9,749.3,1498.6,"On request","On request"]
[null,null,null,"40\" x 40\" x 36\"",1016.0,914.4,{"$f":"E158-2*K158","v":996.94},895.34,{"$f":"E158-2*M158","v":990.6},889,9.53,9.53,12.7,12.7,736.6,749.3,1498.6,"On request","On request"]
[null,null,null,"40\" x 40\" x 38\"",1016.0,965.2,{"$f":"E159-2*K159","v":996.94},946.14,{"$f":"E159-2*M159","v":990.6},939.8,9.53,9.53,12.7,12.7,749.3,749.3,1498.6,"On request","On request"]
[null,null,null,"42\" x 42\" x 16\"",1066.8,406.4,{"$f":"E160-2*K160","v":1047.74},387.34,{"$f":"E160-2*M160","v":1041.4},381,9.53,9.53,12.7,12.7,635.0,762.0,1524,"On request","On request"]
[null,null,null,"42\" x 42\" x 18\"",1066.8,457.2,{"$f":"E161-2*K161","v":1047.74},438.14,{"$f":"E161-2*M161","v":1041.4},431.8,9.53,9.53,12.7,12.7,647.7,762.0,1524,"On request","On request"]
[null,null,null,"42\" x 42\" x 20\"",1066.8,508.0,{"$f":"E162-2*K162","v":1047.74},488.94,{"$f":"E162-2*M162","v":1041.4},482.6,9.53,9.53,12.7,12.7,660.4,762.0,1524,"On request","On request"]
[null,null,null,"42\" x 42\" x 22\"",1066.8,558.8,{"$f":"E163-2*K163","v":1047.74},539.74,{"$f":"E163-2*M163","v":1041.4},533.4,9.53,9.53,12.7,12.7,660.4,762.0,1524,"On request","On request"]
[null,null,null,"42\" x 42\" x 24\"",1066.8,609.6,{"$f":"E164-2*K164","v":1047.74},590.54,{"$f":"E164-2*M164","v":1041.4},584.2,9.53,9.53,12.7,12.7,660.4,762.0,1524,"On request","On request"]
[null,null,null,"42\" x 42\" x 26\"",1066.8,660.4,{"$f":"E165-2*K165","v":1047.74},641.34,{"$f":"E165-2*M165","v":1041.4},635,9.53,9.53,12.7,12.7,698.5,762.0,1524,"On request","On request"]
[null,null,null,"42\" x 42\" x 28\"",1066.8,711.2,{"$f":"E166-2*K166","v":1047.74},692.14,{"$f":"E166-2*M166","v":1041.4},685.8,9.53,9.53,12.7,12.7,698.5,762.0,1524,"On request","On request"]
[null,null,null,"42\" x 42\" x 30\"",1066.8,762.0,{"$f":"E167-2*K167","v":1047.74},742.94,{"$f":"E167-2*M167","v":1041.4},736.6,9.53,9.53,12.7,12.7,711.2,762.0,1524,"On request","On request"]
[null,null,null,"42\" x 42\" x 32\"",1066.8,812.8,{"$f":"E168-2*K168","v":1047.74},793.74,{"$f":"E168-2*M168","v":1041.4},787.4,9.53,9.53,12.7,12.7,711.2,762.0,1524,"On request","On request"]
[null,null,null,"42\" x 42\" x 34\"",1066.8,863.6,{"$f":"E169-2*K169","v":1047.74},844.54,{"$f":"E169-2*M169","v":1041.4},838.2,9.53,9.53,12.7,12.7,711.2,762.0,1524,"On request","On request"]
[null,null,null,"42\" x 42\" x 36\"",1066.8,914.4,{"$f":"E170-2*K170","v":1047.74},895.34,{"$f":"E170-2*M170","v":1041.4},889,9.53,9.53,12.7,12.7,711.2,762.0,1524,"On request","On request"]
[null,null,null,"44\" x 44\" x 24\"",1117.6,609.6,{"$f":"E171-2*K171","v":1098.54},590.54,{"$f":"E171-2*M171","v":1092.2},584.2,9.53,9.53,12.7,12.7,698.5,812.8,1625.6,"On request","On request"]
[null,null,null,"44\" x 44\" x 26\"",1117.6,660.4,{"$f":"E172-2*K172","v":1098.54},641.34,{"$f":"E172-2*M172","v":1092.2},635,9.53,9.53,12.7,12.7,698.5,812.8,1625.6,"On request","On request"]
[null,null,null,"44\" x 44\" x 28\"",1117.6,711.2,{"$f":"E173-2*K173","v":1098.54},692.14,{"$f":"E173-2*M173","v":1092.2},685.8,9.53,9.53,12.7,12.7,698.5,812.8,1625.6,"On request","On request"]
[null,null,null,"44\" x 44\" x 30\"",1117.6,762.0,{"$f":"E174-2*K174","v":1098.54},742.94,{"$f":"E174-2*M174","v":1092.2},736.6,9.53,9.53,12.7,12.7,711.2,812.8,1625.6,"On request","On request"]
[null,null,null,"44\" x 44\" x 32\"",1117.6,812.8,{"$f":"E175-2*K175","v":1098.54},793.74,{"$f":"E175-2*M175","v":1092.2},787.4,9.53,9.53,12.7,12.7,711.2,812.8,1625.6,"On request","On request"]
[null,null,null,"44\" x 44\" x 34\"",1117.6,863.6,{"$f":"E176-2*K176","v":1098.54},844.54,{"$f":"E176-2*M176","v":1092.2},838.2,9.53,9.53,12.7,12.7,723.9,812.8,1625.6,"On request","On request"]
[null,null,null,"44\" x 44\" x 36\"",1117.6,914.4,{"$f":"E177-2*K177","v":1098.54},895.34,{"$f":"E177-2*M177","v":1092.2},889,9.53,9.53,12.7,12.7,723.9,812.8,1625.6,"On request","On request"]
[null,null,null,"44\" x 44\" x 38\"",1117.6,965.2,{"$f":"E178-2*K178","v":1098.54},946.14,{"$f":"E178-2*M178","v":1092.2},939.8,9.53,9.53,12.7,12.7,736.6,812.8,1625.6,"On request","On request"]
[null,null,null,"44\" x 44\" x 40\"",1117.6,1016.0,{"$f":"E179-2*K179","v":1098.54},996.94,{"$f":"E179-2*M179","v":1092.2},990.6,9.53,9.53,12.7,12.7,749.3,812.8,1625.6,"On request","On request"]
[null,null,null,"44\" x 44\" x 42\"",1117.6,1066.8,{"$f":"E180-2*K180","v":1098.54},1047.74,{"$f":"E180-2*M180","v":1092.2},1041.4,9.53,9.53,12.7,12.7,762.0,812.8,1625.6,"On request","On request"]
[null,null,null,"46\" x 46\" x 24\"",1168.4,609.6,{"$f":"E181-2*K181","v":1149.34},590.54,{"$f":"E181-2*M181","v":1143},584.2,9.53,9.53,12.7,12.7,723.9,850.9,1701.8,"On request","On request"]
[null,null,null,"46\" x 46\" x 26\"",1168.4,660.4,{"$f":"E182-2*K182","v":1149.34},641.34,{"$f":"E182-2*M182","v":1143},635,9.53,9.53,12.7,12.7,736.6,850.9,1701.8,"On request","On request"]
[null,null,null,"46\" x 46\" x 28\"",1168.4,711.2,{"$f":"E183-2*K183","v":1149.34},692.14,{"$f":"E183-2*M183","v":1143},685.8,9.53,9.53,12.7,12.7,736.6,850.9,1701.8,"On request","On request"]
[null,null,null,"46\" x 46\" x 30\"",1168.4,762.0,{"$f":"E184-2*K184","v":1149.34},742.94,{"$f":"E184-2*M184","v":1143},736.6,9.53,9.53,12.7,12.7,736.6,850.9,1701.8,"On request","On request"]
[null,null,null,"46\" x 46\" x 32\"",1168.4,812.8,{"$f":"E185-2*K185","v":1149.34},793.74,{"$f":"E185-2*M185","v":1143},787.4,9.53,9.53,12.7,12.7,749.3,850.9,1701.8,"On request","On request"]
[null,null,null,"46\" x 46\" x 34\"",1168.4,863.6,{"$f":"E186-2*K186","v":1149.34},844.54,{"$f":"E186-2*M186","v":1143},838.2,9.53,9.53,12.7,12.7,749.3,850.9,1701.8,"On request","On request"]
[null,null,null,"46\" x 46\" x 36\"",1168.4,914.4,{"$f":"E187-2*K187","v":1149.34},895.34,{"$f":"E187-2*M187","v":1143},889,9.53,9.53,12.7,12.7,762.0,850.9,1701.8,"On request","On request"]
[null,null,null,"46\" x 46\" x 38\"",1168.4,965.2,{"$f":"E188-2*K188","v":1149.34},946.14,{"$f":"E188-2*M188","v":1143},939.8,9.53,9.53,12.7,12.7,762.0,850.9,1701.8,"On request","On request"]
[null,null,null,"46\" x 46\" x 40\"",1168.4,1016.0,{"$f":"E189-2*K189","v":1149.34},996.94,{"$f":"E189-2*M189","v":1143},990.6,9.53,9.53,12.7,12.7,714.7,850.9,1701.8,"On request","On request"]
[null,null,null,"46\" x 46\" x 42\"",1168.4,1066.8,{"$f":"E190-2*K190","v":1149.34},1047.74,{"$f":"E190-2*M190","v":1143},1041.4,9.53,9.53,12.7,12.7,787.4,850.9,1701.8,"On request","On request"]
[null,null,null,"46\" x 46\" x 44\"",1168.4,1117.6,{"$f":"E191-2*K191","v":1149.34},1098.54,{"$f":"E191-2*M191","v":1143},1092.2,9.53,9.53,12.7,12.7,800.1,850.9,1701.8,"On request","On request"]
[null,null,null,"48\" x 48\" x 24\"",1219.2,609.6,{"$f":"E192-2*K192","v":1200.14},590.54,{"$f":"E192-2*M192","v":1193.8},584.2,9.53,9.53,12.7,12.7,736.6,889.0,1778,"On request","On request"]
[null,null,null,"48\" x 48\" x 26\"",1219.2,660.4,{"$f":"E193-2*K193","v":1200.14},641.34,{"$f":"E193-2*M193","v":1193.8},635,9.53,9.53,12.7,12.7,762.0,889.0,1778,"On request","On request"]
[null,null,null,"48\" x 48\" x 28\"",1219.2,711.2,{"$f":"E194-2*K194","v":1200.14},692.14,{"$f":"E194-2*M194","v":1193.8},685.8,9.53,9.53,12.7,12.7,762.0,889.0,1778,"On request","On request"]
[null,null,null,"48\" x 48\" x 30\"",1219.2,762.0,{"$f":"E195-2*K195","v":1200.14},742.94,{"$f":"E195-2*M195","v":1193.8},736.6,9.53,9.53,12.7,12.7,762.0,889.0,1778,"On request","On request"]
[null,null,null,"48\" x 48\" x 32\"",1219.2,812.8,{"$f":"E196-2*K196","v":1200.14},793.74,{"$f":"E196-2*M196","v":1193.8},787.4,9.53,9.53,12.7,12.7,787.4,889.0,1778,"On request","On request"]
[null,null,null,"48\" x 48\" x 34\"",1219.2,863.6,{"$f":"E197-2*K197","v":1200.14},844.54,{"$f":"E197-2*M197","v":1193.8},838.2,9.53,9.53,12.7,12.7,787.4,889.0,1778,"On request","On request"]
[null,null,null,"48\" x 48\" x 36\"",1219.2,914.4,{"$f":"E198-2*K198","v":1200.14},895.34,{"$f":"E198-2*M198","v":1193.8},889,9.53,9.53,12.7,12.7,787.4,889.0,1778,"On request","On request"]
[null,null,null,"48\" x 48\" x 38\"",1219.2,965.2,{"$f":"E199-2*K199","v":1200.14},946.14,{"$f":"E199-2*M199","v":1193.8},939.8,9.53,9.53,12.7,12.7,812.8,889.0,1778,"On request","On request"]
[null,null,null,"48\" x 48\" x 40\"",1219.2,1016.0,{"$f":"E200-2*K200","v":1200.14},996.94,{"$f":"E200-2*M200","v":1193.8},990.6,9.53,9.53,12.7,12.7,812.8,889.0,1778,"On request","On request"]
[null,null,null,"48\" x 48\" x 42\"",1219.2,1066.8,{"$f":"E201-2*K201","v":1200.14},1047.74,{"$f":"E201-2*M201","v":1193.8},1041.4,9.53,9.53,12.7,12.7,812.8,889.0,1778,"On request","On request"]
[null,null,null,"48\" x 48\" x 44\"",1219.2,1117.6,{"$f":"E202-2*K202","v":1200.14},1098.54,{"$f":"E202-2*M202","v":1193.8},1092.2,9.53,9.53,12.7,12.7,838.2,889.0,1778,"On request","On request"]
[null,null,null,"48\" x 48\" x 46\"",1219.2,1168.4,{"$f":"E203-2*K203","v":1200.14},1149.34,{"$f":"E203-2*M203","v":1193.8},1143,9.53,9.53,12.7,12.7,838.2,889.0,1778,"On request","On request"]
[]
["Fitting data:",null,null,"Conc./Excentr.","D outside",null,"D inside std.",null,"D inside XS",null,"Red.","Exc.","Wallth.",null,null,null,"Reducer"]
["Conc. and Exc. Reducers",null,null,"Red. std.","D1","D2","d1","d2","d1","d2","Length  L","M","D1 Std.","D2 Std.","D1 XS","D2 XS","Weight std.","Weight XS"]
[null,1.0,1.0,"3/4\" x 3/8\"",26.67,17.15,{"$f":"E207-2*M207","v":20.93},12.53,{"$f":"E207-2*O207","v":18.85},10.75,38.1,{"$f":"E207/2-F207/2","v":4.76},2.87,2.31,3.91,3.2,0.09,0.11]
[null,null,null,"3/4\" x 1/2\"",26.67,21.34,{"$f":"E208-2*M208","v":20.93},15.8,{"$f":"E208-2*O208","v":18.85},13.88,38.1,2.665,2.87,2.77,3.91,3.73,0.11,0.12]
[null,null,null,"1\" x 3/8\"",33.4,17.15,{"$f":"E209-2*M209","v":26.64},12.53,{"$f":"E209-2*O209","v":24.3},10.75,50.8,8.125,3.38,2.31,4.55,3.2,0.14,0.15]
[null,null,null,"1\" x 1/2\"",33.4,21.34,{"$f":"E210-2*M210","v":26.64},15.8,{"$f":"E210-2*O210","v":24.3},13.88,50.8,6.03,3.38,2.77,4.55,3.73,0.15,0.16]
[null,null,null,"1\" x 3/4\"",33.4,26.67,{"$f":"E211-2*M211","v":26.64},20.93,{"$f":"E211-2*O211","v":24.3},18.85,50.8,3.365,3.38,2.87,4.55,3.91,0.17,0.17]
[null,null,null,"1¼\" x 1/2\"",42.16,21.34,{"$f":"E212-2*M212","v":35.04},15.8,{"$f":"E212-2*O212","v":32.46},13.88,50.8,10.41,3.56,2.77,4.85,3.73,0.19,0.22]
[null,null,null,"1¼\" x 3/4\"",42.16,26.67,{"$f":"E213-2*M213","v":35.04},20.93,{"$f":"E213-2*O213","v":32.46},18.85,50.8,7.745,3.56,2.87,4.85,3.91,0.2,0.23]
[null,null,null,"1¼\" x 1\"",42.16,33.4,{"$f":"E214-2*M214","v":35.04},26.64,{"$f":"E214-2*O214","v":32.46},24.3,50.8,4.38,3.56,3.38,4.85,4.55,0.21,0.24]
[null,null,null,"1½\" x 1/2\"",48.26,21.34,{"$f":"E215-2*M215","v":40.9},15.8,{"$f":"E215-2*O215","v":38.1},13.88,63.5,13.46,3.68,2.77,5.08,3.73,0.22,0.28]
[null,null,null,"1½\" x 3/4\"",48.26,26.67,{"$f":"E216-2*M216","v":40.9},20.93,{"$f":"E216-2*O216","v":38.1},18.85,63.5,10.795,3.68,2.87,5.08,3.91,0.23,0.28]
[null,null,null,"1½\" x 1\"",48.26,33.4,{"$f":"E217-2*M217","v":40.9},26.64,{"$f":"E217-2*O217","v":38.1},24.3,63.5,7.43,3.68,3.38,5.08,4.55,0.24,0.31]
[null,null,null,"1½\" x 1¼\"",48.26,42.16,{"$f":"E218-2*M218","v":40.9},35.04,{"$f":"E218-2*O218","v":38.1},32.46,76.2,3.05,3.68,3.56,5.08,4.85,0.26,0.33]
[null,null,null,"2\" x 3/4\"",60.33,48.26,{"$f":"E219-2*M219","v":52.51},42.52,{"$f":"E219-2*O219","v":49.25},40.44,76.2,6.035,3.91,2.87,5.54,3.91,0.33,0.45]
[null,null,null,"2\" x 1\"",60.33,33.4,{"$f":"E220-2*M220","v":52.51},26.64,{"$f":"E220-2*O220","v":49.25},24.3,76.2,13.465,3.91,3.38,5.54,4.55,0.37,0.46]
[null,null,null,"2\" x 1¼\"",60.33,42.16,{"$f":"E221-2*M221","v":52.51},35.04,{"$f":"E221-2*O221","v":49.25},32.46,76.2,9.085,3.91,3.56,5.54,4.85,0.39,0.53]
[null,null,null,"2\" x 1½\"",60.33,48.26,{"$f":"E222-2*M222","v":52.51},40.9,{"$f":"E222-2*O222","v":49.25},38.1,76.2,6.035,3.91,3.68,5.54,5.08,0.41,0.54]
[null,null,null,"2½\" x 1\"",73.03,33.4,{"$f":"E223-2*M223","v":62.71},26.64,{"$f":"E223-2*O223","v":59.01},24.3,88.9,19.815,5.16,3.38,7.01,4.55,0.59,0.78]
[null,null,null,"2½\" x 1¼\"",73.03,42.16,{"$f":"E224-2*M224","v":62.71},35.04,{"$f":"E224-2*O224","v":59.01},32.46,88.9,15.435,5.16,3.56,7.01,4.85,0.67,0.79]
[null,null,null,"2½\" x 1½\"",73.03,48.26,{"$f":"E225-2*M225","v":62.71},40.9,{"$f":"E225-2*O225","v":59.01},38.1,88.9,12.385,5.16,3.68,7.01,5.08,0.68,0.86]
[null,null,null,"2½\" x 2\"",73.03,60.33,{"$f":"E226-2*M226","v":62.71},52.51,{"$f":"E226-2*O226","v":59.01},49.25,88.9,6.35,5.16,3.91,7.01,5.54,0.73,0.94]
[null,null,null,"3\" x 1¼\"",88.9,42.16,{"$f":"E227-2*M227","v":77.92},35.04,{"$f":"E227-2*O227","v":73.66},32.46,88.9,23.37,5.49,3.56,7.62,4.85,0.77,1.04]
[null,null,null,"3\" x 1½\"",88.9,48.26,{"$f":"E228-2*M228","v":77.92},40.9,{"$f":"E228-2*O228","v":73.66},38.1,88.9,20.32,5.49,3.68,7.62,5.08,0.86,0.99]
[null,null,null,"3\" x 2\"",88.9,60.33,{"$f":"E229-2*M229","v":77.92},52.51,{"$f":"E229-2*O229","v":73.66},49.25,88.9,14.285,5.49,3.91,7.62,5.54,0.91,1.18]
[null,null,null,"3\" x 2½\"",88.9,73.03,{"$f":"E230-2*M230","v":77.92},62.71,{"$f":"E230-2*O230","v":73.66},59.01,88.9,7.935,5.49,5.16,7.62,7.01,0.86,1.29]
[null,null,null,"3½\" x 1¼\"",101.6,42.16,{"$f":"E231-2*M231","v":90.12},35.04,{"$f":"E231-2*O231","v":85.44},32.46,101.6,29.72,5.74,3.56,8.08,4.85,0.91,1.49]
[null,null,null,"3½\" x 1½\"",101.6,48.26,{"$f":"E232-2*M232","v":90.12},40.9,{"$f":"E232-2*O232","v":85.44},38.1,101.6,26.67,5.74,3.68,8.08,5.08,0.98,1.43]
[null,null,null,"3½\" x 2\"",101.6,60.33,{"$f":"E233-2*M233","v":90.12},52.51,{"$f":"E233-2*O233","v":85.44},49.25,101.6,20.635,5.74,3.91,8.08,5.54,1.07,1.61]
[null,null,null,"3½\" x 2½\"",101.6,73.03,{"$f":"E234-2*M234","v":90.12},62.71,{"$f":"E234-2*O234","v":85.44},59.01,101.6,14.285,5.74,5.16,8.08,7.01,1.14,1.75]
[null,null,null,"3½\" x 3\"",101.6,88.9,{"$f":"E235-2*M235","v":90.12},77.92,{"$f":"E235-2*O235","v":85.44},73.66,101.6,6.35,5.74,5.49,8.08,7.62,1.23,1.85]
[null,null,null,"4\" x 1½\"",114.3,48.26,{"$f":"E236-2*M236","v":102.26},40.9,{"$f":"E236-2*O236","v":97.18},38.1,101.6,33.02,6.02,3.68,8.56,5.08,1.24,1.73]
[null,null,null,"4\" x 2\"",114.3,60.33,{"$f":"E237-2*M237","v":102.26},52.51,{"$f":"E237-2*O237","v":97.18},49.25,101.6,26.985,6.02,3.91,8.56,5.54,1.44,1.78]
[null,null,null,"4\" x 2½\"",114.3,73.03,{"$f":"E238-2*M238","v":102.26},62.71,{"$f":"E238-2*O238","v":97.18},59.01,101.6,20.635,6.02,5.16,8.56,7.01,1.52,2.01]
[null,null,null,"4\" x 3\"",114.3,88.9,{"$f":"E239-2*M239","v":102.26},77.92,{"$f":"E239-2*O239","v":97.18},73.66,101.6,12.7,6.02,5.49,8.56,7.62,1.59,2.13]
[null,null,null,"4\" x 3½\"",114.3,101.6,{"$f":"E240-2*M240","v":102.26},90.12,{"$f":"E240-2*O240","v":97.18},85.44,101.6,6.35,6.02,5.74,8.56,8.08,1.64,2.21]
[null,null,null,"5\" x 2\"",141.3,60.33,{"$f":"E241-2*M241","v":128.2},52.51,{"$f":"E241-2*O241","v":122.24},49.25,127.0,40.485,6.55,3.91,9.53,5.54,2.29,3.0]
[null,null,null,"5\" x 2½\"",141.3,73.03,{"$f":"E242-2*M242","v":128.2},62.71,{"$f":"E242-2*O242","v":122.24},59.01,127.0,34.135,6.55,5.16,9.53,7.01,2.51,3.3]
[null,null,null,"5\" x 3\"",141.3,88.9,{"$f":"E243-2*M243","v":128.2},77.92,{"$f":"E243-2*O243","v":122.24},73.66,127.0,26.2,6.55,5.49,9.53,7.62,2.6,3.56]
[null,null,null,"5\" x 3½\"",141.3,101.6,{"$f":"E244-2*M244","v":128.2},90.12,{"$f":"E244-2*O244","v":122.24},85.44,127.0,19.85,6.55,5.74,9.53,8.08,2.66,3.65]
[null,null,null,"5\" x 4\"",141.3,114.3,{"$f":"E245-2*M245","v":128.2},106.48,{"$f":"E245-2*O245","v":122.24},97.18,127.0,13.5,6.55,3.91,9.53,8.56,2.72,3.78]
[null,null,null,"6\" x 2½\"",168.28,73.03,{"$f":"E246-2*M246","v":154.06},62.71,{"$f":"E246-2*O246","v":146.34},59.01,139.7,47.625,7.11,5.16,10.97,7.01,3.45,4.52]
[null,null,null,"6\" x 3\"",168.28,88.9,{"$f":"E247-2*M247","v":154.06},77.92,{"$f":"E247-2*O247","v":146.34},73.66,139.7,39.69,7.11,5.49,10.97,7.62,3.63,5.04]
[null,null,null,"6\" x 3½\"",168.28,101.6,{"$f":"E248-2*M248","v":154.06},90.12,{"$f":"E248-2*O248","v":146.34},85.44,139.7,33.34,7.11,5.74,10.97,8.08,3.69,5.27]
[null,null,null,"6\" x 4\"",168.28,114.3,{"$f":"E249-2*M249","v":154.06},102.26,{"$f":"E249-2*O249","v":146.34},97.18,139.7,26.99,7.11,6.02,10.97,8.56,3.72,5.45]
[null,null,null,"6\" x 5\"",168.28,141.3,{"$f":"E250-2*M250","v":154.06},128.2,{"$f":"E250-2*O250","v":146.34},122.24,139.7,13.49,7.11,6.55,10.97,9.53,3.93,5.73]
[null,null,null,"8\" x 3½\"",219.08,101.6,{"$f":"E251-2*M251","v":202.72},90.12,{"$f":"E251-2*O251","v":193.68},85.44,152.4,58.74,8.18,5.74,12.7,8.08,5.81,7.31]
[null,null,null,"8\" x 4\"",219.08,114.3,{"$f":"E252-2*M252","v":202.72},102.26,{"$f":"E252-2*O252","v":193.68},97.18,152.4,52.39,8.18,6.02,12.7,8.56,5.95,8.44]
[null,null,null,"8\" x 5\"",219.08,141.3,{"$f":"E253-2*M253","v":202.72},128.2,{"$f":"E253-2*O253","v":193.68},122.24,152.4,38.89,8.18,6.55,12.7,9.53,6.08,8.85]
[null,null,null,"8\" x 6\"",219.08,168.28,{"$f":"E254-2*M254","v":202.72},154.06,{"$f":"E254-2*O254","v":193.68},146.34,152.4,25.4,8.18,7.11,12.7,10.97,6.31,9.26]
[null,null,null,"10\" x 4\"",273.05,114.3,{"$f":"E255-2*M255","v":254.51},102.26,{"$f":"E255-2*O255","v":247.65},97.18,177.8,79.375,9.27,6.02,12.7,8.56,9.58,11.5]
[null,null,null,"10\" x 5\"",273.05,141.3,{"$f":"E256-2*M256","v":254.51},128.2,{"$f":"E256-2*O256","v":247.65},122.24,177.8,65.875,9.27,6.55,12.7,9.53,9.9,13.0]
[null,null,null,"10\" x 6\"",273.05,168.28,{"$f":"E257-2*M257","v":254.51},154.06,{"$f":"E257-2*O257","v":247.65},146.34,177.8,52.385,9.27,7.11,12.7,10.97,10.1,13.5]
[null,null,null,"10\" x 8\"",273.05,219.08,{"$f":"E258-2*M258","v":254.51},202.72,{"$f":"E258-2*O258","v":247.65},193.68,177.8,26.985,9.27,8.18,12.7,12.7,10.5,14.2]
[null,null,null,"12\" x 5\"",323.85,141.3,{"$f":"E259-2*M259","v":304.79},128.2,{"$f":"E259-2*O259","v":298.45},122.24,203.2,91.275,9.53,6.55,12.7,9.53,13.8,17.7]
[null,null,null,"12\" x 6\"",323.85,168.28,{"$f":"E260-2*M260","v":304.79},154.06,{"$f":"E260-2*O260","v":298.45},146.34,203.2,77.785,9.53,7.11,12.7,10.97,14.1,18.4]
[null,null,null,"12\" x 8\"",323.85,219.08,{"$f":"E261-2*M261","v":304.79},202.72,{"$f":"E261-2*O261","v":298.45},193.68,203.2,52.385,9.53,8.18,12.7,12.7,14.6,17.0]
[null,null,null,"12\" x 10\"",323.85,273.05,{"$f":"E262-2*M262","v":304.79},254.51,{"$f":"E262-2*O262","v":298.45},247.65,203.2,25.4,9.53,9.27,12.7,12.7,15.2,19.8]
[null,null,null,"14\" x 6\"",355.6,168.28,{"$f":"E263-2*M263","v":336.54},154.06,{"$f":"E263-2*O263","v":330.2},146.34,330.2,93.66,9.53,7.11,12.7,10.97,26.0,33.7]
[null,null,null,"14\" x 8\"",355.6,219.08,{"$f":"E264-2*M264","v":336.54},202.72,{"$f":"E264-2*O264","v":330.2},193.68,330.2,68.26,9.53,8.18,12.7,12.7,27.4,34.9]
[null,null,null,"14\" x 10\"",355.6,273.05,{"$f":"E265-2*M265","v":336.54},254.51,{"$f":"E265-2*O265","v":330.2},247.65,330.2,41.275,9.53,9.27,12.7,12.7,28.8,36.1]
[null,null,null,"14\" x 12\"",355.6,323.85,{"$f":"E266-2*M266","v":336.54},304.79,{"$f":"E266-2*O266","v":330.2},298.45,330.2,15.875,9.53,9.53,12.7,12.7,31.9,37.7]
[null,null,null,"16\" x 8\"",406.4,219.08,{"$f":"E267-2*M267","v":387.34},202.72,{"$f":"E267-2*O267","v":381},193.68,355.6,93.66,9.53,8.18,12.7,12.7,33.1,42.6]
[null,null,null,"16\" x 10\"",406.4,273.05,{"$f":"E268-2*M268","v":387.34},254.51,{"$f":"E268-2*O268","v":381},247.65,355.6,66.675,9.53,9.27,12.7,12.7,33.11,43.7]
[null,null,null,"16\" x 12\"",406.4,323.85,{"$f":"E269-2*M269","v":387.34},304.79,{"$f":"E269-2*O269","v":381},298.45,355.6,41.275,9.53,9.53,12.7,12.7,34.3,45.0]
[null,null,null,"16\" x 14\"",406.4,355.6,{"$f":"E270-2*M270","v":387.34},336.54,{"$f":"E270-2*O270","v":381},330.2,355.6,25.4,9.53,9.53,12.7,12.7,36.2,46.3]
[null,null,null,"18\" x 10\"",457.2,273.05,{"$f":"E271-2*M271","v":438.14},254.51,{"$f":"E271-2*O271","v":431.8},247.65,381.0,92.075,9.53,9.27,12.7,12.7,39.4,51.8]
[null,null,null,"18\" x 12\"",457.2,323.85,{"$f":"E272-2*M272","v":438.14},304.79,{"$f":"E272-2*O272","v":431.8},298.45,381.0,66.675,9.53,9.53,12.7,12.7,40.5,53.6]
[null,null,null,"18\" x 14\"",457.2,355.6,{"$f":"E273-2*M273","v":438.14},336.54,{"$f":"E273-2*O273","v":431.8},330.2,381.0,50.8,9.53,9.53,12.7,12.7,41.3,54.5]
[null,null,null,"18\" x 16\"",457.2,406.4,{"$f":"E274-2*M274","v":438.14},387.34,{"$f":"E274-2*O274","v":431.8},381,381.0,25.4,9.53,9.53,12.7,12.7,42.7,55.8]
[null,null,null,"20\" x 12\"",508.0,323.85,{"$f":"E275-2*M275","v":488.94},304.79,{"$f":"E275-2*O275","v":482.6},298.45,508.0,92.075,9.53,9.53,12.7,12.7,60.8,79.9]
[null,null,null,"20\" x 14\"",508.0,355.6,{"$f":"E276-2*M276","v":488.94},336.54,{"$f":"E276-2*O276","v":482.6},330.2,508.0,76.2,9.53,9.53,12.7,12.7,61.3,81.3]
[null,null,null,"20\" x 16\"",508.0,406.4,{"$f":"E277-2*M277","v":488.94},387.34,{"$f":"E277-2*O277","v":482.6},381,508.0,50.8,9.53,9.53,12.7,12.7,62.6,82.6]
[null,null,null,"20\" x 18\"",508.0,457.2,{"$f":"E278-2*M278","v":488.94},438.14,{"$f":"E278-2*O278","v":482.6},431.8,508.0,25.4,9.53,9.53,12.7,12.7,64.5,84.4]
[null,null,null,"22\" x 14\"",558.8,355.6,{"$f":"E279-2*M279","v":539.74},336.54,{"$f":"E279-2*O279","v":533.4},330.2,508.0,101.6,9.53,9.53,12.7,12.7,67.2,88.5]
[null,null,null,"22\" x 16\"",558.8,406.4,{"$f":"E280-2*M280","v":539.74},387.34,{"$f":"E280-2*O280","v":533.4},381,508.0,76.2,9.53,9.53,12.7,12.7,68.5,89.9]
[null,null,null,"22\" x 18\"",558.8,457.2,{"$f":"E281-2*M281","v":539.74},438.14,{"$f":"E281-2*O281","v":533.4},431.8,508.0,50.8,9.53,9.53,12.7,12.7,69.9,91.7]
[null,null,null,"22\" x 20\"",558.8,508.0,{"$f":"E282-2*M282","v":539.74},488.94,{"$f":"E282-2*O282","v":533.4},482.6,508.0,25.4,9.53,9.53,12.7,12.7,71.3,94.0]
[null,null,null,"24\" x 16\"",609.6,406.4,{"$f":"E283-2*M283","v":590.54},387.34,{"$f":"E283-2*O283","v":584.2},381,508.0,101.6,9.53,9.53,12.7,12.7,72.6,95.8]
[null,null,null,"24\" x 18\"",609.6,457.2,{"$f":"E284-2*M284","v":590.54},438.14,{"$f":"E284-2*O284","v":584.2},431.8,508.0,76.2,9.53,9.53,12.7,12.7,74.0,97.6]
[null,null,null,"24\" x 20\"",609.6,508.0,{"$f":"E285-2*M285","v":590.54},488.94,{"$f":"E285-2*O285","v":584.2},482.6,508.0,50.8,9.53,9.53,12.7,12.7,75.8,99.9]
[null,null,null,"26\" x 18\"",660.4,457.2,{"$f":"E286-2*M286","v":641.34},438.14,{"$f":"E286-2*O286","v":635},431.8,609.6,101.6,9.53,9.53,12.7,12.7,90.7,123.0]
[null,null,null,"26\" x 20\"",660.4,508.0,{"$f":"E287-2*M287","v":641.34},488.94,{"$f":"E287-2*O287","v":635},482.6,609.6,76.2,9.53,9.53,12.7,12.7,90.7,123.0]
[null,null,null,"26\" x 22\"",660.4,558.8,{"$f":"E288-2*M288","v":641.34},539.74,{"$f":"E288-2*O288","v":635},533.4,609.6,50.8,9.53,9.53,12.7,12.7,90.7,123.0]
[null,null,null,"26\" x 24\"",660.4,609.6,{"$f":"E289-2*M289","v":641.34},590.54,{"$f":"E289-2*O289","v":635},584.2,609.6,25.4,9.53,9.53,12.7,12.7,90.7,123.0]
[null,null,null,"28\" x 18\"",711.2,457.2,{"$f":"E290-2*M290","v":692.14},438.14,{"$f":"E290-2*O290","v":685.8},431.8,609.6,127,9.53,9.53,12.7,12.7,95.3,132.0]
[null,null,null,"28\" x 20\"",711.2,508.0,{"$f":"E291-2*M291","v":692.14},488.94,{"$f":"E291-2*O291","v":685.8},482.6,609.6,101.6,9.53,9.53,12.7,12.7,95.3,132.0]
[null,null,null,"28\" x 24\"",711.2,609.6,{"$f":"E292-2*M292","v":692.14},590.54,{"$f":"E292-2*O292","v":685.8},584.2,609.6,50.8,9.53,9.53,12.7,12.7,95.3,132.0]
[null,null,null,"28\" x 26\"",711.2,660.4,{"$f":"E293-2*M293","v":692.14},641.34,{"$f":"E293-2*O293","v":685.8},635,609.6,25.4,9.53,9.53,12.7,12.7,95.3,132.0]
[null,null,null,"30\" x 20\"",762.0,508.0,{"$f":"E294-2*M294","v":742.94},488.94,{"$f":"E294-2*O294","v":736.6},482.6,609.6,127,9.53,9.53,12.7,12.7,100.0,143.0]
[null,null,null,"30\" x 24\"",762.0,609.6,{"$f":"E295-2*M295","v":742.94},590.54,{"$f":"E295-2*O295","v":736.6},584.2,609.6,76.2,9.53,9.53,12.7,12.7,100.0,143.0]
[null,null,null,"30\" x 26\"",762.0,660.4,{"$f":"E296-2*M296","v":742.94},641.34,{"$f":"E296-2*O296","v":736.6},635,609.6,50.8,9.53,9.53,12.7,12.7,100.0,143.0]
[null,null,null,"30\" x 28\"",762.0,711.2,{"$f":"E297-2*M297","v":742.94},692.14,{"$f":"E297-2*O297","v":736.6},685.8,609.6,25.4,9.53,9.53,12.7,12.7,100.0,143.0]
[null,null,null,"32\" x 24\"",812.8,609.6,{"$f":"E298-2*M298","v":793.74},590.54,{"$f":"E298-2*O298","v":787.4},584.2,609.6,101.6,9.53,9.53,12.7,12.7,115.0,150.0]
[null,null,null,"32\" x 26\"",812.8,660.4,{"$f":"E299-2*M299","v":793.74},641.34,{"$f":"E299-2*O299","v":787.4},635,609.6,76.2,9.53,9.53,12.7,12.7,115.0,150.0]
[null,null,null,"32\" x 28\"",812.8,711.2,{"$f":"E300-2*M300","v":793.74},692.14,{"$f":"E300-2*O300","v":787.4},685.8,609.6,50.8,9.53,9.53,12.7,12.7,115.0,150.0]
[null,null,null,"32\" x 30\"",812.8,762.0,{"$f":"E301-2*M301","v":793.74},742.94,{"$f":"E301-2*O301","v":787.4},736.6,609.6,25.4,9.53,9.53,12.7,12.7,115.0,150.0]
[null,null,null,"34\" x 24\"",863.6,609.6,{"$f":"E302-2*M302","v":844.54},590.54,{"$f":"E302-2*O302","v":838.2},584.2,609.6,127,9.53,9.53,12.7,12.7,115.0,157.0]
[null,null,null,"34\" x 26\"",863.6,660.4,{"$f":"E303-2*M303","v":844.54},641.34,{"$f":"E303-2*O303","v":838.2},635,609.6,101.6,9.53,9.53,12.7,12.7,112.0,157.0]
[null,null,null,"34\" x 28\"",863.6,711.2,{"$f":"E304-2*M304","v":844.54},692.14,{"$f":"E304-2*O304","v":838.2},685.8,609.6,76.2,9.53,9.53,12.7,12.7,112.0,157.0]
[null,null,null,"34\" x 30\"",863.6,762.0,{"$f":"E305-2*M305","v":844.54},742.94,{"$f":"E305-2*O305","v":838.2},736.6,609.6,50.8,9.53,9.53,12.7,12.7,112.0,157.0]
[null,null,null,"34\" x 32\"",863.6,812.8,{"$f":"E306-2*M306","v":844.54},793.74,{"$f":"E306-2*O306","v":838.2},787.4,609.6,25.4,9.53,9.53,12.7,12.7,112.0,157.0]
[null,null,null,"36\" x 24\"",914.4,609.6,{"$f":"E307-2*M307","v":895.34},590.54,{"$f":"E307-2*O307","v":889},584.2,609.6,152.4,9.53,9.53,12.7,12.7,129.0,172.0]
[null,null,null,"36\" x 26\"",914.4,660.4,{"$f":"E308-2*M308","v":895.34},641.34,{"$f":"E308-2*O308","v":889},635,609.6,127,9.53,9.53,12.7,12.7,129.0,172.0]
[null,null,null,"36\" x 30\"",914.4,762.0,{"$f":"E309-2*M309","v":895.34},742.94,{"$f":"E309-2*O309","v":889},736.6,609.6,76.2,9.53,9.53,12.7,12.7,129.0,172.0]
[null,null,null,"36\" x 32\"",914.4,812.8,{"$f":"E310-2*M310","v":895.34},793.74,{"$f":"E310-2*O310","v":889},787.4,609.6,50.8,9.53,9.53,12.7,12.7,129.0,172.0]
[null,null,null,"36\" x 34\"",914.4,863.6,{"$f":"E311-2*M311","v":895.34},844.54,{"$f":"E311-2*O311","v":889},838.2,609.6,25.4,9.53,9.53,12.7,12.7,129.0,172.0]
[null,null,null,"38\" x 26\"",965.2,660.4,{"$f":"E312-2*M312","v":946.14},641.34,{"$f":"E312-2*O312","v":939.8},635,609.6,152.4,9.53,9.53,12.7,12.7,136.0,186.0]
[null,null,null,"38\" x 28\"",965.2,711.2,{"$f":"E313-2*M313","v":946.14},692.14,{"$f":"E313-2*O313","v":939.8},685.8,609.6,127,9.53,9.53,12.7,12.7,136.0,186.0]
[null,null,null,"38\" x 30\"",965.2,762.0,{"$f":"E314-2*M314","v":946.14},742.94,{"$f":"E314-2*O314","v":939.8},736.6,609.6,101.6,9.53,9.53,12.7,12.7,136.0,186.0]
[null,null,null,"38\" x 32\"",965.2,812.8,{"$f":"E315-2*M315","v":946.14},793.74,{"$f":"E315-2*O315","v":939.8},787.4,609.6,76.2,9.53,9.53,12.7,12.7,136.0,186.0]
[null,null,null,"38\" x 34\"",965.2,863.6,{"$f":"E316-2*M316","v":946.14},844.54,{"$f":"E316-2*O316","v":939.8},838.2,609.6,50.8,9.53,9.53,12.7,12.7,136.0,186.0]
[null,null,null,"38\" x 36\"",965.2,914.4,{"$f":"E317-2*M317","v":946.14},895.34,{"$f":"E317-2*O317","v":939.8},889,609.6,25.4,9.53,9.53,12.7,12.7,136.0,186.0]
[null,null,null,"40\" x 30\"",1016.0,762.0,{"$f":"E318-2*M318","v":996.94},742.94,{"$f":"E318-2*O318","v":990.6},736.6,609.6,127,9.53,9.53,12.7,12.7,143.0,193.0]
[null,null,null,"40\" x 32\"",1016.0,812.8,{"$f":"E319-2*M319","v":996.94},793.74,{"$f":"E319-2*O319","v":990.6},787.4,609.6,101.6,9.53,9.53,12.7,12.7,143.0,193.0]
[null,null,null,"40\" x 34\"",1016.0,863.6,{"$f":"E320-2*M320","v":996.94},844.54,{"$f":"E320-2*O320","v":990.6},838.2,609.6,76.2,9.53,9.53,12.7,12.7,143.0,193.0]
[null,null,null,"40\" x 36\"",1016.0,914.4,{"$f":"E321-2*M321","v":996.94},895.34,{"$f":"E321-2*O321","v":990.6},889,609.6,50.8,9.53,9.53,12.7,12.7,143.0,193.0]
[null,null,null,"40\" x 38\"",1016.0,965.2,{"$f":"E322-2*M322","v":996.94},946.14,{"$f":"E322-2*O322","v":990.6},939.8,609.6,25.4,9.53,9.53,12.7,12.7,143.0,193.0]
[null,null,null,"42\" x 30\"",1066.8,762.0,{"$f":"E323-2*M323","v":1047.74},742.94,{"$f":"E323-2*O323","v":1041.4},736.6,609.6,152.4,9.53,9.53,12.7,12.7,152.0,201.0]
[null,null,null,"42\" x 32\"",1066.8,812.8,{"$f":"E324-2*M324","v":1047.74},793.74,{"$f":"E324-2*O324","v":1041.4},787.4,609.6,127,9.53,9.53,12.7,12.7,152.0,201.0]
[null,null,null,"42\" x 34\"",1066.8,863.6,{"$f":"E325-2*M325","v":1047.74},844.54,{"$f":"E325-2*O325","v":1041.4},838.2,609.6,101.6,9.53,9.53,12.7,12.7,152.0,201.0]
[null,null,null,"42\" x 36\"",1066.8,914.4,{"$f":"E326-2*M326","v":1047.74},895.34,{"$f":"E326-2*O326","v":1041.4},889,609.6,76.2,9.53,9.53,12.7,12.7,152.0,201.0]
[null,null,null,"42\" x 38\"",1066.8,965.2,{"$f":"E327-2*M327","v":1047.74},946.14,{"$f":"E327-2*O327","v":1041.4},939.8,609.6,50.8,9.53,9.53,12.7,12.7,152.0,201.0]
[null,null,null,"42\" x 40\"",1066.8,1016.0,{"$f":"E328-2*M328","v":1047.74},996.94,{"$f":"E328-2*O328","v":1041.4},990.6,609.6,25.4,9.53,9.53,12.7,12.7,152.0,201.0]
[null,null,null,"44\" x 36\"",1117.6,914.4,{"$f":"E329-2*M329","v":1098.54},895.34,{"$f":"E329-2*O329","v":1092.2},889,609.6,101.6,9.53,9.53,12.7,12.7,159.0,211.0]
[null,null,null,"44\" x 38\"",1117.6,965.2,{"$f":"E330-2*M330","v":1098.54},946.14,{"$f":"E330-2*O330","v":1092.2},939.8,609.6,76.2,9.53,9.53,12.7,12.7,159.0,211.0]
[null,null,null,"44\" x 40\"",1117.6,1016.0,{"$f":"E331-2*M331","v":1098.54},996.94,{"$f":"E331-2*O331","v":1092.2},990.6,609.6,50.8,9.53,9.53,12.7,12.7,159.0,211.0]
[null,null,null,"44\" x 42\"",1117.6,1066.8,{"$f":"E332-2*M332","v":1098.54},1047.74,{"$f":"E332-2*O332","v":1092.2},1041.4,609.6,25.4,9.53,9.53,12.7,12.7,159.0,211.0]
[null,null,null,"46\" x 38\"",1168.4,965.2,{"$f":"E333-2*M333","v":1149.34},946.14,{"$f":"E333-2*O333","v":1143},939.8,711.2,101.6,9.53,9.53,12.7,12.7,170.0,225.0]
[null,null,null,"46\" x 40\"",1168.4,1016.0,{"$f":"E334-2*M334","v":1149.34},996.94,{"$f":"E334-2*O334","v":1143},990.6,711.2,76.2,9.53,9.53,12.7,12.7,170.0,225.0]
[null,null,null,"46\" x 42\"",1168.4,1066.8,{"$f":"E335-2*M335","v":1149.34},1047.74,{"$f":"E335-2*O335","v":1143},1041.4,711.2,50.8,9.53,9.53,12.7,12.7,170.0,225.0]
[null,null,null,"46\" x 44\"",1168.4,1117.6,{"$f":"E336-2*M336","v":1149.34},1098.54,{"$f":"E336-2*O336","v":1143},1092.2,711.2,25.4,9.53,9.53,12.7,12.7,170.0,225.0]
[null,null,null,"48\" x 40\"",1219.2,1016.0,{"$f":"E337-2*M337","v":1200.14},996.94,{"$f":"E337-2*O337","v":1193.8},990.6,711.2,101.6,9.53,9.53,12.7,12.7,181.0,238.0]
[null,null,null,"48\" x 42\"",1219.2,1066.8,{"$f":"E338-2*M338","v":1200.14},1047.74,{"$f":"E338-2*O338","v":1193.8},1041.4,711.2,76.2,9.53,9.53,12.7,12.7,181.0,238.0]
[null,null,null,"48\" x 44\"",1219.2,1117.6,{"$f":"E339-2*M339","v":1200.14},1098.54,{"$f":"E339-2*O339","v":1193.8},1092.2,711.2,50.8,9.53,9.53,12.7,12.7,181.0,238.0]
[null,null,null,"48\" x 46\"",1219.2,1168.4,{"$f":"E340-2*M340","v":1200.14},1149.34,{"$f":"E340-2*O340","v":1193.8},1143,711.2,25.4,9.53,9.53,12.7,12.7,181.0,238.0]

{"sheet":"Swage nipples","index":18,"n_rows":63,"n_cols":6,"rows_kept":63,"cut":false,"hidden":true,"merged":[[0,0,0,7],[30,1,30,2],[30,4,31,6]]}
["DIMENSIONS of SWAGE NIPPLES"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Swage nipples acc. Ansi B 16.5",null,null,null,"Size:"]
["Diameter outside runsize","D1",{"$f":"INDEX('Data swage nipples'!$C$3:$C$39,'Data swage nipples'!$A$3)","v":17.15},"mm"]
["Diameter outside red.size","D2",{"$f":"INDEX('Data swage nipples'!$D$3:$D$39,'Data swage nipples'!$A$3)","v":13.72},"mm"]
["Nipple length","A",{"$f":"INDEX('Data swage nipples'!$E$3:$E$39,'Data swage nipples'!$A$3)","v":64},"mm"]
["Red. neck length","F",{"$f":"INDEX('Data swage nipples'!$F$3:$F$39,'Data swage nipples'!$A$3)","v":16},"mm"]
["Threaded length runsize","H1",{"$f":"INDEX('Data swage nipples'!$G$3:$G$39,'Data swage nipples'!$A$3)","v":10},"mm"]
["Threaded length red.size","H2",{"$f":"INDEX('Data swage nipples'!$H$3:$H$39,'Data swage nipples'!$A$3)","v":8},"mm"]
["Centre to centre","E",{"$f":"INDEX('Data swage nipples'!$I$3:$I$39,'Data swage nipples'!$A$3)","v":1.715},"mm"]
["Weight sch. 40","G",{"$f":"INDEX('Data swage nipples'!$J$3:$J$39,'Data swage nipples'!$A$3)","v":0.08},"kg"]
["Weight sch. 80","G",{"$f":"INDEX('Data swage nipples'!$K$3:$K$39,'Data swage nipples'!$A$3)","v":0.08},"kg"]
["Weight sch. 160","G",{"$f":"INDEX('Data swage nipples'!$L$3:$L$39,'Data swage nipples'!$A$3)","v":0.11},"kg"]
["Weight sch. XXS","G",{"$f":"INDEX('Data swage nipples'!$M$3:$M$39,'Data swage nipples'!$A$3)","v":0.13},"kg"]
[]
[]
[null,null,null,null,"Abbriviations:"]
[]
[null,null,null,null,"BEB","Both Ends Bevelled"]
[null,null,null,null,"BEG","Both Ends Grooved"]
[null,null,null,null,"BEP","Both Ends Plain"]
[null,null,null,null,"BET","Both Ends Threaded"]
[null,null,null,null,"BLE/GSE","Bevelled Large End - Grooved Small End"]
[null,null,null,null,"BLE/PSE","Bevelled Large End - Plain Small End"]
[null,null,null,null,"BLE/TSE","Bevelled Large End - Threaded Small End"]
[null,null,null,null,"BOE","Bevelled One End"]
[null,null,null,null,"GBE","Grooved Both Ends"]
[null,null,null,null,"GOE","Grooved One End"]
[null,null,null,null,"LEBG","Large End Bevelled - small end Bevelled"]
[null,null,null,null,"LEBP","Large End Bevelled - small end Plain"]
[null,null,null,null,"LEBT","Large End Bevelled - small end Threaded"]
[null,null,null,null,"LEGB","Large End Grooved - small end Bevelled"]
[null,null,null,null,"LEGP","Large End Grooved - small end Plain"]
[null,null,null,null,"LEGT","Large End Grooved - small end Threaded"]
[null,null,null,null,"LEPB","Large End Plain - small end Bevelled"]
[null,null,null,null,"LEPG","Large End Plain - small end Grooved"]
[null,null,null,null,"LEPT","Large End Plain - small end Threaded"]
[null,null,null,null,"LETB","Large End Threaded - small end Bevelled"]
[null,null,null,null,"LETP","Large End Threaded - small end Plain"]
[null,null,null,null,"PBE","Plain Both Ends"]
[null,null,null,null,"PLE/BSE","Plain Large End - Bevelled Small End"]
[null,null,null,null,"PLE/GSE","Plain Large End - Grooved Small End"]
[null,null,null,null,"PLE/TSE","Plain Large End - Threaded Small End"]
[null,null,null,null,"POE","Plain One End"]
[null,null,null,null,"TBE","Threaded Both Ends"]
[null,null,null,null,"TLE/BSE","Threaded Large End - Bevelled Small End"]
[null,null,null,null,"TLE/GSE","Threaded Large End - Grooved Small End"]
[null,null,null,null,"TLE/PSE","Threaded Large End - Plain Small End"]
[null,null,null,null,"TOE","Threaded One End"]

{"sheet":"Data swage nipples","index":19,"n_rows":39,"n_cols":13,"rows_kept":39,"cut":false,"hidden":true,"merged":[[0,2,0,3],[0,6,0,7],[0,9,0,12]]}
["Data:","Conc./Excentr.","D outside",null,"Nipple","Red.neck","Threded length",null,"C to C","Weight"]
["Swaged nipples","sw.nipple","D1","D2","length A","Length F","H1","H2","M","Sch 40","Sch 80","Sch 160","Sch XXS"]
[1.0,"3/8\" x 1/4\"",17.15,13.72,64.0,16.0,10.0,8.0,{"$f":"0.5*(C3-D3)","v":1.715},0.08,0.08,0.11,0.13]
[null,"1/2\" x 1/4\"",21.34,13.72,70.0,16.0,11.0,8.0,3.81,0.13,0.14,0.17,0.22]
[null,"1/2\" x 3/8\"",21.34,17.15,70.0,16.0,11.0,10.0,2.095,0.13,0.14,0.17,0.22]
[null,"3/4\" x 1/4\"",26.67,13.72,76.0,16.0,13.0,8.0,6.475,0.2,0.21,0.27,0.34]
[null,"3/4\" x 3/8\"",26.67,17.15,76.0,18.0,13.0,10.0,4.76,0.2,0.21,0.27,0.34]
[null,"3/4\" x 1/2\"",26.67,21.34,76.0,21.0,13.0,11.0,2.665,0.2,0.21,0.27,0.34]
[null,"1\" x 1/4\"",33.4,13.72,89.0,16.0,14.0,8.0,9.84,0.25,0.33,0.42,0.55]
[null,"1\" x 3/8\"",33.4,17.15,89.0,18.0,14.0,10.0,8.125,0.25,0.33,0.42,0.55]
[null,"1\" x 1/2\"",33.4,21.34,89.0,21.0,14.0,11.0,6.03,0.25,0.33,0.42,0.55]
[null,"1\" x 3/4\"",33.4,26.67,89.0,22.5,14.0,13.0,3.365,0.25,0.33,0.42,0.55]
[null,"1¼\" x 1/2\"",42.16,21.34,102.0,21.0,17.0,11.0,10.41,0.38,0.45,0.57,0.79]
[null,"1¼\" x 3/4\"",42.16,26.67,102.0,22.5,17.0,13.0,7.745,0.38,0.45,0.57,0.79]
[null,"1¼\" x 1\"",42.16,33.4,102.0,25.0,17.0,14.0,4.38,0.38,0.45,0.57,0.79]
[null,"1½\" x 1/2\"",48.26,21.34,114.0,21.0,18.0,11.0,13.46,0.45,0.6,0.82,1.06]
[null,"1½\" x 3/4\"",48.26,26.67,114.0,22.5,18.0,13.0,10.795,0.45,0.6,0.82,1.06]
[null,"1½\" x 1\"",48.26,33.4,114.0,25.0,18.0,14.0,7.43,0.45,0.6,0.82,1.06]
[null,"1½\" x 1¼\"",48.26,42.16,114.0,27.0,18.0,17.0,3.05,0.45,0.6,0.82,1.06]
[null,"2\" x 1/2\"",60.33,21.34,165.0,21.0,19.0,11.0,19.495,0.85,1.2,1.8,2.2]
[null,"2\" x 3/4\"",60.33,26.67,165.0,22.5,19.0,13.0,16.83,0.85,1.2,1.8,2.2]
[null,"2\" x 1\"",60.33,33.4,165.0,25.0,19.0,14.0,13.465,0.85,1.2,1.8,2.2]
[null,"2\" x 1¼\"",60.33,42.16,165.0,27.0,19.0,17.0,9.085,0.85,1.2,1.8,2.2]
[null,"2\" x 1½\"",60.33,48.26,165.0,28.0,19.0,18.0,6.035,0.85,1.2,1.8,2.2]
[null,"2½\" x 1\"",73.03,33.4,178.0,25.0,24.0,14.0,19.815,1.3,2.0,2.6,3.6]
[null,"2½\" x 1¼\"",73.03,42.16,178.0,27.0,24.0,17.0,15.435,1.3,2.0,2.6,3.6]
[null,"2½\" x 1½\"",73.03,48.26,178.0,28.0,24.0,18.0,12.385,1.3,2.0,2.6,3.6]
[null,"2½\" x 2\"",73.03,60.33,178.0,29.0,24.0,19.0,6.35,1.3,2.0,2.6,3.6]
[null,"3\" x 1\"",88.9,33.4,203.0,25.0,26.0,14.0,27.75,1.7,3.0,4.3,5.6]
[null,"3\" x 1¼\"",88.9,42.16,203.0,27.0,26.0,17.0,23.37,1.7,3.0,4.3,5.6]
[null,"3\" x 1½\"",88.9,48.26,203.0,28.0,26.0,18.0,20.32,1.7,3.0,4.3,5.6]
[null,"3\" x 2\"",88.9,60.33,203.0,29.0,26.0,19.0,14.285,1.7,3.0,4.3,5.6]
[null,"3\" x 2½\"",88.9,73.03,203.0,41.0,26.0,24.0,7.935,1.7,3.0,4.3,5.6]
[null,"4\" x 1\"",114.3,33.4,229.0,25.0,26.0,14.0,40.45,2.33,5.0,7.5,9.2]
[null,"4\" x 1¼\"",114.3,42.16,229.0,27.0,28.0,17.0,36.07,2.33,5.0,7.5,9.2]
[null,"4\" x 1½\"",114.3,48.26,229.0,28.0,28.0,18.0,33.02,2.33,5.0,7.5,9.2]
[null,"4\" x 2\"",114.3,60.33,229.0,29.0,28.0,19.0,26.985,2.33,5.0,7.5,9.2]
[null,"4\" x 2½\"",114.3,73.03,229.0,41.0,28.0,24.0,20.635,2.33,5.0,7.5,9.2]
[null,"4\" x 3\"",114.3,88.9,229.0,43.0,28.0,26.0,12.7,2.33,5.0,7.5,9.2]

{"sheet":"Weldolets","index":20,"n_rows":52,"n_cols":5,"rows_kept":52,"cut":false,"hidden":true,"merged":[[0,0,0,8]]}
["WELDOLETS-LATROLETS-ELBOWLETS-NIPOLETS"]
[]
["Weldolet - Sockolet - Threadolet",null,null,null,"Size:"]
[]
["Weldolet height","A",null,"mm"]
["Rib diameter","B",null,"mm"]
["Branch diameter","D1",null,"mm"]
["Run diameter","Do",null,"mm"]
["Centre to face","L",null,"mm"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Latrolet acc. ANSI B 16.5",null,null,null,"Size:"]
[]
[null,"E",null,"mm"]
[null,"F",null,"mm"]
[null,"D",null,"mm"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Elbowlet acc. ANSI B 16.5",null,null,null,"Size:"]
["Run-size:"]
[null,"G",null,"mm"]
[null,"D",null,"mm"]
[null,null,null,"mm"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Nipolet acc. ANSI B 16.5",null,null,null,"Size:"]
["Run-size:"]
["Total length","L",null,"mm"]
["Diameter inside","Di",null,"mm"]
["Branch width","B",null,"mm"]

{"sheet":"Data weldolets","index":21,"n_rows":615,"n_cols":7,"rows_kept":615,"cut":false,"hidden":true,"merged":[]}
["Fitting data: Weldolets",null,"Height","Runpipe","Outside diam.","Centre to face","Runsize"]
[null,null,"A","hole B","D","L","Do"]
[261.0,"Weldolet sch. 40   Run 3/8\"    Branch 1/8\"",15.88,15.88,null,{"$f":"C3+0.5*G3","v":24.455},17.15]
[null,"Weldolet sch. 40   Run 3/8\"    Branch 1/4\"",15.88,15.88,null,24.455,17.15]
[null,"Weldolet sch. 40   Run 3/8\"    Branch 3/8\"",19.05,19.15,null,27.625,17.15]
[null,"Weldolet sch. 40   Run 1/2\"    Branch 1/8\"",15.88,15.88,null,26.55,21.34]
[null,"Weldolet sch. 40   Run 1/2\"    Branch 1/4\"",15.88,15.88,null,26.55,21.34]
[null,"Weldolet sch. 40   Run 1/2\"    Branch 3/8\"",19.05,19.15,null,29.72,21.34]
[null,"Weldolet sch. 40   Run 1/2\"    Branch 1/2\"",22.23,23.81,null,32.9,21.34]
[null,"Weldolet sch. 40   Run 3/4\"    Branch 1/8\"",15.88,15.88,null,29.215,26.67]
[null,"Weldolet sch. 40   Run 3/4\"    Branch 1/4\"",15.88,15.88,null,29.215,26.67]
[null,"Weldolet sch. 40   Run 3/4\"    Branch 3/8\"",19.05,19.15,null,32.385,26.67]
[null,"Weldolet sch. 40   Run 3/4\"    Branch 1/2\"",19.05,23.81,null,32.385,26.67]
[null,"Weldolet sch. 40   Run 3/4\"    Branch 3/4\"",22.23,30.16,null,35.565,26.67]
[null,"Weldolet sch. 40   Run 1\"       Branch 1/8\"",15.88,15.88,null,32.58,33.4]
[null,"Weldolet sch. 40   Run 1\"       Branch 1/4\"",15.88,15.88,null,32.58,33.4]
[null,"Weldolet sch. 40   Run 1\"       Branch 3/8\"",19.05,19.15,null,35.75,33.4]
[null,"Weldolet sch. 40   Run 1\"       Branch 1/2\"",19.05,23.81,null,35.75,33.4]
[null,"Weldolet sch. 40   Run 1\"       Branch 3/4\"",22.23,30.16,null,38.93,33.4]
[null,"Weldolet sch. 40   Run 1\"       Branch 1\"",26.99,36.51,null,43.69,33.4]
[null,"Weldolet sch. 40   Run 1¼\"    Branch 1/8\"",15.88,15.88,null,36.96,42.16]
[null,"Weldolet sch. 40   Run 1¼\"    Branch 1/4\"",15.88,15.88,null,36.96,42.16]
[null,"Weldolet sch. 40   Run 1¼\"    Branch 3/8\"",19.05,19.15,null,40.13,42.16]
[null,"Weldolet sch. 40   Run 1¼\"    Branch 1/2\"",19.05,23.81,null,40.13,42.16]
[null,"Weldolet sch. 40   Run 1¼\"    Branch 3/4\"",22.23,30.16,null,43.31,42.16]
[null,"Weldolet sch. 40   Run 1¼\"    Branch 1\"",26.99,36.51,null,48.07,42.16]
[null,"Weldolet sch. 40   Run 1¼\"    Branch 1¼\"",31.75,44.45,null,52.83,42.16]
[null,"Weldolet sch. 40   Run 1½\"    Branch 1/8\"",15.88,15.88,null,40.01,48.26]
[null,"Weldolet sch. 40   Run 1½\"    Branch 1/4\"",15.88,15.88,null,40.01,48.26]
[null,"Weldolet sch. 40   Run 1½\"    Branch 3/8\"",19.05,19.15,null,43.18,48.26]
[null,"Weldolet sch. 40   Run 1½\"    Branch 1/2\"",19.05,23.81,null,43.18,48.26]
[null,"Weldolet sch. 40   Run 1½\"    Branch 3/4\"",22.23,30.16,null,46.36,48.26]
[null,"Weldolet sch. 40   Run 1½\"    Branch 1\"",26.99,36.51,null,51.12,48.26]
[null,"Weldolet sch. 40   Run 1½\"    Branch 1¼\"",31.75,44.45,null,55.88,48.26]
[null,"Weldolet sch. 40   Run 1½\"    Branch 1½\"",33.34,50.8,null,57.47,48.26]
[null,"Weldolet sch. 40   Run 2\"       Branch 1/8\"",15.88,15.88,null,46.03,60.3]
[null,"Weldolet sch. 40   Run 2\"       Branch 1/4\"",15.88,15.88,null,46.03,60.3]
[null,"Weldolet sch. 40   Run 2\"       Branch 3/8\"",19.05,19.15,null,49.2,60.3]
[null,"Weldolet sch. 40   Run 2\"       Branch 1/2\"",19.05,23.81,null,49.2,60.3]
[null,"Weldolet sch. 40   Run 2\"       Branch 3/4\"",22.23,30.16,null,52.38,60.3]
[null,"Weldolet sch. 40   Run 2\"       Branch 1\"",26.99,36.51,null,57.14,60.3]
[null,"Weldolet sch. 40   Run 2\"       Branch 1¼\"",31.75,44.45,null,61.9,60.3]
[null,"Weldolet sch. 40   Run 2\"       Branch 1½\"",33.34,50.8,null,63.49,60.3]
[null,"Weldolet sch. 40   Run 2\"       Branch 2\"",38.1,65.09,null,68.25,60.3]
[null,"Weldolet sch. 40   Run 2½\"    Branch 1/8\"",15.88,15.88,null,52.395,73.03]
[null,"Weldolet sch. 40   Run 2½\"    Branch 1/4\"",15.88,15.88,null,52.395,73.03]
[null,"Weldolet sch. 40   Run 2½\"    Branch 3/8\"",19.05,19.15,null,55.565,73.03]
[null,"Weldolet sch. 40   Run 2½\"    Branch 1/2\"",19.05,23.81,null,55.565,73.03]
[null,"Weldolet sch. 40   Run 2½\"    Branch 3/4\"",22.23,30.16,null,58.745,73.03]
[null,"Weldolet sch. 40   Run 2½\"    Branch 1\"",26.99,36.51,null,63.505,73.03]
[null,"Weldolet sch. 40   Run 2½\"    Branch 1¼\"",31.75,44.45,null,68.265,73.03]
[null,"Weldolet sch. 40   Run 2½\"    Branch 1½\"",33.34,50.8,null,69.855,73.03]
[null,"Weldolet sch. 40   Run 2½\"    Branch 2\"",38.1,65.09,null,74.615,73.03]
[null,"Weldolet sch. 40   Run 2½\"    Branch 2½\"",41.28,76.2,null,77.795,73.03]
[null,"Weldolet sch. 40   Run 3\"       Branch 1/8\"",15.88,15.88,null,60.33,88.9]
[null,"Weldolet sch. 40   Run 3\"       Branch 1/4\"",15.88,15.88,null,60.33,88.9]
[null,"Weldolet sch. 40   Run 3\"       Branch 3/8\"",19.05,19.15,null,63.5,88.9]
[null,"Weldolet sch. 40   Run 3\"       Branch 1/2\"",19.05,23.81,null,63.5,88.9]
[null,"Weldolet sch. 40   Run 3\"       Branch 3/4\"",22.23,30.16,null,66.68,88.9]
[null,"Weldolet sch. 40   Run 3\"       Branch 1\"",26.99,36.51,null,71.44,88.9]
[null,"Weldolet sch. 40   Run 3\"       Branch 1¼\"",31.75,44.45,null,76.2,88.9]
[null,"Weldolet sch. 40   Run 3\"       Branch 1½\"",33.34,50.8,null,77.79,88.9]
[null,"Weldolet sch. 40   Run 3\"       Branch 2\"",38.1,65.09,null,82.55,88.9]
[null,"Weldolet sch. 40   Run 3\"       Branch 2½\"",41.28,76.2,null,85.73,88.9]
[null,"Weldolet sch. 40   Run 3\"       Branch 3\"",44.45,93.66,null,88.9,88.9]
[null,"Weldolet sch. 40   Run 3½\"    Branch 1/8\"",15.88,15.88,null,66.68,101.6]
[null,"Weldolet sch. 40   Run 3½\"    Branch 1/4\"",15.88,15.88,null,66.68,101.6]
[null,"Weldolet sch. 40   Run 3½\"    Branch 3/8\"",19.05,19.15,null,69.85,101.6]
[null,"Weldolet sch. 40   Run 3½\"    Branch 1/2\"",19.05,23.81,null,69.85,101.6]
[null,"Weldolet sch. 40   Run 3½\"    Branch 3/4\"",22.23,30.16,null,73.03,101.6]
[null,"Weldolet sch. 40   Run 3½\"    Branch 1\"",26.99,36.51,null,77.79,101.6]
[null,"Weldolet sch. 40   Run 3½\"    Branch 1¼\"",31.75,44.45,null,82.55,101.6]
[null,"Weldolet sch. 40   Run 3½\"    Branch 1½\"",33.34,50.8,null,84.14,101.6]
[null,"Weldolet sch. 40   Run 3½\"    Branch 2\"",38.1,65.09,null,88.9,101.6]
[null,"Weldolet sch. 40   Run 3½\"    Branch 2½\"",41.28,76.2,null,92.08,101.6]
[null,"Weldolet sch. 40   Run 3½\"    Branch 3\"",44.45,93.66,null,95.25,101.6]
[null,"Weldolet sch. 40   Run 3½\"    Branch 3½\"",47.63,101.6,null,98.43,101.6]
[null,"Weldolet sch. 40   Run 4\"       Branch 1/8\"",15.88,15.88,null,73.03,114.3]
[null,"Weldolet sch. 40   Run 4\"       Branch 1/4\"",15.88,15.88,null,73.03,114.3]
[null,"Weldolet sch. 40   Run 4\"       Branch 3/8\"",19.05,19.15,null,76.2,114.3]
[null,"Weldolet sch. 40   Run 4\"       Branch 1/2\"",19.05,23.81,null,76.2,114.3]
[null,"Weldolet sch. 40   Run 4\"       Branch 3/4\"",22.23,30.16,null,79.38,114.3]
[null,"Weldolet sch. 40   Run 4\"       Branch 1\"",26.99,36.51,null,84.14,114.3]
[null,"Weldolet sch. 40   Run 4\"       Branch 1¼\"",31.75,44.45,null,88.9,114.3]
[null,"Weldolet sch. 40   Run 4\"       Branch 1½\"",33.34,50.8,null,90.49,114.3]
[null,"Weldolet sch. 40   Run 4\"       Branch 2\"",38.1,65.09,null,95.25,114.3]
[null,"Weldolet sch. 40   Run 4\"       Branch 2½\"",41.28,76.2,null,98.43,114.3]
[null,"Weldolet sch. 40   Run 4\"       Branch 3\"",44.45,93.66,null,101.6,114.3]
[null,"Weldolet sch. 40   Run 4\"       Branch 3½\"",47.63,101.6,null,104.78,114.3]
[null,"Weldolet sch. 40   Run 4\"       Branch 4\"",50.8,120.65,null,107.95,114.3]
[null,"Weldolet sch. 40   Run 5\"       Branch 1/8\"",15.88,15.88,null,86.53,141.3]
[null,"Weldolet sch. 40   Run 5\"       Branch 1/4\"",15.88,15.88,null,86.53,141.3]
[null,"Weldolet sch. 40   Run 5\"       Branch 3/8\"",19.05,19.15,null,89.7,141.3]
[null,"Weldolet sch. 40   Run 5\"       Branch 1/2\"",19.05,23.81,null,89.7,141.3]
[null,"Weldolet sch. 40   Run 5\"       Branch 3/4\"",22.23,30.16,null,92.88,141.3]
[null,"Weldolet sch. 40   Run 5\"       Branch 1\"",26.99,36.51,null,97.64,141.3]
[null,"Weldolet sch. 40   Run 5\"       Branch 1¼\"",31.75,44.45,null,102.4,141.3]
[null,"Weldolet sch. 40   Run 5\"       Branch 1½\"",33.34,50.8,null,103.99,141.3]
[null,"Weldolet sch. 40   Run 5\"       Branch 2\"",38.1,65.09,null,108.75,141.3]
[null,"Weldolet sch. 40   Run 5\"       Branch 2½\"",41.28,76.2,null,111.93,141.3]
[null,"Weldolet sch. 40   Run 5\"       Branch 3\"",44.45,93.66,null,115.1,141.3]
[null,"Weldolet sch. 40   Run 5\"       Branch 3½\"",47.63,101.6,null,118.28,141.3]
[null,"Weldolet sch. 40   Run 5\"       Branch 4\"",50.8,120.65,null,121.45,141.3]
[null,"Weldolet sch. 40   Run 5\"       Branch 5\"",57.15,141.29,null,127.8,141.3]
[null,"Weldolet sch. 40   Run 6\"       Branch 1/8\"",15.88,15.88,null,100.02,168.28]
[null,"Weldolet sch. 40   Run 6\"       Branch 1/4\"",15.88,15.88,null,100.02,168.28]
[null,"Weldolet sch. 40   Run 6\"       Branch 3/8\"",19.05,19.15,null,103.19,168.28]
[null,"Weldolet sch. 40   Run 6\"       Branch 1/2\"",19.05,23.81,null,103.19,168.28]
[null,"Weldolet sch. 40   Run 6\"       Branch 3/4\"",22.23,30.16,null,106.37,168.28]
[null,"Weldolet sch. 40   Run 6\"       Branch 1\"",26.99,36.51,null,111.13,168.28]
[null,"Weldolet sch. 40   Run 6\"       Branch 1¼\"",31.75,44.45,null,115.89,168.28]
[null,"Weldolet sch. 40   Run 6\"       Branch 1½\"",33.34,50.8,null,117.48,168.28]
[null,"Weldolet sch. 40   Run 6\"       Branch 2\"",38.1,65.09,null,122.24,168.28]
[null,"Weldolet sch. 40   Run 6\"       Branch 2½\"",41.28,76.2,null,125.42,168.28]
[null,"Weldolet sch. 40   Run 6\"       Branch 3\"",44.45,93.66,null,128.59,168.28]
[null,"Weldolet sch. 40   Run 6\"       Branch 3½\"",47.63,101.6,null,131.77,168.28]
[null,"Weldolet sch. 40   Run 6\"       Branch 4\"",50.8,120.65,null,134.94,168.28]
[null,"Weldolet sch. 40   Run 6\"       Branch 5\"",57.15,141.29,null,141.29,168.28]
[null,"Weldolet sch. 40   Run 6\"       Branch 6\"",60.33,169.86,null,144.47,168.28]
[null,"Weldolet sch. 40   Run 8\"       Branch 1/8\"",15.88,15.88,null,125.42,219.08]
[null,"Weldolet sch. 40   Run 8\"       Branch 1/4\"",15.88,15.88,null,125.42,219.08]
[null,"Weldolet sch. 40   Run 8\"       Branch 3/8\"",19.05,19.15,null,128.59,219.08]
[null,"Weldolet sch. 40   Run 8\"       Branch 1/2\"",19.05,23.81,null,128.59,219.08]
[null,"Weldolet sch. 40   Run 8\"       Branch 3/4\"",22.23,30.16,null,131.77,219.08]
[null,"Weldolet sch. 40   Run 8\"       Branch 1\"",26.99,36.51,null,136.53,219.08]
[null,"Weldolet sch. 40   Run 8\"       Branch 1¼\"",31.75,44.45,null,141.29,219.08]
[null,"Weldolet sch. 40   Run 8\"       Branch 1½\"",33.34,50.8,null,142.88,219.08]
[null,"Weldolet sch. 40   Run 8\"       Branch 2\"",38.1,65.09,null,147.64,219.08]
[null,"Weldolet sch. 40   Run 8\"       Branch 2½\"",41.28,76.2,null,150.82,219.08]
[null,"Weldolet sch. 40   Run 8\"       Branch 3\"",44.45,93.66,null,153.99,219.08]
[null,"Weldolet sch. 40   Run 8\"       Branch 3½\"",47.63,101.6,null,157.17,219.08]
[null,"Weldolet sch. 40   Run 8\"       Branch 4\"",50.8,120.65,null,160.34,219.08]
[null,"Weldolet sch. 40   Run 8\"       Branch 5\"",57.15,141.29,null,166.69,219.08]
[null,"Weldolet sch. 40   Run 8\"       Branch 6\"",60.33,169.86,null,169.87,219.08]
[null,"Weldolet sch. 40   Run 8\"       Branch 8\"",69.85,220.66,null,179.39,219.08]
[null,"Weldolet sch. 40   Run 10\"     Branch 1/8\"",15.88,15.88,null,152.405,273.05]
[null,"Weldolet sch. 40   Run 10\"     Branch 1/4\"",15.88,15.88,null,152.405,273.05]
[null,"Weldolet sch. 40   Run 10\"     Branch 3/8\"",19.05,19.15,null,155.575,273.05]
[null,"Weldolet sch. 40   Run 10\"     Branch 1/2\"",19.05,23.81,null,155.575,273.05]
[null,"Weldolet sch. 40   Run 10\"     Branch 3/4\"",22.23,30.16,null,158.755,273.05]
[null,"Weldolet sch. 40   Run 10\"     Branch 1\"",26.99,36.51,null,163.515,273.05]
[null,"Weldolet sch. 40   Run 10\"     Branch 1¼\"",31.75,44.45,null,168.275,273.05]
[null,"Weldolet sch. 40   Run 10\"     Branch 1½\"",33.34,50.8,null,169.865,273.05]
[null,"Weldolet sch. 40   Run 10\"     Branch 2\"",38.1,65.09,null,174.625,273.05]
[null,"Weldolet sch. 40   Run 10\"     Branch 2½\"",41.28,76.2,null,177.805,273.05]
[null,"Weldolet sch. 40   Run 10\"     Branch 3\"",44.45,93.66,null,180.975,273.05]
[null,"Weldolet sch. 40   Run 10\"     Branch 3½\"",47.63,101.6,null,184.155,273.05]
[null,"Weldolet sch. 40   Run 10\"     Branch 4\"",50.8,120.65,null,187.325,273.05]
[null,"Weldolet sch. 40   Run 10\"     Branch 5\"",57.15,141.29,null,193.675,273.05]
[null,"Weldolet sch. 40   Run 10\"     Branch 6\"",60.33,169.86,null,196.855,273.05]
[null,"Weldolet sch. 40   Run 10\"     Branch 8\"",69.85,220.66,null,206.375,273.05]
[null,"Weldolet sch. 40   Run 10\"     Branch 10\"",77.78,274.64,null,214.305,273.05]
[null,"Weldolet sch. 40   Run 12\"     Branch 1/8\"",15.88,15.88,null,177.805,323.85]
[null,"Weldolet sch. 40   Run 12\"     Branch 1/4\"",15.88,15.88,null,177.805,323.85]
[null,"Weldolet sch. 40   Run 12\"     Branch 3/8\"",19.05,19.15,null,180.975,323.85]
[null,"Weldolet sch. 40   Run 12\"     Branch 1/2\"",19.05,23.81,null,180.975,323.85]
[null,"Weldolet sch. 40   Run 12\"     Branch 3/4\"",22.23,30.16,null,184.155,323.85]
[null,"Weldolet sch. 40   Run 12\"     Branch 1\"",26.99,36.51,null,188.915,323.85]
[null,"Weldolet sch. 40   Run 12\"     Branch 1¼\"",31.75,44.45,null,193.675,323.85]
[null,"Weldolet sch. 40   Run 12\"     Branch 1½\"",33.34,50.8,null,195.265,323.85]
[null,"Weldolet sch. 40   Run 12\"     Branch 2\"",38.1,65.09,null,200.025,323.85]
[null,"Weldolet sch. 40   Run 12\"     Branch 2½\"",41.28,76.2,null,203.205,323.85]
[null,"Weldolet sch. 40   Run 12\"     Branch 3\"",44.45,93.66,null,206.375,323.85]
[null,"Weldolet sch. 40   Run 12\"     Branch 3½\"",47.63,101.6,null,209.555,323.85]
[null,"Weldolet sch. 40   Run 12\"     Branch 4\"",50.8,120.65,null,212.725,323.85]
[null,"Weldolet sch. 40   Run 12\"     Branch 5\"",57.15,141.29,null,219.075,323.85]
[null,"Weldolet sch. 40   Run 12\"     Branch 6\"",60.33,169.86,null,222.255,323.85]
[null,"Weldolet sch. 40   Run 12\"     Branch 8\"",69.85,220.66,null,231.775,323.85]
[null,"Weldolet sch. 40   Run 12\"     Branch 10\"",77.78,274.64,null,239.705,323.85]
[null,"Weldolet sch. 40   Run 12\"     Branch 12\"",85.73,325.44,null,247.655,323.85]
[null,"Weldolet sch. 40   Run 14\"     Branch 1/8\"",15.88,15.88,null,193.68,355.6]
[null,"Weldolet sch. 40   Run 14\"     Branch 1/4\"",15.88,15.88,null,193.68,355.6]
[null,"Weldolet sch. 40   Run 14\"     Branch 3/8\"",19.05,19.15,null,196.85,355.6]
[null,"Weldolet sch. 40   Run 14\"     Branch 1/2\"",19.05,23.81,null,196.85,355.6]
[null,"Weldolet sch. 40   Run 14\"     Branch 3/4\"",22.23,30.16,null,200.03,355.6]
[null,"Weldolet sch. 40   Run 14\"     Branch 1\"",26.99,36.51,null,204.79,355.6]
[null,"Weldolet sch. 40   Run 14\"     Branch 1¼\"",31.75,44.45,null,209.55,355.6]
[null,"Weldolet sch. 40   Run 14\"     Branch 1½\"",33.34,50.8,null,211.14,355.6]
[null,"Weldolet sch. 40   Run 14\"     Branch 2\"",38.1,65.09,null,215.9,355.6]
[null,"Weldolet sch. 40   Run 14\"     Branch 2½\"",41.28,76.2,null,219.08,355.6]
[null,"Weldolet sch. 40   Run 14\"     Branch 3\"",44.45,93.66,null,222.25,355.6]
[null,"Weldolet sch. 40   Run 14\"     Branch 3½\"",47.63,101.6,null,225.43,355.6]
[null,"Weldolet sch. 40   Run 14\"     Branch 4\"",50.8,120.65,null,228.6,355.6]
[null,"Weldolet sch. 40   Run 14\"     Branch 5\"",57.15,141.29,null,234.95,355.6]
[null,"Weldolet sch. 40   Run 14\"     Branch 6\"",60.33,169.86,null,238.13,355.6]
[null,"Weldolet sch. 40   Run 14\"     Branch 8\"",69.85,220.66,null,247.65,355.6]
[null,"Weldolet sch. 40   Run 14\"     Branch 10\"",77.78,274.64,null,255.58,355.6]
[null,"Weldolet sch. 40   Run 14\"     Branch 12\"",85.73,325.44,null,263.53,355.6]
[null,"Weldolet sch. 40   Run 14\"     Branch 14\"",88.9,357.19,null,266.7,355.6]
[null,"Weldolet sch. 40   Run 16\"     Branch 1/8\"",15.88,15.88,null,219.08,406.4]
[null,"Weldolet sch. 40   Run 16\"     Branch 1/4\"",15.88,15.88,null,219.08,406.4]
[null,"Weldolet sch. 40   Run 16\"     Branch 3/8\"",19.05,19.15,null,222.25,406.4]
[null,"Weldolet sch. 40   Run 16\"     Branch 1/2\"",19.05,23.81,null,222.25,406.4]
[null,"Weldolet sch. 40   Run 16\"     Branch 3/4\"",22.23,30.16,null,225.43,406.4]
[null,"Weldolet sch. 40   Run 16\"     Branch 1\"",26.99,36.51,null,230.19,406.4]
[null,"Weldolet sch. 40   Run 16\"     Branch 1¼\"",31.75,44.45,null,234.95,406.4]
[null,"Weldolet sch. 40   Run 16\"     Branch 1½\"",33.34,50.8,null,236.54,406.4]
[null,"Weldolet sch. 40   Run 16\"     Branch 2\"",38.1,65.09,null,241.3,406.4]
[null,"Weldolet sch. 40   Run 16\"     Branch 2½\"",41.28,76.2,null,244.48,406.4]
[null,"Weldolet sch. 40   Run 16\"     Branch 3\"",44.45,93.66,null,247.65,406.4]
[null,"Weldolet sch. 40   Run 16\"     Branch 3½\"",47.63,101.6,null,250.83,406.4]
[null,"Weldolet sch. 40   Run 16\"     Branch 4\"",50.8,120.65,null,254,406.4]
[null,"Weldolet sch. 40   Run 16\"     Branch 5\"",57.15,141.29,null,260.35,406.4]
[null,"Weldolet sch. 40   Run 16\"     Branch 6\"",60.33,169.86,null,263.53,406.4]
[null,"Weldolet sch. 40   Run 16\"     Branch 8\"",69.85,220.66,null,273.05,406.4]
[null,"Weldolet sch. 40   Run 16\"     Branch 10\"",77.78,274.64,null,280.98,406.4]
[null,"Weldolet sch. 40   Run 16\"     Branch 12\"",85.73,325.44,null,288.93,406.4]
[null,"Weldolet sch. 40   Run 16\"     Branch 14\"",88.9,357.19,null,292.1,406.4]
[null,"Weldolet sch. 40   Run 16\"     Branch 16\"",93.66,407.99,null,296.86,406.4]
[null,"Weldolet sch. 40   Run 18\"     Branch 1/8\"",15.88,15.88,null,244.48,457.2]
[null,"Weldolet sch. 40   Run 18\"     Branch 1/4\"",15.88,15.88,null,244.48,457.2]
[null,"Weldolet sch. 40   Run 18\"     Branch 3/8\"",19.05,19.15,null,247.65,457.2]
[null,"Weldolet sch. 40   Run 18\"     Branch 1/2\"",19.05,23.81,null,247.65,457.2]
[null,"Weldolet sch. 40   Run 18\"     Branch 3/4\"",22.23,30.16,null,250.83,457.2]
[null,"Weldolet sch. 40   Run 18\"     Branch 1\"",26.99,36.51,null,255.59,457.2]
[null,"Weldolet sch. 40   Run 18\"     Branch 1¼\"",31.75,44.45,null,260.35,457.2]
[null,"Weldolet sch. 40   Run 18\"     Branch 1½\"",33.34,50.8,null,261.94,457.2]
[null,"Weldolet sch. 40   Run 18\"     Branch 2\"",38.1,65.09,null,266.7,457.2]
[null,"Weldolet sch. 40   Run 18\"     Branch 2½\"",41.28,76.2,null,269.88,457.2]
[null,"Weldolet sch. 40   Run 18\"     Branch 3\"",44.45,93.66,null,273.05,457.2]
[null,"Weldolet sch. 40   Run 18\"     Branch 3½\"",47.63,101.6,null,276.23,457.2]
[null,"Weldolet sch. 40   Run 18\"     Branch 4\"",50.8,120.65,null,279.4,457.2]
[null,"Weldolet sch. 40   Run 18\"     Branch 5\"",57.15,141.29,null,285.75,457.2]
[null,"Weldolet sch. 40   Run 18\"     Branch 6\"",60.33,169.86,null,288.93,457.2]
[null,"Weldolet sch. 40   Run 18\"     Branch 8\"",69.85,220.66,null,298.45,457.2]
[null,"Weldolet sch. 40   Run 18\"     Branch 10\"",77.78,274.64,null,306.38,457.2]
[null,"Weldolet sch. 40   Run 18\"     Branch 12\"",85.73,325.44,null,314.33,457.2]
[null,"Weldolet sch. 40   Run 18\"     Branch 14\"",88.9,357.19,null,317.5,457.2]
[null,"Weldolet sch. 40   Run 18\"     Branch 16\"",93.66,407.99,null,322.26,457.2]
[null,"Weldolet sch. 40   Run 18\"     Branch 18\"",96.84,458.79,null,325.44,457.2]
[null,"Weldolet sch. 40   Run 20\"     Branch 1/8\"",15.88,15.88,null,269.88,508.0]
[null,"Weldolet sch. 40   Run 20\"     Branch 1/4\"",15.88,15.88,null,269.88,508.0]
[null,"Weldolet sch. 40   Run 20\"     Branch 3/8\"",19.05,19.15,null,273.05,508.0]
[null,"Weldolet sch. 40   Run 20\"     Branch 1/2\"",19.05,23.81,null,273.05,508.0]
[null,"Weldolet sch. 40   Run 20\"     Branch 3/4\"",22.23,30.16,null,276.23,508.0]
[null,"Weldolet sch. 40   Run 20\"     Branch 1\"",26.99,36.51,null,280.99,508.0]
[null,"Weldolet sch. 40   Run 20\"     Branch 1¼\"",31.75,44.45,null,285.75,508.0]
[null,"Weldolet sch. 40   Run 20\"     Branch 1½\"",33.34,50.8,null,287.34,508.0]
[null,"Weldolet sch. 40   Run 20\"     Branch 2\"",38.1,65.09,null,292.1,508.0]
[null,"Weldolet sch. 40   Run 20\"     Branch 2½\"",41.28,76.2,null,295.28,508.0]
[null,"Weldolet sch. 40   Run 20\"     Branch 3\"",44.45,93.66,null,298.45,508.0]
[null,"Weldolet sch. 40   Run 20\"     Branch 3½\"",47.63,101.6,null,301.63,508.0]
[null,"Weldolet sch. 40   Run 20\"     Branch 4\"",50.8,120.65,null,304.8,508.0]
[null,"Weldolet sch. 40   Run 20\"     Branch 5\"",57.15,141.29,null,311.15,508.0]
[null,"Weldolet sch. 40   Run 20\"     Branch 6\"",60.33,169.86,null,314.33,508.0]
[null,"Weldolet sch. 40   Run 20\"     Branch 8\"",69.85,220.66,null,323.85,508.0]
[null,"Weldolet sch. 40   Run 20\"     Branch 10\"",77.78,274.64,null,331.78,508.0]
[null,"Weldolet sch. 40   Run 20\"     Branch 12\"",85.73,325.44,null,339.73,508.0]
[null,"Weldolet sch. 40   Run 20\"     Branch 14\"",88.9,357.19,null,342.9,508.0]
[null,"Weldolet sch. 40   Run 20\"     Branch 16\"",93.66,407.99,null,347.66,508.0]
[null,"Weldolet sch. 40   Run 20\"     Branch 18\"",96.84,458.79,null,350.84,508.0]
[null,"Weldolet sch. 40   Run 20\"     Branch 20\"",101.6,508.0,null,355.6,508.0]
[null,"Weldolet sch. 40   Run 24\"     Branch 1/8\"",15.88,15.88,null,320.68,609.6]
[null,"Weldolet sch. 40   Run 24\"     Branch 1/4\"",15.88,15.88,null,320.68,609.6]
[null,"Weldolet sch. 40   Run 24\"     Branch 3/8\"",19.05,19.15,null,323.85,609.6]
[null,"Weldolet sch. 40   Run 24\"     Branch 1/2\"",19.05,23.81,null,323.85,609.6]
[null,"Weldolet sch. 40   Run 24\"     Branch 3/4\"",22.23,30.16,null,327.03,609.6]
[null,"Weldolet sch. 40   Run 24\"     Branch 1\"",26.99,36.51,null,331.79,609.6]
[null,"Weldolet sch. 40   Run 24\"     Branch 1¼\"",31.75,44.45,null,336.55,609.6]
[null,"Weldolet sch. 40   Run 24\"     Branch 1½\"",33.34,50.8,null,338.14,609.6]
[null,"Weldolet sch. 40   Run 24\"     Branch 2\"",38.1,65.09,null,342.9,609.6]
[null,"Weldolet sch. 40   Run 24\"     Branch 2½\"",41.28,76.2,null,346.08,609.6]
[null,"Weldolet sch. 40   Run 24\"     Branch 3\"",44.45,93.66,null,349.25,609.6]
[null,"Weldolet sch. 40   Run 24\"     Branch 3½\"",47.63,101.6,null,352.43,609.6]
[null,"Weldolet sch. 40   Run 24\"     Branch 4\"",50.8,120.65,null,355.6,609.6]
[null,"Weldolet sch. 40   Run 20\"     Branch 5\"",57.15,141.29,null,361.95,609.6]
[null,"Weldolet sch. 40   Run 24\"     Branch 6\"",60.33,169.86,null,365.13,609.6]
[null,"Weldolet sch. 40   Run 24\"     Branch 8\"",69.85,220.66,null,374.65,609.6]
[null,"Weldolet sch. 40   Run 24\"     Branch 10\"",77.78,274.64,null,382.58,609.6]
[null,"Weldolet sch. 40   Run 24\"     Branch 12\"",85.73,325.44,null,390.53,609.6]
[null,"Weldolet sch. 40   Run 24\"     Branch 14\"",88.9,357.19,null,393.7,609.6]
[null,"Weldolet sch. 40   Run 24\"     Branch 16\"",93.66,407.99,null,398.46,609.6]
[null,"Weldolet sch. 40   Run 24\"     Branch 18\"",96.84,458.79,null,401.64,609.6]
[null,"Weldolet sch. 40   Run 24\"     Branch 20\"",101.6,508.0,null,406.4,609.6]
[null,"Weldolet sch. 40   Run 24\"     Branch 24\"",115.89,614.36,null,420.69,609.6]
[null,"Weldolet sch. XS   Run 3/8\"    Branch 1/8\"",15.88,15.88,null,24.455,17.15]
[null,"Weldolet sch. XS   Run 3/8\"    Branch 1/4\"",15.88,15.88,null,24.455,17.15]
[null,"Weldolet sch. XS   Run 1/2\"    Branch 1/8\"",15.88,15.88,null,26.55,21.34]
[null,"Weldolet sch. XS   Run 1/2\"    Branch 1/4\"",15.88,15.88,null,26.55,21.34]
[null,"Weldolet sch. XS   Run 1/2\"    Branch 3/8\"",19.05,19.05,null,29.72,21.34]
[null,"Weldolet sch. XS   Run 1/2\"    Branch 1/2\"",19.05,23.81,null,29.72,21.34]
[null,"Weldolet sch. XS   Run 3/4\"    Branch 1/8\"",15.88,15.88,null,29.215,26.67]
[null,"Weldolet sch. XS   Run 3/4\"    Branch 1/4\"",15.88,15.88,null,29.215,26.67]
[null,"Weldolet sch. XS   Run 3/4\"    Branch 3/8\"",19.05,19.05,null,32.385,26.67]
[null,"Weldolet sch. XS   Run 3/4\"    Branch 1/2\"",19.05,23.81,null,32.385,26.67]
[null,"Weldolet sch. XS   Run 3/4\"    Branch 3/4\"",22.23,30.16,null,35.565,26.67]
[null,"Weldolet sch. XS   Run 1\"       Branch 1/8\"",15.88,15.88,null,32.58,33.4]
[null,"Weldolet sch. XS   Run 1\"       Branch 1/4\"",15.88,15.88,null,32.58,33.4]
[null,"Weldolet sch. XS   Run 1\"       Branch 3/8\"",15.88,19.05,null,32.58,33.4]
[null,"Weldolet sch. XS   Run 1\"       Branch 1/2\"",15.88,23.81,null,32.58,33.4]
[null,"Weldolet sch. XS   Run 1\"       Branch 3/4\"",19.05,30.16,null,35.75,33.4]
[null,"Weldolet sch. XS   Run 1\"       Branch 1\"",26.99,36.51,null,43.69,33.4]
[null,"Weldolet sch. XS   Run 1¼\"    Branch 1/8\"",15.88,15.88,null,36.96,42.16]
[null,"Weldolet sch. XS   Run 1¼\"    Branch 1/4\"",15.88,15.88,null,36.96,42.16]
[null,"Weldolet sch. XS   Run 1¼\"    Branch 3/8\"",15.88,19.05,null,36.96,42.16]
[null,"Weldolet sch. XS   Run 1¼\"    Branch 1/2\"",15.88,23.81,null,36.96,42.16]
[null,"Weldolet sch. XS   Run 1¼\"    Branch 3/4\"",19.05,30.16,null,40.13,42.16]
[null,"Weldolet sch. XS   Run 1¼\"    Branch 1\"",26.99,36.51,null,48.07,42.16]
[null,"Weldolet sch. XS   Run 1¼\"    Branch 1¼\"",31.75,44.45,null,52.83,42.16]
[null,"Weldolet sch. XS   Run 1½\"    Branch 1/8\"",15.88,15.88,null,40.01,48.26]
[null,"Weldolet sch. XS   Run 1½\"    Branch 1/4\"",15.88,15.88,null,40.01,48.26]
[null,"Weldolet sch. XS   Run 1½\"    Branch 3/8\"",15.88,19.05,null,40.01,48.26]
[null,"Weldolet sch. XS   Run 1½\"    Branch 1/2\"",15.88,23.81,null,40.01,48.26]
[null,"Weldolet sch. XS   Run 1½\"    Branch 3/4\"",19.05,30.16,null,43.18,48.26]
[null,"Weldolet sch. XS   Run 1½\"    Branch 1\"",26.99,36.51,null,51.12,48.26]
[null,"Weldolet sch. XS   Run 1½\"    Branch 1¼\"",31.75,44.45,null,55.88,48.26]
[null,"Weldolet sch. XS   Run 1½\"    Branch 1½\"",33.34,50.8,null,57.47,48.26]
[null,"Weldolet sch. XS   Run 2\"       Branch 1/8\"",15.88,15.88,null,46.045,60.33]
[null,"Weldolet sch. XS   Run 2\"       Branch 1/4\"",15.88,15.88,null,46.045,60.33]
[null,"Weldolet sch. XS   Run 2\"       Branch 3/8\"",15.88,19.05,null,46.045,60.33]
[null,"Weldolet sch. XS   Run 2\"       Branch 1/2\"",15.88,23.81,null,46.045,60.33]
[null,"Weldolet sch. XS   Run 2\"       Branch 3/4\"",19.05,30.16,null,49.215,60.33]
[null,"Weldolet sch. XS   Run 2\"       Branch 1\"",26.99,36.51,null,57.155,60.33]
[null,"Weldolet sch. XS   Run 2\"       Branch 1¼\"",31.75,44.45,null,61.915,60.33]
[null,"Weldolet sch. XS   Run 2\"       Branch 1½\"",33.34,50.8,null,63.505,60.33]
[null,"Weldolet sch. XS   Run 2\"       Branch 2\"",38.1,65.09,null,68.265,60.33]
[null,"Weldolet sch. XS   Run 2½\"    Branch 1/8\"",15.88,15.88,null,52.395,73.03]
[null,"Weldolet sch. XS   Run 2½\"    Branch 1/4\"",15.88,15.88,null,52.395,73.03]
[null,"Weldolet sch. XS   Run 2½\"    Branch 3/8\"",15.88,19.05,null,52.395,73.03]
[null,"Weldolet sch. XS   Run 2½\"    Branch 1/2\"",15.88,23.81,null,52.395,73.03]
[null,"Weldolet sch. XS   Run 2½\"    Branch 3/4\"",19.05,30.16,null,55.565,73.03]
[null,"Weldolet sch. XS   Run 2½\"    Branch 1\"",26.99,36.51,null,63.505,73.03]
[null,"Weldolet sch. XS   Run 2½\"    Branch 1¼\"",31.75,44.45,null,68.265,73.03]
[null,"Weldolet sch. XS   Run 2½\"    Branch 1½\"",33.34,50.8,null,69.855,73.03]
[null,"Weldolet sch. XS   Run 2½\"    Branch 2\"",38.1,65.09,null,74.615,73.03]
[null,"Weldolet sch. XS   Run 2½\"    Branch 2½\"",41.28,76.2,null,77.795,73.03]
[null,"Weldolet sch. XS   Run 3\"       Branch 1/8\"",15.88,15.88,null,60.33,88.9]
[null,"Weldolet sch. XS   Run 3\"       Branch 1/4\"",15.88,15.88,null,60.33,88.9]
[null,"Weldolet sch. XS   Run 3\"       Branch 3/8\"",15.88,19.05,null,60.33,88.9]
[null,"Weldolet sch. XS   Run 3\"       Branch 1/2\"",15.88,23.81,null,60.33,88.9]
[null,"Weldolet sch. XS   Run 3\"       Branch 3/4\"",19.05,30.16,null,63.5,88.9]
[null,"Weldolet sch. XS   Run 3\"       Branch 1\"",26.99,36.51,null,71.44,88.9]
[null,"Weldolet sch. XS   Run 3\"       Branch 1¼\"",31.75,44.45,null,76.2,88.9]
[null,"Weldolet sch. XS   Run 3\"       Branch 1½\"",33.34,50.8,null,77.79,88.9]
[null,"Weldolet sch. XS   Run 3\"       Branch 2\"",38.1,65.09,null,82.55,88.9]
[null,"Weldolet sch. XS   Run 3\"       Branch 2½\"",41.28,76.2,null,85.73,88.9]
[null,"Weldolet sch. XS   Run 3\"       Branch 3\"",44.45,93.66,null,88.9,88.9]
[null,"Weldolet sch. XS   Run 3½\"    Branch 1/8\"",15.88,15.88,null,66.68,101.6]
[null,"Weldolet sch. XS   Run 3½\"    Branch 1/4\"",15.88,15.88,null,66.68,101.6]
[null,"Weldolet sch. XS   Run 3½\"    Branch 3/8\"",15.88,19.05,null,66.68,101.6]
[null,"Weldolet sch. XS   Run 3½\"    Branch 1/2\"",15.88,23.81,null,66.68,101.6]
[null,"Weldolet sch. XS   Run 3½\"    Branch 3/4\"",19.05,30.16,null,69.85,101.6]
[null,"Weldolet sch. XS   Run 3½\"    Branch 1\"",26.99,36.51,null,77.79,101.6]
[null,"Weldolet sch. XS   Run 3½\"    Branch 1¼\"",31.75,44.45,null,82.55,101.6]
[null,"Weldolet sch. XS   Run 3½\"    Branch 1½\"",33.34,50.8,null,84.14,101.6]
[null,"Weldolet sch. XS   Run 3½\"    Branch 2\"",38.1,65.09,null,88.9,101.6]
[null,"Weldolet sch. XS   Run 3½\"    Branch 2½\"",41.28,76.2,null,92.08,101.6]
[null,"Weldolet sch. XS   Run 3½\"    Branch 3\"",44.45,93.66,null,95.25,101.6]
[null,"Weldolet sch. XS   Run 3½\"    Branch 3½\"",47.63,101.6,null,98.43,101.6]
[null,"Weldolet sch. XS   Run 4\"       Branch 1/8\"",15.88,15.88,null,73.03,114.3]
[null,"Weldolet sch. XS   Run 4\"       Branch 1/4\"",15.88,15.88,null,73.03,114.3]
[null,"Weldolet sch. XS   Run 4\"       Branch 3/8\"",15.88,19.05,null,73.03,114.3]
[null,"Weldolet sch. XS   Run 4\"       Branch 1/2\"",15.88,23.81,null,73.03,114.3]
[null,"Weldolet sch. XS   Run 4\"       Branch 3/4\"",19.05,30.16,null,76.2,114.3]
[null,"Weldolet sch. XS   Run 4\"       Branch 1\"",26.99,36.51,null,84.14,114.3]
[null,"Weldolet sch. XS   Run 4\"       Branch 1¼\"",31.75,44.45,null,88.9,114.3]
[null,"Weldolet sch. XS   Run 4\"       Branch 1½\"",33.34,50.8,null,90.49,114.3]
[null,"Weldolet sch. XS   Run 4\"       Branch 2\"",38.1,65.09,null,95.25,114.3]
[null,"Weldolet sch. XS   Run 4\"       Branch 2½\"",41.28,76.2,null,98.43,114.3]
[null,"Weldolet sch. XS   Run 4\"       Branch 3\"",44.45,93.66,null,101.6,114.3]
[null,"Weldolet sch. XS   Run 4\"       Branch 3½\"",47.63,101.6,null,104.78,114.3]
[null,"Weldolet sch. XS   Run 4\"       Branch 4\"",20.8,120.65,null,77.95,114.3]
[null,"Weldolet sch. XS   Run 5\"       Branch 1/8\"",15.88,15.88,null,86.53,141.3]
[null,"Weldolet sch. XS   Run 5\"       Branch 1/4\"",15.88,15.88,null,86.53,141.3]
[null,"Weldolet sch. XS   Run 5\"       Branch 3/8\"",15.88,19.05,null,86.53,141.3]
[null,"Weldolet sch. XS   Run 5\"       Branch 1/2\"",15.88,23.81,null,86.53,141.3]
[null,"Weldolet sch. XS   Run 5\"       Branch 3/4\"",19.05,30.16,null,89.7,141.3]
[null,"Weldolet sch. XS   Run 5\"       Branch 1\"",26.99,36.51,null,97.64,141.3]
[null,"Weldolet sch. XS   Run 5\"       Branch 1¼\"",31.75,44.45,null,102.4,141.3]
[null,"Weldolet sch. XS   Run 5\"       Branch 1½\"",33.34,50.8,null,103.99,141.3]
[null,"Weldolet sch. XS   Run 5\"       Branch 2\"",38.1,65.09,null,108.75,141.3]
[null,"Weldolet sch. XS   Run 5\"       Branch 2½\"",41.28,76.2,null,111.93,141.3]
[null,"Weldolet sch. XS   Run 5\"       Branch 3\"",44.45,93.66,null,115.1,141.3]
[null,"Weldolet sch. XS   Run 5\"       Branch 3½\"",47.63,101.6,null,118.28,141.3]
[null,"Weldolet sch. XS   Run 5\"       Branch 4\"",20.8,120.65,null,91.45,141.3]
[null,"Weldolet sch. XS   Run 5\"       Branch 5\"",57.15,141.29,null,127.8,141.3]
[null,"Weldolet sch. XS   Run 6\"       Branch 1/8\"",15.88,15.88,null,100.02,168.28]
[null,"Weldolet sch. XS   Run 6\"       Branch 1/4\"",15.88,15.88,null,100.02,168.28]
[null,"Weldolet sch. XS   Run 6\"       Branch 3/8\"",15.88,19.05,null,100.02,168.28]
[null,"Weldolet sch. XS   Run 6\"       Branch 1/2\"",15.88,23.81,null,100.02,168.28]
[null,"Weldolet sch. XS   Run 6\"       Branch 3/4\"",19.05,30.16,null,103.19,168.28]
[null,"Weldolet sch. XS   Run 6\"       Branch 1\"",26.99,36.51,null,111.13,168.28]
[null,"Weldolet sch. XS   Run 6\"       Branch 1¼\"",31.75,44.45,null,115.89,168.28]
[null,"Weldolet sch. XS   Run 6\"       Branch 1½\"",33.34,50.8,null,117.48,168.28]
[null,"Weldolet sch. XS   Run 6\"       Branch 2\"",38.1,65.09,null,122.24,168.28]
[null,"Weldolet sch. XS   Run 6\"       Branch 2½\"",41.28,76.2,null,125.42,168.28]
[null,"Weldolet sch. XS   Run 6\"       Branch 3\"",44.45,93.66,null,128.59,168.28]
[null,"Weldolet sch. XS   Run 6\"       Branch 3½\"",47.63,101.6,null,131.77,168.28]
[null,"Weldolet sch. XS   Run 6\"       Branch 4\"",20.8,120.65,null,104.94,168.28]
[null,"Weldolet sch. XS   Run 6\"       Branch 5\"",57.15,141.29,null,141.29,168.28]
[null,"Weldolet sch. XS   Run 6\"       Branch 6\"",77.79,169.86,null,161.93,168.28]
[null,"Weldolet sch. XS   Run 8\"       Branch 1/8\"",15.88,15.88,null,125.42,219.08]
[null,"Weldolet sch. XS   Run 8\"       Branch 1/4\"",15.88,15.88,null,125.42,219.08]
[null,"Weldolet sch. XS   Run 8\"       Branch 3/8\"",15.88,19.05,null,125.42,219.08]
[null,"Weldolet sch. XS   Run 8\"       Branch 1/2\"",15.88,23.81,null,125.42,219.08]
[null,"Weldolet sch. XS   Run 8\"       Branch 3/4\"",19.05,30.16,null,128.59,219.08]
[null,"Weldolet sch. XS   Run 8\"       Branch 1\"",26.99,36.51,null,136.53,219.08]
[null,"Weldolet sch. XS   Run 8\"       Branch 1¼\"",31.75,44.45,null,141.29,219.08]
[null,"Weldolet sch. XS   Run 8\"       Branch 1½\"",33.34,50.8,null,142.88,219.08]
[null,"Weldolet sch. XS   Run 8\"       Branch 2\"",38.1,65.09,null,147.64,219.08]
[null,"Weldolet sch. XS   Run 8\"       Branch 2½\"",41.28,76.2,null,150.82,219.08]
[null,"Weldolet sch. XS   Run 8\"       Branch 3\"",44.45,93.66,null,153.99,219.08]
[null,"Weldolet sch. XS   Run 8\"       Branch 3½\"",47.63,101.6,null,157.17,219.08]
[null,"Weldolet sch. XS   Run 8\"       Branch 4\"",20.8,120.65,null,130.34,219.08]
[null,"Weldolet sch. XS   Run 8\"       Branch 5\"",57.15,141.29,null,166.69,219.08]
[null,"Weldolet sch. XS   Run 8\"       Branch 6\"",77.79,169.86,null,187.33,219.08]
[null,"Weldolet sch. XS   Run 8\"       Branch 8\"",98.43,220.66,null,207.97,219.08]
[null,"Weldolet sch. XS   Run 10\"     Branch 1/8\"",15.88,15.88,null,152.405,273.05]
[null,"Weldolet sch. XS   Run 10\"     Branch 1/4\"",15.88,15.88,null,152.405,273.05]
[null,"Weldolet sch. XS   Run 10\"     Branch 3/8\"",15.88,19.05,null,152.405,273.05]
[null,"Weldolet sch. XS   Run 10\"     Branch 1/2\"",15.88,23.81,null,152.405,273.05]
[null,"Weldolet sch. XS   Run 10\"     Branch 3/4\"",19.05,30.16,null,155.575,273.05]
[null,"Weldolet sch. XS   Run 10\"     Branch 1\"",26.99,36.51,null,163.515,273.05]
[null,"Weldolet sch. XS   Run 10\"     Branch 1¼\"",31.75,44.45,null,168.275,273.05]
[null,"Weldolet sch. XS   Run 10\"     Branch 1½\"",33.34,50.8,null,169.865,273.05]
[null,"Weldolet sch. XS   Run 10\"     Branch 2\"",38.1,65.09,null,174.625,273.05]
[null,"Weldolet sch. XS   Run 10\"     Branch 2½\"",41.28,76.2,null,177.805,273.05]
[null,"Weldolet sch. XS   Run 10\"     Branch 3\"",44.45,93.66,null,180.975,273.05]
[null,"Weldolet sch. XS   Run 10\"     Branch 3½\"",47.63,101.6,null,184.155,273.05]
[null,"Weldolet sch. XS   Run 10\"     Branch 4\"",20.8,120.65,null,157.325,273.05]
[null,"Weldolet sch. XS   Run 10\"     Branch 5\"",57.15,141.29,null,193.675,273.05]
[null,"Weldolet sch. XS   Run 10\"     Branch 6\"",77.79,169.86,null,214.315,273.05]
[null,"Weldolet sch. XS   Run 10\"     Branch 8\"",98.43,220.66,null,234.955,273.05]
[null,"Weldolet sch. XS   Run 10\"     Branch 10\"",93.66,265.11,null,230.185,273.05]
[null,"Weldolet sch. XS   Run 12\"     Branch 1/8\"",15.88,15.88,null,177.805,323.85]
[null,"Weldolet sch. XS   Run 12\"     Branch 1/4\"",15.88,15.88,null,177.805,323.85]
[null,"Weldolet sch. XS   Run 12\"     Branch 3/8\"",15.88,19.05,null,177.805,323.85]
[null,"Weldolet sch. XS   Run 12\"     Branch 1/2\"",15.88,23.81,null,177.805,323.85]
[null,"Weldolet sch. XS   Run 12\"     Branch 3/4\"",19.05,30.16,null,180.975,323.85]
[null,"Weldolet sch. XS   Run 12\"     Branch 1\"",26.99,36.51,null,188.915,323.85]
[null,"Weldolet sch. XS   Run 12\"     Branch 1¼\"",31.75,44.45,null,193.675,323.85]
[null,"Weldolet sch. XS   Run 12\"     Branch 1½\"",33.34,50.8,null,195.265,323.85]
[null,"Weldolet sch. XS   Run 12\"     Branch 2\"",38.1,65.09,null,200.025,323.85]
[null,"Weldolet sch. XS   Run 12\"     Branch 2½\"",41.28,76.2,null,203.205,323.85]
[null,"Weldolet sch. XS   Run 12\"     Branch 3\"",44.45,93.66,null,206.375,323.85]
[null,"Weldolet sch. XS   Run 12\"     Branch 3½\"",47.63,101.6,null,209.555,323.85]
[null,"Weldolet sch. XS   Run 12\"     Branch 4\"",20.8,120.65,null,182.725,323.85]
[null,"Weldolet sch. XS   Run 12\"     Branch 5\"",57.15,141.29,null,219.075,323.85]
[null,"Weldolet sch. XS   Run 12\"     Branch 6\"",77.79,169.86,null,239.715,323.85]
[null,"Weldolet sch. XS   Run 12\"     Branch 8\"",98.43,220.66,null,260.355,323.85]
[null,"Weldolet sch. XS   Run 12\"     Branch 10\"",93.66,265.11,null,255.585,323.85]
[null,"Weldolet sch. XS   Run 12\"     Branch 12\"",103.19,317.5,null,265.115,323.85]
[null,"Weldolet sch. XS   Run 14\"     Branch 1/8\"",15.88,15.88,null,193.68,355.6]
[null,"Weldolet sch. XS   Run 14\"     Branch 1/4\"",15.88,15.88,null,193.68,355.6]
[null,"Weldolet sch. XS   Run 14\"     Branch 3/8\"",15.88,19.05,null,193.68,355.6]
[null,"Weldolet sch. XS   Run 14\"     Branch 1/2\"",15.88,23.81,null,193.68,355.6]
[null,"Weldolet sch. XS   Run 14\"     Branch 3/4\"",19.05,30.16,null,196.85,355.6]
[null,"Weldolet sch. XS   Run 14\"     Branch 1\"",26.99,36.51,null,204.79,355.6]
[null,"Weldolet sch. XS   Run 14\"     Branch 1¼\"",31.75,44.45,null,209.55,355.6]
[null,"Weldolet sch. XS   Run 14\"     Branch 1½\"",33.34,50.8,null,211.14,355.6]
[null,"Weldolet sch. XS   Run 14\"     Branch 2\"",38.1,65.09,null,215.9,355.6]
[null,"Weldolet sch. XS   Run 14\"     Branch 2½\"",41.28,76.2,null,219.08,355.6]
[null,"Weldolet sch. XS   Run 14\"     Branch 3\"",44.45,93.66,null,222.25,355.6]
[null,"Weldolet sch. XS   Run 14\"     Branch 3½\"",47.63,101.6,null,225.43,355.6]
[null,"Weldolet sch. XS   Run 14\"     Branch 4\"",20.8,120.65,null,198.6,355.6]
[null,"Weldolet sch. XS   Run 14\"     Branch 5\"",57.15,141.29,null,234.95,355.6]
[null,"Weldolet sch. XS   Run 14\"     Branch 6\"",77.79,169.86,null,255.59,355.6]
[null,"Weldolet sch. XS   Run 14\"     Branch 8\"",98.43,220.66,null,276.23,355.6]
[null,"Weldolet sch. XS   Run 14\"     Branch 10\"",93.66,265.11,null,271.46,355.6]
[null,"Weldolet sch. XS   Run 14\"     Branch 12\"",103.19,317.5,null,280.99,355.6]
[null,"Weldolet sch. XS   Run 14\"     Branch 14\"",100.01,350.94,null,277.81,355.6]
[null,"Weldolet sch. XS   Run 16\"     Branch 1/8\"",15.88,15.88,null,219.08,406.4]
[null,"Weldolet sch. XS   Run 16\"     Branch 1/4\"",15.88,15.88,null,219.08,406.4]
[null,"Weldolet sch. XS   Run 16\"     Branch 3/8\"",15.88,19.05,null,219.08,406.4]
[null,"Weldolet sch. XS   Run 16\"     Branch 1/2\"",15.88,23.81,null,219.08,406.4]
[null,"Weldolet sch. XS   Run 16\"     Branch 3/4\"",19.05,30.16,null,222.25,406.4]
[null,"Weldolet sch. XS   Run 16\"     Branch 1\"",26.99,36.51,null,230.19,406.4]
[null,"Weldolet sch. XS   Run 16\"     Branch 1¼\"",31.75,44.45,null,234.95,406.4]
[null,"Weldolet sch. XS   Run 16\"     Branch 1½\"",33.34,50.8,null,236.54,406.4]
[null,"Weldolet sch. XS   Run 16\"     Branch 2\"",38.1,65.09,null,241.3,406.4]
[null,"Weldolet sch. XS   Run 16\"     Branch 2½\"",41.28,76.2,null,244.48,406.4]
[null,"Weldolet sch. XS   Run 16\"     Branch 3\"",44.45,93.66,null,247.65,406.4]
[null,"Weldolet sch. XS   Run 16\"     Branch 3½\"",47.63,101.6,null,250.83,406.4]
[null,"Weldolet sch. XS   Run 16\"     Branch 4\"",20.8,120.65,null,224,406.4]
[null,"Weldolet sch. XS   Run 16\"     Branch 5\"",57.15,141.29,null,260.35,406.4]
[null,"Weldolet sch. XS   Run 16\"     Branch 6\"",77.79,169.86,null,280.99,406.4]
[null,"Weldolet sch. XS   Run 16\"     Branch 8\"",98.43,220.66,null,301.63,406.4]
[null,"Weldolet sch. XS   Run 16\"     Branch 10\"",93.66,265.11,null,296.86,406.4]
[null,"Weldolet sch. XS   Run 16\"     Branch 12\"",103.19,317.5,null,306.39,406.4]
[null,"Weldolet sch. XS   Run 16\"     Branch 14\"",100.01,350.94,null,303.21,406.4]
[null,"Weldolet sch. XS   Run 16\"     Branch 16\"",106.36,403.23,null,309.56,406.4]
[null,"Weldolet sch. XS   Run 18\"     Branch 1/8\"",15.88,15.88,null,244.48,457.2]
[null,"Weldolet sch. XS   Run 18\"     Branch 1/4\"",15.88,15.88,null,244.48,457.2]
[null,"Weldolet sch. XS   Run 18\"     Branch 3/8\"",15.88,19.05,null,244.48,457.2]
[null,"Weldolet sch. XS   Run 18\"     Branch 1/2\"",15.88,23.81,null,244.48,457.2]
[null,"Weldolet sch. XS   Run 18\"     Branch 3/4\"",19.05,30.16,null,247.65,457.2]
[null,"Weldolet sch. XS   Run 18\"     Branch 1\"",26.99,36.51,null,255.59,457.2]
[null,"Weldolet sch. XS   Run 18\"     Branch 1¼\"",31.75,44.45,null,260.35,457.2]
[null,"Weldolet sch. XS   Run 18\"     Branch 1½\"",33.34,50.8,null,261.94,457.2]
[null,"Weldolet sch. XS   Run 18\"     Branch 2\"",38.1,65.09,null,266.7,457.2]
[null,"Weldolet sch. XS   Run 18\"     Branch 2½\"",41.28,76.2,null,269.88,457.2]
[null,"Weldolet sch. XS   Run 18\"     Branch 3\"",44.45,93.66,null,273.05,457.2]
[null,"Weldolet sch. XS   Run 18\"     Branch 3½\"",47.63,101.6,null,276.23,457.2]
[null,"Weldolet sch. XS   Run 18\"     Branch 4\"",20.8,120.65,null,249.4,457.2]
[null,"Weldolet sch. XS   Run 18\"     Branch 5\"",57.15,141.29,null,285.75,457.2]
[null,"Weldolet sch. XS   Run 18\"     Branch 6\"",77.79,169.86,null,306.39,457.2]
[null,"Weldolet sch. XS   Run 18\"     Branch 8\"",98.43,220.66,null,327.03,457.2]
[null,"Weldolet sch. XS   Run 18\"     Branch 10\"",93.66,265.11,null,322.26,457.2]
[null,"Weldolet sch. XS   Run 18\"     Branch 12\"",103.19,317.5,null,331.79,457.2]
[null,"Weldolet sch. XS   Run 18\"     Branch 14\"",100.01,350.94,null,328.61,457.2]
[null,"Weldolet sch. XS   Run 18\"     Branch 16\"",106.36,403.23,null,334.96,457.2]
[null,"Weldolet sch. XS   Run 18\"     Branch 18\"",111.13,455.61,null,339.73,457.2]
[null,"Weldolet sch. XS   Run 20\"     Branch 1/8\"",15.88,15.88,null,269.88,508.0]
[null,"Weldolet sch. XS   Run 20\"     Branch 1/4\"",15.88,15.88,null,269.88,508.0]
[null,"Weldolet sch. XS   Run 20\"     Branch 3/8\"",15.88,19.05,null,269.88,508.0]
[null,"Weldolet sch. XS   Run 20\"     Branch 1/2\"",15.88,23.81,null,269.88,508.0]
[null,"Weldolet sch. XS   Run 20\"     Branch 3/4\"",19.05,30.16,null,273.05,508.0]
[null,"Weldolet sch. XS   Run 20\"     Branch 1\"",26.99,36.51,null,280.99,508.0]
[null,"Weldolet sch. XS   Run 20\"     Branch 1¼\"",31.75,44.45,null,285.75,508.0]
[null,"Weldolet sch. XS   Run 20\"     Branch 1½\"",33.34,50.8,null,287.34,508.0]
[null,"Weldolet sch. XS   Run 20\"     Branch 2\"",38.1,65.09,null,292.1,508.0]
[null,"Weldolet sch. XS   Run 20\"     Branch 2½\"",41.28,76.2,null,295.28,508.0]
[null,"Weldolet sch. XS   Run 20\"     Branch 3\"",44.45,93.66,null,298.45,508.0]
[null,"Weldolet sch. XS   Run 20\"     Branch 3½\"",47.63,101.6,null,301.63,508.0]
[null,"Weldolet sch. XS   Run 20\"     Branch 4\"",20.8,120.65,null,274.8,508.0]
[null,"Weldolet sch. XS   Run 20\"     Branch 5\"",57.15,141.29,null,311.15,508.0]
[null,"Weldolet sch. XS   Run 20\"     Branch 6\"",77.79,169.86,null,331.79,508.0]
[null,"Weldolet sch. XS   Run 20\"     Branch 8\"",98.43,220.66,null,352.43,508.0]
[null,"Weldolet sch. XS   Run 20\"     Branch 10\"",93.66,265.11,null,347.66,508.0]
[null,"Weldolet sch. XS   Run 20\"     Branch 12\"",103.19,317.5,null,357.19,508.0]
[null,"Weldolet sch. XS   Run 20\"     Branch 14\"",100.01,350.94,null,354.01,508.0]
[null,"Weldolet sch. XS   Run 20\"     Branch 16\"",106.36,403.23,null,360.36,508.0]
[null,"Weldolet sch. XS   Run 20\"     Branch 18\"",111.13,455.61,null,365.13,508.0]
[null,"Weldolet sch. XS   Run 20\"     Branch 20\"",119.06,509.59,null,373.06,508.0]
[null,"Weldolet sch. XS   Run 24\"     Branch 1/8\"",15.88,15.88,null,320.83,609.9]
[null,"Weldolet sch. XS   Run 24\"     Branch 1/4\"",15.88,15.88,null,320.83,609.9]
[null,"Weldolet sch. XS   Run 24\"     Branch 3/8\"",15.88,19.05,null,320.83,609.9]
[null,"Weldolet sch. XS   Run 24\"     Branch 1/2\"",15.88,23.81,null,320.83,609.9]
[null,"Weldolet sch. XS   Run 24\"     Branch 3/4\"",19.05,30.16,null,324,609.9]
[null,"Weldolet sch. XS   Run 24\"     Branch 1\"",26.99,36.51,null,331.94,609.9]
[null,"Weldolet sch. XS   Run 24\"     Branch 1¼\"",31.75,44.45,null,336.7,609.9]
[null,"Weldolet sch. XS   Run 24\"     Branch 1½\"",33.34,50.8,null,338.29,609.9]
[null,"Weldolet sch. XS   Run 24\"     Branch 2\"",38.1,65.09,null,343.05,609.9]
[null,"Weldolet sch. XS   Run 24\"     Branch 2½\"",41.28,76.2,null,346.23,609.9]
[null,"Weldolet sch. XS   Run 24\"     Branch 3\"",44.45,93.66,null,349.4,609.9]
[null,"Weldolet sch. XS   Run 24\"     Branch 3½\"",47.63,101.6,null,352.58,609.9]
[null,"Weldolet sch. XS   Run 24\"     Branch 4\"",20.8,120.65,null,325.75,609.9]
[null,"Weldolet sch. XS   Run 20\"     Branch 5\"",57.15,141.29,null,362.1,609.9]
[null,"Weldolet sch. XS   Run 24\"     Branch 6\"",77.79,169.86,null,382.74,609.9]
[null,"Weldolet sch. XS   Run 24\"     Branch 8\"",98.43,220.66,null,403.38,609.9]
[null,"Weldolet sch. XS   Run 24\"     Branch 10\"",93.66,265.11,null,398.61,609.9]
[null,"Weldolet sch. XS   Run 24\"     Branch 12\"",103.19,317.5,null,408.14,609.9]
[null,"Weldolet sch. XS   Run 24\"     Branch 14\"",100.01,350.94,null,404.96,609.9]
[null,"Weldolet sch. XS   Run 24\"     Branch 16\"",106.36,403.23,null,411.31,609.9]
[null,"Weldolet sch. XS   Run 24\"     Branch 18\"",111.13,455.61,null,416.08,609.9]
[null,"Weldolet sch. XS   Run 24\"     Branch 20\"",119.06,509.59,null,424.01,609.9]
[null,"Weldolet sch. XS   Run 24\"     Branch 24\"",139.7,614.36,null,444.65,609.9]
[null,"Weldolet sch. XXS Run 1/2\"    Branch 1/2\"",28.58,14.29,null,39.25,21.34]
[null,"Weldolet sch. XXS Run 3/4\"    Branch 1/2\"",28.58,14.29,null,41.915,26.67]
[null,"Weldolet sch. XXS Run 3/4\"    Branch 3/4\"",31.75,19.05,null,45.085,26.67]
[null,"Weldolet sch. XXS Run 1\"       Branch 1/2\"",28.58,14.29,null,45.28,33.4]
[null,"Weldolet sch. XXS Run 1\"       Branch 3/4\"",31.75,19.05,null,48.45,33.4]
[null,"Weldolet sch. XXS Run 1\"       Branch 1\"",38.1,25.4,null,54.8,33.4]
[null,"Weldolet sch. XXS Run 1¼\"    Branch 1/2\"",28.58,14.29,null,49.66,42.16]
[null,"Weldolet sch. XXS Run 1¼\"    Branch 3/4\"",31.75,19.05,null,52.83,42.16]
[null,"Weldolet sch. XXS Run 1¼\"    Branch 1\"",38.1,25.4,null,59.18,42.16]
[null,"Weldolet sch. XXS Run 1¼\"    Branch 1¼\"",50.8,33.34,null,71.88,42.16]
[null,"Weldolet sch. XXS Run 1½\"    Branch 1/2\"",28.58,14.29,null,52.71,48.26]
[null,"Weldolet sch. XXS Run 1½\"    Branch 3/4\"",31.75,19.05,null,55.88,48.26]
[null,"Weldolet sch. XXS Run 1½\"    Branch 1\"",38.1,25.4,null,62.23,48.26]
[null,"Weldolet sch. XXS Run 1½\"    Branch 1¼\"",44.45,33.34,null,68.58,48.26]
[null,"Weldolet sch. XXS Run 1½\"    Branch 1½\"",50.8,38.1,null,74.93,48.26]
[null,"Weldolet sch. XXS Run 2\"       Branch 1/2\"",28.58,14.29,null,58.745,60.33]
[null,"Weldolet sch. XXS Run 2\"       Branch 3/4\"",31.75,19.05,null,61.915,60.33]
[null,"Weldolet sch. XXS Run 2\"       Branch 1\"",38.1,25.4,null,68.265,60.33]
[null,"Weldolet sch. XXS Run 2\"       Branch 1½\"",50.8,38.1,null,80.965,60.33]
[null,"Weldolet sch. XXS Run 2\"       Branch 1/2\"",28.58,14.29,null,58.745,60.33]
[null,"Weldolet sch. XXS Run 2\"       Branch 3/4\"",31.75,19.05,null,61.915,60.33]
[null,"Weldolet sch. XXS Run 2\"       Branch 1\"",38.1,25.4,null,68.265,60.33]
[null,"Weldolet sch. XXS Run 2\"       Branch 1¼\"",44.45,33.34,null,74.615,60.33]
[null,"Weldolet sch. XXS Run 2\"       Branch 1½\"",50.8,38.1,null,80.965,60.33]
[null,"Weldolet sch. XXS Run 2\"       Branch 2\"",55.56,42.86,null,92.075,73.03]
[null,"Weldolet sch. XXS Run 2½\"    Branch 1\"",38.1,25.4,null,74.615,73.03]
[null,"Weldolet sch. XXS Run 2½\"    Branch 1¼\"",44.45,33.34,null,80.965,73.03]
[null,"Weldolet sch. XXS Run 2½\"    Branch 1½\"",50.8,38.1,null,87.315,73.03]
[null,"Weldolet sch. XXS Run 2½\"    Branch 2\"",55.56,42.86,null,92.075,73.03]
[null,"Weldolet sch. XXS Run 2½\"    Branch 2½\"",61.91,53.98,null,98.425,73.03]
[null,"Weldolet sch. XXS Run 3\"       Branch 1/2\"",28.58,14.29,null,73.03,88.9]
[null,"Weldolet sch. XXS Run 3\"       Branch 3/4\"",31.75,19.05,null,76.2,88.9]
[null,"Weldolet sch. XXS Run 3\"       Branch 1\"",38.1,25.4,null,82.55,88.9]
[null,"Weldolet sch. XXS Run 3\"       Branch 1¼\"",44.45,33.34,null,88.9,88.9]
[null,"Weldolet sch. XXS Run 3\"       Branch 1½\"",50.8,38.1,null,95.25,88.9]
[null,"Weldolet sch. XXS Run 3\"       Branch 2\"",55.56,42.86,null,100.01,88.9]
[null,"Weldolet sch. XXS Run 3\"       Branch 2½\"",61.91,53.98,null,106.36,88.9]
[null,"Weldolet sch. XXS Run 3\"       Branch 3\"",73.03,73.03,null,117.48,88.9]
[null,"Weldolet sch. XXS Run 4\"       Branch 1/2\"",28.58,14.29,null,85.73,114.3]
[null,"Weldolet sch. XXS Run 4\"       Branch 3/4\"",31.75,19.05,null,88.9,114.3]
[null,"Weldolet sch. XXS Run 4\"       Branch 1\"",38.1,25.4,null,95.25,114.3]
[null,"Weldolet sch. XXS Run 4\"       Branch 1¼\"",44.45,33.34,null,101.6,114.3]
[null,"Weldolet sch. XXS Run 4\"       Branch 1½\"",50.8,38.1,null,107.95,114.3]
[null,"Weldolet sch. XXS Run 4\"       Branch 2\"",55.56,42.86,null,112.71,114.3]
[null,"Weldolet sch. XXS Run 4\"       Branch 2½\"",61.91,53.98,null,119.06,114.3]
[null,"Weldolet sch. XXS Run 4\"       Branch 3\"",73.03,73.03,null,130.18,114.3]
[null,"Weldolet sch. XXS Run 4\"       Branch 4\"",84.14,98.43,null,141.29,114.3]
[null,"Weldolet sch. XXS Run 5\"       Branch 1/2\"",28.58,14.29,null,99.23,141.3]
[null,"Weldolet sch. XXS Run 5\"       Branch 3/4\"",31.75,19.05,null,102.4,141.3]
[null,"Weldolet sch. XXS Run 5\"       Branch 1\"",38.1,25.4,null,108.75,141.3]
[null,"Weldolet sch. XXS Run 5\"       Branch 1¼\"",44.45,33.34,null,115.1,141.3]
[null,"Weldolet sch. XXS Run 5\"       Branch 1½\"",50.8,38.1,null,121.45,141.3]
[null,"Weldolet sch. XXS Run 5\"       Branch 2\"",55.56,42.86,null,126.21,141.3]
[null,"Weldolet sch. XXS Run 5\"       Branch 2½\"",61.91,53.98,null,132.56,141.3]
[null,"Weldolet sch. XXS Run 5\"       Branch 3\"",73.03,73.03,null,143.68,141.3]
[null,"Weldolet sch. XXS Run 5\"       Branch 4\"",84.14,98.43,null,154.79,141.3]
[null,"Weldolet sch. XXS Run 5\"       Branch 5\"",93.66,122.24,null,164.31,141.3]
[null,"Weldolet sch. XXS Run 6\"       Branch 1/2\"",28.58,14.29,null,112.72,168.28]
[null,"Weldolet sch. XXS Run 6\"       Branch 3/4\"",31.75,19.05,null,115.89,168.28]
[null,"Weldolet sch. XXS Run 6\"       Branch 1\"",38.1,25.4,null,122.24,168.28]
[null,"Weldolet sch. XXS Run 6\"       Branch 1¼\"",44.45,33.34,null,128.59,168.28]
[null,"Weldolet sch. XXS Run 6\"       Branch 1½\"",50.8,38.1,null,134.94,168.28]
[null,"Weldolet sch. XXS Run 6\"       Branch 2\"",55.56,42.86,null,139.7,168.28]
[null,"Weldolet sch. XXS Run 6\"       Branch 2½\"",61.91,53.98,null,146.05,168.28]
[null,"Weldolet sch. XXS Run 6\"       Branch 3\"",73.03,73.03,null,157.17,168.28]
[null,"Weldolet sch. XXS Run 6\"       Branch 4\"",84.14,98.43,null,168.28,168.28]
[null,"Weldolet sch. XXS Run 6\"       Branch 5\"",93.66,122.24,null,177.8,168.28]
[null,"Weldolet sch. XXS Run 6\"       Branch 6\"",104.78,146.05,null,188.92,168.28]

{"sheet":"Tolerences","index":22,"n_rows":17,"n_cols":4,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["WN Flange tol. Acc. Ansi:"]
["D","24\"/ DN 600 and <","± 1,6","mm"]
[null,"< 24\"/ DN 600","± 3,2","mm"]
["di","10\"/ DN 250 and <","+ 0,8","mm"]
[null,"12\"-18\"/ DN 300-450","+ 1,6","mm"]
[null,"20\"/ DN 500 and >","- 1,6 / + 3,2","mm"]
["do","5\"/ DN 125 and <","- 0,8 / + 2,4","mm"]
[null,"6\"/ DN 150 and >","- 0,8 / + 4,0","mm"]
["k","All sizes","± 1,6","mm"]
["h","10\"/ DN 250 and <","± 1,6","mm"]
[null,"12\"/ DN 300 and >","± 3,2","mm"]
["b","18\"/ DN 450 and <","+ 3,2","mm"]
[null,"20\"/ DN 500 and >","+ 4,8","mm"]
["d1","If f = 1,6 mm","± 0,8","mm"]
[null,"If f = 6,4 mm","± 0,5","mm"]
["m","24\"/ ø 610 and <","± 1,6","mm"]
[null,"> 24\"/ ø 610","± 3,2","mm"]

{"sheet":"Details & facing","index":23,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":true,"merged":[]}

{"sheet":"Attributes","index":24,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":true,"merged":[]}